{"text_format":"1","workbook":"xlsx","n_sheets":27,"sheets":["How_to_fill_out","FAQ","Cover_Sheet","BST","1_RB-General","15_ED","2_REACH","3_PAH","4_Plasticizers","5_ROHS","6_ELV","7_GADSL","8_Battery directive","9_Manufacturing_Materials","10_Cooling_Lubricants","11_Packaging","GB","GB Handelsware Nicht Automobil","12_Critical Raw Materials","13_IMO","14_CN-RoHS","Translator","16_California_Proposition_65","17_CN-ELV","18_TSCA (Sec. 5(a)(2),Sec 6(h))","19_PFAS World","Change_History"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":72,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"How_to_fill_out","index":0,"n_rows":126,"n_cols":11,"rows_kept":126,"cut":false,"hidden":false,"merged":[[79,0,83,1],[24,1,26,7],[7,5,7,7],[0,0,1,2],[14,0,14,6],[9,0,9,4],[2,0,3,3],[2,4,3,7],[6,0,6,2],[7,0,7,4],[8,0,8,4],[10,0,10,4],[11,0,11,4],[0,6,0,7],[19,1,19,7],[125,1,125,7],[16,1,16,7],[51,1,51,7],[22,1,22,7],[74,1,74,7],[66,1,66,6],[67,1,67,6],[68,1,68,6],[69,1,69,6],[70,1,70,6],[71,1,71,6],[23,1,23,7],[28,1,28,7],[99,1,99,7],[33,0,36,7],[104,0,112,1]]}
[{"$f":"Translator!B870","v":"How to fill out"},null,null,null,null,null,{"$f":"Translator!B5","v":"Edition 2024-04-11"},null,null,null,{"$f":"Translator!C2","v":"English"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!D2","v":"Deutsch"}]
["Please select language\nBitte Sprache wählen",null,null,null,"English",null,null,null,null,null,{"$f":"Translator!E2","v":"中文"}]
[]
[]
[]
[{"$f":"Translator!B60","v":"NOTES - before you start:"}]
[{"$f":"Translator!B57","v":"Please read the text of the Bosch Norm N 2580-1"}]
[{"$f":"Translator!B871","v":"Please enable macro"}]
[{"$f":"Translator!B872","v":"Below you find the working steps"}]
[{"$f":"Translator!B873","v":"If you have questions see the tab \"FAQ\""}]
[{"$f":"Translator!B874","v":"To start click on tab \"Cover_Sheet\""}]
[]
[]
[{"$f":"Translator!B58","v":"5 Steps"}]
[]
[null,{"$f":"Translator!B889","v":"Fill out: cover sheet, at least the yellow lines"}]
[]
[]
[null,{"$f":"Translator!B890","v":"Cover sheet - Selection: Type of supplied material"}]
[]
[]
[null,{"$f":"Translator!B891","v":"Selection: division or Bosch reference list"}]
[]
[null,{"$f":"Translator!B892","v":"Fill out: if necessery, edit opened tabs (fill out the relevant fields only) and complete the cover sheet according the information in the tabs"}]
[]
[]
[]
[null,{"$f":"Translator!B893","v":"Send back "}]
[]
[]
["1.",{"$f":"Translator!B889","v":"Fill out: cover sheet, at least the yellow lines"}]
[]
[{"$f":"Translator!B896","v":"Summary of declarations is possible when the ingredients are identical in type and concentration in the supplied materials (e. g. use of the same material in product series or product families). In these cases several material numbers, supplier- and/or Bosch-part numbers may be entered in the same form sheet."}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["2. ",{"$f":"Translator!B890","v":"Cover sheet - Selection: Type of supplied material"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"Translator!B1139","v":"For \"type of supplied material\" there are following cases:"}]
[null,{"$f":"Translator!B1140","v":"- Remains in or on the Bosch product: continue with step 3"}]
[null,{"$f":"Translator!B1141","v":"- Does not remain in or on the Bosch product: continue with step 4"}]
[null,{"$f":"Translator!B1142","v":"- Merchandise automotive: continue with step 4"}]
[null,{"$f":"Translator!B1143","v":"- Merchandise non-automotive: continue with step 3"}]
[null,{"$f":"Translator!B1144","v":"- Bosch reference list: continue with step 4"}]
[]
[]
["3. ",{"$f":"Translator!B894","v":"Selection: division or Bosch reference list - confirm with OK"}]
[]
[]
[]
[]
[{"$f":"Translator!B897","v":"You cannot select multiple divisions at once. "}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["4. ",{"$f":"Translator!B892","v":"Fill out: if necessery, edit opened tabs (fill out the relevant fields only) and complete the cover sheet according the information in the tabs"}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["5. ",{"$f":"Translator!B895","v":"Send back: Print cover sheet, sign, scan, return to the responsible Bosch purchasing department the scan and the entire Excel file together in one e-mail."}]

{"sheet":"FAQ","index":1,"n_rows":37,"n_cols":3,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["Lead dinitrate","Silicic acid, lead salt","4-Aminoazobenzene"]
[{"$f":"Translator!B912","v":"Sole Representative (Reach)"},null,{"$f":"Translator!B913","v":"Companies from countries outside of the European Union cannot (pre-)register on their own, they need to appoint an Only Representative. The Only Representative represents your company officially and performs your company’s REACH obligations. \nFor further information see: Regulation (EC) No 1907/2006 - REACH Article 8"}]
[{"$f":"Translator!B914","v":"Batteries"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B916","v":"examples:\nportable batteries, traction batteries, accumulators"}]
[{"$f":"Translator!B917","v":"Equipped PCB; electronic assembly; electrical assembly"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B918","v":"examples:\nPCB with electric und electronic elements, relais, displays, switcher, contactor, connector, cables, transformers "}]
[{"$f":"Translator!B919","v":"CE declaration"},{"$f":"Translator!B920","v":"Does the supplier declaration replace the CE conformity declaration for 2013 RoHS?"},{"$f":"Translator!B921","v":"No. The supplier declaration is the basis for completing a CE conformity declaration and/or RoHS as the supplier declaration includes the confirmation of the supplier of compliance with the limit values for substances prohibited by the RoHS. Further it has to be observed: harmonized European standards on the RoHS CE declaration."}]
[{"$f":"Translator!B922","v":"D"},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B924","v":"The concentration of the substance must be declared if it reaches or exceeds the limit value. The declaration of the concentration recommended if it is less than or equal to the limit value."}]
[{"$f":"Translator!B925","v":"Printing"},{"$f":"Translator!B926","v":"How to print the entire file?"},{"$f":"Translator!B927","v":"Click path: File > Print > Entire workbook > OK"}]
[{"$f":"Translator!B928","v":"EC-Directive on batteries and accumulators "},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B930","v":"Directive 2006/66/EC on batteries and accumulators and waste batteries and accumulators"}]
[{"$f":"Translator!B931","v":"EC-ELV "},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B933","v":"Directive 2000/53/EC on End-of Life Vehicles"}]
[{"$f":"Translator!B934","v":"EC-REACH "},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B935","v":"Regulation (EC) No 1907/2006 concerning the Registration, Evaluation, Authorization and Restriction of Chemicals (REACH)"}]
[{"$f":"Translator!B936","v":"EC-RoHS "},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B937","v":"Directive 2011/65/EU and 2015/863/EU on the Restriction Of the use of certain Hazardous Substances in electrical and electronic equipment"}]
[{"$f":"Translator!B938","v":"EC-Directive on packaging and packaging waste "},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B939","v":"Directive 94/62/EC on packaging and packaging waste"}]
[{"$f":"Translator!B940","v":"EPA"},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B941","v":"Environmental Protection Agency of the United States of America"}]
[{"$f":"Translator!B984","v":"Colors; dye; laquers; coating; impregantion; similar material"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B942","v":"examples:\npowder coatings, conductance-, insulation-, resistor-paste"}]
[{"$f":"Translator!B983","v":"Auxiliary manufacturing materials"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B943","v":"examples:\nsolvents, lubricants, cooling lubricants, anticorrosive, electroplating, flux"}]
[{"$f":"Translator!B944","v":"GADSL"},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B945","v":"Global Automotive Declarable Substance List, includes prohibitions of materials and obligations to declare for substances that may be present in an automobile, generated by the Global Automotive Stakeholders Group (GASG)"}]
[{"$f":"Translator!B946","v":"Merchandise automotive"},{"$f":"Translator!B1155","v":"What does \"Merchandise automotive\" mean?"},{"$f":"Translator!B1429","v":"Third-party products, manufactured without or with Bosch spezification by a third-party manufacturer and sold under the name of the external manufacturer or under the label Bosch or another Bosch brand. Applies also to products purchased only once. These products have to comply with the ELV and/or GADSL."}]
[{"$f":"Translator!B1147","v":"Merchandise non-automotive"},{"$f":"Translator!B1156","v":"What does \"Merchandise non-automotive\" mean?"},{"$f":"Translator!B1430","v":"Third-party products, manufactured without or with Bosch spezification by a third-party manufacturer and sold under the name of the external manufacturer or under the label Bosch or another Bosch brand. Applies also to products purchased only once. These products have to comply with EU-RoHS and EU-REACH."}]
[{"$f":"Translator!B948","v":"Wood, no wood-based material or composite"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B949","v":"examples:\nsolid wood"}]
[{"$f":"Translator!B950","v":"IMDS"},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B951","v":"International Material Data System, the Internet declaration system of an association of car makers"}]
[{"$f":"Translator!B952","v":"Ceramics; glass; minerals"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B953","v":"examples:\nearthenware, stoneware, porcelain, optical glas, glass fiber, mineral fiber"}]
[{"$f":"Translator!B954","v":"Adhesives; sealing material; resines"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B955","v":"examples:\npolyurethane adhesive, grouting, epoxy resin"}]
[{"$f":"Translator!B956","v":"Plastic, elastomers"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B957","v":"examples:\nPA, PE, PP, PVC, PS, PUR, NBR, EPDM"}]
[{"$f":"Translator!B958","v":"Metals"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B959","v":"examples:\nsteel, cooper, aluminium, brass, magnesium casting"}]
[{"$f":"Translator!B960","v":"Metallic surface"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B961","v":"examples:\nwear protection, corrosion protection, nickel, cadmium, chrome, zinc"}]
[{"$f":"Translator!B962","v":"P"},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B963","v":"A concentration value must always be given, even if the concentration of the substance is below or reaches the limit value."}]
[{"$f":"Translator!B1133","v":"PAH"},{"$f":"Translator!B1134","v":"Polycyclical aromatic hydrocarbons"},{"$f":"Translator!B1135","v":"formed e.g. during incomplete combustion of organic substances. Occurrence in e.g. mineral oil, bitumen, pitch, tar, carbon black and products made therefrom"}]
[{"$f":"Translator!B964","v":"Product or merchandise does not contain a substance which is released during intended use"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B965","v":"examples:\nbrushless motor, pump in closed loop, LCD-display, DVD-drive"}]
[{"$f":"Translator!B966","v":"Product or merchandise does contain a substance which is released during intended use"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B967","v":"examples\npressure vessel with cleaning agent, printer, metering unit"}]
[{"$f":"Translator!B968","v":"Search"},{"$f":"Translator!B969","v":"How can I search over the entire xls-file?"},{"$f":"Translator!B970","v":"Path: Edit > Find > Options > Click on Drop Down \"Workbook\" > click on Drop Down \"Find what\""}]
[{"$f":"Translator!B971","v":"SVHC"},{"$f":"Translator!B923","v":"What does the abbreviation mean?"},{"$f":"Translator!B972","v":"Substances Of Very High Concern, substances that give rise to particular concern, defined in the nomination listing of the European Chemicals Agency (ECHA)"}]
[{"$f":"Translator!B973","v":"Textile; leather"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B974","v":"examples\nwrapper, ribbon, jacket"}]
[{"$f":"Translator!B975","v":"Unequipped PCB; electronic component"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B976","v":"examples:\nPCB without electronic or electric components, capcitors, resistors, IC, transistors, diodes"}]
[{"$f":"Translator!B1149","v":"Remains in or on the Bosch product"},{"$f":"Translator!B1153","v":"What does \"Remains in or on the Bosch product\" mean?"},{"$f":"Translator!B1150","v":"Includes all materials which the Bosch customer receives with the product."}]
[{"$f":"Translator!B1151","v":"Does not remain in or on the Bosch product"},{"$f":"Translator!B1154","v":"What does \"Does not remain in or on the Bosch product\" mean?"},{"$f":"Translator!B1152","v":"Includes all materials which do not arrive at the Bosch customer."}]
[{"$f":"Translator!B977","v":"Composite"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B978","v":"examples\nplastic coated metal, metal matrix composite, fiber ceramics composite, plywood, OSB panels"}]
[{"$f":"Translator!B979","v":"Packaging"},{"$f":"Translator!B915","v":"What does this cover?"},{"$f":"Translator!B980","v":"examples\npaper, plastic, anti corrosive paper, drying agent, treated wood"}]

{"sheet":"Cover_Sheet","index":2,"n_rows":41,"n_cols":16,"rows_kept":41,"cut":false,"hidden":false,"merged":[[12,3,12,4],[8,3,8,4],[41,0,41,1],[40,0,40,1],[41,3,41,4],[40,3,40,4],[38,0,38,4],[39,0,39,4],[23,0,23,2],[25,0,25,2],[26,0,27,0],[26,1,27,1],[0,0,0,2],[11,3,11,4],[10,3,10,4],[9,3,9,4],[2,3,2,4],[1,3,1,4],[7,3,7,4],[6,3,6,4],[5,3,5,4],[3,3,3,4],[4,3,4,4]]}
[{"$f":"Translator!B6","v":"Cover Sheet Supplier Declaration of Substances"},null,null,"Please select language\nBitte Sprache wählen","English",0,{"$f":"Translator!B8","v":"Please select / Restart"},null,null,{"$f":"Translator!C2","v":"English"},{"$f":"Translator!B8","v":"Please select / Restart"},null,{"$f":"Translator!B8","v":"Please select / Restart"},null,null,{"$f":"Translator!B3794","v":"Yes - all contained CRM declared"}]
[null,{"$f":"Translator!B9","v":"Supplier"},{"$f":"Translator!B12","v":"Name"},null,null,"English",null,null,null,{"$f":"Translator!D2","v":"Deutsch"},{"$f":"Translator!B900","v":"Remains in or on the Bosch product"},null,"Automotive Aftermarket (AA)",null,null,{"$f":"Translator!B3795","v":"No - no CRM contained"}]
[null,null,{"$f":"Translator!B13","v":"Bosch Supplier Number (RBSNO)"},null,null,null,{"$f":"Translator!B644","v":"Battery"},null,null,{"$f":"Translator!E2","v":"中文"},{"$f":"Translator!B901","v":"Does not remain in or on the Bosch product"},null,"Automotive Electronics (AE)"]
[null,null,{"$f":"Translator!B14","v":"Contact person"},null,null,null,{"$f":"Translator!B645","v":"Assembled curcuit board; electronic assembly; electric assembly"},null,null,null,{"$f":"Translator!B902","v":"Merchandise automotive"},null,"Car Multimedia (CM)"]
[null,null,{"$f":"Translator!B899","v":"Name of only representative in accordance with REACH (see FAQ for more information)"},null,null,null,{"$f":"Translator!B646","v":"Color;dye; varnish; coating; impregnation; similar material"},null,null,null,{"$f":"Translator!B903","v":"Merchandise non-automotive"},null,"Chassis Systems Control (CC)"]
[null,{"$f":"Translator!B10","v":"Bosch purchasing"},{"$f":"Translator!B14","v":"Contact person"},null,null,null,{"$f":"Translator!B647","v":"Auxiliary manufacturing material, also cooling lubricants not remaining in or on product"},null,null,null,{"$f":"Translator!B904","v":"Bosch Reference List"},null,"Diesel Systems (DS)"]
[null,{"$f":"Translator!B11","v":"Supplied material"},{"$f":"Translator!B641","v":"Type of supplied material\n"},"Please select / Restart",null,2,{"$f":"Translator!B649","v":"Ceramics; glass; minerals"},null,null,null,null,null,"Electrical Drives (ED)"]
[null,null,{"$f":"Translator!B16","v":"Supplier Material Numbers"},null,null,1,{"$f":"Translator!B650","v":"Adhesive; sealing material; resins"},null,null,null,null,null,"Gasoline Systems (GS)"]
[null,null,{"$f":"Translator!B17","v":"Bosch part numbers"},null,null,null,{"$f":"Translator!B651","v":"Plastic; elastomer"},null,null,null,null,null,"Packaging Technology (PA)"]
[null,null,{"$f":"Translator!B18","v":"Name of Material/Component"},null,null,null,{"$f":"Translator!B652","v":"Metal"},null,null,null,null,null,"Power Tools (PT)"]
[null,null,{"$f":"Translator!B19","v":"Material is part of the following Bosch product- / product series-part numbers"},null,null,null,{"$f":"Translator!B653","v":"Fabric, leather"},null,null,null,null,null,"Security Systems (ST)"]
[null,null,{"$f":"Translator!B642","v":"Content of the delivered material. Exact designation of the material supplied (e.g. Battery, screw made of material xyz or cutting steel made of material 11SMN30, reference to IMDS ID, CDX material"},null,null,null,{"$f":"Translator!B648","v":"Auxiliary manufacturing material, also cooling lubricants which remain in or on product"},null,null,null,null,null,"Drive and Control Technology - Rexroth AG (DC)"]
[null,null,{"$f":"Translator!B660","v":"Selected divisions"},"VM ",null,null,{"$f":"Translator!B654","v":"Unequipped curcuit board; device for curcuit board; electronic component"},null,null,null,null,null,"Solar Energy (SE)"]
[{"$f":"Translator!B20","v":"Tab"},{"$f":"Translator!B21","v":"Regulated Material"},{"$f":"Translator!B22","v":"Regulations valid worldwide for Bosch"},{"$f":"Translator!B24","v":"Is the regulation complied with?\nSelect option from drop down menu"},{"$f":"Translator!B25","v":"Declaration in Tab made?\nSelect option from drop down"},null,{"$f":"Translator!B655","v":"Composite material"},null,null,null,null,null,"Starter Motors and Generators (SG)"]
[1,{"$f":"Translator!B30","v":"All materials"},{"$f":"Translator!B40","v":"Tab: 1_RB-General\nDifferent Regulations covering Asbestos, Mercury, Ozon-depleting substances, Greenhouse gases Radioactive substances, Biocides, substances of Stockholm convention (e.g. PFOS)"},null,null,null,{"$f":"Translator!B656","v":"Packaging"},null,null,{"$f":"Translator!B26","v":"Yes"},{"$f":"Translator!B28","v":"No obligation to declare"},{"$f":"Translator!B29","v":"Other declaration format used"},"Thermotechnology (TT)"]
[2,{"$f":"Translator!B30","v":"All materials"},{"$f":"Translator!B41","v":"Tab: 2_REACH \nEC-REACH"},null,null,null,{"$f":"Translator!B657","v":"Wood, no wood-based material or composite"}]
[3,{"$f":"Translator!B31","v":"All materials which contain polycyclic aromatic hydrocarbons (PAH)"},{"$f":"Translator!B42","v":"Tab: 3_PAH \nRules for polycyclic aromatic hydrocarbons"}]
[4,{"$f":"Translator!B32","v":"All materials which contain plasticizers / phthalates"},{"$f":"Translator!B43","v":"Tab: 4_Plasticizers\nRules for plasticizers / phthalates"}]
[5,{"$f":"Translator!B30","v":"All materials"},{"$f":"Translator!B44","v":"Tab: 5_ROHS\nEC-RoHS"},null,null,null,null,null,null,"Nein"]
[6,{"$f":"Translator!$B$34","v":"All materials for motor vehicles that are subject to EU-ELV"},{"$f":"Translator!$B$45","v":"Tab: 6_ELV\nEC-ELV"}]
[7,{"$f":"Translator!$B$35","v":"All materials destined for customers demanding GADSL"},{"$f":"Translator!$B$46","v":"Tab: 7_GADSL\nGADSL"},null,null,null,null,null,null,{"$f":"Translator!B26","v":"Yes"},{"$f":"Translator!B26","v":"Yes"},{"$f":"Translator!B26","v":"Yes"},{"$f":"Translator!B2698","v":"Yes with declaration"}]
[8,{"$f":"Translator!$B$36","v":"Batteries and accumulators"},{"$f":"Translator!$B$47","v":"Tab: 8_Batteries\nEC-Directive on batteries and accumulators"},null,null,null,null,null,null,{"$f":"Translator!B27","v":"No"},{"$f":"Translator!B27","v":"No"},{"$f":"Translator!B27","v":"No"},{"$f":"Translator!B2699","v":"Nothing to declare"}]
[9,{"$f":"Translator!$B$37","v":"Auxiliary manufacturing materials, e.g. lubricants, cleaning substances, anticorrosive agents"},{"$f":"Translator!$B$48","v":"Tab: 9_Manufacturing_Materials\nRules for auxiliary manufacturing materials excl. cooling lubricants"},null,null,null,null,null,null,{"$f":"Translator!B663","v":"not applicable"},{"$f":"Translator!B2697","v":"Yes with exception"},{"$f":"Translator!B2698","v":"Yes with declaration"}]
[{"$f":"Translator!$B$1214","v":"Safety Data Sheet (SDS) added ?"}]
[10,{"$f":"Translator!$B$38","v":"Cooling lubricants"},{"$f":"Translator!$B$49","v":"Tab: 10_Cooling_Lubricants\nRules for cooling lubricants"},null,null,null,{"$f":"Translator!B1164","v":"Designation of the material that contains the regulated substance and concentration.\n\nExplanation: Enter the designation and concentration of ingredient in the component (s) which the substance is used e.g. 10% Aluminium in a motor; 1% Lead in a resistor, 0,15% silver in a wire."},{"$f":"Translator!B1165","v":"Examples of occurrence"},{"$f":"Translator!B1166","v":"Concentration of ingredient \n[mass%]"}]
[{"$f":"Translator!$B$1214","v":"Safety Data Sheet (SDS) added ?"}]
[11,{"$f":"Translator!$B$39","v":"Packaging and packaging components"},{"$f":"Translator!$B$50","v":"11.a EU Packaging directive 94/62/EC"}]
[null,null,{"$f":"Translator!$B$3799","v":"11. b France Decree No. 2022-105"}]
[12,{"$f":"Translator!$B$30","v":"All materials"},{"$f":"Translator!$B$3030","v":"Tab 12: Critical Raw Materials (EU)\n(high economic importance)"}]
[13,{"$f":"Translator!$B$1428","v":"All materials for ships or equipment for ships impacted by the Resolution MEPC.197(62)"},{"$f":"Translator!$B$1286","v":"Tab: 13 IMO"}]
[14,"CN-RoHS","Register 14: CN-RoHS"]
[15,"Electrical Drives","Register 15: ED"]
[16,{"$f":"Translator!$B$30","v":"All materials"},"Register 16: California Proposition"]
[17,"CN-ELV","Tab: 17 CN-ELV"]
[18,{"$f":"Translator!$B$30","v":"All materials"},{"$f":"Translator!$B$623","v":"Tab: (18_TSCA (Sec. 5(a)(2), Sec 6(h))"}]
[19,{"$f":"Translator!$B$30","v":"All materials"},{"$f":"Translator!$B$2884","v":"Tab 19: PFAS World (based on US Maine PFAS)"}]
["BST","Bosch Sensortec (BST) / Akustica (AKUS)",{"$f":"Translator!$B$638","v":"Tab: BST\nregulations for divisions Bosch Sensortec (BST)"}]
["DC","Drive and Control Technology - Rexroth AG (DC)",{"$f":"Translator!$B$639","v":"Tab: DC\nregulations for division Drive and Control Technology DC (Rexroth)"}]
[{"$f":"Translator!B52","v":"Supplier Signature"}]
[{"$f":"Translator!B53","v":"We declare that all the data in this supplier declaration including all tabs and enclosures is complete and true. All data reflect the current knowledge. If the status of knowledge changes the supplier will send an updated supplier declaration to the responsible Bosch purchasing authority."}]
[{"$f":"Translator!B54","v":"Place, date"},null,{"$f":"Translator!B55","v":"Name of authorized representatives"},{"$f":"Translator!B56","v":"Signature of authorized representatives"}]

{"sheet":"BST","index":3,"n_rows":112,"n_cols":9,"rows_kept":112,"cut":false,"hidden":true,"merged":[[0,0,0,8],[2,0,2,8],[98,0,98,8],[94,3,97,3],[59,3,67,3],[58,0,58,8],[69,3,73,3],[68,0,68,8],[75,3,77,3],[74,0,74,8],[78,0,78,8],[89,0,89,8]]}
[{"$f":"Translator!B638","v":"Tab: BST\nregulations for divisions Bosch Sensortec (BST)"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B95","v":"Limit value"},{"$f":"Translator!B96","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B98","v":"Cont.nr. in REACH"},{"$f":"Translator!B99","v":"Restriction conditions"},{"$f":"Translator!B100","v":"Limits"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B103","v":0},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B124","v":0},null,null,{"$f":"Translator!B1417","v":"=- thermal insulations\n- friction coatings\n- seals\n- building materials"},null,"E2012"]
[{"$f":"Translator!B106","v":"Dimethyl fumarate"},"624-49-7 ","P",{"$f":"Translator!B123","v":"0,1 mg/kg"},null,null,{"$f":"Translator!B1418","v":"Biocide used in packaging against mold "},{"$f":"Translator!B1416","v":"2009/251/EC\nThis Decision is applicable until 15 March 2010.\nincluded in Reach"},"E2012"]
[{"$f":"Translator!B109","v":"Perfluorooctanesulfonic acid and its derivatives (PFOS)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,{"$f":"Translator!B1419","v":"- elastomers\n- impregnation textiles\n- chromium plating\n- lithography\n- fire fighting foam\n- hydraulic fluids"},{"$f":"Translator!B1420","v":"Persistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"E2012"]
[{"$f":"Translator!B110","v":"Comments"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B129","v":0},null,null,{"$f":"Translator!B1421","v":"Contamination in steel"},null,"E2012"]
[{"$f":"Translator!B111","v":"Entry\n- included ( E )\n- changed ( C )"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B128","v":0},null,null,{"$f":"Translator!B1422","v":"- coolants\n- firefighting agents\n- cleaning agents"},{"$f":"Translator!B1423","v":"Regulation (EC) No 1005/2009"},"E2012"]
[{"$f":"Translator!B112","v":"Tricresyl phosphates and isomers (TCP)"},{"$f":"Translator!B122","v":"78-30-8 and 1330-78-5"},"P",{"$f":"Translator!B133","v":"0,1 m%"},null,null,{"$f":"Translator!B1424","v":"=- Flame retardants\n- Plasticizers\n- Lubricants\n- Coolants\n- Solvents"},null,"E2012"]
[{"$f":"Translator!B116","v":"polychlorinated naphthalenes (more than 3 chlorine atoms)"},"70776-03-3","P",{"$f":"Translator!B133","v":"0,1 m%"},null,null,null,null,"E2012"]
[{"$f":"Translator!B1105","v":"Chlorine (Cl)"},"7782-50-5","P","900ppm, Br+Cl 1500ppm",null,null,null,{"$f":"Translator!B1425","v":"Halogen Free Industry Standard, \nref IEC 6124-2-21"},"E2012"]
[{"$f":"Translator!B1106","v":"Bromine (Br)"},"7726-95-6","P","900ppm, Br+Cl 1500ppm",null,null,null,{"$f":"Translator!B1425","v":"Halogen Free Industry Standard, \nref IEC 6124-2-21"},"E2012"]
[{"$f":"Translator!B1107","v":"Br in PCB Laminates"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1108","v":"Cl in PCB Laminates"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1111","v":"Tri-substituted organostannic compounds (tributyl tin or triphenyl tin compounds)"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1112","v":"Phenol,2-(2H-benzotriazol-2-yl)-4,6-bis(1,1-dimethylethyl)"},"3846-71-7","P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1113","v":"Antimony (Sb) and its compounds"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1114","v":"Red phosphorus and its compounds"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1115","v":"Beryllium and its compounds"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1116","v":"Selenium and its compounds"},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1118","v":"Halogenated dioxins and furans"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1132","v":"Prohibition on use"},null,null,null,null,"E2012"]
[{"$f":"Translator!B1119","v":"Tris(2-chloroethyl) phosphate (TCEP)"},"115-96-8","P","0,1 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B111","v":"Entry\n- included ( E )\n- changed ( C )"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B128","v":0},null,null,null,null,"E2012"]
[{"$f":"Translator!B108","v":0},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B128","v":0},null,null,{"$f":"Translator!B1422","v":"- coolants\n- firefighting agents\n- cleaning agents"},{"$f":"Translator!B1423","v":"Regulation (EC) No 1005/2009"},"E2012"]
[{"$f":"Translator!B108","v":0},{"$f":"Translator!B119","v":"Material group"},"P","0,1 m%",null,null,{"$f":"Translator!B1426","v":"Flame retardants"},{"$f":"Translator!B1427","v":"Persistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"E2012"]
[{"$f":"Translator!B1330","v":"Phenol, methyl"},"95-48-7","P","≤ 10ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1331","v":"Phenol, 2-methyl"},"106-44-5","P","≤ 10ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1332","v":"Phenol, 3-methyl"},"108-39-4","P","≤ 10ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1333","v":"Phenol, 4-methyl"},"1319-77-3","P","≤ 10ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B203","v":"Polychlorinated terphenyls (PCT)"},"61788-33-8","P","≤ 5ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1334","v":"Polychlorinated Naphtalene (PCN)"},"70776-03-3","P","≤ 5ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1336","v":"Chloromethyl-methylether (CMME) "},"107-30-2 ","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1337","v":"Depleted uranium"},"7440-61-1","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1338","v":"Formaldehyde"},"50-00-0","P","300ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1339","v":"Dodecachloropentacyclo-1,3,4-Metheno-1H-cyclobuta(cd)pentalene, Mirex"},"2385-85-5","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1340","v":"Hexachlorobenzene"},"118-74-1","P",">10ppb",null,null,null,null,"E2015"]
[{"$f":"Translator!B1341","v":"N-Nitrosamines "},"group ","P","100ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1342","v":"Pentachlorobenzene "},"608-93-5","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1343","v":"Tetrachlorobenzene, all members "},"12408-10-5\n84713-12-2 ","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1344","v":"Tetrafluoromethane"},"75-73-0","P","1000ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1345","v":"Tris...... ,"},"545-55-1","P","1000ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1346","v":"Alpha-Naphthylamine"},"134-32-7","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1347","v":"Ethyleneimine"},"151-56-4","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1348","v":"Beta-Propiolactone"},"57-57-8","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1349","v":"2-Acetylaminofluorene"},"53-96-3","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1350","v":"4-Dimethyl-aminoazobenzene"},"60-11-7","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1351","v":"1,2-dibromo-3-chloropropane"},"96-12-8","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1357","v":"Ethylene oxide"},"75-21-8","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1358","v":"Explosives"},"Group","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1359","v":"Methylethyl ketone (MEK)"},"78-93-3","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1387","v":"Bisphenol-A (BPA)"},"80-05-7","P","1000ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1360","v":"Tetrabromobisphenol A, 2,2-Bis(3,5-dibromo-4-hydroxyphenyl)propane (TBBPA)"},"79-94-7","P","1000ppm",null,null,null,null,"C2015"]
[{"$f":"Translator!B1361","v":"Polyvinylchloride (PVC)"},"9002-86-2","P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1362","v":"Brominated Flame Retardants (other than those specified in other sections of this standard)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"C2015"]
[{"$f":"Translator!B1363","v":"Chlorinated Flame Retardants (other than those specified in other sections of this standard)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1335","v":"any intentionally added content"},null,null,null,null,"C2015"]
[{"$f":"Translator!B1364","v":"Hexachlorobutadiene"},"87-68-3","P",0,null,null,null,null,"E2015"]
[{"$f":"Translator!B1365","v":"Nitrogentrifluoride"},"7783-54-2","P",0,null,null,null,null,"E2015"]
[{"$f":"Translator!B1366","v":"Sulphur hexafluoride"},"2551-62-4","P",0,null,null,null,null,"E2015"]
[{"$f":"Translator!B1367","v":"Azo compound"}]
[{"$f":"Translator!B1368","v":"4-chloro-o-toluidine"},"95-69-2","P",{"$f":"Translator!B1353","v":"0,003% by weight(30 ppm) of the finished textile/leather product Remark 1"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1369","v":"5-nitro-o-toluidine"},"99-55-8","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1370","v":"4-chloroaniline"},"106-47-8","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1371","v":"4-methoxy-m-phenylenediamine"},"615-05-4","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1372","v":"3,3'-dichlorobenzidine"},"91-94-1","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1373","v":"3,3'-dimethoxybenzidine"},"119-90-4","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1374","v":"3,3'-dimethylbenzidine"},"119-93-7","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1375","v":"4,4'-thiodianiline"},"139-65-1","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1376","v":"2,4,5-trimethylaniline"},"137-17-7","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1377","v":"DBT"},null,"P"]
[{"$f":"Translator!B1378","v":"Dibutyltin oxide"},"818-08-6","P",{"$f":"Translator!B1354","v":"The equivalent 0,1% by weight  (1 000 ppm) of tin in a material "},null,null,null,null,"E2015"]
[{"$f":"Translator!B1379","v":"Dibutyltin diacetate"},"1067-33-0","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1380","v":"Dibutyltin dilaurate "},"77-58-7","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1381","v":"Dibutyltin maleate "},"78-04-6","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1382","v":"Other dibutyltin compounds"},"    -","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1383","v":"DOT"},null,"P"]
[{"$f":"Translator!B1384","v":"Dioctyl Tin Oxide "},"870-08-6","P",{"$f":"Translator!B1354","v":"The equivalent 0,1% by weight  (1 000 ppm) of tin in a material "},null,null,null,null,"E2015"]
[{"$f":"Translator!B1385","v":"Dioctyltin dilaurate "},"3648-18-8","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1386","v":"Other Dioctyltin compounds"},"   -","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1388","v":"Halogenated Hydrocarbons"}]
[{"$f":"Translator!B1389","v":"Methyl bromide"},"74-83-9","P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1390","v":"Chlorobromomethane"},"74-97-5","P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1391","v":"nPB (n-bromopropane , 1-Bromopropane)"},"106-94-5","P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1392","v":"Tetrachloroethylene (perchloroethylene) "},"127-18-4","P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1393","v":"Trichloroethylene"},"79-01-6","P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1394","v":"Fluorocarbons (FCs)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1395","v":"Monomethyl dibromo diphenyl methane (DBBT)"},"99688-47-8","P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1396","v":"Perfluorooctane acid (PFOA)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1397","v":"Polychlorinated dibenzodioxins (PCDDs)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1398","v":"Hexachlorocyclohexane isomers (HCHs)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1352","v":"Banned in Production"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1399","v":"Packaging"},null,"P"]
[{"$f":"Translator!B1401","v":"Volatile Organic Compound (VOC)"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1406","v":"VOC free ink for packaging print"},null,null,null,null,"E2015"]
[{"$f":"Translator!B1402","v":"Halogen"},null,"P",{"$f":"Translator!B1407","v":"Br:900 ppm, Cl:900 ppm, and Br+Cl :1500 ppm "},null,null,null,{"$f":"Translator!B1425","v":"Halogen Free Industry Standard, \nref IEC 6124-2-21"},"E2015"]
[{"$f":"Translator!B1403","v":"Phthalate"},{"$f":"Translator!B119","v":"Material group"},"P","<1000 ppm",null,null,null,null,"E2015"]
[{"$f":"Translator!B1404","v":"Chlorine and CFC/HCFC"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B1408","v":"The packaging material is free from chlorine and CFC/HCFC"},null,null,null,null,"E2015"]
[{"$f":"Translator!B481","v":"Lead"},"7439-92-1","P",{"$f":"Translator!B1405","v":"(Cd + Pb + Hg + Cr6+) < 100 ppm;\nCd < 50ppm"},null,null,null,{"$f":"Translator!B146","v":0},"E2015"]
[{"$f":"Translator!B482","v":"Chromium VI"},"14977-61-8","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B483","v":"Cadmium"},"7440-43-9","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B484","v":"Mercury"},"7439-97-6","P",null,null,null,null,null,"E2015"]
[{"$f":"Translator!B102","v":"Substance rated declarable (D)"}]
[{"$f":"Translator!B114","v":"N,N'-di-o-tolylguanidine (DOTG)"},"97-39-2","D","0,1 m%",null,null,{"$f":"Translator!B141","v":"Vulcanization accelerator"},{"$f":"Translator!B147","v":"Listed in GADSL;\nMay contain and emit o-toluidine. With o-toluidine contents >0.1 percent in the mixture\nhas to be considered carcinogenic.  Additionally the material data sheet o-toluidine has to be observed."},"E2012"]
[{"$f":"Translator!B115","v":"Perfluorooctanoic acid (PFOA) and its salts"},{"$f":"Translator!B119","v":"Material group"},"D","0,1 m%",null,null,{"$f":"Translator!B142","v":"Polymerization agents"},{"$f":"Translator!B148","v":"Listed in GADSL ;\nscheduled prohibition acc. to EPA in 2015"},"E2012"]
[{"$f":"Translator!B1122","v":"Perfluorocarbons"},{"$f":"Translator!B119","v":"Material group"},"D","0,01 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1123","v":"Tellurium and its compounds "},{"$f":"Translator!B119","v":"Material group"},"D","0,01 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1124","v":"Tetramethylthiuram disulfide (Thiram)"},{"$f":"Translator!B119","v":"Material group"},"D","0,01 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1125","v":"Barium compounds"},{"$f":"Translator!B119","v":"Material group"},"D","0,01 m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1126","v":"Tantalum (Ta) "},"7440-25-7","D",{"$f":"Translator!B1145","v":"if intentionally added"},null,null,null,"Conflict Mineral (Dodd-Frank Act)","E2012"]
[{"$f":"Translator!B1127","v":"Tin (Sn) "},"7440-31-5","D",{"$f":"Translator!B1145","v":"if intentionally added"},null,null,null,"Conflict Mineral (Dodd-Frank Act)","E2012"]
[{"$f":"Translator!B1128","v":"Gold (Au) "},"7440-57-5","D",{"$f":"Translator!B1145","v":"if intentionally added"},null,null,null,"Conflict Mineral (Dodd-Frank Act)","E2012"]
[{"$f":"Translator!B1129","v":"Tungsten (W) "},"7440-33-7","D",{"$f":"Translator!B1145","v":"if intentionally added"},null,null,null,"Conflict Mineral (Dodd-Frank Act)","E2012"]
[{"$f":"Translator!B1130","v":"Fluorine (F)"},"7782-41-4","D","0,1m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1131","v":"Iodine (I)"},"7553-56-2","D","0,1m%",null,null,null,null,"E2012"]
[{"$f":"Translator!B1117","v":"Bismuth and its compounds"},{"$f":"Translator!B119","v":"Material group"},"D","1000ppm",null,null,null,null,"C2012"]

{"sheet":"1_RB-General","index":4,"n_rows":323,"n_cols":11,"rows_kept":323,"cut":false,"hidden":true,"merged":[[0,0,0,10],[2,0,2,10],[9,2,317,2],[9,3,317,3],[9,8,317,8],[9,9,317,9],[9,10,317,10]]}
[{"$f":"Translator!B92","v":"Diverse Rules (tab 1)"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B2835","v":"Limits"},{"$f":"Translator!B3789","v":"By Substance groups: Name of the contained substances"},{"$f":"Translator!B3790","v":"By Substance groups: CAS of the contained substances"},{"$f":"Translator!B339","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2782","v":"Examples of occurrence"},{"$f":"Translator!B2783","v":"Comments"},{"$f":"Translator!B2784","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B2792","v":"Asbestos, all mineral groups"},{"$f":"Translator!$B$2826","v":"Substance group"},"P",{"$f":"Translator!$B$2836","v":"Prohibition of use, limits and exemptions according specific regulation "},null,null,null,null,{"$f":"Translator!B2837","v":"- thermal insulations\n- friction coatings\n- seals\n- building materials"},{"$f":"Translator!B2844","v":"- Asbestos Convention 1986 (No. 162), \n'- EU-REACh Annex XVII \n'- International Maritime Organization"},"E2011"]
[{"$f":"Translator!B2793","v":"Mercury and ist compounds"},{"$f":"Translator!$B$2826","v":"Substance group"},"P",{"$f":"Translator!$B$2836","v":"Prohibition of use, limits and exemptions according specific regulation "},null,null,null,null,{"$f":"Translator!B2838","v":"electrical contacts"},{"$f":"Translator!B2845","v":"- Minamata Convention 1. Januar 2018 \n'- EU Mercury regulation  2017/852\n'- EU RoHS\n'- EU ELV\n"},"E2021"]
[{"$f":"Translator!B2794","v":"Ozon depleting substances\nz.B.: CFC, Halone"},{"$f":"Translator!$B$2826","v":"Substance group"},"P",{"$f":"Translator!$B$2836","v":"Prohibition of use, limits and exemptions according specific regulation "},null,null,null,null,{"$f":"Translator!B2839","v":"- coolants\n- firefighting agents\n- cleaning agents"},{"$f":"Translator!B2846","v":"- Montreal Protocol 1987\n'- EU 1005/2009"},"C2021"]
[{"$f":"Translator!B2795","v":"Greenhouse gases\nz.B.  carbon dioxide (CO2), Methane (CH4), nitrous oxide (N2O), hydrofluorocarbons (HFCs), perfluorocarbons (PFCs), and sulfur hexafluoride (SF6), Nitrogen trifluoride (NF3). "},{"$f":"Translator!$B$2826","v":"Substance group"},"P",{"$f":"Translator!$B$2836","v":"Prohibition of use, limits and exemptions according specific regulation "},null,null,null,null,{"$f":"Translator!B2840","v":"- coolants\n- firefighting agents\n- cleaning agents"},{"$f":"Translator!B2847","v":"- Kyoto Protokoll 16 February 2005 incl. Doha Annex\n'- EU 2021/1119, 401/2009, 2018/1999 (‘European Climate Law’)"},"E2022"]
[{"$f":"Translator!B2796","v":"Radioactive substances"},{"$f":"Translator!$B$2826","v":"Substance group"},"P",{"$f":"Translator!$B$2843","v":"Prohibition of use, exemption for ionization chamber smoke detector"},null,null,null,null,{"$f":"Translator!B2841","v":"Contamination in steel or other metals"}]
[{"$f":"Translator!B2797","v":"Biocides"},{"$f":"Translator!$B$2826","v":"Substance group"},"P",{"$f":"Translator!$B$2836","v":"Prohibition of use, limits and exemptions according specific regulation "},null,null,null,null,{"$f":"Translator!B2842","v":"Liquids, packaging, coatings on products to which substances have been added/treated to prevent infestation by harmful organisms such as algae, fungi, bacteria, in order to preserve the original properties such as paints, liquids, plastics, sealants and adhesives, binders."},{"$f":"Translator!$B$2848","v":"EU Biocid Regulation EC 528/2012"},"E2013"]
[{"$f":"Translator!B2798","v":"Endosulfan and its isomers"},"-","P",{"$f":"Translator!$B$2836","v":"Prohibition of use, limits and exemptions according specific regulation "},null,null,null,null,null,{"$f":"Translator!$B$2849","v":"- Stockholm Convention\n' EU POP Regulation EU 2019/1021 "},"C2023"]
[{"$f":"Translator!B2799","v":"Endosulfan alpha-isomer"},"959-98-8"]
[{"$f":"Translator!B2800","v":"Endosulfan"},"115-29-7"]
[{"$f":"Translator!B2801","v":"Endosulfan beta-isomer"},"33213-65-9"]
[{"$f":"Translator!B2802","v":"Heptabromodiphenyl ether (Group)"},"-"]
[{"$f":"Translator!B2803","v":"Diphenyl ether, heptabromo derivative"},"68928-80-3"]
[{"$f":"Translator!B2804","v":"Hexabromocyclododecane (HBCDD)"},"-"]
[{"$f":"Translator!B2805","v":"gamma-hexabromocyclododecane"},"134237-52-8"]
[{"$f":"Translator!B2806","v":"beta-hexabromocyclododecane"},"134237-51-7"]
[{"$f":"Translator!B2807","v":"Hexabromocyclododecane"},"25637-99-4"]
[{"$f":"Translator!B2808","v":"1,2,5,6,9,10-hexabromocyclodecane"},"3194-55-6"]
[{"$f":"Translator!B2809","v":"alpha-hexabromocyclododecane"},"134237-50-6"]
[{"$f":"Translator!B2810","v":"Hexabromodiphenyl ether (group)"},"-"]
[{"$f":"Translator!B2811","v":"Diphenyl ether, hexabromo derivative"},"36483-60-0"]
[{"$f":"Translator!B2812","v":"1,2,3-tribromo-4-(2,4,5-tribromophenoxy)benzene"},"182677-30-1"]
[{"$f":"Translator!B2813","v":"Hexachlorocyclohexanes, including lindane"},"-"]
[{"$f":"Translator!B2814","v":"γ-HCH or γ-BHC"},"58-89-9"]
[{"$f":"Translator!B2815","v":"BHC or HCH"},"608-73-1"]
[{"$f":"Translator!B2816","v":"(1α,2β,3α,4β,5α,6β)-1,2,3,4,5,6-hexachlorocyclohexane"},"319-85-7"]
[{"$f":"Translator!B2817","v":"(1α,2α,3β,4α,5β,6β)-1,2,3,4,5,6-hexachlorocyclohexane"},"319-84-6"]
[{"$f":"Translator!B2818","v":"Pentabromodiphenyl ether (group)"},"-"]
[{"$f":"Translator!B2819","v":"Diphenyl ether, pentabromo derivative"},"32534-81-9"]
[{"$f":"Translator!B2820","v":"1,3,5-tribromo-2-(3,4-dibromophenoxy)benzene"},"189084-66-0"]
[{"$f":"Translator!B2821","v":"1,2,3-tribromo-4-(2,4-dibromophenoxy)benzene"},"182346-21-0"]
[{"$f":"Translator!B2822","v":"Pentachlorophenol and its salts and esters"},"-"]
[{"$f":"Translator!B2823","v":"Acetic acid, 2,2-dichloro-, 2,3,4,5,6-pentachlorophenyl ester"},"19745-69-8"]
[{"$f":"Translator!B2824","v":"Carbonic acid, 1,1-dimethylethyl pentachlorophenyl ester"},"18942-25-1"]
[{"$f":"Translator!B2825","v":"Acetic acid, 2,2,2-trichloro-, 2,3,4,5,6-pentachlorophenyl ester"},"2879-60-9"]
[{"$f":"Translator!B2827","v":"Pentachlorophenol"},"87-86-5"]
[{"$f":"Translator!B2828","v":"Sodium pentachlorophenolate"},"131-52-2"]
[{"$f":"Translator!B2829","v":"Pentachlorophenyl laurate"},"3772-94-9"]
[{"$f":"Translator!B2830","v":"Potassium pentachlorophenolate"},"7778-73-6"]
[{"$f":"Translator!B2831","v":"N2-benzyl pentachlorophenyl N2-carboxy-L-(2-aminoglutaramate)"},"13673-51-3"]
[{"$f":"Translator!B2832","v":"Perchlorophenyl N-(benzyloxycarbonyl)-L-isoleucinate"},"13673-53-5"]
[{"$f":"Translator!B2833","v":"Perchlorophenyl S-benzyl-N-(benzyloxycarbonyl)-L-cysteinate"},"13673-54-6"]
[{"$f":"Translator!B2834","v":"Pentachlorophenyl N-[[(4-methoxyphenyl)methoxy]carbonyl]-L-serinate"},"23234-97-1"]
[{"$f":"Translator!B3439","v":"Pentachlorophenol salts"},"-"]
[{"$f":"Translator!B3440","v":"Pentachlorophenol esters"},"-"]
[{"$f":"Translator!B3441","v":"Perchlorophenyl 5-oxo-L-prolinate"},"28990-85-4"]
[{"$f":"Translator!B3442","v":"Zinc bis(pentachlorophenolate)"},"2917-32-0"]
[{"$f":"Translator!B3443","v":"Perfluorohexane-1-sulphonic acid, its salts and related substances"},"-"]
[{"$f":"Translator!B3444","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)"},"341035-71-0"]
[{"$f":"Translator!B3445","v":"Potassium perfluorohexane-1-sulphonate"},"3871-99-6"]
[{"$f":"Translator!B3446","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)"},"350836-93-0"]
[{"$f":"Translator!B3447","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt"},"70136-72-0"]
[{"$f":"Translator!B3448","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)"},"72033-41-1"]
[{"$f":"Translator!B3449","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt"},"82382-12-5"]
[{"$f":"Translator!B3450","v":"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1000597-52-3"]
[{"$f":"Translator!B3451","v":"N,N,N-tributylbutan-1-aminium tridecafluorohexane-1-sulfonate"},"108427-54-9"]
[{"$f":"Translator!B3452","v":"N,N,N-triethylethanaminium tridecafluorohexane-1-sulfonate"},"108427-55-0"]
[{"$f":"Translator!B3453","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)"},"1187817-57-7"]
[{"$f":"Translator!B3454","v":"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1310480-24-0"]
[{"$f":"Translator!B3455","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1310480-27-3"]
[{"$f":"Translator!B3456","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1310480-28-4"]
[{"$f":"Translator!B3457","v":"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"1329995-45-0"]
[{"$f":"Translator!B3458","v":"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"1329995-69-8"]
[{"$f":"Translator!B3459","v":"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"144116-10-9"]
[{"$f":"Translator!B3460","v":"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1462414-59-0"]
[{"$f":"Translator!B3461","v":"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"153443-35-7"]
[{"$f":"Translator!B3462","v":"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"189274-31-5"]
[{"$f":"Translator!B3463","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)"},"202189-84-2"]
[{"$f":"Translator!B3464","v":"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"213740-81-9"]
[{"$f":"Translator!B3465","v":"Ammonium perfluorohexane-1-sulphonate"},"68259-08-5"]
[{"$f":"Translator!B3466","v":"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)"},"70225-16-0"]
[{"$f":"Translator!B3467","v":"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)"},"866621-50-3"]
[{"$f":"Translator!B3468","v":"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"910606-39-2"]
[{"$f":"Translator!B3469","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"911027-68-4"]
[{"$f":"Translator!B3470","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"},"911027-69-5"]
[{"$f":"Translator!B3471","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)"},"92011-17-1"]
[{"$f":"Translator!B3472","v":"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"928049-42-7"]
[{"$f":"Translator!B3473","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)"},"41184-65-0"]
[{"$f":"Translator!B3474","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)"},"41242-12-0"]
[{"$f":"Translator!B3475","v":"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)"},"421555-73-9"]
[{"$f":"Translator!B3476","v":"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic"},"421555-74-0"]
[{"$f":"Translator!B3477","v":"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"425670-70-8"]
[{"$f":"Translator!B3478","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)"},"55120-77-9"]
[{"$f":"Translator!B3479","v":"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"341548-85-4"]
[{"$f":"Translator!B3480","v":"Perfluorooctane sulfonic acid and its derivatives (PFOS)\nPerfluorooctane sulfonates (PFOS) C8F17SO2X (X = OH, Metal salt (O-M+), halide, amide, and other derivatives including polymers)\n"},"1763-23-1\n2795-39-3\n29457-72-5\n29081-56-9\n70225-14-8\n56773-42-3\n251099-16-8\n4151-50-2\n31506-32-8\n1691-99-2\n24448-09-7\n307-35-7 and\nothers"]
[{"$f":"Translator!B3481","v":"Perfluorooctanoic acid (PFOA), its salts and PFOA-related substances"},"-"]
[{"$f":"Translator!B3482","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecanol"},"60699-51-6"]
[{"$f":"Translator!B3483","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl dihydrogen phosphate"},"63295-27-2"]
[{"$f":"Translator!B3484","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl dihydrogen phosphate"},"63295-28-3"]
[{"$f":"Translator!B3485","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl dihydrogen phosphate"},"63295-29-4"]
[{"$f":"Translator!B3486","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodohexadecane"},"65510-55-6"]
[{"$f":"Translator!B3487","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-nonadecafluoro-11-iodoundecane"},"65510-56-7"]
[{"$f":"Translator!B3488","v":"Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs."},"68412-69-1"]
[{"$f":"Translator!B3489","v":"1-(carboxylatomethyl)-1-(2-hydroxyethyl)-4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-oxodecyl)piperazinium"},"71356-38-2"]
[{"$f":"Translator!B3490","v":"Carboxylic acids, C7-13, perfluoro, ammonium salts"},"72968-38-8"]
[{"$f":"Translator!B3491","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-icosafluoro-11-(trifluoromethyl)dodecyl methacrylate"},"74256-14-7"]
[{"$f":"Translator!B3492","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl methacrylate"},"74256-15-8"]
[{"$f":"Translator!B3493","v":"Heptadecafluoro-1-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]nonene"},"84029-60-7"]
[{"$f":"Translator!B3494","v":"2-Propenoic acid, γ-ω-perfluoro-C8-14-alkyl esters"},"85631-54-5"]
[{"$f":"Translator!B3495","v":"2-Propenoic acid, perfluoro-C8-16-alkyl esters"},"85681-64-7"]
[{"$f":"Translator!B3496","v":"N-(3-aminopropyl)-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide"},"85938-56-3"]
[{"$f":"Translator!B3497","v":"Octanoic acid, pentadecafluoro-, branched"},"90480-55-0"]
[{"$f":"Translator!B3498","v":"Octanoic acid, pentadecafluoro-, branched, ammonium salt"},"90480-56-1"]
[{"$f":"Translator!B3499","v":"Alkyl iodides, C6-18, perfluoro"},"90622-71-2"]
[{"$f":"Translator!B3500","v":"Amides, C7-19, α-ω-perfluoro-N,N-bis(hydroxyethyl)"},"90622-99-4"]
[{"$f":"Translator!B3501","v":"Fatty acids, C7-19, perfluoro"},"91032-01-8"]
[{"$f":"Translator!B3502","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl acrylate"},"91615-22-4"]
[{"$f":"Translator!B3503","v":"Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs., aluminum salts"},"93062-53-4"]
[{"$f":"Translator!B3504","v":"1,1'-[oxybis[(1-methylethylene)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol]"},"93776-00-2"]
[{"$f":"Translator!B3505","v":"(2-carboxylatoethyl)(dimethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl)amino]propyl]ammonium"},"93776-12-6"]
[{"$f":"Translator!B3506","v":"(2-carboxylatoethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl)amino]propyl]dimethylammonium"},"93776-13-7"]
[{"$f":"Translator!B3507","v":"(2-carboxylatoethyl)(dimethyl)[[[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl]amino]propyl]mmonium"},"93776-15-9"]
[{"$f":"Translator!B3508","v":"Diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl phosphate"},"93857-44-4"]
[{"$f":"Translator!B3509","v":"Perfluorooctylethyldimethylchlorosilane;Perfluorooctylethyldimethylchlorosilane"},"74612-30-9"]
[{"$f":"Translator!B3510","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl acrylate"},"94158-63-1"]
[{"$f":"Translator!B3511","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl methacrylate"},"94158-64-2"]
[{"$f":"Translator!B3512","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl methacrylate"},"94158-65-3"]
[{"$f":"Translator!B3513","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl dihydrogen phosphate"},"94158-70-0"]
[{"$f":"Translator!B3514","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol"},"94159-79-2"]
[{"$f":"Translator!B3515","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluorotridecan-2-ol"},"94159-80-5"]
[{"$f":"Translator!B3516","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)pentadecan-2-ol"},"94159-82-7"]
[{"$f":"Translator!B3517","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-12-(trifluoromethyl)tridecan-1-ol"},"94159-83-8"]
[{"$f":"Translator!B3518","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl phosphate"},"94200-45-0"]
[{"$f":"Translator!B3519","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl phosphate"},"94200-46-1"]
[{"$f":"Translator!B3520","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl phosphate"},"94200-47-2"]
[{"$f":"Translator!B3521","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonacosafluoro-2-hydroxyheptadecyl phosphate"},"94200-48-3"]
[{"$f":"Translator!B3522","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl phosphate"},"94200-50-7"]
[{"$f":"Translator!B3523","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl phosphate"},"94200-51-8"]
[{"$f":"Translator!B3524","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl phosphate"},"94200-52-9"]
[{"$f":"Translator!B3525","v":"Carbamic acid, [2-(sulfothio)ethyl]-, C-(γ-ω-perfluoro-C6-9-alkyl) esters, monosodium salts"},"95370-51-7"]
[{"$f":"Translator!B3526","v":"Triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)silane"},"101947-16-4"]
[{"$f":"Translator!B3527","v":"Perfluorooctylethyltrichlorosilane;Perfluorooctylethyltrichlorosilane"},"78560-44-8"]
[{"$f":"Translator!B3528","v":"Nonadecafluoro-9-iodononane"},"558-97-4"]
[{"$f":"Translator!B3529","v":"Icosafluoro-10-iodo-2-(trifluoromethyl)decane"},"677-93-0"]
[{"$f":"Translator!B3530","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecan-1-ol"},"678-39-7"]
[{"$f":"Translator!B3531","v":"Bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) hydrogen phosphate"},"678-41-1"]
[{"$f":"Translator!B3532","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecanol"},"865-86-1"]
[{"$f":"Translator!B3533","v":"Bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl] hydrogen phosphate"},"1895-26-7"]
[{"$f":"Translator!B3534","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl methacrylate"},"1996-88-9"]
[{"$f":"Translator!B3535","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iododecane"},"2043-53-0"]
[{"$f":"Translator!B3536","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-henicosafluoro-12-iodododecane"},"2043-54-1"]
[{"$f":"Translator!B3537","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl methacrylate"},"2144-54-9"]
[{"$f":"Translator!B3538","v":"Potassium perfluorooctanoate"},"2395-00-8"]
[{"$f":"Translator!B3539","v":"Ethyl perfluorooctanoate"},"3108-24-5"]
[{"$f":"Translator!B3540","v":"1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-tetracosafluoro-12-iodo-2-(trifluoromethyl)dodecane"},"3248-61-1"]
[{"$f":"Translator!B3541","v":"Octacosafluoro-14-iodo-2-(trifluoromethyl)tetradecane"},"3248-63-3"]
[{"$f":"Translator!B3542","v":"Ammonium pentadecafluorooctanoate"},"3825-26-1"]
[{"$f":"Translator!B3543","v":"N-ethylheptadecafluorooctanesulphonamide"},"4151-50-2"]
[{"$f":"Translator!B3544","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl methacrylate"},"4980-53-4"]
[{"$f":"Translator!B3545","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl methacrylate"},"6014-75-1"]
[{"$f":"Translator!B3546","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl acrylate"},"16083-78-6"]
[{"$f":"Translator!B3547","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl acrylate"},"16083-87-7"]
[{"$f":"Translator!B3548","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl acrylate"},"17741-60-5"]
[{"$f":"Translator!B3549","v":"3,4-bis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]benzenesulphonyl chloride"},"24216-05-5"]
[{"$f":"Translator!B3550","v":"1-bromohenicosafluorodecane"},"307-43-7"]
[{"$f":"Translator!B3551","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-12-iodododecane"},"307-60-8"]
[{"$f":"Translator!B3552","v":"Nonacosafluoro-1-iodotetradecane"},"307-63-1"]
[{"$f":"Translator!B3553","v":"Pentadecafluorooctyl fluoride"},"335-66-0"]
[{"$f":"Translator!B3554","v":"Pentadecafluorooctanoic acid"},"335-67-1"]
[{"$f":"Translator!B3555","v":"Silver(1+) perfluorooctanoate"},"335-93-3"]
[{"$f":"Translator!B3556","v":"Sodium pentadecafluorooctanoate"},"335-95-5"]
[{"$f":"Translator!B3557","v":"Methyl perfluorooctanoate"},"376-27-2"]
[{"$f":"Translator!B3558","v":"Henicosafluoro-10-iododecane"},"423-62-1"]
[{"$f":"Translator!B3559","v":"Heptadecafluoro-1-iodooctane"},"507-63-1"]
[{"$f":"Translator!B3560","v":"Perfluorooctylethyltrimethoxysilane;Perfluorooctylethyltrimethoxysilane"},"83048-65-1"]
[{"$f":"Translator!B3561","v":"Perfluorooctylethyldichloromethyl silane;Perfluorooctylethyldichloromethyl silane"},"3102-79-2"]
[{"$f":"Translator!B3562","v":"Thiols, C8-20, γ-ω-perfluoro, telomers with acrylamide"},"70969-47-0"]
[{"$f":"Translator!B3563","v":"Chromium(3+) perfluorooctanoate"},"68141-02-6"]
[{"$f":"Translator!B3564","v":"Propanamide, 3-[(γ-ω-perfluoro-C4-10-alkyl)thio] derivs."},"68187-42-8"]
[{"$f":"Translator!B3565","v":"Alkyl iodides, C4-20, γ-ω-perfluoro"},"68188-12-5"]
[{"$f":"Translator!B3566","v":"Fatty acids, C7-13, perfluoro"},"68333-92-6"]
[{"$f":"Translator!B3567","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl acrylate"},"27905-45-9"]
[{"$f":"Translator!B3568","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodotetradecane"},"30046-31-2"]
[{"$f":"Translator!B3569","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecene"},"30389-25-4"]
[{"$f":"Translator!B3570","v":"Perfluorooctanoic anhydride"},"33496-48-9"]
[{"$f":"Translator!B3571","v":"2-carboxyethylbis(2-hydroxyethyl)-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]propylammonium hydroxide"},"39186-68-0"]
[{"$f":"Translator!B3572","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecanol"},"39239-77-5"]
[{"$f":"Translator!B3573","v":"N-[3-[bis(2-hydroxyethyl)amino]propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide"},"41358-63-8"]
[{"$f":"Translator!B3574","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl acrylate"},"52956-82-8"]
[{"$f":"Translator!B3575","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl dihydrogen phosphate"},"57678-05-4"]
[{"$f":"Translator!B3576","v":"Butanoic acid, 3,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-2-(trifluoromethyl)-"},"1882109-59-2"]
[{"$f":"Translator!B3577","v":"Hexanoic acid, 2,2,4,4,5,5,6,6,6-nonafluoro-3,3-bis(trifluoromethyl)-"},"1812247-20-3"]
[{"$f":"Translator!B3578","v":"Hexanoic acid, 2,3,4,4,5,5,6,6,6-nonafluoro-2,3-bis(trifluoromethyl)-"},"1812247-18-9"]
[{"$f":"Translator!B3579","v":"Hexanoic acid, 2,2,3,3,4,5,6,6,6-nonafluoro-4,5-bis(trifluoromethyl)-"},"1144512-36-6"]
[{"$f":"Translator!B3580","v":"Hexanoic acid, 2,2,3,3,4,4,6,6,6-nonafluoro-5,5-bis(trifluoromethyl)-"},"1144512-34-4"]
[{"$f":"Translator!B3581","v":"Heptanoic acid, 2,2,3,3,4,4,5,6,6,7,7,7-dodecafluoro-5-(trifluoromethyl)-"},"909009-42-3"]
[{"$f":"Translator!B3582","v":"Heptanoic acid, 2,3,3,4,4,5,5,6,6,7,7,7-dodecafluoro-2-(trifluoromethyl)-"},"207678-51-1"]
[{"$f":"Translator!B3583","v":"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-"},"35605-76-6"]
[{"$f":"Translator!B3584","v":"Ethanaminium, N,N,N-triethyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)"},"98241-25-9"]
[{"$f":"Translator!B3585","v":"Decanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-"},"27854-31-5"]
[{"$f":"Translator!B3586","v":"2-Decenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluoro-"},"70887-84-2"]
[{"$f":"Translator!B3587","v":"1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphate)"},"57678-03-2"]
[{"$f":"Translator!B3588","v":"Hexanoic acid, 2,3,3,4,4,5,6,6,6-nonafluoro-2,5-bis(trifluoromethyl)-"},"1882109-80-9"]
[{"$f":"Translator!B3589","v":"1-Propanaminium,N,N,N-trimethyl-3- [(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl) amino]-, chloride (1:1)"},"53517-98-9"]
[{"$f":"Translator!B3590","v":"1-Propanesulfonic acid,3-[ethyl (2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-,sodium salt (1:1)"},"89685-61-0"]
[{"$f":"Translator!B3591","v":"Phosphine, tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]-"},"325459-92-5"]
[{"$f":"Translator!B3592","v":"Palladium, dichlorobis[tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phosphine-κP]-"},"326475-46-1"]
[{"$f":"Translator!B3593","v":"Butanoic acid, 3,3,4,4,4-pentafluoro-2,2-bis(1,1,2,2,2-pentafluoroethyl)-"},"1882109-58-1"]
[{"$f":"Translator!B3594","v":"Hexanoic acid, 2,3,3,4,5,5,6,6,6-nonafluoro-2,4-bis(trifluoromethyl)-"},"1812247-19-0"]
[{"$f":"Translator!B3595","v":"Hexanoic acid, 3,3,4,4,5,5,6,6,6-nonafluoro-2,2-bis(trifluoromethyl)-"},"1812247-17-8"]
[{"$f":"Translator!B3596","v":"Hexanoic acid, 2,2,3,3,5,5,6,6,6-nonafluoro-4,4-bis(trifluoromethyl)-"},"1192593-79-5"]
[{"$f":"Translator!B3597","v":"Hexanoic acid, 2,2,3,4,4,5,6,6,6-nonafluoro-3,5-bis(trifluoromethyl)-"},"1144512-35-5"]
[{"$f":"Translator!B3598","v":"Heptanoic acid, 2,2,3,3,4,5,5,6,6,7,7,7-dodecafluoro-4-(trifluoromethyl)-"},"1144512-18-4"]
[{"$f":"Translator!B3599","v":"Heptanoic acid, 2,2,3,4,4,5,5,6,6,7,7,7-dodecafluoro-3-(trifluoromethyl)-"},"705240-04-6"]
[{"$f":"Translator!B3600","v":"Isooctanoic acid, pentadecafluoro-"},"123116-17-6"]
[{"$f":"Translator!B3601","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-"},"15166-06-0"]
[{"$f":"Translator!B3602","v":"Octadecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester"},"99955-83-6"]
[{"$f":"Translator!B3603","v":"Pentanedioic acid, 3-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]-2-oxoethyl]-3-hydroxy-, 1,5-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester"},"302911-86-0"]
[{"$f":"Translator!B3604","v":"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C4–10-alkyl)thio]methyl] derivatives, phosphates, ammonium salts"},"148240-85-1"]
[{"$f":"Translator!B3605","v":"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C6–12-alkyl)thio]methyl] derivatives, phosphates, ammonium salts"},"148240-87-3"]
[{"$f":"Translator!B3606","v":"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C10-20-alkyl)thio]methyl] derivs., phosphates, ammonium salts"},"148240-89-5"]
[{"$f":"Translator!B3607","v":"Oxirane, methyl-, polymer with oxirane, mono[2-hydroxy-3-[( γ-ω-perfluoro-C8-20-alkyl)thio]propyl] ethers"},"183146-60-3"]
[{"$f":"Translator!B3608","v":"Pentanoic acid, 4,4-bis[(γ-ω-perfluoro-C8-20-alkyl)thio]derivs., compds. with diethanolamine"},"71608-61-2"]
[{"$f":"Translator!B3609","v":"2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethyl methacrylate, Me methacrylate and γ-ω-perfluoro-C8-14-alkyl acrylate"},"129783-45-5"]
[{"$f":"Translator!B3610","v":"2-Propenoic acid, dodecyl ester, polymers with Bu (1-oxo-2-propenyl)carbamate and γ-ω-perfluoro-C8-14-alkyl acrylate"},"144031-01-6"]
[{"$f":"Translator!B3611","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, homopolymer"},"74049-08-4"]
[{"$f":"Translator!B3612","v":"2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl 2-methyl-2-propenoate, methyl 2-methyl-2-propenoate,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-methyl-2-propenoate and 3,3,4,4,5,5,6,6, 7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate"},"65104-45-2"]
[{"$f":"Translator!B3613","v":"2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, polymer with 2-propenoic acid"},"53515-73-4"]
[{"$f":"Translator!B3614","v":"Hexanoic acid, 2,2,3,4,5,5,6,6,6-nonafluoro-3,4-bis(trifluoromethyl)-"},"1882109-81-0"]
[{"$f":"Translator!B3615","v":"Hexanoic acid, 2,2,3,3,4,5,5,6,6,6-decafluoro-4-(1,1,2,2,2-pentafluoroethyl)-"},"1882109-79-6"]
[{"$f":"Translator!B3616","v":"Hexanoic acid, 2,2,3,4,4,5,5,6,6,6-decafluoro-3-(1,1,2,2,2-pentafluoroethyl)-"},"1882109-78-5"]
[{"$f":"Translator!B3617","v":"Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-(1,1,2,2,3,3,3-heptafluoropropyl)-"},"1882109-77-4"]
[{"$f":"Translator!B3618","v":"Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-"},"1882109-76-3"]
[{"$f":"Translator!B3619","v":"Pentanoic acid, 2,2,3,5,5,5-hexafluoro-3,4,4-tris(trifluoromethyl)-"},"1882109-75-2"]
[{"$f":"Translator!B3620","v":"Pentanoic acid, 2,2,4,5,5,5-hexafluoro-3,3,4-tris(trifluoromethyl)-"},"1882109-74-1"]
[{"$f":"Translator!B3621","v":"Pentanoic acid, 2,3,3,5,5,5-hexafluoro-2,4,4-tris(trifluoromethyl)-"},"1882109-73-0"]
[{"$f":"Translator!B3622","v":"Pentanoic acid, 2,3,4,5,5,5-hexafluoro-2,3,4-tris(trifluoromethyl)-"},"1882109-72-9"]
[{"$f":"Translator!B3623","v":"Pentanoic acid, 2,4,4,5,5,5-hexafluoro-2,3,3-tris(trifluoromethyl)-"},"1882109-71-8"]
[{"$f":"Translator!B3624","v":"Pentanoic acid, 3,3,4,5,5,5-hexafluoro-2,2,4-tris(trifluoromethyl)-"},"1882109-70-7"]
[{"$f":"Translator!B3625","v":"Pentanoic acid, 2,2,3,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-"},"1882109-68-3"]
[{"$f":"Translator!B3626","v":"Pentanoic acid, 2,2,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-"},"1882109-67-2"]
[{"$f":"Translator!B3627","v":"Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-"},"1882109-66-1"]
[{"$f":"Translator!B3628","v":"Pentanoic acid, 2,3,3,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-"},"1882109-65-0"]
[{"$f":"Translator!B3629","v":"Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-"},"1882109-64-9"]
[{"$f":"Translator!B3630","v":"Pentanoic acid, 3,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-"},"1882109-63-8"]
[{"$f":"Translator!B3631","v":"Pentanoic acid, 3,4,4,5,5,5-hexafluoro-2,2,3-(trifluoromethyl)-"},"1882109-69-4"]
[{"$f":"Translator!B3632","v":"Butanoic acid, 4,4,4-trifluoro-2,2,3,3-tetrakis(trifluoromethyl)-"},"1882109-62-7"]
[{"$f":"Translator!B3633","v":"Butanoic acid, 2,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-3-(trifluoromethyl)-"},"1882109-61-6"]
[{"$f":"Translator!B3634","v":"Butanoic acid, 2,3,3,4,4,4-hexafluoro-2-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]-"},"1882109-60-5"]
[{"$f":"Translator!B3635","v":"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2- pentafluoroethyl)-, ammonium salt (1:1)"},"13058-06-5"]
[{"$f":"Translator!B3636","v":"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-, sodium salt (1:1)"},"1195164-59-0"]
[{"$f":"Translator!B3637","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, ammonium salt (1:1)"},"19742-57-5"]
[{"$f":"Translator!B3638","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, iron salt (1:x)"},"61436-04-2"]
[{"$f":"Translator!B3639","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, potassium salt (1:1)"},"29457-73-6"]
[{"$f":"Translator!B3640","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)- , sodium salt (1:1)"},"18017-22-6"]
[{"$f":"Translator!B3641","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, chromium salt (1:x)"},"15739-82-9"]
[{"$f":"Translator!B3642","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, aluminum salt (3:1)"},"15715-47-6"]
[{"$f":"Translator!B3643","v":"Bis(perfluorooctyl)phosphinic acid"},"40143-79-1"]
[{"$f":"Translator!B3644","v":"Perfluorohexylperfluorooctyl phosphinate"},"610800-34-5"]
[{"$f":"Translator!B3645","v":"Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-tricosafluoro-11-iodo-"},"307-50-6"]
[{"$f":"Translator!B3646","v":"Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15-hentriacontafluoro-15-iodo-"},"335-79-5"]
[{"$f":"Translator!B3647","v":"Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-heptacosafluoro-13-iodo-"},"376-04-5"]
[{"$f":"Translator!B3648","v":"Alkyl iodides, C10-12, γ-ω-perfluoro"},"68390-33-0"]
[{"$f":"Translator!B3649","v":"2-Dodecenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-"},"70887-94-4"]
[{"$f":"Translator!B3650","v":"Dodecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-"},"53826-13-4"]
[{"$f":"Translator!B3651","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, hexadecyl 2-propenoate, N-(hydroxymethyl)-2-propenamide, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate"},"115592-83-1"]
[{"$f":"Translator!B3652","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-[(2-methyl-1-oxo-2-propenyl)oxy]poly(oxy-1, 2-ethanediyl), 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl 2-propenoate, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-tritriacontafluorooctadecyl 2-propenoate"},"116984-14-6"]
[{"$f":"Translator!B3653","v":"2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethylmethacrylate, Me methacrylate and perfluoro-C8-14-alkyl acrylate"},"125328-29-2"]
[{"$f":"Translator!B3654","v":"Polychlorinated Biphenyls (PCB)"},"-"]
[{"$f":"Translator!B3655","v":"Chloro-1,1'-biphenyl"},"27323-18-8"]
[{"$f":"Translator!B3656","v":"Dichlorobiphenyl"},"25512-42-9"]
[{"$f":"Translator!B3657","v":"Tetrachloro(tetrachlorophenyl)benzene"},"31472-83-0"]
[{"$f":"Translator!B3658","v":"2,2',4,4',6,6'-hexachlorobiphenyl"},"33979-03-2"]
[{"$f":"Translator!B3659","v":"3,3'-dichlorobiphenyl"},"2050-67-1"]
[{"$f":"Translator!B3660","v":"2,4',5-trichlorobiphenyl"},"16606-02-3"]
[{"$f":"Translator!B3661","v":"2,3',4,4',5-pentachlorobiphenyl"},"31508-00-6"]
[{"$f":"Translator!B3662","v":"2,2',3,4,4',5'-hexachlorobiphenyl"},"35065-28-2"]
[{"$f":"Translator!B3663","v":"2,2',3,4,4',5,5'-heptachlorobiphenyl"},"35065-29-3"]
[{"$f":"Translator!B3664","v":"2,2',4,5,5'-pentachlorobiphenyl"},"37680-73-2"]
[{"$f":"Translator!B3665","v":"2,4,6-Trichlorobiphenyl"},"35693-92-6"]
[{"$f":"Translator!B3666","v":"2,2',5,5'-tetrachlorobiphenyl"},"35693-99-3"]
[{"$f":"Translator!B3667","v":"2,4,5-trichloro-1,1'-biphenyl"},"15862-07-4"]
[{"$f":"Translator!B3668","v":"3,3',4,4'-tetrachloro-1,1'-biphenyl"},"32598-13-3"]
[{"$f":"Translator!B3669","v":"2,2',3,3',4,4',5-heptachlorobiphenyl"},"35065-30-6"]
[{"$f":"Translator!B3670","v":"2,4-PCB"},"34883-43-7"]
[{"$f":"Translator!B3671","v":"Nonachloro-1,1'-biphenyl"},"53742-07-7"]
[{"$f":"Translator!B3672","v":"1,1'-Biphenyl, chloro derivs."},"1336-36-3"]
[{"$f":"Translator!B3673","v":"4,4'-dichlorobiphenyl"},"2050-68-2"]
[{"$f":"Translator!B3674","v":"Decachloro-1,1'-biphenyl"},"2051-24-3"]
[{"$f":"Translator!B3675","v":"2-chlorobiphenyl"},"2051-60-7"]
[{"$f":"Translator!B3676","v":"3-chlorobiphenyl"},"2051-61-8"]
[{"$f":"Translator!B3677","v":"4-chlorobiphenyl"},"2051-62-9"]
[{"$f":"Translator!B3678","v":"2,2',4,4'-tetrachlorobiphenyl"},"2437-79-8"]
[{"$f":"Translator!B3679","v":"2,4,4'-trichlorobiphenyl"},"7012-37-5"]
[{"$f":"Translator!B3680","v":"Pentachloro[1,1'-biphenyl]"},"25429-29-2"]
[{"$f":"Translator!B3681","v":"Heptachloro-1,1'-biphenyl"},"28655-71-2"]
[{"$f":"Translator!B3682","v":"Polychlorinated dibenzo-p-dioxins and dibenzofurans (PCDD/PCDF)"},"-"]
[{"$f":"Translator!B3683","v":"Polychlorinated naphthalenes"},"-"]
[{"$f":"Translator!B3684","v":"Naphthalene, chloro derivs."},"70776-03-3"]
[{"$f":"Translator!B3685","v":"Polycyclic aromatic hydrocarbons (PAHs)"},"-"]
[{"$f":"Translator!B3686","v":"Indeno[1,2,3-cd]pyrene"},"193-39-5"]
[{"$f":"Translator!B3687","v":"Benzo[def]chrysene"},"50-32-8"]
[{"$f":"Translator!B3688","v":"Benzo[k]fluoranthene"},"207-08-9"]
[{"$f":"Translator!B3689","v":"Benzo[e]acephenanthrylene"},"205-99-2"]
[{"$f":"Translator!B3690","v":"Tetrabromodiphenyl ether (group)"},"-"]
[{"$f":"Translator!B3691","v":"1,2-dibromo-4-(3,4-dibromophenoxy)benzene"},"93703-48-1"]
[{"$f":"Translator!B3692","v":"1,2-dibromo-4-(2,6-dibromophenoxy)benzene"},"189084-62-6"]
[{"$f":"Translator!B3693","v":"Diphenyl ether, tetrabromo derivative"},"40088-47-9"]
[{"$f":"Translator!B3694","v":"1,2-dibromo-4-(2,4-dibromophenoxy)benzene"},"189084-61-5"]
[{"$f":"Translator!B3695","v":"1,3,5-tribromo-2-(4-bromophenoxy)benzene"},"189084-63-7"]
[{"$f":"Translator!B3696","v":"Dicofol"},"115-32-2"]
[{"$f":"Translator!B3697","v":"Bis(pentabromophenyl) ether"},"1163-19-5"]
[{"$f":"Translator!B3698","v":"Hexachlorobenzene"},"118-74-1"]
[{"$f":"Translator!B3699","v":"Chlordecone"},"143-50-0"]
[{"$f":"Translator!B3700","v":"Dodecachloropentacyclo[5.2.1.02,6.03,9.05,8]decane"},"2385-85-5"]
[{"$f":"Translator!B3701","v":"Aldrin"},"309-00-2"]
[{"$f":"Translator!B3702","v":"Hexabromo-1,1'-biphenyl"},"36355-01-8"]
[{"$f":"Translator!B3703","v":"Clofenotane"},"50-29-3"]
[{"$f":"Translator!B3704","v":"Chlordane , pur"},"57-74-9"]
[{"$f":"Translator!B3705","v":"Dieldrin"},"60-57-1"]
[{"$f":"Translator!B3706","v":"Pentachlorobenzene"},"608-93-5"]
[{"$f":"Translator!B3707","v":"Endrin"},"72-20-8"]
[{"$f":"Translator!B3708","v":"Heptachlor"},"76-44-8"]
[{"$f":"Translator!B3709","v":"Toxaphene"},"8001-35-2"]
[{"$f":"Translator!B3710","v":"Alkanes, C10-13, chloro"},"85535-84-8, 68920-70-7, 71011-12-6, 85536-22-7, 85681-73-8, 108171-26-2"]
[{"$f":"Translator!B3711","v":"Hexachlorobuta-1,3-diene"},"87-68-3"]
[{"$f":"Translator!B3712","v":"Formaldehyde"},"50-00-0","P",{"$f":"Translator!B3713","v":"0.1 ml/cbm (ppm) in wood-based materials"},null,null,null,null,null,{"$f":"Translator!B3714","v":"ChemVerbotsVGermany\n*The equilibrium concentration of formaldehyde in the air of a test room must be below 0.1 ml/cbm (ppm) with caused by coated and uncoated wood-based materials (chipboard, blockboard, veneer panels and fibreboard). Furniture must comply with the same limit in full body test."},"E 2023"]
[{"$f":"Translator!B3715","v":"PFHxS, its salts and related substances"},{"$f":"Translator!$B$3719","v":"Group"},"P",{"$f":"Translator!B3720","v":"≤ 25 ppb PFHxS\n≤ 1000 ppb PFHxS-related substances (sum)"},null,null,null,null,null,{"$f":"Translator!B3722","v":"Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)"}]
[{"$f":"Translator!B3716","v":"C9-C14 PFCAs and their salts"},{"$f":"Translator!$B$3719","v":"Group"},"P",{"$f":"Translator!B3721","v":"≤ 25 ppb, ≤ 260 ppb (sum)"},null,null,null,null,null,{"$f":"Translator!B3723","v":"Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)"}]
[{"$f":"Translator!B3717","v":"Dechlorane plus (DP)“1,4:7,10-Dimethanodibenzo[a,e]cyclooctene, 1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-, which has the molecular formula C18H12Cl12”"},{"$f":"Translator!$B$3719","v":"Group"},"P",0,null,null,null,null,null,{"$f":"Translator!B3724","v":"Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n"}]
[{"$f":"Translator!B3718","v":"decabromodiphenyl ethane (DBDPE) “Benzene, 1,1′-(1,2-ethanediyl)bis [2,3,4,5,6- pentabromo-, which has the molecular formula C14H4Br10)”"},{"$f":"Translator!$B$3719","v":"Group"},"P",0,null,null,null,null,null,{"$f":"Translator!B3725","v":"Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n"}]

{"sheet":"15_ED","index":5,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":true,"merged":[[0,0,0,6],[2,0,2,6],[12,0,12,6]]}
[{"$f":"Translator!B1488","v":"ED (Register 15)"}]
[{"$f":"Translator!B1489","v":"Regulated substances"},{"$f":"Translator!B1490","v":"CAS number"},null,{"$f":"Translator!B1491","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B1492","v":"Examples occurrence"},{"$f":"Translator!B1493","v":"Comments"},{"$f":"Translator!B1494","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B1519","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B1507","v":"1-Methyl-4-tert-butylbenzene (TBT)"},"98-51-1","P",null,null,null,"E 2015"]
[{"$f":"Translator!B1508","v":"3-(2-Butoxyethoxy)ethanol"},"112-34-5","P",null,null,null,"E 2015"]
[{"$f":"Translator!B1509","v":"1,1 Dichloroethylene"},"75-35-4","P",null,null,null,"E 2015"]
[{"$f":"Translator!B1510","v":"tri-organostannic compounds"},null,"P",null,{"$f":"Translator!B1524","v":"Wood protection agents, polymer\nadditives, catalysts\n"},null,"E 2015"]
[{"$f":"Translator!B1514","v":"Ethenylbenzene (styrol)"},"100-42-5","P",null,{"$f":"Translator!B1528","v":"Plastic parts, seals"},null,"E 2015"]
[{"$f":"Translator!B1501","v":"1,1,2,2-Tetrachloroethane"},"79-34-5","P",null,null,null,"E 2015"]
[{"$f":"Translator!B1502","v":"Pentachloroethane"},"76-01-7","P",null,null,null,"E 2015"]
[{"$f":"Translator!B1503","v":"Trichloromethane (Chloroform) "},"67-66-3 ","P",null,null,null,"E 2015"]
[{"$f":"Translator!B1564","v":"Benzenamine, N-phenyl-,Reaction Products with Styrene and 2,4,4- Trimethylpenten (BNST)"},"68921-45-9","P",null,{"$f":"Translator!B1565","v":"Additive for elastomer compounds and lubricants"},null,"E 2015"]
[{"$f":"Translator!B1495","v":"Substance rated declarable (D)"}]
[{"$f":"Translator!B1496","v":"Bitumen"},"8052-42-4","D",null,{"$f":"Translator!B1520","v":"Anti-drumming materials"},null,"E 2015"]
[{"$f":"Translator!B1497","v":"2-butanone oxime"},"96-29-7","D",null,{"$f":"Translator!B1521","v":"PUR formulations"},null,"E 2015"]
[{"$f":"Translator!B1498","v":"Polyfumaric acid dibutyl ether"},"105-75-9","D",null,{"$f":"Translator!B1522","v":"Drawing oils for aluminum,\nvarnishes, coating defects\n"},null,"E 2015"]
[{"$f":"Translator!B1499","v":"Vinyl acetate"},"108-05-4","D",null,{"$f":"Translator!B1523","v":"PVAC, SMC, soft films, adhesives"},null,"E 2015"]
[{"$f":"Translator!B1500","v":"Carbon disulfide"},"75-15-0","D",null,null,null,"E 2015"]
[{"$f":"Translator!B1504","v":"Long-chained chlorinated \nparaffins (C18 to C28) \n"},null,"D",null,null,null,"E 2015"]
[{"$f":"Translator!B1505","v":"n-hexane"},"110-54-3","D",null,null,null,"E 2015"]
[{"$f":"Translator!B1506","v":"Hydrogen sulfide"},"7783-06-4","D",null,null,null,"E 2015"]
[{"$f":"Translator!B1511","v":"Ethylbenzene"},"100-41-4","D",null,{"$f":"Translator!B1525","v":"Glues, paints, manufacture of\nstyrol\n"},null,"E 2015"]
[{"$f":"Translator!B1512","v":"Xylene"},null,"D",null,{"$f":"Translator!B1526","v":"Solvents, glues, paints"},null,"E 2015"]
[{"$f":"Translator!B1513","v":"Phthalates with a chain length\nof C11, with branches and linear\n"},null,"D",null,{"$f":"Translator!B1527","v":"Plasticizer"},null,"E 2015"]

{"sheet":"2_REACH","index":6,"n_rows":566,"n_cols":19,"rows_kept":566,"cut":false,"hidden":true,"merged":[[560,6,560,8],[565,6,565,8],[556,6,556,8],[557,6,557,8],[558,6,558,8],[559,6,559,8],[504,6,504,8],[505,6,505,8],[506,6,506,8],[507,6,507,8],[508,6,508,8],[509,6,509,8],[510,6,510,8],[511,6,511,8],[512,6,512,8],[518,6,518,8],[519,6,519,8],[520,6,520,8],[521,6,521,8],[522,6,522,8],[523,6,523,8],[524,6,524,8],[529,6,529,8],[530,6,530,8],[531,6,531,8],[532,6,532,8],[554,6,554,8],[555,6,555,8],[482,6,482,8],[483,6,483,8],[484,6,484,8],[485,6,485,8],[486,6,486,8],[487,6,487,8],[488,6,488,8],[489,6,489,8],[490,6,490,8],[496,6,496,8],[497,6,497,8],[498,6,498,8],[499,6,499,8],[500,6,500,8],[501,6,501,8],[513,6,513,8],[514,6,514,8],[515,6,515,8],[516,6,516,8],[517,6,517,8],[527,6,527,8],[528,6,528,8],[469,6,469,8],[470,6,470,8],[471,6,471,8],[472,6,472,8],[473,6,473,8],[474,6,474,8],[475,6,475,8],[476,6,476,8],[491,6,491,8],[477,6,477,8],[525,6,525,8],[480,6,480,8],[481,6,481,8],[492,6,492,8],[493,6,493,8],[494,6,494,8],[495,6,495,8],[526,6,526,8],[478,6,478,8],[479,6,479,8],[465,6,465,8],[466,6,466,8],[467,6,467,8],[459,6,459,8],[455,6,455,8],[456,6,456,8],[457,6,457,8],[458,6,458,8],[468,6,468,8],[454,6,454,8],[460,6,460,8],[461,6,461,8],[462,6,462,8],[463,6,463,8],[464,6,464,8],[452,6,452,8],[453,6,453,8],[417,6,417,8],[418,6,418,8],[419,6,419,8],[420,6,420,8],[421,6,421,8],[422,6,422,8],[423,6,423,8],[424,6,424,8],[425,6,425,8],[439,6,439,8],[440,6,440,8],[441,6,441,8],[442,6,442,8],[433,6,433,8],[434,6,434,8],[435,6,435,8],[428,6,428,8],[429,6,429,8],[430,6,430,8],[405,6,405,8],[406,6,406,8],[407,6,407,8],[144,6,144,8],[145,6,145,8],[146,6,146,8],[147,6,147,8],[148,6,148,8],[149,6,149,8],[274,6,274,8],[275,6,275,8],[276,6,276,8],[160,6,160,8],[161,6,161,8],[162,6,162,8],[163,6,163,8],[164,6,164,8],[165,6,165,8],[166,6,166,8],[167,6,167,8],[168,6,168,8],[169,6,169,8],[170,6,170,8],[171,6,171,8],[172,6,172,8],[173,6,173,8],[174,6,174,8],[135,6,135,8],[136,6,136,8],[137,6,137,8],[138,6,138,8],[139,6,139,8],[140,6,140,8],[141,6,141,8],[142,6,142,8],[143,6,143,8],[0,0,0,13],[3,0,3,13],[2,0,2,13],[5,4,5,13],[13,12,16,12],[34,12,40,12],[69,9,69,10],[70,9,70,10],[71,9,71,10],[60,9,60,10],[61,9,61,10],[62,9,62,10],[63,9,63,10],[64,9,64,10],[65,9,65,10],[66,9,66,10],[67,9,67,10],[68,9,68,10],[51,9,51,10],[52,9,52,10],[53,9,53,10],[54,9,54,10],[55,9,55,10],[56,9,56,10],[72,9,72,10],[73,9,73,10],[74,9,74,10],[79,0,79,14],[72,4,72,5],[73,4,73,5],[74,4,74,5],[75,4,75,5],[75,9,75,10],[78,6,78,8],[76,9,76,10],[77,9,77,10],[76,4,76,5],[77,4,77,5],[41,9,41,10],[57,9,57,10],[58,9,58,10],[59,9,59,10],[42,9,42,10],[43,9,43,10],[44,9,44,10],[45,9,45,10],[46,9,46,10],[47,9,47,10],[48,9,48,10],[49,9,49,10],[50,9,50,10],[17,9,17,10],[18,9,18,10],[19,9,19,10],[20,9,20,10],[21,9,21,10],[22,9,22,10],[23,9,23,10],[24,9,24,10],[25,9,25,10],[1,9,1,10],[4,9,4,10],[6,9,6,10],[7,9,7,10],[8,9,8,10],[9,9,9,10],[10,9,10,10],[11,9,11,10],[12,9,12,10],[67,4,67,5],[68,4,68,5],[284,6,284,8],[285,6,285,8],[286,6,286,8],[85,6,85,8],[86,6,86,8],[87,6,87,8],[88,6,88,8],[89,6,89,8],[90,6,90,8],[91,6,91,8],[92,6,92,8],[93,6,93,8],[113,6,113,8],[114,6,114,8],[115,6,115,8],[116,6,116,8],[117,6,117,8],[118,6,118,8],[119,6,119,8],[120,6,120,8],[98,6,98,8],[99,6,99,8],[11,4,11,5],[12,4,12,5],[13,4,16,5],[17,4,17,5],[46,4,46,5],[47,4,47,5],[48,4,48,5],[49,4,49,5],[50,4,50,5],[41,4,41,5],[42,4,42,5],[43,4,43,5],[44,4,44,5],[45,4,45,5],[94,6,94,8],[95,6,95,8],[96,6,96,8],[97,6,97,8],[100,6,100,8],[101,6,101,8],[102,6,102,8],[268,6,268,8],[269,6,269,8],[108,6,108,8],[109,6,109,8],[110,6,110,8],[111,6,111,8],[112,6,112,8],[103,6,103,8],[104,6,104,8],[105,6,105,8],[106,6,106,8],[107,6,107,8],[130,6,130,8],[131,6,131,8],[132,6,132,8],[133,6,133,8],[134,6,134,8],[438,6,438,8],[431,6,431,8],[432,6,432,8],[385,6,385,8],[386,6,386,8],[387,6,387,8],[388,6,388,8],[389,6,389,8],[401,6,401,8],[402,6,402,8],[403,6,403,8],[404,6,404,8],[397,6,397,8],[398,6,398,8],[390,6,390,8],[391,6,391,8],[392,6,392,8],[393,6,393,8],[394,6,394,8],[395,6,395,8],[396,6,396,8],[399,6,399,8],[400,6,400,8],[436,6,436,8],[382,6,382,8],[383,6,383,8],[384,6,384,8],[448,6,448,8],[449,6,449,8],[450,6,450,8],[451,6,451,8],[408,6,408,8],[409,6,409,8],[410,6,410,8],[411,6,411,8],[412,6,412,8],[413,6,413,8],[414,6,414,8],[415,6,415,8],[416,6,416,8],[443,6,443,8],[444,6,444,8],[445,6,445,8],[446,6,446,8],[447,6,447,8],[426,6,426,8],[427,6,427,8],[437,6,437,8],[373,6,373,8],[374,6,374,8],[375,6,375,8],[376,6,376,8],[377,6,377,8],[378,6,378,8],[379,6,379,8],[380,6,380,8],[381,6,381,8],[364,6,364,8],[365,6,365,8],[366,6,366,8],[367,6,367,8],[368,6,368,8],[369,6,369,8],[370,6,370,8],[371,6,371,8],[372,6,372,8],[355,6,355,8],[356,6,356,8],[357,6,357,8],[358,6,358,8],[359,6,359,8],[360,6,360,8],[361,6,361,8],[362,6,362,8],[363,6,363,8],[121,6,121,8],[122,6,122,8],[123,6,123,8],[124,6,124,8],[185,6,185,8],[186,6,186,8],[187,6,187,8],[188,6,188,8],[189,6,189,8],[125,6,125,8],[126,6,126,8],[127,6,127,8],[128,6,128,8],[129,6,129,8],[150,6,150,8],[151,6,151,8],[152,6,152,8],[153,6,153,8],[154,6,154,8],[155,6,155,8],[156,6,156,8],[157,6,157,8],[158,6,158,8],[159,6,159,8],[84,6,84,8],[51,4,51,5],[52,4,52,5],[53,4,53,5],[54,4,54,5],[55,4,55,5],[56,4,56,5],[57,4,57,5],[58,4,58,5],[59,4,59,5],[60,4,60,5],[61,4,61,5],[62,4,62,5],[63,4,63,5],[64,4,64,5],[69,4,69,5],[70,4,70,5],[71,4,71,5],[80,6,80,8],[81,6,81,8],[82,6,82,8],[83,6,83,8],[65,4,65,5],[66,4,66,5],[30,13,32,13],[36,13,40,13],[25,4,25,5],[26,4,26,5],[27,4,27,5],[28,4,28,5],[29,4,29,5],[30,4,32,5],[33,4,33,5],[34,4,40,5],[34,6,40,6],[30,6,32,6],[26,9,26,10],[27,9,27,10],[28,9,28,10],[29,9,29,10],[30,9,30,10],[31,9,31,10],[32,9,32,10],[33,9,33,10],[5,0,5,2],[1,0,1,7],[1,11,1,12],[4,4,4,5],[13,7,16,7],[13,9,16,10],[13,11,16,11],[34,7,40,7],[34,9,40,10],[34,11,40,11],[18,4,18,5],[19,4,19,5],[20,4,20,5],[21,4,21,5],[22,4,22,5],[23,4,23,5],[24,4,24,5],[6,4,6,5],[7,4,7,5],[8,4,8,5],[9,4,9,5],[10,4,10,5],[30,1,32,1],[13,6,16,6],[175,6,175,8],[176,6,176,8],[177,6,177,8],[178,6,178,8],[179,6,179,8],[180,6,180,8],[181,6,181,8],[182,6,182,8],[183,6,183,8],[184,6,184,8],[194,6,194,8],[190,6,190,8],[191,6,191,8],[192,6,192,8],[193,6,193,8],[195,6,195,8],[196,6,196,8],[197,6,197,8],[198,6,198,8],[199,6,199,8],[200,6,200,8],[201,6,201,8],[202,6,202,8],[203,6,203,8],[204,6,204,8],[205,6,205,8],[206,6,206,8],[207,6,207,8],[208,6,208,8],[209,6,209,8],[210,6,210,8],[211,6,211,8],[212,6,212,8],[213,6,213,8],[214,6,214,8],[215,6,215,8],[216,6,216,8],[217,6,217,8],[218,6,218,8],[219,6,219,8],[220,6,220,8],[221,6,221,8],[222,6,222,8],[223,6,223,8],[224,6,224,8],[225,6,225,8],[226,6,226,8],[227,6,227,8],[228,6,228,8],[229,6,229,8],[230,6,230,8],[231,6,231,8],[232,6,232,8],[233,6,233,8],[234,6,234,8],[235,6,235,8],[236,6,236,8],[237,6,237,8],[238,6,238,8],[239,6,239,8],[240,6,240,8],[241,6,241,8],[242,6,242,8],[243,6,243,8],[244,6,244,8],[245,6,245,8],[246,6,246,8],[247,6,247,8],[248,6,248,8],[249,6,249,8],[250,6,250,8],[251,6,251,8],[309,6,309,8],[310,6,310,8],[311,6,311,8],[266,6,266,8],[267,6,267,8],[273,6,273,8],[325,6,325,8],[328,6,328,8],[329,6,329,8],[330,6,330,8],[331,6,331,8],[332,6,332,8],[333,6,333,8],[334,6,334,8],[335,6,335,8],[342,6,342,8],[349,6,349,8],[350,6,350,8],[345,6,345,8],[346,6,346,8],[347,6,347,8],[348,6,348,8],[351,6,351,8],[352,6,352,8],[353,6,353,8],[354,6,354,8],[294,6,294,8],[295,6,295,8],[296,6,296,8],[252,6,252,8],[253,6,253,8],[254,6,254,8],[255,6,255,8],[256,6,256,8],[257,6,257,8],[272,6,272,8],[277,6,277,8],[278,6,278,8],[279,6,279,8],[280,6,280,8],[281,6,281,8],[282,6,282,8],[292,6,292,8],[293,6,293,8],[258,6,258,8],[260,6,260,8],[261,6,261,8],[262,6,262,8],[263,6,263,8],[264,6,264,8],[265,6,265,8],[270,6,270,8],[271,6,271,8],[343,6,343,8],[344,6,344,8],[316,6,316,8],[340,6,340,8],[341,6,341,8],[297,6,297,8],[298,6,298,8],[299,6,299,8],[300,6,300,8],[301,6,301,8],[302,6,302,8],[303,6,303,8],[304,6,304,8],[323,6,323,8],[305,6,305,8],[306,6,306,8],[307,6,307,8],[79,15,79,18],[502,6,502,8],[503,6,503,8],[324,6,324,8],[308,6,308,8],[336,6,336,8],[337,6,337,8],[338,6,338,8],[339,6,339,8],[317,6,317,8],[318,6,318,8],[319,6,319,8],[312,6,312,8],[313,6,313,8],[314,6,314,8],[315,6,315,8],[283,6,283,8],[287,6,287,8],[288,6,288,8],[289,6,289,8],[290,6,290,8],[291,6,291,8],[320,6,320,8],[322,6,322,8],[551,6,551,8],[552,6,552,8],[553,6,553,8],[541,6,541,8],[542,6,542,8],[543,6,543,8],[544,6,544,8],[545,6,545,8],[546,6,546,8],[547,6,547,8],[548,6,548,8],[549,6,549,8],[533,6,533,8],[534,6,534,8],[535,6,535,8],[536,6,536,8],[537,6,537,8],[538,6,538,8],[539,6,539,8],[540,6,540,8],[550,6,550,8]]}
[{"$f":"Translator!B151","v":"EC-REACH (tab 2)                                                                                                                                                                                                                   "}]
[{"$f":"Translator!B1604","v":"Changes Annex XVII up to 12.12.2023 and candidate list up to 23.01.2024."},null,null,null,null,null,null,null,null,{"$f":"Translator!B658","v":"Show extract"},null,{"$f":"Translator!B659","v":"Reduce extract"}]
[{"$f":"Translator!B876","v":"Annex XVII restrictions: https://echa.europa.eu/substances-restricted-under-reach"}]
[{"$f":"Translator!B875","v":"Candidate List of SVHC for authorisation"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},{"$f":"Translator!B98","v":"Cont.nr. in REACH"},null,{"$f":"Translator!B99","v":"Restriction conditions"},null,{"$f":"Translator!B100","v":"Limits"},{"$f":"Translator!B3789","v":"By Substance groups: Name of the contained substances"},{"$f":"Translator!B3790","v":"By Substance groups: CAS of the contained substances"},{"$f":"Translator!B152","v":"Concentration"},null,{"$f":"Translator!B153","v":"Part name of the specific part (in case of complex parts), regulated substance is contained."},{"$f":"Translator!B154","v":"Comments"},{"$f":"Translator!B1432","v":"Entry\n- included (E)\n- changed (C) \n"}]
[{"$f":"Translator!B155","v":"Prohibited substances (P)\nEU-REACH Annex 17"},null,null,null,{"$f":"Translator!B669","v":"Extract from Regulation (EC) No 1907/2006, Annex 17 (source text see www.eur-lex.europa.eu)"}]
[{"$f":"Translator!B1611","v":"Polychlorinated terphenyls (PCTs)"},"-",1,"P",{"$f":"Translator!B1681","v":"Shall not beplaced on the market, or used:\n-as substances,\n-in mixtures, including waste oils, or in equipment, in concentrations greater than 50 mg/kg (0,005 % by weight)."},null,{"$f":"Translator!$B$1740","v":"0,005 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1612","v":"Chloroethene (vinyl chloride)"},"75-01-4",2,"P",{"$f":"Translator!B1682","v":"Shall not be used aspropellant in aerosols for any use.\nAerosols dispensers containing the substance as propellant shall not be placed on the market"},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1613","v":"Tris (2,3dibromopropyl) phosphate"},"126-72-7",4,"P",{"$f":"Translator!B1683","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin\n\n2. Articles not complying with paragraph 1 shall not be placed on the market."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1614","v":"Benzene"},"71-43-2",5,"P",{"$f":"Translator!B1684","v":" 1. Shall not be used in toys or parts of toys where the concentration of benzene in the free state is greater than 5 mg/kg (0,0005 %) of the weight of the toy or part of toy. \n2. Toys and parts of toys not complying with paragraph 1 shall not be placed on the market. \n3. Shall not be placed on the market, or used, \n- as a substance, \n- as a constituent of other substances, or in mixtures, in concentrations equal to, or greater than 0,1 % by weight. \n\n4. However, paragraph 3 shall not apply to: \n(a) motor fuels which are covered by Directive 98/70/EC; \n(b) substances and mixtures for use in industrial processes not allowing for the emission of benzene in quantities in excess of those laid down in existing legislation. \n(c) natural gas placed on the market for use by consumers, provided that the concentration of benzene remains below 0,1 % volume/volume’.\n"},null,{"$f":"Translator!$B$1738","v":"0,0005 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1615","v":"Asbestos fibres:\n(a) Crocidolite\n\n(b) Amosite\n\n(c) Anthophyllite\n\n(d) Actinolite\n\n(e) Tremolite\n\n(f) Chrysotile"},"a)  12001-28-4\n\nb)  12172-73-5\n\nc)  77536-67-5\n\nd)  77536-66-4\n\ne)  77536-68-6\n\nf)  12001-29-5\n132207-32-0",6,"P",{"$f":"Translator!B1685","v":"1. The manufacture, placing on the market and use of these fibres and of articles and mixtures containing these fibres added intentionally is prohibited.\nHowever, if the use of diaphragms containing chrysotile for electrolysis installations in use on 13 July 2016 had been exempted by a Member State in accordance with the version of this paragraph in force until that date, the first subparagraph shall not apply until 1 July 2025 to the use in those installations of such diaphragms or of chrysotile used exclusively in the maintenance of such diaphragms, provided that such use is carried out in compliance with the conditions of a permit set in accordance with Directive 2010/75/EU of the European Parliament and of the Council (*).\nAny downstream user benefiting from such an exemption shall send, by 31 January of each calendar year to the Member State in which the relevant electrolysis installation is located, a report indicating the amount of chrysotile used in diaphragms pursuant to the exemption. The Member State shall transmit a copy to the European Commission.\nWhere, in order to protect the health and safety of workers, a Member State requires monitoring of chrysotile in air by downstream users, the results shall be included in that report.\n(*) Directive 2010/75/EU of the European Parliament and of the Council of 24 November 2010 on industrial emissions (integrated pollution prevention and control) (OJ L 334, 17.12.2010, p. 17).\n2. The use of articles containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005 shall continue to be permitted until they are disposed of or reach the end of their service life.\nHowever, Member States may, for reasons of protection of human health, restrict, prohibit or make subject to specific conditions, the use of such articles before they are disposed of or reach the end of their service life. Member States may allow placing on the market of articles in their entirety containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005, under specific conditions ensuring a high level of protection of human health. Member States shall communicate these national measures to the Commission by 1 June 2011. The Commission shall make this information publicly available.\n3. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, the placing on the market and use of articles containing these fibres, as permitted according to the preceding derogations, shall be permitted only if suppliers ensure before the placing on the market that articles bear a label in accordance with Appendix 7 to this Annex.\n"},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2013"]
[{"$f":"Translator!B1616","v":"Tris(aziridinyl)phosphinoxide"},"545-55-1",7,"P",{"$f":"Translator!B1686","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.\n"},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1617","v":"Polybromobiphenyls, Polybrominatedbiphenyls (PBB)"},"59536-65-1",8,"P",{"$f":"Translator!B1687","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1618","v":"2-naphthylamine and its salts"},"91-59-8",12,"P",{"$f":"Translator!B1688","v":"The following shall apply to entries 12 to 15: \nShall not be placed on the market, or used, as substances or in mixtures in concentrations greater than 0,1 % by weight."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1619","v":"Benzidine and its salts"},"92-87-5",13,"P",null,null,null,null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1620","v":"4-Nitrobiphenyl"},"92-93-3",14,"P",null,null,null,null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1621","v":"4-Aminobiphenyl xenylamine and its salts"},"92-67-1",15,"P",null,null,null,null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1622","v":"Lead carbonates:\na) Neutral anhydrous carbonate (PbCO3)\n\nb) Trilead-bis(carbonate)-dihydroxide 2PbCO3-Pb(OH)2 "},"a) 598-63-0\n\nb) 1319-46-6",16,"P",{"$f":"Translator!B1689","v":"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint.However, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof"},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2013"]
[{"$f":"Translator!B1623","v":"Lead sulphates:\na) Lead sulphate PbSO4\n\nb) Sulphuric acid, lead salt Pbx SO4"},"a) 7446-14-2\n\nb) 15739-80-7",17,"P",{"$f":"Translator!B1690","v":"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint.However, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2013"]
[{"$f":"Translator!B1624","v":"Mercury compounds"},"-",18,"P",{"$f":"Translator!B1691","v":"Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use: \n(a) to prevent the fouling by micro-organisms, plants or animals of: \n—    the hulls of boats, \n—    cages, floats, nets and any other appliances or equipment used for fish or shellfish farming, \n—    any totally or partly submerged appliances or equipment; \n(b) in the preservation of wood; \n(c) in the impregnation of heavy-duty industrial textiles and yarn intended for their manufacture; \n(d) in the treatment of industrial waters, irrespective of their use."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2011 / C2012"]
[{"$f":"Translator!B1625","v":"Mercury"},"7439-97-6","18a","P",{"$f":"Translator!B1692","v":"1. Shall not be placed on the market:\n(a) in fever thermometers;\n(b) in other measuring devices intended for sale to the general public (such as manometers, barometers, sphygmomanometers, thermometers other than fever thermometers). \n2. The restriction in paragraph 1 shall not apply to measuring devices that were in use in the Community before 3 April 2009. However Member States may restrict or prohibit the placing on the market of such measuring devices. \n3. The restriction in paragraph 1(b) shall not apply to:\n (a) measuring devices more than 50 years old on 3 October 2007; \n(b) barometers (except barometers within point (a)) until 3 October 2009.\n(4.    Regulation (EU) No 847/2012: paragraph 4 is  deleted). \n5. The following mercury-containing measuring devices intended for industrial and professional uses shall not be placed on the market after 10 April 2014: \n(a) barometers;\n(b) hygrometers;\n(c) manometers;\n(d) sphygmomanometers; \n(e) strain gauges to be used with plethysmographs;\n(f) tensiometers;\n(g) thermometers and other non-electrical thermometric applications.\nThe restriction shall also apply to measuring devices under points (a) to (g) which are placed on the market empty if intended to be filled with mercury. \n6. The restriction in paragraph 5 shall not apply to: \n(a) sphygmomanometers to be used: \n(i) in epidemiological studies which are ongoing on 10 October 2012;\n(ii) as reference standards in clinical validation studies of mercury-free sphygmomanometers; \n(b) thermometers exclusively intended to perform tests according to standards that require the use of mercury thermometers until 10 October 2017; \n(c) mercury triple point cells which are used for the calibration of platinum resistance thermometers.\n7. The following mercury-using measuring devices intended for professional and industrial uses shall not be placed on the market after 10 April 2014:\n(a) mercury pycnometers; \n(b) mercury metering devices for determination of the softening point. \n8. The restrictions in paragraphs 5 and 7 shall not apply to: \n(a) measuring devices more than 50 years old on 3 October 2007; \n(b) measuring devices which are to be displayed in public exhibitions for cultural and historical purposes.\n"},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2011 / C2012"]
[{"$f":"Translator!B1626","v":"Arsenic compounds"},"-",19,"P",{"$f":"Translator!B1693","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use to prevent the fouling by micro-organisms, plants or animals of: \n— the hulls of boats, \n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming, \n— any totally or partly submerged appliances or equipment. \n\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters, irrespective of their use. \n\n3. Shall not be used in the preservation of wood. Furthermore, wood so treated shall not be placed on the market. \n\n4. By way of derogation from paragraph 3: \n(a) Relating to the substances and mixtures for the preservation of wood: these may only be used in industrial installations using vacuum or pressure to impregnate wood if they are solutions of inorganic compounds of the copper, chromium, arsenic (CCA) type C and if they are authorised in accordance with Article 5(1) of Directive 98/8/EC. Wood so treated shall not be placed on the market before fixation of the preservative is completed. \n(b) Wood treated with CCA solution in accordance with point (a) may be placed on the market for professional and industrial use provided that the structural integrity of the wood is required for human or livestock safety and skin contact by the general public during its service life is unlikely: \n— as structural timber in public and agricultural buildings, office buildings, and industrial premises, \n— in bridges and bridgework, \n— as constructional timber in freshwater areas and brackish waters, for example jetties and bridges, \n— as noise barriers, — in avalanche control, — in highway safety fencing and barriers, \n— as debarked round conifer livestock fence posts, \n— in earth retaining structures, — as electric power transmission and telecommunications poles, \n— as underground railway sleepers. \n(c) Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that all treated wood placed on the market is individually labelled ‘For professional and industrial installation and use only, contains arsenic’. In addition, all wood placed on the market in packs shall also bear a label stating ‘Wear gloves when handling this wood. Wear a dust mask and eye protection when cutting or otherwise crafting this wood. Waste from this wood shall be treated as hazardous by an authorised undertaking’. \n(d) Treated wood referred to under point (a) shall not be used: — in residential or domestic constructions, whatever the purpose, — in any application where there is a risk of repeated skin contact, — in marine waters, — for agricultural purposes other than for livestock fence posts and structural uses in accordance with point (b), — in any application where the treated wood may come into contact with intermediate or finished products intended for human and/or animal consumption. \n\n5. Wood treated with arsenic compounds that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4 may remain in place and continue to be used until it reaches the end of its service life. \n\n6. Wood treated with CCA type C that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4: \n— may be used or reused subject to the conditions pertaining to its use listed under points 4(b), (c) and (d), \n— may be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).\n\n7. Member States may allow wood treated with other types of CCA solutions that was in use in the Community before 30 September 2007: \n— to be used or reused subject to the conditions pertaining to its use listed under points 4 (b), (c) and (d), \n— to be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d)."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1627","v":"Organostannic compounds"},"-",20,"P",{"$f":"Translator!B1694","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is acting as biocide in free association paint. \n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture acts as biocide to prevent the fouling by micro-organisms, plants or animals of: \n(a) all craft irrespective of their length intended for use in marine, coastal, estuarine and inland waterways and lakes; (b) cages, floats, nets and any other appliances or equipment used for fish or shellfish farming; (c) any totally or partly submerged appliance or equipment. \n3. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters. \n4. Tri-substituted organostannic compounds: \n(a) Tri-substituted organostannic compounds such as tributyltin (TBT) compounds and triphenyltin (TPT) compounds shall not be used after 1 July 2010 in articles where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin. (b) Articles not complying with point (a) shall not be placed on the market after 1 July 2010, except for articles that were already in use in the Community before that date. \n5. Dibutyltin (DBT) compounds: \n(a) Dibutyltin (DBT) compounds shall not be used after 1 January 2012 in mixtures and articles for supply to the general public where the concentration in the mixture or the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin. (b) Articles and mixtures not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date. (c) By way of derogation, points (a) and (b) shall not apply until 1 January 2015 to the following articles and mixtures for supply to the general public: \n— one-component and two-component room temperature vulcanisation sealants (RTV-1 and RTV-2 sealants) and adhesives, \n— paints and coatings containing DBT compounds as catalysts when applied on articles, \n— soft polyvinyl chloride (PVC) profiles whether by themselves or coextruded with hard PVC, \n— fabrics coated with PVC containing DBT compounds as stabilisers when intended for outdoor applications, \n— outdoor rainwater pipes, gutters and fittings, as well as covering material for roofing and façades, \n(d) By way of derogation, points (a) and (b) shall not apply to materials and articles regulated under Regulation (EC) No 1935/2004. \n6. Dioctyltin (DOT) compounds: \n(a) Dioctyltin (DOT) compounds shall not be used after 1 January 2012 in the following articles for supply to, or use by, the general public, where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin: \n— textile articles intended to come into contact with the skin, \n— gloves, \n— footwear or part of footwear intended to come into contact with the skin, \n— wall and floor coverings, \n— childcare articles, \n— female hygiene products, \n— nappies, \n— two-component room temperature vulcanisation moulding kits (RTV-2 moulding kits). \n(b) Articles not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date.\n\n"},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1628","v":"Di-μ-oxo-di-n-butylstanniohydroxyborane / Dibutyltin hydrogen borate C8H19BO3Sn (DBB)"},"75113-37-0",21,"P",{"$f":"Translator!B1695","v":"Shall not be placed on the market, or used, as a substance, or in mixtures in a concentration equal to, or greater than 0,1 % by weight. \nHowever, the first paragraph shall not apply to this substance (DBB) or mixtures containing it if these are intended solely for conversion into articles, among which this substance will no longer feature in a concentration equal to or greater than 0,1 %.\n"},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1629","v":"deleted (originally Pentachlorophenol and its salts and esters)"},"-",22,"P",{"$f":"Translator!B1696","v":"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020"},null,null,null,null,null,null,null,null,"E2009 / C2020"]
[{"$f":"Translator!B1630","v":"Cadmium and its compounds"},"7440-43-9",23,"P",{"$f":"Translator!B1697","v":"For the purpose of this entry, the codes and chapters indicated in square brackets are the codes and chapters of the tariff and statistical nomenclature of Common Customs Tariff as established by Council Regulation (EEC) No 2658/87 (*).\n1. Shall not be used in mixtures and articles produced from the following synthetic organic polymers (hereafter referred to as plastic material):\n— polymers or copolymers of vinyl chloride (PVC) [3904 10] [3904 21] — polyurethane (PUR) [3909 50] — low-density polyethylene (LDPE), with the exception of low-density polyethylene used for the production of coloured masterbatch [3901 10] — cellulose acetate (CA) [3912 11] — cellulose acetate butyrate (CAB) [3912 11] — epoxy resins [3907 30] — melamine-formaldehyde (MF) resins [3909 20] — urea-formaldehyde (UF) resins [3909 10] — unsaturated polyesters (UP) [3907 91] — polyethylene terephthalate (PET) [3907 60] — polybutylene terephthalate (PBT) — transparent/general-purpose polystyrene [3903 11] — acrylonitrile methylmethacrylate (AMMA) — cross-linked polyethylene (VPE) — high-impact polystyrene — polypropylene (PP) [3902 10]\nMixtures and articles produced from plastic material as listed above shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight of the plastic material.\nBy way of derogation, the second subparagraph shall not apply to articles placed on the\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nmarket before 10 December 2011.\nThe first and second subparagraphs apply without prejudice to Council Directive 94/62/ EC (**) and acts adopted on its basis.\nBy 19 November 2012, in accordance with Article 69, the Commission shall ask the European Chemicals Agency to prepare a dossier conforming to the requirements of Annex XV in order to assess whether the use of cadmium and its compounds in plastic material, other than that listed in subparagraph 1, should be restricted.\n2. Shall not be used or placed on the market in paints with codes [3208] [3209] in a concentration (expressed as Cd metal) equal to or greater than 0,01 % by weight.\nFor paints with codes [3208] [3209] with a zinc content exceeding 10 % by weight of the paint, the concentration of cadmium (expressed as Cd metal) shall not be equal to or greater than 0,1 % by weight.\nPainted articles shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,1 % by weight of the paint on the painted article.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to articles coloured with mixtures containing cadmium for safety reasons.\n4. By way of derogation, paragraph 1, second sub paragraph shall not apply to:\n— mixtures produced from PVC waste, hereinafter referred to as ‘recovered PVC’,\n— mixtures and articles containing recovered PVC if their concentration of cadmium (expressed as Cd metal) does not exceed 0,1 % by weight of the plastic material in the following rigid PVC applications:\n(a) profiles and rigid sheets for building applications; (b) doors, windows, shutters, walls, blinds, fences, and roof gutters; (c) decks and terraces; (d) cable ducts; (e) pipes for non-drinking water if the recovered PVC is used in the middle layer of a multilayer pipe and is entirely covered with a layer of newly produced PVC in compliance with paragraph 1 above.\nSuppliers shall ensure, before the placing on the market of mixtures and articles containing recovered PVC for the first time, that these are visibly, legibly and indelibly marked as follows: ‘ Contains recovered PVC ’ or with the following pictogram:\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nIn accordance with Article 69 of this Regulation, the derogation granted in paragraph 4 will be reviewed, in particular with a view to reducing the limit value for cadmium and to reassess the derogation for the applications listed in points (a) to (e), by 31 December 2017.\n5. For the purpose of this entry, ‘cadmium plating’ means any deposit or coating of metallic cadmium on a metallic surface.\nShall not be used for cadmium plating metallic articles or components of the articles used in the following sectors/applications:\n(a) equipment and machinery for:\n— food production [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] — agriculture [8419 31] [8424 81] [8432] [8433] [8434] [8436] — cooling and freezing [8418] — printing and book-binding [8440] [8442] [8443]\n(b) equipment and machinery for the production of:\n— household goods [7321] [8421 12] [8450] [8509] [8516] — furniture [8465] [8466] [9401] [9402] [9403] [9404] — sanitary ware [7324] — central heating and air conditioning plant [7322] [8403] [8404] [8415]\nIn any case, whatever their use or intended final purpose, the placing on the market of cadmium-plated articles or components of such articles used in the sectors/applications listed in points (a) and (b) above and of articles manufactured in the sectors listed in point (b) above is prohibited.\n6. The provisions referred to in paragraph 5 shall also be applicable to cadmium-plated articles or components of such articles when used in the sectors/applications listed in points (a) and (b) below and to articles manufactured in the sectors listed in (b) below:\n(a) equipment and machinery for the production of:\n— paper and board [8419 32] [8439] [8441] textiles and clothing [8444] [8445] [8447] [8448] [8449] [8451] [8452]\n(b) equipment and machinery for the production of:\n— industrial handling equipment and machinery [8425] [8426] [8427] [8428] [8429] [8430] [8431] — road and agricultural vehicles [chapter 87] — rolling stock [chapter 86] — vessels [chapter 89]\n7. However, the restrictions in paragraphs 5 and 6 shall not apply to:\n— articles and components of the articles used in the aeronautical, aerospace, mining, offshore and nuclear sectors whose applications require high safety standards and in safety devices in road and agricultural vehicles, rolling stock\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nand vessels, — electrical contacts in any sector of use, where that is necessary to ensure the reliability required of the apparatus on which they are installed.\n8. Shall not be used in brazing fillers in concentration equal to or greater than 0,01 % by weight.\nBrazing fillers shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight.\nFor the purpose of this paragraph brazing shall mean a joining technique using alloys and undertaken at temperatures above 450 °C.\n9. By way of derogation, paragraph 8 shall not apply to brazing fillers used in defence and aerospace applications and to brazing fillers used for safety reasons.\n10. Shall not be used or placed on the market if the concentration is equal to or greater than 0,01 % by weight of the metal in:\n(i) metal beads and other metal components for jewellery making; (ii) metal parts of jewellery and imitation jewellery articles and hair accessories, including:\n— bracelets, necklaces and rings, — piercing jewellery, — wrist-watches and wrist-wear, — brooches and cufflinks.\n11. By way of derogation, paragraph 10 shall not apply to articles placed on the market before 10 December 2011 and jewellery more than 50 years old on 10 December 2011.\n________ __\n(*) OJ L 256, 7.9.1987, p. 42.\n(**) OJ L 365, 31.12.1994, p. 10"},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009 / C2011 / C2012"]
[{"$f":"Translator!B1631","v":"Monomethyl — tetrachlorodiphenyl methane Trade name: Ugilec 141"},"76253-60-6",24,"P",{"$f":"Translator!B1698","v":"1. Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market.\n2. By way of derogation, paragraph 1 shall not apply:\n(a) in the case of plant and machinery already in service on 18 June 1994, until such plant and machinery is disposed of; (b) in the case of the maintenance of plant and machinery already in service within a Member State on 18 June 1994.\nFor the purposes of point (a) Member States may, on grounds of human health protection and environmental protection, prohibit within their territory the use of such plant or machinery before it is disposed of."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1632","v":"Monomethyl-dichloro-diphenyl methane Trade name: Ugilec 121, Ugilec 21"},"-",25,"P",{"$f":"Translator!B1699","v":"Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1633","v":"Monomethyl-dibromo-diphenyl methane bromobenzylbromotoluene, mixture of isomers Trade name: DBBT"},"99688-47-8",26,"P",{"$f":"Translator!B1700","v":"Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1634","v":"Nickel and its compounds"},"7440-02-0",27,"P",{"$f":"Translator!B1701","v":"1. Shall not be used:\n(a) in any post assemblies which are inserted into pierced ears and other pierced parts of the human body unless the rate of nickel release from such post assemblies is less than 0,2 μg/cm²/week (migration limit); (b) in articles intended to come into direct and prolonged contact with the skin such as:\n— earrings, — necklaces, bracelets and chains, anklets, finger rings, — wrist-watch cases, watch straps and tighteners, — rivet buttons, tighteners, rivets, zippers and metal marks, when these are used in garments,\nif the rate of nickel release from the parts of these articles coming into direct and prolonged contact with the skin is greater than 0,5 μg/cm²/week.\n(c) in articles referred to in point (b) where these have a non-nickel coating unless such coating is sufficient to ensure that the rate of nickel release from those parts of such articles coming into direct and prolonged contact with the skin will not exceed 0,5 μg/cm²/week for a period of at least two years of normal use of the article.\n2. Articles which are the subject of paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. The standards adopted by the European Committee for Standardisation (CEN) shall be used as the test methods for demonstrating the conformity of articles to paragraphs 1 and 2."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1635","v":"Substances which are classified as carcinogen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 1 or Appendix 2, respectively."},"-",28,"P",{"$f":"Translator!B1702","v":"Without prejudice to the other parts of this Annex the following shall apply to entries 28 to 30:\n1. Shall not be placed on the market, or used,\n— as substances, \n— as constituents of other substances, or, \n— in mixtures,\nfor supply to the general public when the individual concentration in the substance or mixture is equal to or greater than:\n— either the relevant specific concentration limit specified in Part 3 of Annex VI to Regulation (EC) No 1272/2008, or,\n— the relevant generic concentration limit specified in Part 3 of Annex I of Regulation (EC) No 1272/2008.\nWithout prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is marked visibly, legibly and indelibly as follows:\n‘Restricted to professional users’.\n2. By way of derogation, paragraph 1 shall not apply to:\n(a) medicinal or veterinary products as defined by Directive 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC;\n(c) the following fuels and oil products:\n— motor fuels which are covered by Directive 98/70/EC,\n— mineral oil products intended for use as fuel in mobile or fixed combustion plants,\n— fuels sold in closed systems (e.g. liquid gas bottles);\n\n(d) artists’ paints covered by Regulation (EC) No 1272/2008;\n(e) the substances listed in Appendix 11, column 1, for the applications or uses listed in Appendix 11, column 2. Where a date is specified in column 2 of Appendix 11, the derogation shall apply until the said date;\n(f) devices covered by Regulation (EU) 2017/745."},null,{"$f":"Translator!$B$1745","v":"0,1 % by weight \n(Repro. Tox: 0,3 % by weight)"},null,null,null,null,null,null,"E2009 / C2011 / C2013 / C2020"]
[{"$f":"Translator!B1636","v":"Substances which are classified as germ cell mutagen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 3 or Appendix 4, respectively."},null,29,"P"]
[{"$f":"Translator!B1637","v":"Substances which are classified as reproductive toxicant category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 5 or Appendix 6, respectively."},null,30,"P"]
[{"$f":"Translator!B1638","v":"(a) Creosote; wash oil\n\n(b) Creosote oil; wash oil\n\n(c) Distillates (coal tar), naphthalene oils; naphthalene oil\n\n(d) Creosote oil, acenaphthene fraction; wash oil\n\n(e) Distillates (coal tar), upper; heavy anthracene oil\n\n(f) Anthracene oil\n\n(g) Tar acids, coal, crude; crude phenols\n\n(h) Creosote, wood\n\n(i) Low temperature tar oil, alkaline; extract residues (coal), low temperature coal tar alkaline"},"a) 8001-58-9\n\nb) 61789-28-4\n\nc) 84650-04-4\n\nd) 90640-84-9\n\ne) 65996-91-0\n\nf) 90640-80-5\n\ng) 65996-85-2\n\nh) 8021-39-4\n\ni) 122384-78-5",31,"P",{"$f":"Translator!B1703","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for the treatment of wood. Furthermore, wood so treated shall not be placed on the market.\n2. By way of derogation from paragraph 1:\n(a) The substances and mixtures may be used for wood treatment in industrial installations or by professionals covered by Community legislation on the protection of workers for in situ retreatment only if they contain:\n(i) benzo[a]pyrene at a concentration of less than 50 mg/kg (0,005 % by weight), and\n(ii) water extractable phenols at a concentration of less than 3 % by weight.\nSuch substances and mixtures for use in wood treatment in industrial installations or by professionals:\n— may be placed on the market only in packaging of a capacity equal to or greater than 20 litres,\n— shall not be sold to consumers.\nWithout prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations or professional treatment only’.\n(b) Wood treated in industrial installations or by professionals according to subparagraph (a) which is placed on the market for the first time or retreated in situ may be used for professional and industrial use only, for example on railways, in electric power transmission and telecommunications, for fencing, for agricultural purposes (for example stakes for tree support) and in harbours and waterways.\n(c) The prohibition in paragraph 1 on the placing on the market shall not apply to wood which has been treated with substances listed in entry 31 (a) to (i) before 31 December 2002 and is placed on the second-hand market for re-use.\n3. Treated wood referred to under paragraph 2(b) and (c) shall not be used:\n— inside buildings, whatever their purpose,\n— in toys,\n— in playgrounds,\n— in parks, gardens, and outdoor recreational and leisure facilities where there is a risk of frequent skin contact,\n— in the manufacture of garden furniture such as picnic tables,\n— for the manufacture and use and any re-treatment of:\n— containers intended for growing purposes,\n— packaging that may come into contact with raw materials, intermediate or finished products destined for human and/or animal consumption,\n— other materials which may contaminate the articles mentioned above."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1639","v":"Chloroform"},"67-66-3\n\n\n",32,"P",{"$f":"Translator!B1704","v":"Without prejudice to the other parts of this Annex, the following shall apply to entries 32,34 to 38:\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or in mixtures in concentrations equal to or greater than 0,1 % by weight,\nwhere the substance or mixture is intended for supply to the general public and/or is intended\nfor diffusive applications such as in surface cleaning and cleaning of fabrics.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures containing them in concentrations equal to or greater than 0,1 % by weight is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations only’.\nBy way of derogation this provision shall not apply to:\n(a) medicinal or veterinary products as defined by\nDirective 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1640","v":"deleted (originally Tetrachloromethane)"},"-",33,"P",null,null,null,null,null,null,null,null,null,"C2009"]
[{"$f":"Translator!B1641","v":"1,1,2-Trichloroethane"},"79-00-5",34,"P",null,null,null,null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1642","v":"1,1,2,2-Tetrachloroethane"},"79-34-5",35,"P"]
[{"$f":"Translator!B1643","v":"1,1,1,2-Tetrachloroethane"},"630-20-6",36,"P"]
[{"$f":"Translator!B1644","v":"Pentachloroethane"},"76-01-7",37,"P"]
[{"$f":"Translator!B1645","v":"1,1-Dichloroethene"},"75-35-4",38,"P"]
[{"$f":"Translator!B1646","v":"deleted (originally 1,1,1-Trichloroethane"},"-",39,null,null,null,null,null,null,null,null,null,null,"C2009"]
[{"$f":"Translator!B1647","v":"Hexachloroethane"}," 67-72-1",41,"P",{"$f":"Translator!B1705","v":"Shall not be placed on the market, or used, as substance or in mixtures, where the substance or mixture is intended for the manufacturing or processing of non-ferrous metals."},null,{"$f":"Translator!$B$1735","v":"0 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1648","v":"deleted (originally Chloroalkanes)"},"-",42,null,null,null,null,null,null,null,null,null,null,"C2013"]
[{"$f":"Translator!B1649","v":"Azocolourants and Azodyes"},"-",43,"P",{"$f":"Translator!B1706","v":"1. Azodyes which, by reductive cleavage of one or more azo groups, may release one or more of the aromatic amines listed in Appendix 8, in detectable concentrations, i.e. above 30 mg/kg (0,003 % by weight) in the articles or in the dyed parts thereof, according to the testing methods listed in Appendix 10, shall not be used, in textile and leather articles which may come into direct and prolonged contact with the human skin or oral cavity, such as:\n— clothing, bedding, towels, hairpieces, wigs, hats, nappies and other sanitary items, sleeping bags,\n— footwear, gloves, wristwatch straps, handbags, purses/wallets, briefcases, chair covers, purses worn round the neck,\n— textile or leather toys and toys which include textile or leather garments,\n— yarn and fabrics intended for use by the final consumer.\n2. Furthermore, the textile and leather articles referred to in paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. Azodyes, which are contained in Appendix 9, ‘List of azodyes’ shall not be placed on the market, or used, as substances, or in mixtures in concentrations greater than 0,1 % by weight, where the substance or the mixture is intended for colouring textile and leather articles."},null,{"$f":"Translator!$B$1739","v":"0,003 % by weight"},null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1650","v":"deleted (originally Diphenylether, pentabromo derivative)"},"-",44,null,null,null,null,null,null,null,null,null,null,"C2011"]
[{"$f":"Translator!B1651","v":"Diphenylether, octabromo derivative C12H2Br8O"},"-",45,"P",{"$f":"Translator!B1707","v":"1. Shall not be placed on the market, or used:\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations greater than 0,1 % by weight.\n2. Articles shall not be placed on the market if they, or flame-retardant parts thereof, contain this substance in concentrations greater than 0,1 % by weight.\n3. By way of derogation, paragraph 2 shall not apply:\n— to articles that were in use in the Community before 15 August 2004,\n— to electrical and electronic equipment within the scope of Directive 2002/95/EC."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1652","v":"a) Nonylphenol C6H4(OH)C9H19\n\nb) Nonylphenol ethoxylates (C2H4O)nC15H24O"},"a) 25154-52-3\n\nb) -",46,"P",{"$f":"Translator!B1708","v":"Shall not be placed on the market, or used, as substances or in mixtures in concentrations equal to or greater than 0,1 % by weight for the following purposes:\n(1) industrial and institutional cleaning except:\n— controlled closed dry cleaning systems where the washing liquid is recycled or incinerated,\n— cleaning systems with special treatment where the washing liquid is recycled or incinerated.\n(2) domestic cleaning;\n(3) textiles and leather processing except:\n— processing with no release into waste water,\n— systems with special treatment where the process water is pre-treated to remove the organic fraction completely prior to biological waste water treatment (degreasing of sheepskin);\n(4) emulsifier in agricultural teat dips;\n(5) metal working except:\n— uses in controlled closed systems where the washing liquid is recycled or incinerated;\n(6) manufacturing of pulp and paper;\n(7) cosmetic products;\n(8) other personal care products except:\n— spermicides;\n(9) co-formulants in pesticides and biocides. However national authorisations for pesticides or biocidal products containing nonylphenol ethoxylates as co-formulant, granted before 17 July 2003, shall not be affected by this restriction until their date of expiry."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1653","v":"Nonylphenol ethoxylates (C2H4O)nC15H24O"},"-","46a","P",{"$f":"Translator!B1709","v":"1. Shall not be placed on the market after 3 February 2021 in textile articles which can reasonably be expected to be washed in water during their normal lifecycle, in concentrations equal to or greater than 0,01 % by weight of that textile article or of each part of the textile article.\n2. Paragraph 1 shall not apply to the placing on the market of second- hand textile articles or of new textile articles produced, without the use of NPE, exclusively from recycled textiles.\n3. For the purposes of paragraphs 1 and 2, “textile article” means any unfinished, semi-finished or finished product which is composed of at least 80 % textile fibres by weight, or any other product that contains a part which is composed of at least 80 % textile fibres by weight, including products such as clothing, accessories, interior textiles, fibres, yarn, fabrics and knitted panels.’"},null,{"$f":"Translator!$B$1741","v":"0,01 % by weight"},null,null,null,null,null,null,"E2009 / C2020"]
[{"$f":"Translator!B1654","v":"Chromium VI compounds"},"-",47,"P",{"$f":"Translator!B1710","v":"1. Cement and cement-containing mixtures shall not be placed on the market, or used, if they contain, when hydrated, more than 2 mg/kg (0,0002%) soluble chromium VI of the total dry weight of the cement.\n2. If reducing agents are used, then without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of cement or cement-containing mixtures is visibly, legibly and indelibly marked with information on the packing date, as well as on the storage conditions and the storage period appropriate to maintaining the activity of the reducing agent and to keeping the content of soluble chromium VI below the limit indicated in paragraph 1.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the placing on the market for, and use in, controlled closed and totally automated processes in which cement and cement-containing mixtures are handled solely by machines and in which there is no possibility of contact with the skin.\n4. The standard adopted by the European Committee for Standardization (CEN) for testing the water-soluble chromium (VI) content of cement and cement-containing mixtures shall be used as the test method for demonstrating conformity with paragraph 1.\n5. Leather articles coming into contact with the skin shall not be placed on the market where they contain chromium VI in concentrations equal to or greater than 3 mg/kg (0,0003 % by weight) of the total dry weight of the leather.\n6. Articles containing leather parts coming into contact with the skin shall not be placed on the market where any of those leather parts contains chromium VI in concentrations equal to or greater than 3 mg/kg (0,0003 % by weight) of the total dry weight of that leather part.\n7. Paragraphs 5 and 6 shall not apply to the placing on the market of second-hand articles which were in end-use in the Union before 1 May 2015."},null,{"$f":"Translator!$B$1737","v":"0,0003 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1655","v":"Toluene"},"108-88-3",48,"P",{"$f":"Translator!B1711","v":"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight where the substance or mixture is used in adhesives or spray paints intended for supply to the general public."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1656","v":"Trichlorobenzene"},"120-82-1",49,"P",{"$f":"Translator!B1712","v":"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight for any use except:\n— as an intermediate of synthesis, or, — as a process solvent in closed chemical applications for chlorination reactions, or,\n— in the manufacture of 1,3,5-triamino-2,4,6-trinitrobenzene (TATB)."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1657","v":"Polycyclic-aromatic hydrocarbons (PAH)\na) Benzo[a]pyrene (BaP)\n\nb) Dibenzo[a,h]anthracene (DBAhA)\n\nc) Benzo[a]anthracene (BaA)\n\nd) Chrysen (CHR)\n\ne) Benzo[j]fluoranthene (BjFA)\n\nf) Benzo[b]fluoranthene (BbFA)\n\ng) Benzo[k]fluoranthene (BkFA) \n\nh) Benzo[e]pyrene (BeP)"},"a) 50-32-8\n\nb) 192-97-2\n\nc) 56-55-3\n\nd) 218-01-9\n\ne) 205-99-2\n\nf) 205-82-3\n\ng) 207-08-9\n\nh) 53-70-3",50,"P",{"$f":"Translator!B1713","v":"1. From 1 January 2010, extender oils shall not be placed on the market, or used for the production of tyres or parts of tyres if they contain:\n— more than 1 mg/kg (0,0001 % by weight) BaP, or,\n— more than 10 mg/kg (0,001 % by weight) of the sum of all listed PAHs.\nThe standard EN 16143:2013 (Petroleum products — Determination of content of Benzo(a)pyrene (BaP) and selected polycyclic aromatic hydrocarbons (PAH) in extender oils — Procedure using double LC cleaning and GC/MS analysis) shall be used as the test method for demonstrating conformity with the limits referred to in the first subparagraph.\nUntil 23 September 2016, the limits referred to in the first subparagraph may be regarded as kept, if the polycyclic aromatics (PCA) extract is less than 3 % by weight as measured by the Institute of Petroleum standard IP 346:1998 (Determination of PCA in unused lubricating base oils and asphaltene free petroleum fractions — Dimethyl sulphoxide extraction refractive index method), provided that compliance with the limits of BaP and of the listed PAHs, as well as the correlation of the measured values with the PCA extract, is measured by the manufacturer or importer every six months or after each major operational change, whichever is earlier.\n2. Furthermore, tyres and treads for retreading manufactured after 1 January 2010 shall not be placed on the market if they contain extender oils exceeding the limits indicated in paragraph 1.\nThese limits shall be regarded as kept, if the vulcanised rubber compounds do not exceed the limit of 0,35 % Bay protons as measured and calculated by ISO 21461 (Rubber vulcanised — Determination of aromaticity of oil in vulcanised rubber compounds).\n3. By way of derogation, paragraph 2 shall not apply to retreaded tyres if their tread does not contain extender oils exceeding the limits referred to in paragraph 1.\n4. For the purpose of this entry ‘tyres’ shall mean tyres for vehicles covered by:\n— Directive 2007/46/EC of the European Parliament and of the Council of 5 September 2007 establishing a framework for the approval of motor vehicles and their trailers (*),\n— Directive 2003/37/EC of the European Parliament and of the Council of 26 May 2003 on type-approval of agricultural or forestry tractors, their trailers and interchangeable towed machinery, together with their systems, components and separate technical units (**), and\n— Directive 2002/24/EC of the European Parliament and of the Council of 18 March 2002 relating to the type-approval of two or three-wheel motor vehicles and repealing Council Directive 92/61/EEC (***).\n5. Articles shall not be placed on the market for supply to the general public, if any of their rubber or plastic components that come into direct as well as prolonged or short-term repetitive contact with the human skin or the oral cavity, under normal or reasonably foreseeable conditions of use, contain more than 1 mg/kg (0,0001 % by weight of this component) of any of the listed PAHs.\nSuch articles include amongst others:\n— sport equipment such as bicycles, golf clubs, racquets\n— household utensils, trolleys, walking frames\n— tools for domestic use\n— clothing, footwear, gloves and sportswear\n— watch-straps, wrist-bands, masks, head-bands\n6. Toys, including activity toys, and childcare articles, shall not be placed on the market, if any of their rubber or plastic components that come into direct as well as prolonged or short-term repetitive contact with the human skin or the oral cavity, under normal or reasonably foreseeable conditions of use, contain more than 0,5 mg/kg (0,00005 % by weight of this component) of any of the listed PAHs.\n7. By way of derogation from paragraphs 5 and 6, these paragraphs shall not apply to articles placed on the market for the first time before 27 December 2015.\n8. By 27 December 2017, the Commission shall review the limit values in paragraphs 5 and 6 in the light of new scientific information, including migration of PAHs from the articles referred to therein, and information on alternative raw materials and, if appropriate, modify these paragraphs accordingly.\n______________\n(*) OJ L 263, 9.10.2007, p. 1.\n(**) OJ L 171, 9.7.2003, p. 1.\n(***) OJ L 124, 9.5.2002, p. 1."},null,{"$f":"Translator!$B$1736","v":"0,0001 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1658","v":"The following phthalates:\n(a) Bis (2-ethylhexyl) phthalate (DEHP)\n\n(b) Dibutyl phthalate (DBP)\n\n(c) Benzyl butyl phthalate (BBP)\n\n(d) Diisobutyl phthalate (DIBP)"},"a) 117-81-7\n\nb) 84-74-2\n\nc) 85-68-7\n\nd) 84-69-5",51,"P",{"$f":"Translator!B1714","v":"1. Shall not be used as substances or in mixtures, individually or in any combination of the phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material, in toys and childcare articles.\n2. Shall not be placed on the market in toys or childcare articles, individually or in any combination of the first three phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material.\nIn addition, DIBP shall not be placed on the market after 7 July 2020 in toys or childcare articles, individually or in any combination with the first three phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material.\n3. Shall not be placed on the market after 7 July 2020 in articles, individually or in any combination of the phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material in the article.\n4. Paragraph 3 shall not apply to:\n(a) articles exclusively for industrial or agricultural use, or for use exclusively in the open air, provided that no plasticised material comes into contact with human mucous membranes or into prolonged contact with human skin;\n(b) aircraft, placed on the market before 7 January 2024, or articles, whenever placed on the market, for use exclusively in the maintenance or repair of those aircraft, where those articles are essential for the safety and airworthiness of the aircraft;\n(c) motor vehicles within the scope of Directive 2007/46/EC, placed on the market before 7 January 2024, or articles, whenever placed on the market, for use exclusively in the maintenance or repair of those vehicles, where the vehicles cannot function as intended without those articles;\n(d) articles placed on the market before 7 July 2020;\n(e) measuring devices for laboratory use, or parts thereof;\n(f) materials and articles intended to come into contact with food within the scope of Regulation (EC) No 1935/2004 or Commission Regulation (EU) No 10/2011 (*);\n(g) medical devices within the scope of Directives 90/385/EEC, 93/42/EEC or 98/79/EC, or parts thereof;\n(h) electrical and electronic equipment within the scope of Directive 2011/65/EU;\n(i) the immediate packaging of medicinal products within the scope of Regulation (EC) No 726/2004, Directive 2001/82/EC or Directive 2001/83/EC;\n(j) toys and childcare articles covered by paragraphs 1 or 2.\n5. For the purposes of paragraphs 1, 2, 3 and 4(a),\n(a) ‘plasticised material’ means any of the following homogeneous materials:\n- polyvinyl chloride (PVC), polyvinylidene chloride (PVDC),polyvinyl acetate (PVA), polyurethanes,\n- any other polymer (including, inter alia, polymer foams and rubber material) except silicone rubber and natural latex coatings,\n- surface coatings, non-slip coatings, finishes, decals, printed designs,\n- adhesives, sealants, paints and inks.\n(b) ‘prolonged contact with human skin’ means continuous contact of more than 10 minutes duration or intermittent contact over a period of 30 minutes, per day.\n(c) ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.\n6. For the purposes of paragraph 4(b), ‘aircraft’ means one of the following:\n(a) a civil aircraft produced in accordance with a type certificate issued under Regulation (EC) No 216/2008 or with a design approval issued under the national regulations of a contracting State of the International Civil Aviation Organisation (ICAO), or for which a certificate of airworthiness has been issued by an ICAO contracting State under Annex 8 to the Convention on International Civil Aviation, signed on December 7, 1944 , in Chicago;\n(b) a military aircraft.\n\n----------------------------\n(*) Commission Regulation (EU) No 10/2011 of 14 January 2011 on plastic materials and articles intended to come into contact with food (OJ L 12, 15.1.2011, p. 1)."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1660","v":"The following phthalates:\n(a) Di-‘isononyl’ phthalate (DINP)\n\n(b) Di-‘isodecyl’ phthalate (DIDP)\n\n(c) Di-n-octyl phthalate (DNOP)"},"\na) 28553-12-0 und 68515-48-0\n\nb) 26761-40-0 und 68515-49-1\n\nc) 117-84-0",52,"P",{"$f":"Translator!B1715","v":"1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles which can be placed in the mouth by children.\n2. Such toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n(3. Regulation (EU) No 326/2015: paragraph 3 is deleted.)\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1661","v":"deleted (originally perfluorooctane sulfonates (PFOS))"},"-",53,null,null,null,null,null,null,null,null,null,null,"C2011"]
[{"$f":"Translator!B1662","v":"2-(2-methoxyethoxy)ethanol (DEGME)"},"111-77-3",54,"P",{"$f":"Translator!B1716","v":"Shall not be placed on the market after 27 June 2010, for supply to the general public, as a constituent of paints, paint strippers, cleaning agents, self-shining emulsions or floor sealants in concentrations equal to or greater than 0,1 % by weight."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1663","v":"2-(2-butoxyethoxy)ethanol (DEGBE)"},"112-34-5",55,"P",{"$f":"Translator!B1717","v":"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of spray paints or spray cleaners in aerosol dispensers in concentrations equal to or greater than 3 % by weight.\n2. Spray paints and spray cleaners in aerosol dispensers containing DEGBE and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that paints other than spray paints containing DEGBE in concentrations equal to or greater than 3 % by weight of that are placed on the market for supply to the general public are visibly, legibly and indelibly marked by 27 December 2010 as follows:\n‘Do not use in paint spraying equipment’."},null,{"$f":"Translator!$B$1751","v":"3 % by weight"},null,null,null,null,null,null,"E2009 / C2011"]
[{"$f":"Translator!B1664","v":"Methylenediphenyl diisocyanate (MDI) including the following specific isomers (See group members):\n(a) 4,4’-Methylenediphenyl diisocyanate:\n\n(b) 2,4’-Methylenediphenyl diisocyanate:\n\n(c) 2,2’-Methylenediphenyl diisocyanate:"},"26447-40-5\n\na) 101-68-8\n\nb) 5873-54-1\n\nc) 2536-05-2",56,"P",{"$f":"Translator!B1718","v":"1. Shall not be placed on the market after 27 December 2010, as a constituent of mixtures in concentrations equal to or greater than 0,1 % by weight of MDI for supply to the general public, unless suppliers shall ensure before the placing on the market that the packaging:\n(a) contains protective gloves which comply with the requirements of Council Directive 89/686/EEC (*);\n(b) is marked visibly, legibly and indelibly as follows, and without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures:\n‘— Persons already sensitised to diisocyanates may develop allergic reactions when using this product.\n— Persons suffering from asthma, eczema or skin problems should avoid contact,\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nincluding dermal contact, with this product.\n— This product should not be used under conditions of poor ventilation unless a protective mask with an appropriate gas filter (i.e. type A1 according to standard EN 14387) is used.’\n2. By way of derogation, paragraph 1(a) shall not apply to hot melt adhesives.\n______________\n(*) OJ L 399, 30.12.1989, p. 18."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1665","v":"Cyclohexane"},"110-82-7",57,"P",{"$f":"Translator!B1719","v":"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of neoprene-based contact adhesives in concentrations equal to or greater than 0,1 % by weight in package sizes greater than 350 g.\n2. Neoprene-based contact adhesives containing cyclohexane and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that neoprene-based contact adhesives containing cyclohexane in concentrations equal to or greater than 0,1 % by weight that are placed on the market for supply to the general public after 27 December 2010 are visibly, legibly and indelibly marked as follows:\n‘— This product is not to be used under conditions of poor ventilation.\n— This product is not to be used for carpet laying.’."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1666","v":"Dichloromethane"},"75-09-2",59,"P",{"$f":"Translator!B1720","v":"1. Paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall not be:\n(a) placed on the market for the first time for supply to the general public or to professionals after 6 December 2010;\n(b) placed on the market for supply to the general public or to professionals after 6 December 2011;\n(c) used by professionals after 6 June 2012.\nFor the purposes of this entry:\n(i) ‘professional’ means any natural or legal person, including workers and self-employed workers undertaking paint stripping in the course of their professional activity outside an industrial installation;\n(ii) ‘industrial installation’ means a facility used for paint stripping activities.\n2. By way of derogation from paragraph 1, Member States may allow on their territories and for certain activities the use, by specifically trained professionals, of paint strippers containing dichloromethane and may allow the placing on the market of such paint strippers for supply to those professionals.\nMember States making use of this derogation shall define appropriate provisions for the protection of the health and safety of those professionals using paint strippers containing dichloromethane and shall inform the Commission thereof.\nThose provisions shall include a requirement that a professional shall hold a certificate that is accepted by the Member State in which that professional operates, or provide other documentary evidence to that effect, or be otherwise approved by that Member State, so as to demonstrate proper training and competence to safely use paint strippers containing dichloromethane.\nThe Commission shall prepare a list of the Member States which have made use of the derogation in this paragraph and make it publicly available over the Internet.\n\n3. A professional benefiting from the derogation referred to in paragraph 2 shall operate only in Member States which have made use of that derogation. The training referred to in paragraph 2 shall cover as a minimum:\n(a) awareness, evaluation and management of risks to health, including information on existing substitutes or processes, which under their conditions of use are less hazardous to the health and safety of workers;\n(b) use of adequate ventilation;\n(c) use of appropriate personal protective equipment that complies with Directive 89/686/EEC.\nEmployers and self-employed workers shall preferably replace dichloromethane with a chemical agent or process which, under its conditions of use, presents no risk, or a lower risk, to the health and safety of workers.\nProfessional shall apply all relevant safety measures in practice, including the use of personal protective equipment.\n4. Without prejudice to other Community legislation on workers protection, paint strippers containing dichloromethane in concentrations equal to or greater than 0,1 % by weight may be used in industrial installations only if the following minimum conditions are met:\n(a) effective ventilation in all processing areas, in particular for the wet processing and the drying of stripped articles: local exhaust ventilation at strip tanks supplemented by forced ventilation in those areas, so as to minimise exposure and to ensure compliance, where technically feasible, with relevant occupational exposure limits;\n(b) measures to minimise evaporation from strip tanks comprising: lids for covering strip tanks except during loading and unloading; suitable loading and unloading arrangements for strip tanks; and wash tanks with water or brine to remove excess solvent after unloading;\n(c) measures for the safe handling of dichloromethane in strip tanks comprising: pumps and pipework for transferring paint stripper to and from strip tanks; and suitable arrangements for safe cleaning of tanks and removal of sludge;\n(d) personal protective equipment that complies with Directive 89/686/EEC comprising: suitable protective gloves, safety goggles and protective clothing; and appropriate respiratory protective equipment where compliance with relevant occupational exposure limits cannot be otherwise achieved;\n(e) adequate information, instruction and training for operators in the use of such equipment.\n5. Without prejudice to other Community provisions concerning the classification, labelling and packaging of substances and mixtures, by 6 December 2011 paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall be visibly, legibly and indelibly marked as follows:\n‘Restricted to industrial use and to professionals approved in certain EU Member States — verify where use is allowed.’"},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1667","v":"Acrylamide"},"79-06-1",60,"P",{"$f":"Translator!B1721","v":"Shall not be placed on the market or used as a substance or constituent of mixtures in a concentration, equal to or greater than 0,1 % by weight for grouting applications after 5 November 2012."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2012"]
[{"$f":"Translator!B1668","v":"Dimethyl fumarate (DMFu)"},"624-49-7",61,"P",{"$f":"Translator!B1722","v":"Shall not be used in articles or any parts thereof in concentrations greater than 0,1 mg/kg.\nArticles or any parts thereof containing DMF in concentrations greater than 0,1 mg/kg shall not be placed on the market."},null,{"$f":"Translator!$B$1746","v":"0,1 mg/kg"},null,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1669","v":"(a) Phenylmercury acetate\n\n(b) Phenylmercury propionate\n\n(c) Phenylmercury 2-ethylhexanoate\n\n(d) Phenylmercury octanoate\n\n(e) Phenylmercury neodecanoate"},"a) 62-38-4\n\nb) 103-27-5\n\nc) 13302-00-6\n\n\nd) 13864-38-5\n\ne) 26545-49-3\n",62,"P",{"$f":"Translator!B1723","v":"1. Shall not be manufactured, placed on the market or used as substances or in mixtures after 10 October 2017 if the concentration of mercury in the mixtures is equal to or greater than 0,01 % by weight.\n\n2. Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight."},null,{"$f":"Translator!$B$1741","v":"0,01 % by weight"},null,null,null,null,null,null,"E2012"]
[{"$f":"Translator!B1670","v":"Lead and its compounds"},"7439-92-1",63,"P",{"$f":"Translator!B1724","v":"1. Shall not be placed on the market or used in any individual part of jewellery articles if the concentration of lead (expressed as metal) in such a part is equal to or greater than 0,05 % by weight.\n2. For the purposes of paragraph 1:\n(i) ‘jewellery articles’ shall include jewellery and imitation jewellery articles and hair accessories, including:\n(a) bracelets, necklaces and rings;\n(b) piercing jewellery;\n(c) wrist watches and wrist-wear;\n(d) brooches and cufflinks;\n(ii) ‘any individual part’ shall include the materials from which the jewellery is made, as well as the individual components of the jewellery articles.\n3. Paragraph 1 shall also apply to individual parts when placed on the market or used for jewellery-making.\n4. By way of derogation, paragraph 1 shall not apply to:\n(a) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Council Directive 69/493/EEC (*);\n(b) internal components of watch timepieces inaccessible to consumers;\n(c) non-synthetic or reconstructed precious and semiprecious stones (CN code 7103, as established by Regulation (EEC) No 2658/87), unless they have been treated with lead or its compounds or mixtures containing these substances;\n(d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of minerals melted at a temperature of at least 500 °C.\n\n5. By way of derogation, paragraph 1 shall not apply to jewellery articles placed on the market for the first time before 9 October 2013 and jewellery articles produced before 10 December 1961.\n6. By 9 October 2017, the Commission shall re-evaluate this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 1 and, if appropriate, modify this entry accordingly.\n7. Shall not be placed on the market or used in articles supplied to the general public, if the concentration of lead (expressed as metal) in those articles or accessible parts thereof is equal to or greater than 0,05 % by weight, and those articles or accessible parts thereof may, during normal or reasonably foreseeable conditions of use, be placed in the mouth by children.\nThat limit shall not apply where it can be demonstrated that the rate of lead release from such an article or any such accessible part of an article, whether coated or uncoated, does not exceed 0,05 μg/cm² per hour (equivalent to 0,05 μg/g/h), and, for coated articles, that the coating is sufficient to ensure that this release rate is not exceeded for a period of at least two years of normal or reasonably foreseeable conditions of use of the article.\nFor the purposes of this paragraph, it is considered that an article or accessible part of an article may be placed in the mouth by children if it is smaller than 5 cm in one dimension or has a detachable or protruding part of that size.\n8. By way of derogation, paragraph 7 shall not apply to:\n(a) jewellery articles covered by paragraph 1;\n(b) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Directive 69/493/ EEC;\n(c) non-synthetic or reconstructed precious and semi-precious stones (CN code 7103 as established by Regulation (EEC) No 2658/ 87) unless they have been treated with lead or its compounds or mixtures containing these substances;\n(d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of mineral melted at a temperature of at least 500 ° C;\n(e) keys and locks, including padlocks;\n(f) musical instruments;\n(g) articles and parts of articles comprising brass alloys, if the concentration of lead (expressed as metal) in the brass alloy does not exceed 0,5 % by weight;\n(h) the tips of writing instruments;\n(i) religious articles;\n(j) portable zinc-carbon batteries and button cell batteries;\n(k) articles within the scope of:\n(i) Directive 94/62/EC;\n(ii) Regulation (EC) No 1935/2004;\n(iii) Directive 2009/48/EC of the European Parliament and of the Council (**);\n(iv) Directive 2011/65/EU of the European Parliament and of the Council (***)\n9. By 1 July 2019, the Commission shall re-evaluate paragraphs 7 and 8(e), (f), (i) and (j) of this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 7, including the requirement on coating integrity, and, if appropriate, modify this entry accordingly.\n10. By way of derogation paragraph 7 shall not apply to articles placed on the market for the first time before 1 June 2016.\n______________\n(*) OJ L 326, 29.12.1969, p. 36.\n(**) Directive 2009/48/EC of the European Parliament and of the Council of 18 June 2009 on the safety of toys (OJ L 170, 30.6.2009, p. 1).\n(***) Directive 2011/65/EU of the European Parliament and of the Council of 8 June 2011 on the restriction of the use of certain hazardous substances in electrical and electronic equipment (OJ L 174, 1.7.2011, p. 88)."},null,{"$f":"Translator!$B$1743","v":"0,05 % by weight"},null,null,null,null,null,null,"E2012"]
[{"$f":"Translator!B1671","v":"1,4-Dichlorobenzene"}," 106-46-7",64,"P",{"$f":"Translator!B1725","v":"Shall not be placed on the market or used, as a substance or as a constituent of mixtures in a concentration equal to or greater than 1 % by weight, where the substance or the mixture is placed on the market for use or used as an air freshener or deodoriser in toilets, homes, offices or other indoor public areas."},null,{"$f":"Translator!$B$1749","v":"1 % by weight"},null,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1672","v":"4,4'-isopropylidenediphenol"},"80-05-7",66,"P",{"$f":"Translator!B1726","v":"Shall not be placed on the market in thermal paper in a concentration equal to or greater than 0,02 % by weight after 2 January 2020."},null,{"$f":"Translator!$B$1742","v":"0,02 % by weight"},null,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B1673","v":"deleted (originally Bis(pentabromophenyl) ether)"},"1163-19-5",67,"P",{"$f":"Translator!B1727","v":"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020"},null,null,null,null,null,null,null,null,"E2018 / C2020"]
[{"$f":"Translator!B2789","v":"Linear and branched perfluorocarboxylic acids of the formula CnF2n+1-C(= O)OH where n = 8, 9, 10, 11, 12, or 13 (C9-C14 PFCAs),including their salts, and any combinations thereof;\nPFNA - Perfluorononan-1-oic acid (C9-PFCA) \nPFDA - Nonadecafluorodecanoic acid (C10-PFCA) \nPFUnDA - Henicosafluoroundecanoic acid (C11-PFCA) \nPFDoDA - Tricosafluorododecanoic acid (C12-PFCA) \nPFTrDA - Pentacosafluorotridecanoic acid (C13-PFCA) \nPFTDA - Heptacosafluorotetradecanoic acid (C14-PFCA)"},"375-95-1\n335-76-2\n2058-94-8\n307-55-1\n72629-94-8\n376-06-7",68,"P",{"$f":"Translator!B2790","v":"1.Shall not be manufactured, or placed on the market as substances on their own from 25 February 2023.\n\n2.Shall not, from 25 February 2023, be used in, or placed on the market in:\n(a)another substance, as a constituent;\n(b)a mixture;\n(c)an article,except\n\n if the concentration in the substance, the mixture, or the article is below 25 ppb for the sum of C9-C14 PFCAs and their salts or 260 ppb for the sum of C9-C14 PFCA-related substances.\n\n3 By way of derogation to paragraph 2, the concentration limit shall be 10 ppm for the sum of C9-C14 PFCAs, their salts and C9-C14 PFCA related substances, where they are present in a substance to be used as a transported isolated intermediate, provided that the conditions in points (a) to (f) of Article 18(4) of this Regulation are met for the manufacturing of fluorochemicals with a perfluoro carbon chain length equal to or shorter than 6 atoms. The Commission shall review this limit no later than 25 August 2023.\n\n4.Paragraph 2 shall apply from 4 July 2023to:\n(i)textiles for oil- and water-repellency for the protection of workers from dangerous liquids that comprise risks to their health and safety;\n(ii)the manufacture of polytetrafluoroethylene (PTFE) and polyvinylidene fluoride (PVDF) for the production of:\n— high performance, corrosion resistant gas filter membranes, water filter membranes and membranes for medical textiles;\n— industrial waste heat exchanger equipment;\n— industrial sealants capable of preventing leakage of volatile organic compounds and PM 2,5 particulates\n\n5.By way of derogation to paragraph 2, the use of C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall be allowed until 4 July 2025for:\n(i)photolithography or etch processes in semiconductor manufacturing;\n(ii)photographic coatings applied to films;\n(iii)invasive and implantable medical devices;\n(iv)fire-fighting foam for liquid fuel vapour suppression and liquid fuel fire (Class B fires) already installed in systems, including both mobile and fixed systems, subject to the following conditions:\n— fire-fighting foam that contains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall not be used for training;\n— fire-fighting foam that contains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall not be used for testing unless all releases are contained;\n— from 1 January 2023, uses of fire-fighting foam that con¬tains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall only be allowed to sites where all releases can be contained;\n— fire-fighting foam stockpiles that contain or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related sub¬stances shall be managed in accordance with Article 5 of Regulation (EU) 2019/1021. \n\n6.Paragraph 2(c) shall not apply to articles placed on the market before 25 February 2023.\n\n7.Paragraph 2 shall not apply to the can coating for  pressurised metered-dose inhalers until 25 August 2028.\n\n8.Paragraph 2 (c) shall apply from 31 December 2023to:\n(a)semiconductors on their own;\n(b)semiconductors incorporated in  semi-finished and  finished electronic equipment.\n\n9.Paragraph 2(c) shall apply from 31  December 2030to semiconductors  used in  spare or  replacement parts  for  finished electronic equipment placed on  the  market before 31  December 2023.\n\n10.Until 25  August  2024,  the  concentration limit referred to  in paragraph 2  shall  be 2 000ppb  for  the  sum  of  C9-C14 PFCAs  in fluoroplastics and  fluoroelastomers that contain perfluoroalkoxy groups. From 25  August  2024,  the  concentration limit  shall  be  100 ppb for  the  sum of  C9-C14 PFCAs, in  fluoroplastics and fluoroelastomers that contain perfluoroalkoxy groups. All emissions of C9-C14 PFCAs  during  the  manufacture  and  use  of  fluoroplastics and fluoroelastomers that contain perfluoroalkoxy groups shall be avoided and,  if  not  possible, reduced as  far  as  technically and  practically possible. This  derogation  shall not  apply to  articles referred to  in paragraph 2(c).  The  Commission shall  review this  derogation  no  later than 25 August 2024.\n\n11.The concentration limit referred to in paragraph 2 shall be 1  000ppb for the sum of C9-C14 PFCAs, where these are present in PTFE micro powders produced by ionising irradiation or by thermal degradation, as  well  as  in  mixtures and  articles for  industrial  and professional uses containing PTFE micro powders. All emissions of C9-C14 PFCAs  during  the  manufacture and  use  of  PTFE micro powders shall be  avoided and,  if  not  possible, reduced as  far  as technically and  practically possible. The  Commission shall review this derogation no later than 25 August 2024.\n\n12.For the purposes of this entry, C9-C14 PFCA-related substances are  substances that, based on  their molecular structure, are considered to  have  the  potential  to degrade or  be  transformed  to C9-C14 PFCAs.’\n"},null,{"$f":"Translator!$B$2791","v":"25 ppb for single substance, sum value 260 ppb"},null,null,null,null,null,null,"C2021"]
[{"$f":"Translator!B1675","v":"Methanol"},"67-56-1",69,"P",{"$f":"Translator!B1729","v":"Shall not be placed on the market to the general public after 9 May 2019 in windscreen washing or defrosting fluids, in a concentration equal to or greater than 0,6 % by weight."},null,{"$f":"Translator!$B$1748","v":"0,6 % by weight"},null,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B1676","v":"Octamethylcyclotetrasiloxane (D4); \nDecamethylcyclopentasiloxane (D5)"},"556-67-2\n541-02-6",70,"P",{"$f":"Translator!B1730","v":"1. Shall not be placed on the market in wash-off cosmetic products in a concentration equal to or greater than 0,1 % by weight of either substance, after 31 January 2020.\n2. For the purposes of this entry, “wash-off cosmetic products” means cosmetic products as defined in Article 2(1)(a) of Regulation (EC) No 12"},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B1677","v":"1-methyl-2-pyrrolidone"},"872-50-4",71,"P",{"$f":"Translator!B1731","v":"1. Shall not be placed on the market as a substance on its own or in mixtures in a concentration equal to or greater than 0,3 % after 9 May 2020 unless manufacturers, importers and downstream users have included in the relevant chemical safety reports and safety data sheets, Derived No-Effect Levels (DNELs) relating to exposure of workers of 14,4 mg/m3 for exposure by inhalation and 4,8 mg/kg/day for dermal exposure.\n2. Shall not be manufactured, or used, as a substance on its own or in mixtures in a concentration equal to or greater than 0,3 % after 9 May 2020 unless manufacturers and downstream users take the appropriate risk management measures and provide the appropriate operational conditions to ensure that exposure of workers is below the DNELs specified in paragraph 1.\n3. By way of derogation from paragraphs 1 and 2, the obligations laid down therein shall apply from 9 May 2024 in relation to placing on the market for use, or use, as a solvent or reactant in the process of coating wires."},null,{"$f":"Translator!$B$1747","v":"0,3 % by weight"},null,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B1678","v":"The following substances which are classified as carcinogenic, mutagenic or toxic for reproduction, category 1A or 1B (See group members)"},"-",72,"P",{"$f":"Translator!B1732","v":"1. Shall not be placed on the market after 1 November 2020 in any of the following:\n(a) clothing or related accessories;\n(b) textiles other than clothing which, under normal or reasonably foreseeable conditions of use, come into contact with human skin to an extent similar to clothing;\n(c) footwear;\nif the clothing, related accessory, textile other than clothing or footwear is for use by consumers and the substance is present in a concentration, measured in homogeneous material, equal to or greater than that specified for that substance in Appendix 12.\n2. By way of derogation, in relation to the placing on the market of formaldehyde [CAS No 50-00-0] in jackets, coats or upholstery, the relevant concentration for the purposes of paragraph 1 shall be 300 mg/kg during the period between 1 November 2020 and 1 November 2023. The concentration specified in Appendix 12 shall apply thereafter.\n3. Paragraph 1 shall not apply to:\n(a) clothing, related accessories or footwear, or parts of clothing, related accessories or footwear, made exclusively of natural leather, fur or hide;\n(b) non-textile fasteners and non-textile decorative attachments;\n(c) second-hand clothing, related accessories, textiles other than clothing or footwear\n(d) wall-to-wall carpets and textile floor coverings for indoor use, rugs and runners.\n4. Paragraph 1 shall not apply to clothing, related accessories, textiles other than clothing, or footwear within the scope of Regulation (EU) 2016/425 of the European Parliament\nand of the Council1 or Regulation (EU) 2017/745 of the European Parliament and of the Council2.\n5. Paragraph 1(b) shall not apply to disposable textiles. ‘Disposable textiles’ means textiles that are designed to be used only once or for a limited time and are not intended for subsequent use for the same or a similar purpose.\n6. Paragraphs 1 and 2 shall apply without prejudice to the application of any stricter restrictions set out in this Annex or in other applicable Union legislation.\n7. The Commission shall review the exemption in paragraph 3(d) and, if appropriate, modify that point accordingly."},null,{"$f":"Translator!$B$1751","v":"3 % by weight"},null,null,null,null,null,null,"E2020"]
[{"$f":"Translator!B1679","v":"(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silanetriol and any of its mono-, di- or tri-O-(alkyl) derivatives"},"-",73,"P",{"$f":"Translator!B1733","v":"1. Shall not be placed on the market for supply to the general public after 2 January 2021 individually or in any combination, in a concentration equal to or greater than 2 ppb by weight of the mixtures containing organic solvents, in spray products.\n2. For the purpose of this entry, “spray products” means aerosol dispensers, pump sprays, trigger sprays, marketed for proofing or impregnation spray applications.\n3. Without prejudice to the implementation of other Union provisions concerning the classification, packaging and labelling of substances and mixtures, the packaging of spray products containing (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) silanetriol and/or TDFAs combined with organic solvents as referred to in paragraph 1 and placed on the market for professional use shall be marked clearly and indelibly: “for professional users only” and “Fatal if inhaled” with the pictogram GHS06.\n4. Section 2.3 of Safety Data Sheets shall contain the following information: “mixtures of (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) silanetriol and/or any of its mono-, di- or tri-O-(alkyl) derivatives in a concentration equal to or greater than 2 ppb and organic solvents in spray products, are for professional users only and marked ‘Fatal if inhaled’”.\n5. Organic solvents referred to in paragraph 1, 3, and 4 include organic solvents used as aerosol propellants."},null,{"$f":"Translator!$B$1750","v":"2 ppb"},null,null,null,null,null,null,"E2020"]
[{"$f":"Translator!B1680","v":"Diisocyanates"},"-",74,"P",{"$f":"Translator!B1734","v":"1. Shall not be used as substances on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) after 24 August 2023, unless:\n(a) the concentration of diisocyanates individually and in combination is less than 0,1 % by weight, or\n(b) the employer or self-employed ensures that industrial or professional user(s) have successfully completed training on the safe use of diisocyanates prior to the use of the substance(s) or mixture(s).\n2. Shall not be placed on the market as substances on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) after 24 February 2022, unless:\n(a) the concentration of diisocyanates individually and in combination is less than 0,1 % by weight, or\n(b) the supplier ensures that the recipient of the substance(s) or mixture(s) is provided with information on the requirements referred to in point (b) of paragraph 1 and the following statement is placed on the packaging, in a manner that is visibly distinct from the rest of the label information: “As from 24 August 2023 adequate training is required before industrial or professional use”.\n3. For the purpose of this entry “industrial and professional user(s)” means any worker or self-employed worker handling diisocyanates on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) or supervising these tasks.\n4. The training referred to in point (b) of paragraph 1 shall include the instructions for the control of dermal and inhalation exposure to diisocyanates at the workplace without prejudice to any national occupational exposure limit value or other appropriate risk management measures at national level. Such training shall be conducted by an expert on occupational safety and health with competence acquired by relevant vocational training. That training shall cover as a minimum:\n(a) the training elements in point (a) of paragraph 5 for all industrial and professional use(s).\n(b) the training elements in points (a) and (b) of paragraph 5 for the following uses:\n— handling open mixtures at ambient temperature (including foam tunnels);\n— spraying in a ventilated booth;\n— application by roller;\n— application by brush;\n— application by dipping and pouring;\n— mechanical post treatment (e.g. cutting) of not fully cured articles which are not warm anymore;\n— cleaning and waste;\n— any other uses with similar exposure through the dermal and/or inhalation route;\n(c) the training elements in points (a), (b) and (c) of paragraph 5 for the following uses:\n— handling incompletely cured articles (e.g. freshly cured, still warm);\n— foundry applications;\n— maintenance and repair that needs access to equipment;\n— open handling of warm or hot formulations (> 45 °C);\n— spraying in open air, with limited or only natural ventilation (includes large industry working halls) and spraying with high energy (e.g. foams, elastomers);\n— and any other uses with similar exposure through the dermal and/or inhalation route.\n5. Training elements:\n(a) general training, including on-line training, on:\n— chemistry of diisocyanates;\n— toxicity hazards (including acute toxicity);\n— exposure to diisocyanates;\n— occupational exposure limit values;\n— how sensitisation can develop;\n— odour as indication of hazard;\n— importance of volatility for risk;\n— viscosity, temperature, and molecular weight of diisocyanates;\n— personal hygiene;\n— personal protective equipment needed, including practical instructions for its correct use and its limitations;\n— risk of dermal contact and inhalation exposure;\n— risk in relation to application process used;\n— skin and inhalation protection scheme;\n— ventilation;\n— cleaning, leakages, maintenance;\n— discarding empty packaging;\n— protection of bystanders;\n— identification of critical handling stages;\n— specific national code systems (if applicable);\n— behaviour-based safety;\n— certification or documented proof that training has been successfully completed\n(b) intermediate level training, including on-line training, on:\n— additional behaviour-based aspects;\n— maintenance;\n— management of change;\n— evaluation of existing safety instructions;\n— risk in relation to application process used;\n— certification or documented proof that training has been successfully completed\n(c) advanced training, including on-line training, on:\n— any additional certification needed for the specific uses covered;\n— spraying outside a spraying booth;\n— open handling of hot or warm formulations (> 45 °C);\n— certification or documented proof that training has been successfully completed\n6. The training shall comply with the provisions set by the Member State in which the industrial or professional user(s) operate. Member States may implement or continue to apply their own national requirements for the use of the substance(s) or mixture(s), as long as the minimum requirements set out in paragraphs 4 and 5 are met.\n7. The supplier referred to in point (b) of paragraph 2 shall ensure that the recipient is provided with training material and courses pursuant to paragraphs 4 and 5 in the official language(s) of the Member State(s) where the substance(s) or mixture(s) are supplied. The training shall take into consideration the specificity of the products supplied, including composition, packaging, and design.\n8. The employer or self-employed shall document the successful completion of the training referred to in paragraphs 4 and 5. The training shall be renewed at least every five years.\n9. Member States shall include in their reports pursuant to Article 117(1) the following information:\n(a) any established training requirements and other risk management measures related to the industrial and professional uses of diisocyanates foreseen in national law;\n(b) the number of cases of reported and recognised occupational asthma and occupational respiratory and dermal diseases in relation to diisocyanates;\n(c) national exposure limits for diisocyanates, if there are any;\n(d) information about enforcement activities related to this restriction.\n10. This restriction shall apply without prejudice to other Union legislation on the protection of safety and health of workers at the workplace."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E2021"]
[{"$f":"Translator!B2850","v":"N,N-Dimethylformamid"},"-",76,"P",{"$f":"Translator!B2851","v":"1. Shall not be placed on the market as a substance on its own, as a constituent of other\nsubstances, or in mixtures in a concentration equal to or greater than 0,3 % after 12\nDecember 2023 unless manufacturers, importers and downstream users have included in\nthe relevant chemical safety reports and safety data sheets, Derived No-Effect Levels\n(DNELs) relating to exposure of workers of 6 mg/m 3 for exposure by inhalation and 1,1\nmg/kg/day for dermal exposure.\n2. Shall not be manufactured, or used, as a substance on its own, as a constituent of other\nsubstances, or in mixtures in a concentration equal to or greater than 0,3 % after 12\nDecember 2023 unless manufacturers and downstream users take the appropriate risk\nmanagement measures and provide the appropriate operational conditions to ensure that\nexposure of workers is below the DNELs specified in paragraph 1.\n3. By way of derogation from paragraphs 1 and 2, the obligations laid down therein shall\napply from 12 December 2024 in relation to placing on the market for use, or use, as a\nsolvent in direct or transfer polyurethane coating processes of textiles and paper material or\nthe production of polyurethane membranes, and from 12 December 2025 in relation to\nplacing on the market for use, or use, as a solvent in the dry and wet spinning processes of\nsynthetic fibres."},null,{"$f":"Translator!$B$1747","v":"0,3 % by weight"},null,null,null,null,null,null,"E2023"]
[{"$f":"Translator!B3803","v":"Formaldehyde\nCAS-Nr. 50-00-0\nEG-Nr. 200-001-8 \nand formaldehyde releasing substances\n "},"50-0-00",77,"P",{"$f":"Translator!B3805","v":"1. Shall not be placed on the market in articles, after 6 August 2026, if, under the test\nconditions specified in Appendix 14, the concentration of formaldehyde released from those\narticles exceeds:\n(a) 0,062 mg/m3 for furniture and wood-based articles;\n(b) 0,080 mg/m3 for articles other than furniture and wood-based articles.\nThe first subparagraph shall not apply to:\n(a) articles in which formaldehyde or formaldehyde releasing substances are exclusively\nnaturally present in the materials from which the articles are produced;\n(b) articles that are exclusively for outdoor use under foreseeable conditions;\n(c) articles in constructions, that are exclusively used outside the building shell and\nvapour barrier and that do not emit formaldehyde into indoor air;\n(d) articles exclusively for industrial or professional use unless formaldehyde released\nfrom them leads to exposure of the general public under foreseeable conditions of use;\n(e) articles for which the restriction laid down in entry 72 applies;\n(f) articles that are biocidal products within the scope of Regulation (EU) No 528/2012 of\nthe European Parliament and of the Council1;\n(g) devices within the scope of Regulation (EU) 2017/745;\n(h) personal protective equipment within the scope of Regulation (EU) 2016/425;\n(i) articles intended to come into contact directly or indirectly with food within the scope\nof Regulation (EC) No 1935/2004;\n(j) second-hand articles.\n2. Shall not be placed on the market in road vehicles after 6 August 2027 if, under the test\nconditions specified in Appendix 14, the concentration of formaldehyde in the interior of\nthose vehicles exceeds 0,062 mg/m3\n.\nThe first subparagraph shall not apply to:\n(a) road vehicles exclusively for industrial or professional use unless the concentration of\nformaldehyde in the interior of those vehicles leads to exposure of the general public\nunder foreseeable conditions of use;\n(b) second-hand vehicles."},null,{"$f":"Translator!$B$3807","v":"a) 0,062 mg/m3 for furniture and wood-based articles;\n(b) 0,080 mg/m3 for articles other than furniture and wood-based articles"},null,null,null,null,null,null,"E 2024"]
[{"$f":"Translator!B3804","v":"Synthetic polymer microparticles:\npolymers that are solid and which fulfil both of the following conditions:\n(a) are contained in particles and constitute at least 1 % by weight of those particles; or\nbuild a continuous surface coating on particles;\n(b) at least 1 % by weight of the particles referred to in point (a) fulfil either of the\nfollowing conditions:\n(i) all dimensions of the particles are equal to or less than 5 mm;\n(ii) the length of the particles is equal to or less than 15 mm and their length to\ndiameter ratio is greater than 3.\nThe following polymers are excluded from this designation:\n(a) polymers that are the result of a polymerisation process that has taken place in\nnature, independently of the process through which they have been extracted, which are\nnot chemically modified substances;\n(b) polymers that are degradable as proved in accordance with Appendix 15;\n(c) polymers that have a solubility greater than 2 g/L as proved in accordance with\nAppendix 16;\n(d) polymers that do not contain carbon atoms in their chemical structure."},"-",78,"P",{"$f":"Translator!B3806","v":"1. Shall not be placed on the market as substances on their own or, where the synthetic\npolymer microparticles are present to confer a sought-after characteristic, in mixtures in a\nconcentration equal to or greater than 0,01 % by weight.\n2. For the purposes of this entry, the following definitions apply:\n(a) “particle” means a minute piece of matter, other than single molecules, with defined\nphysical boundaries;\n(b) “solid” means a substance or mixture other than a liquid or gas;\n(c) “gas” means a substance or mixture which at 50 °C has a vapour pressure greater\nthan 300 kPa (absolute), or is completely gaseous at 20 °C at a standard pressure of\n101,3 kPa;\n(d) “liquid” means a substance or mixture that meets any of the following conditions:\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\n(i) the substance or mixture at 50 °C has a vapour pressure of not more than 300 kPa,\nis not completely gaseous at 20 °C and at a standard pressure of 101,3 kPa, and has a\nmelting point or initial melting point of 20 °C or less at a standard pressure of 101,3\nkPa;\n(ii) the substance or mixture fulfils the criteria in the American Society for Testing and\nMaterials (ASTM) D 4359-90 Standard Test Method for Determining Whether a Material\nIs a Liquid or a Solid;\n(iii) the substance or mixture passes the fluidity test (penetrometer test) described in\nchapter 2.3.4 of Part 2 of Annex A to the European Agreement concerning the\nInternational Carriage of Dangerous Goods by Road (ADR) concluded at Geneva on 30\nSeptember 1957;\n(e) “make-up product” means any substance or mixture intended to be placed in contact\nwith specific external parts of the human body, namely the epidermis, eye brows and eye\nlashes, with a view to, exclusively or mainly, changing their appearance;\n3. Where the concentration of synthetic polymer microparticles covered by this entry cannot\nbe determined by available analytical methods or accompanying documentation, in order to\nverify the compliance with the concentration limit referred to in paragraph 1, only the\nparticles of at least the following size shall be taken into account:\n(a) 0,1 μm for any dimension, for particles where all dimensions are equal to or smaller\nthan 5 mm;\n(b) 0,3 μm in length, for particles that have a length that is equal to or smaller than 15\nmm and a length to diameter ratio greater than 3.\n4. Paragraph 1 shall not apply to the placing on the market of:\n(a) synthetic polymer microparticles, as substances on their own or in mixtures, for use\nat industrial sites;\n(b) medicinal products within the scope of Directive 2001/83/EC and veterinary medicinal\nproducts within the scope of Regulation (EU) 2019/6 of the European Parliament and of\nthe Council;\n(c) EU fertilising products within the scope of Regulation (EU) 2019/1009 of the European\nParliament and of the Council;\n(d) food additives within the scope of Regulation (EC) No 1333/2008 of the European\nParliament and of the Council;\n(e) in vitro diagnostic devices, including devices within the scope of Regulation (EU)\n2017/746 of the European Parliament and of the Council;\n(f) food within the meaning of Article 2 of Regulation (EC) No 178/2002, not covered by\npoint (d) of this paragraph, and feed as defined in Article 3(4) of that Regulation.\n5. Paragraph 1 shall not apply to the placing on the market of the following synthetic\npolymer microparticles, as substances on their own or in mixtures:\n(a) synthetic polymer microparticles which are contained by technical means so that\nreleases to the environment are prevented when used in accordance with the instructions\nfor use during the intended end use;\n(b) synthetic polymer microparticles the physical properties of which are permanently\nmodified during intended end use in such a way that the polymer no longer falls within\nthe scope of this entry;\n(c) synthetic polymer microparticles which are permanently incorporated into a solid\nmatrix during intended end use.\n6. Paragraph 1 shall apply as follows regarding the following uses:\n(a) from 17 October 2029 to synthetic polymer microparticles for use in the encapsulation\nof fragrances;\n(b) from 17 October 2027 for “rinse-off products” as defined in point (1)(a) of the\nPreamble to Annexes II to VI to Regulation (EC) No 1223/2009 unless such products are\ncovered by point (a) of this paragraph or contain synthetic polymer microparticles for use\nas an abrasive, i.e. namely to exfoliate, polish or clean (“microbeads”);\n(c) from 17 October 2035 for lip products as defined in point (1)(e) of the Preamble to\nAnnexes II to VI to Regulation (EC) No 1223/2009, nail products as defined in point\n(1)(g) of the Preamble to Annexes II to VI to that Regulation, and make-up products\nwithin the scope of that Regulation, unless such products are covered by points (a) or (b)\nof this paragraph or contain microbeads;\n(d) from 17 October 2029 for leave-on products, as defined in point (1)(b) of the\nPreamble to Annexes II to VI to Regulation (EC) No 1223/2009, unless such products are\ncovered by points (a) or (c) of this paragraph;\n(e) from 17 October 2028 for detergents, as defined in Article 2(1) of Regulation (EC) No\n648/2004, waxes, polishes and air care products, unless those products are covered by\npoint (a) of this paragraph or contain microbeads;\n(f) from 17 October 2029 for “devices”, within the scope of Regulation (EU) 2017/745 of\nthe European Parliament and of the Council, unless those devices contain microbeads;\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\n(g) from 17 October 2028 for “fertilising products”, as defined in Article 2, point (1), of\nRegulation (EU) 2019/1009, which do not fall within the scope of that Regulation;\n(h) from 17 October 2031 for plant protection products within the meaning of Article 2(1)\nof Regulation (EC) No 1107/2009 of the European Parliament and of the Council6 and\nseeds treated with those products, and biocidal products as defined in Article 3(1), point\n(a), of Regulation (EU) No 528/2012 of the European Parliament and of the Council7;\n(i) from 17 October 2028 for products for agricultural and horticultural uses not covered\nby points (g) or (h);\n(j) from 17 October 2031 for granular infill for use on synthetic sports surfaces.\n7. From 17 October 2025 suppliers of synthetic polymer microparticles referred to in\nparagraph 4, point (a), shall provide the following information:\n(a) instructions for use and disposal explaining to industrial downstream users how to\nprevent releases of synthetic polymer microparticles to the environment;\n(b) the following statement:\n“The synthetic polymer microparticles supplied is subject to conditions laid down by\nentry 78 of Annex XVII to Regulation (EC) No 1907/2006 of the European Parliament\nand of the Council”;\n(c) the information on quantity or, as applicable, concentration of synthetic polymer\nmicroparticles in the substance or mixture;\n(d) generic information on the identity of the polymers contained in the substance or\nmixture that enables manufacturers, industrial downstream users and other suppliers to\ncomply with their obligations laid down in paragraphs 11 and 12.\n8. From 17 October 2026 suppliers of products containing synthetic polymer microparticles\nreferred to in paragraph 4, point (e), and from 17 October 2025 suppliers of products\ncontaining synthetic polymer microparticles referred to in paragraph 4, point (d), and\nparagraph 5, shall provide instructions for use and disposal explaining to professional users\nand the general public how to prevent releases of synthetic polymer microparticles to the\nenvironment.\n9. From 17 October 2031 until 16 October 2035 suppliers of products referred to in\nparagraph 6, point (c), containing synthetic polymer microparticles shall provide the\nfollowing statement: “This product contains microplastics.” However, products placed on the\nmarket before 17 October 2031 are not required to bear that statement until 17 December\n2031.\n10. The information referred to in paragraphs 7, 8 and 9 shall be provided in the form of\nclearly visible, legible and indelible text or, where appropriate regarding the information in\nparagraphs 7 and 8, in the form of pictograms. The text or pictograms shall be placed on the\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\nlabel, the packaging, or the package leaflet of the products containing synthetic polymer\nmicroparticles or, regarding the information in paragraph 7, on the safety data sheet. In\naddition to the text or pictograms, suppliers may provide a digital tool that gives access to\nan electronic version of that information. Where instructions for use and disposal are\nprovided in accordance with paragraphs 7, 8 and 9 in the form of a text, they shall be in the\nofficial languages of the Member States where the substance or mixture is placed on the\nmarket, unless the Member States concerned provide otherwise.\n11. Starting from 2026 manufacturers and industrial downstream users of synthetic polymer\nmicroparticles in the form of pellets, flakes, and powders used as feedstock in plastic\nmanufacturing at industrial sites, and, starting from 2027, other manufacturers of synthetic\npolymer microparticles and other industrial downstream users using synthetic polymer\nmicroparticles at industrial sites shall submit the following information to the Agency by 31\nMay of each year:\n(a) a description of the uses of synthetic polymer microparticles in the previous calendar\nyear;\n(b) for each use of synthetic polymer microparticles, generic information on the identity\nof the polymers used;\n(c) for each use of synthetic polymer microparticles, an estimate of the quantity of\nsynthetic polymer microparticles released to the environment in the previous calendar\nyear, which shall include also the quantity of synthetic polymer microparticles released to\nthe environment during transportation.\n(d) for each use of synthetic polymer microparticles, a reference to the derogation laid\ndown in paragraph 4, point (a).\n12. From 2027, suppliers of products containing synthetic polymer microparticles refe rred to\nin paragraphs 4, points (b), (d) and (e), and paragraph 5, placed on the market for the first\ntime to professional users and the general public, shall submit the following information to\nthe Agency by 31 May of each year:\n(a) a description of the end uses for which the synthetic polymer microparticles were\nplaced on the market in the previous calendar year;\n(b) for each end use for which the synthetic polymer microparticles were placed on the\nmarket, generic information on the identity of the polymers placed on the market in the\nprevious calendar year;\n(c) for each end use for which the synthetic polymer microparticles were placed on the\nmarket, an estimate of the quantity of synthetic polymer microparticles released to the\nenvironment in the previous calendar year, which shall include also the quantity of\nsynthetic polymer microparticles released to the environment during transportation.\n(d) for each use of synthetic polymer microparticles, a reference to the applicable\nderogation or derogations laid down in paragraph 4, point (b), (d) or (e), or 5 point (a),\n(b) or (c).\n13. The Agency shall make the information submitted under paragraphs 11 and 12 available\nto the Member States.\n14. Manufacturers, importers and industrial downstream users of products containing\nsynthetic polymer microparticles shall provide specific information on the identity of\npolymers covered by this entry contained in those products and the function of those\npolymers in the products to competent authorities upon their request. The specific\ninformation on the polymer identity shall be sufficient to unequivocally identify polymers and\nshall at least include the information laid down in points 2.1 to 2.2.3 and points 2.3.5, 2.3.6\nand 2.3.7 of Annex VI, where applicable. If the information is not available to industrial\ndownstream users, they shall request it from their supplier within 7 days from the receipt of\nthe request from the competent authorities and shall inform the authorities of the request\nmade without delay. Having received the request referred to in the second subparagraph,\nthe suppliers shall provide the requested information within 30 days to the industrial\ndownstream user or directly to the competent authority requesting it. Where the supplier\nprovides the information to the industrial downstream user, the industrial downstream user\nshall forward that information to the competent authorities without delay. Where the\nsupplier provides the information directly to the authority, it shall without delay inform the\nindustrial downstream user concerned to that effect.\n15. Manufacturers, importers and industrial downstream users of products containing\npolymers claimed to be excluded from the designation of synthetic polymer microparticles on\ngrounds of degradability or solubility shall provide, without delay, information proving that\nthose polymers are degradable in accordance with Appendix 15 or soluble in accordance with\nAppendix 16, as applicable, to competent authorities upon their request.\n16. Paragraph 1 shall not apply to placing on the market of synthetic polymers\nmicroparticles, on their own or in mixtures, placed on the market before 17 October 2023.\nHowever, the first subparagraph shall not apply to the placing on the market of synthetic\npolymers microparticles for uses listed in paragraph 6."},null,{"$f":"Translator!$B$1744","v":"0,1 % by weight"},null,null,null,null,null,null,"E 2024"]
[{"$f":"Translator!B1753","v":"Regulated Substance"},{"$f":"Translator!B1754","v":"CAS No."},{"$f":"Translator!B1755","v":"Date of inclusion"},null,{"$f":"Translator!B1756","v":"Restriction conditions; to see more text please press \"Show extract\""},{"$f":"Translator!B1757","v":"Examples occurence"},{"$f":"Translator!B1758","v":"Annex XIV requirements"},null,null,{"$f":"Translator!B1759","v":"SCIP-ID"},{"$f":"Translator!B1760","v":"Concentration (specify unit)"},{"$f":"Translator!B1761","v":"Part name of the specific part (in case of complex parts), regulated substance is contained."},{"$f":"Translator!B1762","v":"TARIC Code "},{"$f":"Translator!B1763","v":"Comments"},{"$f":"Translator!B1764","v":"Entry included (E), changed (C)"},"Listed Substance","Listed Substance  Name","Listed Substance Group","Listed Substance Group Name"]
[{"$f":"Translator!B1529","v":"Substances rated declarable (D)\nEU-REACH SVHC Candidate List.\nBased on the EuGH Court decision from 10.9.2015: The concentration has to be determined for each partial product and to be declared for each partial product if above  0,1 mass fraction (w/w)."}]
[{"$f":"Translator!B1766","v":"Triethyl arsenate"},"15606-95-8","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2490","v":"Triethyl arsenate is used, among other things, in semiconductor production."},null,null,null,100102611,null,null,null,null,null,"L00000000001","triethyl arsenate"]
[{"$f":"Translator!B1767","v":"Sodium dichromate\ndihydrat and anhydrid"},"7789-12-0\n10588-01-9","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2491","v":"Applications for sodium dichromates include the production of vitamin K, colour stains (wood preservatives), the production of essential oils and perfumes, the production of coloured glass and ceramic glazes, the production of other chromium compounds, the production of inorganic chromate pigments and anti-corrosion coatings for metals. "},{"$f":"Translator!B2172","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},null,null,100031070,null,null,null,null,"E2009","L00000000066","Sodium-dichromate"]
[{"$f":"Translator!B1768","v":"Diarsenic Pentaoxide"},"1303-28-2","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2492","v":"Diarsenic Pentaoxide is used as a decolorizing agent for glass and enamel, as a refining and oxidizing agent in the production of special glass and lead crystal, as a starting material for elemental arsenic, arsenic alloys and arsenic-containing semiconductors and as a cytostatic agent. The material is also used in metallurgical investigations. "},{"$f":"Translator!B2369","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015"},null,null,100013743,null,null,null,null,"E2009","L00000000006","Arsenic pentoxide"]
[{"$f":"Translator!B1769","v":"Diarsenic Trioxide"},"1327-53-3","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2493","v":"Diarsene trioxide is used as a decolorizing agent for glass and enamel, as a refining and oxidizing agent in the production of special glass and lead crystal, as a starting material for elemental arsenic, arsenic alloys and arsenic-containing semiconductors and as a cytostatic agent. The material is also used in metallurgical investigations. "},{"$f":"Translator!B2369","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015"},null,null,100014075,null,null,null,null,"E2009","L00000000007","Arsenic trioxide"]
[{"$f":"Translator!B1770","v":"Dibutyl phthalate (DBP)"},"84-74-2","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2494","v":"Dibutyl phthalate is used in cosmetic products (e.g. nail polish), in adhesives, in cellophane packaging for food and in children's toys."},{"$f":"Translator!B2370","v":"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n"},null,null,100001416,null,null,null,null,"E2009,C2011","L00000000004","dibutyl phthalate"]
[{"$f":"Translator!B1771","v":"Bis(tributyltin) oxide (TBTO)"},"56-35-9","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2495","v":"Bis(tributyltin) oxide is used in antimicrobial products such as special paints, special coatings, polyurethane foams, upholstered furniture, down or special textiles. "},null,null,null,100000244,null,null,null,null,"E2009,C2011","L00000000011","Bis(tributyltin) oxide"]
[{"$f":"Translator!B1772","v":"Lead hydrogen arsenate"},"7784-40-9","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2496","v":"Lead hydrogen arsenate has been used as a biocide in the past. Today, the material is used in the production of glass, plastic products, lead batteries, electrical appliances, paints, mortars, electronic products, fertilizers, cosmetics and textiles. "},null,null,null,100029149,null,null,null,null,"E2009","L00000000012","Arsenic acid (H3AsO4), lead(2+) salt (1:1)"]
[{"$f":"Translator!B1773","v":"Anthracene"},"120-12-7","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2497","v":"The use of anthracene in the EU is restricted to the manufacture of pyrotechnic and pharmaceutical products and to its use for research purposes. "},null,null,null,100003974,null,null,null,null,"E2009","L00000000002","anthracene"]
[{"$f":"Translator!B1774","v":"Benzyl butyl phthalate (BBP)"},"85-68-7","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2498","v":"Benzyl butyl phthalate is used as a plasticizer for PVC and other polymers to improve extensibility and mobility. It is used for floor coverings, but also for sealants, adhesives, paints, coatings and inks. Consumer products such as sealants, adhesives, car care products, food packaging materials and cosmetics may contain benzyl butyl phthalate. "},{"$f":"Translator!B2370","v":"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n"},null,null,100001475,null,null,null,null,"E2009, C2011","L00000000013","Butylbenzylphthalate"]
[{"$f":"Translator!B1775","v":"4,4’-Diaminodiphenylmethan (MDA)"},"101-77-9","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2499","v":"MDA is used as an amine component in two-component systems."},{"$f":"Translator!B2371","v":"included in Annex 14\n- \nlast application date: \n21. Februar 2013\n- \nsunset date:\n21. August 2014"},null,null,100002705,null,null,null,null,"E2009, C2011","L00000000003","4,4'-Methylenedianiline"]
[{"$f":"Translator!B1776","v":"5-tert-butyl-2,4,6-trinitro-m-xylene (musk xylene)"},"81-15-2","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2500","v":"Musk xylene is used in cosmetic products and detergents as a fragrance or scent enhancer. "},{"$f":"Translator!B2371","v":"included in Annex 14\n- \nlast application date: \n21. Februar 2013\n- \nsunset date:\n21. August 2014"},null,null,100001210,null,null,null,null,"E2009, C2011","L00000000008","5-tert-Butyl-2,4,6-trinitro-m-xylene"]
[{"$f":"Translator!B1777","v":"Alkanes, C10-13, chloro (Short Chain Chlorinated Paraffins)"},"85535-84-8","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2501","v":"Alkanes, C10-13, chloro are used in the production of rubber products, textile coatings, sealants, adhesives and paints."},null,null,null,100079496,null,null,null,null,"E2009, C 2023","L00000000010","Alkanes, C10-13, chloro"]
[{"$f":"Translator!B1778","v":"Hexabromocyclododecane (HBCDD) and all major diastereoisomeric identified compounds: "},"-","2008-10-28","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2502","v":"Hexabromocyclodododecane is used in the production of styrene-containing polymers and in the textile industry due to its flame-retardant properties. These flame-retardant polymers are mainly used as insulating material, packaging material and in electrical appliances. Textiles coated with HBCDD can be found, for example, in car interiors, mattresses, upholstered furniture, curtains, roller blinds and wallpaper."},{"$f":"Translator!B2372","v":"included in Annex 14\n- \nlast application date:\n21. Februar 2014\n- \nsunset date:\n21. August 2015"},null,null,"100.239.157\n\n\n\n\n",null,null,null,null,"E2009, C2011",null,null,"Y00000001083","Hexabromocyclododecane (HBCDD)"]
[{"$f":"Translator!B1779","v":"Hexabromocyclododecane"},"25637-99-4",null,"D",null,null,null,null,null,"100.042.848",null,null,null,null,null,"Y00000001083","Hexabromocyclododecane","Y00000001083","Hexabromocyclododecane (HBCDD)"]
[{"$f":"Translator!B1780","v":"1,2,5,6,9,10-hexabromocyclododecane"},"3194-55-6",null,"D",null,null,null,null,null,"100.019.724",null,null,null,null,null,"Y00000001083","1,2,5,6,9,10-Hexabromocyclododecane","Y00000001083","Hexabromocyclododecane (HBCDD)"]
[{"$f":"Translator!B1781","v":"alpha-hexabromocyclododecane"},"134237-50-6",null,"D",null,null,null,null,null,100131125,null,null,null,null,null,"Y00000001083","Cyclododecane, 1,2,5,6,9,10-hexabromo-, (1R,2R,5S,6R,9R,10S)-rel-","Y00000001083","Hexabromocyclododecane (HBCDD)"]
[{"$f":"Translator!B1782","v":"beta-hexabromocyclododecane"},"134237-51-7",null,"D",null,null,null,null,null,100131015,null,null,null,null,null,"Y00000001083","Cyclododecane, 1,2,5,6,9,10-hexabromo-, (1R,2S,5R,6R,9R,10S)-rel-","Y00000001083","Hexabromocyclododecane (HBCDD)"]
[{"$f":"Translator!B1783","v":"gamma-hexabromocyclododecane"},"134237-52-8",null,"D",null,null,null,null,null,100130841,null,null,null,null,null,"Y00000001083","gamma-Hexabromocyclododecane","Y00000001083","Hexabromocyclododecane (HBCDD)"]
[{"$f":"Translator!B1784","v":"Tris (2-chloroethyl) phosphate"},"115-96-8","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2503","v":"Tris(2-chloroethyl)phosphate is mainly used as a softener additive and viscosity regulator with flame retardant properties for acrylic resins, polyurethane, polyvinyl chloride and other polymers. Other applications include adhesives, coatings, fire resistant paints and lacquers. The main industries using TCEP are the furniture, textile and construction industries."},{"$f":"Translator!B2372","v":"included in Annex 14\n- \nlast application date:\n21. Februar 2014\n- \nsunset date:\n21. August 2015"},null,null,100003744,null,null,null,null,"E2010","L00000000025","Tris(2-chloroethyl) phosphate"]
[{"$f":"Translator!B1785","v":"Coal tar pitch, high temperature"},"65996-93-2","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2504","v":"Coal tar pitch, high temperature is mainly used in the production of electrodes for industrial applications. Smaller quantities are intended for specific applications such as high performance corrosion protection, special purpose paving, production of other materials and the production of clay targets."},{"$f":"Translator!B2373","v":"included in Annex 14\n- \nlast application date: 4. April 2019\n- \nsunset date: 4. Oktober 2020"},null,null,"100.060.007\n",null,null,null,null,"E2010","L00000000024","Pitch, coal tar, high-temp."]
[{"$f":"Translator!B1786","v":"Diisobutyl phthalate (DIBP)"},"84-69-5","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2505","v":"Diisobutyl phthalate is used both as a plasticizer for cellulose nitrate, cellulose ether, polyacrylate and polyacetate dispersions and as a gelling aid in combination with other plasticizers. Diisobutyl phthalate-containing polymers are used for plastics, paints, adhesives, explosives and nail polishes."},{"$f":"Translator!B2374","v":"included in Annex 14\n- \nlast application date: \n21. August 2013\n- \nsunset date:\n21. Februar 2015"},null,null,100001412,null,null,null,null,"E2010","L00000000020","Diisobutyl-phthalate"]
[{"$f":"Translator!B1787","v":"Lead sulfochromate yellow (C.I. Pigment Yellow 34)"},"1344-37-2","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2506","v":"Lead sulphochromate yellow (Colour Index Pigment Yellow 34) is used as a colouring, painting and coating material in industries such as the rubber, plastics and paint, coating and lacquer industry. Applications include the production of agricultural equipment, vehicles and aircraft as well as painting roads and take-off and landing strips. "},{"$f":"Translator!B2369","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015"},null,null,100014267,null,null,null,null,"E2010","L00000000023","Lead sulfochromate yellow"]
[{"$f":"Translator!B1788","v":"Lead chromate"},"7758-97-6","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2507","v":"Lead chromate is used for the production of pigments and dyes, as a pigmenting or coating material in industrial and marine paint products or for the embalming/reproduction of artificial products. Other potential uses include cleaning and bleaching agents, light-sensitive materials and for the production of pyrotechnic powders. "},{"$f":"Translator!B2369","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015"},null,null,100028951,null,null,null,null,"E2010","L00000000021","Lead chromate"]
[{"$f":"Translator!B1789","v":"Lead chromate molybdate sulfate red (C.I. Pigment Red 104)"},"12656-85-8","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2508","v":"Lead chromate molybdate sulphate red (Colour Index Pigment Red 104) is used as a dye, paint and coating material in industries such as the rubber, plastics and paint, coating and lacquer industry. Applications include the production of agricultural equipment, vehicles and aircraft as well as painting roads and take-off and landing strips. "},{"$f":"Translator!B2369","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015"},null,null,100032496,null,null,null,null,"E2010","L00000000022","Lead chromate molybdate sulfate red"]
[{"$f":"Translator!B1790","v":"2,4 - Dinitrotoluene (2,4-DNT)"},"121-14-2","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2509","v":"2,4-dinitrotoluene is used in the production of toluene diisocyanate, which is used in the manufacture of flexible polyurethane foams. The material is also used as a gelling plasticizer for the production of explosive mixtures (e.g. airbags in cars)."},{"$f":"Translator!B2372","v":"included in Annex 14\n- \nlast application date:\n21. Februar 2014\n- \nsunset date:\n21. August 2015"},null,null,100004046,null,null,null,null,"E2010","L00000000014","2,4-Dinitrotoluene"]
[{"$f":"Translator!B1791","v":"Anthracene oil, anthracene-low"},"90640-82-7","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2510","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},null,null,null,100084155,null,null,null,null,"E2010","L00000000019","Anthracene oil, anthracene-low"]
[{"$f":"Translator!B1792","v":"Anthracene oil, anthracene paste, anthracene  fraction\n"},"91995-15-2","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2511","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},null,null,null,100086576,null,null,null,null,"E2010","L00000000017","Anthracene oil, anthracene paste, anthracene fraction"]
[{"$f":"Translator!B1793","v":"Anthracene oil, anthracene paste, distn. Lights"},"91995-17-4","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2512","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},null,null,null,100086578,null,null,null,null,"E2010","L00000000018","Anthracene oil, anthracene paste, distn. lights"]
[{"$f":"Translator!B1794","v":"Anthracene oil, anthracene paste"},"90640-81-6","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2513","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},null,null,null,100084154,null,null,null,null,"E2010","L00000000016","Anthracene oil, anthracene paste"]
[{"$f":"Translator!B1795","v":"Anthracene oil"},"90640-80-5","2010-01-13","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2514","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},{"$f":"Translator!B2375","v":"included in Annex 14\n- \nlast application date: 4. April 2019\n- \nsunset date: 4. Oktober 2020"},null,null,100084153,null,null,null,null,"E2010","L00000000015","Anthracene Oil"]
[{"$f":"Translator!B1796","v":"Acrylamide"},"79-06-1","2010-03-30","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2515","v":"Acrylamide is used almost exclusively for the synthesis of polyacrylamides, which are then used in various applications, especially in waste water treatment and paper processing. Among the minor uses of acrylamide are the preparation of polyacrylamides for research purposes and their use as a cementing agent in civil engineering."},{"$f":"Translator!B2471","v":"included in Annex 17"},null,null,100001067,null,null,null,null,"E2010","L00000000026","Acrylamide"]
[{"$f":"Translator!B1797","v":"Tetraboron disodium heptaoxide, hydrate"},"12267-73-1","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2516","v":"Disodium tetraborate and tetrabic sodium heptaoxide form the same compounds in aqueous solution. Applications include a wide range of applications such as detergents, glass and glass fibers, ceramics, industrial fluids, metallurgy, adhesives, flame retardants, personal care products, biocides and fertilizers. "},null,null,null,100032298,null,null,null,null,"E2010","L00000000031","tetraboron disodium heptaoxide, hydrate"]
[{"$f":"Translator!B1798","v":"Trichloroethylene"},"79-01-6","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2517","v":"Trichloroethene is used in the production of organic chlorine and fluorine compounds. It is also used for cleaning and degreasing metal parts or as a solvent in adhesives. "},{"$f":"Translator!B2472","v":"included in Annex 14\n- \nlast application date: \n21. Oktober 2014\n- \nsunset date:  \n21. April 2016"},null,null,100001062,null,null,null,null,"E2010","L00000000032","Trichloroethylene"]
[{"$f":"Translator!B1799","v":"Sodium chromate"},"7775-11-3","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2518","v":"Sodium chromate is used, for example, in chromium metal production, in the production of chlorates, in the coating of metals, as an analytical agent in the laboratory and in tanning leather and paints. "},{"$f":"Translator!B2172","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},null,null,100028990,null,null,null,null,"E2010","L00000000030","Sodium chromate"]
[{"$f":"Translator!B1800","v":"Disodium tetraborate, anhydrous"},{"$f":"Translator!B1765","v":"1330-43-4, (anhydrous)\n12179-04-3, (pentahydrate)\n1303-96-4, (decahydrate)"},"2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2519","v":"Disodium tetraborate and tetrabic sodium heptaoxide form the same compounds in aqueous solution. Applications include a wide range of applications such as detergents, glass and glass fibers, ceramics, industrial fluids, metallurgy, adhesives, flame retardants, personal care products, biocides and fertilizers."},null,null,null,100014129,null,null,null,null,"E2010","L00000000079","Sodium borate, pentahydrate"]
[{"$f":"Translator!B1801","v":"Potassium chromate"},"7789-00-6","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2520","v":"Potassium chromate is used as a corrosion inhibitor in the treatment and coating of metals, for the production of reagents, chemicals and textiles, as a dye in the production of ceramics, glass and cement, in the production of pigments and inks and as an analytical agent in the laboratory. "},{"$f":"Translator!B2172","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},null,null,100029218,null,null,null,null,"E2010","L00000000028","Potassium-chromate"]
[{"$f":"Translator!B1802","v":"Potassium dichromate"},"7778-50-9","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2521","v":"Potassium dichromate is used for chromium metal production and as a corrosion inhibitor in the treatment and coating of metals. It is also used as a textile etchant, as an analytical agent in the laboratory, for cleaning laboratory glassware, in the manufacture of other reagents and as an oxidizing agent in photolithography."},{"$f":"Translator!B2172","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},null,null,100029005,null,null,null,null,"E2010","L00000000029","potassium dichromate"]
[{"$f":"Translator!B1803","v":"Boric acid"},"-","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2522","v":"Boric acid is used in a wide variety of applications due to its flame-retardant, antiseptic and preservative properties which influence consistency. It is used in detergents and cleaning agents, adhesives, toys, industrial fluids, brake fluids, glass, ceramics, flame retardants, paints, disinfectants, cosmetics, food additives, fertilizers, insecticides and other products."},null,null,null,"100.239.155\n",null,null,null,null,"E2010",null,null,"LG0000002930","boric acid"]
[{"$f":"Translator!B1804","v":"Boric acid"},"10043-35-3",null,"D",null,null,null,null,null,100030114,null,null,null,null,null,"LG0000002930","Boric acid","LG0000002930","boric acid"]
[{"$f":"Translator!B1805","v":"Boric acid, crude natural"},"11113-50-1",null,"D",null,null,null,null,null,100031209,null,null,null,null,null,"LG0000002930","Boric acid","LG0000002930","boric acid"]
[{"$f":"Translator!B1806","v":"Ammonium dichromate"},"  7789-09-5","2010-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2523","v":"Ammonium dichromate is mainly used as an oxidizing agent. Other well-known applications are in the manufacture of light-sensitive screens and as a pickling agent in the manufacture of textiles. Among the minor uses appear to be metal treatment and use as a laboratory analytical agent."},{"$f":"Translator!B2172","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},null,null,100029221,null,null,null,null,"E2010","L00000000027","Ammonium-dichromate"]
[{"$f":"Translator!B1807","v":"Acids generated from chromium trioxide and their oligomers [The group contains: Chromic acid, Chromic acid, Oligomers of chromic acid and dichromic acid]"},"-","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2524","v":"Acids generated from chromium trioxide and their oligomers are mainly used in metal finishing such as electroplating (e.g. hard chromium plating and decorative coating), conversion layers and brighteners. They are also used as fixing agents in water-based wood preservatives. Smaller uses can be found, for example, in the production of pigments and paints/lacquers, in the production of catalysts and cleaning agents and as oxidizing agents."},{"$f":"Translator!B2172","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},null,null,"100.239.153\n\n",null,null,null,null,"E2010",null,null,"LG0000005527","Acids generated from chromium trioxide and their oligomers"]
[{"$f":"Translator!B1808","v":"Chromic acid"},"7738-94-5",null,"D",null,null,null,null,null,100028910,null,null,null,null,null,"LG0000005527","Chromic-acid","LG0000005527","Acids generated from chromium trioxide and their oligomers"]
[{"$f":"Translator!B1809","v":"Oligomers of chromic acid and dichromic acid"},"-",null,"D",null,null,null,null,null,"100.239.160\n",null,null,null,null,null,null,null,"LG0000005527","Acids generated from chromium trioxide and their oligomers"]
[{"$f":"Translator!B1810","v":"Dichromic acid"},"13530-68-2",null,"D",null,null,null,null,null,100033513,null,null,null,null,null,"LG0000005527","Dichromic-acid","LG0000005527","Acids generated from chromium trioxide and their oligomers"]
[{"$f":"Translator!B1811","v":"Cobalt(II) diacetate"},"71-48-7","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2525","v":"Cobalt(II) diacetate is mainly used in the production of catalysts or as a catalyst. Lower uses include the production of other chemicals, including pigments, surface treatments, in alloys, dyes, rubber adhesion promoters and as feed additives."},null,null,null,"100.000.687\n",null,null,null,null,"E2010","L00000000039","Acetic acid, cobalt(2+) salt"]
[{"$f":"Translator!B1812","v":"Cobalt(II) dinitrate"},"10141-05-6","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2526","v":"Cobalt (II) dinitrate is mainly used in the production of other chemicals and in the production of catalysts. Other possible applications are surface treatment and batteries."},null,null,null,100030353,null,null,null,null,"E2010","L00000000040","Cobalt-dinitrate"]
[{"$f":"Translator!B1813","v":"Cobalt(II) carbonate"},"513-79-1","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2527","v":"Cobalt(II) carbonate is mainly used in the production of catalysts. Smaller uses can be found as feed additive, in the production of other chemicals, in the production of pigments and as adhesive in primer frits."},null,null,null,100007428,null,null,null,null,"E2010","L00000000038","Cobalt carbonate"]
[{"$f":"Translator!B1814","v":"Cobalt(II) sulphate"},"10124-43-3","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2528","v":"Cobalt(II) sulphate is mainly used in the manufacture of other chemicals and pigments and possibly catalysts and desiccants. Other applications include surface treatments (e.g. electroplating), corrosion protection, decolourisation (of glass and ceramic goods), in batteries, animal feed additives and soil fertilisers."},null,null,null,100030291,null,null,null,null,"E2010","L00000000041","Cobalt sulphate"]
[{"$f":"Translator!B1815","v":"Chromium trioxide"},"1333-82-0","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2529","v":"Chromium trioxide is mainly used in metal finishing such as electroplating (e.g. hard chromium plating and decorative coating), conversion coatings and brighteners. It is also used as a fixing agent in water-based wood preservatives. Smaller uses are, for example, in the production of pigments and paints/lacquers, in the production of catalysts and cleaning agents and as oxidizing agents."},{"$f":"Translator!B2473","v":"included in Annex 14\n- \nlast application date: \n21. März 2016\n- \nsunset date:  \n21. September 2017"},null,null,100014189,null,null,null,null,"E2010","L00000000037","Chromium-trioxide"]
[{"$f":"Translator!B1816","v":"2-Ethoxyethanol (ethylene glycol monoethyl ether; EGEE)"},"110-80-5","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2530","v":"2-Ethoxyethanol is mainly used as a chemical intermediate. It is less used as a solvent or laboratory chemical."},null,null,null,"100.003.459\n",null,null,null,null,"E2010","L00000000033","2-Ethoxyethanol"]
[{"$f":"Translator!B1817","v":"2-Methoxyethanol (ethylene glycol monomethyl ether; EGME)"},"109-86-4","2010-12-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2531","v":"2-Methoxyethanol is mainly used as a chemical intermediate. It is less used as a solvent or laboratory chemical. "},null,null,null,100003377,null,null,null,null,"E2010","L00000000034","2-Methoxyethanol"]
[{"$f":"Translator!B1818","v":"Strontium chromate"},"7789-06-2 \n","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2532","v":"Strontium chromate is mainly used as a corrosion inhibitor in coating mixtures used in the aerospace, steel and aluminum strip coating and automotive coating sectors."},{"$f":"Translator!B2474","v":"included in Annex 14\n- \nlast application date: 22. Juli 2017 \n- \nsunset date: 22. Januar 2019"},null,null,100029220,null,null,null,null,"E2011","L00000000043","Strontium chromate"]
[{"$f":"Translator!B1819","v":"Hydrazine"},"302-01-2\n7803-57-8","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2533","v":"Hydrazine is mainly used as an intermediate in the production of hydrazine derivatives, as a monomer in polymerisations, as a corrosion inhibitor in water treatment and for metal reduction and chemical refinement. Hydrazine is also used as fuel for spacecraft and as fuel for military (emergency) power units."},null,null,null,100005560,null,null,null,null,"E2011","L00000000081","Hydrazine"]
[{"$f":"Translator!B1820","v":"Cobalt dichloride\n\nCobalt dichloride was originally added to the candidate list as a SVHC substance on 28.10.2008. The entry was supplemented on 20.06.2011 by the reprotoxic properties."},"7646-79-9","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2534","v":"Cobalt dichloride is mainly used as an intermediate in the production of other cobalt compounds, in tire adhesion additives, organic textile dyes and drying agents for paints. It is also used in surface treatment processes, for example in water treatment / corrosion-inhibiting chemicals, as a colorant or for decolorizing in the production of inorganic pigments & frits, glass and ceramics, in varistors and magnets, and in moisture meters."},null,null,null,100028718,null,null,null,null,"E2009","L00000000005","Cobalt-dichloride"]
[{"$f":"Translator!B1821","v":"2-ethoxyethyl acetate (2-EEA)"},"111-15-9","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2535","v":"ECHA has not yet received registration for 2-ethoxyethyl acetate. It can therefore be concluded that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past, the substance was mainly used as a solvent in coatings and in the chemical industry, but also as an intermediate in the production of cyanoacrylate adhesives. "},null,null,null,100003491,null,null,null,null,"E2011","L00000000042","2-Ethoxyethyl acetate"]
[{"$f":"Translator!B1822","v":"1,2,3-trichloropropane"},"96-18-4","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2536","v":"1,2,3-trichloropropane is mainly used as an intermediate in the production of chlorinated solvents and agricultural products. It is also used as a monomer. In the past, 1,2,3-trichloropropane was used as solvent, paint and varnish remover and degreasing agent."},null,null,null,100002261,null,null,null,null,"E2011","L00000000046","1,2,3-Trichloropropane"]
[{"$f":"Translator!B1823","v":"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl esters, C7-rich"},"71888-89-6","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2537","v":"ECHA has not yet received registration for DIHP. Thus, it appears that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past, it was mainly used as a plasticizer in PVC and sealants, coatings and possibly in printing inks."},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,"100.069.214\n",null,null,null,null,"E2011","L00000000047","1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl esters, C7-rich"]
[{"$f":"Translator!B1824","v":"1,2-Benzenedicarboxylic acid, di-C7-11 -branched and linear alkyl esters\n(DHNUP)"},"68515-42-4","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2538","v":"ECHA has not yet received registration for DHNUP. Thus, it appears that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past it was mainly used as a plasticizer in PVC, foam, adhesives and coatings."},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,100064602,null,null,null,null,"E2011","L00000000044","1,2-Benzenedicarboxylic acid, di-C7-11-branched and linear alkyl esters"]
[{"$f":"Translator!B1825","v":"1-Methyl-2-pyrrolidon (NMP)"},"872-50-4","2011-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2539","v":"1-Methyl-2-pyrrolidon findet hauptsächlich Anwendung als Lösungsmittel in Beschichtungen, Reinigungsmitteln, für die Herstellung elektronischer Geräte sowie auch in der Halbleiterindustrie, bei der petrochemischen Verarbeitung, in Arzneimitteln und in Agrochemikalien. "},null,null,null,100011662,null,null,null,null,"E2011 / C 2023","L00000000045","1-Methyl-2-pyrrolidone"]
[{"$f":"Translator!B1826","v":"Trilead diarsenate"},"3687-31-8","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2540","v":"Trilead diarsenate is found in complex raw materials for the production of copper, lead and a number of precious metals. The trible diarsenate contained in the raw materials is converted into calcium arsenate and diarsene trioxide in the metallurgical refining process. While most of the calcium arsenate is apparently disposed of as waste, the diarsene trioxide is still used. "},null,null,null,100020890,null,null,null,null,"E2011","L00000000055","Trilead-diarsenate"]
[{"$f":"Translator!B1827","v":"Zirconia Aluminosilicate Refractory Ceramic Fibres\n\nRefractory zirconium-aluminosilicate ceramic fibres are fibres listed under index number 650-017-00-8 in Annex VI, Part 3, Table 3.1 of Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on the classification, labelling and packaging of substances and mixtures and meet the three following conditions:\n\na. The oxides of aluminium, silicon and zirconium are the main components that occur (in the fibres) in variable concentration ranges\n\nb. The fibres have a length-weighted mean geometric diameter minus twice the geometric standard deviation of 6 or less micrometers (µm)\n\nc. The content of alkali and alkaline earth metal oxides (Na2O+K2O+CaO+MgO+BaO) is less than or equal to 18% by weight."},"-","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2541","v":"Refractory ceramic fibres are used for high-temperature insulation, almost exclusively in industrial applications (insulation of industrial furnaces and equipment, equipment for the automotive and aerospace industries) and for fire protection (buildings and industrial process equipment)."},null,null,null,100239163,null,null,null,null,"E2010",null,null,"Y00000051438","Zirconia Aluminosilicate Refractory Ceramic Fibres"]
[{"$f":"Translator!B1828","v":"Aluminosilicate refractory ceramic fibres"},"142844-00-6",null,"D",null,null,null,null,null,"100.133.434\n",null,null,null,null,null,"Y00000051438","Refractory ceramic fibres","Y00000051438","Zirconia Aluminosilicate Refractory Ceramic Fibres"]
[{"$f":"Translator!B1829","v":"Phenolphthalein"},"77-09-8","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2542","v":"Phenolphthalein is mainly used for laboratory purposes (pH indicator solutions). It is less used in pharmaceutical preparations and in some special applications (e.g. pH indicator paper, invisible inks)."},null,null,null,100000914,null,null,null,null,"E2011","L00000000062","Phenolphthalein"]
[{"$f":"Translator!B1830","v":"Pentazinc chromate octahydroxide"},"49663-84-5","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2543","v":"Pentazinc chromate octahydroxide is mainly used in coatings for the automotive and aerospace industries."},{"$f":"Translator!B2474","v":"included in Annex 14\n- \nlast application date: 22. Juli 2017 \n- \nsunset date: 22. Januar 2019"},null,null,100051272,null,null,null,null,"E2011","L00000000057","Pentazinc chromate octahydroxide"]
[{"$f":"Translator!B1831","v":"Formaldehyde, oligomeric reaction products with aniline\ntechnical MDA"},"25214-70-4","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2544","v":"Technical MDA is mainly used in the production of other materials. Less use as ion exchange resins in nuclear power plants, as hardeners for epoxy resins, e.g. for the manufacture of rollers, pipes and moulds, and adhesives. "},{"$f":"Translator!B2476","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017"},null,null,"100.105.544\n",null,null,null,null,"E2011","L00000000058","Formaldehyde, polymer with benzenamine"]
[{"$f":"Translator!B1832","v":"Potassium hydroxyoctaoxodizincatedichromate(1-)"},"11103-86-9","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2545","v":"Potassium hydroxyoctaoxodizincatedichromate(1-) is mainly used in coatings in the aerospace industry as well as in the coating of steel and aluminium strips and vehicle coatings."},{"$f":"Translator!B2477","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Juli 2017\n- \nsunset date: 22. Januar 2019"},null,null,"100.031.196\n",null,null,null,null,"E2011","L00000000050","Potassium hydroxyoctaoxodizincatedichromate(1-)"]
[{"$f":"Translator!B1833","v":"N,N-Dimethylacetamide (DMAC)"},"127-19-5","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2546","v":"N,N-dimethylacetamide is used as a solvent, mainly in the manufacture of various fabrics and in the manufacture of fibers for clothing and other applications. It is also used as a reagent and in products such as industrial coatings and paints, insulating paper, polyimide films, stripping agents and ink removers. "},null,null,null,100004389,null,null,null,null,"E2011","L00000000052","N,N-Dimethylacetamide"]
[{"$f":"Translator!B1834","v":"Calcium arsenate"},"7778-44-1","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2547","v":"Calcium arsenate is present in complex raw materials (which themselves are by-products of metallurgical processes), which are mainly used for copper and lead refining. The material is used to deposit nickel from molten metal and to produce diarsene trioxide. However, most of the substance appears to be disposed of as waste."},null,null,null,100029003,null,null,null,null,"E2011","L00000000048","Calcium-arsenate"]
[{"$f":"Translator!B1835","v":"Dichromium tris(chromate)"},"24613-89-6","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2548","v":"Dichrom tris(chromate) is mainly used in mixtures for metal surface treatment in the aerospace, steel and aluminium coating sectors. "},{"$f":"Translator!B2478","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Juli 2017\n- \nsunset date: 22. Januar 2019"},null,null,100042127,null,null,null,null,"E2011","L00000000063","Dichromium tris(chromate)"]
[{"$f":"Translator!B1836","v":"Lead diazide, Lead azide"},"13424-46-9","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2549","v":"Lead diazide is mainly used as a detonator or amplifier in detonators for both civil and military applications and as a detonator in pyrotechnic devices."},null,null,null,"100.033.206\n",null,null,null,null,"E2011","L00000000061","Lead-diazide"]
[{"$f":"Translator!B1837","v":"Lead dipicrate"},"6477-64-1","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2550","v":"No registration for lead dipicrate has been submitted to ECHA. As with lead diazide and lead styphnate, the substance is an explosive. It may be used in small quantities in detonator mixtures together with the other two lead compounds mentioned."},null,null,null,"100.026.669\n",null,null,null,null,"E2011","L00000000051","Lead-dipicrate"]
[{"$f":"Translator!B1838","v":"Lead 2,4,6-trinitro-m-phenylene dioxide (lead styphnate)"},"15245-44-0","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2551","v":"Lead styphnate is mainly used as an initial explosive for small calibre and rifle ammunition. Other common applications include ammunition pyrotechnics, ammunition-operated devices such as bolt-firing devices and detonators for civil use. "},null,null,null,100035703,null,null,null,null,"E2011","L00000000064","lead styphnate"]
[{"$f":"Translator!B1839","v":"Arsenic acid"},"7778-39-4","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2552","v":"Arsenic acid is mainly used to remove gas bubbles from ceramic glass melt (clarifying agent) and is used in the manufacture of laminated printed circuit boards. To a lesser extent, the substance is also used in the production of semiconductors and as a laboratory chemical. "},{"$f":"Translator!B2476","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017"},null,null,"100.029.001\n",null,null,null,null,"E2011","L00000000053","Arsenic-acid"]
[{"$f":"Translator!B1840","v":"Bis(2-methoxyethyl) ether (Diglyme)"},"111-96-6","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2553","v":"Bis(2-methoxyethyl)ether is primarily used as a reactive solvent or as a process chemical in a wide range of applications. It is also used for battery electrolytes and possibly in other products such as sealants, adhesives, fuels and car care products. "},{"$f":"Translator!B2479","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017"},null,null,100003568,null,null,null,null,"E2011","L00000000049","Bis(2-methoxyethyl) ether"]
[{"$f":"Translator!B1841","v":"Bis(2-methoxyethyl)phthalate"},"117-82-8","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2554","v":"No registration for bis(2-methoxyethyl)phthalate has been submitted to ECHA. It therefore appears that the substance is not produced or imported into the EU in quantities over 1 tonne per year. The main uses in the past have been as plasticizers in polymeric materials and paints, lacquers and paints, including printing inks. "},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,100003830,null,null,null,null,"E2011","L00000000059","1,2-Benzenedicarboxylic acid, bis(2-methoxyethyl) ester"]
[{"$f":"Translator!B1842","v":"2-Methoxyanilin (o-Anisidine)"},"90-04-0","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2555","v":"2-Methoxyaniline is mainly used in the production of paints (e.g. azo and naphthol dyes) for tattooing and for dyeing paper, polymers and aluminium foil."},null,null,null,100001785,null,null,null,null,"E2011","L00000000054","o-Anisidine"]
[{"$f":"Translator!B1843","v":"4-(1,1,3,3-tetramethylbutyl)phenol\n4-tert-Octylphenol"},"140-66-9","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2556","v":"4-(1,1,3,3-tetramethylbutyl)phenol is mainly used in the production of polymer mixtures, phenolic resins and ethoxylate surfactants. It is also used as a component in adhesives, coatings, inks and rubber products."},null,null,null,100004934,null,null,null,null,"E2011","L00000000060","4-(1,1,3,3-Tetramethylbutyl)phenol"]
[{"$f":"Translator!B1844","v":"Aluminosilicate Refractory Ceramic Fibres\n\nRefractory aluminosilicate ceramic fibres are fibres listed under index number 650-017-00-8 in Annex VI, Part 3, Table 3.1 of Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on the classification, labelling and packaging of substances and mixtures and meet the following three conditions:\n\na. The oxides of aluminium and silicon are the main components that occur (in the fibres) in variable concentration ranges\n\nb. The fibres have a length-weighted mean geometric diameter minus twice the geometric standard deviation of 6 or less micrometers (µm)\n\nc. The content of alkali and alkaline earth metal oxides (Na2O+K2O+CaO+MgO+BaO) is less than or equal to 18% by weight."},"-","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2557","v":"Refractory ceramic fibres are used for high-temperature insulation, almost exclusively in industrial applications (insulation of industrial furnaces and equipment, equipment for the automotive and aerospace industries) and for fire protection (buildings and industrial process equipment)."},null,null,null,100239154,null,null,null,null,"E2010",null,null,"LG0000005357","Zirconia Aluminosilicate Refractory Ceramic Fibres"]
[{"$f":"Translator!B1845","v":"Aluminosilicate refractory ceramic fibres"},"142844-00-6",null,"D",null,null,null,null,null,100133434,null,null,null,null,null,"Y00000051438","Refractory ceramic fibres","Y00000051438","Zirconia Aluminosilicate Refractory Ceramic Fibres"]
[{"$f":"Translator!B1846","v":"1,2-dichloroethane"},"107-06-2","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2558","v":"1,2-dichloroethane is mainly used in the production of other substances (e.g. vinyl chloride). It is partly used as a solvent in the chemical and pharmaceutical industries and in laboratories. "},{"$f":"Translator!B2480","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Mai 2016\n- \nsunset date:  22. November 2017"},null,null,100003145,null,null,null,null,"E2011","L00000000056","1,2-Dichloroethane"]
[{"$f":"Translator!B1847","v":"2,2'-dichloro-4,4'-methylenedianiline (MOCA)"},"101-14-4","2011-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2559","v":"2,2'-dichloro-4,4'-methylenedianiline is mainly used as a hardener in resins and in the manufacture of polymer products such as polyurethane and also for the manufacture of other substances. The material can still be used in construction and art."},{"$f":"Translator!B2480","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Mai 2016\n- \nsunset date:  22. November 2017"},null,null,100002654,null,null,null,null,"E2011","L00000000065","4,4'-Methylenebis[2-chloroaniline]"]
[{"$f":"Translator!B1848","v":"Formamide"},"75-12-7","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2560","v":"Mainly used as an intermediate in the manufacture of agrochemicals, pharmaceuticals and industrial chemicals. Less often used as solvent and laboratory reagent for quality control in forensic laboratories, hospitals, pharmaceutical companies, food and beverage manufacturers and research laboratories. The fabric also seems to be used as a plasticizer."},null,null,null,"100.000.766\n",null,null,null,null,"E2012","L00000000092","Formamide"]
[{"$f":"Translator!B1849","v":"N,N,N',N'-tetramethyl-4,4'-methylenedianiline\n(Michler’s base)"},"101-61-1","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2561","v":"Used as an intermediate in the production of dyes and other substances."},null,null,null,100002691,null,null,null,null,"E2012","L00000000113","N,N,N',N'-tetramethyl-4,4'-methylenedianiline"]
[{"$f":"Translator!B1850","v":"Diboron trioxide"},"1303-86-2","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2562","v":"Broadly used, e.g. in glass and glass fibers, frits, ceramics, flame retardants, catalysts, industrial fluids, metallurgy, nuclear energy, electrical equipment, adhesives, paints/lacquers, film development solutions, detergents and cleaners, reagents, biocides and insecticides."},null,null,null,100013751,null,null,null,null,"E2012","L00000000214","Diboron-trioxide"]
[{"$f":"Translator!B1851","v":"Lead(II) bis(methanesulfonate)"},"17570-76-2","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2563","v":"Mainly used in (electrolytic and electroless) electroplating processes for electronic components (such as printed circuit boards). The material also seems to be used for batteries for special applications."},null,null,null,"100.100.365\n",null,null,null,null,"E2012","L00000001062","lead(II) methanesulphonate"]
[{"$f":"Translator!B1852","v":"4,4'-bis(dimethylamino)-4''-(methylamino)trityl alcohol\nThe substance is proposed only where it contains Michler’s ketone (EC Number: 202-027-5) or/and Michler’s\nbase (EC Number: 202-959-2) ≥ 0.1% (wt/wt)"},"561-41-1","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3032","v":"Used to formulate writing inks and potentially other inks and to dye a wide variety of materials."},{"$f":"Translator!$B3033","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},null,null,"100.008.381\n",null,null,null,null,"E2012 /C 2023","L00000011672","4,4'-bis(dimethylamino)-4''-(methylamino)trityl alcohol"]
[{"$f":"Translator!B1853","v":"4,4'-\nbis(dimethylamino)benzophenone (Michler’s ketone)"},"90-94-8","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2565","v":"Used as an intermediate in the production of triphenylmethane dyes and other substances. Other potential uses as an additive (photosensitizer) in paints and pigments, in dry film products and as a process chemical in the production of electronic circuit boards."},null,null,null,100001843,null,null,null,null,"E2012","L00000000104","4,4'-Bis(dimethylamino)benzophenone"]
[{"$f":"Translator!B1854","v":"[4-[[4-anilino-1-naphthyl][4-\n(dimethylamino)phenyl]methylene]cyclohexa-2,5-dien-1-ylidene]\ndimethylammonium chloride (C.I. Basic Blue 26)"},"2580-56-5","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2566","v":"Used to formulate paints, detergents and coatings and to dye paper, packaging, textiles, plastic products and other types of products. Also used in diagnostic and analytical applications."},null,null,null,"100.018.131\n",null,null,null,null,"E2012","L00000022161","[4-[[4-Anilino-1-naphthyl][4-(dimethylamino)phenyl]methylene]cyclohe..."]
[{"$f":"Translator!B1855","v":"[4-[4,4'-Bis(dimethylamino) benzhydryliden]cyclohexa-2,5-dien-1-yliden]dimethylammonium chlorid\n(C.I. Basic Violet 3) [mit ≥ 0.1% Michler's Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]"},"548-62-9","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2567","v":"Mainly used in paper dyeing and in inks in printer cartridges and ballpoint pens. Also used for dyeing dried flowers, as a marker to increase the visibility of liquids and for dyeing in microbiological and clinical laboratories."},null,null,null,"100.008.140\n",null,null,null,null,"E2012","L00000011408","[4-[4,4'-Bis(dimethylamino)benzhydrylidene]cyclohexa-2,5-dien-1-ylid..."]
[{"$f":"Translator!B1856","v":"1,2-bis(2-methoxyethoxy)ethane (Triglyme)"},"112-49-2","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2568","v":"Mainly used as a solvent or processing aid in the production and formulation of industrial chemicals. Less often used in brake fluids and for repairing motor vehicles."},null,null,null,"100.003.616\n",null,null,null,null,"E2012 /C 2023","L00000000129","Triethylene glycol dimethyl ether"]
[{"$f":"Translator!B1857","v":"1, 2-dimethoxyethane (EGDME)"},"110-71-4","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2569","v":"Mainly used as a solvent or processing aid in the production and formulation of industrial chemicals and as an electrolyte solvent in lithium batteries."},null,null,null,100003451,null,null,null,null,"E2012","L00000000125","1,2-Dimethoxyethane"]
[{"$f":"Translator!B1858","v":"1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinane-2,4,6-trione"},"2451-62-9","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2570","v":"Mainly used as hardener in resins and coatings. Also used in coatings for the printed circuit board industry, electrical insulation materials, resin casting systems, composite boards, screen printing coatings, tools, adhesives, lining materials and stabilizers for plastics."},null,null,null,100017741,null,null,null,null,"E2012","L00000000258","TGIC"]
[{"$f":"Translator!B1859","v":"1,3,5-tris-[(2S and 2R)-2,3-epoxypropyl]-1,3,5-triazine-2,4,6-(1H, 3H, 5H)-\ntrione)"},"59653-74-6","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2571","v":"Mainly used as solder resist in the EU. Also used in electrical insulation materials, resin casting systems, composite panels, screen printing, coatings, tools, adhesives, lining materials and stabilizers for plastics. "},null,null,null,"100.102.195\n",null,null,null,null,"E2012","L00000001164","Teroxirone"]
[{"$f":"Translator!B1860","v":"α,α-Bis[4-(dimethylamino)phenyl]-4\n(phenylamino)naphthalene-1-methanol (C.I. Solvent Blue 4)"},"6786-83-0","2012-06-18","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2572","v":"It is mainly used for formulating printing inks and writing inks, for dyeing paper and in mixtures, such as windscreen washes. "},null,null,null,"100.027.138\n",null,null,null,null,"E2012","L00000031390","1-Naphthalenemethanol, alpha,alpha-bis(4-(dimethylamino)phenyl)-4-(phenylamino)-"]
[{"$f":"Translator!B1861","v":"Hexahydromethylphthalic anhydride\n\nincluding cis- and trans- stereo isomeric forms and all possible combinations of the isomers"},"-","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2573","v":"Production of polyester and alkyd resins and plasticizers for thermoplastic polymers. The anhydrides are also used as curing agents for epoxy resins and chain crosslinkers for thermoplastic polymers."},null,null,null,"100.239.158\n",null,null,null,null,"E2012",null,null,"LG0000001779","Hexahydromethylphthalic anhydride"]
[{"$f":"Translator!B1862","v":"Hexahydromethylphthalic anhydride"},"25550-51-0\n\n\n",null,"D",null,null,null,null,null,"100.042.798\n",null,null,null,null,null,"LG0000001779","Hexahydromethylphthalic-anhydride","LG0000001779","Hexahydromethylphthalic anhydride"]
[{"$f":"Translator!B1863","v":"Hexahydro-4-methylphthalic anhydride"},"19438-60-9",null,"D",null,null,null,null,null,"100.039.141\n",null,null,null,null,null,"LG0000001779","hexahydro-4-methylphthalic anhydride","LG0000001779","Hexahydromethylphthalic anhydride"]
[{"$f":"Translator!B1864","v":"Hexahydro-1-methylphthalic anhydride"},"48122-14-1",null,"D",null,null,null,null,null,"100.051.216\n",null,null,null,null,null,"LG0000001779","Hexahydro-1-methylphthalic anhydride","LG0000001779","Hexahydromethylphthalic anhydride"]
[{"$f":"Translator!B1865","v":"Hexahydro-3-methylphthalic anhydride"},"57110-29-9",null,"D",null,null,null,null,null,"100.055.043\n",null,null,null,null,null,"LG0000001779","Hexahydro-3-methylphthalic anhydride","LG0000001779","Hexahydromethylphthalic anhydride"]
[{"$f":"Translator!B1867","v":"Trilead dioxide phosphonate"},"12141-20-7","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2574","v":"Production of PVC; Use in plastic products"},null,null,null,"100.032.035\n",null,null,null,null,"E2012","L00000000418","Trilead-dioxide-phosphonate"]
[{"$f":"Translator!B1868","v":"Pyrochlore, antimony lead yellow"},"8012-00-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2575","v":"Use in coatings, paints, thinners, paint removers, inks and toners "},null,null,null,"100.029.436\n",null,null,null,null,"E2012","L00000000356","C.I. Pigment Yellow 41"]
[{"$f":"Translator!B1869","v":"Sulfurous acid, lead salt, dibasic"},"62229-08-7","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2576","v":"Production of PVC; Use of lead reinforced plastic materials in building interiors "},null,null,null,"100.057.680\n",null,null,null,null,"E2012","L00000000691","Sulfurous Acid, Lead Salt, Dibasic"]
[{"$f":"Translator!B1870","v":"Tetralead trioxide sulphate"},"12202-17-4","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2577","v":"Production of PVC; Use in plastic products and in electric batteries and accumulators "},null,null,null,"100.032.152\n",null,null,null,null,"E2012","L00000000421","Tetralead-trioxide-sulphate"]
[{"$f":"Translator!B1871","v":"Tetraethyllead"},"78-00-2","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2578","v":"Fuel additives and fuel mixtures "},{"$f":"Translator!B3034","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},null,null,"100.000.979\n",null,null,null,null,"E2012 / C 2023","L00000000095","Tetraethyl lead"]
[{"$f":"Translator!B1872","v":"Trilead bis(carbonate) dihydroxide [Basic lead carbonate]"},"1319-46-6","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2579","v":"Production of PTC ceramics "},null,null,null,"100.013.901\n",null,null,null,null,"E2012","L00000000226","Trilead bis(carbonate) dihydroxide"]
[{"$f":"Translator!B1873","v":"Tricosafluorododecanoic acid"},"307-55-1","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2580","v":"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products"},null,null,null,"100.005.641\n",null,null,null,null,"E2012","L00000008709","Perfluorododecanoic acid"]
[{"$f":"Translator!B1874","v":"N-Methylacetamide"},"79-16-3","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2581","v":"Intermediate and laboratory reagent"},null,null,null,"100.001.075\n",null,null,null,null,"E2012","L00000003178","N-methylacetamide"]
[{"$f":"Translator!B1875","v":"N-Pentyl-isopentyl phthalate"},"776297-69-9","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2582","v":"Plasticizers in plastics "},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,"100.149.209\n",null,null,null,null,"E2012","L00000114641","n-Pentyl-isopentylphthalate"]
[{"$f":"Translator!B1876","v":"o-Aminoazotoluene [4-o-Tolylazo-o-toluidine]"},"97-56-3","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2583","v":"No information available "},null,null,null,"100.002.357\n",null,null,null,null,"E2012","L00000004652","4-o-Tolylazo-o-toluidine"]
[{"$f":"Translator!B1877","v":"Orange lead [Lead tetroxide]"},"1314-41-6","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2584","v":"Production of lead-acid batteries;\nProduction of crystal glass and ceramics;\nProduction of rubber protection;\nExplosives production;\nUsed to repair televisions,\ncomputer monitors and other devices with cathode ray tubes;\nUse in adsorbents, paints and pigments"},null,null,null,"100.013.851\n",null,null,null,null,"E2012","L00000000222","Lead(II,IV)-oxide"]
[{"$f":"Translator!B1878","v":"o-Toluidine"},"95-53-4","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2585","v":"Intermediate and laboratory reagent"},null,null,null,"100.002.209\n",null,null,null,null,"E2012","L00000004485","o-Toluidine"]
[{"$f":"Translator!B1879","v":"Pentalead tetraoxide sulphate"},"12065-90-6","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2586","v":"Production of plastic products;\nUse in electric batteries and accumulators;\nUse of lead-reinforced plastic materials in building interiors"},null,null,null,"100.031.867\n",null,null,null,null,"E2012","L00000000413","Pentalead-tetraoxide-sulphate"]
[{"$f":"Translator!B1880","v":"Pentacosafluorotridecanoic acid"},"72629-94-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2587","v":"Plasticizers in PVC, sealants and printing inks"},null,null,null,"100.069.747\n",null,null,null,null,"E2012","L00000075631","Pentacosafluorotridecanoic acid"]
[{"$f":"Translator!B1881","v":"Dinoseb(ISO); 6-sec-butyl-2,4-dinitrophenol"},"88-85-7","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2588","v":"Production of plastic products, including compounding and conversion;\nmanufacture of bulk chemicals (including petroleum products)"},null,null,null,"100.001.692\n",null,null,null,null,"E2012","L00000003914","Dinoseb"]
[{"$f":"Translator!B1882","v":"Dioxobis(stearato)trilead"},"12578-12-0","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2589","v":"Production of plastic products, including compounding and conversion;\nUse of lead-reinforced plastic materials in building interiors"},null,null,null,"100.032.444\n",null,null,null,null,"E2012","L00000000436","Dioxobis(stearato)trilead"]
[{"$f":"Translator!B1883","v":"Acetic acid, lead salt, basic"},"51404-69-4","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2590","v":"Production of fine chemicals;\nManufacture of computers, electronic and optical products;\nUse as laboratory reagent and intermediate"},null,null,null,100051960,null,null,null,null,"E2012","L00000000662","Acetic Acid, Lead Salt, Basic"]
[{"$f":"Translator!B1884","v":"Fatty acids, C16-18, lead salts"},"91031-62-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2591","v":"Production of plastic products, including compounding and conversion;\nUse of lead reinforced plastic materials in building interiors"},null,null,null,"100.084.483\n",null,null,null,null,"E2012","L00000000918","Fatty Acids, C16-18, Lead Salts"]
[{"$f":"Translator!B1885","v":"Furan"},"110-00-9","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2592","v":"No information available"},null,null,null,"100.003.390\n",null,null,null,null,"E2012","L00000006003","Furan"]
[{"$f":"Translator!B1886","v":"Henicosafluoroundecanoic acid"},"2058-94-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2593","v":"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products"},null,null,null,"100.016.515\n",null,null,null,null,"E2012","L00000020458","Perfluoro-n-undecanoic acid"]
[{"$f":"Translator!B1887","v":"Heptacosafluorotetradecanoic acid"},"376-06-7","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2594","v":"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products"},null,null,null,"100.006.186\n",null,null,null,null,"E2012","L00000009298","Perfluoromyristic acid"]
[{"$f":"Translator!B1888","v":"Silicic acid, lead salt"},"11120-22-2","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2595","v":"Stone, gypsum, cement, glass and ceramic products"},null,null,null,"100.031.227\n",null,null,null,null,"E2012","L00000000390","Silicic acid, lead salt"]
[{"$f":"Translator!B1889","v":"Silicic acid (H2Si2O5), barium salt (1:1), lead-doped [Silicic acid,\nbarium salt, lead-doped]\n[with lead content (Pb) above the applicable general concentration limit for'reproductive toxicity' repr. 1A (CLP) or category 1 (DSD); the substance belongs to a group entry of lead compounds with index number 082-001-00-6 in CLP Regulation (EC) No 1272/2008]"},"68784-75-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2596","v":"For coating glass bulbs;\nFormulation (mixing) of mixtures and/or new packaging"},null,null,null,"100.065.681\n",null,null,null,null,"E2012","L00000000756","Silicic acid (H2Si2O5), barium salt (1:1), lead-doped"]
[{"$f":"Translator!B1890","v":"Methoxyacetic acid (MAA)"},"625-45-6","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2597","v":"Manufacture of chemicals and chemical products for industrial use;\nProduction of cleaning agents or detergents;\nManufacture of food products, manufacture of fabricated metal products.\n\nDisinfectants (for private use), corrosive descaling agents, including products for ovens and stoves, disinfectants for use on surfaces in contact with food, industrial cleaning agents for ultrafiltration membranes or reverse osmosis, cleaning agents for floors and walls in the industrial sector, cleaning agents for wheels and tyres, pH regulator, corrosion inhibitors.>br>\nBasic chemical for the production of biocides.\n\nAdditives for motor fuels, bleaching agents for housings, cationic electrocoating, etching liquids, pesticides."},null,null,null,"100.009.904\n",null,null,null,null,"E2012","L00000013279","methoxyacetic acid"]
[{"$f":"Translator!B1891","v":"Methyloxirane [Propylene oxide]"},"75-56-9","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2598","v":"Intermediate for the production of propylene oxide;\nCellulose modifier;\nApplications in coatings;\nLubricant;\nUse as fuel;\nAgrochemical use;\nDetergent;\nDe-icing and antifreeze;\nfunctional fluid;\nWater treatment chemicals"},null,null,null,"100.000.800\n",null,null,null,null,"E2012","L00000002785","Methyloxirane"]
[{"$f":"Translator!B1893","v":"N,N-dimethylformamide"},"68-12-2","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2599","v":"Production of synthetic/artificial leather in polyurethane;\nProduction of printed circuit boards in the electronics sector;\nReagent and catalyst for syntheses in organic chemistry;\nSolvents in syntheses and for crystallization in the pharmaceutical industry;\nCleaning solution in the textile industry;\nSelective absorption (e.g. acetylene extraction in ethylene streams);\nManufacture of electrical distributors and circuits"},null,null,null,"100.000.617\n",null,null,null,null,"E2012","L00000002480","N,N-Dimethylformamide"]
[{"$f":"Translator!B1894","v":"Diisopentylphthalate (DIPP)"},"605-50-5","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2600","v":"Plasticizers and surface conditioners in fuels;\nPlasticizers for plastics"},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,"100.009.172\n",null,null,null,null,"E2012","L00000012510","1,2-Benzenedicarboxylic acid, bis(3-methylbutyl) ester (9CI)"]
[{"$f":"Translator!B1895","v":"Dimethyl sulphate"},"77-78-1","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2601","v":"Intermediate product as methylating agent"},null,null,null,"100.000.963\n",null,null,null,null,"E2012","L00000002997","Dimethyl sulfate"]
[{"$f":"Translator!B1896","v":"Lead oxide sulfate"},"12036-76-9","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2602","v":"Production of plastic products, including compounding and conversion"},null,null,null,"100.031.672\n",null,null,null,null,"E2012","L00000000407","Lead oxide sulfate (Pb2O(SO4))"]
[{"$f":"Translator!B1897","v":"Lead titanium trioxide"},"12060-00-3","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2603","v":"Semiconductors in machines, apparatus and mechanical devices as well as electrical/electronic products"},null,null,null,"100.031.841\n",null,null,null,null,"E2012","L00000000410","Lead-titanium-trioxide"]
[{"$f":"Translator!B1898","v":"Lead titanium zirconium oxide"},"12626-81-2","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2604","v":"Manufacture of computers, electronic and optical products, intermediate products"},null,null,null,"100.032.467\n",null,null,null,null,"E2012","L00000000438","Lead titanium zirconium oxide"]
[{"$f":"Translator!B1899","v":"Cyclohexane-1,2-dicarboxylic anhydride\nall possible combinations of the cis- and trans-isomers"},"-","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2605","v":"Industrial use: Hardener for epoxy resins, intermediate in chemical synthesis or chemical process, monomer in the production of resins;\nCyclohexane-1,2-dicarboxylic anhydride (HHPA): Preparation of alkyd resins, plasticizers, insect repellents, rust inhibitors"},null,null,null,"100.239.156\n",null,null,null,null,"E2012",null,null,"LG0000006800","Cyclohexane-1,2-dicarboxylic anhydride"]
[{"$f":"Translator!B1900","v":"Cyclohexane-1,2-dicarboxylic anhydride"},"85-42-7",null,"D",null,null,null,null,null,"100.001.459\n",null,null,null,null,null,"LG0000001779","cyclohexane-1,2-dicarboxylic anhydride","LG0000006800","Cyclohexane-1,2-dicarboxylic anhydride"]
[{"$f":"Translator!B1901","v":"cis-cyclohexane-1,2-dicarboxylic anhydride"},"13149-00-3",null,"D",null,null,null,null,null,"100.032.791\n",null,null,null,null,null,"LG0000006800","cis-cyclohexane-1,2-dicarboxylic anhydride","LG0000006800","Cyclohexane-1,2-dicarboxylic anhydride"]
[{"$f":"Translator!B1902","v":"trans-cyclohexane-1,2-dicarboxylic anhydride"},"14166-21-3",null,"D",null,null,null,null,null,"100.034.539\n",null,null,null,null,null,"LG0000006800","trans-cyclohexane-1,2-dicarboxylic anhydride","LG0000006800","Cyclohexane-1,2-dicarboxylic anhydride"]
[{"$f":"Translator!B1903","v":"C,C'-azodi(formamide) (ADCA)\n"},"123-77-3","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2606","v":"blowing agent, aging and bleaching agent, foaming agent, catalyst, insulating material, building material, cement filler, dye, additive, bleaching agent in photography"},null,null,null,100004229,null,null,null,null,"E2012","L00000007064","C,C'-azodi(formamide)"]
[{"$f":"Translator!B1904","v":"Dibutyltin dichloride"},"683-18-1","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2607","v":"Additive in rubber, stabilizer in PVC plastics, catalyst in the production of polyurethanes and silicones; use in insulations and coatings, food packaging, T-shirts, polyurethane gloves, sanitary towels, medical devices, cellophane packaging and soft toys, PVC plastics (water pipes, packaging material, textile products), silicone rubber (sealants, dental products, paper coatings), polyurethanes (foams)."},null,null,null,"100.010.610",null,null,null,null,"E2012","L00000014041","Dibutyltin-dichloride"]
[{"$f":"Translator!B1905","v":"Diethyl sulphate"},"64-67-5","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2608","v":"Production of fine chemicals;\nReactant in polymer synthesis;\nIntermediate product as methylating agent"},null,null,null,"100.000.536",null,null,null,null,"E2012","L00000002348","Diethyl-sulphate"]
[{"$f":"Translator!B1906","v":"Bis(pentabromophenyl)ether (decabromodiphenyl ether; decaBDE)"},"1163-19-5","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2609","v":"Additive in flame retardants, plastics/polymers and textiles"},null,null,null,"100.013.277",null,null,null,null,"E2012","L00000000207","Decabromodiphenylether"]
[{"$f":"Translator!B1907","v":"Lead bis(tetrafluoroborate)"},"13814-96-5","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2610","v":"Use with automated and manual electrolytic lead plating"},null,null,null,"100.034.064",null,null,null,null,"E2012","L00000000478","Borate(1-), tetrafluoro-, lead (2+)"]
[{"$f":"Translator!B1908","v":"Lead cyanamidate"},"20837-86-9","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2611","v":"No information available "},null,null,null,"100.040.052",null,null,null,null,"E2012","L00000000578","Cyanamide, lead(2+) salt (1:1)"]
[{"$f":"Translator!B1909","v":"Lead dinitrate"},"10099-74-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2612","v":"Manufacture of explosives;Manufacture of lead nitrate;Manufacture of weapons and ammunition;\nProduction of pigments and fine chemicals;\nUse in coatings, paints, thinners, paint removers, fillers, fillers, fillers, mortar, modelling clay, finger paints;\nIntermediate;\nlaboratory chemicals "},null,null,null,"100.030.210",null,null,null,null,"E2012","L00000000365","Lead-dinitrate"]
[{"$f":"Translator!B1910","v":"Lead monoxide [Lead oxide]"},"1317-36-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2613","v":"Use for the production of lead oxide; production of lead-acid batteries;\nProduction of crystal glass and ceramics;\nProduction of rubber protection;\nExplosives production;\nUse as intermediate product"},null,null,null,"100.013.880",null,null,null,null,"E2012","L00000000225","Lead-monoxide"]
[{"$f":"Translator!B1911","v":"3-Ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidine"},"143860-04-2","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2614","v":"No information available "},null,null,null,"100.101.975",null,null,null,null,"E2012","L00000113406","3-ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidine"]
[{"$f":"Translator!B1912","v":"4,4'-Methylenedi-o-toluidine"},"838-88-0","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2615","v":"intermediate "},null,null,null,"100.011.508",null,null,null,null,"E2012","L00000014993","4,4'-Methylenedi-o-toluidine"]
[{"$f":"Translator!B1913","v":"4,4'-oxydianiline and its salts"},"-","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2616","v":"intermediate"},null,null,null,"100.239.146",null,null,null,null,"E2012",null,null,"LG0000003120","4,4'-Oxydianiline and its salts"]
[{"$f":"Translator!B1914","v":"4,4'-oxydianiline"},"101-80-4",null,"D",null,null,null,null,null,"100.002.707",null,null,null,null,null,"LG0000003120","4,4'-Oxydianiline","LG0000003120","4,4'-Oxydianiline and its salts"]
[{"$f":"Translator!B1915","v":"4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated \n[covering well-defined\nsubstances and UVCB substances, polymers and homologues]"},"-","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2617","v":"Emulsifier for emulsion polymerization;\nTextile and leather auxiliaries;\nPesticide formulations;\nVeterinary products;\nWater-based paints\nIntermediate for the preparation of octylphenol ether sulfates;\nIn the construction industry\nas a pore generator/foaming agent for concrete;\nas mould release agent on building sites and in the production of precast concrete parts as well as an aid for the cleaning of machines;\nas a component (emulsifier) of bitumen/wax emulsions for painting/sealing in the construction industry or when covering concrete surfaces;\n\nas metalworking fluids;\nas oil for lubrication or for hydraulic equipment"},{"$f":"Translator!B2481","v":"included in Annex 14\n- \nLast application date: 4. Juli 2019\n-\nsunset date: 4. Januar 2021"},null,null,"100.239.147",null,null,null,null,"E2012",null,null,"LG0000006643","4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"]
[{"$f":"Translator!B1916","v":"Poly(oxy-1,2-ethanediyl), α-[(1,1,3,3-tetramethylbutyl)phenyl]-ω-hydroxy-"},"9036-19-5",null,"D",null,null,null,null,null,"100.120.858",null,null,null,null,null,"LG0000006643","Glycols, polyethylene, mono((1,1,3,3-tetramethylbutyl)phenyl) ether","LG0000006643","4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"]
[{"$f":"Translator!B1917","v":"Polyethylene glycol p-(1,1,3,3-tetramethylbutyl)phenyl ether"},"9002-93-1",null,"D",null,null,null,null,null,"100.123.919",null,null,null,null,null,"LG0000006643","Glycols, polyethylene, mono(p-(1,1,3,3-tetramethylbutyl)phenyl) ether","LG0000006643","4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"]
[{"$f":"Translator!B1918","v":"20-[4-(1,1,3,3-tetramethylbutyl)phenoxy]-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"2497-59-8",null,"D",null,null,null,null,null,"100.017.894",null,null,null,null,null,"LG0000006643","20-(4-(1,1,3,3-Tetramethylbutyl)phenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","LG0000006643","4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"]
[{"$f":"Translator!B1919","v":"2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethanol "}," 2315-67-5",null,"D",null,null,null,null,null,"100.150.206",null,null,null,null,null,"LG0000006643","Octoxynol-1","LG0000006643","4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"]
[{"$f":"Translator!B1920","v":"2-[2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethoxy]ethanol"},"2315-61-9",null,"D",null,null,null,null,null,"100.150.202",null,null,null,null,null,"LG0000006643","Octoxynol-2","LG0000006643","4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"]
[{"$f":"Translator!B1921","v":"4-Aminoazobenzene"},"60-09-3","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2618","v":"intermediate "},null,null,null,"100.000.412",null,null,null,null,"E2012","L00000002151","4-Aminoazobenzene"]
[{"$f":"Translator!B1922","v":"Biphenyl-4-ylamine"},"92-67-1","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2619","v":"No information available "},null,null,null,"100.001.980",null,null,null,null,"E2012","L00000004226","4-Aminodiphenyl"]
[{"$f":"Translator!B1923","v":"4-methyl-m-phenylenediamine [Toluene-2,4-diamine]"},"95-80-7","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2620","v":"Intermediate product in the production of sulfur dyes "},null,null,null,"100.002.231",null,null,null,null,"E2012","L00000004514","4-Methyl-m-phenylenediamine"]
[{"$f":"Translator!B1924","v":"4-Nonylphenol, branched and linear: substances with a linear and/or\nbranched alkyl chain with a carbon number of 9 covalently bound in position\n4 to phenol, covering also UVCB- and well-defined substances which include\nany of the individual isomers or a combination thereof"},"-","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2621","v":"Industrial application of coatings or inks;\nAdhesives for the production of tires and rubber products;\nIntermediate in the production of ethoxylates and plastic stabilizer;\nFormulation of adhesives, paints "},null,null,null,"100.239.149",null,null,null,null,"E2012",null,null,"LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1925","v":"4-(1-Ethyl-1,3-dimethylpentyl)phenol"},"186825-36-5",null,"D",null,null,null,null,null,"100.163.283",null,null,null,null,null,"LG0000006376","4-(1-Ethyl-1,3-dimethylpentyl)phenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1926","v":"Phenol, 4-nonyl-, branched"},"84852-15-3",null,"D",null,null,null,null,null,"100.076.631",null,null,null,null,null,"LG0000006376","4-Nonylphenol, branched","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1927","v":"p-(1-methyloctyl)phenol "},"17404-66-9",null,"D",null,null,null,null,null,"100.037.646",null,null,null,null,null,"LG0000006376","p-(1-Methyloctyl)phenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1928","v":"p-(1,1-dimethylheptyl)phenol "},"30784-30-6",null,"D",null,null,null,null,null,"100.045.748",null,null,null,null,null,"LG0000006376","p-(1,1-Dimethylheptyl)phenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1929","v":"p-nonylphenol"},"104-40-5",null,"D",null,null,null,null,null,"100.002.909",null,null,null,null,null,"LG0000006376","p-Nonylphenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1930","v":"4-(1-Ethyl-1,4-dimethylpentyl)phenol "},"142731-63-3",null,"D",null,null,null,null,null,"100.163.285",null,null,null,null,null,"LG0000006376","4-(1-Ethyl-1,4-dimethylpentyl)phenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1931","v":"4-(1-ethyl-1-methylhexyl)phenol "},"52427-13-1",null,"D",null,null,null,null,null,"100.052.625",null,null,null,null,null,"LG0000006376","4-(1-Ethyl-1-methylhexyl)phenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1932","v":"p-isononylphenol"},"26543-97-5",null,"D",null,null,null,null,null,"100.043.412",null,null,null,null,null,"LG0000006376","p-Isononylphenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1933","v":"Phenol, nonyl-, branched"},"90481-04-2",null,"D",null,null,null,null,null,"100.083.463",null,null,null,null,null,"LG0000006376","Phenol, nonyl-, branched","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1934","v":"Isononylphenol"},"11066-49-2",null,"D",null,null,null,null,null,"100.031.156",null,null,null,null,null,"LG0000006376","isononylphenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1935","v":"4-(3-ethylheptan-2-yl)phenol "},"186825-39-8",null,"D",null,null,null,null,null,"100.163.560",null,null,null,null,null,"LG0000006376","4-(2-Ethyl-1-methylhexyl)phenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1936","v":"4-(1,1,5-Trimethylhexyl)phenol"},"521947-27-3",null,"D",null,null,null,null,null,"100.163.282",null,null,null,null,null,"LG0000006376","262-NP","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1937","v":"Nonylphenol "},"25154-52-3",null,"D",null,null,null,null,null,"100.042.414",null,null,null,null,null,"LG0000006376","Nonylphenol","LG0000006376","4-Nonylphenol, branched and linear"]
[{"$f":"Translator!B1938","v":"6-Methoxy-m-toluidine [p-cresidine]"},"120-71-8","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2622","v":"intermediate"},null,null,null,"100.004.018",null,null,null,null,"E2012","L00000006790","6-Methoxy-m-toluidine"]
[{"$f":"Translator!B1939","v":"[Phthalato(2-)]dioxotrilead"},"69011-06-9","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2623","v":"Manufacture of plastic products, including compounding and conversion; use of lead reinforced plastic materials in building interiors "},null,null,null,"100.066.970",null,null,null,null,"E2012","L00000000770","[Phthalato(2-)]dioxotrilead"]
[{"$f":"Translator!B1940","v":"1,2-Benzenedicarboxylic acid dipentylester, branched and linear"},"84777-06-0","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2624","v":"Laboratory chemical for analytical purposes "},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,"100.076.365",null,null,null,null,"E2012","L00000082256","1,2-Benzenedicarboxylic acid, dipentylester, branched and linear"]
[{"$f":"Translator!B1941","v":"1,2-diethoxyethane"},"629-14-1","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2625","v":"Solvents in various formulations such as paints, inks and cleaning fluids;\nUse for glycol ethers, including hydraulic and brake fluids, antifreeze and chemical intermediates"},null,null,null,"100.010.070",null,null,null,null,"E2012","L00000013459","1,2-diethoxyethane"]
[{"$f":"Translator!B1942","v":"1-bromopropane; n-propyl bromide"},"106-94-5","2012-12-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2626","v":"Manufacture of bulk chemicals (including petroleum products); industrial solvent for steam degreasing "},{"$f":"Translator!B2475","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,"100.003.133",null,null,null,null,"E2012","L00000005610","1-Bromopropane"]
[{"$f":"Translator!B1943","v":"Pentadecafluorooctanoic Acid (PFOA)"},"335-67-1","2013-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2627","v":"PFOA is used as a process aid in the production of fluoropolymers. These are used in various industries, such as textiles, the paper industry and electroplating.\nMany products contain residues of PFOA such as textiles, carpets, upholstered furniture, paper, leather, printing ink, cleaning and care products for carpets, sealants, floor wax, paints, impregnating agents, fire-fighting foam, surface-treated carpeting and ski wax. PFOA is also found as an impurity in perfluorooctylsulfonyl fluoride (POSF) based substances."},null,null,null,"100.005.817",null,null,null,null,"E2014","L00000008911","pentadecafluorooctanoic acid"]
[{"$f":"Translator!B1944","v":"Dipentyl phthalate (DPP)"},"131-18-0","2013-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2628","v":"Dipentyl phthalate is mainly used as a plasticizer in polyvinyl chloride (PVC), but DPP is also found in electrodes for membranes. DPP is used as a solvent in personal care products, printing inks, paints, nitrocellulose and synthetic resin paints and in the manufacture of adhesives and rubber."},{"$f":"Translator!B2482","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},null,null,"100.004.563",null,null,null,null,"E2014","L00000007471","Di-n-pentyl phthalate"]
[{"$f":"Translator!B1945","v":"Cadmium"},"7440-43-9","2013-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2629","v":"Electrodes in nickel-cadmium accumulators; coatings of metals (corrosion protection);\n\nas an alloying component, for example in electrical contacts and solders"},null,null,null,"100.028.320",null,null,null,null,"E2014","L00000000309","Cadmium"]
[{"$f":"Translator!B1946","v":"Cadmium oxide"},"1306-19-0","2013-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2630","v":"Raw material for the production of electrodes, alloys, pigments, catalysts and metal coatings; heat stabilizer in polymers; ceramic glazes and glass components; laboratory chemicals."},null,null,null,"100.013.770",null,null,null,null,"E2014","L00000000215","Cadmium oxide"]
[{"$f":"Translator!B3809","v":"Monteponite (CdO)"},"12139-21-8",null,"D",null,null,null,null,null,"100.394.431",null,null,null,null,"E 2024"]
[{"$f":"Translator!B1947","v":"Ammonium pentadecafluorooctanoate (APFO)"},"3825-26-1","2013-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2631","v":"APFO is used as a process aid in the production of fluoropolymers. These are used in various industries, such as textiles, the paper industry and electroplating.\nMany products contain residues of APFO such as textiles, carpets, upholstered furniture, paper, leather, printing ink, cleaning and care products for carpets, sealants, floor wax, paints, impregnating agents, fire-fighting foam, surface-treated carpeting and ski wax."},null,null,null,"100.021.202",null,null,null,null,"E2014","L00000025344","ammonium pentadecafluorooctanoate"]
[{"$f":"Translator!B1948","v":"4-Nonylphenol, branched and linear, ethoxylated \n[substances with a linear and/or branched alkyl chain with a\ncarbon number of 9 covalently bound in position 4 to phenol, ethoxylated covering UVCB- and well-defined\nsubstances, polymers and homologues, which include any of the individual isomers and/or combinations thereof]"},"-","2013-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B2632","v":"Formulation component in mining; component in paints, varnishes, cleaning agents, adhesives and surface treatment agents; process chemical for emulsion polymerization "},{"$f":"Translator!B2483","v":"included in Annex 14 and Annex 17\n- \nLast application date: 04. Juli 2019\n- \nsunset date: 04. Januar 2021\n\n"},null,null,"100.239.148",null,null,null,null,"E2014 / C 2023",null,null,"Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3035","v":"Nonylphenol, ethoxylated (8-EO)"},"9016-45-9",null,"D",null,null,null,null,null,"100.167.113",null,null,null,null,"C 2023","Y00000001050","Nonoxinol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3036","v":"26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol"},"14409-72-4",null,"D",null,null,null,null,null,"100.110.408",null,null,null,null,"C 2023","Y00000001050","Nonaethylene glycol p-nonylphenyl ether","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3037","v":"Nonylphenol, ethoxylated (6,5-EO)"},"9016-45-9",null,"D",null,null,null,null,null,"100.167.712",null,null,null,null,"C 2023","Y00000001050","Nonoxinol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3038","v":"Nonylphenol, branched, ethoxylated"},"68412-54-4",null,"D",null,null,null,null,null,"100.105.700",null,null,null,null,"C 2023","Y00000001050","Poly(oxy-1,2-ethanediyl), alpha-(nonylphenyl)-omega-hydroxy-, branched","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3039","v":"4-Nonylphenol, ethoxylated"},"26027-38-3",null,"D",null,null,null,null,null,"100.105.552",null,null,null,null,"C 2023","Y00000001050","4-Nonylphenol, ethoxylated","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3040","v":"20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"27942-27-4",null,"D",null,null,null,null,null,"100.044.297",null,null,null,null,"C 2023","Y00000001050","20-(4-Nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3041","v":"Nonylphenol, ethoxylated (10-EO)"},"9016-45-9",null,"D",null,null,null,null,null,"100.167.714",null,null,null,null,"C 2023","Y00000001050","Nonoxinol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3042","v":"Nonylphenol, ethoxylated"},"9016-45-9",null,"D",null,null,null,null,null,"100.105.533",null,null,null,null,"C 2023","Y00000001050","Nonoxinol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3043","v":"Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-, branched"},"68412-54-4",null,"D",null,null,null,null,null,"100.193.631",null,null,null,null,"C 2023","Y00000001050","Poly(oxy-1,2-ethanediyl), alpha-(nonylphenyl)-omega-hydroxy-, branched","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3044","v":"Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, branched"},"68412-54-4",null,"D",null,null,null,null,null,"100.170.850",null,null,null,null,"C 2023","Y00000001050","Poly(oxy-1,2-ethanediyl), alpha-(nonylphenyl)-omega-hydroxy-, branched","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3045","v":"2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol"},"7311-27-5",null,"D",null,null,null,null,null,"100.027.972",null,null,null,null,"C 2023","Y00000001050","2-[2-[2-[2-(4-Nonylphenoxy)Ethoxy]Ethoxy]Ethoxy]Ethanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3046","v":"Nonylphenol, ethoxylated (15-EO)"},"9016-45-9",null,"D",null,null,null,null,null,"100.167.715",null,null,null,null,"C 2023","Y00000001050","Nonoxinol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3047","v":"2-[2-(4-nonylphenoxy)ethoxy]ethanol"},"20427-84-3",null,"D",null,null,null,null,null,"100.039.818",null,null,null,null,"C 2023","Y00000001050","2-(2-(4-Nonylphenoxy)ethoxy)ethanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3048","v":"4-Nonylphenol, branched, ethoxylated"},"127087-87-0",null,"D",null,null,null,null,null,"100.169.218",null,null,null,null,"C 2023","Y00000001050","Poly(oxy-1,2-ethanediyl), alpha-(4-nonylphenyl)-omega-hydroxy-,branc...","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3049","v":"4-Nonylphenol, branched, ethoxylated"},"127087-87-0",null,"D",null,null,null,null,null,"100.105.797",null,null,null,null,"C 2023","Y00000001050","Poly(oxy-1,2-ethanediyl), alpha-(4-nonylphenyl)-omega-hydroxy-,branc...","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3050","v":"17-(4-nonylphenoxy)-3,6,9,12,15-pentaoxaheptadecan-1-ol"},"34166-38-6",null,"D",null,null,null,null,null,"100.125.263",null,null,null,null,"C 2023","Y00000001050","p-Nonylphenol hexaethoxylate","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3051","v":"Isononylphenol, ethoxylated"},"37205-87-1",null,"D",null,null,null,null,null,"100.130.672",null,null,null,null,"C 2023","Y00000001050","Poly(oxy-1,2-ethanediyl),alpha-(isononylphenyl)-omega-hydroxy","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3052","v":"Nonylphenol, ethoxylated (polymer)"},"-",null,"D",null,null,null,null,null,"100.224.899",null,null,null,null,"C 2023",null,null,"Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3053","v":"Nonylphenol, ethoxylated (EO = 4)"},"-",null,"D",null,null,null,null,null,"100.228.429",null,null,null,null,"C 2023",null,null,"Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3054","v":"Nonylphenol, ethoxylated (EO = 10)"},"-",null,"D",null,null,null,null,null,"100.228.488",null,null,null,null,"C 2023",null,null,"Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3055","v":"4-t-Nonylphenol-diethoxylate"},"156609-10-8",null,"D",null,null,null,null,null,"100.290.599",null,null,null,null,"C 2023","Y00000001050","4-t-Nonylphenol-diethoxylate","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3056","v":"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-"},"20636-48-0",null,"D",null,null,null,null,null,"100.291.191",null,null,null,null,"C 2023","Y00000001050","3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3057","v":"2-(nonylphenoxy)ethanol"},"27986-36-3",null,"D",null,null,null,null,null,"100.044.314",null,null,null,null,"C 2023","Y00000001050","Ethanol, 2-(nonylphenoxy)-","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3058","v":"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol"},"42173-90-0",null,"D",null,null,null,null,null,"100.050.614",null,null,null,null,"C 2023","Y00000001050","26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan -1-ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3059","v":"44-(nonylphenoxy)-3,6,9,12,15,18,21,24,27,30,33,36,39,42-tetradecaoxatetratetracontanol"},"57321-10-5",null,"D",null,null,null,null,null,"100.055.145",null,null,null,null,"C 2023","Y00000001050","44-(nonylphenoxy)-3,6,9,12,15,18,21,24,27,30,33,36,39,42-tetradecaoxatetratetracontanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3060","v":"20-(isononylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"65455-69-8",null,"D",null,null,null,null,null,"100.059.787",null,null,null,null,"C 2023","Y00000001050","20-(isononylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3061","v":"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-, branched"},"91648-64-5",null,"D",null,null,null,null,null,"100.085.354",null,null,null,null,"C 2023","Y00000001050","3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-, branched","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3062","v":"Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-"},"9016-45-9",null,"D",null,null,null,null,null,"100.166.325",null,null,null,null,"C 2023","Y00000001050","Nonoxinol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3063","v":"3,6,9,12,15,18,21,24,27-Nonaoxanonacosan-1-ol, 29-(isononylphenoxy)-"},"65455-72-3","2023-01-17","D",null,null,null,null,null,"100.305.167",null,null,null,null,"C 2023","Y00000001050","3,6,9,12,15,18,21,24,27-Nonaoxanonacosan-1-ol, 29- (isononylphenoxy)-","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3064","v":"3,6,9,12,15-Pentaoxaheptadecan-1-ol, 17-(nonylphenoxy)-"},"27177-01-1","2023-01-17","D",null,null,null,null,null,"100.305.164",null,null,null,null,"C 2023","Y00000001050","3,6,9,12,15-Pentaoxaheptadecan-1-ol, 17-(nonylphenoxy)-","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3065","v":"2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol"},"1119449-38-5",null,"D",null,null,null,null,null,"100.214.097",null,null,null,null,"C 2023","Y00000001050","2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3066","v":"2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol"},"1119449-37-4",null,"D",null,null,null,null,null,"100.214.096",null,null,null,null,"C 2023","Y00000001050","Nonylphenol polyglycol ether","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3067","v":"Nonylphenolpolyglycolether"},"-",null,"D",null,null,null,null,null,"100.205.448",null,null,null,null,"C 2023",null,null,"Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3068","v":"2-(4-nonylphenoxy)ethanol"},"104-35-8",null,"D",null,null,null,null,null,"100.289.057",null,null,null,null,"C 2023","Y00000001050","Ethanol, 2-(4-nonylphenoxy)-","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3069","v":"29-(nonylphenoxy)-3,6,9,12,15,18,21,24,27-nonaoxanonacosanol"},"27177-08-8",null,"D",null,null,null,null,null,"100.043.889",null,null,null,null,"C 2023","Y00000001050","29-(Nonylphenoxy)-3,6,9,12,15,18,21,24,27-Nonaoxanonacosanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3070","v":"23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol"},"27177-05-5",null,"D",null,null,null,null,null,"100.043.888",null,null,null,null,"C 2023","Y00000001050","23-(Nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3071","v":"20-(nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"27177-03-3",null,"D",null,null,null,null,null,"100.043.887",null,null,null,null,"C 2023","Y00000001050","20-(nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3072","v":"2-[2-(nonylphenoxy)ethoxy]ethanol"},"27176-93-8",null,"D",null,null,null,null,null,"100.043.886",null,null,null,null,"C 2023","Y00000001050","2-[2-(Nonylphenoxy)Ethoxy]Ethanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3073","v":"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol"},"26571-11-9",null,"D",null,null,null,null,null,"100.043.454",null,null,null,null,"C 2023","Y00000001050","26-(Nonylphenoxy)-3,6,9,12,15,18,21,24-Octaoxahexacosan-1-Ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3074","v":"2-(isononylphenoxy)ethanol"},"85005-55-6",null,"D",null,null,null,null,null,"100.077.233",null,null,null,null,"C 2023","Y00000001050","2-(isononylphenoxy)ethanol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3075","v":"14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol"},"26264-02-8",null,"D",null,null,null,null,null,"100.043.217",null,null,null,null,"C 2023","Y00000001050","14-(Nonylphenoxy)-3,6,9,12-Tetraoxatetradecan-1-Ol","Y00000001050","4-Nonylphenol, branched and linear, ethoxylated"]
[{"$f":"Translator!B3076","v":"Trixylyl phosphate"},"25155-23-1","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3328","v":"Use as lubricant, hydraulic fluid, grease, release agent use in polyurethane, PVC, TPE, coatings and textiles\nFlame retardants in plastics production\nUse as plasticizer"},{"$f":"Translator!$B3336","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\nSunset date: 27.05.2023"},null,null,"100.042.419",null,null,null,null,"E2013","L00000047978","trixylyl phosphate"]
[{"$f":"Translator!B3077","v":"Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)"},"573-58-0","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3329","v":"Dyes for textiles and paper\npH indicator\nAdditive for agar culture media (for biological staining of histological samples)\nGelling agent for polyvinyl alcohol"},null,null,null,"100.008.509",null,null,null,null,"E2013","L00000011814","C.I. Direct red 28"]
[{"$f":"Translator!B3078","v":"Imidazolidine-2-thione (2-imidazoline-2-thiol)"},"96-45-7","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3330","v":"Manufacture of rubber products and tyres\nProduction of masterbatches\nPreparation of predispersed imidazolidine-2-thione\nUse as vulcanizing agent\nFor repackaging "},null,null,null,"100.002.280",null,null,null,null,"E2013","L00000004572","Ethylene thiourea"]
[{"$f":"Translator!B3079","v":"Cadmium sulphide"},"1306-23-6","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3331","v":"Component for the production of organic and inorganic cadmium compounds\nComponent for the preparation of inorganic pigments\nLaboratory chemical (intermediate, perfumes, perfumes, cosmetics, personal care products)\nComponent for the production of photovoltaic modules\nAdditive for the production of frits and glasses\nAdditive for the production of electronic components"},null,null,null,"100.013.771",null,null,null,null,"E2013","L00000000216","Cadmium-sulphide"]
[{"$f":"Translator!B3080","v":"Dihexyl phthalate"},"84-75-3","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3332","v":"Plasticizer for cellulose and vinylplastics"},{"$f":"Translator!$B3337","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n- Sunset date: 27.02.2023"},null,null,"100.001.417",null,null,null,null,"E2013","L00000003593","Dihexyl-phthalate"]
[{"$f":"Translator!B3081","v":"Lead di(acetate)"},"301-04-2","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3333","v":"Use as intermediate product\nUse as a laboratory chemical\nFor the production of coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling compounds"},null,null,null,"100.005.551",null,null,null,null,"E2013","L00000000150","Lead di(acetate)"]
[{"$f":"Translator!B3082","v":"Disodium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo] -\n5-hydroxy-6-(phenylazo)naphthalene-2,7-disulphonate (C.I. Direct Black 38)"},"1937-37-7","2013-12-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3334","v":"Dyes for textiles, leather and paper, plastics, wood and biological materials\nIngredient for the preparation of aqueous inks\nUse in hair dyes"},null,null,null,"100.016.101",null,null,null,null,"E2013","L00000020025","C.I. Direct Black 38"]
[{"$f":"Translator!B3083","v":"Sodium perborate; perboric acid, sodium salt"},"-","2014-06-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3335","v":"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products"},{"$f":"Translator!$B3338","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023"},null,null,"100.239.162",null,null,null,null,"E2014",null,null,"Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3084","v":"Perboric acid (H3BO2(O2)), monosodium salt, trihydrate"},"13517-20-9",null,"D",null,null,null,null,null,"100.106.721",null,null,null,null,null,"Y00000020663","perboric acid (H3BO2(O2)), monosodium salt trihydrate","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3085","v":"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)"},"90568-23-3",null,"D",null,null,null,null,null,"100.297.786",null,null,null,null,null,"Y00000020663","Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3086","v":"Perboric acid, sodium salt"}," 11138-47-9",null,"D",null,null,null,null,null,"100.031.251",null,null,null,null,null,"Y00000020663","Perboric acid, sodium salt","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3087","v":"Sodium perborate"},"15120-21-5",null,"D",null,null,null,null,null,"100.035.597",null,null,null,null,null,"Y00000020663","Sodium perborate","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3088","v":"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)"},"125022-34-6",null,"D",null,null,null,null,null,"100.297.787",null,null,null,null,null,"Y00000020663","Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3339","v":"Sodium perborate monohydrate"},"10332-33-9","2023-01-17","D",null,null,null,null,null,"100.107.346",null,null,null,null,"E 2023","Y00000020663","perboric acid (HBO(O2)), sodium salt, monohydrate","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3340","v":"Perboric acid (HBO(O2)), sodium\nsalt, tetrahydrate"},"10486-00-7","2023-01-17","D",null,null,null,null,null,"100.115.659",null,null,null,null,"E 2023","Y00000020663","Perboric acid (HBO(O2)), sodium salt, tetrahydrate","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3341","v":"Perboric acid, sodium salt,\ntetrahydrate"},"37244-98-7","2023-01-17","D",null,null,null,null,null,"100.368.533",null,null,null,null,"E 2023","Y00000020663","Perboric acid, sodium salt, tetrahydrate","Y00000020663","Sodium perborate, perboric acid, sodium salt"]
[{"$f":"Translator!B3089","v":"Sodium peroxometaborate"},"7632-04-4","2014-06-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3343","v":"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products "},{"$f":"Translator!$B3354","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023"},null,null,"100.028.688",null,null,null,null,"E2014","L00000033319","Sodium peroxometaborate"]
[{"$f":"Translator!B3090","v":"Cadmium chloride"},"10108-64-2","2014-06-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3344","v":"Component for the production of organic and inorganic cadmium compounds\nStarting material in electroplating and electroplating\nComponent for the production of photovoltaic modules\nlaboratory chemical\nFungicide"},null,null,null,"100.030.256",null,null,null,null,"E2014","L00000000369","Cadmium-chloride"]
[{"$f":"Translator!B3802","v":"cadmium chloride (CdCl2), hydrate (2:5)"},"7790-78-5",null,"D",null,null,null,null,null,"100.168.753",null,null,null,null,"E 2023"]
[{"$f":"Translator!B3091","v":"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear"},"68515-50-4","2014-06-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3345","v":"Plasticizer in polymers, insulating primer, sealing material, engine oil stabilizer, transmission lubricant for motor vehicles"},{"$f":"Translator!$B3355","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023"},null,null,"100.064.610",null,null,null,null,"E2014","L00000070468","1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear"]
[{"$f":"Translator!B3092","v":"Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of  DOTE und MOTE)"},"-","2014-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3346","v":"PVC heat stabilizer\nUse in plastics processing\nIndustrial use"},{"$f":"Translator!$B3808","v":"Included in Annex XIV:\nlast application date: 01.11.2023\nsunset date: 01.05.2025"},null,null,"100.239.161",null,null,null,null,"E2014 / C 2024","Y00000020427","Reaction mass of 2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate and 2-ethylhexyl 10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (reaction mass DOTE and MOTE)"]
[{"$f":"Translator!B3093","v":"Cadmium fluoride"},"7790-79-6","2014-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3347","v":"Research\nManufacture of glass\nHigh Temperature Dry Film Lubricant\nOptical electronics\nSolar cells"},null,null,null,"100.029.293",null,null,null,null,"E2014","L00000000351","Cadmium-fluoride"]
[{"$f":"Translator!B3094","v":"Cadmium sulphate"},"10124-36-4, 31119-53-6","2014-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3348","v":"Component for the production of inorganic cadmium compounds\nStarting material for the surface treatment of metals\nLaboratory Chemical"},{"$f":"Translator!$B3356","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},null,null,"100.030.288",null,null,null,null,"E2014","L00000000371","Cadmium sulfate"]
[{"$f":"Translator!B3800","v":"Sulfuric acid, cadmium salt, hydrate (3:3:8)"},"7790-84-3",null,"D",null,null,null,null,null,"100.130.541",null,null,null,null,"E 2023"]
[{"$f":"Translator!B3801","v":"Sulfuric acid, cadmium salt (1:1), hydrate"},"15244-35-6",null,"D",null,null,null,null,null,"100.154.769",null,null,null,null,"E 2023"]
[{"$f":"Translator!B3095","v":"Bis(2-ethylhexyl)phthalate (DEHP)"},"117-81-7","2008-10-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3349","v":"Bis(2-ethylhexyl)phthalate is mainly used as a plasticizer in polymer products (mainly PVC) to increase the mobility of the product.\nConsumer exposure occurs through the respiratory tract through building materials (wallpaper, floor coverings), furniture and car interiors, through skin contact with shoes, rainwear, PVC gloves, artificial leather in furniture and car seats as well as toys and through ingestion of some baby and child products and food contact materials"},{"$f":"Translator!$B3357","v":"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n"},null,null,"100.003.829",null,null,null,null,"E2014 /C 2023","L00000000009","DEHP"]
[{"$f":"Translator!B3096","v":"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-\ndithia-4-stannatetradecanoate (DOTE)"},"15571-58-1","2014-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3350","v":"Starting material for the preparation of \"Reaction mass of\" 2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates and 2-ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates (\"\"Reaction mass of\"\" DOTE and MOTE)\nUse in plastics processing\nIndustrial use"},{"$f":"Translator!$B3358","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},null,null,"100.036.005",null,null,null,null,"E2014 / C 2023","L00000041408","2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate"]
[{"$f":"Translator!B3097","v":"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)"},"3846-71-7","2014-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3351","v":"UV stabilizer;\nUV absorbents;\nUV-protective agents"},{"$f":"Translator!$B3359","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},null,null,"100.021.225",null,null,null,null,"E2014","L00000025368","Phenol, 2-(2H-benzotriazol-2-yl)-4,6-bis(1,1-dimethylethyl)-"]
[{"$f":"Translator!B3098","v":"2-(2H-benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)"},"25973-55-1","2014-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3352","v":"UV stabilizer;\nUV absorbents;\nUV-protective agents"},{"$f":"Translator!$B3360","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},null,null,"100.043.062",null,null,null,null,"E2014","L00000048662","2-(2H-Benzotriazol-2-yl)-4,6-ditertpentylphenol"]
[{"$f":"Translator!B3099","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-\nmethyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-\ndimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]\n[covering any of the individual isomers of [1] and [2] or\nany combination thereof]"},"-","2015-06-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3353","v":"This group of substances is mainly used in fragrances."},{"$f":"Translator!$B3361","v":"Included in Annex 14\n\n- Last application date: 27.02.2022\n- Sunset date: 27.08.2023"},null,null,"100.239.151",null,null,null,null,"E2015",null,null,"Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3100","v":"Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane"},"-",null,"D",null,null,null,null,null,"100.225.073",null,null,null,null,null,null,null,"Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3101","v":"2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane"},"117933-89-8",null,"D",null,null,null,null,null,"100.120.617",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3102","v":"Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane "},"117933-89-8",null,"D",null,null,null,null,null,"100.101.291",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3103","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"676367-05-8",null,"D",null,null,null,null,null,"100.287.882",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3104","v":"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"676367-06-9",null,"D",null,null,null,null,null,"100.287.891",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3105","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"676367-09-2",null,"D",null,null,null,null,null,"100.287.884",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3106","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-"},"343934-05-4",null,"D",null,null,null,null,null,"100.287.885",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3107","v":"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"676367-04-7",null,"D",null,null,null,null,null,"100.287.886",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3108","v":"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"676367-08-1",null,"D",null,null,null,null,null,"100.287.887",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3109","v":"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- "},"676367-03-6",null,"D",null,null,null,null,null,"100.287.888",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3110","v":"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"676367-07-0",null,"D",null,null,null,null,null,"100.287.889",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3111","v":"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"676367-02-5",null,"D",null,null,null,null,null,"100.287.890",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3112","v":"1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-"},"186309-28-4",null,"D",null,null,null,null,null,"100.287.881",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3113","v":"5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane"},"-",null,"D",null,null,null,null,null,"100.239.152",null,null,null,null,null,null,"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel","Y00000020680"]
[{"$f":"Translator!B3114","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane"},"-",null,"D",null,null,null,null,null,"100.239.150",null,null,null,null,null,null,"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel","Y00000020680"]
[{"$f":"Translator!B3115","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-"},"343934-04-3",null,"D",null,null,null,null,null,"100.287.883",null,null,null,null,null,"Y00000020680","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel","Y00000020680","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]"]
[{"$f":"Translator!B3116","v":"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters \nwith ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)"},"-","2015-06-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3362","v":"in plasticisers, lubricants, coating agents, building materials, cable components, polymer films, PVC components and artists' supplies (e.g. in modelling clay and in finger paints)"},{"$f":"Translator!$B3364","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023"},null,null,"100.239.145",null,null,null,null,"E2015",null,"1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters","Y00000021479"]
[{"$f":"Translator!B3117","v":"1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters"},"68648-93-1",null,"D",null,null,null,null,null,"100.065.447",null,null,null,null,null,"Y00000021479","1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters","Y00000021479","1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters"]
[{"$f":"Translator!B3118","v":"1,2-Benzenedicarboxylic acid, di-C6-10-alkyl esters"},"68515-51-5",null,"D",null,null,null,null,null,"100.064.611",null,null,null,null,null,"Y00000021479","1,2-Benzenedicarboxylic acid, di-C6-10-alkyl esters","Y00000021479","1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters"]
[{"$f":"Translator!B3119","v":"Perfluorononan-1-oic-acid and its sodium and ammonium salts"},"-","2015-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3363","v":"Processing aid in the manufacture of fluoropolymers; lubricant in oils; wetting agent for fire-fighting foam; cleaning agent; antifouling in textiles; surface agent in polishes; sealant; in liquid crystal display panels."},null,null,null,"100.242.186",null,null,null,null,"E2015",null,null,"LG0000007499","Perfluorononan-1-oic-acid and its sodium and ammonium salts"]
[{"$f":"Translator!B3120","v":"Perfluorononan-1-oic acid"},"375-95-1",null,"D",null,null,null,null,null,"100.006.184",null,null,null,null,null,"LG0000007499","Perfluorononan-1-oic acid","LG0000007499","Perfluorononan-1-oic-acid and its sodium and ammonium salts"]
[{"$f":"Translator!B3121","v":"perfluorononan-1-oic acid sodium salts"},"21049-39-8",null,"D",null,null,null,null,null,"100.242.187",null,null,null,null,null,"LG0000007499","Sodium salts of perfluorononan-1-oic-acid","LG0000007499","Perfluorononan-1-oic-acid and its sodium and ammonium salts"]
[{"$f":"Translator!B3122","v":"perfluorononan-1-oic acid ammonium salts"},"4149-60-4",null,"D",null,null,null,null,null,"100.242.185",null,null,null,null,null,"LG0000007499","Ammonium salts of perfluorononan-1-oic-acid","LG0000007499","Perfluorononan-1-oic-acid and its sodium and ammonium salts"]
[{"$f":"Translator!B3123","v":"Nitrobenzene"},"98-95-3","2015-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3365","v":"Manufacture of other substances"},null,null,null,"100.002.469",null,null,null,null,"E2015","L00000004797","Nitrobenzene"]
[{"$f":"Translator!B3124","v":"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)"},"36437-37-3","2015-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3366","v":"UV stabilizer in coatings, plastics, rubber and cosmetics "},{"$f":"Translator!$B3371","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},null,null,"100.048.200",null,null,null,null,"E2017","L00000053888","2-(2H-Benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol"]
[{"$f":"Translator!B3125","v":"1,3-propanesultone"},"1120-71-4","2015-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3367","v":"Intermediate for the production of fine and bulk chemicals, electrolyte for lithium ion batteries "},null,null,null,"100.013.017",null,null,null,null,"E2015","L00000016586","1,3-Propanesultone"]
[{"$f":"Translator!B3126","v":"2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)"},"3864-99-1","2015-12-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3368","v":"UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika "},{"$f":"Translator!$B3372","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},null,null,"100.021.259",null,null,null,null,"E2015","L00000025402","2,4-Di-tert-butyl-6-(5-chlorobenzotriazol-2-yl)phenol"]
[{"$f":"Translator!B3127","v":"Benzo[def]chrysene (Benzo[a]pyrene)"},"50-32-8","2016-06-20","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3369","v":"Benzo[a]pyrene is not registered. The substance is not normally manufactured, but can be an ingredient or contamination of another substance. "},null,null,null,"100.000.026",null,null,null,null,"E2016","L00000001642","Benzo[a]pyrene"]
[{"$f":"Translator!B3128","v":"4-Heptylphenol, branched and linear (4-HPbl)"},"-","2017-01-12","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3370","v":"Monomer for the preparation of polymers"},null,null,null,"100.244.604",null,null,null,null,"E2017",null,null,"LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3129","v":"Phenol, heptyl derivs."},"72624-02-3",null,"D",null,null,null,null,null,"100.069.745",null,null,null,null,null,"LG0000007719","Phenol, heptyl derivs.","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3130","v":"4-heptylphenol "},"1987-50-4",null,"D",null,null,null,null,null,"100.016.239",null,null,null,null,null,"LG0000007719","4-heptylphenol","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3131","v":"Phenol, 4-(1,1-diethylpropyl)- "},"37872-24-5",null,"D",null,null,null,null,null,"100.287.902",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,1-  diethylpropyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3132","v":"Phenol, 4-(1,1-dimethylpentyl)-"},"30784-31-7",null,"D",null,null,null,null,null,"100.287.903",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,1-  dimethylpentyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3133","v":"Phenol, 4-(1,2,2-trimethylbutyl)-"},"911371-06-7",null,"D",null,null,null,null,null,"100.287.904",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,2,2-  trimethylbutyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3134","v":"Phenol, 4-(1,2-dimethylpentyl)-"},"854904-93-1",null,"D",null,null,null,null,null,"100.287.905",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,2-  dimethylpentyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3135","v":"Phenol, 4-(1,3,3-trimethylbutyl)- "},"911371-07-8",null,"D",null,null,null,null,null,"100.287.906",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,3,3-  trimethylbutyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3136","v":"Phenol, 4-(1,3-dimethylpentyl)-"},"71945-81-8",null,"D",null,null,null,null,null,"100.287.907",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,3-  dimethylpentyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3137","v":"Phenol, 4-(1,4-dimethylpentyl)-"},"857629-71-1",null,"D",null,null,null,null,null,"100.287.908",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,4-  dimethylpentyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3138","v":"Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-"},"861010-65-3",null,"D",null,null,null,null,null,"100.287.910",null,null,null,null,null,"LG0000007719","Phenol, 4-(1-  ethyl-2,2-  dimethylpropyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3139","v":"Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-"},"30784-27-1",null,"D",null,null,null,null,null,"100.291.922",null,null,null,null,null,"LG0000007719","Phenol, 4-(1-  ethyl-1,2-  dimethylpropyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3140","v":"Phenol, 4-(1-ethylpentyl)-"},"6465-74-3",null,"D",null,null,null,null,null,"100.287.912",null,null,null,null,null,"LG0000007719","4-Heptan-3-ylphenol","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3141","v":"Phenol, 4-(1-methylhexyl)-"},"6863-24-7",null,"D",null,null,null,null,null,"100.287.913",null,null,null,null,null,"LG0000007719","4-(Heptan-2-yl)phenol","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3142","v":"Phenol, 4-(1-propylbutyl)-"},"6465-71-0",null,"D",null,null,null,null,null,"100.287.914",null,null,null,null,null,"LG0000007719","4-Heptan-4-ylphenol","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3143","v":"Phenol, 4-(3-ethylpentyl)- "},"911370-98-4",null,"D",null,null,null,null,null,"100.287.915",null,null,null,null,null,"LG0000007719","Phenol, 4-(3-  ethylpentyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3144","v":"Phenol, 4-(3-methylhexyl)- "},"102570-52-5",null,"D",null,null,null,null,null,"100.287.916",null,null,null,null,null,"LG0000007719","4-(3-Methylhexyl)phenol","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3145","v":"Phenol, 4-(4-methylhexyl)-"},"1139800-98-8",null,"D",null,null,null,null,null,"100.287.917",null,null,null,null,null,"LG0000007719","Phenol, 4-(4-  methylhexyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3146","v":"Phenol, 4-(5-methylhexyl)-"},"100532-36-3",null,"D",null,null,null,null,null,"100.287.918",null,null,null,null,null,"LG0000007719","Phenol, 4-(5-  methylhexyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3147","v":"Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-"},"1824346-00-0",null,"D",null,null,null,null,null,"100.287.919",null,null,null,null,null,"LG0000007719","Phenol, 4-[2-  methyl-1-(1-  methylethyl)prop yl]-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3148","v":"4-(2,3-dimethylpentan-2-yl)phenol "},"861011-60-1",null,"D",null,null,null,null,null,"100.304.406",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,1,2-  trimethylbutyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3149","v":"4-(3-methylhexan-3-yl)phenol"},"30784-32-8",null,"D",null,null,null,null,null,"100.305.943",null,null,null,null,null,"LG0000007719","Phenol, 4-(1- ethyl-1- methylbutyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3150","v":"Phenol, 4-tert-heptyl-"},"288864-02-8",null,"D",null,null,null,null,null,"100.291.803",null,null,null,null,null,"LG0000007719","Phenol, 4-  tert  -  heptyl  -","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3151","v":"Phenol, 4-(1,1,3-trimethylbutyl)-"},"33104-11-9",null,"D",null,null,null,null,null,"100.287.901",null,null,null,null,null,"LG0000007719","Phenol, 4-(1,1,3-  trimethylbutyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3152","v":"Phenol, 4-(1,1,2,2-tetramethylpropyl)- "},"72861-06-4",null,"D",null,null,null,null,null,"100.287.899",null,null,null,null,null,"LG0000007719","Phenol,4- (1,1,2,2-  tetramethylpropy l)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3153","v":"Phenol, 4-(1-ethyl-3-methylbutyl)-"},"854904-92-0",null,"D",null,null,null,null,null,"100.287.911",null,null,null,null,null,"LG0000007719","Phenol, 4-(1-  ethyl-3-  methylbutyl)-","LG0000007719","4-heptylphenol, branched and linear"]
[{"$f":"Translator!B3154","v":"p-(1,1-dimethylpropyl)phenol"},"80-46-6","2017-01-12","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3373","v":"For the manufacture of chemicals and plastic products "},null,null,null,"100.001.165",null,null,null,null,"E2017","L00000003304","p-(1,1-dimethylpropyl)phenol"]
[{"$f":"Translator!B3155","v":"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"},"-","2017-01-12","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3374","v":"e.g. as corrosion inhibitor, lubricant, softener "},null,null,null,"100.244.606",null,null,null,null,"E2017",null,null,"Y00000021491","Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"]
[{"$f":"Translator!B3156","v":"Nonadecafluorodecanoic acid"},"335-76-2",null,"D",null,null,null,null,null,"100.005.819",null,null,null,null,null,"Y00000021491","Nonadecafluorodecanoic acid","Y00000021491","Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"]
[{"$f":"Translator!B3157","v":"Ammoniumnonadecafluordecanoat"},"3108-42-7",null,"D",null,null,null,null,null,"100.019.518",null,null,null,null,null,"Y00000021491","Ammonium nonadecafluorodecanoate","Y00000021491","Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"]
[{"$f":"Translator!B3158","v":"sodium nonadecafluorodecanoate "},"3830-45-3",null,"D",null,null,null,null,null,"100.249.275",null,null,null,null,null,"Y00000021491","Nonadecafluorodecanoic acid, sodium salt","Y00000021491","Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"]
[{"$f":"Translator!B3159","v":"Perfluorohexane-1-sulphonic acid and its salts"},"-","2017-07-07","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3375","v":"PFHxS is a known contamination in the production of PFOS. It can also be used as a replacement for PFOS"},null,null,null,"100.244.691",null,null,null,null,"E2017",null,null,"LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3160","v":"Potassium perfluorohexane-1-sulphonate"},"3871-99-6",null,"D",null,null,null,null,null,"100.021.268",null,null,null,null,null,"LG0000007820","Potassium perfluorohexane-1-sulphonate","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3161","v":"Perfluorohexane-1-sulphonic acid"},"355-46-4",null,"D",null,null,null,null,null,"100.005.989",null,null,null,null,null,"LG0000007820","Perfluorohexane-1-sulphonic acid","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3162","v":"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)"},"70225-16-0",null,"D",null,null,null,null,null,"100.067.672",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with 2,2'-iminobis[ethanol] (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3163","v":"Ammonium perfluorohexane-1-sulphonate"},"68259-08-5",null,"D",null,null,null,null,null,"100.063.173",null,null,null,null,null,"LG0000007820","Ammonium perfluorohexane-1-sulphonate","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3164","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)"},"341035-71-0",null,"D",null,null,null,null,null,"100.292.121",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3165","v":"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"341548-85-4",null,"D",null,null,null,null,null,"100.292.124",null,null,null,null,null,"LG0000007820","Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3166","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)"},"350836-93-0",null,"D",null,null,null,null,null,"100.292.165",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3167","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)"},"41184-65-0",null,"D",null,null,null,null,null,"100.292.448",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3168","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)"},"41242-12-0",null,"D",null,null,null,null,null,"100.292.451",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3169","v":"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)"},"421555-73-9",null,"D",null,null,null,null,null,"100.292.489",null,null,null,null,null,"LG0000007820","Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3170","v":"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic"},"421555-74-0",null,"D",null,null,null,null,null,"100.292.490",null,null,null,null,null,"LG0000007820","Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3171","v":"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"425670-70-8",null,"D",null,null,null,null,null,"100.292.521",null,null,null,null,null,"LG0000007820","Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3172","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)"},"55120-77-9",null,"D",null,null,null,null,null,"100.293.154",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3173","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt"},"70136-72-0",null,"D",null,null,null,null,null,"100.295.149",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3174","v":"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"213740-81-9",null,"D",null,null,null,null,null,"100.291.238",null,null,null,null,null,"LG0000007820","Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3175","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt"},"82382-12-5",null,"D",null,null,null,null,null,"100.296.541",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3176","v":"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)"},"866621-50-3",null,"D",null,null,null,null,null,"100.296.787",null,null,null,null,null,"LG0000007820","Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3177","v":"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"910606-39-2",null,"D",null,null,null,null,null,"100.297.036",null,null,null,null,null,"LG0000007820","Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3178","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"911027-68-4",null,"D",null,null,null,null,null,"100.297.038",null,null,null,null,null,"LG0000007820","Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3179","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"},"911027-69-5",null,"D",null,null,null,null,null,"100.297.039",null,null,null,null,null,"LG0000007820","Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)....","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3180","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)"},"92011-17-1",null,"D",null,null,null,null,null,"100.297.059",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3181","v":"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"928049-42-7",null,"D",null,null,null,null,null,"100.297.105",null,null,null,null,null,"LG0000007820","Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3182","v":"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1310480-24-0",null,"D",null,null,null,null,null,"100.289.998",null,null,null,null,null,"LG0000007820","Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3183","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1310480-27-3",null,"D",null,null,null,null,null,"100.289.999",null,null,null,null,null,"LG0000007820","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3184","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1310480-28-4",null,"D",null,null,null,null,null,"100.290.000",null,null,null,null,null,"LG0000007820","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3185","v":"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"1329995-45-0",null,"D",null,null,null,null,null,"100.290.065",null,null,null,null,null,"LG0000007820","Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-) (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3186","v":"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"1329995-69-8",null,"D",null,null,null,null,null,"100.290.066",null,null,null,null,null,"LG0000007820","Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-) (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3187","v":"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"144116-10-9",null,"D",null,null,null,null,null,"100.290.388",null,null,null,null,null,"LG0000007820","Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3188","v":"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1462414-59-0",null,"D",null,null,null,null,null,"100.290.419",null,null,null,null,null,"LG0000007820","Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3189","v":"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"153443-35-7",null,"D",null,null,null,null,null,"100.290.553",null,null,null,null,null,"LG0000007820","Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3190","v":"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"189274-31-5",null,"D",null,null,null,null,null,"100.291.027",null,null,null,null,null,"LG0000007820","Methanaminium, N,N,N-trimethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3191","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)"},"202189-84-2",null,"D",null,null,null,null,null,"100.291.150",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3192","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)"},"1187817-57-7",null,"D",null,null,null,null,null,"100.289.538",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with pyrrolidine (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3193","v":"Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"108427-55-0",null,"D",null,null,null,null,null,"100.289.351",null,null,null,null,null,"LG0000007820","Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3194","v":"1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid"},"108427-54-9",null,"D",null,null,null,null,null,"100.289.350",null,null,null,null,null,"LG0000007820","1-Butanaminium, N,N,N-tributyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3195","v":"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"1000597-52-3",null,"D",null,null,null,null,null,"100.288.877",null,null,null,null,null,"LG0000007820","Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3196","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)"},"72033-41-1",null,"D",null,null,null,null,null,"100.295.489",null,null,null,null,null,"LG0000007820","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","LG0000007820","Perfluorohexane-1-sulphonic acid and its salts"]
[{"$f":"Translator!B3197","v":"4,4'-isopropylidenediphenol (Bisphenol A)"},"80-05-7","2017-01-12","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3376","v":"For the production of epoxy and epoxy hardeners (industrial and professional applications), coating material, for the production of polymers such as polycarbonates and PVC; use in thermal paper (industrial, professional and consumer)"},null,null,null,"100.001.133",null,null,null,null,"E2017","L00000003260","Bisphenol A"]
[{"$f":"Translator!B3198","v":"Reaction products of 1,3,4-thiadiazolidine-2,5-dithione,\nformaldehyde and 4-heptylphenol, branched and linear (RP-HP)\n[with ≥0.1% w/w 4-heptylphenol, branched and linear (4-HPbl)1]"},"-","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3377","v":"Used in greases, lubricating greases and lubricating oils."},{"$f":"Translator!$B3384","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},null,null,"100.253.517",null,null,null,null,"E2018 / C2023",null,null,"Y00000021494","Reaction products of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and 4-heptylphenol, branched and linear (RP-HP)"]
[{"$f":"Translator!B3199","v":"Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs."},"1471311-26-8 ",null,"D",null,null,null,null,null,"100.226.747",null,null,null,null,"C 2023","Y00000021494","Formaldehyde, reaction products with phenol heptyl derivs. and 1,3,4-thiadiazolidine-2,5-dithione","Y00000021494","Reaction products of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and 4-heptylphenol, branched and linear (RP-HP)"]
[{"$f":"Translator!B3200","v":"Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine"},"93925-00-9",null,"D",null,null,null,null,null,"100.091.138",null,null,null,null,null,"Y00000021494","Formaldehyde, reaction products with branched and linear heptylpheno...","Y00000021494","Reaction products of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and 4-heptylphenol, branched and linear (RP-HP)"]
[{"$f":"Translator!B3201","v":"Cadmium carbonate"},"513-78-0","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3378","v":"Used as a pH regulator and in drinking water treatment products, laboratory chemicals, cosmetics and care products."},null,null,null,"100.007.427",null,null,null,null,"E2018","L00000000160","Cadmium-carbonate"]
[{"$f":"Translator!B3202","v":"Cadmium hydroxide, Cd(OH)2\n"},"21041-95-2","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3379","v":"The substance is used in the manufacture of electrical, electronic and optical equipment and in laboratory chemicals. "},null,null,null,"100.040.137",null,null,null,null,"E2018","L00000000581","Cadmium Hydroxide"]
[{"$f":"Translator!B3203","v":"Cadmium nitrate"},"10325-94-7","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3380","v":"Used in the manufacture of glass, ceramic and porcelain products and in laboratory chemicals. "},null,null,null,"100.030.633",null,null,null,null,"E2018","L00000000379","Cadmium-nitrate"]
[{"$f":"Translator!B3204","v":"Benz[a]anthracene"},"56-55-3","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3381","v":"Is not normally produced, but is a component or contamination of other substances."},null,null,null,"100.000.255",null,null,null,null,"E2018","L00000001924","benz[a]anthracene"]
[{"$f":"Translator!B3205","v":"Chrysene"},"218-01-9","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3382","v":"Is not normally produced, but is a component or contamination of other substances."},null,null,null,"100.005.386",null,null,null,null,"E2018","L00000008416","Chrysene"]
[{"$f":"Translator!B3206","v":"1,6,7,8,9,14,15,16,17,17,18,18-\nDodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane\nPlus”TM) [covering any of its individual anti- and syn-isomers or any combination\nthereof]"},"-","2018-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3383","v":"Used as flame retardant in adhesives, sealants and binders."},null,null,null,"100.253.516",null,null,null,null,"E2018",null,null,"Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane Plus”™)"]
[{"$f":"Translator!B3207","v":"(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene"},"135821-03-3",null,"D",null,null,null,null,null,"100.287.892",null,null,null,null,null,"Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1*6,9*.0*2,13*.0*5,10*]octadeca-7,15-diene","Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane Plus”™)"]
[{"$f":"Translator!B3208","v":"1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene"},"13560-89-9",null,"D",null,null,null,null,null,"100.033.575",null,null,null,null,null,"Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene","Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane Plus”™)"]
[{"$f":"Translator!B3209","v":"(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene"},"135821-74-8",null,"D",null,null,null,null,null,"100.287.893",null,null,null,null,null,"Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1*6,9*.0*2,13*.0*5,10*]octadeca-7,15-diene","Y00000020679","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane Plus”™)"]
[{"$f":"Translator!B3210","v":"rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene"},"-",null,"D",null,null,null,null,null,"100.253.518"]
[{"$f":"Translator!B3211","v":"rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene"},"-",null,"D",null,null,null,null,null,"100.253.519"]
[{"$f":"Translator!B3212","v":"Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)"},"552-30-7","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3385","v":"Used in the manufacture of esters and polymers."},null,null,null,"100.008.190",null,null,null,null,"E2018","L00000011463","Benzene-1,2,4-tricarboxylic acid 1,2-anhydride"]
[{"$f":"Translator!B3213","v":"Dicyclohexyl phthalate (DCHP)"},"84-61-7","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3386","v":"Used in plastisol, PVC, rubber and plastic articles. A further use is also as a phlegmatiser and dispersing agent for formulations of organic peroxides."},null,null,null,"100.001.405",null,null,null,null,"E2018","L00000003576","Dicyclohexyl-phthalate"]
[{"$f":"Translator!B3214","v":"Octamethylcyclotetrasiloxane (D4)"},"556-67-2","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3387","v":"Used in washing and cleaning products, polishes and waxes and cosmetics and personal care products."},null,null,null,"100.008.307",null,null,null,null,"E2018","L00000011592","octamethylcyclotetrasiloxane"]
[{"$f":"Translator!B3215","v":"Decamethylcyclopentasiloxane (D5)"},"541-02-6","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3388","v":"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products, textile treatment products and dyes."},null,null,null,"100.007.969",null,null,null,null,"E2018","L00000011211","Decamethylcyclopentasiloxane"]
[{"$f":"Translator!B3216","v":"Dodecamethylcyclohexasiloxane (D6)"},"540-97-6","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3389","v":"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products."},null,null,null,"100.007.967",null,null,null,null,"E2018","L00000011209","Dodecamethylcyclohexasiloxane"]
[{"$f":"Translator!B3217","v":"Lead"},"7439-92-1","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3390","v":"Used in metals, welding and soldering products, metal surface treatment products, and polymers."},null,null,null,"100.028.273",null,null,null,null,"E2018","L00000000307","Lead"]
[{"$f":"Translator!B3218","v":"Disodium octaborate"},"12008-41-2","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3391","v":"Used in anti-freeze products, heat transfer fluids, lubricants and greases, and washing and cleaning products."},null,null,null,"100.031.388",null,null,null,null,"E2018","L00000036591","Disodium-octaborate"]
[{"$f":"Translator!B3219","v":"Benzo[ghi]perylene"},"191-24-2","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3392","v":"Not registered under REACH. Normally not produced intentionally but rather occurs as a constituent or impurity in other substances."},null,null,null,"100.005.350",null,null,null,null,"E2018","L00000008380","Benzo(ghi)perylene"]
[{"$f":"Translator!B3220","v":"Terphenyl hydrogenated"},"61788-32-7","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3393","v":"Used as a plastic additive, solvent, in coatings/inks, in adhesives and sealants, and heat transfer fluids."},null,null,null,"100.057.225",null,null,null,null,"E2018","L00000062993","Terphenyl, hydrogenated"]
[{"$f":"Translator!B3221","v":"Ethylenediamine (EDA)"},"107-15-3","2018-06-27","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3394","v":"Used in adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, pH regulators and water treatment products."},null,null,null,"100.003.154",null,null,null,null,"E2018","L00000005650","Ethylenediamine"]
[{"$f":"Translator!B3222","v":"2,2-bis(4'-hydroxyphenyl)-4-methylpentane"},"6807-17-6","2019-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3395","v":"-"},null,null,null,"100.100.362",null,null,null,null,"E2019","L00000106261","4,4-isobutylethylidenediphenol"]
[{"$f":"Translator!B3223","v":"Benzo[k]fluoranthene"},"207-08-9","2019-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3396","v":"Binder for refractory material"},null,null,null,"100.005.379",null,null,null,null,"E2019","L00000008409","Benzo[k]fluoranthene"]
[{"$f":"Translator!B3224","v":"Fluoranthene"},"206-44-0","2019-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3397","v":"Binder for refractory material"},null,null,null,"100.005.376",null,null,null,null,"E2019","L00000008406","Fluoranthene"]
[{"$f":"Translator!B3225","v":"Phenanthrene"},"85-01-8","2019-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3398","v":"Binder for refractory material"},null,null,null,"100.001.437",null,null,null,null,"E2019","L00000003616","Phenanthrene"]
[{"$f":"Translator!B3226","v":"Pyrene"},"129-00-0","2019-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3399","v":"Used as a transported intermediate for the manufacture of fine chemicals."},null,null,null,"100.004.481",null,null,null,null,"E2019","L00000007373","Pyrene"]
[{"$f":"Translator!B3227","v":"1,7,7-trimethyl-3-(phenylmethylene)bicyclo[2.2.1]heptan-2-one "},"15087-24-8","2019-01-15","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3400","v":"UV filters in sunscreen and other cosmetics"},null,null,null,"100.035.567",null,null,null,null,"E2019","L00000040956","(+-)-1,7,7-Trimethyl-3-(phenylmethylene)bicyclo(2.2.1)heptan-2-one"]
[{"$f":"Translator!B3228","v":"2-Methoxyethyl acetate"},"110-49-6","2019-07-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3401","v":"Solvent  for  gums,  resins,  waxes,  and  oils  and  in  the \nmanufacture of semiconductors, textile printing and photographic films. paints, lacquers, stains, inks, surface coatings, \nsilk-screen  printing,  photographic  and  photo  lithographic  processes,  semiconductors,  textile, \nleather, hydraulic fluids, jet fuel, varnishes, paper, acetate adhesives, nitrocellulose, cellulose \nacetate,  gums,  resins,  waxes,  and  oils,  textile  printing  and  dry-cleaning.  Technical  functions \ninclude solvent, drying retarder, and anti-icing additive, viscosity decreasing agent.\n"},null,null,null,"100.003.431",null,null,null,null,"E2019","L00000006052","2-methoxyethyl acetate"]
[{"$f":"Translator!B3229","v":"Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"},"-","2019-07-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3402","v":"Primarily used as an antioxidant to stabilise polymers."},null,null,null,"100.264.200",null,null,null,null,"E2019",null,null,"Y00000021496","Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"]
[{"$f":"Translator!B3230","v":"Tris(nonylphenyl) phosphite"},"26523-78-4",null,"D",null,null,null,null,null,"100.043.402",null,null,null,null,null,"Y00000021496","Tris(nonylphenyl)phosphite","Y00000021496","Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"]
[{"$f":"Translator!B3231","v":"tris(4-nonylphenyl, branched) phosphite"},"-",null,"D",null,null,null,null,null,"100.242.308",null,null,null,null,null,null,null,"Y00000021496","Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"]
[{"$f":"Translator!B3232","v":"Phenol, 4-nonyl-, phosphite (3:1)"},"3050-88-2",null,"D",null,null,null,null,null,"100.106.542",null,null,null,null,null,"Y00000021496","Phenol, 4-nonyl-, phosphite (3:1)","Y00000021496","Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"]
[{"$f":"Translator!B3233","v":"Phenol, p-isononyl-, phosphite (3:1)"},"31631-13-7",null,"D",null,null,null,null,null,"100.287.920",null,null,null,null,null,"Y00000021496","Phenol, p-isononyl-, phosphite(3:1)","Y00000021496","Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"]
[{"$f":"Translator!B3234","v":"Phenol, p-sec-nonyl-, phosphite"},"106599-06-8",null,"D",null,null,null,null,null,"100.287.898",null,null,null,null,null,"Y00000021496","Phenol, p-sec-nonyl-, phosphite","Y00000021496","Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"]
[{"$f":"Translator!B3235","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides (covering any of their individual isomers and combinations thereof)"},"-","2019-07-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3403","v":"Processing aid in the production of fluorinated polymers."},null,null,null,"100.273.068",null,null,null,null,"E2019",null,null,"Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3236","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride"},"2062-98-8",null,"D",null,null,null,null,null,"100.016.522",null,null,null,null,null,"Y00000021497","Perfluoro(2-methyl-3-oxahexanoyl) fluoride","Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3237","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid"},"13252-13-6",null,"D",null,null,null,null,null,"100.032.928",null,null,null,null,null,"Y00000021497","Perfluoro-2-methyl-3-oxahexanoic acid","Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3238","v":"Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate"},"67118-55-2",null,"D",null,null,null,null,null,"100.060.507",null,null,null,null,null,"Y00000021497","Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3239","v":"Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate"},"62037-80-3",null,"D",null,null,null,null,null,"100.124.803",null,null,null,null,null,"Y00000021497","Ammonium perfluoro-2-methyl-3-oxahexanoate","Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3240","v":"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-"},"75579-39-4",null,"D",null,null,null,null,null,"100.300.930",null,null,null,null,null,"Y00000021497","(2R)-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoic acid","Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3241","v":"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-"},"75579-40-7",null,"D",null,null,null,null,null,"100.300.931",null,null,null,null,null,"Y00000021497","(2S)-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoic acid","Y00000021497","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides"]
[{"$f":"Translator!B3242","v":"4-tert-butylphenol"},"98-54-4","2019-07-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3404","v":"Mainly \nused in the phenolic/epoxy resin industry and is only used as an intermediate /in polymers\nUsed in coating products, polymers, adhesives, sealants and for the synthesis of other substances.\n"},null,null,null,"100.002.436",null,null,null,null,"E2019","L00000004753","4-tert-butylphenol"]
[{"$f":"Translator!B3243","v":"Diisohexyl phthalat"},"71850-09-4","2020-01-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3405","v":"Diisohexyl phthalate is a component (the branched form) of 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear (EC 271-093-5; CAS 68515-50-4). There are indications for potential use of the substances in the same types of applications (e.g. as sealant, plasticiser in polymers etc)."},null,null,null,"100.069.152",null,null,null,null,"E2020","L00000075036","diisohexyl phthalate"]
[{"$f":"Translator!B3244","v":"2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon"},"119313-12-1","2020-01-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3406","v":"2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone is used\nfor the production of printing inks and surface coating based on based on acrylates polymerized by UV radiation.\n"},null,null,null,"100.100.600",null,null,null,null,"E2020","L00000106493","2-Benzyl-2-dimethylamino-4-morpholinobutyrophenone"]
[{"$f":"Translator!B3245","v":"Perfluorobutane sulfonic acid (PFBS) and its salts "},"-","2020-01-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3407","v":"Used as a catalyst/ additive/reactant in polymer manufacture and in chemical synthesis. It is also used as a flame retardant in polycarbonate (for electronic equipment)."},null,null,null,"100.282.094",null,null,null,null,"E2020 /E 2023",null,null,"Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3246","v":"Potassium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate"},"29420-49-3",null,"D",null,null,null,null,null,"100.045.092",null,null,null,null,"E 2023","Y00000021308","1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, potassium salt","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3247","v":"1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonic acid"},"375-73-5",null,"D",null,null,null,null,null,"100.006.176",null,null,null,null,"E 2023","Y00000021308","1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulphonic acid","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3248","v":"bis(4-t-butylphenyl)iodonium perfluorobutanesulfonate"},"194999-85-4",null,"D",null,null,null,null,null,"100.103.091",null,null,null,null,"E 2023","Y00000021308","Bis(4-tert-butylphenyl)iodanium nonafluorobutane-1-sulfonate","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3249","v":"tetrabutyl-phosphonium nonafluoro-butane-1-sulfonate"},"220689-12-3",null,"D",null,null,null,null,null,"100.103.965",null,null,null,null,"E 2023","Y00000021308","tetrabutyl-phosphonium nonafluoro-butane-1-sulfonate","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3250","v":"dimethyl(phenyl)sulfanium perfluorobutanesulfonate"},"220133-51-7",null,"D",null,null,null,null,null,"100.104.333",null,null,null,null,"E 2023","Y00000021308","Sulfonium, dimethylphenyl-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonic acid(1:1)","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3251","v":"Ammonium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate"},"68259-10-9",null,"D",null,null,null,null,null,"100.063.175",null,null,null,null,"E 2023","Y00000021308","1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, ammonium salt","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3252","v":"Triphenylsulfanium perfluorobutane sulfonate"},"144317-44-2",null,"D",null,null,null,null,null,"100.105.187",null,null,null,null,"E 2023","Y00000021308","Sulfonium, triphenyl-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonic acid(1:1)","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3253","v":"N,N,N-triethylethanaminium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate"},"25628-08-4",null,"D",null,null,null,null,null,"100.149.398",null,null,null,null,"E 2023","Y00000021308","N,N,N,-Triethylethanaminium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3254","v":"magnesium perfluorobutanesulfonate"},"507453-86-3",null,"D",null,null,null,null,null,"100.197.427",null,null,null,null,"E 2023","Y00000021308","Magnesium perfluorobutane sulfonate","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3255","v":"lithium perfluorobutanesulfonate"},"131651-65-5",null,"D",null,null,null,null,null,"100.197.428",null,null,null,null,"E 2023","Y00000021308","1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, lithium salt (1:1)","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3256","v":"morpholinium perfluorobutanesulfonate"},"503155-89-3",null,"D",null,null,null,null,null,"100.197.431",null,null,null,null,"E 2023","Y00000021308","Morpholinium perfluorobutane sulfonate","Y00000021308","Perfluorobutane sulfonic acid and its salts"]
[{"$f":"Translator!B3257","v":"1-(4-butoxy-1-naphthalenyl)tetrahydrothiophenium 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate"},"-",null,"D",null,null,null,null,null,"100.104.884",null,null,null,null,"E 2023"]
[{"$f":"Translator!B3258","v":"2-methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-one"},"71868-10-5","2020-01-16","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3408","v":"2-Methyl-1- (4-methylthiophenyl) -2-morpholinopropan-1-one is used as a photoinitiator in the manufacture of formulations and (outer) packaging, coatings, adhesives, printing inks, fiber sizes."},null,null,null,"100.100.260",null,null,null,null,"E2020","L00000106158","1-Propanone, 2-methyl-1-[4-(methylthio)phenyl]-2-(4-morpholinyl)-"]
[{"$f":"Translator!B3259","v":"1-vinylimidazole"},"1072-63-5","2020-06-25","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3409","v":"ECHA has no public registered data indicating whether or in which chemical products the substance might be used."},null,null,null,"100.012.739",null,null,null,null,"E 2023","L00000016299","1-vinylimidazole"]
[{"$f":"Translator!B3260","v":"2-methylimidazole"},"693-98-1","2020-06-25","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3410","v":"ECHA has no public registered data indicating whether or in which chemical products the substance might be used."},null,null,null,"100.010.697",null,null,null,null,"E 2023","L00000014133","2-Methylimidazole"]
[{"$f":"Translator!B3261","v":"Butyl 4-hydroxybenzoate"},"94-26-8","2020-06-25","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3411","v":"This substance is used in the following products: cosmetics and personal care products and pharmaceuticals.\nOther release to the environment of this substance is likely to occur from: indoor use as processing aid"},null,null,null,"100.002.008",null,null,null,null,"E 2023","L00000004368","4-(Butoxycarbonyl)phenol"]
[{"$f":"Translator!B3262","v":"Dibutylbis(pentane-2,4-dionato-O,O')tin"},"22673-19-4","2020-06-25","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3412","v":"This substance is used in the following products: adhesives and sealants."},null,null,null,"100.042.031",null,null,null,null,"E 2023","L00000046564","Dibutylbis(pentane-2,4-dionato-O,O')tin"]
[{"$f":"Translator!B3263","v":"Bis(2-(2-methoxyethoxy)ethyl) ether"},"143-24-8","2021-01-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3413","v":"Bis(2-(2-methoxyethoxy)ethyl)ether is used in inks and toners as a solvent or extractant. Industrial use as a gas absorption liquid, solvent in synthesis reactions or as an extractant."},null,null,null,"100.005.086",null,null,null,null,"E2021","L00000008063","Bis(2-(2-methoxyethoxy)ethyl)ether"]
[{"$f":"Translator!B3264","v":"Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"},"-","2021-01-19","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3414","v":"The main ingredient dioctyltin dilaurate is used in adhesives and sealants and in the manufacture of plastic and rubber tyres"},null,null,null,"100.308.020",null,null,null,null,"E2021",null,null,"Y00000023153","Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"]
[{"$f":"Translator!B3265","v":"Dioctyltin dilaurate"},"3648-18-8",null,"D",null,null,null,null,null,100020804,null,null,null,null,null,"Y00000023153","Dioctyltin dilaurate","Y00000023153","Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"]
[{"$f":"Translator!B3266","v":"dioctyltin dilaurate; stannane, dioctyl-, bis(coco acyloxy) derivs."},"-",null,"D",null,null,null,null,null,100278923,null,null,null,null,null,null,null,"Y00000023153","Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"]
[{"$f":"Translator!B3267","v":"Stannane, dioctyl-, bis(coco acyloxy) derivs."},"91648-39-4",null,"D",null,null,null,null,null,100095331,null,null,null,null,null,"Y00000023153","Stannane, dioctyl-, bis(coco acyloxy) derivs.","Y00000023153","Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"]
[{"$f":"Translator!B3268","v":"Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"},"-","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3415","v":"Preparation of lubricant additive materials and of fuel system cleaners."},null,null,null,100311974,null,null,null,null,"E2021",null,null,"Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3269","v":"Phenol, dodecyl-, branched"},"21158-58-5 ",null,"D",null,null,null,null,null,100100072,null,null,null,null,null,null,null,"Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3270","v":"Phenol, (tetrapropenyl) derivatives"},"74499-35-7 ",null,"D",null,null,null,null,null,100109748,null,null,null,null,null,"Y00000023870","Phenol, (tetrapropenyl) derivs.","Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3271","v":"Phenol, 4-dodecyl, branched"},"210555-94-5 ",null,"D",null,null,null,null,null,100167758,null,null,null,null,null,"Y00000023870","Phenol, 4-dodecyl-, branched","Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3272","v":"4-isododecylphenol"},"27459-10-5",null,"D",null,null,null,null,null,100278034,null,null,null,null,null,"Y00000023870","Phenol, 4-isododecyl-","Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3273","v":"Phenol, tetrapropylene-"},"57427-55-1 ",null,"D",null,null,null,null,null,100278036,null,null,null,null,null,"Y00000023870","Phenol, tetrapropylene","Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3274","v":"Phenol, 4-isododecyl-"},"27147-75-7 ",null,"D",null,null,null,null,null,100124888,null,null,null,null,null,"Y00000023870","Phenol, 4-isododecyl-","Y00000023870","Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"]
[{"$f":"Translator!B3275","v":"orthoboric acid, sodium salt"},"-","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3416","v":"Not registered under REACH. May be used as solvent and corrosion inhibitor. "},null,null,null,100331485,null,null,null,null,"E2021",null,null,"Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3276","v":"boric acid (H3BO3), sodium salt, hydrate"},"25747-83-5 ",null,"D",null,null,null,null,null,100331486,null,null,null,null,null,"Y00000023872","boric acid (H3BO3), sodium salt, hydrate","Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3277","v":"Boric acid (H3BO3), disodium salt"},"22454-04-2 ",null,"D",null,null,null,null,null,100291297,null,null,null,null,null,"Y00000023872","Boric acid (H3BO3), disodium salt","Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3278","v":"Trisodium orthoborate"},"\t14312-40-4 ",null,"D",null,null,null,null,null,100034760,null,null,null,null,null,"Y00000023872","trisodium orthoborate","Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3279","v":"Boric acid, sodium salt"},"1333-73-9 ",null,"D",null,null,null,null,null,100014186,null,null,null,null,null,"Y00000023872","Boric acid, sodium salt","Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3280","v":"Orthoboric acid, sodium salt"},"13840-56-7 ",null,"D",null,null,null,null,null,100034132,null,null,null,null,null,"Y00000023872","Orthoboric acid, sodium salt","Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3281","v":"Boric acid (H3BO3), sodium salt (1:1) "},"14890-53-0 ",null,"D",null,null,null,null,null,100290470,null,null,null,null,null,"Y00000023872","Boric acid (H3BO3), monosodium salt","Y00000023872","orthoboric acid, sodium salt"]
[{"$f":"Translator!B3282","v":"Medium-chain chlorinated paraffins (MCCP)"},"-","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3417","v":"Flame retardants, plasticising additives in plastics, sealants, rubber and textiles"},null,null,null,100323845,null,null,null,null,"E2021",null,null,"Y00000023869","Medium-chain chlorinated paraffins (MCCP)"]
[{"$f":"Translator!B3283","v":"Alkanes, C14-16, chloro"},"1372804-76-6 ",null,"D",null,null,null,null,null,100319589,null,null,null,null,null,"Y00000023869","Alkanes, C14-16, chloro","Y00000023869","Medium-chain chlorinated paraffins (MCCP)"]
[{"$f":"Translator!B3284","v":"Alkanes, C14-17, chloro"},"85535-85-9 ",null,"D",null,null,null,null,null,100079497,null,null,null,null,null,"Y00000023869","Alkanes, C14-17, chloro","Y00000023869","Medium-chain chlorinated paraffins (MCCP)"]
[{"$f":"Translator!B3285","v":"di-, tri- and tetrachlorotetradecane "},"-",null,"D",null,null,null,null,null,100275290,null,null,null,null,null,null,null,"Y00000023869","Medium-chain chlorinated paraffins (MCCP)"]
[{"$f":"Translator!B3286","v":"Tetradecane, chloro derivs."},"198840-65-2 ",null,"D",null,null,null,null,null,100319590,null,null,null,null,null,"Y00000023869","Alkanes, tetrachloro, derivatives","Y00000023869","Medium-chain chlorinated paraffins (MCCP)"]
[{"$f":"Translator!B3287","v":"glutaral"},"111-30-8","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3418","v":"Biocides, leather tanning, x-ray film processing, cosmetics."},null,null,null,100003506,null,null,null,null,"E2021","L00000006159","glutaraldehyde"]
[{"$f":"Translator!B3288","v":"4,4'-(1-methylpropylidene)bisphenol"},"77-40-7","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3419","v":"Not registered under REACH. May be used in manufacture of phenolic and polycarbonate resin. "},null,null,null,100000933,null,null,null,null,"E2021","L00000002962","4,4'-(1-Methylpropylidene)bisphenol"]
[{"$f":"Translator!B3289","v":"2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"},"-","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3420","v":"Cleaning agents, cosmetics, in scented articles, polishes and wax blends."},null,null,null,100313493,null,null,null,null,"E2021",null,null,"Y00000023866","2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"]
[{"$f":"Translator!B3290","v":"(2R)-3-(4-tert-butylphenyl)-2-methylpropanal "},"75166-31-3 ",null,"D",null,null,null,null,null,100313491,null,null,null,null,null,"Y00000023866","(2R)-3-(4-tert-butylphenyl)-2-methylpropanal","Y00000023866","2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"]
[{"$f":"Translator!B3291","v":"2-(4-tert-butylbenzyl)propionaldehyde"},"80-54-6 ",null,"D",null,null,null,null,null,100001173,null,null,null,null,null,"Y00000023866","2-(4-Tert-butylbenzyl)propionaldehyde","Y00000023866","2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"]
[{"$f":"Translator!B3292","v":"(2S)-3-(4-tert-butylphenyl)-2-methylpropanal "},"75166-30-2 ",null,"D",null,null,null,null,null,100313492,null,null,null,null,null,"Y00000023866","(2S)-3-(4-tert-butylphenyl)-2-methylpropanal","Y00000023866","2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"]
[{"$f":"Translator!B3293","v":"2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"},"-","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},null,null,null,null,100316784,null,null,null,null,"E2021",null,null,"Y00000023867","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"]
[{"$f":"Translator!B3294","v":"2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) "},"\t36483-57-5 ",null,"D",null,{"$f":"Translator!$B3421","v":"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate."},null,null,null,100048218,null,null,null,null,null,"Y00000023867","1-Propanol, 2,2-dimethyl-, tribromo deriv.","Y00000023867","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"]
[{"$f":"Translator!B3295","v":"3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)"},"\t1522-92-5",null,"D",null,{"$f":"Translator!$B3422","v":"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate."},null,null,null,100151139,null,null,null,null,null,"Y00000023867","1-PROPANOL, 3-BROMO-2,2-BIS(BROMOETHYL)-","Y00000023867","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"]
[{"$f":"Translator!B3296","v":"2,2-bis(bromomethyl)propane-1,3-diol (BMP)"},"3296-90-0",null,"D",null,{"$f":"Translator!$B3423","v":"BMP: manufacture of polymer resins and in one component foam (OCPF) application."},null,null,null,100019971,null,null,null,null,null,"Y00000023867","Pentaerythritol dibromide","Y00000023867","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"]
[{"$f":"Translator!B3297","v":"2,3-dibromo-1-propanol (2,3-DBPA) "},"96-13-9 ",null,"D",null,{"$f":"Translator!$B3424","v":"DBPA: registered as an intermediate."},null,null,null,100002256,null,null,null,null,null,"Y00000023867","1-Propanol, 2,3-dibromo-","Y00000023867","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"]
[{"$f":"Translator!B3298","v":"1,4-dioxane"},"123-91-1","2021-07-08","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3425","v":"Solvent."},null,null,null,100004239,null,null,null,null,"E2021","L00000007076","1,4-Dioxane"]
[{"$f":"Translator!B3299","v":"tris(2-methoxyethoxy)vinylsilane"},"1067-53-4","2022-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3426","v":"Rubbers, plastics, sealants"},null,null,null,100012668,null,null,null,null,"E 2022","L00000016223","Tris(2-methoxyethoxy)vinylsilane"]
[{"$f":"Translator!B3300","v":"S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261"},"255881-94-8","2022-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3427","v":"Lubricants, greases"},null,null,null,100100373,null,null,null,null,"E 2022","L00000164283","Phosphorodithioic acid, mixed O,O-bis(2-ethylhexyl and iso-Bu and iso-Pr) S-[3a,4,5,6,7,7a-hexahydro-4,7-methano-1H-inden-5(or 6)-yl] esters"]
[{"$f":"Translator!B3301","v":"6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol"},"119-47-1","2022-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3428","v":"Rubbers, lubricants, adhesives, inks, fuels, gaskets"},null,null,null,100003934,null,null,null,null,"E 2022","L00000006697","6,6'-Di-tert-butyl-2,2'-methylenedi-p-cresol"]
[{"$f":"Translator!B3302","v":"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"},"-","2022-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3429","v":"Cosmetics"},null,null,null,100325067,null,null,null,null,"E 2022",null,null,"Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3303","v":"(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"1782069-81-1 ",null,"D",null,null,null,null,null,100332682,null,null,null,null,null,"Y00000024251","(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3304","v":"(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"95342-41-9 ",null,"D",null,null,null,null,null,100347637,null,null,null,null,null,"Y00000024251","(1R,3E,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3305","v":"(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"852541-25-4 ",null,"D",null,null,null,null,null,100347638,null,null,null,null,null,"Y00000024251","(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3306","v":"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one"},"\t36861-47-9 ",null,"D",null,null,null,null,null,100048386,null,null,null,null,null,"Y00000024251","(1)-1,7,7-Trimethyl-3-((4-methylphenyl)methylene)bicyclo(2.2.1)heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3307","v":"(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"741687-98-9 ",null,"D",null,null,null,null,null,100347643,null,null,null,null,null,"Y00000024251","(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3308","v":"(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"852541-30-1 ",null,"D",null,null,null,null,null,100347647,null,null,null,null,null,"Y00000024251","(1S,3E,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3309","v":"(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"852541-21-0 ",null,"D",null,null,null,null,null,100347640,null,null,null,null,null,"Y00000024251","(1R,3Z,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one","Y00000024251","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"]
[{"$f":"Translator!B3342","v":"N-(hydroxymethyl)acrylamide"},"924-42-5","2022-06-10","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3430","v":"ECHA has no public registered data indicating whether or in which chemical products the substance might be used."},null,null,null,"100.011.913",null,null,null,null,"E 2023","L00000015426","N-(hydroxymethyl)acrylamide"]
[{"$f":"Translator!B3310","v":"1,1'-[ethane-1,2-diylbisoxy]bis[2,4,6-tribromobenzene"},"37853-59-1","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3431","v":"While the substance itself is not registered under REACH, identification as an SVHC can be seen as a measure to avoid future regrettable substitution. "},null,null,null,"100.048.794",null,null,null,null,"E 2023","L00000054490","1,1'-[Ethane-1,2-diylbisoxy]bis[2,4,6-tribromobenzene]"]
[{"$f":"Translator!B3311","v":"2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol"},"79-94-7","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3432","v":"As a reactive flame retardant and as an additive flame retardant in the manufacture of polymer resins, in products such as epoxy coated circuit boards, printed circuit boards, paper and textiles."},null,null,null,"100.001.125",null,null,null,null,"E 2023","L00000003251","TBBA"]
[{"$f":"Translator!B3312","v":"4,4'-sulphonyldiphenol"},"80-09-1","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3433","v":"In the manufacture of: pulp, paper and paper products, textile, leather or fur and chemicals."},null,null,null,"100.001.137",null,null,null,null,"E 2023","L00000003268","4,4'-Sulfonyldiphenol"]
[{"$f":"Translator!B3313","v":"Barium diboron tetraoxide"},"13701-59-2","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3434","v":"In paints and coatings."},null,null,null,"100.033.824",null,null,null,null,"E 2023","L00000039137","Barium-diboron-tetraoxide"]
[{"$f":"Translator!B3314","v":"Bis(2-ethylhexyl) tetrabromophthalate covering any of the individual isomers and/or combinations thereof"},"- ","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3435","v":"As a flame retardant and as a plasticiser for flexible polyvinylchloride and for use in wire and cable insulation, film and sheeting, carpet backing, coated fabrics, wall coverings and adhesives."},null,null,null,"100.362.813",null,null,null,null,"E 2023",null,null,"Y00000024897","bis(2-ethylhexyl) tetrabromophthalate covering any of the individual isomers and/or combinations thereof"]
[{"$f":"Translator!B3315","v":"Bis(2-ethylhexyl) tetrabromophthalate"},"26040-51-7",null,"D",null,null,null,null,null,"100.043.099",null,null,null,null,"E 2023","Y00000024897","Bis(2-ethylhexyl) tetrabromophthalate","Y00000024897","bis(2-ethylhexyl) tetrabromophthalate covering any of the individual isomers and/or combinations thereof"]
[{"$f":"Translator!B3316","v":"Isobutyl 4-hydroxybenzoate"},"4247-02-3","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3435","v":"As a flame retardant and as a plasticiser for flexible polyvinylchloride and for use in wire and cable insulation, film and sheeting, carpet backing, coated fabrics, wall coverings and adhesives."},null,null,null,"100.022.008",null,null,null,null,"E 2023","L00000026178","Benzoic acid, 4-hydroxy-, 2-methylpropyl ester (9CI)"]
[{"$f":"Translator!B3317","v":"Melamine"},"108-78-1","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3436","v":"In the manufacture of substances and in the following products: coating products, fillers, putties, plasters, modelling clay and inks and toners."},null,null,null,"100.003.288",null,null,null,null,"E 2023","L00000005853","Melamine"]
[{"$f":"Translator!B3318","v":"Perfluoroheptanoic acid and its salts"},"- ","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3437","v":"In polymers and resins, coating products, adhesives and sealants, leather treatment products, laboratory chemicals."},null,null,null,"100.356.090",null,null,null,null,"E 2023","Y00000024896","Perfluoroheptanoic acid and its salts"]
[{"$f":"Translator!B3319","v":"Ammonium perfluoroheptanoate"},"6130-43-4",null,"D",null,null,null,null,null,"100.025.544",null,null,null,null,"E 2023","Y00000024896","Ammonium perfluoroheptanoate","Y00000024896","Perfluoroheptanoic acid and its salts"]
[{"$f":"Translator!B3320","v":"potassium perfluoroheptanoate"},"21049-36-5",null,"D",null,null,null,null,null,"100.361.353",null,null,null,null,"E 2023","Y00000024896","potassium perfluoroheptanoate","Y00000024896","Perfluoroheptanoic acid and its salts"]
[{"$f":"Translator!B3321","v":"Perfluoroheptanoic acid"},"375-85-9",null,"D",null,null,null,null,null,"100.006.181",null,null,null,null,"E 2023","Y00000024896","Perfluoroheptanoic acid","Y00000024896","Perfluoroheptanoic acid and its salts"]
[{"$f":"Translator!B3322","v":"Sodium perfluoroheptanoate"},"20109-59-5",null,"D",null,null,null,null,null,"100.039.548",null,null,null,null,"E 2023","Y00000024896","Sodium perfluoroheptanoate","Y00000024896","Perfluoroheptanoic acid and its salts"]
[{"$f":"Translator!B3323","v":"reaction mass of 2,2,3,3,5,5,6,6-octafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)morpholine and 2,2,3,3,5,5,6,6-octafluoro-4-(heptafluoropropyl)morpholine"},"- ","2023-01-17","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!$B3324","v":"Used in articles, by professional workers (widespread uses), in formulation or re-packing, at industrial sites and in manufacturing."},null,null,null,"100.105.055",null,null,null,null,"E 2023","Y00000024898","reaction mass of 2,2,3,3,5,5,6,6-octafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)morpholine and 2,2,3,3,5,5,6,6-octafluoro-4-(heptafluoropropyl)morpholine"]
[{"$f":"Translator!B3771","v":"Diphenyl(2,4,6-trimethylbenzoyl)phosphine oxide"},"75980-60-8       ","2023-06-14","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3773","v":"Inks and toners, coating products, photo-chemicals, polymers, adhesives and sealants and fillers, putties, plasters, modelling clay "},null,null,null,"100.071.211",null,null,null,null,"E 2023","L00000077096","Diphenyl(2,4,6-trimethylbenzoyl)phosphine oxide"]
[{"$f":"Translator!B3772","v":"Bis(4-chlorophenyl) sulphone"},"80-07-9","2023-06-14","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3774","v":"Manufacture of chemicals, plastic products and rubber products."},null,null,null,"100.001.135",null,null,null,null,"E 2023","L00000003264","Bis(4-chlorophenyl) sulfon"]
[{"$f":"Translator!B3810","v":"Oligomerisation and alkylation reaction products of 2-phenylpropene and phenol"},"- ","2024-01-23","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3816","v":"Adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, inks and toners and polymers."},null,null,null,100228163,null,null,null,null,"E 2024"]
[{"$f":"Translator!B3811","v":"Phenol, methylstyrenated"},"68512-30-1","2024-01-23","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},null,null,null,null,100064495,null,null,null,null,"E 2024"]
[{"$f":"Translator!B3812","v":"Bumetrizole (UV-326)"},"3896-11-5","2024-01-23","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3817","v":"Coating products, adhesives and sealants and washing and cleaning products."},null,null,null,100021315,null,null,null,null,"E 2024"]
[{"$f":"Translator!B3813","v":"2-(dimethylamino)-2-[(4-methylphenyl)methyl]-1-[4-(morpholin-4-yl)phenyl]butan-1-one"},"119344-86-4","2024-01-23","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3818","v":"Inks and toners, coating products."},null,null,null,100103524,null,null,null,null,"E 2024"]
[{"$f":"Translator!B3814","v":"2-(2H-benzotriazol-2-yl)-4-(1,1,3,3-tetramethylbutyl)phenol (UV-329)"},"3147-75-9","2024-01-23","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3819","v":"Air care products, coating products, adhesives and sealants, lubricants and greases, polishes and waxes and washing and cleaning products."},null,null,null,100019612,null,null,null,null,"E 2024"]
[{"$f":"Translator!B3815","v":"2,4,6-tri-tert-butylphenol"},"732-26-3","2024-01-23","D",{"$f":"Translator!$B$1892","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},{"$f":"Translator!B3820","v":"Manufacture of another substance; formulation of mixtures and in fuel products."},null,null,null,100010900,null,null,null,null,"E 2024"]

{"sheet":"3_PAH","index":7,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":true,"merged":[[0,0,0,7],[2,0,2,7],[3,3,20,3]]}
[{"$f":"Translator!B338","v":"Rules for polycyclical aromatic hydrocarbons (tab 3)"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B340","v":"Limit value according to Regulation 1272/2013 REACh Annex XVII"},{"$f":"Translator!B339","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2786","v":"Comments"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B341","v":"Benzo(a)pyrene"},"50-32-8","D/P",{"$f":"Translator!B1274","v":"General obligation to declare per ea. PAH from 1 ppm\nprohibition per PAH\na) <1 mg/kg (1 ppm) if to be available for the general public and if components of plastic or rubber, which in regular, reasonable or foreseeable use come into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time \nb) <0,5 mg/kg (0,5 ppm) for toys/products for infants and toddlers and components of plastic or rubber which in regular, reasonable or foreseeable use come into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time "},null,null,"EPA* + GADSL + Reach Annex XVII","E2009, C2011"]
[{"$f":"Translator!B342","v":"Acenaphthene "},"83-32-9","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B343","v":"Acenaphthylene "},"208-96-8 ","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B344","v":"Anthracene "},"120-12-7 ","D/P",null,null,null,"REACH + EPA* + GADSL","E2009, C2011"]
[{"$f":"Translator!B345","v":"Benzo(a)anthracene  "},"56-55-3","D/P",null,null,null,"EPA* + GADSL + Reach Annex XVII","E2009, C2011"]
[{"$f":"Translator!B346","v":"Benzo[j]fluoranthene "},"205-82-3","D/P",null,null,null,"Reach Annex XVII","E2009, C2011, C2012"]
[{"$f":"Translator!B347","v":"Benzo(b)fluoranthene (Benz(e)acephenanthrylene) "},"205-99-2 ","D/P",null,null,null,"EPA* + GADSL + Reach Annex XVII","E2009, C2011"]
[{"$f":"Translator!B348","v":"Benzo(e)pyrene"},"192-97-2","D/P",null,null,null,"Reach Annex XVII","E2009, C2011, C2012"]
[{"$f":"Translator!B349","v":"Benzo(ghi)­perylene "},"191-24-2","D/P",null,null,null,"EPA* ","E2009, C2011"]
[{"$f":"Translator!B350","v":"Benzo(k)fluoranthene "},"207-08-9","D/P",null,null,null,"EPA* + GADSL + Reach Annex XVII","E2009, C2011"]
[{"$f":"Translator!B351","v":"Chrysene  "},"218-01-9 ","D/P",null,null,null,"EPA* + GADSL + Reach Annex XVII","E2009, C2011"]
[{"$f":"Translator!B352","v":"Dibenzo(a,h)-anthracene "},"53-70-3 ","D/P",null,null,null,"EPA* + GADSL + Reach Annex XVII","E2009, C2011"]
[{"$f":"Translator!B353","v":"Fluoranthene "},"206-44-0 ","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B354","v":"Fluorene "},"86-73-7","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B355","v":"Indeno[1,2,3-cd]pyrene "},"193-39-5","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B356","v":"Naphthalene "},"91-20-3 ","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B357","v":"Phenanthrene "},"85-01-8 ","D/P",null,null,null,"EPA*","E2009, C2011"]
[{"$f":"Translator!B358","v":"Pyrene "},"129-00-0","D/P",null,null,null,"EPA*","E2009, C2011"]
[null,null,null,null,null,null,{"$f":"Translator!B361","v":"* List of \"Priority Pollutants\" from EPA"}]

{"sheet":"4_Plasticizers","index":8,"n_rows":37,"n_cols":9,"rows_kept":37,"cut":false,"hidden":true,"merged":[[1,0,1,1],[0,0,0,8],[2,0,2,8]]}
[{"$f":"Translator!B362","v":"Rules for plasticizers / phthalates (tab 4)"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},null,null,{"$f":"Translator!B94","v":"CAS number"},{"$f":"Translator!B1313","v":"Limit value [mass-%]"},{"$f":"Translator!B339","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2786","v":"Comments"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B102","v":"Substance rated declarable (D)"}]
[{"$f":"Translator!B363","v":"All plasticizers,added intentionally, below a sample listing, supplement if applicable:"},null,"D",null,0.1,null,null,null,"E2009"]
[{"$f":"Translator!B364","v":"Bis(hydroxyethyl) terephthalate"},"BHET","D","959-26-2",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B365","v":"Butyl cyclohexyl phthalate"},"BCP","D","84-64-0",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B366","v":"Butyl decyl phthalate"},"BDP","D","89-19-0",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B367","v":"Diallyl Phthalate"},"DAP","D","131-17-9",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B368","v":"Dicyclohexyl Phthalate"},"DCP","D","84-61-7",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B369","v":"Diisodecyl phthalate"},"DIDP","D","26761-40-0",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B370","v":"Diethyl phthalate"},"DEP","D","84-66-2",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B371","v":"Diisobutylphthalate"},"DIBP","D","84-69-5",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2009"]
[{"$f":"Translator!B372","v":"Diisoheptylphthalate"},"DIHpP","D","41451-28-9",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B373","v":"Diisohexylphthalate"},"DIHxP","D","146-50-9",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B374","v":"Diisopentylphthalate (DIPP)"},"DIPP","D","605-50-5",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2009"]
[{"$f":"Translator!B375","v":"Diisooctylphthalate"},"DIOP","D","27554-26-3",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B376","v":"Diisotridecylphthalate"},"DIUP","D","68515-47-9 a. 27253-26-5",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B377","v":"Diisoundecylphthalate"},"DIUP","D","85507-79-5",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B378","v":"Dimethyl phthalate"},"DMP","D","131-11-3",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B379","v":"Dimetil tereftalato"},"DMT","D","120-61-6",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B1251","v":"Dihexyl phthalate"},"DNHP","D","84-75-3",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B381","v":"Di-isononil ftalato"},"DINP","D","28553-12-0",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B1270","v":"Dipentyl phthalate"},"DPP","D","131-18-0",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B383","v":"Di-n-propilftalato"},"DPP","D","131-16-8",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B384","v":"Ditridecilftalato"},"DTDP","D","119-06-2",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B385","v":"Diundecilftalato"},"DUP","D","3648-20-2",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B386","v":"Di-n-octil ftalato"},"DNOP","D","117-84-0",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B387","v":"n-Octil n-decil ftalato"},"ODP","D","119-07-3",0.1,null,null,null,"E2009"]
[{"$f":"Translator!B1314","v":"Dibutyl phthalate"},"DBP","D"," 84-74-2",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1315","v":"Bis(2-methoxyethyl)phthalate"},"DMEP","D","117-82-8",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1024","v":"N-pentyl-isopentylphthalate"},null,"D","776297-69-9",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1316","v":"Benzyl butyl phthalate"},"BBP","D","85-68-7",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1317","v":"Bis(2-ethylhexyl)phthalate"},"DEHP","D","117-81-7",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1307","v":"1,2-Benzenedicarboxylic acid, di-C7-11-branched and linear alkyl esters (Di(heptyl, nonyl, undecyl) phthalate (DHNUP; dialkyl phthalate (C7-11) branched and linear)"},null,"D","68515-42-4",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1308","v":"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl ester, C7-rich (C6-8-(branched)-alkyl phthalate, diisoheptyl phthalate)"},null,"D"," 71888-89-6",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1309","v":"1,2-Benzenedicarboxylic acid, dipentylester, branched and linear (dihexylphthalate)"},null,"D","68515-50-4",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]
[{"$f":"Translator!B1311","v":"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear (bis-C5-alkyl-(linear and branched)phthalate)"},null,"D","84777-06-0",0.1,null,null,{"$f":"Translator!B388","v":"SVHC"},"E2014"]

{"sheet":"5_ROHS","index":9,"n_rows":16,"n_cols":12,"rows_kept":16,"cut":false,"hidden":true,"merged":[[0,0,0,11],[2,0,2,11],[15,0,15,11]]}
[{"$f":"Translator!B1610","v":"EC-RoHS (tab 5)\n2011/65/EU and 2015/863/EU"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B391","v":"Limit value [mass% in homogeneous material]"},{"$f":"Translator!B3789","v":"By Substance groups: Name of the contained substances"},{"$f":"Translator!B3790","v":"By Substance groups: CAS of the contained substances"},{"$f":"Translator!B392","v":"Concentration of substance [mass% in homogeneous material]"},{"$f":"Translator!B393","v":"Exception claimed? If so, which one?"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"},{"$f":"Translator!B625","v":"test report enclosed (optional)"},{"$f":"Translator!B637","v":"method of measurement"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B394","v":"Lead"},{"$f":"Translator!B2138","v":"7439-92-1 and its compounds"},"P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B395","v":"Cadmium and it's compounds"},{"$f":"Translator!B2139","v":"7440-43-9 and its compounds"},"P",0.01,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B396","v":"Mercury and it's compounds"},{"$f":"Translator!B2140","v":"7439-97-6 and its compounds"},"P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B397","v":"Chromium VI"},{"$f":"Translator!B2141","v":"1333-82-0 and its compounds"},"P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B398","v":"Polybrominated biphenyles (PBB)"},{"$f":"Translator!B119","v":"Material group"},"P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B399","v":"Polybrominated diphenyl ether (PBDE)"},{"$f":"Translator!B119","v":"Material group"},"P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B1306","v":"Bis(2-ethylhexyl) phthalate (DEHP)"},"117-81-7","P",0.1,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1305","v":"Benzyl butyl phthalate (BBP)"},"85-68-7","P",0.1,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1413","v":"Dibutyl phthalate (DBP)"},"84-74-2","P",0.1,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B1302","v":"Diisobutyl phthalate (DIBP)"},"84-69-5","P",0.1,null,null,null,null,null,"E2015"]
[{"$f":"Translator!B3778","v":"Medium- chained chlorinated paraffins (MCCPs) –Alkanes, C14-17, chloro"},"85535-85-9","D",0.1,null,null,null,null,null,"E2023"]
[{"$f":"Translator!B3779","v":"Tetrabromobisphenol A (TBBP-A, flame retardant) (2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol)"},"79-94-7","D",0.1,null,null,null,null,null,"E2023"]
[{"$f":"Translator!B1598","v":"Regulation Text with exemptions 01.09.2023"}]

{"sheet":"6_ELV","index":10,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":true,"merged":[[0,0,0,9],[2,0,2,9],[7,0,7,9]]}
[{"$f":"Translator!B400","v":"EC-ELV (tab 6) 2000/53/EC"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B391","v":"Limit value [mass% in homogeneous material]"},{"$f":"Translator!B3789","v":"By Substance groups: Name of the contained substances"},{"$f":"Translator!B3790","v":"By Substance groups: CAS of the contained substances"},{"$f":"Translator!B392","v":"Concentration of substance [mass% in homogeneous material]"},{"$f":"Translator!B393","v":"Exception claimed? If so, which one?"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B394","v":"Lead"},"7439-92-1","P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B395","v":"Cadmium and it's compounds"},"7440-43-9","P",0.01,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B396","v":"Mercury and it's compounds"},"7439-97-6","P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B397","v":"Chromium VI"},"1333-82-0","P",0.1,null,null,null,null,null,"E2009"]
[{"$f":"Translator!B888","v":"Regulation Text with exemptions 30.03.2023"}]

{"sheet":"7_GADSL","index":11,"n_rows":2,"n_cols":8,"rows_kept":2,"cut":false,"hidden":true,"merged":[[0,0,0,7],[2,0,2,7]]}
[{"$f":"Translator!B403","v":"GADSL (tab 7) see http://www.gadsl.org/ - Please click on \"GADSL Reference List\" "}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},{"$f":"Translator!B404","v":"P or D\nor\nP / D"},{"$f":"Translator!B391","v":"Limit value [mass% in homogeneous material]"},{"$f":"Translator!B392","v":"Concentration of substance [mass% in homogeneous material]"},{"$f":"Translator!B393","v":"Exception claimed? If so, which one?"},{"$f":"Translator!B97","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"}]

{"sheet":"8_Battery directive","index":12,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":true,"merged":[[20,5,20,6],[12,1,12,3],[15,1,15,3],[18,1,18,3],[0,0,0,6],[3,0,3,6],[11,5,11,6],[10,1,10,3],[11,1,11,3],[1,0,1,6],[21,1,21,3],[12,5,12,6],[13,1,13,3],[13,5,13,6],[14,1,14,3],[14,5,14,6],[15,5,15,6],[16,1,16,3],[16,5,16,6],[17,1,17,3],[17,5,17,6],[21,5,21,6],[18,5,18,6],[19,1,19,3],[19,5,19,6],[20,1,20,3]]}
[{"$f":"Translator!B406","v":"EC-Regulation on batteries and accumulators (tab 8)"}]
[{"$f":"Translator!B3780","v":"2006/66EC, 2008/98/EC, 2019/1020/EC and 2023/1542/EC"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B407","v":"Limit value [mass%]"},{"$f":"Translator!B408","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B393","v":"Exception claimed? If so, which one?"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B395","v":"Cadmium and it's compounds"},"7440-43-9","P",{"$f":"Translator!B3781","v":"0,002 expressed as cadmium metal, for portable battery only"},null,null,"C2023"]
[{"$f":"Translator!B396","v":"Mercury and it's compounds"},"7439-97-6","P",{"$f":"Translator!B3782","v":"0,0005 expressed as merury metal"},null,null,"C2023"]
[{"$f":"Translator!B3783","v":"Lead and its compounds"},"7439-92-1","P",{"$f":"Translator!B3786","v":"0,01 expressed as lead metal, for portable battery from 15.06.2024, not for portable zinc-air button cells until 15.06.2028"},null,null,"E2023"]
[{"$f":"Translator!B3784","v":"Cadmium"},"7440-43-9","D",{"$f":"Translator!B3787","v":2E-3},null,null,"E2023"]
[{"$f":"Translator!B3785","v":"Lead"},"7439-92-1","D",{"$f":"Translator!B3788","v":4.0000000000000001E-3},null,null,"E2023"]
[]
[null,{"$f":"Translator!B1212","v":"Total weight [g]"},null,null,null,null,null,null,null,null,null,"Batteriart","Bauform"]
[{"$f":"Translator!B1167","v":"Battery quantity"},{"$f":"Translator!B1170","v":"Battery type"},null,null,{"$f":"Translator!B1169","v":"Weight [g]"},{"$f":"Translator!B1171","v":"Build"},null,null,null,null,null,{"$f":"Translator!B1188","v":"1 Nickel-Cadmium (NiCd)"},{"$f":"Translator!B1199","v":"Button cell"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1189","v":"2 Nickel-metal hydride (NiMh)"},{"$f":"Translator!B1200","v":"AA"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1190","v":"3 Lithium-Ion (Li-Ion)"},{"$f":"Translator!B1201","v":"AAA"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1191","v":"4 Lithium-Metal (Li-Met)"},{"$f":"Translator!B1202","v":"D"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1192","v":"5 Alkali-Manganese (AlMn)"},{"$f":"Translator!B1203","v":"9-V-Block"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1193","v":"6 Zinc carbon (ZnC)"},{"$f":"Translator!B1204","v":"LR1"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1194","v":"7 Zinc-air (ZnLuft)"},{"$f":"Translator!B1205","v":"2/3A"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1195","v":"8 Lead Gel (Pb-Gel)"},{"$f":"Translator!B1206","v":"N"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1196","v":"9 Kleinblei (Pb)"},{"$f":"Translator!B1207","v":"Prismatic"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1197","v":"10 Silver oxide (AgO)"},{"$f":"Translator!B1208","v":"Pack"}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1198","v":"11 Other"},{"$f":"Translator!B1209","v":"CR2"}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1210","v":"Automotive battery"}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1211","v":"Customized builds"}]

{"sheet":"9_Manufacturing_Materials","index":13,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":true,"merged":[[0,0,0,5],[2,0,2,5],[15,0,15,5]]}
[{"$f":"Translator!B409","v":"Rules for auxiliary manufacturing materials excl. cooling lubricants (tab 9)"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B95","v":"Limit value"},{"$f":"Translator!B339","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B100","v":"Limits"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B410","v":"Alkyl phenoles and their isomers, ethoxylates and esters;"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B425","v":"10 ppm in aqueous cleaning agents, cooling lubricants and emulsion cleaners"},null,"E2009"]
[{"$f":"Translator!B411","v":"Aromatics in dimethyl sulfoxide (DMSO), soluble aromatics fraction of mineral oil products"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B426","v":"3,0 mass% in lubricant base oils"},null,"E2009"]
[{"$f":"Translator!B412","v":"Azo­dyes with carcinogenic amine components"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B427","v":"10 ppm in lubricants, dyes"},null,"E2009"]
[{"$f":"Translator!B413","v":"Lead and its combinations, taken as element"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B428","v":"10 ppm in lubricants"},null,"E2009"]
[{"$f":"Translator!B414","v":"chlorine releaseable, total content, calculated as elemental chlorine"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B429","v":"0,1  m% in anticorrosive agents, aqueous cleaning agents, water miscible cooling lubricants and emulsion cleaners"},null,"E2009, C2011"]
[{"$f":"Translator!B415","v":"Halogenated hydrocarbons"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B431","v":"1 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances"},null,"E2011"]
[{"$f":"Translator!B416","v":"Phenol"},"108-95-2","P",{"$f":"Translator!B431","v":"1 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances"},null,"E2009"]
[{"$f":"Translator!B417","v":"Silicones"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B431","v":"1 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances"},null,"E2009"]
[{"$f":"Translator!B418","v":"Total heavy metals"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B432","v":"10 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances Exemptions for Zn with non-water miscible cooling lubricants"},null,"E2009"]
[{"$f":"Translator!B419","v":"Zinc and its combinations, taken as element"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B433","v":"10 ppm in anticorrosive agents and cooling lubricants. Exemptions with non-water miscible cooling lubricants"},null,"E2009"]
[{"$f":"Translator!B112","v":"Tricresyl phosphates and isomers (TCP)"},"1330-78-5","P",{"$f":"Translator!B671","v":"10 ppm in anticorrosion agents, e,ulsion cleaners\n0,5 % in lubricants and test media"},null,"E2012"]
[{"$f":"Translator!B869","v":"Tricresyl phosphates (TCP)"},"78-30-8","P",{"$f":"Translator!B672","v":"0,1 % in lubricants and test media"},null,"E2012"]
[{"$f":"Translator!B102","v":"Substance rated declarable (D)"}]
[{"$f":"Translator!B420","v":"Anti-aging agents on basis of phenol and amine"},{"$f":"Translator!B119","v":"Material group"},"D",{"$f":"Translator!B434","v":"5 % in lubricants and test media;"},null,"E2009"]
[{"$f":"Translator!B421","v":"Biocides"},{"$f":"Translator!B119","v":"Material group"},"D",{"$f":"Translator!B435","v":"0,1 mass%"},null,"E2009"]
[{"$f":"Translator!B422","v":"Siloxanes"},{"$f":"Translator!B119","v":"Material group"},"D",{"$f":"Translator!B436","v":"0,1 mass% in water miscible metal working fluids"},null,"E2009"]
[{"$f":"Translator!B423","v":"Sulfonates (total)"},{"$f":"Translator!B119","v":"Material group"},"D",{"$f":"Translator!B437","v":"0,1 mass% in lubricants and test media"},null,"E2009"]
[{"$f":"Translator!B424","v":"VCI (Volatile Corrosion Inhibitor)"},{"$f":"Translator!B119","v":"Material group"},"D",{"$f":"Translator!B438","v":"0,1 mass% in anticorrosive agents"},null,"E2009"]

{"sheet":"10_Cooling_Lubricants","index":14,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":true,"merged":[[0,0,0,6],[2,0,2,6]]}
[{"$f":"Translator!B439","v":"Rules for cooling lubricants (tab 10)"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B95","v":"Limit value"},{"$f":"Translator!B96","v":"Concentration of ingredient \n[mass%]"},{"$f":"Translator!B99","v":"Restriction conditions"},{"$f":"Translator!B100","v":"Limits"}]
[{"$f":"Translator!B440","v":"Prohibited substances (P)\nVKIS-VSI Substances"}]
[{"$f":"Translator!B441","v":"1,2-Benzisothiazol-3(2H)-one"},"2634-33-5","P",5.0000000000000001E-4,null,null,"E2009"]
[{"$f":"Translator!B442","v":"1,3,5-Tris(2-hydroxyethyl)-hexahydro-1,3,5-triazine (HHT)"},"4719-04-4","P",1E-3,null,null,"E2009"]
[{"$f":"Translator!B443","v":"2-(Methoxycarbonylamino)-benzimidazol (Carbendazim)"},"10605-21-7","P",1E-3,null,null,"E2009"]
[{"$f":"Translator!B444","v":"2-methylamino-2-methyl-1-propanol"},"27646-80-6","P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2011"]
[{"$f":"Translator!B445","v":"2,2´-Iminodiethanol (Diethanolamin)"},"111-42-2","P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2009"]
[{"$f":"Translator!B446","v":"2-Octyl-2H-isothiazol-3-on"},"26530-20-1","P",5.0000000000000001E-4,null,null,"E2009"]
[{"$f":"Translator!B447","v":"4,4´-Dimethyloxazolidin"},"51200-87-4","P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2009"]
[{"$f":"Translator!B448","v":"5-Chloro-2-methyl-2,3-dihydroisothiazol-3-on and 2-methyl-2,3-dihydroisothiazol-3-on, mixture in ratio 3:1 (CMI/MI)"},{"$f":"Translator!B471","v":"55965-84-9 and 2682-20-4"},"P",{"$f":"Translator!B473","v":"15 ppm water mixed"},null,null,"E2009"]
[{"$f":"Translator!B449","v":"Amides that release secondary amines"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2009"]
[{"$f":"Translator!B450","v":"Amines, secondary, that form carcinogenic N-nitrosamines of categories 1 or 2"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2009"]
[{"$f":"Translator!B451","v":"Barium salts with the exception of barium sulfate"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B474","v":"10 ppm water miscible;\n2 ppm water mixed"},null,null,"E2009"]
[{"$f":"Translator!B452","v":"Benzo-(a)-pyrene (BaP)"},"50-32-8","P","50 ppm",null,null,"E2009"]
[{"$f":"Translator!B453","v":"Bis(2-ethylhexyl)phthalate (DEHP)"},"117-81-7","P",5.0000000000000001E-3,null,"SVHC","E2009"]
[{"$f":"Translator!B454","v":"Boric acid"},"10043-35-3","P",5.5E-2,null,"SVHC","E2009"]
[{"$f":"Translator!B455","v":"carbendazim methyl 1H-benzimidazol-2-ylcarbamate)"},"10605-21-7","P",1E-3,null,null,"E2011"]
[{"$f":"Translator!B456","v":"Chlorinated paraffins, short-chain (C10-C13, SCCP)"},"85535-84-8","P",0.01,null,"SVHC","E2009"]
[{"$f":"Translator!B457","v":"Chlorinated paraffins, long-chain (≥ C18, LCCP)"},"85535-86-0","P",2E-3,null,null,"E2009"]
[{"$f":"Translator!B458","v":"Chlorinated paraffins, medium-chain (C14 – C17, MCCP)"},"85535-85-9","P",2E-3,null,null,"E2009"]
[{"$f":"Translator!B459","v":"Diethanolamine (2,2 -Iminodiethanol)"},"111-42-2","P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2011"]
[{"$f":"Translator!B460","v":"Ethylenediaminetetraacetic acid and salts (EDTA)"},"60-00-4","P",{"$f":"Translator!B475","v":"1 ppm water mixed"},null,null,"E2009"]
[{"$f":"Translator!B461","v":"Glutaraldehyde"},"111-30-8","P",5.0000000000000001E-3,null,null,"E2009"]
[{"$f":"Translator!B462","v":"Morpholine and morpholine releasing combinations"},"110-91-8, \n5625-90-1","P",{"$f":"Translator!B472","v":"0,2 % water miscible"},null,null,"E2009"]
[{"$f":"Translator!B463","v":"Sodium tetraborates"},"a) 1330-43-4\nb) 12179-04-3\nc) 1303-96-4","P","a) 4,5%\nb) 6,5%\nc) 8,5%",null,"SVHC","E2009"]
[{"$f":"Translator!B464","v":"Nitrite and nitrite releasing combinations"},"2224-44-4,\n52-51-7,\n126-11-4","P",{"$f":"Translator!B476","v":"Prohibited water miscible;\n20 mg nitrite/l water mixed"},null,null,"E2009"]
[{"$f":"Translator!B465","v":"Nonylphenol"},"25154-52-3","P",1E-3,null,{"$f":"Translator!B478","v":"REACH Annex XVII"},"E2009"]
[{"$f":"Translator!B466","v":"Nonylphenol ethoxylates"},"9016-45-9","P",1E-3,null,null,"E2009"]
[{"$f":"Translator!B467","v":"Orthoboric acid, sodium salt"},"13840-56-7","P",4.4999999999999998E-2,null,null,"E2009"]
[{"$f":"Translator!B468","v":"Polychlorinated biphenyls - PCB"},"1336-36-3","P","4 ppm",null,null,"E2009, C2011"]
[{"$f":"Translator!B469","v":"Polychlorinated terphenyls – PCT"},"61788-33-8","P","4 ppm",null,{"$f":"Translator!B478","v":"REACH Annex XVII"},"E2009, C2011"]
[{"$f":"Translator!B470","v":"Sodium-2-pyridinethiol-1-oxide (Pyrithione Sodium Salt)"},"3811-73-2","P",{"$f":"Translator!B477","v":"5 % water miscible"},null,null,"E2009"]
[{"$f":"Translator!B112","v":"Tricresyl phosphates and isomers (TCP)"},"1330-78-5","P",{"$f":"Translator!B673","v":"10 ppm in cooling lubricants"},null,null,"E2012"]

{"sheet":"11_Packaging","index":15,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":true,"merged":[[24,1,24,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[18,1,18,3],[19,1,19,3],[20,1,20,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[2,0,2,7],[0,0,0,7],[4,3,7,3],[13,1,13,3],[14,1,14,3],[3,0,3,7],[8,0,8,7]]}
[{"$f":"Translator!B479","v":"Packaging (Tab 11)\nEU-PACKAGING (94/62/EC), France Decree No. 2022-105"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},{"$f":"Translator!B94","v":"CAS number"},null,{"$f":"Translator!B95","v":"Limit value"},{"$f":"Translator!B480","v":"Concentration of substance\n[ppm]"},{"$f":"Translator!B2787","v":"Entry\n- included ( E )\n- changed ( C )"},{"$f":"Translator!B625","v":"test report enclosed (optional)"},{"$f":"Translator!B637","v":"method of measurement"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B3796","v":"11.a EU Packaging directive 94/62/EC"}]
[{"$f":"Translator!B481","v":"Lead"},{"$f":"Translator!B119","v":"Material group"},"P",{"$f":"Translator!B485","v":"cumulative 100 ppm"},null,"E2009"]
[{"$f":"Translator!B482","v":"Chromium VI"},"14977-61-8","P",null,null,"E2009"]
[{"$f":"Translator!B483","v":"Cadmium"},"7440-43-9","P",null,null,"E2009"]
[{"$f":"Translator!B484","v":"Mercury"},"7439-97-6","P",null,null,"E2009"]
[{"$f":"Translator!B3797","v":"11. b France Decree No. 2022-105"}]
[{"$f":"Translator!B3776","v":"MOAH (Mineral Oil Hydrocarbons) with 1-7 aromatic Rings for printing inks"},{"$f":"Translator!B3775","v":"Substance group"},"P","Limit 1%, 1.1.2026 0,1%",null,"E2023"]
[{"$f":"Translator!B3777","v":"MOAH (Mineral Oil Hydrocarbons) with 3-7 aromatic Rings for printing inks"},{"$f":"Translator!B3775","v":"Substance group"},"P","Limit 1%, 1.1.2026 0,0001%",null,"E2023"]
[{"$f":"Translator!B3798","v":"MOSH (Mineral Oil Saturated Hydrocarbons) with 16-35 aromatic Rings for printing inks"},{"$f":"Translator!B3775","v":"Substance group"},"P","Limit 1%, 1.1.2026 0,1%",null,"E2023"]
[]
[null,{"$f":"Translator!B1212","v":"Total weight [g]"},null,null,null,null,null,null,null,null,"Verpackungsart","Batteriart","Bauform"]
[{"$f":"Translator!B1264","v":"Packaging type / quantity"},{"$f":"Translator!B1265","v":"Material"},null,null,{"$f":"Translator!B1169","v":"Weight [g]"},null,null,null,null,null,{"$f":"Translator!B1172","v":"Glass"},{"$f":"Translator!B1188","v":"1 Nickel-Cadmium (NiCd)"},{"$f":"Translator!B1199","v":"Button cell"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1173","v":"Paper/cardboard/carton"},{"$f":"Translator!B1189","v":"2 Nickel-metal hydride (NiMh)"},{"$f":"Translator!B1200","v":"AA"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1174","v":"Tin plate, steel"},{"$f":"Translator!B1190","v":"3 Lithium-Ion (Li-Ion)"},{"$f":"Translator!B1201","v":"AAA"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1175","v":"Aluminum, other metals"},{"$f":"Translator!B1191","v":"4 Lithium-Metal (Li-Met)"},{"$f":"Translator!B1202","v":"D"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1176","v":"Content PET"},{"$f":"Translator!B1192","v":"5 Alkali-Manganese (AlMn)"},{"$f":"Translator!B1203","v":"9-V-Block"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1177","v":"Content HDPE"},{"$f":"Translator!B1193","v":"6 Zinc carbon (ZnC)"},{"$f":"Translator!B1204","v":"LR1"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1178","v":"Content PVC"},{"$f":"Translator!B1194","v":"7 Zinc-air (ZnLuft)"},{"$f":"Translator!B1205","v":"2/3A"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1179","v":"Content LDPE"},{"$f":"Translator!B1195","v":"8 Lead Gel (Pb-Gel)"},{"$f":"Translator!B1206","v":"N"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1180","v":"Content PP"},{"$f":"Translator!B1196","v":"9 Kleinblei (Pb)"},{"$f":"Translator!B1207","v":"Prismatic"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1181","v":"Content EPS"},{"$f":"Translator!B1197","v":"10 Silver oxide (AgO)"},{"$f":"Translator!B1208","v":"Pack"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1182","v":"Content PS"},{"$f":"Translator!B1198","v":"11 Other"},{"$f":"Translator!B1209","v":"CR2"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1183","v":"Content PPS"},null,{"$f":"Translator!B1210","v":"Automotive battery"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1184","v":"Other plastic/unknown"},null,{"$f":"Translator!B1211","v":"Customized builds"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1185","v":"Composite packaging"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1186","v":"Wood without Euro-pallets"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"Translator!B1187","v":"other natural materials"}]

{"sheet":"GB","index":16,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":true,"merged":[[0,0,0,1],[2,0,5,0],[6,0,7,0]]}
[{"$f":"Translator!B667","v":"Advantage: You may reduce the amount of required data by selecting the applicable checkbox (optional). Click \"Ok\" to continue."},null,{"$f":"Translator!B668","v":"Division"},9,15]
[null,null,null,null,null,null,null,"Mobility Aftermarket (MA)"]
["OK",null,null,null,null,null,null,"Electrified Motion (ME)"]
[null,null,null,null,null,null,null,"BCDS"]
[null,null,null,null,null,null,null,"BEG/ITK"]
[null,null,null,null,null,null,null,"BHCS"]
[{"$f":"Translator!B1459","v":"please double click"},null,null,null,null,null,null,"Bosch Sensortec (BST)"]
[null,null,null,null,null,null,null,"Building Technologies (BT)"]
[null,null,null,null,null,null,null,"Cross-Domain Computing Solutions (XC)"]
[null,null,null,null,null,null,null,"Vehicle Motion (VM)"]
[null,null,null,null,null,null,null,"Drive and Control Technology - Rexroth AG (DC)"]
[null,null,null,null,null,null,null,"E-Bike (EB)"]
[null,null,null,null,null,null,null,"Electrified Motion (EM)"]
[null,null,null,null,null,null,null,"ETAS"]
[null,null,null,null,null,null,null,"GROW"]
[null,null,null,null,null,null,null,"GS/TEC"]
[null,null,null,null,null,null,null,"HOME"]
[null,null,null,null,null,null,null,"Home Comfort (HC)"]
[null,null,null,null,null,null,null,"Bosch Manufacturing Solutions (BMG)"]
[null,null,null,null,null,null,null,"Non-Automotive (MA)"]
[null,null,null,null,null,null,null,"Power Tools (PT)"]
[null,null,null,null,null,null,null,"Powertrain Solutions (PS)"]
[null,null,null,null,null,null,null,"PS-SF"]
[null,null,null,null,null,null,null,"Solar Energy (SE)"]
[null,null,null,null,null,null,null,"SO"]

{"sheet":"GB Handelsware Nicht Automobil","index":17,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":true,"merged":[[0,0,0,1],[2,0,5,0],[6,0,7,0]]}
[{"$f":"Translator!B667","v":"Advantage: You may reduce the amount of required data by selecting the applicable checkbox (optional). Click \"Ok\" to continue."},null,{"$f":"Translator!B668","v":"Division"},1,15]
[null,null,null,null,null,null,null,"Building Technologies (BT)"]
["OK"]
[]
[]
[]
[{"$f":"Translator!B1459","v":"please double click"}]

{"sheet":"12_Critical Raw Materials","index":18,"n_rows":68,"n_cols":13,"rows_kept":68,"cut":false,"hidden":true,"merged":[[0,0,0,10],[41,8,46,8],[65,0,65,1],[66,0,66,1],[67,0,67,1]]}
[{"$f":"Translator!B1159","v":"Tab 12: Critical Raw Materials (EU)"}]
[{"$f":"Translator!B1160","v":"Regulated Substances"},{"$f":"Translator!B1161","v":"CAS number"},null,{"$f":"Translator!B3821","v":"Limits [mass %]\nor intentionally added\n\nExplanation: Limit related to mass in complete delivered component (Bosch SNR)"},{"$f":"Translator!B3732","v":"Substance Presence"},{"$f":"Translator!B3770","v":"recovered from manufacturing waste or post-consumer waste, present in permanent magnets incorporated in product"},{"$f":"Translator!B3822","v":"Concentration of ingredient [mass%]\n\nExplanation: Enter the total amount of the Concentration of ingredient in [mass%]"},{"$f":"Translator!B1164","v":"Designation of the material that contains the regulated substance and concentration.\n\nExplanation: Enter the designation and concentration of ingredient in the component (s) which the substance is used e.g. 10% Aluminium in a motor; 1% Lead in a resistor, 0,15% silver in a wire."},{"$f":"Translator!B1165","v":"Examples of occurrence"},{"$f":"Translator!B110","v":"Comments"},{"$f":"Translator!B111","v":"Entry\n- included ( E )\n- changed ( C )"}]
[{"$f":"Translator!B3733","v":"Aluminium"},"7429-90-5 ","D",0.1,null,null,null,null,{"$f":"Translator!B3734","v":"• Capacitors\n• Electronics enclosure"},{"$f":"Translator!B3735","v":"• RB Defined"},"E2023"]
[{"$f":"Translator!B2887","v":"Antimony"},"7440-36-0","D",0.1,null,null,null,null,{"$f":"Translator!B2935","v":"• Flame retardants\n• Lead-acid batteries"},{"$f":"Translator!B2978","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023",null,"yes"]
[{"$f":"Translator!B3736","v":"Arsenic"},"7440-38-2 ","D",0.1,null,null,null,null,{"$f":"Translator!B3737","v":"• Metallurgy\n• Semi-conductors"},{"$f":"Translator!B3738","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023",null,"no"]
[{"$f":"Translator!B2888","v":"Bauxite"},"1318-16-7","D",0.1,null,null,null,null,{"$f":"Translator!B2936","v":"• Aluminium production"},{"$f":"Translator!B2979","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2889","v":"Baryte "},"13462-86-7","D",0.1,null,null,null,null,{"$f":"Translator!B2937","v":"• Fillers\n• Chemicals "},{"$f":"Translator!B2980","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2890","v":"Beryllium"},"7440-41-7","D",0.1,null,null,null,null,{"$f":"Translator!B2938","v":"• Copper-beryllium alloy"},{"$f":"Translator!B2981","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2891","v":"Bismuth"},"7440-69-9","D",0.1,null,null,null,null,{"$f":"Translator!B2939","v":"• Low-melting alloys\n• Metallurgical additives "},{"$f":"Translator!B2982","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2892","v":"Borate"},"35498-15-8","D",0.1,null,null,null,null,{"$f":"Translator!B2940","v":"• Glass and fibreglass applications\n• Ceramics\n• Permanent magnets"},{"$f":"Translator!B2983","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3739","v":"Boron"},"7440-42-8 ","D",0.1,null,null,null,null,{"$f":"Translator!B3740","v":"• Metallurgy grade"},{"$f":"Translator!B3741","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2893","v":"Cobalt"},"7440-48-4","D",0.1,null,null,null,null,{"$f":"Translator!B2941","v":"• Rechargeable battery electrodes\n• Superalloys\n• Hardfacing\n• High speed steel\n• Other alloys \n• Catalysts\n• Magnets"},{"$f":"Translator!B2984","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2894","v":"Coking Coal"},"65996-77-2","D",0.1,null,null,null,null,{"$f":"Translator!B2942","v":"• Steel Production\n• Carbon fibres\n• Battery electrode"},{"$f":"Translator!B2985","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3742","v":"Copper"},"7440-50-8","D",0.1,null,null,null,null,{"$f":"Translator!B3744","v":"• Electrification across all strategic technologies"},{"$f":"Translator!B3746","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3743","v":"Feldspar (silikate)"},"68476-25-5","D",0.1,null,null,null,null,{"$f":"Translator!B3745","v":"• Glass\n• Ceramics"},{"$f":"Translator!B3746","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2895","v":"Fluorite (CaF2) / Fluorspar "},"7789-75-5","D",0.1,null,null,null,null,{"$f":"Translator!B2943","v":"• Aluminium production\n• Steel and iron making"},{"$f":"Translator!B2986","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2896","v":"Gallium "},"7440-55-3","D",0.1,null,null,null,null,{"$f":"Translator!B2944","v":"• Semiconductors\n• Integrated Circuits\n• Sensors\n• Alloys\n• Batteries\n• Magnets"},{"$f":"Translator!B2987","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2897","v":"Germanium"},"7440-56-4","D",0.1,null,null,null,null,{"$f":"Translator!B2945","v":"• Fibre optics\n• Infrared optics \n• Satellite solar cells\n• Polymerisation catalysts"},{"$f":"Translator!B2988","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3748","v":"Gold"},"7440-57-5","D",0.1,null,null,null,null,null,{"$f":"Translator!B3749","v":"• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2898","v":"Hafnium"},"7440-58-6","D",0.1,null,null,null,null,{"$f":"Translator!B2946","v":"• Superalloys\n• Nuclear control rods\n• Refractory ceramics"},{"$f":"Translator!B2989","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3750","v":"Helium "},"7440-59-7","D",0.1,null,null,null,null,{"$f":"Translator!B3752","v":"• Cryogenics manufacturing\n• Semiconductors manufacturing"},{"$f":"Translator!B3753","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3751","v":"Lead"},"7439-92-1","D",0.1,null,null,null,null,null,{"$f":"Translator!B3754","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2900","v":"Lithium"},"7439-93-2","D",0.1,null,null,null,null,{"$f":"Translator!B2948","v":"• Lithium-Ion batteries (battery grade)\n• Photovoltaic cells and photonics\n• Solders"},{"$f":"Translator!B2991","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2901","v":"Magnesium"},"7439-95-4","D",0.1,null,null,null,null,{"$f":"Translator!B2949","v":"• Aluminium alloys "},{"$f":"Translator!B2992","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3755","v":"Manganese "},"7439-96-5","D",0.1,null,null,null,null,{"$f":"Translator!B3757","v":"• Steelmaking\n• Batteries"},{"$f":"Translator!B3759","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3756","v":"Mica"},"12001-26-2","D",0.1,null,null,null,null,{"$f":"Translator!B3758","v":"• Electrical or thermal insulators"},{"$f":"Translator!B3760","v":"• RB Defined"},"E2023"]
[{"$f":"Translator!B2902","v":"Natural Graphite"},"7782-42-5","D",0.1,null,null,null,null,{"$f":"Translator!B2950","v":"• Batteries (battery grade)\n• Refractories for steelmaking"},{"$f":"Translator!B2993","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2903","v":"Natural Rubber"},"9006-04-6","D",0.1,null,null,null,null,{"$f":"Translator!B2951","v":"• Rubber electrical insulators "},{"$f":"Translator!B2994","v":"• RB Defined"},"E2023"]
[{"$f":"Translator!B3761","v":"Nickel"},"7440-02-0","D",0.1,null,null,null,null,{"$f":"Translator!B3762","v":"• Batteries\n• Magnets"},{"$f":"Translator!B3763","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2904","v":"Niobium"},"7440-03-1","D",0.1,null,null,null,null,{"$f":"Translator!B2952","v":"• Steels\n• Superalloys \n• Capacitors\n• Superconducting\n• Magnets"},{"$f":"Translator!B2995","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2905","v":"Phosphate rock "},"65996-94-3","D",0.1,null,null,null,null,{"$f":"Translator!B2953","v":" • Phosphorus production"},{"$f":"Translator!B2996","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2906","v":"Phosphorus"},"7723-14-0","D",0.1,null,null,null,null,{"$f":"Translator!B2954","v":" • Steel production"},{"$f":"Translator!B2997","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B3791","v":"Silver"},"7440-22-4","D",0.1,null,null,null,null,{"$f":"Translator!B3792","v":"• Electronic"},{"$f":"Translator!B3793","v":"• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2907","v":"Scandium"},"7440-20-2","D",0.1,null,null,null,null,{"$f":"Translator!B2955","v":"• Solid oxide fuel cells\n• Aluminium-scandium alloys\n• 3D printing"},{"$f":"Translator!B2998","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2908","v":"Silicon metal"},"7440-21-3","D",0.1,null,null,null,null,{"$f":"Translator!B2956","v":"• Semiconductors\n• Silicones\n• Photovoltaics\n• Electronic components"},{"$f":"Translator!B2999","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2909","v":"Strontium"},"7440-24-6","D",0.1,null,null,null,null,{"$f":"Translator!B2957","v":"• Ceramic capacitors\n• PTC thermistors\n• Aluminium alloys"},{"$f":"Translator!B3000","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2910","v":"Tantalum (coltan)"},"7440-25-7","D",0.1,null,null,null,null,{"$f":"Translator!B2958","v":"• Capacitors\n• Superalloys\n• Sputtering targets "},{"$f":"Translator!B3001","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain "},"E2023"]
[{"$f":"Translator!B3764","v":"Tin (niobium / cassiterite)"},"7440-31-5","D",0.1,null,null,null,null,{"$f":"Translator!B3766","v":"• Superconducting magnets"},{"$f":"Translator!B3768","v":"• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain "},"E2023"]
[{"$f":"Translator!B3765","v":"Titanium metal"},"7440-32-6","D",0.1,null,null,null,null,{"$f":"Translator!B3767","v":"• Lightweight high-strength alloys "},{"$f":"Translator!B3769","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2911","v":" Tungstene"},"7440-33-7","D",0.1,null,null,null,null,{"$f":"Translator!B2959","v":"• Hard metals (tungsten carbide)\n• Alloy steel"},{"$f":"Translator!B3002","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain  "},"E2023"]
[{"$f":"Translator!B2912","v":"Vanadium"},"7440-62-2","D",0.1,null,null,null,null,{"$f":"Translator!B2960","v":"• High-strength low-alloy (HSLA) steels\n• Special steels\n• Chemical catalysts"},{"$f":"Translator!B3003","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2913","v":"Platinum"},"7440-06-4","D",0.1,null,null,null,null,{"$f":"Translator!B2961","v":"• Chemical and automotive catalysts\n• Fuel cells\n• Electronic applications"},{"$f":"Translator!B3004","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2914","v":"Palladium"},"7440-05-3","D",0.1,null,null,null,null,null,{"$f":"Translator!B3005","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2915","v":"Rhodium"},"7440-16-6","D",0.1,null,null,null,null,null,{"$f":"Translator!B3006","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2916","v":"Ruthenium"},"7440-18-8","D",0.1,null,null,null,null,null,{"$f":"Translator!B3007","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2917","v":"Iridium"},"7439-88-5","D",0.1,null,null,null,null,null,{"$f":"Translator!B3008","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2918","v":"Osmium"},"7440-04,2","D",0.1,null,null,null,null,null,{"$f":"Translator!B3009","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"E2023"]
[{"$f":"Translator!B2919","v":"Yttrium"},"7440-65-5","D",0.1,null,null,null,null,{"$f":"Translator!B2962","v":"• Phosphors Lighting "},{"$f":"Translator!B3010","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2920","v":"Terbium"},"7440-27-9","D",0.1,null,null,null,null,{"$f":"Translator!B2963","v":"• Computers Magnets\n• Phosphors Lighting "},{"$f":"Translator!B3011","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2921","v":"Dysprosium"},"7429-91-6","D",0.1,null,null,null,null,{"$f":"Translator!B2964","v":"• Computers Magnets\n• Audio Systems Magnets"},{"$f":"Translator!B3012","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2922","v":"Holmium"},"7440-60-0","D",0.1,null,null,null,null,{"$f":"Translator!B2965","v":"• Magnets"},{"$f":"Translator!B3013","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2923","v":"Erbium"},"7440-52-0","D",0.1,null,null,null,null,{"$f":"Translator!B2966","v":"• Glass Fibre Optics "},{"$f":"Translator!B3014","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2924","v":"Thulium"},"7440-30-4","D",0.1,null,null,null,null,{"$f":"Translator!B2967","v":"• Lightweight portable x-ray machine for medical use"},{"$f":"Translator!B3015","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2925","v":"Ytterbium "},"7440-64-4","D",0.1,null,null,null,null,{"$f":"Translator!B2968","v":"• Memory devices\n• Tunable lasers"},{"$f":"Translator!B3016","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2926","v":"Lutetium"},"7439-94-3","D",0.1,null,null,null,null,{"$f":"Translator!B2969","v":"• Catalyst for cracking hydrocarbons in oil refineries"},{"$f":"Translator!B3017","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2927","v":"Europium"},"7440-53-1","D",0.1,null,null,null,null,{"$f":"Translator!B2970","v":"• Phosphors Lighting "},{"$f":"Translator!B3018","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2928","v":"Gadolinium"},"7440-54-2","D",0.1,null,null,null,null,{"$f":"Translator!B2971","v":"• Phosphors\n• Magnets"},{"$f":"Translator!B3019","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2929","v":"Lanthanum"},"7439-91-0","D",0.1,null,null,null,null,{"$f":"Translator!B2972","v":"• FCC Catalysts\n• Batteries\n• Alloys"},{"$f":"Translator!B3020","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2930","v":"Cerium"},"7440-45-1","D",0.1,null,null,null,null,{"$f":"Translator!B2973","v":"• Mischmetal alloy\n• Flat-screen TVs\n• Low-energy light bulbs"},{"$f":"Translator!B3021","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2931","v":"Praseodymium"},"7440-10-0","D",0.1,null,null,null,null,{"$f":"Translator!B2974","v":"• Computers Magnets\n• Audio Systems Magnets"},{"$f":"Translator!B3022","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2932","v":"Neodymium"},"7440-00-8","D",0.1,null,null,null,null,{"$f":"Translator!B2975","v":"• Magnets\n• Batteries"},{"$f":"Translator!B3023","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2933","v":"Promethium"},"7440-12-2","D",0.1,null,null,null,null,{"$f":"Translator!B2976","v":"• Atomic batteries"},{"$f":"Translator!B3024","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[{"$f":"Translator!B2934","v":"Samarium "},"7440-19-9","D",0.1,null,null,null,null,{"$f":"Translator!B2977","v":"• Magnets\n• Batteries"},{"$f":"Translator!B3025","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"E2023"]
[]
[{"$f":"Translator!B3026","v":"NOTES"}]
[{"$f":"Translator!B3027","v":"Platinum group metals (PGM)"}]
[{"$f":"Translator!B3028","v":"Heavy-group rare earth elements (HREE)"}]
[{"$f":"Translator!B3029","v":"Light-group rare earth elements (LREE)"}]

{"sheet":"13_IMO","index":19,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":true,"merged":[[0,0,0,7],[1,0,1,7],[3,0,3,7],[19,0,19,7],[22,0,22,1],[2,0,2,1],[4,0,4,1],[5,0,5,1],[6,0,14,0],[15,0,17,0],[6,7,14,7],[15,7,17,7],[20,0,20,1],[21,0,21,1],[18,0,18,1],[23,0,23,1],[24,0,24,1],[25,0,25,1],[29,0,29,1],[26,0,26,1],[27,0,27,1],[28,0,28,1]]}
[{"$f":"Translator!B1247","v":"IMO (tab 13)"}]
[{"$f":"Translator!B1468","v":"EU-Regulation No. 1013/2006 and 1257/2013 on ship recycling"}]
[{"$f":"Translator!B93","v":"Regulated Substances"},null,{"$f":"Translator!B391","v":"Limit value [mass% in homogeneous material]"},null,{"$f":"Translator!B1246","v":"Mass"},{"$f":"Translator!B1245","v":"Unit"},{"$f":"Translator!B2782","v":"Examples of occurrence"},{"$f":"Translator!B1471","v":"Comments"}]
[{"$f":"Translator!B101","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B1220","v":"Asbestos"},null,"0 mg/kg","P",null,null,null,{"$f":"Translator!B1472","v":"listed in REACH Annex 17 and Tab RB-General"}]
[{"$f":"Translator!B1221","v":"Polychlorinated biphenyls (PCBs)"},null,"0 mg/kg","P",null,null,null,{"$f":"Translator!B1473","v":"listed in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"}]
[{"$f":"Translator!B1222","v":"Ozone-depleting substances,\nThese controlled substances are defined in Article 1(4) of the Montreal Protocol on Substances that Deplete the Ozone Layer, 1987, listed in Annexes A,B,C or E to that Protocol in force at the time of application or interpretation of this Annex. Ozone-depleting substances that may be found on board ships include, but are not limited to:"},{"$f":"Translator!B1223","v":"Chlorofluorocarbons (CFCs)"},"0 mg/kg","P",null,null,null,{"$f":"Translator!B1474","v":"listed in Tab RB-General,\nRegulation (EC) No 1005/2009"}]
[null,{"$f":"Translator!B1224","v":"Halons"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1225","v":"Other fully halogenated CFCs"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1226","v":"Carbon Tetrachloride"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1227","v":"1,1,1-Trichloroethane"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1228","v":"Hydrochlorofluorocarbons"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1229","v":"Hydrobromofluorocarbons"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1230","v":"Methyl bromide"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1231","v":"Bromochloromethane"},"0 mg/kg","P"]
[{"$f":"Translator!B1232","v":"Anti-fouling systems containing organotin compounds as a biocide"},{"$f":"Translator!B1233","v":"Tributyl Tins"},"0 mg/kg","P",null,null,null,{"$f":"Translator!B1475","v":"REACH Annex 17 as \"Organic tin compounds\""}]
[null,{"$f":"Translator!B1234","v":"Triphenyl Tins"},"0 mg/kg","P"]
[null,{"$f":"Translator!B1235","v":"other"},"0 mg/kg","P"]
[{"$f":"Translator!B1470","v":"Perfluorooctane sulfonic acid (PFOS)"},null,"0 mg/kg","P",null,null,null,{"$f":"Translator!B1476","v":"listed in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"}]
[{"$f":"Translator!B102","v":"Substance rated declarable (D)"}]
[{"$f":"Translator!B1236","v":"Cadmium and cadmium compounds"},null,"100 mg/kg","D",null,null,null,{"$f":"Translator!B1477","v":"equivalent to RoHS limits,\nREACH Annex 17, REACH SVHC"}]
[{"$f":"Translator!B1237","v":"Hexavalent chromium and hexavalent chromium compounds"},null,"1000 mg/kg","D",null,null,null,{"$f":"Translator!B1478","v":"equivalent to RoHS limits,\nREACH SVHC"}]
[{"$f":"Translator!B1238","v":"Lead and lead compounds"},null,"1000 mg/kg","D",null,null,null,{"$f":"Translator!B1479","v":"equivalent to RoHS limits,"}]
[{"$f":"Translator!B1239","v":"Mercury and mercury compounds"},null,"1000 mg/kg","D",null,null,null,{"$f":"Translator!B1480","v":"equivalent to RoHS limits,\nREACH Annex 17"}]
[{"$f":"Translator!B1240","v":"Polybrominated biphenyl (PBBs)"},null,"1000 mg/kg","D",null,null,null,{"$f":"Translator!B1481","v":"equivalent to RoHS limits,\nREACH Annex 17"}]
[{"$f":"Translator!B1241","v":"Polybrominated dephenyl ethers (PBDEs)"},null,"1000 mg/kg","D",null,null,null,{"$f":"Translator!B1482","v":"equivalent to RoHS limits,"}]
[{"$f":"Translator!B1242","v":"Polychloronaphthalanes (Cl => 3)"},null,"0 mg/kg","D",null,null,null,{"$f":"Translator!B1483","v":"listed in Tab DC"}]
[{"$f":"Translator!B1243","v":"Radioactive substances"},null,"0 mg/kg","D",null,null,null,{"$f":"Translator!B1484","v":"listed in Tab RB-General"}]
[{"$f":"Translator!B1244","v":"Certain shortchain chlorinated paraffins"},null,0.01,"D",null,null,null,{"$f":"Translator!B1485","v":"REACH Annex 17 as \"Alkanes, C 10 -C 13, chlorine (short-chain chlorinated paraffins)\""}]
[{"$f":"Translator!B1469","v":"Brominated Flame Retardant (HBCDD)"},null,"0 mg/kg","D",null,null,null,{"$f":"Translator!B1486","v":"listed in REACH Annex 14 and  REACH SVHC as \"Hexabromocyclododecane (HBCDD)\"\nlisted in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"}]

{"sheet":"14_CN-RoHS","index":20,"n_rows":104,"n_cols":12,"rows_kept":104,"cut":false,"hidden":true,"merged":[[80,8,84,8],[80,10,84,10],[91,8,91,10],[94,8,94,10],[102,8,102,10],[50,8,50,10],[0,0,0,11],[2,0,2,11],[9,0,9,11],[10,0,10,3],[10,8,10,10],[12,8,12,10],[22,8,26,8],[28,8,31,8],[33,8,35,8],[38,8,40,8],[42,8,44,8]]}
[{"$f":"Translator!B2173","v":"CN-RoHS (tab 14) Applicable for Products in Compliance Management Catalogue"}]
[{"$f":"Translator!B2174","v":"Regulated substances"},{"$f":"Translator!B2175","v":"CAS number"},null,{"$f":"Translator!B2176","v":"Limit value [mass% in homogeneous material]"},{"$f":"Translator!B3789","v":"By Substance groups: Name of the contained substances"},{"$f":"Translator!B3790","v":"By Substance groups: CAS of the contained substances"},{"$f":"Translator!B2177","v":"Concentration of substance [mass% in homogeneous material]"},{"$f":"Translator!B2178","v":"Exception claimed? If so, which one?"},{"$f":"Translator!B2179","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2180","v":"Entry\n- included ( E )\n- changed ( C )"},{"$f":"Translator!B2181","v":"test report enclosed (optional)"},{"$f":"Translator!B2182","v":"method of measurement"}]
[{"$f":"Translator!B2183","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B2184","v":"Lead"},{"$f":"Translator!B2190","v":"7439-92-1 and its compounds"},"P",0.1,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B2185","v":"Cadmium"},{"$f":"Translator!B2191","v":"7440-43-9 and its compounds"},"P",0.01,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B2186","v":"Mercury"},{"$f":"Translator!B2192","v":"7439-97-6 and its compounds"},"P",0.1,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B2187","v":"Chromium VI"},{"$f":"Translator!B2193","v":"1333-82-0 and its compounds"},"P",0.1,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B2188","v":"Polybrominated biphenyles (PBB)"},{"$f":"Translator!B2194","v":"Material group"},"P",0.1,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B2189","v":"Polybrominated diphenyl ether (PBDE)"},{"$f":"Translator!B2194","v":"Material group"},"P",0.1,null,null,null,null,null,"E2018"]
[{"$f":"Translator!B2195","v":"List of Exemptions (12. March 2018) "}]
[{"$f":"Translator!B2196","v":"Annex 1 Compliance Management Catalogue of Electric Appliances and Electronic Products for Restriction Use Hazardous Substances   (The first batch) "},null,null,null,null,null,null,null,{"$f":"Translator!B2197","v":"Annex II \nApplications Exempted From the Restriction in Product \nCompliance Management Catalogue (effective from 12. March 2019)"}]
[null,null,null,null,null,null,null,null,{"$f":"Translator!B2202","v":"#"},{"$f":"Translator!B2203","v":"Exemption"},{"$f":"Translator!B2204","v":"Restriction Limitation"}]
[{"$f":"Translator!B2198","v":"No."},{"$f":"Translator!B2199","v":"Product name"},{"$f":"Translator!B2200","v":"Product range and definition"},{"$f":"Translator!B2201","v":"Scope of application "},null,null,null,null,{"$f":"Translator!B2241","v":"Hg （Mercury）"}]
[1,{"$f":"Translator!B2205","v":"Refrigerator "},{"$f":"Translator!B2206","v":"A thermally insulated box consisting of one or multiple compartments that can be controlled at prescribed temperature, with appropriate volume and structure, is able to get the cooling capacity using natural or forced convection, and consumes one or many types of energy (volume ≤ 800 liters). "},{"$f":"Translator!B2207","v":"From the point of installation, refrigerators can be divided into upright, portable, wallmounted, embedded, or other types. From the point of usage, refrigerators can be divided into refrigerator-freezer (cabinet), freezer (cabinet), refrigerator (cabinet), freezer, horizontal freezer, display cabinet, wine cabinet, etc. Methods for determination of linear dimensions of refrigerator and measurement of the volume can be found in GB / T 8059-2016 \"Household and similar refrigerating appliances\". "},null,null,null,null,1,{"$f":"Translator!B2242","v":"Mercury in single capped (compact) fluorescent lamps for general lighting purposes"},{"$f":"Translator!B2243","v":"Per Lamp"}]
[2,{"$f":"Translator!B2208","v":"Air conditioner "},{"$f":"Translator!B2209","v":"An equipment for directly providing processed air to confined space, room or area, including room air conditioner and unitary air conditioner (rated cooling capacity ≤14,000 watts). "},{"$f":"Translator!B2210","v":"An air conditioner mainly consists of refrigeration system, air circulation and purification devices for cooling and dehumidification, and/or heating and ventilating devices (they can be assembled in a box structure, or designed as a component system to be used together). Air conditioners include room air conditioners and unitary air conditioners (rated cooling capacity ≤ 14000 watts), where: 1) Room air conditioner mainly includes cooling system and air circulation and purifying devices for cooling and dehumidification, it can also include heating and ventilation devices (they can be assembled in a box structure or designed as a component system to be used together). From the point of structure, room air conditioners can be generally divided into all-inone, split-type, and multiconnected air conditioners, etc.; from the point of function, they can be divided into the types of cold air, heat pump, cold air dehumidification, cold air heat pump dehumidification, auxiliary heat pump electric heating, etc.; and from the point of cooling method, they can be divided into water cooling and air cooling types. 2) Unitary air conditioner mainly includes cooling system and air circulation and purification devices, it can also include heating, humidification and ventilation devices. From the point of function, unitary air conditioners can be divided into cooling only, heat pump, and constant temperature and humidity types; from the point of condenser cooling method, they can be divided into watercooled, and air-cooled types; from the point of heating method, it can be divided into electric heating, and heat pump heating types; from the point of structure, it can be divided into all-in-one, and split-type; from the point of air supplying, it can be divided into direct blow, and air duct types; from the point of air conditioning capacity regulating characteristics, they can be divided into constant capacity and variable capacity types."},null,null,null,null,null,{"$f":"Translator!B2244","v":"< 30 W"},{"$f":"Translator!B2245","v":" 2.5mg"}]
[3,{"$f":"Translator!B2211","v":"Washing machine "},{"$f":"Translator!B2212","v":"An appliance driven by electric power, and washes clothes (including drying function,) through mechanical actions (dry clothes capacity ≤ 10 kg).  "},{"$f":"Translator!B2213","v":"The product range for washing machine with dry clothes capacity  ≤ 10 kg,  includes impeller type washing machine, drum type washing machine, agitator type washing machine, dehydration machine, etc.  "},null,null,null,null,null,{"$f":"Translator!B2246","v":"≥ 30 W and < 50 W"},{"$f":"Translator!B2247","v":" 3.5mg"}]
[4,{"$f":"Translator!B2214","v":"Water heater"},{"$f":"Translator!B2215","v":"A device that turns electrical energy into thermal energy through electric heating elements such as electric heating pipe, electric heating membrane, and so on, to heat water to temperature below boiling point (with capacity≤ 500 ltr.), including water storage type electric water heater, instantaneous electric water heater, etc."},{"$f":"Translator!B2216","v":"Electric water heaters include water storage type electric water heater, instantaneous electric water heater etc. (with capacity ≤ 500 ltr.), but does not include appliances and commercial vending machines with liquid heating capabilities such as coffee pots, egg boilers, stew pot, steamer, yogurt maker, hot water vending machine, etc. Where: 1) Storage type water heater refers to a fixed appliance that heats water and stores water in the container, and is equipped with water temperature control device.  2) Instantaneous water heater refers to an upright device that heats water when water flows "},null,null,null,null,null,{"$f":"Translator!B2248","v":"≥ 50 W and < 150 W"},{"$f":"Translator!B2249","v":" 5mg"}]
[5,{"$f":"Translator!B2217","v":"Printer"},{"$f":"Translator!B2218","v":"An device that receives data from sources such as automatic data processing equipment, network, platform scanners, etc., and prints text, symbol, or image on the printing media through methods such as electrostatic, inkjet, dot matrix, or thermosimaging, etc. It also includes device whose main function is printing, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min)."},{"$f":"Translator!B2219","v":"Printers include laser printer, inkjet printer, dot matrix printer, thermal printer and other equipment that work inline with computers or use cloud printing platform, to convert digital information into text and image and output the result in the form of hardcopy. It also includes devices whose main function is printing, but also has other functions. The printing format and speed shall be in according with the relevant existing standards and regulations. Printers do not include: 1) dot matrix printer with printing head pins ≥ 48; 2) designed only for printing media other than paper, such as cloth, plastic, metal, etc. 3) Needle printers, thermal printers and inkjet printers with a printing width of <110 mm "},null,null,null,null,null,{"$f":"Translator!B2250","v":"≥ 150 W"},{"$f":"Translator!B2251","v":" 15mg"}]
[6,{"$f":"Translator!B2220","v":"Copier "},{"$f":"Translator!B2221","v":"A device to obtain copies of the original writing, drawing, or printing material in the same size, magnified, or reduced in size. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, printing speed ≤ 60 sheets/min). "},{"$f":"Translator!B2222","v":"Copiers include electrostatic copier, ink jet copier, and devices that produce copies of the originals with a variety of different imaging processes. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min). Printing format and speed shall be in accordance with relevant "},null,null,null,null,null,{"$f":"Translator!B2252","v":"with circular or square structural shape and\ntube diameter ≤ 17 mm"},{"$f":"Translator!B2253","v":" 7mg"}]
[7,{"$f":"Translator!B2223","v":"Fax machine "},{"$f":"Translator!B2224","v":"A telecommunication terminal device that converts static images of text, chart, and pictures to electrical signals, sends them out using scanning and photoelectric conversion technology, and receives copies in the form of recording, including equipment whose main function is fax, but also has other functions. "},{"$f":"Translator!B2225","v":"A fax machine has two functions: to send the original; and to receive and copy the original at the same time. It includes laser, inkjet, thermal imaging, as well as multifunction fax machine which integrates two or more of the faxing, printing, scanning, or copying functions. "},null,null,null,null,null,{"$f":"Translator!B2254","v":"For special purposes"},{"$f":"Translator!B2249","v":" 5mg"}]
[8,{"$f":"Translator!B2226","v":"TV set "},{"$f":"Translator!B2227","v":"A receiving device to be used to display TV signals; an electronic product powered by electricity, designed to receive, display, and play analog and/or digital color TV broadcasting signals transmitted through ground, cable, satellite, or network.  TV sets also includes display equipment whose main function is for displaying television signals although it is not equipped with TV tuner (LNB).  "},{"$f":"Translator!B2228","v":"Including cathode-ray tube (black-and-white, color) televisions, LCD TVs, OLED TVs, rear-projection TVs, mobile TV receiving terminals and other TV tuner (tunnels) for receiving signals and restoring images and audio terminal device. Also it includes a device with main function of the display apparatus TV, even though without a television tuner (high frequency head). "},null,null,null,null,null,{"$f":"Translator!B2255","v":"< 30w and life time>= 20000h"},{"$f":"Translator!B2247","v":" 3.5mg"}]
[9,{"$f":"Translator!B2229","v":"Monitor "},{"$f":"Translator!B2230","v":"An image output device which converts video signals to optic image signal, and to display the image of the processed data by way of illustration, including cathode ray tubes (black and white, color) monitor, LCD monitor, etc. that is mainly composed of display components (no tuner). "},{"$f":"Translator!B2231","v":"From the point of material, monitor can be divided into CRT, DLP, LCD, LED, OLED, etc.; from the point of usage, they can be divided into security monitor, supervision monitor, radio and broadcasting monitor, computer monitor, and so on.  "},null,null,null,null,2.1,{"$f":"Translator!B2257","v":"Mercury in Tri-band phosphor with double-capped linear fluorescent lamps for general lighting purposes"},"Per Lamp"]
[10,{"$f":"Translator!B2232","v":"Microcomputer "},{"$f":"Translator!B2233","v":"An entity based on the hardware system of a microcomputer, configured with necessary external device and software, and is suitable for a single user, including desktop PC (including all-inone PC), portable PC, tablet, and pocket PC.  "},{"$f":"Translator!B2234","v":"Microcomputers include desktop PC (including all-in one PC), portable PC, tablet, and pocket PC. Where: 1) Desktop PC refers to PCs that are specifically designed for use on fixed desks in the office or home. It does not include computer servers, workstations that are special suitable for computer work room, and industrial PCs that are special suitable for industrial control and other PCs that have significantly different characters with desktop PCs.  2) Portable PC refers to PC that is characterized by portability, and is equipped with built-in input and output devices (such as monitors, keyboard etc.), as well as battery module; 3) Tablet: PC that takes a plate structure, and uses touch screen as the main component of input and output, and can be used hand-held. 4) Pocket PC (PDA): a handheld computing device that is running on the embedded operating system and application, and is small, lightweight, easy to carry, practical, and inexpensive. "},null,null,null,null,null,{"$f":"Translator!B2258","v":"normal lifetime and a tube diameter < 9 mm (e.g. T2)"},{"$f":"Translator!B2259","v":"4mg"}]
[11,{"$f":"Translator!B2235","v":"Mobile communication handset "},{"$f":"Translator!B2236","v":"A handheld mobile user terminal device supports at least one digital mobile communications technology (e.g., a cellular mobile communication technology GSM / GPRS, CDMA, TDSCDMA, WCDMA, CDMA2000, LTE and its follow-up  evolution and integration technology.) to send or receive phone calls or other sound, image, and data between two sites through electromagnetic wave of the cellular network. "},{"$f":"Translator!B2237","v":"Mobile communication handset does not include wearable products which have positioning, simple calling, and other functions.  "},null,null,null,null,null,{"$f":"Translator!B2260","v":"normal lifetime and a tube diameter ≥ 9 mm and ≤ 17 mm (e.g. T5)"},{"$f":"Translator!B2261","v":"3mg"}]
[12,{"$f":"Translator!B2238","v":"Telephone set "},{"$f":"Translator!B2239","v":"A telephone set is a user terminal telecommunication device that converts voice into signals that can be transmitted to another device, and converts the received signal to voice. "},{"$f":"Translator!B2240","v":"Telephone set includes ordinary PSTN telephone, internet telephone (IP telephone), and other user equipment that converts voice energy into electrical energy and vice versa. Of which: 1) Ordinary PSTN telephone: is the telephone connected to the PSTN public switched telephone network, including wireline telephone and cordless phone. 2) Internet telephone (IP telephone): user terminal equipment that makes and receives calls through the internet. "},null,null,null,null,null,{"$f":"Translator!B2262","v":"normal lifetime and a tube diameter > 17 mm and ≤ 28 mm (e.g. T8)"},{"$f":"Translator!B2247","v":" 3.5mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2263","v":"normal lifetime and a tube diameter > 28 mm (e.g. T12)"},{"$f":"Translator!B2247","v":" 3.5mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2264","v":"long lifetime (≥ 25 000 h)"},{"$f":"Translator!B2249","v":" 5mg"}]
[null,null,null,null,null,null,null,null,2.2000000000000002,{"$f":"Translator!B2266","v":"Mercury in other fluorescent lamps"},{"$f":"Translator!B2243","v":"Per Lamp"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2267","v":"Linear halophosphate lamps with tube > 28 mm (e.g. T10 and T12)"},{"$f":"Translator!B2268","v":"10 mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2269","v":"Non-linear halophosphate lamps (all diameters)"},{"$f":"Translator!B2270","v":"15 mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2271","v":"Non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9)"},{"$f":"Translator!B2270","v":"15 mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2273","v":"Lamps for other general lighting and special purposes (e.g. induction lamps)"},{"$f":"Translator!B2270","v":"15 mg"}]
[null,null,null,null,null,null,null,null,3,{"$f":"Translator!B2274","v":"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes"},{"$f":"Translator!B2243","v":"Per Lamp"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2275","v":"Short length (≤ 500 mm)"},{"$f":"Translator!B2247","v":" 3.5mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2276","v":"Medium length (> 500 mm and ≤ 1 500 mm)"},{"$f":"Translator!B2249","v":" 5mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2277","v":"Long length (> 1 500 mm)"},{"$f":"Translator!B2278","v":"13mg"}]
[null,null,null,null,null,null,null,null,4.0999999999999996,{"$f":"Translator!B2279","v":"other low pressure discharge lamps (per lamp)"},{"$f":"Translator!B2280","v":"Mercury (per lamp) ≤ 15mg"}]
[null,null,null,null,null,null,null,null,4.2,{"$f":"Translator!B2281","v":"High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner) in lamps with improved colour rendering index Ra > 60"},{"$f":"Translator!B2282","v":"Mercury (per lamp)"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2283","v":"P ≤155W"},{"$f":"Translator!B2284","v":"30mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2285","v":"155W＜P≤405W"},{"$f":"Translator!B2286","v":"40mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2287","v":"P＞405W"},{"$f":"Translator!B2286","v":"40mg"}]
[null,null,null,null,null,null,null,null,4.3,{"$f":"Translator!B2288","v":"other High Pressure Sodium (vapour) lamps"},{"$f":"Translator!B2282","v":"Mercury (per lamp)"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2283","v":"P ≤155W"},{"$f":"Translator!B2289","v":"25mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2285","v":"155W＜P≤405W"},{"$f":"Translator!B2284","v":"30mg"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2287","v":"P＞405W"},{"$f":"Translator!B2286","v":"40mg"}]
[null,null,null,null,null,null,null,null,4.4000000000000004,{"$f":"Translator!B2290","v":"Mercury in High Pressure Mercury (vapour) lamps (HPMV)"},{"$f":"Translator!B2291","v":"No limitation of use, until\nDecember 31,2020"}]
[null,null,null,null,null,null,null,null,4.5,{"$f":"Translator!B2292","v":"Mercury in metal halide lamps (MH)"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,4.5999999999999996,{"$f":"Translator!B2294","v":"Mercury in other discharge lamps for special purposes not specifically mentioned in this\nAnnex"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,4.7,{"$f":"Translator!B2295","v":"Mercury in hand crafted luminous discharge tubes (HLDTs) used for signs, decorative or architectural and specialist lighting and light-artwork,\n(a) 20 mg per electrode pair + 0,3 mg per tube length in cm, for outdoor applications and indoor applications exposed to temperatures below 20 °C;\n(b)15 mg per electrode pair + 0,24 mg, for all other indoor application"},{"$f":"Translator!B2296","v":"Mercury / per tube length\nin cm:\n80mg"}]
[null,null,null,null,null,null,null,null,5,{"$f":"Translator!B2297","v":"Mercury used as a cathode sputtering inhibitor in DC plasma displays"},{"$f":"Translator!B2298","v":"with a content ≤ 30 mg"}]
[null,null,null,null,null,null,null,null,{"$f":"Translator!B2299","v":"Pb （lead）"}]
[null,null,null,null,null,null,null,null,6.1,{"$f":"Translator!B2300","v":"Lead in glass of cathode ray tubes"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,6.2,{"$f":"Translator!B2301","v":"Lead in glass of fluorescent tubes"},{"$f":"Translator!B2302","v":"not exceeding 0,2 % by weight"}]
[null,null,null,null,null,null,null,null,7.1,{"$f":"Translator!B2303","v":"Lead as an alloying element in steel for machining purposes and in galvanised steel"},{"$f":"Translator!B2304","v":"containing up to 0,35 %\nlead by weight"}]
[null,null,null,null,null,null,null,null,7.2,{"$f":"Translator!B2305","v":"Lead as an alloying element in aluminium containing"},{"$f":"Translator!B2306","v":"up to 0,4 % lead by weight）"}]
[null,null,null,null,null,null,null,null,7.3,{"$f":"Translator!B2307","v":"Lead as an alloying element in Copper alloy"},{"$f":"Translator!B2308","v":"containing up to 4 % lead\nby weight"}]
[null,null,null,null,null,null,null,null,8.1,{"$f":"Translator!B2309","v":"Lead in high melting temperature type solders (i.e. lead- based alloys containing 85 % by weight or more lead)"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,8.1999999999999993,{"$f":"Translator!B2310","v":"Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission, and network management for telecommunications"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,"8.3.1",{"$f":"Translator!B2311","v":"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g.piezoelectronic devices, or in a glass or ceramic matrix compound"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,"8.3.2",{"$f":"Translator!B2312","v":"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,"8.3.3",{"$f":"Translator!B2313","v":"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,"8.3.4",{"$f":"Translator!B2314","v":"Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors’"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,9,{"$f":"Translator!B2315","v":"Lead in bearing shells and bushes for refrigerant-containing compressors for heating, ventilation, air conditioning and\nrefrigeration (HVACR) applications"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,10.1,{"$f":"Translator!B2316","v":"Lead used in C-press compliant pin connector\nsystems used in spare parts"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,10.199999999999999,{"$f":"Translator!B2317","v":"Lead used in other than C-press compliant pin connector systems"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,11,{"$f":"Translator!B2318","v":"Lead as a coating material for the thermal conduction module C-ring used in spare parts"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,12,{"$f":"Translator!B2319","v":"Lead in white glasses used for optical applications"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,13,{"$f":"Translator!B2320","v":"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors\nwith a lead content of more than 80 % and less than 85 % by weight"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,14,{"$f":"Translator!B2321","v":"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit flip chip packages"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,15,{"$f":"Translator!B2322","v":"Lead in linear incandescent lamps with silicate coated tubes"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,16,{"$f":"Translator!B2323","v":"Lead halide as radiant agent in high intensity discharge (HID) lamps used for professional reprography applications"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,17.100000000000001,{"$f":"Translator!B2324","v":"Lead as activator in the fluorescent powder of discharge lamps when used as speciality\nlamps for diazoprinting reprography,lithography, insect traps, photochemical and curing processes containing phosphors such as SMS（(Sr，Ba)2MgSi2O7:Pb）"},{"$f":"Translator!B2325","v":"lead by weight ≤ 1 %"}]
[null,null,null,null,null,null,null,null,17.2,{"$f":"Translator!B2326","v":"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)"},{"$f":"Translator!B2325","v":"lead by weight ≤ 1 %"}]
[null,null,null,null,null,null,null,null,18,{"$f":"Translator!B2327","v":"Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact energy saving lamps (ESL)"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,19,{"$f":"Translator!B2328","v":"Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCDs)"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,20,{"$f":"Translator!B2329","v":"Lead in finishes of fine pitch components other than connectors with a pitch of 0,65 mm and less"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,21,{"$f":"Translator!B2330","v":"Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,22,{"$f":"Translator!B2331","v":"Lead oxide in surface conduction electron emitter displays (SED) used in structural elements, notably in the seal frit and frit ring"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,23,{"$f":"Translator!B2332","v":"Lead oxide in the glass envelope of black light blue lamps"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,24,{"$f":"Translator!B2333","v":"Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,25,{"$f":"Translator!B2334","v":"Lead bound in 4 categories crystal glass"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2335","v":"1． PbO >=30% (by weight), Density ≥3.00, Refractive ≥1.545"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2336","v":"2．PbO≥24%（by weight）, Density≥2.90，Refractive≥1.545；"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2337","v":"3. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.45，Refractive≥1.520；"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B2338","v":"4. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.40，Surface hardness to Vickers hardness\n550±20。"}]
[null,null,null,null,null,null,null,null,26,{"$f":"Translator!B2339","v":"Lead in soldering materials in mercury free flat fluorescent lamps (which, e.g. are used for liquid crystal displays, design or industrial lighting)"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,27,{"$f":"Translator!B2340","v":"Lead oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,28,{"$f":"Translator!B2341","v":"Lead in solders for the soldering of thin copper wires of 100 μm diameter and less in power transformers"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,29,{"$f":"Translator!B2342","v":"Lead in cermet-based trimmer\npotentiometer elements"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,30,{"$f":"Translator!B2343","v":"Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,31,{"$f":"Translator!B2344","v":"Lead as a thermal stabiliser in polyvinyl chloride (PVC) used as base material in amperometric, potentiometric and conductometric electrochemical sensors which are used in in-vitro diagnostic medical devices for the analysis of blood and other body fluids and body gases. "},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,{"$f":"Translator!B2358","v":"Pb（lead） and Cd（Cadmium）"}]
[null,null,null,null,null,null,null,null,32,{"$f":"Translator!B2359","v":"Cadmium and lead in filter glasses and glasses used for reflectance standards"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,33,{"$f":"Translator!B2360","v":"Lead and cadmium in printing inks for the application of enamels on glasses, such as borosilicate and soda lime glasses"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,{"$f":"Translator!B2345","v":"Cd（Cadmium）"}]
[null,null,null,null,null,null,null,null,34.1,{"$f":"Translator!B2346","v":"one shot pellet type thermal cut-offs"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,34.200000000000003,{"$f":"Translator!B2347","v":"electrical contacts"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,35,{"$f":"Translator!B2348","v":"Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound\npressure levels of 100 dB (A) and more"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,36,{"$f":"Translator!B2349","v":"thick film pastes used on aluminium bonded beryllium oxide"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,37.1,{"$f":"Translator!B2350","v":"colour converting II-VI LEDs for use in solid state illumination or display systems "},{"$f":"Translator!B2351","v":"Cadmium < 10 μg Cd per square millimeter of light-emitting area"}]
[null,null,null,null,null,null,null,null,37.200000000000003,{"$f":"Translator!B2352","v":"Cadmium in cadmium-based semiconductor nanocrystal quantum dots for low energy conversion in display lighting applications\n"},{"$f":"Translator!B2353","v":"< 0.2 μg Cd per square\nmillimeter of screen display area"}]
[null,null,null,null,null,null,null,null,38,{"$f":"Translator!B2354","v":"photoresistors for analogue optocouplers applied in professional audio equipment"},{"$f":"Translator!B2293","v":"No limitation of use"}]
[null,null,null,null,null,null,null,null,{"$f":"Translator!B2355","v":"Cr VI （Hexavalent chromium）"}]
[null,null,null,null,null,null,null,null,39,{"$f":"Translator!B2356","v":"Hexavalent chromium as an anticorrosion agent of the carbon steel cooling system in absorption refrigerators"},{"$f":"Translator!B2357","v":"Hexavalent chromium ≤ 0,75 % by weight in the cooling solution"}]

{"sheet":"Translator","index":21,"n_rows":3980,"n_cols":5,"rows_kept":3980,"cut":false,"hidden":true,"merged":[[485,0,516,0],[478,0,484,0],[405,0,407,0],[389,0,398,0],[399,0,401,0],[408,0,437,0],[438,0,477,0],[402,0,404,0],[361,0,388,0],[1,0,4,0],[91,0,149,0],[5,0,55,0],[56,0,90,0],[150,0,336,0],[337,0,360,0]]}
[null,{"$f":"Cover_Sheet!E1","v":"English"},"English","German","Chinese"]
["Meta",null,"English","Deutsch","中文"]
[null,{"$f":"IF($B$1=\"English\",C3,IF($B$1=\"Deutsch\",D3,IF($B$1=\"中文\",E3,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bosch-Norm N 2580-1 Appendix"},"Bosch-Norm N 2580-1 Appendix","Bosch-Norm N 2580-1 Anhang","博世规范 N 2580-1 附件"]
[null,{"$f":"IF($B$1=\"English\",C4,IF($B$1=\"Deutsch\",D4,IF($B$1=\"中文\",E4,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SUPPLIER DECLARATION"},"SUPPLIER DECLARATION","LIEFERANTENERKLÄRUNG","供应商申报"]
[null,{"$f":"IF($B$1=\"English\",C5,IF($B$1=\"Deutsch\",D5,IF($B$1=\"中文\",E5,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Edition 2024-04-11"},"Edition 2024-04-11","Ausgabe 2024-04-11","编辑日期 2024-04-11"]
["Cover sheet",{"$f":"IF($B$1=\"English\",C6,IF($B$1=\"Deutsch\",D6,IF($B$1=\"中文\",E6,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cover Sheet Supplier Declaration of Substances"},"Cover Sheet Supplier Declaration of Substances","Deckblatt Lieferantenerklärung über Inhaltsstoffe","供应商物质申报封面"]
[null,{"$f":"IF($B$1=\"English\",C7,IF($B$1=\"Deutsch\",D7,IF($B$1=\"中文\",E7,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Language"},"Language","Sprache","语言"]
[null,{"$f":"IF($B$1=\"English\",C8,IF($B$1=\"Deutsch\",D8,IF($B$1=\"中文\",E8,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Please select / Restart"},"Please select / Restart","Bitte Auswahl treffen / Neustart","请选择/刷新"]
[null,{"$f":"IF($B$1=\"English\",C9,IF($B$1=\"Deutsch\",D9,IF($B$1=\"中文\",E9,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Supplier"},"Supplier","Lieferant","供应商"]
[null,{"$f":"IF($B$1=\"English\",C10,IF($B$1=\"Deutsch\",D10,IF($B$1=\"中文\",E10,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bosch purchasing"},"Bosch purchasing","Bosch-Einkauf","博世采购部门"]
[null,{"$f":"IF($B$1=\"English\",C11,IF($B$1=\"Deutsch\",D11,IF($B$1=\"中文\",E11,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Supplied material"},"Supplied material","Geliefertes Material","供应材料"]
[null,{"$f":"IF($B$1=\"English\",C12,IF($B$1=\"Deutsch\",D12,IF($B$1=\"中文\",E12,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Name"},"Name","Name","公司名称"]
[null,{"$f":"IF($B$1=\"English\",C13,IF($B$1=\"Deutsch\",D13,IF($B$1=\"中文\",E13,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bosch Supplier Number (RBSNO)"},"Bosch Supplier Number (RBSNO)","Bosch-Lieferanten-Nummer (RBSNO)","博世供应商编号 (RBSNO)"]
[null,{"$f":"IF($B$1=\"English\",C14,IF($B$1=\"Deutsch\",D14,IF($B$1=\"中文\",E14,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Contact person"},"Contact person","Ansprechpartner","联系人"]
[null,{"$f":"IF($B$1=\"English\",C15,IF($B$1=\"Deutsch\",D15,IF($B$1=\"中文\",E15,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material for Bosch business division(s)"},"Material for Bosch business division(s)","Material ist für Bosch-Geschäftsbereiche","此材料供应给哪个（些）博世事业部"]
[null,{"$f":"IF($B$1=\"English\",C16,IF($B$1=\"Deutsch\",D16,IF($B$1=\"中文\",E16,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Supplier Material Numbers"},"Supplier Material Numbers","Material-Nummern Lieferant","供应商材料号"]
[null,{"$f":"IF($B$1=\"English\",C17,IF($B$1=\"Deutsch\",D17,IF($B$1=\"中文\",E17,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bosch part numbers"},"Bosch part numbers","Bosch-Sachnummern","博世零件号"]
[null,{"$f":"IF($B$1=\"English\",C18,IF($B$1=\"Deutsch\",D18,IF($B$1=\"中文\",E18,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Name of Material/Component"},"Name of Material/Component","Benennung Material","材料/零件名称"]
[null,{"$f":"IF($B$1=\"English\",C19,IF($B$1=\"Deutsch\",D19,IF($B$1=\"中文\",E19,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material is part of the following Bosch product- / product series-part numbers"},"Material is part of the following Bosch product- / product series-part numbers","Material gehört zu folgenden Bosch-Erzeugnis- / Baureihen-Sachnummern","此材料用于以下博世公司产品-/产品系列-零件号"]
[null,{"$f":"IF($B$1=\"English\",C20,IF($B$1=\"Deutsch\",D20,IF($B$1=\"中文\",E20,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab"},"Tab","Register","工作表"]
[null,{"$f":"IF($B$1=\"English\",C21,IF($B$1=\"Deutsch\",D21,IF($B$1=\"中文\",E21,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated Material"},"Regulated Material","Reglementiertes Material","管制材料"]
[null,{"$f":"IF($B$1=\"English\",C22,IF($B$1=\"Deutsch\",D22,IF($B$1=\"中文\",E22,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulations valid worldwide for Bosch"},"Regulations valid worldwide for Bosch","Regelungen, die für Bosch weltweit gültig sind","博世全球适用的法规"]
[null,{"$f":"IF($B$1=\"English\",C23,IF($B$1=\"Deutsch\",D23,IF($B$1=\"中文\",E23,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Does the supply contain regulated material (see second column)?\nOptions for answering:\n- Yes\n- No"},"Does the supply contain regulated material (see second column)?\nOptions for answering:\n- Yes\n- No","Enthält die Lieferung reglementiertes Material (siehe zweite Spalte)?\nAntwortmöglichkeiten:\n- Ja\n- Nein","供给博世的货物是否含有第二栏中的管制材料?\n请选择:\n-是(yes)\n-否(no"]
[null,{"$f":"IF($B$1=\"English\",C24,IF($B$1=\"Deutsch\",D24,IF($B$1=\"中文\",E24,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Is the regulation complied with?\nSelect option from drop down menu"},"Is the regulation complied with?\nSelect option from drop down menu","Wird die Regelung eingehalten?\nAuswahl der Antworten im Drop Down Menü:","是否符合该法规？\n从下拉菜单中选择选项"]
[null,{"$f":"IF($B$1=\"English\",C25,IF($B$1=\"Deutsch\",D25,IF($B$1=\"中文\",E25,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Declaration in Tab made?\nSelect option from drop down"},"Declaration in Tab made?\nSelect option from drop down","Deklarationen im Reiter durchgeführt?\nAuswahl der Antworten im Drop Down Menü","是否在对应工作表中做出申明？\n从下拉菜单中选择选项"]
[null,{"$f":"IF($B$1=\"English\",C26,IF($B$1=\"Deutsch\",D26,IF($B$1=\"中文\",E26,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Yes"},"Yes","Ja","是 "]
[null,{"$f":"IF($B$1=\"English\",C27,IF($B$1=\"Deutsch\",D27,IF($B$1=\"中文\",E27,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No"},"No","Nein","否"]
[null,{"$f":"IF($B$1=\"English\",C28,IF($B$1=\"Deutsch\",D28,IF($B$1=\"中文\",E28,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No obligation to declare"},"No obligation to declare","Keine Deklarationspflicht","不必申报"]
[null,{"$f":"IF($B$1=\"English\",C29,IF($B$1=\"Deutsch\",D29,IF($B$1=\"中文\",E29,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other declaration format used"},"Other declaration format used","Anderes Deklarationsformat verwendet","使用其它的申报表格，例如， IMDS"]
[null,{"$f":"IF($B$1=\"English\",C30,IF($B$1=\"Deutsch\",D30,IF($B$1=\"中文\",E30,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials"},"All materials","Alle Materialien","所有材料"]
[null,{"$f":"IF($B$1=\"English\",C31,IF($B$1=\"Deutsch\",D31,IF($B$1=\"中文\",E31,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials which contain polycyclic aromatic hydrocarbons (PAH)"},"All materials which contain polycyclic aromatic hydrocarbons (PAH)","Alle Materialien, die Polyzyklische Aromatische Kohlenwasserstoffe (PAK) enthalten","所有含有多环芳烃（PAH）的材料"]
[null,{"$f":"IF($B$1=\"English\",C32,IF($B$1=\"Deutsch\",D32,IF($B$1=\"中文\",E32,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials which contain plasticizers / phthalates"},"All materials which contain plasticizers / phthalates","Alle Materialien, die Weichmacher / Phtalate enthalten","所有含有增塑剂/邻苯二甲酸酯的材料"]
[null,{"$f":"IF($B$1=\"English\",C33,IF($B$1=\"Deutsch\",D33,IF($B$1=\"中文\",E33,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials for electrical and electronic devices that are subject to EU-ROHS "},"All materials for electrical and electronic devices that are subject to EU-ROHS ","Alle Materialien für Elektro- und Elektronikgeräte, die unter EU-ROHS fallen ","所有欧盟RoHS 管制的用于电子电气设备的材料"]
[null,{"$f":"IF($B$1=\"English\",C34,IF($B$1=\"Deutsch\",D34,IF($B$1=\"中文\",E34,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials for motor vehicles that are subject to EU-ELV"},"All materials for motor vehicles that are subject to EU-ELV","Alle Materialien für Kraftfahrzeuge, die unter EU-ELV fallen","所有欧盟ELV管制的车用材料"]
[null,{"$f":"IF($B$1=\"English\",C35,IF($B$1=\"Deutsch\",D35,IF($B$1=\"中文\",E35,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials destined for customers demanding GADSL"},"All materials destined for customers demanding GADSL","Alle Materialien, die für Kunden bestimmt sind, die GADSL fordern","所有发往对GADSL有要求的客户的材料"]
[null,{"$f":"IF($B$1=\"English\",C36,IF($B$1=\"Deutsch\",D36,IF($B$1=\"中文\",E36,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Batteries and accumulators"},"Batteries and accumulators","Batterien und Akkumulatoren","干电池和蓄电池"]
[null,{"$f":"IF($B$1=\"English\",C37,IF($B$1=\"Deutsch\",D37,IF($B$1=\"中文\",E37,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Auxiliary manufacturing materials, e.g. lubricants, cleaning substances, anticorrosive agents"},"Auxiliary manufacturing materials, e.g. lubricants, cleaning substances, anticorrosive agents","Fertigungshilfsstoffe, z.B. Schmierstoffe, Reiniger, Korrosionsschutzmittel","辅助生产材料，如：润滑油、清洗剂、防锈剂等"]
[null,{"$f":"IF($B$1=\"English\",C38,IF($B$1=\"Deutsch\",D38,IF($B$1=\"中文\",E38,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cooling lubricants"},"Cooling lubricants","Kühlschmierstoffe","冷却润滑剂"]
[null,{"$f":"IF($B$1=\"English\",C39,IF($B$1=\"Deutsch\",D39,IF($B$1=\"中文\",E39,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging and packaging components"},"Packaging and packaging components","Verpackungen und Verpackungskomponenten","包装及包装用品"]
[null,{"$f":"IF($B$1=\"English\",C40,IF($B$1=\"Deutsch\",D40,IF($B$1=\"中文\",E40,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 1_RB-General\nDifferent Regulations covering Asbestos, Mercury, Ozon-depleting substances, Greenhouse gases Radioactive substances, Biocides, substances of Stockholm convention (e.g. PFOS)"},"Tab: 1_RB-General\nDifferent Regulations covering Asbestos, Mercury, Ozon-depleting substances, Greenhouse gases Radioactive substances, Biocides, substances of Stockholm convention (e.g. PFOS)","Register: 1_RB-General\nVerschiede Regelungen, wie Regelungen zu Asbest, Quecksilber, Ozon-abbauende Substanzen, Treibhausgase, Radioaktive Substanzen, Biozide, Stoffe der Stockholmer Konvention (e.g. PFOS)","表1：RB-常规\n涵盖石棉、汞、消耗臭氧层物质、温室气体、放射性物质、杀菌剂、斯德哥尔摩公约物质（例如，全氟辛烷磺酸PFOS）的不同法规"]
[null,{"$f":"IF($B$1=\"English\",C41,IF($B$1=\"Deutsch\",D41,IF($B$1=\"中文\",E41,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 2_REACH \nEC-REACH"},"Tab: 2_REACH \nEC-REACH","Register: 2_REACH \nEU-REACH","表2：REACH - 欧盟REACH"]
[null,{"$f":"IF($B$1=\"English\",C42,IF($B$1=\"Deutsch\",D42,IF($B$1=\"中文\",E42,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 3_PAH \nRules for polycyclic aromatic hydrocarbons"},"Tab: 3_PAH \nRules for polycyclic aromatic hydrocarbons","Register: 3_PAH \nRegelungen für Polyzyklische Aromatische Kohlenwasserstoffe","表3：PAH - 多环芳烃材料规范"]
[null,{"$f":"IF($B$1=\"English\",C43,IF($B$1=\"Deutsch\",D43,IF($B$1=\"中文\",E43,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 4_Plasticizers\nRules for plasticizers / phthalates"},"Tab: 4_Plasticizers\nRules for plasticizers / phthalates","Register: 4_Plasticizers\nRegelungen für Weichmacher / Phthalate ","表4：Plasticizers - 增塑剂/邻苯二甲酸酯材料规范"]
[null,{"$f":"IF($B$1=\"English\",C44,IF($B$1=\"Deutsch\",D44,IF($B$1=\"中文\",E44,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 5_ROHS\nEC-RoHS"},"Tab: 5_ROHS\nEC-RoHS","Register: 5_ROHS\nEG-RoHS","表5：ROHS - 欧盟RoHS指令"]
[null,{"$f":"IF($B$1=\"English\",C45,IF($B$1=\"Deutsch\",D45,IF($B$1=\"中文\",E45,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 6_ELV\nEC-ELV"},"Tab: 6_ELV\nEC-ELV","Register: 6_ELV\nEG-ELV","表6：ELV - 欧盟报废车辆指令"]
[null,{"$f":"IF($B$1=\"English\",C46,IF($B$1=\"Deutsch\",D46,IF($B$1=\"中文\",E46,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 7_GADSL\nGADSL"},"Tab: 7_GADSL\nGADSL","Register: 7_GADSL\nGADSL","表7：GADSL - 全球汽车申报材料清单"]
[null,{"$f":"IF($B$1=\"English\",C47,IF($B$1=\"Deutsch\",D47,IF($B$1=\"中文\",E47,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 8_Batteries\nEC-Directive on batteries and accumulators"},"Tab: 8_Batteries\nEC-Directive on batteries and accumulators","Register: 8_Batteries\nEG-Batterie- und Akkumulatorenrichtlinie","表8：Batteries - 干电池和蓄电池欧盟指令"]
[null,{"$f":"IF($B$1=\"English\",C48,IF($B$1=\"Deutsch\",D48,IF($B$1=\"中文\",E48,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 9_Manufacturing_Materials\nRules for auxiliary manufacturing materials excl. cooling lubricants"},"Tab: 9_Manufacturing_Materials\nRules for auxiliary manufacturing materials excl. cooling lubricants","Register: 9_Manufacturing_Materials\nRegelungen für Fertigungshilfsstoffe außer Kühlschmierstoffe","表9：Maufacturing materials - 除冷却润滑剂以外的辅助制造材料规范"]
[null,{"$f":"IF($B$1=\"English\",C49,IF($B$1=\"Deutsch\",D49,IF($B$1=\"中文\",E49,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 10_Cooling_Lubricants\nRules for cooling lubricants"},"Tab: 10_Cooling_Lubricants\nRules for cooling lubricants","Register: 10_Cooling_Lubricants\nRegelungen für Kühlschmierstoffe ","表10：Cooling Lubricants - 冷却润滑剂规范"]
[null,{"$f":"IF($B$1=\"English\",C50,IF($B$1=\"Deutsch\",D50,IF($B$1=\"中文\",E50,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"11.a EU Packaging directive 94/62/EC"},"11.a EU Packaging directive 94/62/EC","11.a EU Packaging directive 94/62/EC","11.a EU Packaging directive 94/62/EC"]
[null,{"$f":"IF($B$1=\"English\",C51,IF($B$1=\"Deutsch\",D51,IF($B$1=\"中文\",E51,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Declaration only via IMDS"},"Declaration only via IMDS","Deklaration nur über IMDS","仅通过IMDS申报"]
[null,{"$f":"IF($B$1=\"English\",C52,IF($B$1=\"Deutsch\",D52,IF($B$1=\"中文\",E52,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Supplier Signature"},"Supplier Signature","Unterschrift Lieferant","供应商签名"]
[null,{"$f":"IF($B$1=\"English\",C53,IF($B$1=\"Deutsch\",D53,IF($B$1=\"中文\",E53,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"We declare that all the data in this supplier declaration including all tabs and enclosures is complete and true. All data reflect the current knowledge. If the status of knowledge changes the supplier will send an updated supplier declaration to the responsible Bosch purchasing authority."},"We declare that all the data in this supplier declaration including all tabs and enclosures is complete and true. All data reflect the current knowledge. If the status of knowledge changes the supplier will send an updated supplier declaration to the responsible Bosch purchasing authority.","Wir versichern, dass alle Angaben in dieser Lieferantenerklärung einschließlich aller Register und Anlagen vollständig und richtig sind. Die Angaben entsprechen dem aktuellen Wissensstand. Falls sich der Wissensstand ändert, sendet der Lieferant eine geänderte Lieferantenerklärung an den zuständigen Bosch-Einkauf.","我们声明，该供应商申报（包括所有工作表和附件在内）的所有数据真实而且完整。所有数据反映了现有的知识水平。如果知识水平有变化，我们（供应商）将发送更新的供应商申报表给博世采购部的责任部门。"]
[null,{"$f":"IF($B$1=\"English\",C54,IF($B$1=\"Deutsch\",D54,IF($B$1=\"中文\",E54,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Place, date"},"Place, date","Ort, Datum","签署地，日期"]
[null,{"$f":"IF($B$1=\"English\",C55,IF($B$1=\"Deutsch\",D55,IF($B$1=\"中文\",E55,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Name of authorized representatives"},"Name of authorized representatives","Name der Vertretungsberechtigten","授权代表姓名"]
[null,{"$f":"IF($B$1=\"English\",C56,IF($B$1=\"Deutsch\",D56,IF($B$1=\"中文\",E56,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Signature of authorized representatives"},"Signature of authorized representatives","Unterschrift der Vertretungsberechtigten","授权代表签字"]
["Notes",{"$f":"IF($B$1=\"English\",C57,IF($B$1=\"Deutsch\",D57,IF($B$1=\"中文\",E57,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Please read the text of the Bosch Norm N 2580-1"},"Please read the text of the Bosch Norm N 2580-1","Bitte den Text der Norm N 2580-1 lesen","供应商申报(博世法规N2580-1附录)方法注释"]
[null,{"$f":"IF($B$1=\"English\",C58,IF($B$1=\"Deutsch\",D58,IF($B$1=\"中文\",E58,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5 Steps"},"5 Steps","5 Schritte","5 步驟"]
[null,{"$f":"IF($B$1=\"English\",C59,IF($B$1=\"Deutsch\",D59,IF($B$1=\"中文\",E59,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1) Select: language\n2) Fill in: yellow fields in cover sheet\n3) Select: type of material\n4) Select: business unit\n5) Select: material\n6) Fil in: look at the opened tabs and fill in the respective yellow fields\n7) Fill in: in the cover sheet make entries in accordance with info in the tabs\n8) Print and sign"},"1) Select: language\n2) Fill in: yellow fields in cover sheet\n3) Select: type of material\n4) Select: business unit\n5) Select: material\n6) Fil in: look at the opened tabs and fill in the respective yellow fields\n7) Fill in: in the cover sheet make entries in accordance with info in the tabs\n8) Print and sign","1. Auswählen: Sprache \n2. Ausfüllen: gelbe Felder im Cover Sheet\n3. Auswählen: Art des Materials\n4. Auswählen: Geschäftsbereich\n5. Auswählen: Material\n6. Ausfüllen: die aufgegangenen Register durchgehen und die zutreffenden gelben Felder ausfüllen\n7. Ausfüllen: im Cover Sheet entsprechend nach den Angaben in den Registern ausfüllen\n8. Drucken und Unterschreiben ","1)选择语言\n2)填写表格表头部分，黄色标注的项目为必填项。\n3)选择：材料类别\n4)选择相关的博世事业部\n5)选择：材料\n6)填写所有可以打开的工作表，填写相关的黄色标注项目\n7)根据相应的工作表的填写情况完成封面页的填写\n8)打印，签字"]
[null,{"$f":"IF($B$1=\"English\",C60,IF($B$1=\"Deutsch\",D60,IF($B$1=\"中文\",E60,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"NOTES - before you start:"},"NOTES - before you start:","HINWEISE - Bevor Sie starten: ","填表须知："]
[null,{"$f":"IF($B$1=\"English\",C61,IF($B$1=\"Deutsch\",D61,IF($B$1=\"中文\",E61,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tabs 1 and 2 always have to be processed, that is why \"yes\" has been entered on the cover sheet."},"Tabs 1 and 2 always have to be processed, that is why \"yes\" has been entered on the cover sheet.","Register 1 und 2 müssen immer bearbeitet werden, daher ist auf dem Deckblatt schon \"ja\" vorausgefüllt.","工作表1和2是必填的，所以在封面页中这两项已自动标记为“是”。"]
[null,{"$f":"IF($B$1=\"English\",C62,IF($B$1=\"Deutsch\",D62,IF($B$1=\"中文\",E62,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"D = Declarable (obligation to declare if limit value is exceeded), P = Prohibited (can apply with or without limit value)"},"D = Declarable (obligation to declare if limit value is exceeded), P = Prohibited (can apply with or without limit value)","D = Declarable (Deklarationspflicht, wenn Grenzwert überschritten wird), P = Prohibited (Verbot, kann mit oder ohne Grenzwert gelten)","D=需要申报(如果超过限值有义务申报)\nP=禁用(有或没有阀值都适用)"]
[null,{"$f":"IF($B$1=\"English\",C63,IF($B$1=\"Deutsch\",D63,IF($B$1=\"中文\",E63,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Example \"switch with connecting cable\": "},"Example \"switch with connecting cable\": ","Beispiel \"Schalter mit Anschlusskabel\": ","以“带连接电缆的转换器“的供应商申报为例"]
[null,{"$f":"IF($B$1=\"English\",C64,IF($B$1=\"Deutsch\",D64,IF($B$1=\"中文\",E64,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Re.item 4) \"yes\" was selected because \n- the material contains plasticizers\n- is subject to RoHS \n\"No\" was selected because \n- the material does not contain PAH\n- it is not for automotive applications\n- no batteries, auxiliary manufacturing materials, cooling lubricants and packaging are included\nRe. item 5) All prohibitions/obligations to declare were complied with\nRe. item 6) Only at tabs 2 and 4 declaration limit values were exceeded, the values were entered in the tabs"},"Re.item 4) \"yes\" was selected because \n- the material contains plasticizers\n- is subject to RoHS \n\"No\" was selected because \n- the material does not contain PAH\n- it is not for automotive applications\n- no batteries, auxiliary manufacturing materials, cooling lubricants and packaging are included\nRe. item 5) All prohibitions/obligations to declare were complied with\nRe. item 6) Only at tabs 2 and 4 declaration limit values were exceeded, the values were entered in the tabs","Zu Punkt 4) \"Ja\" wurde gewählt, weil \n- das Material Weichmacher enthält\n- es unter ROHS fällt \n\"Nein\" wurde gewählt, weil \n- das Material keine PAK enthält \n- es nicht in Automobil-Anwendungen geht\n- keine Batterien, Fertigungshilfsstoffe, Kühlschmierstoffe und Verpackungen enthalten sind\nZu Punkt 5) Alle Verbote/Deklarationspflichten wurden eingehalten\nZu Punkt 6) Nur bei Register 2 und 4 wurden Deklarationsgrenzwerte überschritten, die Werte sind in den Registern eingetragen worden","第4项选择\"是\"，因为：\n-该材料中含有增塑剂\n-该材料在欧盟RoHS管控范围内\n其余选择\"否\"，因为：\n-材料不含有PAH\n-不会应用在汽车上\n-材料中无电池、辅助制造材料、冷却液和包装\n\n第5项：所有的禁用和申报要求均符合\n第6项：只在表2和4中有需要申报的物质超过浓度限值，已在对应的工作表中输入实际浓度值"]
[null,{"$f":"IF($B$1=\"English\",C65,IF($B$1=\"Deutsch\",D65,IF($B$1=\"中文\",E65,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What is to be returned?"},"What is to be returned?","Was ist zurückzusenden?","需要返回哪些部分？"]
[null,{"$f":"IF($B$1=\"English\",C66,IF($B$1=\"Deutsch\",D66,IF($B$1=\"中文\",E66,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Send back: print cover sheet, sign, scan, email the scan and the entire Excel file to the responsible Bosch purchasing department "},"Send back: print cover sheet, sign, scan, email the scan and the entire Excel file to the responsible Bosch purchasing department ","Zurücksenden: Deckblatt drucken, unterschreiben, scannen, an den zuständigen Bosch-Einkauf den Scan und die gesamte Excel-Datei zusammen in einer E-Mail zurücksenden","返回：打印封面页，签字，扫描，通过一封电子邮件将签过名的封面页扫描件连同整个Excel表返回相应的博世采购部门；"]
[null,{"$f":"IF($B$1=\"English\",C67,IF($B$1=\"Deutsch\",D67,IF($B$1=\"中文\",E67,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"How to print the entire file?"},"How to print the entire file?","Wie wird die gesamte Datei ausgedruckt?","如何打印整个文件？"]
[null,{"$f":"IF($B$1=\"English\",C68,IF($B$1=\"Deutsch\",D68,IF($B$1=\"中文\",E68,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Click path: File > Print > Entire workbook > OK"},"Click path: File > Print > Entire workbook > OK","Klickpfad: Datei > Drucken > Gesamte Arbeitsmappe > OK","在主菜单中选择：文件 > 打印 > 全部工作表 > OK"]
[null,{"$f":"IF($B$1=\"English\",C69,IF($B$1=\"Deutsch\",D69,IF($B$1=\"中文\",E69,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"How can I search over the entire xls-file?"},"How can I search over the entire xls-file?","Wie kann man über die gesamt xls-Datei suchen?","如何在整个xls-文档中进行搜索?"]
[null,{"$f":"IF($B$1=\"English\",C70,IF($B$1=\"Deutsch\",D70,IF($B$1=\"中文\",E70,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Path: Edit > Find > Options > Click on Drop Down \"Workbook\" > click on Drop Down \"Find what\""},"Path: Edit > Find > Options > Click on Drop Down \"Workbook\" > click on Drop Down \"Find what\"","Klickpfad: Bearbeiten > Suchen > Optionen > Drop Down \"Arbeitsmappe\" anklicken > Drop Down \"Werte\" anklicken","在主菜单中选择：编辑>寻找>选项>点击向下\"工作簿\">点击向下\"查找所有\""]
[null,{"$f":"IF($B$1=\"English\",C71,IF($B$1=\"Deutsch\",D71,IF($B$1=\"中文\",E71,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Explanation of abbreviations"},"Explanation of abbreviations","Erläuterung der Abkürzungen","缩略语说明"]
[null,{"$f":"IF($B$1=\"English\",C72,IF($B$1=\"Deutsch\",D72,IF($B$1=\"中文\",E72,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EPA"},"EPA","EPA","美国环保署(EPA)"]
[null,{"$f":"IF($B$1=\"English\",C73,IF($B$1=\"Deutsch\",D73,IF($B$1=\"中文\",E73,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-Directive on batteries and accumulators "},"EC-Directive on batteries and accumulators ","EG-Batterie- und Akkumulatorenrichtlinie ","干电池和蓄电池欧盟指令"]
[null,{"$f":"IF($B$1=\"English\",C74,IF($B$1=\"Deutsch\",D74,IF($B$1=\"中文\",E74,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-ELV "},"EC-ELV ","EG-ELV ","欧盟ELV指令"]
[null,{"$f":"IF($B$1=\"English\",C75,IF($B$1=\"Deutsch\",D75,IF($B$1=\"中文\",E75,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-REACH "},"EC-REACH ","EG-REACH ","欧盟REACH指令"]
[null,{"$f":"IF($B$1=\"English\",C76,IF($B$1=\"Deutsch\",D76,IF($B$1=\"中文\",E76,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-RoHS "},"EC-RoHS ","EG-ROHS ","欧盟RoHS指令"]
[null,{"$f":"IF($B$1=\"English\",C77,IF($B$1=\"Deutsch\",D77,IF($B$1=\"中文\",E77,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-Directive on packaging and packaging waste "},"EC-Directive on packaging and packaging waste ","EG-Verpackungsrichtlinie ","包装及包装废物欧盟指令 "]
[null,{"$f":"IF($B$1=\"English\",C78,IF($B$1=\"Deutsch\",D78,IF($B$1=\"中文\",E78,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"GADSL "},"GADSL ","GADSL ","GADSL "]
[null,{"$f":"IF($B$1=\"English\",C79,IF($B$1=\"Deutsch\",D79,IF($B$1=\"中文\",E79,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"IMDS "},"IMDS ","IMDS ","IMDS "]
[null,{"$f":"IF($B$1=\"English\",C80,IF($B$1=\"Deutsch\",D80,IF($B$1=\"中文\",E80,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SVHC"},"SVHC","SVHC","SVHC"]
[null,{"$f":"IF($B$1=\"English\",C81,IF($B$1=\"Deutsch\",D81,IF($B$1=\"中文\",E81,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"VKIS-VSI Stoffliste/materials list"},"VKIS-VSI Stoffliste/materials list","VKIS-VSI Stoffliste","VKIS-VSI Stoffliste/材料清单"]
[null,{"$f":"IF($B$1=\"English\",C82,IF($B$1=\"Deutsch\",D82,IF($B$1=\"中文\",E82,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Environmental Protection Agency of the United States of America"},"Environmental Protection Agency of the United States of America","Environmental Protection Agency der Vereinigten Staaten von Amerika","美国环保署"]
[null,{"$f":"IF($B$1=\"English\",C83,IF($B$1=\"Deutsch\",D83,IF($B$1=\"中文\",E83,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 2006/66/EC on batteries and accumulators and waste batteries and accumulators"},"Directive 2006/66/EC on batteries and accumulators and waste batteries and accumulators","Richtlinie 2006/66/EG über Batterien und Akkumulatoren sowie Altbatterien und Altakkumulatoren","有关电池和蓄电池以及废弃的电池和蓄电池欧盟指令2006/66/EC"]
[null,{"$f":"IF($B$1=\"English\",C84,IF($B$1=\"Deutsch\",D84,IF($B$1=\"中文\",E84,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 2000/53/EC on End-of Life Vehicles"},"Directive 2000/53/EC on End-of Life Vehicles","Richtlinie 2000/53/EG über Altfahrzeuge","有关报废车辆的欧盟指令2000/53/EC"]
[null,{"$f":"IF($B$1=\"English\",C85,IF($B$1=\"Deutsch\",D85,IF($B$1=\"中文\",E85,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulation (EC) No 1907/2006 concerning the Registration, Evaluation, Authorization and Restriction of Chemicals (REACH)"},"Regulation (EC) No 1907/2006 concerning the Registration, Evaluation, Authorization and Restriction of Chemicals (REACH)","Verordnung (EG) Nr. 1907/2006 zur Registrierung, Bewertung, Zulassung und Beschränkung chemischer Stoffe (REACH)","有关化学品注册、评估、许可和限制（REACH）的欧盟指令 1907/2006"]
[null,{"$f":"IF($B$1=\"English\",C86,IF($B$1=\"Deutsch\",D86,IF($B$1=\"中文\",E86,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 2002/95/EC on the Restriction Of the use of certain Hazardous Substances in electrical and electronic equipment"},"Directive 2002/95/EC on the Restriction Of the use of certain Hazardous Substances in electrical and electronic equipment","Richtlinie 2002/95/EG zur Beschränkung der Verwendung bestimmter gefährlicher Stoffe in Elektro- und Elektronikgeräten","限制电子电气设备使用某些有害物质的欧盟指令 2002/95/EC"]
[null,{"$f":"IF($B$1=\"English\",C87,IF($B$1=\"Deutsch\",D87,IF($B$1=\"中文\",E87,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 94/62/EC on packaging and packaging waste"},"Directive 94/62/EC on packaging and packaging waste","Richtlinie 94/62/EG über Verpackungen und Verpackungsabfälle","有关包装及包装废物的欧盟指令94/62/EC"]
[null,{"$f":"IF($B$1=\"English\",C88,IF($B$1=\"Deutsch\",D88,IF($B$1=\"中文\",E88,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Global Automotive Declarable Substance List, includes prohibitions of materials and obligations to declare for substances that may be present in an automobile, generated by the Global Automotive Stakeholders Group (GASG)"},"Global Automotive Declarable Substance List, includes prohibitions of materials and obligations to declare for substances that may be present in an automobile, generated by the Global Automotive Stakeholders Group (GASG)","Global Automotive Declarable Substance List, enthält Stoffverbote und Deklarationspflichten für Stoffe, die im Automobil vorkommen können, erstellt durch die Global Automotive Stakeholders Group (GASG)","Global Automotive Declarable Substance List,  全球汽车申报物质清单，包括对有可能存在于汽车上的禁止使用的材料以及有义务申报的材料，由全球汽车营运组织 (GASG) 编制"]
[null,{"$f":"IF($B$1=\"English\",C89,IF($B$1=\"Deutsch\",D89,IF($B$1=\"中文\",E89,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"International Material Data System, the Internet declaration system of an association of car makers"},"International Material Data System, the Internet declaration system of an association of car makers","International Material Data System, ist das Deklarationssystem im Internet eines Verbundes von Automobilherstellern","International Material Data System, 国际材料数据系统，汽车制造商协会的互联网网上申报系统"]
[null,{"$f":"IF($B$1=\"English\",C90,IF($B$1=\"Deutsch\",D90,IF($B$1=\"中文\",E90,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances Of Very High Concern, substances that give rise to particular concern, defined in the nomination listing of the European Chemicals Agency (ECHA)"},"Substances Of Very High Concern, substances that give rise to particular concern, defined in the nomination listing of the European Chemicals Agency (ECHA)","Substances Of Very High Concern, besonders besorgniserregende Stoffe, definiert in der Kandidatenliste durch die Europäische Chemikalienagentur (ECHA)","Substances Of Very High Concern, 高度关注物质，给与特殊关注的物质，由欧洲化学品管理署（ECHA）提名列表。"]
[null,{"$f":"IF($B$1=\"English\",C91,IF($B$1=\"Deutsch\",D91,IF($B$1=\"中文\",E91,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"From the association of users of industrial lubricants, a materials listing for cooling lubricants in accordance with DIN 51385"},"From the association of users of industrial lubricants, a materials listing for cooling lubricants in accordance with DIN 51385","Verbraucherkreis Industrieschmierstoffe - Verband Schmierstoff-Industrie Stoffliste für Kühlschmierstoffe nach DIN 51385","工业润滑剂使用者协会按照 DIN 51385 编制的冷却润滑剂清单"]
[1,{"$f":"IF($B$1=\"English\",C92,IF($B$1=\"Deutsch\",D92,IF($B$1=\"中文\",E92,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diverse Rules (tab 1)"},"Diverse Rules (tab 1)","Diverse Regelung (Register 1)","Diverse - 综合材料规范(表1)"]
[null,{"$f":"IF($B$1=\"English\",C93,IF($B$1=\"Deutsch\",D93,IF($B$1=\"中文\",E93,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated Substances"},"Regulated Substances","Reglementierte Inhaltsstoffe ","管控的物质"]
[null,{"$f":"IF($B$1=\"English\",C94,IF($B$1=\"Deutsch\",D94,IF($B$1=\"中文\",E94,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS number"},"CAS number","CAS-Nummer","CAS编号"]
[null,{"$f":"IF($B$1=\"English\",C95,IF($B$1=\"Deutsch\",D95,IF($B$1=\"中文\",E95,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value"},"Limit value","Grenzwert","限值"]
[null,{"$f":"IF($B$1=\"English\",C96,IF($B$1=\"Deutsch\",D96,IF($B$1=\"中文\",E96,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient \n[mass%]"},"Concentration of ingredient \n[mass%]","Konzentration des Inhaltsstoffs \n[Massen%] ","配料含量"]
[null,{"$f":"IF($B$1=\"English\",C97,IF($B$1=\"Deutsch\",D97,IF($B$1=\"中文\",E97,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Designation of the material that contains the regulated substance"},"Designation of the material that contains the regulated substance","Benennung des Werkstoffs, in dem der reglementierte Inhaltsstoff vorhanden ist","含有管制物质的材料名称"]
[null,{"$f":"IF($B$1=\"English\",C98,IF($B$1=\"Deutsch\",D98,IF($B$1=\"中文\",E98,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cont.nr. in REACH"},"Cont.nr. in REACH","Ifd. Nr. in REACH","在欧盟REACH法规的录入号"]
[null,{"$f":"IF($B$1=\"English\",C99,IF($B$1=\"Deutsch\",D99,IF($B$1=\"中文\",E99,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Restriction conditions"},"Restriction conditions","Beschränkungsbedingungen: um mehr Text zu sehen bitte '' Auszug anzeigen'' drücken","限用条件"]
[null,{"$f":"IF($B$1=\"English\",C100,IF($B$1=\"Deutsch\",D100,IF($B$1=\"中文\",E100,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limits"},"Limits","Grenzwerte","限值"]
[null,{"$f":"IF($B$1=\"English\",C101,IF($B$1=\"Deutsch\",D101,IF($B$1=\"中文\",E101,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited substances (P)"},"Prohibited substances (P)","Verbotene Inhaltsstoffe (P)","禁用物质 (P)"]
[null,{"$f":"IF($B$1=\"English\",C102,IF($B$1=\"Deutsch\",D102,IF($B$1=\"中文\",E102,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substance rated declarable (D)"},"Substance rated declarable (D)","Deklarationspflichtige Inhaltsstoffe (D)","应申报物质（D)"]
[null,{"$f":"IF($B$1=\"English\",C103,IF($B$1=\"Deutsch\",D103,IF($B$1=\"中文\",E103,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C104,IF($B$1=\"Deutsch\",D104,IF($B$1=\"中文\",E104,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"lead"},"lead","Blei","铅"]
[null,{"$f":"IF($B$1=\"English\",C105,IF($B$1=\"Deutsch\",D105,IF($B$1=\"中文\",E105,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"lead, cadmium, chromium VI and mercury in coating materials for varnishing"},"lead, cadmium, chromium VI and mercury in coating materials for varnishing","Blei, Cadmium, Chrom VI und Quecksilber in Beschichtungsstoffen für Lackierung","铅、镉、六价铬和汞"]
[null,{"$f":"IF($B$1=\"English\",C106,IF($B$1=\"Deutsch\",D106,IF($B$1=\"中文\",E106,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethyl fumarate"},"Dimethyl fumarate","Dimethylfumarat","富马酸二甲酯"]
[null,{"$f":"IF($B$1=\"English\",C107,IF($B$1=\"Deutsch\",D107,IF($B$1=\"中文\",E107,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Aldrin\n- Chlordane\n- DDT\n- Dieldrin\n- Endrin\n- Heptachlor\n- Hexachlorobenzene\n- Mirex\n- Polychlorinated biphenyls (PCB)\n- Toxaphene \n- Hexachlorcyclohexane, invl. Lindane\n- Chlordecone\n- Pentachlorobenzene\n- Hexabromobiphenyl\n- Chloralkene C10-C13 (SCCP)"},"- Aldrin\n- Chlordane\n- DDT\n- Dieldrin\n- Endrin\n- Heptachlor\n- Hexachlorobenzene\n- Mirex\n- Polychlorinated biphenyls (PCB)\n- Toxaphene \n- Hexachlorcyclohexane, invl. Lindane\n- Chlordecone\n- Pentachlorobenzene\n- Hexabromobiphenyl\n- Chloralkene C10-C13 (SCCP)","- Aldrin\n- Chlordane\n- DDT\n- Dieldrin\n- Endrin\n- Heptachlor\n- Hexachlorobenzene\n- Mirex\n- Polychlorinated biphenyls (PCB)\n- Toxaphene \n- Hexachlorcyclohexane, invl. Lindane\n- Chlordecone\n- Pentachlorobenzene\n- Hexabromobiphenyl\n- Chloralkene C10-C13 (SCCP)","-艾试剂\n-氯丹\n-DDT\n-狄试剂\n-异狄氏剂\n-七氯\n-六氯苯\n-灭蚁灵\n-多氯联苯(PCB)\n-毒杀芬\n-六六六,包括林丹\n-开蓬\n-五氯苯\n-六溴联苯"]
[null,{"$f":"IF($B$1=\"English\",C108,IF($B$1=\"Deutsch\",D108,IF($B$1=\"中文\",E108,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C109,IF($B$1=\"Deutsch\",D109,IF($B$1=\"中文\",E109,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctanesulfonic acid and its derivatives (PFOS)"},"Perfluorooctanesulfonic acid and its derivatives (PFOS)","Perfluoroctansulfonsäure und ihre Derivate (PFOS)","全氟辛烷磺酸及其衍生物(PFOS)"]
[null,{"$f":"IF($B$1=\"English\",C110,IF($B$1=\"Deutsch\",D110,IF($B$1=\"中文\",E110,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Bemerkungen","备注"]
[null,{"$f":"IF($B$1=\"English\",C111,IF($B$1=\"Deutsch\",D111,IF($B$1=\"中文\",E111,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included ( E )\n- changed ( C )"},"Entry\n- included ( E )\n- changed ( C )","Eintrag\n- aufgenommen ( E )\n- geändert ( C )","录入记录\n-首次录入(E)\n-更新(C)"]
[null,{"$f":"IF($B$1=\"English\",C112,IF($B$1=\"Deutsch\",D112,IF($B$1=\"中文\",E112,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tricresyl phosphates and isomers (TCP)"},"Tricresyl phosphates and isomers (TCP)","Trikresylphosphat und Isomere (TKP)","磷酸三甲苯酯及其异构体 (TCP)"]
[null,{"$f":"IF($B$1=\"English\",C113,IF($B$1=\"Deutsch\",D113,IF($B$1=\"中文\",E113,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3',5,5'-Tetrabrombisphenol A (TBBPA) "},"3,3',5,5'-Tetrabrombisphenol A (TBBPA) ","3,3',5,5'-Tetrabrombisphenol A (TBBPA) ","3,3',5,5'-四溴双酚 A (TBBPA) "]
[null,{"$f":"IF($B$1=\"English\",C114,IF($B$1=\"Deutsch\",D114,IF($B$1=\"中文\",E114,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N'-di-o-tolylguanidine (DOTG)"},"N,N'-di-o-tolylguanidine (DOTG)","N,N'-Di-o-tolylguanidin (DOTG)","N,N'-二邻甲苯胍 (促进剂DOTG)"]
[null,{"$f":"IF($B$1=\"English\",C115,IF($B$1=\"Deutsch\",D115,IF($B$1=\"中文\",E115,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctanoic acid (PFOA) and its salts"},"Perfluorooctanoic acid (PFOA) and its salts","Perfluoroctansäure (PFOA) und seine Salze","全氟辛酸 (PFOA)及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C116,IF($B$1=\"Deutsch\",D116,IF($B$1=\"中文\",E116,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"polychlorinated naphthalenes (more than 3 chlorine atoms)"},"polychlorinated naphthalenes (more than 3 chlorine atoms)","Polychlorierte Naphthaline (mehr als 3 Chloratome)","多氯化萘(三个氯原子以上)"]
[null,{"$f":"IF($B$1=\"English\",C117,IF($B$1=\"Deutsch\",D117,IF($B$1=\"中文\",E117,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicones"},"Silicones","Silikone","硅"]
[null,{"$f":"IF($B$1=\"English\",C118,IF($B$1=\"Deutsch\",D118,IF($B$1=\"中文\",E118,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Zinc compounds"},"Zinc compounds","Zinkverbindungen ","锌化合物"]
[null,{"$f":"IF($B$1=\"English\",C119,IF($B$1=\"Deutsch\",D119,IF($B$1=\"中文\",E119,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material group"},"Material group","Stoffgruppe","材料组"]
[null,{"$f":"IF($B$1=\"English\",C120,IF($B$1=\"Deutsch\",D120,IF($B$1=\"中文\",E120,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- 309-00-2\n- 57-74-9\n- 50-29-3\n- 60-57-1\n- 72-20-8\n- 76-44-8\n- 118-74-1\n- 2385-85-5\n- 1336-36-3 and others\n- 8001-35-2\n- 58-89-9, 319-84-6, 319-85-7, 608-73-1\n- 143-50-0\n- 608-93-5\n- 36355-01-8\n- 85535-84-8"},"- 309-00-2\n- 57-74-9\n- 50-29-3\n- 60-57-1\n- 72-20-8\n- 76-44-8\n- 118-74-1\n- 2385-85-5\n- 1336-36-3 and others\n- 8001-35-2\n- 58-89-9, 319-84-6, 319-85-7, 608-73-1\n- 143-50-0\n- 608-93-5\n- 36355-01-8\n- 85535-84-8","- 309-00-2\n- 57-74-9\n- 50-29-3\n- 60-57-1\n- 72-20-8\n- 76-44-8\n- 118-74-1\n- 2385-85-5\n- 1336-36-3 und andere\n- 8001-35-2\n- 58-89-9, 319-84-6, 319-85-7, 608-73-1\n- 143-50-0\n- 608-93-5\n- 36355-01-8\n- 85535-84-8","- 309-00-2\n- 57-74-9\n- 50-29-3\n- 60-57-1\n- 72-20-8\n- 76-44-8\n- 118-74-1\n- 2385-85-5\n- 1336-36-3 及其它\n- 8001-35-2\n- 58-89-9, 319-84-6, 319-85-7, 608-73-1\n- 143-50-0\n- 608-93-5\n- 36355-01-8"]
[null,{"$f":"IF($B$1=\"English\",C121,IF($B$1=\"Deutsch\",D121,IF($B$1=\"中文\",E121,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibition to use, exceptions see regulation"},"Prohibition to use, exceptions see regulation","Verwendungsverbot, Ausnahmen siehe Verordnung","禁用，例外情况参见法规"]
[null,{"$f":"IF($B$1=\"English\",C122,IF($B$1=\"Deutsch\",D122,IF($B$1=\"中文\",E122,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"78-30-8 and 1330-78-5"},"78-30-8 and 1330-78-5","78-30-8 und 1330-78-5","78-30-8 及 1330-78-5"]
[null,{"$f":"IF($B$1=\"English\",C123,IF($B$1=\"Deutsch\",D123,IF($B$1=\"中文\",E123,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mg/kg"},"0,1 mg/kg","0,1 mg/kg","0.1 mg/kg"]
[null,{"$f":"IF($B$1=\"English\",C124,IF($B$1=\"Deutsch\",D124,IF($B$1=\"中文\",E124,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C125,IF($B$1=\"Deutsch\",D125,IF($B$1=\"中文\",E125,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"600 ppm in contact surfaces in final product"},"600 ppm in contact surfaces in final product","600 ppm in berührbaren Oberflächen im Endprodukt ","最终产品的接触表面不超过600PPM"]
[null,{"$f":"IF($B$1=\"English\",C126,IF($B$1=\"Deutsch\",D126,IF($B$1=\"中文\",E126,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 m%"},"0,1 m%","0,1 m%","质量百分比0.1%"]
[null,{"$f":"IF($B$1=\"English\",C127,IF($B$1=\"Deutsch\",D127,IF($B$1=\"中文\",E127,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"prohibition of use"},"prohibition of use","Verwendungsverbot","禁止使用"]
[null,{"$f":"IF($B$1=\"English\",C128,IF($B$1=\"Deutsch\",D128,IF($B$1=\"中文\",E128,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C129,IF($B$1=\"Deutsch\",D129,IF($B$1=\"中文\",E129,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C130,IF($B$1=\"Deutsch\",D130,IF($B$1=\"中文\",E130,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 m% "},"0,1 m% ","0,1 m% ","质量百分比0.1%"]
[null,{"$f":"IF($B$1=\"English\",C131,IF($B$1=\"Deutsch\",D131,IF($B$1=\"中文\",E131,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 m% in coating materials for the lacquer"},"0,1 m% in coating materials for the lacquer","0,1 m% in Beschichtungsstoffen für die Lackierung","在用于上漆的涂层材料中，质量百分比0.1%"]
[null,{"$f":"IF($B$1=\"English\",C132,IF($B$1=\"Deutsch\",D132,IF($B$1=\"中文\",E132,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 m% in hydraulic oils"},"0,1 m% in hydraulic oils","0,1 m% in Hydraulikölen","在液压油中，质量百分比0.1%"]
[null,{"$f":"IF($B$1=\"English\",C133,IF($B$1=\"Deutsch\",D133,IF($B$1=\"中文\",E133,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 m%"},"0,1 m%","0,1 m%","质量百分比0.1%"]
[null,{"$f":"IF($B$1=\"English\",C134,IF($B$1=\"Deutsch\",D134,IF($B$1=\"中文\",E134,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C135,IF($B$1=\"Deutsch\",D135,IF($B$1=\"中文\",E135,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biocide used in packaging against mold "},"Biocide used in packaging against mold ","in Verpackungen eingesetztes Biozid gegen Schimmelpilz","用于包装中的防霉剂 "]
[null,{"$f":"IF($B$1=\"English\",C136,IF($B$1=\"Deutsch\",D136,IF($B$1=\"中文\",E136,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C137,IF($B$1=\"Deutsch\",D137,IF($B$1=\"中文\",E137,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C138,IF($B$1=\"Deutsch\",D138,IF($B$1=\"中文\",E138,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C139,IF($B$1=\"Deutsch\",D139,IF($B$1=\"中文\",E139,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C140,IF($B$1=\"Deutsch\",D140,IF($B$1=\"中文\",E140,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Flame retardants\n- Plasticizers\n- Lubricants\n- Coolants\n- Solvents"},"- Flame retardants\n- Plasticizers\n- Lubricants\n- Coolants\n- Solvents","- Flammschutz\n- Weichmacher\n- Schmiermittel\n- Kühlmittel\n- Lösungsmittel","- 阻燃剂\n- 增塑剂\n- 润滑剂\n- 冷却剂\n- 溶剂"]
[null,{"$f":"IF($B$1=\"English\",C141,IF($B$1=\"Deutsch\",D141,IF($B$1=\"中文\",E141,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Vulcanization accelerator"},"Vulcanization accelerator","Vulkanisations-beschleuniger","硫化促进剂"]
[null,{"$f":"IF($B$1=\"English\",C142,IF($B$1=\"Deutsch\",D142,IF($B$1=\"中文\",E142,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polymerization agents"},"Polymerization agents","Polymerisationshilfe","合成助剂"]
[null,{"$f":"IF($B$1=\"English\",C143,IF($B$1=\"Deutsch\",D143,IF($B$1=\"中文\",E143,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2009/251/EC\nThis Decision is applicable until 15 March 2010.\nincluded in Reach\n"},"2009/251/EC\nThis Decision is applicable until 15 March 2010.\nincluded in Reach\n","2009/251/EG\nDiese Entscheidung gilt bis 15.03.2010.\naufgenommen in Reach","2009/251/EC\n此决定在2010年3月15日之前有效。已含在REACh中"]
[null,{"$f":"IF($B$1=\"English\",C144,IF($B$1=\"Deutsch\",D144,IF($B$1=\"中文\",E144,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Persistent organic pollutants (POP), Regulation (EC) No 850/2004"},"Persistent organic pollutants (POP), Regulation (EC) No 850/2004","Persistente organische Schadstoffe (POP), Verordnung (EG) Nr. 850/2004","持续性有机污染物(POP)，(EC)法规编号 850/2004"]
[null,{"$f":"IF($B$1=\"English\",C145,IF($B$1=\"Deutsch\",D145,IF($B$1=\"中文\",E145,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C146,IF($B$1=\"Deutsch\",D146,IF($B$1=\"中文\",E146,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C147,IF($B$1=\"Deutsch\",D147,IF($B$1=\"中文\",E147,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Listed in GADSL;\nMay contain and emit o-toluidine. With o-toluidine contents >0.1 percent in the mixture\nhas to be considered carcinogenic.  Additionally the material data sheet o-toluidine has to be observed."},"Listed in GADSL;\nMay contain and emit o-toluidine. With o-toluidine contents >0.1 percent in the mixture\nhas to be considered carcinogenic.  Additionally the material data sheet o-toluidine has to be observed.","in GADSL gelistet;\nkann o-Toluidin enthalten und abgeben. Bei o-Toluidingehalten ab 0,1 Prozent ist das Gemisch\nals krebserzeugend zu betrachten und zusätzlich das Stoffdatenblatt o-Toluidin zu beachten.","列于 GADSL;\n可能含有并释放出邻甲苯胺。如果邻甲苯胺在配制品中的含量超过0.1%，则应认定为致癌物质，同时要求另外查看邻甲苯胺的材料数据表。"]
[null,{"$f":"IF($B$1=\"English\",C148,IF($B$1=\"Deutsch\",D148,IF($B$1=\"中文\",E148,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Listed in GADSL ;\nscheduled prohibition acc. to EPA in 2015"},"Listed in GADSL ;\nscheduled prohibition acc. to EPA in 2015","in GADSL gelistet;\ngeplantes Verbot lt. EPA in 2015","列于 GADSL ;\n根据美国环保署 (EPA)，计划于 2015 年禁用。"]
[null,{"$f":"IF($B$1=\"English\",C149,IF($B$1=\"Deutsch\",D149,IF($B$1=\"中文\",E149,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"\"Green Passport\" Shipbuilding"},"\"Green Passport\" Shipbuilding","\"Green Passport\" Schiffbau","\"绿色护照\"造船"]
[null,{"$f":"IF($B$1=\"English\",C150,IF($B$1=\"Deutsch\",D150,IF($B$1=\"中文\",E150,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"see special prohibitions in certain auxiliary manufacturing materials (tab 9)"},"see special prohibitions in certain auxiliary manufacturing materials (tab 9)","siehe spezielle Verbote in bestimmten Fertigungshilfsstoffen (Register 9)","参见某些辅助制造材料的特别禁用（工作表9）"]
[2,{"$f":"IF($B$1=\"English\",C151,IF($B$1=\"Deutsch\",D151,IF($B$1=\"中文\",E151,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-REACH (tab 2)                                                                                                                                                                                                                   "},"EC-REACH (tab 2)                                                                                                                                                                                                                   ","EG-REACH (Register 2)                                                                                                                                                                                                                ","REACH-欧盟指令《化学品注册、评估、许可和限制》（工作表2）"]
[null,{"$f":"IF($B$1=\"English\",C152,IF($B$1=\"Deutsch\",D152,IF($B$1=\"中文\",E152,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration"},"Concentration","Konzentration [Einheit angeben]","含量"]
[null,{"$f":"IF($B$1=\"English\",C153,IF($B$1=\"Deutsch\",D153,IF($B$1=\"中文\",E153,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Part name of the specific part (in case of complex parts), regulated substance is contained."},"Part name of the specific part (in case of complex parts), regulated substance is contained.","Name des spezifischen Bauteils (bei zusammengesetzen Bauteilen), in dem der gegulierte Inhaltsstoff enthalten ist. ","含有管控物质的特定零部件的名称（如果是复杂多个零件组合）"]
[null,{"$f":"IF($B$1=\"English\",C154,IF($B$1=\"Deutsch\",D154,IF($B$1=\"中文\",E154,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Bemerkungen","评论"]
[null,{"$f":"IF($B$1=\"English\",C155,IF($B$1=\"Deutsch\",D155,IF($B$1=\"中文\",E155,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited substances (P)\nEU-REACH Annex 17"},"Prohibited substances (P)\nEU-REACH Annex 17","Verbotene Inhaltsstoffe (P)\nEG-REACH Anhang 17","禁用物质 (P)\nEU-REACH 附件 17 "]
[null,{"$f":"IF($B$1=\"English\",C156,IF($B$1=\"Deutsch\",D156,IF($B$1=\"中文\",E156,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances rated declarable (D)\nEU-REACH SVHC Candidate List"},"Substances rated declarable (D)\nEU-REACH SVHC Candidate List","Deklarationspflichtige Inhaltsstoffe (D)\nEG-REACH SVHC Kandidatenliste","应申报物质（D)\n欧盟REACH 高度关注物质SVHC候选清单"]
[null,{"$f":"IF($B$1=\"English\",C157,IF($B$1=\"Deutsch\",D157,IF($B$1=\"中文\",E157,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2-tetrachloroethane"},"1,1,1,2-tetrachloroethane","1,1,1,2-Tetrachlorethan","1, 1, 1, 2-四氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C158,IF($B$1=\"Deutsch\",D158,IF($B$1=\"中文\",E158,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,2,2-tetrachloroethane"},"1,1,2,2-tetrachloroethane","1,1,2,2-Tetrachlorethan","1,1,2,2-四氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C159,IF($B$1=\"Deutsch\",D159,IF($B$1=\"中文\",E159,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,2-trichloroethane"},"1,1,2-trichloroethane","1,1,2-Trichlorethan","1, 1, 2-三氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C160,IF($B$1=\"Deutsch\",D160,IF($B$1=\"中文\",E160,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1-Dichloroethylene"},"1,1-Dichloroethylene","1,1-Dichlorethen","1, 1-二氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C161,IF($B$1=\"Deutsch\",D161,IF($B$1=\"中文\",E161,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2-butoxyethoxy)ethanol (DEGBE)"},"2-(2-butoxyethoxy)ethanol (DEGBE)","2-(2-Butoxyethoxy)ethanol (DEGBE)","2-(2-丁氧基乙氧基)乙醇 (DEGBE)"]
[null,{"$f":"IF($B$1=\"English\",C162,IF($B$1=\"Deutsch\",D162,IF($B$1=\"中文\",E162,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2-methoxyethoxy)ethanol (DEGME)"},"2-(2-methoxyethoxy)ethanol (DEGME)","2-(2-Methoxyethoxy)ethanol (DEGME)","2-(2-甲氧基乙氧基)乙醇 (DEGME)"]
[null,{"$f":"IF($B$1=\"English\",C163,IF($B$1=\"Deutsch\",D163,IF($B$1=\"中文\",E163,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2­naphthylamine"},"2­naphthylamine","2-Naphthylamin","2-萘胺"]
[null,{"$f":"IF($B$1=\"English\",C164,IF($B$1=\"Deutsch\",D164,IF($B$1=\"中文\",E164,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-aminobiphenyl, xenylamine"},"4-aminobiphenyl, xenylamine","4-Aminobiphenyl, Xenylamin","4-氨基联苯；苯基苯胺"]
[null,{"$f":"IF($B$1=\"English\",C165,IF($B$1=\"Deutsch\",D165,IF($B$1=\"中文\",E165,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-nitrobiphenyl"},"4-nitrobiphenyl","4-Nitrobiphenyl","4-硝基联苯"]
[null,{"$f":"IF($B$1=\"English\",C166,IF($B$1=\"Deutsch\",D166,IF($B$1=\"中文\",E166,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) Creosote; wash oil\nb) Creosote oil, wash oil\nc) Distillates (coal tar), naphthalene oils; naphthalene oil\nd) Creosote oil, acenaphthene fraction;\nwash oil\ne) Higher-boiling distillates (coal tar);\nheavy anthracene oil\nf) Anthracene oil\ng) Tar acids, coal, crude oil; crude phenols\nh) Creosote, wood\ni) Low-temperature coal tar alkaline,\nextraction residue (coal)"},"a) Creosote; wash oil\nb) Creosote oil, wash oil\nc) Distillates (coal tar), naphthalene oils; naphthalene oil\nd) Creosote oil, acenaphthene fraction;\nwash oil\ne) Higher-boiling distillates (coal tar);\nheavy anthracene oil\nf) Anthracene oil\ng) Tar acids, coal, crude oil; crude phenols\nh) Creosote, wood\ni) Low-temperature coal tar alkaline,\nextraction residue (coal)","a) Kreosot; Waschöl\nb) Kreosotöl, Waschöl\nc) Destillate (Kohlenteer), Naphthalinöle;\nNaphtalinöl\nd) Kreosotöl, Acenaphthen-Fraktion;\nWaschöl\ne) höher siedende Destillate (Kohlenteer);\nschweres Anthracenöl\nf) Anthracenöl\ng) Teersäuren, Kohle, Rohöl; Rohphenole\nh) Kreosot, Holz\ni) Niedrigtemperatur-Kohleteeralkalin,\nExtraktrückstände\n(Kohle)","a) 杂酚油; 清洗用油\nb) 杂酚油; 清洗用油\nc) 石脑油蒸馏物\nd) 杂酚油，苊的馏分；清洗用油\ne) 干馏油（煤焦油），上层馏分；重蒽油\nf) 蒽油\ng) 焦油酸，煤，原油；粗苯酚\nh) 杂酚油，木材\ni) 碱性的低温焦油；煤取物中的碱性低温焦油"]
[null,{"$f":"IF($B$1=\"English\",C167,IF($B$1=\"Deutsch\",D167,IF($B$1=\"中文\",E167,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) Powder of Panama bark\nb) Powder of the root of the green and the black hellebore\nc) Powder of the root of the white hellebore and the black False hellebore\nd) Benzidine and/or its derivatives\ne) Benzole\nf) O-nitrobenzaldehyde\ng) Dust\nh) Ammonium sulfide\ni) Ammonium hydrogensulfide\nj) Ammonium polysulfide\nk) Methyl bromoacetate\nl) Ethyl bromoacetate \nm) Propyl bromoacetate\nn) Butyl bromoacetate"},"a) Powder of Panama bark\nb) Powder of the root of the green and the black hellebore\nc) Powder of the root of the white hellebore and the black False hellebore\nd) Benzidine and/or its derivatives\ne) Benzole\nf) O-nitrobenzaldehyde\ng) Dust\nh) Ammonium sulfide\ni) Ammonium hydrogensulfide\nj) Ammonium polysulfide\nk) Methyl bromoacetate\nl) Ethyl bromoacetate \nm) Propyl bromoacetate\nn) Butyl bromoacetate","a) Panamarindenpulver\nb) Pulver aus der Wurzel der grünen und der schwarzen Nieswurz\nc) Pulver aus der Wurzel der weißen Nieswurz und des schwarzen Germer\nd) Benzidin und/oder seine Derivate\ne) Benzol\nf) o-Nitrobenzaldehyd\ng) Holzstaub\nh) Ammoniumsulfid\ni) Ammoniumhydrogensulfid\nj) Ammoniumpolysulfid\nk) Methylbromacetat\nl) Ethylbromacetat\nm) Propylbromacetat\nn) Butylbromacetat","a) 巴拿马树皮的粉末\nb) 绿藜芦与黑藜芦根的粉末\nc) 白藜芦与黑藜芦根的粉末\nd) 对二氨基联苯和/或其衍生物\ne) 不纯苯\nf) 邻-硝基苯甲醛\ng) 灰尘\nh) 硫化铵\ni) 硫氢化铵\nj) 多硫化铵\nk) 溴乙酸甲酯\nl) 溴乙酸乙酯\nm) 溴乙酸丙酯\nn) 溴乙酸丁酯"]
[null,{"$f":"IF($B$1=\"English\",C168,IF($B$1=\"Deutsch\",D168,IF($B$1=\"中文\",E168,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C 10 -C 13 , chlorine (short-chain chlorinated paraffins)"},"Alkanes, C 10 -C 13 , chlorine (short-chain chlorinated paraffins)","Alkane, C 10 -C 13 , Chlor (kurzkettige\nChlorparaffine)","氯化烷烃(10-13个碳原子)；短链\n氯化石蜡"]
[null,{"$f":"IF($B$1=\"English\",C169,IF($B$1=\"Deutsch\",D169,IF($B$1=\"中文\",E169,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium nitrate (AN) in fertilizer"},"Ammonium nitrate (AN) in fertilizer","Ammoniumnitrat (AN) in Dünger","肥料中的硝酸铵 (AN)"]
[null,{"$f":"IF($B$1=\"English\",C170,IF($B$1=\"Deutsch\",D170,IF($B$1=\"中文\",E170,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Arsenic and its combinations"},"Arsenic and its combinations","Arsen und seine Verbindungen","砷及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C171,IF($B$1=\"Deutsch\",D171,IF($B$1=\"中文\",E171,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Asbestos"},"Asbestos","Asbest\n","石棉"]
[null,{"$f":"IF($B$1=\"English\",C172,IF($B$1=\"Deutsch\",D172,IF($B$1=\"中文\",E172,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Azo dyes with aromatic amines"},"Azo dyes with aromatic amines","Azofarbstoffe mit aromatischen Aminen","含有芳香胺的偶氮染料"]
[null,{"$f":"IF($B$1=\"English\",C173,IF($B$1=\"Deutsch\",D173,IF($B$1=\"中文\",E173,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzidine"},"Benzidine","Benzidin","对二氨基联苯"]
[null,{"$f":"IF($B$1=\"English\",C174,IF($B$1=\"Deutsch\",D174,IF($B$1=\"中文\",E174,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzole except in fuels"},"Benzole except in fuels","Benzol ausser in Treibstoffen","苯，燃料中的苯除外"]
[null,{"$f":"IF($B$1=\"English\",C175,IF($B$1=\"Deutsch\",D175,IF($B$1=\"中文\",E175,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead carbonates in colors"},"Lead carbonates in colors","Bleicarbonate in Farben","颜料中的碳酸铅"]
[null,{"$f":"IF($B$1=\"English\",C176,IF($B$1=\"Deutsch\",D176,IF($B$1=\"中文\",E176,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead sulfates in colors"},"Lead sulfates in colors","Bleisulfate in Farben","颜色中的硫酸铅"]
[null,{"$f":"IF($B$1=\"English\",C177,IF($B$1=\"Deutsch\",D177,IF($B$1=\"中文\",E177,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium in certain applications"},"Cadmium in certain applications","Cadmium in bestimmten Anwendungen","某些应用中的镉"]
[null,{"$f":"IF($B$1=\"English\",C178,IF($B$1=\"Deutsch\",D178,IF($B$1=\"中文\",E178,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloroethene (vinyl chloride) as propellant for aerosols"},"Chloroethene (vinyl chloride) as propellant for aerosols","Chlorethen (Vinylchlorid) als Treibgas für Aerosole","作为气溶胶推进物的氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C179,IF($B$1=\"Deutsch\",D179,IF($B$1=\"中文\",E179,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloroform"},"Chloroform","Chloroform","氯仿"]
[null,{"$f":"IF($B$1=\"English\",C180,IF($B$1=\"Deutsch\",D180,IF($B$1=\"中文\",E180,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium-VI-combinations in cement and cementitious mixtures"},"Chromium-VI-combinations in cement and cementitious mixtures","Chrom-VI-Verbindungen in Zement und zementhaltigen Gemischen","水泥和水泥配制品中的六价铬化合物"]
[null,{"$f":"IF($B$1=\"English\",C181,IF($B$1=\"Deutsch\",D181,IF($B$1=\"中文\",E181,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cyclohexane"},"Cyclohexane","Cyclohexan","环己烷"]
[null,{"$f":"IF($B$1=\"English\",C182,IF($B$1=\"Deutsch\",D182,IF($B$1=\"中文\",E182,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"dichloromethane (DCM)"},"dichloromethane (DCM)","Dichlormethan (DCM)","二氯甲烷（DCM）"]
[null,{"$f":"IF($B$1=\"English\",C183,IF($B$1=\"Deutsch\",D183,IF($B$1=\"中文\",E183,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl ether octabromium derivative"},"Diphenyl ether octabromium derivative","Diphenylether-Octabromderivat","二苯醚的八溴代衍生物"]
[null,{"$f":"IF($B$1=\"English\",C184,IF($B$1=\"Deutsch\",D184,IF($B$1=\"中文\",E184,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl ether pentabromium derivative"},"Diphenyl ether pentabromium derivative","Diphenylether-Pentabromderivat","二苯醚的五溴代衍生物"]
[null,{"$f":"IF($B$1=\"English\",C185,IF($B$1=\"Deutsch\",D185,IF($B$1=\"中文\",E185,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-μ-oxo-di-n-butylstanniohydroxyborane,\ndibutyl tin hydrogen borate\nC 8 H 19 BO 3 Sn (DBB)"},"Di-μ-oxo-di-n-butylstanniohydroxyborane,\ndibutyl tin hydrogen borate\nC 8 H 19 BO 3 Sn (DBB)","Di-μ-oxo-di-n-butylstanniohydroxyboran,\nDibutylzinnhydrogenborat\nC 8 H 19 BO 3 Sn (DBB)","二-μ-氧-正丁基锡羟基硼烷，二丁基锡氢硼烷C 8 H 19 BO 3 Sn (DBB)"]
[null,{"$f":"IF($B$1=\"English\",C186,IF($B$1=\"Deutsch\",D186,IF($B$1=\"中文\",E186,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mutagenic materials of category 1A or 1B acc. to GHS (1 or 2 acc. to 67/548/EWG)"},"Mutagenic materials of category 1A or 1B acc. to GHS (1 or 2 acc. to 67/548/EWG)","Erbgutverändernde Stoffe der Kategorie 1A oder 1B gemäß GHS (1 oder 2 gemäß 67/548/EWG)","根据GHS，1A或1B类诱导有机体突变物质 （或根据67/548/EWG， 1类或2类诱变物质）"]
[null,{"$f":"IF($B$1=\"English\",C187,IF($B$1=\"Deutsch\",D187,IF($B$1=\"中文\",E187,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Liquid substances or mixtures rated hazardous in accordance with the definitions in guideline 67/548/EWG and guideline 1999/45/EG"},"Liquid substances or mixtures rated hazardous in accordance with the definitions in guideline 67/548/EWG and guideline 1999/45/EG","Flüssige Stoffe oder Gemische, die nach den Definitionen in der Richtlinie 67/548/EWG und der Richtlinie 1999/45/EG als gefährlich gelten","根据指令67/548/EWG和指令1999/45/EG视为危险的液体物质或配制品\n"]
[null,{"$f":"IF($B$1=\"English\",C188,IF($B$1=\"Deutsch\",D188,IF($B$1=\"中文\",E188,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Repro-toxic materials of category 1A or 1B acc. to GHS (1 or 2 acc. to 67/548/EWG)"},"Repro-toxic materials of category 1A or 1B acc. to GHS (1 or 2 acc. to 67/548/EWG)","Fortpflanzungsgefährdende Stoffe der Kategorie 1A oder 1B gemäß GHS (1 oder 2 gemäß 67/548/EWG)","根据GHS，1A或1B类生殖毒性物质 （或根据67/548/EWG， 1类或2类生殖毒性物质）"]
[null,{"$f":"IF($B$1=\"English\",C189,IF($B$1=\"Deutsch\",D189,IF($B$1=\"中文\",E189,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachloroethane"},"Hexachloroethane","Hexachlorethan","六氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C190,IF($B$1=\"Deutsch\",D190,IF($B$1=\"中文\",E190,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Carcinogenic materials of category 1A or 1B acc. to GHS (1 or 2 acc. to 67/548/EWG)"},"Carcinogenic materials of category 1A or 1B acc. to GHS (1 or 2 acc. to 67/548/EWG)","Krebserzeugende Stoffe der Kategorie 1A oder 1B gemäß GHS (1 oder 2 gemäß 67/548/EWG)","根据GHS，1A或1B类致癌物质 （或根据67/548/EWG， 1类或2类致癌物质）"]
[null,{"$f":"IF($B$1=\"English\",C191,IF($B$1=\"Deutsch\",D191,IF($B$1=\"中文\",E191,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methylenediphenyl diisocyanate (MDI)\nincluding the following specific isomers:\n(a) 4,4’-Methylenediphenyl diisocyanate (MDI)\n(b) 2,4’-Methylenediphenyl diisocyanate (MDI)\n(c) 2,2’-Methylenediphenyl diisocyanate (MDI)\n"},"Methylenediphenyl diisocyanate (MDI)\nincluding the following specific isomers:\n(a) 4,4’-Methylenediphenyl diisocyanate (MDI)\n(b) 2,4’-Methylenediphenyl diisocyanate (MDI)\n(c) 2,2’-Methylenediphenyl diisocyanate (MDI)\n","Methylendiphenyl-Diisocyanat (MDI)\neinschließlich der nachstehenden spezifischen Isomere:\na) 4,4’-Methylendiphenyl-Diisocyanat (MDI)\nb) 2,4’-Methylendiphenyl-Diisocyanat (MDI)\nc) 2,2’-Methylendiphenyl-Diisocyanat (MDI)\n","二苯基甲烷二异氰酸酯 (MDI)，包括以下同分异构体：\n(a) 4,4’-二苯基甲烷二异氰酸酯 (MDI)\n(b) 2,4’-二苯基甲烷二异氰酸酯 (MDI)\n(c) 2,2’-二苯基甲烷二异氰酸酯 (MDI)"]
[null,{"$f":"IF($B$1=\"English\",C192,IF($B$1=\"Deutsch\",D192,IF($B$1=\"中文\",E192,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyldibromodiphenyl-methane\nbromobenzylbromotoluene, isomeric compound (DBBT)"},"Monomethyldibromodiphenyl-methane\nbromobenzylbromotoluene, isomeric compound (DBBT)","Monomethyldibromdiphenylmethan\nBrombenzylbromtoluol, Isomerengemisch (DBBT)","单甲基二溴二苯基甲烷；溴苯甲基溴甲苯异构物配制品(DBBT)"]
[null,{"$f":"IF($B$1=\"English\",C193,IF($B$1=\"Deutsch\",D193,IF($B$1=\"中文\",E193,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyldichlordiphenyl-methane (Ugilec 121) "},"Monomethyldichlordiphenyl-methane (Ugilec 121) ","Monomethyldichlordiphenylmethan (Ugilec 121) ","单甲基二氯二苯基甲烷(Ugilec 121) "]
[null,{"$f":"IF($B$1=\"English\",C194,IF($B$1=\"Deutsch\",D194,IF($B$1=\"中文\",E194,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyl-tetrachloro-diphenyl methane (Ugilec 141) "},"Monomethyl-tetrachloro-diphenyl methane (Ugilec 141) ","Monomethyltetrachlordiphenylmethan (Ugilec 141) ","单甲基四氯二苯基甲烷(Ugilec 141) "]
[null,{"$f":"IF($B$1=\"English\",C195,IF($B$1=\"Deutsch\",D195,IF($B$1=\"中文\",E195,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nickel and its combinations"},"Nickel and its combinations","Nickel und seine Verbindungen","镍及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C196,IF($B$1=\"Deutsch\",D196,IF($B$1=\"中文\",E196,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol"},"Nonylphenol","Nonylphenol","壬基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C197,IF($B$1=\"Deutsch\",D197,IF($B$1=\"中文\",E197,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol ethoxylates"},"Nonylphenol ethoxylates","Nonylphenolethoxylate","壬基酚聚乙氧基醚"]
[null,{"$f":"IF($B$1=\"English\",C198,IF($B$1=\"Deutsch\",D198,IF($B$1=\"中文\",E198,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachloroethane "},"Pentachloroethane ","Pentachlorethan","五氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C199,IF($B$1=\"Deutsch\",D199,IF($B$1=\"中文\",E199,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenol (PCP)"},"Pentachlorophenol (PCP)","Pentachlorphenol (PCP)","五氯苯酚 (PCP)"]
[null,{"$f":"IF($B$1=\"English\",C200,IF($B$1=\"Deutsch\",D200,IF($B$1=\"中文\",E200,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctane sulfonate (PFOS)"},"Perfluorooctane sulfonate (PFOS)","Perfluoroctansulfonate (PFOS)","十七氟辛烷磺酸 (PFOS)"]
[null,{"$f":"IF($B$1=\"English\",C201,IF($B$1=\"Deutsch\",D201,IF($B$1=\"中文\",E201,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phthalates\na) Di-2-ethylhexyl phthalate (DEHP)\nb) Dibutyl phthalate (DBP)\nc) Butyl benzyl phthalate  (BBP)\nd) Diisononyl Phthalate (DINP)\ne) Diisodecyl Phthalate (DIDP)\nf) Di-n-octylphthalate (DNOP)"},"Phthalates\na) Di-2-ethylhexyl phthalate (DEHP)\nb) Dibutyl phthalate (DBP)\nc) Butyl benzyl phthalate  (BBP)\nd) Diisononyl Phthalate (DINP)\ne) Diisodecyl Phthalate (DIDP)\nf) Di-n-octylphthalate (DNOP)","Phthalate\na) Di(2-ethylhexyl)phthalat (DEHP)\nb) Dibutylphthalat (DBP)\nc) Benzylbutylphtalat (BBP)\nd) Diisononylphthalat (DINP)\ne) Diisodecylphthalat (DIDP)\nf) Di-n-octylphthalat (DNOP)","邻苯二甲酸酯\na) 邻苯二甲酸二(2-乙基)己酯  (DEHP)\nb) 邻苯二甲酸二丁酯 (DBP)\nc) 邻苯二甲酸丁基苄基酯  (BBP)\nd) 邻苯二甲酸二异壬酯  (DINP)\ne) 邻苯二甲酸二异癸酯  (DIDP)\nf) 邻苯二甲酸二正辛酯 (DNOP)"]
[null,{"$f":"IF($B$1=\"English\",C202,IF($B$1=\"Deutsch\",D202,IF($B$1=\"中文\",E202,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated biphenyles (PBB)"},"Polybrominated biphenyles (PBB)","Polybrombiphenyle; polybromierte Biphenyle (PBB)","聚溴化二苯 (PBB)"]
[null,{"$f":"IF($B$1=\"English\",C203,IF($B$1=\"Deutsch\",D203,IF($B$1=\"中文\",E203,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated terphenyls (PCT)"},"Polychlorinated terphenyls (PCT)","Polychlorierte Terphenyle (PCT)","多氯代三联苯 (PCT)"]
[null,{"$f":"IF($B$1=\"English\",C204,IF($B$1=\"Deutsch\",D204,IF($B$1=\"中文\",E204,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polycyclic aromatic hydrocarbons (PAK)\na) Benzo(a)pyrene (BaP)\nb) Benzo[e]pyrene (BeP)\nc) Benz[a]anthracene (BaA)\nd) Chrysene (CHR)\ne) Benzo[b]fluoranthene (BbFA)\nf) Benzo(j)fluoranthene (BjFA)\ng) Benzo[k]fluoranthene (BkFA)\nh) Dibenz(a,h)anthracene (DBAhA)"},"Polycyclic aromatic hydrocarbons (PAK)\na) Benzo(a)pyrene (BaP)\nb) Benzo[e]pyrene (BeP)\nc) Benz[a]anthracene (BaA)\nd) Chrysene (CHR)\ne) Benzo[b]fluoranthene (BbFA)\nf) Benzo(j)fluoranthene (BjFA)\ng) Benzo[k]fluoranthene (BkFA)\nh) Dibenz(a,h)anthracene (DBAhA)","Polyzyklische aromatische Kohlenwasserstoffe (PAK)\na) Benzo(a)pyren (BaP)\nb) Benzo(e)pyren (BeP)\nc) Benzo(a)anthracen (BaA)\nd) Chrysen (CHR)\ne) Benzo(b)fluoranthen (BbFA)\nf) Benzo(j)fluoranthen (BjFA)\ng) Benzo(k)fluoranthen (BkFA)\nh) Dibenzo(a,h)anthracen (DBAhA)","多环芳烃 (PAK)\na) 苯并 (a) 芘  (BaP)\nb) 苯并 (e) 芘  (BeP)\nc) 苯并(a)蒽 (BaA)\nd) 屈 (CHR)\ne) 苯并(b)荧蒽 (BbFA)\nf) 苯并(j)荧蒽 (BjFA)\ng) 苯并(k)荧蒽 (BkFA)\nh) 二苯(a,h)蒽 (DBAhA)"]
[null,{"$f":"IF($B$1=\"English\",C205,IF($B$1=\"Deutsch\",D205,IF($B$1=\"中文\",E205,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury and its combinations "},"Mercury and its combinations ","Quecksilber und seine Verbindungen ","汞及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C206,IF($B$1=\"Deutsch\",D206,IF($B$1=\"中文\",E206,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances rated, following the criteria\nof guideline 67/548/EWG, \nflammable, highly flammable\nor extremely flammable,\nregardless of whether they are listed \nin Annex VI Part 3\nof the ordinance (EG) number\n1272/2008"},"Substances rated, following the criteria\nof guideline 67/548/EWG, \nflammable, highly flammable\nor extremely flammable,\nregardless of whether they are listed \nin Annex VI Part 3\nof the ordinance (EG) number\n1272/2008","Stoffe, die gemäß den Kriterien\nder Richtlinie 67/548/EWG als\nentzündlich, leicht entzündlich\noder hoch entzündlich eingestuft\nwurden, und zwar unabhängig\ndavon, ob sie in Anhang VI Teil 3\nder Verordnung (EG) Nr.\n1272/2008 aufgeführt sind","根据欧盟67/548/EWG指令的划分标准，被界定为可燃、易燃和极易燃三类物质，无论其是否被列入法规（EG）1272/2008号的附件VI第三部分"]
[null,{"$f":"IF($B$1=\"English\",C207,IF($B$1=\"Deutsch\",D207,IF($B$1=\"中文\",E207,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Toluene in adhesives and pressurized paint dispensers "},"Toluene in adhesives and pressurized paint dispensers ","Toluol in Klebstoffen und Farbsprühdosen","粘合剂及加压涂料分配器中的甲苯"]
[null,{"$f":"IF($B$1=\"English\",C208,IF($B$1=\"Deutsch\",D208,IF($B$1=\"中文\",E208,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris-(2,3-dibromopropyl)phosphate "},"Tris-(2,3-dibromopropyl)phosphate ","Tri-(2,3-Dibrompropyl)-Phosphat","磷酸三(2,3-二溴丙基)酯  "]
[null,{"$f":"IF($B$1=\"English\",C209,IF($B$1=\"Deutsch\",D209,IF($B$1=\"中文\",E209,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichlorobenzene"},"Trichlorobenzene","Trichlorbenzol","三氯苯"]
[null,{"$f":"IF($B$1=\"English\",C210,IF($B$1=\"Deutsch\",D210,IF($B$1=\"中文\",E210,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris-(aziridinyl)-phosphine oxide"},"Tris-(aziridinyl)-phosphine oxide","Tris-(aziridinyl)-phosphinoxid","三-(吖丙啶基)氧化膦"]
[null,{"$f":"IF($B$1=\"English\",C211,IF($B$1=\"Deutsch\",D211,IF($B$1=\"中文\",E211,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Organic tin compounds"},"Organic tin compounds","Zinnorganische Verbindungen","有机锡化合物"]
[null,{"$f":"IF($B$1=\"English\",C212,IF($B$1=\"Deutsch\",D212,IF($B$1=\"中文\",E212,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) 68990-67-0\nb) None\nc) None\nd) 92-87-5\ne) 71-43-2\nf) 552-89-6\ng) None\nh) 12135-76-1\ni) 12124-99-1\nj) 9080-17-5\nk) 96-32-2\nl) 105-36-2\nm) 35223-80-4\nn) 18991-98-5"},"a) 68990-67-0\nb) None\nc) None\nd) 92-87-5\ne) 71-43-2\nf) 552-89-6\ng) None\nh) 12135-76-1\ni) 12124-99-1\nj) 9080-17-5\nk) 96-32-2\nl) 105-36-2\nm) 35223-80-4\nn) 18991-98-5","a) 68990-67-0\nb) keine\nc) keine\nd) 92-87-5\ne) 71-43-2\nf) 552-89-6\ng) keine\nh) 12135-76-1\ni) 12124-99-1\nj) 9080-17-5\nk) 96-32-2\nl) 105-36-2\nm) 35223-80-4\nn) 18991-98-5","a) 68990-67-0\nb) 无\nc) 无\nd) 92-87-5\ne) 71-43-2\nf) 552-89-6\ng) 无\nh) 12135-76-1\ni) 12124-99-1\nj) 9080-17-5\nk) 96-32-2\nl) 105-36-2\nm) 35223-80-4\nn) 18991-98-5"]
[null,{"$f":"IF($B$1=\"English\",C213,IF($B$1=\"Deutsch\",D213,IF($B$1=\"中文\",E213,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"None"},"None","Keine","无"]
[null,{"$f":"IF($B$1=\"English\",C214,IF($B$1=\"Deutsch\",D214,IF($B$1=\"中文\",E214,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) 117-81-7\nb) 84-74-2\nc) 85-68-7\nd) 28553-12-0 and 68515-48-0\ne) 26761-40-0 and 68515-49-1\nf) 117-84-0"},"a) 117-81-7\nb) 84-74-2\nc) 85-68-7\nd) 28553-12-0 and 68515-48-0\ne) 26761-40-0 and 68515-49-1\nf) 117-84-0","a) 117-81-7\nb) 84-74-2\nc) 85-68-7\nd) 28553-12-0 und 68515-48-0\ne) 26761-40-0 und 68515-49-1\nf) 117-84-0","a) 117-81-7\nb) 84-74-2\nc) 85-68-7\nd) 28553-12-0 和 68515-48-0\ne) 26761-40-0 和 68515-49-1\nf) 117-84-0"]
[null,{"$f":"IF($B$1=\"English\",C215,IF($B$1=\"Deutsch\",D215,IF($B$1=\"中文\",E215,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"18 and 18a"},"18 and 18a","18 und 18a","18 及 18a"]
[null,{"$f":"IF($B$1=\"English\",C216,IF($B$1=\"Deutsch\",D216,IF($B$1=\"中文\",E216,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Without prejudice to the other parts of this Annex, the following shall apply to entries 32 to 38.\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or in mixtures in concentrations equal to or greater than 0,1 % by weight, where the substance or mixture is intended for supply to the general public and/or is intended for diffusive applications such as in surface cleaning and cleaning of fabrics.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures containing them in concentrations equal to or greater than 0,1 % by weight is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations only’. However this requirement does not apply to: medication or veterinary medication according to the definition in the Directive 2001/82/EG and the directive 2001/83/EG ; cosmetics according to the definition in the directive 76/768/EWG of the Council."},"Without prejudice to the other parts of this Annex, the following shall apply to entries 32 to 38.\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or in mixtures in concentrations equal to or greater than 0,1 % by weight, where the substance or mixture is intended for supply to the general public and/or is intended for diffusive applications such as in surface cleaning and cleaning of fabrics.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures containing them in concentrations equal to or greater than 0,1 % by weight is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations only’. However this requirement does not apply to: medication or veterinary medication according to the definition in the Directive 2001/82/EG and the directive 2001/83/EG ; cosmetics according to the definition in the directive 76/768/EWG of the Council.","Unbeschadet der übrigen Teile dieses Anhangs gilt Folgendes für die Einträge 32 bis 38:\n1. Dürfen nicht in Verkehr gebracht oder verwendet werden:\n    als Stoffe,\n    als Bestandteile anderer Stoffe oder in Gemischen in Konzentrationen von 0,1 Gew: % oder mehr,\nwenn der Stoff oder das Gemisch für die Abgabe an die breite Öffentlichkeit und/oder die Anwendung in Formen bestimmt ist, bei denen eine Freisetzung nicht ausgeschlossen ist (beispielsweise Oberflächenreinigung und Reinigung von Textilien).\n2. Unbeschadet anderer Vorschriften der Gemeinschaft für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung solcher Stoffe und Gemische, in denen sie in Konzentrationen von > 0,1 Gew: % enthalten sind, gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n\"Nur zur Verwendung in Industrieanlagen\".\nDiese Anforderung gilt jedoch nicht für:\n    Arznei- oder Tierarzneimittel gemäß der Begriffsbestimmung in der Richtlinie 2001/82/EG und der Richtlinie 2001/83/EG ;\n    kosmetische Mittel gemäß der Begriffsbestimmung in der Richtlinie 76/768/EWG des Rates. ","在不违反本附件的其他部分的前提下，以下条款适用于条目32至38：\n1.以下情况下不可以销售或使用：\n1)作为纯物质,\n2)作为别的物质的组成部分，或者作为质量百分比大于等于0.1%的配制品的组成部分,如果此物质或此配制品将面向广大公众的供应，并且/或者将被广泛应用，如用于表面清洁剂和纺织物的清洗剂中\n\n2.不影响其它关于物质和配制品的分类、包装和标签等方面的公共规定，供应商应在投放市场之前确保，对于这些物质含量大于等于0.1%的物质和配制品，其包装上应该清晰易见且永久的标记有以下文字：\n“仅允许在工业设施的使用”。\n但是，这些要求不用于： \n根据指令2001/82/EG和2001/83/ EC定义的药品和兽药;\n根据指令76/768/EWG定义的化妆品\n"]
[null,{"$f":"IF($B$1=\"English\",C217,IF($B$1=\"Deutsch\",D217,IF($B$1=\"中文\",E217,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of spray paints or spray cleaners in aerosol dispensers in concentrations equal to or greater than 3 % by weight.\n2. Spray paints and spray cleaners in aerosol dispensers containing DEGBE and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that paints other than spray paints containing DEGBE in concentrations equal to or greater than 3 % by weight of that are placed on the market for supply to the general public are visibly, legibly and indelibly marked by 27 December 2010 as follows:\n‘Do not use in paint spraying equipment’."},"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of spray paints or spray cleaners in aerosol dispensers in concentrations equal to or greater than 3 % by weight.\n2. Spray paints and spray cleaners in aerosol dispensers containing DEGBE and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that paints other than spray paints containing DEGBE in concentrations equal to or greater than 3 % by weight of that are placed on the market for supply to the general public are visibly, legibly and indelibly marked by 27 December 2010 as follows:\n‘Do not use in paint spraying equipment’.","1. Darf nach dem 27. Juni 2010 nicht zur Abgabe an die breite Öffentlichkeit in Spritzfarben oder Reinigungssprays in Aerosolpackungen in einer Konzentration von >3 Gew: % erstmalig in Verkehr gebracht werden.\n2. Nach dem 27. Dezember 2010 dürfen DEGBE-haltige Spritzfarben und Reinigungssprays in Aerosolpackungen, die den Anforderungen unter Absatz 1 nicht entsprechen, nicht mehr zur Abgabe an die breite Öffentlichkeit in Verkehr gebracht werden.\n3. Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften über die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte DEGBE-haltige Farben, die nicht zum Verspritzen bestimmt sind, in einer Konzentration von 3 Gew. % oder mehr ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n\"Darf nicht in Farbspritzausrüstung verwendet werden\".","1.作为喷漆或喷雾清洁剂的组分在气溶胶喷罐中的浓度质量百分比大于3%时，不得在2010年6月27日以后首次投放市场销售给普通公众。\n2.喷漆或喷雾清洁剂如含DEGBE并且不符合本条第1款的规定，2010年12月27日后不得投放市场销售给普通公众。\n3.不影响其它关于物质和配制品的分类、包装和标签等方面的公共规定，供应商应在投放市场之前确保，销售给普通公众的涂料（除喷漆外）若含DEGBE质量百分比大于等于3%，从2010年12月27日起其包装上应该清晰易见且永久的标记有以下文字：“不得在涂料喷涂设备中使用”"]
[null,{"$f":"IF($B$1=\"English\",C218,IF($B$1=\"Deutsch\",D218,IF($B$1=\"中文\",E218,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market after 27 June 2010, for supply to the general public, as a constituent of paints, paint strippers, cleaning agents, self-shining emulsions or floor sealants in concentrations equal to or greater than 0,1 % by weight."},"Shall not be placed on the market after 27 June 2010, for supply to the general public, as a constituent of paints, paint strippers, cleaning agents, self-shining emulsions or floor sealants in concentrations equal to or greater than 0,1 % by weight.","Darf nach dem 27. Juni 2010 nicht zur Abgabe an die breite Öffentlichkeit in Farben, Abbeizmitteln, Reinigungsmitteln, selbstglänzenden Emulsionen oder Fußbodenversiegelungsmitteln in einer Konzentration von > 0,1 Gew: % in Verkehr gebracht werden.","作为油漆、油漆去除剂、清洁剂、自发光乳液或地板密封剂的组分，重量百分比大于等于0.1%的，  2010-06-27日起不得投放市场销售给公众。"]
[null,{"$f":"IF($B$1=\"English\",C219,IF($B$1=\"Deutsch\",D219,IF($B$1=\"中文\",E219,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures in concentrations greater than 0,1 % by weight."},"Shall not be placed on the market, or used, as substances or in mixtures in concentrations greater than 0,1 % by weight.","Dürfen weder als Stoffe noch in Gemischen in Konzentrationen von > 0,1 Gew: % in Verkehr gebracht oder verwendet werden.","禁止此物质或此物质的重量百分比大于0.1%的配制品投放市场和使用"]
[null,{"$f":"IF($B$1=\"English\",C220,IF($B$1=\"Deutsch\",D220,IF($B$1=\"中文\",E220,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for the treatment of wood. Furthermore, wood so treated shall not be placed on the market.\n2. By way of derogation from paragraph 1:\n(a) The substances and mixtures may be used for wood treatment in industrial installations or by professionals covered by Community legislation on the protection of workers for in situ retreatment only if they contain:\n(i) benzo[a]pyrene at a concentration of less than 50 mg/kg (0,005 % by weight), and\n(ii) water extractable phenols at a concentration of less than 3 % by weight. Such substances and mixtures for use in wood treatment in industrial installations or by professionals: — may be placed on the market only in packaging of a capacity equal to or greater than 20 litres, — shall not be sold to consumers. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is visibly, legibly and indelibly marked as follows: ‘For use in industrial installations or professional treatment only’.\n(b) Wood treated in industrial installations or by professionals according to subparagraph (a) which is placed on the market for the first time or retreated in situ may be used for professional and industrial use only, for example on railways, in electric power transmission and telecommunications, for fencing, for agricultural purposes (for example stakes for tree support) and in harbours and waterways.\n(c) The prohibition in paragraph 1 on the placing on the market shall not apply to wood which has been treated with substances listed in entry 31 (a) to (i) before 31 December 2002 and is placed on the second-hand market for re-use.\n3. Treated wood referred to under paragraph 2(b) and (c) shall not be used:\n— inside buildings, whatever their purpose,\n— in toys,\n— in playgrounds,\n— in parks, gardens, and outdoor recreational and leisure facilities where there is a risk of frequent skin contact,\n— in the manufacture of garden furniture such as picnic tables,\n— for the manufacture and use and any re-treatment of:\n— containers intended for growing purposes,\n— packaging that may come into contact with raw materials, intermediate or finished products destined for human and/or animal consumption,\n— other materials which may contaminate the articles mentioned above."},"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for the treatment of wood. Furthermore, wood so treated shall not be placed on the market.\n2. By way of derogation from paragraph 1:\n(a) The substances and mixtures may be used for wood treatment in industrial installations or by professionals covered by Community legislation on the protection of workers for in situ retreatment only if they contain:\n(i) benzo[a]pyrene at a concentration of less than 50 mg/kg (0,005 % by weight), and\n(ii) water extractable phenols at a concentration of less than 3 % by weight. Such substances and mixtures for use in wood treatment in industrial installations or by professionals: — may be placed on the market only in packaging of a capacity equal to or greater than 20 litres, — shall not be sold to consumers. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is visibly, legibly and indelibly marked as follows: ‘For use in industrial installations or professional treatment only’.\n(b) Wood treated in industrial installations or by professionals according to subparagraph (a) which is placed on the market for the first time or retreated in situ may be used for professional and industrial use only, for example on railways, in electric power transmission and telecommunications, for fencing, for agricultural purposes (for example stakes for tree support) and in harbours and waterways.\n(c) The prohibition in paragraph 1 on the placing on the market shall not apply to wood which has been treated with substances listed in entry 31 (a) to (i) before 31 December 2002 and is placed on the second-hand market for re-use.\n3. Treated wood referred to under paragraph 2(b) and (c) shall not be used:\n— inside buildings, whatever their purpose,\n— in toys,\n— in playgrounds,\n— in parks, gardens, and outdoor recreational and leisure facilities where there is a risk of frequent skin contact,\n— in the manufacture of garden furniture such as picnic tables,\n— for the manufacture and use and any re-treatment of:\n— containers intended for growing purposes,\n— packaging that may come into contact with raw materials, intermediate or finished products destined for human and/or animal consumption,\n— other materials which may contaminate the articles mentioned above.","1. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Holzbehandlung bestimmt sind. Ferner darf damit behandeltes Holz nicht in Verkehr gebracht werden.\n2. Abweichend von Absatz 1 bestehen jedoch folgende Ausnahmen:\n    Diese Stoffe und Gemische dürfen zur Holzbehandlung in industriellen Anlagen oder zu gewerblichen Zwecken, für die die gemeinschaftlichen Rechtsvorschriften über den Schutz der Arbeitnehmer bei der Wiederbehandlung vor Ort gelten, nur dann verwendet werden, wenn sie\n        Benzo[a]pyren in einer Konzentration von weniger als 50 mg/kg (0,005 Gew: %) und\n        wasserlösliche Phenole in einer Konzentration von weniger als 3 Gew:% enthalten.\n    Solche Stoffe und Gemische zur Verwendung bei der Holzbehandlung in industriellen Anlagen oder zu gewerblichen Zwecken dürfen nur in Verpackungen mit einem Fassungsvermögen von 20 Litern oder mehr in den Verkehr gebracht werden,\n        nicht an Verbraucher abgegeben werden. \n    Unbeschadet der übrigen gemeinschaftlichen Vorschriften auf dem Gebiet der Einstufung, Verpackung und Etikettierung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung solcher Stoffe und Gemische gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n    \"Verwendung nur in Industrieanlagen und zu gewerblichen Zwecken\".\n    Für nach Buchstabe a in industriellen Anlagen oder zu gewerblichen Zwecken behandeltes Holz, das zum ersten Mal in Verkehr gebracht wird oder vor Ort wieder behandelt wird, gilt: Die Verwendung ist ausschließlich für gewerbliche und industrielle Zwecke erlaubt (z.B. Eisenbahn, Stromtransport, Telekommunikation, Zäune, für landwirtschaftliche Zwecke - etwa Baumstützen -, Häfen, Wasserwege).\n    Das Verbot für das Inverkehrbringen nach Absatz 1 gilt nicht für Holz, das vor dem 31. Dezember 2002 mit unter Eintrag 31 Buchstaben a bis i aufgeführten Stoffen behandelt wurde und zur Wiederverwendung auf dem Gebrauchtmarkt angeboten wird. \n3. Die Verwendung von behandeltem Holz nach Absatz 2 Buchstaben b und c ist jedoch verboten:\n    innerhalb von Gebäuden, unabhängig von deren Zweckbestimmung;\n    bei Spielzeugen;\n    auf Spielplätzen;\n    in Parks, Gärten und anderen Orten im Freien, die der Freizeitgestaltung und der Erholung dienen und bei denen die Gefahr eines häufigen Hautkontakts besteht;\n    für die Anfertigung von Gartenmobiliar wie etwa Picknicktischen;\n    für die Anfertigung, Verwendung und Wiederaufarbeitung von:\n    Behältern für lebende Pflanzen,\n    Verpackungen, die mit Rohmaterialien, Zwischen- und/oder Enderzeugnissen für die menschliche und/oder tierische Ernährung in Berührung kommen,\n    anderem Material, das die oben genannten Erzeugnisse kontaminieren kann. ","1.不得投放到市场或使用作为木材处理剂或添加在木材处理剂中。此外，经处理过的木材也不得投放市场。\n2. 然而，第1款的例外如下：\n(a)这种物质和制剂，可用于工业装置中的木材处理，依据欧共体法规对劳工保护规定，如果含有下列情形者，仅能于现场再处理：\ni）含苯并[a]芘的浓度小于50毫克/公斤（质量百分比0.005%），而且\nii）可被水萃取的酚的质量浓度低于3%。\n此类物质及制剂用于工业设施或由专业作业人员使用于木材处理时，只有当包装容量大于等于20升时才可以投放市场，而且不得出售给消费者。\n在不违反其它关于物质和配制品的分类、包装和标签等方面规定的前提下，供应商应在投放市场之前确保，对于这些物质含量大于等于0.1%的材料和配制品，其包装上应该清晰易见且永久的标记有以下文字：\n“仅供工业设施或专业用途使用”\n(b)根据前述(a)点，在工业设备中或由专业人员处理的木材，首次投放市场或者现场再处理，仅允许用于专业和工业用途，例如用在铁路，电力传输和通信中，用作围栏，用于农业用途，比如树木保护桩，用在港口和航运。\n(c)第1款禁用不适用于已经在2002年12月31日前用条款31(a)至(i)中的物质处理过的木材，投放到二手市场进行再利用。\n3. 小节2(b)和(c)提及的处理过的木材禁止用于：\n- 建筑物内部，无论什么用途的建筑物\n- 玩具；\n- 操场；\n-公园，花园和及其它与皮肤有频繁接触的风险的户外休闲娱乐设施;\n-庭院类家具，如野餐桌；\n-包括以下内容在内的任何用于制造，使用和再处理的物品：\n    -种植用容器；\n    -可能与原料，中间产品，或预定为人或动物消费的产品接触的包装；\n    -其它可能污染上述物品的材料\n"]
[null,{"$f":"IF($B$1=\"English\",C221,IF($B$1=\"Deutsch\",D221,IF($B$1=\"中文\",E221,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used, in jokes and hoaxes or in mixtures or articles intended to be used as such, for instance as a constituent of sneezing powder and stink bombs.\n2. Jokes and hoaxes, or mixtures or articles intended to be used as such, not complying with paragraph 1 shall not be placed on the market.\n3. However, paragraphs 1 and 2 shall not apply to stink bombs containing not more than 1,5 ml of liquid."},"1. Shall not be used, in jokes and hoaxes or in mixtures or articles intended to be used as such, for instance as a constituent of sneezing powder and stink bombs.\n2. Jokes and hoaxes, or mixtures or articles intended to be used as such, not complying with paragraph 1 shall not be placed on the market.\n3. However, paragraphs 1 and 2 shall not apply to stink bombs containing not more than 1,5 ml of liquid.","1. Darf nicht verwendet werden in Scherzartikeln oder Gemischen oder Erzeugnissen, die dazu bestimmt sind, als solche verwendet zu werden, beispielsweise als Bestandteil von Niespulver und Stinkbomben.\n2. Scherzartikel oder Gemische oder Erzeugnisse, die dazu bestimmt sind, als solche verwendet zu werden, dürfen nicht in Verkehr gebracht werden, wenn sie Absatz 1 nicht erfüllen.\n3. Die Absätze 1 und 2 gelten jedoch nicht für Stinkbomben, deren Inhalt 1,5 ml Flüssigkeit nicht überschreitet.","1.不可用于戏法和恶作剧或者用在用于此类用途的物品中，例如使人打喷嚏的粉末和臭气弹中；\n2.不符合第1条的戏法和恶作剧用品，不得投放市场\n3. 但是，第1、2条不适用于含不超过1.5ml液体的臭气弹。"]
[null,{"$f":"IF($B$1=\"English\",C222,IF($B$1=\"Deutsch\",D222,IF($B$1=\"中文\",E222,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used as substances, or as constituents of other substances or in mixtures in concentrations greater than 1 % by weight, where the substance or mixture is intended for:\n— metalworking,\n— fat liquoring of leather."},"Shall not be placed on the market, or used as substances, or as constituents of other substances or in mixtures in concentrations greater than 1 % by weight, where the substance or mixture is intended for:\n— metalworking,\n— fat liquoring of leather.","Dürfen nicht als Stoffe oder Bestandteile von anderen Stoffen oder in Gemischen in Konzentrationen von über 1 Gew: % in Verkehr gebracht oder verwendet werden, wenn der Stoff oder das Gemisch bestimmt ist:\n    für die Metallver- und Metallbearbeitung,\n    zum Fetten von Leder. ","禁止此物质、或作为其它物质的组成部分，或此物质的重量百分比大于1%的配制品投放市场和使用，物质或配制品用于：\n -- 金属加工，\n -- 皮革油质浸泡液"]
[null,{"$f":"IF($B$1=\"English\",C223,IF($B$1=\"Deutsch\",D223,IF($B$1=\"中文\",E223,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market for the first time after 27 June 2010 as a substance, or in mixtures that contain more than 28 % by weight of nitrogen in relation to ammonium nitrate, for use as a solid fertiliser, straight or compound, unless the fertiliser complies with the technical provisions for ammonium nitrate fertilisers of high nitrogen content set out in Annex III to Regulation (EC) No 2003/2003 of the European Parliament and of the Council (***********).\n2. Shall not be placed on the market after 27 June 2010 as a substance, or in mixtures that contain 16 % or more by weight of nitrogen in relation to ammonium nitrate except for supply to:\n(a) downstream users and distributors, including natural or legal persons licensed or authorised in accordance with Council Directive 93/15/EEC (************);\n(b) farmers for use in agricultural activities, either full time or part time and not necessarily related to the size of the land area. For the purposes of this subparagraph:\n(i) ‘farmer’ shall mean a natural or legal person, or a group of natural or legal persons, whatever legal status is granted to the group and its members by national law, whose holding is situated within Community territory, as referred to in Article 299 of the Treaty, and who exercises an agricultural activity;\n(ii) ‘agricultural activity’ shall mean the production, rearing or growing of agricultural products including harvesting, milking, breeding animals and keeping animals for farming purposes, or maintaining the land in good agricultural and environmental condition as established under Article 5 of Council Regulation (EC) No 1782/2003 (*************); (c) natural or legal persons engaged in professional activities such as horticulture, plant growing in greenhouses, maintenance of parks, gardens or sport pitches, forestry or other similar activities. \n3. However, for the restrictions in paragraph 2, Member States may until 1 July 2014, for socioeconomic reasons, apply a limit of up to 20 % by weight of nitrogen in relation to ammonium nitrate for substances and mixtures placed on the market within their territories. They shall inform the Commission and other Member States thereof.\n______________ \n(***********) OJ L 304, 21.11.2003, p. 1. \n(************) OJ L 121, 15.5.1993, p. 20. \n(*************) OJ L 270, 21.10.2003, p. 1."},"1. Shall not be placed on the market for the first time after 27 June 2010 as a substance, or in mixtures that contain more than 28 % by weight of nitrogen in relation to ammonium nitrate, for use as a solid fertiliser, straight or compound, unless the fertiliser complies with the technical provisions for ammonium nitrate fertilisers of high nitrogen content set out in Annex III to Regulation (EC) No 2003/2003 of the European Parliament and of the Council (***********).\n2. Shall not be placed on the market after 27 June 2010 as a substance, or in mixtures that contain 16 % or more by weight of nitrogen in relation to ammonium nitrate except for supply to:\n(a) downstream users and distributors, including natural or legal persons licensed or authorised in accordance with Council Directive 93/15/EEC (************);\n(b) farmers for use in agricultural activities, either full time or part time and not necessarily related to the size of the land area. For the purposes of this subparagraph:\n(i) ‘farmer’ shall mean a natural or legal person, or a group of natural or legal persons, whatever legal status is granted to the group and its members by national law, whose holding is situated within Community territory, as referred to in Article 299 of the Treaty, and who exercises an agricultural activity;\n(ii) ‘agricultural activity’ shall mean the production, rearing or growing of agricultural products including harvesting, milking, breeding animals and keeping animals for farming purposes, or maintaining the land in good agricultural and environmental condition as established under Article 5 of Council Regulation (EC) No 1782/2003 (*************); (c) natural or legal persons engaged in professional activities such as horticulture, plant growing in greenhouses, maintenance of parks, gardens or sport pitches, forestry or other similar activities. \n3. However, for the restrictions in paragraph 2, Member States may until 1 July 2014, for socioeconomic reasons, apply a limit of up to 20 % by weight of nitrogen in relation to ammonium nitrate for substances and mixtures placed on the market within their territories. They shall inform the Commission and other Member States thereof.\n______________ \n(***********) OJ L 304, 21.11.2003, p. 1. \n(************) OJ L 121, 15.5.1993, p. 20. \n(*************) OJ L 270, 21.10.2003, p. 1.","1. Darf nach dem 27. Juni 2010 nicht mehr als Stoff oder in Gemischen mit einem Stickstoffgehalt im Verhältnis zum Ammoniumnitrat über 28 Gew: % zur Verwendung als fester Ein- oder Mehrnährstoffdünger erstmalig in Verkehr gebracht werden, wenn der Dünger nicht den in Anhang III der Verordnung (EG) Nr. 2003/2003 des Europäischen Parlaments und des Rates (***************) festgelegten technischen Anforderungen an Ammoniumnitratdünger mit hohem Stickstoffgehalt entspricht.\n2. Darf nach dem 27. Juni 2010 nicht mehr als Stoff oder in Gemischen in Verkehr gebracht werden, deren Stickstoffgehalt im Verhältnis zum Ammoniumnitrat 16 Gew. % oder mehr beträgt, mit Ausnahme der Abgabe an folgende Abnehmer:\n    nachgeschaltete Anwender und Händler, einschließlich natürliche oder juristische Personen, die gemäß der Richtlinie 93/15/EWG des Rates (***********) über eine entsprechende Zulassung oder Genehmigung verfügen;\n    Landwirte, zur Verwendung im Rahmen ihrer als Vollzeit- oder als Teilzeitbeschäftigung ausgeübten landwirtschaftlichen Tätigkeiten und unabhängig von der Größe der Nutzfläche, für die Zwecke des vorliegenden Buchstaben bezeichnet der Ausdruck:\n        \"Landwirt\" eine natürliche oder juristische Person oder eine Vereinigung natürlicher oder juristischer Personen, unabhängig davon, welchen rechtlichen Status die Vereinigung und ihre Mitglieder aufgrund nationalen Rechts haben, deren Betrieb sich im Gebiet der Gemeinschaft im Sinne des Artikels 299 des Vertrags befindet und die eine landwirtschaftliche Tätigkeit ausübt;\n        \"landwirtschaftliche Tätigkeit\" die Erzeugung, die Zucht oder den Anbau landwirtschaftlicher Erzeugnisse, einschließlich Ernten, Melken, Zucht von Tieren und Haltung von Tieren für landwirtschaftliche Zwecke, oder die Erhaltung von Flächen in gutem landwirtschaftlichen und ökologischen Zustand gemäß Artikel 5 der Verordnung (EG) Nr. 1782/2003 des Rates (*************); \n    natürliche oder juristische Personen, die gewerblich einer Tätigkeit wie Gartenbau, Pflanzenanbau in Gewächshäusern, Park-, Garten- oder Sportflächenpflege, Forstwirtschaft oder anderen vergleichbaren Tätigkeiten nachgehen.\n3. Die Mitgliedstaaten können jedoch in Hinblick auf die Einschränkungen in Absatz 2 aus sozioökonomischen Gründen bis zum 1. Juli 2014 einen Grenzwert von bis zu 20 Gew. % für den zulässigen Stickstoffgehalt im Verhältnis zum Ammoniumnitrat von in ihrem Hoheitsgebiet in Verkehr gebrachten Stoffen oder Gemischen anwenden. Hiervon unterrichten sie die Kommission und die übrigen Mitgliedstaaten.\n______________ \n(***********) OJ L 304, 21.11.2003, S. 1. \n(************) OJ L 121, 15.5.1993, S. 20. \n(*************) OJ L 270, 21.10.2003, S. 1.","1.禁止此物质，或者含有此物质的制剂（涉及到硝酸铵的含氮量超过28%）在2010年6月27日后首次投放市场销售，用作固体化肥（无论是单一肥料或者复合肥料），除非该化肥符合欧洲议会与欧洲理事会（EC）2003/2003法规附件三中的高含氮量的硝酸铵化肥规定的技术要求。\n2.禁止此物质，或者含有此物质的制剂（涉及到硝酸铵的含氮量大于等于16%）在2010年6月27日后首次投放市场销售，除非销售给：\n（a）下游用户和分销商，包括自然人和根据欧盟理事会93/15/ EEC指令许可和授权的法人;\n（b）农民，无论是全职或兼职从事农业活动，也不管其土地的使用面积大小。以下是针对（b）小节的一些注释： \n（i）\"农民\"，是指自然人或者法人亦或是自然人及/或法人的联合体，无论此联合体及其成员基于国家法律的规定有怎样的法律地位，其企业位于《条约》之299条所指团体的领域并且其从事农业生产活动\n（ii）“农业活动”，是指生产，养殖或者种植农产品，包括针对农业目的的收割，挤奶，为农业目的养殖动物，或者根据规定（EC）1782/2003第五条之规定，对土地的良好农业状况及环境状况进行维护.\n（c）自然人或法人是指商业化地从事诸如园艺，在温室中的植物种植，针对公园，花园或运动场的地面护理，林业，或着其他类似活动的人.\n\n3。但是，成员国可以就关于第2款的限制来自社会的原因，直到2014年7月1日在其领土上的物质或配制品的使用 ，其含氮于硝酸铵的比例的限制值高达20的重量百分比。他们应通知委员会和其他成员国。\n"]
[null,{"$f":"IF($B$1=\"English\",C224,IF($B$1=\"Deutsch\",D224,IF($B$1=\"中文\",E224,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use to prevent the fouling by micro-organisms, plants or animals of:\n— the hulls of boats,\n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming,\n— any totally or partly submerged appliances or equipment.\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters, irrespective of their use.\n3. Shall not be used in the preservation of wood. Furthermore, wood so treated shall not be placed on the market.4. By way of derogation from paragraph 3:\n(a) Relating to the substances and mixtures for the preservation of wood: these may only be used in industrial installations using vacuum or pressure to impregnate wood if they are solutions of inorganic compounds of the copper, chromium, arsenic (CCA) type C and if they are authorised in accordance with Article 5(1) of Directive 98/8/EC. Wood so treated shall not be placed on the market before fixation of the preservative is completed.\n(b) Wood treated with CCA solution in accordance with point (a) may be placed on the market for professional and industrial use provided that the structural integrity of the wood is required for human or livestock safety and skin contact by the general public during its service life is unlikely:\n— as structural timber in public and agricultural buildings, office buildings, and industrial premises,\n— in bridges and bridgework,\n— as constructional timber in freshwater areas and brackish waters, for example jetties and bridges,\n— as noise barriers,\n— in avalanche control,\n— in highway safety fencing and barriers,\n— as debarked round conifer livestock fence posts,\n— in earth retaining structures,\n— as electric power transmission and telecommunications poles,\n— as underground railway sleepers.\n(c) Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that all treated wood placed on the market is individually labelled ‘For professional and industrial installation and use only, contains arsenic’. In addition, all wood placed on the market in packs shall also bear a label stating ‘Wear gloves when handling this wood. Wear a dust mask and eye protection when cutting or otherwise crafting this wood. Waste from this wood shall be treated as hazardous by an authorised undertaking’.\n(d) Treated wood referred to under point (a) shall not be used:\n— in residential or domestic constructions, whatever the purpose,\n— in any application where there is a risk of repeated skin contact,\n— in marine waters,\n— for agricultural purposes other than for livestock fence posts and structural uses in accordance with point (b),\n— in any application where the treated wood may come into contact with intermediate or finished products intended for human and/or animal consumption.\n5. Wood treated with arsenic compounds that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4 may remain in place and continue to be used until it reaches the end of its service life.\n\n6. Wood treated with CCA type C that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4:\n— may be used or reused subject to the conditions pertaining to its use listed under points 4(b), (c) and (d),\n— may be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).\n\n7. Member States may allow wood treated with other types of CCA solutions that was in use in the Community before 30 September 2007:\n— to be used or reused subject to the conditions pertaining to its use listed under points 4 (b), (c) and (d),\n— to be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d)."},"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use to prevent the fouling by micro-organisms, plants or animals of:\n— the hulls of boats,\n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming,\n— any totally or partly submerged appliances or equipment.\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters, irrespective of their use.\n3. Shall not be used in the preservation of wood. Furthermore, wood so treated shall not be placed on the market.4. By way of derogation from paragraph 3:\n(a) Relating to the substances and mixtures for the preservation of wood: these may only be used in industrial installations using vacuum or pressure to impregnate wood if they are solutions of inorganic compounds of the copper, chromium, arsenic (CCA) type C and if they are authorised in accordance with Article 5(1) of Directive 98/8/EC. Wood so treated shall not be placed on the market before fixation of the preservative is completed.\n(b) Wood treated with CCA solution in accordance with point (a) may be placed on the market for professional and industrial use provided that the structural integrity of the wood is required for human or livestock safety and skin contact by the general public during its service life is unlikely:\n— as structural timber in public and agricultural buildings, office buildings, and industrial premises,\n— in bridges and bridgework,\n— as constructional timber in freshwater areas and brackish waters, for example jetties and bridges,\n— as noise barriers,\n— in avalanche control,\n— in highway safety fencing and barriers,\n— as debarked round conifer livestock fence posts,\n— in earth retaining structures,\n— as electric power transmission and telecommunications poles,\n— as underground railway sleepers.\n(c) Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that all treated wood placed on the market is individually labelled ‘For professional and industrial installation and use only, contains arsenic’. In addition, all wood placed on the market in packs shall also bear a label stating ‘Wear gloves when handling this wood. Wear a dust mask and eye protection when cutting or otherwise crafting this wood. Waste from this wood shall be treated as hazardous by an authorised undertaking’.\n(d) Treated wood referred to under point (a) shall not be used:\n— in residential or domestic constructions, whatever the purpose,\n— in any application where there is a risk of repeated skin contact,\n— in marine waters,\n— for agricultural purposes other than for livestock fence posts and structural uses in accordance with point (b),\n— in any application where the treated wood may come into contact with intermediate or finished products intended for human and/or animal consumption.\n5. Wood treated with arsenic compounds that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4 may remain in place and continue to be used until it reaches the end of its service life.\n\n6. Wood treated with CCA type C that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4:\n— may be used or reused subject to the conditions pertaining to its use listed under points 4(b), (c) and (d),\n— may be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).\n\n7. Member States may allow wood treated with other types of CCA solutions that was in use in the Community before 30 September 2007:\n— to be used or reused subject to the conditions pertaining to its use listed under points 4 (b), (c) and (d),\n— to be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).","1. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die bestimmt sind zur Verhinderung des Bewuchses durch Mikroorganismen, Pflanzen oder Tiere an:\n    Bootskörpern;\n    Kästen, Schwimmern, Netzen sowie anderen Geräten oder Einrichtungen für die Fisch- und Muschelzucht;\n    völlig oder teilweise untergetauchten Geräten oder Einrichtungen jeder Art. \n2. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Aufbereitung von Wasser im industriellen, gewerblichen und kommunalen Bereich bestimmt sind, unabhängig von seiner Verwendung.\n3. Dürfen nicht als Holzschutzmittel verwendet werden. Ferner darf damitbehandeltes Holz nicht in Verkehr gebracht werden.\n4. Abweichend von Absatz 3 bestehen jedoch folgende Ausnahmen:\n    Für Stoffe und Gemische für den Holzschutz: Diese dürfen lediglich in Industrieanlagen im Vakuum oder unter Druck zur Imprägnierung von Holz in Form von Lösungen anorganischer Verbindungen von Kupfer-Chrom-Arsen (CCA), Typ C, zum Einsatz kommen, sofern sie nach Artikel 5 Absatz 1 der Richtlinie 98/8/EG zugelassen sind. Holz, das so behandelt ist, darf nicht in Verkehr gebracht werden, bevor das Schutzmittel vollständig fixiert ist.\n    Mit CCA-Lösungen behandeltes Holz gemäß Buchstabe a darf für die gewerbliche und industrielle Verwendung in Verkehr gebracht werden, sofern die Unversehrtheit der Holzstruktur zur Sicherheit von Mensch oder Vieh erforderlich ist und ein Hautkontakt der allgemeinen Bevölkerung während der Einsatzdauer unwahrscheinlich ist:\n        als Bauholz in öffentlichen und landwirtschaftlichen Gebäuden, Bürogebäuden und Industriebetrieben,\n        in Brücken und bei Brückenbauarbeiten,\n        als Bauholz in Binnengewässern und Brackwasser, z.B. für Molen und Brücken,\n        als Lärmschutz,\n        als Lawinenschutz,\n        als Leitplanken und Schranken an Straßen,\n        als entrindete Rundnadelhölzer für Weidezäune,\n        in Erdstützwänden,\n        als Strom- und Telekommunikationsmasten,\n        als Bahnschwellen für Untergrundbahnen. \n    Unbeschadet anderer Gemeinschaftsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen müssen die Lieferanten vor dem Inverkehrbringen gewährleisten, dass sämtliches behandeltes Holz einzeln mit der Aufschrift versehen ist: Verwendung nur in Industrieanlagen und zu gewerblichen Zwecken, enthält Arsen.' Darüber hinaus muss sämtliches in Paketen in Verkehr gebrachtes Holz mit der Aufschrift versehen ist: Bei der Handhabung des Holzes Handschuhe tragen. Wird dieses Holz geschnitten oder anderweitig bearbeitet, Staubmaske und Augenschutz tragen. Abfälle dieses Holzes sind von zugelassenen Unternehmen als gefährliche Abfälle zu behandeln.'\n    Die Verwendung von behandeltem Holz nach Buchstabea ist jedoch verboten:\n        in Wohnbauten, unabhängig von ihrer Zweckbestimmung,\n        in Anwendungen mit dem Risiko eines wiederholten Hautkontakts,\n        in Meeresgewässern,\n        für landwirtschaftliche Zwecke außer Weidezäunen und Bauholz gemäß Buchstabe b,\n        in Anwendungen, bei denen das behandelte Holz mit Zwischenoder Enderzeugnissen in Kontakt kommen kann, die für den menschlichen und/oder tierischen Verzehr bestimmt sind.\n5. Mit Arsenverbindungen behandeltes Holz, das vor dem 30. September 2007 in der Gemeinschaft genutzt oder gemäß Absatz 4 in Verkehr gebracht wurde, kann bis zum Ende seiner Nutzungsdauer eingebaut bleiben und weiterverwendet werden.\n6. Mit CCA-Lösungen, Typ C, behandeltes Holz, das vor dem 30. September 2007 in der Gemeinschaft genutzt oder gemäß Absatz 4 in Verkehr gebracht wurde:\n    kann unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen genutzt oder wiederverwendet werden,\n    kann unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen in Verkehr gebracht werden. \n7. Die Mitgliedstaaten können zulassen, dass mit anderen Typen von CCA-Lösungen behandeltes Holz, das vor dem 30. September 2007 in der Gemeinschaft genutzt wurde:\n    unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen genutzt oder wiederverwendet wird,\n    unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen in Verkehr gebracht wird.","1.不可以作为物质或在配制品里被销售或使用，这是为了防止由微生物，植物或动物引起的污染：\n-船的船体；\n-笼子，浮标，用于鱼或贝类养殖网和其它任何电器或设备;\n-完全或部分淹没的此类型的器具或设备。\n2.不可以作为物质或制剂的成分于以下用途:：被销售或使用，这是用于处理水用于工业，商业和市政部门，与他的使用无关。\n3不可仪作为树木保护剂使用。如果已被处理过的木材，不可以在市场上销售。\n4对于第3条存在以下例外：\n(a)对于针对木材防腐的物质和配制品：这些只允许在真空的工业装置中或者在对木材浸泡的压力下被使用（此浸泡是指通过由铜铬砷（CCA），C型组成的无机化合物的溶液完成的），只要这些根据指导方针98/8/EG的第5条第1款是被允许的。通过这种方式处理的木头在防护剂完全固定以前不允许被投放于市场。\n(b)含有CCA溶液进行处理过的木材根据(a)可允许被销售用于企业和工业，前提是木结构用于人或牲畜安全性是必需的，以及与一般人的皮肤接触在时间周期是不大可能的：\n-作为在公共和农业建筑，写字楼和工业厂房的结构木材，\n-桥梁及桥梁工程，\n-作为在淡水区和咸水水域的结构用材，如码头，桥梁，\n-作为隔音屏障，\n-作为雪崩防护， \n-作为高速公路的防护栏和障碍， \n-用去了皮的树杆作为牲畜的围栏， \n- 作为土挡墙， \n-作为电力和通讯桅杆， \n-作为铁路枕木用于地铁。\n(c)在不影响共同规定对于物质和配制品的分类，包装和标签等，供应商应在投放市场之前应该确保，所有处理过的木材都单独配有标字：只使用于工业设施和商业目的，含有砷。此外，所有要销售的木材的包装上必须配有标字：处理这种木材时请戴上手套。这种木材切割或以其他方式处理，请戴上防尘面具和护目镜。这个木材的废料应以相符的公司作为危险废物处理。\n\n使用处理过的木材根据字母a不被使用：\n-在住宅楼宇，与其目的无关，\n-在使用中有反复与皮肤接触危险，\n-在海洋水域，\n-根据b，用于除了牲畜栅栏外的农业目的和结构用途，\n-在应用中，处理过的木材可能会接触中间或最终产品，这些产品用于人类和/或动物的消耗。\n5. 含被砷化合物处理过的木材，其在2007年9月30号之前在公共情况下被使用或者根据段落4在市场上销售，可以保留和继续使用直到其使用寿命结束时。    \n6.被CCA溶液，TypC处理过的木材，其在2007年9月30号之前在公共情况下被使用或者根据段落4在市场上销售：\n-也可根据第4段中字母b，c和d的规定中提到的使用条件，可以使用或重复使用\n-也可根据第4段中字母b，c和d的规定中提到的使用条件，在市场上销售\n7. 成员国可以允许，用其他类型的CCA溶液处理的木材在2007年9月30日前在公共社区可以被使用:\n-也可根据第4段中字母b，c和d的规定中提到的使用条件，可以使用或重复使用\n也可根据第4段中字母b，c和d规定中提到的使用条件，在市场上销售"]
[null,{"$f":"IF($B$1=\"English\",C225,IF($B$1=\"Deutsch\",D225,IF($B$1=\"中文\",E225,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. The manufacture, placing on the market and use of these fibres and of articles and mixtures containing these fibres added intentionally is prohibited. \nHowever, Member States may exempt the placing on the market and use of diaphragms containing chrysotile (point (f)) for existing electrolysis installations until they reach the end of their service life, or until suitable asbestos-free substitutes become available, whichever is the sooner.\nBy 1 June 2011 Member States making use of this exemption shall provide a report to the Commission on the availability of asbestos free substitutes for electrolysis installations and the efforts undertaken to develop such alternatives, on the protection of the health of workers in the installations, on the source and quantities of chrysotile, on the source and quantities of diaphragms containing chrysotile, and the envisaged date of the end of the exemption. The Commission shall make this information publicly available.\nFollowing receipt of those reports, the Commission shall request the Agency to prepare a dossier in accordance with Article 69 with a view to prohibit the placing on the market and use of diaphragms containing chrysotile.\n2. The use of articles containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005 shall continue to be permitted until they are disposed of or reach the end of their service life. However, Member States may, for reasons of protection of human health, restrict, prohibit or make subject to specific conditions, the use of such articles before they are disposed of or reach the end of their service life.\nMember States may allow placing on the market of articles in their entirety containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005, under specific conditions ensuring a high level of protection of human health. Member States shall communicate these national measures to the Commission by 1 June 2011. The Commission shall make this information publicly available.\n3. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, the placing on the market and use of articles containing these fibres, as permitted according to the preceding derogations, shall be permitted only if suppliers ensure before the placing on the market that articles bear a label in accordance with Appendix 7 to this Annex."},"1. The manufacture, placing on the market and use of these fibres and of articles and mixtures containing these fibres added intentionally is prohibited. \nHowever, Member States may exempt the placing on the market and use of diaphragms containing chrysotile (point (f)) for existing electrolysis installations until they reach the end of their service life, or until suitable asbestos-free substitutes become available, whichever is the sooner.\nBy 1 June 2011 Member States making use of this exemption shall provide a report to the Commission on the availability of asbestos free substitutes for electrolysis installations and the efforts undertaken to develop such alternatives, on the protection of the health of workers in the installations, on the source and quantities of chrysotile, on the source and quantities of diaphragms containing chrysotile, and the envisaged date of the end of the exemption. The Commission shall make this information publicly available.\nFollowing receipt of those reports, the Commission shall request the Agency to prepare a dossier in accordance with Article 69 with a view to prohibit the placing on the market and use of diaphragms containing chrysotile.\n2. The use of articles containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005 shall continue to be permitted until they are disposed of or reach the end of their service life. However, Member States may, for reasons of protection of human health, restrict, prohibit or make subject to specific conditions, the use of such articles before they are disposed of or reach the end of their service life.\nMember States may allow placing on the market of articles in their entirety containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005, under specific conditions ensuring a high level of protection of human health. Member States shall communicate these national measures to the Commission by 1 June 2011. The Commission shall make this information publicly available.\n3. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, the placing on the market and use of articles containing these fibres, as permitted according to the preceding derogations, shall be permitted only if suppliers ensure before the placing on the market that articles bear a label in accordance with Appendix 7 to this Annex.","1. 1. Die Herstellung, das Inverkehrbringen und die Verwendung dieser Fasern sowie von Erzeugnissen und Gemischen, denen diese Fasern absichtlich zugesetzt werden, ist verboten.Die Mitgliedstaaten dürfen jedoch Diaphragmen, die Chrysotil enthalten (Buchstabe 4 für bestehende Elektrolyseanlagen von dieser Regelung ausnehmen, bis deren Nutzungsdauer abgelaufen ist, oder bis geeignete asbestfreie Substitute verfügbar werden, je nachdem, welcher dieser beiden Fälle zuerst eintritt.\nMitgliedstaaten, die von dieser Ausnahmeregelung Gebrauch machen, müssen der Kommission bis zum 1. Juni 2011 über die Verfügbarkeit asbestfreier Substitute für Elektrolyseanlagen, über die getroffenen Maßnahmen zur Entwicklung solcher Alternativen, über den Gesundheitsschutz für die Arbeitskräfte in diesen Anlagen, über die Mengen an Chrysotil und dessen Quelle, über die Quelle und die Mengen der Chrysotil enthaltenden Diaphragmen und über das Datum, an dem die Ausnahmeregelung auslaufen soll, Bericht erstatten. Die Angaben werden von der Kommission veröffentlicht.\nNach Eingang der Berichte lässt die Kommission durch die Agentur ein Dossier gemäß Artikel 69 zum Zweck des Verbots des Inverkehrbringens und der Verwendung Chrysotil enthaltender Diaphragmen erstellen.\n2. Die Verwendung von Erzeugnissen, die Asbestfasern gemäß Absatz 1 enthalten und die schon vor dem 1. Januar 2005 installiert bzw. in Betrieb waren, ist weiterhin erlaubt, bis diese Erzeugnisse beseitigt werden oder bis ihre Nutzungsdauer abgelaufen ist. Jedoch können die Mitgliedstaaten zum Schutz der menschlichen Gesundheit die Verwendung solcher Erzeugnisse, bis sie beseitigt werden oder ihre Nutzungsdauer abgelaufen ist, einschränken, verbieten oder bestimmten Bedingungen unterwerfen.\nDie Mitgliedstaaten können das Inverkehrbringen kompletter Erzeugnisse, die Asbestfasern gemäß Absatz 1 enthalten und die schon vor dem 1. Januar 2005 installiert bzw. in Betrieb waren, unter bestimmten, ein hohes Maß an Schutz der menschlichen Gesundheit gewährleistenden Bedingungen gestatten. Die Mitgliedstaaten müssen die Kommission bis zum 1. Juni 2011 von solchen einzelstaatlichen Maßnahmen unterrichten. Die Angaben werden von der Kommission veröffentlicht.\n3. Unbeschadet der Anwendung anderer Gemeinschaftsvorschriften über die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen ist das gemäß den vorstehenden Ausnahmeregelungen erfolgende Inverkehrbringen und die gemäß den vorstehenden Ausnahmeregelungen erfolgende Verwendung von Erzeugnissen, die diese Fasern enthalten, nur zulässig, wenn der Lieferant vor dem Inverkehrbringen gewährleistet, dass die Erzeugnisse ein Etikett gemäß Anlage 7 dieses Anhangs tragen.","1.禁止生产，销售和使用这些石棉纤维以及含有有意添加此类纤维产品和配制品。但是，成员国可以销售和使用含有温石棉（第f点）的隔膜在已有的的电解装置控制中，直到其使用寿命到期，或直到有合适的不含石棉的替代品出现，这取决于这两种情况哪中先发生。\n成员国如果要应用这一豁免，须在2011年6月1日之前向欧盟管理委员会提交一份报告，分析在电解装置中使用不含石棉的替代品的可行性，为开发替代品所做出的努力，为保护操作该装置的工人的健康采取的措施，温石棉的数量和其来源，含有温石棉的隔膜的数量和其来源，以及预计结束应用这一豁免的日期。该委员会将公开这份报告。\n在收到报告后，委员会将要求管理署根据第69条准备一份卷宗，以禁止销售和使用含温石棉的膜片。\n2.含第1条所指的含有石棉纤维产品，如果在2005年1月1日前已安装并投入运营，允许继续使用，直到这些产品被处置或使用寿命结束。但是，为了保护人类健康，成员国可以在这些产品被处置或使用寿命结束之前，就限制、禁止或一定的条件下限制这类产品。\n在人体健康能够得到充分保障的特殊情况下，成员国可以销售在2005年1月1日前已安装并/或投入运营的含有第1款所指石棉纤维的产品。2011年6月1日之前，各成员国必须通知该委员会本国的措施。委员会将公布此信息。\n3.在不违反委员会的其它关于物质和配制品分类、包装和标签法规的前提下，只有当供应商在投放市场之前确保该产品张贴了本附件的附录7要求的标签，含石棉纤维的产品才能投放市场和使用。\n"]
[null,{"$f":"IF($B$1=\"English\",C226,IF($B$1=\"Deutsch\",D226,IF($B$1=\"中文\",E226,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Azodyes which, by reductive cleavage of one or more azo groups, may release one or more of the aromatic amines listed in Appendix 8, in detectable concentrations, i.e. above 30 mg/kg (0,003 % by weight) in the articles or in the dyed parts thereof, according to the testing methods listed in Appendix 10, shall not be used, in textile and leather articles which may come into direct and prolonged contact with the human skin or oral cavity, such as:\n— clothing, bedding, towels, hairpieces, wigs, hats, nappies and other sanitary items, sleeping bags,\n— footwear, gloves, wristwatch straps, handbags, purses/wallets, briefcases, chair covers, purses worn round the neck,\n— textile or leather toys and toys which include textile or leather garments,\n— yarn and fabrics intended for use by the final consumer.\n2. Furthermore, the textile and leather articles referred to in paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. Azodyes, which are contained in Appendix 9, ‘List of azodyes’ shall not be placed on the market, or used, as substances, or in mixtures in concentrations greater than 0,1 % by weight, where the substance or the mixture is intended for colouring textile and leather articles."},"1. Azodyes which, by reductive cleavage of one or more azo groups, may release one or more of the aromatic amines listed in Appendix 8, in detectable concentrations, i.e. above 30 mg/kg (0,003 % by weight) in the articles or in the dyed parts thereof, according to the testing methods listed in Appendix 10, shall not be used, in textile and leather articles which may come into direct and prolonged contact with the human skin or oral cavity, such as:\n— clothing, bedding, towels, hairpieces, wigs, hats, nappies and other sanitary items, sleeping bags,\n— footwear, gloves, wristwatch straps, handbags, purses/wallets, briefcases, chair covers, purses worn round the neck,\n— textile or leather toys and toys which include textile or leather garments,\n— yarn and fabrics intended for use by the final consumer.\n2. Furthermore, the textile and leather articles referred to in paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. Azodyes, which are contained in Appendix 9, ‘List of azodyes’ shall not be placed on the market, or used, as substances, or in mixtures in concentrations greater than 0,1 % by weight, where the substance or the mixture is intended for colouring textile and leather articles.","1. Azofarbstoffe, die durch reduktive Spaltung einer oder mehrerer Azogruppen eines oder mehrere der in Anlage 8 aufgeführten aromatischen Amine in - gemäß den in Anlage 10 aufgeführten Prüfverfahren - nachweisbaren Konzentrationen, d. h. > 30 mg/kg (0,003 Gew.%) im Fertigerzeugnis oder in gefärbten Teilen davon, freisetzen können, dürfen nicht in Textil- und Ledererzeugnissen verwendet werden, die mit der menschlichen Haut oder der Mundhöhle direkt und längere Zeit in Berührung kommen können, wie beispielsweise:\n    kleidung, Bettwäsche, Handtücher, Haarteile, Perücken, Hüte, Windeln und sonstige Toilettenartikel, Schlafsäcke,\n    Schuhe, Handschuhe, Armbanduhren, Handtaschen, Geldbeutel und Brieftaschen, Aktentaschen, Stuhlüberzüge, Brustbeutel,\n    Textil- und Lederspielwaren und Spielwaren mit Textil- oder Lederbekleidung,\n    für den Endverbraucher bestimmte Garne und Gewebe. \n2. Außerdem dürfen die in Absatz 1 genannten Textil- und Ledererzeugnisse nicht in Verkehr gebracht werden, wenn sie nicht den in diesem Absatz festgelegten Anforderungen entsprechen.\n3. Die in Anlage 9, \"Liste der Azofarbstoffe\", dieser Verordnung aufgeführten Azofarbstoffe dürfen weder als Stoffe noch in Gemischen in Konzentrationen von über 0,1 Gew: % in Verkehr gebracht oder verwendet werden, wenn diese zum Färben von Textil- oder Ledererzeugnissen bestimmt sind.","1.偶氮染料，经由一个或多个偶氮基团还原裂解后，可能会释放出一个或多个可探测浓度的附录8中列出的芳香胺。也就是依据附录10中的测试方法，在其成品或上料组件可检测浓度高于30PPM者，不可用于下列可能与皮肤或口腔直接或长时间接触的纺织或皮革制品：\n—服装，床上用品，毛巾，假发，假发，帽子，尿布及其它卫生用品，睡袋\n—鞋类，手套，手表带，手提袋，钱包和钱夹，公文包，椅子套\n—织物和皮革玩具，以及穿着织物或皮革服装的玩具\n—最终消费者使用的纱线和布料。\n2.另外，第1款提到的纺织品和皮革制品，应符合该项规定要求，否则不可投放市场。\n3.在附录9中列出的偶氮染料，其物质或制备浓度大于0.1重量百分比时，不可置于市场用于纺织品或皮革制品的染色。"]
[null,{"$f":"IF($B$1=\"English\",C227,IF($B$1=\"Deutsch\",D227,IF($B$1=\"中文\",E227,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Cement and cement-containing mixtures shall not be placed on the market, or used, if they contain, when hydrated, more than 2 mg/kg (0,0002 %) soluble chromium VI of the total dry weight of the cement.\n2. If reducing agents are used, then without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of cement or cement-containing mixtures is visibly, legibly and indelibly marked with information on the packing date, as well as on the storage conditions and the storage period appropriate to maintaining the activity of the reducing agent and to keeping the content of soluble chromium VI below the limit indicated in paragraph 1.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the placing on the market for, and use in, controlled closed and totally automated processes in which cement and cement-containing mixtures are handled solely by machines and in which there is no possibility of contact with the skin."},"1. Cement and cement-containing mixtures shall not be placed on the market, or used, if they contain, when hydrated, more than 2 mg/kg (0,0002 %) soluble chromium VI of the total dry weight of the cement.\n2. If reducing agents are used, then without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of cement or cement-containing mixtures is visibly, legibly and indelibly marked with information on the packing date, as well as on the storage conditions and the storage period appropriate to maintaining the activity of the reducing agent and to keeping the content of soluble chromium VI below the limit indicated in paragraph 1.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the placing on the market for, and use in, controlled closed and totally automated processes in which cement and cement-containing mixtures are handled solely by machines and in which there is no possibility of contact with the skin.","1. Zement und zementhaltige Gemische dürfen nicht verwendet oder in Verkehr gebracht werden, wenn der Gehalt an löslichem Chrom VI in der Trockenmasse des Zements nach Hydratisierung mehr als 2 mg/kg (0,0002 %) beträgt.\n2. Werden Reduktionsmittel verwendet, so muss der Lieferant unbeschadet der Gültigkeit anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen vor dem Inverkehrbringen gewährleisten, dass auf der Verpackung von Zement oder zementhaltigen Gemischen gut sichtbar, leserlich und unverwischbar angegeben ist, wann das Erzeugnis abgepackt wurde sowie unter welchen Bedingungen und wie lange es gelagert werden kann, ohne dass die Wirkung des Reduktionsmittels nachlässt und der Gehalt an löslichem Chrom VI den in Absatz 1 genannten Grenzwert überschreitet.\n3. Die Absätze 1 und 2 gelten jedoch nicht für das Inverkehrbringen im Hinblick auf überwachte geschlossene und vollautomatische Prozesse und auf die Verwendung in solchen Prozessen, bei denen Zement und zementhaltige Gemische ausschließlich mit Maschinen in Berührung kommen und keine Gefahr von Hautkontakt besteht.","1.水泥和含水泥的制剂，如含有（水合时）的可溶性六价铬的含量超过水泥总干重的0.0002％，不得使用或投放到市场上。\n2.如果使用还原剂，在不违反委员会的其它关于物质和配制品分类、包装和标签法规的前提下，供应商必须保证水泥或含水泥配制品的包装上的标签清晰，可读和不可磨损，标明产品的包装日期、储存条件和适合的储存期，以维持还原剂的活性，并使可溶性六价铬的含量低于第1项中的限值。\n3.但是，上述第1项和第2项不适用于仅由机器操作，且无皮肤接触可能的封闭且完全自动化的系统"]
[null,{"$f":"IF($B$1=\"English\",C228,IF($B$1=\"Deutsch\",D228,IF($B$1=\"中文\",E228,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of neoprene-based contact adhesives in concentrations equal to or greater than 0,1 % by weight in package sizes greater than 350 g.\n2. Neoprene-based contact adhesives containing cyclohexane and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that neoprene-based contact adhesives containing cyclohexane in concentrations equal to or greater than 0,1 % by weight that are placed on the market for supply to the general public after 27 December 2010 are visibly, legibly and indelibly marked as follows:\n‘— This product is not to be used under conditions of poor ventilation.\n— This product is not to be used for carpet laying.’."},"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of neoprene-based contact adhesives in concentrations equal to or greater than 0,1 % by weight in package sizes greater than 350 g.\n2. Neoprene-based contact adhesives containing cyclohexane and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that neoprene-based contact adhesives containing cyclohexane in concentrations equal to or greater than 0,1 % by weight that are placed on the market for supply to the general public after 27 December 2010 are visibly, legibly and indelibly marked as follows:\n‘— This product is not to be used under conditions of poor ventilation.\n— This product is not to be used for carpet laying.’.","1. Darf nach dem 27. Juni 2010 zur Abgabe an die breite Öffentlichkeit in Kontaktklebstoffen auf Neoprenbasis nicht in einer Konzentration von > 0,1 Gew. % in Packungsgrößen von mehr als 350 g erstmalig in Verkehr gebracht werden.\n2. Cyclohexanhaltige Kontaktklebstoffe auf Neoprenbasis, die den Anforderungen unter Absatz 1 nicht entsprechen, dürfen nach dem 27. Dezember 2010 nicht mehr zur Abgabe an die breite Öffentlichkeit in Verkehr gebracht werden.\n3. Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte Kontaktklebstoffe auf Neoprenbasis, die Cyclohexan in einer Konzentration von 0,1 Gew: % oder mehr enthalten, ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n    \"Dieses Produkt darf nicht bei ungenügender Lüftung verarbeitet werden.\n    Dieses Produkt darf nicht zum Verlegen von Teppichböden verwendet werden.\" ","1.作为氯丁橡胶接触粘合剂的成分，其浓度大于等于0.1%（重量百分比）销售包装超过350克，不得投放市场销售给普通大众。\n2.含有环己烷的氯丁橡胶接触粘合剂，如不符合本条第1款的规定，2010年12月27日之后不得投放市场销售给普通大众。\n3.如2010年12月27日之后销售该物质浓度大于等于0.1%的含有环己烷的氯丁橡胶接触粘合剂，在不违反委员会的其它关于物质和配制品分类、包装和标签法规的前提下，供应商必须保证粘合剂以不可磨损的方式，标记以下文字：\n—此产品不得在通风不良时使用。 \n—该产品不能用于地毯铺设。\n"]
[null,{"$f":"IF($B$1=\"English\",C229,IF($B$1=\"Deutsch\",D229,IF($B$1=\"中文\",E229,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall not be:\n(a) placed on the market for the first time for supply to the general public or to professionals after 6 December 2010;\n(b) placed on the market for supply to the general public or to professionals after 6 December 2011;\n(c) used by professionals after 6 June 2012. For the purposes of this entry:\n(i) ‘professional’ means any natural or legal person, including workers and self-employed workers undertaking paint stripping in the course of their professional activity outside an industrial installation;\n(ii) ‘industrial installation’ means a facility used for paint stripping activities.\n2. By way of derogation from paragraph 1, Member States may allow on their territories and for certain activities the use, by specifically trained professionals, of paint strippers containing dichloromethane and may allow the placing on the market of such paint strippers for supply to those professionals.\nMember States making use of this derogation shall define appropriate provisions for the protection of the health and safety of those professionals using paint strippers containing dichloromethane and shall inform the Commission thereof.\nThose provisions shall include a requirement that a professional shall hold a certificate that is accepted by the Member State in which that professional operates, or provide other documentary evidence to that effect, or be otherwise approved by that Member State, so as to demonstrate proper training and competnce to safely use paint strippers containing dichloromethane.\nThe Commission shall prepare a list of the Member States which have made use of the derogation in this paragraph and make it publicly available over the Internet.\n3. A professional benefiting from the derogation referred to in paragraph 2 shall operate only in Member States which have made use of that derogation. The training referred to in paragraph 2 shall cover as a minimum:\n(a) awareness, evaluation and management of risks to health, including information on existing substitutes or processes, which under their conditions of use are less hazardous to the health and safety of workers;\n(b) use of adequate ventilation;\n(c) use of appropriate personal protective equipment that complies with Directive 89/686/EEC.\nEmployers and self-employed workers shall preferably replace dichloromethane with a chemical agent or process which, under its conditions of use, presents no risk, or a lower risk, to the health and safety of workers.\nProfessional shall apply all relevant safety measures in practice, including the use of personal protective equipment.\n4. Without prejudice to other Community legislation on workers protection, paint strippers containing dichloromethane in concentrations equal to or greater than 0,1 % by weight may be used in industrial installations only if the following minimum conditions are met:\n(a) effective ventilation in all processing areas, in particular for the wet processing and the drying of stripped articles: local exhaust ventilation at strip tanks supplemented by forced ventilation in those areas, so as to minimise exposure and to ensure compliance, where technically feasible, with relevant occupational exposure limits;\n(b) measures to minimise evaporation from strip tanks comprising: lids for covering strip tanks except during loading and unloading; suitable loading and unloading arrangements for strip tanks; and wash tanks with water or brine to remove excess solvent after unloading;\n(c) measures for the safe handling of dichloromethane in strip tanks comprising: pumps and pipework for transferring paint stripper to and from strip tanks; and suitable arrangements for safe cleaning of tanks and removal of sludge;\n(d) personal protective equipment that complies with Directive 89/686/EEC comprising: suitable protective gloves, safety goggles and protective clothing; and appropriate respiratory protective equipment where compliance with relevant occupational exposure limits cannot be otherwise achieved;\n(e) adequate information, instruction and training for operators in the use of such equipment.\n5. Without prejudice to other Community provisions concerning the classification, labelling and packaging of substances and mixtures, by 6 December 2011 paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall be visibly, legibly and indelibly marked as follows:\n‘Restricted to industrial use and to professionals approved in certain EU Member States — verify where use is allowed.’"},"1. Paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall not be:\n(a) placed on the market for the first time for supply to the general public or to professionals after 6 December 2010;\n(b) placed on the market for supply to the general public or to professionals after 6 December 2011;\n(c) used by professionals after 6 June 2012. For the purposes of this entry:\n(i) ‘professional’ means any natural or legal person, including workers and self-employed workers undertaking paint stripping in the course of their professional activity outside an industrial installation;\n(ii) ‘industrial installation’ means a facility used for paint stripping activities.\n2. By way of derogation from paragraph 1, Member States may allow on their territories and for certain activities the use, by specifically trained professionals, of paint strippers containing dichloromethane and may allow the placing on the market of such paint strippers for supply to those professionals.\nMember States making use of this derogation shall define appropriate provisions for the protection of the health and safety of those professionals using paint strippers containing dichloromethane and shall inform the Commission thereof.\nThose provisions shall include a requirement that a professional shall hold a certificate that is accepted by the Member State in which that professional operates, or provide other documentary evidence to that effect, or be otherwise approved by that Member State, so as to demonstrate proper training and competnce to safely use paint strippers containing dichloromethane.\nThe Commission shall prepare a list of the Member States which have made use of the derogation in this paragraph and make it publicly available over the Internet.\n3. A professional benefiting from the derogation referred to in paragraph 2 shall operate only in Member States which have made use of that derogation. The training referred to in paragraph 2 shall cover as a minimum:\n(a) awareness, evaluation and management of risks to health, including information on existing substitutes or processes, which under their conditions of use are less hazardous to the health and safety of workers;\n(b) use of adequate ventilation;\n(c) use of appropriate personal protective equipment that complies with Directive 89/686/EEC.\nEmployers and self-employed workers shall preferably replace dichloromethane with a chemical agent or process which, under its conditions of use, presents no risk, or a lower risk, to the health and safety of workers.\nProfessional shall apply all relevant safety measures in practice, including the use of personal protective equipment.\n4. Without prejudice to other Community legislation on workers protection, paint strippers containing dichloromethane in concentrations equal to or greater than 0,1 % by weight may be used in industrial installations only if the following minimum conditions are met:\n(a) effective ventilation in all processing areas, in particular for the wet processing and the drying of stripped articles: local exhaust ventilation at strip tanks supplemented by forced ventilation in those areas, so as to minimise exposure and to ensure compliance, where technically feasible, with relevant occupational exposure limits;\n(b) measures to minimise evaporation from strip tanks comprising: lids for covering strip tanks except during loading and unloading; suitable loading and unloading arrangements for strip tanks; and wash tanks with water or brine to remove excess solvent after unloading;\n(c) measures for the safe handling of dichloromethane in strip tanks comprising: pumps and pipework for transferring paint stripper to and from strip tanks; and suitable arrangements for safe cleaning of tanks and removal of sludge;\n(d) personal protective equipment that complies with Directive 89/686/EEC comprising: suitable protective gloves, safety goggles and protective clothing; and appropriate respiratory protective equipment where compliance with relevant occupational exposure limits cannot be otherwise achieved;\n(e) adequate information, instruction and training for operators in the use of such equipment.\n5. Without prejudice to other Community provisions concerning the classification, labelling and packaging of substances and mixtures, by 6 December 2011 paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall be visibly, legibly and indelibly marked as follows:\n‘Restricted to industrial use and to professionals approved in certain EU Member States — verify where use is allowed.’","1. Farbabbeizer, die Dichlormethan (DCM) in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, dürfen\n    zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2010 nicht mehr erstmalig in Verkehr gebracht werden;\n    zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2011 nicht mehr in Verkehr gebracht werden;\n    nach dem 6. Juni 2012 nicht mehr von gewerblichen Verwendern benutzt werden. \nFür die Zwecke dieses Eintrags bezeichnet der Ausdruck\n    'gewerblicher Verwender' eine natürliche oder juristische Person, einschließlich Angestellte und Selbstständige, die im Zuge ihrer beruflichen Tätigkeit außerhalb einer Industrieanlage Abbeizarbeiten durchführt;\n    'Industrieanlage' eine Anlage, die zum Abbeizen von Farbe genutzt wird. \n2. Abweichend von Absatz 1 können die Mitgliedstaaten in ihren Hoheitsgebieten für bestimmte Tätigkeiten die Verwendung von DCM-haltigen Farbabbeizern durch speziell geschulte gewerbliche Verwender und das Inverkehrbringen solcher Farbabbeizer zur Abgabe an diese gewerblichen Verwender gestatten.\nMitgliedstaaten, die von dieser Ausnahmeregelung Gebrauch machen, legen angemessene Bestimmungen zur Gewährleistung des Gesundheitsschutzes und der Sicherheit für gewerbliche Verwender fest, die DCM-haltige Farbabbeizer verwenden, und unterrichten die Kommission darüber.\nDiese Bestimmungen enthalten die Anforderung, dass ein gewerblicher Verwender über einen Sachkundenachweis verfügen muss, der in dem Mitgliedstaat, in dem er tätig ist, anerkannt wird, oder andere diesbezügliche Nachweisdokumente vorlegen oder eine anderweitige Zulassung desselben Mitgliedstaats besitzen muss, damit nachgewiesen werden kann, dass der gewerbliche Verwender im Umgang mit DCM-haltigen Farbabbeizern ordnungsgemäß geschult wurde und qualifiziert ist, sicher mit ihnen umzugehen.\nDie Kommission erstellt ein Verzeichnis der Mitgliedstaaten, die von der in diesem Absatz genannten Ausnahmeregelung Gebrauch machen, und veröffentlicht dieses Verzeichnis im Internet.\n3. Ein gewerblicher Verwender, der von der in Absatz 2 genannten Ausnahmeregelung Gebrauch macht, darf nur in Mitgliedstaaten tätig werden, die diese Ausnahmeregelung anwenden. Die in Absatz 2 genannte Schulung muss mindestens folgende Bereiche abdecken:\n    Kenntnis, Bewertung und Beherrschung der Gesundheitsrisiken, einschließlich Unterrichtung über bestehende Ersatzstoffe oder Verfahren, die unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender weniger gefährlich sind;\n    Verwendung ausreichender Belüftung;\n    Verwendung geeigneter persönlichen Schutzausrüstungen gemäß der Richtlinie 89/686/EWG. \nArbeitgeber und Selbstständige ersetzen DCM vorrangig durch einen chemischen Arbeitsstoff oder ein Verfahren, der bzw. das unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender nicht oder weniger gefährlich ist.\nDer gewerbliche Verwender setzt alle einschlägigen Sicherheitsmaßnahmen in die Praxis um, einschließlich der Verwendung einer persönlichen Schutzausrüstung.\n4. Unbeschadet anderer Arbeitnehmerschutzvorschriften der Gemeinschaft dürfen Farbabbeizer, die DCM in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, in Industrieanlagen nur verwendet werden, wenn mindestens folgende Bedingungen erfüllt sind:\n    wirksame Belüftung in allen Arbeitsräumen, insbesondere bei der Nassbehandlung und der Trocknung abgebeizter Gegenstände: lokale Absauganlagen an Abbeizbehältnissen, die durch Zwangsbelüftungsanlagen in diesen Bereichen ergänzt werden, um die Exposition zu minimieren und die maßgeblichen Arbeitsplatzgrenzwerte, soweit technisch möglich, einzuhalten;\n    Maßnahmen zur weitestgehenden Verringerung der Verdampfung aus Abbeizbehältnissen, die Folgendes umfassen: Abdeckungen für Abbeizbehältnisse, außer bei der Beladung und Entladung; angemessene Vorkehrungen für die Beladung und Entladung der Abbeizbehältnisse; Reinigungsbehälter, mit Wasser oder Lauge gefüllt, um nach der Entladung das überschüssige Lösemittel vom Abbeizgut zu entfernen;\n    Maßnahmen für die sichere Handhabung von DCM enthaltenden Abbeizbehältnissen, die Folgendes umfassen: Pumpen und Rohrleitungen für die Überleitung des Abbeizmittels aus den und in die Behältnisse; angemessene Vorkehrungen für die sichere Reinigung der Behältnisse und die Beseitigung von Schlämmen;\n    persönliche Schutzausrüstungen gemäß der Richtlinie 89/686/EWG, die Folgendes umfassen: geeignete Schutzhandschuhe, Schutzbrillen und Schutzkleidung; geeignete Atemschutzgeräte, für den Fall, dass die Arbeitsplatzgrenzwerte nicht anderweitig eingehalten werden können;\n    angemessene Informationen, Anweisungen und Übungen zur Verwendung solcher Ausrüstungsgegenstände für die Verwender. \n5. Unbeschadet anderer gemeinschaftlicher Bestimmungen für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen müssen Farbabbeizer, die Dichlormethan in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, ab dem 6. Dezember 2011 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sein:\n'Nur für die industrielle Verwendung und für gewerbliche Verwender, die über eine Zulassung in bestimmten EU-Mitgliedstaaten verfügen. Überprüfen Sie, in welchem Mitgliedstaat die Verwendung genehmigt ist.'","1.二氯甲烷（DCM）含量大于等于0.1（重量百分比）的脱漆剂，不得： (a)在2010年12月6日以后将不再有新产品首次投放市场，销售给普通大众或专业用户；\n(b)在2011年12月6日以后将不再投放市场，销售给广大市民或专业用户；\n(c)在2012年12月6以后，专业用户也不得使用。\n以下是关于这条款的一些注释：\n(i)“专业用户”是指自然人或法人，包括雇员及个体经营人士，他们不是在工业装置上进行脱漆作业；\n(ii)“工业装置”是指用于脱漆的设备。\n2.作为第1款的豁免条款，成员国可以允许在他们国家范围内，在由经过专门培训的专业人员从事的某些特定的工作中使用含DCM脱漆剂；也允许将这类脱漆剂投放市场销售给专业人员。\n各成员国在应用这一豁免时，应同时制定法规，以确保专业人员使用含DCM的脱漆剂时的健康与安全，并通知委员会。 \n这些规定包括专业用户必须持有成员国认可的能力证书，或提交其他有关有效的证明文件，以证明专业人员用户已经过适当的培训，有能力安全地使用含DCM的脱漆剂。\n委员会应准备一份应用该豁免的成员国名单，并公布在互联网上\n3.专业人员只能在应用该豁免的成员国内参考第2段应用该豁免。第2段中提及的培训应该至少包括：\n(a)告知健康风险，如何评估和管理风险，包括现有的替代产品，以及能够降低对员工健康和安全危害的工艺；\n(b) 充分通风换气；\n(c) 使用合适的符合89/686/EEC指令的个人防护用品。\n雇员或个体劳动者应优先考虑用对员工健康和安全无风险或者低风险的化学品或者工艺替代DCM。\n专业人员在操作时应确保所有的安全措施，包括个人防护用品。\n4.在不违反其它劳动保护法规的前提下，含DCM浓度重量百分比大于等于0.1%的脱漆剂，只有在符合以下条件下，可以用在工业装置中：\n(a)在所有加工区域，尤其是湿式加工和脱机物品烘干区域，确保有效通风：所有上述区域的强制通风外加脱漆槽的局部排风，以尽可能减少曝露。\n(b)采取措施尽可能减少脱漆剂挥发，包括：除了上下料，其它时间脱漆槽必须加盖；妥善安排脱漆槽的上下料过程；下料后，用水或盐水清洗脱漆槽，除去多余的溶剂\n(c)采取措施安全处理脱漆槽中的DCM，包括：转移脱漆剂进入、排出脱漆槽的泵和管路（防止泄露）；清理脱漆槽和去除污泥时合理安排\n(d)符合89/686/EEC指令的劳动防护用品，包括：合适的防护手套，安全眼镜，防护服；如果采取措施也不能够符合相关的职业危害曝露限值的话，还需要采用合时的呼吸保护设备。\n(e)为使用该设备的员工提供充分的信息，培训和指导。\n5．在不违背理事会其他关于物质和配制品分类、标签和包装法规的前提下，在2011年12月6日之后，含DCM质量百分比大于等于0.1%的脱漆剂应使用清晰、明显、永久性标识标记如下：‘仅限于在特定的欧盟成员国内用于工业用途或仅供专业人士使用 – 请核实是否允许使用’。"]
[null,{"$f":"IF($B$1=\"English\",C230,IF($B$1=\"Deutsch\",D230,IF($B$1=\"中文\",E230,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited in toys, decorative objects, fuels"},"Prohibited in toys, decorative objects, fuels","Verbot in Spielzeug, Dekorationsgegenständen, Brennstoffen","在玩具，装饰物，燃料中禁止使用"]
[null,{"$f":"IF($B$1=\"English\",C231,IF($B$1=\"Deutsch\",D231,IF($B$1=\"中文\",E231,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited for the manufacturing or machining of nonferrous metals"},"Prohibited for the manufacturing or machining of nonferrous metals","Darf nicht als Stoff oder in Gemischen zur Herstellung oder Verarbeitung von Nichteisenmetallen in Verkehr gebracht oder verwendet werden.","制造或加工非金属材料时禁止使用"]
[null,{"$f":"IF($B$1=\"English\",C232,IF($B$1=\"Deutsch\",D232,IF($B$1=\"中文\",E232,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. After 2010-12-27, mixtures containing this substance in a concentration of >0,1 weight-% MDI must not be brought to the market to be used by the general public unless the supplier guarantees before bringing the product to the market that the packaging                                                  \nContains protective gloves corresponding to the requirements of the regulation 89/686/EU in accordance with 9;         \nBesides other legal stipulations of the community for classification, identification and packaging of substances and mixtures, provides the following information in a visible, legible and non-wipeable manner:                                   \nWith persons that are already sensitized to diisocyanate, handling of this product may trigger allergic reactions.            \nWith asthma, eczema or skin problems, avoid any contact, including skin contact with the product.                            \nDo not use the product in case of insufficient aeration, or wear protective mask with appropriate gas filter (type A1 as per EN 14387).                                                               \n2. Paragraph 1 Letter a does not apply to hot adhesives."},"1. After 2010-12-27, mixtures containing this substance in a concentration of >0,1 weight-% MDI must not be brought to the market to be used by the general public unless the supplier guarantees before bringing the product to the market that the packaging                                                  \nContains protective gloves corresponding to the requirements of the regulation 89/686/EU in accordance with 9;         \nBesides other legal stipulations of the community for classification, identification and packaging of substances and mixtures, provides the following information in a visible, legible and non-wipeable manner:                                   \nWith persons that are already sensitized to diisocyanate, handling of this product may trigger allergic reactions.            \nWith asthma, eczema or skin problems, avoid any contact, including skin contact with the product.                            \nDo not use the product in case of insufficient aeration, or wear protective mask with appropriate gas filter (type A1 as per EN 14387).                                                               \n2. Paragraph 1 Letter a does not apply to hot adhesives.","1. Darf nach dem 27. Dezember 2010 nicht zur Abgabe an die breite Öffentlichkeit in Gemischen, die diesen Stoff in einer Konzentration von >0,1 Gew. % MDI enthalten, in Verkehr gebracht werden; es sei denn, der Lieferant gewährleistet vor dem Inverkehrbringen, dass die Verpackung\n    Schutzhandschuhe enthält, die den Anforderungen der Richtlinie 89/686/EWG des Rates entsprechen 9;\n    unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n        Bei Personen, die bereits für Diisocyanate sensibilisiert sind, kann der Umgang mit diesem Produkt allergische Reaktionen auslösen.\n        Bei Asthma, ekzematösen Hauterkrankungen oder Hautproblemen Kontakt, einschließlich Hautkontakt, mit dem Produkt vermeiden.\n        Das Produkt nicht bei ungenügender Lüftung verwenden oder Schutzmaske mit entsprechendem Gasfilter (Typ A1 nach EN 14387) tragen. \n2. Absatz 1 Buchstabe a gilt nicht für Heißklebstoffe.","1.配制品中含有二苯基甲烷二异氰酸酯(MDI)的重量百分比大于等于0,1%的，2010年12月27日之后不得投放市场供应给普通大众，除非供应商投放市场之前应确保：\na)包装中附有符合委员会指令89/686/EEC要求的防护手套\nb)在不违背理事会其他关于物质和配制品分类、标签和包装法规的前提下，包装上应使用清晰、明显、永久性标识标记如下：\n-对二异氰酸酯很敏感的人在使用本产品时，会引起过敏反应。\n-有哮喘，湿疹或皮肤问题的人应避免接触该产品，包括皮肤接触。\n-不要在通风不足的情况下使用该产品，除非佩戴含有气体过滤器的防护面罩（根据标准EN14387，A1型）。\n2. 作为豁免条款，1(a)不适用于热熔粘合剂。\n"]
[null,{"$f":"IF($B$1=\"English\",C233,IF($B$1=\"Deutsch\",D233,IF($B$1=\"中文\",E233,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited as pure substance and 0,1 in mixtures in certain applications"},"Prohibited as pure substance and 0,1 in mixtures in certain applications","Verbot als Reinstoff und 0,1 in Gemischen in bestimmten Anwendungen","作为纯物质禁用。在某些应用的配制品中，限值为0.1"]
[null,{"$f":"IF($B$1=\"English\",C234,IF($B$1=\"Deutsch\",D234,IF($B$1=\"中文\",E234,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited as pure substance and 0,1 in mixtures with exceptions"},"Prohibited as pure substance and 0,1 in mixtures with exceptions","Verbot als Reinstoff und 0,1 in Gemischen mit Ausnahmen","作为纯物质禁止使用，除豁免之外配制品中限值为0.1"]
[null,{"$f":"IF($B$1=\"English\",C235,IF($B$1=\"Deutsch\",D235,IF($B$1=\"中文\",E235,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- as substance or component of mixtures 0,005 with exceptions  \n- in products 0,1 m% with exceptions  "},"- as substance or component of mixtures 0,005 with exceptions  \n- in products 0,1 m% with exceptions  ","- als Stoff oder Bestandteil von Gemischen 0,005 mit Ausnahmen  \n- in Erzeugnissen 0,1 m% mit Ausnahmen  ","- 除豁免情况外，作为物质或配制品的组分，限值为0.005\n- 除豁免情况外，在产品中，0.1（质量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C236,IF($B$1=\"Deutsch\",D236,IF($B$1=\"中文\",E236,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"51:\n1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles.\n2. Toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n3. The Commission shall re-evaluate, by 16 January 2010, the measures provided for in relation to this entry in the light of new scientific information on such substances and their substitutes, and if justified, these measures shall be modified accordingly.\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.\n52:\n1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles which can be placed in the mouth by children.\n2. Such toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n3. The Commission shall re-evaluate, by 16 January 2010, the measures provided for in relation to this entry in the light of new scientific information on such substances and their substitutes, and if justified, these measures shall be modified accordingly.\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children."},"51:\n1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles.\n2. Toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n3. The Commission shall re-evaluate, by 16 January 2010, the measures provided for in relation to this entry in the light of new scientific information on such substances and their substitutes, and if justified, these measures shall be modified accordingly.\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.\n52:\n1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles which can be placed in the mouth by children.\n2. Such toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n3. The Commission shall re-evaluate, by 16 January 2010, the measures provided for in relation to this entry in the light of new scientific information on such substances and their substitutes, and if justified, these measures shall be modified accordingly.\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.","51:\n1. Dürfen nicht als Stoffe oder in Gemischen in Konzentrationen von mehr als 0,1 Gew: % des weichmacherhaltigen Materials in Spielzeug und Babyartikeln verwendet werden.\n2. Spielzeug und Babyartikel, die diese Phthalate in Konzentrationen von mehr als 0,1 Gew. % des weichmacherhaltigen Materials enthalten, dürfen nicht in Verkehr gebracht werden.\n3. Die Kommission nimmt bis zum 16. Januar 2010 eine Neubewertung der im Zusammenhang mit diesem Eintrag vorgesehenen Maßnahmen im Lichte neuer wissenschaftlicher Erkenntnisse über diese Stoffe und ihre Substitute vor; erforderlichenfalls werden die Maßnahmen entsprechend geändert.\n4. Für die Zwecke dieses Eintrags bezeichnet der Begriff \"Babyartikel\" jedes Erzeugnis, das dazu bestimmt ist, den Schlaf, die Entspannung, die Hygiene, das Füttern und das Saugen von Kindern zu erleichtern.\n52:\n1. Dürfen nicht als Stoffe oder in Gemischen in Konzentrationen von mehr als 0,1 Gew: % des weichmacherhaltigen Materials in Spielzeug und Babyartikeln verwendet werden, die von Kindern in den Mund genommen werden können.\n2. Spielzeug und Babyartikel, die diese Phthalate in Konzentrationen von mehr als 0,1 Gew. % des weichmacherhaltigen Materials enthalten, dürfen nicht in Verkehr gebracht werden.\n3. Die Kommission nimmt bis zum 16. Januar 2010 eine Neubewertung der im Zusammenhang mit diesem Eintrag vorgesehenen Maßnahmen im Lichte neuer wissenschaftlicher Erkenntnisse über diese Stoffe und ihre Substitute vor; erforderlichenfalls werden die Maßnahmen entsprechend geändert.\n4. Für die Zwecke dieses Eintrags bezeichnet der Begriff \"Babyartikel\" jedes Erzeugnis, das dazu bestimmt ist, den Schlaf, die Entspannung, die Hygiene, das Füttern und das Saugen von Kindern zu erleichtern.","51:\n1.不得用作纯物质或用于玩具和儿童用品中，在塑性材料中重量百分比浓度不大于0.1%。\n2.玩具和儿童用品，如果使用了含邻苯二甲酸盐的浓度大于0.1％的塑性材料料，不得投放市场。\n3.在2010年1月16日之前，委员会会依据当时此类物质及其替代物质的科技能力，对为这个项目提供的措施进行重新评估，如需要，对这些措施进行相应地修改。\n4.对于这个项目，“儿童用品”，是指帮助促进睡眠，放松，卫生护理，喂养或吸吮的产品。\n52：\n1.不得用作纯物质或在用于可能被孩子放入嘴里的玩具和儿童用品的塑性材料中重量百分比浓度大于0.1%。\n2.此类玩具和儿童用品，如果使用了含邻苯二甲酸盐的浓度大于0.1％的塑性材料料，不得投放市场。\n3.在2010年1月16日之前，委员会会依据当时此类物质及其替代物质的科技能力，对为这个项目提供的措施进行重新评估，如需要，对这些措施进行相应地修改。\n4.对于这个项目，“儿童用品”，是指帮助促进睡眠，放松，卫生护理，喂养或吸吮的产品。\n"]
[null,{"$f":"IF($B$1=\"English\",C237,IF($B$1=\"Deutsch\",D237,IF($B$1=\"中文\",E237,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited as pure substance and 0,005 in mixtures"},"Prohibited as pure substance and 0,005 in mixtures","Verbot als Reinstoff und 0,005 in Gemischen","作为纯物质禁止使用，在配制品中，0.005"]
[null,{"$f":"IF($B$1=\"English\",C238,IF($B$1=\"Deutsch\",D238,IF($B$1=\"中文\",E238,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. From 1 January 2010, extender oils shall not be placed on the market, or used for the production of tyres or parts of tyres if they contain:\n— more than 1 mg/kg (0,0001 % by weight) BaP, or,\n— more than 10 mg/kg (0,001 % by weight) of the sum of all listed PAHs.\nThese limits shall be regarded as kept, if the polycyclic aromatics (PCA) extract is less than 3 % by weight as measured by the Institute of Petroleum standard IP346: 1998 (Determination of PCA in unused lubricating base oils and asphaltene free petroleum fractions — Dimethyl sulphoxide extraction refractive index method), provided that compliance with the limit values of BaP and of the listed PAHs, as well as the correlation of the measured values with the PCA extract, is controlled by the manufacturer or importer every six months or after each major operational change, whichever is earlier. \n2. Furthermore, tyres and treads for retreading manufactured after 1 January 2010 shall not be placed on the market if they contain extender oils exceeding the limits indicated in paragraph 1.\nThese limits shall be regarded as kept, if the vulcanised rubber compounds do not exceed the limit of 0,35 % Bay protons as measured and calculated by ISO 21461 (Rubber vulcanised — Determination of aromaticity of oil in vulcanised rubber compounds). \n3. By way of derogation, paragraph 2 shall not apply to retreaded tyres if their tread does not contain extender oils exceeding the limits referred to in paragraph 1.\n4. For the purpose of this entry ‘tyres’ shall mean tyres for vehicles covered by:\n— Directive 2007/46/EC of the European Parliament and of the Council of 5 September 2007 establishing a framework for the approval of motor vehicles and their trailers (*****),\n— Directive 2003/37/EC of the European Parliament and of the Council of 26 May 2003 on type-approval of agricultural or forestry tractors, their trailers and interchangeable towed machinery, together with their systems, components and separate technical units (******), and\n— Directive 2002/24/EC of the European Parliament and of the Council of 18 March 2002 relating to the type-approval of two or three-wheel motor vehicles and repealing Council Directive 92/61/EEC(*******). \n______________\n(*****) OJ L 263, 9.10.2007, p. 1. (******) OJ L 171, 9.7.2003, p. 1. (*******) OJ L 124, 9.5.2002, p. 1."},"1. From 1 January 2010, extender oils shall not be placed on the market, or used for the production of tyres or parts of tyres if they contain:\n— more than 1 mg/kg (0,0001 % by weight) BaP, or,\n— more than 10 mg/kg (0,001 % by weight) of the sum of all listed PAHs.\nThese limits shall be regarded as kept, if the polycyclic aromatics (PCA) extract is less than 3 % by weight as measured by the Institute of Petroleum standard IP346: 1998 (Determination of PCA in unused lubricating base oils and asphaltene free petroleum fractions — Dimethyl sulphoxide extraction refractive index method), provided that compliance with the limit values of BaP and of the listed PAHs, as well as the correlation of the measured values with the PCA extract, is controlled by the manufacturer or importer every six months or after each major operational change, whichever is earlier. \n2. Furthermore, tyres and treads for retreading manufactured after 1 January 2010 shall not be placed on the market if they contain extender oils exceeding the limits indicated in paragraph 1.\nThese limits shall be regarded as kept, if the vulcanised rubber compounds do not exceed the limit of 0,35 % Bay protons as measured and calculated by ISO 21461 (Rubber vulcanised — Determination of aromaticity of oil in vulcanised rubber compounds). \n3. By way of derogation, paragraph 2 shall not apply to retreaded tyres if their tread does not contain extender oils exceeding the limits referred to in paragraph 1.\n4. For the purpose of this entry ‘tyres’ shall mean tyres for vehicles covered by:\n— Directive 2007/46/EC of the European Parliament and of the Council of 5 September 2007 establishing a framework for the approval of motor vehicles and their trailers (*****),\n— Directive 2003/37/EC of the European Parliament and of the Council of 26 May 2003 on type-approval of agricultural or forestry tractors, their trailers and interchangeable towed machinery, together with their systems, components and separate technical units (******), and\n— Directive 2002/24/EC of the European Parliament and of the Council of 18 March 2002 relating to the type-approval of two or three-wheel motor vehicles and repealing Council Directive 92/61/EEC(*******). \n______________\n(*****) OJ L 263, 9.10.2007, p. 1. (******) OJ L 171, 9.7.2003, p. 1. (*******) OJ L 124, 9.5.2002, p. 1.","1. Ab dem 1. Januar 2010 dürfen Weichmacheröle nicht für die Herstellung von Reifen oder Reifenbestandteilen in Verkehr gebracht oder verwendet werden, wenn\n    sie mehr als 1 mg/kg (0,0001 Gew.%) BaP enthalten oder\n    der Gehalt aller aufgeführten PAK zusammen mehr als 10 mg/kg (0,001 Gew: %) beträgt. \nDiese Grenzwerte gelten als eingehalten, wenn der PAK-Extrakt weniger als 3 Gew: % beträgt - gemessen gemäß der Norm IP346: 1998 des Institute of Petroleum (Bestimmung der PAK in unbenutzten Schmierölen und asphaltenfreien Erdölfraktionen - Dimethylsulfoxid-Extraktion- Brechungsindex- Methode) -, sofern die Einhaltung der Grenzwerte für BaP und für die aufgeführten PAK sowie die Korrelation der Messwerte mit dem PAK-Extrakt vom Hersteller oder Importeur alle sechs Monate oder nach jeder größeren Änderung der Betriebsverfahren überprüft werden, wobei jeweils der frühere Zeitpunkt maßgeblich ist.\n2. Außerdem dürfen nach dem 1. Januar 2010 hergestellte Reifen und Profile für die Runderneuerung nicht in Verkehr gebracht werden, wenn sie Weichmacheröle enthalten, die die in Absatz 1 angegebenen Grenzwerte überschreiten. Diese Grenzwerte gelten als eingehalten, wenn die vulkanisierte Gummimasse den Grenzwert von 0,35 % HBay - gemessen und berechnet gemäß der ISO-Norm 21461 (Vulkanisierter Gummi - Bestimmung der Aromatizität von Öl in vulkanisierter Gummimasse) - nicht überschreitet.\n3. Ausgenommen von Absatz 2 sind runderneuerte Reifen, wenn ihr Profil keine Weichmacheröle enthält, die die in Absatz 1 angegebenen Grenzwerte überschreiten.\n4. \"Reifen\" im Sinne dieses Eintrags sind Reifen für Fahrzeuge, die unter folgende Richtlinien fallen:\n    Richtlinie 2007/46/EG des Europäischen Parlaments und des Rates vom 5. September 2007 zur Schaffung eines Rahmens für die Genehmigung von Kraftfahrzeugen und Kraftfahrzeuganhängern 4;\n    Richtlinie 2003/37/EG des Europäischen Parlaments und des Rates vom 26. Mai 2003 über die Typgenehmigung für land- oder forstwirtschaftliche Zugmaschinen, ihre Anhänger und die von ihnen gezogenen auswechselbaren Maschinen sowie für Systeme, Bauteile und selbstständige technische Einheiten dieser Fahrzeuge 5 und\n    Richtlinie 2002/24/EG des Europäischen Parlaments und des Rates vom 18. März 2002 über die Typgenehmigung für zweirädrige oder dreirädrige Kraftfahrzeuge und zur Aufhebung der Richtlinie 92/61/EWG des Rates 6. ","1.从2010年1月1日起，填充油不允许投放市场或者用于轮胎/轮胎零件的生产，如果它们含有\n-超过1mg/kg（重量百分比0.0001％）的BaP，或者\n-所有列出的多环芳烃（PAH）的总含量超过10mg/kg（0.001％）。\n当多环芳烃（PCA）提取物少于3%（根据石油研究所标准IP346:1998 干净润滑油和无沥青的石油馏出物中多环芳烃的测定-二甲基亚砜萃取折射率法 进行测试），只要其中BaP和所列的PA含量不超过极限值，以及测量值与制造商或进口商提供的多环芳烃提取物的相关性会在每六个月或者在操作程序发生巨大变化之后进行审查，可以认为符合上述限值。\n2.此外，在2010年1月1日以后生产的针对翻新的轮胎和轮胎花纹被允许被投放市场，只要包含了超过在第1款所指出的极限值的填充油。此极限值被视为遵守，当硫化橡胶化合物未超过0.35％HBay的极限值- 根据ISO标准21461测量和计算所得（硫化橡胶-确定在硫化橡胶化合物中油的方向性）。\n3.第2款的例外是翻新的车胎，如果他们的胎面不包含那种超过了在第1款中指出的极限值的填充油。 \n4.在此条目中，“轮胎”是指机动车辆的轮胎，此机动车涉及以下准则： \n1）在2007年9月5日，欧洲议会与理事会的2007/46/EC指令，此指令建立了机动车辆及其挂车车型批准的框架(*****)。\n2）在2003年5月26日，欧洲议会与理事会的2003/37/EC指令，此指令是关于农业/林业拖拉机及其挂车和被其牵引的可替换机械，以及针对机动车的系统、部件和独立技术单元的型式批准(*****)。 \n3）在2002年3月18日，欧洲议会与理事会的2002/24/EC指令，此指令是关于二轮或三轮机动车的车型批准，同时废止理事会的92/61/EC指令(*******)。\n"]
[null,{"$f":"IF($B$1=\"English\",C239,IF($B$1=\"Deutsch\",D239,IF($B$1=\"中文\",E239,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited in toys, decorative objects"},"Prohibited in toys, decorative objects","Verbot in Spielzeug, Dekorationsgegenständen","在玩具，装饰物品中禁止使用"]
[null,{"$f":"IF($B$1=\"English\",C240,IF($B$1=\"Deutsch\",D240,IF($B$1=\"中文\",E240,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Solvents\n- Making polymers\n- Making of dyes"},"- Solvents\n- Making polymers\n- Making of dyes","- Lösemittel\n- Polymerherstellung\n- Farbstoffherstellung","- 溶剂\n- 制备高分子材料\n- 制备染料"]
[null,{"$f":"IF($B$1=\"English\",C241,IF($B$1=\"Deutsch\",D241,IF($B$1=\"中文\",E241,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Solvents\n- Cleaning agents\n- Caking of semiconductors\n- Caking of printed circuit boards\n- Cutting oils"},"- Solvents\n- Cleaning agents\n- Caking of semiconductors\n- Caking of printed circuit boards\n- Cutting oils","- Lösemittel\n- Reinigungsmittel\n- Halbleiterherstellung\n- Leiterplattenherstellung\n- Schneidöle","- 溶剂\n- 清洁剂\n- 胶结半导体\n- 胶结印刷电路板\n- 切削油"]
[null,{"$f":"IF($B$1=\"English\",C242,IF($B$1=\"Deutsch\",D242,IF($B$1=\"中文\",E242,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvents"},"Solvents","Lösemittel","溶剂"]
[null,{"$f":"IF($B$1=\"English\",C243,IF($B$1=\"Deutsch\",D243,IF($B$1=\"中文\",E243,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate dye products"},"Intermediate dye products","Farbstoffzwischenprodukte","染料产品中间体"]
[null,{"$f":"IF($B$1=\"English\",C244,IF($B$1=\"Deutsch\",D244,IF($B$1=\"中文\",E244,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dyes"},"Dyes","Farbstoffe","染料"]
[null,{"$f":"IF($B$1=\"English\",C245,IF($B$1=\"Deutsch\",D245,IF($B$1=\"中文\",E245,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Lamp glass\n- wood preservatives\n- dyes"},"- Lamp glass\n- wood preservatives\n- dyes","- Lampenglas\n- Holzschutzmittel\n- Farbstoffe","-灯泡玻璃\n-木材防腐剂\n-染料"]
[null,{"$f":"IF($B$1=\"English\",C246,IF($B$1=\"Deutsch\",D246,IF($B$1=\"中文\",E246,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Building materials\n- Thermal insulation material\n- Brake and clutch linings\n- Protective clothing"},"- Building materials\n- Thermal insulation material\n- Brake and clutch linings\n- Protective clothing","- Baustoffe\n- Wärmeisolationsmaterial\n- Brems- und Kupplungsbeläge\n- Schutzkleidung","- 建筑材料\n- 绝热材料\n- 刹车和离合衬套\n- 防护服"]
[null,{"$f":"IF($B$1=\"English\",C247,IF($B$1=\"Deutsch\",D247,IF($B$1=\"中文\",E247,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Dyes\n- Coating materials"},"- Dyes\n- Coating materials","- Farbstoffe\n- Beschichtungsstoffe","-染料\n-涂层材料"]
[null,{"$f":"IF($B$1=\"English\",C248,IF($B$1=\"Deutsch\",D248,IF($B$1=\"中文\",E248,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Dyes\n- Blood test"},"- Dyes\n- Blood test","- Farbstoffe\n- Blutnachweis","- 染料\n- 验血"]
[null,{"$f":"IF($B$1=\"English\",C249,IF($B$1=\"Deutsch\",D249,IF($B$1=\"中文\",E249,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Fuels\n- Basic substance in chemical industry"},"- Fuels\n- Basic substance in chemical industry","- Treibstoffe\n- Grundstoff in chemischer Industrie","- 燃料\n- 化工行业中的基础物质"]
[null,{"$f":"IF($B$1=\"English\",C250,IF($B$1=\"Deutsch\",D250,IF($B$1=\"中文\",E250,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- stabilizers in plastics\n- dyes"},"- stabilizers in plastics\n- dyes","- Stabilisatoren in Kunsstoffen\n- Farbstoffe","-塑料中的稳定剂\n-染料"]
[null,{"$f":"IF($B$1=\"English\",C251,IF($B$1=\"Deutsch\",D251,IF($B$1=\"中文\",E251,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvents\n- raw material for nylon production\n- calibration material"},"- solvents\n- raw material for nylon production\n- calibration material","- Lösemittel\n- Rohstoff für Nylonherstellung\n- Kalibrierungsstoff","-溶剂\n-尼龙产品的原料\n-校对材料"]
[null,{"$f":"IF($B$1=\"English\",C252,IF($B$1=\"Deutsch\",D252,IF($B$1=\"中文\",E252,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PVC production"},"PVC production","PVC-Herstellung","PVC 生产"]
[null,{"$f":"IF($B$1=\"English\",C253,IF($B$1=\"Deutsch\",D253,IF($B$1=\"中文\",E253,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Flame retarders"},"Flame retarders","Flammschutz","阻燃剂"]
[null,{"$f":"IF($B$1=\"English\",C254,IF($B$1=\"Deutsch\",D254,IF($B$1=\"中文\",E254,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Explosives\n- Vulcanization accelerators\n- Degassifiers in aluminum foundries "},"- Explosives\n- Vulcanization accelerators\n- Degassifiers in aluminum foundries ","- Explosivstoffe\n- Vulkanisationsbeschleuniger\n- Entgasungsmittel in Aluminium-Gießereien ","- 炸药\n- 硫化促进剂\n- 铝铸造中的去瓦斯剂"]
[null,{"$f":"IF($B$1=\"English\",C255,IF($B$1=\"Deutsch\",D255,IF($B$1=\"中文\",E255,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage:\n- Insulation material refrigerators\n- hardening agent in polyurethane-lacquers\n- binding agent for the production of wood plates\n- two-component-(polyurethane-)lacquers\n- adhesive agents\n- underbody protection for automobiles\nProduction:\n- polyurethanes\n- thermoplastic polyurethane-elastomers\n- polyurethane-caoutchouc\n- copolymers\n"},"Usage:\n- Insulation material refrigerators\n- hardening agent in polyurethane-lacquers\n- binding agent for the production of wood plates\n- two-component-(polyurethane-)lacquers\n- adhesive agents\n- underbody protection for automobiles\nProduction:\n- polyurethanes\n- thermoplastic polyurethane-elastomers\n- polyurethane-caoutchouc\n- copolymers\n","Verwendung:\n- Isolationsmaterial Kühlgeräte\n- Härter in Polyurethan-Lacken\n- Bindemittel in der Holzplattenherstellung\n- Zweikomponenten-(Polyurethan-)Lacken\n- Klebstoffen\n- Unterbodenschutz von Automobilen\nHerstellung:\n- Polyurethanen\n- thermoplastischen Polyurethan-Elastomeren\n- Polyurethan-Kautschuk\n- Copolymeren\n","用途：\n- 冰箱绝缘材料\n- 在聚氨酯涂料中的固化剂\n- 木板制造中的粘合剂\n- 双组份（聚氨酯）清漆\n- 胶粘剂\n- 汽车制造中的车体底部保护\n- 聚氨酯\n- 热塑性聚氨酯弹性体\n- 聚氨酯生橡胶\n- 共聚物"]
[null,{"$f":"IF($B$1=\"English\",C256,IF($B$1=\"Deutsch\",D256,IF($B$1=\"中文\",E256,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- insulating oil\n- lubricating oil"},"- insulating oil\n- lubricating oil","- Isolationsöl\n- Schmieröl","-绝缘油\n-润滑油"]
[null,{"$f":"IF($B$1=\"English\",C257,IF($B$1=\"Deutsch\",D257,IF($B$1=\"中文\",E257,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Replaces PCB"},"Replaces PCB","Ersatz für PCB","PCB替代品"]
[null,{"$f":"IF($B$1=\"English\",C258,IF($B$1=\"Deutsch\",D258,IF($B$1=\"中文\",E258,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- alloys\n- surface coatings"},"- alloys\n- surface coatings","- Legierungen\n- Oberflächenbeschichtung","-合金\n-表面涂层"]
[null,{"$f":"IF($B$1=\"English\",C259,IF($B$1=\"Deutsch\",D259,IF($B$1=\"中文\",E259,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Hardening agents and cross-linking agents for plastics\n- Non-ionic surfactant and emulsifying agent \n- Production of fuel and lubricating oil additives, drilling auxiliary agents, textile auxiliaries, stabilizers for ethylcellulose, plasticizers for cellulose esters, rubber chemicals, of coating materials for metals, of fungicides and bactericides"},"- Hardening agents and cross-linking agents for plastics\n- Non-ionic surfactant and emulsifying agent \n- Production of fuel and lubricating oil additives, drilling auxiliary agents, textile auxiliaries, stabilizers for ethylcellulose, plasticizers for cellulose esters, rubber chemicals, of coating materials for metals, of fungicides and bactericides","- Härter und Vernetzer für Kunststoffe\n- nichtionisches Tensid und Emulgator \n- Herstellung von Kraftstoff- und Schmieröladditiven, Bohrhilfsmitteln, Textilhilfsmitteln, Stabilisatoren für Ethylcellulose, Weichmachern für Celluloseester, Kautschuk-Chemikalien, von Beschichtungsmaterialien für Metalle, von Fungiziden und Bakteriziden ","- 塑胶的硬化助剂及交联助剂\n- 非电离的表面活化与乳化助剂 \n- 生产燃料和润滑油添加剂， 钻孔辅助助剂，纺织助剂，乙基纤维素的稳定剂，纤维素脂的稳定剂，橡胶助剂，金属的涂层材料，杀真菌剂以及杀菌剂"]
[null,{"$f":"IF($B$1=\"English\",C260,IF($B$1=\"Deutsch\",D260,IF($B$1=\"中文\",E260,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Surfactant\n- Textil dyeing\n- Photographic materials\n- Lubricants\n- Emulsifying agent \n- Spermicides"},"- Surfactant\n- Textil dyeing\n- Photographic materials\n- Lubricants\n- Emulsifying agent \n- Spermicides","- Tensid\n- Textilfärbung\n- photographischen Materialien\n- Schmierstoffe\n- Emulgator \n- Spermizide","- 表面活性剂\n- 织物染色\n- 摄影材料\n- 润滑剂\n- 乳化剂\n- 杀精子剂"]
[null,{"$f":"IF($B$1=\"English\",C261,IF($B$1=\"Deutsch\",D261,IF($B$1=\"中文\",E261,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Solvents\n- Degreasers\nfor metal - floatation agents"},"- Solvents\n- Degreasers\nfor metal - floatation agents","- Lösemittel\n- Metall-Entfettungsmittel\n- Flotationsmittel","- 溶剂\n- 用于金属浮选助剂的脱脂剂\n"]
[null,{"$f":"IF($B$1=\"English\",C262,IF($B$1=\"Deutsch\",D262,IF($B$1=\"中文\",E262,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Wood preservation\n- Textile and leather industries \n- Printing colors"},"- Wood preservation\n- Textile and leather industries \n- Printing colors","- Holzschutz\n- Textil- und Lederindustrie \n- Druckfarben","- 木材贮藏\n- 纺织与皮革工业 \n- 印刷染料"]
[null,{"$f":"IF($B$1=\"English\",C263,IF($B$1=\"Deutsch\",D263,IF($B$1=\"中文\",E263,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Elastomers\n- Impregnation of textiles, carpets and paper \n- Chrome-plating\n- Photography\n- Fire-fighting foams\n- Hydraulic fluids"},"- Elastomers\n- Impregnation of textiles, carpets and paper \n- Chrome-plating\n- Photography\n- Fire-fighting foams\n- Hydraulic fluids","- Elastomere\n- Imprägnierung Textilien, Teppiche und Papier \n- Verchromung\n- Fotografie\n- Feuerlöschschäumen\n- Hydraulikflüssigkeiten ","- 弹性体\n- 织物，地毯与纸的浸润剂\n- 镀铬\n- 摄影\n- 灭火泡沫\n- 液压用液体"]
[null,{"$f":"IF($B$1=\"English\",C264,IF($B$1=\"Deutsch\",D264,IF($B$1=\"中文\",E264,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Plasticizers\n- Solvents\n- Anti-foamers\n- Textile auxiliaries"},"- Plasticizers\n- Solvents\n- Anti-foamers\n- Textile auxiliaries","- Weichmacher\n- Lösemittel\n- Schaumverhütungsmittel\n- Textilhilfsmittel","- 增塑剂\n- 溶剂\n- 防沫剂\n- 纺织助剂"]
[null,{"$f":"IF($B$1=\"English\",C265,IF($B$1=\"Deutsch\",D265,IF($B$1=\"中文\",E265,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Textiles"},"Textiles","Textilien","纺织品"]
[null,{"$f":"IF($B$1=\"English\",C266,IF($B$1=\"Deutsch\",D266,IF($B$1=\"中文\",E266,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Flame retardants\n- Insecticides "},"- Flame retardants\n- Insecticides ","-Flammhemmer\n- Insektizide ","- 防火剂\n- 杀虫剂 "]
[null,{"$f":"IF($B$1=\"English\",C267,IF($B$1=\"Deutsch\",D267,IF($B$1=\"中文\",E267,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Incomplete combustion (carbon black)"},"Incomplete combustion (carbon black)","unvollständige Verbrennung (Ruß)","不完全燃烧（炭黑）"]
[null,{"$f":"IF($B$1=\"English\",C268,IF($B$1=\"Deutsch\",D268,IF($B$1=\"中文\",E268,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- fluorescent tubes\n- measuring instruments\n- switches\n- wood preservatives\n- electrodes"},"- fluorescent tubes\n- measuring instruments\n- switches\n- wood preservatives\n- electrodes","- Leuchtstoffröhren\n- Meßgeräte\n- Schalter\n- Holzschutzmittel\n- Elektroden","- 荧光灯管\n- 测量仪器\n- 开关\n- 木材防腐剂\n- 电极"]
[null,{"$f":"IF($B$1=\"English\",C269,IF($B$1=\"Deutsch\",D269,IF($B$1=\"中文\",E269,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvents"},"Solvents","Lösemittel","溶剂"]
[null,{"$f":"IF($B$1=\"English\",C270,IF($B$1=\"Deutsch\",D270,IF($B$1=\"中文\",E270,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Solvents \n- Paints"},"- Solvents \n- Paints","- Lösemittel \n- Lacke","- 溶剂 \n- 涂料"]
[null,{"$f":"IF($B$1=\"English\",C271,IF($B$1=\"Deutsch\",D271,IF($B$1=\"中文\",E271,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4-Dinitrotoluene"},"2,4-Dinitrotoluene","2,4-Dinitrotoluol (2,4-DNT) ","2,4-二硝基甲苯"]
[null,{"$f":"IF($B$1=\"English\",C272,IF($B$1=\"Deutsch\",D272,IF($B$1=\"中文\",E272,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Ethoxyethanol"},"2-Ethoxyethanol","2-Ethoxyethanol","2-乙氧基乙醇"]
[null,{"$f":"IF($B$1=\"English\",C273,IF($B$1=\"Deutsch\",D273,IF($B$1=\"中文\",E273,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyethanol"},"2-Methoxyethanol","2-Methoxyethanol","2 - 甲氧基乙醇"]
[null,{"$f":"IF($B$1=\"English\",C274,IF($B$1=\"Deutsch\",D274,IF($B$1=\"中文\",E274,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-diaminodiphenylmethane (MDA)"},"4,4'-diaminodiphenylmethane (MDA)","4,4'-Diaminodiphenylmethan (MDA)","4,4'-二氨基二苯甲烷 (MDA)"]
[null,{"$f":"IF($B$1=\"English\",C275,IF($B$1=\"Deutsch\",D275,IF($B$1=\"中文\",E275,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-tert-Butyl-2,4,6-trinitro-m-xylene"},"5-tert-Butyl-2,4,6-trinitro-m-xylene","5-tert-Butyl-2,4,6-trinitro-m-xylol","二甲苯麝香"]
[null,{"$f":"IF($B$1=\"English\",C276,IF($B$1=\"Deutsch\",D276,IF($B$1=\"中文\",E276,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acrylamide"},"Acrylamide","Acrylamid","丙烯酰胺"]
[null,{"$f":"IF($B$1=\"English\",C277,IF($B$1=\"Deutsch\",D277,IF($B$1=\"中文\",E277,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aluminosilicate Refractory Ceramic Fibres"},"Aluminosilicate Refractory Ceramic Fibres","Aluminiumsilikat, hochschmelzende keramische Fasern","硅酸铝耐火陶瓷纤维"]
[null,{"$f":"IF($B$1=\"English\",C278,IF($B$1=\"Deutsch\",D278,IF($B$1=\"中文\",E278,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium dichromate"},"Ammonium dichromate","Ammoniumdichromat","重铬酸铵"]
[null,{"$f":"IF($B$1=\"English\",C279,IF($B$1=\"Deutsch\",D279,IF($B$1=\"中文\",E279,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene"},"Anthracene","Anthracen","蒽"]
[null,{"$f":"IF($B$1=\"English\",C280,IF($B$1=\"Deutsch\",D280,IF($B$1=\"中文\",E280,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil"},"Anthracene oil","Anthracenöl","蒽油"]
[null,{"$f":"IF($B$1=\"English\",C281,IF($B$1=\"Deutsch\",D281,IF($B$1=\"中文\",E281,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene paste"},"Anthracene oil, anthracene paste","Anthracenöl, Anthracenpaste","蒽油，蒽糊"]
[null,{"$f":"IF($B$1=\"English\",C282,IF($B$1=\"Deutsch\",D282,IF($B$1=\"中文\",E282,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene paste, anthracene fraction"},"Anthracene oil, anthracene paste, anthracene fraction","Anthracenöl, Anthracenpaste, Anthracenfraktion","蒽油，蒽糊，蒽馏分"]
[null,{"$f":"IF($B$1=\"English\",C283,IF($B$1=\"Deutsch\",D283,IF($B$1=\"中文\",E283,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene paste,distn. lights"},"Anthracene oil, anthracene paste,distn. lights","Anthracenöl, Anthracenpaste, destn.leicht","蒽油，蒽糊，轻油"]
[null,{"$f":"IF($B$1=\"English\",C284,IF($B$1=\"Deutsch\",D284,IF($B$1=\"中文\",E284,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene-low"},"Anthracene oil, anthracene-low","Anthracenöl, Anthracen-frei","蒽油，含蒽量少"]
[null,{"$f":"IF($B$1=\"English\",C285,IF($B$1=\"Deutsch\",D285,IF($B$1=\"中文\",E285,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzylbutylphthalate (BBP)"},"Benzylbutylphthalate (BBP)","Benzylbutylphthalat (BBP)","邻苯二甲酸丁苄酯 (BBP)"]
[null,{"$f":"IF($B$1=\"English\",C286,IF($B$1=\"Deutsch\",D286,IF($B$1=\"中文\",E286,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate (DEHP)"},"Bis(2-ethylhexyl)phthalate (DEHP)","Bis(2-ethylhexyl)phthalat (DEHP)","邻苯二甲酸二（2-乙基己基)酯 (DEHP)"]
[null,{"$f":"IF($B$1=\"English\",C287,IF($B$1=\"Deutsch\",D287,IF($B$1=\"中文\",E287,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(tributyl tin)oxide"},"Bis(tributyl tin)oxide","Bis(tributylzinn)oxid","三丁基氧化锡 "]
[null,{"$f":"IF($B$1=\"English\",C288,IF($B$1=\"Deutsch\",D288,IF($B$1=\"中文\",E288,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead chromate"},"Lead chromate","Bleichromat","铬酸铅"]
[null,{"$f":"IF($B$1=\"English\",C289,IF($B$1=\"Deutsch\",D289,IF($B$1=\"中文\",E289,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead chromate molybdate sulphate red (C.I. Pigment Red 104)"},"Lead chromate molybdate sulphate red (C.I. Pigment Red 104)","Bleichromatmolybdatsulfatrot (C.I. Pigmentrot 104)","钼铬红(C.I.颜料红 104)"]
[null,{"$f":"IF($B$1=\"English\",C290,IF($B$1=\"Deutsch\",D290,IF($B$1=\"中文\",E290,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead hydrogenarsenate"},"Lead hydrogenarsenate","Bleihydrogenarsenat","砷酸铅"]
[null,{"$f":"IF($B$1=\"English\",C291,IF($B$1=\"Deutsch\",D291,IF($B$1=\"中文\",E291,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead sulfochromate yellow (C.I. Pigment Yellow 34)"},"Lead sulfochromate yellow (C.I. Pigment Yellow 34)","Bleisulfochromatgelb (C.I. Pigmentgelb 34)","铅铬黄（ C.I.颜料黄 34）"]
[null,{"$f":"IF($B$1=\"English\",C292,IF($B$1=\"Deutsch\",D292,IF($B$1=\"中文\",E292,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid"},"Boric acid","Borsäure","硼酸"]
[null,{"$f":"IF($B$1=\"English\",C293,IF($B$1=\"Deutsch\",D293,IF($B$1=\"中文\",E293,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorinated alkanes, C10 – C13 (SCCP)"},"Chlorinated alkanes, C10 – C13 (SCCP)","Chloralkane, C10 – C13 (SCCP)","C10 – C13 短链氯化石蜡(SCCP)"]
[null,{"$f":"IF($B$1=\"English\",C294,IF($B$1=\"Deutsch\",D294,IF($B$1=\"中文\",E294,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromic acid, Oligomers of chromic acid and dichromic acid, Dichromic acid"},"Chromic acid, Oligomers of chromic acid and dichromic acid, Dichromic acid","Chromschwefelsäure, Oligomer der Chromschwefelsäure und Dichromatschwefelsäure, dichromatische Säure","铬酸,铬酸和重铬酸的低聚物,重铬酸"]
[null,{"$f":"IF($B$1=\"English\",C295,IF($B$1=\"Deutsch\",D295,IF($B$1=\"中文\",E295,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium trioxide"},"Chromium trioxide","Chromtrioxid","三氧化铬"]
[null,{"$f":"IF($B$1=\"English\",C296,IF($B$1=\"Deutsch\",D296,IF($B$1=\"中文\",E296,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) carbonate"},"Cobalt(II) carbonate","Cobalt(II)carbonat","碳酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C297,IF($B$1=\"Deutsch\",D297,IF($B$1=\"中文\",E297,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) diacetate"},"Cobalt(II) diacetate","Cobalt(II)diacetat","二乙酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C298,IF($B$1=\"Deutsch\",D298,IF($B$1=\"中文\",E298,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) dinitrate"},"Cobalt(II) dinitrate","Cobalt(II)dinitrat","二硝酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C299,IF($B$1=\"Deutsch\",D299,IF($B$1=\"中文\",E299,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) sulphate"},"Cobalt(II) sulphate","Cobalt(II)sulfat","硫酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C300,IF($B$1=\"Deutsch\",D300,IF($B$1=\"中文\",E300,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt dichloride"},"Cobalt dichloride","Cobaltdichlorid","二氯化钴"]
[null,{"$f":"IF($B$1=\"English\",C301,IF($B$1=\"Deutsch\",D301,IF($B$1=\"中文\",E301,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diarsenic pentaoxide"},"Diarsenic pentaoxide","Diarsenpentaoxid","五氧化二砷"]
[null,{"$f":"IF($B$1=\"English\",C302,IF($B$1=\"Deutsch\",D302,IF($B$1=\"中文\",E302,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diarsenic trioxide"},"Diarsenic trioxide","Diarsentrioxid","三氧化二砷"]
[null,{"$f":"IF($B$1=\"English\",C303,IF($B$1=\"Deutsch\",D303,IF($B$1=\"中文\",E303,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyl phthalate (DBP)"},"Dibutyl phthalate (DBP)","Dibutylphthalat (DBP)","邻苯二甲酸二丁酯  (DBP)"]
[null,{"$f":"IF($B$1=\"English\",C304,IF($B$1=\"Deutsch\",D304,IF($B$1=\"中文\",E304,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisobutyl phthalate (DIBP)"},"Diisobutyl phthalate (DIBP)","Diisobutylphthalat (DIBP)","邻苯二甲酸二异丁酯（DIBP）"]
[null,{"$f":"IF($B$1=\"English\",C305,IF($B$1=\"Deutsch\",D305,IF($B$1=\"中文\",E305,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium tetraborate, anhydrous"},"Disodium tetraborate, anhydrous","Dinatriumtetraborat, anhydrisch","无水四硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C306,IF($B$1=\"Deutsch\",D306,IF($B$1=\"中文\",E306,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromocyclododecane (HBCDD)"},"Hexabromocyclododecane (HBCDD)","Hexabromocyclododecan (HBCDD)","六溴环十二烷 (HBCDD)"]
[null,{"$f":"IF($B$1=\"English\",C307,IF($B$1=\"Deutsch\",D307,IF($B$1=\"中文\",E307,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium dichromate, dihydrate"},"Sodium dichromate, dihydrate","Natriumdichromat, Dihydrat","重铬酸钠，二水合物"]
[null,{"$f":"IF($B$1=\"English\",C308,IF($B$1=\"Deutsch\",D308,IF($B$1=\"中文\",E308,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pitch, coal tar, high temp."},"Pitch, coal tar, high temp.","Pech, Steinkohlenteer, hochtemp.","沥青，煤焦油，高温"]
[null,{"$f":"IF($B$1=\"English\",C309,IF($B$1=\"Deutsch\",D309,IF($B$1=\"中文\",E309,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium chromate"},"Potassium chromate","Kaliumchromat","铬酸钾"]
[null,{"$f":"IF($B$1=\"English\",C310,IF($B$1=\"Deutsch\",D310,IF($B$1=\"中文\",E310,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium dichromate"},"Potassium dichromate","Kaliumdichromat","重铬酸钾"]
[null,{"$f":"IF($B$1=\"English\",C311,IF($B$1=\"Deutsch\",D311,IF($B$1=\"中文\",E311,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium chromate"},"Sodium chromate","Natriumchromat","重铬酸钠"]
[null,{"$f":"IF($B$1=\"English\",C312,IF($B$1=\"Deutsch\",D312,IF($B$1=\"中文\",E312,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetraboron disodium heptaoxide, hydrate"},"Tetraboron disodium heptaoxide, hydrate","Tetrabordinatriumheptaoxid, hydrat","水合四硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C313,IF($B$1=\"Deutsch\",D313,IF($B$1=\"中文\",E313,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichloroethylene"},"Trichloroethylene","Trichlorethylen","三氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C314,IF($B$1=\"Deutsch\",D314,IF($B$1=\"中文\",E314,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Triethylarsenate"},"Triethylarsenate","Triethylarsenat","三乙基砷酸酯 "]
[null,{"$f":"IF($B$1=\"English\",C315,IF($B$1=\"Deutsch\",D315,IF($B$1=\"中文\",E315,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(2-chloroethyl)phosphate"},"Tris(2-chloroethyl)phosphate","Tris(2-chlorethyl)phosphat (TCEP)","三（2 - 氯乙基）磷酸"]
[null,{"$f":"IF($B$1=\"English\",C316,IF($B$1=\"Deutsch\",D316,IF($B$1=\"中文\",E316,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Zirconia Aluminosilicate Refractory Ceramic Fibres"},"Zirconia Aluminosilicate Refractory Ceramic Fibres","Zirconium-Aluminiumsilikat-Keramikfasern, feuerfest","氧化锆硅酸铝耐火陶瓷纤维"]
[null,{"$f":"IF($B$1=\"English\",C317,IF($B$1=\"Deutsch\",D317,IF($B$1=\"中文\",E317,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Extracted from Index no.: \n650-017-00-8"},"Extracted from Index no.: \n650-017-00-8","Auszug aus Index-Nummer 650-017-00-8 in Anhang VI, Teil 3, Tabelle 3.1 der Verordnung (EG) Nr. 1272/2008","从目录编号650-017-00-8中提取"]
[null,{"$f":"IF($B$1=\"English\",C318,IF($B$1=\"Deutsch\",D318,IF($B$1=\"中文\",E318,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"25637-99-4 and 3194-55-6\n(134237-51-7, 134237-50-6, 134237-52-8)"},"25637-99-4 and 3194-55-6\n(134237-51-7, 134237-50-6, 134237-52-8)","25637-99-4 und 3194-55-6\n(134237-51-7, 134237-50-6, 134237-52-8)","25637-99-4 和 3194-55-6\n(134237-51-7, 134237-50-6, 134237-52-8)"]
[null,{"$f":"IF($B$1=\"English\",C319,IF($B$1=\"Deutsch\",D319,IF($B$1=\"中文\",E319,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Extracted from Index no. 650-017-00-8"},"Extracted from Index no. 650-017-00-8","Auszug aus Index Nr. 650-017-00-8","从目录编号650-017-00-8中提取"]
[null,{"$f":"IF($B$1=\"English\",C320,IF($B$1=\"Deutsch\",D320,IF($B$1=\"中文\",E320,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1, however prohibited if material is new development or material is changed"},"0,1, however prohibited if material is new development or material is changed","0,1, jedoch Verbot bei Neuentwicklung von Materialien oder bei Material-Änderungen ","0.1。 但是禁止用于开发新材料或者作为替代材料"]
[null,{"$f":"IF($B$1=\"English\",C321,IF($B$1=\"Deutsch\",D321,IF($B$1=\"中文\",E321,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Hardening agents for epoxy resins and adhesives\n- Intermediate product for diphenylmethanediisocyanate (MDI) - important starting material for PUR-foam\n- Intermediate product for other polymers and monomers"},"- Hardening agents for epoxy resins and adhesives\n- Intermediate product for diphenylmethanediisocyanate (MDI) - important starting material for PUR-foam\n- Intermediate product for other polymers and monomers","- Härter für Epoxidharze und Kleber\n- Zwischenprodukt für Diphenylmethandiisocyanate (MDI) - wichtiger Ausgangsstoff für PUR-Schaum\n- Zwischenprodukt für andere Polymere und Monomere","- 环氧树脂和粘合剂的硬化剂\n- 中间产品， 作为二苯基甲烷二异氰酸酯 (MDI)-聚氨酯泡沫的重要原材料\n- 其它高分子材料以及单体的中间产品"]
[null,{"$f":"IF($B$1=\"English\",C322,IF($B$1=\"Deutsch\",D322,IF($B$1=\"中文\",E322,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Odorous substance, e.g. in cleaning agents, perfume, fabrics, fabric softeners (China is major source)"},"Odorous substance, e.g. in cleaning agents, perfume, fabrics, fabric softeners (China is major source)","Geruchsstoff, z.B. in Reinigungsmittel, Parfüm, Tücher, Weichspüler (Hauptquelle ist China)","有气味的物质，例如清洁剂，香水，织物，织物柔软剂（中国是主要来源）"]
[null,{"$f":"IF($B$1=\"English\",C323,IF($B$1=\"Deutsch\",D323,IF($B$1=\"中文\",E323,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Tar-containing wood impregnation, tar  dyes, arred tape, tar-containg sealing materials\n- Tar, tar oil\n- Soiling in black pigments (carbon black)\n- Intermediate product for antracene-9-aldehyde and anthraquinone"},"- Tar-containing wood impregnation, tar  dyes, arred tape, tar-containg sealing materials\n- Tar, tar oil\n- Soiling in black pigments (carbon black)\n- Intermediate product for antracene-9-aldehyde and anthraquinone","- teerhaltige Holzimprägnierung, Teerfarben, Teerbändern, teerhaltigen Dichtmaterialien\n- Teer, Teeröl\n- Verunreinigung in schwarzen Pigmenten (Ruß)\n- Zwischenprodukt für Antracen-9-aldehyd und Anthrachinon","- 含焦油的木材浸渍，煤焦油染料， 含焦油的密封材料\n- 焦油\n- 黑颜料中的变污剂（炭黑）\n- 蒽-9-醛与蒽醌的中间产品"]
[null,{"$f":"IF($B$1=\"English\",C324,IF($B$1=\"Deutsch\",D324,IF($B$1=\"中文\",E324,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Plasticizer, e.g. in polyvinyl chloride, sealants, fabrics, leather, sealings\n- Adhesives\n- Paints and varnishes, colors and inks\n- Coatings\n- Cosmetics"},"- Plasticizer, e.g. in polyvinyl chloride, sealants, fabrics, leather, sealings\n- Adhesives\n- Paints and varnishes, colors and inks\n- Coatings\n- Cosmetics","- Weichmacher, z.B. in PVC, Dichtmassen, Textil, Leder, Versiegelungen\n- Kleber\n- Lacke, Farben und Tinten\n- Beschichtungsmittel\n- Kosmetika","- 增塑剂，例如用于聚氯乙烯， 密封剂，织物，皮革，密封条\n- 粘合剂\n- 油漆与清漆，颜色与油墨\n- 涂层\n- 化妆品"]
[null,{"$f":"IF($B$1=\"English\",C325,IF($B$1=\"Deutsch\",D325,IF($B$1=\"中文\",E325,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Plasticizers, e.g. in polyvinyl chloride, artificial leather, rubber, latex, fibers, packaging\n- Colors and paints and varnishes\n- Adhesives\n- Fillers\n- Printing inks and pigments\n- Dielectric liquids in capacitors\n- Sealants and cements\n- Lubricants\n- Special solvents"},"- Plasticizers, e.g. in polyvinyl chloride, artificial leather, rubber, latex, fibers, packaging\n- Colors and paints and varnishes\n- Adhesives\n- Fillers\n- Printing inks and pigments\n- Dielectric liquids in capacitors\n- Sealants and cements\n- Lubricants\n- Special solvents","- Weichmacher, z.B. in PVC, Lederimitat, Gummi, Latex, Fasern, Verpackung\n- Farben und Lacken\n- Klebern\n- Füllstoffe\n- Druckertinten und Pigmenten\n- dielektrischen Flüssigkeiten in Kondensatoren\n- Dichtmittel und Kitten\n- Schmierstoffen\n- Speziallösemitteln","- 增塑剂，例如用于聚氯乙烯， 人造皮革，橡胶，乳胶，纤维，包装\n- 颜色，油漆与清漆\n- 粘合剂\n- 填料\n- 印刷油墨和颜料\n- 电容器中的绝缘液体\n- 密封剂和水泥\n- 润滑剂\n- 特殊的溶剂 "]
[null,{"$f":"IF($B$1=\"English\",C326,IF($B$1=\"Deutsch\",D326,IF($B$1=\"中文\",E326,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Anti Fouling Agent in marine paints, leather, textiles, wood, paper\n- Polyvinyl chloride stabilizer"},"- Anti Fouling Agent in marine paints, leather, textiles, wood, paper\n- Polyvinyl chloride stabilizer","- Anti Fouling Agent in Schiffsfarben, Leder, Textilien, Holz, Papier\n- PVC-Stabilisator","- 用于船舶漆，皮革，纺织品， 木材，纸张中的抗污剂\n- 聚氯乙烯稳定剂"]
[null,{"$f":"IF($B$1=\"English\",C327,IF($B$1=\"Deutsch\",D327,IF($B$1=\"中文\",E327,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Wood preservatives"},"Wood preservatives","Holzschutzmittel","木材防腐剂"]
[null,{"$f":"IF($B$1=\"English\",C328,IF($B$1=\"Deutsch\",D328,IF($B$1=\"中文\",E328,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Flame retardants\n- Plasticizers\n- Cooling lubricants\n- Hydraulic oils"},"- Flame retardants\n- Plasticizers\n- Cooling lubricants\n- Hydraulic oils","- Flammhemmer\n- Weichmacher\n- Kühlschmierstoffe\n- Hydrauliköle","- 阻燃剂\n- 增塑剂\n- 冷却润滑剂\n- 液压油"]
[null,{"$f":"IF($B$1=\"English\",C329,IF($B$1=\"Deutsch\",D329,IF($B$1=\"中文\",E329,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Moisture indicator in drying agents (blue silica gel)\n- Glass coloring \n- Electroplating"},"- Moisture indicator in drying agents (blue silica gel)\n- Glass coloring \n- Electroplating","- Feuchtigkeitsindikator in Trockenmitteln (Blaugel)\n- Glasfärbung \n- Galvani","- 干燥剂中的水分指示剂 （蓝色的硅胶）\n- 玻璃着色 \n- 电镀"]
[null,{"$f":"IF($B$1=\"English\",C330,IF($B$1=\"Deutsch\",D330,IF($B$1=\"中文\",E330,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Glass making\n- Wood preservatives\n- Preservative agents in the leather industry\n- Rat poison\n- Intermediate product for the production of other arsenic compounds"},"- Glass making\n- Wood preservatives\n- Preservative agents in the leather industry\n- Rat poison\n- Intermediate product for the production of other arsenic compounds","- Glasherstellung\n- Holzschutzmittel\n- Konservierungsmittel in der Lederindustrie\n- Rattengift\n- Zwischenprodukt für die Herstellung anderer Arsenverbindungen","- 玻璃制备\n- 木材防腐剂\n- 皮革工业中的防腐剂\n- 毒鼠药\n- 生产其它砷的化合物的中间产品"]
[null,{"$f":"IF($B$1=\"English\",C331,IF($B$1=\"Deutsch\",D331,IF($B$1=\"中文\",E331,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Plasticizers\n- Adhesives (paper, wood, automotive)\n- Printing colors\n- Coatings\n- Cosmetics"},"- Plasticizers\n- Adhesives (paper, wood, automotive)\n- Printing colors\n- Coatings\n- Cosmetics","- Weichmacher\n- Kleber (Papier, Holz, Automotive)\n- Druckfarben\n- Beschichtungsmittel\n- Kosmetika","- 增塑剂\n- 粘合剂(纸，木材，汽车)\n- 印刷油墨\n- 涂层\n- 化妆品"]
[null,{"$f":"IF($B$1=\"English\",C332,IF($B$1=\"Deutsch\",D332,IF($B$1=\"中文\",E332,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Flame retardants, e.g. in polystyrene, textiles"},"Flame retardants, e.g. in polystyrene, textiles","Flammhemmer, z.B. in Polystyrol, Textilien","阻燃剂，例如聚苯乙烯，纺织品"]
[null,{"$f":"IF($B$1=\"English\",C333,IF($B$1=\"Deutsch\",D333,IF($B$1=\"中文\",E333,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Treatment of metal surfaces\n- Wood impregnation\n- Anti-corrosion pigments"},"- Treatment of metal surfaces\n- Wood impregnation\n- Anti-corrosion pigments","- Metalloberflächenbehandlung\n- Holz-Imprägnierung\n- Korrosionsschutzpigmente","- 金属表面处理\n- 木材浸渍\n- 防腐颜料"]
[null,{"$f":"IF($B$1=\"English\",C334,IF($B$1=\"Deutsch\",D334,IF($B$1=\"中文\",E334,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Semiconductor industry\n- Plant protection agents\n- Wood preservatives"},"- Semiconductor industry\n- Plant protection agents\n- Wood preservatives","- Halbleiterindustrie\n- Pflanzenschutzmittel\n- Holzschutzmittel","- 半导体工业\n- 植物保护助剂\n- 木材防腐剂"]
[null,{"$f":"IF($B$1=\"English\",C335,IF($B$1=\"Deutsch\",D335,IF($B$1=\"中文\",E335,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"replaced by Commission Regulation (EU) No 757/2010, s. tab 1"},"replaced by Commission Regulation (EU) No 757/2010, s. tab 1","ersetzt durch Verordnung (EU) Nr. 757/2010, siehe Register 1","被委员会法规(欧盟) No 757/2010取代，见表1"]
[null,{"$f":"IF($B$1=\"English\",C336,IF($B$1=\"Deutsch\",D336,IF($B$1=\"中文\",E336,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14"},"included in Annex 14","aufgenommen in Anhang 14","包含在附录14中"]
[null,{"$f":"IF($B$1=\"English\",C337,IF($B$1=\"Deutsch\",D337,IF($B$1=\"中文\",E337,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For annex 14 prioritized through ECHA"},"For annex 14 prioritized through ECHA","für Anhang 14 priorisiert durch ECHA","对于附件14，由欧洲化学品管理署（ECHA）确定优先次序"]
[3,{"$f":"IF($B$1=\"English\",C338,IF($B$1=\"Deutsch\",D338,IF($B$1=\"中文\",E338,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rules for polycyclical aromatic hydrocarbons (tab 3)"},"Rules for polycyclical aromatic hydrocarbons (tab 3)","Regelungen für Polyzyklische Aromatische Kohlenwasserstoffe (Register 3)","PAH - 多环芳烃材料规范（工作表3）"]
[null,{"$f":"IF($B$1=\"English\",C339,IF($B$1=\"Deutsch\",D339,IF($B$1=\"中文\",E339,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient \n[mass%]"},"Concentration of ingredient \n[mass%]","Konzentration des Inhaltsstoffs \n[Massen%]","配料含量\n[质量%]"]
[null,{"$f":"IF($B$1=\"English\",C340,IF($B$1=\"Deutsch\",D340,IF($B$1=\"中文\",E340,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value according to Regulation 1272/2013 REACh Annex XVII"},"Limit value according to Regulation 1272/2013 REACh Annex XVII","Grenzwert nach VO 1272/2013 REACh Annex XVII","限值来自欧盟法规1272/2013 REACh 附件17"]
[null,{"$f":"IF($B$1=\"English\",C341,IF($B$1=\"Deutsch\",D341,IF($B$1=\"中文\",E341,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(a)pyrene"},"Benzo(a)pyrene","Benzo(a)pyren","苯并 (a) 芘"]
[null,{"$f":"IF($B$1=\"English\",C342,IF($B$1=\"Deutsch\",D342,IF($B$1=\"中文\",E342,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acenaphthene "},"Acenaphthene ","Acenaphthen ","苊 "]
[null,{"$f":"IF($B$1=\"English\",C343,IF($B$1=\"Deutsch\",D343,IF($B$1=\"中文\",E343,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acenaphthylene "},"Acenaphthylene ","Acenaphthylen ","苊烯"]
[null,{"$f":"IF($B$1=\"English\",C344,IF($B$1=\"Deutsch\",D344,IF($B$1=\"中文\",E344,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene "},"Anthracene ","Anthracen ","蒽 "]
[null,{"$f":"IF($B$1=\"English\",C345,IF($B$1=\"Deutsch\",D345,IF($B$1=\"中文\",E345,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(a)anthracene  "},"Benzo(a)anthracene  ","Benzo(a)anthracen  ","苯并 (a) 蒽   "]
[null,{"$f":"IF($B$1=\"English\",C346,IF($B$1=\"Deutsch\",D346,IF($B$1=\"中文\",E346,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[j]fluoranthene "},"Benzo[j]fluoranthene ","Benzo(j)fluoranthen ","苯并 (j) 荧蒽 "]
[null,{"$f":"IF($B$1=\"English\",C347,IF($B$1=\"Deutsch\",D347,IF($B$1=\"中文\",E347,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(b)fluoranthene (Benz(e)acephenanthrylene) "},"Benzo(b)fluoranthene (Benz(e)acephenanthrylene) ","Benzo(b)fluoranthen (Benz(e)acephenanthrylen) ","苯并 (b) 荧蒽"]
[null,{"$f":"IF($B$1=\"English\",C348,IF($B$1=\"Deutsch\",D348,IF($B$1=\"中文\",E348,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(e)pyrene"},"Benzo(e)pyrene","Benzo(e)pyren","苯并 (e) 芘"]
[null,{"$f":"IF($B$1=\"English\",C349,IF($B$1=\"Deutsch\",D349,IF($B$1=\"中文\",E349,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(ghi)­perylene "},"Benzo(ghi)­perylene ","Benzo(ghi)-perylen ","苯并 (ghi) 芘烯"]
[null,{"$f":"IF($B$1=\"English\",C350,IF($B$1=\"Deutsch\",D350,IF($B$1=\"中文\",E350,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(k)fluoranthene "},"Benzo(k)fluoranthene ","Benzo(k)fluoranthen ","苯并 (k) 荧蒽 "]
[null,{"$f":"IF($B$1=\"English\",C351,IF($B$1=\"Deutsch\",D351,IF($B$1=\"中文\",E351,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chrysene  "},"Chrysene  ","Chrysen  ","多环芳烃[屈]"]
[null,{"$f":"IF($B$1=\"English\",C352,IF($B$1=\"Deutsch\",D352,IF($B$1=\"中文\",E352,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibenzo(a,h)-anthracene "},"Dibenzo(a,h)-anthracene ","Dibenzo(a,h)-anthracen ","二苯并(a,h)蒽"]
[null,{"$f":"IF($B$1=\"English\",C353,IF($B$1=\"Deutsch\",D353,IF($B$1=\"中文\",E353,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluoranthene "},"Fluoranthene ","Fluoranthen ","荧蒽 "]
[null,{"$f":"IF($B$1=\"English\",C354,IF($B$1=\"Deutsch\",D354,IF($B$1=\"中文\",E354,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluorene "},"Fluorene ","Fluoren ","芴 "]
[null,{"$f":"IF($B$1=\"English\",C355,IF($B$1=\"Deutsch\",D355,IF($B$1=\"中文\",E355,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Indeno[1,2,3-cd]pyrene "},"Indeno[1,2,3-cd]pyrene ","Indeno(1,2,3-cd)pyren ","茚并(1.2.3-C.D)芘"]
[null,{"$f":"IF($B$1=\"English\",C356,IF($B$1=\"Deutsch\",D356,IF($B$1=\"中文\",E356,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Naphthalene "},"Naphthalene ","Naphthalin ","萘  "]
[null,{"$f":"IF($B$1=\"English\",C357,IF($B$1=\"Deutsch\",D357,IF($B$1=\"中文\",E357,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenanthrene "},"Phenanthrene ","Phenanthren ","菲  "]
[null,{"$f":"IF($B$1=\"English\",C358,IF($B$1=\"Deutsch\",D358,IF($B$1=\"中文\",E358,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pyrene "},"Pyrene ","Pyren ","芘  "]
[null,{"$f":"IF($B$1=\"English\",C359,IF($B$1=\"Deutsch\",D359,IF($B$1=\"中文\",E359,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- general obligation to declare from 1 ppm\n- prohibition as follows\na) < 0,2 ppm in materials meant to be put in the mouth, or materials of toys for children < 36 months\nb) 1 ppm in materials not under a) with foreseeable skin contact  more than 30 s\nc) 20 ppm in materials not under a) nor b) with foreseeable skin contact  up to 30 s"},"- general obligation to declare from 1 ppm\n- prohibition as follows\na) < 0,2 ppm in materials meant to be put in the mouth, or materials of toys for children < 36 months\nb) 1 ppm in materials not under a) with foreseeable skin contact  more than 30 s\nc) 20 ppm in materials not under a) nor b) with foreseeable skin contact  up to 30 s","- Deklarationspflicht generell ab 1ppm\n- Verbot wie folgt\na) <0,2ppm in Materialien, die dazu bestimmt sind, in den Mund genommen zu werden, oder Materialien von Spielzeug für Kinder < 36 Monaten\nb) 1ppm in Materialien, die nicht unter a) fallen, mit vorhersehbarem Hautkontakt länger als 30s\nc) 20ppm in Materialien, die nicht unter a) oder b) fallen, mit vorhersehbarem Hautkontakt bis zu 30s","- 一般情况下，超过1ppm有义务申报\n- 以下情况下禁用：\na)在可能会入口的材料中，或者是低龄儿童（小于36个月）的玩具材料，<0.2 ppm\nb)不属于a)情况的材料，但是可预见的皮肤接触可能会超过30秒，1ppm\nc)不属于a)类也不属于b)类情况，可预见的皮肤接触不超过30秒的材料中，20ppm"]
[null,{"$f":"IF($B$1=\"English\",C360,IF($B$1=\"Deutsch\",D360,IF($B$1=\"中文\",E360,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- general obligation to declare per PAK 10 ppm or cumulative value for all PAK 10 ppm\n- prohibition for total (sum) 18 PAK as follows\na) < 0,2 ppm in materials meant to be put in the mouth, or materials of toys for children < 36 months\nb) 10 ppm in materials not under a) with foreseeable skin contact for more than 30 s\nc) 200 ppm in materials not under a) nor b) with foreseeable skin contact for up to 30 s"},"- general obligation to declare per PAK 10 ppm or cumulative value for all PAK 10 ppm\n- prohibition for total (sum) 18 PAK as follows\na) < 0,2 ppm in materials meant to be put in the mouth, or materials of toys for children < 36 months\nb) 10 ppm in materials not under a) with foreseeable skin contact for more than 30 s\nc) 200 ppm in materials not under a) nor b) with foreseeable skin contact for up to 30 s","- Deklarationspflicht generell je PAK 10 ppm oder Summenwert für alle PAK 10 ppm\n- Verbot für Summe 18 PAK wie folgt\na) < 0,2 ppm in Materialien, die dazu bestimmt sind, in den Mund genommen zu werden, oder Materialien von Spielzeug für Kinder < 36 Monaten\nb) 10 ppm in Materialien, die nicht unter a) fallen, mit vorhersehbarem Hautkontakt länger als 30 s\nc) 200 ppm in Materialien, die nicht unter a) oder b) fallen, mit vorhersehbarem Hautkontakt bis zu 30 s","- 一般情况下，任何一种多环芳烃超过10ppm或者所有\n多环芳烃的累积值超过10ppm，有义务申报\n-根据美国环保署（EPA）多环芳烃禁用要求，对16种\n多环芳烃累计含量的限值：\na)在可能会入口的材料中，或者是低龄儿童（小于36个月）的玩具材料，<0.2 ppm\nb)不属于a)情况的材料，但是可预见的皮肤接触可能会超过30秒，10ppm\nc)不属于a)类也不属于b)类情况，可预见的皮肤接触不超过30秒的材料中，200ppm"]
[null,{"$f":"IF($B$1=\"English\",C361,IF($B$1=\"Deutsch\",D361,IF($B$1=\"中文\",E361,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"* List of \"Priority Pollutants\" from EPA"},"* List of \"Priority Pollutants\" from EPA","* Liste der \"Priority Pollutants\" der EPA","* 美国环保署（EPA）\"优先污染物表\""]
[4,{"$f":"IF($B$1=\"English\",C362,IF($B$1=\"Deutsch\",D362,IF($B$1=\"中文\",E362,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rules for plasticizers / phthalates (tab 4)"},"Rules for plasticizers / phthalates (tab 4)","Regelungen für Weichmacher / Phthalate (Register 4)","Plasticizers - 增塑剂/邻苯二甲酸酯材料规范 (工作表4)"]
[null,{"$f":"IF($B$1=\"English\",C363,IF($B$1=\"Deutsch\",D363,IF($B$1=\"中文\",E363,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All plasticizers,added intentionally, below a sample listing, supplement if applicable:"},"All plasticizers,added intentionally, below a sample listing, supplement if applicable:","Alle absichtlich hinzugefügten Weichmacher, im Folgenden eine Beispiel-Liste, ggf. ergänzen:","所有有意添加的增塑剂。下面是增塑剂列表，如果有其它的增塑剂可以补充:"]
[null,{"$f":"IF($B$1=\"English\",C364,IF($B$1=\"Deutsch\",D364,IF($B$1=\"中文\",E364,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(hydroxyethyl) terephthalate"},"Bis(hydroxyethyl) terephthalate","Bis(hydroxyethyl)terephthalat","对苯二酸双(羟乙)酯"]
[null,{"$f":"IF($B$1=\"English\",C365,IF($B$1=\"Deutsch\",D365,IF($B$1=\"中文\",E365,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butyl cyclohexyl phthalate"},"Butyl cyclohexyl phthalate","Butylcyclohexylphthalat","邻苯二甲酸丁基环己酯"]
[null,{"$f":"IF($B$1=\"English\",C366,IF($B$1=\"Deutsch\",D366,IF($B$1=\"中文\",E366,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butyl decyl phthalate"},"Butyl decyl phthalate","Butyldecylphthalat","邻苯二甲酸丁基正癸酯"]
[null,{"$f":"IF($B$1=\"English\",C367,IF($B$1=\"Deutsch\",D367,IF($B$1=\"中文\",E367,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diallyl Phthalate"},"Diallyl Phthalate","Diallylphthalat","邻苯二甲酸二烯丙酯"]
[null,{"$f":"IF($B$1=\"English\",C368,IF($B$1=\"Deutsch\",D368,IF($B$1=\"中文\",E368,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dicyclohexyl Phthalate"},"Dicyclohexyl Phthalate","Dicyclohexylphthalat","邻苯二甲酸二环己酯"]
[null,{"$f":"IF($B$1=\"English\",C369,IF($B$1=\"Deutsch\",D369,IF($B$1=\"中文\",E369,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisodecyl phthalate"},"Diisodecyl phthalate","Di-isodecyl-phthalat","邻苯二甲酸二异癸酯"]
[null,{"$f":"IF($B$1=\"English\",C370,IF($B$1=\"Deutsch\",D370,IF($B$1=\"中文\",E370,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diethyl phthalate"},"Diethyl phthalate","Diethylphthalat","邻苯二甲酸二乙酯"]
[null,{"$f":"IF($B$1=\"English\",C371,IF($B$1=\"Deutsch\",D371,IF($B$1=\"中文\",E371,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisobutylphthalate"},"Diisobutylphthalate","Diisobutylphthalat","邻苯二甲酸二异丁酯"]
[null,{"$f":"IF($B$1=\"English\",C372,IF($B$1=\"Deutsch\",D372,IF($B$1=\"中文\",E372,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisoheptylphthalate"},"Diisoheptylphthalate","Diisoheptylphthalat","邻苯二甲酸二异庚酯"]
[null,{"$f":"IF($B$1=\"English\",C373,IF($B$1=\"Deutsch\",D373,IF($B$1=\"中文\",E373,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisohexylphthalate"},"Diisohexylphthalate","Diisohexylphthalat","邻苯二甲酸二异己酯 "]
[null,{"$f":"IF($B$1=\"English\",C374,IF($B$1=\"Deutsch\",D374,IF($B$1=\"中文\",E374,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisopentylphthalate (DIPP)"},"Diisopentylphthalate (DIPP)","Diisopentylphthalat","邻苯二甲酸二异戊酯"]
[null,{"$f":"IF($B$1=\"English\",C375,IF($B$1=\"Deutsch\",D375,IF($B$1=\"中文\",E375,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisooctylphthalate"},"Diisooctylphthalate","Diisooctylphthalat","邻苯二甲酸二异辛酯"]
[null,{"$f":"IF($B$1=\"English\",C376,IF($B$1=\"Deutsch\",D376,IF($B$1=\"中文\",E376,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisotridecylphthalate"},"Diisotridecylphthalate","Diisotridecylphthalat","邻苯二甲酸二异(十三烷基)酯 "]
[null,{"$f":"IF($B$1=\"English\",C377,IF($B$1=\"Deutsch\",D377,IF($B$1=\"中文\",E377,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisoundecylphthalate"},"Diisoundecylphthalate","Diisoundecylphthalat","邻苯二甲酸二异(十一烷基)酯 "]
[null,{"$f":"IF($B$1=\"English\",C378,IF($B$1=\"Deutsch\",D378,IF($B$1=\"中文\",E378,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethyl phthalate"},"Dimethyl phthalate","Dimethylphthalat","邻苯二甲酸二甲酯"]
[null,{"$f":"IF($B$1=\"English\",C379,IF($B$1=\"Deutsch\",D379,IF($B$1=\"中文\",E379,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimetil tereftalato"},"Dimetil tereftalato","Dimethylterephthalat","对苯二甲酸二甲酯"]
[null,{"$f":"IF($B$1=\"English\",C380,IF($B$1=\"Deutsch\",D380,IF($B$1=\"中文\",E380,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-n-hexilftalato"},"Di-n-hexilftalato","Di-n-hexylphthalat","邻苯二甲酸二己酯"]
[null,{"$f":"IF($B$1=\"English\",C381,IF($B$1=\"Deutsch\",D381,IF($B$1=\"中文\",E381,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-isononil ftalato"},"Di-isononil ftalato","Di-isononyl-phthalat","邻苯二甲酸二异壬酯"]
[null,{"$f":"IF($B$1=\"English\",C382,IF($B$1=\"Deutsch\",D382,IF($B$1=\"中文\",E382,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-n-pentilftalato"},"Di-n-pentilftalato","Di-n-pentylphthalat","邻苯二甲酸二戊酯 "]
[null,{"$f":"IF($B$1=\"English\",C383,IF($B$1=\"Deutsch\",D383,IF($B$1=\"中文\",E383,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-n-propilftalato"},"Di-n-propilftalato","Di-n-propylphthalat","邻苯二甲酸二丙酯 "]
[null,{"$f":"IF($B$1=\"English\",C384,IF($B$1=\"Deutsch\",D384,IF($B$1=\"中文\",E384,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ditridecilftalato"},"Ditridecilftalato","Ditridecylphthalat","邻苯二甲酸二(十三烷基)酯 "]
[null,{"$f":"IF($B$1=\"English\",C385,IF($B$1=\"Deutsch\",D385,IF($B$1=\"中文\",E385,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diundecilftalato"},"Diundecilftalato","Diundecylphthalat","邻苯二甲酸二(十一烷基)酯 "]
[null,{"$f":"IF($B$1=\"English\",C386,IF($B$1=\"Deutsch\",D386,IF($B$1=\"中文\",E386,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-n-octil ftalato"},"Di-n-octil ftalato","Di-n-octylphthalat","邻苯二甲酸二辛酯 "]
[null,{"$f":"IF($B$1=\"English\",C387,IF($B$1=\"Deutsch\",D387,IF($B$1=\"中文\",E387,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"n-Octil n-decil ftalato"},"n-Octil n-decil ftalato","n-Octyl-n-decyl-phthalat","邻苯二甲酸正辛基正癸酯"]
[null,{"$f":"IF($B$1=\"English\",C388,IF($B$1=\"Deutsch\",D388,IF($B$1=\"中文\",E388,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SVHC"},"SVHC","SVHC","SVHC 高关注度物质清单"]
[null,{"$f":"IF($B$1=\"English\",C389,IF($B$1=\"Deutsch\",D389,IF($B$1=\"中文\",E389,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Listed in GADSL "},"Listed in GADSL ","in GADSL gelistet","收录在GADSL中 "]
[5,{"$f":"IF($B$1=\"English\",C390,IF($B$1=\"Deutsch\",D390,IF($B$1=\"中文\",E390,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-RoHS (tab 5)\n2011/65/EU"},"EC-RoHS (tab 5)\n2011/65/EU","EG-ROHS (Register 5)\n2011/65/EU","ROHS - 欧盟RoHS指令（工作表5）\n2011/65/EU"]
[null,{"$f":"IF($B$1=\"English\",C391,IF($B$1=\"Deutsch\",D391,IF($B$1=\"中文\",E391,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value [mass% in homogeneous material]"},"Limit value [mass% in homogeneous material]","Grenzwert [Massen% im homogenen Werkstoff]","限值 [均质材料中的质量% ]"]
[null,{"$f":"IF($B$1=\"English\",C392,IF($B$1=\"Deutsch\",D392,IF($B$1=\"中文\",E392,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of substance [mass% in homogeneous material]"},"Concentration of substance [mass% in homogeneous material]","Konzentration des Inhaltsstoffs [Massen% im homogenen Werkstoff]","物质含量 [均质材料中的质量%]"]
[null,{"$f":"IF($B$1=\"English\",C393,IF($B$1=\"Deutsch\",D393,IF($B$1=\"中文\",E393,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Exception claimed? If so, which one?"},"Exception claimed? If so, which one?","Ausnahme in Anspruch genommen? Wenn ja, welche?","是否可以豁免？如果可以，符合豁免清单中的哪一条?"]
[null,{"$f":"IF($B$1=\"English\",C394,IF($B$1=\"Deutsch\",D394,IF($B$1=\"中文\",E394,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Blei","铅"]
[null,{"$f":"IF($B$1=\"English\",C395,IF($B$1=\"Deutsch\",D395,IF($B$1=\"中文\",E395,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and it's compounds"},"Cadmium and it's compounds","Kadmium und seine Verbindungen","鎘及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C396,IF($B$1=\"Deutsch\",D396,IF($B$1=\"中文\",E396,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury and it's compounds"},"Mercury and it's compounds","Quecksilber und seine Verbindungen ","汞及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C397,IF($B$1=\"Deutsch\",D397,IF($B$1=\"中文\",E397,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium VI"},"Chromium VI","Chrom VI","六价铬"]
[null,{"$f":"IF($B$1=\"English\",C398,IF($B$1=\"Deutsch\",D398,IF($B$1=\"中文\",E398,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated biphenyles (PBB)"},"Polybrominated biphenyles (PBB)","Polybromierte Biphenyle (PBB)","多溴联苯 (PBB)"]
[null,{"$f":"IF($B$1=\"English\",C399,IF($B$1=\"Deutsch\",D399,IF($B$1=\"中文\",E399,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated diphenyl ether (PBDE)"},"Polybrominated diphenyl ether (PBDE)","Polybromierte Diphenylether (PBDE)","多溴联苯醚(PBDE)"]
[6,{"$f":"IF($B$1=\"English\",C400,IF($B$1=\"Deutsch\",D400,IF($B$1=\"中文\",E400,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-ELV (tab 6) 2000/53/EC"},"EC-ELV (tab 6) 2000/53/EC","EG-ELV (Register 6) 2000/53/EG","ELV - 欧盟报废车辆指令（工作表6） 2000/53/EC"]
[null,{"$f":"IF($B$1=\"English\",C401,IF($B$1=\"Deutsch\",D401,IF($B$1=\"中文\",E401,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Declaration only through IMDS (www.mdsystem.com)"},"Declaration only through IMDS (www.mdsystem.com)","Deklaration nur über IMDS (www.mdsystem.com)","仅通过 IMDS申报 (www.mdsystem.com)"]
[null,{"$f":"IF($B$1=\"English\",C402,IF($B$1=\"Deutsch\",D402,IF($B$1=\"中文\",E402,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content of the regulation see directive of the European Union 2000/53/EC \"End Of Life Vehicles\" "},"Content of the regulation see directive of the European Union 2000/53/EC \"End Of Life Vehicles\" ","Inhalt der Regelung siehe Richtlinie der Europäischen Union 2000/53/EG \"End Of Life Vehicles\" ","法规内容详见欧盟指令2000/53/EC \"报废车辆\" "]
[7,{"$f":"IF($B$1=\"English\",C403,IF($B$1=\"Deutsch\",D403,IF($B$1=\"中文\",E403,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"GADSL (tab 7) see http://www.gadsl.org/ - Please click on \"GADSL Reference List\" "},"GADSL (tab 7) see http://www.gadsl.org/ - Please click on \"GADSL Reference List\" ","GADSL (Register 7) siehe http://www.gadsl.org/ - bitte auf \"GADSL Reference List\" klicken","GADSL - 全球汽车申报物质清单（工作表7）\nhttp://www.gadsl.org/"]
[null,{"$f":"IF($B$1=\"English\",C404,IF($B$1=\"Deutsch\",D404,IF($B$1=\"中文\",E404,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P or D\nor\nP / D"},"P or D\nor\nP / D","P oder D\noder\nP / D","P或者 D\n或者\nP / D"]
[null,{"$f":"IF($B$1=\"English\",C405,IF($B$1=\"Deutsch\",D405,IF($B$1=\"中文\",E405,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content of the regulation see \"Global Automotive Declarable Substance List\" (www.gadsl.org) "},"Content of the regulation see \"Global Automotive Declarable Substance List\" (www.gadsl.org) ","Inhalt der Regelung siehe \"Global Automotive Declarable Substance List\" (www.gadsl.org)","内容详见 \"全球汽车申报物质清单\" (www.gadsl.org) "]
[8,{"$f":"IF($B$1=\"English\",C406,IF($B$1=\"Deutsch\",D406,IF($B$1=\"中文\",E406,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-Regulation on batteries and accumulators (tab 8)"},"EC-Regulation on batteries and accumulators (tab 8)","EG-Batterie- und Akkumulatorregulierung (Register 8)","Batteries-欧共体-电池和蓄电池法规（第 8 页）"]
[null,{"$f":"IF($B$1=\"English\",C407,IF($B$1=\"Deutsch\",D407,IF($B$1=\"中文\",E407,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value [mass%]"},"Limit value [mass%]","Grenzwert [Massen%]","限定值[质量%]"]
[null,{"$f":"IF($B$1=\"English\",C408,IF($B$1=\"Deutsch\",D408,IF($B$1=\"中文\",E408,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient \n[mass%]"},"Concentration of ingredient \n[mass%]","Konzentration des Inhaltsstoffs \n[Massen%]","配料含量\n[%]"]
[9,{"$f":"IF($B$1=\"English\",C409,IF($B$1=\"Deutsch\",D409,IF($B$1=\"中文\",E409,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rules for auxiliary manufacturing materials excl. cooling lubricants (tab 9)"},"Rules for auxiliary manufacturing materials excl. cooling lubricants (tab 9)","Regelungen für Fertigungshilfsstoffe außer Kühlschmierstoffe (Register 9)","Manufacturing materials - 除冷却润滑剂以外的辅助制造材料规范（工作表9）"]
[null,{"$f":"IF($B$1=\"English\",C410,IF($B$1=\"Deutsch\",D410,IF($B$1=\"中文\",E410,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkyl phenoles and their isomers, ethoxylates and esters;"},"Alkyl phenoles and their isomers, ethoxylates and esters;","Alkylphenole und deren Isomere, Ethoxylate und Ester","烷基苯酚及其异构体，乙氧化物和酯"]
[null,{"$f":"IF($B$1=\"English\",C411,IF($B$1=\"Deutsch\",D411,IF($B$1=\"中文\",E411,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aromatics in dimethyl sulfoxide (DMSO), soluble aromatics fraction of mineral oil products"},"Aromatics in dimethyl sulfoxide (DMSO), soluble aromatics fraction of mineral oil products","Aromaten in Dimethylsulfoxid (DMSO), Löslicher Aromantenanteil von Mineralölprodukten","二甲基亚砜(DMSO)中的芳香化合物，矿物油产品中可溶的芳香化合物"]
[null,{"$f":"IF($B$1=\"English\",C412,IF($B$1=\"Deutsch\",D412,IF($B$1=\"中文\",E412,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Azo­dyes with carcinogenic amine components"},"Azo­dyes with carcinogenic amine components","Azo-Farbstoffe mit karzinogenen Aminkomponenten","带有致癌胺的含氮染料"]
[null,{"$f":"IF($B$1=\"English\",C413,IF($B$1=\"Deutsch\",D413,IF($B$1=\"中文\",E413,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and its combinations, taken as element"},"Lead and its combinations, taken as element","Blei und seine Verbindungen, gerechnet als Element","铅及其化合物，按元素计"]
[null,{"$f":"IF($B$1=\"English\",C414,IF($B$1=\"Deutsch\",D414,IF($B$1=\"中文\",E414,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"chlorine releaseable, total content, calculated as elemental chlorine"},"chlorine releaseable, total content, calculated as elemental chlorine","Chlor freisetzbar, Gesamgehalt, gerechnet als elementares Chlor","可释放的氯，按氯元素总量计"]
[null,{"$f":"IF($B$1=\"English\",C415,IF($B$1=\"Deutsch\",D415,IF($B$1=\"中文\",E415,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Halogenated hydrocarbons"},"Halogenated hydrocarbons","Halogenierte Kohlenwasserstoffe ","卤代烃"]
[null,{"$f":"IF($B$1=\"English\",C416,IF($B$1=\"Deutsch\",D416,IF($B$1=\"中文\",E416,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol"},"Phenol","Phenol","苯酚"]
[null,{"$f":"IF($B$1=\"English\",C417,IF($B$1=\"Deutsch\",D417,IF($B$1=\"中文\",E417,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicones"},"Silicones","Silikone","硅"]
[null,{"$f":"IF($B$1=\"English\",C418,IF($B$1=\"Deutsch\",D418,IF($B$1=\"中文\",E418,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Total heavy metals"},"Total heavy metals","Summe Schwermetalle","重金属总量"]
[null,{"$f":"IF($B$1=\"English\",C419,IF($B$1=\"Deutsch\",D419,IF($B$1=\"中文\",E419,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Zinc and its combinations, taken as element"},"Zinc and its combinations, taken as element","Zink und seine Verbindungen, gerechnet als Element","锌及其化合物，按元素计"]
[null,{"$f":"IF($B$1=\"English\",C420,IF($B$1=\"Deutsch\",D420,IF($B$1=\"中文\",E420,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anti-aging agents on basis of phenol and amine"},"Anti-aging agents on basis of phenol and amine","Alterungsschutzmittel auf Phenol- und Aminbasis","以苯酚和胺为基质的抗老化剂"]
[null,{"$f":"IF($B$1=\"English\",C421,IF($B$1=\"Deutsch\",D421,IF($B$1=\"中文\",E421,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biocides"},"Biocides","Biozide","杀虫剂"]
[null,{"$f":"IF($B$1=\"English\",C422,IF($B$1=\"Deutsch\",D422,IF($B$1=\"中文\",E422,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Siloxanes"},"Siloxanes","Siloxane","硅氧烷"]
[null,{"$f":"IF($B$1=\"English\",C423,IF($B$1=\"Deutsch\",D423,IF($B$1=\"中文\",E423,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonates (total)"},"Sulfonates (total)","Sulfonate (Summe)","磺酸盐 (总量)"]
[null,{"$f":"IF($B$1=\"English\",C424,IF($B$1=\"Deutsch\",D424,IF($B$1=\"中文\",E424,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"VCI (Volatile Corrosion Inhibitor)"},"VCI (Volatile Corrosion Inhibitor)","VCI (Volatile Corrosion Inhibitor)","VCI (挥发性防腐剂)"]
[null,{"$f":"IF($B$1=\"English\",C425,IF($B$1=\"Deutsch\",D425,IF($B$1=\"中文\",E425,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in aqueous cleaning agents, cooling lubricants and emulsion cleaners"},"10 ppm in aqueous cleaning agents, cooling lubricants and emulsion cleaners","10 ppm in wässrigen Reinigungsmitteln, Kühlschmierstoffen und Emulsionsreinigern","在水基清洗剂、冷却润滑剂，乳状清洁剂中，10 ppm"]
[null,{"$f":"IF($B$1=\"English\",C426,IF($B$1=\"Deutsch\",D426,IF($B$1=\"中文\",E426,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,0 mass% in lubricant base oils"},"3,0 mass% in lubricant base oils","3 Massen% in Schmierstoffgrundölen","在冷却润滑剂中， 质量百分比3.0%"]
[null,{"$f":"IF($B$1=\"English\",C427,IF($B$1=\"Deutsch\",D427,IF($B$1=\"中文\",E427,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in lubricants, dyes"},"10 ppm in lubricants, dyes","10 ppm in Schmierstoffen, Farbstoffen","在润滑剂、着色剂中，10 ppm"]
[null,{"$f":"IF($B$1=\"English\",C428,IF($B$1=\"Deutsch\",D428,IF($B$1=\"中文\",E428,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in lubricants"},"10 ppm in lubricants","10 ppm in Schmierstoffen","在润滑剂中，10 ppm"]
[null,{"$f":"IF($B$1=\"English\",C429,IF($B$1=\"Deutsch\",D429,IF($B$1=\"中文\",E429,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1  m% in anticorrosive agents, aqueous cleaning agents, water miscible cooling lubricants and emulsion cleaners"},"0,1  m% in anticorrosive agents, aqueous cleaning agents, water miscible cooling lubricants and emulsion cleaners","0,1 m% in Korrosionsschutzmitteln, wässrigen Reinigungsmitteln, wassermischbaren Kühlschmierstoffen und Emulsionsreinigern","在防腐剂、水性清洗剂、水溶性冷却润滑剂和乳液清洁剂中，质量百分比 0.1%"]
[null,{"$f":"IF($B$1=\"English\",C430,IF($B$1=\"Deutsch\",D430,IF($B$1=\"中文\",E430,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 m% as solvent for surface treatment, incl. cleaning"},"0,1 m% as solvent for surface treatment, incl. cleaning","0,1 m% als Lösemittel für die Oberflächenbehandlung, inkl. Reinigung","在用于表面处理（含清洁）的溶剂中，质量百分比 0.1%"]
[null,{"$f":"IF($B$1=\"English\",C431,IF($B$1=\"Deutsch\",D431,IF($B$1=\"中文\",E431,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances"},"1 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances","1 ppm in Korrosionsschutzmitteln, wässrigen Reinigungsmitteln, Kühlschmierstoffen, Emulsionsreinigern und KW-Reinigern","在防腐剂、水基清洗剂、冷却润滑剂、乳状清洁剂以及烃类清洁物质中，1ppm"]
[null,{"$f":"IF($B$1=\"English\",C432,IF($B$1=\"Deutsch\",D432,IF($B$1=\"中文\",E432,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances Exemptions for Zn with non-water miscible cooling lubricants"},"10 ppm in anticorrosive agents, aqueous cleaning agents, cooling lubricants, emulsion cleaners and hydrocarbon­cleaning substances Exemptions for Zn with non-water miscible cooling lubricants","10 ppm in Korrosionsschutzmitteln, wässrigen Reinigungsmitteln, Kühlschmierstoffen, Emulsionsreinigern und KW-Reinigern. Ausnahmen für Zn bei nicht wassermischbaren Kühlschmierstoffen","在防腐剂、水基清洗剂、冷却润滑剂、乳状清洁剂以及烃类清洁物质中为10ppm。非水溶性冷却润滑剂中的锌可以豁免"]
[null,{"$f":"IF($B$1=\"English\",C433,IF($B$1=\"Deutsch\",D433,IF($B$1=\"中文\",E433,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in anticorrosive agents and cooling lubricants. Exemptions with non-water miscible cooling lubricants"},"10 ppm in anticorrosive agents and cooling lubricants. Exemptions with non-water miscible cooling lubricants","10 ppm in Korrosionsschutzmitteln und Kühlschmierstoffen. Ausnahmen bei nicht wassermischbaren Kühlschmierstoffen.","防腐剂、冷却润滑剂中为10ppm。\n非水溶性冷却润滑剂可以豁免。"]
[null,{"$f":"IF($B$1=\"English\",C434,IF($B$1=\"Deutsch\",D434,IF($B$1=\"中文\",E434,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5 % in lubricants and test media;"},"5 % in lubricants and test media;","5 % in Schmierstoffen und Prüfmedien","润滑剂和测试介质中，5%"]
[null,{"$f":"IF($B$1=\"English\",C435,IF($B$1=\"Deutsch\",D435,IF($B$1=\"中文\",E435,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass%"},"0,1 mass%","0,1 Massen%","质量百分比 0.1%"]
[null,{"$f":"IF($B$1=\"English\",C436,IF($B$1=\"Deutsch\",D436,IF($B$1=\"中文\",E436,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass% in water miscible metal working fluids"},"0,1 mass% in water miscible metal working fluids","0,1 Massen% in wassermischbaren Kühlschmierstoffen","在水溶性金属工作介质，质量百分比 0.1%"]
[null,{"$f":"IF($B$1=\"English\",C437,IF($B$1=\"Deutsch\",D437,IF($B$1=\"中文\",E437,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass% in lubricants and test media"},"0,1 mass% in lubricants and test media","0,1 Massen% in Schmierstoffen und Prüfmedien","在润滑剂及测试介质中，质量百分比 0.1%"]
[null,{"$f":"IF($B$1=\"English\",C438,IF($B$1=\"Deutsch\",D438,IF($B$1=\"中文\",E438,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass% in anticorrosive agents"},"0,1 mass% in anticorrosive agents","0,1 Massen% in Korrosionsschutzmitteln","在防腐剂中，质量百分比 0.1%"]
[10,{"$f":"IF($B$1=\"English\",C439,IF($B$1=\"Deutsch\",D439,IF($B$1=\"中文\",E439,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rules for cooling lubricants (tab 10)"},"Rules for cooling lubricants (tab 10)","Reglungen für Kühlschmierstoffe (Register 10)","Cooling Lubricants - 冷却润滑剂材料规范（工作表10）"]
[null,{"$f":"IF($B$1=\"English\",C440,IF($B$1=\"Deutsch\",D440,IF($B$1=\"中文\",E440,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited substances (P)\nVKIS-VSI Substances"},"Prohibited substances (P)\nVKIS-VSI Substances","Verbotene Inhaltsstoffe (P)\nVKIS-VSI Stoffliste","禁用物质 (P)\nVKIS-VSI 物质列表 "]
[null,{"$f":"IF($B$1=\"English\",C441,IF($B$1=\"Deutsch\",D441,IF($B$1=\"中文\",E441,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzisothiazol-3(2H)-one"},"1,2-Benzisothiazol-3(2H)-one","1,2-Benzisothiazol-3(2H)-on","1,2-苯并异噻唑基-3(2H)-酮"]
[null,{"$f":"IF($B$1=\"English\",C442,IF($B$1=\"Deutsch\",D442,IF($B$1=\"中文\",E442,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-Tris(2-hydroxyethyl)-hexahydro-1,3,5-triazine (HHT)"},"1,3,5-Tris(2-hydroxyethyl)-hexahydro-1,3,5-triazine (HHT)","1,3,5-Tris-(2-hydroxyethyl)-hexahydro-1,3,5-triazin (HHT)","1,3,5-三(2-羟乙基)-S-六氢三嗪"]
[null,{"$f":"IF($B$1=\"English\",C443,IF($B$1=\"Deutsch\",D443,IF($B$1=\"中文\",E443,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(Methoxycarbonylamino)-benzimidazol (Carbendazim)"},"2-(Methoxycarbonylamino)-benzimidazol (Carbendazim)","2-(Methoxycarbonylamino)-benzimidazol (Carbendazim)","2-(甲氧基碳酰氨基)苯并咪唑 (多菌灵)"]
[null,{"$f":"IF($B$1=\"English\",C444,IF($B$1=\"Deutsch\",D444,IF($B$1=\"中文\",E444,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-methylamino-2-methyl-1-propanol"},"2-methylamino-2-methyl-1-propanol","2-Methylamino-2-methyl-1-propanol","2-甲氨基- 2-甲基- 1-丙醇"]
[null,{"$f":"IF($B$1=\"English\",C445,IF($B$1=\"Deutsch\",D445,IF($B$1=\"中文\",E445,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2´-Iminodiethanol (Diethanolamin)"},"2,2´-Iminodiethanol (Diethanolamin)","2,2´-Iminodiethanol (Diethanolamin)","2,2'-亚氨基二乙醇(二乙醇胺)"]
[null,{"$f":"IF($B$1=\"English\",C446,IF($B$1=\"Deutsch\",D446,IF($B$1=\"中文\",E446,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Octyl-2H-isothiazol-3-on"},"2-Octyl-2H-isothiazol-3-on","2-Octyl-2H-isothiazol-3-on","2-辛基-2H-异噻唑啉-3-酮"]
[null,{"$f":"IF($B$1=\"English\",C447,IF($B$1=\"Deutsch\",D447,IF($B$1=\"中文\",E447,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4´-Dimethyloxazolidin"},"4,4´-Dimethyloxazolidin","4,4´-Dimethyloxazolidin","4,4-二甲基恶唑啉"]
[null,{"$f":"IF($B$1=\"English\",C448,IF($B$1=\"Deutsch\",D448,IF($B$1=\"中文\",E448,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-Chloro-2-methyl-2,3-dihydroisothiazol-3-on and 2-methyl-2,3-dihydroisothiazol-3-on, mixture in ratio 3:1 (CMI/MI)"},"5-Chloro-2-methyl-2,3-dihydroisothiazol-3-on and 2-methyl-2,3-dihydroisothiazol-3-on, mixture in ratio 3:1 (CMI/MI)","5-Chlor-2-methyl-2,3-dihydroisothiazol-3-on und 2-Methyl-2,3-dihydroisothiazol-3-on, Gemisch im Verhältnis 3:1 (CMI/MI)","5-氯-2-甲基-2,3-二异噻唑啉-3-酮和 2-甲基-2,3-二异噻唑啉-3-酮的配制品，比例为 3:1 (CMI/MI)   "]
[null,{"$f":"IF($B$1=\"English\",C449,IF($B$1=\"Deutsch\",D449,IF($B$1=\"中文\",E449,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Amides that release secondary amines"},"Amides that release secondary amines","Amide, die sekundäre Amine abspalten","能释放出仲胺的酰胺类物质"]
[null,{"$f":"IF($B$1=\"English\",C450,IF($B$1=\"Deutsch\",D450,IF($B$1=\"中文\",E450,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Amines, secondary, that form carcinogenic N-nitrosamines of categories 1 or 2"},"Amines, secondary, that form carcinogenic N-nitrosamines of categories 1 or 2","Amine, sekundäre, die krebserzeugende N-Nitrosamine der Kategorien 1 oder 2 bilden","仲胺类物质，能形成第1、2类致癌物质N-亚硝胺"]
[null,{"$f":"IF($B$1=\"English\",C451,IF($B$1=\"Deutsch\",D451,IF($B$1=\"中文\",E451,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Barium salts with the exception of barium sulfate"},"Barium salts with the exception of barium sulfate","Bariumsalze mit Ausnahme von Bariumsulfat","钡盐，硫酸钡除外"]
[null,{"$f":"IF($B$1=\"English\",C452,IF($B$1=\"Deutsch\",D452,IF($B$1=\"中文\",E452,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo-(a)-pyrene (BaP)"},"Benzo-(a)-pyrene (BaP)","Benzo-(a)-pyren (BaP)","苯并(a)芘 (BaP)"]
[null,{"$f":"IF($B$1=\"English\",C453,IF($B$1=\"Deutsch\",D453,IF($B$1=\"中文\",E453,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate (DEHP)"},"Bis(2-ethylhexyl)phthalate (DEHP)","Bis-(2-ethylhexyl)-phthalat (DEHP)","邻苯二甲酸二(2-乙基己基)酯 (DEHP)"]
[null,{"$f":"IF($B$1=\"English\",C454,IF($B$1=\"Deutsch\",D454,IF($B$1=\"中文\",E454,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid"},"Boric acid","Borsäure","硼酸"]
[null,{"$f":"IF($B$1=\"English\",C455,IF($B$1=\"Deutsch\",D455,IF($B$1=\"中文\",E455,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"carbendazim methyl 1H-benzimidazol-2-ylcarbamate)"},"carbendazim methyl 1H-benzimidazol-2-ylcarbamate)","Carbendazim (2-(Methoxycarbonylamino)-\nbenzimidazol)","多菌灵 甲基1H-苯并咪唑-2 - 基氨基甲酸"]
[null,{"$f":"IF($B$1=\"English\",C456,IF($B$1=\"Deutsch\",D456,IF($B$1=\"中文\",E456,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorinated paraffins, short-chain (C10-C13, SCCP)"},"Chlorinated paraffins, short-chain (C10-C13, SCCP)","Chlorparaffine, kurzkettig (C10-C13, SCCP)","短链氯化石蜡 (C10-C13, SCCP)"]
[null,{"$f":"IF($B$1=\"English\",C457,IF($B$1=\"Deutsch\",D457,IF($B$1=\"中文\",E457,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorinated paraffins, long-chain (≥ C18, LCCP)"},"Chlorinated paraffins, long-chain (≥ C18, LCCP)","Chlorparaffine, langkettig (≥ C18, LCCP)","长链氯化石蜡 (≥ C18, LCCP)"]
[null,{"$f":"IF($B$1=\"English\",C458,IF($B$1=\"Deutsch\",D458,IF($B$1=\"中文\",E458,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorinated paraffins, medium-chain (C14 – C17, MCCP)"},"Chlorinated paraffins, medium-chain (C14 – C17, MCCP)","Chlorparaffine, mittelkettig (C14 – C17, MCCP)","中链氯化石蜡 (C14 – C17, MCCP)"]
[null,{"$f":"IF($B$1=\"English\",C459,IF($B$1=\"Deutsch\",D459,IF($B$1=\"中文\",E459,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diethanolamine (2,2 -Iminodiethanol)"},"Diethanolamine (2,2 -Iminodiethanol)","Diethanolamin (2,2 -Iminodiethanol)","二乙醇胺(2,2'-二乙醇胺)"]
[null,{"$f":"IF($B$1=\"English\",C460,IF($B$1=\"Deutsch\",D460,IF($B$1=\"中文\",E460,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethylenediaminetetraacetic acid and salts (EDTA)"},"Ethylenediaminetetraacetic acid and salts (EDTA)","Ethylendiamintetraessigsäure und Salze (EDTA)","乙二胺四乙酸及其盐类 (EDTA)"]
[null,{"$f":"IF($B$1=\"English\",C461,IF($B$1=\"Deutsch\",D461,IF($B$1=\"中文\",E461,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Glutaraldehyde"},"Glutaraldehyde","Glutardialdehyd","戊二醛"]
[null,{"$f":"IF($B$1=\"English\",C462,IF($B$1=\"Deutsch\",D462,IF($B$1=\"中文\",E462,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Morpholine and morpholine releasing combinations"},"Morpholine and morpholine releasing combinations","Morpholin und Morpholin freisetzende Verbindungen","吗啡啉及其释放的化合物"]
[null,{"$f":"IF($B$1=\"English\",C463,IF($B$1=\"Deutsch\",D463,IF($B$1=\"中文\",E463,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium tetraborates"},"Sodium tetraborates","Natriumtetraborate","四硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C464,IF($B$1=\"Deutsch\",D464,IF($B$1=\"中文\",E464,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nitrite and nitrite releasing combinations"},"Nitrite and nitrite releasing combinations","Nitrit und Nitrit freisetzende Verbindungen","亚硝酸盐及能释放除亚硝酸根的化合物"]
[null,{"$f":"IF($B$1=\"English\",C465,IF($B$1=\"Deutsch\",D465,IF($B$1=\"中文\",E465,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol"},"Nonylphenol","Nonylphenol","壬基酚"]
[null,{"$f":"IF($B$1=\"English\",C466,IF($B$1=\"Deutsch\",D466,IF($B$1=\"中文\",E466,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol ethoxylates"},"Nonylphenol ethoxylates","Nonylphenolethoxylate","乙氧基化壬基酚"]
[null,{"$f":"IF($B$1=\"English\",C467,IF($B$1=\"Deutsch\",D467,IF($B$1=\"中文\",E467,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Orthoboric acid, sodium salt"},"Orthoboric acid, sodium salt","Orthoborsäure, Natriumsalz","硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C468,IF($B$1=\"Deutsch\",D468,IF($B$1=\"中文\",E468,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated biphenyls - PCB"},"Polychlorinated biphenyls - PCB","Polychlorierte Biphenyle - PCB","多氯联苯 - PCB"]
[null,{"$f":"IF($B$1=\"English\",C469,IF($B$1=\"Deutsch\",D469,IF($B$1=\"中文\",E469,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated terphenyls – PCT"},"Polychlorinated terphenyls – PCT","Polychlorierte Terphenyle – PCT","多氯三联苯 – PCT"]
[null,{"$f":"IF($B$1=\"English\",C470,IF($B$1=\"Deutsch\",D470,IF($B$1=\"中文\",E470,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium-2-pyridinethiol-1-oxide (Pyrithione Sodium Salt)"},"Sodium-2-pyridinethiol-1-oxide (Pyrithione Sodium Salt)","Pyridin-2-thiol-N-oxid (Natriumpyrithion)","2-巯基吡啶氧化物钠盐"]
[null,{"$f":"IF($B$1=\"English\",C471,IF($B$1=\"Deutsch\",D471,IF($B$1=\"中文\",E471,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"55965-84-9 and 2682-20-4"},"55965-84-9 and 2682-20-4","55965-84-9 und 2682-20-4","55965-84-9 和2682-20-4"]
[null,{"$f":"IF($B$1=\"English\",C472,IF($B$1=\"Deutsch\",D472,IF($B$1=\"中文\",E472,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,2 % water miscible"},"0,2 % water miscible","0,2 % wassermischbar","0.2% 水溶性"]
[null,{"$f":"IF($B$1=\"English\",C473,IF($B$1=\"Deutsch\",D473,IF($B$1=\"中文\",E473,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"15 ppm water mixed"},"15 ppm water mixed","15 ppm wassergemischt","15 ppm 与水混合"]
[null,{"$f":"IF($B$1=\"English\",C474,IF($B$1=\"Deutsch\",D474,IF($B$1=\"中文\",E474,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm water miscible;\n2 ppm water mixed"},"10 ppm water miscible;\n2 ppm water mixed","10 ppm wassermischbar;\n2 ppm wassergemischt","10 ppm 水溶性；\n2 ppm 与水混合"]
[null,{"$f":"IF($B$1=\"English\",C475,IF($B$1=\"Deutsch\",D475,IF($B$1=\"中文\",E475,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1 ppm water mixed"},"1 ppm water mixed","1 ppm wassergemischt","1 ppm 与水混合"]
[null,{"$f":"IF($B$1=\"English\",C476,IF($B$1=\"Deutsch\",D476,IF($B$1=\"中文\",E476,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited water miscible;\n20 mg nitrite/l water mixed"},"Prohibited water miscible;\n20 mg nitrite/l water mixed","Verbot wassermischbar;\n20 mg Nitrit/l wassergemischt","禁止 水溶性；\n20mg亚硝酸盐/升 与水混合"]
[null,{"$f":"IF($B$1=\"English\",C477,IF($B$1=\"Deutsch\",D477,IF($B$1=\"中文\",E477,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5 % water miscible"},"5 % water miscible","5 % wassermischbar","5% 水溶性"]
[null,{"$f":"IF($B$1=\"English\",C478,IF($B$1=\"Deutsch\",D478,IF($B$1=\"中文\",E478,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"REACH Annex XVII"},"REACH Annex XVII","REACH Anhang XVII","REACH 附件 17"]
[11,{"$f":"IF($B$1=\"English\",C479,IF($B$1=\"Deutsch\",D479,IF($B$1=\"中文\",E479,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging (Tab 11)\nEU-PACKAGING (94/62/EC), France Decree No. 2022-105"},"Packaging (Tab 11)\nEU-PACKAGING (94/62/EC), France Decree No. 2022-105","Verpackungsrichtlinie (Register 11)\nEU-PACKAGING (94/62/EC), France Decree No. 2022-105","Packaging - 欧盟包装材料指令（工作表 11）\n94/62/EC 与 2004/12/EC, France Decree No. 2020-105"]
[null,{"$f":"IF($B$1=\"English\",C480,IF($B$1=\"Deutsch\",D480,IF($B$1=\"中文\",E480,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of substance\n[ppm]"},"Concentration of substance\n[ppm]","Konzentration des Inhaltsstoffs \n[ppm]","物质含量\n[ppm]"]
[null,{"$f":"IF($B$1=\"English\",C481,IF($B$1=\"Deutsch\",D481,IF($B$1=\"中文\",E481,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Blei","铅"]
[null,{"$f":"IF($B$1=\"English\",C482,IF($B$1=\"Deutsch\",D482,IF($B$1=\"中文\",E482,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium VI"},"Chromium VI","Chrom VI","六价铬"]
[null,{"$f":"IF($B$1=\"English\",C483,IF($B$1=\"Deutsch\",D483,IF($B$1=\"中文\",E483,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Kadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C484,IF($B$1=\"Deutsch\",D484,IF($B$1=\"中文\",E484,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury"},"Mercury","Quecksilber","汞"]
[null,{"$f":"IF($B$1=\"English\",C485,IF($B$1=\"Deutsch\",D485,IF($B$1=\"中文\",E485,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"cumulative 100 ppm"},"cumulative 100 ppm","kumulativ 100 ppm","累计 100 ppm"]
[2,{"$f":"IF($B$1=\"English\",C486,IF($B$1=\"Deutsch\",D486,IF($B$1=\"中文\",E486,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 17"},"included in Annex 17","aufgenommen in Anhang 17","包含在附件17中"]
[null,{"$f":"IF($B$1=\"English\",C487,IF($B$1=\"Deutsch\",D487,IF($B$1=\"中文\",E487,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acrylamide"},"Acrylamide","Acrylamid","丙烯酰胺"]
[null,{"$f":"IF($B$1=\"English\",C488,IF($B$1=\"Deutsch\",D488,IF($B$1=\"中文\",E488,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No longer in use."},"No longer in use.","Nicht mehr in Verwendung: Verbot als Reinstoff und 0,1 in Gemischen für Abdichtungsanwendungen wie beispielsweise Injektion, Verpressung, Verfugung oder Verguss in Verkehr gebracht oder verwendet werden.","不再使用"]
[null,{"$f":"IF($B$1=\"English\",C489,IF($B$1=\"Deutsch\",D489,IF($B$1=\"中文\",E489,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"the substances are listed in appendix 3 and 4 of annex 17 REACH"},"the substances are listed in appendix 3 and 4 of annex 17 REACH","die Stoffliste befindet sich in Anlage 3 und Anlage 4 zu Anhang 17 REACH .","见材料列表附录3和附录4和REACH附件17"]
[null,{"$f":"IF($B$1=\"English\",C490,IF($B$1=\"Deutsch\",D490,IF($B$1=\"中文\",E490,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"the substances are listed in appendix 5 and 6 of annex 17 REACH"},"the substances are listed in appendix 5 and 6 of annex 17 REACH","die Stoffliste befindet sich in Anlage 5 und Anlage 6 zu Anhang 17 REACH .","见材料列表附录5和附录6和REACH附件17"]
[null,{"$f":"IF($B$1=\"English\",C491,IF($B$1=\"Deutsch\",D491,IF($B$1=\"中文\",E491,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"the substances are listed in appendix 1 and 2 of annex 17 REACH"},"the substances are listed in appendix 1 and 2 of annex 17 REACH","die Stoffliste befindet sich in Anlage 1 und Anlage 2 zu Anhang 17 REACH .","见材料列表附录1和附录2和REACH附件17"]
[null,{"$f":"IF($B$1=\"English\",C492,IF($B$1=\"Deutsch\",D492,IF($B$1=\"中文\",E492,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1,1,3,3-tetramethylbutyl)phenol"},"4-(1,1,3,3-tetramethylbutyl)phenol","4-(1,1,3,3-Tetramethylbutyl)phenol","4-(1,1,3,3-四甲基丁基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C493,IF($B$1=\"Deutsch\",D493,IF($B$1=\"中文\",E493,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichromium tris(chromate)"},"Dichromium tris(chromate)","Dichromtris(chromat)","二铬 三铬（铬酸盐）"]
[null,{"$f":"IF($B$1=\"English\",C494,IF($B$1=\"Deutsch\",D494,IF($B$1=\"中文\",E494,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyaniline; o-Anisidine,"},"2-Methoxyaniline; o-Anisidine,","2-Methoxyanilin (o-Anisidin)","邻甲氧基苯胺；邻茴香胺"]
[null,{"$f":"IF($B$1=\"English\",C495,IF($B$1=\"Deutsch\",D495,IF($B$1=\"中文\",E495,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead styphnate"},"Lead styphnate","Bleistyphnat","收敛酸铅"]
[null,{"$f":"IF($B$1=\"English\",C496,IF($B$1=\"Deutsch\",D496,IF($B$1=\"中文\",E496,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentazinc chromate octahydroxide"},"Pentazinc chromate octahydroxide","Pentazinkchromat-octahydroxid","锌黄"]
[null,{"$f":"IF($B$1=\"English\",C497,IF($B$1=\"Deutsch\",D497,IF($B$1=\"中文\",E497,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N-dimethylacetamide"},"N,N-dimethylacetamide","N,N-Dimethylacetamid","N,N-二甲基乙酰胺"]
[null,{"$f":"IF($B$1=\"English\",C498,IF($B$1=\"Deutsch\",D498,IF($B$1=\"中文\",E498,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl) phthalate"},"Bis(2-methoxyethyl) phthalate","Bis(2-methoxyethyl)phthalat","邻苯二甲酸二甲氧乙酯"]
[null,{"$f":"IF($B$1=\"English\",C499,IF($B$1=\"Deutsch\",D499,IF($B$1=\"中文\",E499,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dichloroethane"},"1,2-dichloroethane","1,2-Dichlorethan","1,2-二氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C500,IF($B$1=\"Deutsch\",D500,IF($B$1=\"中文\",E500,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenolphthalein"},"Phenolphthalein","Phenolphthalein","酚酞"]
[null,{"$f":"IF($B$1=\"English\",C501,IF($B$1=\"Deutsch\",D501,IF($B$1=\"中文\",E501,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Arsenic acid"},"Arsenic acid","Arsensäure","亚砷酸"]
[null,{"$f":"IF($B$1=\"English\",C502,IF($B$1=\"Deutsch\",D502,IF($B$1=\"中文\",E502,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead diazide, Lead azide"},"Lead diazide, Lead azide","Bleidiazid, Bleiazid","迭氮化铅"]
[null,{"$f":"IF($B$1=\"English\",C503,IF($B$1=\"Deutsch\",D503,IF($B$1=\"中文\",E503,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium hydroxyoctaoxodizincatedichromate"},"Potassium hydroxyoctaoxodizincatedichromate","Kaliumhydroxyoctaoxo-dizinkat-dichromat","氢氧化铬酸锌钾"]
[null,{"$f":"IF($B$1=\"English\",C504,IF($B$1=\"Deutsch\",D504,IF($B$1=\"中文\",E504,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde, oligomeric reaction products with aniline"},"Formaldehyde, oligomeric reaction products with aniline","Formaldehyd, oligomeres Reaktionsprodukt mit Anilin (technisches MDA)","甲醛和苯胺的低聚反应产物（技术MDA）"]
[null,{"$f":"IF($B$1=\"English\",C505,IF($B$1=\"Deutsch\",D505,IF($B$1=\"中文\",E505,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead dipicrate"},"Lead dipicrate"," Bleidipikrat","三硝基苯酚铅"]
[null,{"$f":"IF($B$1=\"English\",C506,IF($B$1=\"Deutsch\",D506,IF($B$1=\"中文\",E506,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead diarsenate"},"Trilead diarsenate"," Tribleidiarsenat","砷酸铅"]
[null,{"$f":"IF($B$1=\"English\",C507,IF($B$1=\"Deutsch\",D507,IF($B$1=\"中文\",E507,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl) ether"},"Bis(2-methoxyethyl) ether","Bis(2-methoxyethyl)ether"," 二乙二醇二甲醚"]
[null,{"$f":"IF($B$1=\"English\",C508,IF($B$1=\"Deutsch\",D508,IF($B$1=\"中文\",E508,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Calcium arsenate"},"Calcium arsenate","Calciumarsenat","砷酸钙"]
[null,{"$f":"IF($B$1=\"English\",C509,IF($B$1=\"Deutsch\",D509,IF($B$1=\"中文\",E509,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2'-dichloro-4,4'-methylenedianiline"},"2,2'-dichloro-4,4'-methylenedianiline","2,2'-Dichlor-4,4'-methylendianilin","2，2′-二氯-4，4'-亚甲基二苯胺"]
[null,{"$f":"IF($B$1=\"English\",C510,IF($B$1=\"Deutsch\",D510,IF($B$1=\"中文\",E510,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Strontium chromate"},"Strontium chromate"," Strontiumchromat","铬酸锶"]
[null,{"$f":"IF($B$1=\"English\",C511,IF($B$1=\"Deutsch\",D511,IF($B$1=\"中文\",E511,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C7-11-branched and linear alkyl esters"},"1,2-Benzenedicarboxylic acid, di-C7-11-branched and linear alkyl esters","1,2-Benzoldicarbonsäure, Di-C7-11-verzweigte und lineare Alkylester (DHNUP)","邻苯二甲酸，二-C 7-C11支链和直链烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C512,IF($B$1=\"Deutsch\",D512,IF($B$1=\"中文\",E512,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,3-Trichloropropane"},"1,2,3-Trichloropropane"," 1,2,3-Trichlorpropan","1,2,3-三氯丙烷"]
[null,{"$f":"IF($B$1=\"English\",C513,IF($B$1=\"Deutsch\",D513,IF($B$1=\"中文\",E513,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Ethoxyethyl acetate"},"2-Ethoxyethyl acetate","2-Ethoxyethylacetat","乙二醇乙醚醋酸酯"]
[null,{"$f":"IF($B$1=\"English\",C514,IF($B$1=\"Deutsch\",D514,IF($B$1=\"中文\",E514,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Methyl-2-pyrrolidone"},"1-Methyl-2-pyrrolidone","1-Methyl-2-pyrrolidon","1-甲基-2-吡咯烷酮 "]
[null,{"$f":"IF($B$1=\"English\",C515,IF($B$1=\"Deutsch\",D515,IF($B$1=\"中文\",E515,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl esters, C7-rich"},"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl esters, C7-rich"," 1,2-Benzoldicarbonsäure, Di-C6-8-verzweigte Alkylester, C7-reich (DIHP)","邻苯二甲酸二C6-8支链烷基酯(富C7) "]
[null,{"$f":"IF($B$1=\"English\",C516,IF($B$1=\"Deutsch\",D516,IF($B$1=\"中文\",E516,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydrazine"},"Hydrazine","Hydrazin","肼类"]
[null,{"$f":"IF($B$1=\"English\",C517,IF($B$1=\"Deutsch\",D517,IF($B$1=\"中文\",E517,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14 and Annex 17"},"Included in Annex 14 and Annex 17","Aufgenommen in Anhang 14 und Anhang17","包含在附件14和附件17中"]
[null,{"$f":"IF($B$1=\"English\",C518,IF($B$1=\"Deutsch\",D518,IF($B$1=\"中文\",E518,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethylfumarate (DMF)"},"Dimethylfumarate (DMF)","Dimethylfumarat (DMF)","富马酸二甲酯 (DMF)"]
[null,{"$f":"IF($B$1=\"English\",C519,IF($B$1=\"Deutsch\",D519,IF($B$1=\"中文\",E519,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in annex 14\n- Latest application date: \n21 February 2013\n- Sunset date:\n21 August 2014"},"included in annex 14\n- Latest application date: \n21 February 2013\n- Sunset date:\n21 August 2014","aufgenommen in Anhang 14\n- Antragsschluss: \n21. Februar 2013\n- Ablauftermin:\n21. August 2014","包含在附件14\n- 申请截止日期为：: \n21. 02. 2013\n- 过期:\n21. 08. 2014"]
[null,{"$f":"IF($B$1=\"English\",C520,IF($B$1=\"Deutsch\",D520,IF($B$1=\"中文\",E520,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in annex 14\n- Latest application date: \n21 February 2014\n- Sunset date:\n21 August 2015"},"included in annex 14\n- Latest application date: \n21 February 2014\n- Sunset date:\n21 August 2015","aufgenommen in Anhang 14\n- Antragsschluss:\n21. Februar 2014\n- Ablauftermin:\n21. August 2015","包含在附件14\n- 申请截止日期为：: \n21. 02. 2014\n- 过期:\n21. 08. 2015"]
[null,{"$f":"IF($B$1=\"English\",C521,IF($B$1=\"Deutsch\",D521,IF($B$1=\"中文\",E521,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in annex 14 and annex 17\n- Latest application date: \n21 August 2013\n- Sunset date:\n21 February 2015"},"included in annex 14 and annex 17\n- Latest application date: \n21 August 2013\n- Sunset date:\n21 February 2015","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss:\n21. August 2013\n- Ablauftermin:\n21. Februar 2015\n","包含在附件14和附件17\n- 申请截止日期为：: \n21. 08. 2013\n- 过期:\n21. 02. 2015"]
[null,{"$f":"IF($B$1=\"English\",C522,IF($B$1=\"Deutsch\",D522,IF($B$1=\"中文\",E522,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in annex 14\n- Latest application date: \n21 August 2013\n- Sunset date\n21 February 2015"},"included in annex 14\n- Latest application date: \n21 August 2013\n- Sunset date\n21 February 2015","aufgenommen in Anhang 14\n- Antragsschluss: \n21. August 2013\n- Ablauftermin:\n21. Februar 2015","包含在附件14\n- 申请截止日期为：: \n21. 08. 2013\n- 过期:\n21. 02. 2015"]
[null,{"$f":"IF($B$1=\"English\",C523,IF($B$1=\"Deutsch\",D523,IF($B$1=\"中文\",E523,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in annex 14\n- Latest application date:\n21 November 2013\n- Sunset date:\n21 May 2015"},"included in annex 14\n- Latest application date:\n21 November 2013\n- Sunset date:\n21 May 2015","aufgenommen in Anhang 14\n- Antragsschluss:\n21. November 2013\n- Ablauftermin:\n21. Mai 2015","包含在附件14\n- 申请截止日期为：: \n21. 11. 2013\n- 过期:\n21. 05. 2015"]
[null,{"$f":"IF($B$1=\"English\",C524,IF($B$1=\"Deutsch\",D524,IF($B$1=\"中文\",E524,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvents\n- detergents\n- production of electronic devices\n- semiconductor industry\n- petrochemical processing\n- pharmaceuticals\n- agrochemicals\n"},"- solvents\n- detergents\n- production of electronic devices\n- semiconductor industry\n- petrochemical processing\n- pharmaceuticals\n- agrochemicals\n","- Lösungsmittel\n- Reinigungsmittel\n- Herstellung elektronischer Geräte\n- Halbleiterindustrie\n- petrochemische Verarbeitung\n- Arzneimittel\n- Agrochemikalien","- 溶剂\n- 清洗剂\n- 电子制造产品\n- 半导体产业\n- 石油化工加工\n- 药物\n- 农用化学品"]
[null,{"$f":"IF($B$1=\"English\",C525,IF($B$1=\"Deutsch\",D525,IF($B$1=\"中文\",E525,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- plasticizer in PVC and sealants\n- coatings\n- printing color"},"- plasticizer in PVC and sealants\n- coatings\n- printing color","- Weichmacher in PVC und Dichtungsmitteln\n- Beschichtungen\n- Druckfarben","- 在PVC中的增塑剂和密封剂\n- 涂层\n- 印刷油墨"]
[null,{"$f":"IF($B$1=\"English\",C526,IF($B$1=\"Deutsch\",D526,IF($B$1=\"中文\",E526,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- plasticizer in PVC\n- foam material\n- adhesives\n- coatings"},"- plasticizer in PVC\n- foam material\n- adhesives\n- coatings","- Weichmacher in PVC\n- Schaumstoff\n- Klebstoffen\n- Beschichtungen","- 在PVC中的增塑剂\n- 泡沫材料\n- 粘合剂\n- 涂层"]
[null,{"$f":"IF($B$1=\"English\",C527,IF($B$1=\"Deutsch\",D527,IF($B$1=\"中文\",E527,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of further substances (e.g. vinyl chloride)\n- solvents"},"- production of further substances (e.g. vinyl chloride)\n- solvents","- Herstellung weiterer Stoffe (z. B. Vinylchlorid)\n- Lösungsmittel","- 制造其他物质 (例如： 氯乙烯)\n- 溶剂"]
[null,{"$f":"IF($B$1=\"English\",C528,IF($B$1=\"Deutsch\",D528,IF($B$1=\"中文\",E528,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- intermediate product at production of chlorinated solvents and agricultural products\n- monomer\n- solvents\n- paint- and varnish remover\n- degreasing agent"},"- intermediate product at production of chlorinated solvents and agricultural products\n- monomer\n- solvents\n- paint- and varnish remover\n- degreasing agent","- Zwischenprodukt bei der Herstellung von chlorierten Lösungsmitteln und Agrarprodukten\n- Monomer \n- Lösungsmittel\n- Farb- und Lackentferner\n- Entfettungsmittel","- 在生产氯化溶剂和农业产品过程中的过渡产品\n- 单体\n- 溶剂\n- 颜料和漆去除剂\n- 除油剂"]
[null,{"$f":"IF($B$1=\"English\",C529,IF($B$1=\"Deutsch\",D529,IF($B$1=\"中文\",E529,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvents\n- intermediate product at production of cyanoacrylate adhesives"},"- solvents\n- intermediate product at production of cyanoacrylate adhesives","- Lösungsmittel\n- Zwischenprodukt bei der Herstellung von Cyanoacrylat-Klebstoffen.","- 溶剂\n-在生产氰基丙烯酸酯粘合剂过程中的过渡产品。"]
[null,{"$f":"IF($B$1=\"English\",C530,IF($B$1=\"Deutsch\",D530,IF($B$1=\"中文\",E530,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of toluendiisocyanat \n- production of flexible polyurethane foams\n- plasticizer for the production of explosive mixtures (e.g. airbags in cars)"},"- production of toluendiisocyanat \n- production of flexible polyurethane foams\n- plasticizer for the production of explosive mixtures (e.g. airbags in cars)","- Produktion von Toluendiisocyanat \n- Herstellung von flexiblen Polyurethanschäumen \n- Gelier-Plastifizierungsmittel für die Herstellung von Sprengstoffgemischen (z. B. Airbags in Autos)","- 生产甲苯二异氰酸酯\n- 生产软聚氨酯泡沫塑料\n- 胶凝增塑剂为了生产爆炸性配制品 (例如: 汽车的安全气囊)"]
[null,{"$f":"IF($B$1=\"English\",C531,IF($B$1=\"Deutsch\",D531,IF($B$1=\"中文\",E531,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- chemical intermediate product\n- solvents\n- laboratory chemicals"},"- chemical intermediate product\n- solvents\n- laboratory chemicals","- chemisches Zwischenprodukt\n- Lösungsmittel\n- Laborchemikalie","- 化学的过渡产品\n- 溶剂\n- 化学实验室"]
[null,{"$f":"IF($B$1=\"English\",C532,IF($B$1=\"Deutsch\",D532,IF($B$1=\"中文\",E532,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":". Production of azo dyes and pharmaceuticals"},". Production of azo dyes and pharmaceuticals","- Herstellung von Azofarbstoffen und Pharmazeutika","-偶氮染料和药品的生产"]
[null,{"$f":"IF($B$1=\"English\",C533,IF($B$1=\"Deutsch\",D533,IF($B$1=\"中文\",E533,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of polymer mixtures, phenolic resins and ethoxylate detergents\n- adhesives\n- coatings\n- inks\n- rubber products\n"},"- production of polymer mixtures, phenolic resins and ethoxylate detergents\n- adhesives\n- coatings\n- inks\n- rubber products\n","- Herstellung von Polymer-Gemischen, Phenolische Harze und Ethoxylat-Tensiden\n- Klebstoffe\n- Beschichtungen\n- Tinten\n- Gummierzeugnissen.","- 聚合物的配制品，酚醛树脂，和乙氧基化物表面活\n性剂的生产\n- 粘合剂\n- 涂层\n- 墨水\n- 橡胶产品"]
[null,{"$f":"IF($B$1=\"English\",C534,IF($B$1=\"Deutsch\",D534,IF($B$1=\"中文\",E534,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- synthesis of polyacrylamides\n- waste water treatment and paper processing\n- polyacrylamides\n- cement"},"- synthesis of polyacrylamides\n- waste water treatment and paper processing\n- polyacrylamides\n- cement","- Synthese von Polyacrylamiden\n- Abwasserbehandlung und Papierverarbeitung \n- Polyacrylamiden\n- Zementierstoff","- 合成聚丙烯酰胺\n- 废水处理和纸张加工\n- 聚丙烯酰胺\n- 水泥物质\n"]
[null,{"$f":"IF($B$1=\"English\",C535,IF($B$1=\"Deutsch\",D535,IF($B$1=\"中文\",E535,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- high temperature insulation\n- fire prevention"},"- high temperature insulation\n- fire prevention","- Hochtemperaturisolierung \n- Brandschutz","- 高温绝缘\n- 防火"]
[null,{"$f":"IF($B$1=\"English\",C536,IF($B$1=\"Deutsch\",D536,IF($B$1=\"中文\",E536,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- oxidant\n- photosensitive screens\n- corrosive\n- metal treatment\n- laboratory analytical agent"},"- oxidant\n- photosensitive screens\n- corrosive\n- metal treatment\n- laboratory analytical agent","- Oxidationsmittel \n- lichtempfindliche Bildschirme\n- Beizmittel \n- Metallbehandlung \n- laboranalytisches Agens","- 氧化剂\n- 光感屏\n- 媒介\n- 金属处理 \n- 实验室分析试剂"]
[null,{"$f":"IF($B$1=\"English\",C537,IF($B$1=\"Deutsch\",D537,IF($B$1=\"中文\",E537,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of other substances such as anthracene and carbon-black\n- reductant in furnaces\n- components in bunker oil\n- impregnation\n- sealing\n- anticorrosive\n"},"- production of other substances such as anthracene and carbon-black\n- reductant in furnaces\n- components in bunker oil\n- impregnation\n- sealing\n- anticorrosive\n","- Herstellung von anderen Stoffen wie z.B. Anthracen und Ruß\n- Reduktionsmittel in Hochöfen\n- Komponenten in Bunkeröl\n- Imprägnierung\n- Abdichtung\n- Korrosionsschutz","- 制造其他物质 （例如：蒽和炭黑）\n- 还原剂在高炉\n- 燃油成分\n- 注入\n- 密封\n- 防腐蚀保护"]
[null,{"$f":"IF($B$1=\"English\",C538,IF($B$1=\"Deutsch\",D538,IF($B$1=\"中文\",E538,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- clarifying agent\n- production of laminated curcuit boards\n- production of semiconductors\n- laboratory chemicals"},"- clarifying agent\n- production of laminated curcuit boards\n- production of semiconductors\n- laboratory chemicals","- Klärmittel\n- Herstellung von laminierten Leiterplatten\n- Herstellung von Halbleitern\n- Laborchemikalie","- 澄清剂\n- 制造层压印刷电路板\n- 半导体制造\n- 化学实验室"]
[null,{"$f":"IF($B$1=\"English\",C539,IF($B$1=\"Deutsch\",D539,IF($B$1=\"中文\",E539,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvents\n- distillation agent\n- diesel fuels"},"- solvents\n- distillation agent\n- diesel fuels","- Lösemittel\n- Azeotropdestillationsmittel oder Schleppmittel\n- Dieselkraftstoffe","- 溶剂\n- 共沸或类共沸剂\n- 柴油燃料"]
[null,{"$f":"IF($B$1=\"English\",C540,IF($B$1=\"Deutsch\",D540,IF($B$1=\"中文\",E540,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- complex raw materials which are mainly used for copper and lead refining\n- seperate nickel from melted metal\n- production of diarsenic trioxide"},"- complex raw materials which are mainly used for copper and lead refining\n- seperate nickel from melted metal\n- production of diarsenic trioxide","- komplexe Rohstoffe, die hauptsächlich für die Kupfer- und Bleiraffination Verwendung finden\n- Nickel aus geschmolzenem Metall abscheiden\n- Diarsentrioxid herstellen","- 复杂的原料，主要用于铜和铅精炼\n-  镍从被融化的金属分离\n- 生产三氧化二砷"]
[null,{"$f":"IF($B$1=\"English\",C541,IF($B$1=\"Deutsch\",D541,IF($B$1=\"中文\",E541,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of pigments and dyes\n- pigmentation- and coating substances\n- embalming/recovery of artworks\n- detergents and bleach\n- photo-sensitive materials\n- production of pyrotechnic powder"},"- production of pigments and dyes\n- pigmentation- and coating substances\n- embalming/recovery of artworks\n- detergents and bleach\n- photo-sensitive materials\n- production of pyrotechnic powder","- Herstellung von Pigmenten und Farbstoffen \n- Pigmentier- oder Beschichtungsstoff \n- Einbalsamierung/Wiederherstellung von Kunstprodukten\n- Reinigungs- und Bleichmittel\n- lichtempfindliche Materialien\n- Herstellung von pyrotechnischem Pulver","- 生产颜料和染料\n-  着色或涂层材料\n-  防腐/恢复器物\n-  清洗和漂白剂\n-  感光材料\n-  制造火药粉"]
[null,{"$f":"IF($B$1=\"English\",C542,IF($B$1=\"Deutsch\",D542,IF($B$1=\"中文\",E542,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- dye-, paint- and coating substance\n- production of agricultural devices, vehicles and airplanes\n- marking of streets and runways\n"},"- dye-, paint- and coating substance\n- production of agricultural devices, vehicles and airplanes\n- marking of streets and runways\n","- Färbe-, Anstrich- und Beschichtungsstoff \n- Produktion von landwirtschaftlichen Geräten, Fahrzeugen und Flugzeugen\n- Anstreichen von Straßen und Start- und Landestreifen.","- 印染，油漆和涂料\n- 生产农用设备，车和飞机\n- 勾画出道路和飞机起飞和着陆带。"]
[null,{"$f":"IF($B$1=\"English\",C543,IF($B$1=\"Deutsch\",D543,IF($B$1=\"中文\",E543,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- exploder or booster in detonators\n- exploder in pyrotechnical appliances\n"},"- exploder or booster in detonators\n- exploder in pyrotechnical appliances\n","- Zünder oder Verstärker in Detonatoren \n- Zünder in pyrotechnischen Vorrichtungen","- 点火器或增压器在雷管\n- 点火器在打火装置"]
[null,{"$f":"IF($B$1=\"English\",C544,IF($B$1=\"Deutsch\",D544,IF($B$1=\"中文\",E544,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- explosive\n- detonator mixtures"},"- explosive\n- detonator mixtures","- Explosivstoff\n- Detonator-Gemische","- 易爆物\n- 雷管-配制品"]
[null,{"$f":"IF($B$1=\"English\",C545,IF($B$1=\"Deutsch\",D545,IF($B$1=\"中文\",E545,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- initiating explosive for small calibre and rifle ammunition\n- ammunition pyrotechnics, munition operated appliances\n- explosive-actuated tool\n- detonators for civil usage\n"},"- initiating explosive for small calibre and rifle ammunition\n- ammunition pyrotechnics, munition operated appliances\n- explosive-actuated tool\n- detonators for civil usage\n","- Initialsprengstoff für Kleinkaliber- und Gewehrmunition\n- Munitionspyrotechnik, munitionsbetriebenen Vorrichtungen\n- Bolzensetzgeräte\n- Detonatoren für zivile Verwendungen","- 火药剂为小口径枪和弹药\n- 火药制造术弹药，弹药驱动设备\n- 火药工具\n- 雷管为民用"]
[null,{"$f":"IF($B$1=\"English\",C546,IF($B$1=\"Deutsch\",D546,IF($B$1=\"中文\",E546,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- washing agents and detergents\n- adhesives\n- toys\n- industrial liquids, brake fluids\n- glass, ceramics\n- flame retardants\n- colors\n- disinfectants\n- cosmetics\n- food additives\n- fertiliser, insecticide\n- other products"},"- washing agents and detergents\n- adhesives\n- toys\n- industrial liquids, brake fluids\n- glass, ceramics\n- flame retardants\n- colors\n- disinfectants\n- cosmetics\n- food additives\n- fertiliser, insecticide\n- other products","- Wasch- und Reinigungsmittel\n- Klebstoffe\n- Spielsachen\n- Industrieflüssigkeiten, Bremsflüssigkeiten\n- Glas, Keramik\n- Flammschutzmitteln\n- Farben\n- Desinfektionsmittel\n- Kosmetika\n- Lebensmittelzusatzstoffe\n- Düngemitteln, Insektizide\n- anderen Produkte","- 洗涤和清洗剂\n- 黏合剂\n- 玩具\n- 工业油，刹车油\n- 玻璃，陶瓷\n- 阻燃剂\n- 颜料\n- 消毒剂\n- 化妆品\n- 食品添加剂\n- 化肥，杀虫剂\n- 其他产品"]
[null,{"$f":"IF($B$1=\"English\",C547,IF($B$1=\"Deutsch\",D547,IF($B$1=\"中文\",E547,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- metal refinement such as galvanoplasty (e.g. hard chromium plating and decoration coating)\n- conversion layers\n- brightener\n-  fixative in wood preservatives\n- production of pigments and color/varnish\n- production of catalysts\n- detergents\n- oxidant\n\n"},"- metal refinement such as galvanoplasty (e.g. hard chromium plating and decoration coating)\n- conversion layers\n- brightener\n-  fixative in wood preservatives\n- production of pigments and color/varnish\n- production of catalysts\n- detergents\n- oxidant\n\n","- Metallveredelung wie Galvanoplastik (z. B. Hartverchromen und Dekorationsbeschichtung)\n- Konversionsschichten\n- Aufheller\n- Fixiermittel in Holzkonservierungsmitteln\n- Herstellung von Pigmenten und Farben/Lacken\n- Herstellung von Katalysatoren\n- Reinigungsmittel\n- Oxidationsmittel","- 金属加工例如电镀 (例如 镀硬铬，装饰涂料)\n- 转换层\n- 增白剂\n- 固定液在木材防腐剂\n- 制造颜料和油漆/清漆\n- 制造催化剂\n- 洗涤剂\n- 氧化剂"]
[null,{"$f":"IF($B$1=\"English\",C548,IF($B$1=\"Deutsch\",D548,IF($B$1=\"中文\",E548,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of catalysts\n- feed additive\n- production of other chemicals\n- production of pigments\n- adhesive in priming frits"},"- production of catalysts\n- feed additive\n- production of other chemicals\n- production of pigments\n- adhesive in priming frits","- Herstellung von Katalysatoren\n- Futterzusatz\n- Herstellung von anderen Chemikalien\n- Herstellung von  Pigmenten\n- Klebstoff in Grundierungsfritten","- 制造催化剂\n- 饲料添加剂\n- 生产其他化学品\n- 生产颜料\n- 底漆中的粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C549,IF($B$1=\"Deutsch\",D549,IF($B$1=\"中文\",E549,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of catalysts\n- as a catalyst\n- production of other chemicals\n- production of pigments\n- surface treatment\n- in alloys, dyes, adhesion promotor\n- feed additive\n"},"- production of catalysts\n- as a catalyst\n- production of other chemicals\n- production of pigments\n- surface treatment\n- in alloys, dyes, adhesion promotor\n- feed additive\n","- Herstellung von Katalysatoren\n- als Katalysator \n- Herstellung von anderen Chemikalien\n- Herstellung von Pigmenten\n- Oberflächenbehandlungen\n- in Legierungen, Farbstoffen, Gummihaftvermittlern\n- Futterzusatz","- 制造催化剂\n- 作为催化剂\n- 生产其他化学品\n- 生产颜料\n- 表面处理\n- 在合金中，染料，橡胶粘合促进剂\n- 饲料添加剂"]
[null,{"$f":"IF($B$1=\"English\",C550,IF($B$1=\"Deutsch\",D550,IF($B$1=\"中文\",E550,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of other chemicals\n- production of catalysts\n- surface treatment\n- batteries\n"},"- production of other chemicals\n- production of catalysts\n- surface treatment\n- batteries\n","- Herstellung von anderen Chemikalien\n- Herstellung von Katalysatoren\n- Oberflächenbehandlung\n- Batterien","- 生产其他化学品\n- 制造催化剂\n- 表面处理\n- 电池"]
[null,{"$f":"IF($B$1=\"English\",C551,IF($B$1=\"Deutsch\",D551,IF($B$1=\"中文\",E551,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of other chemicals and pigments\n- catalysts\n- drying agent\n- surface treatment\n- anticorrosive\n- decolour (of glass and ceramics)\n- batteries\n- feed additives\n- soil fertilizer"},"- production of other chemicals and pigments\n- catalysts\n- drying agent\n- surface treatment\n- anticorrosive\n- decolour (of glass and ceramics)\n- batteries\n- feed additives\n- soil fertilizer","- Herstellung von anderen Chemikalien und Pigmenten\n- Katalysatoren\n- Trockenmittel\n- Oberflächenbehandlungen (z. B. Galvanoplastik)\n- Korrosionsschutz\n- Entfärben (von Glas- und Keramikwaren)\n- Batterien\n- Tierfutterzusätze\n- Bodendüngemittel","- 生产其他化学品和颜料\n- 催化剂\n- 干燥剂\n- 表面处理\n- 防腐蚀保护\n- 脱色 (来自玻璃和陶瓷)\n- 电池\n- 动物饲料添加剂\n- 土壤肥料"]
[null,{"$f":"IF($B$1=\"English\",C552,IF($B$1=\"Deutsch\",D552,IF($B$1=\"中文\",E552,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- plasticizer for cellulose nitrate, cellulose ether, polyacrylate\n- gelling aid in combination with other plasticizers\n- plastics\n- varnishes\n- adhesives\n- explosives\n- nailpolish"},"- plasticizer for cellulose nitrate, cellulose ether, polyacrylate\n- gelling aid in combination with other plasticizers\n- plastics\n- varnishes\n- adhesives\n- explosives\n- nailpolish","- Weichmacher für Cellulosenitrat, Celluloseether, Polyacrylat und Polyacetatdispersionen\n- Gelierhilfe in der Kombination mit anderen Weichmachern\n- Kunststoffe\n- Lacke\n- Kleber\n- Explosivstoffe\n- Nagelpoliermittel","- 软化剂 对于 硝酸纤维素,  乙基-2-羟基乙基纤维素 , 聚丙烯酸酯 和聚醋酸乙烯酯乳液\n- 胶凝在与其他软化剂结合时\n- 塑料\n- 涂料\n- 粘合\n- 易爆物\n- 指甲油"]
[null,{"$f":"IF($B$1=\"English\",C553,IF($B$1=\"Deutsch\",D553,IF($B$1=\"中文\",E553,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- in washing agents and detergents\n- in glass and glassfibres\n- ceramics\n- industrial liquids\n- metalurgy\n- adhesives\n- flame retardants\n- body care products\n- biocides\n- fertiliser"},"- in washing agents and detergents\n- in glass and glassfibres\n- ceramics\n- industrial liquids\n- metalurgy\n- adhesives\n- flame retardants\n- body care products\n- biocides\n- fertiliser","- in Wasch- und Reinigungsmitteln\n- in Glas und Glasfasern\n- Keramik\n- Industrieflüssigkeiten\n- Metallurgie\n- Klebstoffe\n- Flammschutzmittel\n- Körperpflegeprodukte\n- Biozide\n- Düngemittel","- 在洗涤和清洗剂\n- 在玻璃和玻璃纤维\n- 陶瓷\n- 工业流体\n- 冶金\n- 黏合剂\n- 阻燃剂\n- 个人护理产品\n- 杀菌剂\n- 肥料"]
[null,{"$f":"IF($B$1=\"English\",C554,IF($B$1=\"Deutsch\",D554,IF($B$1=\"中文\",E554,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of other substances\n- ion exchange resins in atomic plants\n- as a hardener for epoxy resins, e.g. for the production of rolls, pipes and forms as well as adhesives"},"- production of other substances\n- ion exchange resins in atomic plants\n- as a hardener for epoxy resins, e.g. for the production of rolls, pipes and forms as well as adhesives","- Herstellung von anderen Stoffen\n- Ionenaustauschharze in Kernkraftwerken\n- als Härter für Epoxidharze, z. B. für die Herstellung von Rollen, Rohren und Formen sowie Klebstoffe","- 生产其他物质\n- 离子交换树脂在核电厂\n- 作为环氧树脂的硬化剂, 例如用于卷筒，管材和形状，\n以及黏合剂的制造"]
[null,{"$f":"IF($B$1=\"English\",C555,IF($B$1=\"Deutsch\",D555,IF($B$1=\"中文\",E555,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- intermediate product at the production of hydrazine derivate\n- as monomer in polymerisations\n- as a corrosion inhibitor during water treatment\n- metal reduction\n- refinement of chemicals\n- fuel for space ships and for military (emergency) power aggregate\n"},"- intermediate product at the production of hydrazine derivate\n- as monomer in polymerisations\n- as a corrosion inhibitor during water treatment\n- metal reduction\n- refinement of chemicals\n- fuel for space ships and for military (emergency) power aggregate\n","- Zwischenprodukt bei der Herstellung von Hydrazinderivaten\n- als Monomer in Polymerisationen\n- als Korrosionsinhibitor bei der Wasseraufbereitung\n- Metallreduktion\n- Veredelung von Chemikalien\n- Treibstoff für Raumfahrzeuge und als Brennstoff für militärische (Not-) Energieaggregate","- 在生产肼衍生物时的过渡产品\n- 作为单体在聚合时\n- 作为缓蚀剂在水处理时\n- 金属还原\n- 化学精炼\n-燃料用于航天飞机和作为燃料用于军事（应急）电\n源装置"]
[null,{"$f":"IF($B$1=\"English\",C556,IF($B$1=\"Deutsch\",D556,IF($B$1=\"中文\",E556,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- coatings in automotive industry and aerospace industry"},"- coatings in automotive industry and aerospace industry","- Beschichtungen im Fahrzeugwesen und in der Luft- und Raumfahrtindustrie","- 涂料在汽车工业和在航空和航天工业"]
[null,{"$f":"IF($B$1=\"English\",C557,IF($B$1=\"Deutsch\",D557,IF($B$1=\"中文\",E557,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- for laboratory purposes (acid-base indicator)\n- in pharmaceutic mixtures\n- in some special applications (e.g. acid-base indicator slip, invisible inks)"},"- for laboratory purposes (acid-base indicator)\n- in pharmaceutic mixtures\n- in some special applications (e.g. acid-base indicator slip, invisible inks)","- für Laborzwecke (pH-Indikatorlösungen)\n- in pharmazeutischen Zubereitungen\n- in einigen Spezialapplikationen (z. B. pH-Indikatorpapier, unsichtbare Tinten)","- 用于试验目的 (pH-指示剂)\n- 在药物制剂中\n- 在一些特殊的应用 (例如： pH-试纸, 隐形墨水)"]
[null,{"$f":"IF($B$1=\"English\",C558,IF($B$1=\"Deutsch\",D558,IF($B$1=\"中文\",E558,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- corrosion inhibitor for treatment and coating of metals\n- production of reagents, chemicals and textiles\n- dye for ceramics, glass and cement production\n- production of pigments/inks\n- analytical agent in laboratories"},"- corrosion inhibitor for treatment and coating of metals\n- production of reagents, chemicals and textiles\n- dye for ceramics, glass and cement production\n- production of pigments/inks\n- analytical agent in laboratories","- Korrosionshemmer bei der Behandlung und Beschichtung von Metallen\n- Herstellung von Reagenzien, Chemikalien und Textilien\n- als Farbstoff bei der Keramik-, Glas- und Zementherstellung\n- Herstellung von Pigmenten/Tinten\n- im Labor als analytisches Agens","- 缓蚀剂在金属的处理和涂层\n- 试剂，化学品和纺织品的生产\n- 作为陶瓷，玻璃及水泥生产的染料\n- 颜料/墨水的生产\n- 在实验室中，作为分析试剂"]
[null,{"$f":"IF($B$1=\"English\",C559,IF($B$1=\"Deutsch\",D559,IF($B$1=\"中文\",E559,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of chrome metal\n- corrosion inhibitor for treatment and coating of metals\n- corrosive for textiles\n- analytical agent in laboratories\n- cleaning of laboratory glasswares\n- production of other reagents\n- oxidant for fotolitography"},"- production of chrome metal\n- corrosion inhibitor for treatment and coating of metals\n- corrosive for textiles\n- analytical agent in laboratories\n- cleaning of laboratory glasswares\n- production of other reagents\n- oxidant for fotolitography","- Chrommetallherstellung\n- Korrosionshemmer bei der Behandlung und Beschichtung von Metallen\n- als Textilbeizmittel\n- als analytisches Agens im Labor\n- Reinigung von Laborglasgeräten\n- Herstellung anderer Reagenzien\n- als Oxidationsmittel in der Fotolithografie","- 铬金属生产\n- 在金属的处理和涂层中做缓蚀剂\n- 纺织品媒染剂\n- 作为实验室分析试剂\n- 实验室玻璃器皿的清洗\n- 制造其他试剂\n- 影印技术中作为氧化剂"]
[null,{"$f":"IF($B$1=\"English\",C560,IF($B$1=\"Deutsch\",D560,IF($B$1=\"中文\",E560,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- coatings for aerospace industry\n- coatings of steel and aluminium straps und automotive coatings"},"- coatings for aerospace industry\n- coatings of steel and aluminium straps und automotive coatings","- in Beschichtungen in der Luft- und Raumfahrtindustrie\n- Beschichtung von Stahl- und Aluminiumbändern und Fahrzeugbeschichtung","- 航空和航天工业用涂料\n- 钢铁和铝线圈和车辆涂装的涂料"]
[null,{"$f":"IF($B$1=\"English\",C561,IF($B$1=\"Deutsch\",D561,IF($B$1=\"中文\",E561,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of chrome metal\n- production of chlorate\n- coating of metals\n- analytical agent in laboratories\n- tanning of leather\n- in colors"},"- production of chrome metal\n- production of chlorate\n- coating of metals\n- analytical agent in laboratories\n- tanning of leather\n- in colors","- Chrommetallherstellung\n- Herstellung von Chloraten\n- Beschichtung von Metallen\n- als analytisches Agens im Labor\n- Gerben von Leder\n- in Farben","- 铬金属生产\n- 氯酸盐生产\n- 金属涂料\n- 作为实验室分析试剂\n- 皮革鞣制\n- 用于颜色中"]
[null,{"$f":"IF($B$1=\"English\",C562,IF($B$1=\"Deutsch\",D562,IF($B$1=\"中文\",E562,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvent\n- production of several substances\n- production of fibres for clothes and other applications\n- reagent\n- in products such as industral color/varnish, insulation paper, polyimide films, paint removers and ink removers"},"- solvent\n- production of several substances\n- production of fibres for clothes and other applications\n- reagent\n- in products such as industral color/varnish, insulation paper, polyimide films, paint removers and ink removers","- als Lösungsmittel\n- Herstellung verschiedener Stoffe\n- Herstellung von Fasern für Kleidung und bei anderen Applikationen\n- Reagens\n- in Produkten wie Industrielacken und -farben, Isolierpapier, Polyimidfolien, Abbeizmitteln und Tintenentfernern","- 作为溶剂\n- 用于一些物质的生产\n- 用于服装纤维的生产和其它应用\n- 试剂\n-在一些产品中含有，如工业涂料和油漆，绝缘纸，聚\n酰亚胺薄膜，脱漆剂和除墨水"]
[null,{"$f":"IF($B$1=\"English\",C563,IF($B$1=\"Deutsch\",D563,IF($B$1=\"中文\",E563,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of electrodes for industrial applications\n- high performance corrosion inhibitor"},"- production of electrodes for industrial applications\n- high performance corrosion inhibitor","- Produktion von Elektroden für industrielle Anwendungen \n- Hochleistungskorrosionsschutz","- 生产工业应用的电极\n- 高性能的防腐蚀保护"]
[null,{"$f":"IF($B$1=\"English\",C564,IF($B$1=\"Deutsch\",D564,IF($B$1=\"中文\",E564,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- corrosion inhibitor in coating mixtures"},"- corrosion inhibitor in coating mixtures","- als Korrosionsinhibitor in Beschichtungsmischungen","- 作为缓蚀剂在涂层配制品"]
[null,{"$f":"IF($B$1=\"English\",C565,IF($B$1=\"Deutsch\",D565,IF($B$1=\"中文\",E565,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- washing agents and detergents\n- in glass and glassfibres\n- ceramics\n- industrial liquids\n- metalurgy\n- adhesives\n- flame retardant\n- body care products\n- biocide, fertilizer\n"},"- washing agents and detergents\n- in glass and glassfibres\n- ceramics\n- industrial liquids\n- metalurgy\n- adhesives\n- flame retardant\n- body care products\n- biocide, fertilizer\n","- in Wasch- und Reinigungsmitteln\n- in Glas und Glasfasern\n- Keramik\n- Industrieflüssigkeiten\n- Metallurgie\n- Klebstoffen\n- Flammschutzmitteln\n- Körperpflegeprodukten\n- Biozide, Düngemittel","- 洗涤剂和清洗剂\n- 玻璃和玻璃纤维\n- 陶瓷\n- 工业流体\n- 冶金\n- 胶粘剂\n- 阻燃剂\n- 个人护理产品\n- 杀菌剂，肥料"]
[null,{"$f":"IF($B$1=\"English\",C566,IF($B$1=\"Deutsch\",D566,IF($B$1=\"中文\",E566,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- production of organic chlorine compounds and fluorine compounds\n- cleaning and degreasing of metalparts\n- solvent in adhesives"},"- production of organic chlorine compounds and fluorine compounds\n- cleaning and degreasing of metalparts\n- solvent in adhesives","- Herstellung organischer Chlor- und Fluor-Verbindungen\n- zum Reinigen und Entfetten von Metallteilen\n- als Lösungsmittel in Klebstoffen","- 生产有机氯和氟化合物\n- 清洗和金属部件的脱脂\n- 作为粘合剂的溶剂"]
[null,{"$f":"IF($B$1=\"English\",C567,IF($B$1=\"Deutsch\",D567,IF($B$1=\"中文\",E567,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- complex raw materials for the production of copper, lead and a number of noble metals\n- gets transformed to calcium arsenate and diarsenic trioxide in metallurgic refinement process"},"- complex raw materials for the production of copper, lead and a number of noble metals\n- gets transformed to calcium arsenate and diarsenic trioxide in metallurgic refinement process","- in komplexen Rohstoffen für die Herstellung von Kupfer, Blei und einer Reihe von Edelmetallen\n- wird im metallurgischen Veredelungsprozess in Calciumarsenat und Diarsentrioxid umgewandelt","- 用于生产铜，铅，和一系列的贵金属的复杂的原料中\n- 被转换成砷酸钙和三氧化二砷在冶金细化过程"]
[null,{"$f":"IF($B$1=\"English\",C568,IF($B$1=\"Deutsch\",D568,IF($B$1=\"中文\",E568,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- high temperature insulation\n- fire protection"},"- high temperature insulation\n- fire protection","- Hochtemperaturisolierung\n- Feuerschutz","- 高温绝缘\n- 防火"]
[null,{"$f":"IF($B$1=\"English\",C569,IF($B$1=\"Deutsch\",D569,IF($B$1=\"中文\",E569,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- additive for baking enamels\n- component of dye solvents for printing paste, endorsing and leather dyes\n- solvent for greases, oils and waxes\n- solvent for ball pen pastes"},"- additive for baking enamels\n- component of dye solvents for printing paste, endorsing and leather dyes\n- solvent for greases, oils and waxes\n- solvent for ball pen pastes","- Zusatz zu Einbrennlacken\n- Bestandteil von Farbstoff-Lösemittel für Druckpasten Stempelfarben und Lederfarbstoffe\n- Lösemittel für Fette, Öle und Wachse\n- Lösemittel in Kugelschreiberpasten","- 添置烤漆\n-染料溶剂印花色浆的组成部分用于邮票的颜色和皮革染料\n- 作为脂肪，油和蜡的溶剂\n- 圆珠笔油墨的溶剂"]
[null,{"$f":"IF($B$1=\"English\",C570,IF($B$1=\"Deutsch\",D570,IF($B$1=\"中文\",E570,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- flocking agent for water treatment\n- paper processing\n- plastics\n- cement"},"- flocking agent for water treatment\n- paper processing\n- plastics\n- cement","- Flockungsmittel zur Wasseraufbereitung\n- Papierverarbeitung\n- Kunststoffe\n- Zementierstoff","- 絮凝剂用于水处理\n- 纸张加工\n- 塑料\n- 水泥物质"]
[null,{"$f":"IF($B$1=\"English\",C571,IF($B$1=\"Deutsch\",D571,IF($B$1=\"中文\",E571,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- plasticizer\n- binding agent\n- flame retardant\n- plastics, varnishes, rubber, paper\n- joint compo and seal compo"},"- plasticizer\n- binding agent\n- flame retardant\n- plastics, varnishes, rubber, paper\n- joint compo and seal compo","- Weichmacher\n- Bindemittel\n- Flammschutzmittel\n- Kunstoffen, Lacken, Gummi, Papier\n- Fugen- und Dichtungsmassen","- 塑化剂\n- 粘合剂\n- 阻燃剂\n- 塑料，涂料，橡胶，造纸\n- 接头和密封剂"]
[null,{"$f":"IF($B$1=\"English\",C572,IF($B$1=\"Deutsch\",D572,IF($B$1=\"中文\",E572,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvent for polar and unpolar substances\n-  extracting agent (e.g. pharma industry, extraction of greases, decaffeination of coffee etc.)\n- paint remover\n- energy transfer medium\n- aerosols (e.g. hairspray)\n- degreasing of metal surfaces\n- movie and electronic industry"},"- solvent for polar and unpolar substances\n-  extracting agent (e.g. pharma industry, extraction of greases, decaffeination of coffee etc.)\n- paint remover\n- energy transfer medium\n- aerosols (e.g. hairspray)\n- degreasing of metal surfaces\n- movie and electronic industry","- Lösemittel für polare und unpolare Subtanzen\n- Extraktionsmittel (z.B. in der Pharmaindustrie, zur Gewinnung von Fetten, zur Entcoffeinierung von Kaffee etc.)\n- Farbentferner\n- Kälteübertragungsmittel in Kühlanlagen\n- Aerosolen (z.B. Haarsprays)\n- Entfettung von Metalloberflächen\n- der Film- und Elektronikindustrie","- 溶剂用于极性和非极性物质\n-萃取剂（例如，在制药工业中，用于生产脂肪，用于咖啡的脱咖啡因等）\n- 脱漆剂\n- 在冷却系统中冷转移\n- 气雾剂（如发胶）\n- 金属表面除油\n- 胶片和电子行业"]
[null,{"$f":"IF($B$1=\"English\",C573,IF($B$1=\"Deutsch\",D573,IF($B$1=\"中文\",E573,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in toys or parts of toys where the concentration of benzene in the free state is greater than 5 mg/kg (0,0005 %) of the weight of the toy or part of toy.\n\n2. Toys and parts of toys not complying with paragraph 1 shall not be placed on the market.\n\n3. Shall not be placed on the market, or used,\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations equal to, or greater than 0,1 % by weight.\n\n4. However, paragraph 3 shall not apply to:\n(a) motor fuels which are covered by Directive 98/70/EC;\n(b) substances and mixtures for use in industrial processes not allowing for the emission of benzene in quantities in excess of those laid down in existing legislation."},"1. Shall not be used in toys or parts of toys where the concentration of benzene in the free state is greater than 5 mg/kg (0,0005 %) of the weight of the toy or part of toy.\n\n2. Toys and parts of toys not complying with paragraph 1 shall not be placed on the market.\n\n3. Shall not be placed on the market, or used,\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations equal to, or greater than 0,1 % by weight.\n\n4. However, paragraph 3 shall not apply to:\n(a) motor fuels which are covered by Directive 98/70/EC;\n(b) substances and mixtures for use in industrial processes not allowing for the emission of benzene in quantities in excess of those laid down in existing legislation.","1. Darf nicht verwendet werden in Spielwaren oder Teilen von Spielwaren, wenn die Konzentration an frei verfügbarem Benzol höher als 5 mg/kg (0,0005 %) des Gewichts des Spielzeugs bzw. des Teils eines Spielzeugs ist.\n2. Spielwaren und Teile von Spielwaren, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.\n3. Darf nicht in Verkehr gebracht oder verwendet werden:\n    als Stoff,\n    als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von > 0,1 Gew: %. \n4. Absatz 3 gilt jedoch nicht für:\n    Treibstoffe, die unter die Richtlinie 98/70/EG fallen,\n    Stoffe und Gemische, die bei industriellen Verfahren zur Anwendung kommen, bei denen Benzol nicht in höheren Konzentrationen freigesetzt werden darf, als in bestehenden Rechtsvorschriften festgelegt ist. ","1. 在玩具或者玩具的零部件中, 自由状态下苯酚浓度不得高于5mg/kg (0,0005%)；\n\n2. 不满足第1项的玩具或者玩具零件，不得投放市场。.\n\n3. 物质或者制剂中以质量百分比浓度大于0,1%时，不得投放市场或使用\n\n4. 然而，在以下情况下第3项不适用：\n（a）98/70/EC指令中覆盖的发动机燃料；\n（b）工业工艺中用到的物质和配制品，但苯的释放量不得超过其它现有法规的规定 "]
[null,{"$f":"IF($B$1=\"English\",C574,IF($B$1=\"Deutsch\",D574,IF($B$1=\"中文\",E574,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market or used as a substance or constituent of mixtures in a concentration, equal to or greater than 0,1 % by weight for grouting applications after 5 November 2012."},"Shall not be placed on the market or used as a substance or constituent of mixtures in a concentration, equal to or greater than 0,1 % by weight for grouting applications after 5 November 2012.","Darf nach dem 5. November 2012 weder als Stoff noch in Gemischen in Konzentrationen von > 0,1 Gew.- % für Abdichtungsanwendungen wie beispielsweise Injektion, Verpressung, Verfugung oder Verguss in Verkehr gebracht oder verwendet werden.","当物质或制剂中该成分质量百分比浓度大于等于0.1%，在2012年11月5日之后不得投放市场或者用于注浆"]
[null,{"$f":"IF($B$1=\"English\",C575,IF($B$1=\"Deutsch\",D575,IF($B$1=\"中文\",E575,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint. \n\nHowever, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof. "},"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint. \n\nHowever, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof. ","Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Verwendung als Farben bestimmt sind.\nDie Mitgliedstaaten können jedoch gemäß dem IAO-Übereinkommen Nr. 13 in ihrem Hoheitsgebiet die Verwendung des Stoffs oder Gemischs zur Restaurierung und Unterhaltung von Kunstwerken sowie von historischen Gebäuden und ihren Inneneinrichtungen ebenso genehmigen wie das Inverkehrbringen für eine solche Verwendung. Ein Mitgliedstaat, der diese Ausnahmeregelung in Anspruch nimmt, unterrichtet die Kommission darüber. ","物质或含该物质的制剂不得投放市场，或者作为涂料使用。\n\n但是，成员国可以许可，按照国际劳工组织第13号公约，在其领土内使用物质或含该物质的制剂用于恢复和维护艺术品和历史建筑和室内设计，以及许可其销售作此用途。一个成员国如要行使这项豁免，应通知欧盟委员会。"]
[null,{"$f":"IF($B$1=\"English\",C576,IF($B$1=\"Deutsch\",D576,IF($B$1=\"中文\",E576,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in mixtures and articles produced from synthetic organic polymers (hereafter referred to as plastic material) such as:\n— polymers or copolymers of vinyl chloride (PVC) [3904 10] [3904 21]\n— polyurethane (PUR) [3909 50]\n— low-density polyethylene (LDPE), with the exception of low-density polyethylene used for the production of coloured masterbatch [3901 10]\n— cellulose acetate (CA) [3912 11]\n— cellulose acetate butyrate (CAB) [3912 11]\n— epoxy resins [3907 30]\n— melamine-formaldehyde (MF) resins [3909 20]\n— urea-formaldehyde (UF) resins [3909 10]\n— unsaturated polyesters (UP) [3907 91]\n— polyethylene terephthalate (PET) [3907 60]\n— polybutylene terephthalate (PBT)\n— transparent/general-purpose polystyrene [3903 11]\n— acrylonitrile methylmethacrylate (AMMA)\n— cross-linked polyethylene (VPE)\n— high-impact polystyrene\n— polypropylene (PP) [3902 10]\n— high-density polyethylene (HDPE) [3901 20]\n— acrylonitrile butadiene styrene (ABS) [3903 30]\n— poly(methyl methacrylate) (PMMA) [3906 10].\n\nMixtures and articles produced from plastic material shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight of the plastic material.\n\nBy way of derogation, the second subparagraph shall not apply to articles placed on the market before 10 December 2011. \n\nThe first and second subparagraphs apply without prejudice to Council Directive 94/62/EC (**) and acts adopted on its basis.\n\n2. Shall not be used in paints [3208] [3209].\n\nFor paints with a zinc content exceeding 10 % by weight of the paint, the concentration of cadmium (expressed as Cd metal) shall not be equal to or greater than 0,1 % by weight.\n\nPainted articles shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,1 % by weight of the paint on the painted article.\n\n3. By way of derogation, paragraphs 1 and 2 shall not apply to articles coloured with mixtures containing cadmium for safety reasons.\n\n4. By way of derogation, paragraph 1, second subparagraph shall not apply to:\n— mixtures produced from PVC waste, hereinafter referred to as ‘recovered PVC’,\n— mixtures and articles containing recovered PVC if their concentration of cadmium (expressed as Cd metal) does not exceed 0,1 % by weight of the plastic material in the following rigid PVC applications:\n(a) profiles and rigid sheets for building applications;\n(b) doors, windows, shutters, walls, blinds, fences, and roof gutters;\n(c) decks and terraces;\n(d) cable ducts;\n(e) pipes for non-drinking water if the recovered PVC is used in the middle layer of a multilayer pipe and is entirely covered with a layer of newly produced PVC in compliance with paragraph 1 above.\n\nSuppliers shall ensure, before the placing on the market of mixtures and articles containing recovered PVC for the first time, that these are visibly, legibly and indelibly marked as follows: ‘Contains recovered PVC’ or with the following pictogram:\n\nIn accordance with Article 69 of this Regulation, the derogation granted in paragraph 4 will be reviewed, in particular with a view to reducing the limit value for cadmium and to reassess the derogation for the applications listed in points (a) to (e), by 31 December 2017. \n\n5. For the purpose of this entry, ‘cadmium plating’ means any deposit or coating of metallic cadmium on a metallic surface.\n\nShall not be used for cadmium plating metallic articles or components of the articles used in the following sectors/applications:\n(a) equipment and machinery for: — food production [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] — agriculture [8419 31] [8424 81] [8432] [8433] [8434] [8436] — cooling and freezing [8418] — printing and book-binding [8440] [8442] [8443]\n(b) equipment and machinery for the production of:\n— household goods [7321] [8421 12] [8450] [8509] [8516]\n— furniture [8465] [8466] [9401] [9402] [9403] [9404]\n— sanitary ware [7324]\n— central heating and air conditioning plant [7322] [8403] [8404] [8415]\nIn any case, whatever their use or intended final purpose, the placing on the market of cadmium-plated articles or components of such articles used in the sectors/applications listed in points (a) and (b) above and of articles manufactured in the sectors listed in point (b) above is prohibited.\n\n6. The provisions referred to in paragraph 5 shall also be applicable to cadmium-plated articles or components of such articles when used in the sectors/applications listed in points (a) and (b) below and to articles manufactured in the sectors listed in (b) below:\n(a) equipment and machinery for the production of:\n— paper and board [8419 32] [8439] [8441] textiles and clothing [8444] [8445] [8447] [8448] [8449] [8451] [8452]\n(b) equipment and machinery for the production of:\n— industrial handling equipment and machinery [8425] [8426] [8427] [8428] [8429] [8430] [8431]\n— road and agricultural vehicles [chapter 87]\n— rolling stock [chapter 86]\n— vessels [chapter 89]\n\n7. However, the restrictions in paragraphs 5 and 6 shall not apply to: — articles and components of the articles used in the aeronautical, aerospace, mining, offshore and nuclear sectors whose applications require high safety standards and in safety devices in road and agricultural vehicles, rolling stock and vessels, — electrical contacts in any sector of use, where that is necessary to ensure the reliability required of the apparatus on which they are installed. \n\n8. Shall not be used in brazing fillers in concentration equal to or greater than 0,01 % by weight. Brazing fillers shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight. For the purpose of this paragraph brazing shall mean a joining technique using alloys and under- taken at temperatures above 450 °C.\n\n9. By way of derogation, paragraph 8 shall not apply to brazing fillers used in defence and aerospace applications and to brazing fillers used for safety reasons.\n\n10. Shall not be used or placed on the market if the concentration is equal to or greater than 0,01 % by weight of the metal in: (i) metal beads and other metal components for jewellery making; (ii) metal parts of jewellery and imitation jewellery articles and hair accessories, including: — bracelets, necklaces and rings, — piercing jewellery, — wrist-watches and wrist-wear, — brooches and cufflinks.\n\n11. By way of derogation, paragraph 10 shall not apply to articles placed on the market before 10 December 2011 and jewellery more than 50 years old on 10 December 2011. "},"1. Shall not be used in mixtures and articles produced from synthetic organic polymers (hereafter referred to as plastic material) such as:\n— polymers or copolymers of vinyl chloride (PVC) [3904 10] [3904 21]\n— polyurethane (PUR) [3909 50]\n— low-density polyethylene (LDPE), with the exception of low-density polyethylene used for the production of coloured masterbatch [3901 10]\n— cellulose acetate (CA) [3912 11]\n— cellulose acetate butyrate (CAB) [3912 11]\n— epoxy resins [3907 30]\n— melamine-formaldehyde (MF) resins [3909 20]\n— urea-formaldehyde (UF) resins [3909 10]\n— unsaturated polyesters (UP) [3907 91]\n— polyethylene terephthalate (PET) [3907 60]\n— polybutylene terephthalate (PBT)\n— transparent/general-purpose polystyrene [3903 11]\n— acrylonitrile methylmethacrylate (AMMA)\n— cross-linked polyethylene (VPE)\n— high-impact polystyrene\n— polypropylene (PP) [3902 10]\n— high-density polyethylene (HDPE) [3901 20]\n— acrylonitrile butadiene styrene (ABS) [3903 30]\n— poly(methyl methacrylate) (PMMA) [3906 10].\n\nMixtures and articles produced from plastic material shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight of the plastic material.\n\nBy way of derogation, the second subparagraph shall not apply to articles placed on the market before 10 December 2011. \n\nThe first and second subparagraphs apply without prejudice to Council Directive 94/62/EC (**) and acts adopted on its basis.\n\n2. Shall not be used in paints [3208] [3209].\n\nFor paints with a zinc content exceeding 10 % by weight of the paint, the concentration of cadmium (expressed as Cd metal) shall not be equal to or greater than 0,1 % by weight.\n\nPainted articles shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,1 % by weight of the paint on the painted article.\n\n3. By way of derogation, paragraphs 1 and 2 shall not apply to articles coloured with mixtures containing cadmium for safety reasons.\n\n4. By way of derogation, paragraph 1, second subparagraph shall not apply to:\n— mixtures produced from PVC waste, hereinafter referred to as ‘recovered PVC’,\n— mixtures and articles containing recovered PVC if their concentration of cadmium (expressed as Cd metal) does not exceed 0,1 % by weight of the plastic material in the following rigid PVC applications:\n(a) profiles and rigid sheets for building applications;\n(b) doors, windows, shutters, walls, blinds, fences, and roof gutters;\n(c) decks and terraces;\n(d) cable ducts;\n(e) pipes for non-drinking water if the recovered PVC is used in the middle layer of a multilayer pipe and is entirely covered with a layer of newly produced PVC in compliance with paragraph 1 above.\n\nSuppliers shall ensure, before the placing on the market of mixtures and articles containing recovered PVC for the first time, that these are visibly, legibly and indelibly marked as follows: ‘Contains recovered PVC’ or with the following pictogram:\n\nIn accordance with Article 69 of this Regulation, the derogation granted in paragraph 4 will be reviewed, in particular with a view to reducing the limit value for cadmium and to reassess the derogation for the applications listed in points (a) to (e), by 31 December 2017. \n\n5. For the purpose of this entry, ‘cadmium plating’ means any deposit or coating of metallic cadmium on a metallic surface.\n\nShall not be used for cadmium plating metallic articles or components of the articles used in the following sectors/applications:\n(a) equipment and machinery for: — food production [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] — agriculture [8419 31] [8424 81] [8432] [8433] [8434] [8436] — cooling and freezing [8418] — printing and book-binding [8440] [8442] [8443]\n(b) equipment and machinery for the production of:\n— household goods [7321] [8421 12] [8450] [8509] [8516]\n— furniture [8465] [8466] [9401] [9402] [9403] [9404]\n— sanitary ware [7324]\n— central heating and air conditioning plant [7322] [8403] [8404] [8415]\nIn any case, whatever their use or intended final purpose, the placing on the market of cadmium-plated articles or components of such articles used in the sectors/applications listed in points (a) and (b) above and of articles manufactured in the sectors listed in point (b) above is prohibited.\n\n6. The provisions referred to in paragraph 5 shall also be applicable to cadmium-plated articles or components of such articles when used in the sectors/applications listed in points (a) and (b) below and to articles manufactured in the sectors listed in (b) below:\n(a) equipment and machinery for the production of:\n— paper and board [8419 32] [8439] [8441] textiles and clothing [8444] [8445] [8447] [8448] [8449] [8451] [8452]\n(b) equipment and machinery for the production of:\n— industrial handling equipment and machinery [8425] [8426] [8427] [8428] [8429] [8430] [8431]\n— road and agricultural vehicles [chapter 87]\n— rolling stock [chapter 86]\n— vessels [chapter 89]\n\n7. However, the restrictions in paragraphs 5 and 6 shall not apply to: — articles and components of the articles used in the aeronautical, aerospace, mining, offshore and nuclear sectors whose applications require high safety standards and in safety devices in road and agricultural vehicles, rolling stock and vessels, — electrical contacts in any sector of use, where that is necessary to ensure the reliability required of the apparatus on which they are installed. \n\n8. Shall not be used in brazing fillers in concentration equal to or greater than 0,01 % by weight. Brazing fillers shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight. For the purpose of this paragraph brazing shall mean a joining technique using alloys and under- taken at temperatures above 450 °C.\n\n9. By way of derogation, paragraph 8 shall not apply to brazing fillers used in defence and aerospace applications and to brazing fillers used for safety reasons.\n\n10. Shall not be used or placed on the market if the concentration is equal to or greater than 0,01 % by weight of the metal in: (i) metal beads and other metal components for jewellery making; (ii) metal parts of jewellery and imitation jewellery articles and hair accessories, including: — bracelets, necklaces and rings, — piercing jewellery, — wrist-watches and wrist-wear, — brooches and cufflinks.\n\n11. By way of derogation, paragraph 10 shall not apply to articles placed on the market before 10 December 2011 and jewellery more than 50 years old on 10 December 2011. ","1. Dürfen nicht in Gemischen und Erzeugnissen verwendet werden, die aus synthetischen organischen Polymeren (nachstehend Kunststoff genannt) hergestellt werden, wie z.B.\n    Polymere oder Copolymere aus Vinylchlorid (PVC) [3904 10] [3904 21],\n    Polyurethan (PUR) [3909 50],\n    Polyethylen niedriger Dichte (LDPE) mit Ausnahme des für die Herstellung von Pigmentpräparationen (\"master batch\") verwendeten Polyethylens niedriger Dichte [3901 10]\n    Celluloseacetat (CA) [3912 11],\n    Celluloseacetobutyrat (CAB) [3912 11],\n    Epoxydharze [3907 30],\n    Melaminharzformaldehyd (MF) [3909 20],\n    Harnstoffformaldehyd (UF) [3909 10],\n    ungesättigte Polyester (UP) [3907 91],\n    Polyethylenterephtalat (PET) [3907 60],\n    Polybuthylenterephtalat (PBT),\n    Polystyrol glasklar/Standard [3903 11],\n    Acrylnitrilmethylmetacrylat (AMMA),\n    vernetztes Polyethylen (VPE),\n    Polystyrol, schlagfest (SB),\n    Polypropylen (PP) [3902 10],\n    Polyethylen hoher Dichte (HDPE) [3901 20],\n    Acrylnitril-Butadien-Styrol-Copolymere (ABS) [3903 30],\n    Poly(methylmethacrylat) (PMMA) [3906 10]. \nAus Kunststoffen hergestellte Gemische und Erzeugnisse dürfen nicht in Verkehr gebracht werden, wenn ihr Cadmiumgehalt (Cd-Metall) 0,01 Gew. -% des Kunststoffs oder mehr beträgt.\nAbweichend davon gilt Unterabsatz 2 nicht für Erzeugnisse, die vor dem 10. Dezember 2011 in Verkehr gebracht wurden.\nUnterabsatz 1 und 2 gelten unbeschadet der Richtlinie 94/62/EG des Rates * und der auf ihrer Grundlage erlassenen Rechtsakte.\n2. Dürfen nicht in Anstrichfarben und Lacken [3208] [3209] verwendet werden\nBei Anstrichfarben und Lacken mit einem Zinkgehalt von mehr als 10 Gew.- % der Anstrichfarbe bzw. des Lackes darf der Cadmiumgehalt (Cd-Metall) nicht 0,1 Gew. -% oder mehr betragen.\nGestrichene/lackierte Erzeugnisse dürfen nicht in Verkehr gebracht werden, wenn ihr Cadmiumgehalt (Cd-Metall) 0,1 Gew.- % der Anstrichfarbe/des Lackes auf dem gestrichenen/lackierten Erzeugnis oder mehr beträgt.\n3. Abweichend davon gelten die Absätze 1 und 2 nicht für Erzeugnisse, die aus Sicherheitsgründen mit cadmiumhaltigen Gemischen gefärbt sind.\n4. Abweichend davon gilt Absatz 1 Unterabsatz 2 nicht für:\n    aus PVC-Abfall hergestellte Gemische, nachstehend \"Recycling-PVC' genannt,\n    Gemische und Erzeugnisse, die Recycling-PVC enthalten, sofern ihr Cadmiumgehalt (Cd-Metall) 0,1 Gew.-% des Kunststoffs in folgenden Hart-PVC-Anwendungen nicht übersteigt:\n        Profile und Hart-PVC-Platten für den Einsatz im Bauwesen,\n        Türen, Fenster, Fensterläden, Wände, Jalousien, Zäune und Dachrinnen,\n        Boden- und Terrassenbeläge,\n        Kabelführungen,\n        Wasserrohre, ausgenommen Trinkwasserrohre, sofern das Recycling-PVC in der mittleren Schicht eines mehrschichtigen Rohrs verwendet wird und vollständig mit einer Schicht von neu hergestelltem PVC nach Absatz 1 überzogen ist. \nDie Lieferanten gewährleisten vor dem erstmaligen Inverkehrbringen von Gemischen und Erzeugnissen, die Recycling-PVC enthalten, dass diese gut sichtbar, leserlich und unverwischbar mit der Aufschrift \"Enthält Recycling-PVC\" oder mit folgendem Piktogramm versehen sind:\nDie in Absatz 4 gewährte Ausnahmeregelung wird gemäß Artikel 69 dieser Verordnung bis zum 31. Dezember 2017 insbesondere im Hinblick darauf überprüft, den Grenzwert für Cadmium zu senken und die Ausnahmeregelung für die unter den Buchstaben a bis e aufgeführten Anwendungen erneut zu beurteilen.\n5. Für die Zwecke dieses Eintrags bedeutet Cadmium-Oberflächenbehandlung (Cadmierung) jeglichen Auftrag von Cadmium auf Metalloberflächen oder jegliche Beschichtung von Metalloberflächen mit Cadmium.\nDürfen nicht verwendet werden zur Cadmierung von Metallerzeugnissen oder Bestandteilen der in den folgenden Sektoren bzw. zu den folgenden Zwecken eingesetzten Erzeugnisse:\n    Geräte und Maschinen:\n        zur Herstellung von Lebensmitteln [8210] [8417 20] [8419 81] [8421.111 [8421 22] [8422] [8435] [8437] [8438] [8476 11],\n        für die Landwirtschaft [8419 31] [8424 81] [8432] [8433] [8434] [8436],\n        für das Gefrieren und Tiefgefrieren [8418],\n        für die Druckerei und Presse [8440] [8442] [8443], \n    Geräte und Maschinen zur Herstellung von:\n        Haushaltsgeräten [7321] [8421 12] [8450] [8509] [8516],\n        Möbeln [8465] [8466] [9401] [9402] [9403] [9404],\n        sanitären Anlagen [7324],\n        Zentralheizungen und Klimaanlagen [7322] [8403] [8404] [8415], \nDas Inverkehrbringen von cadmierten Erzeugnissen oder von Bestandteilen solcher Erzeugnisse, die in den in den vorstehenden Buchstaben a und b genannten Sektoren bzw. zu den dort genannten Zwecken eingesetzt werden, sowie das Inverkehrbringen von gewerblichen Erzeugnissen, die in den unter dem vorstehenden Buchstaben b genannten Sektoren hergestellt wurden, ist auf jeden Fall - unabhängig von ihrer Verwendung oder endgültigen Bestimmung - verboten.\n6. Absatz 5 gilt ferner für cadmierte Erzeugnisse oder Bestandteile solcher Erzeugnisse, die in den in den nachstehenden Buchstaben a und b genannten Sektoren bzw. zu den dort genannten Zwecken eingesetzt werden, sowie für gewerbliche Erzeugnisse, die in den unter dem vorstehenden Buchstaben b genannten Sektoren hergestellt wurden:\n    Geräte und Maschinen zur Herstellung von:\n        Papier und Pappe [8419 32] [8439] [8441], Textilien und Bekleidung [8444] [8445] [8447] [8448] [8449] [8451] [8452]; \n    Geräte und Maschinen zur Herstellung von:\n        in der Materialflusstechnik eingesetzten Einrichtungen [8425] [8426] [8427] [8428] [8429] [8430] [8431],\n        Pkw und landwirtschaftlichen Fahrzeugen [Kapitel 87],\n        Zügen [Kapitel 86],\n        Schiffen [Kapitel 89]. \n7. Die Beschränkungen der Absätze 5 und 6 gelten jedoch nicht für:\n    Erzeugnisse und Bestandteile von Erzeugnissen, die in der Luft- und Raumfahrt, im Bergbau, in der 'Offshore'-Technik sowie im Kernenergiebereich eingesetzt werden, wenn die Anwendungen ein hohes Sicherheitsniveau erfordern, sowie Komponenten von Sicherheitseinrichtungen in Straßenverkehrsmitteln, landwirtschaftlichen Fahrzeugen, Eisenbahnen und Schiffen,\n    elektrische Kontakte in allen Verwendungssektoren aus Gründen der Zuverlässigkeit der Geräte, in denen sie eingesetzt werden. \n8. Dürfen nicht in Konzentrationen von 0,01 Gew.- % oder mehr in Hartloten verwendet werden.\nHartlote dürfen nicht in Verkehr gebracht werden, wenn der Cadmiumgehalt (Cd- Metall) 0,01 Gew. -% oder mehr beträgt.\nFür die Zwecke dieses Absatzes bedeutet Hartlöten eine Verbindungstechnik, bei der mit Legierungen bei Temperaturen über 450 °C gearbeitet wird.\n9. Abweichend davon gilt Absatz 8 weder für Hartlote, die in Verteidigungs- sowie Luft- und Raumfahrtanwendungen eingesetzt werden, noch für Hartlote, die aus Sicherheitsgründen verwendet werden.\n10. Dürfen nicht in Konzentrationen von 0,01 Gew. -% des Metalls oder mehr in folgenden Erzeugnissen verwendet oder in Verkehr gebracht werden:\n    Metallperlen und andere metallische Teile für die Herstellung von Schmuckstücken,\n    Metallteile für Schmuck- und Fantasieschmuckerzeugnisse sowie Haarschmuck, einschließlich:\n        Armbänder, Halsketten und Ringe,\n        Piercingschmuck,\n        Armbanduhren und Armschmuck,\n        Broschen und Manschettenknöpfe. \n11. Abweichend davon gilt Absatz 10 weder für Erzeugnisse, die vor dem 10. Dezember 2011 in Verkehr gebracht wurden, noch für Schmuck, der am 10. Dezember 2011 mehr als 50 Jahre alt ist.","1.不得用于由下列合成有机聚合物（此后简称塑料材料）制造的物质和制剂中：\n—氯乙烯(PVC) [3904 10] [3904 21], \n—聚氨酯(PUR) [3909 50], \n—低密度聚乙烯(LDPE)，用于制造彩色母料时除外 [3901 10]  \n—醋酸纤维素(CA) [3912 11]\n—醋酸丁酸纤维素(CAB) [3912 11],  \n—环氧树脂[3907 30],\n— 密胺树脂(MF) [3909 20], \n—尿素甲醛（UF）树脂 [3909 10],\n —不饱和聚酯（UP）[3909 10]\n —聚乙烯对苯二酸酯(PET) [3907 60]\n —聚丁烯对苯二酸酯(PBT)\n —透明/一般用途聚苯乙烯 [3903 11]\n—丙烯腈甲基丙烯酸甲酯共聚物(AMMA)\n—交聯聚乙烯(VPE)\n —高耐重聚苯乙烯(high-impact polyethylene)\n—聚丙烯(PP) [390210]\n—高密度聚乙烯 (HDPE) [3901 20]\n—丙烯腈-丁二烯-苯乙烯 (ABS) [3903 30]\n—聚(甲基丙烯酸甲酯) (PMMA) [3906 10]\n由塑料材料制成的配制品和物品，若其镉含量（以金属镉计）大于或等于0.01%，则其不得投放市场.\n作为豁免，第2段不适用于2012年1月10前已投放到市场的物品。\n第1段和第2段无任何偏見地運用到理事会指令94/62/EC和法令中，并且以此为基础运作。\n\n2. 不可用于颜料[3208][3209]\n对于锌含量超过10%的颜料，镉（以金属镉的形式表达）的质量分数不可超过0.1%。\n颜料中的镉（以金属镉的形式表达）的质量分数（在涂装产品中颜料的质量分数）超过0.1%的，则不可投放市场。\n3.作为豁免，第1段和第2段不适用于基于安全原因而用含有镉的配制品染色了的物品。\n\n4. 作为豁免，第1段，第2分段不适用于:\n— 由PVC废弃物制得的配制品，以下简称“回收PVC”，\n—含有回收PVC的配制品或物质，若镉（以金属镉的形式表达）在以下刚性PVC应用中，含量不超过0.1%（塑料材料的质量分数）：\n(a) 用于建筑的外层和夹心层；\n(b) 门，窗，百叶窗，墙，气窗，篱笆和屋顶排水沟；\n(c)甲板和台阶；\n(d) 电缆管道\n(e)回收PVC作为中间层使用，且完全被全新的PVC覆盖的，符合第1段要求的非饮用水管道。\n供应商必须保证，在第一次投放含有回收PVC的配制品或物品进入市场前，应使用清晰、明显、永久性 “含有回收PVC” 的标识或以下标识：\n依据本法规第69条，在2017年12月31日前，第4段的豁免授权将被审核，特别要考虑进一步降低镉的险值和重新评估第(a)至(e)的豁免。\n\n5. 在本法规中，“镉电镀”是指金属表面上任何形式的金属镉沉积或涂层。\n镉电镀金属制品或制品零件中不可用于以下领域：\na） 用于以下用途的设备和机器：\n—食品加工production [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] \n—农业 [8419 31] [8424 81] [8432] [8433] [8434] [8436]\n — 冷冻设备 [8418] \n— 印刷和书本装订[8440] [8442] [8443]\nb） 用于生产以下物品的设备和机器：\n—家用制品[7321] [8421 12] [8450] [8509] [8516]\n— 家具 [8465] [8466] [9401] [9402] [9403] [9404]\n— 洁具 [7324]\n— 中央空调及中央供暖设备 [7322] [8403] [8404] [8415]\n在任何情况下，不管其用途和最终目的，镉电镀成品及其部件，当用于a）和b）中提及的领域/用途的成品时，不可在市场上出售。\n\n6．第5项所提及的规定也适用于以下a)和b)中涉及的领域/用途镉电镀成品或成品的组成部分，以及以下b)中列出的领域生产的成品：\na)用于生产以下物品的设备和机器：\n—纸和纸板[8419 32] [8439] [8441] \n—纺织品和服装 [8444] [8445] [8447] [8448] [8449] [8451] [8452]\n(b) 用于生产以下物品的设备和机器：\n—工业加工设备和机器[8425] [8426] [8427] [8428] [8429] [8430] [8431]\n— 公路与农用车辆[第87章]\n— 铁路或汽车公司的运输工具[第86章]\n—船舶 [第89章]\n\n7．但是第5、6项的限制不适用于：\n—用于航空的、太空的，矿产开采的，近海的和核能的成品或成品的组成部分，因其用于公路与农用车辆，铁路或汽车公司的运输工具和船舶等，需要较高的安全标准与设施；\n—出于安全设备可靠性的考虑，用于任何用途的电气插头。\n\n8.不能用於镉的质量分数超过0.01%的铜焊填料。\n 若镉（以金属镉的形式表达）的质量分数超过0.01%，则铜焊填料不可投放欧盟市場。在本段中，铜焊是指结合了使用合金的连接技术，其温度在450℃以上.\n\n9.作为豁免，第8段不可应用在用於防护和航空的铜焊填料，和因为安全原因运用的铜焊填料中。 \n\n10.若金属含量高于0.01%，则其不可投放市场：\n(i) 用于制造珠宝的金属珠或其他金属组件；\n(ii) 珠宝的金属部分和仿造珠宝及头饰，包括:\n— 手镯、项链和戒指\n— 穿透性的珠宝；\n— 腕表和腕带,\n— 胸针和袖口 \n\n11.作为豁免，第10段不可应用于在2012年1月10日前已投放市场的产品和在2012年1月10日时已有50年之久的首饰。"]
[null,{"$f":"IF($B$1=\"English\",C577,IF($B$1=\"Deutsch\",D577,IF($B$1=\"中文\",E577,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be used as propellant in aerosols for any use.\n\nAerosols dispensers containing the substance as propellant shall not be placed on the market."},"Shall not be used as propellant in aerosols for any use.\n\nAerosols dispensers containing the substance as propellant shall not be placed on the market.","Darf für keinen Verwendungszweck als Treibgas für Aerosole verwendet werden.\nAerosolpackungen, die diesen Stoff als Treibgas enthalten, dürfen nicht in Verkehr gebracht werden.","不得用于任何用途的喷雾器中作为推进剂。\n\n含有该物质作为推进剂的喷雾器，不得投放市场。"]
[null,{"$f":"IF($B$1=\"English\",C578,IF($B$1=\"Deutsch\",D578,IF($B$1=\"中文\",E578,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be used in articles or any parts thereof in concentrations greater than 0,1 mg/kg.\n\nArticles or any parts thereof containing DMF in concentrations greater than 0,1 mg/kg shall not be placed on the market.’"},"Shall not be used in articles or any parts thereof in concentrations greater than 0,1 mg/kg.\n\nArticles or any parts thereof containing DMF in concentrations greater than 0,1 mg/kg shall not be placed on the market.’","Darf nicht in Erzeugnissen oder Bestandteilen davon in Konzentrationen von über 0,1 mg/kg verwendet werden.\nErzeugnisse oder deren Bestandteile, die DMF in einer Konzentration von über 0,1 mg/kg enthalten, dürfen nicht in den Verkehr gebracht werden.","在任何物品或者部件中含量不得超过0,1mg/kg。\n\nDMF的含量超过0,1mg/kg的任何产品或部件，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C579,IF($B$1=\"Deutsch\",D579,IF($B$1=\"中文\",E579,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used:\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations greater than 0,1 % by weight.\n\n2. Articles shall not be placed on the market if they, or flame-retardant parts thereof, contain this substance in concentrations greater than 0,1 % by weight.\n\n3. By way of derogation, paragraph 2 shall not apply:\n— to articles that were in use in the Community before 15 August 2004,\n— to electrical and electronic equipment within the scope of Directive 2002/95/EC."},"1. Shall not be placed on the market, or used:\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations greater than 0,1 % by weight.\n\n2. Articles shall not be placed on the market if they, or flame-retardant parts thereof, contain this substance in concentrations greater than 0,1 % by weight.\n\n3. By way of derogation, paragraph 2 shall not apply:\n— to articles that were in use in the Community before 15 August 2004,\n— to electrical and electronic equipment within the scope of Directive 2002/95/EC.","1. Darf nicht in Verkehr gebracht oder verwendet werden:\n    als Stoff,\n    als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von 0,1 Gew: % oder mehr. \n2. Erzeugnisse dürfen nicht in Verkehr gebracht werden, wenn sie oder ihre mit Flammschutzmittel behandelten Teile diesen Stoff in einer Konzentration von mehr als 0,1 Gew: % enthalten.\n3. Absatz 2 gilt jedoch nicht für:\n    Erzeugnisse, die vor dem 15. August 2004 in der Gemeinschaft verwendet wurden,\n    Elektro- und Elektronikgeräte, die unter die Richtlinie 2002/95/EG fallen ","1. 以下情况不得投放市场或使用：\n  — 作为纯物质；\n  — 作为别的物质的组分，或者在配制品中，浓度大于等于0,1%时\n2.物品中或者其阻燃剂处理过的部件中该物质含量超过0.1%时，该物品不得投放市场。\n3. 第2段在以下情况下不适用：\n— 在15.08.2004年前已投入使用的物品；\n— 符合2002/95/EC范围内的电子电气设备"]
[null,{"$f":"IF($B$1=\"English\",C580,IF($B$1=\"Deutsch\",D580,IF($B$1=\"中文\",E580,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance, or in mixtures in a concentration equal to, or greater than 0,1 % by weight. \n\nHowever, the first paragraph shall not apply to this substance (DBB) or mixtures containing it if these are intended solely for conversion into articles, among which this substance will no longer feature in a concentration equal to or greater than 0,1 %."},"Shall not be placed on the market, or used, as a substance, or in mixtures in a concentration equal to, or greater than 0,1 % by weight. \n\nHowever, the first paragraph shall not apply to this substance (DBB) or mixtures containing it if these are intended solely for conversion into articles, among which this substance will no longer feature in a concentration equal to or greater than 0,1 %.","Dürfen weder als Stoffe noch in Gemischen in Konzentrationen von > 0,1 Gew: % in Verkehr gebracht oder verwendet werden.\nAbsatz 1 gilt jedoch nicht, wenn dieser Stoff (DBB) oder die ihn enthaltenden Gemische ausschließlich zu Erzeugnissen verarbeitet werden, in denen er nicht mehr in einer Konzentration von > 0,1 Gew: % vorhanden ist.","当物质或者制剂中该物质浓度大于等于0.1%时，不得投放市场或者使用。\n但是当其仅用于转化到成品时，此规定对这一物质(DBB)或其制剂无效，在此过程中，物质无法显现其特性浓度大于或等于0.1%"]
[null,{"$f":"IF($B$1=\"English\",C581,IF($B$1=\"Deutsch\",D581,IF($B$1=\"中文\",E581,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Without prejudice to the other parts of this Annex the following shall apply to entries 28 to 30:\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or,\n— in mixtures,\nfor supply to the general public when the individual concentration in the substance or mixture is equal to or greater than:\n— either the relevant specific concentration limit specified in Part 3 of Annex VI to Regulation (EC) No 1272/2008, or,\n— the relevant concentration specified in Directive 1999/45/EC where no specific concentration limit is set out in Part 3 of Annex VI to Regulation (EC) No 1272/2008.\nWithout prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is marked visibly, legibly and indelibly as follows:\n‘Restricted to professional users’.\n2. By way of derogation, paragraph 1 shall not apply to:\n(a) medicinal or veterinary products as defined by Directive 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC;\n(c) the following fuels and oil products:\n— motor fuels which are covered by Directive 98/70/EC,\n— mineral oil products intended for use as fuel in mobile or fixed combustion plants,\n— fuels sold in closed systems (e.g. liquid gas bottles);\n(d) artists’ paints covered by Directive 1999/45/ EC; \n(e) the substances listed in Appendix 11, column 1, for the applications or uses listed in Appendix 11, column 2. Where a date is specified in column 2 of Appendix 11, the derogation shall apply until the said date."},"Without prejudice to the other parts of this Annex the following shall apply to entries 28 to 30:\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or,\n— in mixtures,\nfor supply to the general public when the individual concentration in the substance or mixture is equal to or greater than:\n— either the relevant specific concentration limit specified in Part 3 of Annex VI to Regulation (EC) No 1272/2008, or,\n— the relevant concentration specified in Directive 1999/45/EC where no specific concentration limit is set out in Part 3 of Annex VI to Regulation (EC) No 1272/2008.\nWithout prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is marked visibly, legibly and indelibly as follows:\n‘Restricted to professional users’.\n2. By way of derogation, paragraph 1 shall not apply to:\n(a) medicinal or veterinary products as defined by Directive 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC;\n(c) the following fuels and oil products:\n— motor fuels which are covered by Directive 98/70/EC,\n— mineral oil products intended for use as fuel in mobile or fixed combustion plants,\n— fuels sold in closed systems (e.g. liquid gas bottles);\n(d) artists’ paints covered by Directive 1999/45/ EC; \n(e) the substances listed in Appendix 11, column 1, for the applications or uses listed in Appendix 11, column 2. Where a date is specified in column 2 of Appendix 11, the derogation shall apply until the said date.","\"Unbeschadet der übrigen Teile dieses Anhangs gilt Folgendes für die Einträge 28 bis 30:\n1. Dürfen nicht in Verkehr gebracht oder verwendet werden:\n- als Stoffe,\n- (Gültig ab 01.06.2015 gemäß Art. 59 der VO (EG) 1272/2008 die jeweiligen in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 festgelegten allgemeinen Konzentrationsgrenzwerte.) als Bestandteile anderer Stoffe oder\n- in Gemischen, die zum Verkauf an die breite Öffentlichkeit bestimmt sind, wenn die Einzelkonzentration des Stoffs oder Gemischs folgende Werte erreicht oder übersteigt:\n- die jeweiligen in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 festgelegten spezifischen Konzentrationsgrenzwerte oder\n- die jeweiligen in der Richtlinie 1999/45/EG festgelegten Konzentrationen, sofern in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 kein spezifischer Konzentrationsgrenzwert festgelegt ist.\nUnbeschadet der übrigen gemeinschaftlichen Vorschriften auf dem Gebiet der Einstufung, Verpackung und Etikettierung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung solcher Stoffe und Gemische gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n\"Nur für gewerbliche Anwender.\"\n2. Absatz 1 gilt jedoch nicht für:\na. a) Arznei- oder Tierarzneimittel gemäß der Begriffsbestimmung in der Richtlinie 2001/82/EG und der Richtlinie 2001/83/EG;\nb. kosmetische Mittel gemäß der Richtlinie 76/768/EWG;\nc. folgende Brennstoffe und Mineralölerzeugnisse:\n- Kraftstoffe, die Gegenstand der Richtlinie 98/70/EG sind,\n- Mineralölerzeugnisse, die zur Verwendung als Brennstoff oder Kraftstoff in beweglichen oder feststehenden Verbrennungsanlagen bestimmt sind,\n- Brennstoffe, die in geschlossenen Systemen (z.B. Flüssiggasflaschen) verkauft werden; \n(Gültig ab 01.06.2010 gemäß Art. 59 der VO (EG) 1272/2008\nd. Farben für Künstler gemäß der Verordnung (EG) Nr. 1272/2008)\nFarben für Künstler gemäß der Richtlinie 1999/45/EG.\ne.  in Anlage 11 Spalte 1 aufgeführte Stoffe für die in Anlage 11 Spalte 2 aufgeführten Anwendungen. Ist in Anlage 11 Spalte 2 ein Datum angegeben, gilt die Ausnahmeregelung bis zu diesem Datum.) \"\n","\n在不违背本附录其它规定的情况下，下列规定适用于28项至30项：\n1.不应用于个别浓度大于或等于以下规定的物质或制剂，投放市场销售给一般大众：\n-指令1272/2008/EC附件VI所具体规定的相关浓度；\n-指令1999/45/EC所具体规定的相关浓度，其中指令1272/2008/EC附件VI没有设置具体的浓度限制；\n在不违反欧盟危险物质与制剂分离、包装和标识的欧盟法规规定的情况下，该物质或制剂包装应以不可磨灭的方式清楚标示如下字样：\n”Restricted to professional users禁止非专业人员使用”\n2.作为免除项目，第一项不适用于：\na)指令2001/82/EC和指令2001/83/EC所定义的医药和兽药；\nb)指令76/768/EEC所定义的化妆品；\nc)以下燃料和油品：\n-指令98/70/EC覆盖的汽车燃料，\n-车辆或定点燃烧所用矿物油， \n-销售给密闭系统的燃料，如液化气瓶\nd)指令1999/45/EC涵盖的绘画颜料；\ne)附件11的第一列中列出的物质应用于附件11的第二列中列出的应用时。免除项目可适用至附件11的第二列中指定的时间为止。"]
[null,{"$f":"IF($B$1=\"English\",C582,IF($B$1=\"Deutsch\",D582,IF($B$1=\"中文\",E582,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in:\n— ornamental articles intended to produce light or colour effects by means of different phases, for example in ornamental lamps and ashtrays,\n— tricks and jokes,\n— games for one or more participants, or any article intended to be used as such, even with ornamental aspects,\n2. Articles not complying with paragraph 1 shall not be placed on the market.\n3. Shall not be placed on the market if they contain a colouring agent, unless required for fiscal reasons, or perfume, or both, if they: \n— can be used as fuel in decorative oil lamps for supply to the general public, and,\n— present an aspiration hazard and are labelled with R65 or H304,\n4. Decorative oil lamps for supply to the general public shall not be placed on the market unless they conform to the European Standard on Decorative oil lamps (EN 14059) adopted by the European Committee for Standardisation (CEN).\n5. Without prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of dangerous substances and mixtures, suppliers shall ensure, before the placing on the market, that the following requirements are met:\n(a) lamp oils, labelled with R65 or H304, intended for supply to the general public are visibly, legibly and indelibly marked as follows: ‘Keep lamps filled with this liquid out of the reach of children’; and, by 1 December 2010, ‘Just a sip of lamp oil — or even sucking the wick of lamps — may lead to life-threatening lung damage’;\n(b) grill lighter fluids, labelled with R65 or H304, intended for supply to the general public are legibly and indelibly marked by 1 December 2010 as follows: ‘Just a sip of grill lighter may lead to life threatening lung damage’;\n(c) lamp oils and grill lighters, labelled with R65 or H304, intended for supply to the general public are packaged in black opaque containers not exceeding 1 litre by 1 December 2010.\n6. No later than 1 June 2014, the Commission shall request the European Chemicals Agency to prepare a dossier, in accordance with Article 69 of the present Regulation with a view to ban, if appropriate, grill lighter fluids and fuel for decorative lamps, labelled R65 or H304, intended for supply to the general public.\n7. Natural or legal persons placing on the market for the first time lamp oils and grill lighter fluids, labelled with R65 or H304, shall by 1 December 2011, and annually thereafter, provide data on alternatives to lamp oils and grill lighter fluids labelled R65 or H304 to the competent authority in the Member State concerned. Member States shall make those data available to the Commission."},"1. Shall not be used in:\n— ornamental articles intended to produce light or colour effects by means of different phases, for example in ornamental lamps and ashtrays,\n— tricks and jokes,\n— games for one or more participants, or any article intended to be used as such, even with ornamental aspects,\n2. Articles not complying with paragraph 1 shall not be placed on the market.\n3. Shall not be placed on the market if they contain a colouring agent, unless required for fiscal reasons, or perfume, or both, if they: \n— can be used as fuel in decorative oil lamps for supply to the general public, and,\n— present an aspiration hazard and are labelled with R65 or H304,\n4. Decorative oil lamps for supply to the general public shall not be placed on the market unless they conform to the European Standard on Decorative oil lamps (EN 14059) adopted by the European Committee for Standardisation (CEN).\n5. Without prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of dangerous substances and mixtures, suppliers shall ensure, before the placing on the market, that the following requirements are met:\n(a) lamp oils, labelled with R65 or H304, intended for supply to the general public are visibly, legibly and indelibly marked as follows: ‘Keep lamps filled with this liquid out of the reach of children’; and, by 1 December 2010, ‘Just a sip of lamp oil — or even sucking the wick of lamps — may lead to life-threatening lung damage’;\n(b) grill lighter fluids, labelled with R65 or H304, intended for supply to the general public are legibly and indelibly marked by 1 December 2010 as follows: ‘Just a sip of grill lighter may lead to life threatening lung damage’;\n(c) lamp oils and grill lighters, labelled with R65 or H304, intended for supply to the general public are packaged in black opaque containers not exceeding 1 litre by 1 December 2010.\n6. No later than 1 June 2014, the Commission shall request the European Chemicals Agency to prepare a dossier, in accordance with Article 69 of the present Regulation with a view to ban, if appropriate, grill lighter fluids and fuel for decorative lamps, labelled R65 or H304, intended for supply to the general public.\n7. Natural or legal persons placing on the market for the first time lamp oils and grill lighter fluids, labelled with R65 or H304, shall by 1 December 2011, and annually thereafter, provide data on alternatives to lamp oils and grill lighter fluids labelled R65 or H304 to the competent authority in the Member State concerned. Member States shall make those data available to the Commission.","1. Dürfen nicht verwendet werden\n    in Dekorationsgegenständen, die zur Erzeugung von Licht- oder Farbeffekten (durch Phasenwechsel), z.B. in Stimmungslampen und Aschenbechern, bestimmt sind;\n    in Scherzspielen;\n    in Spielen für einen oder mehrere Teilnehmer oder in Erzeugnissen, die zur Verwendung als solche, auch zur Dekoration, bestimmt sind. \n2. Erzeugnisse, die die Anforderungen von Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.\n3. Dürfen nicht in Verkehr gebracht werden, wenn sie einen Farbstoff - außer aus steuerlichen Gründen - und/oder ein Parfüm enthalten, sofern\n    sie als für die Abgabe an die breite Öffentlichkeit bestimmter Brennstoff in dekorativen Öllampen verwendet werden können und\n    ihre Aspiration als gefährlich eingestuft ist und sie mit R65 oder H304 gekennzeichnet sind. \n4. Für die Abgabe an die breite Öffentlichkeit bestimmte dekorative Öllampen dürfen nicht in Verkehr gebracht werden, es sei denn, sie erfüllen die vom Europäischen Komitee für Normung (CEN) verabschiedete europäische Norm für dekorative Öllampen (EN 14059).\n5. Unbeschadet der Durchführung anderer Gemeinschaftsbestimmungen über die Einstufung, Verpackung und Kennzeichnung gefährlicher Stoffe und Gemische stellen die Lieferanten vor dem Inverkehrbringen sicher, dass folgende Anforderungen erfüllt sind:\n    Mit R65 oder H304 gekennzeichnete und für die Abgabe an die breite Öffentlichkeit bestimmte Lampenöle tragen gut sichtbar, leserlich und unverwischbar folgende Aufschriften: 'Mit dieser Flüssigkeit gefüllte Lampen sind für Kinder unzugänglich aufzubewahren' sowie ab dem 1. Dezember 2010 'Bereits ein kleiner Schluck Lampenöl - oder auch nur das Saugen an einem Lampendocht - kann zu einer lebensbedrohlichen Schädigung der Lunge führen'.\n    Mit R65 oder H304 gekennzeichnete und für die Abgabe an die breite Öffentlichkeit bestimmte flüssige Grillanzünder tragen ab dem 1. Dezember 2010 leserlich und unverwischbar folgende Aufschrift: 'Bereits ein kleiner Schluck Grillanzünder kann zu einer lebensbedrohlichen Schädigung der Lunge führen'.\n    Mit R65 oder H304 gekennzeichnete und für die Abgabe an die breite Öffentlichkeit bestimmte Lampenöle und Grillanzünder werden ab dem 1. Dezember 2010 in schwarzen undurchsichtigen Behältern mit höchstens 1 Liter Füllmenge abgepackt. \n6. Bis spätestens 1. Juni 2014 ersucht die Kommission die Europäische Chemikalienagentur, ein Dossier gemäß Artikel 69 dieser Verordnung auszuarbeiten, damit gegebenenfalls ein Verbot von mit R65 oder H304 gekennzeichneten und für die Abgabe an die breite Öffentlichkeit bestimmten flüssigen Grillanzündern und Brennstoffen für dekorative Lampen erlassen wird.\n7. Natürliche oder juristische Personen, die mit R65 oder H304 gekennzeichnete Lampenöle und flüssige Grillanzünder erstmals in Verkehr bringen, übermitteln bis 1. Dezember 2011 sowie danach jährlich der zuständigen Behörde des betreffenden Mitgliedstaats Daten über Alternativen zu mit R65 oder H304 gekennzeichneten Lampenölen und flüssigen Grillanzündern. Die Mitgliedstaaten machen diese Daten der Kommission zugänglich.","1. 不得用于\n- 通过不同相产生声光效果的装饰物品，例如在观赏灯和烟灰缸中；\n- 恶作剧和笑话；\n-一个或多个参与者的游戏，或者意在用于游戏目的的产品，即便只是装饰用途\n2. 不满足第1段要求的物品，不得投放市场。\n3.具有如下性质的物质或制剂，除非由于财政因素或者香料需要或两者共同因素，含有着色剂时不得投放市场：\n- 可作为装饰灯的燃料供应给广大市民，\n-存在呼吸危害且被标记为R65或者H304.\n4. 出售给广大市民的装饰油灯不得投放市场，除非它们符合欧洲标准化委员会（CEN）通过了欧洲装饰油灯标准(EN 14059)。\n5.在不违反其它有关危险物质和制剂分类、包装和标识欧盟法规的情况下，供应商要保证在销售之前满足以下条件：\n（a）有R65或H304所标记的、用于作为出售给广大市民的灯油要有清晰可见的，不会磨损的标签：“含有此液体的灯必须远离儿童”；以及自2010年12月1日起，再加上“微量吸入灯油甚至灯芯，都可能导致危及生命的肺部损伤”的标示。\n（b）有R65或H304所标记的、用于作为出售给广大市民的液体烧烤点火液，自2010年12月1日起要有清晰可见的，不会磨损的标签： “微量吸入灯油甚至灯芯，都可能导致危及生命的肺部损伤”。\n（c）有R65或H304所标记的、用于作为出售给广大市民的灯油和液体烧烤点火液，自2010年12月1日起要包装在黑色不透光的容器，且容器容量不超过1升。\n6.最迟到2014年6月1日，委员会将要求欧洲\"化学品管理署\"根据目前法规69条的规定准备一个卷宗，建议如果可能的话，禁止此类有R65或H304所标记、用于作为出售给广大市民的液体烧烤点火液和装饰灯油。\n7.自然人和法人，把有标记R65或H304的灯油和液体烧烤点火液投放市场销售的，在2011年12月1日前以及往后每年，须向成员国的相关主管机关提交有R65或H304标记的灯油和烧烤烧烤点火液的替代方案和时间表。成员国应提供给委员会这一信息。"]
[null,{"$f":"IF($B$1=\"English\",C583,IF($B$1=\"Deutsch\",D583,IF($B$1=\"中文\",E583,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures.\n\nArticles containing the substance shall not be placed on the market."},"Shall not be placed on the market, or used, as a substance or in mixtures.\n\nArticles containing the substance shall not be placed on the market.","Darf weder als Stoff noch in Gemischen in Verkehr gebracht oder verwendet werden.\nErzeugnisse, die diesen Stoff enthalten, dürfen nicht in Verkehr gebracht werden.","物质或含有该物质的制剂，不得投放市场销售。含有该物质的物品，也不得投放市场销售。"]
[null,{"$f":"IF($B$1=\"English\",C584,IF($B$1=\"Deutsch\",D584,IF($B$1=\"中文\",E584,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as a substance or in mixtures. Articles containing the substance shall not be placed on the market.\n2. By way of derogation, paragraph 1 shall not apply:\n(a) in the case of plant and machinery already in service on 18 June 1994, until such plant and machinery is disposed of;\n(b) in the case of the maintenance of plant and machinery already in service within a Member State on 18 June 1994.\nFor the purposes of point (a) Member States may, on grounds of human health protection and environmental protection, prohibit within their territory the use of such plant or machinery before it is disposed of."},"1. Shall not be placed on the market, or used, as a substance or in mixtures. Articles containing the substance shall not be placed on the market.\n2. By way of derogation, paragraph 1 shall not apply:\n(a) in the case of plant and machinery already in service on 18 June 1994, until such plant and machinery is disposed of;\n(b) in the case of the maintenance of plant and machinery already in service within a Member State on 18 June 1994.\nFor the purposes of point (a) Member States may, on grounds of human health protection and environmental protection, prohibit within their territory the use of such plant or machinery before it is disposed of.","1. Darf weder als Stoff noch in Gemischen in Verkehr gebracht oder verwendet werden.\nErzeugnisse, die diesen Stoff enthalten, dürfen nicht in Verkehr gebracht werden.\n2. Absatz 1 gilt jedoch nicht für:\n    Anlagen und Maschinenteile, die sich am 18. Juni 1994 bereits im Betrieb befanden, bis diese Anlagen und Maschinenteile entsorgt werden,\n    die Wartung von Anlagen und Maschinenteilen, die sich am 18. Juni 1994 bereits in einem Mitgliedstaat im Betrieb befanden. \nFür die Zwecke von Buchstabe a können die Mitgliedstaaten jedoch aus Gründen des Gesundheits- und des Umweltschutzes in ihrem Hoheitsgebiet die Verwendung dieser Anlagen und Maschinenteile vor deren Entsorgung untersagen.","1.物质或含有该物质的制剂，不得投放市场销售。含有该物质的物品，也不得投放市场销售。\n2. 作为免除项目，第1项不适用于：\n（a）对于1994年6月18日前已投入使用的工厂和机器设备，可一直使用至机器的组件和设备报废\n（b）维修1994年6月18日前已在成员国投入使用的工厂和机器设备。\n对于免除项（a），成员国可以因为健康和环境的保护的原因，禁止在其境内使用这种工厂或设备，哪怕它们尚未报废。"]
[null,{"$f":"IF($B$1=\"English\",C585,IF($B$1=\"Deutsch\",D585,IF($B$1=\"中文\",E585,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used:\n(a) in any post assemblies which are inserted into pierced ears and other pierced parts of the human body unless the rate of nickel release from such post assemblies is less than 0,2 μg/cm 2 /week (migration limit);\n(b) in articles intended to come into direct and prolonged contact with the skin such as:\n— earrings,\n— necklaces, bracelets and chains, anklets, finger rings,\n— wrist-watch cases, watch straps and tighteners,\n— rivet buttons, tighteners, rivets, zippers and metal marks, when these are used in garments, if the rate of nickel release from the parts of these articles coming into direct and prolonged contact with the skin is greater than 0,5 μg/cm 2 /week.\n(c) in articles referred to in point (b) where these have a non-nickel coating unless such coating is sufficient to ensure that the rate of nickel release from those parts of such articles coming into direct and prolonged contact with the skin will not exceed 0,5 μg/cm 2 /week for a period of at least two years of normal use of the article.\n2. Articles which are the subject of paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph. \n3. The standards adopted by the European Committee for Standardisation (CEN) shall be used as the test methods for demonstrating the conformity of articles to paragraphs 1 and 2."},"1. Shall not be used:\n(a) in any post assemblies which are inserted into pierced ears and other pierced parts of the human body unless the rate of nickel release from such post assemblies is less than 0,2 μg/cm 2 /week (migration limit);\n(b) in articles intended to come into direct and prolonged contact with the skin such as:\n— earrings,\n— necklaces, bracelets and chains, anklets, finger rings,\n— wrist-watch cases, watch straps and tighteners,\n— rivet buttons, tighteners, rivets, zippers and metal marks, when these are used in garments, if the rate of nickel release from the parts of these articles coming into direct and prolonged contact with the skin is greater than 0,5 μg/cm 2 /week.\n(c) in articles referred to in point (b) where these have a non-nickel coating unless such coating is sufficient to ensure that the rate of nickel release from those parts of such articles coming into direct and prolonged contact with the skin will not exceed 0,5 μg/cm 2 /week for a period of at least two years of normal use of the article.\n2. Articles which are the subject of paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph. \n3. The standards adopted by the European Committee for Standardisation (CEN) shall be used as the test methods for demonstrating the conformity of articles to paragraphs 1 and 2.","1. Darf nicht verwendet werden:\n    in sämtlichen Stäben, die in durchstochene Ohren oder andere durchstochene Körperteile eingeführt werden, außer wenn die Nickelabgabe aus solchen Stäben unter 0,2 µg/cm2/Woche liegt (Migrationslimit);\n    in Erzeugnissen, die dazu bestimmt sind, unmittelbar und länger mit der Haut in Berührung zu kommen, wie zum Beispiel:\n        Ohrringen,\n        Halsketten, Armbändern und Ketten, Fußringen und Fingerringen,\n        Armbanduhrgehäusen, Uhrarmbändern und Spannern,\n        Nietknöpfen, Spangen, Nieten, Reißverschlüssen und Metallmarkierungen, wenn sie in Kleidungsstücken verwendet werden, \n    sofern die Nickelfreisetzung von den Teilen dieser Erzeugnisse, die unmittelbar und länger mit der Haut in Berührung kommen, 0,5 µg/cm2/Woche übersteigt;\n    in den in Buchstabe b aufgeführten Erzeugnissen, die eine Nichtnickelbeschichtung haben, es sei denn, diese Beschichtung reicht aus, um sicherzustellen, dass die Nickelfreisetzung von den Teilen solcher Erzeugnisse, die unmittelbar und länger mit der Haut in Berührung kommen, 0,5 µg/cm2/Woche für einen Zeitraum von mindestens zwei Jahren normaler Verwendung des Erzeugnisses nicht übersteigen. \n2. Erzeugnisse, für die Absatz 1 gilt, dürfen nicht in Verkehr gebracht werden, wenn sie nicht den Bestimmungen dieses Absatzes entsprechen.\n3. Zum Nachweis der Vereinbarkeit der Erzeugnisse mit Absatz 1 und 2 sind als Testmethoden die vom Europäischen Komitee für Normung (CEN) verabschiedeten Normen zu verwenden.","1. 不得用于：\na）耳洞和人体其它穿刺部位使用的配件，无论这种物品最终是否被除去。除非镍的释出速率小于0.2g/cm2/周(迁移限值)\nb）与皮肤有直接及长期接触的成品，如：\n-耳环\n-项链，手镯和项圈，脚环，戒指\n-手表壳、表带和带扣\n-铆扣、搭扣、铆钉、拉链和金属标牌等用作服装上的物件\n-如果这些与皮肤有直接及长期接触的成品中镍的释放速率超过了0.5g/cm2/周\nc）对于具有非镍镀层的1（b）中列出的成品，除非这种镀层足以保证在至少两年的正常使用过程中，从这些成品的与皮肤有直接或长期接触的部位释放出来的镍的速率不超过0.5g/cm2/周者，不受此限制。\n2.前项中的成品，除非其符合那些项目的要求，否则不能投放市场。\n3. 欧洲标准委员会(CEN)所采用的标准可作为证明成品是否符合第1、2项要求的测试方法。\n"]
[null,{"$f":"IF($B$1=\"English\",C586,IF($B$1=\"Deutsch\",D586,IF($B$1=\"中文\",E586,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures in concentrations equal to or greater than 0,1 % by weight for the following purposes:\n(1) industrial and institutional cleaning except:\n— controlled closed dry cleaning systems where the washing liquid is recycled or incinerated,\n— cleaning systems with special treatment where the washing liquid is recycled or incinerated.\n(2) domestic cleaning;\n(3) textiles and leather processing except:\n— processing with no release into waste water,\n— systems with special treatment where the process water is pre-treated to remove the organic fraction completely prior to biological waste water treatment (degreasing of sheepskin);\n(4) emulsifier in agricultural teat dips;\n(5) metal working except:\nuses in controlled closed systems where the washing liquid is recycled or incinerated;\n(6) manufacturing of pulp and paper;\n(7) cosmetic products;\n(8) other personal care products except:\nspermicides;\n(9) co-formulants in pesticides and biocides. However national authorisations for pesticides or biocidal products containing nonylphenol ethoxylates as co-formulant, granted before 17 July 2003, shall not be affected by this restriction until their date of expiry."},"Shall not be placed on the market, or used, as substances or in mixtures in concentrations equal to or greater than 0,1 % by weight for the following purposes:\n(1) industrial and institutional cleaning except:\n— controlled closed dry cleaning systems where the washing liquid is recycled or incinerated,\n— cleaning systems with special treatment where the washing liquid is recycled or incinerated.\n(2) domestic cleaning;\n(3) textiles and leather processing except:\n— processing with no release into waste water,\n— systems with special treatment where the process water is pre-treated to remove the organic fraction completely prior to biological waste water treatment (degreasing of sheepskin);\n(4) emulsifier in agricultural teat dips;\n(5) metal working except:\nuses in controlled closed systems where the washing liquid is recycled or incinerated;\n(6) manufacturing of pulp and paper;\n(7) cosmetic products;\n(8) other personal care products except:\nspermicides;\n(9) co-formulants in pesticides and biocides. However national authorisations for pesticides or biocidal products containing nonylphenol ethoxylates as co-formulant, granted before 17 July 2003, shall not be affected by this restriction until their date of expiry.","Darf für die folgenden Zwecke weder als Stoff noch in Gemischen in Konzentrationen von >0,1 Gew: % oder mehr in Verkehr gebracht oder verwendet werden:\n1. gewerbliche Reinigung, ausgenommen:\n    überwachte geschlossene Systeme für die chemische Reinigung, in denen die Reinigungsflüssigkeit recycelt oder verbrannt wird,\n    Spezialreinigungssysteme, in denen die Reinigungsflüssigkeit recycelt oder verbrannt wird; \n2. Haushaltsreinigung;\n3. Textil- und Lederverarbeitung, ausgenommen:\n    Behandlungen, bei denen kein NPE in das Abwasser gelangt,\n    Anlagen für spezielle Behandlungen, bei denen die organische Fraktion vor der biologischen Abwasserbehandlung vollständig aus dem Prozesswasser entfernt wird (Entfetten von Schafshäuten); \n4. Emulgator in Melkfett;\n5. Metallverarbeitung, ausgenommen:\nAnwendungen in überwachten geschlossenen Systemen, bei denen die Reinigungsflüssigkeit recycelt oder verbrannt wird;\n6. Herstellung von Zellstoff und Papier;\n7. kosmetische Mittel;\n8. sonstige Körperpflegemittel, ausgenommen: Spermizide;\n9. Formulierungshilfsstoffe in Pestiziden und Bioziden. Zulassungen der Mitgliedstaaten für Pestizide oder Biozide, die Nonylphenolethoxylate als Formulierungshilfsstoffe enthalten, bleiben jedoch, wenn sie vor dem 17. Juni 2003 erteilt wurden, bis zu ihrem Auslaufen unberührt von dieser Einschränkung.","不得以下述目的投放市场或用作物质或制剂的成分，如果浓度大于等于0.1%：\n（1） 工业和公共机构用清洁剂，但下列除外：\n-受控的密闭干洗系统，其清洁剂将回收或焚烧处理；\n-特殊处理的清洗系统，其清洁剂将回收或焚烧处理；\n（2）家用清洗；\n（3）纺织品和皮革制品的处理，但下列除外：\n-不会排出废水的处理方式\n-特殊处理的系统，在该系统下，废水经过生物废水处理前，会先完全去除其中的有机成分（羊皮脱脂）；\n（4）农用喷洒药剂中的乳化剂\n（5）金属加工，但下列除外：\n-使用受控的密闭系统，其清洗液将回收或焚烧处理\n（6）纸浆和纸张的制造；\n（7）化妆品；\n（8）其他个人护理用品，但杀精剂除外；\n（9）杀虫剂或抗生素的配方。但是2003年6月17日之前国家授权的含有壬基酚聚氧乙烯醚作为配方助剂农药或生物农药产品，不受此限制，直至其过期为止。\n"]
[null,{"$f":"IF($B$1=\"English\",C587,IF($B$1=\"Deutsch\",D587,IF($B$1=\"中文\",E587,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used,\n— as a substance,\n— as a constituent in other substances, or in mixtures, in a concentration equal to or greater than 0,1 % by weight."},"Shall not be placed on the market, or used,\n— as a substance,\n— as a constituent in other substances, or in mixtures, in a concentration equal to or greater than 0,1 % by weight.","Darf nicht in Verkehr gebracht oder verwendet werden:\n    als Stoff,\n    als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von > 0,1 Gew: %. ","当物质或制剂中该成分浓度大于等于0.1%，不得投放市场或使用"]
[null,{"$f":"IF($B$1=\"English\",C588,IF($B$1=\"Deutsch\",D588,IF($B$1=\"中文\",E588,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market."},"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.","1. Dürfen nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2. Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr ge- bracht werden.","\n1.不可用于纺织品，例如服装、内衣及家庭日用织品等会与皮肤接触的物品\n2.产品不满足第1项，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C589,IF($B$1=\"Deutsch\",D589,IF($B$1=\"中文\",E589,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used:\n— as substances,\n— in mixtures, including waste oils, or in equipment, in concentrations greater than 50 mg/kg (0,005 % by weight)."},"Shall not be placed on the market, or used:\n— as substances,\n— in mixtures, including waste oils, or in equipment, in concentrations greater than 50 mg/kg (0,005 % by weight).","Dürfen nicht in Verkehr gebracht oder verwendet werden:\n    als Stoffe,\n    in Gemischen, einschließlich Altölen, die mehr als 0,005 Gew: % PCT enthalten. ","当物质或配制品中（包括废油）或在设备中，该成分浓度大于等于50mg/kg （0.005%），不得投放市场或使用"]
[null,{"$f":"IF($B$1=\"English\",C590,IF($B$1=\"Deutsch\",D590,IF($B$1=\"中文\",E590,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"18:\nShall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use:\n(a) to prevent the fouling by micro-organisms, plants or animals of:\n— the hulls of boats,\n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming,\n— any totally or partly submerged appliances or equipment;\n(b) in the preservation of wood;\n(c) in the impregnation of heavy-duty industrial textiles and yarn intended for their manufacture;\n(d) in the treatment of industrial waters, irrespective of their use. \n\n18a:\n1. Shall not be placed on the market:\n(a) in fever thermometers;\n(b) in other measuring devices intended for sale to the general public (such as manometers, barometers, sphygmomanometers, thermometers other than fever thermometers).\n2. The restriction in paragraph 1 shall not apply to measuring devices that were in use in the Community before 3 April 2009. However Member States may restrict or prohibit the placing on the market of such measuring devices.\n3. The restriction in paragraph 1(b) shall not apply to:\n(a) measuring devices more than 50 years old on 3 October 2007;\n(b) barometers (except barometers within point (a)) until 3 October 2009.\n4. By 3 October 2009 the Commission shall carry out a review of the availability of reliable safer alternatives that are technically and economically feasible for mercury containing sphygmomanometers and other measuring devices in healthcare and in other professional and industrial uses. On the basis of this review or as soon as new information on reliable safer alternatives for sphygmomanometers and other measuring devices containing mercury becomes available, the Commission shall, if appropriate, present a legislative proposal to extend the restrictions in paragraph 1 to sphygmomanometers and other measuring devices in healthcare and in other professional and industrial uses, so that mercury in measuring devices is phased out whenever technically and economically feasible."},"18:\nShall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use:\n(a) to prevent the fouling by micro-organisms, plants or animals of:\n— the hulls of boats,\n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming,\n— any totally or partly submerged appliances or equipment;\n(b) in the preservation of wood;\n(c) in the impregnation of heavy-duty industrial textiles and yarn intended for their manufacture;\n(d) in the treatment of industrial waters, irrespective of their use. \n\n18a:\n1. Shall not be placed on the market:\n(a) in fever thermometers;\n(b) in other measuring devices intended for sale to the general public (such as manometers, barometers, sphygmomanometers, thermometers other than fever thermometers).\n2. The restriction in paragraph 1 shall not apply to measuring devices that were in use in the Community before 3 April 2009. However Member States may restrict or prohibit the placing on the market of such measuring devices.\n3. The restriction in paragraph 1(b) shall not apply to:\n(a) measuring devices more than 50 years old on 3 October 2007;\n(b) barometers (except barometers within point (a)) until 3 October 2009.\n4. By 3 October 2009 the Commission shall carry out a review of the availability of reliable safer alternatives that are technically and economically feasible for mercury containing sphygmomanometers and other measuring devices in healthcare and in other professional and industrial uses. On the basis of this review or as soon as new information on reliable safer alternatives for sphygmomanometers and other measuring devices containing mercury becomes available, the Commission shall, if appropriate, present a legislative proposal to extend the restrictions in paragraph 1 to sphygmomanometers and other measuring devices in healthcare and in other professional and industrial uses, so that mercury in measuring devices is phased out whenever technically and economically feasible.","18:\nDürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die für folgende Verwendungen bestimmt sind:\na) zur Verhinderung des Bewuchses durch Mikroorganismen, Pflanzen oder Tiere an:\n    Bootskörpern;\n    Kästen, Schwimmern, Netzen sowie anderen Geräten oder Einrichtungen für die Fisch- und Muschelzucht;\n    völlig oder teilweise untergetauchten Geräten oder Einrichtungen jeder Art; \nb) zum Schutz von Holz;\nc) zur Imprägnierung von schweren industriellen Textilien und von zu deren Herstellung vorgesehenen Garnen;\nd) zur Aufbereitung von Wasser im industriellen, gewerblichen und kommunalen Bereich, unabhängig von seiner Verwendung.\n18a:\n1. Darf nicht in Verkehr gebracht werden:\n    in Fieberthermometern;\n    in anderen zum Verkauf an die breite Öffentlichkeit bestimmten Messinstrumenten (z.B. Manometer, Barometer, Sphygmomanometer, andere Thermometer als Fieberthermometer). \n2. Die in Absatz 1 genannte Beschränkung gilt nicht für Messinstrumente, die vor dem 3. April 2009 in der Gemeinschaft in Gebrauch waren. Die Mitgliedstaaten können jedoch das Inverkehrbringen solcher Messinstrumente einschränken oder verbieten.\n3. Die in Absatz 1 Buchstabe b genannte Beschränkung gilt nicht für:\n    Messinstrumente, die am 3. Oktober 2007 älter als 50 Jahre sind,\n    Barometer (ausgenommen Barometer im Sinne von Buchstabe a) bis zum 3. Oktober 2009. \n4. Bis zum 3. Oktober 2009 prüft die Kommission, ob für quecksilberhaltige Sphygmomanometer und andere quecksilberhaltige Messinstrumente zur Verwendung im medizinischen Bereich oder für andere gewerbliche und industrielle Zwecke zuverlässige, technisch und wirtschaftlich durchführbare und weniger bedenkliche Alternativen verfügbar sind. Auf der Grundlage dieser Prüfung oder sobald neue Erkenntnisse über zuverlässige und weniger bedenkliche Alternativen für quecksilberhaltige Sphygmomanometer und andere quecksilberhaltige Messinstrumente vorliegen, unterbreitet die Kommission gegebenenfalls einen Legislativvorschlag, um die Beschränkung nach Absatz 1 auf Sphygmomanometer und andere Messinstrumente zur Verwendung im medizinischen Bereich oder für andere gewerbliche und industrielle Zwecke auszudehnen, so dass quecksilberhaltige Messinstrumente nicht mehr zum Einsatz kommen, wann immer dies technisch und wirtschaftlich durchführbar ist.","18. 不得作为物质或者制剂的成分投放市场或者用作以下用途：\na) 防止微生物，植物或动物对于以下物品的污染；\n-船的船体；\n-笼子，浮标，网及其他用于鱼或贝类养殖的任何装置或设备；\n-完全或部分潜在水里的装置或设备;\nb)木材防腐；\nc) 用于重型工业纺织品和用于制造该纺织品的纱线浸泡；\nd) 用于处理各种工业废水。\n18a:\n1.以下情况下不得投放市场：\n-在体温计; 在销售给普通公众的某些等测量仪器（如压力计，气压计，血压计，温度计比体温计等）\n2.第1段的限制不适用于2009年4月3日前已经投入使用的测量工具。但是，成员国可以限制或禁止此类测量仪器投放市场。\n3.在1（b）中所述的限制不用于：\n（a）在2007年10月3日已超过50年的测量仪器，\n（b）气压表（（a）中所述气压表除外）可豁免至2009年10月3日。\n4. 2009年10月3日前，委员会需要调查清楚，对于那些在医疗领域使用或者应用于其他商业及工业的含汞血压计及其他含汞的测量仪器来说，是否存在一个可靠准确、技术和经济上可实施以及不会令人产生过多疑虑的替代品。基于此调查，抑或如果我们发现上述所说的那种对于含汞血压计及其他含汞的测量仪器来说可靠准确、不会令人产生过多疑虑的替代品存在的话，那么委员会应该在可能的情况下呈交一份立法建议书，如果可能，将第1段中的限制进一步扩展到在医疗领域使用或者应用于其他商业及工业的含汞血压计及其他含汞的测量仪器。这样，只要技术和经济上可行，含汞的测量仪器将淘汰。"]
[null,{"$f":"IF($B$1=\"English\",C591,IF($B$1=\"Deutsch\",D591,IF($B$1=\"中文\",E591,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used, as substance or as mixtures in aerosol dispensers where these aerosol dispensers are intended for supply to the general public for entertainment and decorative purposes such as the following:\n— metallic glitter intended mainly for decoration,\n— artificial snow and frost,\n— ‘whoopee’ cushions,\n— silly string aerosols,\n— imitation excrement,\n— horns for parties,\n— decorative flakes and foams,\n— artificial cobwebs,\n— stink bombs.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances, suppliers shall ensure before the placing on the market that the packaging of aerosol dispensers referred to above is marked visibly, legibly and indelibly with:\n‘For professional users only’.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the aerosol dispensers referred to Article 8 (1a) of Council Directive 75/324/EEC (***).\n4. The aerosol dispensers referred to in paragraphs 1 and 2 shall not be placed on the market unless they conform to the requirements indicated.\n___________\n(***) OJ L 147, 9.6.1975, p. 40."},"1. Shall not be used, as substance or as mixtures in aerosol dispensers where these aerosol dispensers are intended for supply to the general public for entertainment and decorative purposes such as the following:\n— metallic glitter intended mainly for decoration,\n— artificial snow and frost,\n— ‘whoopee’ cushions,\n— silly string aerosols,\n— imitation excrement,\n— horns for parties,\n— decorative flakes and foams,\n— artificial cobwebs,\n— stink bombs.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances, suppliers shall ensure before the placing on the market that the packaging of aerosol dispensers referred to above is marked visibly, legibly and indelibly with:\n‘For professional users only’.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the aerosol dispensers referred to Article 8 (1a) of Council Directive 75/324/EEC (***).\n4. The aerosol dispensers referred to in paragraphs 1 and 2 shall not be placed on the market unless they conform to the requirements indicated.\n___________\n(***) OJ L 147, 9.6.1975, p. 40.","1. Dürfen weder als Stoff noch als Gemisch in Aerosolpackungen verwendet werden, die dazu bestimmt sind, für Unterhaltungs- und Dekorationszwecke an die breite Öffentlichkeit abgegeben zu werden, wie z.B. für\n    Dekorationen mit metallischen Glanzeffekten, insbesondere für Festlichkeiten,\n    künstlichen Schnee und Reif,\n    unanständige Geräusche,\n    Luftschlangen,\n    Scherzexkremente,\n    Horntöne für Vergnügungen,\n    Schäume und Flocken zu Dekorationszwecken,\n    künstliche Spinnweben,\n    Stinkbomben. \n2. Unbeschadet der Anwendung sonstiger gemeinschaftlicher Vorschriften auf dem Gebiet der Einstufung, Verpackung und Etikettierung von Stoffen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung der oben genannten Aerosolpackungen gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n\"Nur für gewerbliche Anwender\".\n3. Abweichend davon gelten die Absätze 1 und 2 nicht für die in Artikel 8 Absatz 1 Buchstabe a der Richtlinie 75/324/EWG des Rates 2 genannten Aerosolpackungen.\n4. Die in Absatz 1 und 2 genannten Aerosolpackungen dürfen nur in Verkehr gebracht werden, wenn sie den dort aufgeführten Anforderungen entsprechen.","1.不得作为物质或者制剂的成分用在供应给广大市民的气溶胶喷雾器中用于娱乐或装饰的目的，如：\n-装饰用的金属闪光亮片\n-人工造雪和人造霜\n-”whoopee“软垫\n-喷射彩条\n-人造粪便\n-聚会时用的号角\n-装饰片和泡沫\n-人造蜘蛛网\n-臭气弹等\n2.在不违反其它有关危险物质和制剂分类、包装和标识欧盟法规的情况下，供应商必须保证，在销售前这些气溶胶喷雾器的包装上以清晰可见且不易磨损方式标示，\"For professional users only 仅供专业人士使用\"。\n3.作为免除项目，第1和2项，不适用于委员会指令75/324/EEC（***）第8（1a）款所述的喷雾器。\n4.在第1和第2款所述的喷雾器不得投放市场，除非他们符合要求。\n___________\n(***) OJ L 147, 9.6.1975, p. 40."]
[null,{"$f":"IF($B$1=\"English\",C592,IF($B$1=\"Deutsch\",D592,IF($B$1=\"中文\",E592,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight where the substance or mixture is used in adhesives or spray paints intended for supply to the general public."},"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight where the substance or mixture is used in adhesives or spray paints intended for supply to the general public.","Darf nicht als Stoff oder in Gemischen in Konzentrationen von > 0,1 Gew: % in für die Abgabe an die breite Öffentlichkeit bestimmten Klebstoffen und Farbsprühdosen in Verkehr gebracht oder verwendet werden.","不得投放市场或使用在销售给大众的粘着剂及喷漆中用作物质或制剂的成分，如果其浓度大于等于0.1%"]
[null,{"$f":"IF($B$1=\"English\",C593,IF($B$1=\"Deutsch\",D593,IF($B$1=\"中文\",E593,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market."},"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.","1. Darf nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2. Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.","1.不可用于纺织品，例如服装、内衣及家庭日用织品等会与皮肤接触的物品\n2.产品不满足第1项，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C594,IF($B$1=\"Deutsch\",D594,IF($B$1=\"中文\",E594,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight for any use except:\n— as an intermediate of synthesis, or,\n— as a process solvent in closed chemical applications for chlorination reactions, or,\n— in the manufacture of 1,3,5-triamino — 2,4,6- trinitrobenzene (TATB)."},"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight for any use except:\n— as an intermediate of synthesis, or,\n— as a process solvent in closed chemical applications for chlorination reactions, or,\n— in the manufacture of 1,3,5-triamino — 2,4,6- trinitrobenzene (TATB).","Darf weder als Stoff noch in Gemischen in einer Konzentration von >0,1 Gew. % zu keinem Verwendungszweck in Verkehr gebracht oder verwendet werden, außer:\n    als Synthese-Zwischenprodukt,\n    als Prozesslösungsmittel in geschlossenen chemischen Anwendungen für Chlorreaktionen oder\n    bei der Herstellung von 1,3,5-Trinitro-2,4,6-Triaminobenzol (TATB). ","不得投放市场或以浓度大于等于0.1%用作物质或制剂的成分的所有用途，除了以下项目：\n- 合成用的中间体；或\n- 进行密闭的氯化反应时的工艺用溶剂；或\n- 生产1,3,5-三胺基-2,4,6-三硝基苯（TATB）"]
[null,{"$f":"IF($B$1=\"English\",C595,IF($B$1=\"Deutsch\",D595,IF($B$1=\"中文\",E595,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market."},"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.","1. Darf nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2. Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.","1.不可用于纺织品，例如服装、内衣及家庭日用织品等会与皮肤接触的物品\n2.产品不满足第1项，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C596,IF($B$1=\"Deutsch\",D596,IF($B$1=\"中文\",E596,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is acting as biocide in free association paint.\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture acts as biocide to prevent the fouling by micro-organisms, plants or animals of:\n(a) all craft irrespective of their length intended for use in marine, coastal, estuarine and inland waterways and lakes;\n(b) cages, floats, nets and any other appliances or equipment used for fish or shellfish farming;\n(c) any totally or partly submerged appliance or equipment.\n3. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters.\n4. Tri-substituted organostannic compounds:\n(a) Tri-substituted organostannic compounds such as tributyltin (TBT) compounds and triphenyltin (TPT) compounds shall not be used after 1 July 2010 in articles where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin.\n(b) Articles not complying with point (a) shall not be placed on the market after 1 July 2010, except for articles that were already in use in the Community before that date.\n5. Dibutyltin (DBT) compounds:\n(a) Dibutyltin (DBT) compounds shall not be used after 1 January 2012 in mixtures and articles for supply to the general public where the concentration in the mixture or the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin.\n(b) Articles and mixtures not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date.\n(c) By way of derogation, points (a) and (b) shall not apply until 1 January 2015 to the following articles and mixtures for supply to the general public:\n— one-component and two-component room temperature vulcanisation sealants (RTV-1 and RTV-2 sealants) and adhesives,\n— paints and coatings containing DBT compounds as catalysts when applied on articles,\n— soft polyvinyl chloride (PVC) profiles whether by themselves or coextruded with hard PVC,\n— fabrics coated with PVC containing DBT compounds as stabilisers when intended for outdoor applications,\n— outdoor rainwater pipes, gutters and fittings, as well as covering material for roofing and façades,\n(d) By way of derogation, points (a) and (b) shall not apply to materials and articles regulated under Regulation (EC) No 1935/2004. 6. Dioctyltin (DOT) compound:\n(a) Dioctyltin (DOT) compounds shall not be used after 1 January 2012 in the following articles for supply to, or use by, the general public, where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin:\n— textile articles intended to come into contact with the skin,\n— gloves,\n— footwear or part of footwear intended to come into contact with the skin,\n— wall and floor coverings,\n— childcare articles,\n— female hygiene products,\n— nappies,\n— two-component room temperature vulcanisation moulding kits (RTV-2 moulding kits).\n(b) Articles not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date."},"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is acting as biocide in free association paint.\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture acts as biocide to prevent the fouling by micro-organisms, plants or animals of:\n(a) all craft irrespective of their length intended for use in marine, coastal, estuarine and inland waterways and lakes;\n(b) cages, floats, nets and any other appliances or equipment used for fish or shellfish farming;\n(c) any totally or partly submerged appliance or equipment.\n3. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters.\n4. Tri-substituted organostannic compounds:\n(a) Tri-substituted organostannic compounds such as tributyltin (TBT) compounds and triphenyltin (TPT) compounds shall not be used after 1 July 2010 in articles where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin.\n(b) Articles not complying with point (a) shall not be placed on the market after 1 July 2010, except for articles that were already in use in the Community before that date.\n5. Dibutyltin (DBT) compounds:\n(a) Dibutyltin (DBT) compounds shall not be used after 1 January 2012 in mixtures and articles for supply to the general public where the concentration in the mixture or the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin.\n(b) Articles and mixtures not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date.\n(c) By way of derogation, points (a) and (b) shall not apply until 1 January 2015 to the following articles and mixtures for supply to the general public:\n— one-component and two-component room temperature vulcanisation sealants (RTV-1 and RTV-2 sealants) and adhesives,\n— paints and coatings containing DBT compounds as catalysts when applied on articles,\n— soft polyvinyl chloride (PVC) profiles whether by themselves or coextruded with hard PVC,\n— fabrics coated with PVC containing DBT compounds as stabilisers when intended for outdoor applications,\n— outdoor rainwater pipes, gutters and fittings, as well as covering material for roofing and façades,\n(d) By way of derogation, points (a) and (b) shall not apply to materials and articles regulated under Regulation (EC) No 1935/2004. 6. Dioctyltin (DOT) compound:\n(a) Dioctyltin (DOT) compounds shall not be used after 1 January 2012 in the following articles for supply to, or use by, the general public, where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin:\n— textile articles intended to come into contact with the skin,\n— gloves,\n— footwear or part of footwear intended to come into contact with the skin,\n— wall and floor coverings,\n— childcare articles,\n— female hygiene products,\n— nappies,\n— two-component room temperature vulcanisation moulding kits (RTV-2 moulding kits).\n(b) Articles not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date.","1. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, wenn diese als Biozide in Farben wirken, deren Bestandteile chemisch nicht gebunden sind.\n2. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die als Biozide dazu dienen, an folgenden Gegenständen den Bewuchs durch Mikroorganismen, Pflanzen oder Tiere zu verhindern:\n    an allen Fahrzeugen unabhängig von ihrer Länge, die auf Seewasserstraßen, Wasserstraßen im Küsten- und Ästuarbereich, Binnenwasserstraßen sowie Seen eingesetzt werden;\n    an Kästen, Schwimmern, Netzen sowie anderen Geräten oder Einrichtungen für die Fisch- und Muschelzucht;\n    an völlig oder teilweise untergetauchten Geräten oder Einrichtungen jeder Art. \n3. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Aufbereitung von Wasser im industriellen, gewerblichen und kommunalen Bereich bestimmt sind.\n4. Trisubstituierte zinnorganische Verbindungen:\n    Trisubstituierte zinnorganische Verbindungen wie etwa Tributylzinnverbindungen (TBT) und Triphenylzinnverbindungen\n    (TPT) dürfen nach dem 1. Juli 2010 nicht mehr in Erzeugnissen verwendet werden, wenn die Konzentration von Zinn in dem Erzeugnis oder in Teilen davon 0,1 Gewichtsprozent übersteigt.\n    Erzeugnisse, die nicht mit Buchstabe a in Einklang stehen, dürfen nach dem 1. Juli 2010 nicht mehr in Verkehr gebracht werden; ausgenommen davon sind Erzeugnisse, die bereits vor diesem Zeitpunkt in der Gemeinschaft in Verwendung waren. \n5. Dibutylzinnverbindungen (DBT):\n    Dibutylzinnverbindungen (DBT) dürfen nach dem 1. Januar 2012 nicht mehr in Gemischen und Erzeugnissen verwendet werden, die dazu bestimmt sind, an die breite Öffentlichkeit abgegeben zu werden, wenn die Konzentration von Zinn in dem Gemisch oder Erzeugnis bzw. in Teilen davon\n    0,1 Gewichtsprozent übersteigt.\n    Erzeugnisse und Gemische, die nicht mit Buchstabe a in Einklang stehen, dürfen nach dem 1. Januar 2012 nicht mehr in Verkehr gebracht werden; ausgenommen davon sind Erzeugnisse, die bereits vor diesem Zeitpunkt in der Gemeinschaft in Verwendung waren.\n    Abweichend davon gelten die Buchstaben a und b bis zum 1. Januar 2015 nicht für die nachstehenden Erzeugnisse und Gemische, die für die Abgabe an die breite Öffentlichkeit bestimmt sind:\n        Ein-Komponenten- und Zwei-Komponenten-Raumtemperaturvulkanisierungs-Dichtungsmittel (RTV-1- und RTV-2- Dichtungsmittel) und Klebstoffe;\n        Farben und Beschichtungen, die DBT-Verbindungen als Katalysatoren enthalten, wenn diese auf Erzeugnissen aufgetragen sind;\n        weiche Polyvinylchlorid-(PVC)-Profile, mit Hart-PVC koextrudiert oder nicht;\n        Gewebe, die mit PVC beschichtet sind, das DBT-Verbindungen als Stabilisatoren enthält, wenn sie für die Verwendung im Freien vorgesehen sind;\n        im Freien befindliche Regenwasserleitungen, Regenrinnen und Anschlussteile sowie Dach- und Fassadenverkleidungsmaterial. \n    Abweichend davon gelten die Buchstaben a und b nicht für Materialien und Erzeugnisse, die unter die Verordnung (EG) Nr. 1935/2004 fallen. \n6. Dioctylzinnverbindungen (DOT):\n    Dioctylzinnverbindungen (DOT) dürfen nach dem 1. Januar 2012 nicht mehr in den nachstehend aufgeführten Erzeugnissen verwendet werden, die dazu bestimmt sind, an die breite Öffentlichkeit abgegeben oder von dieser verwendet zu werden, wenn die Konzentration von Zinn in dem Erzeugnis oder in Teilen davon 0,1 Gewichtsprozent übersteigt:\n        Textilartikel, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen;\n        Handschuhe;\n        Schuhe oder Teile davon, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen;\n        Wand- und Bodenverkleidungen;\n        Babyartikel;\n        Damenhygieneartikel;\n        Windeln;\n        Zwei-Komponenten-Raumtemperaturvulkanisierungs-Abform-Sets (RTV-2-Abform-Sets). \n    Erzeugnisse, die nicht mit Buchstabe a in Einklang stehen, dürfen nach dem 1. Januar 2012 nicht mehr in Verkehr gebracht werden; ausgenommen davon sind Erzeugnisse, die bereits vor diesem Zeitpunkt in der Gemeinschaft in Verwendung waren. ","1．作为自由组合涂料的生物杀虫剂的物质或制剂的成分不得投放市场\n2.不得作为物质或者制剂的成分投放市场或者用于防止微生物，植物或动物对于以下物品的污染：\n（a）航行于海洋、海岸、河口和内河、湖泊的船舶(无论船舶长度)；\n（b）笼子，浮标，网及其他用于鱼或贝类养殖的任何装置或设备；\n（c）任何完全或部分潜在水里的装置或设备;\n3. 用于处理各种工业废水。\n4. 三取代物有机锡化合物：\n（a）三取代物有机锡化合物，如三丁基锡（TBT）化合物和三苯基锡（TPT）化合物，在2010年7月1日之后不得用于产品，当其中锡的含量在成品或一部分其浓度超过0.1的重量百分比。\n（b）不符合(a)要求的产品，不可以在2010年7月1日在市场上销售；除非在这个日期之前已经被公众使用的产品。\n5. 二丁基锡（DBT）化合物：\n（a）二丁基锡（DBT）化合物在2012年1月1日之后不得作为配制品和成品在市场上销售给大众，当其成品或部件中锡的含量其浓度超过0.1的重量百分比。\n（b）不符合(a)要求的产品，不可以在2012年1月1日在市场上销售；除非在这个日期之前已经被公众使用的产品。\n（c）作为免除项目，条款（a）和（b）在2015年1月1号前对以下要提供给公众产品及配制品可以豁免：\n-单组分和双组分室温硫化密封剂（RTV-1和RTV-2密封剂）和粘合剂;\n-已经涂敷到物品上的含有二丁基锡作为催化剂在颜料和涂层；\n-单一的软质的聚氯乙烯（PVC）型材，或硬质软质聚氯乙烯（PVC）复合的型材;\n-用于室外的织物，如果上面涂覆有以DBT二丁基锡作为稳定剂的聚氯乙烯PVC涂层;\n-位于户外雨水管道，排水沟和配件，以及屋顶和覆面材料。\n（d）作为免除项目，条款（a）和（b）不适用于欧盟法规(EC) No 1935/2004规范的产品及配制品。\n6. 二辛基锡（DOT）化合物：\n（a）二辛基锡（DOT）化合物在2012年1月1日之后不得用于以下销售给大众的物品中，当其成品或部件中锡的含量其浓度超过0.1的重量百分比：\n-会与皮肤接触的纺织产品\n-手套\n-会与皮肤接触的鞋子或其一部分；\n-墙壁和地板覆盖物; \n-儿童用品\n-女士卫生产品\n-纸尿片\n- 双组分室温硫化模型套（RTV-2的模型套）。\n（b）不符合(a)要求的产品，不可以在2012年1月1日在市场上销售；除非在这个日期之前已经被公众使用的产品。"]
[null,{"$f":"IF($B$1=\"English\",C597,IF($B$1=\"Deutsch\",D597,IF($B$1=\"中文\",E597,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[4-[4,4'-bis(dimethylamino) benzhydrylidene]cyclohexa-2,5-dien-1-ylidene]dimethylammonium chloride (C.I. Basic Violet 3) [with ≥ 0.1% of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]"},"[4-[4,4'-bis(dimethylamino) benzhydrylidene]cyclohexa-2,5-dien-1-ylidene]dimethylammonium chloride (C.I. Basic Violet 3) [with ≥ 0.1% of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]","[4-[4,4'-Bis(dimethylamino) benzhydryliden]cyclohexa-2,5-dien-1-yliden]dimethylammonium chlorid\n(C.I. Basic Violet 3) [mit ≥ 0.1% Michler’s Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","\n[4 - [4,4' - 双（二甲氨基）二苯亚甲基]环己-2,5 - 二烯-1 - 亚基]二甲基氯化铵（CI碱性紫3）[含≥0.1％ 米氏酮（EG-Nr.202-027-5）或者米氏碱（EC 202-959-2）]"]
[null,{"$f":"IF($B$1=\"English\",C598,IF($B$1=\"Deutsch\",D598,IF($B$1=\"中文\",E598,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-tris[(2S and 2R)-2,3-epoxypropyl]-1,3,5-triazine-2,4,6-(1H,3H,5H)-trione (β-TGIC) "},"1,3,5-tris[(2S and 2R)-2,3-epoxypropyl]-1,3,5-triazine-2,4,6-(1H,3H,5H)-trione (β-TGIC) ","1,3,5-Tris[(2S und 2R)-2,3-epoxypropyl]-1,3,5-triazin-2,4,6-(1H,3H,5H)-trion\n(β-TGIC)","\n“1,3,5 - 三[（2R和2S）-2,3 - 环氧丙基] -1,3,5 - 三嗪-2,4,6 - （1H，3H，5H） - 三酮(β-TGIC)"]
[null,{"$f":"IF($B$1=\"English\",C599,IF($B$1=\"Deutsch\",D599,IF($B$1=\"中文\",E599,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-bis(2-methoxyethoxy)ethane (TEGDME; triglyme)"},"1,2-bis(2-methoxyethoxy)ethane (TEGDME; triglyme)","1,2-Bis(2-methoxyethoxy)ethan\n(TEGDME; triglyme)","“1,2 - 二（2 - 甲氧基乙氧基）乙烷\n（TEGDME，三甘醇二甲醚）“"]
[null,{"$f":"IF($B$1=\"English\",C600,IF($B$1=\"Deutsch\",D600,IF($B$1=\"中文\",E600,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-bis(dimethylamino)-4''-(methylamino)trityl alcohol [with ≥ 0,1 % of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]"},"4,4'-bis(dimethylamino)-4''-(methylamino)trityl alcohol [with ≥ 0,1 % of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]","4,4'-Bis(dimethylamino)-4''-(methylamino)tritylalkohol\n[mit ≥ 0.1% Michler’s Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","4,4-二[(二甲氨基)苯基]-4-甲氨基苯甲醇\n[随着≥0.1％米氏酮（EC编号202-027-5）或米氏碱（EC编号202-959-2）]"]
[null,{"$f":"IF($B$1=\"English\",C601,IF($B$1=\"Deutsch\",D601,IF($B$1=\"中文\",E601,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead(II) bis(methanesulfonate)"},"Lead(II) bis(methanesulfonate)","Blei(II)bis(methansulfonat)","铅（II）二（甲磺酸）"]
[null,{"$f":"IF($B$1=\"English\",C602,IF($B$1=\"Deutsch\",D602,IF($B$1=\"中文\",E602,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dimethoxyethane; ethylene glycol dimethyl ether (EGDME)"},"1,2-dimethoxyethane; ethylene glycol dimethyl ether (EGDME)","1,2-Dimethoxyethan; Ethylenglycoldimethylether\n(EGDME)"," 乙二醇二甲醚; 乙二醇二甲醚\n(EGDME)"]
[null,{"$f":"IF($B$1=\"English\",C603,IF($B$1=\"Deutsch\",D603,IF($B$1=\"中文\",E603,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diboron trioxide"},"Diboron trioxide","Dibortrioxid","三氧化二硼"]
[null,{"$f":"IF($B$1=\"English\",C604,IF($B$1=\"Deutsch\",D604,IF($B$1=\"中文\",E604,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"α,α-Bis[4-(dimethylamino)phenyl]-4 (phenylamino)naphthalene-1-methanol (C.I. Solvent Blue 4) [with ≥ 0.1% of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]"},"α,α-Bis[4-(dimethylamino)phenyl]-4 (phenylamino)naphthalene-1-methanol (C.I. Solvent Blue 4) [with ≥ 0.1% of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]","alpha,alpha-Bis[4-(dimethylamino)phenyl]-4-(phenylamino)naphthalin-1-methanol\n(C.I. Solvent Blue 4) [mit ≥ 0.1% Michler's Keton (EG- Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","\nα，α-双[4 - （二甲基氨基）苯基] -4（苯基氨基）萘-1 - 甲醇（溶剂蓝4） [与米氏酮的≥0.1％（EC号202-027-5）或米氏碱（EC号202-959-2）]"]
[null,{"$f":"IF($B$1=\"English\",C605,IF($B$1=\"Deutsch\",D605,IF($B$1=\"中文\",E605,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinane-2,4,6-trione (TGIC)"},"1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinane-2,4,6-trione (TGIC)","1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinan-2,4,6-trion\n(TGIC)","1,3,5-三缩水甘油-S-三嗪三酮 (TGIC)"]
[null,{"$f":"IF($B$1=\"English\",C606,IF($B$1=\"Deutsch\",D606,IF($B$1=\"中文\",E606,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-bis(dimethylamino)benzophenone (Michler's ketone)"},"4,4'-bis(dimethylamino)benzophenone (Michler's ketone)","4,4'-Bis(dimethylamino)benzophenon\n(Michler’s Keton)","4,4'-二(N,N-二甲氨基)二苯甲酮（米氏酮）"]
[null,{"$f":"IF($B$1=\"English\",C607,IF($B$1=\"Deutsch\",D607,IF($B$1=\"中文\",E607,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N,N',N'-tetramethyl-4,4'-methylenedianiline (Michler's base)"},"N,N,N',N'-tetramethyl-4,4'-methylenedianiline (Michler's base)"," N,N,N',N'-Tetramethyl-4,4'-methylendianilin\n(Michler’s Base)","4,4'-(對二甲氨基)二苯基甲烷(米氏碱)"]
[null,{"$f":"IF($B$1=\"English\",C608,IF($B$1=\"Deutsch\",D608,IF($B$1=\"中文\",E608,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formamide"},"Formamide","Formamid","甲酰胺"]
[null,{"$f":"IF($B$1=\"English\",C609,IF($B$1=\"Deutsch\",D609,IF($B$1=\"中文\",E609,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[4-[[4-anilino-1-naphthyl][4-(dimethylamino)phenyl]methylene]cyclohexa-2,5-dien-1-ylidene] dimethylammonium chloride (C.I. Basic Blue 26) [with ≥ 0,1% of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]"},"[4-[[4-anilino-1-naphthyl][4-(dimethylamino)phenyl]methylene]cyclohexa-2,5-dien-1-ylidene] dimethylammonium chloride (C.I. Basic Blue 26) [with ≥ 0,1% of Michler's ketone (EC No. 202-027-5) or Michler's base (EC No. 202-959-2)]","[4-[[4-Anilino-1-naphthyl][4-(dimethylamino)phenyl]methylen]cyclohexa-2,5-dien-1-yliden] dimethylammonium chlorid\n(C.I. Basic Blue 26) [mit ≥ 0,1% Michler’s Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","[4 - [[4 - 苯胺基-1 - 萘基] [4 - （二甲基氨基）苯基]亚甲基]环己-2,5 - 二烯-1 - 亚基]二甲基氯化铵（碱性蓝26) [与米氏酮的≥0.1％（EC号202-027-5）或米氏碱（EC号202-959-2）]"]
[null,{"$f":"IF($B$1=\"English\",C610,IF($B$1=\"Deutsch\",D610,IF($B$1=\"中文\",E610,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- formulation of printing and writing inks\n- paper coloring\n- mixtures such as windscreen washing agents"},"- formulation of printing and writing inks\n- paper coloring\n- mixtures such as windscreen washing agents","- Druck- und Schreibtinten\n- Papierfärbung\n- Mischungen wie Windschutzscheibenreiniger","- 印刷和书写墨水的组分\n- 纸的染色\n- 配制品，如挡风玻璃清洁器"]
[null,{"$f":"IF($B$1=\"English\",C611,IF($B$1=\"Deutsch\",D611,IF($B$1=\"中文\",E611,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- formulation of inks, cleaners, and coatings\n- paper coloring, packaging, textiles, plastic products, and other types of articles\n- diagnostic and analytical applications."},"- formulation of inks, cleaners, and coatings\n- paper coloring, packaging, textiles, plastic products, and other types of articles\n- diagnostic and analytical applications.","- Ansetzen von Tinten, Reinigern und Beschichtungen\n- Färbung von Papier, Verpackung, Textilien, Kunsstoffprodukten und anderen Artikeln\n- Diagnose- und Analyseanwendungen","- 油墨，清洁剂和涂料的组分\n- 纸张染色，包装，纺织，塑料制品等其他物品\n- 诊断和分析应用"]
[null,{"$f":"IF($B$1=\"English\",C612,IF($B$1=\"Deutsch\",D612,IF($B$1=\"中文\",E612,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- paper coloring and inks supplied in printer cartridges and ball pens\n- staining of dried plants\n- marker for increasing the visibility of liquids\n- staining in microbial and clinical laboratories"},"- paper coloring and inks supplied in printer cartridges and ball pens\n- staining of dried plants\n- marker for increasing the visibility of liquids\n- staining in microbial and clinical laboratories","- Papierfarbe und -tinten in Druckerpatronen und Kugelschreibern\n- Färbung von getrockneten Pflanzen\n- Marker zur Erhöhung der Sichtbarkeit von Flüssigkeiten\n- Färbung in mikrobiellen und klinischen Laboren","- 纸张颜色和打印机墨盒及墨水笔\n- 干植物染色\n- 标记，以提高液体的清晰度\n- 在微生物和临床实验室中染色"]
[null,{"$f":"IF($B$1=\"English\",C613,IF($B$1=\"Deutsch\",D613,IF($B$1=\"中文\",E613,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvent\n- processing aid in the manufacture and formulation of industrial chemicals\n- brake fluids and repair of motor vehicles"},"- solvent\n- processing aid in the manufacture and formulation of industrial chemicals\n- brake fluids and repair of motor vehicles","- Lösungsmittel\n- Prozesshilfsstoff für Industriechemikalien\n- Bremsflüssigkeiten und Reperatur von Kfz","-溶剂\n- 工艺辅料和工业化学品的构成\n- 刹车油和机动车维修"]
[null,{"$f":"IF($B$1=\"English\",C614,IF($B$1=\"Deutsch\",D614,IF($B$1=\"中文\",E614,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solvent\n- processing aid of industrial chemicals, including use as an electrolyte solvent in lithium batteries"},"- solvent\n- processing aid of industrial chemicals, including use as an electrolyte solvent in lithium batteries","- Lösungsmittel\n- Fertigungshilfsstoff für Industriechemikalien, inkl. Elektrolyt in Lithiumbatterien","- 溶剂\n- 制造业辅助料用于工业化学品，包括电解质的锂电池"]
[null,{"$f":"IF($B$1=\"English\",C615,IF($B$1=\"Deutsch\",D615,IF($B$1=\"中文\",E615,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- solder mask ink \n- electrical insulation material\n- resin moulding systems\n- laminated sheeting\n- silk screen printing\n- coatings\n- tools\n- adhesives\n- lining materials\n- stabilisers for plastics"},"- solder mask ink \n- electrical insulation material\n- resin moulding systems\n- laminated sheeting\n- silk screen printing\n- coatings\n- tools\n- adhesives\n- lining materials\n- stabilisers for plastics","- Lötmasken\n- Isolationsmaterial für Elektriktische Anwendungen\n- Harzspritzguss\n- Verbundplatten\n- Siebdruck\n- Beschichtungen\n- Werkzeug\n- Klebstoffe\n- Futterstoff\n- Stabilisator für Kunststoffe\n\n\n\n","- 阻焊层\n- 绝缘材料用于电气应用\n- 树脂注射\n- 复合板\n- 网版印刷\n- 涂层\n- 工具\n- 胶粘剂\n- 家庭日用织品\n- 稳定剂用于塑料\n\n\n\n"]
[null,{"$f":"IF($B$1=\"English\",C616,IF($B$1=\"Deutsch\",D616,IF($B$1=\"中文\",E616,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- hardener in resins and coatings\n- inks for the printed circuit board industry\n- electrical insulation material\n- resin moulding systems\n- laminated sheeting\n- silk screen printing coatings\n- tools\n- adhesives\n- lining materials\n- stabilisers for plastics"},"- hardener in resins and coatings\n- inks for the printed circuit board industry\n- electrical insulation material\n- resin moulding systems\n- laminated sheeting\n- silk screen printing coatings\n- tools\n- adhesives\n- lining materials\n- stabilisers for plastics","- Härter für Harze und Beschichtungen\n- Tinten für Leiterplatten-Industrie\n- Isolationsmaterial für Elektriktrische Anwendungen\n- Harzspritzguss\n- Verbundplatten\n- Siebdruckbeschichtungen\n- Werkzeuge\n- Klebstoffe\n- Futtermaterial\n- Stabilisatoren für Kunststoffe","- 硬化剂用于树脂和涂料\n- 油墨用于印刷电路板产业\n- 绝缘材料用于电气应用\n- 树脂注射\n- 复合板\n- 网版印刷涂料\n- 工具\n- 胶粘剂\n- 家庭日用织品\n- 稳定剂用于塑料"]
[null,{"$f":"IF($B$1=\"English\",C617,IF($B$1=\"Deutsch\",D617,IF($B$1=\"中文\",E617,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- writing inks and potentially other inks\n- coloring a variety of materials"},"- writing inks and potentially other inks\n- coloring a variety of materials","- Tinte zum Schreiben und andere Tinten\n- Färbung von verschiedenen Materialien","- 墨水用于书写及其他墨水\n- 不同材料的染色"]
[null,{"$f":"IF($B$1=\"English\",C618,IF($B$1=\"Deutsch\",D618,IF($B$1=\"中文\",E618,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- intermediate in the manufacture of coloring and other substances.\n- additive (photosensitiser) in colors and pigments\n- dry film products\n- process chemical in the production of electronic circuit boards"},"- intermediate in the manufacture of coloring and other substances.\n- additive (photosensitiser) in colors and pigments\n- dry film products\n- process chemical in the production of electronic circuit boards","- Zwischenprodukt bei der Herstellung von Farben und anderen Substanzen\n- Zusatz (Photosensibilisator) in Farben und Pigmenten\n- Trockenfilm Produkte\n- Prozesschemikalien bei der Herstellung von elektronischen Leiterplatten","- 中间产物在油漆和其他物质制造时\n- 附加（光敏剂）在涂料和颜料\n- 干薄膜产品\n- 化学工艺在生产电子电路板时"]
[null,{"$f":"IF($B$1=\"English\",C619,IF($B$1=\"Deutsch\",D619,IF($B$1=\"中文\",E619,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- glass and glass fibres\n- frits\n- ceramics\n- flame retardants\n- catalysts\n- industrial fluids\n- metallurgy\n- nuclear\n- electrical equipment\n- adhesives\n- inks/paints\n- film developing solutions\n- detergents and cleaners\n- reagent chemicals\n- biocides and insecticides"},"- glass and glass fibres\n- frits\n- ceramics\n- flame retardants\n- catalysts\n- industrial fluids\n- metallurgy\n- nuclear\n- electrical equipment\n- adhesives\n- inks/paints\n- film developing solutions\n- detergents and cleaners\n- reagent chemicals\n- biocides and insecticides","- Glas und Glasfasern\n- Fritten\n- Keramik\n- Flammhemmer\n- Katalysatoren\n- Industrieflüssigkeiten\n- Metallurgie\n- Atomkraft\n- elektrische Geräte\n- Klebstoffe\n- Tinten/Farben\n- Anwendungen bei der Filmentwicklung\n- Waschmittel und Reiniger\n- Reagenzchemikalien\n- Biozide und Insektizide","- 玻璃和玻璃纤维\n- 熔结\n- 陶瓷\n- 阻燃剂\n- 催化剂\n-工业流体\n- 冶金\n- 核电\n- 电气设备\n- 胶粘剂\n- 油墨/颜色\n- 显影剂\n- 洗涤剂和清洁剂\n- 化学试剂\n- 杀菌剂和杀虫剂"]
[null,{"$f":"IF($B$1=\"English\",C620,IF($B$1=\"Deutsch\",D620,IF($B$1=\"中文\",E620,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- plating processes (both electrolytic and electroless) for electronic components (such as printed circuit boards)\n- batteries "},"- plating processes (both electrolytic and electroless) for electronic components (such as printed circuit boards)\n- batteries ","- Beschichtungsprozesse (elektrolytisch und stromlos) für elektronische Komponenten (z.B. bedruckte Leiterplatten)\n- Batterien ","- 电镀工艺（包括电解和化学镀）用于电子元器件 (例如印刷电路板)\n- 电池"]
[null,{"$f":"IF($B$1=\"English\",C621,IF($B$1=\"Deutsch\",D621,IF($B$1=\"中文\",E621,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- intermediate in the manufacture of agrochemicals, pharmaceuticals and industrial chemicals\n- solvent\n- laboratory reagent for quality control purposes in forensic laboratories, hospitals, pharmaceutical companies, food and drinks manufacturers and research laboratories\n- plasticiser"},"- intermediate in the manufacture of agrochemicals, pharmaceuticals and industrial chemicals\n- solvent\n- laboratory reagent for quality control purposes in forensic laboratories, hospitals, pharmaceutical companies, food and drinks manufacturers and research laboratories\n- plasticiser","- Zwischenprodukt bei der Herstellung von Agrochemikalien, Pharmazeutika und Industriechemikalien\n- Lösungsmittel\n- Reagenzstoff für Qualitätskontrolle in der Gerichtsmedizin/Forensik, Krankenhäusern, Pharmaunternehmen, Essen- und Getränke-Hersteller und Forschungslabore\n- Weichmacher","- 农用化学品，医药和工业化学品制造中的中间体\n- 溶剂\n- 试剂用于法医/法医，医院，药厂，食品和饮料制造商和研究实验室的质量控制\n-塑化剂"]
[null,{"$f":"IF($B$1=\"English\",C622,IF($B$1=\"Deutsch\",D622,IF($B$1=\"中文\",E622,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- intermediate in the manufacture of colors and other substances"},"- intermediate in the manufacture of colors and other substances","- Zwischenprodukt bei der Herstellung von Farben und  anderen Substanzen","- 在颜料和其他物质制造的过渡产品"]
[null,{"$f":"IF($B$1=\"English\",C623,IF($B$1=\"Deutsch\",D623,IF($B$1=\"中文\",E623,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: (18_TSCA (Sec. 5(a)(2), Sec 6(h))"},"Tab: (18_TSCA (Sec. 5(a)(2), Sec 6(h))","Register: (18_TSCA (Sec. 5(a)(2), Sec 6(h))","Tab: (18_TSCA (Sec. 5(a)(2), Sec 6(h))"]
[null,{"$f":"IF($B$1=\"English\",C624,IF($B$1=\"Deutsch\",D624,IF($B$1=\"中文\",E624,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % in plastic- and elastomer parts"},"0,1 % in plastic- and elastomer parts","0,1 % in Kunststoff- und Elastomer-Teilen","在塑料和橡胶部件中，0.1％质量百分比 "]
[null,{"$f":"IF($B$1=\"English\",C625,IF($B$1=\"Deutsch\",D625,IF($B$1=\"中文\",E625,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"test report enclosed (optional)"},"test report enclosed (optional)","Testbericht beigelegt (optional)","附测试报告（可选项）"]
[null,{"$f":"IF($B$1=\"English\",C626,IF($B$1=\"Deutsch\",D626,IF($B$1=\"中文\",E626,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,01 % in PVC"},"0,01 % in PVC","0,01  % in PVC"," 在PVC中，0.1％质量百分比 "]
[null,{"$f":"IF($B$1=\"English\",C627,IF($B$1=\"Deutsch\",D627,IF($B$1=\"中文\",E627,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % in hard-PVC"},"0,1 % in hard-PVC","0,1  % in Hart-PVC mit Recyclat-Anteil","在硬质PVC中， 0.1％质量百分比 "]
[null,{"$f":"IF($B$1=\"English\",C628,IF($B$1=\"Deutsch\",D628,IF($B$1=\"中文\",E628,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % in colors on product parts"},"0,1 % in colors on product parts","0,1 % in Farben auf Produkt-Teilen","在产品零件上的颜料中，0.1％质量百分比 "]
[null,{"$f":"IF($B$1=\"English\",C629,IF($B$1=\"Deutsch\",D629,IF($B$1=\"中文\",E629,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"XRF X-ray fluorescence spectroscopy"},"XRF X-ray fluorescence spectroscopy","XRF X-ray fluorescence spectroscopy","XRF，X射线荧光光谱仪"]
[null,{"$f":"IF($B$1=\"English\",C630,IF($B$1=\"Deutsch\",D630,IF($B$1=\"中文\",E630,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm 18 PAK in total"},"10 ppm 18 PAK in total","10 ppm Summe 18 PAK","18种多环芳烃总量不超过10 ppm "]
[null,{"$f":"IF($B$1=\"English\",C631,IF($B$1=\"Deutsch\",D631,IF($B$1=\"中文\",E631,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ZEK 01.4-08"},"ZEK 01.4-08","ZEK 01.4-08","ZEK 01.4-08"]
[null,{"$f":"IF($B$1=\"English\",C632,IF($B$1=\"Deutsch\",D632,IF($B$1=\"中文\",E632,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Black plastic and elastomer parts, e.g. cables, grommets, soft grips"},"Black plastic and elastomer parts, e.g. cables, grommets, soft grips","Schwarze Kunststoff- und Elastomer-Teile, z. B. Kabel, Tüllen, Griffe","黑色的塑料和橡胶部件，如电缆，喷口，把手"]
[null,{"$f":"IF($B$1=\"English\",C633,IF($B$1=\"Deutsch\",D633,IF($B$1=\"中文\",E633,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Yes"},"Yes","Ja","是"]
[null,{"$f":"IF($B$1=\"English\",C634,IF($B$1=\"Deutsch\",D634,IF($B$1=\"中文\",E634,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"plasticizer"},"plasticizer","Weichmacher","塑化剂"]
[null,{"$f":"IF($B$1=\"English\",C635,IF($B$1=\"Deutsch\",D635,IF($B$1=\"中文\",E635,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"heavy metals"},"heavy metals","Schwermetalle","重金属"]
[null,{"$f":"IF($B$1=\"English\",C636,IF($B$1=\"Deutsch\",D636,IF($B$1=\"中文\",E636,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PAH polycyclical aromatic hydrocarbons"},"PAH polycyclical aromatic hydrocarbons","PAK Polyzyklische Aromatische Kohlenwasserstoffe","PAH 多环芳烃"]
[null,{"$f":"IF($B$1=\"English\",C637,IF($B$1=\"Deutsch\",D637,IF($B$1=\"中文\",E637,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"method of measurement"},"method of measurement","Messmethode","检测方法"]
[null,{"$f":"IF($B$1=\"English\",C638,IF($B$1=\"Deutsch\",D638,IF($B$1=\"中文\",E638,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: BST\nregulations for divisions Bosch Sensortec (BST)"},"Tab: BST\nregulations for divisions Bosch Sensortec (BST)","Register: BST\nRegelungen für Geschäftseinheit Bosch Sensortec (BST)","工作表：BST\n适用于博世传感器技术事业部(BST)的法规"]
[null,{"$f":"IF($B$1=\"English\",C639,IF($B$1=\"Deutsch\",D639,IF($B$1=\"中文\",E639,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: DC\nregulations for division Drive and Control Technology DC (Rexroth)"},"Tab: DC\nregulations for division Drive and Control Technology DC (Rexroth)","Register: DC\nRegelungen für Geschäftsbereich Drive and Control Technology DC (Rexroth)","工作表：DC\n适用于博世驱动和控制技术DC事业部的法规"]
[null,{"$f":"IF($B$1=\"English\",C640,IF($B$1=\"Deutsch\",D640,IF($B$1=\"中文\",E640,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Unknown"},"Unknown","Unbekannt","未知"]
[null,{"$f":"IF($B$1=\"English\",C641,IF($B$1=\"Deutsch\",D641,IF($B$1=\"中文\",E641,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Type of supplied material\n"},"Type of supplied material\n","Art des gelieferten Materials","供应给博世的材料类型"]
[null,{"$f":"IF($B$1=\"English\",C642,IF($B$1=\"Deutsch\",D642,IF($B$1=\"中文\",E642,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content of the delivered material. Exact designation of the material supplied (e.g. Battery, screw made of material xyz or cutting steel made of material 11SMN30, reference to IMDS ID, CDX material"},"Content of the delivered material. Exact designation of the material supplied (e.g. Battery, screw made of material xyz or cutting steel made of material 11SMN30, reference to IMDS ID, CDX material","Inhalt des gelieferten Materials. Genau Benennung des gelieferten Materials (z.B. Batterie, Schraube aus Werkstoff xyz oder Automatenstahl aus Werkstoff 11SMN30, Referenz zu IMDSID, CDX-Werkstoff)","交付材料的组成。供应的材料的确切名称（例如电池、由某某材料制成的螺钉或由11SMN30 材料制成的切割钢，参考 IMDS ID、CDX 材料）"]
[null,{"$f":"IF($B$1=\"English\",C643,IF($B$1=\"Deutsch\",D643,IF($B$1=\"中文\",E643,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other than mentioned above or unknown"},"Other than mentioned above or unknown","andere als oben genannt oder unbekannt","其他或未知"]
[null,{"$f":"IF($B$1=\"English\",C644,IF($B$1=\"Deutsch\",D644,IF($B$1=\"中文\",E644,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Battery"},"Battery","Batterie","电池"]
[null,{"$f":"IF($B$1=\"English\",C645,IF($B$1=\"Deutsch\",D645,IF($B$1=\"中文\",E645,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Assembled curcuit board; electronic assembly; electric assembly"},"Assembled curcuit board; electronic assembly; electric assembly","bestückte Leiterplatte; Elektronik-Baugruppe; Elektrik-Baugruppe","印刷电路板组件;电子组件;电器组件"]
[null,{"$f":"IF($B$1=\"English\",C646,IF($B$1=\"Deutsch\",D646,IF($B$1=\"中文\",E646,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Color;dye; varnish; coating; impregnation; similar material"},"Color;dye; varnish; coating; impregnation; similar material","Farbe; Farbstoff; Lack; Beschichtung; Imprägnierung; ähnliches Material","颜料;染料;油漆;涂料;浸漆;类似的材料"]
[null,{"$f":"IF($B$1=\"English\",C647,IF($B$1=\"Deutsch\",D647,IF($B$1=\"中文\",E647,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Auxiliary manufacturing material, also cooling lubricants not remaining in or on product"},"Auxiliary manufacturing material, also cooling lubricants not remaining in or on product","Fertigungshilfsstoff auch Kühlschmierstoff der nicht im oder am Produkt verbleibt","不在产品上有残余的制造辅助材料和冷却剂"]
[null,{"$f":"IF($B$1=\"English\",C648,IF($B$1=\"Deutsch\",D648,IF($B$1=\"中文\",E648,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Auxiliary manufacturing material, also cooling lubricants which remain in or on product"},"Auxiliary manufacturing material, also cooling lubricants which remain in or on product","Fertigungshilfsstoff auch Kühlschmierstoff der im oder am Produkt verbleibt","在产品上有残余的制造辅助材料和冷却剂"]
[null,{"$f":"IF($B$1=\"English\",C649,IF($B$1=\"Deutsch\",D649,IF($B$1=\"中文\",E649,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ceramics; glass; minerals"},"Ceramics; glass; minerals","Keramik; Glas; Mineralie","陶瓷;玻璃;矿物"]
[null,{"$f":"IF($B$1=\"English\",C650,IF($B$1=\"Deutsch\",D650,IF($B$1=\"中文\",E650,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Adhesive; sealing material; resins"},"Adhesive; sealing material; resins","Klebstoff; Dichtstoff; Harze","胶粘剂;密封胶;树脂"]
[null,{"$f":"IF($B$1=\"English\",C651,IF($B$1=\"Deutsch\",D651,IF($B$1=\"中文\",E651,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plastic; elastomer"},"Plastic; elastomer","Kunststoff; Elastomer","塑料;弹性体"]
[null,{"$f":"IF($B$1=\"English\",C652,IF($B$1=\"Deutsch\",D652,IF($B$1=\"中文\",E652,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Metal"},"Metal","Metall","金属"]
[null,{"$f":"IF($B$1=\"English\",C653,IF($B$1=\"Deutsch\",D653,IF($B$1=\"中文\",E653,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fabric, leather"},"Fabric, leather","Textilie; Leder","纺织品;皮革"]
[null,{"$f":"IF($B$1=\"English\",C654,IF($B$1=\"Deutsch\",D654,IF($B$1=\"中文\",E654,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Unequipped curcuit board; device for curcuit board; electronic component"},"Unequipped curcuit board; device for curcuit board; electronic component","unbestückte Leiterplatte; Bauelement für Leiterplatte; Elektronikkomponente","印刷电路板裸板;组件的印刷电路板装置;电子元件"]
[null,{"$f":"IF($B$1=\"English\",C655,IF($B$1=\"Deutsch\",D655,IF($B$1=\"中文\",E655,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Composite material"},"Composite material","Verbundwerkstoff","复合材料"]
[null,{"$f":"IF($B$1=\"English\",C656,IF($B$1=\"Deutsch\",D656,IF($B$1=\"中文\",E656,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging"},"Packaging","Verpackung","包装"]
[null,{"$f":"IF($B$1=\"English\",C657,IF($B$1=\"Deutsch\",D657,IF($B$1=\"中文\",E657,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Wood, no wood-based material or composite"},"Wood, no wood-based material or composite","Holz, kein Holzwerkstoff oder Verbundwerkstoff","木头，非木质材料或复合材料"]
[null,{"$f":"IF($B$1=\"English\",C658,IF($B$1=\"Deutsch\",D658,IF($B$1=\"中文\",E658,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Show extract"},"Show extract","Auszug anzeigen","显示完整摘录"]
[null,{"$f":"IF($B$1=\"English\",C659,IF($B$1=\"Deutsch\",D659,IF($B$1=\"中文\",E659,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reduce extract"},"Reduce extract","Auszug verkleinern","显示部分摘录"]
[null,{"$f":"IF($B$1=\"English\",C660,IF($B$1=\"Deutsch\",D660,IF($B$1=\"中文\",E660,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Selected divisions"},"Selected divisions","Ausgewählte Geschäftseinheiten","选定的事业部"]
[null,{"$f":"IF($B$1=\"English\",C661,IF($B$1=\"Deutsch\",D661,IF($B$1=\"中文\",E661,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Auxiliary manufacturing material, also cooling lubricants which doesn't remain in or on product"},"Auxiliary manufacturing material, also cooling lubricants which doesn't remain in or on product","Fertigungshilfsstoff auch Kühlschmierstoff der nicht im oder am Produkt verbleibt","不在产品上有残余的制造辅助材料和冷却剂"]
[null,{"$f":"IF($B$1=\"English\",C662,IF($B$1=\"Deutsch\",D662,IF($B$1=\"中文\",E662,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other than mentioned above"},"Other than mentioned above","Andere als oben angenannt","其他"]
[null,{"$f":"IF($B$1=\"English\",C663,IF($B$1=\"Deutsch\",D663,IF($B$1=\"中文\",E663,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"not applicable"},"not applicable","nicht anwendbar","不适用"]
[null,{"$f":"IF($B$1=\"English\",C664,IF($B$1=\"Deutsch\",D664,IF($B$1=\"中文\",E664,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Complex product or unknown type of material"},"Complex product or unknown type of material","Komplexes Produkt oder unbekannte Materialarten","复杂的产品或未知类型的材料"]
[null,{"$f":"IF($B$1=\"English\",C665,IF($B$1=\"Deutsch\",D665,IF($B$1=\"中文\",E665,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated biphenyls (PCB)"},"Polychlorinated biphenyls (PCB)","Polychlorierte Biphenyle (PCB)","多氯联苯（PCB）"]
[null,{"$f":"IF($B$1=\"English\",C666,IF($B$1=\"Deutsch\",D666,IF($B$1=\"中文\",E666,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1336-36-3 and others"},"1336-36-3 and others","1336-36-3 und andere","1336-36-3 和其他"]
[null,{"$f":"IF($B$1=\"English\",C667,IF($B$1=\"Deutsch\",D667,IF($B$1=\"中文\",E667,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Advantage: You may reduce the amount of required data by selecting the applicable checkbox (optional). Click \"Ok\" to continue."},"Advantage: You may reduce the amount of required data by selecting the applicable checkbox (optional). Click \"Ok\" to continue.","Vorteil: Sie können durch Anklicken der zutreffenden Check-Box die Anzahl der gefragten Daten reduzieren (optional). Fortfahren mit \"Ok\".","优点：您可以通过点击相应的复选框check-box(可选项)，缩减 相关的数据的数量。单击“确定”继续。"]
[null,{"$f":"IF($B$1=\"English\",C668,IF($B$1=\"Deutsch\",D668,IF($B$1=\"中文\",E668,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Division"},"Division","Geschäftseinheit","事业部"]
[null,{"$f":"IF($B$1=\"English\",C669,IF($B$1=\"Deutsch\",D669,IF($B$1=\"中文\",E669,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Extract from Regulation (EC) No 1907/2006, Annex 17 (source text see www.eur-lex.europa.eu)"},"Extract from Regulation (EC) No 1907/2006, Annex 17 (source text see www.eur-lex.europa.eu)","Auszug aus Verordnung (EG) Nr. 1907/2006, Anhang 17 (Original-Text siehe www.eur-lex.europa.eu)","摘自法规(EC) NO. 1907/2006, 附件17 (原稿请见 www.eur-lex.europa.eu)"]
[null,{"$f":"IF($B$1=\"English\",C670,IF($B$1=\"Deutsch\",D670,IF($B$1=\"中文\",E670,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Listed in REACH Annex 17 No 3"},"Listed in REACH Annex 17 No 3","Fällt unter REACH Anhang 17 Nr. 3","REACH法规附件17，第3项"]
[null,{"$f":"IF($B$1=\"English\",C671,IF($B$1=\"Deutsch\",D671,IF($B$1=\"中文\",E671,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in anticorrosion agents, e,ulsion cleaners\n0,5 % in lubricants and test media"},"10 ppm in anticorrosion agents, e,ulsion cleaners\n0,5 % in lubricants and test media","10 ppm in Korrosionsschutzmitteln, Emulsionsreinigern\n0,5% in Schmierstoffen und Prüfmedien","在防锈剂、乳化液、清洁剂中，10ppm\n在润滑剂和测试液中，0.5％"]
[null,{"$f":"IF($B$1=\"English\",C672,IF($B$1=\"Deutsch\",D672,IF($B$1=\"中文\",E672,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % in lubricants and test media"},"0,1 % in lubricants and test media","0,1% in Schmierstoffen und Prüfmedien","在润滑剂和测试液中，0.1％"]
[null,{"$f":"IF($B$1=\"English\",C673,IF($B$1=\"Deutsch\",D673,IF($B$1=\"中文\",E673,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 ppm in cooling lubricants"},"10 ppm in cooling lubricants","10 ppm in Kühlschmierstoffen","在冷却润滑剂中， 10 ppm"]
[null,{"$f":"IF($B$1=\"English\",C674,IF($B$1=\"Deutsch\",D674,IF($B$1=\"中文\",E674,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"RoHS ANNEX V, valid from january 2013:\nApplications for granting, renewing and revoking exemptions as referred to in Article 5"},"RoHS ANNEX V, valid from january 2013:\nApplications for granting, renewing and revoking exemptions as referred to in Article 5","RoHS ANHANG V, gültig ab Januar 2013:\nAnträge auf Gewährung, Erneuerung und Widerruf von Ausnahmen gemäß Artikel 5","“RoHS附件五，从2013年1月起生效：\n提出，更新和撤销豁免的申请（参考第5条）"]
[null,{"$f":"IF($B$1=\"English\",C675,IF($B$1=\"Deutsch\",D675,IF($B$1=\"中文\",E675,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Exemption"},"Exemption","Ausnahme","豁免"]
[null,{"$f":"IF($B$1=\"English\",C676,IF($B$1=\"Deutsch\",D676,IF($B$1=\"中文\",E676,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in single capped (compact) fluorescent lamps not exceeding (per burner):"},"Mercury in single capped (compact) fluorescent lamps not exceeding (per burner):","Quecksilber in einseitig gesockelten (Kompakt-) Leuchtstofflampen, die folgende Werte (je Brennstelle) nicht übersteigen:","紧凑型荧光灯中的汞含量不超过（每盏）："]
[null,{"$f":"IF($B$1=\"English\",C677,IF($B$1=\"Deutsch\",D677,IF($B$1=\"中文\",E677,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For general lighting purposes < 30 W: 5 mg"},"For general lighting purposes < 30 W: 5 mg","Für allgemeine Beleuchtungszwecke < 30 W: 5 mg","普通照明用<30 W：5 mg"]
[null,{"$f":"IF($B$1=\"English\",C678,IF($B$1=\"Deutsch\",D678,IF($B$1=\"中文\",E678,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For general lighting purposes ≥ 30 W and < 50 W: 5 mg"},"For general lighting purposes ≥ 30 W and < 50 W: 5 mg","Für allgemeine Beleuchtungszwecke ≥ 30 W und < 50 W: 5 mg","普通照明用≥30 W且<50 W：5 mg"]
[null,{"$f":"IF($B$1=\"English\",C679,IF($B$1=\"Deutsch\",D679,IF($B$1=\"中文\",E679,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For general lighting purposes ≥ 50 W and < 150 W: 5 mg"},"For general lighting purposes ≥ 50 W and < 150 W: 5 mg","Für allgemeine Beleuchtungszwecke ≥ 50 W und < 150 W: 5 mg","普通照明用≥50 W且<150 W：5 mg"]
[null,{"$f":"IF($B$1=\"English\",C680,IF($B$1=\"Deutsch\",D680,IF($B$1=\"中文\",E680,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For general lighting purposes ≥ 150 W: 15 mg"},"For general lighting purposes ≥ 150 W: 15 mg","Für allgemeine Beleuchtungszwecke ≥ 150 W: 15 mg","普通照明用≥150 W：15 mg"]
[null,{"$f":"IF($B$1=\"English\",C681,IF($B$1=\"Deutsch\",D681,IF($B$1=\"中文\",E681,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For general lighting purposes with circular or square structural shape and tube diameter ≤ 17 mm"},"For general lighting purposes with circular or square structural shape and tube diameter ≤ 17 mm","Für allgemeine Beleuchtungszwecke mit runder oder quadratischer Bauform und einem Röhrendurchmesser von ≤ 17 mm","普通照明用，且为环状或方形，管直径≤17 mm"]
[null,{"$f":"IF($B$1=\"English\",C682,IF($B$1=\"Deutsch\",D682,IF($B$1=\"中文\",E682,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For special purposes: 5 mg"},"For special purposes: 5 mg","Für besondere Verwendungszwecke: 5 mg","对于特殊用途：5mg"]
[null,{"$f":"IF($B$1=\"English\",C683,IF($B$1=\"Deutsch\",D683,IF($B$1=\"中文\",E683,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in double-capped linear fluorescent lamps for general lighting purposes not exceeding (per lamp):"},"Mercury in double-capped linear fluorescent lamps for general lighting purposes not exceeding (per lamp):","Quecksilber in beidseitig gesockelten linearen Leuchtstofflampen für allgemeine Beleuchtungszwecke, die folgende Werte (je Lampe) nicht übersteigen:","在用于普通照明的双端直管荧光灯，（每盏灯）汞含量不超过下列数值："]
[null,{"$f":"IF($B$1=\"English\",C684,IF($B$1=\"Deutsch\",D684,IF($B$1=\"中文\",E684,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-band phosphor with normal lifetime and a tube diameter < 9 mm (e.g. T2): 5 mg"},"Tri-band phosphor with normal lifetime and a tube diameter < 9 mm (e.g. T2): 5 mg","Tri-Phosphor-Lampen mit normaler Lebensdauer und einem Röhrendurchmesser von < 9 mm (z. B. T2): 5 mg","正常寿命、管直径<9mm的三基色荧光灯（例如T2）：5mg"]
[null,{"$f":"IF($B$1=\"English\",C685,IF($B$1=\"Deutsch\",D685,IF($B$1=\"中文\",E685,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-band phosphor with normal lifetime and a tube diameter ≥ 9 mm and ≤ 17 mm (e.g. T5): 5 mg"},"Tri-band phosphor with normal lifetime and a tube diameter ≥ 9 mm and ≤ 17 mm (e.g. T5): 5 mg","Tri-Phosphor-Lampen mit normaler Lebensdauer und einem Röhrendurchmesser von ≥ 9 mm und ≤ 17 mm (z. B. T5): 5 mg","正常寿命、管直径≥ 9 mm但是 ≤ 17 mm的三基色荧光灯 (例如 T5): 5 mg"]
[null,{"$f":"IF($B$1=\"English\",C686,IF($B$1=\"Deutsch\",D686,IF($B$1=\"中文\",E686,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-band phosphor with normal lifetime and a tube diameter > 17 mm and ≤ 28 mm (e.g. T8): 5 mg"},"Tri-band phosphor with normal lifetime and a tube diameter > 17 mm and ≤ 28 mm (e.g. T8): 5 mg","Tri-Phosphor-Lampen mit normaler Lebensdauer und einem Röhrendurchmesser von > 17 mm und ≤ 28 mm (z. B. T8): 5 mg","正常寿命、管直径> 17 mm但是 ≤ 28 mm的三基色荧光灯 (例如 T8): 5 mg"]
[null,{"$f":"IF($B$1=\"English\",C687,IF($B$1=\"Deutsch\",D687,IF($B$1=\"中文\",E687,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-band phosphor with normal lifetime and a tube diameter > 28 mm (e.g. T12): 5 mg"},"Tri-band phosphor with normal lifetime and a tube diameter > 28 mm (e.g. T12): 5 mg","Tri-Phosphor-Lampen mit normaler Lebensdauer und einem Röhrendurchmesser von > 28 mm (z. B. T12): 5 mg","正常寿命、管直径> 28 mm的三基色荧光灯 (例如 T12): 5 mg"]
[null,{"$f":"IF($B$1=\"English\",C688,IF($B$1=\"Deutsch\",D688,IF($B$1=\"中文\",E688,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-band phosphor with long lifetime (≥ 25 000 h): 8 mg"},"Tri-band phosphor with long lifetime (≥ 25 000 h): 8 mg","Tri-Phosphor-Lampen mit langer Lebensdauer (≥ 25 000 Std.): 8 mg","长寿命（≥ 25000小时）的三基色荧光灯: 8 mg"]
[null,{"$f":"IF($B$1=\"English\",C689,IF($B$1=\"Deutsch\",D689,IF($B$1=\"中文\",E689,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in other fluorescent lamps not exceeding (per lamp):"},"Mercury in other fluorescent lamps not exceeding (per lamp):","Quecksilber in anderen Leuchtstofflampen, die folgende Werte (je Lampe) nicht übersteigen:","在其他荧光灯中，（每盏）汞含量不超过下列数值："]
[null,{"$f":"IF($B$1=\"English\",C690,IF($B$1=\"Deutsch\",D690,IF($B$1=\"中文\",E690,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Linear halophosphate lamps with tube > 28 mm (e.g. T10 and T12): 10 mg"},"Linear halophosphate lamps with tube > 28 mm (e.g. T10 and T12): 10 mg","Lineare Halophosphatlampen mit Röhrendurchmesser von > 28 mm (z. B. T10 und T12): 10 mg","直的卤化磷酸盐灯管，其管直径> 28 mm (例如T10和 T12): 10 mg"]
[null,{"$f":"IF($B$1=\"English\",C691,IF($B$1=\"Deutsch\",D691,IF($B$1=\"中文\",E691,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Non-linear halophosphate lamps (all diameters): 15 mg"},"Non-linear halophosphate lamps (all diameters): 15 mg","Nichtlineare Halophosphatlampen (alle Durchmesser): 15 mg","非直的卤化磷酸盐灯管（所有直径）15 mg"]
[null,{"$f":"IF($B$1=\"English\",C692,IF($B$1=\"Deutsch\",D692,IF($B$1=\"中文\",E692,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9)"},"Non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9)","Nichtlineare Tri-Phosphor-Lampen mit einem Röhrendurchmesser von > 17 mm (z. B. T9)","非直的三基色灯，其管直径> 17 mm (例如 T9)"]
[null,{"$f":"IF($B$1=\"English\",C693,IF($B$1=\"Deutsch\",D693,IF($B$1=\"中文\",E693,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lamps for other general lighting and special purposes (e.g. induction lamps)"},"Lamps for other general lighting and special purposes (e.g. induction lamps)","Lampen für andere allgemeine Beleuchtungszwecke und für besondere Verwendungszwecke (z. B. Induktionslampen)","用于别的一般照明用途和特殊用途的灯（如感应灯）"]
[null,{"$f":"IF($B$1=\"English\",C694,IF($B$1=\"Deutsch\",D694,IF($B$1=\"中文\",E694,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes not exceeding (per lamp):"},"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes not exceeding (per lamp):","Quecksilber in CCFL- (cold cathode fluorescent lamps) und EEFL-Lampen (external electrode fluorescent lamps) für besondere Verwendungszwecke, die folgende Werte (je Lampe) nicht übersteigen:","用于特殊用途的CCFL(冷阴极荧光灯)和EEFL灯(外部电极荧光灯)，（每盏）汞含量不超过："]
[null,{"$f":"IF($B$1=\"English\",C695,IF($B$1=\"Deutsch\",D695,IF($B$1=\"中文\",E695,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Short length (≤ 500 mm)"},"Short length (≤ 500 mm)","Kurze Lampen (≤ 500 mm)","短灯(≤ 500 mm)"]
[null,{"$f":"IF($B$1=\"English\",C696,IF($B$1=\"Deutsch\",D696,IF($B$1=\"中文\",E696,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Medium length (> 500 mm and ≤ 1 500 mm)"},"Medium length (> 500 mm and ≤ 1 500 mm)","Mittellange Lampen (> 500 mm und ≤ 1 500 mm)","中长灯 (> 500 mm und ≤ 1 500 mm)"]
[null,{"$f":"IF($B$1=\"English\",C697,IF($B$1=\"Deutsch\",D697,IF($B$1=\"中文\",E697,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Long length (> 1 500 mm)"},"Long length (> 1 500 mm)","Lange Lampen (> 1 500 mm)","长灯(> 1 500 mm)"]
[null,{"$f":"IF($B$1=\"English\",C698,IF($B$1=\"Deutsch\",D698,IF($B$1=\"中文\",E698,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in other low pressure discharge lamps (per lamp)"},"Mercury in other low pressure discharge lamps (per lamp)","Quecksilber in anderen Niederdruckentladungslampen (je Lampe)","在其他低压放电灯（每盏）汞含量"]
[null,{"$f":"IF($B$1=\"English\",C699,IF($B$1=\"Deutsch\",D699,IF($B$1=\"中文\",E699,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner) in lamps with improved colour rendering index Ra > 60:"},"Mercury in High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner) in lamps with improved colour rendering index Ra > 60:","Quecksilber in Hochdrucknatrium(dampf)lampen für allgemeine Beleuchtungszwecke, die bei Lampen mit verbessertem Farbwiedergabeindex Ra > 60 folgende Werte (je Brennstelle) nicht übersteigen:","在用于一般照明的高压钠（蒸气）灯，灯具与改进显色指数Ra>60，（每盏）汞含量不超过："]
[null,{"$f":"IF($B$1=\"English\",C700,IF($B$1=\"Deutsch\",D700,IF($B$1=\"中文\",E700,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P ≤ 155 W"},"P ≤ 155 W","P ≤ 155 W","功率 ≤ 155 W"]
[null,{"$f":"IF($B$1=\"English\",C701,IF($B$1=\"Deutsch\",D701,IF($B$1=\"中文\",E701,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"155 W < P ≤ 405 W"},"155 W < P ≤ 405 W","155 W < P ≤ 405 W","155 W < 功率 ≤ 405 W"]
[null,{"$f":"IF($B$1=\"English\",C702,IF($B$1=\"Deutsch\",D702,IF($B$1=\"中文\",E702,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P > 405 W"},"P > 405 W","P > 405 W","功率 > 405 W"]
[null,{"$f":"IF($B$1=\"English\",C703,IF($B$1=\"Deutsch\",D703,IF($B$1=\"中文\",E703,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in other High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner):"},"Mercury in other High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner):","Quecksilber in anderen Hochdrucknatrium(dampf)lampen für allgemeine Beleuchtungszwecke, die folgende Werte (je Brennstelle) nicht übersteigen:","在其他用于特殊照明的高压钠（蒸气）灯，（每盏）汞含量不超过："]
[null,{"$f":"IF($B$1=\"English\",C704,IF($B$1=\"Deutsch\",D704,IF($B$1=\"中文\",E704,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P ≤ 155 W"},"P ≤ 155 W","P ≤ 155 W","功率 ≤ 155 W"]
[null,{"$f":"IF($B$1=\"English\",C705,IF($B$1=\"Deutsch\",D705,IF($B$1=\"中文\",E705,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"155 W < P ≤ 405 W"},"155 W < P ≤ 405 W","155 W < P ≤ 405 W","155 W < 功率 ≤ 405 W"]
[null,{"$f":"IF($B$1=\"English\",C706,IF($B$1=\"Deutsch\",D706,IF($B$1=\"中文\",E706,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P > 405 W"},"P > 405 W","P > 405 W","功率 > 405 W"]
[null,{"$f":"IF($B$1=\"English\",C707,IF($B$1=\"Deutsch\",D707,IF($B$1=\"中文\",E707,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in High Pressure Mercury (vapour) lamps (HPMV)"},"Mercury in High Pressure Mercury (vapour) lamps (HPMV)","Quecksilber in Hochdruckquecksilber(dampf)lampen (HPMV)","在其他高压钠（蒸气）灯(HPMV)中的汞含量"]
[null,{"$f":"IF($B$1=\"English\",C708,IF($B$1=\"Deutsch\",D708,IF($B$1=\"中文\",E708,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in metal halide lamps (MH)"},"Mercury in metal halide lamps (MH)","Quecksilber in Metallhalidlampen (MH)","在金属卤化物灯（MH）中的汞含量"]
[null,{"$f":"IF($B$1=\"English\",C709,IF($B$1=\"Deutsch\",D709,IF($B$1=\"中文\",E709,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in other discharge lamps for special purposes not specifically mentioned in this Annex"},"Mercury in other discharge lamps for special purposes not specifically mentioned in this Annex","Quecksilber in anderen Entladungslampen für besondere Verwendungszwecke, die in diesem Anhang nicht gesondert aufgeführt sind","在本附件中未明确提到的用作特殊用途的其他的灯具中的汞含量"]
[null,{"$f":"IF($B$1=\"English\",C710,IF($B$1=\"Deutsch\",D710,IF($B$1=\"中文\",E710,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in glass of cathode ray tubes"},"Lead in glass of cathode ray tubes","Blei im Glas von Kathodenstrahlröhren","阴极射线管的玻璃中的铅含量"]
[null,{"$f":"IF($B$1=\"English\",C711,IF($B$1=\"Deutsch\",D711,IF($B$1=\"中文\",E711,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in glass of fluorescent tubes not exceeding 0,2 % by weight"},"Lead in glass of fluorescent tubes not exceeding 0,2 % by weight","Blei im Glas von Leuchtstoffröhren mit einem Massenanteil von höchstens 0,2 % Blei","在荧光灯管的玻璃中铅含量不含有超过0.2％"]
[null,{"$f":"IF($B$1=\"English\",C712,IF($B$1=\"Deutsch\",D712,IF($B$1=\"中文\",E712,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in steel for machining purposes and in galvanized steel containing up to 0,35 % lead by weight"},"Lead as an alloying element in steel for machining purposes and in galvanized steel containing up to 0,35 % lead by weight","Blei als Legierungselement in Stahl für Bearbeitungszwecke und in verzinktem Stahl mit einem Massenanteil von höchstens 0,35 % Blei","机械加工用钢材和镀锌钢，铅≤0.35 %"]
[null,{"$f":"IF($B$1=\"English\",C713,IF($B$1=\"Deutsch\",D713,IF($B$1=\"中文\",E713,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in aluminium containing up to 0,4 % lead by weight"},"Lead as an alloying element in aluminium containing up to 0,4 % lead by weight","Blei als Legierungselement in Aluminium mit einem Massenanteil von höchstens 0,4 % Blei","铝合金，铅≤0.4％"]
[null,{"$f":"IF($B$1=\"English\",C714,IF($B$1=\"Deutsch\",D714,IF($B$1=\"中文\",E714,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Copper alloy containing up to 4 % lead by weight"},"Copper alloy containing up to 4 % lead by weight","Kupferlegierung mit einem Massenanteil von bis zu 4 % Blei","铜合金，铅 ≤ 4%"]
[null,{"$f":"IF($B$1=\"English\",C715,IF($B$1=\"Deutsch\",D715,IF($B$1=\"中文\",E715,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in high melting temperature type solders (i.e. lead-based alloys containing 85 % by weight or more lead)"},"Lead in high melting temperature type solders (i.e. lead-based alloys containing 85 % by weight or more lead)","Blei in hochschmelzenden Loten (d. h. Lötlegierungen auf Bleibasis mit einem Massenanteil von mindestens 85 % Blei)","高熔点焊料中的铅（如铅含量重量比在85%及以上）"]
[null,{"$f":"IF($B$1=\"English\",C716,IF($B$1=\"Deutsch\",D716,IF($B$1=\"中文\",E716,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission, and network management for telecommunications"},"Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission, and network management for telecommunications","Blei in Loten für Server, Speichersysteme und Speicherarrays sowie Netzinfrastrukturausrüstungen für Vermittlung, Signalweiterleitung, Übertragung und Netzmanagement im Telekommunikationsbereich","用于服务器,存储器和存储系统中的铅,用于交换,信号和传输,以及电信网络管理的网络基础设施设备中焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C717,IF($B$1=\"Deutsch\",D717,IF($B$1=\"中文\",E717,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g. piezoelectronic devices, or in a glass or ceramic matrix compound"},"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g. piezoelectronic devices, or in a glass or ceramic matrix compound","Blei enthaltende elektrische und elektronische Bauteile in Glas oder Keramikwerkstoffen außer dielektrischer Keramik in Kondensatoren, z. B. piezoelektronische Geräte, oder in einer Glas- oder Keramikmatrixverbindung","除电容器的介电陶瓷外的其他电子电气元器件中陶瓷或者玻璃中的铅，例如压电设备，或玻璃、陶瓷基的复合材料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C718,IF($B$1=\"Deutsch\",D718,IF($B$1=\"中文\",E718,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher"},"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher","Blei in dielektrischer Keramik in Kondensatoren für eine Nennspannung von 125 V AC oder 250 V DC oder darüber","额定电压大于等于交流125 V或直流250 V的电容器介电陶瓷中的铅"]
[null,{"$f":"IF($B$1=\"English\",C719,IF($B$1=\"Deutsch\",D719,IF($B$1=\"中文\",E719,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC"},"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC","Blei in dielektrischer Keramik in Kondensatoren für eine Nennspannung von weniger als 125 V AC oder 250 V DC","额定电压低于交流125 V或直流250 V的电容器介电陶瓷中的铅"]
[null,{"$f":"IF($B$1=\"English\",C720,IF($B$1=\"Deutsch\",D720,IF($B$1=\"中文\",E720,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors"},"Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors","Blei in PZT-basierten dielektrischen Keramikwerkstoffen für Kondensatoren, die Teil integrierter Schaltkreise oder diskreter Halbleiter sind","电容器的电陶瓷材料PZT中的铅，该电容器是集成电路或分离半导体的组成部分"]
[null,{"$f":"IF($B$1=\"English\",C721,IF($B$1=\"Deutsch\",D721,IF($B$1=\"中文\",E721,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and its compounds in one shot pellet type thermal cut-offs"},"Cadmium and its compounds in one shot pellet type thermal cut-offs","Cadmium und Cadmiumverbindungen in Thermosicherungen vom Typ „one shot pellet“","热熔断体中的镉及镉化合物"]
[null,{"$f":"IF($B$1=\"English\",C722,IF($B$1=\"Deutsch\",D722,IF($B$1=\"中文\",E722,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and its compounds in electrical contacts"},"Cadmium and its compounds in electrical contacts","Cadmium und Cadmiumverbindungen in elektrischen Kontakten","电气连接的触点中的镉及化合物"]
[null,{"$f":"IF($B$1=\"English\",C723,IF($B$1=\"Deutsch\",D723,IF($B$1=\"中文\",E723,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexavalent chromium as an anticorrosion agent of the carbon steel cooling system in absorption refrigerators up to 0,75 % by weight in the cooling solution"},"Hexavalent chromium as an anticorrosion agent of the carbon steel cooling system in absorption refrigerators up to 0,75 % by weight in the cooling solution","Sechswertiges Chrom als Korrosionsschutzmittel des Kohlenstoffstahl-Kühlsystems in Absorptionskühlschränken bis zu einem Massenanteil von 0,75 % in der Kühllösung","在吸收式电冰箱中作为碳钢冷却系统防腐剂的六价铬，其在冷却液中超过了0.75%（重量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C724,IF($B$1=\"Deutsch\",D724,IF($B$1=\"中文\",E724,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in bearing shells and bushes for refrigerant-containing compressors for heating, ventilation, air conditioning and refrigeration (HVACR) applications"},"Lead in bearing shells and bushes for refrigerant-containing compressors for heating, ventilation, air conditioning and refrigeration (HVACR) applications","Blei in Lagerschalen und -buchsen für Kältemittel enthaltende Kompressoren für Heiz-, Belüftungs-, Klima- und Kühlanwendungen (HVACR)","用于加热、通风、空调和制冷（HVACR）的冰箱零部件的轴承外壳及其轴衬中的铅"]
[null,{"$f":"IF($B$1=\"English\",C725,IF($B$1=\"Deutsch\",D725,IF($B$1=\"中文\",E725,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead used in C-press compliant pin connector systems"},"Lead used in C-press compliant pin connector systems","Blei in „C-Press“-Einpresssteckverbindern mit flexibler Zone","C-顺应针连接器系统中使用的铅"]
[null,{"$f":"IF($B$1=\"English\",C726,IF($B$1=\"Deutsch\",D726,IF($B$1=\"中文\",E726,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead used in other than C-press compliant pin connector systems"},"Lead used in other than C-press compliant pin connector systems","Blei in anderen als „C-Press“-Einpresssteckverbindern mit flexibler Zone","除C-顺应针连接器系统外使用的铅"]
[null,{"$f":"IF($B$1=\"English\",C727,IF($B$1=\"Deutsch\",D727,IF($B$1=\"中文\",E727,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as a coating material for the thermal conduction module C-ring"},"Lead as a coating material for the thermal conduction module C-ring","Blei als Beschichtungsmaterial für ein wärmeleitendes C-Ring-Modul.","用于C－环型导热模块的表面涂层中的铅"]
[null,{"$f":"IF($B$1=\"English\",C728,IF($B$1=\"Deutsch\",D728,IF($B$1=\"中文\",E728,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in white glasses used for optical applications"},"Lead in white glasses used for optical applications","Blei in Weißglas für optische Anwendungen","光学仪器中使用的白玻璃中的铅"]
[null,{"$f":"IF($B$1=\"English\",C729,IF($B$1=\"Deutsch\",D729,IF($B$1=\"中文\",E729,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and lead in filter glasses and glasses used for reflectance standards"},"Cadmium and lead in filter glasses and glasses used for reflectance standards","Cadmium und Blei in Filterglas und Glas für Reflexionsstandards","在光学玻璃和滤光玻璃中的铅或镉"]
[null,{"$f":"IF($B$1=\"English\",C730,IF($B$1=\"Deutsch\",D730,IF($B$1=\"中文\",E730,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors with a lead content of more than 80 % and less than 85 % by weight"},"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors with a lead content of more than 80 % and less than 85 % by weight","Blei in Loten aus mehr als zwei Elementen zur Verbindung zwischen den Anschlussstiften und der Mikroprozessor-Baugruppe mit einem Massenanteil von mehr als 80 % und weniger als 85 % Blei","用于微处理器的封装体与插针之间连接的铅含量占80%～85%的、含两种以上元素的焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C731,IF($B$1=\"Deutsch\",D731,IF($B$1=\"中文\",E731,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit flip chip packages"},"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit flip chip packages","Blei in Loten zum Herstellen einer stabilen elektrischen Verbindung zwischen dem Halbleiterchip und dem Schaltungsträger in integrierten Flip-Chip-Baugruppen","用于集成电路覆晶基板之内连接半导体模块和载波器的焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C732,IF($B$1=\"Deutsch\",D732,IF($B$1=\"中文\",E732,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in linear incandescent lamps with silicate coated tubes"},"Lead in linear incandescent lamps with silicate coated tubes","Blei in stabförmigen Glühlampen mit eingeschmolzener Innenbeschichtung des Kolbens","线形白炽灯硅酸盐灯管中的铅"]
[null,{"$f":"IF($B$1=\"English\",C733,IF($B$1=\"Deutsch\",D733,IF($B$1=\"中文\",E733,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead halide as radiant agent in high intensity discharge (HID) lamps used for professional reprography applications"},"Lead halide as radiant agent in high intensity discharge (HID) lamps used for professional reprography applications","Bleihalogenide als Strahlungszusatz in Hochdruck-Gasentladungslampen (HID-Lampen) für professionelle Reprografieanwendungen","用于专业复印设备的高强度放电灯（HID）中用作辐射剂的卤化铅"]
[null,{"$f":"IF($B$1=\"English\",C734,IF($B$1=\"Deutsch\",D734,IF($B$1=\"中文\",E734,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as speciality lamps for diazoprinting reprography, lithography, insect traps, photochemical and curing processes containing phosphors such as SMS ((Sr,Ba)2MgSi2O7:Pb)"},"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as speciality lamps for diazoprinting reprography, lithography, insect traps, photochemical and curing processes containing phosphors such as SMS ((Sr,Ba)2MgSi2O7:Pb)","Blei als Aktivator im Leuchtstoffpulver (davon Massenanteil Blei von 1 % oder weniger) von Gasentladungslampen bei Verwendung als Speziallampen für Reprografie auf Basis des Lichtpausverfahrens, Lithografie, Insektenfallen, fotochemische und Belichtungsprozesse mit Leuchtstoffen wie Magnesiumsilikat ((Sr,Ba)2MgSi2O7:Pb)","当放电灯被用作重氮复印、平板印刷、捕虫器、光化学和食物加工过程的特种灯，含有磷时，比如SMS（(Sr，Ba)2MgSi2O7:Pb），作为放电灯中的荧光粉（铅含量占其重量的1%或以下）触媒剂的铅"]
[null,{"$f":"IF($B$1=\"English\",C735,IF($B$1=\"Deutsch\",D735,IF($B$1=\"中文\",E735,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)"},"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)","Blei als Aktivator im Leuchtstoffpulver (davon Massenanteil Blei von 1 % oder weniger) von Gasentladungslampen bei Verwendung als Bräunungslampen mit Leuchtstoffen wie Bariumsilikat (BaSi2O5:Pb)","当放电灯被用作含磷的仿日晒灯（sun tanning lamps），比如含有BSP（BaSi2O5:Pb），作为放电灯中的荧光粉（铅含量占其重量的1%或以下）触媒剂的铅"]
[null,{"$f":"IF($B$1=\"English\",C736,IF($B$1=\"Deutsch\",D736,IF($B$1=\"中文\",E736,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact energy saving lamps (ESL)"},"Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact energy saving lamps (ESL)","Blei mit PbBiSn-Hg und PbInSn-Hg in speziellen Verbindungen als Hauptamalgam und mit PbSn-Hg als Zusatzamalgam in superkompakten Energiesparlampen","作为主要汞合金的特定成分中的含PbBiSn-Hg和PbInSg-Hg的铅以及紧凑型节能灯（ESL）中作为辅助汞合金的含PbSn-Hg的铅"]
[null,{"$f":"IF($B$1=\"English\",C737,IF($B$1=\"Deutsch\",D737,IF($B$1=\"中文\",E737,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCDs)"},"Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCDs)","Bleioxid in Glasloten zur Verbindung der vorderen und hinteren Glasscheibe von flachen Leuchtstofflampen für Flüssigkristallanzeigen (LCD)","液晶显示器（LCDs）的平面荧光灯前后基片连接用的玻璃中的氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C738,IF($B$1=\"Deutsch\",D738,IF($B$1=\"中文\",E738,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and cadmium in printing inks for the application of enamels on glasses, such as borosilicate and soda lime glasses"},"Lead and cadmium in printing inks for the application of enamels on glasses, such as borosilicate and soda lime glasses","Blei und Cadmium in Druckfarben zum Aufbringen von Emails auf Glas wie Borosilicatglas und Kalk-Natron-Glas","用于硼硅酸盐玻璃釉质的印墨所含的铅及镉"]
[null,{"$f":"IF($B$1=\"English\",C739,IF($B$1=\"Deutsch\",D739,IF($B$1=\"中文\",E739,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in finishes of fine pitch components other than connectors with a pitch of 0,65 mm and less"},"Lead in finishes of fine pitch components other than connectors with a pitch of 0,65 mm and less","Blei in der Beschichtung von Fine-Pitch-Komponenten — anderen als Steckverbindern — mit einem Pitch von 0,65 mm oder weniger","小螺距零部件表面抛光中的铅，螺距不超过0.65mm"]
[null,{"$f":"IF($B$1=\"English\",C740,IF($B$1=\"Deutsch\",D740,IF($B$1=\"中文\",E740,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors"},"Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors","Blei in Loten für discoidale und Planar-Array-Vielschicht-Keramikkondensatoren mit metallisierten Löchern","通孔盘状及平面阵列陶瓷多层电容器焊料所含的铅"]
[null,{"$f":"IF($B$1=\"English\",C741,IF($B$1=\"Deutsch\",D741,IF($B$1=\"中文\",E741,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in surface conduction electron emitter displays (SED) used in structural elements, notably in the seal frit and frit ring"},"Lead oxide in surface conduction electron emitter displays (SED) used in structural elements, notably in the seal frit and frit ring","Bleioxid in Strukturelementen von SED-Displays (surface conduction electron emitter displays (SED), insbesondere in der Glasfritte für die Befestigung (seal frit) und dem Glasfrittering (frit ring)","表面传导式电子发射显示器（SED）的构件，特别是熔接密封和环状玻璃，所用的氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C742,IF($B$1=\"Deutsch\",D742,IF($B$1=\"中文\",E742,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in the glass envelope of black light blue lamps"},"Lead oxide in the glass envelope of black light blue lamps","Bleioxid im Glasmantel von BLB-Lampen (Schwarzlichtlampen)","蓝黑灯管（BLB）玻璃外罩所含的氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C743,IF($B$1=\"Deutsch\",D743,IF($B$1=\"中文\",E743,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers"},"Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers","Bleilegierungen als Lote für Wandler in leistungsstarken Lautsprechern (für mehrstündigen Betrieb bei einem Schalldruck von 125 dB/SPL und darüber)","在大功率（要在125dB声压级下连续运行多个小时）扬声器作为转换器焊料的铅合金"]
[null,{"$f":"IF($B$1=\"English\",C744,IF($B$1=\"Deutsch\",D744,IF($B$1=\"中文\",E744,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead bound in crystal glass as defined in Annex I (Categories 1, 2, 3 and 4) of Council Directive 69/493/EEC (1)"},"Lead bound in crystal glass as defined in Annex I (Categories 1, 2, 3 and 4) of Council Directive 69/493/EEC (1)","Gebundenes Blei in Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/EWG des Rates (1)","欧盟委员会指令69/493/EEC附录I（第1、2、3和4类）中定义的水晶玻璃中的铅"]
[null,{"$f":"IF($B$1=\"English\",C745,IF($B$1=\"Deutsch\",D745,IF($B$1=\"中文\",E745,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound pressure levels of 100 dB (A) and more"},"Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound pressure levels of 100 dB (A) and more","Cadmiumlegierungen als elektrische/mechanische Lötmittel für elektrische Leiter, die direkt auf der Schwingspule in Wandlern in leistungsstarken Lautsprechern mit Schalldruck von 100 dB (A) und darüber verwendet werden","直接位于声压级大于等于100 dB (A)的高功率扬声器的传感器音圈的导电体的镉合金电器/机械焊点"]
[null,{"$f":"IF($B$1=\"English\",C746,IF($B$1=\"Deutsch\",D746,IF($B$1=\"中文\",E746,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in soldering materials in mercury free flat fluorescent lamps (which e.g. are used for liquid crystal displays, design or industrial lighting)"},"Lead in soldering materials in mercury free flat fluorescent lamps (which e.g. are used for liquid crystal displays, design or industrial lighting)","Blei in Lötmitteln in quecksilberfreien flachen Leuchtstofflampen (z. B. für Flüssigkristallanzeigen, Design- oder Industriebeleuchtung)","无汞平面荧光灯（例如用于液晶显示器、设计或工业照明）的焊接材料的铅"]
[null,{"$f":"IF($B$1=\"English\",C747,IF($B$1=\"Deutsch\",D747,IF($B$1=\"中文\",E747,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes"},"Lead oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes","Bleioxid in Glasfritten zur Befestigung von Glasscheiben für Argon- und Krypton- Laserröhren","用于为氩气和氪激光管制造窗口组件的密封熔块的氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C748,IF($B$1=\"Deutsch\",D748,IF($B$1=\"中文\",E748,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders for the soldering of thin copper wires of 100 μm diameter and less in power transformers"},"Lead in solders for the soldering of thin copper wires of 100 μm diameter and less in power transformers","Blei in Loten für das Löten von dünnen Kupferdrähten mit höchstens 100 μm Durchmesser in Leistungstransformatoren","电力变压器中直径100微米及以下细铜线所用焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C749,IF($B$1=\"Deutsch\",D749,IF($B$1=\"中文\",E749,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in cermet-based trimmer potentiometer elements"},"Lead in cermet-based trimmer potentiometer elements","Blei in Trimmpotentiometern auf Cermet-Basis.","金属陶瓷质的微调电位计中的铅"]
[null,{"$f":"IF($B$1=\"English\",C750,IF($B$1=\"Deutsch\",D750,IF($B$1=\"中文\",E750,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury used as a cathode sputtering inhibitor in DC plasma displays with a content up to 30 mg per display"},"Mercury used as a cathode sputtering inhibitor in DC plasma displays with a content up to 30 mg per display","Quecksilber als Inhibitor zur Vermeidung von Kathodensputtering bei DC-Plasmadisplays mit einem Gehalt von bis zu 30 mg pro Display","直流等离子显示器中阴极溅射抑制剂中的汞，其含量不得超过30毫克/显示器"]
[null,{"$f":"IF($B$1=\"English\",C751,IF($B$1=\"Deutsch\",D751,IF($B$1=\"中文\",E751,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body"},"Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body","Blei in der Beschichtung von Hochspannungsdioden auf der Grundlage eines Zinkborat-Glasgehäuses","以硼酸锌玻璃体为基础的高压二极管的电镀层的铅"]
[null,{"$f":"IF($B$1=\"English\",C752,IF($B$1=\"Deutsch\",D752,IF($B$1=\"中文\",E752,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and cadmium oxide in thick film pastes used on aluminium bonded beryllium oxide"},"Cadmium and cadmium oxide in thick film pastes used on aluminium bonded beryllium oxide","Cadmium und Cadmiumoxid in Dickschichtpasten, die auf Aluminium-gebundenem Berylliumoxid eingesetzt werden","用氧化铍连接铝制成的厚膜浆料中镉和氧化镉"]
[null,{"$f":"IF($B$1=\"English\",C753,IF($B$1=\"Deutsch\",D753,IF($B$1=\"中文\",E753,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium in colour converting II-VI LEDs (< 10 μg Cd per mm2 of light-emitting area) for use in solid state illumination or display systems"},"Cadmium in colour converting II-VI LEDs (< 10 μg Cd per mm2 of light-emitting area) for use in solid state illumination or display systems","Cadmium in farbkonvertierenden II–VI-basierten LEDs (< 10 μg Cd je mm2 Licht emittierende Fläche) zur Verwendung in Halbleiter-Beleuchtungen oder Display-Systemen","用于固态照明或显示系统中的彩色转换II-VI族LEDs内所含的镉（每平方毫米发光区域的镉小于10微克）"]
[null,{"$f":"IF($B$1=\"English\",C754,IF($B$1=\"Deutsch\",D754,IF($B$1=\"中文\",E754,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium in photoresistors for analogue optocouplers applied in professional audio equipment"},"Cadmium in photoresistors for analogue optocouplers applied in professional audio equipment","Cadmium in Fotowiderständen für analoge Optokoppler in professionellen Audioanlagen","专业的音频设备中使用的模拟光耦合器中的光敏电阻器中的镉"]
[null,{"$f":"IF($B$1=\"English\",C755,IF($B$1=\"Deutsch\",D755,IF($B$1=\"中文\",E755,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1) OJ L 326, 29.12.1969, p. 36."},"(1) OJ L 326, 29.12.1969, p. 36.","(1) ABl. L 326 vom 29.12.1969, S. 36.","(1) OJ L 326 中的 29.12.1969, 第36.页"]
[null,{"$f":"IF($B$1=\"English\",C756,IF($B$1=\"Deutsch\",D756,IF($B$1=\"中文\",E756,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Note: For the purposes of Article 5(1)(a) of Directive 2002/95/EC, a maximum concentration value of 0,1 % by weight in homogeneous materials for lead, mercury, hexavalent chromium, polybrominated biphenyls (PBB) and polybrominated diphenyl ethers (PBDE) and of 0,01 % by weight in homogeneous materials for cadmium shall be tolerated."},"Note: For the purposes of Article 5(1)(a) of Directive 2002/95/EC, a maximum concentration value of 0,1 % by weight in homogeneous materials for lead, mercury, hexavalent chromium, polybrominated biphenyls (PBB) and polybrominated diphenyl ethers (PBDE) and of 0,01 % by weight in homogeneous materials for cadmium shall be tolerated.","Anmerkung: Für die Zwecke von Artikel 5 Absatz 1 Buchstabe a der Richtlinie 2002/95/EG wird als Konzentrationshöchstwert ein Massenanteil von jeweils 0,1 % Blei, Quecksilber, sechswertigem Chrom, polybromierten Biphenylen (PBB) oder polybromierten Diphenylethern (PBDE) je homogenem Werkstoff und von 0,01 % Cadmium je homogenem Werkstoff toleriert.","注：根据指令2002/95/EC的5(1)(a)，在均质材料中铅，汞，六价铬，多溴联苯（PBB）或多溴二苯醚（PBDE）含量的质量百分比最大运许值为0.1%，镉含量的质量百分比最大允许值为0.01%。"]
[null,{"$f":"IF($B$1=\"English\",C757,IF($B$1=\"Deutsch\",D757,IF($B$1=\"中文\",E757,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Will be RoHS \"Annex III\"  from January 2013"},"Will be RoHS \"Annex III\"  from January 2013","Bisher \"Anhang\" zu RoHS, ab Januar 2013: Anhang III von RoHS","从2013年1月起，将为RoHS的附件3"]
[null,{"$f":"IF($B$1=\"English\",C758,IF($B$1=\"Deutsch\",D758,IF($B$1=\"中文\",E758,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Scope and dates of applicability"},"Scope and dates of applicability","Anwendungsbereich und Gültigkeitsdaten","范围及有效期"]
[null,{"$f":"IF($B$1=\"English\",C759,IF($B$1=\"Deutsch\",D759,IF($B$1=\"中文\",E759,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C760,IF($B$1=\"Deutsch\",D760,IF($B$1=\"中文\",E760,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2011; 3,5 mg may be used per burner after 31 December 2011 until 31 December 2012; 2,5 mg shall be used per burner after 31 December 2012"},"Expires on 31 December 2011; 3,5 mg may be used per burner after 31 December 2011 until 31 December 2012; 2,5 mg shall be used per burner after 31 December 2012","Läuft am 31. Dezember 2011 ab; nach dem 31. Dezember 2011 dürfen bis zum 31. Dezember 2012 3,5 mg je Brennstelle verwendet werden; nach dem 31. Dezember 2012 dürfen 2,5 mg je Brennstelle verwendet werden.","豁免期至2011年12月31日；每个点火器中含量小于等于3.5mg可再延至2012年12月31日，每个点火器中含量小于等于2.5mg在2012年12月31日后仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C761,IF($B$1=\"Deutsch\",D761,IF($B$1=\"中文\",E761,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2011; 3,5 mg may be used per burner after 31 December 2011"},"Expires on 31 December 2011; 3,5 mg may be used per burner after 31 December 2011","Läuft am 31. Dezember 2011 ab; nach dem 31. Dezember 2011 dürfen 3,5 mg je Brennstelle verwendet werden.","\n豁免期至2011年12月31日；每个点火器中含量小于等于3.5mg在2011年12月31日以后仍可使用。"]
[null,{"$f":"IF($B$1=\"English\",C762,IF($B$1=\"Deutsch\",D762,IF($B$1=\"中文\",E762,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C763,IF($B$1=\"Deutsch\",D763,IF($B$1=\"中文\",E763,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C764,IF($B$1=\"Deutsch\",D764,IF($B$1=\"中文\",E764,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 7 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 7 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 7 mg je Brennstelle verwendet werden.","2011年12月31日前无限制；每个点火器中含量小于等于7mg在2011年12月31日后仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C765,IF($B$1=\"Deutsch\",D765,IF($B$1=\"中文\",E765,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C766,IF($B$1=\"Deutsch\",D766,IF($B$1=\"中文\",E766,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C767,IF($B$1=\"Deutsch\",D767,IF($B$1=\"中文\",E767,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2011; 4 mg may be used per lamp after 31 December 2011"},"Expires on 31 December 2011; 4 mg may be used per lamp after 31 December 2011","Läuft am 31. Dezember 2011 ab; nach dem 31. Dezember 2011 dürfen 4 mg je Lampe verwendet werden.","豁免期至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于4毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C768,IF($B$1=\"Deutsch\",D768,IF($B$1=\"中文\",E768,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2011; 3 mg may be used per lamp after 31 December 2011"},"Expires on 31 December 2011; 3 mg may be used per lamp after 31 December 2011","Läuft am 31. Dezember 2011 ab; nach dem 31. Dezember 2011 dürfen 3 mg je Lampe verwendet werden.","豁免期至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于3毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C769,IF($B$1=\"Deutsch\",D769,IF($B$1=\"中文\",E769,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2011; 3,5 mg may be used per lamp after 31 December 2011"},"Expires on 31 December 2011; 3,5 mg may be used per lamp after 31 December 2011","Läuft am 31. Dezember 2011 ab; nach dem 31. Dezember 2011 dürfen 3,5 mg je Lampe verwendet werden.","豁免期至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于3.5毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C770,IF($B$1=\"Deutsch\",D770,IF($B$1=\"中文\",E770,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2012; 3,5 mg may be used per lamp after 31 December 2012"},"Expires on 31 December 2012; 3,5 mg may be used per lamp after 31 December 2012","Läuft am 31. Dezember 2012 ab; nach dem 31. Dezember 2012 dürfen 3,5 mg je Lampe verwendet werden.","豁免期至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于3.5毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C771,IF($B$1=\"Deutsch\",D771,IF($B$1=\"中文\",E771,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2011; 5 mg may be used per lamp after 31 December 2011"},"Expires on 31 December 2011; 5 mg may be used per lamp after 31 December 2011","Läuft am 31. Dezember 2011 ab; nach dem 31. Dezember 2011 dürfen 5 mg je Lampe verwendet werden.","豁免期至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于5毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C772,IF($B$1=\"Deutsch\",D772,IF($B$1=\"中文\",E772,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C773,IF($B$1=\"Deutsch\",D773,IF($B$1=\"中文\",E773,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 13 April 2012"},"Expires on 13 April 2012","Läuft am 13. April 2012 ab.","豁免期至2012年04月13日"]
[null,{"$f":"IF($B$1=\"English\",C774,IF($B$1=\"Deutsch\",D774,IF($B$1=\"中文\",E774,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 13 April 2016"},"Expires on 13 April 2016","Läuft am 13. April 2016 ab.","豁免期至2016年04月13日"]
[null,{"$f":"IF($B$1=\"English\",C775,IF($B$1=\"Deutsch\",D775,IF($B$1=\"中文\",E775,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 15 mg may be used per lamp after 31 December 2011"},"No limitation of use until 31 December 2011; 15 mg may be used per lamp after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 15 mg je Lampe verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于15毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C776,IF($B$1=\"Deutsch\",D776,IF($B$1=\"中文\",E776,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 15 mg may be used per lamp after 31 December 2011"},"No limitation of use until 31 December 2011; 15 mg may be used per lamp after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 15 mg je Lampe verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于15毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C777,IF($B$1=\"Deutsch\",D777,IF($B$1=\"中文\",E777,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C778,IF($B$1=\"Deutsch\",D778,IF($B$1=\"中文\",E778,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 3,5 mg may be used per lamp after 31 December 2011"},"No limitation of use until 31 December 2011; 3,5 mg may be used per lamp after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 3,5 mg je Lampe verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于3.5毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C779,IF($B$1=\"Deutsch\",D779,IF($B$1=\"中文\",E779,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 5 mg may be used per lamp after 31 December 2011"},"No limitation of use until 31 December 2011; 5 mg may be used per lamp after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 5 mg je Lampe verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于5毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C780,IF($B$1=\"Deutsch\",D780,IF($B$1=\"中文\",E780,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 13 mg may be used per lamp after 31 December 2011"},"No limitation of use until 31 December 2011; 13 mg may be used per lamp after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 13 mg je Lampe verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于13毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C781,IF($B$1=\"Deutsch\",D781,IF($B$1=\"中文\",E781,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 15 mg may be used per lamp after 31 December 2011"},"No limitation of use until 31 December 2011; 15 mg may be used per lamp after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 15 mg je Lampe verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个灯中含量小于等于15毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C782,IF($B$1=\"Deutsch\",D782,IF($B$1=\"中文\",E782,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C783,IF($B$1=\"Deutsch\",D783,IF($B$1=\"中文\",E783,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 30 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 30 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 30 mg je Brennstelle verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个点火器中含量小于等于30毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C784,IF($B$1=\"Deutsch\",D784,IF($B$1=\"中文\",E784,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 40 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 40 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 40 mg je Brennstelle verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个点火器中含量小于等于40毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C785,IF($B$1=\"Deutsch\",D785,IF($B$1=\"中文\",E785,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 40 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 40 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 40 mg je Brennstelle verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个点火器中含量小于等于40毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C786,IF($B$1=\"Deutsch\",D786,IF($B$1=\"中文\",E786,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C787,IF($B$1=\"Deutsch\",D787,IF($B$1=\"中文\",E787,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 25 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 25 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 25 mg je Brennstelle verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个点火器中含量小于等于25毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C788,IF($B$1=\"Deutsch\",D788,IF($B$1=\"中文\",E788,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 30 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 30 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 30 mg je Brennstelle verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个点火器中含量小于等于30毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C789,IF($B$1=\"Deutsch\",D789,IF($B$1=\"中文\",E789,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use until 31 December 2011; 40 mg may be used per burner after 31 December 2011"},"No limitation of use until 31 December 2011; 40 mg may be used per burner after 31 December 2011","Unbegrenzte Verwendung bis 31. Dezember 2011; nach dem 31. Dezember 2011 dürfen 40 mg je Brennstelle verwendet werden.","无限制使用至2011年12月31日；2011年12月31日之后，每个点火器中含量小于等于40毫克可以被使用。"]
[null,{"$f":"IF($B$1=\"English\",C790,IF($B$1=\"Deutsch\",D790,IF($B$1=\"中文\",E790,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 13 April 2015"},"Expires on 13 April 2015","Läuft am 13. April 2015 ab.","截至2015年04月13日"]
[null,{"$f":"IF($B$1=\"English\",C791,IF($B$1=\"Deutsch\",D791,IF($B$1=\"中文\",E791,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C792,IF($B$1=\"Deutsch\",D792,IF($B$1=\"中文\",E792,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C793,IF($B$1=\"Deutsch\",D793,IF($B$1=\"中文\",E793,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C794,IF($B$1=\"Deutsch\",D794,IF($B$1=\"中文\",E794,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C795,IF($B$1=\"Deutsch\",D795,IF($B$1=\"中文\",E795,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C796,IF($B$1=\"Deutsch\",D796,IF($B$1=\"中文\",E796,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C797,IF($B$1=\"Deutsch\",D797,IF($B$1=\"中文\",E797,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C798,IF($B$1=\"Deutsch\",D798,IF($B$1=\"中文\",E798,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C799,IF($B$1=\"Deutsch\",D799,IF($B$1=\"中文\",E799,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C800,IF($B$1=\"Deutsch\",D800,IF($B$1=\"中文\",E800,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C801,IF($B$1=\"Deutsch\",D801,IF($B$1=\"中文\",E801,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C802,IF($B$1=\"Deutsch\",D802,IF($B$1=\"中文\",E802,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 January 2013 and after that date may be used in spare parts for EEE placed on the market before 1 January 2013"},"Expires on 1 January 2013 and after that date may be used in spare parts for EEE placed on the market before 1 January 2013","Läuft am 1. Januar 2013 ab. Danach Verwendung zulässig in Ersatzteilen für Elektro- und Elektronikgeräte, die vor dem 1. Januar 2013 in Verkehr gebracht wurden.","豁免至2013年1月1日，在该日期之后，2013年1月1前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C803,IF($B$1=\"Deutsch\",D803,IF($B$1=\"中文\",E803,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C804,IF($B$1=\"Deutsch\",D804,IF($B$1=\"中文\",E804,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 January 2012 and after that date may be used in spare parts for EEE placed on the market before 1 January 2012"},"Expires on 1 January 2012 and after that date may be used in spare parts for EEE placed on the market before 1 January 2012","Läuft am 1. Januar 2012 ab. Danach Verwendung zulässig in Ersatzteilen für Elektro- und Elektronikgeräte, die vor dem 1. Januar 2012 in Verkehr gebracht wurden.","豁免至2012年1月1日，在该日期之后，2012年1月1前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C805,IF($B$1=\"Deutsch\",D805,IF($B$1=\"中文\",E805,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C806,IF($B$1=\"Deutsch\",D806,IF($B$1=\"中文\",E806,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C807,IF($B$1=\"Deutsch\",D807,IF($B$1=\"中文\",E807,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C808,IF($B$1=\"Deutsch\",D808,IF($B$1=\"中文\",E808,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"May be used in spare parts for EEE placed on the market before 24 September 2010"},"May be used in spare parts for EEE placed on the market before 24 September 2010","Darf in Ersatzteilen für Elektro- und Elektronikgeräte verwendet werden, die vor dem 24. September 2010 in Verkehr gebracht wurden","2010年9月24前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C809,IF($B$1=\"Deutsch\",D809,IF($B$1=\"中文\",E809,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 January 2013 and after that date may be used in spare parts for EEE placed on the market before 1 January 2013"},"Expires on 1 January 2013 and after that date may be used in spare parts for EEE placed on the market before 1 January 2013","Läuft am 1. Januar 2013 ab. Danach Verwendung zulässig in Ersatzteilen für Elektro- und Elektronikgeräte, die vor dem 1. Januar 2013 in Verkehr gebracht wurden.","豁免至2013年1月1日，在该日期之后，2013年1月1前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C810,IF($B$1=\"Deutsch\",D810,IF($B$1=\"中文\",E810,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"May be used in spare parts for EEE placed on the market before 24 September 2010"},"May be used in spare parts for EEE placed on the market before 24 September 2010","Darf in Ersatzteilen für Elektro- und Elektronikgeräte verwendet werden, die vor dem 24. September 2010 in Verkehr gebracht wurden","2010年9月24前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C811,IF($B$1=\"Deutsch\",D811,IF($B$1=\"中文\",E811,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C812,IF($B$1=\"Deutsch\",D812,IF($B$1=\"中文\",E812,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C813,IF($B$1=\"Deutsch\",D813,IF($B$1=\"中文\",E813,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 January 2011 and after that date may be used in spare parts for EEE placed on the market before 1 January 2011"},"Expires on 1 January 2011 and after that date may be used in spare parts for EEE placed on the market before 1 January 2011","Läuft am 1. Januar 2011 ab. Danach Verwendung zulässig in Ersatzteilen für Elektro- und Elektronikgeräte, die vor dem 1. Januar 2011 in Verkehr gebracht wurden.","豁免至2011年1月1日，在该日期之后，2013年1月1前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C814,IF($B$1=\"Deutsch\",D814,IF($B$1=\"中文\",E814,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C815,IF($B$1=\"Deutsch\",D815,IF($B$1=\"中文\",E815,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 September 2013"},"Expires on 1 September 2013","Läuft am 1. September 2013 ab.","豁免至2013年09月01日"]
[null,{"$f":"IF($B$1=\"English\",C816,IF($B$1=\"Deutsch\",D816,IF($B$1=\"中文\",E816,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C817,IF($B$1=\"Deutsch\",D817,IF($B$1=\"中文\",E817,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 January 2011"},"Expires on 1 January 2011","Läuft am 1. Januar 2011 ab.","豁免至2011年01月01日"]
[null,{"$f":"IF($B$1=\"English\",C818,IF($B$1=\"Deutsch\",D818,IF($B$1=\"中文\",E818,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C819,IF($B$1=\"Deutsch\",D819,IF($B$1=\"中文\",E819,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 June 2011"},"Expires on 1 June 2011","Läuft am 1. Juni 2011 ab.","豁免至2011年06月01日"]
[null,{"$f":"IF($B$1=\"English\",C820,IF($B$1=\"Deutsch\",D820,IF($B$1=\"中文\",E820,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 June 2011"},"Expires on 1 June 2011","Läuft am 1. Juni 2011 ab.","豁免至2011年06月01日"]
[null,{"$f":"IF($B$1=\"English\",C821,IF($B$1=\"Deutsch\",D821,IF($B$1=\"中文\",E821,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C822,IF($B$1=\"Deutsch\",D822,IF($B$1=\"中文\",E822,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"May be used in spare parts for electric and electronic devices placed on the market before 24 September 2010"},"May be used in spare parts for electric and electronic devices placed on the market before 24 September 2010","Darf in Ersatzteilen für Elektro- und Elektronikgeräte verwendet werden, die vor dem 24. September 2010 in Verkehr gebracht wurden.","2010年9月24前投放市场的电子电气产品的备件中仍可使用"]
[null,{"$f":"IF($B$1=\"English\",C823,IF($B$1=\"Deutsch\",D823,IF($B$1=\"中文\",E823,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C824,IF($B$1=\"Deutsch\",D824,IF($B$1=\"中文\",E824,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C825,IF($B$1=\"Deutsch\",D825,IF($B$1=\"中文\",E825,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 June 2011"},"Expires on 1 June 2011","Läuft am 1. Juni 2011 ab.","豁免至2011年06月01日"]
[null,{"$f":"IF($B$1=\"English\",C826,IF($B$1=\"Deutsch\",D826,IF($B$1=\"中文\",E826,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expired on 24 September 2010"},"Expired on 24 September 2010","Am 24. September 2010 abgelaufen.","豁免至2010年09月24日"]
[null,{"$f":"IF($B$1=\"English\",C827,IF($B$1=\"Deutsch\",D827,IF($B$1=\"中文\",E827,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C828,IF($B$1=\"Deutsch\",D828,IF($B$1=\"中文\",E828,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C829,IF($B$1=\"Deutsch\",D829,IF($B$1=\"中文\",E829,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C830,IF($B$1=\"Deutsch\",D830,IF($B$1=\"中文\",E830,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C831,IF($B$1=\"Deutsch\",D831,IF($B$1=\"中文\",E831,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C832,IF($B$1=\"Deutsch\",D832,IF($B$1=\"中文\",E832,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C833,IF($B$1=\"Deutsch\",D833,IF($B$1=\"中文\",E833,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expired on 1 July 2010"},"Expired on 1 July 2010","Läuft am 1. Juli 2010 ab.","豁免至2010年07月01日"]
[null,{"$f":"IF($B$1=\"English\",C834,IF($B$1=\"Deutsch\",D834,IF($B$1=\"中文\",E834,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C835,IF($B$1=\"Deutsch\",D835,IF($B$1=\"中文\",E835,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-"]
[null,{"$f":"IF($B$1=\"English\",C836,IF($B$1=\"Deutsch\",D836,IF($B$1=\"中文\",E836,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 July 2014"},"Expires on 1 July 2014","Läuft am 1. Juli 2014 ab.","豁免至2014年07月01日"]
[null,{"$f":"IF($B$1=\"English\",C837,IF($B$1=\"Deutsch\",D837,IF($B$1=\"中文\",E837,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 31 December 2013"},"Expires on 31 December 2013","Läuft am 31. Dezember 2013 ab.","豁免至2013年12月31日"]
[null,{"$f":"IF($B$1=\"English\",C838,IF($B$1=\"Deutsch\",D838,IF($B$1=\"中文\",E838,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Equipment utilising or detecting ionising radiation"},"Equipment utilising or detecting ionising radiation","Geräte, die ionisierende Strahlung verwenden bzw  nachweisen","使用或检测电离辐射的设备"]
[null,{"$f":"IF($B$1=\"English\",C839,IF($B$1=\"Deutsch\",D839,IF($B$1=\"中文\",E839,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead, cadmium and mercury in detectors for ionising radiation"}," Lead, cadmium and mercury in detectors for ionising radiation"," Blei, Cadmium und Quecksilber in Detektoren für ionisierende Strahlung","电离辐射探测器中的铅，镉和汞"]
[null,{"$f":"IF($B$1=\"English\",C840,IF($B$1=\"Deutsch\",D840,IF($B$1=\"中文\",E840,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead bearings in X-ray tubes"}," Lead bearings in X-ray tubes"," Bleilager in Röntgenröhren","X射线管轴承中的铅"]
[null,{"$f":"IF($B$1=\"English\",C841,IF($B$1=\"Deutsch\",D841,IF($B$1=\"中文\",E841,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in electromagnetic radiation amplification devices: micro-channel plate and capillary plate"}," Lead in electromagnetic radiation amplification devices: micro-channel plate and capillary plate"," Blei in Verstärkern von elektromagnetischer Strahlung: Mikrokanalplatte und Kapillarplatte","电磁辐射放大器—微通道板和毛细板中的铅"]
[null,{"$f":"IF($B$1=\"English\",C842,IF($B$1=\"Deutsch\",D842,IF($B$1=\"中文\",E842,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in glass frit of X-ray tubes and image intensifiers and lead in glass frit binder for assembly of gas lasers and for vacuum tubes that convert electromagnetic radiation into electrons"}," Lead in glass frit of X-ray tubes and image intensifiers and lead in glass frit binder for assembly of gas lasers and for vacuum tubes that convert electromagnetic radiation into electrons"," Blei in Glasfritten von Röntgenröhren und Bildverstärkern und Blei in Glasfritten-Bindern zur Befestigung von Gaslasern und für Vakuumröhren, die elektromagnetische Strahlung in Elektronen umwandeln","X射线管和图像增强器的玻璃材料中的铅，以及用于气体激光器组件和将电磁辐射转换成电子的真空管的玻璃材料粘合剂中的铅"]
[null,{"$f":"IF($B$1=\"English\",C843,IF($B$1=\"Deutsch\",D843,IF($B$1=\"中文\",E843,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in shielding for ionising radiation"}," Lead in shielding for ionising radiation"," Blei in Abschirmungen gegen ionisierende Strahlung","电离辐射隔离屏中的铅"]
[null,{"$f":"IF($B$1=\"English\",C844,IF($B$1=\"Deutsch\",D844,IF($B$1=\"中文\",E844,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in X-ray test objects"}," Lead in X-ray test objects"," Blei in Testobjekten im Röntgenbereich","X射线测试对象中的铅"]
[null,{"$f":"IF($B$1=\"English\",C845,IF($B$1=\"Deutsch\",D845,IF($B$1=\"中文\",E845,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead stearate X-ray diffraction crystals"}," Lead stearate X-ray diffraction crystals"," Bleistearat-Kristalle zur Beugung von Röntgenstrahlen","\n硬脂酸铅晶体用于X射线衍射"]
[null,{"$f":"IF($B$1=\"English\",C846,IF($B$1=\"Deutsch\",D846,IF($B$1=\"中文\",E846,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Radioactive cadmium isotope source for portable X-ray fluorescence spectrometers"}," Radioactive cadmium isotope source for portable X-ray fluorescence spectrometers"," Quelle von radioaktiven Cadmiumisotopen für tragbare Röntgenfluoreszenz-Spektrometer","用于便携式X射线荧光光谱仪的放射性镉同位素源"]
[null,{"$f":"IF($B$1=\"English\",C847,IF($B$1=\"Deutsch\",D847,IF($B$1=\"中文\",E847,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sensors, detectors and electrodes"},"Sensors, detectors and electrodes","Sensoren, Detektoren und Elektroden","传感器，检测器和电极"]
[null,{"$f":"IF($B$1=\"English\",C848,IF($B$1=\"Deutsch\",D848,IF($B$1=\"中文\",E848,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead and cadmium in ion selective electrodes including glass of pH electrodes"}," Lead and cadmium in ion selective electrodes including glass of pH electrodes"," Blei und Cadmium in ionenselektiven Elektroden, einschließlich Glas von pH-Elektroden","离子选择性电极包括pH玻璃电极中的铅和镉"]
[null,{"$f":"IF($B$1=\"English\",C849,IF($B$1=\"Deutsch\",D849,IF($B$1=\"中文\",E849,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead anodes in electrochemical oxygen sensors"}," Lead anodes in electrochemical oxygen sensors"," Bleianoden in elektrochemischen Sauerstoffsensoren","电化学氧传感器中的铅阳极"]
[null,{"$f":"IF($B$1=\"English\",C850,IF($B$1=\"Deutsch\",D850,IF($B$1=\"中文\",E850,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead, cadmium and mercury in infra-red light detectors"}," Lead, cadmium and mercury in infra-red light detectors"," Blei, Cadmium und Quecksilber in Infrarotdetektoren","红外探测器中的铅，镉和汞"]
[null,{"$f":"IF($B$1=\"English\",C851,IF($B$1=\"Deutsch\",D851,IF($B$1=\"中文\",E851,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Mercury in reference electrodes: low chloride mercury chloride, mercury sulphate and mercury oxide"}," Mercury in reference electrodes: low chloride mercury chloride, mercury sulphate and mercury oxide"," Quecksilber in Referenzelektroden: Quecksilberchlorid mit niedrigem Chloridgehalt, Quecksilbersulfat und Quecksilberoxid","参照电极中的汞：低氯氯化汞，硫酸汞和氧化汞"]
[null,{"$f":"IF($B$1=\"English\",C852,IF($B$1=\"Deutsch\",D852,IF($B$1=\"中文\",E852,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Others"},"Others","Andere","其他"]
[null,{"$f":"IF($B$1=\"English\",C853,IF($B$1=\"Deutsch\",D853,IF($B$1=\"中文\",E853,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Cadmium in helium-cadmium lasers"}," Cadmium in helium-cadmium lasers"," Cadmium in Helium-Cadmium-Lasern","氦 - 镉-激光器中的镉"]
[null,{"$f":"IF($B$1=\"English\",C854,IF($B$1=\"Deutsch\",D854,IF($B$1=\"中文\",E854,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead and cadmium in atomic absorption spectroscopy lamps"}," Lead and cadmium in atomic absorption spectroscopy lamps"," Blei und Cadmium in Atomabsorptionsspektroskopielampen","原子吸收光谱灯中的铅和镉"]
[null,{"$f":"IF($B$1=\"English\",C855,IF($B$1=\"Deutsch\",D855,IF($B$1=\"中文\",E855,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in alloys as a superconductor and thermal conductor in MRI"}," Lead in alloys as a superconductor and thermal conductor in MRI"," Blei in Legierungen als Supraleiter und Wärmeleiter in der MRI","MRI中超导和热导合金中的铅"]
[null,{"$f":"IF($B$1=\"English\",C856,IF($B$1=\"Deutsch\",D856,IF($B$1=\"中文\",E856,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead and cadmium in metallic bonds to superconducting materials in MRI and SQUID detectors"}," Lead and cadmium in metallic bonds to superconducting materials in MRI and SQUID detectors"," Blei und Cadmium in metallischen Bindungen von Supraleitern in MRI- und SQUID-Detektoren","MRI和SQUID探测器的超导材料金属键中的铅和镉"]
[null,{"$f":"IF($B$1=\"English\",C857,IF($B$1=\"Deutsch\",D857,IF($B$1=\"中文\",E857,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in counterweights"}," Lead in counterweights"," Blei in Gegengewichten","配重中的铅"]
[null,{"$f":"IF($B$1=\"English\",C858,IF($B$1=\"Deutsch\",D858,IF($B$1=\"中文\",E858,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in single crystal piezoelectric materials for ultrasonic transducers"}," Lead in single crystal piezoelectric materials for ultrasonic transducers"," Blei in piezoelektrischen Einkristallen für Ultraschallwandler","超声换能器的单晶压电材料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C859,IF($B$1=\"Deutsch\",D859,IF($B$1=\"中文\",E859,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in solders for bonding to ultrasonic transducers"}," Lead in solders for bonding to ultrasonic transducers"," Blei in Verbindungsloten für Ultraschallwandler","超声换能器粘结焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C860,IF($B$1=\"Deutsch\",D860,IF($B$1=\"中文\",E860,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Mercury in very high accuracy capacitance and loss measurement bridges and in high frequency RF switches and relays in monitoring and control instruments not exceeding 20 mg of mercury per switch or relay"}," Mercury in very high accuracy capacitance and loss measurement bridges and in high frequency RF switches and relays in monitoring and control instruments not exceeding 20 mg of mercury per switch or relay"," Quecksilber in Höchstpräzisions-Kapazitäts- und Verlustfaktor-Messbrücken und in Hochfrequenz-RF-Schaltern und -Relais in Überwachungs- und Kontrollinstrumenten mit höchstens 20 mg Quecksilber je Schalter bzw  Relais","超高精度电容和损耗电桥中的汞，监控仪器的高频RF开关和继电器中的汞，每个开关和续电器中汞含量不超过20mg"]
[null,{"$f":"IF($B$1=\"English\",C861,IF($B$1=\"Deutsch\",D861,IF($B$1=\"中文\",E861,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in solders in portable emergency defibrillators"}," Lead in solders in portable emergency defibrillators"," Blei in Loten für tragbare Notfalldefibrillatoren","便携式应急除颤器焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C862,IF($B$1=\"Deutsch\",D862,IF($B$1=\"中文\",E862,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in solders of high performance infrared imaging modules to detect in the range 8-14 μm"}," Lead in solders of high performance infrared imaging modules to detect in the range 8-14 μm"," Blei in Loten für Hochleistungs-Infrarot-Bildgebungsmodule zur Detektion im Bereich 8-14 μm","检测范围为8-14微米的高性能红外成像模块焊料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C863,IF($B$1=\"Deutsch\",D863,IF($B$1=\"中文\",E863,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Lead in Liquid crystal on silicon (LCoS) displays"}," Lead in Liquid crystal on silicon (LCoS) displays"," Blei in LCoS-Displays (Flüssigkristall auf Silizium)","硅基液晶显示器中的铅"]
[null,{"$f":"IF($B$1=\"English\",C864,IF($B$1=\"Deutsch\",D864,IF($B$1=\"中文\",E864,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Cadmium in X-ray measurement filters"}," Cadmium in X-ray measurement filters"," Cadmium in Messfiltern für Röntgenstrahlen","X射线测量过滤器中的镉"]
[null,{"$f":"IF($B$1=\"English\",C865,IF($B$1=\"Deutsch\",D865,IF($B$1=\"中文\",E865,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Commitment"},"Commitment","Verpflichtungserklärung","承诺"]
[null,{"$f":"IF($B$1=\"English\",C866,IF($B$1=\"Deutsch\",D866,IF($B$1=\"中文\",E866,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"We do not accept substances of the SVHC-list above 0,1% in products or there spare parts. The supplier is obliged to track SVHC candidate list regularly (e.g. on ECHA homepage) and to inform Bosch purchasing contact immediately if he gets information that any substance stated in SVHC-candidate list may be included in supplied material ( ≥ 0,1 %)."},"We do not accept substances of the SVHC-list above 0,1% in products or there spare parts. The supplier is obliged to track SVHC candidate list regularly (e.g. on ECHA homepage) and to inform Bosch purchasing contact immediately if he gets information that any substance stated in SVHC-candidate list may be included in supplied material ( ≥ 0,1 %).","Wir akzeptieren keine  Stoffe der SVHC-Liste in einer Konzentration > 0,1 % in unseren Produkten oder in deren Einzelteilen. Der Lieferant ist verpflichtet, die SVHC Kandidatenliste regelmäßig zu verfolgen (z.B. auf der ECHA Homepage). Er ist verpflichtet,den Bosch Einkauf sofort zu kontaktieren, wenn der Lieferant Informationen hat, dass eine Substanz, die in der SVHC Kandidaten liste gelistet ist, im gelieferten Material enthalten sein kann (>_0.1%)“. ","供应商有义务定期跟进SVHC的候选列表（例如在ECHA的主页上）。当供应商发现任何在SVHC的候选列表中的物质可能在已经供应给博世的材料中含有（>_0.1%)，应该立即告知他们在博世采购部的联系人。"]
[null,{"$f":"IF($B$1=\"English\",C867,IF($B$1=\"Deutsch\",D867,IF($B$1=\"中文\",E867,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SVHC Candidate List"},"SVHC Candidate List","SVHC Kandidatenliste:","SVHC候选清单："]
[null,{"$f":"IF($B$1=\"English\",C868,IF($B$1=\"Deutsch\",D868,IF($B$1=\"中文\",E868,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SVHC in supplied material:"},"SVHC in supplied material:","SVHC in der Lieferung:","供应给博世的材料中含有的SVHC："]
[null,{"$f":"IF($B$1=\"English\",C869,IF($B$1=\"Deutsch\",D869,IF($B$1=\"中文\",E869,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tricresyl phosphates (TCP)"},"Tricresyl phosphates (TCP)","Trikresylphosphat (TKP)","磷酸三甲苯酯（TCP）"]
[null,{"$f":"IF($B$1=\"English\",C870,IF($B$1=\"Deutsch\",D870,IF($B$1=\"中文\",E870,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"How to fill out"},"How to fill out","Hinweise zur Bearbeitung","如何填写"]
[null,{"$f":"IF($B$1=\"English\",C871,IF($B$1=\"Deutsch\",D871,IF($B$1=\"中文\",E871,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Please enable macro"},"Please enable macro","Bitte Makros aktivieren ","请启用宏"]
[null,{"$f":"IF($B$1=\"English\",C872,IF($B$1=\"Deutsch\",D872,IF($B$1=\"中文\",E872,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Below you find the working steps"},"Below you find the working steps","Im Folgenden sehen Sie die Bearbeitungsschritte","下面是填写步骤"]
[null,{"$f":"IF($B$1=\"English\",C873,IF($B$1=\"Deutsch\",D873,IF($B$1=\"中文\",E873,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"If you have questions see the tab \"FAQ\""},"If you have questions see the tab \"FAQ\"","Bei zusätzlichen Fragen bitte im Register \"FAQ\" nachschauen","如有疑问，请参见“常见问题解答”"]
[null,{"$f":"IF($B$1=\"English\",C874,IF($B$1=\"Deutsch\",D874,IF($B$1=\"中文\",E874,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"To start click on tab \"Cover_Sheet\""},"To start click on tab \"Cover_Sheet\"","Zum Start in den Register \"Cover_Sheet\" wechseln","跳转到启动选项卡中“Cover_Sheet”"]
[null,{"$f":"IF($B$1=\"English\",C875,IF($B$1=\"Deutsch\",D875,IF($B$1=\"中文\",E875,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Candidate List of SVHC for authorisation"},"Candidate List of SVHC for authorisation","Candidate List of SVHC for authorisation","SVHC授权候选清单"]
[null,{"$f":"IF($B$1=\"English\",C876,IF($B$1=\"Deutsch\",D876,IF($B$1=\"中文\",E876,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Annex XVII restrictions: https://echa.europa.eu/substances-restricted-under-reach"},"Annex XVII restrictions: https://echa.europa.eu/substances-restricted-under-reach","Annex XVII restrictions: https://echa.europa.eu/substances-restricted-under-reach","附件XVII限制物质: https://echa.europa.eu/substances-restricted-under-reach"]
[null,{"$f":"IF($B$1=\"English\",C877,IF($B$1=\"Deutsch\",D877,IF($B$1=\"中文\",E877,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Applications for exemptions, renewal of exemptions or, mutatis mutandis, for revoking an exemption may be submitted by a manufacturer, the authorised representative of a manufacturer, or any economic operator in the supply chain and shall include at least the following:"},"Applications for exemptions, renewal of exemptions or, mutatis mutandis, for revoking an exemption may be submitted by a manufacturer, the authorised representative of a manufacturer, or any economic operator in the supply chain and shall include at least the following:","Anträge auf Ausnahmen, Erneuerung von Ausnahmen oder auf Widerruf von Ausnahmen können von einem Hersteller, einem Bevollmächtigten des Herstellers oder einem Wirtschaftsakteur in der Lieferkette eingereicht werden und müssen Folgendes enthalten:","制造商，制造商的委托人，或者供应链的经济参与者可以提出豁免申请、豁免更新申请、豁免调整申请以及豁免撤销申请。这些申请中必须包含以下内容："]
[null,{"$f":"IF($B$1=\"English\",C878,IF($B$1=\"Deutsch\",D878,IF($B$1=\"中文\",E878,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(a) the name, address and contact details of the applicant;"},"(a) the name, address and contact details of the applicant;","a) Namen, Anschrift und Kontaktdaten des Antragstellers;","a）申请人的名称，地址和具体联系方式;"]
[null,{"$f":"IF($B$1=\"English\",C879,IF($B$1=\"Deutsch\",D879,IF($B$1=\"中文\",E879,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(b) information on the material or component and the specific uses of the substance in the material and component for which an exemption, or its revocation, is requested and its particular characteristics;"},"(b) information on the material or component and the specific uses of the substance in the material and component for which an exemption, or its revocation, is requested and its particular characteristics;","b) Angaben über den Werkstoff oder das Bauteil und die spezifischen Verwendungen des Stoffes im Werkstoff oder Bauteil, für den eine Ausnahme bzw. dessen Widerruf beantragt wird, sowie über seine besonderen Eigenschaften;","b）需要申请豁免或撤销豁免的材料或零部件的信息，物质在该材料或零部件中的具体用途，及其特性"]
[null,{"$f":"IF($B$1=\"English\",C880,IF($B$1=\"Deutsch\",D880,IF($B$1=\"中文\",E880,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(c) verifiable and referenced justification for an exemption, or its revocation, in line with the conditions established in Article 5;"},"(c) verifiable and referenced justification for an exemption, or its revocation, in line with the conditions established in Article 5;","c) eine überprüfbare und belegte Begründung für eine Ausnahme oder deren Widerruf, in Übereinstimmung mit den gemäß Artikel 5 festgelegten Bedingungen;","c)按照第5条中设定的情况，申请豁免或撤销豁免的有说服力的正当理由"]
[null,{"$f":"IF($B$1=\"English\",C881,IF($B$1=\"Deutsch\",D881,IF($B$1=\"中文\",E881,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(d) an analysis of possible alternative substances, materials or designs on a life-cycle basis, including, when available, information about independent research, peer-review studies and development activities by the applicant and an analysis of the availability of such alternatives;"},"(d) an analysis of possible alternative substances, materials or designs on a life-cycle basis, including, when available, information about independent research, peer-review studies and development activities by the applicant and an analysis of the availability of such alternatives;","d) eine am Lebenszykluskonzept ausgerichtete Analyse möglicher alternativer Stoffe, Werkstoffe oder Designs, einschließlich — soweit verfügbar — Informationen über unabhängige wissenschaftliche Untersuchungen, nach dem Peer-Review-Verfahren erstellte Studien und die Entwicklungstätigkeiten des Antragstellers sowie eine Analyse der Verfügbarkeit solcher Alternativen;","d)基于产品生命周期理念，分析可能的替代物质、替代材料或替代设计，包括申请者所做的独立研究的信息，同行评审研究和开发活动（如果有的话），以及针对此种替代品的可用性所做的分析"]
[null,{"$f":"IF($B$1=\"English\",C882,IF($B$1=\"Deutsch\",D882,IF($B$1=\"中文\",E882,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(e) information on the possible preparation for reuse or recycling of materials from waste EEE, and on the provisions relating to the appropriate treatment of waste according to Annex II to Directive 2002/96/EC;"},"(e) information on the possible preparation for reuse or recycling of materials from waste EEE, and on the provisions relating to the appropriate treatment of waste according to Annex II to Directive 2002/96/EC;","e) Informationen zur möglichen Vorbereitung von Werkstoffen aus Elektro- und Elektronik-Altgeräten zur Wiederverwendung oder zum Recycling und zu den Vorschriften über die angemessene Behandlung von Abfällen gemäß Anhang II der Richtlinie 2002/96/EG;","e)根据2002/96/EC号指令（WEEE）附件II，为了能对废弃的电子电气产品进行再利用或回收利用材料，可能做的准备工作，以及关于废弃物进行适当处理的预备工作。\n"]
[null,{"$f":"IF($B$1=\"English\",C883,IF($B$1=\"Deutsch\",D883,IF($B$1=\"中文\",E883,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(f) other relevant information;"},"(f) other relevant information;","f) sonstige relevante Informationen;","其他相关资料;"]
[null,{"$f":"IF($B$1=\"English\",C884,IF($B$1=\"Deutsch\",D884,IF($B$1=\"中文\",E884,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(g) the proposed actions to develop, request the development and/or to apply possible alternatives including a timetable for such actions by the applicant;"},"(g) the proposed actions to develop, request the development and/or to apply possible alternatives including a timetable for such actions by the applicant;","g) die vorgeschlagenen Schritte zur Entwicklung, zur Anforderung der Entwicklung und/oder zur Verwendung möglicher Alternativen einschließlich eines Zeitplans für solche Schritte durch den Antragsteller;","g)申请人建议采取何种行动进行开发、要求开发和/或申请可能的替代品，以及行动时间表"]
[null,{"$f":"IF($B$1=\"English\",C885,IF($B$1=\"Deutsch\",D885,IF($B$1=\"中文\",E885,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(h) where appropriate, an indication of the information which should be regarded as proprietary accompanied by verifiable justification;"},"(h) where appropriate, an indication of the information which should be regarded as proprietary accompanied by verifiable justification;","h) gegebenenfalls die Angabe der Informationen, die als proprietär angesehen werden sollten, wobei eine nachprüfbare Begründung zu geben ist;","h）如果可能，还可以提供能够作为申请理由佐证的其它信息"]
[null,{"$f":"IF($B$1=\"English\",C886,IF($B$1=\"Deutsch\",D886,IF($B$1=\"中文\",E886,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(i) when applying for an exemption, proposal for a precise and clear wording for the exemption;"},"(i) when applying for an exemption, proposal for a precise and clear wording for the exemption;","i) bei der Beantragung einer Ausnahme, einen Vorschlag für einen präzisen und eindeutigen Wortlaut der Ausnahme;","i)如提交豁免申请，建议该豁免条款应如何清晰准确的措辞"]
[null,{"$f":"IF($B$1=\"English\",C887,IF($B$1=\"Deutsch\",D887,IF($B$1=\"中文\",E887,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(j) a summary of the application."},"(j) a summary of the application.","j) eine Zusammenfassung des Antrags.","该申请的总结。"]
[null,{"$f":"IF($B$1=\"English\",C888,IF($B$1=\"Deutsch\",D888,IF($B$1=\"中文\",E888,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulation Text with exemptions 30.03.2023"},"Regulation Text with exemptions 30.03.2023","Text der Regulierung und Ausnahmen 30.03.2023","包含豁免的法規文本 30.03.2023"]
[null,{"$f":"IF($B$1=\"English\",C889,IF($B$1=\"Deutsch\",D889,IF($B$1=\"中文\",E889,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fill out: cover sheet, at least the yellow lines"},"Fill out: cover sheet, at least the yellow lines","Ausfüllen: Deckblatt, mindestens die gelben Felder","填写：封面页，黄色单元格为必填项"]
[null,{"$f":"IF($B$1=\"English\",C890,IF($B$1=\"Deutsch\",D890,IF($B$1=\"中文\",E890,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cover sheet - Selection: Type of supplied material"},"Cover sheet - Selection: Type of supplied material","Deckblatt - Auswählen: Art des gelieferten Materials","封面-选择:所提供材料的类型"]
[null,{"$f":"IF($B$1=\"English\",C891,IF($B$1=\"Deutsch\",D891,IF($B$1=\"中文\",E891,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Selection: division or Bosch reference list"},"Selection: division or Bosch reference list","Auswählen: Geschäftseinheit oder Bosch Reference List","选择:事业部或博世参考列表"]
[null,{"$f":"IF($B$1=\"English\",C892,IF($B$1=\"Deutsch\",D892,IF($B$1=\"中文\",E892,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fill out: if necessery, edit opened tabs (fill out the relevant fields only) and complete the cover sheet according the information in the tabs"},"Fill out: if necessery, edit opened tabs (fill out the relevant fields only) and complete the cover sheet according the information in the tabs","Ausfüllen: Angezeigte Register wenn notwendig bearbeiten (nur die zutreffenden Felder ausfüllen) und Angaben im Deckblatt entsprechend vervollständigen","填写:如有必要，编辑打开的标签(仅填写相关字段)，并根据标签中的信息填写封面"]
[null,{"$f":"IF($B$1=\"English\",C893,IF($B$1=\"Deutsch\",D893,IF($B$1=\"中文\",E893,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Send back "},"Send back ","Zurücksenden ","寄回"]
[null,{"$f":"IF($B$1=\"English\",C894,IF($B$1=\"Deutsch\",D894,IF($B$1=\"中文\",E894,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Selection: division or Bosch reference list - confirm with OK"},"Selection: division or Bosch reference list - confirm with OK","Auswählen: Geschäftseinheit oder Bosch Reference List - mit OK bestätigen","选择:事业部或博世参考列表 - OK确认"]
[null,{"$f":"IF($B$1=\"English\",C895,IF($B$1=\"Deutsch\",D895,IF($B$1=\"中文\",E895,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Send back: Print cover sheet, sign, scan, return to the responsible Bosch purchasing department the scan and the entire Excel file together in one e-mail."},"Send back: Print cover sheet, sign, scan, return to the responsible Bosch purchasing department the scan and the entire Excel file together in one e-mail.","Zurücksenden: Deckblatt drucken, unterschreiben, scannen, an den zuständigen Bosch-Einkauf den Scan und die gesamte Excel-Datei zusammen in einer E-Mail zurücksenden","退回:打印封面、签名、扫描，将扫描结果和整个电子表格文件一起通过电子邮件退回给负责的博世采购部门。"]
[null,{"$f":"IF($B$1=\"English\",C896,IF($B$1=\"Deutsch\",D896,IF($B$1=\"中文\",E896,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Summary of declarations is possible when the ingredients are identical in type and concentration in the supplied materials (e. g. use of the same material in product series or product families). In these cases several material numbers, supplier- and/or Bosch-part numbers may be entered in the same form sheet."},"Summary of declarations is possible when the ingredients are identical in type and concentration in the supplied materials (e. g. use of the same material in product series or product families). In these cases several material numbers, supplier- and/or Bosch-part numbers may be entered in the same form sheet.","Zusammenfassung von Deklarationen möglich, wenn die Inhaltsstoffe nach Art und Konzentration in den gelieferten Materialien identisch sind (z. B. Verwendung desselben Werkstoffs in Baureihen oder Produktfamilien). Dann können mehrere Material-Nummern, Lieferant- bzw. Bosch-Sachnummern auf demselben Formblatt eingetragen werden.","如果多个供应材料的构成成分类型和浓度完全一致（例如，使用相同的材料在产品系列和产品家族中），也可以进行综合申报。也就是说，可以将这几个材料的物料编号，供应商或博世零件号填在同一个表格进行申报。"]
[null,{"$f":"IF($B$1=\"English\",C897,IF($B$1=\"Deutsch\",D897,IF($B$1=\"中文\",E897,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"You cannot select multiple divisions at once. "},"You cannot select multiple divisions at once. ","Es ist nicht möglich mehrere Geschäftseinheiten gleichzeitig auszuwählen. ","不可同时选择多个事业部。"]
[null,{"$f":"IF($B$1=\"English\",C898,IF($B$1=\"Deutsch\",D898,IF($B$1=\"中文\",E898,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tabs to work on"},"Tabs to work on","Zu bearbeitende Register","待处理的选项"]
[null,{"$f":"IF($B$1=\"English\",C899,IF($B$1=\"Deutsch\",D899,IF($B$1=\"中文\",E899,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Name of only representative in accordance with REACH (see FAQ for more information)"},"Name of only representative in accordance with REACH (see FAQ for more information)","Name des Alleinvertreters gemäß REACH\n(für mehr Informationen s. FAQ)","REACH独家代理的名称\n（欲了解更多信息，请参见常见问题解答）“"]
[null,{"$f":"IF($B$1=\"English\",C900,IF($B$1=\"Deutsch\",D900,IF($B$1=\"中文\",E900,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Remains in or on the Bosch product"},"Remains in or on the Bosch product","Verbleibt im oder am Bosch-Produkt","保留在博世产品里或产品上"]
[null,{"$f":"IF($B$1=\"English\",C901,IF($B$1=\"Deutsch\",D901,IF($B$1=\"中文\",E901,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Does not remain in or on the Bosch product"},"Does not remain in or on the Bosch product","Verbleibt nicht im oder am Bosch-Produkt","不保留在博世产品里或产品上"]
[null,{"$f":"IF($B$1=\"English\",C902,IF($B$1=\"Deutsch\",D902,IF($B$1=\"中文\",E902,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Merchandise automotive"},"Merchandise automotive","Handelsware Automobil","汽车商品"]
[null,{"$f":"IF($B$1=\"English\",C903,IF($B$1=\"Deutsch\",D903,IF($B$1=\"中文\",E903,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Merchandise non-automotive"},"Merchandise non-automotive","Handelsware Nicht-Automobil","非汽车的商品"]
[null,{"$f":"IF($B$1=\"English\",C904,IF($B$1=\"Deutsch\",D904,IF($B$1=\"中文\",E904,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bosch Reference List"},"Bosch Reference List","Bosch Reference List","博世参考列表"]
[null,{"$f":"IF($B$1=\"English\",C905,IF($B$1=\"Deutsch\",D905,IF($B$1=\"中文\",E905,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydraulic oils"},"Hydraulic oils","Hydrauliköle","液压油"]
[null,{"$f":"IF($B$1=\"English\",C906,IF($B$1=\"Deutsch\",D906,IF($B$1=\"中文\",E906,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Metallic surface"},"Metallic surface","Metallische Oberfläche","金属表面"]
[null,{"$f":"IF($B$1=\"English\",C907,IF($B$1=\"Deutsch\",D907,IF($B$1=\"中文\",E907,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product or merchandise, does not contain substances that are released in  proper use"},"Product or merchandise, does not contain substances that are released in  proper use","Produkt oder Handelsware, enthält keine Stoffe, die im bestimmungsgemäßen Gebrauch freigesetzt werden","产品或商品，不包含正常使用下会挥发的物质"]
[null,{"$f":"IF($B$1=\"English\",C908,IF($B$1=\"Deutsch\",D908,IF($B$1=\"中文\",E908,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product or merchandise contains substances that are released in proper use"},"Product or merchandise contains substances that are released in proper use","Produkt oder Handelsware, enthält Stoffe, die im bestimmungsgemäßen Gebrauch freigesetzt werden","产品或商品，包含正常使用下会挥发的物质"]
[null,{"$f":"IF($B$1=\"English\",C909,IF($B$1=\"Deutsch\",D909,IF($B$1=\"中文\",E909,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Keyword"},"Keyword","Stichwort","关键词"]
[null,{"$f":"IF($B$1=\"English\",C910,IF($B$1=\"Deutsch\",D910,IF($B$1=\"中文\",E910,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Question"},"Question","Frage","问题"]
[null,{"$f":"IF($B$1=\"English\",C911,IF($B$1=\"Deutsch\",D911,IF($B$1=\"中文\",E911,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Answer"},"Answer","Antwort","回复"]
[null,{"$f":"IF($B$1=\"English\",C912,IF($B$1=\"Deutsch\",D912,IF($B$1=\"中文\",E912,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sole Representative (Reach)"},"Sole Representative (Reach)","Alleinvertreter (Reach)","独家代理（REACH）"]
[null,{"$f":"IF($B$1=\"English\",C913,IF($B$1=\"Deutsch\",D913,IF($B$1=\"中文\",E913,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Companies from countries outside of the European Union cannot (pre-)register on their own, they need to appoint an Only Representative. The Only Representative represents your company officially and performs your company’s REACH obligations. \nFor further information see: Regulation (EC) No 1907/2006 - REACH Article 8"},"Companies from countries outside of the European Union cannot (pre-)register on their own, they need to appoint an Only Representative. The Only Representative represents your company officially and performs your company’s REACH obligations. \nFor further information see: Regulation (EC) No 1907/2006 - REACH Article 8","Unternehmen aus Ländern außerhalb der EU können sich nicht selbst (vor)registrieren; sie brauchen dazu einen Alleinvertreter. Der Alleinvertreter vertritt offiziell Ihr Unternehmen und sorgt für die Einhaltung der REACH-Verpflichtungen durch ihr Unternehmen. Für mehr Informationen s. Verordnung (EG) Nr. 1907/2006 Artikel 8","来自欧盟以外国家的公司不能自己（预）注册化学品；他们需要指定独家代理。独家代理正式代表您的公司处理您公司的REACH法规要求。欲了解更多信息，请参阅（EC）1907/2006号法规 - REACH 第8条"]
[null,{"$f":"IF($B$1=\"English\",C914,IF($B$1=\"Deutsch\",D914,IF($B$1=\"中文\",E914,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Batteries"},"Batteries","Batterie","电池"]
[null,{"$f":"IF($B$1=\"English\",C915,IF($B$1=\"Deutsch\",D915,IF($B$1=\"中文\",E915,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What does this cover?"},"What does this cover?","Was fällt darunter?","包含哪些内容？"]
[null,{"$f":"IF($B$1=\"English\",C916,IF($B$1=\"Deutsch\",D916,IF($B$1=\"中文\",E916,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nportable batteries, traction batteries, accumulators"},"examples:\nportable batteries, traction batteries, accumulators","Beispiele:\nGerätebatterien, Fahrzeug-Antriebsbatterien, Akkumulatoren","“例子：\n便携电池，车辆牵引电池，充电电池“"]
[null,{"$f":"IF($B$1=\"English\",C917,IF($B$1=\"Deutsch\",D917,IF($B$1=\"中文\",E917,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Equipped PCB; electronic assembly; electrical assembly"},"Equipped PCB; electronic assembly; electrical assembly","bestückte Leiterplatte; Elektronik-Baugruppe; Elektrik-Baugruppe","印刷电路板组件；电子组装；电气组装"]
[null,{"$f":"IF($B$1=\"English\",C918,IF($B$1=\"Deutsch\",D918,IF($B$1=\"中文\",E918,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nPCB with electric und electronic elements, relais, displays, switcher, contactor, connector, cables, transformers "},"examples:\nPCB with electric und electronic elements, relais, displays, switcher, contactor, connector, cables, transformers ","Beispiele:\nLeiterplatte mit elektronischen und elektrischen Elementen, Relais, Anzeigen, Schalter, Schütze, Stecker, Kabel, Trafos","“例子：\n带有电子和电气元件、继电器、显示器、开关、接触器、连接器、电缆、变压器的印刷电路板"]
[null,{"$f":"IF($B$1=\"English\",C919,IF($B$1=\"Deutsch\",D919,IF($B$1=\"中文\",E919,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CE declaration"},"CE declaration","CE-Erklärung","CE-申明"]
[null,{"$f":"IF($B$1=\"English\",C920,IF($B$1=\"Deutsch\",D920,IF($B$1=\"中文\",E920,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Does the supplier declaration replace the CE conformity declaration for 2013 RoHS?"},"Does the supplier declaration replace the CE conformity declaration for 2013 RoHS?","Kann die Lieferantenerklärung die CE Konformitätserklärung für die RoHS ab 2013 ersetzen?","供应商的声明可以替代对2013版RoHS法规的CE符合性声明吗？"]
[null,{"$f":"IF($B$1=\"English\",C921,IF($B$1=\"Deutsch\",D921,IF($B$1=\"中文\",E921,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No. The supplier declaration is the basis for completing a CE conformity declaration and/or RoHS as the supplier declaration includes the confirmation of the supplier of compliance with the limit values for substances prohibited by the RoHS. Further it has to be observed: harmonized European standards on the RoHS CE declaration."},"No. The supplier declaration is the basis for completing a CE conformity declaration and/or RoHS as the supplier declaration includes the confirmation of the supplier of compliance with the limit values for substances prohibited by the RoHS. Further it has to be observed: harmonized European standards on the RoHS CE declaration.","Nein. Die Lieferantenerklärung ist Grundlage, um eine CE Konformitätserklärung bzgl. RoHS auszustellen, denn die Lieferantenerklärung enthält die Bestätigung des Lieferaten über die Einhaltung der Grenzwerte von verbotenen Stoffen in der RoHS. Weiterhin zu beachten:  harmonisierte europäische Normen zur RoHS CE Erklärung.","不可以。 该供应商声明表是CE申明的基础。请考虑欧洲关于CE符合性申明的规范。"]
[null,{"$f":"IF($B$1=\"English\",C922,IF($B$1=\"Deutsch\",D922,IF($B$1=\"中文\",E922,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"D"},"D","D","D"]
[null,{"$f":"IF($B$1=\"English\",C923,IF($B$1=\"Deutsch\",D923,IF($B$1=\"中文\",E923,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What does the abbreviation mean?"},"What does the abbreviation mean?","Was bedeutet die Abkürzung? ","缩写是什么意思？"]
[null,{"$f":"IF($B$1=\"English\",C924,IF($B$1=\"Deutsch\",D924,IF($B$1=\"中文\",E924,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The concentration of the substance must be declared if it reaches or exceeds the limit value. The declaration of the concentration recommended if it is less than or equal to the limit value."},"The concentration of the substance must be declared if it reaches or exceeds the limit value. The declaration of the concentration recommended if it is less than or equal to the limit value.","Die Konzentration des Inhaltsstoffs muss deklariert werden, wenn sie den Grenzwert erreicht oder über dem Grenzwert liegt. Die Angabe der Konzentration empfohlen, wenn sie kleiner oder gleich dem Grenzwert ist.","如果物质的浓度达到或超过极限值，必须申报。浓度小于或等于限值时推荐申报。"]
[null,{"$f":"IF($B$1=\"English\",C925,IF($B$1=\"Deutsch\",D925,IF($B$1=\"中文\",E925,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Printing"},"Printing","Drucken","打印"]
[null,{"$f":"IF($B$1=\"English\",C926,IF($B$1=\"Deutsch\",D926,IF($B$1=\"中文\",E926,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"How to print the entire file?"},"How to print the entire file?","Wie kann über die gesamte xls-Datei gedruckt werden?","\n怎样可以打印出整个xls文件？"]
[null,{"$f":"IF($B$1=\"English\",C927,IF($B$1=\"Deutsch\",D927,IF($B$1=\"中文\",E927,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Click path: File > Print > Entire workbook > OK"},"Click path: File > Print > Entire workbook > OK","Klickpfad in Excel: Datei > Drucken > Gesamte Arbeitsmappe > OK","单击路径在Excel中：文件>打印>整个工作簿>确定"]
[null,{"$f":"IF($B$1=\"English\",C928,IF($B$1=\"Deutsch\",D928,IF($B$1=\"中文\",E928,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-Directive on batteries and accumulators "},"EC-Directive on batteries and accumulators ","EG-Batterie- und Akkumulatorenrichtlinie","欧盟电池和蓄电池指令"]
[null,{"$f":"IF($B$1=\"English\",C929,IF($B$1=\"Deutsch\",D929,IF($B$1=\"中文\",E929,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What is this written out?"},"What is this written out?","Wie lautet die rechtliche Regelung?","\n怎样的法律制度？"]
[null,{"$f":"IF($B$1=\"English\",C930,IF($B$1=\"Deutsch\",D930,IF($B$1=\"中文\",E930,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 2006/66/EC on batteries and accumulators and waste batteries and accumulators"},"Directive 2006/66/EC on batteries and accumulators and waste batteries and accumulators","Richtlinie 2006/66/EG über Batterien und Akkumulatoren sowie Altbatterien und Altakkumulatoren","电池和蓄电池以及废旧电池和蓄电池的指令2006/66/EC"]
[null,{"$f":"IF($B$1=\"English\",C931,IF($B$1=\"Deutsch\",D931,IF($B$1=\"中文\",E931,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-ELV "},"EC-ELV ","EG-ELV","欧盟 ELV"]
[null,{"$f":"IF($B$1=\"English\",C932,IF($B$1=\"Deutsch\",D932,IF($B$1=\"中文\",E932,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What is this written out?"},"What is this written out?","Wie lautet die rechtliche Regelung?","\n怎样的法律制度？"]
[null,{"$f":"IF($B$1=\"English\",C933,IF($B$1=\"Deutsch\",D933,IF($B$1=\"中文\",E933,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 2000/53/EC on End-of Life Vehicles"},"Directive 2000/53/EC on End-of Life Vehicles","Richtlinie 2000/53/EG über Altfahrzeuge (End of Life Vehicles)","报废汽车指令 2000/53/EC"]
[null,{"$f":"IF($B$1=\"English\",C934,IF($B$1=\"Deutsch\",D934,IF($B$1=\"中文\",E934,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-REACH "},"EC-REACH ","EG-REACH","欧盟 REACH"]
[null,{"$f":"IF($B$1=\"English\",C935,IF($B$1=\"Deutsch\",D935,IF($B$1=\"中文\",E935,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulation (EC) No 1907/2006 concerning the Registration, Evaluation, Authorization and Restriction of Chemicals (REACH)"},"Regulation (EC) No 1907/2006 concerning the Registration, Evaluation, Authorization and Restriction of Chemicals (REACH)","Verordnung (EG) Nr. 1907/2006 zur Registrierung, Bewertung, Zulassung und Beschränkung chemischer Stoffe","（EC）1907/2006法规-关于化学品的注册，评估，许可和限制的法规"]
[null,{"$f":"IF($B$1=\"English\",C936,IF($B$1=\"Deutsch\",D936,IF($B$1=\"中文\",E936,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-RoHS "},"EC-RoHS ","EG-ROHS","欧盟 ROHS"]
[null,{"$f":"IF($B$1=\"English\",C937,IF($B$1=\"Deutsch\",D937,IF($B$1=\"中文\",E937,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 2011/65/EU and 2015/863/EU on the Restriction Of the use of certain Hazardous Substances in electrical and electronic equipment"},"Directive 2011/65/EU and 2015/863/EU on the Restriction Of the use of certain Hazardous Substances in electrical and electronic equipment","Richtlinie 2011/65/EU und 2015/863/EU zur Beschränkung der Verwendung bestimmter gefährlicher Stoffe in Elektro- und Elektronikgeräten","关于限制在电气和电子设备中使用某些危险物质的第2011/65/EU号和第2015/863/EU号指令"]
[null,{"$f":"IF($B$1=\"English\",C938,IF($B$1=\"Deutsch\",D938,IF($B$1=\"中文\",E938,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-Directive on packaging and packaging waste "},"EC-Directive on packaging and packaging waste ","EG-Verpackungsrichtlinie","欧盟包装指令"]
[null,{"$f":"IF($B$1=\"English\",C939,IF($B$1=\"Deutsch\",D939,IF($B$1=\"中文\",E939,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Directive 94/62/EC on packaging and packaging waste"},"Directive 94/62/EC on packaging and packaging waste","Richtlinie 94/62/EG über Verpackungen und Verpackungsabfälle","指令94/62/EC关于包装和包装废弃物"]
[null,{"$f":"IF($B$1=\"English\",C940,IF($B$1=\"Deutsch\",D940,IF($B$1=\"中文\",E940,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EPA"},"EPA","EPA","EPA"]
[null,{"$f":"IF($B$1=\"English\",C941,IF($B$1=\"Deutsch\",D941,IF($B$1=\"中文\",E941,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Environmental Protection Agency of the United States of America"},"Environmental Protection Agency of the United States of America","Umweltbundesbehörde der Vereinigten Staaten von Amerika","\n美国环保署"]
[null,{"$f":"IF($B$1=\"English\",C942,IF($B$1=\"Deutsch\",D942,IF($B$1=\"中文\",E942,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\npowder coatings, conductance-, insulation-, resistor-paste"},"examples:\npowder coatings, conductance-, insulation-, resistor-paste","Beispiele: \nPulverlacke, Leit-, Isolier-, Widerstandspasten","“例子：\n粉末涂料，导电性，绝缘性，耐糊剂“"]
[null,{"$f":"IF($B$1=\"English\",C943,IF($B$1=\"Deutsch\",D943,IF($B$1=\"中文\",E943,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nsolvents, lubricants, cooling lubricants, anticorrosive, electroplating, flux"},"examples:\nsolvents, lubricants, cooling lubricants, anticorrosive, electroplating, flux","Beispiele:\nLösungsmittel, Schmierstoffe, Kühlschmierstoffe, Korrosionsschutzmittel, Galvanik, Flussmittel","“例子：\n溶剂，润滑剂，金属加工液，缓蚀剂，电镀，焊剂“"]
[null,{"$f":"IF($B$1=\"English\",C944,IF($B$1=\"Deutsch\",D944,IF($B$1=\"中文\",E944,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"GADSL"},"GADSL","GADSL","GADSL"]
[null,{"$f":"IF($B$1=\"English\",C945,IF($B$1=\"Deutsch\",D945,IF($B$1=\"中文\",E945,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Global Automotive Declarable Substance List, includes prohibitions of materials and obligations to declare for substances that may be present in an automobile, generated by the Global Automotive Stakeholders Group (GASG)"},"Global Automotive Declarable Substance List, includes prohibitions of materials and obligations to declare for substances that may be present in an automobile, generated by the Global Automotive Stakeholders Group (GASG)","Global Automotive Declarable Substance List\nListe enthält Stoffverbote und Deklarationspflichten für Stoffe, die in Automobil vorkommen können, erstellt durch die Global Automotive Stakeholders Group (GASG)","“全球汽车申报物质清单\n清单包含可能会出现在汽车产品中的违禁物质和有义务申报的物质，由全球汽车运营商集团（GASG）创建"]
[null,{"$f":"IF($B$1=\"English\",C946,IF($B$1=\"Deutsch\",D946,IF($B$1=\"中文\",E946,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Merchandise automotive"},"Merchandise automotive","Handelsware Automobil","商品汽车"]
[null,{"$f":"IF($B$1=\"English\",C947,IF($B$1=\"Deutsch\",D947,IF($B$1=\"中文\",E947,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Non-Bosch items distributed\nwithout modification under the name of the external manufacturer. Also applies to onceonly\nbought-in items. These items fall under ELV respectively GADSL. \n\n"},"Non-Bosch items distributed\nwithout modification under the name of the external manufacturer. Also applies to onceonly\nbought-in items. These items fall under ELV respectively GADSL. \n\n","Fremderzeugnisse, die unverändert unter dem Namen des externen Herstellers vertrieben werden. Zutreffend auch für einmalig zuge-kaufte Erzeugnisse. Diese Erzeugnisse fallen unter ELV bzw. GADSL.","不做任何加工，依旧以外部供应商生产者名义销售的第三方产品。 此亦适用于一次性额外购买的产品。此产品属于ELV或者GADSL的管控范畴。"]
[null,{"$f":"IF($B$1=\"English\",C948,IF($B$1=\"Deutsch\",D948,IF($B$1=\"中文\",E948,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Wood, no wood-based material or composite"},"Wood, no wood-based material or composite","Holz, kein Holzwerkstoff oder Verbundwerkstoff","木材，非木质材料或者合成材料"]
[null,{"$f":"IF($B$1=\"English\",C949,IF($B$1=\"Deutsch\",D949,IF($B$1=\"中文\",E949,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nsolid wood"},"examples:\nsolid wood","Beispiele:\nVollholz, Massivholz","例子：\n实木"]
[null,{"$f":"IF($B$1=\"English\",C950,IF($B$1=\"Deutsch\",D950,IF($B$1=\"中文\",E950,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"IMDS"},"IMDS","IMDS","IMDS"]
[null,{"$f":"IF($B$1=\"English\",C951,IF($B$1=\"Deutsch\",D951,IF($B$1=\"中文\",E951,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"International Material Data System, the Internet declaration system of an association of car makers"},"International Material Data System, the Internet declaration system of an association of car makers","International Material Data System\nEs ist das Deklarationssystem im Internet eines Verbundes von Automobilherstellern","国际材料数据系统\n它是汽车制造商联盟在互联网上申报系统"]
[null,{"$f":"IF($B$1=\"English\",C952,IF($B$1=\"Deutsch\",D952,IF($B$1=\"中文\",E952,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ceramics; glass; minerals"},"Ceramics; glass; minerals","Keramik; Glas; Mineralie","陶瓷;玻璃;矿产"]
[null,{"$f":"IF($B$1=\"English\",C953,IF($B$1=\"Deutsch\",D953,IF($B$1=\"中文\",E953,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nearthenware, stoneware, porcelain, optical glas, glass fiber, mineral fiber"},"examples:\nearthenware, stoneware, porcelain, optical glas, glass fiber, mineral fiber","Beispiele:\nSteingut, Steinzeug, Porzellan, optisches Glas, Glasfasern, Mineralfasern","\n“例子：\n陶瓷，陶土，瓷器，光学玻璃，玻璃纤维，矿物纤维“"]
[null,{"$f":"IF($B$1=\"English\",C954,IF($B$1=\"Deutsch\",D954,IF($B$1=\"中文\",E954,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Adhesives; sealing material; resines"},"Adhesives; sealing material; resines","Klebstoff; Dichtstoff; Harze","胶粘剂;密封胶;树脂"]
[null,{"$f":"IF($B$1=\"English\",C955,IF($B$1=\"Deutsch\",D955,IF($B$1=\"中文\",E955,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\npolyurethane adhesive, grouting, epoxy resin"},"examples:\npolyurethane adhesive, grouting, epoxy resin","Beispiele:\nPolyurethan-Klebstoffe, Vergussmassen, Epoxid-Harze","“例子：\n聚氨酯胶粘剂，灌封化合物，环氧树脂“"]
[null,{"$f":"IF($B$1=\"English\",C956,IF($B$1=\"Deutsch\",D956,IF($B$1=\"中文\",E956,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plastic, elastomers"},"Plastic, elastomers","Kunststoff; Elastomer","塑料;弹性体"]
[null,{"$f":"IF($B$1=\"English\",C957,IF($B$1=\"Deutsch\",D957,IF($B$1=\"中文\",E957,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nPA, PE, PP, PVC, PS, PUR, NBR, EPDM"},"examples:\nPA, PE, PP, PVC, PS, PUR, NBR, EPDM","Beispiele:\nPA, PE, PP, PVC, PS, PUR, NBR, EPDM","例子:\nPA, PE, PP, PVC, PS, PUR, NBR, EPDM"]
[null,{"$f":"IF($B$1=\"English\",C958,IF($B$1=\"Deutsch\",D958,IF($B$1=\"中文\",E958,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Metals"},"Metals","Metall","金属"]
[null,{"$f":"IF($B$1=\"English\",C959,IF($B$1=\"Deutsch\",D959,IF($B$1=\"中文\",E959,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nsteel, cooper, aluminium, brass, magnesium casting"},"examples:\nsteel, cooper, aluminium, brass, magnesium casting","Beispiele:\nStahl, Kupfer, Aluminium, Messing, Magnesiumguß","\n“例子：\n钢，铜，铝，铜，镁铸造“"]
[null,{"$f":"IF($B$1=\"English\",C960,IF($B$1=\"Deutsch\",D960,IF($B$1=\"中文\",E960,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Metallic surface"},"Metallic surface","Metallische Oberfläche","金属表面"]
[null,{"$f":"IF($B$1=\"English\",C961,IF($B$1=\"Deutsch\",D961,IF($B$1=\"中文\",E961,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nwear protection, corrosion protection, nickel, cadmium, chrome, zinc"},"examples:\nwear protection, corrosion protection, nickel, cadmium, chrome, zinc","Beispiele:\nVerschleiss-Schutz, Korrosionsschutz, Nickel-, Cadmium-, Chrom-, Zink-Verbindungen ","“例子：\n耐磨，防腐蚀，镍，镉，铬，锌化合物“"]
[null,{"$f":"IF($B$1=\"English\",C962,IF($B$1=\"Deutsch\",D962,IF($B$1=\"中文\",E962,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P"},"P","P","P"]
[null,{"$f":"IF($B$1=\"English\",C963,IF($B$1=\"Deutsch\",D963,IF($B$1=\"中文\",E963,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A concentration value must always be given, even if the concentration of the substance is below or reaches the limit value."},"A concentration value must always be given, even if the concentration of the substance is below or reaches the limit value.","Es muss immer ein Konzentrationswert angegeben werden, auch wenn die Konzentration des Inhaltsstoffs unter dem Grenzwert liegt oder diesen erreicht.","即使物质的浓度低于或达到极限值，也必须始终给出浓度值。"]
[null,{"$f":"IF($B$1=\"English\",C964,IF($B$1=\"Deutsch\",D964,IF($B$1=\"中文\",E964,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product or merchandise does not contain a substance which is released during intended use"},"Product or merchandise does not contain a substance which is released during intended use","Produkt oder Handelsware, enthält keine Stoffe, die im bestimmungsgemäßen Gebrauch freigesetzt werden","\n不包含在正常使用下会挥发物质的产品或商品。"]
[null,{"$f":"IF($B$1=\"English\",C965,IF($B$1=\"Deutsch\",D965,IF($B$1=\"中文\",E965,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nbrushless motor, pump in closed loop, LCD-display, DVD-drive"},"examples:\nbrushless motor, pump in closed loop, LCD-display, DVD-drive","Beispiele:\nbürstenloser Elektromotor, Pumpe im geschlossenen Kreislauf, LCD-Display, DVD-Laufwerk","“例子：\n无刷电机，封闭回路中的泵，LCD显示屏，DVD光驱“"]
[null,{"$f":"IF($B$1=\"English\",C966,IF($B$1=\"Deutsch\",D966,IF($B$1=\"中文\",E966,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product or merchandise does contain a substance which is released during intended use"},"Product or merchandise does contain a substance which is released during intended use","Produkt oder Handelsware, enthält Stoffe, die im bestimmungsgemäßen Gebrauch freigesetzt werden","\n包含在正常使用下会挥发的物质的产品或商品"]
[null,{"$f":"IF($B$1=\"English\",C967,IF($B$1=\"Deutsch\",D967,IF($B$1=\"中文\",E967,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples\npressure vessel with cleaning agent, printer, metering unit"},"examples\npressure vessel with cleaning agent, printer, metering unit","Beispiele:\nDruckbehälter mit Reinigungsflüssigkeit, Drucker, Dosiergerät","“例子：\n带有清洗液的压力容器，打印机，计量装置"]
[null,{"$f":"IF($B$1=\"English\",C968,IF($B$1=\"Deutsch\",D968,IF($B$1=\"中文\",E968,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Search"},"Search","Suchen","查找 "]
[null,{"$f":"IF($B$1=\"English\",C969,IF($B$1=\"Deutsch\",D969,IF($B$1=\"中文\",E969,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"How can I search over the entire xls-file?"},"How can I search over the entire xls-file?","Wie kann man über die gesamte xls-Datei suchen?","\n怎样可以在整个xls文件中查找？"]
[null,{"$f":"IF($B$1=\"English\",C970,IF($B$1=\"Deutsch\",D970,IF($B$1=\"中文\",E970,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Path: Edit > Find > Options > Click on Drop Down \"Workbook\" > click on Drop Down \"Find what\""},"Path: Edit > Find > Options > Click on Drop Down \"Workbook\" > click on Drop Down \"Find what\"","Klickpfad in Excel: Bearbeiten > Suchen > Optionen > Drop Down \"Arbeitsmappe\" anklicken > Drop Down \"Werte\" anklicken","单击Excel中的路径：编辑>查找>选项>下拉菜单“工作簿”>下拉“价值”："]
[null,{"$f":"IF($B$1=\"English\",C971,IF($B$1=\"Deutsch\",D971,IF($B$1=\"中文\",E971,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SVHC"},"SVHC","SVHC","SVHC"]
[null,{"$f":"IF($B$1=\"English\",C972,IF($B$1=\"Deutsch\",D972,IF($B$1=\"中文\",E972,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances Of Very High Concern, substances that give rise to particular concern, defined in the nomination listing of the European Chemicals Agency (ECHA)"},"Substances Of Very High Concern, substances that give rise to particular concern, defined in the nomination listing of the European Chemicals Agency (ECHA)","Substances Of Very High Concern = besonders besorgniserregende Stoffe \ndefiniert in der Kandidatenliste durch die Euopäische Chemikalienagentur (ECHA)","高度关注的物质，由欧洲化学品管理署（ECHA）在候选清单中定义的需要特别物质"]
[null,{"$f":"IF($B$1=\"English\",C973,IF($B$1=\"Deutsch\",D973,IF($B$1=\"中文\",E973,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Textile; leather"},"Textile; leather","Textilie; Leder","纺织;皮革"]
[null,{"$f":"IF($B$1=\"English\",C974,IF($B$1=\"Deutsch\",D974,IF($B$1=\"中文\",E974,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples\nwrapper, ribbon, jacket"},"examples\nwrapper, ribbon, jacket","Beispiele:\nSchutzhüllen, Bänder, Ummantelungen","例子：\n包装材料，胶带，护套"]
[null,{"$f":"IF($B$1=\"English\",C975,IF($B$1=\"Deutsch\",D975,IF($B$1=\"中文\",E975,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Unequipped PCB; electronic component"},"Unequipped PCB; electronic component","unbestückte Leiterplatte; Bauelement für Leiterplatte; Elektronikkomponente","PCB裸板；电子元件"]
[null,{"$f":"IF($B$1=\"English\",C976,IF($B$1=\"Deutsch\",D976,IF($B$1=\"中文\",E976,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples:\nPCB without electronic or electric components, capcitors, resistors, IC, transistors, diodes"},"examples:\nPCB without electronic or electric components, capcitors, resistors, IC, transistors, diodes","Beispiele:\nLeiterplatte ohne elektronische und elektrische Elemente, Kondensatoren, Widerstände, Integrierte Schaltkreise, Transistoren, Dioden","例子：\n不带有电子和电气元件，电容器，电阻器，集成电路，晶体管，二极管的电路板"]
[null,{"$f":"IF($B$1=\"English\",C977,IF($B$1=\"Deutsch\",D977,IF($B$1=\"中文\",E977,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Composite"},"Composite","Verbundwerkstoff","复合材料"]
[null,{"$f":"IF($B$1=\"English\",C978,IF($B$1=\"Deutsch\",D978,IF($B$1=\"中文\",E978,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples\nplastic coated metal, metal matrix composite, fiber ceramics composite, plywood, OSB panels"},"examples\nplastic coated metal, metal matrix composite, fiber ceramics composite, plywood, OSB panels","Beispiele:\nkunststoffumspritztes Metall, Metallmatrix-Verbunde, Faser-Keramik-Verbunde, Sperrholz, OSB-Platten","例子：\n塑料涂覆金属，金属基复合材料，纤维-陶瓷复合材料，复合板，OSB板"]
[null,{"$f":"IF($B$1=\"English\",C979,IF($B$1=\"Deutsch\",D979,IF($B$1=\"中文\",E979,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging"},"Packaging","Verpackung","包装"]
[null,{"$f":"IF($B$1=\"English\",C980,IF($B$1=\"Deutsch\",D980,IF($B$1=\"中文\",E980,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"examples\npaper, plastic, anti corrosive paper, drying agent, treated wood"},"examples\npaper, plastic, anti corrosive paper, drying agent, treated wood","Beispiele:\nPapier, Kunststoff, Korrosionsschutzpapier, Trocknungsmittel, behandeltes Holz","“例子：\n纸，塑料，防腐纸，干燥剂，经过处理的木材“"]
[null,{"$f":"IF($B$1=\"English\",C981,IF($B$1=\"Deutsch\",D981,IF($B$1=\"中文\",E981,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C982,IF($B$1=\"Deutsch\",D982,IF($B$1=\"中文\",E982,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C983,IF($B$1=\"Deutsch\",D983,IF($B$1=\"中文\",E983,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Auxiliary manufacturing materials"},"Auxiliary manufacturing materials","Fertigungshilfsstoff","制造辅助材料"]
[null,{"$f":"IF($B$1=\"English\",C984,IF($B$1=\"Deutsch\",D984,IF($B$1=\"中文\",E984,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Colors; dye; laquers; coating; impregantion; similar material"},"Colors; dye; laquers; coating; impregantion; similar material","Farbe; Farbstoff; Lack; Beschichtung; Imprägnierung; ähnliches Material","色;染料;涂料;涂料;浸渍;类似的材料"]
[null,{"$f":"IF($B$1=\"English\",C985,IF($B$1=\"Deutsch\",D985,IF($B$1=\"中文\",E985,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All yellow fields in the worksheet \"Cover_Sheet\" must be filled."},"All yellow fields in the worksheet \"Cover_Sheet\" must be filled.","Alle gelben Felder im Tabellenblatt \"Cover_Sheet\" müssen ausgefüllt sein.","工作表“Cover_Sheet”中的所有黄色区域必须完成。"]
[null,{"$f":"IF($B$1=\"English\",C986,IF($B$1=\"Deutsch\",D986,IF($B$1=\"中文\",E986,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Save anyway?"},"Save anyway?","Trotzdem speichern?","仍然保存？"]
[null,{"$f":"IF($B$1=\"English\",C987,IF($B$1=\"Deutsch\",D987,IF($B$1=\"中文\",E987,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Additional details on the material supplied"},"Additional details on the material supplied","Zusätzliche Angaben zum gelieferten Material","提供物质上的其他信息"]
[null,{"$f":"IF($B$1=\"English\",C988,IF($B$1=\"Deutsch\",D988,IF($B$1=\"中文\",E988,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) Phenylmercury acetate\nb) Phenylmercury propionate \nc) Phenylmercury 2-ethylhexanoate\nd) Phenylmercury octanoate\ne) Phenylmercury neodecanoate"},"a) Phenylmercury acetate\nb) Phenylmercury propionate \nc) Phenylmercury 2-ethylhexanoate\nd) Phenylmercury octanoate\ne) Phenylmercury neodecanoate","a) Phenylquecksilberacetat\nb) Phenylquecksilberpropionat\nc) Phenylquecksilber-2-ethylhexanoat\nd) Phenylquecksilberoctanoat\ne) Phenylquecksilberneodecanoat","a)苯基醋酸汞\nb) 丙酸苯汞\nc) 苯基汞-2-乙酸乙酯\nd) 辛酸苯汞酯\ne) 新癸酸苯汞"]
[null,{"$f":"IF($B$1=\"English\",C989,IF($B$1=\"Deutsch\",D989,IF($B$1=\"中文\",E989,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and its compounds"},"Lead and its compounds","Blei und seine Verbindungen","铅及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C990,IF($B$1=\"Deutsch\",D990,IF($B$1=\"中文\",E990,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be manufactured, placed on the market or used as substances or in mixtures after 10 October 2017 if the concentration of mercury in the mixtures is equal to or greater than 0,01 % by weight.\n\n2. Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight.\n"},"1. Shall not be manufactured, placed on the market or used as substances or in mixtures after 10 October 2017 if the concentration of mercury in the mixtures is equal to or greater than 0,01 % by weight.\n\n2. Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight.\n","1. Darf nach dem 10. Oktober 2017 weder als Stoff noch in Gemischen hergestellt, in Verkehr gebracht oder verwendet werden, wenn die Quecksilberkonzentration in den Gemischen 0,01 Gewichtsprozent beträgt oder übersteigt. \n\n2. Erzeugnisse oder deren Bestandteile, die einen oder mehrere dieser Stoffe enthalten, dürfen nach dem 10. Oktober 2017 nicht in Verkehr gebracht werden, wenn die Quecksilberkonzentration in den Erzeugnissen bzw. deren Bestandteilen 0,01 Gewichtsprozent beträgt oder übersteigt.","1.当汞在配制品中浓度大于等于0.01％（重量），在2017年10月10日后不得生产或者投放市场。\n2.当产品或其组件中汞的浓度大于等于0.01％（重量），该产品获组件在2017年10月10日之后不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C991,IF($B$1=\"Deutsch\",D991,IF($B$1=\"中文\",E991,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market or used in any individual part of jewellery articles if the concentration of lead (expressed as metal) in such a part is equal to or greater than 0,05 % by weight.\n2. For the purposes of paragraph 1: \n(i) “jewellery articles” shall include jewellery and imitation jewellery articles and hair accessories, including:\n (a) bracelets, necklaces and rings;\n (b) piercing jewellery;\n (c) wrist watches and wrist-wear;\n (d) brooches and cufflinks; \n(ii) “any individual part” shall include the materials from which the jewellery is made, as well as the individual components of the jewellery articles. \n3. Paragraph 1 shall also apply to individual parts when placed on the market or used for jewellery-making. \n4. By way of derogation, paragraph 1 shall not apply to:\n (a) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Council Directive 69/493/EEC (*);\n (b) internal components of watch timepieces inaccessible to consumers;\n (c) non-synthetic or reconstructed precious and semiprecious stones (CN code 7103, as established by Regulation (EEC) No 2658/87), unless they have been treated with lead or its compounds or mixtures containing these substances;\n (d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of minerals melted at a temperature of at least 500 °C. \n5. By way of derogation, paragraph 1 shall not apply to jewellery articles placed on the market for the first time before 9 October 2013 and jewellery articles produced before 10 December 1961. \n6. By 9 October 2017, the Commission shall re-evaluate this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 1 and, if appropriate, modify this entry accordingly.\n•  Dürfen nicht in Verkehr gebracht oder in Erzeugnissen, die zur Abgabe an die breite Öffentlichkeit bestimmt sind, verwendet werden, wenn der Bleigehalt (in Metall) des betreffenden Erzeugnisses oder der zugänglichen Teile davon 0,05 % oder mehr des Gewichts beträgt und diese Erzeugnisse bzw. die zugänglichen Teile davon unter normalen oder vernünftigerweise vorhersehbaren Verwendungsbedingungen von Kindern in den Mund genommen werden könnten. Dieser Grenzwert gilt nicht, wenn die Freisetzungsrate von Blei aus einem solchen Erzeugnis oder den zugänglichen Teilen eines Erzeugnisses, seien sie beschichtet oder nicht, 0,05 μg/cm2 pro Stunde (entspricht 0,05 μg/g/h) nachweislich nicht überschreitet und — bei beschichteten Erzeugnissen — die Beschichtung ausreicht, damit diese Rate für einen Zeitraum von mindestens zwei Jahren bei normalen oder vernünftigerweise vorhersehbaren Bedingungen der Verwendung des Erzeugnisses nicht überschritten wird. Für die Zwecke dieses Absatzes gilt, dass ein Erzeugnis oder ein zugänglicher Teil eines Erzeugnisses von Kindern in den Mund genommen werden kann, wenn eines der Maße weniger als 5 cm beträgt oder wenn das Erzeugnis bzw. der Teil desselben ein abnehmbares oder hervorstehendes Teil dieser Größe aufweist.\n•  Absatz 7 gilt jedoch nicht für: \na) Schmuckwaren gemäß Absatz 1; \nb) Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/EWG; \nc) nicht synthetische oder rekonstituierte Edel- und Schmucksteine (KN-Code 7103 gemäß der Verordnung (EWG) Nr. 2658/87), sofern sie nicht mit Blei oder Bleiverbindungen oder Gemischen, die diese Stoffe enthalten, behandelt wurden;\nd)Email, definiert als verglasbare Gemische aus dem Schmelzen, Verglasen oder Sintern von Mineralien bei Temperaturen von mindestens 500 °C; \ne) Schlüssel und Schlösser einschließlich Vorhängeschlössern; \nf) Musikinstrumente; \ng) Erzeugnisse und Teile von Erzeugnissen, die Messinglegierungen enthalten, sofern der Bleigehalt (in Metall) im Messing 0,5 % des Gewichts nicht überschreitet; \nh) die Spitzen von Schreibgeräten; \ni) Devotionalien; \nj) Zink-Kohle-Gerätebatterien und Knopfzellen; \nk) Erzeugnisse im Anwendungsbereich der: i) Richtlinie 94/62/EG; ii) Verordnung (EG) Nr. 1935/2004; iii) Richtlinie 2009/48/EG des Europäischen Parlaments und des Rates(*); iv) Richtlinie 2011/65/EU des Europäischen Parlaments und des Rates(**).\n•  Bis zum 1. Juli 2019 nimmt die Kommission eine Neubewertung von Absatz 7 und Absatz 8 Buchstaben e, f, i und j dieses Eintrags im Lichte neuer wissenschaftlicher Erkenntnisse vor; dabei werden auch die Verfügbarkeit von Alternativen und die Migration von Blei aus den in Absatz 7 genannten Erzeugnissen sowie die Anforderungen an die Unversehrtheit der Beschichtung berücksichtigt, und dieser Eintrag wird gegebenenfalls entsprechend geändert.\n•  Absatz 7 gilt jedoch nicht für Erzeugnisse, die vor dem 1. Juni 2016 erstmals in Verkehr gebracht wurden.\n"},"1. Shall not be placed on the market or used in any individual part of jewellery articles if the concentration of lead (expressed as metal) in such a part is equal to or greater than 0,05 % by weight.\n2. For the purposes of paragraph 1: \n(i) “jewellery articles” shall include jewellery and imitation jewellery articles and hair accessories, including:\n (a) bracelets, necklaces and rings;\n (b) piercing jewellery;\n (c) wrist watches and wrist-wear;\n (d) brooches and cufflinks; \n(ii) “any individual part” shall include the materials from which the jewellery is made, as well as the individual components of the jewellery articles. \n3. Paragraph 1 shall also apply to individual parts when placed on the market or used for jewellery-making. \n4. By way of derogation, paragraph 1 shall not apply to:\n (a) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Council Directive 69/493/EEC (*);\n (b) internal components of watch timepieces inaccessible to consumers;\n (c) non-synthetic or reconstructed precious and semiprecious stones (CN code 7103, as established by Regulation (EEC) No 2658/87), unless they have been treated with lead or its compounds or mixtures containing these substances;\n (d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of minerals melted at a temperature of at least 500 °C. \n5. By way of derogation, paragraph 1 shall not apply to jewellery articles placed on the market for the first time before 9 October 2013 and jewellery articles produced before 10 December 1961. \n6. By 9 October 2017, the Commission shall re-evaluate this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 1 and, if appropriate, modify this entry accordingly.\n•  Dürfen nicht in Verkehr gebracht oder in Erzeugnissen, die zur Abgabe an die breite Öffentlichkeit bestimmt sind, verwendet werden, wenn der Bleigehalt (in Metall) des betreffenden Erzeugnisses oder der zugänglichen Teile davon 0,05 % oder mehr des Gewichts beträgt und diese Erzeugnisse bzw. die zugänglichen Teile davon unter normalen oder vernünftigerweise vorhersehbaren Verwendungsbedingungen von Kindern in den Mund genommen werden könnten. Dieser Grenzwert gilt nicht, wenn die Freisetzungsrate von Blei aus einem solchen Erzeugnis oder den zugänglichen Teilen eines Erzeugnisses, seien sie beschichtet oder nicht, 0,05 μg/cm2 pro Stunde (entspricht 0,05 μg/g/h) nachweislich nicht überschreitet und — bei beschichteten Erzeugnissen — die Beschichtung ausreicht, damit diese Rate für einen Zeitraum von mindestens zwei Jahren bei normalen oder vernünftigerweise vorhersehbaren Bedingungen der Verwendung des Erzeugnisses nicht überschritten wird. Für die Zwecke dieses Absatzes gilt, dass ein Erzeugnis oder ein zugänglicher Teil eines Erzeugnisses von Kindern in den Mund genommen werden kann, wenn eines der Maße weniger als 5 cm beträgt oder wenn das Erzeugnis bzw. der Teil desselben ein abnehmbares oder hervorstehendes Teil dieser Größe aufweist.\n•  Absatz 7 gilt jedoch nicht für: \na) Schmuckwaren gemäß Absatz 1; \nb) Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/EWG; \nc) nicht synthetische oder rekonstituierte Edel- und Schmucksteine (KN-Code 7103 gemäß der Verordnung (EWG) Nr. 2658/87), sofern sie nicht mit Blei oder Bleiverbindungen oder Gemischen, die diese Stoffe enthalten, behandelt wurden;\nd)Email, definiert als verglasbare Gemische aus dem Schmelzen, Verglasen oder Sintern von Mineralien bei Temperaturen von mindestens 500 °C; \ne) Schlüssel und Schlösser einschließlich Vorhängeschlössern; \nf) Musikinstrumente; \ng) Erzeugnisse und Teile von Erzeugnissen, die Messinglegierungen enthalten, sofern der Bleigehalt (in Metall) im Messing 0,5 % des Gewichts nicht überschreitet; \nh) die Spitzen von Schreibgeräten; \ni) Devotionalien; \nj) Zink-Kohle-Gerätebatterien und Knopfzellen; \nk) Erzeugnisse im Anwendungsbereich der: i) Richtlinie 94/62/EG; ii) Verordnung (EG) Nr. 1935/2004; iii) Richtlinie 2009/48/EG des Europäischen Parlaments und des Rates(*); iv) Richtlinie 2011/65/EU des Europäischen Parlaments und des Rates(**).\n•  Bis zum 1. Juli 2019 nimmt die Kommission eine Neubewertung von Absatz 7 und Absatz 8 Buchstaben e, f, i und j dieses Eintrags im Lichte neuer wissenschaftlicher Erkenntnisse vor; dabei werden auch die Verfügbarkeit von Alternativen und die Migration von Blei aus den in Absatz 7 genannten Erzeugnissen sowie die Anforderungen an die Unversehrtheit der Beschichtung berücksichtigt, und dieser Eintrag wird gegebenenfalls entsprechend geändert.\n•  Absatz 7 gilt jedoch nicht für Erzeugnisse, die vor dem 1. Juni 2016 erstmals in Verkehr gebracht wurden.\n","1. Dürfen nicht in Verkehr gebracht oder in einem einzelnen Teil einer Schmuckware verwendet werden, wenn der Bleigehalt (in Metall) des betreffenden Teils 0,05 % oder mehr des Gewichts beträgt.\n2. Für die Zwecke des Absatzes 1 bezeichnet der Ausdruck:\ni) „Schmuckwaren“ Schmuck und Fantasieschmuck sowie Haarschmuck, einschließlich:\na) Armbänder, Halsketten und Ringe, \nb) Piercingschmuck, \nc) Armbanduhren und Armschmuck, \nd) Broschen und Manschettenknöpfe;\nii) „in einem einzelnen Teil“ auch die Materialien, aus denen der Schmuck hergestellt wurde, sowie die einzelnen Bestandteile der Schmuckwaren.\n3. Absatz 1 gilt auch für einzelne Teile, die für die Schmuckherstellung in Verkehr gebracht oder verwendet werden.\n4. Absatz 1 gilt jedoch nicht für:\na) Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/EWG des Rates (*),\nb) Einbauteile von Armband- und Taschenuhren sowie Zeitmessern, die für Verbraucher nicht zugänglich sind,\nc) nicht synthetische oder rekonstituierte Edel- und Schmucksteine (KN-Code 7103 gemäß Verordnung (EWG) Nr. 2658/87), sofern sie nicht mit Blei oder Bleiverbindungen oder Gemischen, die diese Stoffe enthalten, behandelt wurden,\nd) Email, definiert als verglasbare Gemische aus dem Schmelzen, Verglasen oder Sintern von Mineralien bei Temperaturen von mindestens 500 °C.\n5. Absatz 1 gilt jedoch nicht für Schmuckwaren, die vor dem 9. Oktober 2013 erstmals in Verkehr gebracht, und Schmuckwaren, die vor dem 10. Dezember 1961 hergestellt wurden.\n6. Bis zum 9. Oktober 2017 nimmt die Kommission eine Neubewertung dieses Eintrags im Lichte neuer wissenschaftlicher Erkenntnisse vor; dabei wird auch die Verfügbarkeit von Alternativen und die Migration von Blei aus den in Absatz 1 genannten Erzeugnissen berücksichtigt und dieser Eintrag gegebenenfalls entsprechend geändert.\n•  Dürfen nicht in Verkehr gebracht oder in Erzeugnissen, die zur Abgabe an die breite Öffentlichkeit bestimmt sind, verwendet werden, wenn der Bleigehalt (in Metall) des betreffenden Erzeugnisses oder der zugänglichen Teile davon 0,05 % oder mehr des Gewichts beträgt und diese Erzeugnisse bzw. die zugänglichen Teile davon unter normalen oder vernünftigerweise vorhersehbaren Verwendungsbedingungen von Kindern in den Mund genommen werden könnten. Dieser Grenzwert gilt nicht, wenn die Freisetzungsrate von Blei aus einem solchen Erzeugnis oder den zugänglichen Teilen eines Erzeugnisses, seien sie beschichtet oder nicht, 0,05 μg/cm2 pro Stunde (entspricht 0,05 μg/g/h) nachweislich nicht überschreitet und — bei beschichteten Erzeugnissen — die Beschichtung ausreicht, damit diese Rate für einen Zeitraum von mindestens zwei Jahren bei normalen oder vernünftigerweise vorhersehbaren Bedingungen der Verwendung des Erzeugnisses nicht überschritten wird. Für die Zwecke dieses Absatzes gilt, dass ein Erzeugnis oder ein zugänglicher Teil eines Erzeugnisses von Kindern in den Mund genommen werden kann, wenn eines der Maße weniger als 5 cm beträgt oder wenn das Erzeugnis bzw. der Teil desselben ein abnehmbares oder hervorstehendes Teil dieser Größe aufweist.\n•  Absatz 7 gilt jedoch nicht für: \na) Schmuckwaren gemäß Absatz 1; \nb) Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/EWG; \nc) nicht synthetische oder rekonstituierte Edel- und Schmucksteine (KN-Code 7103 gemäß der Verordnung (EWG) Nr. 2658/87), sofern sie nicht mit Blei oder Bleiverbindungen oder Gemischen, die diese Stoffe enthalten, behandelt wurden;\nd)Email, definiert als verglasbare Gemische aus dem Schmelzen, Verglasen oder Sintern von Mineralien bei Temperaturen von mindestens 500 °C; \ne) Schlüssel und Schlösser einschließlich Vorhängeschlössern; \nf) Musikinstrumente; \ng) Erzeugnisse und Teile von Erzeugnissen, die Messinglegierungen enthalten, sofern der Bleigehalt (in Metall) im Messing 0,5 % des Gewichts nicht überschreitet; \nh) die Spitzen von Schreibgeräten; \ni) Devotionalien; \nj) Zink-Kohle-Gerätebatterien und Knopfzellen; \nk) Erzeugnisse im Anwendungsbereich der: i) Richtlinie 94/62/EG; ii) Verordnung (EG) Nr. 1935/2004; iii) Richtlinie 2009/48/EG des Europäischen Parlaments und des Rates(*); iv) Richtlinie 2011/65/EU des Europäischen Parlaments und des Rates(**).\n•  Bis zum 1. Juli 2019 nimmt die Kommission eine Neubewertung von Absatz 7 und Absatz 8 Buchstaben e, f, i und j dieses Eintrags im Lichte neuer wissenschaftlicher Erkenntnisse vor; dabei werden auch die Verfügbarkeit von Alternativen und die Migration von Blei aus den in Absatz 7 genannten Erzeugnissen sowie die Anforderungen an die Unversehrtheit der Beschichtung berücksichtigt, und dieser Eintrag wird gegebenenfalls entsprechend geändert.\n•  Absatz 7 gilt jedoch nicht für Erzeugnisse, die vor dem 1. Juni 2016 erstmals in Verkehr gebracht wurden.\n","1.如果零件中的铅含量（以金属计）占重量的0.05％或以上，该零件不得投放市场或用做任何珠宝首饰的单个零件。 \n2.对于第1条：\ni)珠宝首饰”应该包括珠宝及仿制首饰和发饰，包括：\na)手镯，项链和戒指，\nb)穿孔饰品，\nc)手表和手镯，\nd)胸针和袖扣;\nii)“单个零件”应该包括制造珠宝首饰的材料，以及首饰的单个部件。\n3.第1段也适用于那些在市场上销售的或用于珠宝制作的单个零件。\n4.第1段不适用于：\na)根据69/493/EEC（*）指令附件I（水晶玻璃类型1，2，3和4）中的定义的水晶玻璃；\nb)手表和怀表以及钟表中消费者接触不到的内部零件；\nc)非合成或再造的宝石和首饰宝石（按照法规（EEC）2658/87，CN代码7103），除非他们在加工过程中使用了含铅或铅化合物或者其它含铅配制品；\nd)搪瓷，被定义为在至少500℃的高温下，矿物被熔化，烧结或瓷化后形成的配制品。\n5)第1段不适用于已在2013年10月9日前已经投放市场的珠宝首饰和在1961年12月10日之前已制造好的珠宝首饰。\n6)在2017年10月9日之前，委员会会依据当时的科技能力对这个项目进行重新评估，包括替代品的可用性和在第一条中提到的珠宝首饰中铅的迁出情况，从而进行相应地修改。"]
[null,{"$f":"IF($B$1=\"English\",C992,IF($B$1=\"Deutsch\",D992,IF($B$1=\"中文\",E992,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pyrochlore, antimony lead yellow"},"Pyrochlore, antimony lead yellow","Pyrochlor, Antimonbleigelb","烧绿石，黄锑铅"]
[null,{"$f":"IF($B$1=\"English\",C993,IF($B$1=\"Deutsch\",D993,IF($B$1=\"中文\",E993,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"6-methoxy-m-toluidine (p-cresidine)"},"6-methoxy-m-toluidine (p-cresidine)","6-Methoxy-m-toluidin","2-甲氧基-5-甲基苯胺"]
[null,{"$f":"IF($B$1=\"English\",C994,IF($B$1=\"Deutsch\",D994,IF($B$1=\"中文\",E994,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Henicosafluoroundecanoic acid"},"Henicosafluoroundecanoic acid","Henicosafluorundecansäure","全氟十一烷酸"]
[null,{"$f":"IF($B$1=\"English\",C995,IF($B$1=\"Deutsch\",D995,IF($B$1=\"中文\",E995,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexahydromethylphthalic anhydride [1], Hexahydro-4-methylphthalic anhydride [2], Hexahydro-1-methylphthalic anhydride [3], Hexahydro-3-methylphthalic anhydride [4] [The individual isomers [2], [3] and [4] (including their cis- and trans- stereo isomeric forms) and all possible combinations of the isomers [1] are covered by this entry]"},"Hexahydromethylphthalic anhydride [1], Hexahydro-4-methylphthalic anhydride [2], Hexahydro-1-methylphthalic anhydride [3], Hexahydro-3-methylphthalic anhydride [4] [The individual isomers [2], [3] and [4] (including their cis- and trans- stereo isomeric forms) and all possible combinations of the isomers [1] are covered by this entry]","Hexahydromethylphthalsäureanhydrid [1], Hexahydro-4-methylphtalsäureanhydrid [2], Hexahydro-1-methylphtalsäureanhydrid [3], Hexahydro-3-methylphtalsäureanhydrid [4] [The individual isomers [2], [3] and [4] (including their cis- and trans- stereo isomeric forms) and all possible combinations of the isomers [1] are covered by this entry]","甲基六氢邻苯二甲酸酐 [1], 4-甲基六氢苯酐 [2], 六氢-1 - 甲基邻苯二甲酸酐 [3], 甲基六氢邻苯二甲酸酐 [4] [个人的同分异构体[2], [3] 和 [4] (包括其顺式 - 和反式立体异构体形式) 和异构体[1]的所有可能的组合都包括在本项]"]
[null,{"$f":"IF($B$1=\"English\",C996,IF($B$1=\"Deutsch\",D996,IF($B$1=\"中文\",E996,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cyclohexane-1,2-dicarboxylic anhydride [1], cis-cyclohexane-1,2-dicarboxylic anhydride [2], trans-cyclohexane-1,2-dicarboxylic anhydride [3] [The individual cis- [2] and trans- [3] isomer substances and all possible combinations of the cis- and trans-isomers [1] are covered by this entry]"},"Cyclohexane-1,2-dicarboxylic anhydride [1], cis-cyclohexane-1,2-dicarboxylic anhydride [2], trans-cyclohexane-1,2-dicarboxylic anhydride [3] [The individual cis- [2] and trans- [3] isomer substances and all possible combinations of the cis- and trans-isomers [1] are covered by this entry]","Cyclohexan-1,2-dicarbonsäureanhydrid [1],cis-Cyclohexan-1,2-dicarbonsäureanhydrid [2], trans-Cyclohexan-1,2-discarbonsäureanhydrid [3] [The individual cis- [2] and trans- [3] isomer substances and all possible combinations of the cis- and trans-isomers [1] are covered by this entry]","六氢甲基邻苯二甲酸酐 [1], \n六氢-4-甲基苯酐 [2], \n六氢-1-甲基邻苯二甲酸酐 [3], \n六氢-3-甲基邻苯二甲酸酐 [4]\n [各同分异构体[2], [3] 和 [4] (包括其顺式 - 和反式立体异构体形式)和异构体[1]的所有 可能的组合都包括在本项]"]
[null,{"$f":"IF($B$1=\"English\",C997,IF($B$1=\"Deutsch\",D997,IF($B$1=\"中文\",E997,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyltin dichloride (DBTC)"},"Dibutyltin dichloride (DBTC)","Dibutylzinndichlorid (DBTC)","二丁基二氯化锡 (DBTC)"]
[null,{"$f":"IF($B$1=\"English\",C998,IF($B$1=\"Deutsch\",D998,IF($B$1=\"中文\",E998,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead bis(tetrafluoroborate)"},"Lead bis(tetrafluoroborate)","Bleibis(tetrafluoroborat)","四氟硼酸铅"]
[null,{"$f":"IF($B$1=\"English\",C999,IF($B$1=\"Deutsch\",D999,IF($B$1=\"中文\",E999,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead dinitrate"},"Lead dinitrate","Blei(II)-nitrat","硝酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1000,IF($B$1=\"Deutsch\",D1000,IF($B$1=\"中文\",E1000,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicic acid, lead salt"},"Silicic acid, lead salt","Kieselsäure, Bleisalz","硅酸，铅盐"]
[null,{"$f":"IF($B$1=\"English\",C1001,IF($B$1=\"Deutsch\",D1001,IF($B$1=\"中文\",E1001,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Aminoazobenzene"},"4-Aminoazobenzene","4-Aminoazobenzol","4-阿基苯甲酯"]
[null,{"$f":"IF($B$1=\"English\",C1002,IF($B$1=\"Deutsch\",D1002,IF($B$1=\"中文\",E1002,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead titanium zirconium oxide"},"Lead titanium zirconium oxide","Bleititanzirkonoxid","钛酸铅锆镧"]
[null,{"$f":"IF($B$1=\"English\",C1003,IF($B$1=\"Deutsch\",D1003,IF($B$1=\"中文\",E1003,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead monoxide (lead oxide)"},"Lead monoxide (lead oxide)","Blei(II)-oxid","氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C1004,IF($B$1=\"Deutsch\",D1004,IF($B$1=\"中文\",E1004,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"o-Toluidine"},"o-Toluidine","o-Toluidin","邻甲基苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1005,IF($B$1=\"Deutsch\",D1005,IF($B$1=\"中文\",E1005,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3-ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidine"},"3-ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidine","3-Ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidin","3-乙基-2-甲基-2-(3-甲基丁基)-1,3-恶唑烷"]
[null,{"$f":"IF($B$1=\"English\",C1006,IF($B$1=\"Deutsch\",D1006,IF($B$1=\"中文\",E1006,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicic acid (H2Si2O5), barium salt (1:1), lead-doped"},"Silicic acid (H2Si2O5), barium salt (1:1), lead-doped","Kieselsäure (H2Si2O5), Bariumsalz (1:1), Blei-dotiert","原硅酸钠 "]
[null,{"$f":"IF($B$1=\"English\",C1007,IF($B$1=\"Deutsch\",D1007,IF($B$1=\"中文\",E1007,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead bis(carbonate)dihydroxide"},"Trilead bis(carbonate)dihydroxide","Tribleibis(carbonat)dihydroxid","碱式碳酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1008,IF($B$1=\"Deutsch\",D1008,IF($B$1=\"中文\",E1008,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Furan"},"Furan","Furan","呋喃"]
[null,{"$f":"IF($B$1=\"English\",C1009,IF($B$1=\"Deutsch\",D1009,IF($B$1=\"中文\",E1009,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N-dimethylformamide"},"N,N-dimethylformamide","N,N-Dimethylformamid","N,N-二甲基甲酰胺"]
[null,{"$f":"IF($B$1=\"English\",C1010,IF($B$1=\"Deutsch\",D1010,IF($B$1=\"中文\",E1010,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated"},"4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated","4-(1,1,3,3-Tetramethylbutyl)phenol, ethoxyliert","\n4 - （1,1,3,3 - 四甲基丁基）苯酚，乙氧基化的"]
[null,{"$f":"IF($B$1=\"English\",C1011,IF($B$1=\"Deutsch\",D1011,IF($B$1=\"中文\",E1011,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched and linear"},"4-Nonylphenol, branched and linear","4-Nonylphenol, verzweigt und linear","4-壬基酚，支链和直链"]
[null,{"$f":"IF($B$1=\"English\",C1012,IF($B$1=\"Deutsch\",D1012,IF($B$1=\"中文\",E1012,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-methylenedi-o-toluidine"},"4,4'-methylenedi-o-toluidine","4,4'-Methylendi-o-toluidin","4,4'-二氨基-3,3'-二甲基联苯基甲烷"]
[null,{"$f":"IF($B$1=\"English\",C1013,IF($B$1=\"Deutsch\",D1013,IF($B$1=\"中文\",E1013,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diethyl sulphate"},"Diethyl sulphate","Diethylsulfat","硫酸二乙酯"]
[null,{"$f":"IF($B$1=\"English\",C1014,IF($B$1=\"Deutsch\",D1014,IF($B$1=\"中文\",E1014,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethyl sulphate"},"Dimethyl sulphate","Dimethylsulfat","硫酸二甲酯"]
[null,{"$f":"IF($B$1=\"English\",C1015,IF($B$1=\"Deutsch\",D1015,IF($B$1=\"中文\",E1015,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide sulfate"},"Lead oxide sulfate","Bleisulfat, basisch","石灰浆 "]
[null,{"$f":"IF($B$1=\"English\",C1016,IF($B$1=\"Deutsch\",D1016,IF($B$1=\"中文\",E1016,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead titanium trioxide"},"Lead titanium trioxide","Bleititantrioxid","钛酸铅 "]
[null,{"$f":"IF($B$1=\"English\",C1017,IF($B$1=\"Deutsch\",D1017,IF($B$1=\"中文\",E1017,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acetic acid, lead salt, basic"},"Acetic acid, lead salt, basic"," Essigsäure, Bleisalz, basisch","醋酸，油酸铅，碱式碳酸铜 "]
[null,{"$f":"IF($B$1=\"English\",C1018,IF($B$1=\"Deutsch\",D1018,IF($B$1=\"中文\",E1018,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[Phthalato(2-)]dioxotrilead"},"[Phthalato(2-)]dioxotrilead","[Phthalato(2-)]dioxotriblei"," [1,2-苯二羧酸根合]二氧化三铅"]
[null,{"$f":"IF($B$1=\"English\",C1019,IF($B$1=\"Deutsch\",D1019,IF($B$1=\"中文\",E1019,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(pentabromophenyl) ether (decabromodiphenyl ether; DecaBDE)"},"Bis(pentabromophenyl) ether (decabromodiphenyl ether; DecaBDE)","Decabromidiphenylether DecaBDE","十溴联苯醚（decaBDE）"]
[null,{"$f":"IF($B$1=\"English\",C1020,IF($B$1=\"Deutsch\",D1020,IF($B$1=\"中文\",E1020,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-methylacetamide"},"N-methylacetamide","N-Methylacetamid","N-甲基乙酰胺"]
[null,{"$f":"IF($B$1=\"English\",C1021,IF($B$1=\"Deutsch\",D1021,IF($B$1=\"中文\",E1021,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dinoseb (6-sec-butyl-2,4-dinitrophenol)"},"Dinoseb (6-sec-butyl-2,4-dinitrophenol)","Dinoseb (6-sec-butyl-2,4-dinitrophenol)","地乐酚"]
[null,{"$f":"IF($B$1=\"English\",C1022,IF($B$1=\"Deutsch\",D1022,IF($B$1=\"中文\",E1022,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Diethoxyethane"},"1,2-Diethoxyethane","1,2-Diethoxyethan","1,2-乙二醇二乙醚"]
[null,{"$f":"IF($B$1=\"English\",C1023,IF($B$1=\"Deutsch\",D1023,IF($B$1=\"中文\",E1023,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetralead trioxide sulphate"},"Tetralead trioxide sulphate","Tetrableitrioxidsulfat","三碱式硫酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1024,IF($B$1=\"Deutsch\",D1024,IF($B$1=\"中文\",E1024,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-pentyl-isopentylphthalate"},"N-pentyl-isopentylphthalate","N-pentyl-isopentylphthalate","邻苯二甲酸正戊基异戊基酯"]
[null,{"$f":"IF($B$1=\"English\",C1025,IF($B$1=\"Deutsch\",D1025,IF($B$1=\"中文\",E1025,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioxobis(stearato)trilead"},"Dioxobis(stearato)trilead","Dioxobis(stearato)triblei"," 双(十八酸基)二氧代三铅"]
[null,{"$f":"IF($B$1=\"English\",C1026,IF($B$1=\"Deutsch\",D1026,IF($B$1=\"中文\",E1026,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetraethyllead"},"Tetraethyllead","Tetraethylblei","四乙基铅"]
[null,{"$f":"IF($B$1=\"English\",C1027,IF($B$1=\"Deutsch\",D1027,IF($B$1=\"中文\",E1027,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentalead tetraoxide sulphate"},"Pentalead tetraoxide sulphate"," Pentableitetraoxidsulfat"," 氧化铅与硫酸铅的复合物"]
[null,{"$f":"IF($B$1=\"English\",C1028,IF($B$1=\"Deutsch\",D1028,IF($B$1=\"中文\",E1028,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentacosafluorotridecanoic acid"},"Pentacosafluorotridecanoic acid","Pentacosafluortridecansäure","全氟十三酸"]
[null,{"$f":"IF($B$1=\"English\",C1029,IF($B$1=\"Deutsch\",D1029,IF($B$1=\"中文\",E1029,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tricosafluorododecanoic acid"},"Tricosafluorododecanoic acid","Tricosafluordodecansäure","全氟十二烷酸"]
[null,{"$f":"IF($B$1=\"English\",C1030,IF($B$1=\"Deutsch\",D1030,IF($B$1=\"中文\",E1030,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptacosafluorotetradecanoic acid"},"Heptacosafluorotetradecanoic acid","Heptacosafluortetradecansäure","全氟代十四酸"]
[null,{"$f":"IF($B$1=\"English\",C1031,IF($B$1=\"Deutsch\",D1031,IF($B$1=\"中文\",E1031,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-bromopropane (n-propyl bromide)"},"1-bromopropane (n-propyl bromide)","1-Brompropan (n-Propylbromid)"," 正丙基溴"]
[null,{"$f":"IF($B$1=\"English\",C1032,IF($B$1=\"Deutsch\",D1032,IF($B$1=\"中文\",E1032,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methoxyacetic acid"},"Methoxyacetic acid","Methoxyessigsäure","甲氧基乙酸"]
[null,{"$f":"IF($B$1=\"English\",C1033,IF($B$1=\"Deutsch\",D1033,IF($B$1=\"中文\",E1033,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-methyl-m-phenylenediamine (toluene-2,4-diamine)"},"4-methyl-m-phenylenediamine (toluene-2,4-diamine)","4-Methyl-m-phenylendiamin (Toluen-2,4-diamin)","正丙基溴"]
[null,{"$f":"IF($B$1=\"English\",C1034,IF($B$1=\"Deutsch\",D1034,IF($B$1=\"中文\",E1034,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methyloxirane (Propylene oxide)"},"Methyloxirane (Propylene oxide)","Methyloxiran (Propylenoxid)","环氧丙烷"]
[null,{"$f":"IF($B$1=\"English\",C1035,IF($B$1=\"Deutsch\",D1035,IF($B$1=\"中文\",E1035,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead dioxide phosphonate"},"Trilead dioxide phosphonate","Tribleidioxidphosphonat","二碱式亚磷酸铅 "]
[null,{"$f":"IF($B$1=\"English\",C1036,IF($B$1=\"Deutsch\",D1036,IF($B$1=\"中文\",E1036,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"o-aminoazotoluene"},"o-aminoazotoluene","o-Aminoazotoluol","邻氨基偶氮甲苯"]
[null,{"$f":"IF($B$1=\"English\",C1037,IF($B$1=\"Deutsch\",D1037,IF($B$1=\"中文\",E1037,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, dipentylester, branched and linear"},"1,2-Benzenedicarboxylic acid, dipentylester, branched and linear","1,2-Benzoldicarbonsäure, Diphetylester, verzweigt und linear","邻苯二甲酸,碳酸二戊酯,分支和线性"]
[null,{"$f":"IF($B$1=\"English\",C1038,IF($B$1=\"Deutsch\",D1038,IF($B$1=\"中文\",E1038,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-oxydianiline and its salts"},"4,4'-oxydianiline and its salts","4,4'-Oxydianilin","4,4'-二氨基二苯醚"]
[null,{"$f":"IF($B$1=\"English\",C1039,IF($B$1=\"Deutsch\",D1039,IF($B$1=\"中文\",E1039,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Orange lead (lead tetroxide)"},"Orange lead (lead tetroxide)"," Orangemennige (Bleitetraoxid)"," 四氧化三铅"]
[null,{"$f":"IF($B$1=\"English\",C1040,IF($B$1=\"Deutsch\",D1040,IF($B$1=\"中文\",E1040,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biphenyl-4-ylamine"},"Biphenyl-4-ylamine","Biphenyl-4-ylamin","4-氨基联苯酚酯"]
[null,{"$f":"IF($B$1=\"English\",C1041,IF($B$1=\"Deutsch\",D1041,IF($B$1=\"中文\",E1041,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisopentylphthalate"},"Diisopentylphthalate","Diisopentylphthalat"," 邻苯二甲酸二异戊酯"]
[null,{"$f":"IF($B$1=\"English\",C1042,IF($B$1=\"Deutsch\",D1042,IF($B$1=\"中文\",E1042,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fatty acids, C16-18, lead salts"},"Fatty acids, C16-18, lead salts","Fettsäuren, C16-18-, Bleisalze","脂肪酸，C16-18-，硝酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1043,IF($B$1=\"Deutsch\",D1043,IF($B$1=\"中文\",E1043,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diazen-1,2-dicarboxamid (C,C'-azodi(formamid))"},"Diazen-1,2-dicarboxamid (C,C'-azodi(formamid))","Diazen-1,2-dicarboxamid (C,C'-azodi(formamid))","偶氮[二]甲醯胺"]
[null,{"$f":"IF($B$1=\"English\",C1044,IF($B$1=\"Deutsch\",D1044,IF($B$1=\"中文\",E1044,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfurous acid, lead salt, dibasic"},"Sulfurous acid, lead salt, dibasic","Schweflige Säure, Bleisalz, dibasisch","亚硫酸，硝酸铅，二碱式亚磷酸铅 "]
[null,{"$f":"IF($B$1=\"English\",C1045,IF($B$1=\"Deutsch\",D1045,IF($B$1=\"中文\",E1045,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead cyanamidate"},"Lead cyanamidate","Blei(II)cyanamid","氨基氰铅(2+)盐(1:1) "]
[null,{"$f":"IF($B$1=\"English\",C1046,IF($B$1=\"Deutsch\",D1046,IF($B$1=\"中文\",E1046,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- coating material\n- colors\n- diluent\n- color remover\n- inks\n- toner\n- dyeing of ceramics\n- formulation of pyrochlore in glass"},"Usage\n- coating material\n- colors\n- diluent\n- color remover\n- inks\n- toner\n- dyeing of ceramics\n- formulation of pyrochlore in glass","Verwendung\n- Beschichtungsmittel\n- Farben\n- Verdünner\n- Farbentferner\n- Tinten\n- Toner\n- Einfärbung für Keramik\n- Formulierung von Pyrochlor in Glas","使用：\n- 涂层剂\n- 颜色\n- 稀释剂\n- 脱漆剂\n- 油墨\n- 调色剂\n- 对于陶瓷的着色\n- 烧绿石的方法用在玻璃上"]
[null,{"$f":"IF($B$1=\"English\",C1047,IF($B$1=\"Deutsch\",D1047,IF($B$1=\"中文\",E1047,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- textiles\n- cosmetics\n- dyes\n- pigments\nIntermediate\n- dyes"},"Usage\n- textiles\n- cosmetics\n- dyes\n- pigments\nIntermediate\n- dyes","Verwendung\n- Textilien\n- Kosmetikprodukte\n- Farbstoffe\n- Pigmente\nZwischenprodukt\n- Farbstoffe","使用\n- 纺织品\n- 美容产品\n- 染料\n- 颜料\n中间产品\n- 染料"]
[null,{"$f":"IF($B$1=\"English\",C1048,IF($B$1=\"Deutsch\",D1048,IF($B$1=\"中文\",E1048,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers and fluorotelomers"},"Usage\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers and fluorotelomers","Verwendung\n- Zusatzstoff und Komponente in Verbraucher- und Industrieprodukten\nHerstellung\n- fluorierte Polymere und fluorierte Telomere","\n使用\n- 添加剂以及组件在消费者和工业产品\n- 含氟聚合物和含氟调聚物“\n\n"]
[null,{"$f":"IF($B$1=\"English\",C1049,IF($B$1=\"Deutsch\",D1049,IF($B$1=\"中文\",E1049,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- hardener for epoxy resins\n- chain cross-linkers for thermoplastic polymers\n- chemical industry\nProduction\n- polyester and alkyd resins\n- plasticizers for thermoplastic polymer\n\n[2]:\nUsage\n- as soldifying agent for epoxy resins\n- electrical and electronic field\n- compounding matter with alicyclic epoxy resin\n- in dipping of coil of electric apparatus\n- casting of electric parts and sealing semiconductor.\n- as adhesive\n- cohering optical parts\n- as insecticide\n- plasticizer\n- antirust\n- etc."},"Usage\n- hardener for epoxy resins\n- chain cross-linkers for thermoplastic polymers\n- chemical industry\nProduction\n- polyester and alkyd resins\n- plasticizers for thermoplastic polymer\n\n[2]:\nUsage\n- as soldifying agent for epoxy resins\n- electrical and electronic field\n- compounding matter with alicyclic epoxy resin\n- in dipping of coil of electric apparatus\n- casting of electric parts and sealing semiconductor.\n- as adhesive\n- cohering optical parts\n- as insecticide\n- plasticizer\n- antirust\n- etc.","Verwendung\n- Härter für Epoxidharze\n- Kettenvernetzer für thermoplastische Polymere\n- chemische Industrie\nHerstellung\n- Polyester und Alkydharze\n- Weichmacher für thermoplastische Polymere\n\n[2]:\nVerwendung\n- Festigungsmittel für Epoxidharze\n- elektronischer und elektrischer Bereich\n- Kompoundierungsmaterial für alizyklische Epoxidharze\n- Tauchbad für elektrische Geräte\n- gießen elektrischer Teile und Abdichtung von Halbleitern\n- als Kleber\n- zusammenkleben optischer Teile\n- als Insektizid\n- Weichmacher\n- Rostschutz\n- etc.\n\n\n","使用\n- 固化剂用于环氧树脂\n- 网状的用于热塑料性的聚合物\n- 化学工业 \n生产\n- 聚酯和醇酸树脂\n- 柔软剂用于热塑料性聚合物\n\n[2]:\n使用\n- 加强剂用于环氧树脂\n- 电子和电器系列\n- 堆制材料用于脂环式环氧树脂\n- 浸渍用于电气设备\n- 电气部件浇注和半导体密封\n- 作为粘合剂\n- 粘在一起的光学部件\n- 作为一种杀虫剂\n- 增塑剂\n- 防锈\n- 等等。"]
[null,{"$f":"IF($B$1=\"English\",C1050,IF($B$1=\"Deutsch\",D1050,IF($B$1=\"中文\",E1050,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[all]:\nUsage\n- hardener for epoxy resins\nHerstellung\n- monomer in the manufacture of resins\n- polyester resins and alkyd resins\n- plasticizers (for thermoplastic polymers)\nIntermediate\n- in chemical synthesis or process\n- plasticizer\n- insect repellents\n- rust inhibitors\n\n[1]:\nUsage\n- chemical industry\n- synthesis of asymmetrical rigid polyamides\n- chain cross-linkers for thermoplastic polymers\n- plasticizers\n- insect repellents\n- rust inhibitors\n- monomer in the manufacture of resins\n- hardener in epoxy resins\nProduction\n- polyester \n- insect repellents\n- rust inhibitors\n- bright polyester- and alkyd resins\n\n[3]:\nUsage\n- chain cross-linkers for thermoplastic polymers\nFor HHPA specific the following uses are identified\n- alkyd resins\n- plasticizers\n- insect repellents\n- rust inhibitors\n- hardener in epoxy resins (Keskinen 2004)\nProduction\n- polyester"},"[all]:\nUsage\n- hardener for epoxy resins\nHerstellung\n- monomer in the manufacture of resins\n- polyester resins and alkyd resins\n- plasticizers (for thermoplastic polymers)\nIntermediate\n- in chemical synthesis or process\n- plasticizer\n- insect repellents\n- rust inhibitors\n\n[1]:\nUsage\n- chemical industry\n- synthesis of asymmetrical rigid polyamides\n- chain cross-linkers for thermoplastic polymers\n- plasticizers\n- insect repellents\n- rust inhibitors\n- monomer in the manufacture of resins\n- hardener in epoxy resins\nProduction\n- polyester \n- insect repellents\n- rust inhibitors\n- bright polyester- and alkyd resins\n\n[3]:\nUsage\n- chain cross-linkers for thermoplastic polymers\nFor HHPA specific the following uses are identified\n- alkyd resins\n- plasticizers\n- insect repellents\n- rust inhibitors\n- hardener in epoxy resins (Keskinen 2004)\nProduction\n- polyester","[alle]:\nVerwendung\n- Härter für Epoxidharze\nHerstellung\n- Monomer bei der Herstellung von Harzen\n- Polyesterharze und Alkydharze\n- Weichmacher (für thermoplastische Polymere)\nZwischenprodukt\n- bei der chemischen Synthese oder beim chemischen Prozess\n- Weichmacher\n- Insektenschutz\n- Rostschutzmittel\n\n[1]:\nVerwendung\n- chemische Industrie\n- die Synthese asymmetrischer starrer Plyamide\n- Kettenvernetzer für thermoplastische Polymere\n-  Weichmacher\n- Insektenschutz\n- Rostschutz\n- Monomer bei der Herstellung von Harzen\n- Härter in Epoxidharzen\nHerstellung\n- Polyester\n- Insektenschutzmittel\n- Rostinhibitoren\n- helle Alkyd- und Polysterharze\n\n[3]:\nVerwendung\n- Kettenvernetzer für  thermoplastische Polymere\nspezifisch für \"HHPA\"wurden die folgenden Verwendungen identifiziert worden:\n-  Alkydharze\n- Weichmacher\n- Insektenschutz\n- Rostschutzmittel\n- Härter für Epoxidharze (Keskinen 2004)\nHerstellung\n- Polyester\n","[全部]：\n使用\n- 固化剂用于环氧树脂的生产\n- 单体在生产树脂\n- 聚酯树脂和醇酸树脂\n- 软化剂（热塑性聚合物）的中间产品\n- 在化学合成或化学工艺\n- 软化剂\n- 杀虫剂\n- 防锈剂\n\n[1]：\n使用\n- 化学工业 \n- 非对称刚性聚酰胺的合成\n- 网状的热塑性聚合物\n- 软化剂\n- 杀虫剂\n- 防锈\n- 单体在生产树脂\n- 固化剂的环氧树脂生产\n- 涤纶\n- 驱蚊\n- 防锈剂\n- 明亮的醇-酸树脂\n\n[3]：\n使用\n- 网状的热塑性聚合物\n专门用于“HHPA”，已经确定下列用途：\n- 醇酸树脂\n- 软化剂\n- 杀虫剂\n- 防锈剂\n- 固化剂用于环氧树脂（2004 Keskinen）生产\n- 涤纶"]
[null,{"$f":"IF($B$1=\"English\",C1051,IF($B$1=\"Deutsch\",D1051,IF($B$1=\"中文\",E1051,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- insulations and coatings\n- food packging\n- T-shirts\n- polyurethane gloves\n- sanitary napkins\n- medical equipment\n- cellophane wrap\n- soft toys\n- PVC plastics (water pipes, packaging materials, textile products)\n- silicone rubber (sealants, dental products, paper coatings)\n- polyurethanes (foam plastics, glue/sealants)\n- glass (coatings)\n- insulators in electronics and cables\n- deworming agent for poultry\n- polyurethanes\n- transparent plastics\n- additive in rubber\n- stabilizer in PVC plastics\nProduction\n- catalyzer in the production of polyurethanes and silicones\n- catalyzer for esterification\n"},"Usage\n- insulations and coatings\n- food packging\n- T-shirts\n- polyurethane gloves\n- sanitary napkins\n- medical equipment\n- cellophane wrap\n- soft toys\n- PVC plastics (water pipes, packaging materials, textile products)\n- silicone rubber (sealants, dental products, paper coatings)\n- polyurethanes (foam plastics, glue/sealants)\n- glass (coatings)\n- insulators in electronics and cables\n- deworming agent for poultry\n- polyurethanes\n- transparent plastics\n- additive in rubber\n- stabilizer in PVC plastics\nProduction\n- catalyzer in the production of polyurethanes and silicones\n- catalyzer for esterification\n","Verwendung\n- Isolierungen und Beschichtungen\n- Lebensmittelverpackungen\n- T-Shirts\n- Polyurethan-Handschuhe\n- Hygienebinden\n- medizinische Geräten\n- Cellophan-Verpackungen\n- Plüschtiere\n- PVC-Kunststoffe (Wasserleitungen, Verpackungsmaterial, Textilprodukte)\n- Silikonkautschuk (Dichtungsmittel, Dentalprodukte, Papierbeschichtungen)\n- Polyurethane (Schaumkunststoffe, Kleb-/Dichtstoffe)\n- Glas (Beschichtungen)\n- Isolierungen in elektronischen Erzeugnissen und Kabeln\n- Entwurmungsmitteln für Geflügel\n- Polyurethane\n- transparente Kunststoffe\n- Zusatzstoff in Kautschuk/Gummi\n- Stabilisator in PVC-Kunststoffen\nHerstellung \n- Katalysator bei der Herstellung von Polyurethanen und Silikonen\n- Veresterungskatalysatoren\n","使用\n- 绝缘涂料\n- 食品包装\n- T恤\n- 聚氨酯手套\n- 卫生巾\n- 医疗设备\n- 玻璃纸包装\n- 毛绒玩具\n- 聚氯乙烯塑料（水管，包装材料，纺织产品）\n- 硅橡胶（密封剂，牙科产品，纸张涂料）\n- 聚氨酯（泡沫塑料，胶粘剂和密封剂）\n- 玻璃（涂料）\n- 电子产品和电缆用的绝缘材料   \n- 驱虫药品\n- 聚氨酯\n- 透明塑料\n- 橡胶/橡胶添加剂\n- 稳定剂PVC塑料制品的生产\n- 催化剂用于生产聚氨酯和有机硅，\n- 酯催化剂"]
[null,{"$f":"IF($B$1=\"English\",C1052,IF($B$1=\"Deutsch\",D1052,IF($B$1=\"中文\",E1052,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- automatic and manual electrolytic lead\n- in electroplate liquid for lead and its alloy\n- curing agent for epoxy resins\n- metal finishing\nProduction:\n- linear polyesters\n"},"Usage\n- automatic and manual electrolytic lead\n- in electroplate liquid for lead and its alloy\n- curing agent for epoxy resins\n- metal finishing\nProduction:\n- linear polyesters\n","Verwendung\n- bei automatisiertem und manuellem elektrolytischen verbleien\n- in Galvanisierungsflüssigkeit für Blei und seine Gemische/Verbindungen\n- Härtungsmittel für Epoxidharze\n- Endbearbeitung von Metall \nHerstellung\n- lineare Polyester","使用：\n- 自动和手动电解铅涂层\n- 在电镀铅及其配制品/化合物\n- 固化剂用于环氧树脂\n- 金属时表面处理\n生产：\n- 线性聚酯"]
[null,{"$f":"IF($B$1=\"English\",C1053,IF($B$1=\"Deutsch\",D1053,IF($B$1=\"中文\",E1053,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- coating\n- color\n- diluent\n- paint remover\n- filler\n- putty\n- mortar\n- modeling clay\n- finger paint\n- oxidizing agentl in dye industry\n- heat stabilizer in nylon\nProduction\n- textile mordant\n- matches\n- special explosive materials\n- etching solution\n- for pearl coloring\n- explosive material\n- lead dinitrate\n- weapons and ammunition\n- pigments and fine chemicals\nIntermediate\n- laboratory chemicals"},"Usage\n- coating\n- color\n- diluent\n- paint remover\n- filler\n- putty\n- mortar\n- modeling clay\n- finger paint\n- oxidizing agentl in dye industry\n- heat stabilizer in nylon\nProduction\n- textile mordant\n- matches\n- special explosive materials\n- etching solution\n- for pearl coloring\n- explosive material\n- lead dinitrate\n- weapons and ammunition\n- pigments and fine chemicals\nIntermediate\n- laboratory chemicals","Verwendung\n- Beschichtungsmitteln\n- Farben\n- Verdünner\n- Farbentferner\n- Füllstoffe\n- Spachtelmassen\n- Mörtel\n- Modellierton\n- Fingerfarben\n- Oxidationsmittel in der Farbstoffindustrie\n- Hitzestabilisator bei Nylon\nHerstellung\n- Textilbeizen\n- Streichhölzer\n- Spezialexplosivstoffe\n- Ätzlösungen\n- Perlmuttfärbung\n- Sprengstoffe\n- Bleidinitrat\n- Waffen und Munition\n- Pigmenten und Feinchemikalien\nZwischenprodukt\n- Laborchemikalien","使用\n- 涂层剂\n- 颜色\n- 稀释剂\n- 脱漆剂\n- 填料\n- 填充剂\n- 砂浆\n- 模型粘土\n- 指画颜料\n- 在染料工业的氧化剂\n- 尼龙生产时的热稳定剂\n生产\n- 纺织酸洗\n- 配对\n- 特殊爆炸物\n- 腐蚀剂\n- 珍珠色素\n- 爆炸物\n- 硝酸钡\n- 武器和弹药\n- 颜料和精细化学品的中间产品\n- 实验室化学品"]
[null,{"$f":"IF($B$1=\"English\",C1054,IF($B$1=\"Deutsch\",D1054,IF($B$1=\"中文\",E1054,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- stone-, gypsum-, cement-, and ceramic products\n- lead crystal articles"},"Usage\n- stone-, gypsum-, cement-, and ceramic products\n- lead crystal articles","Verwendung\n- Stein-, Gips-, Zement-, Glas- und Keramikerzeugnisse\n- Bleikristallware","使用\n- 石头，石膏，水泥，玻璃和陶瓷制品\n- 铅水晶器皿"]
[null,{"$f":"IF($B$1=\"English\",C1055,IF($B$1=\"Deutsch\",D1055,IF($B$1=\"中文\",E1055,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- dyeing agent in microscopy\n- in pyrotechnics for generating yellow smoke\n- as yellow pigment in inks (also inkjet printers)\n- insecticide\n- dyeing agent for varnishes, waxes and plastics\n- starting material for other dyes\n- lacquer\n- varnishes\n- wax products\n- oil stains\n- styrene resins\nProduction\n- diazo dyes\n- indulines\nIntermediate"},"Usage\n- dyeing agent in microscopy\n- in pyrotechnics for generating yellow smoke\n- as yellow pigment in inks (also inkjet printers)\n- insecticide\n- dyeing agent for varnishes, waxes and plastics\n- starting material for other dyes\n- lacquer\n- varnishes\n- wax products\n- oil stains\n- styrene resins\nProduction\n- diazo dyes\n- indulines\nIntermediate","Verwendung\n- Anfärbemittel in der Mikroskopie\n- in der Pyrotechnik zur Erzeugung von gelbem Rauch\n- als gelbes Pigment in Tinten (auch Tintenstrahldruckern)\n- Insektizid\n- als Anfärbemittel für Lacke, Wachse und Kunsstoffe\n- Ausgangsstoff für andere Farbstoffe\n- Lack\n- Firnis\n- Wachsprodukte\n- Beize\n- Styrenharze\nHerstellung\n- Diazo-Farbstoffe\n- Induline\nZwischenprodukt","使用\n- 染色在显微镜下\n- 在烟火制造术产生黄烟\n- 作为黄色颜料在油墨中（包括喷墨打印机）\n- 杀虫剂\n- 作为染色剂用于涂料，蜡和塑料\n- 其他染料原料\n- 油漆\n- 清漆\n- 蜡产品\n- 染色;\n生产\n- 苯乙烯树脂\n- 重氮染料\n- 引杜林的中间产品“"]
[null,{"$f":"IF($B$1=\"English\",C1056,IF($B$1=\"Deutsch\",D1056,IF($B$1=\"中文\",E1056,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- computer\n- electronic and optical products\n- electro-ceramic components\nIntermediate"},"Usage\n- computer\n- electronic and optical products\n- electro-ceramic components\nIntermediate","Herstellung\n- Computer\n- elektronische und optische Produkte\n- elektronische-keramische Komponenten\n- Zwischenprodukt","生产\n- 电脑\n- 电子及光学产品\n- 电子陶瓷元件\n中间产品"]
[null,{"$f":"IF($B$1=\"English\",C1057,IF($B$1=\"Deutsch\",D1057,IF($B$1=\"中文\",E1057,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- lead soap\n- ointments and lead plasters\n- ceramic, porcelain painting, glass painting\n- electronic components\nProduction\n- lead oxide\n- flint glass\n- varnish\n- glass putty\n- metal putty\n- accumulators\n- lead acid battery\n- activators for rubber\n- crystall glass and ceramics\n- rubber protection\n- explosive\nIntermediate"},"Usage\n- lead soap\n- ointments and lead plasters\n- ceramic, porcelain painting, glass painting\n- electronic components\nProduction\n- lead oxide\n- flint glass\n- varnish\n- glass putty\n- metal putty\n- accumulators\n- lead acid battery\n- activators for rubber\n- crystall glass and ceramics\n- rubber protection\n- explosive\nIntermediate","Verwendung\n- Bleiseifen\n- Salben und Bleipflaster\n- Keramik, Porzellanmalerei und Glasmalerei\n- elektronische Komponenten\nHerstellung\n- Bleioxid\n- Flintglas\n- Firnissen\n- Glaskitten\n- Metallkitten\n- Akkumulatoren\n- Blei-Säure-Batterien\n- Aktivatoren für Kautschuk\n- Kristallglas und Keramik\n- Gummischutz\n- Sprengstoff\nZwischenprodukt","使用\n- 铅皂\n- 软膏和铅膏\n- 陶瓷，瓷板画和彩色玻璃\n- 电子元件\n生产\n- 氧化铅\n- 火石玻璃\n- 清漆\n- 玻璃灰\n- 金属灰\n- 蓄电池\n- 铅酸电池\n- 活化橡胶\n- 水晶玻璃和陶瓷\n- 橡胶保护\n- 炸药的中间产品"]
[null,{"$f":"IF($B$1=\"English\",C1058,IF($B$1=\"Deutsch\",D1058,IF($B$1=\"中文\",E1058,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- laboratory reagent\nProduction\n- dyes (intermediate)\n- vulcanization accelerator\n- textile auxiliary substances\n- herbicide agents\n- chlorotoluidine and nitrated toluidine\n- pharmaceuticals\n- dyes and pigments\nIntermediate\n- synthetic rubber"},"Usage\n- laboratory reagent\nProduction\n- dyes (intermediate)\n- vulcanization accelerator\n- textile auxiliary substances\n- herbicide agents\n- chlorotoluidine and nitrated toluidine\n- pharmaceuticals\n- dyes and pigments\nIntermediate\n- synthetic rubber","Verwendung\n- Laborreagenz\nHerstellung\n- Farbstoffe (Zwischenprodukt)\n- Vulkanisationsbeschleuniger\n- Textilhilfsmittel\n- Herbizide\n- Chlortoluidine und nitrierten Toluidine\n- Pharmazeutika\n- Farbstoffe und Pigmente\nZwischenprodukt\n- Synthesekautschuk","使用\n- 实验室试剂\n生产\n- 染料（中间产品）\n- 硫化\n- 纺织辅助剂\n- 除草剂\n- 氯引杜林(水溶)和渗氮甲基苯胺\n- 制药\n- 染料和颜料\n中间产品\n- 合成橡胶"]
[null,{"$f":"IF($B$1=\"English\",C1059,IF($B$1=\"Deutsch\",D1059,IF($B$1=\"中文\",E1059,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- paints for poly urethane \n- polyurethane finishings and sealants"},"Usage\n- paints for poly urethane \n- polyurethane finishings and sealants","Verwendung\n- Farben für Polyurethan\n- polyurethane finishings and sealants\n","使用\n- 颜料用于聚氨酯\n- 聚氨酯的表面处理和密封剂"]
[null,{"$f":"IF($B$1=\"English\",C1060,IF($B$1=\"Deutsch\",D1060,IF($B$1=\"中文\",E1060,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- coating of glass lamp bulbs\n- formulation of mixtures and/or re-packaging"},"Usage\n- coating of glass lamp bulbs\n- formulation of mixtures and/or re-packaging","Verwendung\n- Beschichtung von Glaslampenkolben\n- Formulierung (Mischen) von Gemischen und/oder Neuverpackungen","使用\n- 玻璃灯管的涂层\n- 制剂配方（混合）的配制品和/或重新包装"]
[null,{"$f":"IF($B$1=\"English\",C1061,IF($B$1=\"Deutsch\",D1061,IF($B$1=\"中文\",E1061,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production\n- PTC ceramic\n- colors for restoration of artworks and historical parts\n- polyester, polythenes\n- strand isolation\n- ceramic glaze\n- pigment- and color component\n- heat stabilizer for PVC\n- parchment processing"},"Production\n- PTC ceramic\n- colors for restoration of artworks and historical parts\n- polyester, polythenes\n- strand isolation\n- ceramic glaze\n- pigment- and color component\n- heat stabilizer for PVC\n- parchment processing","Herstellung\n- PTC-Keramik\n- Farben zur originalgetreuen Wiederherstellung von Kunstwerken und historischen Bestandteilen\n- in Polyester, Polyethene\n- Drahtisolation\n- Keramikglasur\n- Pigment- und Farbkomponente\n- Hitzestabilisator bei PVC\n- Pergamentverarbeitung\n","生产\n- PTC陶瓷\n- 色彩用于艺术和历史的成品的原始恢复\n- 在聚酯，聚乙烯\n- 电线绝缘\n- 陶瓷釉料\n- 颜料和彩色分量\n- 热稳定剂的PVC\n- 羊皮纸处理"]
[null,{"$f":"IF($B$1=\"English\",C1062,IF($B$1=\"Deutsch\",D1062,IF($B$1=\"中文\",E1062,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- formation of lacquers\n- solvent for resins\nProduction\n- related compounds, e.g. tetrahydrofuran and also different polymers and pharmaceuticals\n- hydrogenation to cyclic ether tetrahydro..?, which is often used as a solvent\n- mixed with sand as mold material in molding boxes"},"Usage\n- formation of lacquers\n- solvent for resins\nProduction\n- related compounds, e.g. tetrahydrofuran and also different polymers and pharmaceuticals\n- hydrogenation to cyclic ether tetrahydro..?, which is often used as a solvent\n- mixed with sand as mold material in molding boxes","Verwendung\n- Formulierung von Lacke\n- Lösungsmittel von Harzen\nHerstellung\n- verwandte Verbindungen z.B. Tetrahydrofuran sowie verschiedener Polymere und Pharmazeutika\n- Hydrierung zum cyclischen Ether Tetrahydrofun, der oft als Lösungsmittel verwendet wird. \n- mit Sand vermischt, als Formwerkstoff in Formkästen\n","使用\n- 涂料配方\n- 树脂的溶剂\n生产\n- 相关化合物，如四氢呋喃，和各种聚合物和药物\n- 氢化的环醚Tetrahydrofun，它通常被用作溶剂。\n- 混合砂在箱子的形式模具材料 "]
[null,{"$f":"IF($B$1=\"English\",C1063,IF($B$1=\"Deutsch\",D1063,IF($B$1=\"中文\",E1063,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- specific plastic coating (e.g. for heat- and corrosion-resistant coatings like wire enamel)\n- paint remover\n- pesticide formulations\n- solvent for a wide range of solid, liquid or gaseous substances, for polymers such as polyacrylonitrile, PVC, polyamides, polyurethanes, epoxy resins, cellulose and their derivatives\n- solvent in syntheses and for solidification in pharma industry\n- cleaning solvent in the leather or artificial leather industry, and more generally in the textile industry\n- laboratory chemical\n- additive in aviation gasoline\n- reagent and catalyst for syntheses in organic chemistry\n- in electronics, mainly in the manufacture of printed circuit boards\n- formulation of preparations (by workers in industrial settings)\n- selective absorption (e.g. extraction of acetylene in ethene currents)\n- polyacylic fibers\n- Orlon\n- polyurethane coatings\n- high voltage capacitors\n- industrial paint stipping applications\n- solvents\nProduction\n- synthetic/artificial leather of polyurethane\n- circuit boards in field of electronics\n- electric distributors and curcuits\n- formulation of preperations\n- catalyst in the production of acid chlorides from carboxylic acids and oxalychloride?\n- chemicals\n- other substances\nIntermediate\n\n\n"},"Usage\n- specific plastic coating (e.g. for heat- and corrosion-resistant coatings like wire enamel)\n- paint remover\n- pesticide formulations\n- solvent for a wide range of solid, liquid or gaseous substances, for polymers such as polyacrylonitrile, PVC, polyamides, polyurethanes, epoxy resins, cellulose and their derivatives\n- solvent in syntheses and for solidification in pharma industry\n- cleaning solvent in the leather or artificial leather industry, and more generally in the textile industry\n- laboratory chemical\n- additive in aviation gasoline\n- reagent and catalyst for syntheses in organic chemistry\n- in electronics, mainly in the manufacture of printed circuit boards\n- formulation of preparations (by workers in industrial settings)\n- selective absorption (e.g. extraction of acetylene in ethene currents)\n- polyacylic fibers\n- Orlon\n- polyurethane coatings\n- high voltage capacitors\n- industrial paint stipping applications\n- solvents\nProduction\n- synthetic/artificial leather of polyurethane\n- circuit boards in field of electronics\n- electric distributors and curcuits\n- formulation of preperations\n- catalyst in the production of acid chlorides from carboxylic acids and oxalychloride?\n- chemicals\n- other substances\nIntermediate\n\n\n","Verwendung\n- spezielle Kunststoffbeschichtung (z.B. für wärme- und korrosionsbeständige Beschichtungen wie Drahtlacke)\n- Abbeizmittel\n- Pflanzschutzmittel-Formulierung\n- Lösungsmittel für eine Vielzahl von festen, flüssigen oder gasförmigen Stoffen, für Polymere wie bspw. Polyacrylnitril, PVC, Polyamide, Polyurethane, Epoxidharze, für Cellulose und deren Derrivate\n- Lösungsmittel in Synthesen und Zur Kristallisierung in der Pharmaindustrie\n- Laborchemikalie\n- Zusatzstoff in Flugbenzin\n- Reagenz und Katalysator für Synthesen in der organischen Chemie\n- in Elektronik, hauptsächlich in der Herstellung von Leiterplatten\n- als Reinigungslösung in der Leder- or Kunstlederindustrie und allgemein in der Textilindustrie\n- Formulierung von Zubereitungen (von Arbeitern im industriellen Umfeld)\n- selektive Absorption (z. B. Acetylenextraktion in Ethenströmen)\n- Polyacrylfaser\n- Orlon\n- Polyurethanbeschichtungen\n- Hochspannungskondensatoren\n- industrielle Abbeiz-Anwendungen\n- Lösungen\nHerstellung\n- Synthetischem / künstlichen Leder aus Polyurethan\n- Leiterplatten im Elektronikbereich \n- elektrische Verteiler und Schaltkreise\n- Formulierung von Zubereitung \n- Katalysator bei der Herstellung von Säurechloriden aus Carbonsäuren und Oxalychlorid\n- Herstellung anderer Stoffe\n- chemische Produkten\nZwischenprodukt\n- in der Synthese von Acetalen, Aldehyden, Carbonsäureestern und Nitrilen\n- als Reagenz und Katalysator für Synthesen in der organischen Chemie","使用\n- 特殊塑料涂层（如耐热和耐腐蚀涂层，如漆包线）\n- 脱漆剂\n- 植物保护剂配方\n- 溶剂用于各种固体，液体或气体的物质，例如\n聚丙烯腈，聚氯乙烯，聚酰胺，聚氨酯，环氧树脂，纤维素聚合物，以及为衍生物\n- 溶剂在合成物和为了结晶化在制药工业中\n- 化学实验室\n- 在航空燃油添加剂\n- 试剂和催化剂用于合成有机化学\n- 在电子技术中，特别是在印刷电路板的制造\n-在皮革或人造皮革行业和普通的纺织行业中作为清洗液\n- 制剂配方（工人在工业环境中）\n- 选择吸收（如Acetylenextraktion在Ethenströmen）\n- 聚丙烯\n- 腈纶\n- 聚氨酯涂料\n- 高压电容器\n- 工业中的剥离应用\n- 溶剂\n生产\n- 合成/人造皮革制成的聚氨酯\n- 电子行业印刷电路板\n- 配电和电路\n- 配制配方\n- 自羧酸和草酰氯来制备酰氯的制造中的催化剂\n- 制造其他物质\n- 化学产品\n- 其它物质\n中间体"]
[null,{"$f":"IF($B$1=\"English\",C1064,IF($B$1=\"Deutsch\",D1064,IF($B$1=\"中文\",E1064,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- water-based paint\n- formulation of paints\n- consumer and professional end-use of products (e.g. paints)\n- ethoxylates in emulsion polymerisation\n- oil for lubrication or for hydraulic devices\n- metal working liquids\n- building industry\n- textile and leather auxiliaries\n- as component (emulgent) of bitumen-/wax emulsions for paint/seal in building industry or covering of concrete surfaces\n- mold release agents on building sites and production of precast concrete components and also as auxiliary agent to clean machines\n- emulgent for emulsion polymerization\n- veterinary Medical products\n- pesticide formulations\n- pore forming agent/foaming agent for concrete \n- surfactants\n- cleaning of metal surfaces\nIntermediate\n- production of octylphenolethersulfate\n- production of other sulphates\n"},"Usage\n- water-based paint\n- formulation of paints\n- consumer and professional end-use of products (e.g. paints)\n- ethoxylates in emulsion polymerisation\n- oil for lubrication or for hydraulic devices\n- metal working liquids\n- building industry\n- textile and leather auxiliaries\n- as component (emulgent) of bitumen-/wax emulsions for paint/seal in building industry or covering of concrete surfaces\n- mold release agents on building sites and production of precast concrete components and also as auxiliary agent to clean machines\n- emulgent for emulsion polymerization\n- veterinary Medical products\n- pesticide formulations\n- pore forming agent/foaming agent for concrete \n- surfactants\n- cleaning of metal surfaces\nIntermediate\n- production of octylphenolethersulfate\n- production of other sulphates\n","Verwendung\n- Wasserbasierte Anstrichfarben\n- Formulierung von Farben\n- Verbraucher und professioneller Endverbrauch von Produkten (z.B. Farben)\n- Ethoxylate bei Emulsionpolymerisation \n- Öl zur Schmierung oder für hydraulische Geräte\n- Metallbearbeitungsflüssigkeiten\n- In der Bauindustrie\n- Textil- und Lederhilfsmittel\n- als Bestandteil (Emulgator) von Bitumen-/Wachsemulsionen zum Anstrich/Abdichten in der Bauindustrie bzw. beim Abdecken von Betonoberflächen\n- Formentrennmittel auf Baustellen und bei der Betonfertigteilherstellung sowie als Hilfsmittel für das Reinigen von Maschinen\n- Emulgator für Emulsionspolymerisation\n- Veterinärmedizinische Produkte\n- Pestizidformulierungen\n- Porenbildner/Schäumungsmittel für Beton \n- oberflächenaktiver Stoff \n- Reinigung von metallischer Oberfläche\nZwischenprodukt\n- für der Herstellung von Octylphenolethersulfaten\n- für die Produktion von anderen Sulfaten\n","使用\n- 水性涂料\n- 颜色配方\n- 消费者和专业最终使用的产品（如颜色）\n- 乙氧基化物在乳液聚合\n- 润滑或液压设备用油\n- 金属加工液\n- 建筑工业\n- 纺织和皮革辅助剂\n-作为沥青/蜡乳化剂的组成部分用来涂装/密封在建筑行业或者覆盖在混凝土表面\n-脱模剂用于建筑工地和预制混凝土生产以及作为辅助方法用于机器的清理\n- 乳化剂用于乳液聚合\n- 兽医产品\n- 农药制品\n- 造孔剂/发泡剂混凝土\n- 表面活性剂\n- 金属表面清洗\n中间体\n- 硫酸辛基酚乙醚的生产\n- 用于生产其他硫酸盐"]
[null,{"$f":"IF($B$1=\"English\",C1065,IF($B$1=\"Deutsch\",D1065,IF($B$1=\"中文\",E1065,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- formulation of adhesives, paints\n- pressure-sensitive adhesive in production of tires and rubber products \n- industrial use of coatings or inks \n- washing of imported textiles\n- Pulp, paper and board industry\n- in paper production as a component of phenolic resins used in coatings, e.g. for carbonless copy paper\n- other NP-resins used for printing inks\n- antioxidants and plasticizers in plastic products\nIntermediate\n- production of ethoxylates? and plastic stabilizer\n"},"Usage\n- formulation of adhesives, paints\n- pressure-sensitive adhesive in production of tires and rubber products \n- industrial use of coatings or inks \n- washing of imported textiles\n- Pulp, paper and board industry\n- in paper production as a component of phenolic resins used in coatings, e.g. for carbonless copy paper\n- other NP-resins used for printing inks\n- antioxidants and plasticizers in plastic products\nIntermediate\n- production of ethoxylates? and plastic stabilizer\n","Verwendung\n- Formulierung von Klebstoffen, Anstrichfarben\n- Haftkleber bei der Herstellung von Reifen und Gummiprodukten\n- Industrielle Anwendung von Beschichtungen oder Tinten\n- Waschen von importierten Textilien \n- in der Zellstoff-, Papier- und Pappindustrie\n- in der Papierproduktion als Komponente von Phenolharzen in Beschichtungen verwendet,z.B.. für selbstdurchschreibendes Kopierpapier\n- andere NP-Harze, die für Druckertinten verwendet werden\n- Antioxidationsmittel und Weichmacher in Plastik \nZwischenprodukt\n- Herstellung von Ethoxylaten und Kunststoffstabilisator\n","使用\n- 胶粘剂配方，涂料，\n- 胶粘剂用于轮胎和橡胶制品的制造\n- 涂料或油墨的工业应用\n- 进口纺织品的洗涤\n- 在纸浆，纸和纸板行业\n-在造纸时用作酚醛树脂涂料的成分做表面涂层，如无碳复印纸。\n-其它 NP树脂，用于印刷油墨\n- 塑料制造中的抗氧化剂和塑化剂\n中间产品\n- 制造乙氧基化物和塑料稳定剂"]
[null,{"$f":"IF($B$1=\"English\",C1066,IF($B$1=\"Deutsch\",D1066,IF($B$1=\"中文\",E1066,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- in research about high-performance polymers\nIntermediate\n- dyes"},"Usage\n- in research about high-performance polymers\nIntermediate\n- dyes","Verwendung\n- in der Forschung über Hochleistungspolymere\nZwischenprodukt\n- Farbstoffe","使用\n- 关于高性能聚合物研究\n中间产品\n- 染料"]
[null,{"$f":"IF($B$1=\"English\",C1067,IF($B$1=\"Deutsch\",D1067,IF($B$1=\"中文\",E1067,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- alkylation of phenols, amines and thiols \n- ethylation, especially for production of pharmaceuticals\n- Accelerator of sulfate agglomeration on ethene\n- in sulfonations\n- reactant in polymer synthesis\n- finishing agent in textile manufacture\n- dye-set agent in carbonless paper\nProduction\n- fine chemicals\n- dyes\n- pigment production\nIntermediate\n- methylation agent"},"Usage\n- alkylation of phenols, amines and thiols \n- ethylation, especially for production of pharmaceuticals\n- Accelerator of sulfate agglomeration on ethene\n- in sulfonations\n- reactant in polymer synthesis\n- finishing agent in textile manufacture\n- dye-set agent in carbonless paper\nProduction\n- fine chemicals\n- dyes\n- pigment production\nIntermediate\n- methylation agent","Verwendung\n- Alkylierung von Phenolen, Aminen und Thiolen \n- Ethylierung, insbesondere zur Herstellung von Pharmazeutika\n- als Beschleuniger der Sulfat-Anlagerung an Ethen\n- in Sulfonierungen\n- Reaktant bei der Polymersynthese\n- Textilherstellung\n- Farbstoffassistent in der farblosen Papierherstellung\nHerstellung\n- Feinchemikalien\n- Farbstoff\n- pigment production\nZwischenprodukt\n- Methylierungsmittel\n","使用\n- 酚类，胺类和硫醇的烷基化反应\n- 乙基化，尤其是用于药物生产\n- 作为硫酸盐加成乙烯的加速器\n- 在sulfonations\n- 反应物在合成聚合物时\n- 纺织制造\n- 染料助手在生产无色纸造纸\n- 精细化工\n- 染料\n- 颜料生产的中间产品\n- 甲基化剂"]
[null,{"$f":"IF($B$1=\"English\",C1068,IF($B$1=\"Deutsch\",D1068,IF($B$1=\"中文\",E1068,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- methylation of carboxylic acid, phenols, thiophenols, amines and other compounds\n- raw material for production of cosmetics, colors, pharmaceuticals and agricultural products\n- polyurethane-based adhesives\n- fabric softeners\n- dyes\n- DNA sequencing\nIntermediate\n- methylation agent"},"Usage\n- methylation of carboxylic acid, phenols, thiophenols, amines and other compounds\n- raw material for production of cosmetics, colors, pharmaceuticals and agricultural products\n- polyurethane-based adhesives\n- fabric softeners\n- dyes\n- DNA sequencing\nIntermediate\n- methylation agent","Verwendung:\n- zur Methylierung von Carbonsäuren, Phenolen, Thiophenolen, Aminen und andere Verbindungen\n- Rohstoff für die Herstellung von Kosmetika, Farben, Arzneimitteln und Agrarprodukten\n- Polyurethan-Klebstoffe\n- Weichspüler\n- Farbstoffe\n- der DNA-Sequenzierung\nZwischenprodukt:\n- als Methylierungsmittel","使用\n- 为羧酸，酚，硫酚，胺和其他化合物的甲基化\n- 用于化妆品，涂料，医药和农业产品的生产原料\n- 聚氨酯胶粘剂\n- 织物柔软剂\n- 染料\n- DNA测序\n中间产品\n- 作为甲基化剂"]
[null,{"$f":"IF($B$1=\"English\",C1069,IF($B$1=\"Deutsch\",D1069,IF($B$1=\"中文\",E1069,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- car batteries\nProduction\n- plastics, including compounding and conversion"},"Usage\n- car batteries\nProduction\n- plastics, including compounding and conversion","Verwendung\n- Platten/Elektroden von Autobatterien\nHerstellung:\n- Kunststoffprodukte, einschließlich Compoundierung und Konversion\n","使用\n-汽车电池\n生产\n- 塑料产品，包括混合和转换 "]
[null,{"$f":"IF($B$1=\"English\",C1070,IF($B$1=\"Deutsch\",D1070,IF($B$1=\"中文\",E1070,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- utilization of their ferroelectric properties\n- as pigments\n- semiconductor in machines, devices and mechanical appliances, also in electric and electronic products\nProduction\n- computers\n"},"Usage\n- utilization of their ferroelectric properties\n- as pigments\n- semiconductor in machines, devices and mechanical appliances, also in electric and electronic products\nProduction\n- computers\n","Verwendung\n- Ausnutzung ihrer ferroelektrischen Eigenschaften\n- als Pigmente\n- Halbleiter in Maschinen, Apparaten und mechanischen Geräten sowie elektrischen/elektronischen Erzeugnissen\nHerstellung\n- Computer\n","使用\n- 利用其铁电特性\n- 作为颜料\n- 半导体用在机器及机械器具，电气/电子产品\n生产\n- 电脑"]
[null,{"$f":"IF($B$1=\"English\",C1071,IF($B$1=\"Deutsch\",D1071,IF($B$1=\"中文\",E1071,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- laboratory reagent\n- intermediate\nProduction\n- fine chemicals\n- computers, electronic and optical products"},"Usage\n- laboratory reagent\n- intermediate\nProduction\n- fine chemicals\n- computers, electronic and optical products","Verwendung\n- Laborreagenz\n- Zwischenprodukt\nHerstellung \n- Feinchemikalien\n- Computern, elektronische und optische Produkten","使用\n- 实验室试剂\n- 中间产品\n生产\n- 精细化工\n- 电脑，电子及光学器件"]
[null,{"$f":"IF($B$1=\"English\",C1072,IF($B$1=\"Deutsch\",D1072,IF($B$1=\"中文\",E1072,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plastics used for wire and cables\n- plastics used for exterior construction\n- plastics use water pipes\n- plastics for mini-blinds\n- protection pipes and profiles for cables, gas pipes\n- lead enhanced plastic materials in inside parts of buildings\nHerstellung \n- plastic products, including compounding and conversion\n"},"Usage\n- plastics used for wire and cables\n- plastics used for exterior construction\n- plastics use water pipes\n- plastics for mini-blinds\n- protection pipes and profiles for cables, gas pipes\n- lead enhanced plastic materials in inside parts of buildings\nHerstellung \n- plastic products, including compounding and conversion\n","Verwendung\n- Kunststoffe für Drahte und Kabel\n- Kunsstoffe für den Außenbau\n- Kunsstoffe für Wasserleitungen\n- Kunsstoffe für Minirolläden\n- Schutzrohre und Profile für Kabel, Gasrohre\n- bleiverstärkte Kunststoffmaterialien in Gebäudeinnenteilen\nHerstellung \n- Kunststoffprodukten, einschließlich Compoundierung und Konversion\n","使用\n- 塑料用于电线电缆\n- 塑料用于建造外观\n- 塑胶用于水管\n- 塑胶用于迷你百叶窗\n- 管道保护和型材用于煤气管道管材和电缆\n- 铅强化的塑料材料在建筑内部零件生产\n- 塑料产品，包括混合和转换"]
[null,{"$f":"IF($B$1=\"English\",C1073,IF($B$1=\"Deutsch\",D1073,IF($B$1=\"中文\",E1073,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- additive in flame retardants, plastics/polymers and textiles\nflame retardants\n- electric and electronic devices\n- vehicles\n- textiles (e.g. upholstered furniture) \n- plastics (building industry)\n- types of plastics: HIPS, polyethylene, polypropylene, unsaturated polyesters und polybutylene terephthalate\n- plastics (mostly in high impact polystyrene) \n- binders \n- paints\n- varnishers \n- floor\n- covering materials\n- home- including mobile telephone equipment\n- textile applications\n- upholstery\n- cables\n- insulation materials\nProduction\n- printed circuit boards\n"},"Usage\n- additive in flame retardants, plastics/polymers and textiles\nflame retardants\n- electric and electronic devices\n- vehicles\n- textiles (e.g. upholstered furniture) \n- plastics (building industry)\n- types of plastics: HIPS, polyethylene, polypropylene, unsaturated polyesters und polybutylene terephthalate\n- plastics (mostly in high impact polystyrene) \n- binders \n- paints\n- varnishers \n- floor\n- covering materials\n- home- including mobile telephone equipment\n- textile applications\n- upholstery\n- cables\n- insulation materials\nProduction\n- printed circuit boards\n","Verwendung\n- Additiv in Flammschutzmitteln, Kunststoffen/Polymeren und Textilien\n- Flammschutzmittel\n- elektrische und elektronische Geräten\n- Fahrzeuge\n- Textilien (z.B. Polstermöbel) \n- Kunststoffe (der Baubranche)\n- Kunststofftypen: HIPS, Polyethylen, Polypropylen, ungesättigte Polyester und Polybutylenterephthalat\n- alle Polymer-Kunststoffklassen (vorallem schlagfestes Polystyren)\n- Bindemittel\n- Farben\n- Lacke\n- Fußboden\n- Abdeckmaterial\n- Heim- und Mobiltelefongeräte\n- textile Anwendungen\n- Polster\n- Kabel\n- Dämm- bzw. Isoliermaterial\nHerstellung\n- Leiterplatten","使用\n- 添加剂在阻燃剂，塑料/聚合物和纺织品中的阻燃剂\n- 电气和电子设备\n- 车辆\n- 纺织品（如软垫家具）\n- 塑料（建筑行业）\n-塑料类型：高抗冲聚苯乙烯，聚乙烯，聚丙烯，未饱和的聚酯和 聚对苯二甲酸丁二酯\n- 所有塑料聚合物的类型（主要是高冲击聚苯乙烯）\n- 装订\n- 颜色\n- 清漆\n- 地板\n- 覆盖材料\n- 家庭和移动设备\n- 纺织应用\n- 内饰\n- 电缆\n- 绝缘材料\n生产\n- 印刷电路板"]
[null,{"$f":"IF($B$1=\"English\",C1074,IF($B$1=\"Deutsch\",D1074,IF($B$1=\"中文\",E1074,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- high-boiling solvent\n- polar reaction medium\n- laboratory reagent\nIntermediate:\n- production of pesticides"},"Usage\n- high-boiling solvent\n- polar reaction medium\n- laboratory reagent\nIntermediate:\n- production of pesticides","Verwendung:\n- Hochsiedendes Lösungsmittel\n- polares Reaktionsmedium\n- Laborreagenz\nZwischenprodukt:\n- bei der Herstellung von Pestizide","使用\n- 高沸点溶剂\n- 极地反应介质\n- 实验室试剂\n中间产品\n- 农药制造"]
[null,{"$f":"IF($B$1=\"English\",C1075,IF($B$1=\"Deutsch\",D1075,IF($B$1=\"中文\",E1075,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plant protection\nProduction\n- plastic products\n- compounding and conversion\n- production of mass chemicals (including mineral oil products)\n- resins\n- adhesives\n- rubbers\n- polymers"},"Usage\n- plant protection\nProduction\n- plastic products\n- compounding and conversion\n- production of mass chemicals (including mineral oil products)\n- resins\n- adhesives\n- rubbers\n- polymers","Verwendung\n-Pflanzenschutz\nHerstellung:\n- Kunststoffprodukte\n- Compoundierung und Konversion\n- Herstellung von Massenchemikalien (einschließlich Mineralölprodukten)\n- Harze\n- Klebstoffe\n- Gummi\n- Polymere\n","使用\n-植物保护\n生产：\n- 塑料制品\n- 复利和转换\n- 生产的散装化学品（包括石油产品）\n- 树脂\n- 胶粘剂\n- 橡胶\n- 聚合物"]
[null,{"$f":"IF($B$1=\"English\",C1076,IF($B$1=\"Deutsch\",D1076,IF($B$1=\"中文\",E1076,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- synthesis chemicals\n- solvent for ester gum and some resins\n- solvent in various formulations like paints, inks, cleaning fluids\n- glycol ether, including hydraulic- and break fluids\n- antifreeze \n- chemical intermediates\n- diluent for cleaning agents"},"Usage\n- synthesis chemicals\n- solvent for ester gum and some resins\n- solvent in various formulations like paints, inks, cleaning fluids\n- glycol ether, including hydraulic- and break fluids\n- antifreeze \n- chemical intermediates\n- diluent for cleaning agents","Verwendung\n- Synthesechemikalie\n- Lösungsmittel für Estergummi und einige Harze\n- Lösungsmittel in verschiedenen Formulierungen wie (Anstrich-)Farben, Tinten, Reinigungsflüssigkeiten\n- Glykolether, einschließlich Hydraulik- und Bremsflüssigkeiten\n- Frostschutzmittel\n- chemische Zwischenprodukte\n- Verdünnungsmittel für Reinigungsmittel\n","使用\n- 化学合成\n- 溶剂用于酯胶及一些树脂\n-溶剂用于各种剂型，如（油漆）的颜色，油墨，清洁剂\n- 乙二醇醚，包括液压和制动液\n- 防冻液\n- 化工中间产品\n- 稀释剂用于清洁剂"]
[null,{"$f":"IF($B$1=\"English\",C1077,IF($B$1=\"Deutsch\",D1077,IF($B$1=\"中文\",E1077,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plastic products\n- electric batteries and accumulators\n- weight\n- preparation of boiled (linseed) oil\n- colorless paint\n- PVC stabilizer\n- activator for azodicarbonamide Treibmittel for vinyl foams\nProduction\n- red lead\n- PVC"},"Usage\n- plastic products\n- electric batteries and accumulators\n- weight\n- preparation of boiled (linseed) oil\n- colorless paint\n- PVC stabilizer\n- activator for azodicarbonamide Treibmittel for vinyl foams\nProduction\n- red lead\n- PVC","Verwendung\n- Kunststofferzeugnisse\n- elektrische Batterien und Akkumulatoren\n- Beschwerung\n- Bereitung von Leinölfirnis\n- farblose Malerfarbe\n- PVC-Stabilisator\n- Aktivator für Azodicarbonamid Treibmittel für Vinyl-Schäume\nHerstellung\n- Mennige\n- PVC","使用\n- 塑料制品\n- 电池和蓄电池\n- 秤\n-（亚麻籽）油的准备\n- 无色画家的色彩\n- PVC稳定剂\n- 活化剂为乙烯泡沫偶氮二甲酰胺发泡剂\n生产\n- 铅丹\n- PVC"]
[null,{"$f":"IF($B$1=\"English\",C1078,IF($B$1=\"Deutsch\",D1078,IF($B$1=\"中文\",E1078,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plasticisers in plastic material"},"Usage\n- plasticisers in plastic material","Verwendung:\n- Weichmacher in Kunststoffen","使用\n- 塑料材料的塑化剂"]
[null,{"$f":"IF($B$1=\"English\",C1079,IF($B$1=\"Deutsch\",D1079,IF($B$1=\"中文\",E1079,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n-plastics for wire and cables\n-plastics for exterior construction\n-plastics water pipes\n-plastics mini-blinds\n-protection pipes and profiles for cables\n-gas pipes\n- lead enhanced plastic materials in inner parts of buildings\nProduction \n- plastics\n- compounding and conversion"},"Usage\n-plastics for wire and cables\n-plastics for exterior construction\n-plastics water pipes\n-plastics mini-blinds\n-protection pipes and profiles for cables\n-gas pipes\n- lead enhanced plastic materials in inner parts of buildings\nProduction \n- plastics\n- compounding and conversion","Verwendung\n- Kunstoffe für Leitungen und Kabel\n- Kunsstoffe für den Außenbau\n- Kunsstoffe für Wasserleitungen\n- Kunststoffe für Minirolläden\n- Schutzleitungen und Profile für Kabel\n- Gasleitungen\n- bleiverstärkte Kunststoffmaterialien in Gebäudeinnenteilen\nHerstellung \n- Kunststoffprodukten\n- Compoundierung und Konversion","使用\n- 电线电缆用塑料\n- 建造外观用塑料\n- 塑料水管\n- 塑料的迷你百叶窗\n- 电缆的保护套管和型材\n- 煤气管道\n-建筑内部零件的铅强化的塑料材料\n生产\n-塑料产品\n-化合和转换"]
[null,{"$f":"IF($B$1=\"English\",C1080,IF($B$1=\"Deutsch\",D1080,IF($B$1=\"中文\",E1080,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- fuel additives and fuel mixtures\n- anti-knock additive in gasoline\n- gasoline\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers\n"},"Usage\n- fuel additives and fuel mixtures\n- anti-knock additive in gasoline\n- gasoline\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers\n","Verwendung\n- Kraftstoffzusätze und Kraftstoffmischungen\n- Antiklopfmittel \n- Benzin\n- Zusatzstoff und Komponente in Verbraucher- und Industrieprodukten\nHerstellung\n- Fluorpolymer\n- Fluortelomer","使用\n- 燃油添加剂和混合燃料\n- 抗爆\n- 汽油\n- 添加剂以及消费者和工业产品组件\n生产\n- 含氟聚合物\n- 氟调聚物"]
[null,{"$f":"IF($B$1=\"English\",C1081,IF($B$1=\"Deutsch\",D1081,IF($B$1=\"中文\",E1081,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- electric batteries and accumulators\n- lead enhanced plastic materials in inner parts of buildings\nProduction\n- plastic material"},"Usage\n- electric batteries and accumulators\n- lead enhanced plastic materials in inner parts of buildings\nProduction\n- plastic material","Verwendung\n- elektrische Batterien und Akkumulatoren\n- bleiverstärkte Kunststoffmaterialien in Gebäudeinnenteilen\nHerstellung\n- Kunststoffprodukte","使用\n- 电池和蓄电池\n- 铅 - 钢材料在建筑内部零件\n生产\n- 塑料制品"]
[null,{"$f":"IF($B$1=\"English\",C1082,IF($B$1=\"Deutsch\",D1082,IF($B$1=\"中文\",E1082,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plasticizer in PVC\n- sealants\n- print color\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers"},"Usage\n- plasticizer in PVC\n- sealants\n- print color\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers","Verwendung\n- Weichmacher in PVC\n- Dichtungsmittel\n- Druckfarben\n- Zusatzstoff und Komponente in Verbraucher- und Industrieprodukten\nHerstellung\n- Fluoropolymere\n- Fluorotelomere","使用\n- PVC软化剂\n- 密封胶\n- 印刷油墨\n- 添加剂以及消费者和工业产品组件\n生产\n-  氟化聚合物\n- 氟调聚物"]
[null,{"$f":"IF($B$1=\"English\",C1083,IF($B$1=\"Deutsch\",D1083,IF($B$1=\"中文\",E1083,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers"},"Usage\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers","Verwendung\n- Zusatzstoff und Komponente in Verbraucher- und Industrieprodukten\nHerstellung\n- fluorierten Polymere\n- fluorierten Telomere\n","使用\n- 消费品和工业产品中的添加剂和组件\n生产\n- 氟化聚合物\n- 氟调聚物"]
[null,{"$f":"IF($B$1=\"English\",C1084,IF($B$1=\"Deutsch\",D1084,IF($B$1=\"中文\",E1084,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers\n\n"},"Usage\n- additives and components in consumer and industrial products\nProduction\n- fluoropolymers\n- fluorotelomers\n\n","Verwendung\n- Zusatzstoff und Komponente in Verbraucher- und Industrieprodukten\nHerstellung\n- fluorierte Polymere\n- fluorierte Telomere\n","使用\n- 消费品和工业产品中的添加剂和组件\n生产\n- 氟化聚合物\n- 氟调聚物"]
[null,{"$f":"IF($B$1=\"English\",C1085,IF($B$1=\"Deutsch\",D1085,IF($B$1=\"中文\",E1085,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- alkylating agents\n- industrial solvent for vapour degreasing\nProduction\n- mass chemicals (including mineral oil products)\n- Grignard compounds\n- local anaesthetics, acaricides, fungicides\n- aerosols\n- textiles\n- adhesives\n- inks\n- coatings"},"Usage\n- alkylating agents\n- industrial solvent for vapour degreasing\nProduction\n- mass chemicals (including mineral oil products)\n- Grignard compounds\n- local anaesthetics, acaricides, fungicides\n- aerosols\n- textiles\n- adhesives\n- inks\n- coatings","Verwendung:\n-Alkylierungsmittel\n- industrielles Lösemittel für Dampfentfettung\nHerstellung \n- Massenchemikalien (einschließlich Mineralölprodukten)\n- Grignard-Verbindungen\n- Lokal-Anästhetika, Akarizide, Fungizide\n- Aerosole\n- Textilien\n- Kleber\n- Tinte\n- Beschichtung","使用\n- 烷化剂\n- 工业溶剂蒸气脱脂\n生产\n- 散装化学品（包括石油产品）\n- 格氏化合物\n- 局部麻醉剂，杀螨剂，杀真菌剂\n- 气雾剂\n- 纺织品\n- 胶\n- 墨水\n- 涂层"]
[null,{"$f":"IF($B$1=\"English\",C1086,IF($B$1=\"Deutsch\",D1086,IF($B$1=\"中文\",E1086,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- disinfection agent (for private purposes)\n- corrosive decalcifying agent, including products for ovens and stoves\n- disinfection agent used on surfaces which are in contact with food\n- industrial detergent for ultra filtration membranes or reverse osmosis\n- detergent for floors, walls in industrial sector\n- detergent for wheels and tires\n- pH-regulator\n- anticorrosive\n- additives for engine fuels\n- bleach for casings\n- cationic electrocoating\n- etching liquid\n- pesticide\n- service to buildings and landscape activities\n- category cleaning/washing agents\n- specialized construction activities\n- trade and repair of motor vehicles\nProduction\n- chemicals and chemicals products\n- cleaning/washing agents\n- food products\n- fabricated metal product\n- base chemical for biocides"},"Usage\n- disinfection agent (for private purposes)\n- corrosive decalcifying agent, including products for ovens and stoves\n- disinfection agent used on surfaces which are in contact with food\n- industrial detergent for ultra filtration membranes or reverse osmosis\n- detergent for floors, walls in industrial sector\n- detergent for wheels and tires\n- pH-regulator\n- anticorrosive\n- additives for engine fuels\n- bleach for casings\n- cationic electrocoating\n- etching liquid\n- pesticide\n- service to buildings and landscape activities\n- category cleaning/washing agents\n- specialized construction activities\n- trade and repair of motor vehicles\nProduction\n- chemicals and chemicals products\n- cleaning/washing agents\n- food products\n- fabricated metal product\n- base chemical for biocides","Verwendung\n- Desinfektionsmittel (für private Zwecke)\n- korrosive Entkalkungsmittel einschließlich Produkte für Öfen und Herde\n- Desinfektionsmittel zur Verwendung auf Oberflächen im Kontakt mit Lebensmitteln\n- industrielles Reinigungsmittel für Ultrafiltrationsmembranen oder Umkehrosmose\n- Reinigungsmittel für Böden und Wände im industriellen Bereich\n- Reinigungsmittel für Räder und Reifen\n- pH-Regulator\n- Korrosionsschutzmittel\n- Zusatzstoffe für Motorenkraftstoffe\n- Bleichmittel für Gehäuse\n- kationische Elektrobeschichtung\n- Ätzflüssigkeiten\n- Schädlingsbekämpfungsmittel\n- Gebäudeinstandhaltung und Landschaftsaktivitäten\n- Reinigungs- und Waschmittel\n- spezielle Bauaktivitäten\n- Handel und Reperatur von Motorfahrzeugen\nHerstellung\n- Chemikalien und chemische Produkte\n- Reinigungs oder Waschmittel\n- Nahrungsmittel(produkte)\n- Metallerzeugnisse\n- Basischemikalie bei Bioziden\n\n\n\n\n\n","用法\n- 消毒剂（用于私人用途）\n- 腐蚀脱钙剂，包括产品的烤箱和火炉\n- 消毒剂用于表面直接与食品接触\n- 工业清洁剂用于超滤或反渗透膜\n- 清洁剂用于地板和墙壁在工业部门\n- 洗涤剂的轮毂和轮胎\n- PH调节剂\n- 防腐蚀剂\n- 添加剂用于发动机燃料\n- 漂白剂用于房屋\n- 阳离子电涂料\n- 蚀刻剂\n- 农药\n- 建筑和景观活动的维护\n- 清洁，洗涤\n- 特殊建筑项目\n- 汽车贸易及维修\n生产\n- 化学品及化学产品\n- 清洁或清洁剂\n- 食品（产品）\n- 金属\n- 基本化学用于杀菌剂"]
[null,{"$f":"IF($B$1=\"English\",C1087,IF($B$1=\"Deutsch\",D1087,IF($B$1=\"中文\",E1087,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- dyes\n- isocyanates for polyurethane production\n- urethanes, which are base for polyurethane plastics \n- smaller amounts are generated during synthesis of industry dyes\n- impact resins\n- polyimides with superior wire coating properties\nIntermediate\n- production of sulfur dye"},"Usage\n- dyes\n- isocyanates for polyurethane production\n- urethanes, which are base for polyurethane plastics \n- smaller amounts are generated during synthesis of industry dyes\n- impact resins\n- polyimides with superior wire coating properties\nIntermediate\n- production of sulfur dye","Herstellung\n- Farbstoffen \n- Isocyanate für Polyurethan-Herstellung\n- Urethane, die Grundlage für Polyurethan-Kunststoffe sind\n- Kleinere Mengen werden bei der Synthese von Industrie-Farbstoffen gebildet\n- Harze\n- Polyimide mit überlegener Drahtbeschichtung Eigenschaften\nZwischenprodukt\n- Herstellung von Schwefelfarbstoffen","生产\n- 染料\n- 异氰酸酯用于聚氨酯的生产\n- 氨基甲酸乙酯，它是依据聚氨酯塑料\n- 较小的量被做成在工业染料的合成时\n- 树脂\n- 聚酰亚胺具有超强的金属丝涂层性能\n中间产品\n- 硫化染料的生产"]
[null,{"$f":"IF($B$1=\"English\",C1088,IF($B$1=\"Deutsch\",D1088,IF($B$1=\"中文\",E1088,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- cellulose modifier\n- in coatings\n- lubricants\n- as fuel\n- agrochemical use\n- detergents\n- de-icer agent and antifreeze \n- functional fluids\n- chemicals for water treatment\nProduction\n- propylene glycol and dipropylene glycol\n- propylene glycol ether and isopropanolamines\n- washing agent\nIntermediate\n- production of propylene oxide"},"Usage\n- cellulose modifier\n- in coatings\n- lubricants\n- as fuel\n- agrochemical use\n- detergents\n- de-icer agent and antifreeze \n- functional fluids\n- chemicals for water treatment\nProduction\n- propylene glycol and dipropylene glycol\n- propylene glycol ether and isopropanolamines\n- washing agent\nIntermediate\n- production of propylene oxide","Verwendung\n- Zellulose-Modifikator\n- in Beschichtungen\n- Schmiermittel\n- als Kraftstoff\n- Agrochemische Verwendung\n- Reinigungsmittel\n- Enteisungs- und Frostschutzmittel\n- Funktionsflüssigkeit\n- Chemikalien zur Wasserbehandlung\nHerstellung\n- Propylenglycol und Dipropylenglycol\n- Propylenglycolether und Isopropanolamine\n- Waschmittel\nZwischenprodukt\n- Herstellung von Propylenoxid\n","使用\n- 纤维素改性剂\n- 在涂料\n- 润滑剂\n- 作为燃料\n- 农药使用\n- 清洁用品\n- 防冰和防冻\n- 功能液\n-化学品用于水处理\n生产\n- 丙二醇和一缩二丙二醇\n- 丙二醇和异丙醇胺\n- 洗涤剂\n中间产品\n- 环氧丙烷的生产"]
[null,{"$f":"IF($B$1=\"English\",C1089,IF($B$1=\"Deutsch\",D1089,IF($B$1=\"中文\",E1089,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plastic products\nProduction\n- PVC"},"Usage\n- plastic products\nProduction\n- PVC","Verwendung\n- Kunststofferzeugnisse\nHerstellung\n- PVC","使用\n- 塑料产品的生产\n- 聚氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C1090,IF($B$1=\"Deutsch\",D1090,IF($B$1=\"中文\",E1090,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production\n- dyes"},"Production\n- dyes","Herstellung:\n- Farbstoffe","制作：\n- 染料"]
[null,{"$f":"IF($B$1=\"English\",C1091,IF($B$1=\"Deutsch\",D1091,IF($B$1=\"中文\",E1091,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- plasticisers in plastic material\n- laboratory chemicals for analytical purposes\nProduction\n- dyes"},"Usage\n- plasticisers in plastic material\n- laboratory chemicals for analytical purposes\nProduction\n- dyes","Verwendung\n- Weichmacher in Kunststoff(material)\n- Laborchemikalie für analytische Zwecke\nHerstellung:\nFarbstoffe","使用\n- 塑料增塑剂（材料）\n- 实验室用于化学分析为目的制作：\n- 染料"]
[null,{"$f":"IF($B$1=\"English\",C1092,IF($B$1=\"Deutsch\",D1092,IF($B$1=\"中文\",E1092,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- temperature-resistant properties \n- wire enamels\n- coatings \n- film\n- adhesives\n- insulating varnishes\n- coated fabrics\n- flame-retardant fibers \n- oil sealants and retainers\n- insulation for cables and printed circuits\n- laminates and composite for aerospace vehicles\n- Intermediate\nProduction\n- polymer resins\n- production of polyamide and poly(ester)imide resins\n"},"Usage\n- temperature-resistant properties \n- wire enamels\n- coatings \n- film\n- adhesives\n- insulating varnishes\n- coated fabrics\n- flame-retardant fibers \n- oil sealants and retainers\n- insulation for cables and printed circuits\n- laminates and composite for aerospace vehicles\n- Intermediate\nProduction\n- polymer resins\n- production of polyamide and poly(ester)imide resins\n","Verwendung\n- temperaturbeständige Eigenschaften\n- Drahtlack\n- Beschichtungen\n- Filme\n- Klebstoffe\n- Isolierlacke\n- beschichtete Gewebe\n- flammhemmende Fasern\n- Öldichtungen und -halter/-auffänger\n- Isolation für Kabel und Leiterplatten\n- Hartgewebe? und Gemische?/Verbundwerkstoffe? für Luft- und Raumfahrzeuge\n- Zwischenprodukt\nHerstellung\n- Polymerharze\n- Herstellung von Polyamid und Poly(ester)imidharze\n\n\n\n","使用\n- 耐温性能\n- 丝珐琅\n- 涂料\n- 电影\n- 胶粘剂\n- 绝缘\n- 涂层织物\n- 耐火纤维\n- 油封和-夹具/-接受器\n- 绝缘电缆和印刷电路板\n- 航天器的层压板和复合材料\n- 中间产品\n生产\n- 高分子树脂\n- 生产聚酰胺，和聚（酯基）亚胺"]
[null,{"$f":"IF($B$1=\"English\",C1093,IF($B$1=\"Deutsch\",D1093,IF($B$1=\"中文\",E1093,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n-pyrotechnics, dye synthesis, organic elementary analysis, porcelain- and glass painting\n- ceramic, flint glass, varnishes, glass- and metal putty, ointments and lead plasters\n- pigment\n- anti-rust paint\n- medicine plaster\n- repair of television sets, computer monitors and other devices with cathode ray tubes\n- in adsorbents, colors and pigments\n- positive battery plates\n- electrically conductive polymer\nProduction\n- anticorrosive primary coat for steel, lead soaps, accumulators, activators for rubber, matches\n- lead acid batteries\n- crystall glass and ceramic\n- rubber protection\n- explosive"},"Usage\n-pyrotechnics, dye synthesis, organic elementary analysis, porcelain- and glass painting\n- ceramic, flint glass, varnishes, glass- and metal putty, ointments and lead plasters\n- pigment\n- anti-rust paint\n- medicine plaster\n- repair of television sets, computer monitors and other devices with cathode ray tubes\n- in adsorbents, colors and pigments\n- positive battery plates\n- electrically conductive polymer\nProduction\n- anticorrosive primary coat for steel, lead soaps, accumulators, activators for rubber, matches\n- lead acid batteries\n- crystall glass and ceramic\n- rubber protection\n- explosive","Verwendung\n-Feuerwerkerei, Farbstoff-Synthese, organischen Elementaranalyse, Porzellan- und Glasmalerei\n-Keramik, Flintglas, Firnissen, Glas- u. Metallkitten, Salben und Bleipflastern\n-Pigment\n-Rostschutzfarbe\n-Arzneipflaster\n- Reparatur von Fernsehgeräten, Computermonitoren und anderen Geräten mit Kathodenstrahlröhren\n- in Adsorptionsmitteln, Farben und Pigmenten\n- Batterien\n- elektrisch leitendes Polymer\nHerstellung\n-Korrosionsschutz-Grundanstrichen für Stahl, Bleiseifen, Akkumulatoren, Aktivatoren für Kautschuk, Zündhölzer\n- Blei-Säure-Batterien\n- Kristallglas und Keramik\n- Gummischutz\n- Sprengstoff","使用\n- 烟火，染料合成，有机元素分析，瓷器和玻璃画\n-陶器，火石玻璃，油漆，玻璃和金属固井，药膏和膏药引起\n-色素\n- 防锈颜料\n- 贴剂\n- 电视，电脑显示器和其他设备含有阴极射线管的维修\n- 在吸附剂，染料和颜料\n- 电池\n- 导电聚合物\n生产\n- 防腐蚀涂料用于钢铁，铅皂，电池，活化剂适用于橡胶，火柴\n- 铅酸电池\n- 水晶玻璃和陶瓷\n- 橡胶保护\n- 炸药"]
[null,{"$f":"IF($B$1=\"English\",C1094,IF($B$1=\"Deutsch\",D1094,IF($B$1=\"中文\",E1094,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- rubber antioxidant\n- textile- or leather products\nIntermediate\n- production of azo dyes"},"Usage\n- rubber antioxidant\n- textile- or leather products\nIntermediate\n- production of azo dyes","Verwendung\n- Gummi-Antioxidans\n- Textilien oder Ledererzeugnissen\nZwischenprodukt\n- Herstellung von Azofarbstoffen","使用\n- 橡胶防老剂\n- 纺织品或皮革制品\n中间产品\n- 偶氮染料的生产"]
[null,{"$f":"IF($B$1=\"English\",C1095,IF($B$1=\"Deutsch\",D1095,IF($B$1=\"中文\",E1095,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- as plasticiser for PVC products and other polymers \n- used in many PVC formulations, principally for ease of gelation used in conjunction with higher molecular mass esters\n- similar manner\n- plasticizer and surface conditioner in fuels\n- plasticizer for plastics"},"Usage\n- as plasticiser for PVC products and other polymers \n- used in many PVC formulations, principally for ease of gelation used in conjunction with higher molecular mass esters\n- similar manner\n- plasticizer and surface conditioner in fuels\n- plasticizer for plastics","Verwendung\n- als Weichmacher für PVC-Produkte und andere Polymere\n- wird in vielen PVC-Formulierungen verwendet, vorwiegend um die Vergelung zusammen mit Hochmolekularmasse-Estern zu erleichtern\n- ähnliche Methoden\n- Weichmacher und Oberflächenkonditionierer in Treibstoffen\n- Weichmacher für Kunststoffe","使用\n- 软化剂用于PVC产品及其他聚合物，\n- 用于许多PVC配方，主要是在高分子量酯类的粘结中容易形成凝胶\n- 类似的方法\n- 软化和表面调节器在燃料中\n- 软化剂用于塑料"]
[null,{"$f":"IF($B$1=\"English\",C1096,IF($B$1=\"Deutsch\",D1096,IF($B$1=\"中文\",E1096,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- household detergents and cleaning products \n- lead enhanced plastic materials in inner parts of buildings\nProduction\n- plastic products, including compunding and conversion"},"Usage\n- household detergents and cleaning products \n- lead enhanced plastic materials in inner parts of buildings\nProduction\n- plastic products, including compunding and conversion","Verwendung\n- Waschmittel (im Haushalt) und Reinigungsmittel \n- bleiverstärkte Kunststoffmaterialien in Gebäudeinnenteilen\nHerstellung\n- Kunststoffprodukte, einschließlich Compoundierung und Konversion","使用\n- 洗涤剂（家居）和清洁产品\n- 铅 - 塑料材料用于建筑内部零件\n生产\n- 塑料产品，包括化合和转换"]
[null,{"$f":"IF($B$1=\"English\",C1097,IF($B$1=\"Deutsch\",D1097,IF($B$1=\"中文\",E1097,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- blowing agent for foaming thermoplastics and elastomers\n- blowing agent in the rubber and plastics industry\n- expansion agent\n- aging- and bleaching agent\n- foaming agent\n- catalyst\n- insulation material\n- building material\n- cement filler\n- dye\n- additive\n- bleaching agent in photography\n\n"},"Usage\n- blowing agent for foaming thermoplastics and elastomers\n- blowing agent in the rubber and plastics industry\n- expansion agent\n- aging- and bleaching agent\n- foaming agent\n- catalyst\n- insulation material\n- building material\n- cement filler\n- dye\n- additive\n- bleaching agent in photography\n\n","Verwendung\n- Treibmittel zum Verschäumen von Thermoplasten und Elastomeren\n- Blähmittel in der Gummi- und Kunststoffindustrie\n- Blähmittel\n- Alterungs- und Bleichmittel\n- Schäumungsmittel\n- Katalysator\n- Isoliermaterial\n- Baumaterial\n- Zementfüller\n- Farbstoff\n- Zusatzstoff\n- Bleichmittel bei der Fotografie","使用\n- 吹发泡热塑性剂和弹性体\n- 发泡剂在橡胶和塑料工业\n- 发泡剂\n- 老化剂和漂白剂\n- 泡沫\n- 催化剂\n- 隔离材料\n- 建筑材料\n- 水泥填料\n- 颜料\n- 补充料\n- 漂白剂在照相时"]
[null,{"$f":"IF($B$1=\"English\",C1098,IF($B$1=\"Deutsch\",D1098,IF($B$1=\"中文\",E1098,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage\n- lead enhanced plastic material in inner parts of buildings\nProduction\n- PVC"},"Usage\n- lead enhanced plastic material in inner parts of buildings\nProduction\n- PVC","Verwendung\n- bleiverstärkte Kunststoffmaterialien in Gebäudeinnenteilen\nHerstellung\n- PVC\n","使用\n- 铅 - 塑料材料在建筑内部零件\n生产\n- 聚氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C1099,IF($B$1=\"Deutsch\",D1099,IF($B$1=\"中文\",E1099,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Usage:\n- anticorrosive pigment"},"Usage:\n- anticorrosive pigment","Verwendung\n- Korrisionsschutzpigment","使用\n- 防腐颜料"]
[null,{"$f":"IF($B$1=\"English\",C1100,IF($B$1=\"Deutsch\",D1100,IF($B$1=\"中文\",E1100,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"biocide in packaging"},"biocide in packaging","Biozid in Verpackungen","生物杀灭剂在包装"]
[null,{"$f":"IF($B$1=\"English\",C1101,IF($B$1=\"Deutsch\",D1101,IF($B$1=\"中文\",E1101,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Catalyst for PU production remains in the product, eg seals, encapsulation of electronic components, vibration dampes, shoe soles\n- corrosive"},"- Catalyst for PU production remains in the product, eg seals, encapsulation of electronic components, vibration dampes, shoe soles\n- corrosive","- Katalysator bei PU Herstellung, verbleibt im Produkt, z.B. Dichtungen, Kapselung von elektronischen Bauteilen, Schwingungsdämpfer, Schuhsolen\n- Beizmittel","‘- 在聚氨酯生产时的催化剂，残留在产品中，例如电子元件，减震器和鞋底的密封，封装\n- 媒染剂"]
[null,{"$f":"IF($B$1=\"English\",C1102,IF($B$1=\"Deutsch\",D1102,IF($B$1=\"中文\",E1102,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- costume jewelery\n- children jewelery"},"- costume jewelery\n- children jewelery","- Mode-Schmuck\n- Kinder-Schmuck","- 时尚饰品\n- 儿童珠宝"]
[null,{"$f":"IF($B$1=\"English\",C1103,IF($B$1=\"Deutsch\",D1103,IF($B$1=\"中文\",E1103,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"manufacturing plastic"},"manufacturing plastic","Kunststoff-Herstellung","塑料制造"]
[null,{"$f":"IF($B$1=\"English\",C1104,IF($B$1=\"Deutsch\",D1104,IF($B$1=\"中文\",E1104,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Annex XIV  \"List of substances subject to authorisation\""},"Annex XIV  \"List of substances subject to authorisation\"","Anhang XIV \"Verzeichnis der zulassungspflichtigen Stoffe\"","\n附件14 “需要授权的物质清单”"]
[null,{"$f":"IF($B$1=\"English\",C1105,IF($B$1=\"Deutsch\",D1105,IF($B$1=\"中文\",E1105,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorine (Cl)"},"Chlorine (Cl)","Chlor (Cl)","氯（Cl）"]
[null,{"$f":"IF($B$1=\"English\",C1106,IF($B$1=\"Deutsch\",D1106,IF($B$1=\"中文\",E1106,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bromine (Br)"},"Bromine (Br)","Brom (Br)","溴（Br）"]
[null,{"$f":"IF($B$1=\"English\",C1107,IF($B$1=\"Deutsch\",D1107,IF($B$1=\"中文\",E1107,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Br in PCB Laminates"},"Br in PCB Laminates","Br in PCB Beschichtung","\n印刷电路板涂层中的溴"]
[null,{"$f":"IF($B$1=\"English\",C1108,IF($B$1=\"Deutsch\",D1108,IF($B$1=\"中文\",E1108,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cl in PCB Laminates"},"Cl in PCB Laminates","Cl in PCB Beschichtung","\n印刷电路板涂层中的氯"]
[null,{"$f":"IF($B$1=\"English\",C1109,IF($B$1=\"Deutsch\",D1109,IF($B$1=\"中文\",E1109,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Br in Brominated Flame Retardants"},"Br in Brominated Flame Retardants","Br in bromierten Flammschutzmittel","溴化阻燃剂中的溴"]
[null,{"$f":"IF($B$1=\"English\",C1110,IF($B$1=\"Deutsch\",D1110,IF($B$1=\"中文\",E1110,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cl in Chlorinated Flame Retardants"},"Cl in Chlorinated Flame Retardants","Halogenarm, Br in chlorierten Flammschutzmittel","氯化阻燃剂中的氯"]
[null,{"$f":"IF($B$1=\"English\",C1111,IF($B$1=\"Deutsch\",D1111,IF($B$1=\"中文\",E1111,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-substituted organostannic compounds (tributyl tin or triphenyl tin compounds)"},"Tri-substituted organostannic compounds (tributyl tin or triphenyl tin compounds)","Trisubstituierte zinnorganische Verbindungen (Tributylzinn oder Triphenylzinn und Verbindungen","三取代有机锡化合物（三丁基锡和三苯基锡和化合物）"]
[null,{"$f":"IF($B$1=\"English\",C1112,IF($B$1=\"Deutsch\",D1112,IF($B$1=\"中文\",E1112,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol,2-(2H-benzotriazol-2-yl)-4,6-bis(1,1-dimethylethyl)"},"Phenol,2-(2H-benzotriazol-2-yl)-4,6-bis(1,1-dimethylethyl)","Phenol,2-(2H-benzotriazol-2-yl)-4,6-bis(1,1-dimethylethyl)","苯酚, 2-(2H-苯并三唑-2-基)-4,6-二(1,1-二甲基乙基)"]
[null,{"$f":"IF($B$1=\"English\",C1113,IF($B$1=\"Deutsch\",D1113,IF($B$1=\"中文\",E1113,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Antimony (Sb) and its compounds"},"Antimony (Sb) and its compounds","Antimon (Sb) und ihre Komponenten","锑（Sb），和它的组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1114,IF($B$1=\"Deutsch\",D1114,IF($B$1=\"中文\",E1114,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Red phosphorus and its compounds"},"Red phosphorus and its compounds","Roter Phosphor und ihre Komponenten","红磷和它的组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1115,IF($B$1=\"Deutsch\",D1115,IF($B$1=\"中文\",E1115,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beryllium and its compounds"},"Beryllium and its compounds","Beryllium und ihre Komponenten","\n铍及其组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1116,IF($B$1=\"Deutsch\",D1116,IF($B$1=\"中文\",E1116,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Selenium and its compounds"},"Selenium and its compounds","Selen und ihre Komponenten","硒及其组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1117,IF($B$1=\"Deutsch\",D1117,IF($B$1=\"中文\",E1117,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bismuth and its compounds"},"Bismuth and its compounds","Bismut und ihre Komponenten","铋及其组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1118,IF($B$1=\"Deutsch\",D1118,IF($B$1=\"中文\",E1118,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Halogenated dioxins and furans"},"Halogenated dioxins and furans","Halogenisierten Dioxine und Furane","卤化二恶英和呋喃"]
[null,{"$f":"IF($B$1=\"English\",C1119,IF($B$1=\"Deutsch\",D1119,IF($B$1=\"中文\",E1119,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(2-chloroethyl) phosphate (TCEP)"},"Tris(2-chloroethyl) phosphate (TCEP)","Tris(2-chlorethyl)phosphat\n","磷酸三(2-氯乙基)酯"]
[null,{"$f":"IF($B$1=\"English\",C1120,IF($B$1=\"Deutsch\",D1120,IF($B$1=\"中文\",E1120,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polyvinyl Chloride (PVC) "},"Polyvinyl Chloride (PVC) ","Polyvinylchlorid (PVC)","聚氯乙烯（PVC）"]
[null,{"$f":"IF($B$1=\"English\",C1121,IF($B$1=\"Deutsch\",D1121,IF($B$1=\"中文\",E1121,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfur hexafluoride"},"Sulfur hexafluoride","Schwefelhexafluorid","六氟化硫"]
[null,{"$f":"IF($B$1=\"English\",C1122,IF($B$1=\"Deutsch\",D1122,IF($B$1=\"中文\",E1122,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorocarbons"},"Perfluorocarbons","perfluorierte Kohlenwasserstoffe (FKW) ","全氟碳水化合物"]
[null,{"$f":"IF($B$1=\"English\",C1123,IF($B$1=\"Deutsch\",D1123,IF($B$1=\"中文\",E1123,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tellurium and its compounds "},"Tellurium and its compounds ","Tellur und ihre Komponenten","碲及其组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1124,IF($B$1=\"Deutsch\",D1124,IF($B$1=\"中文\",E1124,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetramethylthiuram disulfide (Thiram)"},"Tetramethylthiuram disulfide (Thiram)","Tetramethylthiuram Disulfide (Thiram)","促进剂 T"]
[null,{"$f":"IF($B$1=\"English\",C1125,IF($B$1=\"Deutsch\",D1125,IF($B$1=\"中文\",E1125,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Barium compounds"},"Barium compounds","Barium und ihre Komponenten","钡及其组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1126,IF($B$1=\"Deutsch\",D1126,IF($B$1=\"中文\",E1126,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tantalum (Ta) "},"Tantalum (Ta) ","Tantal (Ta)","钽（Ta）"]
[null,{"$f":"IF($B$1=\"English\",C1127,IF($B$1=\"Deutsch\",D1127,IF($B$1=\"中文\",E1127,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tin (Sn) "},"Tin (Sn) ","Zinn (Sn)","锡（Sn）"]
[null,{"$f":"IF($B$1=\"English\",C1128,IF($B$1=\"Deutsch\",D1128,IF($B$1=\"中文\",E1128,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gold (Au) "},"Gold (Au) ","Gold (Au)","金（Au）"]
[null,{"$f":"IF($B$1=\"English\",C1129,IF($B$1=\"Deutsch\",D1129,IF($B$1=\"中文\",E1129,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tungsten (W) "},"Tungsten (W) ","Wolfram (W)","钨（W）"]
[null,{"$f":"IF($B$1=\"English\",C1130,IF($B$1=\"Deutsch\",D1130,IF($B$1=\"中文\",E1130,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluorine (F)"},"Fluorine (F)","Fluor (F)","\n氟（F）"]
[null,{"$f":"IF($B$1=\"English\",C1131,IF($B$1=\"Deutsch\",D1131,IF($B$1=\"中文\",E1131,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodine (I)"},"Iodine (I)","Jod (I)","碘（I）"]
[null,{"$f":"IF($B$1=\"English\",C1132,IF($B$1=\"Deutsch\",D1132,IF($B$1=\"中文\",E1132,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibition on use"},"Prohibition on use","Verwendungsverbot","禁止使用"]
[null,{"$f":"IF($B$1=\"English\",C1133,IF($B$1=\"Deutsch\",D1133,IF($B$1=\"中文\",E1133,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PAH"},"PAH","PAK","PAH（多环芳烃）"]
[null,{"$f":"IF($B$1=\"English\",C1134,IF($B$1=\"Deutsch\",D1134,IF($B$1=\"中文\",E1134,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polycyclical aromatic hydrocarbons"},"Polycyclical aromatic hydrocarbons","Polyzyklische aromatische Kohlenwasserstoffe","多环芳烃"]
[null,{"$f":"IF($B$1=\"English\",C1135,IF($B$1=\"Deutsch\",D1135,IF($B$1=\"中文\",E1135,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"formed e.g. during incomplete combustion of organic substances. Occurrence in e.g. mineral oil, bitumen, pitch, tar, carbon black and products made therefrom"},"formed e.g. during incomplete combustion of organic substances. Occurrence in e.g. mineral oil, bitumen, pitch, tar, carbon black and products made therefrom","entstehen u.a. bei unvollständiger Verbrennung organischer Stoffe. Vorkommen in z.B. Mineralölen, Bitumen, Pech, Teer, Ruß und daraus hergestellten Produkten","出现在有机物质的不完全燃烧时。例如在矿物油，沥青，沥青，焦油，烟灰和由其生产的产品"]
[null,{"$f":"IF($B$1=\"English\",C1136,IF($B$1=\"Deutsch\",D1136,IF($B$1=\"中文\",E1136,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances listed in annex 14 of EU-REACH need authorization by ECHA before usage. Those substances are prohibited for Bosch Power Tools and must not be contained in materials delivered to Bosch Power Tools."},"Substances listed in annex 14 of EU-REACH need authorization by ECHA before usage. Those substances are prohibited for Bosch Power Tools and must not be contained in materials delivered to Bosch Power Tools.","Die Verwendung der in EU-REACH Anhang XIV gelisteten Stoffe bedarf einer spezifischen Zulassung durch ECHA. Diese Stoffe sind bei Bosch Power Tools verboten und dürfen nicht in Materalien enthalten sein, die an Bosch Power Tools geliefert werden.","欧盟REACH法规附件14所列物质的使用，需要由欧洲化学品管理局特别授权。这些物质被禁止用在博世电动工具，并且不能包含在其中提供给博世电动工具材料中。"]
[null,{"$f":"IF($B$1=\"English\",C1137,IF($B$1=\"Deutsch\",D1137,IF($B$1=\"中文\",E1137,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials delivered to Bosch Power Tools shall comply with the prohibitions of substances listed in annex 17 of EU-REACH."},"All materials delivered to Bosch Power Tools shall comply with the prohibitions of substances listed in annex 17 of EU-REACH.","Die in EU-REACH Anhang XVII gelisteten Stoffverbote sind für alle an Bosch Power Tools gelieferten Materialien einzuhalten.","所用供给博世电动工具的材料都应符合在欧盟REACH法规附件17所列出的物质禁用要求"]
[null,{"$f":"IF($B$1=\"English\",C1138,IF($B$1=\"Deutsch\",D1138,IF($B$1=\"中文\",E1138,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Annex XVII \"Prohibitions of Substances\""},"Annex XVII \"Prohibitions of Substances\"","Anhang XVII \"Stoffverbote\"","附件17“禁止使用的物质”"]
[null,{"$f":"IF($B$1=\"English\",C1139,IF($B$1=\"Deutsch\",D1139,IF($B$1=\"中文\",E1139,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For \"type of supplied material\" there are following cases:"},"For \"type of supplied material\" there are following cases:","Für \"Art des gelieferten Materials\" gibt es folgende Fälle:","\n对于“供应的材料类型”，有下列情况："]
[null,{"$f":"IF($B$1=\"English\",C1140,IF($B$1=\"Deutsch\",D1140,IF($B$1=\"中文\",E1140,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Remains in or on the Bosch product: continue with step 3"},"- Remains in or on the Bosch product: continue with step 3","- Verbleibt im oder am Bosch Produkt: weiter mit Schritt 3","\n- 保留在博世产品里或产品上：继续执行步骤3"]
[null,{"$f":"IF($B$1=\"English\",C1141,IF($B$1=\"Deutsch\",D1141,IF($B$1=\"中文\",E1141,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Does not remain in or on the Bosch product: continue with step 4"},"- Does not remain in or on the Bosch product: continue with step 4","- Verbleibt nicht im oder am Bosch-Produkt: weiter mit Schritt 4","\n- 不保留在博世产品里或产品上：继续执行步骤4"]
[null,{"$f":"IF($B$1=\"English\",C1142,IF($B$1=\"Deutsch\",D1142,IF($B$1=\"中文\",E1142,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Merchandise automotive: continue with step 4"},"- Merchandise automotive: continue with step 4","- Handelsware Automobil: weiter mit Schritt 4","\n- 汽车商品：继续执行步骤4"]
[null,{"$f":"IF($B$1=\"English\",C1143,IF($B$1=\"Deutsch\",D1143,IF($B$1=\"中文\",E1143,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Merchandise non-automotive: continue with step 3"},"- Merchandise non-automotive: continue with step 3","- Handelsware Nicht-Automobil: weiter mit Schritt 3","\n- 非汽车商品：继续执行步骤3"]
[null,{"$f":"IF($B$1=\"English\",C1144,IF($B$1=\"Deutsch\",D1144,IF($B$1=\"中文\",E1144,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Bosch reference list: continue with step 4"},"- Bosch reference list: continue with step 4","- Bosch Reference List: weiter mit Schritt 4","‘- 博世推荐列表: 继续执行步骤4"]
[null,{"$f":"IF($B$1=\"English\",C1145,IF($B$1=\"Deutsch\",D1145,IF($B$1=\"中文\",E1145,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"if intentionally added"},"if intentionally added","absichtlich hinzugefügt","有意添加"]
[null,{"$f":"IF($B$1=\"English\",C1146,IF($B$1=\"Deutsch\",D1146,IF($B$1=\"中文\",E1146,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"List of Exemptions (08 June 2011)"},"List of Exemptions (08 June 2011)","Liste der Ausnahmen (08.06.2011)","豁免清单（2011年6月8日）"]
[null,{"$f":"IF($B$1=\"English\",C1147,IF($B$1=\"Deutsch\",D1147,IF($B$1=\"中文\",E1147,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Merchandise non-automotive"},"Merchandise non-automotive","Handelsware Nicht-Automobil","非汽车商品"]
[null,{"$f":"IF($B$1=\"English\",C1148,IF($B$1=\"Deutsch\",D1148,IF($B$1=\"中文\",E1148,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Non-Bosch items distributed\nwithout modification under the name of the external manufacturer. Also applies to onceonly\nbought-in items. These items fall not under ELV respectively GADSL. \n\n"},"Non-Bosch items distributed\nwithout modification under the name of the external manufacturer. Also applies to onceonly\nbought-in items. These items fall not under ELV respectively GADSL. \n\n","Fremderzeugnisse, die unverändert unter dem Namen des externen Herstellers vertrieben werden. Zutreffend auch für einmalig zuge-kaufte Erzeugnisse. Diese Erzeugnisse fallen nicht unter ELV bzw. GADSL.","不做任何加工，依旧以外部供应商生产者名义销售的第三方产品。 此亦适用于一次性额外购买的产品。此产品不属于ELV或者GADSL的管控范畴。"]
[null,{"$f":"IF($B$1=\"English\",C1149,IF($B$1=\"Deutsch\",D1149,IF($B$1=\"中文\",E1149,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Remains in or on the Bosch product"},"Remains in or on the Bosch product","Verbleibt im oder am Bosch-Produkt","保留在博世产品里或产品上"]
[null,{"$f":"IF($B$1=\"English\",C1150,IF($B$1=\"Deutsch\",D1150,IF($B$1=\"中文\",E1150,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Includes all materials which the Bosch customer receives with the product."},"Includes all materials which the Bosch customer receives with the product.","Beinhaltet alle Materialien, die der Bosch-Kunde mit dem Produkt erhält.","包括博世客户能够和产品一起收到的所有材料。"]
[null,{"$f":"IF($B$1=\"English\",C1151,IF($B$1=\"Deutsch\",D1151,IF($B$1=\"中文\",E1151,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Does not remain in or on the Bosch product"},"Does not remain in or on the Bosch product","Verbleibt nicht im oder am Bosch-Produkt","不保留在博世产品里或产品上"]
[null,{"$f":"IF($B$1=\"English\",C1152,IF($B$1=\"Deutsch\",D1152,IF($B$1=\"中文\",E1152,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Includes all materials which do not arrive at the Bosch customer."},"Includes all materials which do not arrive at the Bosch customer.","Beinhaltet alle Materialien, die den Bosch-Kunden nicht erreichen.","包括所有不能送达博世客户的材料"]
[null,{"$f":"IF($B$1=\"English\",C1153,IF($B$1=\"Deutsch\",D1153,IF($B$1=\"中文\",E1153,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What does \"Remains in or on the Bosch product\" mean?"},"What does \"Remains in or on the Bosch product\" mean?","Was bedeutet \"Verbleibt im oder am Bosch-Produkt\"?","什么是“保留在博世产品里或产品上”？"]
[null,{"$f":"IF($B$1=\"English\",C1154,IF($B$1=\"Deutsch\",D1154,IF($B$1=\"中文\",E1154,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What does \"Does not remain in or on the Bosch product\" mean?"},"What does \"Does not remain in or on the Bosch product\" mean?","Was bedeutet \"Verbleibt nicht im oder am Bosch-Produkt\"?","什么是“不保留在博世产品里或产品上”？"]
[null,{"$f":"IF($B$1=\"English\",C1155,IF($B$1=\"Deutsch\",D1155,IF($B$1=\"中文\",E1155,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What does \"Merchandise automotive\" mean?"},"What does \"Merchandise automotive\" mean?","Was bedeutet \"Handelsware Automobil\"?","\n什么是“ 汽车商品”？"]
[null,{"$f":"IF($B$1=\"English\",C1156,IF($B$1=\"Deutsch\",D1156,IF($B$1=\"中文\",E1156,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"What does \"Merchandise non-automotive\" mean?"},"What does \"Merchandise non-automotive\" mean?","Was bedeutet \"Handelsware Nicht-Automobil\"?","\n什么是“ 非汽车商品”？"]
[null,{"$f":"IF($B$1=\"English\",C1157,IF($B$1=\"Deutsch\",D1157,IF($B$1=\"中文\",E1157,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"YES"},"YES","JA","是"]
[null,{"$f":"IF($B$1=\"English\",C1158,IF($B$1=\"Deutsch\",D1158,IF($B$1=\"中文\",E1158,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"NO"},"NO","NEIN","不是"]
[null,{"$f":"IF($B$1=\"English\",C1159,IF($B$1=\"Deutsch\",D1159,IF($B$1=\"中文\",E1159,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab 12: Critical Raw Materials (EU)"},"Tab 12: Critical Raw Materials (EU)","Register 12: Critical Raw Materials (EU)","表 12: 关键原材料 (EU)"]
[null,{"$f":"IF($B$1=\"English\",C1160,IF($B$1=\"Deutsch\",D1160,IF($B$1=\"中文\",E1160,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated Substances"},"Regulated Substances","Reglementierte Inhaltsstoffe ","管控的物质"]
[null,{"$f":"IF($B$1=\"English\",C1161,IF($B$1=\"Deutsch\",D1161,IF($B$1=\"中文\",E1161,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS number"},"CAS number","CAS-Nummer","CAS编号"]
[null,{"$f":"IF($B$1=\"English\",C1162,IF($B$1=\"Deutsch\",D1162,IF($B$1=\"中文\",E1162,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limits [mass %]\nor intentionally added"},"Limits [mass %]\nor intentionally added","Grenzwerte [Massen %]\noder absichtlich hinzugefügt","限度[質量%]\n或有意添加"]
[null,{"$f":"IF($B$1=\"English\",C1163,IF($B$1=\"Deutsch\",D1163,IF($B$1=\"中文\",E1163,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient \n[mass%]"},"Concentration of ingredient \n[mass%]","Konzentration des Inhaltsstoffs \n[Massen%]","配料含量\n[质量%]"]
[null,{"$f":"IF($B$1=\"English\",C1164,IF($B$1=\"Deutsch\",D1164,IF($B$1=\"中文\",E1164,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Designation of the material that contains the regulated substance and concentration.\n\nExplanation: Enter the designation and concentration of ingredient in the component (s) which the substance is used e.g. 10% Aluminium in a motor; 1% Lead in a resistor, 0,15% silver in a wire."},"Designation of the material that contains the regulated substance and concentration.\n\nExplanation: Enter the designation and concentration of ingredient in the component (s) which the substance is used e.g. 10% Aluminium in a motor; 1% Lead in a resistor, 0,15% silver in a wire.","Benennung und Konzentration des Werkstoffs, in dem der reglementierte Inhaltsstoff vorhanden ist\n\nErklärung: Angabe der Bezeichnung und die Konzentration des Bestandteils in dem (den) Bauteil(en) an, in dem (denen) der Stoff verwendet wird, z. B. 10% Aluminium in einem Motor; 1% Blei in einem Widerstand, 0,15% Silber in einem Draht.","Designation of the material that contains the regulated substance and concentration.\n\nExplanation: Enter the designation and concentration of ingredient in the component (s) which the substance is used e.g. 10% Aluminium in a motor; 1% Lead in a resistor, 0,15% silver in a wire."]
[null,{"$f":"IF($B$1=\"English\",C1165,IF($B$1=\"Deutsch\",D1165,IF($B$1=\"中文\",E1165,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Examples of occurrence"},"Examples of occurrence","Beispiele Vorkommen","物质常见用途示例"]
[null,{"$f":"IF($B$1=\"English\",C1166,IF($B$1=\"Deutsch\",D1166,IF($B$1=\"中文\",E1166,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient \n[mass%]"},"Concentration of ingredient \n[mass%]","Konzentration des Inhaltsstoffs \n[Massen%]","配料含量\n[质量%]"]
[null,{"$f":"IF($B$1=\"English\",C1167,IF($B$1=\"Deutsch\",D1167,IF($B$1=\"中文\",E1167,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Battery quantity"},"Battery quantity","Anzahl Batterien","电池数量"]
[null,{"$f":"IF($B$1=\"English\",C1168,IF($B$1=\"Deutsch\",D1168,IF($B$1=\"中文\",E1168,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging type"},"Packaging type","Verpackungsart","包装种类"]
[null,{"$f":"IF($B$1=\"English\",C1169,IF($B$1=\"Deutsch\",D1169,IF($B$1=\"中文\",E1169,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Weight [g]"},"Weight [g]","Gewicht [g]","重量 [g]"]
[null,{"$f":"IF($B$1=\"English\",C1170,IF($B$1=\"Deutsch\",D1170,IF($B$1=\"中文\",E1170,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Battery type"},"Battery type","Batterieart","电池型号"]
[null,{"$f":"IF($B$1=\"English\",C1171,IF($B$1=\"Deutsch\",D1171,IF($B$1=\"中文\",E1171,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Build"},"Build","Bauform","式样"]
[null,{"$f":"IF($B$1=\"English\",C1172,IF($B$1=\"Deutsch\",D1172,IF($B$1=\"中文\",E1172,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Glass"},"Glass","Glas","玻璃"]
[null,{"$f":"IF($B$1=\"English\",C1173,IF($B$1=\"Deutsch\",D1173,IF($B$1=\"中文\",E1173,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Paper/cardboard/carton"},"Paper/cardboard/carton","Papier/Pappe/Karton","纸/纸板/纸箱"]
[null,{"$f":"IF($B$1=\"English\",C1174,IF($B$1=\"Deutsch\",D1174,IF($B$1=\"中文\",E1174,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tin plate, steel"},"Tin plate, steel","Weißblech, Stahl","镀锡板，不锈钢"]
[null,{"$f":"IF($B$1=\"English\",C1175,IF($B$1=\"Deutsch\",D1175,IF($B$1=\"中文\",E1175,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aluminum, other metals"},"Aluminum, other metals","Aluminium, andere Metalle","铝，其它金属"]
[null,{"$f":"IF($B$1=\"English\",C1176,IF($B$1=\"Deutsch\",D1176,IF($B$1=\"中文\",E1176,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content PET"},"Content PET","Anteil PET","PET的比例"]
[null,{"$f":"IF($B$1=\"English\",C1177,IF($B$1=\"Deutsch\",D1177,IF($B$1=\"中文\",E1177,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content HDPE"},"Content HDPE","Anteil HDPE","HDPE的比例"]
[null,{"$f":"IF($B$1=\"English\",C1178,IF($B$1=\"Deutsch\",D1178,IF($B$1=\"中文\",E1178,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content PVC"},"Content PVC","Anteil PVC","PVC的比例"]
[null,{"$f":"IF($B$1=\"English\",C1179,IF($B$1=\"Deutsch\",D1179,IF($B$1=\"中文\",E1179,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content LDPE"},"Content LDPE","Anteil LDPE","LDPE的比例"]
[null,{"$f":"IF($B$1=\"English\",C1180,IF($B$1=\"Deutsch\",D1180,IF($B$1=\"中文\",E1180,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content PP"},"Content PP","Anteil PP","PP的比例"]
[null,{"$f":"IF($B$1=\"English\",C1181,IF($B$1=\"Deutsch\",D1181,IF($B$1=\"中文\",E1181,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content EPS"},"Content EPS","Anteil EPS","EPS的比例"]
[null,{"$f":"IF($B$1=\"English\",C1182,IF($B$1=\"Deutsch\",D1182,IF($B$1=\"中文\",E1182,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content PS"},"Content PS","Anteil PS","PS的比例"]
[null,{"$f":"IF($B$1=\"English\",C1183,IF($B$1=\"Deutsch\",D1183,IF($B$1=\"中文\",E1183,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content PPS"},"Content PPS","Anteil PPS","PPS的比例"]
[null,{"$f":"IF($B$1=\"English\",C1184,IF($B$1=\"Deutsch\",D1184,IF($B$1=\"中文\",E1184,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other plastic/unknown"},"Other plastic/unknown","Anderer Kunsstoff/unbekannt","别的塑料材料/未知"]
[null,{"$f":"IF($B$1=\"English\",C1185,IF($B$1=\"Deutsch\",D1185,IF($B$1=\"中文\",E1185,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Composite packaging"},"Composite packaging","Verbundverpackungen","复合包装"]
[null,{"$f":"IF($B$1=\"English\",C1186,IF($B$1=\"Deutsch\",D1186,IF($B$1=\"中文\",E1186,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Wood without Euro-pallets"},"Wood without Euro-pallets","Holz (ohne Europaletten)","木材（欧式托盘除外）"]
[null,{"$f":"IF($B$1=\"English\",C1187,IF($B$1=\"Deutsch\",D1187,IF($B$1=\"中文\",E1187,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"other natural materials"},"other natural materials","andere Naturmaterialien","其他天然材料"]
[null,{"$f":"IF($B$1=\"English\",C1188,IF($B$1=\"Deutsch\",D1188,IF($B$1=\"中文\",E1188,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1 Nickel-Cadmium (NiCd)"},"1 Nickel-Cadmium (NiCd)","1 Nickel-Cadmium (NiCd)","1镍镉（NiCd）"]
[null,{"$f":"IF($B$1=\"English\",C1189,IF($B$1=\"Deutsch\",D1189,IF($B$1=\"中文\",E1189,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2 Nickel-metal hydride (NiMh)"},"2 Nickel-metal hydride (NiMh)","2 Nickel-Metallhydrid (NiMh)","2镍金属氢化物（镍氢）"]
[null,{"$f":"IF($B$1=\"English\",C1190,IF($B$1=\"Deutsch\",D1190,IF($B$1=\"中文\",E1190,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3 Lithium-Ion (Li-Ion)"},"3 Lithium-Ion (Li-Ion)","3 Lithium-Ion (Li-Ion)","3锂离子电池（Li-Ion）"]
[null,{"$f":"IF($B$1=\"English\",C1191,IF($B$1=\"Deutsch\",D1191,IF($B$1=\"中文\",E1191,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4 Lithium-Metal (Li-Met)"},"4 Lithium-Metal (Li-Met)","4 Lithium-Metall (Li-Met)","4锂金属（Li-Met）"]
[null,{"$f":"IF($B$1=\"English\",C1192,IF($B$1=\"Deutsch\",D1192,IF($B$1=\"中文\",E1192,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5 Alkali-Manganese (AlMn)"},"5 Alkali-Manganese (AlMn)","5 Alkali-Mangan (AlMn)","5 碱锰电池（AlMn）"]
[null,{"$f":"IF($B$1=\"English\",C1193,IF($B$1=\"Deutsch\",D1193,IF($B$1=\"中文\",E1193,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"6 Zinc carbon (ZnC)"},"6 Zinc carbon (ZnC)","6 Zink Kohle (ZnC)","6锌 碳(ZnC)"]
[null,{"$f":"IF($B$1=\"English\",C1194,IF($B$1=\"Deutsch\",D1194,IF($B$1=\"中文\",E1194,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7 Zinc-air (ZnLuft)"},"7 Zinc-air (ZnLuft)","7 Zink-Luft (ZnLuft)","7锌-空气(ZnLuft)"]
[null,{"$f":"IF($B$1=\"English\",C1195,IF($B$1=\"Deutsch\",D1195,IF($B$1=\"中文\",E1195,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"8 Lead Gel (Pb-Gel)"},"8 Lead Gel (Pb-Gel)","8 Blei Gel (Pb-Gel)","8铅 凝胶(Pb-Gel)"]
[null,{"$f":"IF($B$1=\"English\",C1196,IF($B$1=\"Deutsch\",D1196,IF($B$1=\"中文\",E1196,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"9 Kleinblei (Pb)"},"9 Kleinblei (Pb)","9 Kleinblei (Pb)","9铅 (Pb)"]
[null,{"$f":"IF($B$1=\"English\",C1197,IF($B$1=\"Deutsch\",D1197,IF($B$1=\"中文\",E1197,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 Silver oxide (AgO)"},"10 Silver oxide (AgO)","10 Silberoxid (AgO)","10氧化银 (AgO)"]
[null,{"$f":"IF($B$1=\"English\",C1198,IF($B$1=\"Deutsch\",D1198,IF($B$1=\"中文\",E1198,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"11 Other"},"11 Other","11 Andere","11其他"]
[null,{"$f":"IF($B$1=\"English\",C1199,IF($B$1=\"Deutsch\",D1199,IF($B$1=\"中文\",E1199,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Button cell"},"Button cell","Knopfzelle","纽扣电池"]
[null,{"$f":"IF($B$1=\"English\",C1200,IF($B$1=\"Deutsch\",D1200,IF($B$1=\"中文\",E1200,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"AA"},"AA","AA","AA"]
[null,{"$f":"IF($B$1=\"English\",C1201,IF($B$1=\"Deutsch\",D1201,IF($B$1=\"中文\",E1201,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"AAA"},"AAA","AAA","AAA"]
[null,{"$f":"IF($B$1=\"English\",C1202,IF($B$1=\"Deutsch\",D1202,IF($B$1=\"中文\",E1202,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"D"},"D","D","D"]
[null,{"$f":"IF($B$1=\"English\",C1203,IF($B$1=\"Deutsch\",D1203,IF($B$1=\"中文\",E1203,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"9-V-Block"},"9-V-Block","9-V-Block","9-V-Block"]
[null,{"$f":"IF($B$1=\"English\",C1204,IF($B$1=\"Deutsch\",D1204,IF($B$1=\"中文\",E1204,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"LR1"},"LR1","LR1","LR1"]
[null,{"$f":"IF($B$1=\"English\",C1205,IF($B$1=\"Deutsch\",D1205,IF($B$1=\"中文\",E1205,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2/3A"},"2/3A","2/3A","2/3A"]
[null,{"$f":"IF($B$1=\"English\",C1206,IF($B$1=\"Deutsch\",D1206,IF($B$1=\"中文\",E1206,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N"},"N","N","N"]
[null,{"$f":"IF($B$1=\"English\",C1207,IF($B$1=\"Deutsch\",D1207,IF($B$1=\"中文\",E1207,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prismatic"},"Prismatic","Prismatic","棱形"]
[null,{"$f":"IF($B$1=\"English\",C1208,IF($B$1=\"Deutsch\",D1208,IF($B$1=\"中文\",E1208,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pack"},"Pack","Pack","包装"]
[null,{"$f":"IF($B$1=\"English\",C1209,IF($B$1=\"Deutsch\",D1209,IF($B$1=\"中文\",E1209,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CR2"},"CR2","CR2","CR2"]
[null,{"$f":"IF($B$1=\"English\",C1210,IF($B$1=\"Deutsch\",D1210,IF($B$1=\"中文\",E1210,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Automotive battery"},"Automotive battery","Fahrzeugbatterie","汽车电池"]
[null,{"$f":"IF($B$1=\"English\",C1211,IF($B$1=\"Deutsch\",D1211,IF($B$1=\"中文\",E1211,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Customized builds"},"Customized builds","Kundenspezifische Bauformen","顾客定制版本"]
[null,{"$f":"IF($B$1=\"English\",C1212,IF($B$1=\"Deutsch\",D1212,IF($B$1=\"中文\",E1212,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Total weight [g]"},"Total weight [g]","Gesamtgewicht [g]","总重量g"]
[null,{"$f":"IF($B$1=\"English\",C1213,IF($B$1=\"Deutsch\",D1213,IF($B$1=\"中文\",E1213,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Calculate"},"Calculate","Berechnen","计算"]
[null,{"$f":"IF($B$1=\"English\",C1214,IF($B$1=\"Deutsch\",D1214,IF($B$1=\"中文\",E1214,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Safety Data Sheet (SDS) added ?"},"Safety Data Sheet (SDS) added ?","Sicherheits Datenblatt (SDB) beigelegt ?","加入安全数据表（SDS）？"]
[null,{"$f":"IF($B$1=\"English\",C1215,IF($B$1=\"Deutsch\",D1215,IF($B$1=\"中文\",E1215,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1216,IF($B$1=\"Deutsch\",D1216,IF($B$1=\"中文\",E1216,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1217,IF($B$1=\"Deutsch\",D1217,IF($B$1=\"中文\",E1217,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1218,IF($B$1=\"Deutsch\",D1218,IF($B$1=\"中文\",E1218,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging"},"Packaging","Verpackung","包装"]
[null,{"$f":"IF($B$1=\"English\",C1219,IF($B$1=\"Deutsch\",D1219,IF($B$1=\"中文\",E1219,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1220,IF($B$1=\"Deutsch\",D1220,IF($B$1=\"中文\",E1220,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Asbestos"},"Asbestos","Asbest","石棉"]
[null,{"$f":"IF($B$1=\"English\",C1221,IF($B$1=\"Deutsch\",D1221,IF($B$1=\"中文\",E1221,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated biphenyls (PCBs)"},"Polychlorinated biphenyls (PCBs)","Polychloriertes Biphenyl (PCB)","多氯联苯 (PCBs)"]
[null,{"$f":"IF($B$1=\"English\",C1222,IF($B$1=\"Deutsch\",D1222,IF($B$1=\"中文\",E1222,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ozone-depleting substances,\nThese controlled substances are defined in Article 1(4) of the Montreal Protocol on Substances that Deplete the Ozone Layer, 1987, listed in Annexes A,B,C or E to that Protocol in force at the time of application or interpretation of this Annex. Ozone-depleting substances that may be found on board ships include, but are not limited to:"},"Ozone-depleting substances,\nThese controlled substances are defined in Article 1(4) of the Montreal Protocol on Substances that Deplete the Ozone Layer, 1987, listed in Annexes A,B,C or E to that Protocol in force at the time of application or interpretation of this Annex. Ozone-depleting substances that may be found on board ships include, but are not limited to:","Ozonabbauende Substanzen,\ndies sind Stoffe im Sinne des Artikels 1 Nummer 4 des Montrealer Protokolls von 1987 über Stoffe, die zu einem Abbau der Ozonschicht führen, aufgeführt in den Anlagen A, B, C bzw. E dieses Protokolls, soweit es zum Zeitpunkt der Anwendung oder Auslegung des vorliegenden Anhangs in Kraft ist. Zu den Ozon abbauenden Stoffe, die an Bord von Schiffen vorkommen können, zählen unter anderem:","消耗臭氧层物质，是指在《关于消耗臭氧层物质的蒙特利尔议定书（1987》第1（4）款中定义的、列举在议定书附件A，B，C或E中，根据议定书中设定的推进时间表或附件的释义来确定的物质。消耗臭氧层物质可能在船的甲板等某些零件上，包括单不限于："]
[null,{"$f":"IF($B$1=\"English\",C1223,IF($B$1=\"Deutsch\",D1223,IF($B$1=\"中文\",E1223,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorofluorocarbons (CFCs)"},"Chlorofluorocarbons (CFCs)","Fluorchlorkohlenstoffe (FCK)","氯氟烃(CFCs)"]
[null,{"$f":"IF($B$1=\"English\",C1224,IF($B$1=\"Deutsch\",D1224,IF($B$1=\"中文\",E1224,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Halons"},"Halons","Halone","卤代烷"]
[null,{"$f":"IF($B$1=\"English\",C1225,IF($B$1=\"Deutsch\",D1225,IF($B$1=\"中文\",E1225,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other fully halogenated CFCs"},"Other fully halogenated CFCs","Andere vollhalogenierte FCK","\n其他全卤化氟氯化碳"]
[null,{"$f":"IF($B$1=\"English\",C1226,IF($B$1=\"Deutsch\",D1226,IF($B$1=\"中文\",E1226,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Carbon Tetrachloride"},"Carbon Tetrachloride","Tetrachlormethan","四氯化碳"]
[null,{"$f":"IF($B$1=\"English\",C1227,IF($B$1=\"Deutsch\",D1227,IF($B$1=\"中文\",E1227,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1-Trichloroethane"},"1,1,1-Trichloroethane","1,1,1-Trichlorethan","1,1,1-三氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1228,IF($B$1=\"Deutsch\",D1228,IF($B$1=\"中文\",E1228,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydrochlorofluorocarbons"},"Hydrochlorofluorocarbons","Fluorchlorkohlenwasserstoffe","氢氯氟烃"]
[null,{"$f":"IF($B$1=\"English\",C1229,IF($B$1=\"Deutsch\",D1229,IF($B$1=\"中文\",E1229,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydrobromofluorocarbons"},"Hydrobromofluorocarbons","Bromchlorkohlenwasserstoffe","溴氟烃"]
[null,{"$f":"IF($B$1=\"English\",C1230,IF($B$1=\"Deutsch\",D1230,IF($B$1=\"中文\",E1230,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methyl bromide"},"Methyl bromide","Brommethan","溴甲烷"]
[null,{"$f":"IF($B$1=\"English\",C1231,IF($B$1=\"Deutsch\",D1231,IF($B$1=\"中文\",E1231,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bromochloromethane"},"Bromochloromethane","Bromchlormethan","溴氯甲烷"]
[null,{"$f":"IF($B$1=\"English\",C1232,IF($B$1=\"Deutsch\",D1232,IF($B$1=\"中文\",E1232,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anti-fouling systems containing organotin compounds as a biocide"},"Anti-fouling systems containing organotin compounds as a biocide","Antifoulingsysteme, die als Biozide zinnorganische Verbindungen enthalten","含有有机锡化合物的除污系统作为一种杀菌剂(抗生素)"]
[null,{"$f":"IF($B$1=\"English\",C1233,IF($B$1=\"Deutsch\",D1233,IF($B$1=\"中文\",E1233,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tributyl Tins"},"Tributyl Tins","Tributylzinn","三丁基锡"]
[null,{"$f":"IF($B$1=\"English\",C1234,IF($B$1=\"Deutsch\",D1234,IF($B$1=\"中文\",E1234,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Triphenyl Tins"},"Triphenyl Tins","Triphenylzinn","三苯基锡"]
[null,{"$f":"IF($B$1=\"English\",C1235,IF($B$1=\"Deutsch\",D1235,IF($B$1=\"中文\",E1235,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"other"},"other","andere","其他"]
[null,{"$f":"IF($B$1=\"English\",C1236,IF($B$1=\"Deutsch\",D1236,IF($B$1=\"中文\",E1236,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and cadmium compounds"},"Cadmium and cadmium compounds","Kadmium und Kadmiumverbindungen","镉和镉的化合物"]
[null,{"$f":"IF($B$1=\"English\",C1237,IF($B$1=\"Deutsch\",D1237,IF($B$1=\"中文\",E1237,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexavalent chromium and hexavalent chromium compounds"},"Hexavalent chromium and hexavalent chromium compounds","Sechswertiges Chrom und sechswertige Chromverbindungen","六价铬和六价铬的化合物"]
[null,{"$f":"IF($B$1=\"English\",C1238,IF($B$1=\"Deutsch\",D1238,IF($B$1=\"中文\",E1238,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and lead compounds"},"Lead and lead compounds","Blei und Bleiverbindungen","铅和铅的化合物"]
[null,{"$f":"IF($B$1=\"English\",C1239,IF($B$1=\"Deutsch\",D1239,IF($B$1=\"中文\",E1239,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury and mercury compounds"},"Mercury and mercury compounds","Quecksilber und Quecksilberverbindungen","汞和汞的化合物"]
[null,{"$f":"IF($B$1=\"English\",C1240,IF($B$1=\"Deutsch\",D1240,IF($B$1=\"中文\",E1240,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated biphenyl (PBBs)"},"Polybrominated biphenyl (PBBs)","Polybromierte Biphenyle (PBB)","多溴联苯（PBBs）"]
[null,{"$f":"IF($B$1=\"English\",C1241,IF($B$1=\"Deutsch\",D1241,IF($B$1=\"中文\",E1241,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated dephenyl ethers (PBDEs)"},"Polybrominated dephenyl ethers (PBDEs)","Polybromierte Diphenylether (PBDE)","多溴二苯醚（PBDEs）"]
[null,{"$f":"IF($B$1=\"English\",C1242,IF($B$1=\"Deutsch\",D1242,IF($B$1=\"中文\",E1242,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychloronaphthalanes (Cl => 3)"},"Polychloronaphthalanes (Cl => 3)","Polychlornaphthalene (Cl => 3)","多氯合萘(CL => 3)"]
[null,{"$f":"IF($B$1=\"English\",C1243,IF($B$1=\"Deutsch\",D1243,IF($B$1=\"中文\",E1243,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Radioactive substances"},"Radioactive substances","Radioaktive Substanzen","放射性物质"]
[null,{"$f":"IF($B$1=\"English\",C1244,IF($B$1=\"Deutsch\",D1244,IF($B$1=\"中文\",E1244,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Certain shortchain chlorinated paraffins"},"Certain shortchain chlorinated paraffins","Bestimmte kurzkettige chlorierte Paraffine","某些短链氯化石蜡"]
[null,{"$f":"IF($B$1=\"English\",C1245,IF($B$1=\"Deutsch\",D1245,IF($B$1=\"中文\",E1245,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Unit"},"Unit","Einheit","单位"]
[null,{"$f":"IF($B$1=\"English\",C1246,IF($B$1=\"Deutsch\",D1246,IF($B$1=\"中文\",E1246,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mass"},"Mass","Masse","质量"]
[null,{"$f":"IF($B$1=\"English\",C1247,IF($B$1=\"Deutsch\",D1247,IF($B$1=\"中文\",E1247,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"IMO (tab 13)"},"IMO (tab 13)","IMO (Register 13)","IMO 工作表13)"]
[null,{"$f":"IF($B$1=\"English\",C1248,IF($B$1=\"Deutsch\",D1248,IF($B$1=\"中文\",E1248,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product or mechandise might contain chemical substances or combinations that could be released"},"Product or mechandise might contain chemical substances or combinations that could be released","Produkt oder Handelsware kann chemischen Stoffe oder Verbindungen enthalten, die freigesetzt werden können","产品或商品可能含有会释放出来的化学物质或化合物"]
[null,{"$f":"IF($B$1=\"English\",C1249,IF($B$1=\"Deutsch\",D1249,IF($B$1=\"中文\",E1249,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product sticker"},"Product sticker","Produktaufkleber","产品标签"]
[null,{"$f":"IF($B$1=\"English\",C1250,IF($B$1=\"Deutsch\",D1250,IF($B$1=\"中文\",E1250,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium sulfide"},"Cadmium sulfide","Cadmiumsulfid","硫化镉"]
[null,{"$f":"IF($B$1=\"English\",C1251,IF($B$1=\"Deutsch\",D1251,IF($B$1=\"中文\",E1251,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dihexyl phthalate"},"Dihexyl phthalate","Dihexyl phthalate","邻苯二甲酸二己酯"]
[null,{"$f":"IF($B$1=\"English\",C1252,IF($B$1=\"Deutsch\",D1252,IF($B$1=\"中文\",E1252,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dinatrium 3,3'-[[1,1'-biphenyl]-4,4'-diylbis(azo)]bis(4-aminonaphthalen-1-sulfonat) (C.I. Direct Red 28)"},"Dinatrium 3,3'-[[1,1'-biphenyl]-4,4'-diylbis(azo)]bis(4-aminonaphthalen-1-sulfonat) (C.I. Direct Red 28)","Dinatrium 3,3'-[[1,1'-biphenyl]-4,4'-diylbis(azo)]bis(4-aminonaphthalen-1-sulfonat) (C.I. Direct Red 28)","刚果红"]
[null,{"$f":"IF($B$1=\"English\",C1253,IF($B$1=\"Deutsch\",D1253,IF($B$1=\"中文\",E1253,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dinatrium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo]-5-hydroxy-6-(phenylazo)naphthalen-2,7-disulfonat (C.I. Direct Black 38)"},"Dinatrium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo]-5-hydroxy-6-(phenylazo)naphthalen-2,7-disulfonat (C.I. Direct Black 38)","Dinatrium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo]-5-hydroxy-6-(phenylazo)naphthalen-2,7-disulfonat (C.I. Direct Black 38)","直接黑 38"]
[null,{"$f":"IF($B$1=\"English\",C1254,IF($B$1=\"Deutsch\",D1254,IF($B$1=\"中文\",E1254,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Imidazolidin-2-thione; 2-Imidazolin-2-thiol"},"Imidazolidin-2-thione; 2-Imidazolin-2-thiol","Imidazolidin-2-thion; 2-Imidazolin-2-thiol","咪唑烷-2-硫酮；2-咪唑啉-2-硫醇"]
[null,{"$f":"IF($B$1=\"English\",C1255,IF($B$1=\"Deutsch\",D1255,IF($B$1=\"中文\",E1255,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead(II)-acetate"},"Lead(II)-acetate","Bleidiacetat","指示剂试纸-乙酸铅试纸 "]
[null,{"$f":"IF($B$1=\"English\",C1256,IF($B$1=\"Deutsch\",D1256,IF($B$1=\"中文\",E1256,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trixylyl phosphate"},"Trixylyl phosphate","Trixylylphosphat","磷酸三(二甲苯)酯"]
[null,{"$f":"IF($B$1=\"English\",C1257,IF($B$1=\"Deutsch\",D1257,IF($B$1=\"中文\",E1257,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"pigment (e.g. glass and plastic), semiconductors and photoelectronic applications (e.g. solar cells), stabilizers"},"pigment (e.g. glass and plastic), semiconductors and photoelectronic applications (e.g. solar cells), stabilizers","Pigmente (z. B. Glas und Plastik), Halbleiter und photoelectronische Anwendungen (z. B. Solarzellen), Stabilisatoren","颜料绿7（例如玻璃和塑料），半导体和光电应用（如太阳能电池），稳定剂"]
[null,{"$f":"IF($B$1=\"English\",C1258,IF($B$1=\"Deutsch\",D1258,IF($B$1=\"中文\",E1258,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Can be used in the making of plastisols that are subsequently used in the manufacture of automobile parts (air filters, battery covers) and dip-moulded products (tool handles, dishwasher baskets). Commercial phthalate substances containing DnHP may be added to the PVC utilised in the manufacture of flooring, canvas tarps, and notebook covers. Substances containing DnHP may also be used in traffic cones, toys, vinyl gloves, weather stripping, flea collars, shoes, and conveyor belts used in food packaging operations."},"Can be used in the making of plastisols that are subsequently used in the manufacture of automobile parts (air filters, battery covers) and dip-moulded products (tool handles, dishwasher baskets). Commercial phthalate substances containing DnHP may be added to the PVC utilised in the manufacture of flooring, canvas tarps, and notebook covers. Substances containing DnHP may also be used in traffic cones, toys, vinyl gloves, weather stripping, flea collars, shoes, and conveyor belts used in food packaging operations.","Kann verwendet werden zur Herstellung von Plastisolen, die anschließend in der Herstellung von Automobilteilen  (Luftfilter, Batterieabdeckungen) und tauchgeformten Produkten (Werkzeuggriffe, Geschirrspülerkörbe) verwendet werden. Handelsübliche Phthalate, die DnHP beinhalten, dürfen PVC zugesetzt werden zur Herstellung von Bodelbelägen,Planen, und Notebookabdeckungen. DnHP-haltige Substanzen dürfen auch  may also be used in Verkehrspylonen, Spielzeug, Vinyl-Handschuhe, Abdichtungsstreifen, Flohhalsbänder, Schuhe, und Förderbänder zur Lebensmittelverpackung.","可以用在增塑的制作中，随后用在汽车零部件（空气过滤器，电池盖）和浸渍成型产品（工具手柄，洗碗机筐）。含有DnHP的商业苯二甲酸物质可以被添加到PVC用在地板，帆布防水布，和笔记本盖的制造中。含有DnHP的物质也可用在交通路标，玩具，塑料手套，挡风雨条，杀蚤项圈，鞋子，传送带用于食品包装的操作。"]
[null,{"$f":"IF($B$1=\"English\",C1259,IF($B$1=\"Deutsch\",D1259,IF($B$1=\"中文\",E1259,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"dye for fabrics and paper; pH indicator, additive for culture media (for biological staining as in histology gelling); gelling agent for polyvinyl alcohol"},"dye for fabrics and paper; pH indicator, additive for culture media (for biological staining as in histology gelling); gelling agent for polyvinyl alcohol","Färbemittel für Textilien und Papier\npH-Indikator\nZusatz für Agarnährböden  (zur biologischen Färbung histologischer Proben)\nGeliermittel für Polyvinylalkohol","纤维和纸张的染色剂，pH指示剂，培养基的添加剂（用于在组织凝胶中进行生物染色），聚乙烯醇的胶凝剂。"]
[null,{"$f":"IF($B$1=\"English\",C1260,IF($B$1=\"Deutsch\",D1260,IF($B$1=\"中文\",E1260,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"dye for fabrics, leather and paper, plastic material, wood and biological materials;  used to produce aqueous inks; used in hair colorants"},"dye for fabrics, leather and paper, plastic material, wood and biological materials;  used to produce aqueous inks; used in hair colorants","    Färbemittel für Textilien, Leder und Papier, Kunststoff, Holz und biologische Materialen\n    Bestandteil zur Herstellung wässriger Tinten\n    Verwendung in Haarfärbemitteln","织物、皮革、纸张、塑料材料、木材和生物材料等的染色剂；用于制造水性油墨；用于染发剂"]
[null,{"$f":"IF($B$1=\"English\",C1261,IF($B$1=\"Deutsch\",D1261,IF($B$1=\"中文\",E1261,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"used in the production of rubber goods and tyres; of master batches; for making predispersed imidazolidin-2-thione; used for vulcanization for repackaging"},"used in the production of rubber goods and tyres; of master batches; for making predispersed imidazolidin-2-thione; used for vulcanization for repackaging","    Herstellung von Gummiwaren und Reifen\n    Herstellung von Masterbatches\n    Herstellung von vordispergiertem Imidazolidin-2-thion\n    Verwendung als Vulkanisierungsmittel\n    Zur Wiederverpackung","用于制造橡皮货品和轮胎；用于大批量生产；制造预分散咪唑烷-2-硫酮， 用作为橡胶硫化重新包装"]
[null,{"$f":"IF($B$1=\"English\",C1262,IF($B$1=\"Deutsch\",D1262,IF($B$1=\"中文\",E1262,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"used as intermediate product; as a laboratory chemical; for making coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling clay"},"used as intermediate product; as a laboratory chemical; for making coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling clay","    Verwendung als Zwischenprodukt\n    Verwendung als Laborchemikalie\n    Zur Herstellung von Beschichtungen und Farben, Verdünnungsmittel, Farbentferner, Füllmittel, Kitte, Pflaster, Modelliermassen","使用作为中间产品\n使用作为化学实验室\n涂层，颜色，稀释剂，颜料，填料，腻子，石膏，造型的制作"]
[null,{"$f":"IF($B$1=\"English\",C1263,IF($B$1=\"Deutsch\",D1263,IF($B$1=\"中文\",E1263,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"used as lubricant, hydraulic fluid, grease, separator; used in polyurethane, PVC, TPE as well as for coatings and fabrics;  as flame retardant in the production of plastics; used as plasticizer"},"used as lubricant, hydraulic fluid, grease, separator; used in polyurethane, PVC, TPE as well as for coatings and fabrics;  as flame retardant in the production of plastics; used as plasticizer","Verwendung als Schmiermittel, hydraulische Flüssigkeit, Fett, Trennmittel\nVerwendung in Polyurethan, PVC, TPE sowie in Beschichtungen und Textilien\nFlammschutzmittel in der Kunststoffproduktion\nVerwendung als Weichmache","使用作为润滑油，液压油，润滑脂，脱模剂\n使用在聚氨酯，聚氯乙烯，热塑性弹性体以及在涂料和纺织品\n在塑料中的阻燃剂\n使用作为增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C1264,IF($B$1=\"Deutsch\",D1264,IF($B$1=\"中文\",E1264,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging type / quantity"},"Packaging type / quantity","Verpackungsart / Menge","包装种类/数量"]
[null,{"$f":"IF($B$1=\"English\",C1265,IF($B$1=\"Deutsch\",D1265,IF($B$1=\"中文\",E1265,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material"},"Material","Material","材料"]
[null,{"$f":"IF($B$1=\"English\",C1266,IF($B$1=\"Deutsch\",D1266,IF($B$1=\"中文\",E1266,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched and linear, ethoxylated\n[materials with a linear and/or branched alkyl chain of 9 covalently bonded C-atoms in position 4 to phenol, ethoxylated including UVCB- and well-defined substances, polymers and homologs, containing random individual isomers or a combination thereof]"},"4-Nonylphenol, branched and linear, ethoxylated\n[materials with a linear and/or branched alkyl chain of 9 covalently bonded C-atoms in position 4 to phenol, ethoxylated including UVCB- and well-defined substances, polymers and homologs, containing random individual isomers or a combination thereof]","4-Nonylphenol, verzweigt und linear, ethoxyliert\n[Stoffe mit einer linearen und/oder verzweigten Alkylkette von 9 kovalent gebundenen C-Atomen in Position 4 zu Phenol, ethoxyliert inklusive UVCB- und wohldefinierten Stoffen, Polymere und Homologe, die beliebige individuelle Isomere oder einer Kombination davon beinhalten]","乙氧基化的支链和直链的4-壬基酚（直链和/或支链的具有9个碳原子的烷基链共价键合在4位的乙氧基酚，囊括了UVCB和定义明确的物质、聚合物及同系物，其中包括任何单独的异构体和/或他们的组合）"]
[null,{"$f":"IF($B$1=\"English\",C1267,IF($B$1=\"Deutsch\",D1267,IF($B$1=\"中文\",E1267,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium pentadecafluorooctanoate (APFO)"},"Ammonium pentadecafluorooctanoate (APFO)","Ammonium Pentadecafluoroktanoat (APFO)","全氟辛酸铵 （APFO）"]
[null,{"$f":"IF($B$1=\"English\",C1268,IF($B$1=\"Deutsch\",D1268,IF($B$1=\"中文\",E1268,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C1269,IF($B$1=\"Deutsch\",D1269,IF($B$1=\"中文\",E1269,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium oxide"},"Cadmium oxide","Cadmiumoxid","氧化镉"]
[null,{"$f":"IF($B$1=\"English\",C1270,IF($B$1=\"Deutsch\",D1270,IF($B$1=\"中文\",E1270,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dipentyl phthalate"},"Dipentyl phthalate","Dipentyl phthalate","邻苯二甲酸二戊酯"]
[null,{"$f":"IF($B$1=\"English\",C1271,IF($B$1=\"Deutsch\",D1271,IF($B$1=\"中文\",E1271,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentadeca fluorooctane acid (PFOA)"},"Pentadeca fluorooctane acid (PFOA)","Pentadecafluoroktansäure (PFOA)","全氟辛酸 （PFOA）"]
[null,{"$f":"IF($B$1=\"English\",C1272,IF($B$1=\"Deutsch\",D1272,IF($B$1=\"中文\",E1272,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n- Latest application date: 21 October 2014\n\n- Sunset date  21 April 2016"},"Included in Annex 14\n- Latest application date: 21 October 2014\n\n- Sunset date  21 April 2016","Aufgenommen in Anhang 14\n- Antragsschluss: 21. Oktober 2014\n\n- Ablauftermin:  21. April 2016","收录在附录14\n- 申请截止日期：2014年10月21日\n- 日落之日（到期日）：2016年4月21日"]
[null,{"$f":"IF($B$1=\"English\",C1273,IF($B$1=\"Deutsch\",D1273,IF($B$1=\"中文\",E1273,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n- Latest application date: 21 March 2016\n\n- Sunset date  21 September 2017"},"Included in Annex 14\n- Latest application date: 21 March 2016\n\n- Sunset date  21 September 2017","Aufgenommen in Anhang 14\n- Antragsschluss: 21. März 2016\n\n- Ablauftermin:  21. September 2017","收录在附录14\n- 申请截止日期：2016年3月21日\n- 日落之日（到期日）：2017年9月21日"]
[null,{"$f":"IF($B$1=\"English\",C1274,IF($B$1=\"Deutsch\",D1274,IF($B$1=\"中文\",E1274,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"General obligation to declare per ea. PAH from 1 ppm\nprohibition per PAH\na) <1 mg/kg (1 ppm) if to be available for the general public and if components of plastic or rubber, which in regular, reasonable or foreseeable use come into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time \nb) <0,5 mg/kg (0,5 ppm) for toys/products for infants and toddlers and components of plastic or rubber which in regular, reasonable or foreseeable use come into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time "},"General obligation to declare per ea. PAH from 1 ppm\nprohibition per PAH\na) <1 mg/kg (1 ppm) if to be available for the general public and if components of plastic or rubber, which in regular, reasonable or foreseeable use come into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time \nb) <0,5 mg/kg (0,5 ppm) for toys/products for infants and toddlers and components of plastic or rubber which in regular, reasonable or foreseeable use come into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time ","Generell Deklarationspflicht je PAK ab 1ppm\nVerbot: je PAK\na) <1mg/kg (1ppm) wenn für allgemeine Öffentlichkeit bestimmt und Bestandteile aus Kunststoff oder Gummi, die bei normaler oder vernünftiger vorhersehbarer Verwendung unmittelbar, länger oder wiederholt für kurze Zeit mit Haut oder Mundhöhle in Berührung kommt \nb) <0,5mg/kg (0,5ppm) für Spielzeug/Artikel für Säuglinge und Kleinkinder und Bestandteile aus Kunststoff oder Gummi, die bei normaler oder vernünftiger vorhersehbarer Verwendung unmittelbar, länger oder wiederholt für kurze Zeit mit Haut oder Mundhöhle in Berührung kommt ","一般申报要求：任何一种多环芳烃超过1ppm，有义务申报\n禁用要求：任何一种多环芳烃\na)如果普通大众都能够接触到，而且其中的塑料或橡胶零部件在正常使用或者可预见的使用中可能会与皮肤或口腔接触长时间接触或虽短时间但反复接触， < 1 mg/kg (1 ppm) \nb)婴幼儿的玩具或其它产品，而且其中的塑料或橡胶零部件在正常使用或者可预见的使用中可能会与皮肤或口腔接触长时间接触或虽短时间但反复接触， < 0.5 mg/kg (0.5 ppm) \n"]
[null,{"$f":"IF($B$1=\"English\",C1275,IF($B$1=\"Deutsch\",D1275,IF($B$1=\"中文\",E1275,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tri-(2,3-dibromopropyl)-phosphate"},"Tri-(2,3-dibromopropyl)-phosphate","Tri-(2,3-Dibrompropyl)-Phosphat","磷酸三(2,3-二溴丙基)酯 "]
[null,{"$f":"IF($B$1=\"English\",C1276,IF($B$1=\"Deutsch\",D1276,IF($B$1=\"中文\",E1276,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"polycyclic aromatic hydrocarbons PAH\nmaterial group"},"polycyclic aromatic hydrocarbons PAH\nmaterial group","polyzyklische aromatische Kohlenwasserstoffe PAK\nStoffgruppe","多环芳香烃碳水化合物PAH\n材料组"]
[null,{"$f":"IF($B$1=\"English\",C1277,IF($B$1=\"Deutsch\",D1277,IF($B$1=\"中文\",E1277,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1) Must not be used in textile products made to come into contact with the skin, such as garments, underwear and linen\n2) Products not in compliance with para. 1 must not be placed on the market"},"1) Must not be used in textile products made to come into contact with the skin, such as garments, underwear and linen\n2) Products not in compliance with para. 1 must not be placed on the market","1)Darf nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2) Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden","1）不得用于可以接触到皮肤的纺织制品，如外衣，内衣和内衣 \n2）不符合第1款产品，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C1278,IF($B$1=\"Deutsch\",D1278,IF($B$1=\"中文\",E1278,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polycyclic aromatic hydrocarbons PAH : Benzo[a]pyrene, Benzo[e]pyrene, Benzo[a]anthracene, Chrysene, Benzo[b]fluoranthene, Benzo[j]fluoranthene, Benzo[k]fluoranthene und Dibenzo[a,h]anthracene,\n5.Products must not be put on the market for the general public if one of their components of plastic or rubber, which in regular or reasonably foreseeable use comes into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time, more than 1,0 mg/kg (0,0001 mass fraction w/w of this component) includes one of the listed PAH. \nThese are examples of those products: \n— sports equipment such as bikes, golf clubs, rackets \n— household appliances, wheeled wagons; walkers; \n— tools for private use, \n— clothes, shoes, gloves and sports garments, \n— wrist bands, masks, headbands.  \n6.Toys, including activity equipment, and products for infants and toddlers are not placed on the market if one of their components of plastic or rubber, which in regular or reasonably foreseeable use comes into immediate contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time, if more than 0,5 mg/kg (0,00005 mass fraction w/w of this component) contains one of the listed  PAH.\n7. By deviation the paragraphs 5 and 6 are not valid for products that were first brought into the market prior to 27 December 2015. \n8. The commission reviews the limit values as per paragraphs 5 and 6 until 27 Deczember 2017 in the light of new scientific findings, also on the migration of PAH out of the listed products as well as on alternative raw materials, and if applicable changes these paragraphs accordingly.“"},"Polycyclic aromatic hydrocarbons PAH : Benzo[a]pyrene, Benzo[e]pyrene, Benzo[a]anthracene, Chrysene, Benzo[b]fluoranthene, Benzo[j]fluoranthene, Benzo[k]fluoranthene und Dibenzo[a,h]anthracene,\n5.Products must not be put on the market for the general public if one of their components of plastic or rubber, which in regular or reasonably foreseeable use comes into contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time, more than 1,0 mg/kg (0,0001 mass fraction w/w of this component) includes one of the listed PAH. \nThese are examples of those products: \n— sports equipment such as bikes, golf clubs, rackets \n— household appliances, wheeled wagons; walkers; \n— tools for private use, \n— clothes, shoes, gloves and sports garments, \n— wrist bands, masks, headbands.  \n6.Toys, including activity equipment, and products for infants and toddlers are not placed on the market if one of their components of plastic or rubber, which in regular or reasonably foreseeable use comes into immediate contact with skin or the mouth cavity for a longer time, or repeatedly for a shorter time, if more than 0,5 mg/kg (0,00005 mass fraction w/w of this component) contains one of the listed  PAH.\n7. By deviation the paragraphs 5 and 6 are not valid for products that were first brought into the market prior to 27 December 2015. \n8. The commission reviews the limit values as per paragraphs 5 and 6 until 27 Deczember 2017 in the light of new scientific findings, also on the migration of PAH out of the listed products as well as on alternative raw materials, and if applicable changes these paragraphs accordingly.“","polyzyklische aromatische Kohlenwasserstoffe PAK : Benzo[a]pyren, Benzo[e]pyren, Benzo[a]anthracen, Chrysen, Benzo[b]fluoranthen, Benzo[j]fluoranthen, Benzo[k]fluoranthen und Dibenzo[a,h]anthracen,\n5.Erzeugnisse dürfen nicht für die allgemeine Öffentlichkeit in Verkehr gebracht werden, wenn einer ihrer Bestandteile aus Kunststoff oder Gummi, der bei normaler oder vernünftigerweise vorhersehbarer Verwendung unmittelbar, länger oder wiederholt für kurze Zeit mit der menschlichen Haut oder der Mundhöhle in Berührung kommt, mehr als 1,0 mg/kg (0,0001 Massenprozent w/w dieses Bestandteils) eines der aufgeführten PAK enthält. \nZu diesen Erzeugnissen zählen unter anderem: \n— Sportgeräte wie Fahrräder, Golfschläger, Schläger, \n— Haushaltsgeräte, mit Rädern versehene Wagen, Laufhilfen, \n— Werkzeuge für den privaten Gebrauch, \n— Bekleidung, Schuhe, Handschuhe und Sportkleidung, \n— Uhrenarmbänder, Armbänder, Masken, Stirnbänder.  \n6.Spielzeug, einschließlich Aktivitätsspielzeug, und Artikel für Säuglinge und Kleinkinder werden nicht in Verkehr gebracht, wenn einer ihrer Bestandteile aus Kunststoff oder Gummi, der bei normaler oder vernünftigerweise vorhersehbarer Verwendung unmittelbar, länger oder wiederholt für kurze Zeit mit der menschlichen Haut oder der Mundhöhle in Berührung kommt, mehr als 0,5 mg/kg (0,00005 Massenprozent w/w dieses Bestandteils) eines der aufgeführten PAK enthält.\n7. Davon abweichend gelten die Absätze 5 und 6 nicht für Erzeugnisse, die vor dem 27. Dezember 2015 erstmals in Verkehr gebracht wurden. \n8. Bis zum 27. Dezember 2017 überprüft die Kommission die Grenzwerte gemäß den Absätzen 5 und 6 im Lichte neuer wissenschaftlicher Erkenntnisse, auch über die Migration von PAK aus den darin genannten Erzeugnissen, sowie über alternative Rohstoffe und ändert diese Absätze gegebenenfalls entsprechend.“","多环芳烃 PAH：\n苯并(a)芘, 苯并[e]芘, 1,2-苯并[a]蒽, 屈, 苯并(b)荧蒽, 苯并(j)荧蒽, 苯并(k)荧蒽, 二苯并[a,h]蒽-\n5.如果产品的塑料或橡胶零部件在正常可预见的使用中可能会与皮肤或口腔接触长时间接触或虽短时间但反复接触，其中上述所列任何一种PAH的含量 超过 1.0 mg/kg(以这个零件的总质 量为基数计算) 时，该产品不得投放市场销售给普通大众。\n下列产品属于其中:\n- 体育器械，例如自行车，高尔夫球棒，球棒\n- 家居用品，轮式手推车，帮助走路的车\n- 供私人使用的工具，\n- 服装，鞋，手套，运动服，\n- 表带，手链，口罩，头巾。\n6.婴幼儿玩具，包括婴幼儿活动器材和产品，如果其塑料或橡胶零部件在正常可预见的使用中可能会与皮肤或口腔接触长时间接触或虽短时间但反复接触，其中上述所列任何一种PAH的含量 超过 0.5 mg/kg (以这个零件的总质量为基数计算) 时，该婴幼儿产品不能投放市场\n7. 第5和第6条不适用于在2015年12月27日之前已投放市场的产品。\n8.在2017年12月27日之前，欧盟委员会会依据当时的科技能力，包括PAH从上述产品中迁出以及替代原材料，重新评估第5和第6条中的限值，从而对这些段落进行相应地修改。\n"]
[null,{"$f":"IF($B$1=\"English\",C1279,IF($B$1=\"Deutsch\",D1279,IF($B$1=\"中文\",E1279,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plastic or rubber parts, cables, dark plastic materials"},"Plastic or rubber parts, cables, dark plastic materials","Kunststoff- oder Gummiteile, Kabel, dunkle Kunststoffe","塑料或橡胶件，电缆，暗塑料"]
[null,{"$f":"IF($B$1=\"English\",C1280,IF($B$1=\"Deutsch\",D1280,IF($B$1=\"中文\",E1280,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component in paints, varnishes, cleaning substances adhesives and agents for surface treatment, process chemicals for polymerization of emulsions"},"Component in paints, varnishes, cleaning substances adhesives and agents for surface treatment, process chemicals for polymerization of emulsions"," Bestandteil in Farben, Lacken, Reinigungsmitteln, Klebstoffen und Mitteln zur Oberflächenbehandlung; Prozesschemikalie zur Emulsionspolymerisation","油漆，涂料，清洁剂，粘合剂，表面处理剂，乳液聚合反应的工艺化学品等的成分"]
[null,{"$f":"IF($B$1=\"English\",C1281,IF($B$1=\"Deutsch\",D1281,IF($B$1=\"中文\",E1281,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"APFO is used as an auxiliary material for the production of fluoropolymers. These are used in various different branches of industry, such as e. g. in the textile area, in pulp and paper industry and in galvanics.\nMany products contain remains of APFO as e. g. textile materials, carpets, upholstery, paper, leather, printing ink, cleaning and care agents for carpets, sealing agents, floor wax, paints, impregnating agents, fire extinguishing foam, surface-treated wall-to-wall carpeting, skiing wax.\n"},"APFO is used as an auxiliary material for the production of fluoropolymers. These are used in various different branches of industry, such as e. g. in the textile area, in pulp and paper industry and in galvanics.\nMany products contain remains of APFO as e. g. textile materials, carpets, upholstery, paper, leather, printing ink, cleaning and care agents for carpets, sealing agents, floor wax, paints, impregnating agents, fire extinguishing foam, surface-treated wall-to-wall carpeting, skiing wax.\n"," Verwendet wird APFo als Prozesshilfsstoff in der Herstellung von Fluorpolymeren. Diese werden in verschiedenen Industriezweigen verwendet, wie z. B. im Textilbereich, der Papierindustrie und in der Galvanik.\n\nViele Produkte enthalten Reste von APFO wie z. B. Textilstoffe, Teppiche, Polstermöbel, Papier, Leder, Druckerfarbe, Reinigungsmittel und Pflegemittel für Teppiche, Dichtungsmittel, Bodenwachs, Farben, Imprägnierungsmittel, Feuerlöschschaum, oberflächenbehandelte Auslegeware und Ski Wachs","APFO在含氟聚合物的制造中被用作工艺添加剂。这些含氟聚合物应用于多种行业，如纺织行业，造纸行业和电镀。\n\n很多产品中含有APFO的残留，例如，纺织面料，地毯，软垫家具，造纸，皮革，油墨，清洁剂和保养产品用于地毯，密封剂，地板蜡，油漆，防水产品，灭火器泡沫，表面处理过的地毯和滑雪蜡"]
[null,{"$f":"IF($B$1=\"English\",C1282,IF($B$1=\"Deutsch\",D1282,IF($B$1=\"中文\",E1282,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electrodes in Nickel-cadmium accumulators, coatings of metals (corrosion protection); as an alloying constituent e. g. in electrical contacts and solders"},"Electrodes in Nickel-cadmium accumulators, coatings of metals (corrosion protection); as an alloying constituent e. g. in electrical contacts and solders","Elektroden in Nickel-Cadmium Akkumulatoren; Beschichtungen von Metallen (Korrosionsschutz); als Legierungsbestandteil zum Beispiel in elektrischen Kontakten und Loten\n","镍镉蓄电池电极，金属涂层（防腐），作为合金中的成分，如电触头和焊料中"]
[null,{"$f":"IF($B$1=\"English\",C1283,IF($B$1=\"Deutsch\",D1283,IF($B$1=\"中文\",E1283,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Raw material for electrodes, alloys, pigments (red), catalyzers and coatings of metals; thermal stabilizers in polymers; ceramic glaze and glass component; laboratory chemicals."},"Raw material for electrodes, alloys, pigments (red), catalyzers and coatings of metals; thermal stabilizers in polymers; ceramic glaze and glass component; laboratory chemicals."," Rohstoff für die Produktion von Elektroden, Legierungen, Pigmenten (rot), Katalysatoren und Beschichtung von Metallen; Hitzestabilisator in Polymeren; Keramikglasuren und Glasbestandteil; Laborchemikalien.","用于生产电极，金属合金，颜料（红），催化剂和金属涂层的原材料；聚合物中的热稳定剂；陶瓷釉料和玻璃部件；实验室的化学品。"]
[null,{"$f":"IF($B$1=\"English\",C1284,IF($B$1=\"Deutsch\",D1284,IF($B$1=\"中文\",E1284,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dipentyl phtalate is maily used as a softener in polyvinyl chloride (PVC), but DPP is also found in electrodes for membranes. DPP is usesas a solvent in body care products, printer inks, paints, nitrocellulose and synthetic resins and in the production of adhesives and rubber."},"Dipentyl phtalate is maily used as a softener in polyvinyl chloride (PVC), but DPP is also found in electrodes for membranes. DPP is usesas a solvent in body care products, printer inks, paints, nitrocellulose and synthetic resins and in the production of adhesives and rubber.","Dipentylphthtalat wird hauptsächlich als Weichmacher in Polyvinylchlorid (PVC) verwendet, jedoch findet man DPP ebenfalls in Elektroden für Membranen. Eingesetzt wird DPP als Lösungsmittel in Körperpflegeprodukten, Druckerfarben, Farben, Nitrozellulose und Kunstharzlacken und in der Herstellung von Klebstoffen und Gummi.","邻苯二甲酸二戊酯(DPP)主要被用作聚氯乙烯（PVC）的增塑剂（软化剂），然而DPP也同样能在膜的电极中发现。DPP被用作个人护理产品、打印机油墨、涂料、硝化纤维、合成树脂清漆以及制造粘合剂和橡胶时所用的溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C1285,IF($B$1=\"Deutsch\",D1285,IF($B$1=\"中文\",E1285,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PFOA  is used as an auxiliary material for the production of fluoropolymers. These are used in various different branches of industry, such as e. g. in the textile area, in pulp and paper industry and in galvanics. \n\nMany products contain remains of PFOA as e. g. textile materials, carpets, upholstery, paper, leather, printing ink, cleaning and care agents for carpets, sealing agents, floor wax, paints, impregnating agents, fire extinguishing foam, surface-treated wall-to-wall carpeting, skiing wax. As an impurity PFOA is also found in materials based on perfluorooctanesulfonyl fluoride (POSF). "},"PFOA  is used as an auxiliary material for the production of fluoropolymers. These are used in various different branches of industry, such as e. g. in the textile area, in pulp and paper industry and in galvanics. \n\nMany products contain remains of PFOA as e. g. textile materials, carpets, upholstery, paper, leather, printing ink, cleaning and care agents for carpets, sealing agents, floor wax, paints, impregnating agents, fire extinguishing foam, surface-treated wall-to-wall carpeting, skiing wax. As an impurity PFOA is also found in materials based on perfluorooctanesulfonyl fluoride (POSF). ","Verwendet wird PFOA als Prozesshilfsstoff in der Herstellung von Fluorpolymeren. Diese werden in verschiedenen Industriezweigen verwendet, wie z. B. im Textilbereich, der Papierindustrie und in der Galvanik.\n\nViele Produkte enthalten Reste von PFOA wie z. B. Textilstoffe, Teppiche, Polstermöbel, Papier, Leder, Druckerfarbe, Reinigungsmittel und Pflegemittel für Teppiche, Dichtungsmittel, Bodenwachs, Farben, Imprägnierungsmittel, Feuerlöschschaum, oberflächenbehandelte Auslegeware und Ski Wachs. Als Verunreinigung ist PFOA auch in Perfluoroctylsulfonylfluorid (POSF) basierten Stoffen zu finden.","全氟辛酸铵(PFOA)被用作生产含氟聚合物的工艺添加剂。它被用在不同的行业中，例如纺织行业，造纸行业和电镀行业。\n\n很多产品中含有PFOA的残留物，如纺织面料，地毯，软垫家具，造纸，皮革，印刷油墨，清洁剂，地毯的保养剂，密封剂，地板蜡，油漆，防水产品，灭火器泡沫，表面处理过的地毯织物和滑雪蜡。作为一种杂质，PFOA也可见于以全氟辛基磺酰氟（POSF）为基质的材料中。"]
[null,{"$f":"IF($B$1=\"English\",C1286,IF($B$1=\"Deutsch\",D1286,IF($B$1=\"中文\",E1286,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab: 13 IMO"},"Tab: 13 IMO","Register: 13_IMO","工作表： 13 IMO"]
[null,{"$f":"IF($B$1=\"English\",C1287,IF($B$1=\"Deutsch\",D1287,IF($B$1=\"中文\",E1287,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"<1mg/kg (1ppm) each PAH"},"<1mg/kg (1ppm) each PAH","< 1mg/kg (1ppm) je PAK","每种多环芳烃PAH<1mg/kg (1ppm) "]
[null,{"$f":"IF($B$1=\"English\",C1288,IF($B$1=\"Deutsch\",D1288,IF($B$1=\"中文\",E1288,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyl phthalate (DBP)"},"Dibutyl phthalate (DBP)","Dibutylphthalate (DBP)","邻苯二甲酸二丁酯 (DBP)"]
[null,{"$f":"IF($B$1=\"English\",C1289,IF($B$1=\"Deutsch\",D1289,IF($B$1=\"中文\",E1289,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisobutylphthalat"},"Diisobutylphthalat","Diisobutylphthalat","邻苯二甲酸二异丁酯"]
[null,{"$f":"IF($B$1=\"English\",C1290,IF($B$1=\"Deutsch\",D1290,IF($B$1=\"中文\",E1290,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis (2-ethylhexyl)phthalate (DEHP)"},"Bis (2-ethylhexyl)phthalate (DEHP)","Bis(2-ethylhexyl)phthalat (DEHP)","邻苯二甲酸二(2-乙基)己酯  (DEHP)"]
[null,{"$f":"IF($B$1=\"English\",C1291,IF($B$1=\"Deutsch\",D1291,IF($B$1=\"中文\",E1291,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis (2-methoxyethyl) phtalate"},"Bis (2-methoxyethyl) phtalate","Bis(2-methoxyethyl)phtalat","邻苯二甲酸二甲氧乙酯"]
[null,{"$f":"IF($B$1=\"English\",C1292,IF($B$1=\"Deutsch\",D1292,IF($B$1=\"中文\",E1292,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear \n(=Dihexylphthalate, branched and linear) "},"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear \n(=Dihexylphthalate, branched and linear) ","1,2-Benzoldicarbonsäure, Dihexylester, verzweigt und linear \n(=Dihexylphthalat, verzweigt und linear) ","1,2-苯二甲酸二己基酯，支链和直链\n= 邻苯二甲酸二己酯（支链和直链）"]
[null,{"$f":"IF($B$1=\"English\",C1293,IF($B$1=\"Deutsch\",D1293,IF($B$1=\"中文\",E1293,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium chloride "},"Cadmium chloride ","Cadmiumchlorid ","氯化镉"]
[null,{"$f":"IF($B$1=\"English\",C1294,IF($B$1=\"Deutsch\",D1294,IF($B$1=\"中文\",E1294,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perborate; perboric acid, sodium salt "},"Sodium perborate; perboric acid, sodium salt ","Natriumperborat; Perborsäure, Natriumsalz ","水合高硼酸钠盐类"]
[null,{"$f":"IF($B$1=\"English\",C1295,IF($B$1=\"Deutsch\",D1295,IF($B$1=\"中文\",E1295,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium peroxometaborate "},"Sodium peroxometaborate ","Natriumperoxometaborat","过硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1296,IF($B$1=\"Deutsch\",D1296,IF($B$1=\"中文\",E1296,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"occurs in chemical mixtures on the Nordic market (Sweden, Denmark and Finland), including consumer\navailable products; in sealant/jointing agents; as a component in engine oil stabilizer; in automotive gear lubricant; if technically possible, the C6 phthalate 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear might be used as a substitute for other low/transitional phthalates of carbon backbone lengths of C4-C6 that are being phased out.\n"},"occurs in chemical mixtures on the Nordic market (Sweden, Denmark and Finland), including consumer\navailable products; in sealant/jointing agents; as a component in engine oil stabilizer; in automotive gear lubricant; if technically possible, the C6 phthalate 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear might be used as a substitute for other low/transitional phthalates of carbon backbone lengths of C4-C6 that are being phased out.\n","Kommt vor in chemischen Mischungen im nordischen Markt (Schweden, Dänemark, Finnland) ebenso in Verbrauchsgütern; in Dichtungs- und Verbindungsmitteln; als Bestandteil im Stabilisator von Motorenöl; in Schmiermitteln von Automobilgetrieben; sofern möglich, soll  \nC6 Phtalat 1,2-Benzoldicarbonsäure, Dihexylester, verzweigt und linear, als Ersatz verwendet werden für andere niedrige/übergehende Phtalate des Kohlenstoffgerüsts von C4-C6, die aus dem Verkehr gezogen werden. ","在下列情况发生：在北欧市场（瑞典、丹麦和芬兰）的化学配制品中，包括向消费者提供的产品；在密封剂/接合剂中；作为发动机油稳定剂组成成分；在汽车齿轮润滑剂中；如果技术上可行，C6邻苯二甲酸酯，支链和直链的1,2-苯二甲酸二己酯，可能用于替代被逐步淘汰的碳主链长度C4-C6的其他低/过渡的邻苯二甲酸酯。"]
[null,{"$f":"IF($B$1=\"English\",C1297,IF($B$1=\"Deutsch\",D1297,IF($B$1=\"中文\",E1297,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"is used as raw material for synthesis of other cadmium compounds, in electroplating and electrogalvanizing, for manufacturing of solar cells and as a laboratory reagent; anti-corrosion coatings for metal, laboratory reagent,  manufacturing of battery and photovoltaic modules (semiconductors) "},"is used as raw material for synthesis of other cadmium compounds, in electroplating and electrogalvanizing, for manufacturing of solar cells and as a laboratory reagent; anti-corrosion coatings for metal, laboratory reagent,  manufacturing of battery and photovoltaic modules (semiconductors) "," Wird verwendet in Rohstoffen für die Synthese von anderen Kadmiumverbindungen, zum Galvanisieren und galvanisch Verzinken, zur Herstellung von Solarzellen und als Laborreagens; als Korrosionsschutzschicht für Metalle, Laborreagens, zur Produktion von Batterien und Photovoltaikmodulen (Halbleiter)","在电镀和电镀锌时，为太阳能电池的制造和作为实验室试剂，用于其他镉化合物的合成原料；防腐金属涂料，实验室试剂，电池和光伏组件（半导体）制造"]
[null,{"$f":"IF($B$1=\"English\",C1298,IF($B$1=\"Deutsch\",D1298,IF($B$1=\"中文\",E1298,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"bleaching agent in laundry and dishwashing detergents; are only used in chemical preparations such as bleaching agents, cleaning agents and cosmetic \nproducts; no use in articles has been identified; are only used in the detergent industry and to some (smaller) degree in the cosmetic products industry\n"},"bleaching agent in laundry and dishwashing detergents; are only used in chemical preparations such as bleaching agents, cleaning agents and cosmetic \nproducts; no use in articles has been identified; are only used in the detergent industry and to some (smaller) degree in the cosmetic products industry\n","Bleichmittel in Waschmitteln und Geschirrspülmitteln; wird nur verwendet in chemischen Präparaten, z. B. Bleichmitteln, Reinigungsmitteln und Kosmetikprodukten; wurde in keinen Artikeln gefunden; wird nur in industriellen Reinigungsmitteln und in geringem Umfang in der Kosmetikindustrie verwendet\n","洗衣液和餐具洗涤剂中的漂白剂；只用于化学制剂如漂白剂，清洁剂和化妆品；未见用于物品中；仅用于洗涤剂行业，在一定（较小）程度上用于化妆品行业"]
[null,{"$f":"IF($B$1=\"English\",C1299,IF($B$1=\"Deutsch\",D1299,IF($B$1=\"中文\",E1299,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"bleaching agent in laundry detergents and machine dishwashing products; are only used in chemical preparations such as bleaching agents, cleaning agents and cosmetic products; no use of in articles has been identified"},"bleaching agent in laundry detergents and machine dishwashing products; are only used in chemical preparations such as bleaching agents, cleaning agents and cosmetic products; no use of in articles has been identified","Bleichmittel in Waschmitteln und Geschirrspülmitteln; wird nur verwendet in chemischen Präparaten, z. B. Bleichmitteln, Reinigungsmitteln und Kosmetikprodukten; wurde in keinen Artikeln gefunden","洗衣液和餐具洗涤剂中的漂白剂；只用于化学制剂如漂白剂，清洁剂和化妆品；未见用于物品中；"]
[null,{"$f":"IF($B$1=\"English\",C1300,IF($B$1=\"Deutsch\",D1300,IF($B$1=\"中文\",E1300,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Changes until 2014-07-14 and SVHC candidates list of 2014-06-16"},"Changes until 2014-07-14 and SVHC candidates list of 2014-06-16","Änderungen bis 14.07.14 und SVHC Kandidatenliste vom 16.06.14","直到2014-07-14更改和2014-06-16 的SVHC候选清单"]
[null,{"$f":"IF($B$1=\"English\",C1301,IF($B$1=\"Deutsch\",D1301,IF($B$1=\"中文\",E1301,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging Technology (Register 14)"},"Packaging Technology (Register 14)","Verpackungstechnik (Register 14)","包装技术 （工作表 14）"]
[null,{"$f":"IF($B$1=\"English\",C1302,IF($B$1=\"Deutsch\",D1302,IF($B$1=\"中文\",E1302,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisobutyl phthalate (DIBP)"},"Diisobutyl phthalate (DIBP)","Diisobutylphthalat (DIBP)","邻苯二甲酸二异丁酯（DIBP）"]
[null,{"$f":"IF($B$1=\"English\",C1303,IF($B$1=\"Deutsch\",D1303,IF($B$1=\"中文\",E1303,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl)phthalate (DMEP)"},"Bis(2-methoxyethyl)phthalate (DMEP)","Bis(2-methoxyethyl)phthalat (DMEP)","双（ 2-甲氧基乙基）邻苯二甲酸酯（DMEP）"]
[null,{"$f":"IF($B$1=\"English\",C1304,IF($B$1=\"Deutsch\",D1304,IF($B$1=\"中文\",E1304,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisopentyl phthalate (DIPP)"},"Diisopentyl phthalate (DIPP)","Diisopentyl phthalat (DIPP)","邻苯二酸二异戊酯 （DIPP）"]
[null,{"$f":"IF($B$1=\"English\",C1305,IF($B$1=\"Deutsch\",D1305,IF($B$1=\"中文\",E1305,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzyl butyl phthalate (BBP)"},"Benzyl butyl phthalate (BBP)","Benzyl butyl phthalat (BBP)","邻苯二甲酸丁基苄酯（BBP）"]
[null,{"$f":"IF($B$1=\"English\",C1306,IF($B$1=\"Deutsch\",D1306,IF($B$1=\"中文\",E1306,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl) phthalate (DEHP)"},"Bis(2-ethylhexyl) phthalate (DEHP)","Bis(2-ethylhexyl) phthalat (DEHP)","邻苯二甲酸二(2-乙基己基)酯 (DEHP)"]
[null,{"$f":"IF($B$1=\"English\",C1307,IF($B$1=\"Deutsch\",D1307,IF($B$1=\"中文\",E1307,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C7-11-branched and linear alkyl esters (Di(heptyl, nonyl, undecyl) phthalate (DHNUP; dialkyl phthalate (C7-11) branched and linear)"},"1,2-Benzenedicarboxylic acid, di-C7-11-branched and linear alkyl esters (Di(heptyl, nonyl, undecyl) phthalate (DHNUP; dialkyl phthalate (C7-11) branched and linear)","1,2-Benzoldicarbonsäure, di-C7-11-verzweigte und lineare Alkylester (Di(heptyl, nonyl, undecyl) phthalat (DHNUP; Dialkylphthalat (C7-11) verzweigt und linear)","邻苯二甲酸二（C7-11支链和直链）烷基酯（二（庚基，壬基，十一烷基）酯（DHNUP;二烷基邻苯二甲酸酯（C7-11）支链和直链）"]
[null,{"$f":"IF($B$1=\"English\",C1308,IF($B$1=\"Deutsch\",D1308,IF($B$1=\"中文\",E1308,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl ester, C7-rich (C6-8-(branched)-alkyl phthalate, diisoheptyl phthalate)"},"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl ester, C7-rich (C6-8-(branched)-alkyl phthalate, diisoheptyl phthalate)","1,2-Benzoldicarbonsäure, Di-C6-8-verzweigte Alkylester, C7-reich (C6-8-(verzweigt)-Alkylphthalat, Diisoheptyl phthalat)"," 邻苯二甲酸二（C6-8支链）烷基酯，富C7（C6-8-（支链）烷基酯，邻苯二甲酸二异戊酯）"]
[null,{"$f":"IF($B$1=\"English\",C1309,IF($B$1=\"Deutsch\",D1309,IF($B$1=\"中文\",E1309,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, dipentylester, branched and linear (dihexylphthalate)"},"1,2-Benzenedicarboxylic acid, dipentylester, branched and linear (dihexylphthalate)","1,2-Benzoldicarbonsäure, Dipentylester, verzweigt und linear (Dihexylphthalat)","支链和直链1，2-苯二羧二戊酯（邻苯二酸二已酯）（DHXP）"]
[null,{"$f":"IF($B$1=\"English\",C1310,IF($B$1=\"Deutsch\",D1310,IF($B$1=\"中文\",E1310,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dipentyl phthalate (DPP)"},"Dipentyl phthalate (DPP)","Dipentylphthalat (DPP)","邻苯二甲酸二戊酯（DPP）"]
[null,{"$f":"IF($B$1=\"English\",C1311,IF($B$1=\"Deutsch\",D1311,IF($B$1=\"中文\",E1311,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear (bis-C5-alkyl-(linear and branched)phthalate)"},"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear (bis-C5-alkyl-(linear and branched)phthalate)","1,2-Benzoldicarbonsäure, Dihexylester, verzweigt und linear (bis-C5-Alkyl-(linear und verzweigt)phthalat)","邻苯二甲酸二己酯，支链和直链（双-C5-烷基- （直链和支链）邻苯二甲酸酯）"]
[null,{"$f":"IF($B$1=\"English\",C1312,IF($B$1=\"Deutsch\",D1312,IF($B$1=\"中文\",E1312,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ROHS Future (register 5a)"},"ROHS Future (register 5a)","ROHS Future (Register 5a)","将来的 ROHS (登记表 5a)"]
[null,{"$f":"IF($B$1=\"English\",C1313,IF($B$1=\"Deutsch\",D1313,IF($B$1=\"中文\",E1313,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value [mass-%]"},"Limit value [mass-%]","Grenzwert [Massen%]","限值 （质量%）"]
[null,{"$f":"IF($B$1=\"English\",C1314,IF($B$1=\"Deutsch\",D1314,IF($B$1=\"中文\",E1314,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyl phthalate"},"Dibutyl phthalate","Dibutylphthalat","邻苯二甲酸二丁酯"]
[null,{"$f":"IF($B$1=\"English\",C1315,IF($B$1=\"Deutsch\",D1315,IF($B$1=\"中文\",E1315,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl)phthalate"},"Bis(2-methoxyethyl)phthalate","Bis(2-methoxyethyl)phthalat","双（2-甲氧基乙基）邻苯二甲酸酯"]
[null,{"$f":"IF($B$1=\"English\",C1316,IF($B$1=\"Deutsch\",D1316,IF($B$1=\"中文\",E1316,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzyl butyl phthalate"},"Benzyl butyl phthalate","Benzylbutylphthalat","邻苯二甲酸丁基苄酯"]
[null,{"$f":"IF($B$1=\"English\",C1317,IF($B$1=\"Deutsch\",D1317,IF($B$1=\"中文\",E1317,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate"},"Bis(2-ethylhexyl)phthalate","Bis(2-ethylhexyl)phthalat","邻苯二甲酸二(2-乙基己基)酯"]
[null,{"$f":"IF($B$1=\"English\",C1318,IF($B$1=\"Deutsch\",D1318,IF($B$1=\"中文\",E1318,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium fluoride"},"Cadmium fluoride","Cadmiumfluorid","氟化镉"]
[null,{"$f":"IF($B$1=\"English\",C1319,IF($B$1=\"Deutsch\",D1319,IF($B$1=\"中文\",E1319,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium sulphate"},"Cadmium sulphate","Cadmiumsulfat","硫酸镉"]
[null,{"$f":"IF($B$1=\"English\",C1320,IF($B$1=\"Deutsch\",D1320,IF($B$1=\"中文\",E1320,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)"},"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)","2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)","2-苯并三唑-2-基-4,6-二叔丁基苯酚（紫外线吸收剂UV-320）"]
[null,{"$f":"IF($B$1=\"English\",C1321,IF($B$1=\"Deutsch\",D1321,IF($B$1=\"中文\",E1321,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4,6-di-tert-pentylphenol \n(UV-328)\n"},"2-(2H-benzotriazol-2-yl)-4,6-di-tert-pentylphenol \n(UV-328)\n","2-(2H-benzotriazol-2-yl)-4,6-di-tert-pentylphenol \n(UV-328)\n","2-（2H-苯并三唑-2-基）-4,6-二叔戊基苯酚\n（紫外线吸收剂 UV-328）"]
[null,{"$f":"IF($B$1=\"English\",C1322,IF($B$1=\"Deutsch\",D1322,IF($B$1=\"中文\",E1322,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (DOTE)"},"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (DOTE)","2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (DOTE)","二正辛基-双（巯乙酸2-乙基己酯）锡（DOTE）"]
[null,{"$f":"IF($B$1=\"English\",C1323,IF($B$1=\"Deutsch\",D1323,IF($B$1=\"中文\",E1323,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of \n2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate and \n2-ethylhexyl 10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (reaction mass of DOTE and MOTE)\n"},"Reaction mass of \n2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate and \n2-ethylhexyl 10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (reaction mass of DOTE and MOTE)\n","Reaktionsmasse aus \n2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und \n2-ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaktionsmasse von DOTE und MOTE)\n","二正辛基-双（巯乙酸2-乙基己酯）锡和\n单辛基-三（2-乙基己基巯基乙酸酯）惜的反应产物（DOTE和 MOTE的反应产物）"]
[null,{"$f":"IF($B$1=\"English\",C1324,IF($B$1=\"Deutsch\",D1324,IF($B$1=\"中文\",E1324,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"joining and fusible alloys (brazing alloys); in articles: phosphorus, solar cells, glass, optical electronics; others: research chemical, high-temp. dry-film lubricant;\nCadmium fluoride is fluorescent and can therefore be used in certain phosphorus for luminescent screens.\n"},"joining and fusible alloys (brazing alloys); in articles: phosphorus, solar cells, glass, optical electronics; others: research chemical, high-temp. dry-film lubricant;\nCadmium fluoride is fluorescent and can therefore be used in certain phosphorus for luminescent screens.\n","Verbindungs- und Schmelzlegierungen (Hartlotlegierungen); in Produkten: Phosphor, Solarzellen, Glas, Optoelektronik; Andere: Forschungschemikalie, Hochtemperatur-Festschmierstoff;\nCadmiumfluorid ist fluoreszierend und kann deshalb in bestimmten Phosphorverbindungen für lumineszierende Schirme verwendet werden.\n","结合合金和易熔合金（铜合金）；在下列物品中：磷，太阳能电池，玻璃，光学电子；其他：研究化学，耐高温干膜润滑剂；\n氟化镉是一种荧光剂，可用于某些磷的发光屏。"]
[null,{"$f":"IF($B$1=\"English\",C1325,IF($B$1=\"Deutsch\",D1325,IF($B$1=\"中文\",E1325,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"in articles: impurity in pigment (plastic, ceramic, glass, rubber, paper, ink); others: laboratory reagent (?),high-temp. dry-film lubricant (?);\nUse as an intermediate for industrial production of inorganic cadmium compounds.\nAs a raw material for metal surface coating and for restoring of lead acid batteries. \n"},"in articles: impurity in pigment (plastic, ceramic, glass, rubber, paper, ink); others: laboratory reagent (?),high-temp. dry-film lubricant (?);\nUse as an intermediate for industrial production of inorganic cadmium compounds.\nAs a raw material for metal surface coating and for restoring of lead acid batteries. \n","In Produkten: Verunreinigung in Pigmenten (Kunststoff, Keramik, Glas, Gummi, Papier, Tinte); Andere: Laborreagenzien (?), Hochtemperatur-Festschmierstoff (?);\nVerwendung als Zwischenprodukt zur industriellen Herstellung von anorganischen Cadmiumverbindungen. \nAls Rohstoff für metallische Oberflächenbeschichtung und zum Aufladen von Bleiakkumulatoren. \n","在下列物品中：颜料（塑料，陶瓷，玻璃，橡胶，纸，墨）中的杂质 ;其他：实验室试剂(?)，耐高温干膜润滑剂(?) ;\n作为工业生产的无机镉化合物的中间产品。用作金属表面涂层原料和用作修复铅酸电池的原料。"]
[null,{"$f":"IF($B$1=\"English\",C1326,IF($B$1=\"Deutsch\",D1326,IF($B$1=\"中文\",E1326,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"are used as UV-stabilisers (technically the most important UV-absorbers, especially for transparent plastic materials); 50 % are used as UV-protection agents in coatings especially for cars and special industrial wood coatings; ca. 40% are used as UV-protection agents for plastics, rubber and polyurethanes; used as UV-stabiliser for plastics, polyurethanes and rubber and constituent in formulations used for coating of surfaces, e.g. cars or special industrial wood coatings\n"},"are used as UV-stabilisers (technically the most important UV-absorbers, especially for transparent plastic materials); 50 % are used as UV-protection agents in coatings especially for cars and special industrial wood coatings; ca. 40% are used as UV-protection agents for plastics, rubber and polyurethanes; used as UV-stabiliser for plastics, polyurethanes and rubber and constituent in formulations used for coating of surfaces, e.g. cars or special industrial wood coatings\n","Verwendung als UV-Stabilisatoren (technisch die wichtigsten UV-Absorber, besonders for transparente Kunststoffe); 50 % werden verwendet als UV-Schutzmittel in Beschichtungen, besonders for Autos und spezielle industrielle Holzbeschichtung; ca. 40% werden verwendet als UV-Schutzmittel für Kunststoffe, Gummi und Polyurethane; Verwendung als UV-Stabilisatoren für Kunststoff, Polyurethane und Gummi und Bestandteil in Formulierungen für Oberflächenbeschichtungen, z. B. für Autos oder spezielle industrielle Holzbeschichtung.\n","用作紫外线稳定剂（技术上最重要的紫外线吸收剂，特别是对透明的塑料材料）；50％用于涂料中，特别是汽车和特殊工业木材涂料中，作为紫外线防护剂；约40％被用作塑料，橡胶和聚氨酯的紫外线防护剂;用作紫外线稳定剂用于塑料，聚氨酯和橡胶，用于表面涂层的组成成分，例如汽车或特殊工业木器涂料中"]
[null,{"$f":"IF($B$1=\"English\",C1327,IF($B$1=\"Deutsch\",D1327,IF($B$1=\"中文\",E1327,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"are used as UV-stabilisers (technically the most important UV-absorbers, especially for transparent plastic materials); 50 % are used as UV-protection agents in coatings especially for cars and special industrial wood coatings; ca. 40% are used as UV-protection agents for plastics, rubber and polyurethanes; also used for light stabilizing in coatings, ABS resin, epoxy resin, fiber resin, propylene and polyvinyl chloride; also effective in light stabilization of unsaturated polyester, polyacrylate and polycarbonate\n"},"are used as UV-stabilisers (technically the most important UV-absorbers, especially for transparent plastic materials); 50 % are used as UV-protection agents in coatings especially for cars and special industrial wood coatings; ca. 40% are used as UV-protection agents for plastics, rubber and polyurethanes; also used for light stabilizing in coatings, ABS resin, epoxy resin, fiber resin, propylene and polyvinyl chloride; also effective in light stabilization of unsaturated polyester, polyacrylate and polycarbonate\n","Verwendung als UV-Stabilisatoren (technisch die wichtigsten UV-Absorber, besonders for transparente Kunststoffe); 50 % werden verwendet als UV-Schutzmittel in Beschichtungen, besonders for Autos und spezielle industrielle Holzbeschichtung; ca. 40% werden verwendet als UV-Schutzmittel für Kunststoffe, Gummi und Polyurethane; auch verwendet als Lichtschutzmittel in Beschichtungen, ABS Harz, Epoxidharz, Faserharz, Propylen und Polyvinylchlorid; auch wirksam in Lichtschutzmitteln aus ungesättigten Polyestern, Polyacrylaten und Polycarbonaten.\n","用作紫外线稳定剂（技术上最重要的紫外线吸收剂，特别是对透明的塑料材料）；50％用于涂料中，特别是汽车和特殊工业木材涂料中，作为紫外线防护剂；约40％被用作塑料，橡胶和聚氨酯的紫外线防护剂；也可作为光稳定剂，用于涂料，ABS树脂，环氧树脂，纤维树脂，丙烯和聚氯乙烯中;也是不饱和聚酯，聚丙烯酸酯和聚碳酸酯的有效光稳定剂"]
[null,{"$f":"IF($B$1=\"English\",C1328,IF($B$1=\"Deutsch\",D1328,IF($B$1=\"中文\",E1328,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"DOTE:MOTE reaction mass is used as a heat stabiliser in the production of PVC to prevent the elimination of HCl; DOTE:MOTE is predominantly used in the\nproduction of un-plasticised PVC; it is present in various different types of consumer articles, such as packaging material (food and pharmaceutical packaging) and credit cards; the reaction mass is used for window profiles, pipes (e.g. drinking pipes) and bottles used to keep shampoos, shower gels and detergents\n"},"DOTE:MOTE reaction mass is used as a heat stabiliser in the production of PVC to prevent the elimination of HCl; DOTE:MOTE is predominantly used in the\nproduction of un-plasticised PVC; it is present in various different types of consumer articles, such as packaging material (food and pharmaceutical packaging) and credit cards; the reaction mass is used for window profiles, pipes (e.g. drinking pipes) and bottles used to keep shampoos, shower gels and detergents\n","DOTE:MOTE Reaktionsmasse verwendet als Hitzestabilisator in der Produktion von PVC um die Freisetzung von HCl zu verhindern; DOTE:MOTE wird überweigend in der\nProduktion von weichmacherfreiem PVC verwendet; es ist vorhanden in verschiedenen Konsumartikelen, z. B. Verpackungsmaterial (Lebensmittel- und pharmazeutischer Verpackung) und Kreditkarten; die Reaktionsmasse wird für Fensterprofile, Rohre (z. B. Trinkhalme) und Flaschen für Shampoo, Duschgel und Reinigungsmittel\n","DOTE:MOTE反应产物被用作生产PVC的热稳定剂，以防止盐酸的消除；DOTE:MOTE主要用于生产非塑化PVC；它存在于各种不同类型的消费制品中，如包装材料（食品和药品包装）和信用卡；反应产物​​用于窗型材，管道（例如饮用水管道）和装香波，沐浴露和洗涤剂的瓶子"]
[null,{"$f":"IF($B$1=\"English\",C1329,IF($B$1=\"Deutsch\",D1329,IF($B$1=\"中文\",E1329,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"see uses under „2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (DOTE)“  \n"},"see uses under „2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (DOTE)“  \n","siehe Verwendung unter „2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (DOTE)“  \n","见“二正辛基-双（巯乙酸2-乙基己酯）锡（DOTE）”的用途"]
[null,{"$f":"IF($B$1=\"English\",C1330,IF($B$1=\"Deutsch\",D1330,IF($B$1=\"中文\",E1330,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, methyl"},"Phenol, methyl","Phenol, methyl","苯酚，甲基"]
[null,{"$f":"IF($B$1=\"English\",C1331,IF($B$1=\"Deutsch\",D1331,IF($B$1=\"中文\",E1331,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 2-methyl"},"Phenol, 2-methyl","Phenol, 2-methyl","苯酚，2-甲基"]
[null,{"$f":"IF($B$1=\"English\",C1332,IF($B$1=\"Deutsch\",D1332,IF($B$1=\"中文\",E1332,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 3-methyl"},"Phenol, 3-methyl","Phenol, 3-methyl","苯酚，3-甲基"]
[null,{"$f":"IF($B$1=\"English\",C1333,IF($B$1=\"Deutsch\",D1333,IF($B$1=\"中文\",E1333,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-methyl"},"Phenol, 4-methyl","Phenol, 4-methyl","苯酚，4-甲基"]
[null,{"$f":"IF($B$1=\"English\",C1334,IF($B$1=\"Deutsch\",D1334,IF($B$1=\"中文\",E1334,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated Naphtalene (PCN)"},"Polychlorinated Naphtalene (PCN)","Polychloriertes Naphtalen (PCN)","聚氯化萘（ PCN ）"]
[null,{"$f":"IF($B$1=\"English\",C1335,IF($B$1=\"Deutsch\",D1335,IF($B$1=\"中文\",E1335,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"any intentionally added content"},"any intentionally added content","jeglicher absichtlich beigefügter Bestandteil","任何有意添加的成分"]
[null,{"$f":"IF($B$1=\"English\",C1336,IF($B$1=\"Deutsch\",D1336,IF($B$1=\"中文\",E1336,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloromethyl-methylether (CMME) "},"Chloromethyl-methylether (CMME) ","Chlormethyl-methylether (CMME) ","氯甲基甲醚（ CMME ）"]
[null,{"$f":"IF($B$1=\"English\",C1337,IF($B$1=\"Deutsch\",D1337,IF($B$1=\"中文\",E1337,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Depleted uranium"},"Depleted uranium","Abgereichertes Uran","贫铀"]
[null,{"$f":"IF($B$1=\"English\",C1338,IF($B$1=\"Deutsch\",D1338,IF($B$1=\"中文\",E1338,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde"},"Formaldehyde","Formaldehyd","甲醛"]
[null,{"$f":"IF($B$1=\"English\",C1339,IF($B$1=\"Deutsch\",D1339,IF($B$1=\"中文\",E1339,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dodecachloropentacyclo-1,3,4-Metheno-1H-cyclobuta(cd)pentalene, Mirex"},"Dodecachloropentacyclo-1,3,4-Metheno-1H-cyclobuta(cd)pentalene, Mirex","Dodecachloropentacyclo-1,3,4-Metheno-1H-cyclobuta(cd)pentalene, Mirex","十二氯代八氢-1，3，4-次甲基-1H-环丁并(c，d)双茂，灭蚁灵"]
[null,{"$f":"IF($B$1=\"English\",C1340,IF($B$1=\"Deutsch\",D1340,IF($B$1=\"中文\",E1340,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorobenzene"},"Hexachlorobenzene","Hexachlorobenzen","六氯苯"]
[null,{"$f":"IF($B$1=\"English\",C1341,IF($B$1=\"Deutsch\",D1341,IF($B$1=\"中文\",E1341,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-Nitrosamines "},"N-Nitrosamines ","N-Nitrosamine","亚硝胺"]
[null,{"$f":"IF($B$1=\"English\",C1342,IF($B$1=\"Deutsch\",D1342,IF($B$1=\"中文\",E1342,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorobenzene "},"Pentachlorobenzene ","Pentachlorobenzen","五氯苯"]
[null,{"$f":"IF($B$1=\"English\",C1343,IF($B$1=\"Deutsch\",D1343,IF($B$1=\"中文\",E1343,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrachlorobenzene, all members "},"Tetrachlorobenzene, all members ","Tetrachlorobenzen, alle Vertreter","四氯苯，所有同分异构体"]
[null,{"$f":"IF($B$1=\"English\",C1344,IF($B$1=\"Deutsch\",D1344,IF($B$1=\"中文\",E1344,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrafluoromethane"},"Tetrafluoromethane","Tetrafluormethan","四氟"]
[null,{"$f":"IF($B$1=\"English\",C1345,IF($B$1=\"Deutsch\",D1345,IF($B$1=\"中文\",E1345,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris...... ,"},"Tris...... ,","Tris...... ,","三...... ，"]
[null,{"$f":"IF($B$1=\"English\",C1346,IF($B$1=\"Deutsch\",D1346,IF($B$1=\"中文\",E1346,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alpha-Naphthylamine"},"Alpha-Naphthylamine","Alpha-Naphthylamin","α-萘胺"]
[null,{"$f":"IF($B$1=\"English\",C1347,IF($B$1=\"Deutsch\",D1347,IF($B$1=\"中文\",E1347,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethyleneimine"},"Ethyleneimine","Ethylenimin","亚胺"]
[null,{"$f":"IF($B$1=\"English\",C1348,IF($B$1=\"Deutsch\",D1348,IF($B$1=\"中文\",E1348,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beta-Propiolactone"},"Beta-Propiolactone","Beta-Propiolacton","β-丙内酯"]
[null,{"$f":"IF($B$1=\"English\",C1349,IF($B$1=\"Deutsch\",D1349,IF($B$1=\"中文\",E1349,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Acetylaminofluorene"},"2-Acetylaminofluorene","2-Acetylaminofluoren","2-乙酰氨基芴"]
[null,{"$f":"IF($B$1=\"English\",C1350,IF($B$1=\"Deutsch\",D1350,IF($B$1=\"中文\",E1350,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Dimethyl-aminoazobenzene"},"4-Dimethyl-aminoazobenzene","4-Dimethylaminoazobenzen","4-二甲基氨基偶氮苯"]
[null,{"$f":"IF($B$1=\"English\",C1351,IF($B$1=\"Deutsch\",D1351,IF($B$1=\"中文\",E1351,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dibromo-3-chloropropane"},"1,2-dibromo-3-chloropropane","1,2-dibrom-3-chlorpropan","1,2-二溴-3-氯丙烷"]
[null,{"$f":"IF($B$1=\"English\",C1352,IF($B$1=\"Deutsch\",D1352,IF($B$1=\"中文\",E1352,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Banned in Production"},"Banned in Production","Verboten in der Produktion","禁止在生产"]
[null,{"$f":"IF($B$1=\"English\",C1353,IF($B$1=\"Deutsch\",D1353,IF($B$1=\"中文\",E1353,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,003% by weight(30 ppm) of the finished textile/leather product Remark 1"},"0,003% by weight(30 ppm) of the finished textile/leather product Remark 1","0,003 Gewichts-% (30 ppm) des fertigen Textil-/Lederprodukts Anmerkung 1","成品纺织/皮革产品中重量百分比 0.003 ％(30PPM) - 见备注1"]
[null,{"$f":"IF($B$1=\"English\",C1354,IF($B$1=\"Deutsch\",D1354,IF($B$1=\"中文\",E1354,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The equivalent 0,1% by weight  (1 000 ppm) of tin in a material "},"The equivalent 0,1% by weight  (1 000 ppm) of tin in a material ","Entsprechend 0,1 Gewichts-% (1 000 ppm) Zinn im Material ","在材料中锡的重量百分比相当于0.1％(1 000 ppm)"]
[null,{"$f":"IF($B$1=\"English\",C1355,IF($B$1=\"Deutsch\",D1355,IF($B$1=\"中文\",E1355,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beryllium"},"Beryllium","Beryllium","铍"]
[null,{"$f":"IF($B$1=\"English\",C1356,IF($B$1=\"Deutsch\",D1356,IF($B$1=\"中文\",E1356,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beryllium Oxide"},"Beryllium Oxide","Berylliumoxid","氧化铍"]
[null,{"$f":"IF($B$1=\"English\",C1357,IF($B$1=\"Deutsch\",D1357,IF($B$1=\"中文\",E1357,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethylene oxide"},"Ethylene oxide","Ethylenoxid","环氧乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1358,IF($B$1=\"Deutsch\",D1358,IF($B$1=\"中文\",E1358,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Explosives"},"Explosives","Explosive Stoffe","爆炸物"]
[null,{"$f":"IF($B$1=\"English\",C1359,IF($B$1=\"Deutsch\",D1359,IF($B$1=\"中文\",E1359,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methylethyl ketone (MEK)"},"Methylethyl ketone (MEK)","Methylethylketon (MEK)","甲基乙基酮（MEK）"]
[null,{"$f":"IF($B$1=\"English\",C1360,IF($B$1=\"Deutsch\",D1360,IF($B$1=\"中文\",E1360,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrabromobisphenol A, 2,2-Bis(3,5-dibromo-4-hydroxyphenyl)propane (TBBPA)"},"Tetrabromobisphenol A, 2,2-Bis(3,5-dibromo-4-hydroxyphenyl)propane (TBBPA)","Tetrabrombisphenol A, 2,2-Bis(3,5-dibromo-4-hydroxyphenyl)propan (TBBPA)","四溴双酚A ， 2,2-双（3,5-二溴-4-羟基苯基）丙烷（四溴双酚A ）"]
[null,{"$f":"IF($B$1=\"English\",C1361,IF($B$1=\"Deutsch\",D1361,IF($B$1=\"中文\",E1361,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polyvinylchloride (PVC)"},"Polyvinylchloride (PVC)","Polyvinylchlorid (PVC)","聚氯乙烯（PVC）"]
[null,{"$f":"IF($B$1=\"English\",C1362,IF($B$1=\"Deutsch\",D1362,IF($B$1=\"中文\",E1362,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Brominated Flame Retardants (other than those specified in other sections of this standard)"},"Brominated Flame Retardants (other than those specified in other sections of this standard)","Bromierte Flammschutzmittel (abweichend von in anderen Abschnitten dieser Norm spezifizierten Flammschutzmitteln)","溴化阻燃剂（该标准的其他部分另有规定时除外）"]
[null,{"$f":"IF($B$1=\"English\",C1363,IF($B$1=\"Deutsch\",D1363,IF($B$1=\"中文\",E1363,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorinated Flame Retardants (other than those specified in other sections of this standard)"},"Chlorinated Flame Retardants (other than those specified in other sections of this standard)","Chloriertes Flammschutzmittel (abweichend von in anderen Abschnitten dieser Norm spezifizierten Flammschutzmitteln)","氯化阻燃剂（该标准的其他部分另有规定时除外）"]
[null,{"$f":"IF($B$1=\"English\",C1364,IF($B$1=\"Deutsch\",D1364,IF($B$1=\"中文\",E1364,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorobutadiene"},"Hexachlorobutadiene","Hexachlorbutadien","六氯丁二烯"]
[null,{"$f":"IF($B$1=\"English\",C1365,IF($B$1=\"Deutsch\",D1365,IF($B$1=\"中文\",E1365,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nitrogentrifluoride"},"Nitrogentrifluoride","Nitrogentrifluorid","三氟化氮"]
[null,{"$f":"IF($B$1=\"English\",C1366,IF($B$1=\"Deutsch\",D1366,IF($B$1=\"中文\",E1366,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulphur hexafluoride"},"Sulphur hexafluoride","Schwefelhexafluorid","六氟化硫"]
[null,{"$f":"IF($B$1=\"English\",C1367,IF($B$1=\"Deutsch\",D1367,IF($B$1=\"中文\",E1367,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Azo compound"},"Azo compound","Azo-Verbindung","偶氮化合物"]
[null,{"$f":"IF($B$1=\"English\",C1368,IF($B$1=\"Deutsch\",D1368,IF($B$1=\"中文\",E1368,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-chloro-o-toluidine"},"4-chloro-o-toluidine","4-chlor-o-toluidin","4-氯 - 邻 - 甲苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1369,IF($B$1=\"Deutsch\",D1369,IF($B$1=\"中文\",E1369,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-nitro-o-toluidine"},"5-nitro-o-toluidine","5-nitro-o-toluidin","5-硝基 - 邻甲苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1370,IF($B$1=\"Deutsch\",D1370,IF($B$1=\"中文\",E1370,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-chloroaniline"},"4-chloroaniline","4-chloranilin","4-氯苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1371,IF($B$1=\"Deutsch\",D1371,IF($B$1=\"中文\",E1371,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-methoxy-m-phenylenediamine"},"4-methoxy-m-phenylenediamine","4-methoxy-m-phenylendiamin","4-甲氧基 - 间 - 苯二胺"]
[null,{"$f":"IF($B$1=\"English\",C1372,IF($B$1=\"Deutsch\",D1372,IF($B$1=\"中文\",E1372,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3'-dichlorobenzidine"},"3,3'-dichlorobenzidine","3,3'-dichlorbenzidin","3,3′-二氯联苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1373,IF($B$1=\"Deutsch\",D1373,IF($B$1=\"中文\",E1373,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3'-dimethoxybenzidine"},"3,3'-dimethoxybenzidine","3,3'-dimethoxybenzidin","3,3’-二甲氧基联苯胺 "]
[null,{"$f":"IF($B$1=\"English\",C1374,IF($B$1=\"Deutsch\",D1374,IF($B$1=\"中文\",E1374,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3'-dimethylbenzidine"},"3,3'-dimethylbenzidine","3,3'-dimethylbenzidin","3,3’-联邻甲苯胺 "]
[null,{"$f":"IF($B$1=\"English\",C1375,IF($B$1=\"Deutsch\",D1375,IF($B$1=\"中文\",E1375,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-thiodianiline"},"4,4'-thiodianiline","4,4'-thiodianilin","4,4´-硫代二苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1376,IF($B$1=\"Deutsch\",D1376,IF($B$1=\"中文\",E1376,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4,5-trimethylaniline"},"2,4,5-trimethylaniline","2,4,5-trimethylanilin","2,4,5-三甲基苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1377,IF($B$1=\"Deutsch\",D1377,IF($B$1=\"中文\",E1377,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"DBT"},"DBT","DBT","DBT"]
[null,{"$f":"IF($B$1=\"English\",C1378,IF($B$1=\"Deutsch\",D1378,IF($B$1=\"中文\",E1378,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyltin oxide"},"Dibutyltin oxide","Dibutylzinnoxid","二丁基氧化锡"]
[null,{"$f":"IF($B$1=\"English\",C1379,IF($B$1=\"Deutsch\",D1379,IF($B$1=\"中文\",E1379,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyltin diacetate"},"Dibutyltin diacetate","Dibutylzinndiacetat","二乙酸二丁基锡"]
[null,{"$f":"IF($B$1=\"English\",C1380,IF($B$1=\"Deutsch\",D1380,IF($B$1=\"中文\",E1380,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyltin dilaurate "},"Dibutyltin dilaurate ","Dibutylzinndilaurat ","二月桂酸二丁基"]
[null,{"$f":"IF($B$1=\"English\",C1381,IF($B$1=\"Deutsch\",D1381,IF($B$1=\"中文\",E1381,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyltin maleate "},"Dibutyltin maleate ","Dibutylzinnmaleat ","马来酸二丁锡"]
[null,{"$f":"IF($B$1=\"English\",C1382,IF($B$1=\"Deutsch\",D1382,IF($B$1=\"中文\",E1382,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other dibutyltin compounds"},"Other dibutyltin compounds","Andere Dibutylzinn-Verbindungen","其他二丁基锡化合物"]
[null,{"$f":"IF($B$1=\"English\",C1383,IF($B$1=\"Deutsch\",D1383,IF($B$1=\"中文\",E1383,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"DOT"},"DOT","DOT","DOT"]
[null,{"$f":"IF($B$1=\"English\",C1384,IF($B$1=\"Deutsch\",D1384,IF($B$1=\"中文\",E1384,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioctyl Tin Oxide "},"Dioctyl Tin Oxide ","Dioctylzinnoxide ","辛锡氧化物"]
[null,{"$f":"IF($B$1=\"English\",C1385,IF($B$1=\"Deutsch\",D1385,IF($B$1=\"中文\",E1385,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioctyltin dilaurate "},"Dioctyltin dilaurate ","Dioctylzinndilaurat ","二辛基锡二月桂酸"]
[null,{"$f":"IF($B$1=\"English\",C1386,IF($B$1=\"Deutsch\",D1386,IF($B$1=\"中文\",E1386,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Other Dioctyltin compounds"},"Other Dioctyltin compounds","Andere Dioctylzinn-Verbindungen","其他二辛基锡化合物"]
[null,{"$f":"IF($B$1=\"English\",C1387,IF($B$1=\"Deutsch\",D1387,IF($B$1=\"中文\",E1387,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bisphenol-A (BPA)"},"Bisphenol-A (BPA)","Bisphenol-A (BPA)","双酚A（BPA）"]
[null,{"$f":"IF($B$1=\"English\",C1388,IF($B$1=\"Deutsch\",D1388,IF($B$1=\"中文\",E1388,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Halogenated Hydrocarbons"},"Halogenated Hydrocarbons","Halogenierte Kohlenwasserstoffe","卤代烃"]
[null,{"$f":"IF($B$1=\"English\",C1389,IF($B$1=\"Deutsch\",D1389,IF($B$1=\"中文\",E1389,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methyl bromide"},"Methyl bromide","Methylbromid","甲基溴"]
[null,{"$f":"IF($B$1=\"English\",C1390,IF($B$1=\"Deutsch\",D1390,IF($B$1=\"中文\",E1390,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorobromomethane"},"Chlorobromomethane","Chlorbrommethan","溴氯甲烷"]
[null,{"$f":"IF($B$1=\"English\",C1391,IF($B$1=\"Deutsch\",D1391,IF($B$1=\"中文\",E1391,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"nPB (n-bromopropane , 1-Bromopropane)"},"nPB (n-bromopropane , 1-Bromopropane)","nPB (n-brompropan, 1-Brompropan)","正丙基溴（正溴丙烷，1-溴丙烷）"]
[null,{"$f":"IF($B$1=\"English\",C1392,IF($B$1=\"Deutsch\",D1392,IF($B$1=\"中文\",E1392,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrachloroethylene (perchloroethylene) "},"Tetrachloroethylene (perchloroethylene) ","Tetrachlorethylen (perchlorethylen) ","四氯乙烯（四氯乙烯）"]
[null,{"$f":"IF($B$1=\"English\",C1393,IF($B$1=\"Deutsch\",D1393,IF($B$1=\"中文\",E1393,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichloroethylene"},"Trichloroethylene","Trichlorethylen","三氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C1394,IF($B$1=\"Deutsch\",D1394,IF($B$1=\"中文\",E1394,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluorocarbons (FCs)"},"Fluorocarbons (FCs)","Fluorierte Kohlenstoffe ","碳氟化合物（FCS）"]
[null,{"$f":"IF($B$1=\"English\",C1395,IF($B$1=\"Deutsch\",D1395,IF($B$1=\"中文\",E1395,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyl dibromo diphenyl methane (DBBT)"},"Monomethyl dibromo diphenyl methane (DBBT)","Monomethyldibromdiphenylmethan (DBBT)","单甲基二溴二苯基甲烷（DBBT）"]
[null,{"$f":"IF($B$1=\"English\",C1396,IF($B$1=\"Deutsch\",D1396,IF($B$1=\"中文\",E1396,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctane acid (PFOA)"},"Perfluorooctane acid (PFOA)","Perfluoroctansäure (PFOA)","全氟辛酸（PFOA）"]
[null,{"$f":"IF($B$1=\"English\",C1397,IF($B$1=\"Deutsch\",D1397,IF($B$1=\"中文\",E1397,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated dibenzodioxins (PCDDs)"},"Polychlorinated dibenzodioxins (PCDDs)","Polychloriiertes Dibenzodioxin (PCDDs)","多氯二苯二恶英（PCDDs）"]
[null,{"$f":"IF($B$1=\"English\",C1398,IF($B$1=\"Deutsch\",D1398,IF($B$1=\"中文\",E1398,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorocyclohexane isomers (HCHs)"},"Hexachlorocyclohexane isomers (HCHs)","Hexachlorcyclohexanisomer (HCHs)","六氯环己烷异构体（六六六）"]
[null,{"$f":"IF($B$1=\"English\",C1399,IF($B$1=\"Deutsch\",D1399,IF($B$1=\"中文\",E1399,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Packaging"},"Packaging","Verpackung","包装"]
[null,{"$f":"IF($B$1=\"English\",C1400,IF($B$1=\"Deutsch\",D1400,IF($B$1=\"中文\",E1400,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C1401,IF($B$1=\"Deutsch\",D1401,IF($B$1=\"中文\",E1401,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Volatile Organic Compound (VOC)"},"Volatile Organic Compound (VOC)","Flüchtige organische Verbindung (VOC)","挥发性有机化合物（VOC）"]
[null,{"$f":"IF($B$1=\"English\",C1402,IF($B$1=\"Deutsch\",D1402,IF($B$1=\"中文\",E1402,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Halogen"},"Halogen","Halogen","卤素"]
[null,{"$f":"IF($B$1=\"English\",C1403,IF($B$1=\"Deutsch\",D1403,IF($B$1=\"中文\",E1403,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phthalate"},"Phthalate","Phthalat","邻苯二甲酸酯（盐）"]
[null,{"$f":"IF($B$1=\"English\",C1404,IF($B$1=\"Deutsch\",D1404,IF($B$1=\"中文\",E1404,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlorine and CFC/HCFC"},"Chlorine and CFC/HCFC","Chlor und CFC/HCFC (en.)","氯和CFC/HCFC （氟氯烃/含氢氟氯烃）"]
[null,{"$f":"IF($B$1=\"English\",C1405,IF($B$1=\"Deutsch\",D1405,IF($B$1=\"中文\",E1405,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(Cd + Pb + Hg + Cr6+) < 100 ppm;\nCd < 50ppm"},"(Cd + Pb + Hg + Cr6+) < 100 ppm;\nCd < 50ppm","(Cd + Pb + Hg + Cr6+) < 100 ppm;\nCd < 50ppm","(Cd + Pb + Hg + Cr6+) < 100 ppm;\nCd < 50ppm"]
[null,{"$f":"IF($B$1=\"English\",C1406,IF($B$1=\"Deutsch\",D1406,IF($B$1=\"中文\",E1406,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"VOC free ink for packaging print"},"VOC free ink for packaging print","VOC-frei Tinte für Verpackungsdruck","无VOC油墨包装印刷"]
[null,{"$f":"IF($B$1=\"English\",C1407,IF($B$1=\"Deutsch\",D1407,IF($B$1=\"中文\",E1407,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Br:900 ppm, Cl:900 ppm, and Br+Cl :1500 ppm "},"Br:900 ppm, Cl:900 ppm, and Br+Cl :1500 ppm ","Br:900 ppm, Cl:900 ppm, und Br+Cl :1500 ppm ","Br:900 ppm, Cl:900 ppm, 和 Br+Cl :1500 ppm "]
[null,{"$f":"IF($B$1=\"English\",C1408,IF($B$1=\"Deutsch\",D1408,IF($B$1=\"中文\",E1408,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The packaging material is free from chlorine and CFC/HCFC"},"The packaging material is free from chlorine and CFC/HCFC","Das Verpackungsmaterial ist frei von Chlor und CFC/HCFC (en.)","包装材料不含氯和CFC/HCFC （氟氯烃/含氢氟氯烃）"]
[null,{"$f":"IF($B$1=\"English\",C1409,IF($B$1=\"Deutsch\",D1409,IF($B$1=\"中文\",E1409,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % w/w"},"0,1 % w/w","0,1 % w/w","0,1 % w/w （质量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C1410,IF($B$1=\"Deutsch\",D1410,IF($B$1=\"中文\",E1410,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"in plastic and elastomer parts"},"in plastic and elastomer parts","in Kunststoff- und Elastomer-Teilen","塑料和橡胶部件"]
[null,{"$f":"IF($B$1=\"English\",C1411,IF($B$1=\"Deutsch\",D1411,IF($B$1=\"中文\",E1411,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"US customer requirement"},"US customer requirement","US Kundenanforderung","美国的客户需求"]
[null,{"$f":"IF($B$1=\"English\",C1412,IF($B$1=\"Deutsch\",D1412,IF($B$1=\"中文\",E1412,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"method of measurement\n\nPlasticizer = DIN EN ISO 14389\nHeavy metals =  RoHS test\nPAH = ZEK 01.4-08"},"method of measurement\n\nPlasticizer = DIN EN ISO 14389\nHeavy metals =  RoHS test\nPAH = ZEK 01.4-08","Messmethode\n\nWeichmacher = DIN EN ISO 14389\nSchwermetalle =  RoHS test\nPAH = ZEK 01.4-08","检测方法\n\n增塑剂= DIN EN ISO 14389\n重金属= RoHS检测\nPAH = ZEK 01.4-08"]
[null,{"$f":"IF($B$1=\"English\",C1413,IF($B$1=\"Deutsch\",D1413,IF($B$1=\"中文\",E1413,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyl phthalate (DBP)"},"Dibutyl phthalate (DBP)","Dibutylphthalat (DBP)","邻苯二甲酸二丁酯（DBP）"]
[null,{"$f":"IF($B$1=\"English\",C1414,IF($B$1=\"Deutsch\",D1414,IF($B$1=\"中文\",E1414,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ROHS Future (Register 5a)"},"ROHS Future (Register 5a)","ROHS Future (Register 5a)","未来ROHS（工作表5a）"]
[null,{"$f":"IF($B$1=\"English\",C1415,IF($B$1=\"Deutsch\",D1415,IF($B$1=\"中文\",E1415,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials for electrical and electronic devices that are subject to EU-ROHS Future"},"All materials for electrical and electronic devices that are subject to EU-ROHS Future","Alle Materialien für Elektro- und Elektronikgeräte, die unter EU-ROHS Future fallen ","所有适用于欧盟未来ROHS的电气和电子设备用材料"]
[null,{"$f":"IF($B$1=\"English\",C1416,IF($B$1=\"Deutsch\",D1416,IF($B$1=\"中文\",E1416,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2009/251/EC\nThis Decision is applicable until 15 March 2010.\nincluded in Reach"},"2009/251/EC\nThis Decision is applicable until 15 March 2010.\nincluded in Reach","2009/251/EC\nDiese Entscheidung ist gültig bis 15. März 2010. Integriert in Reach"," 2009/251/EC\n这个决定适用到2010年3月15日为止。\n包含在REACH"]
[null,{"$f":"IF($B$1=\"English\",C1417,IF($B$1=\"Deutsch\",D1417,IF($B$1=\"中文\",E1417,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"=- thermal insulations\n- friction coatings\n- seals\n- building materials"},"=- thermal insulations\n- friction coatings\n- seals\n- building materials","Wärmeisolierung\nGleitbeschichtung\nVersiegelungen\nBaumaterialien"," = - 隔热材料\n - 摩擦涂层\n - 密封件\n - 建筑材料"]
[null,{"$f":"IF($B$1=\"English\",C1418,IF($B$1=\"Deutsch\",D1418,IF($B$1=\"中文\",E1418,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biocide used in packaging against mold "},"Biocide used in packaging against mold ","Biozide verwendet in Verpackungen gegen Schimmel","包装用霉菌杀菌剂"]
[null,{"$f":"IF($B$1=\"English\",C1419,IF($B$1=\"Deutsch\",D1419,IF($B$1=\"中文\",E1419,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- elastomers\n- impregnation textiles\n- chromium plating\n- lithography\n- fire fighting foam\n- hydraulic fluids"},"- elastomers\n- impregnation textiles\n- chromium plating\n- lithography\n- fire fighting foam\n- hydraulic fluids","- Elastomere\n- Impregnierte Textilien\n- Chrombeschichten\n- Lithographie\n- Feuerlöschschaum\n- Hydraulikflüssigkeit","“ - 弹性体\n - 浸渍纺织品\n - 镀铬\n - 光刻\n - 消防泡沫\n - 液压油"]
[null,{"$f":"IF($B$1=\"English\",C1420,IF($B$1=\"Deutsch\",D1420,IF($B$1=\"中文\",E1420,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Persistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"Persistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010","Persistente organische Schadstoffe (POP), Richtlinie (EG) Nr. 850/2004, 757/2010","持久性有机污染物（POP） ，法规（EC） 850/2004， 757/2010"]
[null,{"$f":"IF($B$1=\"English\",C1421,IF($B$1=\"Deutsch\",D1421,IF($B$1=\"中文\",E1421,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Contamination in steel"},"Contamination in steel","Kontamination im Stahl","钢铁中的污染"]
[null,{"$f":"IF($B$1=\"English\",C1422,IF($B$1=\"Deutsch\",D1422,IF($B$1=\"中文\",E1422,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- coolants\n- firefighting agents\n- cleaning agents"},"- coolants\n- firefighting agents\n- cleaning agents","- Kühlmittel\n- Feuerlöschmittel\n- Reinigungsmittel"," - 冷却液\n - 消防剂\n - 清洁剂"]
[null,{"$f":"IF($B$1=\"English\",C1423,IF($B$1=\"Deutsch\",D1423,IF($B$1=\"中文\",E1423,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulation (EC) No 1005/2009"},"Regulation (EC) No 1005/2009","Richtlinie (EG) Nr. 1005/2009","法规 (EC) No 1005/2009"]
[null,{"$f":"IF($B$1=\"English\",C1424,IF($B$1=\"Deutsch\",D1424,IF($B$1=\"中文\",E1424,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"=- Flame retardants\n- Plasticizers\n- Lubricants\n- Coolants\n- Solvents"},"=- Flame retardants\n- Plasticizers\n- Lubricants\n- Coolants\n- Solvents","=- Flammschutzmittel\n- Weichmacher\n- Schmierstoffe\n- Kühlmittel\n- Lösemittel","’ = - 阻燃剂\n - 增塑剂\n - 润滑剂\n - 冷却液\n - 溶剂"]
[null,{"$f":"IF($B$1=\"English\",C1425,IF($B$1=\"Deutsch\",D1425,IF($B$1=\"中文\",E1425,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Halogen Free Industry Standard, \nref IEC 6124-2-21"},"Halogen Free Industry Standard, \nref IEC 6124-2-21","Internationale Norm zur Definition von \"Halogen-frei\"  gem.\nIEC 61249-2-21","无卤素行业标准，参考IEC 6124-2-21 "]
[null,{"$f":"IF($B$1=\"English\",C1426,IF($B$1=\"Deutsch\",D1426,IF($B$1=\"中文\",E1426,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Flame retardants"},"Flame retardants","Flammschutzmittel","阻燃剂"]
[null,{"$f":"IF($B$1=\"English\",C1427,IF($B$1=\"Deutsch\",D1427,IF($B$1=\"中文\",E1427,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Persistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"Persistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010","Persistente organische Schadstoffe (POP), Richtlinie (EG) Nr. 850/2004, 757/2010","持久性有机污染物（ POP ） ，法规（EC） 850/2004， 757/2010"]
[null,{"$f":"IF($B$1=\"English\",C1428,IF($B$1=\"Deutsch\",D1428,IF($B$1=\"中文\",E1428,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All materials for ships or equipment for ships impacted by the Resolution MEPC.197(62)"},"All materials for ships or equipment for ships impacted by the Resolution MEPC.197(62)","Alle Materialien für Schiffe oder Einrichtungen von Schiffen die unter die Resolution MEPC.197(62) fallen","国际海事组织《MEPC.197(62)导则》适用的船舶材料或船舶设备"]
[null,{"$f":"IF($B$1=\"English\",C1429,IF($B$1=\"Deutsch\",D1429,IF($B$1=\"中文\",E1429,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Third-party products, manufactured without or with Bosch spezification by a third-party manufacturer and sold under the name of the external manufacturer or under the label Bosch or another Bosch brand. Applies also to products purchased only once. These products have to comply with the ELV and/or GADSL."},"Third-party products, manufactured without or with Bosch spezification by a third-party manufacturer and sold under the name of the external manufacturer or under the label Bosch or another Bosch brand. Applies also to products purchased only once. These products have to comply with the ELV and/or GADSL.","Fremderzeugnisse, die ohne oder mit Bosch Spezifikation bei einem Fremdhersteller gebaut werden und unter dem Namen des externen Herstellers oder unter dem Label Bosch oder einer anderen Bosch eignen Marke vertrieben werden. Zutreffend auch für einmalig zugekaufte Erzeugnisse. Diese Erzeugnisse fallen unter ELV bzw. GADSL","第三方的产品，指由第三方制造的产品，无论有或没有参照博世规范，也无论是以外部制造商的名义销售，或以博世的标签已经博世旗下的其它品牌销售。也适用于一次性购买的产品。这些产品都必须符合ELV和/或GADSL 。"]
[null,{"$f":"IF($B$1=\"English\",C1430,IF($B$1=\"Deutsch\",D1430,IF($B$1=\"中文\",E1430,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Third-party products, manufactured without or with Bosch spezification by a third-party manufacturer and sold under the name of the external manufacturer or under the label Bosch or another Bosch brand. Applies also to products purchased only once. These products have to comply with EU-RoHS and EU-REACH."},"Third-party products, manufactured without or with Bosch spezification by a third-party manufacturer and sold under the name of the external manufacturer or under the label Bosch or another Bosch brand. Applies also to products purchased only once. These products have to comply with EU-RoHS and EU-REACH.","Fremderzeugnisse, die ohne oder mit Bosch Spezifikation bei einem Fremdhersteller gebaut werden und unter dem Namen des externen Herstellers oder unter dem Label Bosch oder einer anderen Bosch eignen Marke vertrieben werden. Zutreffend auch für einmalig zugekaufte Erzeugnisse. Diese Erzeugnisse müssen EU-RoHS und EU-REACh einhalten.","第三方的产品，指由第三方制造的产品，无论有或没有参照博世规范，也无论是以外部制造商的名义销售，或以博世的标签以及博世旗下的其它品牌销售。也适用于一次性购买的产品。这些产品都必须符合RoHS和/或REACh 。"]
[null,{"$f":"IF($B$1=\"English\",C1431,IF($B$1=\"Deutsch\",D1431,IF($B$1=\"中文\",E1431,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alterations until 2014-07-14 and SVHC candidats list of 2016-06-20"},"Alterations until 2014-07-14 and SVHC candidats list of 2016-06-20","Änderungen bis 14.07.14 und SVHC Kandidatenliste vom 15.06.2015","直到 2014-07-14 的替代，和 2015-06-15 的SVHC候选清单"]
[null,{"$f":"IF($B$1=\"English\",C1432,IF($B$1=\"Deutsch\",D1432,IF($B$1=\"中文\",E1432,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included (E)\n- changed (C) \n"},"Entry\n- included (E)\n- changed (C) \n","Eintrag aufgenommen (E) - geändert (C) ","录入记录\n-首次录入(E)\n-更新(C)"]
[null,{"$f":"IF($B$1=\"English\",C1433,IF($B$1=\"Deutsch\",D1433,IF($B$1=\"中文\",E1433,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. In deviation, it is permissible to produce, place on the market or use materials and preparations that contain SCCP in a concentration of less than 1 weight-%.\n2. In deviation, the manufacture, placing on the market and the use of the following purposes are permitted in as far as the member states of the commission report on their proceedings in eliminating SCCP every four years: \n a) Flame retardants for rubber used in conveyor belts in the extractive industries; \n b) Flame retardants in sealing compounds. \n3. Products containing SCCP that have been produced before 2012-07-10, may be merchandised until 2013-01-10. \n4. Products containing SCCP that have already been used before or on 2012-07-10 may be merchandised and used. \n5. Article 4 Sect. 2 Sub-chapters 3 and 4 apply to products in accordance with numbers 1 and 2. \n\nAs soon as new information on use and safe alternative materials and technologies are available the commission will revised the deviations as per number 2 in order to cease the use of SCCP."},"1. In deviation, it is permissible to produce, place on the market or use materials and preparations that contain SCCP in a concentration of less than 1 weight-%.\n2. In deviation, the manufacture, placing on the market and the use of the following purposes are permitted in as far as the member states of the commission report on their proceedings in eliminating SCCP every four years: \n a) Flame retardants for rubber used in conveyor belts in the extractive industries; \n b) Flame retardants in sealing compounds. \n3. Products containing SCCP that have been produced before 2012-07-10, may be merchandised until 2013-01-10. \n4. Products containing SCCP that have already been used before or on 2012-07-10 may be merchandised and used. \n5. Article 4 Sect. 2 Sub-chapters 3 and 4 apply to products in accordance with numbers 1 and 2. \n\nAs soon as new information on use and safe alternative materials and technologies are available the commission will revised the deviations as per number 2 in order to cease the use of SCCP.","1. Abweichend dürfen Stoffe und Zubereitungen, die SCCP in Konzentrationen von weniger als 1 Gew.-% enthalten, hergestellt, in Verkehr gebracht und verwendet werden.\n2. Abweichend sind die Herstellung, das Inverkehrbringen und die Verwendung für die nachstehend genannten Zwecke gestattet, sofern die Mitgliedstaaten der Kommission bis spätestens 2015 und anschließend alle vier Jahre über ihre Fortschritte bei der Beseitigung von SCCP Bericht erstatten: \n a) Flammschutzmittel für in Förderbändern in der mineralgewinnenden Industrie verwendetes Gummi; \n b) Flammschutzmittel in Dichtungsmassen. \n3. SCCP als Bestandteil enthaltende Artikel, die vor dem oder am 10. Juli 2012 hergestellt wurden, dürfen bis 10. Januar 2013 in Verkehr gebracht und verwendet werden. \n4. SCCP als Bestandteil enthaltende Artikel, die vor dem oder am 10. Juli 2012 bereits verwendet wurden, dürfen in Verkehr gebracht und verwendet werden. \n5. Artikel 4 Absatz 2 Unterabsätze 3 und 4 finden auf Artikel gemäß den Nummern 1 und 2 Anwendung. \n\nSobald neue Informationen über Verwendungen und sicherere alternative Stoffe oder Technologien vorliegen, überprüft die Kommission die Abweichungen gemäß Nummer 2, damit die Verwendungen von SCCP schrittweise eingestellt werden können.","1.在特殊情况下，允许生产，销售或使用含重量百分比小于1％的SCCP（短链氯化石蜡）的配制品的材料和制剂包。\n2.在特殊情况下，只要欧盟成员国每四年报告一次消除SCCP的进程，制造，销售和下列用途的使用是允许的，：\n a）阻燃剂，用于采掘业输送带用橡胶上;\n b）密封化合物的阻燃剂。\n3. 2012-07-10之前生产的产品如果含SCCP，可继续销售到2013-01-10。\n4. 2012-07-10之前已投入使用的产品如果含SCCP，可继续生产 和使用（SCCP）。\n5.第4.2第三章和第四章适用于第1、2项中的产品。\n\n一旦有了新的安全使用信息和安全的替代材料和替代技术时，欧盟委员会将修订第2项豁免，以停止使用SCCP."]
[null,{"$f":"IF($B$1=\"English\",C1434,IF($B$1=\"Deutsch\",D1434,IF($B$1=\"中文\",E1434,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizer = DIN EN ISO 14389"},"Plasticizer = DIN EN ISO 14389","Weichmacher = DIN EN ISO 14389","增塑剂 = DIN EN ISO 14389"]
[null,{"$f":"IF($B$1=\"English\",C1435,IF($B$1=\"Deutsch\",D1435,IF($B$1=\"中文\",E1435,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"RoHS test"},"RoHS test","RoHS Test","RoHS 检测"]
[null,{"$f":"IF($B$1=\"English\",C1436,IF($B$1=\"Deutsch\",D1436,IF($B$1=\"中文\",E1436,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"AFP-GS-2014:01 PAK"},"AFP-GS-2014:01 PAK","AFP-GS-2014:01 PAK","AFP-GS-2014:01 PAK (GS标志认证中多环芳烃的检测和评估规范)"]
[null,{"$f":"IF($B$1=\"English\",C1437,IF($B$1=\"Deutsch\",D1437,IF($B$1=\"中文\",E1437,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Method of measurement\n\nPlasticizer = DIN EN ISO 14389\nHeavy metals =  RoHS test\nPAH = AFP-GS-2014:01 PAK"},"Method of measurement\n\nPlasticizer = DIN EN ISO 14389\nHeavy metals =  RoHS test\nPAH = AFP-GS-2014:01 PAK","Messmethoden\n\nWeichmacher = DIN EN ISO 14389\nSchwermetalle =  RoHS Test\nPAH = AFP-GS-2014:01 PAK","检测方法\n\n增塑剂 = DIN EN ISO 14389\n重金属 = RoHS检测\n多环芳烃 = AFP-GS-2014:01 PAK (GS标志认证中多环芳烃的检测和评估规范)"]
[null,{"$f":"IF($B$1=\"English\",C1438,IF($B$1=\"Deutsch\",D1438,IF($B$1=\"中文\",E1438,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[a]pyrene"},"Benzo[a]pyrene","Benzo[a]pyren","苯并[a]芘 "]
[null,{"$f":"IF($B$1=\"English\",C1439,IF($B$1=\"Deutsch\",D1439,IF($B$1=\"中文\",E1439,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[e]pyrene"},"Benzo[e]pyrene","Benzo[e]pyren","苯并[e]芘 "]
[null,{"$f":"IF($B$1=\"English\",C1440,IF($B$1=\"Deutsch\",D1440,IF($B$1=\"中文\",E1440,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[a]anthracene"},"Benzo[a]anthracene","Benzo[a]anthracen","苯并[a]蒽 "]
[null,{"$f":"IF($B$1=\"English\",C1441,IF($B$1=\"Deutsch\",D1441,IF($B$1=\"中文\",E1441,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[b]fluoranthene"},"Benzo[b]fluoranthene","Benzo[b]fluoranthen","苯并[b]荧蒽 "]
[null,{"$f":"IF($B$1=\"English\",C1442,IF($B$1=\"Deutsch\",D1442,IF($B$1=\"中文\",E1442,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[j]fluoranthene"},"Benzo[j]fluoranthene","Benzo[j]fluoranthen","苯并[j]荧蒽 "]
[null,{"$f":"IF($B$1=\"English\",C1443,IF($B$1=\"Deutsch\",D1443,IF($B$1=\"中文\",E1443,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[k]fluoranthene"},"Benzo[k]fluoranthene","Benzo[k]fluoranthen","苯并[k]荧蒽 "]
[null,{"$f":"IF($B$1=\"English\",C1444,IF($B$1=\"Deutsch\",D1444,IF($B$1=\"中文\",E1444,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chrysene"},"Chrysene","Chrysen","䓛"]
[null,{"$f":"IF($B$1=\"English\",C1445,IF($B$1=\"Deutsch\",D1445,IF($B$1=\"中文\",E1445,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibenzo[a,h]anthracene"},"Dibenzo[a,h]anthracene","Dibenzo[a,h]anthracen","二苯并[a,h]蒽(DBA)"]
[null,{"$f":"IF($B$1=\"English\",C1446,IF($B$1=\"Deutsch\",D1446,IF($B$1=\"中文\",E1446,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[ghi]perylene"},"Benzo[ghi]perylene","Benzo[ghi]perylen","苯并（ghi）北（二萘嵌苯）"]
[null,{"$f":"IF($B$1=\"English\",C1447,IF($B$1=\"Deutsch\",D1447,IF($B$1=\"中文\",E1447,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"lndeno[1‚2,3-cd]pyrene "},"lndeno[1‚2,3-cd]pyrene ","lndeno[1‚2,3-cd]pyren ","茚苯（1,2,3-cd）芘"]
[null,{"$f":"IF($B$1=\"English\",C1448,IF($B$1=\"Deutsch\",D1448,IF($B$1=\"中文\",E1448,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acenaphthylene, \nAcenaphthene, \nFluorene, \nPhenanthrene, \nPyrene, \nAnthracene, \nFluoranthene"},"Acenaphthylene, \nAcenaphthene, \nFluorene, \nPhenanthrene, \nPyrene, \nAnthracene, \nFluoranthene","Acenaphthylen, \nAcenaphthen, \nFluoren, \nPhenanthren, \nPyren, \nAnthracen, \nFluoranthen","苊烯，\n苊，\n芴，\n菲，\n芘，\n蒽，\n荧蒽"]
[null,{"$f":"IF($B$1=\"English\",C1449,IF($B$1=\"Deutsch\",D1449,IF($B$1=\"中文\",E1449,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Naphtalene"},"Naphtalene","Naphthalin","萘"]
[null,{"$f":"IF($B$1=\"English\",C1450,IF($B$1=\"Deutsch\",D1450,IF($B$1=\"中文\",E1450,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sum 18 PAH"},"Sum 18 PAH","Summe 18 PAH","18种多环芳烃的总量"]
[null,{"$f":"IF($B$1=\"English\",C1451,IF($B$1=\"Deutsch\",D1451,IF($B$1=\"中文\",E1451,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For operating elements such as soft grips or switches the Bosch business division PT is allowed to demand that all below listed 18 PAK remain under the detection limit of 0,1PPM (PAK-free). The requirement “PAK-free” will then be agreed separately in the parts specifications or by an agreement/contract between supplier and PT. In all other cases the following limit values have to be met."},"For operating elements such as soft grips or switches the Bosch business division PT is allowed to demand that all below listed 18 PAK remain under the detection limit of 0,1PPM (PAK-free). The requirement “PAK-free” will then be agreed separately in the parts specifications or by an agreement/contract between supplier and PT. In all other cases the following limit values have to be met.","Für Bedienelemente wie z.B. Softgriffe oder Schalter kann die Bosch-PT Einheit zusätzlich einfordern, dass sämtliche unten aufgeführten 18 PAK unter der Nachweisgrenze von 0.1PPM liegen („PAK frei“). Die Forderung „PAK-frei“ wird dann separat in den Teilespezifikationen oder mittels einer Vereinbarung / Vertrag zwischen dem Lieferanten und Bosch-PT vereinbart werden. In allen anderen Fällen sind folgende Grenzwerte einzuhalten.","对于操作部件，如软触感把手或开关，博世PT事业部允许要求以下所列18种多环芳烃(PAH)的残留量均低于检测限0.1PPM（完全不含多环芳烃）。“完全不含多环芳烃”要求会在PT给供应商的零件规范或协议/合同中另外商定。其它情况下，应符合以下限值。"]
[null,{"$f":"IF($B$1=\"English\",C1452,IF($B$1=\"Deutsch\",D1452,IF($B$1=\"中文\",E1452,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"< 0.5 mg/kg (0,5 ppm)"},"< 0.5 mg/kg (0,5 ppm)","< 0.5 mg/kg (0,5 ppm)","< 0.5 mg/kg (0,5 ppm)"]
[null,{"$f":"IF($B$1=\"English\",C1453,IF($B$1=\"Deutsch\",D1453,IF($B$1=\"中文\",E1453,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sum < 10 mg/kg (10 ppm)"},"Sum < 10 mg/kg (10 ppm)","Summe < 10 mg/kg (10 ppm)","总和 < 10 mg/kg (10 ppm)"]
[null,{"$f":"IF($B$1=\"English\",C1454,IF($B$1=\"Deutsch\",D1454,IF($B$1=\"中文\",E1454,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"< 2 mg/kg (2 ppm)"},"< 2 mg/kg (2 ppm)","< 2 mg/kg (2 ppm)","< 2 mg/kg (2 ppm)"]
[null,{"$f":"IF($B$1=\"English\",C1455,IF($B$1=\"Deutsch\",D1455,IF($B$1=\"中文\",E1455,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sum < 10 mg/kg (10 ppm)"},"Sum < 10 mg/kg (10 ppm)","Summe < 10 mg/kg (10 ppm)","总和 < 10 mg/kg (10 ppm)"]
[null,{"$f":"IF($B$1=\"English\",C1456,IF($B$1=\"Deutsch\",D1456,IF($B$1=\"中文\",E1456,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Black plastic and elastomer \nparts, e.g. cables, grommets, soft grips;\nextender oil;\ncolors, carbon black"},"Black plastic and elastomer \nparts, e.g. cables, grommets, soft grips;\nextender oil;\ncolors, carbon black","Schwarze Kunststoffe und Elastomerteile \nz. B. Kabel, Gummidichtungen, Softgriffe;\nExtenderöl;\nFarben, Ruß","黑色塑料和弹性体零件，如电线， 垫圈，软触感把手；\n填充油；\n颜料，炭黑"]
[null,{"$f":"IF($B$1=\"English\",C1457,IF($B$1=\"Deutsch\",D1457,IF($B$1=\"中文\",E1457,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reach Annex XVII / AFP-GS-2014:01 PAK"},"Reach Annex XVII / AFP-GS-2014:01 PAK","Reach Anhang XVII / AFP-GS-2014:01 PAK","Reach 附录17 / AFP-GS-2014:01 PAK (GS标志认证中多环芳烃的测试和评估规范)"]
[null,{"$f":"IF($B$1=\"English\",C1458,IF($B$1=\"Deutsch\",D1458,IF($B$1=\"中文\",E1458,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"AFP-GS-2014:01 PAK"},"AFP-GS-2014:01 PAK","AFP-GS-2014:01 PAK","AFP-GS-2014:01 PAK (GS标志认证中多环芳烃的测试和评估规范)"]
[null,{"$f":"IF($B$1=\"English\",C1459,IF($B$1=\"Deutsch\",D1459,IF($B$1=\"中文\",E1459,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"please double click"},"please double click","bitte doppelt klicken","请双击"]
[null,{"$f":"IF($B$1=\"English\",C1460,IF($B$1=\"Deutsch\",D1460,IF($B$1=\"中文\",E1460,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters; 1,2-benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters with ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)"},"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters; 1,2-benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters with ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)","1,2-Benzendicarboxylsäure, Di-C6-10-alkylester; 1,2-Benzendicarboxylsäure, gemischte Decyl und Hexyl und Octyl-Diester mit ≥ 0.3% Dihexylphthalat (EC No. 201-559-5)","邻苯二甲酸二（C6-C6）烷基酯：(癸基，己基，辛基）酯与1，2-邻苯二甲酸的复合物且邻苯二甲酸二己酯含量≥ 0.3% (EC编码: 201-559-5)"]
[null,{"$f":"IF($B$1=\"English\",C1461,IF($B$1=\"Deutsch\",D1461,IF($B$1=\"中文\",E1461,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"plasticisers and lubricants, including use in adhesives, coatings, building material, cable compounding, polymer foils, PVC compounds"},"plasticisers and lubricants, including use in adhesives, coatings, building material, cable compounding, polymer foils, PVC compounds","Weichmacher und Schmiermittel, inkl. Verwendung in Klebern, Beschichtungen, Baustoffen, Kabelkompundierung, Polymerfolien, PVC-Vergussmassen","增塑剂和润滑油，应用于粘结剂，涂层，建筑材料，电缆膏，高分子箔片，PVC化学物"]
[null,{"$f":"IF($B$1=\"English\",C1462,IF($B$1=\"Deutsch\",D1462,IF($B$1=\"中文\",E1462,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2] [covering any of the individual stereoisomers of [1] and [2] or any combination thereof]"},"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2] [covering any of the individual stereoisomers of [1] and [2] or any combination thereof]","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxan [1], 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxan [2] [deckt alle einzelnen Stereoisomere von [1] und [2] ab oder jede mögliche ihrer Kombinationen]","[1] 5-二級丁基-2-(2,4-二甲基环己-3-烯-1-基)-5-甲基-1,3-二氧六环  [2] 5-二級丁基-2-(4,6-二甲基環 己-3-烯-1-基)-5-甲基-1,3-二氧六环  [包含以上[1]和[2]任何异构体或组合]"]
[null,{"$f":"IF($B$1=\"English\",C1463,IF($B$1=\"Deutsch\",D1463,IF($B$1=\"中文\",E1463,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substance Group"},"Substance Group","Stoffgruppe","物质组"]
[null,{"$f":"IF($B$1=\"English\",C1464,IF($B$1=\"Deutsch\",D1464,IF($B$1=\"中文\",E1464,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"fragrance ingredient"},"fragrance ingredient","Duft-Inhaltsstofffe","香味成分"]
[null,{"$f":"IF($B$1=\"English\",C1465,IF($B$1=\"Deutsch\",D1465,IF($B$1=\"中文\",E1465,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters; 1,2-benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters with ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)"},"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters; 1,2-benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters with ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)","1,2-Benzendicarboxylsäure, Di-C6-10-alkylester; 1,2-Benzendicarboxylsäure, gemischte Decyl und Hexyl und Octyl-Diester mit ≥ 0.3% Dihexylphthalat (EC No. 201-559-5)","邻苯二甲酸二（C6-C6）烷基酯：(癸基，己基，辛基）酯与1，2-邻苯二甲酸的复合物且邻苯二甲酸二己酯含量≥ 0.3% (EC编码: 201-559-5)"]
[null,{"$f":"IF($B$1=\"English\",C1466,IF($B$1=\"Deutsch\",D1466,IF($B$1=\"中文\",E1466,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"plasticisers and lubricants, including use in adhesives, coatings, building material, cable compounding, polymer foils, PVC compounds"},"plasticisers and lubricants, including use in adhesives, coatings, building material, cable compounding, polymer foils, PVC compounds","Weichmacher und Schmiermittel, inkl. Verwendung in Klebern, Beschichtungen, Baustoffen, Kabelkompundierung, Polymerfolien, PVC-Vergussmassen","增塑剂和润滑油，应用于粘结剂，涂层，建筑材料，电缆膏，高分子箔片，PVC化学物"]
[null,{"$f":"IF($B$1=\"English\",C1467,IF($B$1=\"Deutsch\",D1467,IF($B$1=\"中文\",E1467,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2015/863"},"2015/863","2015/863","2015/863"]
[null,{"$f":"IF($B$1=\"English\",C1468,IF($B$1=\"Deutsch\",D1468,IF($B$1=\"中文\",E1468,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EU-Regulation No. 1013/2006 and 1257/2013 on ship recycling"},"EU-Regulation No. 1013/2006 and 1257/2013 on ship recycling","EU-Verordnung Nr. 1013/2006 und 1257/2013 zum Schiffsrecycling","欧盟1013/2006和1257/2013号船舶回收法规"]
[null,{"$f":"IF($B$1=\"English\",C1469,IF($B$1=\"Deutsch\",D1469,IF($B$1=\"中文\",E1469,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Brominated Flame Retardant (HBCDD)"},"Brominated Flame Retardant (HBCDD)","Bromierte Flammschutzmittel (HBCDD)","溴系阻燃剂（六溴环十二烷 HBCDD)"]
[null,{"$f":"IF($B$1=\"English\",C1470,IF($B$1=\"Deutsch\",D1470,IF($B$1=\"中文\",E1470,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctane sulfonic acid (PFOS)"},"Perfluorooctane sulfonic acid (PFOS)","Perfluoroktansulfonsäure (PFOS)","全氟辛烷磺酸(PFOS)"]
[null,{"$f":"IF($B$1=\"English\",C1471,IF($B$1=\"Deutsch\",D1471,IF($B$1=\"中文\",E1471,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Bemerkungen","备注"]
[null,{"$f":"IF($B$1=\"English\",C1472,IF($B$1=\"Deutsch\",D1472,IF($B$1=\"中文\",E1472,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in REACH Annex 17 and Tab RB-General"},"listed in REACH Annex 17 and Tab RB-General","Ebenfalls unter REACH Anhang 17 und Tab RB-General gelistet","列在REACH附件17和表RB-General中"]
[null,{"$f":"IF($B$1=\"English\",C1473,IF($B$1=\"Deutsch\",D1473,IF($B$1=\"中文\",E1473,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"listed in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010","Ebenfalls im Tab RB-General,\nPersistente organische Schadstoffe (POP), Verordnung (EG) Nr. 850/2004, 757/2010","列在表RB-常规中，\n持久性有机污染物，第850/2004、757/2010号条例"]
[null,{"$f":"IF($B$1=\"English\",C1474,IF($B$1=\"Deutsch\",D1474,IF($B$1=\"中文\",E1474,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in Tab RB-General,\nRegulation (EC) No 1005/2009"},"listed in Tab RB-General,\nRegulation (EC) No 1005/2009","Ebenfalls im Tab RB-General,\nVerordnung (EG) Nr. 1005/2009 gelistet","列在表RB-常规中，\n(EC)第1005/2009号条例"]
[null,{"$f":"IF($B$1=\"English\",C1475,IF($B$1=\"Deutsch\",D1475,IF($B$1=\"中文\",E1475,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"REACH Annex 17 as \"Organic tin compounds\""},"REACH Annex 17 as \"Organic tin compounds\"","In REACH Anhang 17 als \"Zinnorganische Verbindungen\" gelistet","REACh附件17，“有机锡化合物”"]
[null,{"$f":"IF($B$1=\"English\",C1476,IF($B$1=\"Deutsch\",D1476,IF($B$1=\"中文\",E1476,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"listed in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010","Ebenfalls im Tab RB-General,\nPersistente organische Schadstoffe (POP), Verordnung (EG) Nr. 850/2004, 757/2010","列在表RB-常规中，\n持久性有机污染物，第850/2004、757/2010号条例"]
[null,{"$f":"IF($B$1=\"English\",C1477,IF($B$1=\"Deutsch\",D1477,IF($B$1=\"中文\",E1477,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"equivalent to RoHS limits,\nREACH Annex 17, REACH SVHC"},"equivalent to RoHS limits,\nREACH Annex 17, REACH SVHC","Entsprechend den RoHS Grenzwerten,\nREACH Anhang 17, REACH SVHC","相当于欧盟RoHS指令限值标准， REACH 附件17，REACH法规中的高度关注物质（SVHC）"]
[null,{"$f":"IF($B$1=\"English\",C1478,IF($B$1=\"Deutsch\",D1478,IF($B$1=\"中文\",E1478,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"equivalent to RoHS limits,\nREACH SVHC"},"equivalent to RoHS limits,\nREACH SVHC","Entsprechend den RoHS Grenzwerten,\nREACH SVHC","相当于欧盟RoHS指令限值标准， REACH法规中的高度关注物质（SVHC）"]
[null,{"$f":"IF($B$1=\"English\",C1479,IF($B$1=\"Deutsch\",D1479,IF($B$1=\"中文\",E1479,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"equivalent to RoHS limits,"},"equivalent to RoHS limits,","Entsprechend den RoHS Grenzwerten,","相当于欧盟RoHS指令限值标准"]
[null,{"$f":"IF($B$1=\"English\",C1480,IF($B$1=\"Deutsch\",D1480,IF($B$1=\"中文\",E1480,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"equivalent to RoHS limits,\nREACH Annex 17"},"equivalent to RoHS limits,\nREACH Annex 17","Entsprechend den RoHS Grenzwerten,\nREACH Anhang 17","相当于欧盟RoHS指令限值标准， REACH 附件17"]
[null,{"$f":"IF($B$1=\"English\",C1481,IF($B$1=\"Deutsch\",D1481,IF($B$1=\"中文\",E1481,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"equivalent to RoHS limits,\nREACH Annex 17"},"equivalent to RoHS limits,\nREACH Annex 17","Entsprechend den RoHS Grenzwerten,\nREACH Anhang 17","相当于欧盟RoHS指令限值标准， REACH 附件17"]
[null,{"$f":"IF($B$1=\"English\",C1482,IF($B$1=\"Deutsch\",D1482,IF($B$1=\"中文\",E1482,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"equivalent to RoHS limits,"},"equivalent to RoHS limits,","Entsprechend den RoHS Grenzwerten,","相当于欧盟RoHS指令限值标准"]
[null,{"$f":"IF($B$1=\"English\",C1483,IF($B$1=\"Deutsch\",D1483,IF($B$1=\"中文\",E1483,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in Tab DC"},"listed in Tab DC","Ebenfalls im Tab DC gelistet","收录在表格 DC 中"]
[null,{"$f":"IF($B$1=\"English\",C1484,IF($B$1=\"Deutsch\",D1484,IF($B$1=\"中文\",E1484,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in Tab RB-General"},"listed in Tab RB-General","Ebenfalls im Tab RB-General gelistet","列于表RB-常规"]
[null,{"$f":"IF($B$1=\"English\",C1485,IF($B$1=\"Deutsch\",D1485,IF($B$1=\"中文\",E1485,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"REACH Annex 17 as \"Alkanes, C 10 -C 13, chlorine (short-chain chlorinated paraffins)\""},"REACH Annex 17 as \"Alkanes, C 10 -C 13, chlorine (short-chain chlorinated paraffins)\"","REACH Anhang 17 als \"Alkane, C 10 -C 13 , Chlor (kurzkettige Chlorparaffine)\"","REACH 附件17， \"氯化烷烃(10-13个碳原子)；短链\n氯化石蜡\""]
[null,{"$f":"IF($B$1=\"English\",C1486,IF($B$1=\"Deutsch\",D1486,IF($B$1=\"中文\",E1486,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"listed in REACH Annex 14 and  REACH SVHC as \"Hexabromocyclododecane (HBCDD)\"\nlisted in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010"},"listed in REACH Annex 14 and  REACH SVHC as \"Hexabromocyclododecane (HBCDD)\"\nlisted in Tab RB-General,\nPersistent organic pollutants (POP), Regulation (EC) No 850/2004, 757/2010","Ebenfalls unter REACH Anhang 14 sowie REACH SVHC gelistet als \"Hexabromocyclododecan (HBCDD)\",\nTab RB-General,\nPersistente organische Schadstoffe (POP), Verordnung (EG) Nr. 850/2004, 757/2010","被列入REACH附件14，REACH SVHC为“六溴环十二烷(六溴环十二烷)”\n列在表RB-常规中，\n持久性有机污染物，第850/2004、757/2010号条例"]
[null,{"$f":"IF($B$1=\"English\",C1487,IF($B$1=\"Deutsch\",D1487,IF($B$1=\"中文\",E1487,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Persistent organic pollutants (POP), Regulation (EC) No 850/2004 Stockholm Convention.\nAlso listed in REACH Annex 17 and IMO"},"Persistent organic pollutants (POP), Regulation (EC) No 850/2004 Stockholm Convention.\nAlso listed in REACH Annex 17 and IMO","Persistente organische Schadstoffe (POP), Verordnung (EG) Nr. 850/2004 Stockholm Convention\nEbenfalls in REACH Annex 17 und IMO gelistet","持续性有机污染物(POP)，(EC)法规编号 850/2004 Stockholm Convention.\n同时收录在 REACH附件17和表格IMO中"]
[null,{"$f":"IF($B$1=\"English\",C1488,IF($B$1=\"Deutsch\",D1488,IF($B$1=\"中文\",E1488,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ED (Register 15)"},"ED (Register 15)","ED (Register 15)","ED事业部 (登记号15)"]
[null,{"$f":"IF($B$1=\"English\",C1489,IF($B$1=\"Deutsch\",D1489,IF($B$1=\"中文\",E1489,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated substances"},"Regulated substances","Reglementierte Inhaltsstoffe","管制物质"]
[null,{"$f":"IF($B$1=\"English\",C1490,IF($B$1=\"Deutsch\",D1490,IF($B$1=\"中文\",E1490,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS number"},"CAS number","CAS-Nummer","CAS编号"]
[null,{"$f":"IF($B$1=\"English\",C1491,IF($B$1=\"Deutsch\",D1491,IF($B$1=\"中文\",E1491,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient \n[mass%]"},"Concentration of ingredient \n[mass%]","Konzentration des Inhaltsstoffs \n[Massen%]","配料含量\n[质量%]"]
[null,{"$f":"IF($B$1=\"English\",C1492,IF($B$1=\"Deutsch\",D1492,IF($B$1=\"中文\",E1492,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Examples occurrence"},"Examples occurrence","Beispiele Vorkommen","物质常见用途示例"]
[null,{"$f":"IF($B$1=\"English\",C1493,IF($B$1=\"Deutsch\",D1493,IF($B$1=\"中文\",E1493,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Bemerkungen","备注"]
[null,{"$f":"IF($B$1=\"English\",C1494,IF($B$1=\"Deutsch\",D1494,IF($B$1=\"中文\",E1494,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included ( E )\n- changed ( C )"},"Entry\n- included ( E )\n- changed ( C )","Eintrag\n- aufgenommen ( E )\n- geändert ( C )","录入记录\n-首次录入(E)\n-更新(C)"]
[null,{"$f":"IF($B$1=\"English\",C1495,IF($B$1=\"Deutsch\",D1495,IF($B$1=\"中文\",E1495,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substance rated declarable (D)"},"Substance rated declarable (D)","Deklarationspflichtige Inhaltsstoffe (D)","应申报物质（D)"]
[null,{"$f":"IF($B$1=\"English\",C1496,IF($B$1=\"Deutsch\",D1496,IF($B$1=\"中文\",E1496,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bitumen"},"Bitumen","Bitumen","沥青 "]
[null,{"$f":"IF($B$1=\"English\",C1497,IF($B$1=\"Deutsch\",D1497,IF($B$1=\"中文\",E1497,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-butanone oxime"},"2-butanone oxime","2-Butanonoxim","丁酮肟 "]
[null,{"$f":"IF($B$1=\"English\",C1498,IF($B$1=\"Deutsch\",D1498,IF($B$1=\"中文\",E1498,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polyfumaric acid dibutyl ether"},"Polyfumaric acid dibutyl ether","Polyfumarsäure Dibutylether","聚反丁烯二酸丁醚"]
[null,{"$f":"IF($B$1=\"English\",C1499,IF($B$1=\"Deutsch\",D1499,IF($B$1=\"中文\",E1499,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Vinyl acetate"},"Vinyl acetate","Vinylacetat","醋酸乙烯酯 "]
[null,{"$f":"IF($B$1=\"English\",C1500,IF($B$1=\"Deutsch\",D1500,IF($B$1=\"中文\",E1500,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Carbon disulfide"},"Carbon disulfide","Carbondisulfid","二硫化碳 "]
[null,{"$f":"IF($B$1=\"English\",C1501,IF($B$1=\"Deutsch\",D1501,IF($B$1=\"中文\",E1501,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,2,2-Tetrachloroethane"},"1,1,2,2-Tetrachloroethane","1,1,2,2-Tetrachlorethan","1,1,2,2-四氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1502,IF($B$1=\"Deutsch\",D1502,IF($B$1=\"中文\",E1502,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachloroethane"},"Pentachloroethane","Pentachlorethan","五氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1503,IF($B$1=\"Deutsch\",D1503,IF($B$1=\"中文\",E1503,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichloromethane (Chloroform) "},"Trichloromethane (Chloroform) ","Trichlormethan (Chloroform)","三氯甲烷（氯仿）"]
[null,{"$f":"IF($B$1=\"English\",C1504,IF($B$1=\"Deutsch\",D1504,IF($B$1=\"中文\",E1504,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Long-chained chlorinated \nparaffins (C18 to C28) \n"},"Long-chained chlorinated \nparaffins (C18 to C28) \n","langkettige Chlorparaffine (C18 bis C28) ","长链氯化烷烃（C18-C28） \n"]
[null,{"$f":"IF($B$1=\"English\",C1505,IF($B$1=\"Deutsch\",D1505,IF($B$1=\"中文\",E1505,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"n-hexane"},"n-hexane","n-Hexan","正己烷"]
[null,{"$f":"IF($B$1=\"English\",C1506,IF($B$1=\"Deutsch\",D1506,IF($B$1=\"中文\",E1506,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydrogen sulfide"},"Hydrogen sulfide","Hydrogensulfid","硫化氢 "]
[null,{"$f":"IF($B$1=\"English\",C1507,IF($B$1=\"Deutsch\",D1507,IF($B$1=\"中文\",E1507,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Methyl-4-tert-butylbenzene (TBT)"},"1-Methyl-4-tert-butylbenzene (TBT)","1-Methyl-4-tert-butylbenzen (TBT)","1-甲基-4-叔丁基苯 (TBT)"]
[null,{"$f":"IF($B$1=\"English\",C1508,IF($B$1=\"Deutsch\",D1508,IF($B$1=\"中文\",E1508,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3-(2-Butoxyethoxy)ethanol"},"3-(2-Butoxyethoxy)ethanol","3-(2-Butoxyethoxy)ethanol","3 -（2 -丁氧基乙氧基）乙醇 "]
[null,{"$f":"IF($B$1=\"English\",C1509,IF($B$1=\"Deutsch\",D1509,IF($B$1=\"中文\",E1509,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1 Dichloroethylene"},"1,1 Dichloroethylene","1,1 Dichlorethylen","1,1-二氯乙烯 "]
[null,{"$f":"IF($B$1=\"English\",C1510,IF($B$1=\"Deutsch\",D1510,IF($B$1=\"中文\",E1510,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"tri-organostannic compounds"},"tri-organostannic compounds","tri-zinnorganische Verbindungen","三-有机锡化合物 "]
[null,{"$f":"IF($B$1=\"English\",C1511,IF($B$1=\"Deutsch\",D1511,IF($B$1=\"中文\",E1511,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethylbenzene"},"Ethylbenzene","Ethylbenzen","乙苯\n"]
[null,{"$f":"IF($B$1=\"English\",C1512,IF($B$1=\"Deutsch\",D1512,IF($B$1=\"中文\",E1512,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Xylene"},"Xylene","Xylen ","二甲苯 "]
[null,{"$f":"IF($B$1=\"English\",C1513,IF($B$1=\"Deutsch\",D1513,IF($B$1=\"中文\",E1513,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phthalates with a chain length\nof C11, with branches and linear\n"},"Phthalates with a chain length\nof C11, with branches and linear\n","Phthalate mit einer Kettenlänge  C11, mit Verzweigungen und linear","碳链长度11个碳的邻苯二甲酸酯，有支链和直链 "]
[null,{"$f":"IF($B$1=\"English\",C1514,IF($B$1=\"Deutsch\",D1514,IF($B$1=\"中文\",E1514,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethenylbenzene (styrol)"},"Ethenylbenzene (styrol)","Ethenylbenzen (Styrol)","乙烯基苯（苯乙烯）"]
[null,{"$f":"IF($B$1=\"English\",C1515,IF($B$1=\"Deutsch\",D1515,IF($B$1=\"中文\",E1515,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anti-drumming materials"},"Anti-drumming materials","Anti-Dröhnmaterialien","隔声材料 \n"]
[null,{"$f":"IF($B$1=\"English\",C1516,IF($B$1=\"Deutsch\",D1516,IF($B$1=\"中文\",E1516,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PUR formulations"},"PUR formulations","PUR formulations","聚氨酯配方 "]
[null,{"$f":"IF($B$1=\"English\",C1517,IF($B$1=\"Deutsch\",D1517,IF($B$1=\"中文\",E1517,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Drawing oils for aluminum,\nvarnishes, coating defects\n"},"Drawing oils for aluminum,\nvarnishes, coating defects\n","Ziehöle für Aluminium, Lacke, Beschichtungsfehler","铝拉延油，清漆，涂层缺陷 "]
[null,{"$f":"IF($B$1=\"English\",C1518,IF($B$1=\"Deutsch\",D1518,IF($B$1=\"中文\",E1518,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PVAC, SMC, soft films, adhesives"},"PVAC, SMC, soft films, adhesives","PVAC, SMC, weiche Überzüge, Klebstoffe","聚醋酸乙烯酯（PVAC）、SMC、柔性薄膜、粘合剂 "]
[null,{"$f":"IF($B$1=\"English\",C1519,IF($B$1=\"Deutsch\",D1519,IF($B$1=\"中文\",E1519,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited substances (P)"},"Prohibited substances (P)","Verbotene Inhaltsstoffe (P)","禁用物质 (P)"]
[null,{"$f":"IF($B$1=\"English\",C1520,IF($B$1=\"Deutsch\",D1520,IF($B$1=\"中文\",E1520,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anti-drumming materials"},"Anti-drumming materials","Anti-Dröhnmaterialien","隔声材料 \n"]
[null,{"$f":"IF($B$1=\"English\",C1521,IF($B$1=\"Deutsch\",D1521,IF($B$1=\"中文\",E1521,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PUR formulations"},"PUR formulations","PUR-Zubereitungen","聚氨酯配方 "]
[null,{"$f":"IF($B$1=\"English\",C1522,IF($B$1=\"Deutsch\",D1522,IF($B$1=\"中文\",E1522,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Drawing oils for aluminum,\nvarnishes, coating defects\n"},"Drawing oils for aluminum,\nvarnishes, coating defects\n","Ziehöle für Aluminium, Lacke, Beschichtungsfehler ","铝拉延油，清漆，涂层缺陷 \n"]
[null,{"$f":"IF($B$1=\"English\",C1523,IF($B$1=\"Deutsch\",D1523,IF($B$1=\"中文\",E1523,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PVAC, SMC, soft films, adhesives"},"PVAC, SMC, soft films, adhesives","PVAC, SMC, weiche Überzüge, Klebstoffe","聚醋酸乙烯酯（PVAC）、SMC、柔性薄膜、粘合剂 "]
[null,{"$f":"IF($B$1=\"English\",C1524,IF($B$1=\"Deutsch\",D1524,IF($B$1=\"中文\",E1524,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Wood protection agents, polymer\nadditives, catalysts\n"},"Wood protection agents, polymer\nadditives, catalysts\n","Holzschutzmittel, Polymerzusatzstoffe, Katalysatoren","木材保护剂、聚合物添加剂、催化剂 \n"]
[null,{"$f":"IF($B$1=\"English\",C1525,IF($B$1=\"Deutsch\",D1525,IF($B$1=\"中文\",E1525,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Glues, paints, manufacture of\nstyrol\n"},"Glues, paints, manufacture of\nstyrol\n","Klebstoffe, Farben, Herstellung von Styrol","胶水，油漆，苯乙烯的合成 \n"]
[null,{"$f":"IF($B$1=\"English\",C1526,IF($B$1=\"Deutsch\",D1526,IF($B$1=\"中文\",E1526,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvents, glues, paints"},"Solvents, glues, paints","Lösemittel, Klebstoffe, Farben","溶剂、胶水、涂料 "]
[null,{"$f":"IF($B$1=\"English\",C1527,IF($B$1=\"Deutsch\",D1527,IF($B$1=\"中文\",E1527,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizer"},"Plasticizer","Weichmacher","增塑剂 "]
[null,{"$f":"IF($B$1=\"English\",C1528,IF($B$1=\"Deutsch\",D1528,IF($B$1=\"中文\",E1528,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plastic parts, seals"},"Plastic parts, seals","Kunststoffteile, Dichtungen","塑料件、密封件 "]
[null,{"$f":"IF($B$1=\"English\",C1529,IF($B$1=\"Deutsch\",D1529,IF($B$1=\"中文\",E1529,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances rated declarable (D)\nEU-REACH SVHC Candidate List.\nBased on the EuGH Court decision from 10.9.2015: The concentration has to be determined for each partial product and to be declared for each partial product if above  0,1 mass fraction (w/w)."},"Substances rated declarable (D)\nEU-REACH SVHC Candidate List.\nBased on the EuGH Court decision from 10.9.2015: The concentration has to be determined for each partial product and to be declared for each partial product if above  0,1 mass fraction (w/w).","Deklarationspflichtige Inhaltsstoffe (D)\nEG-REACH SVHC Kandidatenliste\nBased in the EuGH Court decision from 10.9.2015: Die Konzentration ist für jedes Teil-Erzeugnis zu bestimmen und wenn über  0,1 Massenprozent (w/w) für jedes Teilerzeugnis zu deklarieren.","应申报物质（D)\n欧盟REACH 高度关注物质SVHC候选清单\n根据欧盟法院(EuGH)2015年9月10日的决定：浓度基于每一部分来确定，如果超过0.1%（w / w，质量比），需要为每个部分进行声明。 "]
[null,{"$f":"IF($B$1=\"English\",C1530,IF($B$1=\"Deutsch\",D1530,IF($B$1=\"中文\",E1530,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di(2-ethylhexyl)phthalate (DEHP)\nDibutyl phthalate (DBP) \nBenzyl butyl phtalate (BBP) \nDi-„isononyl“phthalate (DINP)\n Di-„isodecyl“phthalate (DIDP) \nDi-n-octylphthalate (DNOP) "},"Di(2-ethylhexyl)phthalate (DEHP)\nDibutyl phthalate (DBP) \nBenzyl butyl phtalate (BBP) \nDi-„isononyl“phthalate (DINP)\n Di-„isodecyl“phthalate (DIDP) \nDi-n-octylphthalate (DNOP) ","Di(2-ethylhexyl)phthalat (DEHP)\nDibutylphthalat (DBP) \nBenzylbutylphtalat (BBP) \nDi-„isononyl“phthalat (DINP)\n Di-„isodecyl“phthalat (DIDP) \nDi-n-octylphthalat (DNOP) ","邻苯二甲酸二（2-乙基己基）酯（DEHP） \n邻苯二甲酸二丁酯（DBP）                                                                                                     邻苯二甲酸苄丁酯（BBP）                                                    邻苯二甲酸二异壬酯（DINP）                                                邻苯二甲酸二异癸酯（DIDP）                                                    邻苯二甲酸二正辛酯（DNOP）                                             "]
[null,{"$f":"IF($B$1=\"English\",C1531,IF($B$1=\"Deutsch\",D1531,IF($B$1=\"中文\",E1531,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2-Methoxyethoxy)ethanol (DEGME) "},"2-(2-Methoxyethoxy)ethanol (DEGME) ","2-(2-Methoxyethoxy)ethanol (DEGME) ","2 -（2-甲氧基乙氧基）乙醇（DEGME） "]
[null,{"$f":"IF($B$1=\"English\",C1532,IF($B$1=\"Deutsch\",D1532,IF($B$1=\"中文\",E1532,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methylene diphenyl-diisocyanate (MDI) \n 4,4’-Methylene diphenyl-diisocyanate (MDI) \n2,4’-Methylene  diphenyl-diisocyanate (MDI)  \n 2,2’-Methylene diphenyl-diisocyanate (MDI) "},"Methylene diphenyl-diisocyanate (MDI) \n 4,4’-Methylene diphenyl-diisocyanate (MDI) \n2,4’-Methylene  diphenyl-diisocyanate (MDI)  \n 2,2’-Methylene diphenyl-diisocyanate (MDI) ","Methylendiphenyl-Diisocyanat (MDI) \n 4,4’-Methylendiphenyl-Diisocyanat (MDI) \n2,4’-Methylendiphenyl-Diisocyanat (MDI)  \n 2,2’-Methylendiphenyl-Diisocyanat (MDI) ","二氯甲烷二苯基二端异氰酸酯（MDI）                                     4,4’-二氯甲烷二苯基二端异氰酸酯（MDI）                                 2,4’-二氯甲烷二苯基二端异氰酸酯（MDI）                              2,2’-二氯甲烷二苯基二端异氰酸酯（MDI）"]
[null,{"$f":"IF($B$1=\"English\",C1533,IF($B$1=\"Deutsch\",D1533,IF($B$1=\"中文\",E1533,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cyclohexane "},"Cyclohexane ","Cyclohexan ","环己烷"]
[null,{"$f":"IF($B$1=\"English\",C1534,IF($B$1=\"Deutsch\",D1534,IF($B$1=\"中文\",E1534,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichloromethane"},"Dichloromethane","Dichlormethan","二氯甲烷 "]
[null,{"$f":"IF($B$1=\"English\",C1535,IF($B$1=\"Deutsch\",D1535,IF($B$1=\"中文\",E1535,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acrylamide "},"Acrylamide ","Acrylamid ","丙烯酰胺 "]
[null,{"$f":"IF($B$1=\"English\",C1536,IF($B$1=\"Deutsch\",D1536,IF($B$1=\"中文\",E1536,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethyl fumarate (DMF)"},"Dimethyl fumarate (DMF)","Dimethylfumarat (DMF)","富马酸二甲酯(DMF)"]
[null,{"$f":"IF($B$1=\"English\",C1537,IF($B$1=\"Deutsch\",D1537,IF($B$1=\"中文\",E1537,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,4-Dichlorobenzene"},"1,4-Dichlorobenzene","1,4-Dichlorbenzol","1,4-二氯苯 "]
[null,{"$f":"IF($B$1=\"English\",C1538,IF($B$1=\"Deutsch\",D1538,IF($B$1=\"中文\",E1538,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Must not be used as substances or in mixtures in concentrations of more than 0,1 mass-% of the plasticizer-containing material in toys and infant supplies.\nToys and infant supplies which contain these phthalates in concentrations of more than 0,1 mass-% of the plasticizer-containing material must not be placed on the market"},"Must not be used as substances or in mixtures in concentrations of more than 0,1 mass-% of the plasticizer-containing material in toys and infant supplies.\nToys and infant supplies which contain these phthalates in concentrations of more than 0,1 mass-% of the plasticizer-containing material must not be placed on the market","Dürfen nicht als Stoffe oder in Gemischen in Konzentrationen von mehr als 0,1 Gew.-% des weichmacherhaltigen Materials in Spielzeug und Babyartikeln verwendet werden.\nSpielzeug und Babyartikel, die diese Phthalate in Konzentrationen von mehr als 0,1 Gew.-% des weichmacherhaltigen Materials enthalten, dürfen nicht in Verkehr gebracht werden","不得用作纯物质或用于玩具和儿童用品中，在塑性材料中重量百分比浓度不大于0.1%。\n玩具和儿童用品，如果使用了含邻苯二甲酸盐的浓度大于0.1％的塑性材料，不得投放市场。"]
[null,{"$f":"IF($B$1=\"English\",C1539,IF($B$1=\"Deutsch\",D1539,IF($B$1=\"中文\",E1539,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"    After 27 June, 2010 must not be placed on the market for the first time to be available for the general public in spray paints or spray cleaners in aerosol packages in a\n    concentration of ≥ 3 mass-%.\n    After 27 December, 2010 spray paints and spray cleaners containing DEGBE in aerosol packages which do not conform to the requirements in paragraph 1 must not be placed on the market for the use of the general public. \n\n    Without prejudice to the provisions of other Community regulations on the classification, packaging and labelling of substances and mixtures, the supplier has to guarantee, prior to placing on the market, that paints containing DEGBE not intended for spraying and in a concentration of 3 mass % or more, from 27 December 2010 carry the following wording, well visible, legible and permanent :\n    „Must not be used in paint spray equipment“."},"    After 27 June, 2010 must not be placed on the market for the first time to be available for the general public in spray paints or spray cleaners in aerosol packages in a\n    concentration of ≥ 3 mass-%.\n    After 27 December, 2010 spray paints and spray cleaners containing DEGBE in aerosol packages which do not conform to the requirements in paragraph 1 must not be placed on the market for the use of the general public. \n\n    Without prejudice to the provisions of other Community regulations on the classification, packaging and labelling of substances and mixtures, the supplier has to guarantee, prior to placing on the market, that paints containing DEGBE not intended for spraying and in a concentration of 3 mass % or more, from 27 December 2010 carry the following wording, well visible, legible and permanent :\n    „Must not be used in paint spray equipment“.","    Darf nach dem 27. Juni 2010 nicht zur Abgabe an die breite Öffentlichkeit in Spritzfarben oder Reinigungssprays in Aerosolpackungen in einer\n    Konzentration von ≥ 3 Gew.-% erstmalig in Verkehr gebracht werden.\n    Nach dem 27. Dezember 2010 dürfen DEGBE-haltige Spritzfarben und Reinigungssprays in Aerosolpackungen, die den Anforderungen unter Absatz 1 nicht entsprechen, nicht mehr zur Abgabe an die breite Öffentlichkeit in Verkehr gebracht werden.\n\n    Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften über die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte DEGBE-haltige Farben, die nicht zum Verspritzen bestimmt sind, in einer Konzentration von 3 Gew.- % oder mehr ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n\n    „Darf nicht in Farbspritzausrüstung verwendet werden“.","作为喷漆或喷雾清洁剂的组分在气溶胶喷罐中的浓度质量百分比大于3%时，不得在2010年6月27日以后首次投放市场销售给普通公众。\n\n喷漆或喷雾清洁剂如含DEGBE并且不符合本条第1款的规定，2010年12月27日后不得投放市场销售给普通公众。\n\n不影响其它关于物质和配制品的分类、包装和标签等方面的公共规定，供应商应在投放市场之前确保，销售给普通公众的涂料（除喷漆外）若含DEGBE质量百分比大于等于3%，从2010年12月27日起其包装上应该清晰易见且永久的标记有以下文字：“不得在涂料喷涂设备中使用”"]
[null,{"$f":"IF($B$1=\"English\",C1540,IF($B$1=\"Deutsch\",D1540,IF($B$1=\"中文\",E1540,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"    After 27 December, 2010 must not be placed on the market for the use of the general public in mixtures containing this substance in a concentration of ≥ 0,1 mass-% MDI; unless the supplier guarantees before placing on the market that the packaging \n\n    a) contains protective gloves conforming to the requirements of the directive 89/686/EWG of the council (*******);\n\n    b) without prejudice to the provisions of other Community regulations on the classification, packaging and labelling of substances and mixtures, carries the following wording, \nwell visible, legible and permanent:\n\n    „— In persons already sensitive to diisocyanates the handling of this product may cause allergic reactions.\n\n    — In case of asthma, eczematous skin diseases or skin problems avoid contact, including skin contact, with the product.\n\n    — Do not use the product with insufficient ventilation or wear protective mask with corresponding gas filter (Type A1 as per EN 14387) tragen.“\n    Paragraph 1 letter a is not valid for hot-melt adhesives."},"    After 27 December, 2010 must not be placed on the market for the use of the general public in mixtures containing this substance in a concentration of ≥ 0,1 mass-% MDI; unless the supplier guarantees before placing on the market that the packaging \n\n    a) contains protective gloves conforming to the requirements of the directive 89/686/EWG of the council (*******);\n\n    b) without prejudice to the provisions of other Community regulations on the classification, packaging and labelling of substances and mixtures, carries the following wording, \nwell visible, legible and permanent:\n\n    „— In persons already sensitive to diisocyanates the handling of this product may cause allergic reactions.\n\n    — In case of asthma, eczematous skin diseases or skin problems avoid contact, including skin contact, with the product.\n\n    — Do not use the product with insufficient ventilation or wear protective mask with corresponding gas filter (Type A1 as per EN 14387) tragen.“\n    Paragraph 1 letter a is not valid for hot-melt adhesives.","    Darf nach dem 27. Dezember 2010 nicht zur Abgabe an die breite Öffentlichkeit in Gemischen, die diesen Stoff in einer Konzentration von ≥ 0,1 Gew.-% MDI enthalten, in Verkehr gebracht werden; es sei denn, der Lieferant gewährleistet vor dem Inverkehrbringen, dass die Verpackung\n\n    a) Schutzhandschuhe enthält, die den Anforderungen der Richtlinie 89/686/EWG des Rates entsprechen (*******);\n\n    b) unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n\n    „— Bei Personen, die bereits für Diisocyanate sensibilisiert sind, kann der Umgang mit diesem Produkt allergische Reaktionen auslösen.\n\n    — Bei Asthma, ekzematösen Hauterkrankungen oder Hautproblemen Kontakt, einschließlich Hautkontakt, mit dem Produkt vermeiden.\n\n    — Das Produkt nicht bei ungenügender Lüftung verwenden oder Schutzmaske mit entsprechendem Gasfilter (Typ A1 nach EN 14387) tragen.“\n    Absatz 1 Buchstabe a gilt nicht für Heißklebstoffe.","1.配制品中含有二苯基甲烷二异氰酸酯(MDI)的重量百分比大于等于0,1%的，2010年12月27日之后不得投放市场供应给普通大众，除非供应商投放市场之前应确保：\na)包装中附有符合委员会指令89/686/EEC要求的防护手套\nb)在不违背理事会其他关于物质和配制品分类、标签和包装法规的前提下，包装上应使用清晰、明显、永久性标识标记如下：\n—对二异氰酸酯很敏感的人在使用本产品时，会引起过敏反应。\n—有哮喘，湿疹或皮肤问题的人应避免接触该产品，包括皮肤接触。\n—不要在通风不足的情况下使用该产品，除非佩戴含有气体过滤器的防护面罩（根据标准EN14387，A1型）。\n2. 作为豁免条款，1(a)不适用于热熔粘合剂。"]
[null,{"$f":"IF($B$1=\"English\",C1541,IF($B$1=\"Deutsch\",D1541,IF($B$1=\"中文\",E1541,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"    After 27 June, 2010 must not be placed on the market for the first time to be available for the general public, in contact adhesives on the basis of neoprene, not in a concentration of ≥ 0,1 mass-% in package sizes of more than 350 g. \n    Contact adhesives on the basis of neoprene which contain cyclohexane, when they do not meet the requirements under paragraph 1, must not be placed on the market for being available to the general public after  27 Dezember, 2010.\n\n    Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte Kontaktklebstoffe auf Neoprenbasis, die Cyclohexan in einer Konzentration von 0,1 Gew.-% oder mehr enthalten, ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n\n    „— Dieses Produkt darf nicht bei ungenügender Lüftung verarbeitet werden.\n\n    — Dieses Produkt darf nicht zum Verlegen von Teppichböden verwendet werden.“"},"    After 27 June, 2010 must not be placed on the market for the first time to be available for the general public, in contact adhesives on the basis of neoprene, not in a concentration of ≥ 0,1 mass-% in package sizes of more than 350 g. \n    Contact adhesives on the basis of neoprene which contain cyclohexane, when they do not meet the requirements under paragraph 1, must not be placed on the market for being available to the general public after  27 Dezember, 2010.\n\n    Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte Kontaktklebstoffe auf Neoprenbasis, die Cyclohexan in einer Konzentration von 0,1 Gew.-% oder mehr enthalten, ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n\n    „— Dieses Produkt darf nicht bei ungenügender Lüftung verarbeitet werden.\n\n    — Dieses Produkt darf nicht zum Verlegen von Teppichböden verwendet werden.“","    Darf nach dem 27. Juni 2010 zur Abgabe an die breite Öffentlichkeit in Kontaktklebstoffen auf Neoprenbasis nicht in einer Konzentration von ≥ 0,1 Gew.-% in Packungsgrößen von mehr als 350 g erstmalig in Verkehr gebracht werden.\n    Cyclohexanhaltige Kontaktklebstoffe auf Neoprenbasis, die den Anforderungen unter Absatz 1 nicht entsprechen, dürfen nach dem 27. Dezember 2010 nicht mehr zur Abgabe an die breite Öffentlichkeit in Verkehr gebracht werden.\n\n    Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte Kontaktklebstoffe auf Neoprenbasis, die Cyclohexan in einer Konzentration von 0,1 Gew.-% oder mehr enthalten, ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n\n    „— Dieses Produkt darf nicht bei ungenügender Lüftung verarbeitet werden.\n\n    — Dieses Produkt darf nicht zum Verlegen von Teppichböden verwendet werden.“"," 1.作为氯丁橡胶接触粘合剂的成分，其浓度大于等于0.1%（重量百分比）销售包装超过350克，不得投放市场销售给普通大众。\n2.含有环己烷的氯丁橡胶接触粘合剂，如不符合本条第1款的规定，2010年12月27日之后不得投放市场销售给普通大众。\n3.如2010年12月27日之后销售该物质浓度大于等于0.1%的含有环己烷的氯丁橡胶接触粘合剂，在不违反委员会的其它关于物质和配制品分类、包装和标签法规的前提下，供应商必须保证粘合剂以不可磨损的方式，标记以下文字：\n—此产品不得在通风不良时使用。 \n—该产品不能用于地毯铺设。"]
[null,{"$f":"IF($B$1=\"English\",C1542,IF($B$1=\"Deutsch\",D1542,IF($B$1=\"中文\",E1542,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"    Farbabbeizer, die Dichlormethan (DCM) in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, dürfen\n\n    a) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2010 nicht mehr erstmalig in Verkehr gebracht werden;\n\n    b) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2011 nicht mehr in Verkehr gebracht werden;\n\n    c) nach dem 6. Juni 2012 nicht mehr von gewerblichen Verwendern benutzt werden.\n\n    Für die Zwecke dieses Eintrags bezeichnet der Ausdruck\n\n    i) „gewerblicher Verwender“ eine natürliche oder juristische Person, einschließlich Angestellte und Selbstständige, die im Zuge ihrer beruflichen Tätigkeit außerhalb einer Industrieanlage Abbeizarbeiten durchführt;\n\n    ii) „Industrieanlage“ eine Anlage, die zum Abbeizen von Farbe genutzt wird.\n\n    Abweichend von Absatz 1 können die Mitgliedstaaten in ihren Hoheitsgebieten für bestimmte Tätigkeiten die Verwendung von DCM-haltigen Farbabbeizern durch speziell geschulte gewerbliche Verwender und das Inverkehrbringen solcher Farbabbeizer zur Abgabe an diese gewerblichen Verwender gestatten.\n\n    Mitgliedstaaten, die von dieser Ausnahmeregelung Gebrauch machen, legen angemessene Bestimmungen zur Gewährleistung des Gesundheitsschutzes und der Sicherheit für gewerbliche Verwender fest, die DCM-haltige Farbabbeizer verwenden, und unterrichten die Kommission darüber.\n\n    Diese Bestimmungen enthalten die Anforderung, dass ein gewerblicher Verwender über einen Sachkundenachweis verfügen muss, der in dem Mitgliedstaat, in dem er tätig ist, anerkannt wird, oder andere diesbezügliche Nachweisdokumente vorlegen oder eine anderweitige Zulassung desselben Mitgliedstaats besitzen muss, damit nachgewiesen werden kann, dass der gewerbliche Verwender im Umgang mit DCM-haltigen Farbabbeizern ordnungsgemäß geschult wurde und qualifiziert ist, sicher mit ihnen umzugehen.\n\n    Die Kommission erstellt ein Verzeichnis der Mitgliedstaaten, die von der in diesem Absatz genannten Ausnahmeregelung Gebrauch machen, und veröffentlicht dieses Verzeichnis im Internet.\n\n    Ein gewerblicher Verwender, der von der in Absatz 2 genannten Ausnahmeregelung Gebrauch macht, darf nur in Mitgliedstaaten tätig werden, die diese Ausnahmeregelung anwenden. Die in Absatz 2 genannte Schulung muss mindestens folgende Bereiche abdecken:\n\n    a) Kenntnis, Bewertung und Beherrschung der Gesundheitsrisiken, einschließlich Unterrichtung über bestehende Ersatzstoffe oder Verfahren, die unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender weniger gefährlich sind;\n\n    b) Verwendung ausreichender Belüftung;\n\n    c) Verwendung geeigneter persönlichen Schutzausrüstungen gemäß der Richtlinie 89/686/EWG.\n\n    Arbeitgeber und Selbstständige ersetzen DCM vorrangig durch einen chemischen Arbeitsstoff oder ein Verfahren, der bzw. das unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender nicht oder weniger gefährlich ist.\n\n    Der gewerbliche Verwender setzt alle einschlägigen Sicherheitsmaßnahmen in die Praxis um, einschließlich der Verwendung einer persönlichen Schutzausrüstung.\n\n    Unbeschadet anderer Arbeitnehmerschutzvorschriften der Gemeinschaft dürfen Farbabbeizer, die DCM in einer Konzentration von 0,1 Gewichtsprozent\n    oder mehr enthalten, in Industrieanlagen nur verwendet werden, wenn mindestens folgende Bedingungen erfüllt sind:\n\n    a) wirksame Belüftung in allen Arbeitsräumen, insbesondere bei der Nassbehandlung und der Trocknung abgebeizter Gegenstände: lokale Absauganlagen\n    an Abbeizbehältnissen, die durch Zwangsbelüftungsanlagen in diesen Bereichen ergänzt werden, um die Exposition zu minimieren und die maßgeblichen Arbeitsplatzgrenzwerte, soweit technisch möglich, einzuhalten;\n\n    b) Maßnahmen zur weitestgehenden Verringerung der Verdampfung aus Abbeizbehältnissen, die Folgendes umfassen: Abdeckungen für Abbeizbehältnisse,\n    außer bei der Beladung und Entladung; angemessene Vorkehrungen für die Beladung und Entladung der Abbeizbehältnisse; Reinigungsbehälter, mit Wasser oder Lauge gefüllt, um nach der Entladung das überschüssige Lösemittel vom Abbeizgut zu entfernen;\n\n    c) Maßnahmen für die sichere Handhabung von DCM enthaltenden Abbeizbehältnissen, die Folgendes umfassen: Pumpen und Rohrleitungen für die Überleitung des Abbeizmittels aus den und in die Behältnisse; angemessene Vorkehrungen für die sichere Reinigung der Behältnisse und die Beseitigung von Schlämmen;\n\n    d) persönliche Schutzausrüstungen gemäß der Richtlinie 89/686/EWG, die Folgendes umfassen: geeignete Schutzhandschuhe, Schutzbrillen und Schutzkleidung; geeignete Atemschutzgeräte, für den Fall, dass die Arbeitsplatzgrenzwerte nicht anderweitig eingehalten werden können;\n\n    e) angemessene Informationen, Anweisungen und Übungen zur Verwendung solcher Ausrüstungsgegenstände für die Verwender.\n\n    Unbeschadet anderer gemeinschaftlicher Bestimmungen für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen müssen\n    Farbabbeizer, die Dichlormethan in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, ab dem 6. Dezember 2011 gut sichtbar, leserlich\n    und unverwischbar mit folgender Aufschrift versehen sein:\n\n    „Nur für die industrielle Verwendung und für gewerbliche Verwender, die über eine Zulassung in bestimmten EU-Mitgliedstaaten verfügen. Überprüfen\n    Sie, in welchem Mitgliedstaat die Verwendung genehmigt ist.“"},"    Farbabbeizer, die Dichlormethan (DCM) in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, dürfen\n\n    a) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2010 nicht mehr erstmalig in Verkehr gebracht werden;\n\n    b) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2011 nicht mehr in Verkehr gebracht werden;\n\n    c) nach dem 6. Juni 2012 nicht mehr von gewerblichen Verwendern benutzt werden.\n\n    Für die Zwecke dieses Eintrags bezeichnet der Ausdruck\n\n    i) „gewerblicher Verwender“ eine natürliche oder juristische Person, einschließlich Angestellte und Selbstständige, die im Zuge ihrer beruflichen Tätigkeit außerhalb einer Industrieanlage Abbeizarbeiten durchführt;\n\n    ii) „Industrieanlage“ eine Anlage, die zum Abbeizen von Farbe genutzt wird.\n\n    Abweichend von Absatz 1 können die Mitgliedstaaten in ihren Hoheitsgebieten für bestimmte Tätigkeiten die Verwendung von DCM-haltigen Farbabbeizern durch speziell geschulte gewerbliche Verwender und das Inverkehrbringen solcher Farbabbeizer zur Abgabe an diese gewerblichen Verwender gestatten.\n\n    Mitgliedstaaten, die von dieser Ausnahmeregelung Gebrauch machen, legen angemessene Bestimmungen zur Gewährleistung des Gesundheitsschutzes und der Sicherheit für gewerbliche Verwender fest, die DCM-haltige Farbabbeizer verwenden, und unterrichten die Kommission darüber.\n\n    Diese Bestimmungen enthalten die Anforderung, dass ein gewerblicher Verwender über einen Sachkundenachweis verfügen muss, der in dem Mitgliedstaat, in dem er tätig ist, anerkannt wird, oder andere diesbezügliche Nachweisdokumente vorlegen oder eine anderweitige Zulassung desselben Mitgliedstaats besitzen muss, damit nachgewiesen werden kann, dass der gewerbliche Verwender im Umgang mit DCM-haltigen Farbabbeizern ordnungsgemäß geschult wurde und qualifiziert ist, sicher mit ihnen umzugehen.\n\n    Die Kommission erstellt ein Verzeichnis der Mitgliedstaaten, die von der in diesem Absatz genannten Ausnahmeregelung Gebrauch machen, und veröffentlicht dieses Verzeichnis im Internet.\n\n    Ein gewerblicher Verwender, der von der in Absatz 2 genannten Ausnahmeregelung Gebrauch macht, darf nur in Mitgliedstaaten tätig werden, die diese Ausnahmeregelung anwenden. Die in Absatz 2 genannte Schulung muss mindestens folgende Bereiche abdecken:\n\n    a) Kenntnis, Bewertung und Beherrschung der Gesundheitsrisiken, einschließlich Unterrichtung über bestehende Ersatzstoffe oder Verfahren, die unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender weniger gefährlich sind;\n\n    b) Verwendung ausreichender Belüftung;\n\n    c) Verwendung geeigneter persönlichen Schutzausrüstungen gemäß der Richtlinie 89/686/EWG.\n\n    Arbeitgeber und Selbstständige ersetzen DCM vorrangig durch einen chemischen Arbeitsstoff oder ein Verfahren, der bzw. das unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender nicht oder weniger gefährlich ist.\n\n    Der gewerbliche Verwender setzt alle einschlägigen Sicherheitsmaßnahmen in die Praxis um, einschließlich der Verwendung einer persönlichen Schutzausrüstung.\n\n    Unbeschadet anderer Arbeitnehmerschutzvorschriften der Gemeinschaft dürfen Farbabbeizer, die DCM in einer Konzentration von 0,1 Gewichtsprozent\n    oder mehr enthalten, in Industrieanlagen nur verwendet werden, wenn mindestens folgende Bedingungen erfüllt sind:\n\n    a) wirksame Belüftung in allen Arbeitsräumen, insbesondere bei der Nassbehandlung und der Trocknung abgebeizter Gegenstände: lokale Absauganlagen\n    an Abbeizbehältnissen, die durch Zwangsbelüftungsanlagen in diesen Bereichen ergänzt werden, um die Exposition zu minimieren und die maßgeblichen Arbeitsplatzgrenzwerte, soweit technisch möglich, einzuhalten;\n\n    b) Maßnahmen zur weitestgehenden Verringerung der Verdampfung aus Abbeizbehältnissen, die Folgendes umfassen: Abdeckungen für Abbeizbehältnisse,\n    außer bei der Beladung und Entladung; angemessene Vorkehrungen für die Beladung und Entladung der Abbeizbehältnisse; Reinigungsbehälter, mit Wasser oder Lauge gefüllt, um nach der Entladung das überschüssige Lösemittel vom Abbeizgut zu entfernen;\n\n    c) Maßnahmen für die sichere Handhabung von DCM enthaltenden Abbeizbehältnissen, die Folgendes umfassen: Pumpen und Rohrleitungen für die Überleitung des Abbeizmittels aus den und in die Behältnisse; angemessene Vorkehrungen für die sichere Reinigung der Behältnisse und die Beseitigung von Schlämmen;\n\n    d) persönliche Schutzausrüstungen gemäß der Richtlinie 89/686/EWG, die Folgendes umfassen: geeignete Schutzhandschuhe, Schutzbrillen und Schutzkleidung; geeignete Atemschutzgeräte, für den Fall, dass die Arbeitsplatzgrenzwerte nicht anderweitig eingehalten werden können;\n\n    e) angemessene Informationen, Anweisungen und Übungen zur Verwendung solcher Ausrüstungsgegenstände für die Verwender.\n\n    Unbeschadet anderer gemeinschaftlicher Bestimmungen für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen müssen\n    Farbabbeizer, die Dichlormethan in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, ab dem 6. Dezember 2011 gut sichtbar, leserlich\n    und unverwischbar mit folgender Aufschrift versehen sein:\n\n    „Nur für die industrielle Verwendung und für gewerbliche Verwender, die über eine Zulassung in bestimmten EU-Mitgliedstaaten verfügen. Überprüfen\n    Sie, in welchem Mitgliedstaat die Verwendung genehmigt ist.“","    Farbabbeizer, die Dichlormethan (DCM) in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, dürfen\n\n    a) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2010 nicht mehr erstmalig in Verkehr gebracht werden;\n\n    b) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2011 nicht mehr in Verkehr gebracht werden;\n\n    c) nach dem 6. Juni 2012 nicht mehr von gewerblichen Verwendern benutzt werden.\n\n    Für die Zwecke dieses Eintrags bezeichnet der Ausdruck\n\n    i) „gewerblicher Verwender“ eine natürliche oder juristische Person, einschließlich Angestellte und Selbstständige, die im Zuge ihrer beruflichen Tätigkeit außerhalb einer Industrieanlage Abbeizarbeiten durchführt;\n\n    ii) „Industrieanlage“ eine Anlage, die zum Abbeizen von Farbe genutzt wird.\n\n    Abweichend von Absatz 1 können die Mitgliedstaaten in ihren Hoheitsgebieten für bestimmte Tätigkeiten die Verwendung von DCM-haltigen Farbabbeizern durch speziell geschulte gewerbliche Verwender und das Inverkehrbringen solcher Farbabbeizer zur Abgabe an diese gewerblichen Verwender gestatten.\n\n    Mitgliedstaaten, die von dieser Ausnahmeregelung Gebrauch machen, legen angemessene Bestimmungen zur Gewährleistung des Gesundheitsschutzes und der Sicherheit für gewerbliche Verwender fest, die DCM-haltige Farbabbeizer verwenden, und unterrichten die Kommission darüber.\n\n    Diese Bestimmungen enthalten die Anforderung, dass ein gewerblicher Verwender über einen Sachkundenachweis verfügen muss, der in dem Mitgliedstaat, in dem er tätig ist, anerkannt wird, oder andere diesbezügliche Nachweisdokumente vorlegen oder eine anderweitige Zulassung desselben Mitgliedstaats besitzen muss, damit nachgewiesen werden kann, dass der gewerbliche Verwender im Umgang mit DCM-haltigen Farbabbeizern ordnungsgemäß geschult wurde und qualifiziert ist, sicher mit ihnen umzugehen.\n\n    Die Kommission erstellt ein Verzeichnis der Mitgliedstaaten, die von der in diesem Absatz genannten Ausnahmeregelung Gebrauch machen, und veröffentlicht dieses Verzeichnis im Internet.\n\n    Ein gewerblicher Verwender, der von der in Absatz 2 genannten Ausnahmeregelung Gebrauch macht, darf nur in Mitgliedstaaten tätig werden, die diese Ausnahmeregelung anwenden. Die in Absatz 2 genannte Schulung muss mindestens folgende Bereiche abdecken:\n\n    a) Kenntnis, Bewertung und Beherrschung der Gesundheitsrisiken, einschließlich Unterrichtung über bestehende Ersatzstoffe oder Verfahren, die unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender weniger gefährlich sind;\n\n    b) Verwendung ausreichender Belüftung;\n\n    c) Verwendung geeigneter persönlichen Schutzausrüstungen gemäß der Richtlinie 89/686/EWG.\n\n    Arbeitgeber und Selbstständige ersetzen DCM vorrangig durch einen chemischen Arbeitsstoff oder ein Verfahren, der bzw. das unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender nicht oder weniger gefährlich ist.\n\n    Der gewerbliche Verwender setzt alle einschlägigen Sicherheitsmaßnahmen in die Praxis um, einschließlich der Verwendung einer persönlichen Schutzausrüstung.\n\n    Unbeschadet anderer Arbeitnehmerschutzvorschriften der Gemeinschaft dürfen Farbabbeizer, die DCM in einer Konzentration von 0,1 Gewichtsprozent\n    oder mehr enthalten, in Industrieanlagen nur verwendet werden, wenn mindestens folgende Bedingungen erfüllt sind:\n\n    a) wirksame Belüftung in allen Arbeitsräumen, insbesondere bei der Nassbehandlung und der Trocknung abgebeizter Gegenstände: lokale Absauganlagen\n    an Abbeizbehältnissen, die durch Zwangsbelüftungsanlagen in diesen Bereichen ergänzt werden, um die Exposition zu minimieren und die maßgeblichen Arbeitsplatzgrenzwerte, soweit technisch möglich, einzuhalten;\n\n    b) Maßnahmen zur weitestgehenden Verringerung der Verdampfung aus Abbeizbehältnissen, die Folgendes umfassen: Abdeckungen für Abbeizbehältnisse,\n    außer bei der Beladung und Entladung; angemessene Vorkehrungen für die Beladung und Entladung der Abbeizbehältnisse; Reinigungsbehälter, mit Wasser oder Lauge gefüllt, um nach der Entladung das überschüssige Lösemittel vom Abbeizgut zu entfernen;\n\n    c) Maßnahmen für die sichere Handhabung von DCM enthaltenden Abbeizbehältnissen, die Folgendes umfassen: Pumpen und Rohrleitungen für die Überleitung des Abbeizmittels aus den und in die Behältnisse; angemessene Vorkehrungen für die sichere Reinigung der Behältnisse und die Beseitigung von Schlämmen;\n\n    d) persönliche Schutzausrüstungen gemäß der Richtlinie 89/686/EWG, die Folgendes umfassen: geeignete Schutzhandschuhe, Schutzbrillen und Schutzkleidung; geeignete Atemschutzgeräte, für den Fall, dass die Arbeitsplatzgrenzwerte nicht anderweitig eingehalten werden können;\n\n    e) angemessene Informationen, Anweisungen und Übungen zur Verwendung solcher Ausrüstungsgegenstände für die Verwender.\n\n    Unbeschadet anderer gemeinschaftlicher Bestimmungen für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen müssen\n    Farbabbeizer, die Dichlormethan in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, ab dem 6. Dezember 2011 gut sichtbar, leserlich\n    und unverwischbar mit folgender Aufschrift versehen sein:\n\n    „Nur für die industrielle Verwendung und für gewerbliche Verwender, die über eine Zulassung in bestimmten EU-Mitgliedstaaten verfügen. Überprüfen\n    Sie, in welchem Mitgliedstaat die Verwendung genehmigt ist.“","   1.二氯甲烷（DCM）含量大于等于0.1（重量百分比）的脱漆剂，不得： (a)在2010年12月6日以后将不再有新产品首次投放市场，销售给普通大众或专业用户；\n(b)在2011年12月6日以后将不再投放市场，销售给广大市民或专业用户；\n(c)在2012年12月6以后，专业用户也不得使用。\n以下是关于这条款的一些注释：\n(i)“专业用户”是指自然人或法人，包括雇员及个体经营人士，他们不是在工业装置上进行脱漆作业；\n(ii)“工业装置”是指用于脱漆的设备。\n2.作为第1款的豁免条款，成员国可以允许在他们国家范围内，在由经过专门培训的专业人员从事的某些特定的工作中使用含DCM脱漆剂；也允许将这类脱漆剂投放市场销售给专业人员。\n各成员国在应用这一豁免时，应同时制定法规，以确保专业人员使用含DCM的脱漆剂时的健康与安全，并通知委员会。 \n这些规定包括专业用户必须持有成员国认可的能力证书，或提交其他有关有效的证明文件，以证明专业人员用户已经过适当的培训，有能力安全地使用含DCM的脱漆剂。\n委员会应准备一份应用该豁免的成员国名单，并公布在互联网上\n3.专业人员只能在应用该豁免的成员国内参考第2段应用该豁免。第2段中提及的培训应该至少包括：\n(a)告知健康风险，如何评估和管理风险，包括现有的替代产品，以及能够降低对员工健康和安全危害的工艺；\n(b) 充分通风换气；\n(c) 使用合适的符合89/686/EEC指令的个人防护用品。\n雇员或个体劳动者应优先考虑用对员工健康和安全无风险或者低风险的化学品或者工艺替代DCM。\n专业人员在操作时应确保所有的安全措施，包括个人防护用品。\n4.在不违反其它劳动保护法规的前提下，含DCM浓度重量百分比大于等于0.1%的脱漆剂，只有在符合以下条件下，可以用在工业装置中：\n(a)在所有加工区域，尤其是湿式加工和脱机物品烘干区域，确保有效通风：所有上述区域的强制通风外加脱漆槽的局部排风，以尽可能减少曝露。\n(b)采取措施尽可能减少脱漆剂挥发，包括：除了上下料，其它时间脱漆槽必须加盖；妥善安排脱漆槽的上下料过程；下料后，用水或盐水清洗脱漆槽，除去多余的溶剂\n(c)采取措施安全处理脱漆槽中的DCM，包括：转移脱漆剂进入、排出脱漆槽的泵和管路（防止泄露）；清理脱漆槽和去除污泥时合理安排\n(d)符合89/686/EEC指令的劳动防护用品，包括：合适的防护手套，安全眼镜，防护服；如果采取措施也不能够符合相关的职业危害曝露限值的话，还需要采用合时的呼吸保护设备。\n(e)为使用该设备的员工提供充分的信息，培训和指导。\n5．在不违背理事会其他关于物质和配制品分类、标签和包装法规的前提下，在2011年12月6日之后，含DCM质量百分比大于等于0.1%的脱漆剂应使用清晰、明显、永久性标识标记如下：‘仅限于在特定的欧盟成员国内用于工业用途或仅供专业人士使用 – 请核实是否允许使用’。"]
[null,{"$f":"IF($B$1=\"English\",C1543,IF($B$1=\"Deutsch\",D1543,IF($B$1=\"中文\",E1543,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"After 5 November, 2012 must not be placed on the market nor used as a substance or in mixtures in concentrations of  ≥ 0,1 mass-% for sealing applications such as injection, compression, grouting or pouring. "},"After 5 November, 2012 must not be placed on the market nor used as a substance or in mixtures in concentrations of  ≥ 0,1 mass-% for sealing applications such as injection, compression, grouting or pouring. ","Darf nach dem 5. November 2012 weder als Stoff noch in Gemischen in Konzentrationen von ≥ 0,1 Gew.-% für Abdichtungsanwendungen wie beispielsweise\nInjektion, Verpressung, Verfugung oder Verguss in Verkehr gebracht oder verwendet werden.","当物质或制剂中该成分含量大于等于0.1%，在2012年11月5日之后不得投放市场或者用于注浆"]
[null,{"$f":"IF($B$1=\"English\",C1544,IF($B$1=\"Deutsch\",D1544,IF($B$1=\"中文\",E1544,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Darf nicht in Erzeugnissen oder Bestandteilen davon in Konzentrationen von über 0,1 mg/kg verwendet werden.\n\nErzeugnisse oder deren Bestandteile, die DMF in einer Konzentration von über 0,1 mg/kg enthalten, dürfen nicht in den Verkehr gebracht werden."},"Darf nicht in Erzeugnissen oder Bestandteilen davon in Konzentrationen von über 0,1 mg/kg verwendet werden.\n\nErzeugnisse oder deren Bestandteile, die DMF in einer Konzentration von über 0,1 mg/kg enthalten, dürfen nicht in den Verkehr gebracht werden.","Darf nicht in Erzeugnissen oder Bestandteilen davon in Konzentrationen von über 0,1 mg/kg verwendet werden.\n\nErzeugnisse oder deren Bestandteile, die DMF in einer Konzentration von über 0,1 mg/kg enthalten, dürfen nicht in den Verkehr gebracht werden.","在成品或组件上含量大于等于0.1%不得使用。\n\n成品或组件上含DMF()浓度大于等于0.1%的产品不得投放市场。"]
[null,{"$f":"IF($B$1=\"English\",C1545,IF($B$1=\"Deutsch\",D1545,IF($B$1=\"中文\",E1545,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Must not be placed on the market or used as substance or constituent of mixtures in a concentration of 1 % mass fraction or more if the substance or the mixture are placed on the market or used as an air freshener or a deoderant in toilets, private households, offices or other inside rooms that are open to the public.  "},"Must not be placed on the market or used as substance or constituent of mixtures in a concentration of 1 % mass fraction or more if the substance or the mixture are placed on the market or used as an air freshener or a deoderant in toilets, private households, offices or other inside rooms that are open to the public.  ","Darf als Stoff oder Bestandteil von Gemischen in einer Konzentration von 1 Gewichtsprozent oder mehr nicht in Verkehr gebracht oder verwendet werden, wenn der Stoff oder das Gemisch zur Verwendung als Lufterfrischer oder Deodorant in Toiletten, Privathaushalten, Büros oder anderen öffentlich zugänglichen Innenräumen in Verkehr gebracht oder als solche verwendet wird.","当物质或制剂作为用于卫生间、私人住宅、办公室或者其它公共室内场所的空气清新剂或除臭剂投放市场或者投入使用时，在上述物质或制剂中的质量百分比不得超过1%"]
[null,{"$f":"IF($B$1=\"English\",C1546,IF($B$1=\"Deutsch\",D1546,IF($B$1=\"中文\",E1546,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nitrobenzene"},"Nitrobenzene","Nitrobenzene","硝基苯 "]
[null,{"$f":"IF($B$1=\"English\",C1547,IF($B$1=\"Deutsch\",D1547,IF($B$1=\"中文\",E1547,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4-di-tert-butyl-6-(5-chlorobenzotriazol-2-yl)phenol (UV-327)"},"2,4-di-tert-butyl-6-(5-chlorobenzotriazol-2-yl)phenol (UV-327)","2,4-di-tert-butyl-6-(5-chlorobenzotriazol-2-yl)phenol (UV-327)","2,4-二叔丁基-6-(5-氯-2-苯并三唑)苯酚 UV-327"]
[null,{"$f":"IF($B$1=\"English\",C1548,IF($B$1=\"Deutsch\",D1548,IF($B$1=\"中文\",E1548,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)"},"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)","2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)","2-(2’-羟基-3’-仲-丁基-5’-叔-丁基苯基) 苯並三唑 (UV-350)"]
[null,{"$f":"IF($B$1=\"English\",C1549,IF($B$1=\"Deutsch\",D1549,IF($B$1=\"中文\",E1549,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-propanesultone"},"1,3-propanesultone","1,3-propanesultone","1,3-丙基磺酸内酯"]
[null,{"$f":"IF($B$1=\"English\",C1550,IF($B$1=\"Deutsch\",D1550,IF($B$1=\"中文\",E1550,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorononan-1-oic-acid and its sodium and ammonium saltspropanesultone"},"Perfluorononan-1-oic-acid and its sodium and ammonium saltspropanesultone","Perfluorononan-1-oic-acid and its sodium and ammonium saltspropanesultone","全氟壬酸及其钠盐、铵盐 "]
[null,{"$f":"IF($B$1=\"English\",C1551,IF($B$1=\"Deutsch\",D1551,IF($B$1=\"中文\",E1551,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of other substances"},"Manufacture of other substances","Herstellung anderer Substanzen","其它物质的生产"]
[null,{"$f":"IF($B$1=\"English\",C1552,IF($B$1=\"Deutsch\",D1552,IF($B$1=\"中文\",E1552,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV-protection agents in coatings, plastics, rubber and cosmetics "},"UV-protection agents in coatings, plastics, rubber and cosmetics ","UV-Schutzmittel in Beschichtungen, Kunststoffen,  Gummi und Kosmetika","涂层、塑料、橡胶和化妆品中的紫外线防护剂 "]
[null,{"$f":"IF($B$1=\"English\",C1553,IF($B$1=\"Deutsch\",D1553,IF($B$1=\"中文\",E1553,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV-protection agents in coatings, plastics, rubber and cosmetics"},"UV-protection agents in coatings, plastics, rubber and cosmetics","UV-Schutzmittel in Beschichtungen, Kunststoffen,  Gummi und Kosmetika","涂层、塑料、橡胶和化妆品中的紫外线防护剂 "]
[null,{"$f":"IF($B$1=\"English\",C1554,IF($B$1=\"Deutsch\",D1554,IF($B$1=\"中文\",E1554,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electrolyte fluid of lithium ion batteries"},"Electrolyte fluid of lithium ion batteries","Electrolytflüssigkeiten von Lithium-Ionen-Batterien","锂离子电池中的电解液 "]
[null,{"$f":"IF($B$1=\"English\",C1555,IF($B$1=\"Deutsch\",D1555,IF($B$1=\"中文\",E1555,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Processing aid for fluoropolymer manufacture/lubricating oil additive/surdactant for fire extinguishers/cleaning agent/textile antifouling finishing agent/polishing surfactant/waterproofing agents and in liquid crystal display panels"},"Processing aid for fluoropolymer manufacture/lubricating oil additive/surdactant for fire extinguishers/cleaning agent/textile antifouling finishing agent/polishing surfactant/waterproofing agents and in liquid crystal display panels","Verarbeitungshilfe für Fluorpolymerherstellung/Schmieröluisatz/surdactant für Feuerlöscher/Reinigungsmittel/textile antifouling finishing agent/polishing surfactant/waterproofing agents and in liquid crystal display panels","作为含氟聚合物用于制造润滑油添加剂/ 灭火剂/ 清洗剂/ 纺织品防水防污整理剂/ 表面抛光活性剂/ 防水剂/ 液晶显示面板 "]
[null,{"$f":"IF($B$1=\"English\",C1556,IF($B$1=\"Deutsch\",D1556,IF($B$1=\"中文\",E1556,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1557,IF($B$1=\"Deutsch\",D1557,IF($B$1=\"中文\",E1557,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1558,IF($B$1=\"Deutsch\",D1558,IF($B$1=\"中文\",E1558,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SSCP"},"SSCP","SSCP","SSCP"]
[null,{"$f":"IF($B$1=\"English\",C1559,IF($B$1=\"Deutsch\",D1559,IF($B$1=\"中文\",E1559,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloralkene C10-C13 (SCCP)"},"Chloralkene C10-C13 (SCCP)","Chloralken C10-C13 (SCCP)","氯代烃C10-C13（短链氯化石蜡SCCP）"]
[null,{"$f":"IF($B$1=\"English\",C1560,IF($B$1=\"Deutsch\",D1560,IF($B$1=\"中文\",E1560,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"POP ordinance 850/2004, 2015/2030"},"POP ordinance 850/2004, 2015/2030","POP Verordnung 850/2004, 2015/2030","持续性有机污染物(POP)行政立法 ,850/2004,2015/2030"]
[null,{"$f":"IF($B$1=\"English\",C1561,IF($B$1=\"Deutsch\",D1561,IF($B$1=\"中文\",E1561,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"GC-MS"},"GC-MS","GC-MS","气相色谱-质谱联用 "]
[null,{"$f":"IF($B$1=\"English\",C1562,IF($B$1=\"Deutsch\",D1562,IF($B$1=\"中文\",E1562,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,15 % w/w"},"0,15 % w/w","0,15 % w/w","0,15 % 重量百分比"]
[null,{"$f":"IF($B$1=\"English\",C1563,IF($B$1=\"Deutsch\",D1563,IF($B$1=\"中文\",E1563,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alterations until 2016-06-20 and SVHC candidates list of 2016-06-20"},"Alterations until 2016-06-20 and SVHC candidates list of 2016-06-20","Änderungen bis 20.06.2016 und SVHC Kandidatenliste vom 20.06.2016","2014-07-14更新，2015-12-17的SVHC候选清单 "]
[null,{"$f":"IF($B$1=\"English\",C1564,IF($B$1=\"Deutsch\",D1564,IF($B$1=\"中文\",E1564,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzenamine, N-phenyl-,Reaction Products with Styrene and 2,4,4- Trimethylpenten (BNST)"},"Benzenamine, N-phenyl-,Reaction Products with Styrene and 2,4,4- Trimethylpenten (BNST)","Benzenamin, N-phenyl-, Reaktionsprodukte mit  Styren und 2,4,4- Trimethylpenten (BNST)","苯胺、N-苯基-、与苯乙烯和2，2，4三-三甲基戊烯反应产物（BNST）"]
[null,{"$f":"IF($B$1=\"English\",C1565,IF($B$1=\"Deutsch\",D1565,IF($B$1=\"中文\",E1565,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Additive for elastomer compounds and lubricants"},"Additive for elastomer compounds and lubricants","Zusatzstoffe für Elastomerverbindungfen und Schmiermittel","弹性体化合物和润滑剂的添加剂 "]
[null,{"$f":"IF($B$1=\"English\",C1566,IF($B$1=\"Deutsch\",D1566,IF($B$1=\"中文\",E1566,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material group"},"Material group","Stoffgruppe","材料组 "]
[null,{"$f":"IF($B$1=\"English\",C1567,IF($B$1=\"Deutsch\",D1567,IF($B$1=\"中文\",E1567,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"see tab 5_ROHS"},"see tab 5_ROHS","siehe Reiter 5_ROHS","见表格5 - RoHS"]
[null,{"$f":"IF($B$1=\"English\",C1568,IF($B$1=\"Deutsch\",D1568,IF($B$1=\"中文\",E1568,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C1569,IF($B$1=\"Deutsch\",D1569,IF($B$1=\"中文\",E1569,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury"},"Mercury","Quecksilber","汞"]
[null,{"$f":"IF($B$1=\"English\",C1570,IF($B$1=\"Deutsch\",D1570,IF($B$1=\"中文\",E1570,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"hexavalent chromium"},"hexavalent chromium","Chrom VI","六价铬"]
[null,{"$f":"IF($B$1=\"English\",C1571,IF($B$1=\"Deutsch\",D1571,IF($B$1=\"中文\",E1571,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Flame ratardants"},"Flame ratardants","Flammschutzmittel","阻燃剂 "]
[null,{"$f":"IF($B$1=\"English\",C1572,IF($B$1=\"Deutsch\",D1572,IF($B$1=\"中文\",E1572,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated biphenyls (PBB)"},"Polybrominated biphenyls (PBB)","Polybromierte Biphenyle (PBB)","多溴联苯（PBB） "]
[null,{"$f":"IF($B$1=\"English\",C1573,IF($B$1=\"Deutsch\",D1573,IF($B$1=\"中文\",E1573,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated diphenyl ethers (PBDE)"},"Polybrominated diphenyl ethers (PBDE)","Polybromierte Diphenylether (PBDE)","多溴二苯醚（PBDE） "]
[null,{"$f":"IF($B$1=\"English\",C1574,IF($B$1=\"Deutsch\",D1574,IF($B$1=\"中文\",E1574,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo(a)pyrene, Benzo(def)chrysene"},"Benzo(a)pyrene, Benzo(def)chrysene","Benzo(a)pyrene, Benzo(def)chrysene","苯并 (a) 芘，苯并(def)屈"]
[null,{"$f":"IF($B$1=\"English\",C1575,IF($B$1=\"Deutsch\",D1575,IF($B$1=\"中文\",E1575,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The substance is a PAH, that is typically contained in black carbon for coloring black cables, rubber or plastic or tires."},"The substance is a PAH, that is typically contained in black carbon for coloring black cables, rubber or plastic or tires.","PAK, typischerweise in Kohlenstoff zum Einfärben schwarzer Kabel, Gummi oder Kunststoff oder Reifen.","该物质为多环芳烃，常用于给黑色导线、橡胶、塑料或轮胎上色的炭黑中"]
[null,{"$f":"IF($B$1=\"English\",C1576,IF($B$1=\"Deutsch\",D1576,IF($B$1=\"中文\",E1576,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alterations until 2017-01-27 and SVHC candidates list of 2017-01-12"},"Alterations until 2017-01-27 and SVHC candidates list of 2017-01-12","Änderungen bis 27.01.2017 und Kandidatenliste 12. Januar 2017","2014-07-14更新，2015-12-17的SVHC候选清单 "]
[null,{"$f":"IF($B$1=\"English\",C1577,IF($B$1=\"Deutsch\",D1577,IF($B$1=\"中文\",E1577,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-isopropylidendiphenol\nBisphenol A\n"},"4,4'-isopropylidendiphenol\nBisphenol A\n","4,4'-isopropylidendiphenol\nBisphenol A\n","4,4'-异丙基二苯酚A"]
[null,{"$f":"IF($B$1=\"English\",C1578,IF($B$1=\"Deutsch\",D1578,IF($B$1=\"中文\",E1578,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the production of epoxies and epoxy hardeners (industrial and professional applications), coating material, for the preparation of polymers, such as e.g. Polycarbonates and PVC; Use in thermal paper (industrial, professional and consumer)"},"For the production of epoxies and epoxy hardeners (industrial and professional applications), coating material, for the preparation of polymers, such as e.g. Polycarbonates and PVC; Use in thermal paper (industrial, professional and consumer)","Zur Herstellung von Epoxiden und Expoxid Härtern (industrielle und professionelle Anwendungen), Beschichtungsmaterial, Zur Herstellung von Polymeren, wie z.B. Polycarbonaten und PVC; Verwendung in Thermopapier (industriell, professionell und Verbraucher)","用于制造环氧化物和环氧化物硬化剂（工业和专业用途）、涂料；用于制备聚合物，例如聚碳酸酯和PVC；用于热敏纸（工业、专业和消费用途）"]
[null,{"$f":"IF($B$1=\"English\",C1579,IF($B$1=\"Deutsch\",D1579,IF($B$1=\"中文\",E1579,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-heptylphenol, branched and linear - (4-HPbl)\n"},"4-heptylphenol, branched and linear - (4-HPbl)\n","4-Heptylphenol, verzweigt und linear                     -  (4-HPbl)\n","4-庚基酚，支链和直链 - （4-HPbl）"]
[null,{"$f":"IF($B$1=\"English\",C1580,IF($B$1=\"Deutsch\",D1580,IF($B$1=\"中文\",E1580,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomer for the production of polymers"},"Monomer for the production of polymers","Monomer zur Herstellung von Polymeren","单体，用于制备聚合物"]
[null,{"$f":"IF($B$1=\"English\",C1581,IF($B$1=\"Deutsch\",D1581,IF($B$1=\"中文\",E1581,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts\nnonadecafluorodecanoic\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat\n3) nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts\nnonadecafluorodecanoic\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat"},"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts\nnonadecafluorodecanoic\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat\n3) nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts\nnonadecafluorodecanoic\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat","Nonadecafluorodecansäure (PFDA) und ihre Natrium- und Ammonium-Salze\nNonadecafluordecansäure\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat\n3) Nonadecafluorodecansäure (PFDA) und ihre Natrium- und Ammonium-Salze\nNonadecafluordecansäure\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat\n","十九氟癸酸（PFDA）及其钠盐和铵盐\n十九氟癸酸\n十九氟十一酸铵\n十九碳芥酸钠\n3）十九氟癸酸（PFDA）及其钠盐和铵盐\n十九氟癸酸\n十九氟十一酸铵\n十九氟十一酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1582,IF($B$1=\"Deutsch\",D1582,IF($B$1=\"中文\",E1582,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"et al as a corrosion inhibitor, lubricants, plasticizers"},"et al as a corrosion inhibitor, lubricants, plasticizers","u.a. als Korrosionsinhibitor, Schmiermittel, Weichmacher","例如，作为防腐剂，润滑剂，增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C1583,IF($B$1=\"Deutsch\",D1583,IF($B$1=\"中文\",E1583,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-(1,1-dimethylpropyl)phenol\n4-tert-Pentylphenol (PTAP)"},"p-(1,1-dimethylpropyl)phenol\n4-tert-Pentylphenol (PTAP)","p-(1,1-dimethylpropyl)phenol\n4-tert-Pentylphenol (PTAP)","对 - （1,1-二甲基丙基）苯酚\n4-叔戊基苯酚（PTAP）"]
[null,{"$f":"IF($B$1=\"English\",C1584,IF($B$1=\"Deutsch\",D1584,IF($B$1=\"中文\",E1584,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the manufacture of chemicals and plastic products"},"For the manufacture of chemicals and plastic products","Zur Herstellung von Chemikalien und Erzeugnissen aus Plastik","用于制造化学品和塑料制品"]
[null,{"$f":"IF($B$1=\"English\",C1585,IF($B$1=\"Deutsch\",D1585,IF($B$1=\"中文\",E1585,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in steel for machining purposes and in galvanised steel containing up to 0,35 % lead by weight"},"Lead as an alloying element in steel for machining purposes and in galvanised steel containing up to 0,35 % lead by weight","Blei  als  Legierungselement  in  Stahl  für  Bearbei­ tungszwecke  und  in  verzinktem  Stahl  mit  einem Massenanteil  von  höchstens  0,35 %  Blei","机械加工用钢材和镀锌钢，铅≤0.35 %"]
[null,{"$f":"IF($B$1=\"English\",C1586,IF($B$1=\"Deutsch\",D1586,IF($B$1=\"中文\",E1586,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in aluminium containing up to 0,4 % lead by weight"},"Lead as an alloying element in aluminium containing up to 0,4 % lead by weight","Blei  als  Legierungselement  in  Aluminium  mit  einem  Massenanteil  von  höchstens  0,4 %  Blei","铝合金，铅≤0.4％"]
[null,{"$f":"IF($B$1=\"English\",C1587,IF($B$1=\"Deutsch\",D1587,IF($B$1=\"中文\",E1587,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Copper alloy containing up to 4 % lead by weight"},"Copper alloy containing up to 4 % lead by weight","Kupferlegierung  mit  einem  Massenanteil  von  bis zu  4 %  Blei","铜合金，铅 ≤ 4%"]
[null,{"$f":"IF($B$1=\"English\",C1588,IF($B$1=\"Deutsch\",D1588,IF($B$1=\"中文\",E1588,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in high melting temperature type solders (i.e. lead-based alloys containing 85 % by weight or more lead)"},"Lead in high melting temperature type solders (i.e. lead-based alloys containing 85 % by weight or more lead)","Blei  in  hochschmelzenden  Loten  (d.  h.  Lötlegierungen  auf  Bleibasis  mit  einem  Massenanteil  von mindestens  85 %  Blei)","高熔点焊料中的铅（如铅含量重量比在85%及以上）"]
[null,{"$f":"IF($B$1=\"English\",C1589,IF($B$1=\"Deutsch\",D1589,IF($B$1=\"中文\",E1589,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g. piezoelectronic devices, or in a glass or ceramic matrix compound"},"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g. piezoelectronic devices, or in a glass or ceramic matrix compound","Blei enthaltende elektrische und elektronische Bauteile  in  Glas  oder  Keramikwerkstoffen  außer  di­ elektrischer  Keramik  in  Kondensatoren,  z.  B.  piezoelektronische  Geräte,  oder  in  einer  Glas-  oder Keramikmatrixverbindung","除电容器的介电陶瓷外的其他电子电气元器件中陶瓷或者玻璃中的铅，例如压电设备，或玻璃、陶瓷基的复合材料中的铅"]
[null,{"$f":"IF($B$1=\"English\",C1590,IF($B$1=\"Deutsch\",D1590,IF($B$1=\"中文\",E1590,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher"},"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher","Blei  in  dielektrischer  Keramik  in  Kondensatoren für  eine  Nennspannung  von  125  V  AC  oder  250 V  DC  oder  darüber","额定电压大于等于交流125 V或直流250 V的电容器介电陶瓷中的铅"]
[null,{"$f":"IF($B$1=\"English\",C1591,IF($B$1=\"Deutsch\",D1591,IF($B$1=\"中文\",E1591,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC"},"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC","Blei  in  dielektrischer  Keramik  in  Kondensatoren für  eine  Nennspannung   von  weniger  als  125  V AC  oder  250  V  DC","额定电压低于交流125 V或直流250 V的电容器介电陶瓷中的铅"]
[null,{"$f":"IF($B$1=\"English\",C1592,IF($B$1=\"Deutsch\",D1592,IF($B$1=\"中文\",E1592,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in PZT based dielectric ceramic materials for capacitors which are part of integrated circuits or discrete semiconductors"},"Lead in PZT based dielectric ceramic materials for capacitors which are part of integrated circuits or discrete semiconductors","Blei in PZT-basierten dielektrischen Keramikwerkstoffen   für   Kondensatoren,   die   Teil   integrierter Schaltkreise  oder  diskreter  Halbleiter  sind","电容器的电陶瓷材料PZT中的铅，该电容器是集成电路或分离半导体的组成部分"]
[null,{"$f":"IF($B$1=\"English\",C1593,IF($B$1=\"Deutsch\",D1593,IF($B$1=\"中文\",E1593,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 January 2013 and after that date may be used in spare parts for EEE placed on the market before 1 January 2013"},"Expires on 1 January 2013 and after that date may be used in spare parts for EEE placed on the market before 1 January 2013","Läuft  am  1.  Januar  2013  ab.  Danach  Verwendung zulässig  in  Ersatzteilen für  Elektro-  und  Elektronik­ geräte,  die  vor  dem  1.  Januar  2013  in  Verkehr  ge­ bracht  wurden.","豁免期至2013年1月1日，在该日期之后，2013年1月1前投放市场的电子电气产品的备件中仍可使用。"]
[null,{"$f":"IF($B$1=\"English\",C1594,IF($B$1=\"Deutsch\",D1594,IF($B$1=\"中文\",E1594,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 21 July 2016"},"Expires on 21 July 2016","Läuft  am  21.  Juli  2016  ab.","豁免期至2016年7月21日。"]
[null,{"$f":"IF($B$1=\"English\",C1595,IF($B$1=\"Deutsch\",D1595,IF($B$1=\"中文\",E1595,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Expires on 1 July 2014"},"Expires on 1 July 2014","Läuft  am  1.  Juli  2014  ab.","豁免至2014年7月1日。"]
[null,{"$f":"IF($B$1=\"English\",C1596,IF($B$1=\"Deutsch\",D1596,IF($B$1=\"中文\",E1596,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SCCP"},"SCCP","SCCP","SCCP"]
[null,{"$f":"IF($B$1=\"English\",C1597,IF($B$1=\"Deutsch\",D1597,IF($B$1=\"中文\",E1597,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"RoHS 2019"},"RoHS 2019","RoHS 2019","RoHS 2019"]
[null,{"$f":"IF($B$1=\"English\",C1598,IF($B$1=\"Deutsch\",D1598,IF($B$1=\"中文\",E1598,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulation Text with exemptions 01.09.2023"},"Regulation Text with exemptions 01.09.2023","Text der Regulierung und Ausnahmen 01.09.2023","包含豁免的法規文本 01.09.2023"]
[null,{"$f":"IF($B$1=\"English\",C1599,IF($B$1=\"Deutsch\",D1599,IF($B$1=\"中文\",E1599,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient "},"Concentration of ingredient ","Konzentration des Inhaltsstoffs ","组分含量"]
[null,{"$f":"IF($B$1=\"English\",C1600,IF($B$1=\"Deutsch\",D1600,IF($B$1=\"中文\",E1600,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 [mass% in homogeneous material]"},"0,1 [mass% in homogeneous material]","0,1 [Massen% im homogenen Werkstoff]","0,1 [均质材料中质量百分数％]"]
[null,{"$f":"IF($B$1=\"English\",C1601,IF($B$1=\"Deutsch\",D1601,IF($B$1=\"中文\",E1601,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n- Last Application Date: 4. January 2019\n- Sunset Date: 4. July 2020"},"Included in Annex 14\n- Last Application Date: 4. January 2019\n- Sunset Date: 4. July 2020","Aufgenommen in Anhang 14\n- Antragsschluss: 4. Januar 2019\n- Ablauftermin: 4. Juli 2020","已包括在附件14中\n-申请截止日期：2019年1月4日\n-日落之日（废止日期）：2020年7月4日\n"]
[null,{"$f":"IF($B$1=\"English\",C1602,IF($B$1=\"Deutsch\",D1602,IF($B$1=\"中文\",E1602,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n- Last Application Date: 4. April 2019\n- Sunset Date: 4. October 2020\n"},"Included in Annex 14\n- Last Application Date: 4. April 2019\n- Sunset Date: 4. October 2020\n","Aufgenommen in Anhang 14\n- Antragsschluss: 4. April 2019\n- Ablauftermin: 4. Oktober 2020","已包括在附件14中\n-申请截止日期：2019年4月4日\n-日落之日（废止日期）：2020年10月4日\n\n"]
[null,{"$f":"IF($B$1=\"English\",C1603,IF($B$1=\"Deutsch\",D1603,IF($B$1=\"中文\",E1603,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n- Last Application Date: 4. July 2019\n- Sunset Date: 4. January 2021"},"Included in Annex 14\n- Last Application Date: 4. July 2019\n- Sunset Date: 4. January 2021","Aufgenommen in Anhang 14\n- Antragsschluss: 4. Juli 2019\n- Ablauftermin: 4. Januar 2021","已包括在附件14中\n-申请截止日期：2019年7月4日\n-日落之日（废止日期）：2021年7月4日\n"]
[null,{"$f":"IF($B$1=\"English\",C1604,IF($B$1=\"Deutsch\",D1604,IF($B$1=\"中文\",E1604,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Changes Annex XVII up to 12.12.2023 and candidate list up to 23.01.2024."},"Changes Annex XVII up to 12.12.2023 and candidate list up to 23.01.2024.","Änderungen Annex XVII bis 12.12.2023 und Kandidatenliste bis 23.01.2024.","截至 2023 年 12 月 12 日更改附件十七，並於 2024 年 01 月 23 日更改候選名單。"]
[null,{"$f":"IF($B$1=\"English\",C1605,IF($B$1=\"Deutsch\",D1605,IF($B$1=\"中文\",E1605,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexane-1-sulfonic acid and its salts (PFHxS)"},"Perfluorohexane-1-sulfonic acid and its salts (PFHxS)","Perfluorhexansulfonsäure und seine Salze (PFHxS)","全氟己基磺酸及其盐类（PFHxS）"]
[null,{"$f":"IF($B$1=\"English\",C1606,IF($B$1=\"Deutsch\",D1606,IF($B$1=\"中文\",E1606,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"May be used as a plasticiser, lubricant, surfactant, wetting agent, corrosion inhibitor and in fire-fighting foams."},"May be used as a plasticiser, lubricant, surfactant, wetting agent, corrosion inhibitor and in fire-fighting foams.","May be used as a plasticiser, lubricant, surfactant, wetting agent, corrosion inhibitor and in fire-fighting foams.","可用作增塑剂，润滑剂，表面活性剂，润湿剂，缓蚀剂，或添加于泡沫灭火剂中"]
[null,{"$f":"IF($B$1=\"English\",C1607,IF($B$1=\"Deutsch\",D1607,IF($B$1=\"中文\",E1607,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisodecylphthalat (DIDP)"},"Diisodecylphthalat (DIDP)","Diisodecylphthalat (DIDP)","邻苯二甲酸二异癸酯 （DIDP）"]
[null,{"$f":"IF($B$1=\"English\",C1608,IF($B$1=\"Deutsch\",D1608,IF($B$1=\"中文\",E1608,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisononylphthalat (DINP)"},"Diisononylphthalat (DINP)","Diisononylphthalat (DINP)","邻苯二甲酸二异壬酯 （DINP）"]
[null,{"$f":"IF($B$1=\"English\",C1609,IF($B$1=\"Deutsch\",D1609,IF($B$1=\"中文\",E1609,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Only for declaration, concentration above limit value allowed, mandatory to declare concentration about limit value"},"Only for declaration, concentration above limit value allowed, mandatory to declare concentration about limit value","Deklarationspflichtig, darf auch in einer Konzentration über dem Grenzwert enthalten sein. \nAngabe der vorhandenen Konzentration über dem Grenzwert verpflichtend.","仅需要申报，浓度允许超过限值，当浓度超过限值，强制要求申报。"]
[null,{"$f":"IF($B$1=\"English\",C1610,IF($B$1=\"Deutsch\",D1610,IF($B$1=\"中文\",E1610,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EC-RoHS (tab 5)\n2011/65/EU and 2015/863/EU"},"EC-RoHS (tab 5)\n2011/65/EU and 2015/863/EU","EG-ROHS (Register 5)\n2011/65/EU und 2015/863/EU","ROHS - 欧盟RoHS指令（工作表5）\n2011/65/欧盟"]
[null,{"$f":"IF($B$1=\"English\",C1611,IF($B$1=\"Deutsch\",D1611,IF($B$1=\"中文\",E1611,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated terphenyls (PCTs)"},"Polychlorinated terphenyls (PCTs)","Polychlorierte Terphenyle (PCT)","多氯代三联苯 (PCTs)"]
[null,{"$f":"IF($B$1=\"English\",C1612,IF($B$1=\"Deutsch\",D1612,IF($B$1=\"中文\",E1612,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloroethene (vinyl chloride)"},"Chloroethene (vinyl chloride)","Chlorethen (Vinylchlorid)","氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C1613,IF($B$1=\"Deutsch\",D1613,IF($B$1=\"中文\",E1613,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris (2,3dibromopropyl) phosphate"},"Tris (2,3dibromopropyl) phosphate","Tri-(2,3-Dibrompropyl)-Phosphat","磷酸三(2,3-二溴丙基)酯 "]
[null,{"$f":"IF($B$1=\"English\",C1614,IF($B$1=\"Deutsch\",D1614,IF($B$1=\"中文\",E1614,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzene"},"Benzene","Benzol","苯"]
[null,{"$f":"IF($B$1=\"English\",C1615,IF($B$1=\"Deutsch\",D1615,IF($B$1=\"中文\",E1615,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Asbestos fibres:\n(a) Crocidolite\n\n(b) Amosite\n\n(c) Anthophyllite\n\n(d) Actinolite\n\n(e) Tremolite\n\n(f) Chrysotile"},"Asbestos fibres:\n(a) Crocidolite\n\n(b) Amosite\n\n(c) Anthophyllite\n\n(d) Actinolite\n\n(e) Tremolite\n\n(f) Chrysotile","Asbestfasern:\na) Krokydolith\n\nb) Amosit\n\nc) Anthophyllit\n\nd) Aktinolith\n\ne) Tremolit\n\nf) Chrysotil","石棉纤维：\n(a) 青石棉\n\n(b) 铁石棉\n\n(c) 直闪石\n\n(d) 阳起石\n\n(e) 透闪石\n\n(f) 温石棉"]
[null,{"$f":"IF($B$1=\"English\",C1616,IF($B$1=\"Deutsch\",D1616,IF($B$1=\"中文\",E1616,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(aziridinyl)phosphinoxide"},"Tris(aziridinyl)phosphinoxide","Tris-(aziridinyl)-phosphinoxid","三（吖丙啶基）氧化膦"]
[null,{"$f":"IF($B$1=\"English\",C1617,IF($B$1=\"Deutsch\",D1617,IF($B$1=\"中文\",E1617,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybromobiphenyls, Polybrominatedbiphenyls (PBB)"},"Polybromobiphenyls, Polybrominatedbiphenyls (PBB)","Polybrombiphenyle; polybromierte Biphenyle (PBB)","多溴联苯（PBB） "]
[null,{"$f":"IF($B$1=\"English\",C1618,IF($B$1=\"Deutsch\",D1618,IF($B$1=\"中文\",E1618,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-naphthylamine and its salts"},"2-naphthylamine and its salts","2-Naphthylamin und seine Salze","2-萘胺及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C1619,IF($B$1=\"Deutsch\",D1619,IF($B$1=\"中文\",E1619,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzidine and its salts"},"Benzidine and its salts","Benzidin und seine Salze","聯苯胺及其鹽"]
[null,{"$f":"IF($B$1=\"English\",C1620,IF($B$1=\"Deutsch\",D1620,IF($B$1=\"中文\",E1620,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nitrobiphenyl"},"4-Nitrobiphenyl"," 4-Nitrobiphenyl","4-硝基联苯"]
[null,{"$f":"IF($B$1=\"English\",C1621,IF($B$1=\"Deutsch\",D1621,IF($B$1=\"中文\",E1621,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Aminobiphenyl xenylamine and its salts"},"4-Aminobiphenyl xenylamine and its salts","4-Aminobiphenyl, Xenylamin und seine Salze","4-氨基联苯 苯基苯胺 及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C1622,IF($B$1=\"Deutsch\",D1622,IF($B$1=\"中文\",E1622,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead carbonates:\na) Neutral anhydrous carbonate (PbCO3)\n\nb) Trilead-bis(carbonate)-dihydroxide 2PbCO3-Pb(OH)2 "},"Lead carbonates:\na) Neutral anhydrous carbonate (PbCO3)\n\nb) Trilead-bis(carbonate)-dihydroxide 2PbCO3-Pb(OH)2 ","Bleicarbonate:\na) wasserfreies neutrales Karbonat PbCO3\n\nb) Triblei-bis(carbonat)-dihydroxid 2PbCO3-Pb(OH)2","碳酸铅：\na) 中性無水碳酸鹽（PbCO3）\n\nb) 三鉛-雙(碳酸鹽)-二氫氧化物2PbCO3-Pb(OH)2"]
[null,{"$f":"IF($B$1=\"English\",C1623,IF($B$1=\"Deutsch\",D1623,IF($B$1=\"中文\",E1623,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead sulphates:\na) Lead sulphate PbSO4\n\nb) Sulphuric acid, lead salt Pbx SO4"},"Lead sulphates:\na) Lead sulphate PbSO4\n\nb) Sulphuric acid, lead salt Pbx SO4","Bleisulfate:\na) Bleisulfat PbSO4\n\nb) Schwefelsäure, Bleisalz Pbx SO4","硫酸铅：\na) 硫酸铅 PbSO4\n\nb) 硫酸，铅盐 Pbx SO4"]
[null,{"$f":"IF($B$1=\"English\",C1624,IF($B$1=\"Deutsch\",D1624,IF($B$1=\"中文\",E1624,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury compounds"},"Mercury compounds","Quecksilberverbindungen","汞的化合物"]
[null,{"$f":"IF($B$1=\"English\",C1625,IF($B$1=\"Deutsch\",D1625,IF($B$1=\"中文\",E1625,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury"},"Mercury","Quecksilber","汞"]
[null,{"$f":"IF($B$1=\"English\",C1626,IF($B$1=\"Deutsch\",D1626,IF($B$1=\"中文\",E1626,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Arsenic compounds"},"Arsenic compounds","Arsenverbindungen","砷化合物"]
[null,{"$f":"IF($B$1=\"English\",C1627,IF($B$1=\"Deutsch\",D1627,IF($B$1=\"中文\",E1627,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Organostannic compounds"},"Organostannic compounds","Zinnorganische Verbindungen","有机锡化合物 "]
[null,{"$f":"IF($B$1=\"English\",C1628,IF($B$1=\"Deutsch\",D1628,IF($B$1=\"中文\",E1628,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Di-μ-oxo-di-n-butylstanniohydroxyborane / Dibutyltin hydrogen borate C8H19BO3Sn (DBB)"},"Di-μ-oxo-di-n-butylstanniohydroxyborane / Dibutyltin hydrogen borate C8H19BO3Sn (DBB)","Di-μ-oxo-di-n-butylstanniohydroxyboran, Dibutylzinnhydrogenborat C8H19BO3Sn (DBB)","二-μ-氧-正丁基锡羟基硼烷，二丁基锡氢硼烷 C8H19BO3Sn (DBB)"]
[null,{"$f":"IF($B$1=\"English\",C1629,IF($B$1=\"Deutsch\",D1629,IF($B$1=\"中文\",E1629,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally Pentachlorophenol and its salts and esters)"},"deleted (originally Pentachlorophenol and its salts and esters)","gestrichen (ursprünglich Pentachlorphenol und seine Salze und Ester)","删除（原五氯苯酚及其盐类和酯类）。"]
[null,{"$f":"IF($B$1=\"English\",C1630,IF($B$1=\"Deutsch\",D1630,IF($B$1=\"中文\",E1630,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and its compounds"},"Cadmium and its compounds","Cadmium","镉及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C1631,IF($B$1=\"Deutsch\",D1631,IF($B$1=\"中文\",E1631,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyl — tetrachlorodiphenyl methane Trade name: Ugilec 141"},"Monomethyl — tetrachlorodiphenyl methane Trade name: Ugilec 141","Monomethyl–tetrachlordiphenylmethan\nHandelsname: Ugilec 141","单甲基四氯二苯基甲烷 商品名：Ugilec 141"]
[null,{"$f":"IF($B$1=\"English\",C1632,IF($B$1=\"Deutsch\",D1632,IF($B$1=\"中文\",E1632,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyl-dichloro-diphenyl methane Trade name: Ugilec 121, Ugilec 21"},"Monomethyl-dichloro-diphenyl methane Trade name: Ugilec 121, Ugilec 21","Monomethyl–dichlordiphenylmethan\nHandelsname: Ugilec 121","单甲基二氯二苯甲烷 商品名：Ugilec 121, Ugilec 21"]
[null,{"$f":"IF($B$1=\"English\",C1633,IF($B$1=\"Deutsch\",D1633,IF($B$1=\"中文\",E1633,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomethyl-dibromo-diphenyl methane bromobenzylbromotoluene, mixture of isomers Trade name: DBBT"},"Monomethyl-dibromo-diphenyl methane bromobenzylbromotoluene, mixture of isomers Trade name: DBBT","Monomethyl–dibromdiphenylmethan Brombenzylbromtoluol, Isomerengemisch\nHandelsname: DBBT","单甲基二溴二苯基甲烷 溴苯甲基溴甲苯 及其异构体的混合物 商品名称：DBBT"]
[null,{"$f":"IF($B$1=\"English\",C1634,IF($B$1=\"Deutsch\",D1634,IF($B$1=\"中文\",E1634,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nickel and its compounds"},"Nickel and its compounds","Nickel und seine Verbindungen","镍及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C1635,IF($B$1=\"Deutsch\",D1635,IF($B$1=\"中文\",E1635,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances which are classified as carcinogen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 1 or Appendix 2, respectively."},"Substances which are classified as carcinogen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 1 or Appendix 2, respectively.","Stoffe, die in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 als krebserzeugend der Kategorie 1A oder 1B eingestuft werden und in Anlage 1 bzw. Anlage 2 aufgeführt werden.","在法规1272/2008/EC附件VI第3部分中被列为1A或1B类致癌物，并分别列于附录1或附录2的物质。"]
[null,{"$f":"IF($B$1=\"English\",C1636,IF($B$1=\"Deutsch\",D1636,IF($B$1=\"中文\",E1636,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances which are classified as germ cell mutagen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 3 or Appendix 4, respectively."},"Substances which are classified as germ cell mutagen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 3 or Appendix 4, respectively.","Stoffe, die in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 als erbgutverändernd der Kategorie 1A oder 1B eingestuft werden und in Anlage 3 bzw. Anlage 4 aufgeführt werden.","在法规1272/2008/EC附件VI第3部分中被列为1A或1B类生殖细胞诱变剂，并分别列于附录3或附录4的物质。"]
[null,{"$f":"IF($B$1=\"English\",C1637,IF($B$1=\"Deutsch\",D1637,IF($B$1=\"中文\",E1637,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substances which are classified as reproductive toxicant category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 5 or Appendix 6, respectively."},"Substances which are classified as reproductive toxicant category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 5 or Appendix 6, respectively.","Stoffe, die in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 als fortpflanzungsgefährdend der Kategorie 1A oder 1B eingestuft werden und in Anlage 5 bzw. Anlage 6 aufgeführt werden.","在法规1272/2008/EC附件VI第3部分中被列为1A或1B类生殖毒性物，并分别列于附录5或附录6的物质。"]
[null,{"$f":"IF($B$1=\"English\",C1638,IF($B$1=\"Deutsch\",D1638,IF($B$1=\"中文\",E1638,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(a) Creosote; wash oil\n\n(b) Creosote oil; wash oil\n\n(c) Distillates (coal tar), naphthalene oils; naphthalene oil\n\n(d) Creosote oil, acenaphthene fraction; wash oil\n\n(e) Distillates (coal tar), upper; heavy anthracene oil\n\n(f) Anthracene oil\n\n(g) Tar acids, coal, crude; crude phenols\n\n(h) Creosote, wood\n\n(i) Low temperature tar oil, alkaline; extract residues (coal), low temperature coal tar alkaline"},"(a) Creosote; wash oil\n\n(b) Creosote oil; wash oil\n\n(c) Distillates (coal tar), naphthalene oils; naphthalene oil\n\n(d) Creosote oil, acenaphthene fraction; wash oil\n\n(e) Distillates (coal tar), upper; heavy anthracene oil\n\n(f) Anthracene oil\n\n(g) Tar acids, coal, crude; crude phenols\n\n(h) Creosote, wood\n\n(i) Low temperature tar oil, alkaline; extract residues (coal), low temperature coal tar alkaline","a) Kreosot; Waschöl\n\nb) Kreosotöl, Waschöl\n\nc) Destillate (Kohlenteer), Naphthalinöle; Naphtalinöl\n\nd) Kreosotöl, Acenaphthen-Fraktion; Waschöl\n\ne) höher siedende Destillate (Kohlenteer); schweres Anthracenöl\n\nf) Anthracenöl\n\ng) Teersäuren, Kohle, Rohöl; Rohphenole\n\nh) Kreosot, Holz\n\ni) Niedrigtemperatur-Kohleteeralkalin, Extraktrückstände (Kohle)","(a) 杂酚油; 清洗用油\n\n(b) 杂酚油; 清洗用油\n\n(c) 石脑油蒸馏物\n\n(d) 杂酚油，苊的馏分；清洗用油\n\n(e) 干馏油（煤焦油），上层馏分；重蒽油\n\n(f) 蒽油\n\n(g) 焦油酸，煤，原油；粗苯酚\n\n(h) 杂酚油，木材\n\n(i) 碱性的低温焦油；煤取物中的碱性低温焦油；低温煤焦油碱 "]
[null,{"$f":"IF($B$1=\"English\",C1639,IF($B$1=\"Deutsch\",D1639,IF($B$1=\"中文\",E1639,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloroform"},"Chloroform","Chloroform","氯仿"]
[null,{"$f":"IF($B$1=\"English\",C1640,IF($B$1=\"Deutsch\",D1640,IF($B$1=\"中文\",E1640,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally Tetrachloromethane)"},"deleted (originally Tetrachloromethane)","gestrichen (ursprünglich Tetrachlormethan)","删除（原为四氯甲烷） "]
[null,{"$f":"IF($B$1=\"English\",C1641,IF($B$1=\"Deutsch\",D1641,IF($B$1=\"中文\",E1641,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,2-Trichloroethane"},"1,1,2-Trichloroethane","1,1,2-Trichlorethan","1, 1, 2-三氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1642,IF($B$1=\"Deutsch\",D1642,IF($B$1=\"中文\",E1642,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,2,2-Tetrachloroethane"},"1,1,2,2-Tetrachloroethane","1,1,2,2-Tetrachlorethan","1,1,2,2-四氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1643,IF($B$1=\"Deutsch\",D1643,IF($B$1=\"中文\",E1643,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2-Tetrachloroethane"},"1,1,1,2-Tetrachloroethane","1,1,1,2-Tetrachlorethan","1,1,1,2-四氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1644,IF($B$1=\"Deutsch\",D1644,IF($B$1=\"中文\",E1644,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachloroethane"},"Pentachloroethane","Pentachlorethan","五氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1645,IF($B$1=\"Deutsch\",D1645,IF($B$1=\"中文\",E1645,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1-Dichloroethene"},"1,1-Dichloroethene","1,1-Dichlorethen","1,1-二氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C1646,IF($B$1=\"Deutsch\",D1646,IF($B$1=\"中文\",E1646,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally 1,1,1-Trichloroethane"},"deleted (originally 1,1,1-Trichloroethane","gestrichen (urspünglich 1,1,1-Trichlorethan)","删除（原为1, 1, 1-三氯乙烷）"]
[null,{"$f":"IF($B$1=\"English\",C1647,IF($B$1=\"Deutsch\",D1647,IF($B$1=\"中文\",E1647,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachloroethane"},"Hexachloroethane","Hexachlorethan","六氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1648,IF($B$1=\"Deutsch\",D1648,IF($B$1=\"中文\",E1648,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally Chloroalkanes)"},"deleted (originally Chloroalkanes)","gestrichen (urspünglich Chloralkane)","删除（原为氯烷烃）"]
[null,{"$f":"IF($B$1=\"English\",C1649,IF($B$1=\"Deutsch\",D1649,IF($B$1=\"中文\",E1649,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Azocolourants and Azodyes"},"Azocolourants and Azodyes","Azofarbstoffe","偶氮着色剂及偶氮染料"]
[null,{"$f":"IF($B$1=\"English\",C1650,IF($B$1=\"Deutsch\",D1650,IF($B$1=\"中文\",E1650,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally Diphenylether, pentabromo derivative)"},"deleted (originally Diphenylether, pentabromo derivative)","gestrichen (ursprünglich Diphenylether-Pentabromderivat )","删除（原为二苯醚，五溴衍生物）"]
[null,{"$f":"IF($B$1=\"English\",C1651,IF($B$1=\"Deutsch\",D1651,IF($B$1=\"中文\",E1651,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenylether, octabromo derivative C12H2Br8O"},"Diphenylether, octabromo derivative C12H2Br8O","Diphenylether-Octabromderivat\nC12H2Br8O","二苯醚，八溴衍生物C12H2Br8O"]
[null,{"$f":"IF($B$1=\"English\",C1652,IF($B$1=\"Deutsch\",D1652,IF($B$1=\"中文\",E1652,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) Nonylphenol C6H4(OH)C9H19\n\nb) Nonylphenol ethoxylates (C2H4O)nC15H24O"},"a) Nonylphenol C6H4(OH)C9H19\n\nb) Nonylphenol ethoxylates (C2H4O)nC15H24O","a) Nonylphenol\nC6H4(OH)C9H19\n\nb) Nonylphenolethoxylate\n(C2H4O)nC15H24O","a) 壬基苯酚 C6H4(OH)C9H19\n\nb) 壬基酚聚乙氧基醚 (C2H4O)nC15H24O"]
[null,{"$f":"IF($B$1=\"English\",C1653,IF($B$1=\"Deutsch\",D1653,IF($B$1=\"中文\",E1653,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol ethoxylates (C2H4O)nC15H24O"},"Nonylphenol ethoxylates (C2H4O)nC15H24O","Nonylphenolethoxylate (NPE) (C2H4O)nC15H24O","壬基酚聚乙氧基醚 (C2H4O)nC15H24O"]
[null,{"$f":"IF($B$1=\"English\",C1654,IF($B$1=\"Deutsch\",D1654,IF($B$1=\"中文\",E1654,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium VI compounds"},"Chromium VI compounds","Chrom-VI-Verbindungen","六价铬化合物 "]
[null,{"$f":"IF($B$1=\"English\",C1655,IF($B$1=\"Deutsch\",D1655,IF($B$1=\"中文\",E1655,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Toluene"},"Toluene","Toluol","甲苯"]
[null,{"$f":"IF($B$1=\"English\",C1656,IF($B$1=\"Deutsch\",D1656,IF($B$1=\"中文\",E1656,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichlorobenzene"},"Trichlorobenzene","Trichlorbenzol","三氯苯"]
[null,{"$f":"IF($B$1=\"English\",C1657,IF($B$1=\"Deutsch\",D1657,IF($B$1=\"中文\",E1657,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polycyclic-aromatic hydrocarbons (PAH)\na) Benzo[a]pyrene (BaP)\n\nb) Dibenzo[a,h]anthracene (DBAhA)\n\nc) Benzo[a]anthracene (BaA)\n\nd) Chrysen (CHR)\n\ne) Benzo[j]fluoranthene (BjFA)\n\nf) Benzo[b]fluoranthene (BbFA)\n\ng) Benzo[k]fluoranthene (BkFA) \n\nh) Benzo[e]pyrene (BeP)"},"Polycyclic-aromatic hydrocarbons (PAH)\na) Benzo[a]pyrene (BaP)\n\nb) Dibenzo[a,h]anthracene (DBAhA)\n\nc) Benzo[a]anthracene (BaA)\n\nd) Chrysen (CHR)\n\ne) Benzo[j]fluoranthene (BjFA)\n\nf) Benzo[b]fluoranthene (BbFA)\n\ng) Benzo[k]fluoranthene (BkFA) \n\nh) Benzo[e]pyrene (BeP)","Polyzyklische aromatische Kohlenwasserstoffe (PAK)\na) Benzo(a)pyren (BaP)\nCAS-Nr. 50-32-8\n\nb) Benzo(e)pyren (BeP)\nCAS-Nr. 192-97-2\n\nc) Benzo(a)anthracen (BaA)\nCAS-Nr. 56-55-3\n\nd) Chrysen (CHR)\nCAS-Nr. 218-01-9\n\ne) Benzo(b)fluoranthen (BbFA)\nCAS-Nr. 205-99-2\n\nf) Benzo(j)fluoranthen (BjFA)\nCAS-Nr. 205-82-3\n\ng) Benzo(k)fluoranthen (BkFA)\nCAS-Nr. 207-08-9\n\nh) Dibenzo(a,h)anthracen (DBAhA)\nCAS-Nr. 53-70-3","多环芳烃(PAH)\na) 苯并[a]芘 (BaP)\n\nb) 二苯并[a,h]蒽(DBAhA)\n\nc) 苯并[a]蒽(BaA)\n\nd) 屈 (CHR)\n\ne) 苯并[j]荧蒽 (BjFA)\n\nf) 苯并[b]荧蒽(BbFA)\n\ng) 苯并[k]荧蒽(BkFA) \n\nh) 苯并[e]芘 (BeP)"]
[null,{"$f":"IF($B$1=\"English\",C1658,IF($B$1=\"Deutsch\",D1658,IF($B$1=\"中文\",E1658,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The following phthalates:\n(a) Bis (2-ethylhexyl) phthalate (DEHP)\n\n(b) Dibutyl phthalate (DBP)\n\n(c) Benzyl butyl phthalate (BBP)\n\n(d) Diisobutyl phthalate (DIBP)"},"The following phthalates:\n(a) Bis (2-ethylhexyl) phthalate (DEHP)\n\n(b) Dibutyl phthalate (DBP)\n\n(c) Benzyl butyl phthalate (BBP)\n\n(d) Diisobutyl phthalate (DIBP)","Folgende Phthalate:\na) Bis(2-ethylhexyl)phthalat (DEHP)\n\nb) Dibutylphthalat (DBP)\n\nc) Benzylbutylphthalat (BBP)\n\nd) Diisobutylphthalat (DIBP)","以下邻苯二甲酸酯:\n(a) 邻苯二甲酸二(2-乙基)己酯  (DEHP)\n\n(b) 邻苯二甲酸二丁酯 (DBP)\n\n(c) 邻苯二甲酸丁基苄基酯  (BBP)\n\n(d) 邻苯二甲酸二异丁酯 (DIBP)"]
[null,{"$f":"IF($B$1=\"English\",C1659,IF($B$1=\"Deutsch\",D1659,IF($B$1=\"中文\",E1659,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octamethylcyclotetrasiloxane (D4)               \nDecamethylcyclopentasiloxane (D5) "},"Octamethylcyclotetrasiloxane (D4)               \nDecamethylcyclopentasiloxane (D5) ","Octamethylcyclotetrasiloxan (D4)               Decamethylcyclopentasiloxan (D5) ","八甲基环四硅氧烷（D4）\n十甲基环五硅氧烷（D5）"]
[null,{"$f":"IF($B$1=\"English\",C1660,IF($B$1=\"Deutsch\",D1660,IF($B$1=\"中文\",E1660,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The following phthalates:\n(a) Di-‘isononyl’ phthalate (DINP)\n\n(b) Di-‘isodecyl’ phthalate (DIDP)\n\n(c) Di-n-octyl phthalate (DNOP)"},"The following phthalates:\n(a) Di-‘isononyl’ phthalate (DINP)\n\n(b) Di-‘isodecyl’ phthalate (DIDP)\n\n(c) Di-n-octyl phthalate (DNOP)","Folgende Phthalate:\na) Di-„isononyl“phthalat (DINP)\n\nb) Di-„isodecyl“phthalat (DIDP)\n\nc) Di-n-octylphthalat (DNOP)","以下邻苯二甲酸酯：\n(a) 邻苯二甲酸二异壬酯（DINP）   \n\n(b) 邻苯二甲酸二异癸酯（DIDP）   \n\n(c) 邻苯二甲酸二正辛酯（DNOP） "]
[null,{"$f":"IF($B$1=\"English\",C1661,IF($B$1=\"Deutsch\",D1661,IF($B$1=\"中文\",E1661,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally perfluorooctane sulfonates (PFOS))"},"deleted (originally perfluorooctane sulfonates (PFOS))","gestrichen (ursprünglich Perfluoroctansulfonat (PFOS))","删除 （原为 十七氟辛烷磺酸 (PFOS)）"]
[null,{"$f":"IF($B$1=\"English\",C1662,IF($B$1=\"Deutsch\",D1662,IF($B$1=\"中文\",E1662,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2-methoxyethoxy)ethanol (DEGME)"},"2-(2-methoxyethoxy)ethanol (DEGME)","2-(2-Methoxyethoxy)ethanol (DEGME)","2 -（2-甲氧基乙氧基）乙醇（DEGME） "]
[null,{"$f":"IF($B$1=\"English\",C1663,IF($B$1=\"Deutsch\",D1663,IF($B$1=\"中文\",E1663,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2-butoxyethoxy)ethanol (DEGBE)"},"2-(2-butoxyethoxy)ethanol (DEGBE)"," 2-(2-Butoxyethoxy)ethanol (DEGBE)","2-(2-丁氧基乙氧基)乙醇 (DEGBE)"]
[null,{"$f":"IF($B$1=\"English\",C1664,IF($B$1=\"Deutsch\",D1664,IF($B$1=\"中文\",E1664,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methylenediphenyl diisocyanate (MDI) including the following specific isomers (See group members):\n(a) 4,4’-Methylenediphenyl diisocyanate:\n\n(b) 2,4’-Methylenediphenyl diisocyanate:\n\n(c) 2,2’-Methylenediphenyl diisocyanate:"},"Methylenediphenyl diisocyanate (MDI) including the following specific isomers (See group members):\n(a) 4,4’-Methylenediphenyl diisocyanate:\n\n(b) 2,4’-Methylenediphenyl diisocyanate:\n\n(c) 2,2’-Methylenediphenyl diisocyanate:","Methylendiphenyl-Diisocyanat (MDI)\n\neinschließlich der nachstehenden spezifischen Isomere:\na)  4,4’-Methylendiphenyl-Diisocyanat (MDI)\n\nb) 2,4’-Methylendiphenyl-Diisocyanat (MDI)\n\nc) 2,2’-Methylendiphenyl-Diisocyanat (MDI)","二苯基甲烷二异氰酸酯 (MDI)，包括以下同分异构体：\n(a) 4,4’-二苯基甲烷二异氰酸酯 (MDI)\n(b) 2,4’-二苯基甲烷二异氰酸酯 (MDI)\n(c) 2,2’-二苯基甲烷二异氰酸酯 (MDI)"]
[null,{"$f":"IF($B$1=\"English\",C1665,IF($B$1=\"Deutsch\",D1665,IF($B$1=\"中文\",E1665,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cyclohexane"},"Cyclohexane","Cyclohexan","环己烷"]
[null,{"$f":"IF($B$1=\"English\",C1666,IF($B$1=\"Deutsch\",D1666,IF($B$1=\"中文\",E1666,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichloromethane"},"Dichloromethane","Dichlormethan","二氯甲烷"]
[null,{"$f":"IF($B$1=\"English\",C1667,IF($B$1=\"Deutsch\",D1667,IF($B$1=\"中文\",E1667,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acrylamide"},"Acrylamide","Acrylamid","丙烯酰胺 "]
[null,{"$f":"IF($B$1=\"English\",C1668,IF($B$1=\"Deutsch\",D1668,IF($B$1=\"中文\",E1668,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethyl fumarate (DMFu)"},"Dimethyl fumarate (DMFu)","Dimethylfumarat (DMF)","富马酸二甲酯 (DMFu)"]
[null,{"$f":"IF($B$1=\"English\",C1669,IF($B$1=\"Deutsch\",D1669,IF($B$1=\"中文\",E1669,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(a) Phenylmercury acetate\n\n(b) Phenylmercury propionate\n\n(c) Phenylmercury 2-ethylhexanoate\n\n(d) Phenylmercury octanoate\n\n(e) Phenylmercury neodecanoate"},"(a) Phenylmercury acetate\n\n(b) Phenylmercury propionate\n\n(c) Phenylmercury 2-ethylhexanoate\n\n(d) Phenylmercury octanoate\n\n(e) Phenylmercury neodecanoate","a) Phenylquecksilberacetat\n\nb) Phenylquecksilberpropionat\n\nc) Phenylquecksilber-2-ethylhexanoat\n\nd) Phenylquecksilberoctanoat\n\ne) Phenylquecksilberneodecanoat","(a) 苯基醋酸汞\n\n(b) 丙酸苯汞\n\n(c) 苯基汞-2-乙酸乙酯\n\n(d) 辛酸苯汞酯\n\n(e) 新癸酸苯汞"]
[null,{"$f":"IF($B$1=\"English\",C1670,IF($B$1=\"Deutsch\",D1670,IF($B$1=\"中文\",E1670,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and its compounds"},"Lead and its compounds","Blei und seine Verbindungen","铅及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C1671,IF($B$1=\"Deutsch\",D1671,IF($B$1=\"中文\",E1671,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,4-Dichlorobenzene"},"1,4-Dichlorobenzene","1,4-Dichlorbenzol","1,4-二氯苯 "]
[null,{"$f":"IF($B$1=\"English\",C1672,IF($B$1=\"Deutsch\",D1672,IF($B$1=\"中文\",E1672,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-isopropylidenediphenol"},"4,4'-isopropylidenediphenol","Bisphenol A","4,4’-异丙基二苯酚"]
[null,{"$f":"IF($B$1=\"English\",C1673,IF($B$1=\"Deutsch\",D1673,IF($B$1=\"中文\",E1673,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally Bis(pentabromophenyl) ether)"},"deleted (originally Bis(pentabromophenyl) ether)","gestrichen (ursprünglich Bis(pentabromphenyl)ether)","删除（原为十溴联苯醚）"]
[null,{"$f":"IF($B$1=\"English\",C1674,IF($B$1=\"Deutsch\",D1674,IF($B$1=\"中文\",E1674,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"deleted (originally Perfluorooctanoic acid (PFOA), its salts and PFOA-related substances)\nAny related substance (including its salts and polymers) having a linear or branched perfluoroheptyl group with the formula C7F15- directly attached to another carbon atom, as one of the structural elements.\nAny related substance (including its salts and polymers) having a linear or branched perfluorooctyl group with the formula C8F17- as one of the structural elements.\nThe following substances are excluded from this designation:\n— C8F17-X, where X = F, Cl, Br.\n— C8F17-C(=O)OH, C8F17-C(=O)O-X′ or C8F17-CF2-X′ (where X′ = any group, including salts)."},"deleted (originally Perfluorooctanoic acid (PFOA), its salts and PFOA-related substances)\nAny related substance (including its salts and polymers) having a linear or branched perfluoroheptyl group with the formula C7F15- directly attached to another carbon atom, as one of the structural elements.\nAny related substance (including its salts and polymers) having a linear or branched perfluorooctyl group with the formula C8F17- as one of the structural elements.\nThe following substances are excluded from this designation:\n— C8F17-X, where X = F, Cl, Br.\n— C8F17-C(=O)OH, C8F17-C(=O)O-X′ or C8F17-CF2-X′ (where X′ = any group, including salts).","gestrichen (ursprünglich Perfluoroctansäure (PFOA))","删除（原全氟辛酸（PFOA）、其盐类和全氟辛酸相关物质）\n任何具有直链或支链全氟庚基的相关物质（包括其盐类和聚合物），其化学式为C7F15-直接连接到另一个碳原子上，作为结构元素之一。\n任何相关物质（包括其盐类和聚合物），其结构元素之一为式为C8F17-的直链或支链全氟辛烷。\n下列物质不在此指定之列。\n- C8F17-X，其中X=F、Cl、Br。\n- C8F17-C(=O)OH，C8F17-C(=O)O-X′或 C8F17-CF2-X′（其中 X′=任何基团，包括盐类）。"]
[null,{"$f":"IF($B$1=\"English\",C1675,IF($B$1=\"Deutsch\",D1675,IF($B$1=\"中文\",E1675,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanol"},"Methanol","Methanol","甲醇"]
[null,{"$f":"IF($B$1=\"English\",C1676,IF($B$1=\"Deutsch\",D1676,IF($B$1=\"中文\",E1676,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octamethylcyclotetrasiloxane (D4); \nDecamethylcyclopentasiloxane (D5)"},"Octamethylcyclotetrasiloxane (D4); \nDecamethylcyclopentasiloxane (D5)","Octamethylcyclotetrasiloxan (D4)\nDecamethylcyclopentasiloxan (D5","八甲基环四硅氧烷（D4）\n十甲基环五硅氧烷（D5）"]
[null,{"$f":"IF($B$1=\"English\",C1677,IF($B$1=\"Deutsch\",D1677,IF($B$1=\"中文\",E1677,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-methyl-2-pyrrolidone"},"1-methyl-2-pyrrolidone","1-Methyl-2-pyrrolidon (NMP)","1-甲基-2-吡咯烷酮 "]
[null,{"$f":"IF($B$1=\"English\",C1678,IF($B$1=\"Deutsch\",D1678,IF($B$1=\"中文\",E1678,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The following substances which are classified as carcinogenic, mutagenic or toxic for reproduction, category 1A or 1B (See group members)"},"The following substances which are classified as carcinogenic, mutagenic or toxic for reproduction, category 1A or 1B (See group members)","Die in Spalte 1 der Tabelle in \nAnlage 12 der REACH VO aufgeführten Stoffe","下列被列为1A或1B类致癌、致突变或对生殖系统有毒的物质（详见法规）"]
[null,{"$f":"IF($B$1=\"English\",C1679,IF($B$1=\"Deutsch\",D1679,IF($B$1=\"中文\",E1679,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silanetriol and any of its mono-, di- or tri-O-(alkyl) derivatives"},"(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silanetriol and any of its mono-, di- or tri-O-(alkyl) derivatives","(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoroctyl)-silantriol seine Mono-, Di- oder Tri-O- (Alkyl)-Derivate","（3,3,4,4,5,5,6,6,7,8,8,8-十三氟辛基）硅烷三醇及其任意单、 双或三-邻-（烷基）衍生物"]
[null,{"$f":"IF($B$1=\"English\",C1680,IF($B$1=\"Deutsch\",D1680,IF($B$1=\"中文\",E1680,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisocyanates"},"Diisocyanates","Diisocyanate, O=C=N-R-N=C=O, wobei R eine aliphatische oder aromatische Kohlenwasserstoffeinheit beliebiger Länge ist","二异氰酸酯"]
[null,{"$f":"IF($B$1=\"English\",C1681,IF($B$1=\"Deutsch\",D1681,IF($B$1=\"中文\",E1681,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not beplaced on the market, or used:\n-as substances,\n-in mixtures, including waste oils, or in equipment, in concentrations greater than 50 mg/kg (0,005 % by weight)."},"Shall not beplaced on the market, or used:\n-as substances,\n-in mixtures, including waste oils, or in equipment, in concentrations greater than 50 mg/kg (0,005 % by weight).","Dürfen nicht in Verkehr gebracht oder verwendet werden:\n- als Stoffe,\n- in Gemischen, einschließlich Altölen, die mehr als 0,005 Gew.-% PCT enthalten.","不得在市场上投放或使用：\n-作为物质\n-用于混合物中，包括废油；或在设备中，浓度超过50mg/kg（0,005 %（重量））"]
[null,{"$f":"IF($B$1=\"English\",C1682,IF($B$1=\"Deutsch\",D1682,IF($B$1=\"中文\",E1682,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be used aspropellant in aerosols for any use.\nAerosols dispensers containing the substance as propellant shall not be placed on the market"},"Shall not be used aspropellant in aerosols for any use.\nAerosols dispensers containing the substance as propellant shall not be placed on the market","Darf für keinen Verwendungszweck als Treibgas für Aerosole verwendet werden.\n\nAerosolpackungen, die diesen Stoff als Treibgas enthalten, dürfen nicht in Verkehr gebracht werden.","不得在任何用途的气雾剂中使用助推剂。\n含有该物质作为推进剂的气雾剂分装器不得投放市场。"]
[null,{"$f":"IF($B$1=\"English\",C1683,IF($B$1=\"Deutsch\",D1683,IF($B$1=\"中文\",E1683,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin\n\n2. Articles not complying with paragraph 1 shall not be placed on the market."},"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin\n\n2. Articles not complying with paragraph 1 shall not be placed on the market.","1. Darf nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2. Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.","1.不可用于纺织品，例如服装、内衣及家庭日用织品等会与皮肤接触的物品\n2.产品不满足第1项，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C1684,IF($B$1=\"Deutsch\",D1684,IF($B$1=\"中文\",E1684,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" 1. Shall not be used in toys or parts of toys where the concentration of benzene in the free state is greater than 5 mg/kg (0,0005 %) of the weight of the toy or part of toy. \n2. Toys and parts of toys not complying with paragraph 1 shall not be placed on the market. \n3. Shall not be placed on the market, or used, \n- as a substance, \n- as a constituent of other substances, or in mixtures, in concentrations equal to, or greater than 0,1 % by weight. \n\n4. However, paragraph 3 shall not apply to: \n(a) motor fuels which are covered by Directive 98/70/EC; \n(b) substances and mixtures for use in industrial processes not allowing for the emission of benzene in quantities in excess of those laid down in existing legislation. \n(c) natural gas placed on the market for use by consumers, provided that the concentration of benzene remains below 0,1 % volume/volume’.\n"}," 1. Shall not be used in toys or parts of toys where the concentration of benzene in the free state is greater than 5 mg/kg (0,0005 %) of the weight of the toy or part of toy. \n2. Toys and parts of toys not complying with paragraph 1 shall not be placed on the market. \n3. Shall not be placed on the market, or used, \n- as a substance, \n- as a constituent of other substances, or in mixtures, in concentrations equal to, or greater than 0,1 % by weight. \n\n4. However, paragraph 3 shall not apply to: \n(a) motor fuels which are covered by Directive 98/70/EC; \n(b) substances and mixtures for use in industrial processes not allowing for the emission of benzene in quantities in excess of those laid down in existing legislation. \n(c) natural gas placed on the market for use by consumers, provided that the concentration of benzene remains below 0,1 % volume/volume’.\n","1. Darf nicht verwendet werden in Spielwaren oder Teilen von Spielwaren, wenn die Konzentration an frei verfügbarem Benzol höher als 5 mg/kg (0,0005 %) des Gewichts des Spielzeugs bzw. des Teils eines Spielzeugs ist.\n2. Spielwaren und Teile von Spielwaren, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.\n3. Darf nicht in Verkehr gebracht oder verwendet werden:\n - als Stoff,\n- als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von ≥ 0,1 Gew.-%.\n4. Absatz 3 gilt jedoch nicht für:\na) Treibstoffe, die unter die Richtlinie 98/70/EG fallen,\nb) Stoffe und Gemische, die bei industriellen Verfahren zur Anwendung kommen, bei denen Benzol nicht in höheren Konzentrationen freigesetzt werden darf, als in bestehenden Rechtsvorschriften festgelegt ist.\nc) Erdgas, das zur Verbrauchernutzung in Verkehr gebracht wird, unter der Voraussetzung, dass die Benzolkonzentration\nunter einem Wert von 0,1 Vol.- % bleibt.","1. 在玩具或者玩具的零部件中, 自由状态下苯酚浓度不得高于5mg/kg (0,0005%)；\n\n2. 不满足第1项的玩具或者玩具零件，不得投放市场。.\n\n3. 物质或者制剂中以重量计浓度大于0,1%时，不得投放市场或使用\n\n4. 然而，在以下情况下第3项不适用：\n（a）98/70/EC指令中覆盖的发动机燃料；\n（b）工业工艺中用到的物质和配制品，但苯的释放量不得超过其它现有法规的规定\n（c）投放市场供消费者使用的天然气，需满足苯的浓度保持在0.1%（体积）以下。 "]
[null,{"$f":"IF($B$1=\"English\",C1685,IF($B$1=\"Deutsch\",D1685,IF($B$1=\"中文\",E1685,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. The manufacture, placing on the market and use of these fibres and of articles and mixtures containing these fibres added intentionally is prohibited.\nHowever, if the use of diaphragms containing chrysotile for electrolysis installations in use on 13 July 2016 had been exempted by a Member State in accordance with the version of this paragraph in force until that date, the first subparagraph shall not apply until 1 July 2025 to the use in those installations of such diaphragms or of chrysotile used exclusively in the maintenance of such diaphragms, provided that such use is carried out in compliance with the conditions of a permit set in accordance with Directive 2010/75/EU of the European Parliament and of the Council (*).\nAny downstream user benefiting from such an exemption shall send, by 31 January of each calendar year to the Member State in which the relevant electrolysis installation is located, a report indicating the amount of chrysotile used in diaphragms pursuant to the exemption. The Member State shall transmit a copy to the European Commission.\nWhere, in order to protect the health and safety of workers, a Member State requires monitoring of chrysotile in air by downstream users, the results shall be included in that report.\n(*) Directive 2010/75/EU of the European Parliament and of the Council of 24 November 2010 on industrial emissions (integrated pollution prevention and control) (OJ L 334, 17.12.2010, p. 17).\n2. The use of articles containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005 shall continue to be permitted until they are disposed of or reach the end of their service life.\nHowever, Member States may, for reasons of protection of human health, restrict, prohibit or make subject to specific conditions, the use of such articles before they are disposed of or reach the end of their service life. Member States may allow placing on the market of articles in their entirety containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005, under specific conditions ensuring a high level of protection of human health. Member States shall communicate these national measures to the Commission by 1 June 2011. The Commission shall make this information publicly available.\n3. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, the placing on the market and use of articles containing these fibres, as permitted according to the preceding derogations, shall be permitted only if suppliers ensure before the placing on the market that articles bear a label in accordance with Appendix 7 to this Annex.\n"},"1. The manufacture, placing on the market and use of these fibres and of articles and mixtures containing these fibres added intentionally is prohibited.\nHowever, if the use of diaphragms containing chrysotile for electrolysis installations in use on 13 July 2016 had been exempted by a Member State in accordance with the version of this paragraph in force until that date, the first subparagraph shall not apply until 1 July 2025 to the use in those installations of such diaphragms or of chrysotile used exclusively in the maintenance of such diaphragms, provided that such use is carried out in compliance with the conditions of a permit set in accordance with Directive 2010/75/EU of the European Parliament and of the Council (*).\nAny downstream user benefiting from such an exemption shall send, by 31 January of each calendar year to the Member State in which the relevant electrolysis installation is located, a report indicating the amount of chrysotile used in diaphragms pursuant to the exemption. The Member State shall transmit a copy to the European Commission.\nWhere, in order to protect the health and safety of workers, a Member State requires monitoring of chrysotile in air by downstream users, the results shall be included in that report.\n(*) Directive 2010/75/EU of the European Parliament and of the Council of 24 November 2010 on industrial emissions (integrated pollution prevention and control) (OJ L 334, 17.12.2010, p. 17).\n2. The use of articles containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005 shall continue to be permitted until they are disposed of or reach the end of their service life.\nHowever, Member States may, for reasons of protection of human health, restrict, prohibit or make subject to specific conditions, the use of such articles before they are disposed of or reach the end of their service life. Member States may allow placing on the market of articles in their entirety containing asbestos fibres referred to in paragraph 1 which were already installed and/or in service before 1 January 2005, under specific conditions ensuring a high level of protection of human health. Member States shall communicate these national measures to the Commission by 1 June 2011. The Commission shall make this information publicly available.\n3. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, the placing on the market and use of articles containing these fibres, as permitted according to the preceding derogations, shall be permitted only if suppliers ensure before the placing on the market that articles bear a label in accordance with Appendix 7 to this Annex.\n","1. Die Herstellung, das Inverkehrbringen und die Verwendung dieser Fasern sowie von Erzeugnissen und Gemischen, denen diese Fasern absichtlich zugesetzt werden, ist verboten. Hatte jedoch ein Mitgliedstaat die Verwendung von chrysotilhaltigen Diaphragmen in Elektrolyseanlagen, die am 13. Juli 2016 in Betrieb waren, gemäß der bis zu dem genannten Tag geltenden Fassung dieses Absatzes ausnahmsweise gestattet, findet Unterabsatz 1 bis zum 1. Juli 2025 keine Anwendung auf die Verwendung von solchen Diaphragmen oder von Chrysotil, das ausschließlich bei der Wartung dieser Diaphragmen eingesetzt wird, in den betreffenden Anlagen, sofern diese Verwendung unter Beachtung der Auflagen einer Genehmigung erfolgt, die im Einklang mit der Richtlinie 2010/75/EU des Europäischen Parlaments und des Rates(*) festgelegt wurden. Nachgeschaltete Anwender, die in den Genuss einer solchen Ausnahmeregelung kommen, übermitteln dem Mitgliedstaat, in dem sich die betreffende Elektrolyseanlage befindet, bis zum 31. Januar eines jeden Kalenderjahres einen Bericht, aus dem die Menge an Chrysotil hervorgeht, die in Diaphragmen, die unter die Ausnahmeregelung fallen, verwendet wird. Der Mitgliedstaat übermittelt der Europäischen Kommission eine Kopie des Berichts. Schreibt ein Mitgliedstaat den nachgeschalteten Anwendern zum Schutz der Sicherheit und Gesundheit der Arbeitnehmer die Überwachung des Chrysotilgehalts in der Luft vor, müssen die Ergebnisse in den Bericht aufgenommen werden.\n2. Die Verwendung von Erzeugnissen, die Asbestfasern gemäß Absatz 1 enthalten und die schon vor dem 1. Januar 2005 installiert bzw. in Betrieb waren, ist weiterhin erlaubt, bis diese Erzeugnisse beseitigt werden oder bis ihre Nutzungsdauer abgelaufen ist. Jedoch können die Mitgliedstaaten zum Schutz der menschlichen Gesundheit die Verwendung solcher Erzeugnisse, bis sie beseitigt werden oder ihre Nutzungsdauer abgelaufen ist, einschränken, verbieten oder bestimmten Bedingungen unterwerfen.\nDie Mitgliedstaaten können das Inverkehrbringen kompletter Erzeugnisse, die Asbestfasern gemäß Absatz 1 enthalten und die schon vor dem 1. Januar 2005 installiert bzw. in Betrieb waren, unter bestimmten, ein hohes Maß an Schutz der menschlichen Gesundheit gewährleistenden Bedingungen gestatten. Die Mitgliedstaaten müssen die Kommission bis zum 1. Juni 2011 von solchen einzelstaatlichen Maßnahmen unterrichten. Die Angaben werden von der Kommission veröffentlicht.\n\n3. Unbeschadet der Anwendung anderer Gemeinschaftsvorschriften über die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen ist das gemäß den vorstehenden Ausnahmeregelungen erfolgende Inverkehrbringen und die gemäß den vorstehenden Ausnahmeregelungen erfolgende Verwendung von Erzeugnissen, die diese Fasern enthalten, nur zulässig, wenn der Lieferant vor dem Inverkehrbringen gewährleistet, dass die Erzeugnisse ein Etikett gemäß Anlage 7 dieses Anhangs tragen.\n___________\n(*) Richtlinie 2010/75/EU des Europäischen Parlaments und des Rates vom 24. November 2010 über Industrieemissionen (integrierte Vermeidung und Verminderung der Umweltverschmutzung) (ABl. L 334 vom 17.12.2010, S. 17).","1. 禁止制造、投放市场和使用这些纤维以及故意添加这些纤维的物品和混合物。\n但是，如果在2016年7月13日使用的电解装置中使用含有温石棉的隔膜已被成员国根据该日之前有效的本款版本豁免，则在2025年7月1日之前，第一项不适用于在这些装置中使用这种隔膜或专门用于维护这种隔膜的温石棉，条件是这种使用符合根据欧洲议会和理事会第2010/75/EU号指令（*）规定的许可证条件。\n任何受益于这种豁免的下游用户应在每个日历年的1月31日之前向相关电解装置所在的成员国发送一份报告，说明根据豁免规定用于隔膜的温石棉的数量。该成员国应向欧盟委员会转交一份副本。\n如果为了保护工人的健康和安全，成员国要求下游用户对空气中的温石棉进行监测，其结果应包括在该报告中。\n(*) 欧洲议会和理事会2010年11月24日关于工业排放（综合污染防治）的第2010/75/EU号指令（OJ L 334, 17.12.2010, p. 17）。\n2.在2005年1月1日之前已经安装和/或投入使用的第1项所述含石棉纤维的物品应继续允许使用，直到它们被处置或达到其使用寿命的终点。\n然而，成员国可以出于保护人类健康的原因，限制、禁止或在特定条件下，在这些物品被处置或达到其使用寿命之前使用这些物品。成员国可以允许在确保高度保护人类健康的特定条件下，将第1款中提及的、在2005年1月1日前已经安装和/或投入使用的含有石棉纤维的物品整体投放市场。成员国应在2011年6月1日前向委员会通报这些国家措施。委员会应公开提供这些信息。\n3.在不影响共同体关于物质和混合物的分类、包装和标签的其他规定的情况下，根据前述减损规定所允许的含有这些纤维的物品的投放市场和使用，只有在供应商在投放市场前确保物品上有符合本附件附录7的标签的情况下，才应允许。"]
[null,{"$f":"IF($B$1=\"English\",C1686,IF($B$1=\"Deutsch\",D1686,IF($B$1=\"中文\",E1686,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.\n"},"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.\n","1. Darf nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2. Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.","1.不可用于纺织品，例如服装、内衣及家庭日用织品等会与皮肤接触的物品\n2.产品不满足第1项，不得投放市场\n"]
[null,{"$f":"IF($B$1=\"English\",C1687,IF($B$1=\"Deutsch\",D1687,IF($B$1=\"中文\",E1687,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market."},"1. Shall not be used in textile articles, such as garments, undergarments and linen, intended to come into contact with the skin.\n2. Articles not complying with paragraph 1 shall not be placed on the market.","1. Dürfen nicht verwendet werden in Textilerzeugnissen, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen, beispielsweise in Oberbekleidung, Unterwäsche und Wäsche.\n2. Erzeugnisse, die Absatz 1 nicht erfüllen, dürfen nicht in Verkehr gebracht werden.","1.不可用于纺织品，例如服装、内衣及家庭日用织品等会与皮肤接触的物品\n2.产品不满足第1项，不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C1688,IF($B$1=\"Deutsch\",D1688,IF($B$1=\"中文\",E1688,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The following shall apply to entries 12 to 15: \nShall not be placed on the market, or used, as substances or in mixtures in concentrations greater than 0,1 % by weight."},"The following shall apply to entries 12 to 15: \nShall not be placed on the market, or used, as substances or in mixtures in concentrations greater than 0,1 % by weight.","Folgendes gilt für die Einträge 12 bis 15:\nDürfen weder als Stoffe noch in Gemischen in Konzentrationen von > 0,1 Gew.-% in Verkehr gebracht oder verwendet werden.","以下内容应适用于条目12至15:\n当其浓度按重量计超过0.1%,不得作为物质或混合物在市场上投放或使用。"]
[null,{"$f":"IF($B$1=\"English\",C1689,IF($B$1=\"Deutsch\",D1689,IF($B$1=\"中文\",E1689,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint.However, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof"},"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint.However, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof","Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Verwendung als Farben bestimmt sind.\n\nDie Mitgliedstaaten können jedoch gemäß dem IAO-Übereinkommen Nr. 13 in ihrem Hoheitsgebiet die Verwendung des Stoffs oder Gemischs\nzur Restaurierung und Unterhaltung von Kunstwerken sowie von historischen Gebäuden und ihren Inneneinrichtungen ebenso genehmigen wie das Inverkehrbringen für eine solche Verwendung. Ein Mitgliedstaat, der diese Ausnahmeregelung in Anspruch nimmt, unterrichtet die Kommission darüber.","物质或含该物质的制剂不得投放市场，或者作为涂料使用。但是，成员国可以许可，按照国际劳工组织第13号公约，在其领土内使用物质或含该物质的制剂用于恢复和维护艺术品和历史建筑和室内设计，以及许可其销售作此用途。一个成员国如要行使这项豁免，应通知欧盟委员会。"]
[null,{"$f":"IF($B$1=\"English\",C1690,IF($B$1=\"Deutsch\",D1690,IF($B$1=\"中文\",E1690,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint.However, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof."},"Shall not be placed on the market, or used, as substances or in mixtures, where the substance or mixture is intended for use as paint.However, Member States may, in accordance with the provisions of International Labour Organization (ILO) Convention 13, permit the use on their territory of the substance or mixture for the restoration and maintenance of works of art and historic buildings and their interiors, as well as the placing on the market for such use. Where a Member State makes use of this derogation, it shall inform the Commission thereof.","Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Verwendung als Farben bestimmt sind.\n\nDie Mitgliedstaaten können jedoch gemäß dem IAO-Übereinkommen Nr. 13 in ihrem Hoheitsgebiet die Verwendung des Stoffs oder Gemischs zur Restaurierung und Unterhaltung von Kunstwerken sowie von historischen Gebäuden und ihren Inneneinrichtungen ebenso genehmigen wie das Inverkehrbringen für eine solche Verwendung. Ein Mitgliedstaat, der diese Ausnahmeregelung in Anspruch nimmt, unterrichtet die Kommission darüber.","物质或含该物质的制剂不得投放市场，或者作为涂料使用。但是，成员国可以许可，按照国际劳工组织第13号公约，在其领土内使用物质或含该物质的制剂用于恢复和维护艺术品和历史建筑和室内设计，以及许可其销售作此用途。一个成员国如要行使这项豁免，应通知欧盟委员会"]
[null,{"$f":"IF($B$1=\"English\",C1691,IF($B$1=\"Deutsch\",D1691,IF($B$1=\"中文\",E1691,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use: \n(a) to prevent the fouling by micro-organisms, plants or animals of: \n—    the hulls of boats, \n—    cages, floats, nets and any other appliances or equipment used for fish or shellfish farming, \n—    any totally or partly submerged appliances or equipment; \n(b) in the preservation of wood; \n(c) in the impregnation of heavy-duty industrial textiles and yarn intended for their manufacture; \n(d) in the treatment of industrial waters, irrespective of their use."},"Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use: \n(a) to prevent the fouling by micro-organisms, plants or animals of: \n—    the hulls of boats, \n—    cages, floats, nets and any other appliances or equipment used for fish or shellfish farming, \n—    any totally or partly submerged appliances or equipment; \n(b) in the preservation of wood; \n(c) in the impregnation of heavy-duty industrial textiles and yarn intended for their manufacture; \n(d) in the treatment of industrial waters, irrespective of their use.","Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die für folgende Verwendungen bestimmt sind:\na) zur Verhinderung des Bewuchses durch Mikroorganismen, Pflanzen oder Tiere an:\n- Bootskörpern;\n- Kästen, Schwimmern, Netzen sowie anderen Geräten oder Einrichtungen für die Fisch- und Muschelzucht;\n- völlig oder teilweise untergetauchten Geräten oder Einrichtungen jeder Art;\nb) zum Schutz von Holz;\nc) zur Imprägnierung von schweren industriellen Textilien und von zu deren Herstellung vorgesehenen Garnen;\nd) zur Aufbereitung von Wasser im industriellen, gewerblichen und kommunalen Bereich, unabhängig von seiner Verwendung.","不得作为物质或者制剂的成分投放市场或者用作以下用途：\na) 防止微生物，植物或动物对于以下物品的污染；\n-船的船体；\n-笼子，浮标，网及其他用于鱼或贝类养殖的任何装置或设备；\n-完全或部分潜在水里的装置或设备;\nb)木材防腐；\nc) 用于重型工业纺织品和用于制造该纺织品的纱线浸泡；\nd) 用于处理各种工业废水。"]
[null,{"$f":"IF($B$1=\"English\",C1692,IF($B$1=\"Deutsch\",D1692,IF($B$1=\"中文\",E1692,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market:\n(a) in fever thermometers;\n(b) in other measuring devices intended for sale to the general public (such as manometers, barometers, sphygmomanometers, thermometers other than fever thermometers). \n2. The restriction in paragraph 1 shall not apply to measuring devices that were in use in the Community before 3 April 2009. However Member States may restrict or prohibit the placing on the market of such measuring devices. \n3. The restriction in paragraph 1(b) shall not apply to:\n (a) measuring devices more than 50 years old on 3 October 2007; \n(b) barometers (except barometers within point (a)) until 3 October 2009.\n(4.    Regulation (EU) No 847/2012: paragraph 4 is  deleted). \n5. The following mercury-containing measuring devices intended for industrial and professional uses shall not be placed on the market after 10 April 2014: \n(a) barometers;\n(b) hygrometers;\n(c) manometers;\n(d) sphygmomanometers; \n(e) strain gauges to be used with plethysmographs;\n(f) tensiometers;\n(g) thermometers and other non-electrical thermometric applications.\nThe restriction shall also apply to measuring devices under points (a) to (g) which are placed on the market empty if intended to be filled with mercury. \n6. The restriction in paragraph 5 shall not apply to: \n(a) sphygmomanometers to be used: \n(i) in epidemiological studies which are ongoing on 10 October 2012;\n(ii) as reference standards in clinical validation studies of mercury-free sphygmomanometers; \n(b) thermometers exclusively intended to perform tests according to standards that require the use of mercury thermometers until 10 October 2017; \n(c) mercury triple point cells which are used for the calibration of platinum resistance thermometers.\n7. The following mercury-using measuring devices intended for professional and industrial uses shall not be placed on the market after 10 April 2014:\n(a) mercury pycnometers; \n(b) mercury metering devices for determination of the softening point. \n8. The restrictions in paragraphs 5 and 7 shall not apply to: \n(a) measuring devices more than 50 years old on 3 October 2007; \n(b) measuring devices which are to be displayed in public exhibitions for cultural and historical purposes.\n"},"1. Shall not be placed on the market:\n(a) in fever thermometers;\n(b) in other measuring devices intended for sale to the general public (such as manometers, barometers, sphygmomanometers, thermometers other than fever thermometers). \n2. The restriction in paragraph 1 shall not apply to measuring devices that were in use in the Community before 3 April 2009. However Member States may restrict or prohibit the placing on the market of such measuring devices. \n3. The restriction in paragraph 1(b) shall not apply to:\n (a) measuring devices more than 50 years old on 3 October 2007; \n(b) barometers (except barometers within point (a)) until 3 October 2009.\n(4.    Regulation (EU) No 847/2012: paragraph 4 is  deleted). \n5. The following mercury-containing measuring devices intended for industrial and professional uses shall not be placed on the market after 10 April 2014: \n(a) barometers;\n(b) hygrometers;\n(c) manometers;\n(d) sphygmomanometers; \n(e) strain gauges to be used with plethysmographs;\n(f) tensiometers;\n(g) thermometers and other non-electrical thermometric applications.\nThe restriction shall also apply to measuring devices under points (a) to (g) which are placed on the market empty if intended to be filled with mercury. \n6. The restriction in paragraph 5 shall not apply to: \n(a) sphygmomanometers to be used: \n(i) in epidemiological studies which are ongoing on 10 October 2012;\n(ii) as reference standards in clinical validation studies of mercury-free sphygmomanometers; \n(b) thermometers exclusively intended to perform tests according to standards that require the use of mercury thermometers until 10 October 2017; \n(c) mercury triple point cells which are used for the calibration of platinum resistance thermometers.\n7. The following mercury-using measuring devices intended for professional and industrial uses shall not be placed on the market after 10 April 2014:\n(a) mercury pycnometers; \n(b) mercury metering devices for determination of the softening point. \n8. The restrictions in paragraphs 5 and 7 shall not apply to: \n(a) measuring devices more than 50 years old on 3 October 2007; \n(b) measuring devices which are to be displayed in public exhibitions for cultural and historical purposes.\n","1. Darf nicht in Verkehr gebracht werden:\na) in Fieberthermometern;\nb) in anderen zum Verkauf an die breite Öffentlichkeit bestimmten Messinstrumenten (z. B. Manometer, Barometer, Sphygmomanometer, andere Thermometer als Fieberthermometer).\n2. Die in Absatz 1 genannte Beschränkung gilt nicht für Messinstrumente, die vor dem 3. April 2009 in der Gemeinschaft in Gebrauch waren. Die Mitgliedstaaten können jedoch das Inverkehrbringen solcher Messinstrumente einschränken oder verbieten.\n3. Die in Absatz 1 Buchstabe b genannte Beschränkung gilt nicht für:\na) Messinstrumente, die am 3. Oktober 2007 älter als 50 Jahre sind,\nb) Barometer (ausgenommen Barometer im Sinne von Buchstabe a) bis zum 3. Oktober 2009.\n4. Gestrichen\n5. Die folgenden quecksilberhaltigen Messinstrumente zur Verwendung für gewerbliche und industrielle Zwecke dürfen nach dem 10. April 2014 nicht mehr in Verkehr gebracht werden:\na) Barometer;\nb) Hygrometer;\nc) Manometer;\nd) Sphygmomanometer;\ne) Dehnungsmessstreifen zur Verwendung in Plethysmographen;\nf) Tensiometer;\ng) Thermometer und andere nichtelektrische thermometrische Anwendungen. Die Beschränkung gilt auch für Messinstrumente nach den Buchstaben a bis g, die leer in Verkehr gebracht werden, wenn sie für die Befüllung mit Quecksilber bestimmt sind.\n6. Die Beschränkung in Absatz 5 gilt nicht für:\na) Sphygmomanometer zur Verwendung:\ni) bei epidemiologischen Studien, die am 10. Oktober 2012 noch laufen;\nii) als Bezugsnormal in klinischen Studien zur Validierung quecksilberfreier Sphygmomanometer;\nb) Thermometer, die ausschließlich dazu bestimmt sind, Prüfungen anhand von Normen durchzuführen, die die Verwendung von Quecksilberthermometern vorschreiben, bis zum 10. Oktober 2017;\nc) quecksilberhaltige Tripelpunktzellen, die zur Kalibrierung von Platin-Widerstandsthermometern verwendet werden.\n7. Die folgenden quecksilberhaltigen Messinstrumente zur Verwendung für gewerbliche und industrielle Zwecke dürfen nach dem 10. April 2014 nicht mehr in Verkehr gebracht werden:\na) quecksilberhaltige Pyknometer;\nb) quecksilberhaltige Messinstrumente zur Bestimmung des Erweichungspunktes.\n8. Die Beschränkungen der Absätze 5 und 7 gelten nicht für:\na) Messinstrumente, die am 3. Oktober 2007 älter als 50 Jahre waren;\nb) in öffentlichen Ausstellungen zu kulturellen und historischen Zwecken auszustellende Messinstrumente.","1. 1.以下情况下不得投放市场：\n-在体温计; 在销售给普通公众的某些等测量仪器（如压力计，气压计，血压计，温度计比体温计等）\n2.第1段的限制不适用于2009年4月3日前已经投入使用的测量工具。但是，成员国可以限制或禁止此类测量仪器投放市场。\n3.在1（b）中所述的限制不用于：\n（a）在2007年10月3日已超过50年的测量仪器，\n（b）气压表（（a）中所述气压表除外）可豁免至2009年10月3日。\n4.（(欧盟)法规847/2012号条例：第4段被删除）。\n5. 以下用于工业和专业用途的含汞测量装置不得在2014年4月10日后投放市场：\n(a) 气压计\n(b) 湿度计\n(c) 压力计\n(d) 血压计\n(e) 与胸腔镜一起使用的应变仪\n(f) 张力计\n(g) 温度计和其他非电力测温应用\n该限制也应适用于(a)至(g)相关的测量设备，即使需要填充汞，也应在市场上保持空置。\n6. 第5项的限制不应适用于 \n(a) 拟使用的血压计\n(i) 截至2012年10月10日，处于进行中的流行病学研究\n(ii) 作为无汞血压计临床验证研究中的参考标准\n(b) 截至2017年10月10日，专门用于按照要求使用汞温度计的标准进行测试的温度计\n(c) 用于校准铂金电阻温度计的汞三点电池\n7. 以下用于专业和工业用途的用汞测量装置在2014年4月10日后不得投放市场。\n(a) 汞比色计\n(b) 用于测定软化点的汞计量装置\n8. 第5和第7款中的限制不应适用于 \n(a) 在2007年10月3日已使用50年以上的测量装置\n(b) 为文化和历史目的而在公开展览中展示的测量设备"]
[null,{"$f":"IF($B$1=\"English\",C1693,IF($B$1=\"Deutsch\",D1693,IF($B$1=\"中文\",E1693,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use to prevent the fouling by micro-organisms, plants or animals of: \n— the hulls of boats, \n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming, \n— any totally or partly submerged appliances or equipment. \n\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters, irrespective of their use. \n\n3. Shall not be used in the preservation of wood. Furthermore, wood so treated shall not be placed on the market. \n\n4. By way of derogation from paragraph 3: \n(a) Relating to the substances and mixtures for the preservation of wood: these may only be used in industrial installations using vacuum or pressure to impregnate wood if they are solutions of inorganic compounds of the copper, chromium, arsenic (CCA) type C and if they are authorised in accordance with Article 5(1) of Directive 98/8/EC. Wood so treated shall not be placed on the market before fixation of the preservative is completed. \n(b) Wood treated with CCA solution in accordance with point (a) may be placed on the market for professional and industrial use provided that the structural integrity of the wood is required for human or livestock safety and skin contact by the general public during its service life is unlikely: \n— as structural timber in public and agricultural buildings, office buildings, and industrial premises, \n— in bridges and bridgework, \n— as constructional timber in freshwater areas and brackish waters, for example jetties and bridges, \n— as noise barriers, — in avalanche control, — in highway safety fencing and barriers, \n— as debarked round conifer livestock fence posts, \n— in earth retaining structures, — as electric power transmission and telecommunications poles, \n— as underground railway sleepers. \n(c) Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that all treated wood placed on the market is individually labelled ‘For professional and industrial installation and use only, contains arsenic’. In addition, all wood placed on the market in packs shall also bear a label stating ‘Wear gloves when handling this wood. Wear a dust mask and eye protection when cutting or otherwise crafting this wood. Waste from this wood shall be treated as hazardous by an authorised undertaking’. \n(d) Treated wood referred to under point (a) shall not be used: — in residential or domestic constructions, whatever the purpose, — in any application where there is a risk of repeated skin contact, — in marine waters, — for agricultural purposes other than for livestock fence posts and structural uses in accordance with point (b), — in any application where the treated wood may come into contact with intermediate or finished products intended for human and/or animal consumption. \n\n5. Wood treated with arsenic compounds that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4 may remain in place and continue to be used until it reaches the end of its service life. \n\n6. Wood treated with CCA type C that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4: \n— may be used or reused subject to the conditions pertaining to its use listed under points 4(b), (c) and (d), \n— may be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).\n\n7. Member States may allow wood treated with other types of CCA solutions that was in use in the Community before 30 September 2007: \n— to be used or reused subject to the conditions pertaining to its use listed under points 4 (b), (c) and (d), \n— to be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d)."},"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use to prevent the fouling by micro-organisms, plants or animals of: \n— the hulls of boats, \n— cages, floats, nets and any other appliances or equipment used for fish or shellfish farming, \n— any totally or partly submerged appliances or equipment. \n\n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters, irrespective of their use. \n\n3. Shall not be used in the preservation of wood. Furthermore, wood so treated shall not be placed on the market. \n\n4. By way of derogation from paragraph 3: \n(a) Relating to the substances and mixtures for the preservation of wood: these may only be used in industrial installations using vacuum or pressure to impregnate wood if they are solutions of inorganic compounds of the copper, chromium, arsenic (CCA) type C and if they are authorised in accordance with Article 5(1) of Directive 98/8/EC. Wood so treated shall not be placed on the market before fixation of the preservative is completed. \n(b) Wood treated with CCA solution in accordance with point (a) may be placed on the market for professional and industrial use provided that the structural integrity of the wood is required for human or livestock safety and skin contact by the general public during its service life is unlikely: \n— as structural timber in public and agricultural buildings, office buildings, and industrial premises, \n— in bridges and bridgework, \n— as constructional timber in freshwater areas and brackish waters, for example jetties and bridges, \n— as noise barriers, — in avalanche control, — in highway safety fencing and barriers, \n— as debarked round conifer livestock fence posts, \n— in earth retaining structures, — as electric power transmission and telecommunications poles, \n— as underground railway sleepers. \n(c) Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that all treated wood placed on the market is individually labelled ‘For professional and industrial installation and use only, contains arsenic’. In addition, all wood placed on the market in packs shall also bear a label stating ‘Wear gloves when handling this wood. Wear a dust mask and eye protection when cutting or otherwise crafting this wood. Waste from this wood shall be treated as hazardous by an authorised undertaking’. \n(d) Treated wood referred to under point (a) shall not be used: — in residential or domestic constructions, whatever the purpose, — in any application where there is a risk of repeated skin contact, — in marine waters, — for agricultural purposes other than for livestock fence posts and structural uses in accordance with point (b), — in any application where the treated wood may come into contact with intermediate or finished products intended for human and/or animal consumption. \n\n5. Wood treated with arsenic compounds that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4 may remain in place and continue to be used until it reaches the end of its service life. \n\n6. Wood treated with CCA type C that was in use in the Community before 30 September 2007, or that was placed on the market in accordance with paragraph 4: \n— may be used or reused subject to the conditions pertaining to its use listed under points 4(b), (c) and (d), \n— may be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).\n\n7. Member States may allow wood treated with other types of CCA solutions that was in use in the Community before 30 September 2007: \n— to be used or reused subject to the conditions pertaining to its use listed under points 4 (b), (c) and (d), \n— to be placed on the market subject to the conditions pertaining to its use listed under points 4(b), (c) and (d).","1. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die bestimmt sind zur Verhinderung des Bewuchses durch Mikroorganismen, Pflanzen oder Tiere an:\n• Bootskörpern;\n• Kästen, Schwimmern, Netzen sowie anderen Geräten oder Einrichtungen für die Fisch- und Muschelzucht;\n• völlig oder teilweise untergetauchten Geräten oder Einrichtungen jeder Art.\n2. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Aufbereitung von Wasser im industriellen, gewerblichen und kommunalen Bereich bestimmt sind, unabhängig von seiner Verwendung.\n3. Dürfen nicht als Holzschutzmittel verwendet werden. Ferner darf damit behandeltes Holz nicht in Verkehr gebracht werden.\n4. Abweichend von Absatz 3 bestehen jedoch folgende Ausnahmen:\na) Für Stoffe und Gemische für den Holzschutz: Diese dürfen lediglich in Industrieanlagen im Vakuum oder unter Druck zur Imprägnierung von Holz in Form von Lösungen anorganischer Verbindungen von Kupfer-Chrom-Arsen (CCA), Typ C, zum Einsatz kommen, sofern sie nach Artikel 5 Absatz 1 der Richtlinie 98/8/EG zugelassen sind. Holz, das so behandelt ist, darf nicht in Verkehr gebracht werden, bevor das Schutzmittel vollständig fixiert ist.\nb) Mit CCA-Lösungen behandeltes Holz gemäß Buchstabe a darf für die gewerbliche und industrielle Verwendung in Verkehr gebracht werden, sofern die Unversehrtheit der Holzstruktur zur Sicherheit von Mensch oder Vieh erforderlich ist und ein Hautkontakt der allgemeinen Bevölkerung während der Einsatzdauer unwahrscheinlich ist:\n• als Bauholz in öffentlichen und landwirtschaftlichen Gebäuden, Bürogebäuden und Industriebetrieben,\n• in Brücken und bei Brückenbauarbeiten,\n• als Bauholz in Binnengewässern und Brackwasser, z. B. für Molen und Brücken,\n• als Lärmschutz,\n• als Lawinenschutz,\n• als Leitplanken und Schranken an Straßen,\n• als entrindete Rundnadelhölzer für Weidezäune,\n• in Erdstützwänden,\n• als Strom- und Telekommunikationsmasten,\n• als Bahnschwellen für Untergrundbahnen.\nc) Unbeschadet anderer Gemeinschaftsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen müssen die Lieferanten vor dem Inverkehrbringen gewährleisten, dass sämtliches behandeltes Holz einzeln mit der Aufschrift versehen ist: „Verwendung nur in Industrieanlagen und zu gewerblichen Zwecken, enthält Arsen.“ Darüber hinaus muss sämtliches in Paketen in Verkehr gebrachtes Holz mit der Aufschrift versehen ist: „Bei der Handhabung des Holzes Handschuhe tragen. Wird dieses Holz geschnitten oder anderweitig bearbeitet, Staubmaske und Augenschutz tragen. Abfälle dieses Holzes sind von zugelassenen Unternehmen als gefährliche Abfälle zu behandeln.“\n\nd) Die Verwendung von behandeltem Holz nach Buchstabe a ist jedoch verboten:\n• in Wohnbauten, unabhängig von ihrer Zweckbestimmung,\n• in Anwendungen mit dem Risiko eines wiederholten Hautkontakts,\n• in Meeresgewässern,\n• für landwirtschaftliche Zwecke außer Weidezäunen und Bauholz gemäß Buchstabe b,\n• in Anwendungen, bei denen das behandelte Holz mit Zwischen- oder Enderzeugnissen in Kontakt kommen kann, die für den menschlichen und/oder tierischen Verzehr bestimmt sind.\n5. Mit Arsenverbindungen behandeltes Holz, das vor dem 30. September 2007 in der Gemeinschaft genutzt oder gemäß Absatz 4 in Verkehr gebracht wurde, kann bis zum Ende seiner Nutzungsdauer eingebaut bleiben und weiterverwendet werden.\n6. Mit CCA-Lösungen, Typ C, behandeltes Holz, das vor dem 30. September 2007 in der Gemeinschaft genutzt oder gemäß Absatz 4 in Verkehr gebracht wurde:\n• kann unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen genutzt oder wiederverwendet werden,\n• kann unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen in Verkehr gebracht werden.\n7. Die Mitgliedstaaten können zulassen, dass mit anderen Typen von CCA-Lösungen behandeltes Holz, das vor dem 30. September 2007 in der Gemeinschaft genutzt wurde:\n• unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen genutzt oder wiederverwendet wird,\n• unter den unter Absatz 4 Buchstaben b, c und d genannten Verwendungsbedingungen in Verkehr gebracht wird.\n","1.不可以作为物质或在配制品里被销售或使用，这是为了防止由微生物，植物或动物引起的污染：\n-船的船体；\n-笼子，浮标，用于鱼或贝类养殖网和其它任何电器或设备;\n-完全或部分淹没的此类型的器具或设备。\n2.不可以作为物质或制剂的成分于以下用途:：被销售或使用，这是用于处理水用于工业，商业和市政部门，与他的使用无关。\n3不可仪作为树木保护剂使用。如果已被处理过的木材，不可以在市场上销售。\n4对于第3条存在以下例外：\n(a)对于针对木材防腐的物质和配制品：这些只允许在真空的工业装置中或者在对木材浸泡的压力下被使用（此浸泡是指通过由铜铬砷（CCA），C型组成的无机化合物的溶液完成的），只要这些根据指导方针98/8/EG的第5条第1款是被允许的。通过这种方式处理的木头在防护剂完全固定以前不允许被投放于市场。\n(b)含有CCA溶液进行处理过的木材根据(a)可允许被销售用于企业和工业，前提是木结构用于人或牲畜安全性是必需的，以及与一般人的皮肤接触在时间周期是不大可能的：\n-作为在公共和农业建筑，写字楼和工业厂房的结构木材，\n-桥梁及桥梁工程，\n-作为在淡水区和咸水水域的结构用材，如码头，桥梁，\n-作为隔音屏障，\n-作为雪崩防护， \n-作为高速公路的防护栏和障碍， \n-用去了皮的树杆作为牲畜的围栏， \n- 作为土挡墙， \n-作为电力和通讯桅杆， \n-作为铁路枕木用于地铁。\n(c)在不影响共同规定对于物质和配制品的分类，包装和标签等，供应商应在投放市场之前应该确保，所有处理过的木材都单独配有标字：只使用于工业设施和商业目的，含有砷。此外，所有要销售的木材的包装上必须配有标字：处理这种木材时请戴上手套。这种木材切割或以其他方式处理，请戴上防尘面具和护目镜。这个木材的废料应以相符的公司作为危险废物处理。\n\n使用处理过的木材根据字母a不被使用：\n-在住宅楼宇，与其目的无关，\n-在使用中有反复与皮肤接触危险，\n-在海洋水域，\n-根据b，用于除了牲畜栅栏外的农业目的和结构用途，\n-在应用中，处理过的木材可能会接触中间或最终产品，这些产品用于人类和/或动物的消耗。\n5. 含被砷化合物处理过的木材，其在2007年9月30号之前在公共情况下被使用或者根据段落4在市场上销售，可以保留和继续使用直到其使用寿命结束时。    \n6.被CCA溶液，TypC处理过的木材，其在2007年9月30号之前在公共情况下被使用或者根据段落4在市场上销售：\n-也可根据第4段中字母b，c和d的规定中提到的使用条件，可以使用或重复使用\n-也可根据第4段中字母b，c和d的规定中提到的使用条件，在市场上销售\n7. 成员国可以允许，用其他类型的CCA溶液处理的木材在2007年9月30日前在公共社区可以被使用:\n-也可根据第4段中字母b，c和d的规定中提到的使用条件，可以使用或重复使用\n也可根据第4段中字母b，c和d规定中提到的使用条件，在市场上销售"]
[null,{"$f":"IF($B$1=\"English\",C1694,IF($B$1=\"Deutsch\",D1694,IF($B$1=\"中文\",E1694,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is acting as biocide in free association paint. \n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture acts as biocide to prevent the fouling by micro-organisms, plants or animals of: \n(a) all craft irrespective of their length intended for use in marine, coastal, estuarine and inland waterways and lakes; (b) cages, floats, nets and any other appliances or equipment used for fish or shellfish farming; (c) any totally or partly submerged appliance or equipment. \n3. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters. \n4. Tri-substituted organostannic compounds: \n(a) Tri-substituted organostannic compounds such as tributyltin (TBT) compounds and triphenyltin (TPT) compounds shall not be used after 1 July 2010 in articles where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin. (b) Articles not complying with point (a) shall not be placed on the market after 1 July 2010, except for articles that were already in use in the Community before that date. \n5. Dibutyltin (DBT) compounds: \n(a) Dibutyltin (DBT) compounds shall not be used after 1 January 2012 in mixtures and articles for supply to the general public where the concentration in the mixture or the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin. (b) Articles and mixtures not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date. (c) By way of derogation, points (a) and (b) shall not apply until 1 January 2015 to the following articles and mixtures for supply to the general public: \n— one-component and two-component room temperature vulcanisation sealants (RTV-1 and RTV-2 sealants) and adhesives, \n— paints and coatings containing DBT compounds as catalysts when applied on articles, \n— soft polyvinyl chloride (PVC) profiles whether by themselves or coextruded with hard PVC, \n— fabrics coated with PVC containing DBT compounds as stabilisers when intended for outdoor applications, \n— outdoor rainwater pipes, gutters and fittings, as well as covering material for roofing and façades, \n(d) By way of derogation, points (a) and (b) shall not apply to materials and articles regulated under Regulation (EC) No 1935/2004. \n6. Dioctyltin (DOT) compounds: \n(a) Dioctyltin (DOT) compounds shall not be used after 1 January 2012 in the following articles for supply to, or use by, the general public, where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin: \n— textile articles intended to come into contact with the skin, \n— gloves, \n— footwear or part of footwear intended to come into contact with the skin, \n— wall and floor coverings, \n— childcare articles, \n— female hygiene products, \n— nappies, \n— two-component room temperature vulcanisation moulding kits (RTV-2 moulding kits). \n(b) Articles not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date.\n\n"},"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is acting as biocide in free association paint. \n2. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture acts as biocide to prevent the fouling by micro-organisms, plants or animals of: \n(a) all craft irrespective of their length intended for use in marine, coastal, estuarine and inland waterways and lakes; (b) cages, floats, nets and any other appliances or equipment used for fish or shellfish farming; (c) any totally or partly submerged appliance or equipment. \n3. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for use in the treatment of industrial waters. \n4. Tri-substituted organostannic compounds: \n(a) Tri-substituted organostannic compounds such as tributyltin (TBT) compounds and triphenyltin (TPT) compounds shall not be used after 1 July 2010 in articles where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin. (b) Articles not complying with point (a) shall not be placed on the market after 1 July 2010, except for articles that were already in use in the Community before that date. \n5. Dibutyltin (DBT) compounds: \n(a) Dibutyltin (DBT) compounds shall not be used after 1 January 2012 in mixtures and articles for supply to the general public where the concentration in the mixture or the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin. (b) Articles and mixtures not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date. (c) By way of derogation, points (a) and (b) shall not apply until 1 January 2015 to the following articles and mixtures for supply to the general public: \n— one-component and two-component room temperature vulcanisation sealants (RTV-1 and RTV-2 sealants) and adhesives, \n— paints and coatings containing DBT compounds as catalysts when applied on articles, \n— soft polyvinyl chloride (PVC) profiles whether by themselves or coextruded with hard PVC, \n— fabrics coated with PVC containing DBT compounds as stabilisers when intended for outdoor applications, \n— outdoor rainwater pipes, gutters and fittings, as well as covering material for roofing and façades, \n(d) By way of derogation, points (a) and (b) shall not apply to materials and articles regulated under Regulation (EC) No 1935/2004. \n6. Dioctyltin (DOT) compounds: \n(a) Dioctyltin (DOT) compounds shall not be used after 1 January 2012 in the following articles for supply to, or use by, the general public, where the concentration in the article, or part thereof, is greater than the equivalent of 0,1 % by weight of tin: \n— textile articles intended to come into contact with the skin, \n— gloves, \n— footwear or part of footwear intended to come into contact with the skin, \n— wall and floor coverings, \n— childcare articles, \n— female hygiene products, \n— nappies, \n— two-component room temperature vulcanisation moulding kits (RTV-2 moulding kits). \n(b) Articles not complying with point (a) shall not be placed on the market after 1 January 2012, except for articles that were already in use in the Community before that date.\n\n","1. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, wenn diese als Biozide in Farben wirken, deren Bestandteile chemisch nicht gebunden sind.\n2. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die als Biozide dazu dienen, an folgenden Gegenständen den Bewuchs durch Mikroorganismen, Pflanzen oder Tiere zu verhindern:\na) an allen Fahrzeugen unabhängig von ihrer Länge, die auf Seewasserstraßen, Wasserstraßen im Küsten- und Ästuarbereich, Binnenwasserstraßen sowie Seen eingesetzt werden;\nb) an Kästen, Schwimmern, Netzen sowie anderen Geräten oder Einrichtungen für die Fisch- und Muschelzucht;\nc) an völlig oder teilweise untergetauchten Geräten oder Einrichtungen jeder Art.\n3. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Aufbereitung von Wasser im industriellen, gewerblichen und kommunalen Bereich bestimmt sind.\n4. Trisubstituierte zinnorganische Verbindungen:\na) Trisubstituierte zinnorganische Verbindungen wie etwa Tributylzinnverbindungen (TBT) und Triphenylzinnverbindungen (TPT) dürfen nach dem 1. Juli 2010 nicht mehr in Erzeugnissen verwendet werden, wenn die Konzentration von Zinn in dem Erzeugnis oder in Teilen davon 0,1 Gewichtsprozent übersteigt.\nb) Erzeugnisse, die nicht mit Buchstabe a in Einklang stehen, dürfen nach dem 1. Juli 2010 nicht mehr in Verkehr gebracht werden; ausgenommen davon sind Erzeugnisse, die bereits vor diesem Zeitpunkt in der Gemeinschaft in Verwendung waren.\n5. Dibutylzinnverbindungen (DBT):\na) Dibutylzinnverbindungen (DBT) dürfen nach dem 1. Januar 2012 nicht mehr in Gemischen und Erzeugnissen verwendet werden, die dazu bestimmt sind, an die breite Öffentlichkeit abgegeben zu werden, wenn die Konzentration von Zinn in dem Gemisch oder Erzeugnis bzw. in Teilen davon 0,1 Gewichtsprozent übersteigt.\nb) Erzeugnisse und Gemische, die nicht mit Buchstabe a in Einklang stehen, dürfen nach dem 1. Januar 2012 nicht mehr in Verkehr gebracht werden; ausgenommen davon sind Erzeugnisse, die bereits vor diesem Zeitpunkt in der Gemeinschaft in Verwendung waren.\nc) Abweichend davon gelten die Buchstaben a und b bis zum 1. Januar 2015 nicht für die nachstehenden Erzeugnisse und Gemische, die für die Abgabe an die breite Öffentlichkeit bestimmt sind:\no Ein-Komponenten- und Zwei-Komponenten- Raumtemperaturvulkanisierungs-Dichtungsmittel (RTV-1- und RTV-2-Dichtungsmittel) und Klebstoffe;\no Farben und Beschichtungen, die DBT-Verbindungen als Katalysatoren enthalten, wenn diese auf Erzeugnissen aufgetragen sind;\no weiche Polyvinylchlorid-(PVC)-Profile, mit Hart-PVC koextrudiert oder nicht;\no Gewebe, die mit PVC beschichtet sind, das DBT-Verbindungen als Stabilisatoren enthält, wenn sie für die Verwendung im Freien vorgesehen sind;\no im Freien befindliche Regenwasserleitungen, Regenrinnen und Anschlussteile sowie Dach- und Fassadenverkleidungsmaterial.\nd) Abweichend davon gelten die Buchstaben a und b nicht für Materialien und Erzeugnisse, die unter die Verordnung (EG) Nr. 1935/2004 fallen.\n6. Dioctylzinnverbindungen (DOT):\na) Dioctylzinnverbindungen (DOT) dürfen nach dem 1. Januar 2012 nicht mehr in den nachstehend aufgeführten Erzeugnissen verwendet werden, die dazu bestimmt sind, an die breite Öffentlichkeit abgegeben oder von dieser verwendet zu werden, wenn die Konzentration von Zinn in dem Erzeugnis oder in Teilen davon 0,1 Gewichtsprozent übersteigt:\no Textilartikel, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen;\no Handschuhe;\no Schuhe oder Teile davon, die dazu bestimmt sind, mit der Haut in Kontakt zu kommen;\no Wand- und Bodenverkleidungen;\no Babyartikel;\no Damenhygieneartikel;\no Windeln;\no Zwei-Komponenten-Raumtemperaturvulkanisierungs-Abform-Sets (RTV-2-Abform-Sets).\nb) Erzeugnisse, die nicht mit Buchstabe a in Einklang stehen, dürfen nach dem 1. Januar 2012 nicht mehr in Verkehr gebracht werden; ausgenommen davon sind Erzeugnisse, die bereits vor diesem Zeitpunkt in der Gemeinschaft in Verwendung waren.","1．作为自由组合涂料的生物杀虫剂的物质或制剂的成分不得投放市场\n2.不得作为物质或者制剂的成分投放市场或者用于防止微生物，植物或动物对于以下物品的污染：\n（a）航行于海洋、海岸、河口和内河、湖泊的船舶(无论船舶长度)；\n（b）笼子，浮标，网及其他用于鱼或贝类养殖的任何装置或设备；\n（c）任何完全或部分潜在水里的装置或设备;\n3. 用于处理各种工业废水。\n4. 三取代物有机锡化合物：\n（a）三取代物有机锡化合物，如三丁基锡（TBT）化合物和三苯基锡（TPT）化合物，在2010年7月1日之后不得用于产品，当其中锡的含量在成品或一部分其浓度超过0.1的重量百分比。\n（b）不符合(a)要求的产品，不可以在2010年7月1日在市场上销售；除非在这个日期之前已经被公众使用的产品。\n5. 二丁基锡（DBT）化合物：\n（a）二丁基锡（DBT）化合物在2012年1月1日之后不得作为配制品和成品在市场上销售给大众，当其成品或部件中锡的含量其浓度超过0.1的重量百分比。\n（b）不符合(a)要求的产品，不可以在2012年1月1日在市场上销售；除非在这个日期之前已经被公众使用的产品。\n（c）作为免除项目，条款（a）和（b）在2015年1月1号前对以下要提供给公众产品及配制品可以豁免：\n-单组分和双组分室温硫化密封剂（RTV-1和RTV-2密封剂）和粘合剂;\n-已经涂敷到物品上的含有二丁基锡作为催化剂在颜料和涂层；\n-单一的软质的聚氯乙烯（PVC）型材，或硬质软质聚氯乙烯（PVC）复合的型材;\n-用于室外的织物，如果上面涂覆有以DBT二丁基锡作为稳定剂的聚氯乙烯PVC涂层;\n-位于户外雨水管道，排水沟和配件，以及屋顶和覆面材料。\n（d）作为免除项目，条款（a）和（b）不适用于欧盟法规(EC) No 1935/2004规范的产品及配制品。\n6. 二辛基锡（DOT）化合物：\n（a）二辛基锡（DOT）化合物在2012年1月1日之后不得用于以下销售给大众的物品中，当其成品或部件中锡的含量其浓度超过0.1的重量百分比：\n-会与皮肤接触的纺织产品\n-手套\n-会与皮肤接触的鞋子或其一部分；\n-墙壁和地板覆盖物; \n-儿童用品\n-女士卫生产品\n-纸尿片\n- 双组分室温硫化模型套（RTV-2的模型套）。\n（b）不符合(a)要求的产品，不可以在2012年1月1日在市场上销售；除非在这个日期之前已经被公众使用的产品。"]
[null,{"$f":"IF($B$1=\"English\",C1695,IF($B$1=\"Deutsch\",D1695,IF($B$1=\"中文\",E1695,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance, or in mixtures in a concentration equal to, or greater than 0,1 % by weight. \nHowever, the first paragraph shall not apply to this substance (DBB) or mixtures containing it if these are intended solely for conversion into articles, among which this substance will no longer feature in a concentration equal to or greater than 0,1 %.\n"},"Shall not be placed on the market, or used, as a substance, or in mixtures in a concentration equal to, or greater than 0,1 % by weight. \nHowever, the first paragraph shall not apply to this substance (DBB) or mixtures containing it if these are intended solely for conversion into articles, among which this substance will no longer feature in a concentration equal to or greater than 0,1 %.\n","Dürfen weder als Stoffe noch in Gemischen in Konzentrationen von ≥ 0,1 Gew.-% in Verkehr gebracht oder verwendet werden.\n\nAbsatz 1 gilt jedoch nicht, wenn dieser Stoff (DBB) oder die ihn enthaltenden Gemische ausschließlich zu Erzeugnissen verarbeitet werden, in denen er nicht mehr in einer Konzentration von ≥ 0,1 Gew.-% vorhanden ist.","当物质或者制剂中该物质浓度大于等于0.1%时，不得投放市场或者使用。\n但是当其仅用于转化到成品时，此规定对这一物质(DBB)或其制剂无效，在此过程中，物质无法显现其特性浓度大于或等于0.1%"]
[null,{"$f":"IF($B$1=\"English\",C1696,IF($B$1=\"Deutsch\",D1696,IF($B$1=\"中文\",E1696,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020"},"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020","Gestrichen nach VERORDNUNG (EU) 2020/2096 vom 15. Dezember 2020","根据2020年12月15日发布的法规2020/2096/EU删除"]
[null,{"$f":"IF($B$1=\"English\",C1697,IF($B$1=\"Deutsch\",D1697,IF($B$1=\"中文\",E1697,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the purpose of this entry, the codes and chapters indicated in square brackets are the codes and chapters of the tariff and statistical nomenclature of Common Customs Tariff as established by Council Regulation (EEC) No 2658/87 (*).\n1. Shall not be used in mixtures and articles produced from the following synthetic organic polymers (hereafter referred to as plastic material):\n— polymers or copolymers of vinyl chloride (PVC) [3904 10] [3904 21] — polyurethane (PUR) [3909 50] — low-density polyethylene (LDPE), with the exception of low-density polyethylene used for the production of coloured masterbatch [3901 10] — cellulose acetate (CA) [3912 11] — cellulose acetate butyrate (CAB) [3912 11] — epoxy resins [3907 30] — melamine-formaldehyde (MF) resins [3909 20] — urea-formaldehyde (UF) resins [3909 10] — unsaturated polyesters (UP) [3907 91] — polyethylene terephthalate (PET) [3907 60] — polybutylene terephthalate (PBT) — transparent/general-purpose polystyrene [3903 11] — acrylonitrile methylmethacrylate (AMMA) — cross-linked polyethylene (VPE) — high-impact polystyrene — polypropylene (PP) [3902 10]\nMixtures and articles produced from plastic material as listed above shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight of the plastic material.\nBy way of derogation, the second subparagraph shall not apply to articles placed on the\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nmarket before 10 December 2011.\nThe first and second subparagraphs apply without prejudice to Council Directive 94/62/ EC (**) and acts adopted on its basis.\nBy 19 November 2012, in accordance with Article 69, the Commission shall ask the European Chemicals Agency to prepare a dossier conforming to the requirements of Annex XV in order to assess whether the use of cadmium and its compounds in plastic material, other than that listed in subparagraph 1, should be restricted.\n2. Shall not be used or placed on the market in paints with codes [3208] [3209] in a concentration (expressed as Cd metal) equal to or greater than 0,01 % by weight.\nFor paints with codes [3208] [3209] with a zinc content exceeding 10 % by weight of the paint, the concentration of cadmium (expressed as Cd metal) shall not be equal to or greater than 0,1 % by weight.\nPainted articles shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,1 % by weight of the paint on the painted article.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to articles coloured with mixtures containing cadmium for safety reasons.\n4. By way of derogation, paragraph 1, second sub paragraph shall not apply to:\n— mixtures produced from PVC waste, hereinafter referred to as ‘recovered PVC’,\n— mixtures and articles containing recovered PVC if their concentration of cadmium (expressed as Cd metal) does not exceed 0,1 % by weight of the plastic material in the following rigid PVC applications:\n(a) profiles and rigid sheets for building applications; (b) doors, windows, shutters, walls, blinds, fences, and roof gutters; (c) decks and terraces; (d) cable ducts; (e) pipes for non-drinking water if the recovered PVC is used in the middle layer of a multilayer pipe and is entirely covered with a layer of newly produced PVC in compliance with paragraph 1 above.\nSuppliers shall ensure, before the placing on the market of mixtures and articles containing recovered PVC for the first time, that these are visibly, legibly and indelibly marked as follows: ‘ Contains recovered PVC ’ or with the following pictogram:\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nIn accordance with Article 69 of this Regulation, the derogation granted in paragraph 4 will be reviewed, in particular with a view to reducing the limit value for cadmium and to reassess the derogation for the applications listed in points (a) to (e), by 31 December 2017.\n5. For the purpose of this entry, ‘cadmium plating’ means any deposit or coating of metallic cadmium on a metallic surface.\nShall not be used for cadmium plating metallic articles or components of the articles used in the following sectors/applications:\n(a) equipment and machinery for:\n— food production [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] — agriculture [8419 31] [8424 81] [8432] [8433] [8434] [8436] — cooling and freezing [8418] — printing and book-binding [8440] [8442] [8443]\n(b) equipment and machinery for the production of:\n— household goods [7321] [8421 12] [8450] [8509] [8516] — furniture [8465] [8466] [9401] [9402] [9403] [9404] — sanitary ware [7324] — central heating and air conditioning plant [7322] [8403] [8404] [8415]\nIn any case, whatever their use or intended final purpose, the placing on the market of cadmium-plated articles or components of such articles used in the sectors/applications listed in points (a) and (b) above and of articles manufactured in the sectors listed in point (b) above is prohibited.\n6. The provisions referred to in paragraph 5 shall also be applicable to cadmium-plated articles or components of such articles when used in the sectors/applications listed in points (a) and (b) below and to articles manufactured in the sectors listed in (b) below:\n(a) equipment and machinery for the production of:\n— paper and board [8419 32] [8439] [8441] textiles and clothing [8444] [8445] [8447] [8448] [8449] [8451] [8452]\n(b) equipment and machinery for the production of:\n— industrial handling equipment and machinery [8425] [8426] [8427] [8428] [8429] [8430] [8431] — road and agricultural vehicles [chapter 87] — rolling stock [chapter 86] — vessels [chapter 89]\n7. However, the restrictions in paragraphs 5 and 6 shall not apply to:\n— articles and components of the articles used in the aeronautical, aerospace, mining, offshore and nuclear sectors whose applications require high safety standards and in safety devices in road and agricultural vehicles, rolling stock\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nand vessels, — electrical contacts in any sector of use, where that is necessary to ensure the reliability required of the apparatus on which they are installed.\n8. Shall not be used in brazing fillers in concentration equal to or greater than 0,01 % by weight.\nBrazing fillers shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight.\nFor the purpose of this paragraph brazing shall mean a joining technique using alloys and undertaken at temperatures above 450 °C.\n9. By way of derogation, paragraph 8 shall not apply to brazing fillers used in defence and aerospace applications and to brazing fillers used for safety reasons.\n10. Shall not be used or placed on the market if the concentration is equal to or greater than 0,01 % by weight of the metal in:\n(i) metal beads and other metal components for jewellery making; (ii) metal parts of jewellery and imitation jewellery articles and hair accessories, including:\n— bracelets, necklaces and rings, — piercing jewellery, — wrist-watches and wrist-wear, — brooches and cufflinks.\n11. By way of derogation, paragraph 10 shall not apply to articles placed on the market before 10 December 2011 and jewellery more than 50 years old on 10 December 2011.\n________ __\n(*) OJ L 256, 7.9.1987, p. 42.\n(**) OJ L 365, 31.12.1994, p. 10"},"For the purpose of this entry, the codes and chapters indicated in square brackets are the codes and chapters of the tariff and statistical nomenclature of Common Customs Tariff as established by Council Regulation (EEC) No 2658/87 (*).\n1. Shall not be used in mixtures and articles produced from the following synthetic organic polymers (hereafter referred to as plastic material):\n— polymers or copolymers of vinyl chloride (PVC) [3904 10] [3904 21] — polyurethane (PUR) [3909 50] — low-density polyethylene (LDPE), with the exception of low-density polyethylene used for the production of coloured masterbatch [3901 10] — cellulose acetate (CA) [3912 11] — cellulose acetate butyrate (CAB) [3912 11] — epoxy resins [3907 30] — melamine-formaldehyde (MF) resins [3909 20] — urea-formaldehyde (UF) resins [3909 10] — unsaturated polyesters (UP) [3907 91] — polyethylene terephthalate (PET) [3907 60] — polybutylene terephthalate (PBT) — transparent/general-purpose polystyrene [3903 11] — acrylonitrile methylmethacrylate (AMMA) — cross-linked polyethylene (VPE) — high-impact polystyrene — polypropylene (PP) [3902 10]\nMixtures and articles produced from plastic material as listed above shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight of the plastic material.\nBy way of derogation, the second subparagraph shall not apply to articles placed on the\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nmarket before 10 December 2011.\nThe first and second subparagraphs apply without prejudice to Council Directive 94/62/ EC (**) and acts adopted on its basis.\nBy 19 November 2012, in accordance with Article 69, the Commission shall ask the European Chemicals Agency to prepare a dossier conforming to the requirements of Annex XV in order to assess whether the use of cadmium and its compounds in plastic material, other than that listed in subparagraph 1, should be restricted.\n2. Shall not be used or placed on the market in paints with codes [3208] [3209] in a concentration (expressed as Cd metal) equal to or greater than 0,01 % by weight.\nFor paints with codes [3208] [3209] with a zinc content exceeding 10 % by weight of the paint, the concentration of cadmium (expressed as Cd metal) shall not be equal to or greater than 0,1 % by weight.\nPainted articles shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,1 % by weight of the paint on the painted article.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to articles coloured with mixtures containing cadmium for safety reasons.\n4. By way of derogation, paragraph 1, second sub paragraph shall not apply to:\n— mixtures produced from PVC waste, hereinafter referred to as ‘recovered PVC’,\n— mixtures and articles containing recovered PVC if their concentration of cadmium (expressed as Cd metal) does not exceed 0,1 % by weight of the plastic material in the following rigid PVC applications:\n(a) profiles and rigid sheets for building applications; (b) doors, windows, shutters, walls, blinds, fences, and roof gutters; (c) decks and terraces; (d) cable ducts; (e) pipes for non-drinking water if the recovered PVC is used in the middle layer of a multilayer pipe and is entirely covered with a layer of newly produced PVC in compliance with paragraph 1 above.\nSuppliers shall ensure, before the placing on the market of mixtures and articles containing recovered PVC for the first time, that these are visibly, legibly and indelibly marked as follows: ‘ Contains recovered PVC ’ or with the following pictogram:\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nIn accordance with Article 69 of this Regulation, the derogation granted in paragraph 4 will be reviewed, in particular with a view to reducing the limit value for cadmium and to reassess the derogation for the applications listed in points (a) to (e), by 31 December 2017.\n5. For the purpose of this entry, ‘cadmium plating’ means any deposit or coating of metallic cadmium on a metallic surface.\nShall not be used for cadmium plating metallic articles or components of the articles used in the following sectors/applications:\n(a) equipment and machinery for:\n— food production [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] — agriculture [8419 31] [8424 81] [8432] [8433] [8434] [8436] — cooling and freezing [8418] — printing and book-binding [8440] [8442] [8443]\n(b) equipment and machinery for the production of:\n— household goods [7321] [8421 12] [8450] [8509] [8516] — furniture [8465] [8466] [9401] [9402] [9403] [9404] — sanitary ware [7324] — central heating and air conditioning plant [7322] [8403] [8404] [8415]\nIn any case, whatever their use or intended final purpose, the placing on the market of cadmium-plated articles or components of such articles used in the sectors/applications listed in points (a) and (b) above and of articles manufactured in the sectors listed in point (b) above is prohibited.\n6. The provisions referred to in paragraph 5 shall also be applicable to cadmium-plated articles or components of such articles when used in the sectors/applications listed in points (a) and (b) below and to articles manufactured in the sectors listed in (b) below:\n(a) equipment and machinery for the production of:\n— paper and board [8419 32] [8439] [8441] textiles and clothing [8444] [8445] [8447] [8448] [8449] [8451] [8452]\n(b) equipment and machinery for the production of:\n— industrial handling equipment and machinery [8425] [8426] [8427] [8428] [8429] [8430] [8431] — road and agricultural vehicles [chapter 87] — rolling stock [chapter 86] — vessels [chapter 89]\n7. However, the restrictions in paragraphs 5 and 6 shall not apply to:\n— articles and components of the articles used in the aeronautical, aerospace, mining, offshore and nuclear sectors whose applications require high safety standards and in safety devices in road and agricultural vehicles, rolling stock\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nand vessels, — electrical contacts in any sector of use, where that is necessary to ensure the reliability required of the apparatus on which they are installed.\n8. Shall not be used in brazing fillers in concentration equal to or greater than 0,01 % by weight.\nBrazing fillers shall not be placed on the market if the concentration of cadmium (expressed as Cd metal) is equal to or greater than 0,01 % by weight.\nFor the purpose of this paragraph brazing shall mean a joining technique using alloys and undertaken at temperatures above 450 °C.\n9. By way of derogation, paragraph 8 shall not apply to brazing fillers used in defence and aerospace applications and to brazing fillers used for safety reasons.\n10. Shall not be used or placed on the market if the concentration is equal to or greater than 0,01 % by weight of the metal in:\n(i) metal beads and other metal components for jewellery making; (ii) metal parts of jewellery and imitation jewellery articles and hair accessories, including:\n— bracelets, necklaces and rings, — piercing jewellery, — wrist-watches and wrist-wear, — brooches and cufflinks.\n11. By way of derogation, paragraph 10 shall not apply to articles placed on the market before 10 December 2011 and jewellery more than 50 years old on 10 December 2011.\n________ __\n(*) OJ L 256, 7.9.1987, p. 42.\n(**) OJ L 365, 31.12.1994, p. 10","Für die Zwecke dieses Eintrags entsprechen die in eckigen Klammern stehenden Codes und Kapitel jenen der zolltariflichen und statistischen Nomenklatur des Gemeinsamen Zolltarifs gemäß der Verordnung (EWG) Nr. 2658/87 des Rates (*).\n1. Dürfen nicht in Gemischen und Erzeugnissen verwendet werden, die aus den folgenden synthetischen organischen Polymeren (nachstehend Kunststoff genannt) hergestellt werden:\no Polymere oder Copolymere aus Vinylchlorid (PVC) [3904 10] [3904 21],\no Polyurethan (PUR) [3909 50],\no Polyethylen niedriger Dichte (LDPE) mit Ausnahme des für die Herstellung von Pigmentpräparationen („master batch“) verwendeten Polyethylens niedriger Dichte [3901 10],\no Celluloseacetat (CA) [3912 11],\no Celluloseacetobutyrat (CAB) [3912 11],\no Epoxydharze [3907 30],\no Melaminharzformaldehyd (MF) [3909 20],\no Harnstoffformaldehyd (UF) [3909 10],\no ungesättigte Polyester (UP) [3907 91],\no Polyethylenterephtalat (PET) [3907 60],\no Polybuthylenterephtalat (PBT),\no Polystyrol glasklar/Standard [3903 11],\no Acrylnitrilmethylmetacrylat (AMMA),\no vernetztes Polyethylen (VPE),\no Polystyrol, schlagfest (SB),\no Polypropylen (PP) [3902 10].\nAus Kunststoffen hergestellte Gemische und Erzeugnisse wie die oben aufgeführten dürfen nicht in Verkehr gebracht werden, wenn ihr Cadmiumgehalt (Cd-Metall) 0,01 Gew.-% des Kunststoffs oder mehr beträgt.\nAbweichend davon gilt Unterabsatz 2 nicht für Erzeugnisse, die vor dem 10. Dezember 2011 in Verkehr gebracht wurden.\nUnterabsatz 1 und 2 gelten unbeschadet der Richtlinie 94/62/EG des Rates (**) und der auf ihrer Grundlage erlassenen Rechtsakte.\nBis zum 19. November 2012 fordert die Kommission gemäß Artikel 69 die Europäische Chemikalienagentur auf, ein Dossier entsprechend den Anforderungen des Anhangs XV zu erstellen, um zu bewerten, ob die Verwendung von Cadmium und Cadmiumverbindungen in anderen Kunststoffarten als den in Unterabsatz 1 aufgeführten beschränkt werden sollte.\n2. Dürfen nicht in Konzentrationen (Cd-Metall) von ≥ 0,01 Gew.-% in Anstrichfarben und Lacken mit den Codes [3208] [3209] verwendet oder in Verkehr gebracht werden.\nBei Anstrichfarben und Lacken mit den Codes [3208] [3209] mit einem Zinkgehalt > 10 Gew.-% der Anstrichfarbe bzw. des Lackes darf der Cadmiumgehalt (Cd-Metall) nicht ≥ 0,1 Gew.-% betragen.\nGestrichene/Lackierte Erzeugnisse dürfen nicht in Verkehr gebracht werden, wenn ihr Cadmiumgehalt (Cd-Metall) ≥ 0,1 Gew.-% der Anstrichfarbe/des Lackes auf dem gestrichenen/lackierten Erzeugnis beträgt.“\n3. Abweichend davon gelten die Absätze 1 und 2 nicht für Erzeugnisse, die aus Sicherheitsgründen mit cadmiumhaltigen Gemischen gefärbt sind.\n4. Abweichend davon gilt Absatz 1 Unterabsatz 2 nicht für:\no aus PVC-Abfall hergestellte Gemische, nachstehend -„Recycling-PVC“ genannt,\no Gemische und Erzeugnisse, die Recycling-PVC enthalten, sofern ihr Cadmiumgehalt (Cd-Metall) 0,1 Gew.-% des Kunststoffs in folgenden Hart-PVC-Anwendungen nicht übersteigt:\na) Profile und Hart-PVC-Platten für den Einsatz im Bauwesen,\nb) Türen, Fenster, Fensterläden, Wände, Jalousien, Zäune und Dachrinnen,\nc) Boden- und Terrassenbeläge,\nd) Kabelführungen,\ne) Wasserrohre, ausgenommen Trinkwasserrohre, sofern das Recycling-PVC in der mittleren Schicht eines mehrschichtigen Rohrs verwendet wird und vollständig mit einer Schicht von neu hergestelltem PVC nach Absatz 1 überzogen ist.\n5. Die Lieferanten gewährleisten vor dem erstmaligen Inverkehrbringen von Gemischen und Erzeugnissen, die Recycling-PVC enthalten, dass diese gut sichtbar, leserlich und unverwischbar mit der Aufschrift „Enthält Recycling-PVC“ oder mit folgendem Piktogramm versehen sind:\n\n6. Die in Absatz 4 gewährte Ausnahmeregelung wird gemäß Artikel 69 dieser Verordnung bis zum 31. Dezember 2017 insbesondere im Hinblick darauf überprüft, den Grenzwert für Cadmium zu senken und die Ausnahmeregelung für die unter den Buchstaben a bis e aufgeführten Anwendungen erneut zu beurteilen.\n7. Für die Zwecke dieses Eintrags bedeutet Cadmium-Oberflächenbehandlung (Cadmierung) jeglichen Auftrag von Cadmium auf Metalloberflächen oder jegliche Beschichtung von Metalloberflächen mit Cadmium.\nDürfen nicht verwendet werden zur Cadmierung von Metallerzeugnissen oder Bestandteilen der in den folgenden Sektoren bzw. zu den folgenden Zwecken eingesetzten Erzeugnisse:\na) Geräte und Maschinen:\no zur Herstellung von Lebensmitteln [8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11],\no für die Landwirtschaft [8419 31] [8424 81] [8432] [8433] [8434] [8436],\no für das Gefrieren und Tiefgefrieren [8418],\no für die Druckerei und Presse [8440] [8442] [8443],\nb) Geräte und Maschinen zur Herstellung von:\no Haushaltsgeräten [7321] [8421 12] [8450] [8509] [8516],\no Möbeln [8465] [8466] [9401] [9402] [9403] [9404],\no sanitären Anlagen [7324],\no Zentralheizungen und Klimaanlagen [7322] [8403] [8404] [8415],\nDas Inverkehrbringen von cadmierten Erzeugnissen oder von Bestandteilen solcher Erzeugnisse, die in den in den vorstehenden Buchstaben a und b genannten Sektoren bzw. zu den dort genannten Zwecken eingesetzt werden, sowie das Inverkehrbringen von Erzeugnissen, die in den unter dem vorstehenden Buchstaben b genannten Sektoren hergestellt wurden, ist auf jeden Fall - unabhängig von ihrer Verwendung oder endgültigen Bestimmung - verboten.\n8. Absatz 5 gilt ferner für cadmierte Erzeugnisse oder Bestandteile solcher Erzeugnisse, die in den in den nachstehenden Buchstaben a und b genannten Sektoren bzw. zu den dort genannten Zwecken eingesetzt werden, sowie für Erzeugnisse, die in den unter dem nachstehenden Buchstaben b genannten Sektoren hergestellt wurden:\na) Geräte und Maschinen zur Herstellung von:\no Papier und Pappe [8419 32] [8439] [8441],\nTextilien und Bekleidung [8444] [8445] [8447] [8448] [8449] [8451] [8452];\nb) Geräte und Maschinen zur Herstellung von:\no in der Materialflusstechnik eingesetzten Einrichtungen [8425] [8426] [8427] [8428] [8429] [8430] [8431],\no Pkw und landwirtschaftlichen Fahrzeugen [Kapitel 87],\no Zügen [Kapitel 86],\no Schiffen [Kapitel 89].\n9. Die Beschränkungen der Absätze 5 und 6 gelten jedoch nicht für:\no Erzeugnisse und Bestandteile von Erzeugnissen, die in der Luft- und Raumfahrt, im Bergbau, in der „Off-shore“-Technik sowie im Kernenergiebereich eingesetzt werden, wenn die Anwendungen ein hohes Sicherheitsniveau erfordern, sowie Komponenten von Sicherheitseinrichtungen in Straßenverkehrsmitteln, landwirtschaftlichen Fahrzeugen, Eisenbahnen und Schiffen,\no elektrische Kontakte in allen Verwendungssektoren aus Gründen der Zuverlässigkeit der Geräte, in denen sie eingesetzt werden.\n10. Dürfen nicht in Konzentrationen von 0,01 Gew.-% oder mehr in Hartloten verwendet werden.\nHartlote dürfen nicht in Verkehr gebracht werden, wenn der Cadmiumgehalt (Cd-Metall) 0,01 Gew.- % oder mehr beträgt.\nFür die Zwecke dieses Absatzes bedeutet Hartlöten eine Verbindungstechnik, bei der mit Legierungen bei Temperaturen über 450 °C gearbeitet wird.\n11. Abweichend davon gilt Absatz 8 weder für Hartlote, die in Verteidigungs- sowie Luft- und Raumfahrtanwendungen eingesetzt werden, noch für Hartlote, die aus Sicherheitsgründen verwendet werden.\n12. Dürfen nicht in Konzentrationen von 0,01 Gew.-% des Metalls oder mehr in folgenden Erzeugnissen verwendet oder in Verkehr gebracht werden:\ni) Metallperlen und andere metallische Teile für die Herstellung von Schmuckstücken,\nii) Metallteile für Schmuck- und Fantasiesch- muckerzeugnisse sowie Haarschmuck, einschließlich:\no Armbänder, Halsketten und Ringe,\no Piercingschmuck,\no Armbanduhren und Armschmuck,\no Broschen und Manschettenknöpfe.\n13. Abweichend davon gilt Absatz 10 weder für Erzeugnisse, die vor dem 10. Dezember 2011 in Verkehr gebracht wurden, noch für Schmuck, der am 10. Dezember 2011 mehr als 50 Jahre alt ist.\n___________\n(*) ABl. L 256 vom 7.9.1987, S. 42. (**) ABl. L 365 vom 31.12.1994, S. 10.\n","就本条目而言，方括号内的编码和章节的依据是委员会条例（EEC）第2658/87号（*）制定的共同海关关税的关税和统计术语。\n1. 不得用于由下列合成有机聚合物（以下简称塑料材料）生产的混合物和物品：\n氯乙烯（PVC）的聚合物或共聚物[3904 10] [3904 21] ， 聚氨酯（PUR）[3909 50] ，低密度聚乙烯（LDPE）（但用于生产有色颜料的低密度聚乙烯除外），醋酸纤维素（CA） [3912 11] ，醋酸纤维素丁酸酯（CAB） [3912 11]，环氧树脂 [3907 30] ，三聚氰胺甲醛树脂(MF) [3909 20] ，  尿素甲醛树脂（UF），不饱和聚酯（UP）[3907 91] ，聚对苯二甲酸乙二醇酯（PET）[3907 60]，聚对苯二甲酸丁二醇酯（PBT），透明/通用聚苯乙烯[3903 11] ，丙烯腈甲基丙烯酸酯（AMMA），交联聚乙烯（VPE），高抗冲聚苯乙烯-聚丙烯（PP）[3902 10] 。\n用上述塑料材料生产的混合物和物品，如果镉的浓度（以金属镉表示）等于或大于塑料材料重量的0.01%，则不得投放市场。\n作为减损，第二项不适用于2011年12月10日之前投放市场的商品。\n第一和第二项的适用不影响委员会指令94/62/ EC（**）和在其基础上通过的法案。\n在2012年11月19日之前，根据第69条，委员会应要求欧洲化学品管理局准备一份符合附件XV要求的档案，以评估是否应限制镉及其化合物在第1项所列以外的塑料材料中的使用。\n2. 若编码为[3208][3209]的涂料浓度（以金属镉表示）等于或大于0.01%（重量），不得使用或投入市场。\n若编码为[3208][3209]的涂料中锌含量超过涂料重量的10%时，镉的浓度（以金属镉表示）不得等于或大于重量的0.1%。\n如果镉的浓度（以金属镉表示）等于或大于被涂物上的油漆重量的0.1%，则被涂物不得投放市场。\n3. 出于安全考虑，第1和第2项不应适用于用含镉混合物着色的物品。\n4. 作为减损，第1项第二条不应适用于：\n- 由PVC废料生产的混合物，以下称为 \"回收的PVC\"。\n- 含有回收PVC的混合物和物品，如果在以下硬质PVC产品中，其镉的浓度（以金属镉表示）不超过塑料材料重量的0.1％。\n(a) 建筑用型材和硬质板材；(b) 门窗、百叶窗、墙壁、百叶窗、栅栏和屋顶排水沟；(c) 甲板和露台 ；(d) 电缆管道；(e) 非饮用水管道，如果回收的PVC用于多层管道的中间层，并且完全被符合上述第1项的新生产的PVC层覆盖。\n供应商应确保在首次将含有回收PVC的混合物和物品投放市场之前，明显、清晰、不可损毁地标明“含有回收的PVC\"，或带有如下图像标志。\n根据本条例第69条，将在2017年12月31日之前对第4项给予的减损进行审查，尤其是对于降低镉的限值，并对(a)至(e)所列的申请重新评估减损情况。\n5. 在本条目中，\"镀镉 \"是指在金属表面上的任何金属镉的沉积或涂层。\n不得用于对以下部门/应用中的金属物品或物品的部件进行镀镉：\n(a) 用于以下方面的设备和机械：\n食品生产[8210] [8417 20] [8419 81] [8421 11] [8421 22] [8422] [8435] [8437] [8438] [8476 11] ，农业[8419 31] [8424 81] [8432] [8433] [8434] [8436]，冷却和冷冻[8418] ，印刷和书籍装订[8440] [8442] [8443]\n用于生产的设备和机器：\n家居用品[7321] [8421 12] [8450] [8509] [8516] ，家具[8465] [8466] [9401] [9402] [9403] [9404] ，卫生洁具[7324] ，中央供热和空调设备[7322] [8403] [8404] [8415]\n在任何情况下，无论其用途或最终目的如何，禁止将上述(a)和(b)所列行业/应用中使用的镀镉物品或此类物品的部件以及上述(b)点所列行业中生产的物品投放市场。\n6.  第5项所述规定也应适用于用于以下(a)和(b)点所列部门/应用的镀镉物品或此类物品的部件，以及以下(b)点所列部门制造的物品。\n(a) 用于生产的设备和机器。\n- 纸和纸板[8419 32] [8439] [8441]， 纺织品和服装[8444] [8445] [8447] [8448] [8449] [8451] [8452]。\n用于生产的设备和机械：\n- 工业搬运设备和机械 [8425] [8426] [8427] [8428] [8429] [8430] [8431] ，公路和农业车辆 [第87章] ，机车车辆 [第86章] ，船舶 [第89章]\n7. 但是，第5项和第6项的限制不应适用于\n-需要很高安全标准的航空、航天、采矿、近海和核部门使用的物品及其部件；公路和农业车辆、机车车辆的安全装置；以及在任何使用领域中的电气触点，如果这对确保其安装的设备的可靠性是必要的。\n8. 不得在钎焊填料中使用浓度等于或大于0.01%（重量百分比）的填料。\n钎焊填料中的镉（以金属镉表示）的浓度等于或大于0.01%（重量）时，不得投放市场。\n在本项中，钎焊是指使用合金并在450℃以上温度下进行的连接技术。\n9. 作为减损，第8项不应适用于国防和航空航天应用中使用的钎焊填料和出于安全原因使用的钎焊填料。\n10. 如果在以下金属中的浓度等于或大于0.01%（重量），不得使用或投放市场。\n(i) 用于制造珠宝的金属珠和其他金属部件；(ii) 珠宝和仿制珠宝制品及发饰的金属部件，包括\n- 手镯、项链和戒指， - 穿孔首饰， - 手表和腕带， - 胸针和袖扣。\n11. 作为减损，第10项不应适用于2011年12月10日之前投放市场的物品和2011年12月10日超过50年的珠宝。\n"]
[null,{"$f":"IF($B$1=\"English\",C1698,IF($B$1=\"Deutsch\",D1698,IF($B$1=\"中文\",E1698,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market.\n2. By way of derogation, paragraph 1 shall not apply:\n(a) in the case of plant and machinery already in service on 18 June 1994, until such plant and machinery is disposed of; (b) in the case of the maintenance of plant and machinery already in service within a Member State on 18 June 1994.\nFor the purposes of point (a) Member States may, on grounds of human health protection and environmental protection, prohibit within their territory the use of such plant or machinery before it is disposed of."},"1. Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market.\n2. By way of derogation, paragraph 1 shall not apply:\n(a) in the case of plant and machinery already in service on 18 June 1994, until such plant and machinery is disposed of; (b) in the case of the maintenance of plant and machinery already in service within a Member State on 18 June 1994.\nFor the purposes of point (a) Member States may, on grounds of human health protection and environmental protection, prohibit within their territory the use of such plant or machinery before it is disposed of.","Darf weder als Stoff noch in Gemischen in Verkehr gebracht oder verwendet werden. Erzeugnisse, die diesen Stoff enthalten, dürfen nicht in Verkehr gebracht werden.\nAbsatz 1 gilt jedoch nicht für:\na) Anlagen und Maschinenteile, die sich am 18. Juni 1994 bereits im Betrieb befanden, bis diese Anlagen und Maschinenteile entsorgt werden,\nb) die Wartung von Anlagen und Maschinenteilen, die sich am 18. Juni 1994 bereits in einem Mitgliedstaat im Betrieb befanden. Für die Zwecke von Buchstabe a können die Mitgliedstaaten jedoch aus Gründen des Gesundheits- und des Umweltschutzes in ihrem Hoheitsgebiet die Verwendung dieser Anlagen und Maschinenteile vor deren Entsorgung untersagen.","1.物质或含有该物质的制剂，不得投放市场销售。含有该物质的物品，也不得投放市场销售。\n2. 作为免除项目，第1项不适用于：\n（a）对于1994年6月18日前已投入使用的工厂和机器设备，可一直使用至机器的组件和设备报废\n（b）维修1994年6月18日前已在成员国投入使用的工厂和机器设备。\n对于免除项（a），成员国可以因为健康和环境的保护的原因，禁止在其境内使用这种工厂或设备，哪怕它们尚未报废。"]
[null,{"$f":"IF($B$1=\"English\",C1699,IF($B$1=\"Deutsch\",D1699,IF($B$1=\"中文\",E1699,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market."},"Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market.","Darf weder als Stoff noch in Gemischen in Verkehr gebracht oder verwendet werden.\n\nErzeugnisse, die diesen Stoff enthalten, dürfen nicht in Verkehr gebracht werden.","物质或含有该物质的制剂，不得投放市场销售。含有该物质的物品，也不得投放市场销售。"]
[null,{"$f":"IF($B$1=\"English\",C1700,IF($B$1=\"Deutsch\",D1700,IF($B$1=\"中文\",E1700,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market."},"Shall not be placed on the market, or used, as a substance or in mixtures.\nArticles containing the substance shall not be placed on the market.","Darf weder als Stoff noch in Gemischen in Verkehr gebracht oder verwendet werden.\n\nErzeugnisse, die diesen Stoff enthalten, dürfen nicht in Verkehr gebracht werden.","物质或含有该物质的制剂，不得投放市场销售。含有该物质的物品，也不得投放市场销售。"]
[null,{"$f":"IF($B$1=\"English\",C1701,IF($B$1=\"Deutsch\",D1701,IF($B$1=\"中文\",E1701,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used:\n(a) in any post assemblies which are inserted into pierced ears and other pierced parts of the human body unless the rate of nickel release from such post assemblies is less than 0,2 μg/cm²/week (migration limit); (b) in articles intended to come into direct and prolonged contact with the skin such as:\n— earrings, — necklaces, bracelets and chains, anklets, finger rings, — wrist-watch cases, watch straps and tighteners, — rivet buttons, tighteners, rivets, zippers and metal marks, when these are used in garments,\nif the rate of nickel release from the parts of these articles coming into direct and prolonged contact with the skin is greater than 0,5 μg/cm²/week.\n(c) in articles referred to in point (b) where these have a non-nickel coating unless such coating is sufficient to ensure that the rate of nickel release from those parts of such articles coming into direct and prolonged contact with the skin will not exceed 0,5 μg/cm²/week for a period of at least two years of normal use of the article.\n2. Articles which are the subject of paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. The standards adopted by the European Committee for Standardisation (CEN) shall be used as the test methods for demonstrating the conformity of articles to paragraphs 1 and 2."},"1. Shall not be used:\n(a) in any post assemblies which are inserted into pierced ears and other pierced parts of the human body unless the rate of nickel release from such post assemblies is less than 0,2 μg/cm²/week (migration limit); (b) in articles intended to come into direct and prolonged contact with the skin such as:\n— earrings, — necklaces, bracelets and chains, anklets, finger rings, — wrist-watch cases, watch straps and tighteners, — rivet buttons, tighteners, rivets, zippers and metal marks, when these are used in garments,\nif the rate of nickel release from the parts of these articles coming into direct and prolonged contact with the skin is greater than 0,5 μg/cm²/week.\n(c) in articles referred to in point (b) where these have a non-nickel coating unless such coating is sufficient to ensure that the rate of nickel release from those parts of such articles coming into direct and prolonged contact with the skin will not exceed 0,5 μg/cm²/week for a period of at least two years of normal use of the article.\n2. Articles which are the subject of paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. The standards adopted by the European Committee for Standardisation (CEN) shall be used as the test methods for demonstrating the conformity of articles to paragraphs 1 and 2.","1. Darf nicht verwendet werden:\na) in sämtlichen Stäben, die in durchstochene Ohren oder andere durchstochene Körperteile eingeführt werden, außer wenn die Nickelabgabe aus solchen Stäben unter 0,2 μg/cm 2 /Woche liegt (Migrationslimit);\nb) in Erzeugnissen, die dazu bestimmt sind, unmittelbar und länger mit der Haut in Berührung zu kommen, wie zum Beispiel:\n- Ohrringen,\n- Halsketten, Armbändern und Ketten, Fußringen und Fingerringen,\n- Armbanduhrgehäusen, Uhrarmbändern und Spannern,\n- Nietknöpfen, Spangen, Nieten, Reißverschlüssen und Metallmarkierungen, wenn   sie in Kleidungsstücken verwendet werden,\nsofern die Nickelfreisetzung von den Teilen dieser Erzeugnisse, die unmittelbar und länger mit der Haut in Berührung kommen, 0,5 μg/ cm 2 /Woche übersteigt;\nc) in den in Buchstabe b aufgeführten Erzeugnissen, die eine Nichtnickelbeschichtung haben, es sei denn, diese Beschichtung reicht aus, um sicherzustellen, dass die Nickelfreisetzung von den Teilen solcher Erzeugnisse, die unmittelbar und länger mit der Haut in Berührung kommen, 0,5 μg/cm 2 /Woche für einen Zeitraum von mindestens zwei Jahren normaler Verwendung des Erzeugnisses nicht übersteigen.\n\n2. Erzeugnisse, für die Absatz 1 gilt, dürfen nicht in Verkehr gebracht werden, wenn sie nicht den Bestimmungen dieses Absatzes entsprechen.\n3. Zum Nachweis der Vereinbarkeit der Erzeugnisse mit Absatz 1 und 2 sind als Testmethoden die vom Europäischen Komitee für Normung (CEN) verabschiedeten Normen zu verwenden.","1. 不得用于：\na）耳洞和人体其它穿刺部位使用的配件，无论这种物品最终是否被除去。除非镍的释出速率小于0.2g/cm2/周(迁移限值)\nb）与皮肤有直接及长期接触的成品，如：\n-耳环\n-项链，手镯和项圈，脚环，戒指\n-手表壳、表带和带扣\n-铆扣、搭扣、铆钉、拉链和金属标牌等用作服装上的物件\n-如果这些与皮肤有直接及长期接触的成品中镍的释放速率超过了0.5g/cm2/周\nc）对于具有非镍镀层的1（b）中列出的成品，除非这种镀层足以保证在至少两年的正常使用过程中，从这些成品的与皮肤有直接或长期接触的部位释放出来的镍的速率不超过0.5g/cm2/周者，不受此限制。\n2.前项中的成品，除非其符合那些项目的要求，否则不能投放市场。\n3. 欧洲标准委员会(CEN)所采用的标准可作为证明成品是否符合第1、2项要求的测试方法。"]
[null,{"$f":"IF($B$1=\"English\",C1702,IF($B$1=\"Deutsch\",D1702,IF($B$1=\"中文\",E1702,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Without prejudice to the other parts of this Annex the following shall apply to entries 28 to 30:\n1. Shall not be placed on the market, or used,\n— as substances, \n— as constituents of other substances, or, \n— in mixtures,\nfor supply to the general public when the individual concentration in the substance or mixture is equal to or greater than:\n— either the relevant specific concentration limit specified in Part 3 of Annex VI to Regulation (EC) No 1272/2008, or,\n— the relevant generic concentration limit specified in Part 3 of Annex I of Regulation (EC) No 1272/2008.\nWithout prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is marked visibly, legibly and indelibly as follows:\n‘Restricted to professional users’.\n2. By way of derogation, paragraph 1 shall not apply to:\n(a) medicinal or veterinary products as defined by Directive 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC;\n(c) the following fuels and oil products:\n— motor fuels which are covered by Directive 98/70/EC,\n— mineral oil products intended for use as fuel in mobile or fixed combustion plants,\n— fuels sold in closed systems (e.g. liquid gas bottles);\n\n(d) artists’ paints covered by Regulation (EC) No 1272/2008;\n(e) the substances listed in Appendix 11, column 1, for the applications or uses listed in Appendix 11, column 2. Where a date is specified in column 2 of Appendix 11, the derogation shall apply until the said date;\n(f) devices covered by Regulation (EU) 2017/745."},"Without prejudice to the other parts of this Annex the following shall apply to entries 28 to 30:\n1. Shall not be placed on the market, or used,\n— as substances, \n— as constituents of other substances, or, \n— in mixtures,\nfor supply to the general public when the individual concentration in the substance or mixture is equal to or greater than:\n— either the relevant specific concentration limit specified in Part 3 of Annex VI to Regulation (EC) No 1272/2008, or,\n— the relevant generic concentration limit specified in Part 3 of Annex I of Regulation (EC) No 1272/2008.\nWithout prejudice to the implementation of other Community provisions relating to the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is marked visibly, legibly and indelibly as follows:\n‘Restricted to professional users’.\n2. By way of derogation, paragraph 1 shall not apply to:\n(a) medicinal or veterinary products as defined by Directive 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC;\n(c) the following fuels and oil products:\n— motor fuels which are covered by Directive 98/70/EC,\n— mineral oil products intended for use as fuel in mobile or fixed combustion plants,\n— fuels sold in closed systems (e.g. liquid gas bottles);\n\n(d) artists’ paints covered by Regulation (EC) No 1272/2008;\n(e) the substances listed in Appendix 11, column 1, for the applications or uses listed in Appendix 11, column 2. Where a date is specified in column 2 of Appendix 11, the derogation shall apply until the said date;\n(f) devices covered by Regulation (EU) 2017/745.","Unbeschadet der übrigen Teile dieses Anhangs gilt Folgendes für die Einträge 28 bis 30:\n1. Dürfen nicht in Verkehr gebracht oder verwendet werden:\no als Stoffe,\no als Bestandteile anderer Stoffe oder\no in Gemischen,\ndie zum Verkauf an die breite Öffentlichkeit bestimmt sind, wenn die Einzelkonzentration des Stoffs oder Gemischs folgende Werte erreicht oder übersteigt:\no die jeweiligen in Anhang VI Teil 3 der Verordnung (EG) Nr. 1272/2008 festgelegten spezifischen Konzentrationsgrenzwerte oder\no die jeweiligen in Anhang I Teil 3 der Verordnung (EG) Nr. 1272/2008 festgelegten allgemeinen Konzentrationsgrenzwerte.\nUnbeschadet der übrigen gemeinschaftlichen Vorschriften auf dem Gebiet der Einstufung, Verpackung und Etikettierung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung solcher Stoffe und Gemische gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist: „Nur für gewerbliche Anwender.“\n2. Absatz 1 gilt jedoch nicht für:\na) Arznei- oder Tierarzneimittel gemäß der Begriffsbestimmung in der Richtlinie 2001/82/EG und der Richtlinie 2001/83/EG;\nb) kosmetische Mittel gemäß der Richtlinie 76/ 768/EWG; c) folgende Brennstoffe und Mineralölerzeugnisse:\no Kraftstoffe, die Gegenstand der Richtlinie 98/70/EG sind,\no Mineralölerzeugnisse, die zur Verwendung als Brennstoff oder Kraftstoff in beweglichen oder feststehenden Verbrennungsanlagen bestimmt sind,\no Brennstoffe, die in geschlossenen Systemen (z. B. Flüssiggasflaschen) verkauft werden;\nd) Farben für Künstler gemäß der Verordnung (EG) Nr. 1272/2008;\ne) in Anlage 11 Spalte 1 aufgeführte Stoffe für die in Anlage 11 Spalte 2 aufgeführten Anwendungen. Ist in Anlage 11 Spalte 2 ein Datum angegeben, gilt die Ausnahmeregelung bis zu diesem Datum.\nf) Produkte, die Gegenstand der Verordnung (EU) 2017/745 sind","\n在不违背本附录其它规定的情况下，下列规定适用于28项至30项：\n1.不应用于个别浓度大于或等于以下规定的物质或制剂，投放市场销售给一般大众：\n-法规1272/2008/EC附件VI所具体规定的相关浓度；\n-法规1999/45/EC所具体规定的相关浓度，其中法规1272/2008/EC法规VI没有设置具体的浓度限制；\n在不违反欧盟危险物质与制剂分离、包装和标识的欧盟法规规定的情况下，该物质或制剂包装应以不可磨灭的方式清楚标示如下字样：\n”Restricted to professional users禁止非专业人员使用”\n2.作为免除项目，第一项不适用于：\na)法规2001/82/EC和法规2001/83/EC所定义的医药和兽药；\nb)法规76/768/EEC所定义的化妆品；\nc)以下燃料和油品：\n-法规98/70/EC覆盖的汽车燃料，\n-车辆或定点燃烧所用矿物油， \n-销售给密闭系统的燃料，如液化气瓶\nd)法规11272/2008/EC涵盖的绘画颜料；\ne)附件11的第一列中列出的物质应用于附件11的第二列中列出的应用时。免除项目可适用至附件11的第二列中指定的时间为止。"]
[null,{"$f":"IF($B$1=\"English\",C1703,IF($B$1=\"Deutsch\",D1703,IF($B$1=\"中文\",E1703,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for the treatment of wood. Furthermore, wood so treated shall not be placed on the market.\n2. By way of derogation from paragraph 1:\n(a) The substances and mixtures may be used for wood treatment in industrial installations or by professionals covered by Community legislation on the protection of workers for in situ retreatment only if they contain:\n(i) benzo[a]pyrene at a concentration of less than 50 mg/kg (0,005 % by weight), and\n(ii) water extractable phenols at a concentration of less than 3 % by weight.\nSuch substances and mixtures for use in wood treatment in industrial installations or by professionals:\n— may be placed on the market only in packaging of a capacity equal to or greater than 20 litres,\n— shall not be sold to consumers.\nWithout prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations or professional treatment only’.\n(b) Wood treated in industrial installations or by professionals according to subparagraph (a) which is placed on the market for the first time or retreated in situ may be used for professional and industrial use only, for example on railways, in electric power transmission and telecommunications, for fencing, for agricultural purposes (for example stakes for tree support) and in harbours and waterways.\n(c) The prohibition in paragraph 1 on the placing on the market shall not apply to wood which has been treated with substances listed in entry 31 (a) to (i) before 31 December 2002 and is placed on the second-hand market for re-use.\n3. Treated wood referred to under paragraph 2(b) and (c) shall not be used:\n— inside buildings, whatever their purpose,\n— in toys,\n— in playgrounds,\n— in parks, gardens, and outdoor recreational and leisure facilities where there is a risk of frequent skin contact,\n— in the manufacture of garden furniture such as picnic tables,\n— for the manufacture and use and any re-treatment of:\n— containers intended for growing purposes,\n— packaging that may come into contact with raw materials, intermediate or finished products destined for human and/or animal consumption,\n— other materials which may contaminate the articles mentioned above."},"1. Shall not be placed on the market, or used, as substances or in mixtures where the substance or mixture is intended for the treatment of wood. Furthermore, wood so treated shall not be placed on the market.\n2. By way of derogation from paragraph 1:\n(a) The substances and mixtures may be used for wood treatment in industrial installations or by professionals covered by Community legislation on the protection of workers for in situ retreatment only if they contain:\n(i) benzo[a]pyrene at a concentration of less than 50 mg/kg (0,005 % by weight), and\n(ii) water extractable phenols at a concentration of less than 3 % by weight.\nSuch substances and mixtures for use in wood treatment in industrial installations or by professionals:\n— may be placed on the market only in packaging of a capacity equal to or greater than 20 litres,\n— shall not be sold to consumers.\nWithout prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations or professional treatment only’.\n(b) Wood treated in industrial installations or by professionals according to subparagraph (a) which is placed on the market for the first time or retreated in situ may be used for professional and industrial use only, for example on railways, in electric power transmission and telecommunications, for fencing, for agricultural purposes (for example stakes for tree support) and in harbours and waterways.\n(c) The prohibition in paragraph 1 on the placing on the market shall not apply to wood which has been treated with substances listed in entry 31 (a) to (i) before 31 December 2002 and is placed on the second-hand market for re-use.\n3. Treated wood referred to under paragraph 2(b) and (c) shall not be used:\n— inside buildings, whatever their purpose,\n— in toys,\n— in playgrounds,\n— in parks, gardens, and outdoor recreational and leisure facilities where there is a risk of frequent skin contact,\n— in the manufacture of garden furniture such as picnic tables,\n— for the manufacture and use and any re-treatment of:\n— containers intended for growing purposes,\n— packaging that may come into contact with raw materials, intermediate or finished products destined for human and/or animal consumption,\n— other materials which may contaminate the articles mentioned above.","1. Dürfen nicht als Stoffe oder in Gemischen in Verkehr gebracht oder verwendet werden, die zur Holzbehandlung bestimmt sind. Ferner darf damit behandeltes Holz nicht in Verkehr gebracht werden.\n2. Abweichend von Absatz 1 bestehen jedoch folgende Ausnahmen:\na) Diese Stoffe und Gemische dürfen zur Holzbehandlung in industriellen Anlagen oder zu gewerblichen Zwecken, für die die gemeinschaftlichen Rechtsvorschriften über den Schutz der Arbeitnehmer bei der Wiederbehandlung vor Ort gelten, nur dann verwendet werden, wenn sie\ni) Benzo[a]pyren in einer Konzentration von weniger als 50 mg/kg (0,005 Gew.-%) und\nii) wasserlösliche Phenole in einer Konzentration von weniger als 3 Gew.-% enthalten.\nSolche Stoffe und Gemische zur Verwendung bei der Holzbehandlung in industriellen Anlagen oder zu gewerblichen Zwecken dürfen\no nur in Verpackungen mit einem Fassungsvermögen von 20 Litern oder mehr in den Verkehr gebracht werden,\no nicht an Verbraucher abgegeben werden.\nUnbeschadet der übrigen gemeinschaftlichen Vorschriften auf dem Gebiet der Einstufung, Verpackung und Etikettierung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung solcher Stoffe und Gemische gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n„Verwendung nur in Industrieanlagen und zu gewerblichen Zwecken“.\nb) Für nach Buchstabe a in industriellen Anlagen oder zu gewerblichen Zwecken behandeltes Holz, das zum ersten Mal in Verkehr gebracht wird oder vor Ort wieder behandelt wird, gilt: Die Verwendung ist ausschließlich für gewerbliche und industrielle Zwecke erlaubt (z. B. Eisenbahn, Stromtransport, Telekommunikation, Zäune, für landwirtschaftliche Zwecke - etwa Baumstützen -, Häfen, Wasserwege).\nc) Das Verbot für das Inverkehrbringen nach Absatz 1 gilt nicht für Holz, das vor dem 31. Dezember 2002 mit unter Eintrag 31 Buchstaben a bis i aufgeführten Stoffen behandelt wurde und zur Wiederverwendung auf dem Gebrauchtmarkt angeboten wird.\n3. Die Verwendung von behandeltem Holz nach Absatz 2 Buchstaben b und c ist jedoch verboten:\no innerhalb von Gebäuden, unabhängig von deren Zweckbestimmung;\no bei Spielzeugen;\no auf Spielplätzen;\no in Parks, Gärten und anderen Orten im Freien, die der Freizeitgestaltung und der Erholung dienen und bei denen die Gefahr eines häufigen Hautkontakts besteht;\no für die Anfertigung von Gartenmobiliar wie etwa Picknicktischen;\no für die Anfertigung, Verwendung und Wiederaufarbeitung von:\n­ Behältern für lebende Pflanzen,\n­ Verpackungen, die mit Rohmaterialien, Zwischen- und/oder Enderzeugnissen für die menschliche und/oder tierische Ernährung in Berührung kommen,\n­ anderem Material, das die oben genannten Erzeugnisse kontaminieren kann.\n\n","1.不得投放到市场或使用作为木材处理剂或添加在木材处理剂中。此外，经处理过的木材也不得投放市场。\n2. 然而，第1款的例外如下：\n(a)这种物质和制剂，可用于工业装置中的木材处理，依据欧共体法规对劳工保护规定，如果含有下列情形者，仅能于现场再处理：\ni）含苯并[a]芘的浓度小于50毫克/公斤（质量百分比0.005%），而且\nii）可被水萃取的酚的质量浓度低于3%。\n此类物质及制剂用于工业设施或由专业作业人员使用于木材处理时，只有当包装容量大于等于20升时才可以投放市场，而且不得出售给消费者。\n在不违反其它关于物质和配制品的分类、包装和标签等方面规定的前提下，供应商应在投放市场之前确保，对于这些物质含量大于等于0.1%的材料和配制品，其包装上应该清晰易见且永久的标记有以下文字：\n“仅供工业设施或专业用途使用”\n(b)根据前述(a)点，在工业设备中或由专业人员处理的木材，首次投放市场或者现场再处理，仅允许用于专业和工业用途，例如用在铁路，电力传输和通信中，用作围栏，用于农业用途，比如树木保护桩，用在港口和航运。\n(c)第1款禁用不适用于已经在2002年12月31日前用条款31(a)至(i)中的物质处理过的木材，投放到二手市场进行再利用。\n3. 小节2(b)和(c)提及的处理过的木材禁止用于：\n- 建筑物内部，无论什么用途的建筑物\n- 玩具；\n- 操场；\n-公园，花园和及其它与皮肤有频繁接触的风险的户外休闲娱乐设施;\n-庭院类家具，如野餐桌；\n-包括以下内容在内的任何用于制造，使用和再处理的物品：\n    -种植用容器；\n    -可能与原料，中间产品，或预定为人或动物消费的产品接触的包装；\n    -其它可能污染上述物品的材料"]
[null,{"$f":"IF($B$1=\"English\",C1704,IF($B$1=\"Deutsch\",D1704,IF($B$1=\"中文\",E1704,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Without prejudice to the other parts of this Annex, the following shall apply to entries 32,34 to 38:\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or in mixtures in concentrations equal to or greater than 0,1 % by weight,\nwhere the substance or mixture is intended for supply to the general public and/or is intended\nfor diffusive applications such as in surface cleaning and cleaning of fabrics.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures containing them in concentrations equal to or greater than 0,1 % by weight is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations only’.\nBy way of derogation this provision shall not apply to:\n(a) medicinal or veterinary products as defined by\nDirective 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC."},"Without prejudice to the other parts of this Annex, the following shall apply to entries 32,34 to 38:\n1. Shall not be placed on the market, or used,\n— as substances,\n— as constituents of other substances, or in mixtures in concentrations equal to or greater than 0,1 % by weight,\nwhere the substance or mixture is intended for supply to the general public and/or is intended\nfor diffusive applications such as in surface cleaning and cleaning of fabrics.\n2. Without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of such substances and mixtures containing them in concentrations equal to or greater than 0,1 % by weight is visibly, legibly and indelibly marked as follows:\n‘For use in industrial installations only’.\nBy way of derogation this provision shall not apply to:\n(a) medicinal or veterinary products as defined by\nDirective 2001/82/EC and Directive 2001/83/EC;\n(b) cosmetic products as defined by Directive 76/768/EEC.","Unbeschadet der übrigen Teile dieses Anhangs gilt Folgendes für die Einträge 32, 34 bis 38:\n1. Dürfen nicht in Verkehr gebracht oder verwendet werden:\no als Stoffe,\no als Bestandteile anderer Stoffe oder in Gemischen in Konzentrationen von 0,1 Gew.-% oder mehr,\nwenn der Stoff oder das Gemisch für die Abgabe an die breite Öffentlichkeit und/oder die Anwendung in Formen bestimmt ist, bei denen eine Freisetzung\nnicht ausgeschlossen ist (beispielsweise Oberflächenreinigung und Reinigung von Textilien).\n2. Unbeschadet anderer Vorschriften der Gemeinschaft für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass die Verpackung solcher Stoffe und Gemische, in denen sie in Konzentrationen von ≥ 0,1 Gew.-% enthalten sind, gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n„Nur zur Verwendung in Industrieanlagen“.\nDiese Anforderung gilt jedoch nicht für:\na) Arznei- oder Tierarzneimittel gemäß der Begriffsbestimmung in der Richtlinie 2001/82/EG und der Richtlinie 2001/83/EG;\nb) kosmetische Mittel gemäß der Begriffsbestimmung in der Richtlinie 76/768/EWG des Rates.","在不违反本附件的其他部分的前提下，以下条款适用于条目32至38：\n1.以下情况下不可以销售或使用：\n1)作为纯物质,\n2)作为别的物质的组成部分，或者作为质量百分比大于等于0.1%的配制品的组成部分,如果此物质或此配制品将面向广大公众的供应，并且/或者将被广泛应用，如用于表面清洁剂和纺织物的清洗剂中\n\n2.不影响其它关于物质和配制品的分类、包装和标签等方面的公共规定，供应商应在投放市场之前确保，对于这些物质含量大于等于0.1%的物质和配制品，其包装上应该清晰易见且永久的标记有以下文字：\n“仅允许在工业设施的使用”。\n但是，这些要求不用于： \n根据指令2001/82/EG和2001/83/ EC定义的药品和兽药;\n根据指令76/768/EWG定义的化妆品\n"]
[null,{"$f":"IF($B$1=\"English\",C1705,IF($B$1=\"Deutsch\",D1705,IF($B$1=\"中文\",E1705,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substance or in mixtures, where the substance or mixture is intended for the manufacturing or processing of non-ferrous metals."},"Shall not be placed on the market, or used, as substance or in mixtures, where the substance or mixture is intended for the manufacturing or processing of non-ferrous metals.","Darf nicht als Stoff oder in Gemischen zur Herstellung oder Verarbeitung von Nichteisenmetallen in Verkehr gebracht oder verwendet werden.","物质或混合物不得投放市场或用于有色金属的生产或加工。 "]
[null,{"$f":"IF($B$1=\"English\",C1706,IF($B$1=\"Deutsch\",D1706,IF($B$1=\"中文\",E1706,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Azodyes which, by reductive cleavage of one or more azo groups, may release one or more of the aromatic amines listed in Appendix 8, in detectable concentrations, i.e. above 30 mg/kg (0,003 % by weight) in the articles or in the dyed parts thereof, according to the testing methods listed in Appendix 10, shall not be used, in textile and leather articles which may come into direct and prolonged contact with the human skin or oral cavity, such as:\n— clothing, bedding, towels, hairpieces, wigs, hats, nappies and other sanitary items, sleeping bags,\n— footwear, gloves, wristwatch straps, handbags, purses/wallets, briefcases, chair covers, purses worn round the neck,\n— textile or leather toys and toys which include textile or leather garments,\n— yarn and fabrics intended for use by the final consumer.\n2. Furthermore, the textile and leather articles referred to in paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. Azodyes, which are contained in Appendix 9, ‘List of azodyes’ shall not be placed on the market, or used, as substances, or in mixtures in concentrations greater than 0,1 % by weight, where the substance or the mixture is intended for colouring textile and leather articles."},"1. Azodyes which, by reductive cleavage of one or more azo groups, may release one or more of the aromatic amines listed in Appendix 8, in detectable concentrations, i.e. above 30 mg/kg (0,003 % by weight) in the articles or in the dyed parts thereof, according to the testing methods listed in Appendix 10, shall not be used, in textile and leather articles which may come into direct and prolonged contact with the human skin or oral cavity, such as:\n— clothing, bedding, towels, hairpieces, wigs, hats, nappies and other sanitary items, sleeping bags,\n— footwear, gloves, wristwatch straps, handbags, purses/wallets, briefcases, chair covers, purses worn round the neck,\n— textile or leather toys and toys which include textile or leather garments,\n— yarn and fabrics intended for use by the final consumer.\n2. Furthermore, the textile and leather articles referred to in paragraph 1 shall not be placed on the market unless they conform to the requirements set out in that paragraph.\n3. Azodyes, which are contained in Appendix 9, ‘List of azodyes’ shall not be placed on the market, or used, as substances, or in mixtures in concentrations greater than 0,1 % by weight, where the substance or the mixture is intended for colouring textile and leather articles.","1. Azofarbstoffe, die durch reduktive Spaltung einer oder mehrerer Azogruppen eines oder mehrere der in Anlage 8 aufgeführten aromatischen Amine in - gemäß den in Anlage 10 aufgeführten Prüfverfahren - nachweisbaren Konzentrationen, d. h. > 30 mg/kg (0,003 Gew.-%) im Fertigerzeugnis\noder in gefärbten Teilen davon, freisetzen können, dürfen nicht in Textil- und Ledererzeugnissen verwendet werden, die mit der menschlichen\nHaut oder der Mundhöhle direkt und längere Zeit in Berührung kommen können, wie beispielsweise:\no Kleidung, Bettwäsche, Handtücher, Haarteile, Perücken, Hüte, Windeln und sonstige Toilettenartikel, Schlafsäcke,\no Schuhe, Handschuhe, Armbanduhren, Handtaschen, Geldbeutel und Brieftaschen, Aktentaschen, Stuhlüberzüge, Brustbeutel,\no Textil- und Lederspielwaren und Spielwaren mit Textil- oder Lederbekleidung,\no für den Endverbraucher bestimmte Garne und Gewebe.\n2. Außerdem dürfen die in Absatz 1 genannten Textil- und Ledererzeugnisse nicht in Verkehr gebracht werden, wenn sie nicht den in diesem Absatz\nfestgelegten Anforderungen entsprechen.\n3. Die in Anlage 9, „Liste der Azofarbstoffe“, dieser Verordnung aufgeführten Azofarbstoffe dürfen weder als Stoffe noch in Gemischen in Konzentrationen\nvon über 0,1 Gew.-% in Verkehr gebracht oder verwendet werden, wenn diese zum Färben von Textil- oder Ledererzeugnissen bestimmt sind.","1.偶氮染料，经由一个或多个偶氮基团还原裂解后，可能会释放出一个或多个可探测浓度的附录8中列出的芳香胺。也就是依据附录10中的测试方法，在其成品或上料组件可检测浓度高于30PPM者，不可用于下列可能与皮肤或口腔直接或长时间接触的纺织或皮革制品：\n—服装，床上用品，毛巾，假发，假发，帽子，尿布及其它卫生用品，睡袋\n—鞋类，手套，手表带，手提袋，钱包和钱夹，公文包，椅子套\n—织物和皮革玩具，以及穿着织物或皮革服装的玩具\n—最终消费者使用的纱线和布料。\n2.另外，第1款提到的纺织品和皮革制品，应符合该项规定要求，否则不可投放市场。\n3.在附录9中列出的偶氮染料，其物质或制备浓度大于0.1重量百分比时，不可置于市场用于纺织品或皮革制品的染色"]
[null,{"$f":"IF($B$1=\"English\",C1707,IF($B$1=\"Deutsch\",D1707,IF($B$1=\"中文\",E1707,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market, or used:\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations greater than 0,1 % by weight.\n2. Articles shall not be placed on the market if they, or flame-retardant parts thereof, contain this substance in concentrations greater than 0,1 % by weight.\n3. By way of derogation, paragraph 2 shall not apply:\n— to articles that were in use in the Community before 15 August 2004,\n— to electrical and electronic equipment within the scope of Directive 2002/95/EC."},"1. Shall not be placed on the market, or used:\n— as a substance,\n— as a constituent of other substances, or in mixtures, in concentrations greater than 0,1 % by weight.\n2. Articles shall not be placed on the market if they, or flame-retardant parts thereof, contain this substance in concentrations greater than 0,1 % by weight.\n3. By way of derogation, paragraph 2 shall not apply:\n— to articles that were in use in the Community before 15 August 2004,\n— to electrical and electronic equipment within the scope of Directive 2002/95/EC.","1. Darf nicht in Verkehr gebracht oder verwendet werden:\no als Stoff,\no als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von 0,1 Gew.-% oder mehr.\n2. Erzeugnisse dürfen nicht in Verkehr gebracht werden, wenn sie oder ihre mit Flammschutzmittel behandelten Teile diesen Stoff in einer Konzentration\nvon mehr als 0,1 Gew.-% enthalten.\n3. Absatz 2 gilt jedoch nicht für:\no Erzeugnisse, die vor dem 15. August 2004 in der Gemeinschaft verwendet wurden,\no Elektro- und Elektronikgeräte, die unter die Richtlinie 2002/95/EG fallen.","1. 以下情况不得投放市场或使用：\n  — 作为纯物质；\n  — 作为别的物质的组分，或者在配制品中，浓度大于等于0,1%时\n2.物品中或者其阻燃剂处理过的部件中该物质含量超过0.1%时，该物品不得投放市场。\n3. 第2段在以下情况下不适用：\n— 在15.08.2004年前已投入使用的物品；\n— 符合2002/95/EC范围内的电子电气设备"]
[null,{"$f":"IF($B$1=\"English\",C1708,IF($B$1=\"Deutsch\",D1708,IF($B$1=\"中文\",E1708,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as substances or in mixtures in concentrations equal to or greater than 0,1 % by weight for the following purposes:\n(1) industrial and institutional cleaning except:\n— controlled closed dry cleaning systems where the washing liquid is recycled or incinerated,\n— cleaning systems with special treatment where the washing liquid is recycled or incinerated.\n(2) domestic cleaning;\n(3) textiles and leather processing except:\n— processing with no release into waste water,\n— systems with special treatment where the process water is pre-treated to remove the organic fraction completely prior to biological waste water treatment (degreasing of sheepskin);\n(4) emulsifier in agricultural teat dips;\n(5) metal working except:\n— uses in controlled closed systems where the washing liquid is recycled or incinerated;\n(6) manufacturing of pulp and paper;\n(7) cosmetic products;\n(8) other personal care products except:\n— spermicides;\n(9) co-formulants in pesticides and biocides. However national authorisations for pesticides or biocidal products containing nonylphenol ethoxylates as co-formulant, granted before 17 July 2003, shall not be affected by this restriction until their date of expiry."},"Shall not be placed on the market, or used, as substances or in mixtures in concentrations equal to or greater than 0,1 % by weight for the following purposes:\n(1) industrial and institutional cleaning except:\n— controlled closed dry cleaning systems where the washing liquid is recycled or incinerated,\n— cleaning systems with special treatment where the washing liquid is recycled or incinerated.\n(2) domestic cleaning;\n(3) textiles and leather processing except:\n— processing with no release into waste water,\n— systems with special treatment where the process water is pre-treated to remove the organic fraction completely prior to biological waste water treatment (degreasing of sheepskin);\n(4) emulsifier in agricultural teat dips;\n(5) metal working except:\n— uses in controlled closed systems where the washing liquid is recycled or incinerated;\n(6) manufacturing of pulp and paper;\n(7) cosmetic products;\n(8) other personal care products except:\n— spermicides;\n(9) co-formulants in pesticides and biocides. However national authorisations for pesticides or biocidal products containing nonylphenol ethoxylates as co-formulant, granted before 17 July 2003, shall not be affected by this restriction until their date of expiry.","Darf für die folgenden Zwecke weder als Stoff noch in Gemischen in Konzentrationen von ≥ 0,1 Gew.-% oder mehr in Verkehr gebracht oder verwendet werden:\n1. gewerbliche Reinigung, ausgenommen:\no überwachte geschlossene Systeme für die chemische Reinigung, in denen die Reinigungsflüssigkeit recycelt oder verbrannt wird,\no Spezialreinigungssysteme, in denen die Reinigungsflüssigkeit recycelt oder verbrannt wird;\n2. Haushaltsreinigung;\n3. Textil- und Lederverarbeitung, ausgenommen:\no Behandlungen, bei denen kein NPE in das Abwasser gelangt,\no Anlagen für spezielle Behandlungen, bei denen die organische Fraktion vor der biologischen Abwasserbehandlung vollständig aus dem Prozesswasser entfernt wird (Entfetten von Schafshäuten);\n4. Emulgator in Melkfett;\n5. Metallverarbeitung, ausgenommen:\nAnwendungen in überwachten geschlossenen Systemen, bei denen die Reinigungsflüssigkeit recycelt oder verbrannt wird;\n6. Herstellung von Zellstoff und Papier;\n7. kosmetische Mittel;\n8. sonstige Körperpflegemittel, ausgenommen:\nSpermizide;\n9. Formulierungshilfsstoffe in Pestiziden und Bioziden. Zulassungen der Mitgliedstaaten für Pestizide oder Biozide, die Nonylphenolethoxylate als Formulierungshilfsstoffe enthalten, bleiben jedoch, wenn sie vor dem 17. Juni 2003 erteilt wurden, bis zu ihrem Auslaufen unberührt von dieser Einschränkung.","不得以下述目的投放市场或用作物质或制剂的成分，如果浓度大于等于0.1%：\n（1） 工业和公共机构用清洁剂，但下列除外：\n-受控的密闭干洗系统，其清洁剂将回收或焚烧处理；\n-特殊处理的清洗系统，其清洁剂将回收或焚烧处理；\n（2）家用清洗；\n（3）纺织品和皮革制品的处理，但下列除外：\n-不会排出废水的处理方式\n-特殊处理的系统，在该系统下，废水经过生物废水处理前，会先完全去除其中的有机成分（羊皮脱脂）；\n（4）农用喷洒药剂中的乳化剂\n（5）金属加工，但下列除外：\n-使用受控的密闭系统，其清洗液将回收或焚烧处理\n（6）纸浆和纸张的制造；\n（7）化妆品；\n（8）其他个人护理用品，但杀精剂除外；\n（9）杀虫剂或抗生素的配方。但是2003年6月17日之前国家授权的含有壬基酚聚氧乙烯醚作为配方助剂农药或生物农药产品，不受此限制，直至其过期为止。\n"]
[null,{"$f":"IF($B$1=\"English\",C1709,IF($B$1=\"Deutsch\",D1709,IF($B$1=\"中文\",E1709,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market after 3 February 2021 in textile articles which can reasonably be expected to be washed in water during their normal lifecycle, in concentrations equal to or greater than 0,01 % by weight of that textile article or of each part of the textile article.\n2. Paragraph 1 shall not apply to the placing on the market of second- hand textile articles or of new textile articles produced, without the use of NPE, exclusively from recycled textiles.\n3. For the purposes of paragraphs 1 and 2, “textile article” means any unfinished, semi-finished or finished product which is composed of at least 80 % textile fibres by weight, or any other product that contains a part which is composed of at least 80 % textile fibres by weight, including products such as clothing, accessories, interior textiles, fibres, yarn, fabrics and knitted panels.’"},"1. Shall not be placed on the market after 3 February 2021 in textile articles which can reasonably be expected to be washed in water during their normal lifecycle, in concentrations equal to or greater than 0,01 % by weight of that textile article or of each part of the textile article.\n2. Paragraph 1 shall not apply to the placing on the market of second- hand textile articles or of new textile articles produced, without the use of NPE, exclusively from recycled textiles.\n3. For the purposes of paragraphs 1 and 2, “textile article” means any unfinished, semi-finished or finished product which is composed of at least 80 % textile fibres by weight, or any other product that contains a part which is composed of at least 80 % textile fibres by weight, including products such as clothing, accessories, interior textiles, fibres, yarn, fabrics and knitted panels.’","1. Darf nach dem 3. Februar 2021 in Textilerzeugnissen, bei denen vernünftigerweise davon ausgegangen werden kann, dass sie während ihres normalen Lebenszyklus in Wasser gewaschen werden, in Konzentrationen von ≥ 0,01 Gew.-% dieses Textilerzeugnisses oder von Teilen davon nicht in Verkehr gebracht werden.\n2. Absatz 1 gilt nicht für das Inverkehrbringen von gebrauchten Textilerzeugnissen oder von neuen ausschließlich aus Recyclingtextilien ohne Verwendung von NPE hergestellten Textilerzeugnissen.\n3. Für die Zwecke der Absätze 1 und 2 wird ‚Textilerzeugnis‘ definiert als unfertiges Erzeugnis, Halbfertigerzeugnis und Fertigerzeugnis mit einem Gewichtsanteil an Textilfasern von mindestens 80 % sowie als jedes andere Erzeugnis, das in einem seiner Teile einen Gewichtsanteil an Textilfasern von mindestens 80 % aufweist, einschließlich Erzeugnisse wie Bekleidung, Accessoires, Heimtextilien, Fasern, Garn und Gewebe sowie Gestrickteile.\n\n","1.2021年2月3日以后，不得将可以合理预期在其正常生命周期中用水洗涤的纺织品以其等于或大于该纺织品或各部分重量的0.01％的浓度投放市场。\n2.第1项不适用于仅由再生纺织品在不使用NPE的情况下将二手纺织品或新生产的纺织品投放市场。\n3.就第1项和第2项而言，“纺织品”是指由至少80％重量的纺织纤维组成的任何未加工，半成品或成品，或任何其他包含以下组分的产品：至少80％的纺织纤维按重量计，包括诸如服装，配件，室内纺织品，纤维，纱线，织物和针织面板之类的产品。 "]
[null,{"$f":"IF($B$1=\"English\",C1710,IF($B$1=\"Deutsch\",D1710,IF($B$1=\"中文\",E1710,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Cement and cement-containing mixtures shall not be placed on the market, or used, if they contain, when hydrated, more than 2 mg/kg (0,0002%) soluble chromium VI of the total dry weight of the cement.\n2. If reducing agents are used, then without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of cement or cement-containing mixtures is visibly, legibly and indelibly marked with information on the packing date, as well as on the storage conditions and the storage period appropriate to maintaining the activity of the reducing agent and to keeping the content of soluble chromium VI below the limit indicated in paragraph 1.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the placing on the market for, and use in, controlled closed and totally automated processes in which cement and cement-containing mixtures are handled solely by machines and in which there is no possibility of contact with the skin.\n4. The standard adopted by the European Committee for Standardization (CEN) for testing the water-soluble chromium (VI) content of cement and cement-containing mixtures shall be used as the test method for demonstrating conformity with paragraph 1.\n5. Leather articles coming into contact with the skin shall not be placed on the market where they contain chromium VI in concentrations equal to or greater than 3 mg/kg (0,0003 % by weight) of the total dry weight of the leather.\n6. Articles containing leather parts coming into contact with the skin shall not be placed on the market where any of those leather parts contains chromium VI in concentrations equal to or greater than 3 mg/kg (0,0003 % by weight) of the total dry weight of that leather part.\n7. Paragraphs 5 and 6 shall not apply to the placing on the market of second-hand articles which were in end-use in the Union before 1 May 2015."},"1. Cement and cement-containing mixtures shall not be placed on the market, or used, if they contain, when hydrated, more than 2 mg/kg (0,0002%) soluble chromium VI of the total dry weight of the cement.\n2. If reducing agents are used, then without prejudice to the application of other Community provisions on the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that the packaging of cement or cement-containing mixtures is visibly, legibly and indelibly marked with information on the packing date, as well as on the storage conditions and the storage period appropriate to maintaining the activity of the reducing agent and to keeping the content of soluble chromium VI below the limit indicated in paragraph 1.\n3. By way of derogation, paragraphs 1 and 2 shall not apply to the placing on the market for, and use in, controlled closed and totally automated processes in which cement and cement-containing mixtures are handled solely by machines and in which there is no possibility of contact with the skin.\n4. The standard adopted by the European Committee for Standardization (CEN) for testing the water-soluble chromium (VI) content of cement and cement-containing mixtures shall be used as the test method for demonstrating conformity with paragraph 1.\n5. Leather articles coming into contact with the skin shall not be placed on the market where they contain chromium VI in concentrations equal to or greater than 3 mg/kg (0,0003 % by weight) of the total dry weight of the leather.\n6. Articles containing leather parts coming into contact with the skin shall not be placed on the market where any of those leather parts contains chromium VI in concentrations equal to or greater than 3 mg/kg (0,0003 % by weight) of the total dry weight of that leather part.\n7. Paragraphs 5 and 6 shall not apply to the placing on the market of second-hand articles which were in end-use in the Union before 1 May 2015.","1. Zement und zementhaltige Gemische dürfen nicht verwendet oder in Verkehr gebracht werden, wenn der Gehalt an löslichem Chrom VI in der Trockenmasse des Zements nach Hydratisierung mehr als 2 mg/kg (0,0002 %) beträgt.\n2. Werden Reduktionsmittel verwendet, so muss der Lieferant unbeschadet der Gültigkeit anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung,\nVerpackung und Kennzeichnung von Stoffen und Gemischen vor dem Inverkehrbringen gewährleisten, dass auf der Verpackung von Zement oder zementhaltigen Gemischen gut sichtbar, leserlich und unverwischbar angegeben ist, wann das Erzeugnis abgepackt wurde sowie unter welchen Bedingungen und wie lange es gelagert werden kann, ohne dass die Wirkung des Reduktionsmittels nachlässt und der Gehalt an löslichem Chrom VI den in Absatz 1 genannten Grenzwert überschreitet.\n3. Die Absätze 1 und 2 gelten jedoch nicht für das Inverkehrbringen im Hinblick auf überwachte geschlossene und vollautomatische Prozesse und auf die Verwendung in solchen Prozessen, bei denen Zement und zementhaltige Gemische ausschließlich mit Maschinen in Berührung kommen und keine Gefahr von Hautkontakt besteht.\n4. Die vom Europäischen Komitee für Normung (CEN) für die Prüfung des Gehalts an wasserlöslichem Chrom VI von Zement und zementhaltigen Gemischen verabschiedete Norm ist als das Verfahren zum Nachweis der Einhaltung von Absatz 1 einzusetzen.\n5. Ledererzeugnisse, die mit der Haut in Berührung kommen, dürfen nicht in Verkehr gebracht werden, wenn sie einen Chrom(VI)-Gehalt von 3 mg/kg (0,0003 Gewichtsprozent) oder mehr des gesamten Trockengewichts des Leders aufweisen.\n6. Erzeugnisse, die Lederteile enthalten, die mit der Haut in Berührung kommen, dürfen nicht in Verkehr gebracht werden, wenn sie einen Chrom(VI)-Gehalt von 3 mg/kg (0,0003 Gewichtsprozent) oder mehr des gesamten Trockengewichts des Leders aufweisen.\n7. Die Absätze 5 und 6 gelten nicht für das Inverkehrbringen von gebrauchten Erzeugnissen, die vor dem 1. Mai 2015 bereits in den Endverbrauch gelangt waren.","1.水泥和含水泥的制剂，如含有（水合时）的可溶性六价铬的含量超过水泥总干重的0.0002％，不得使用或投放到市场上。\n2.如果使用还原剂，在不违反委员会的其它关于物质和配制品分类、包装和标签法规的前提下，供应商必须保证水泥或含水泥配制品的包装上的标签清晰，可读和不可磨损，标明产品的包装日期、储存条件和适合的储存期，以维持还原剂的活性，并使可溶性六价铬的含量低于第1项中的限值。\n3.但是，上述第1项和第2项不适用于仅由机器操作，且无皮肤接触可能的封闭且完全自动化的系统。\n4.第1项的测试方法应符合欧洲标准化委员会（CEN）通过的测试水泥和含水泥的制剂中水溶性六价铬含量的标准。\n5.与皮肤接触的皮革制品，如果其六价铬含量等于或大于皮革总干重的3mg/kg（0,0003%（重量）），则不得投放市场。\n6.含有与皮肤接触的皮革部分的物品，如果其中任何皮革部分的六价铬含量等于或超过该皮革部分总干重的3mg/kg(0,0003 %)，则不得投放市场。\n7.第5项和第6项不适用于2015年5月1日前在欧盟最终使用的二手物品的上市。"]
[null,{"$f":"IF($B$1=\"English\",C1711,IF($B$1=\"Deutsch\",D1711,IF($B$1=\"中文\",E1711,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight where the substance or mixture is used in adhesives or spray paints intended for supply to the general public."},"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight where the substance or mixture is used in adhesives or spray paints intended for supply to the general public.","Darf nicht als Stoff oder in Gemischen in Konzentrationen von ≥ 0,1 Gew.-% in für die Abgabe an die breite Öffentlichkeit bestimmten Klebstoffen und Farbsprühdosen in Verkehr gebracht oder verwendet werden.","当向公众供应的粘合剂或喷漆中的浓度等于或高于0.1%（重量），不得作为物质或混合物投放市场或使用。"]
[null,{"$f":"IF($B$1=\"English\",C1712,IF($B$1=\"Deutsch\",D1712,IF($B$1=\"中文\",E1712,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight for any use except:\n— as an intermediate of synthesis, or, — as a process solvent in closed chemical applications for chlorination reactions, or,\n— in the manufacture of 1,3,5-triamino-2,4,6-trinitrobenzene (TATB)."},"Shall not be placed on the market, or used, as a substance or in mixtures in a concentration equal to or greater than 0,1 % by weight for any use except:\n— as an intermediate of synthesis, or, — as a process solvent in closed chemical applications for chlorination reactions, or,\n— in the manufacture of 1,3,5-triamino-2,4,6-trinitrobenzene (TATB).","Darf weder als Stoff noch in Gemischen in einer Konzentration von ≥ 0,1 Gew.-% zu keinem Verwendungszweck in Verkehr gebracht oder verwendet\nwerden, außer:\n• als Synthese-Zwischenprodukt,\n• als Prozesslösungsmittel in geschlossenen chemischen Anwendungen für Chlorreaktionen oder\n• bei der Herstellung von 1,3,5-Trinitro-2,4,6- Triaminobenzol (TATB).\n\n","不得投放市场或以浓度大于等于0.1%用作物质或制剂的成分的所有用途，除了以下项目：\n- 合成用的中间体；或\n- 进行密闭的氯化反应时的工艺用溶剂；或\n- 生产1,3,5-三胺基-2,4,6-三硝基苯（TATB）"]
[null,{"$f":"IF($B$1=\"English\",C1713,IF($B$1=\"Deutsch\",D1713,IF($B$1=\"中文\",E1713,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. From 1 January 2010, extender oils shall not be placed on the market, or used for the production of tyres or parts of tyres if they contain:\n— more than 1 mg/kg (0,0001 % by weight) BaP, or,\n— more than 10 mg/kg (0,001 % by weight) of the sum of all listed PAHs.\nThe standard EN 16143:2013 (Petroleum products — Determination of content of Benzo(a)pyrene (BaP) and selected polycyclic aromatic hydrocarbons (PAH) in extender oils — Procedure using double LC cleaning and GC/MS analysis) shall be used as the test method for demonstrating conformity with the limits referred to in the first subparagraph.\nUntil 23 September 2016, the limits referred to in the first subparagraph may be regarded as kept, if the polycyclic aromatics (PCA) extract is less than 3 % by weight as measured by the Institute of Petroleum standard IP 346:1998 (Determination of PCA in unused lubricating base oils and asphaltene free petroleum fractions — Dimethyl sulphoxide extraction refractive index method), provided that compliance with the limits of BaP and of the listed PAHs, as well as the correlation of the measured values with the PCA extract, is measured by the manufacturer or importer every six months or after each major operational change, whichever is earlier.\n2. Furthermore, tyres and treads for retreading manufactured after 1 January 2010 shall not be placed on the market if they contain extender oils exceeding the limits indicated in paragraph 1.\nThese limits shall be regarded as kept, if the vulcanised rubber compounds do not exceed the limit of 0,35 % Bay protons as measured and calculated by ISO 21461 (Rubber vulcanised — Determination of aromaticity of oil in vulcanised rubber compounds).\n3. By way of derogation, paragraph 2 shall not apply to retreaded tyres if their tread does not contain extender oils exceeding the limits referred to in paragraph 1.\n4. For the purpose of this entry ‘tyres’ shall mean tyres for vehicles covered by:\n— Directive 2007/46/EC of the European Parliament and of the Council of 5 September 2007 establishing a framework for the approval of motor vehicles and their trailers (*),\n— Directive 2003/37/EC of the European Parliament and of the Council of 26 May 2003 on type-approval of agricultural or forestry tractors, their trailers and interchangeable towed machinery, together with their systems, components and separate technical units (**), and\n— Directive 2002/24/EC of the European Parliament and of the Council of 18 March 2002 relating to the type-approval of two or three-wheel motor vehicles and repealing Council Directive 92/61/EEC (***).\n5. Articles shall not be placed on the market for supply to the general public, if any of their rubber or plastic components that come into direct as well as prolonged or short-term repetitive contact with the human skin or the oral cavity, under normal or reasonably foreseeable conditions of use, contain more than 1 mg/kg (0,0001 % by weight of this component) of any of the listed PAHs.\nSuch articles include amongst others:\n— sport equipment such as bicycles, golf clubs, racquets\n— household utensils, trolleys, walking frames\n— tools for domestic use\n— clothing, footwear, gloves and sportswear\n— watch-straps, wrist-bands, masks, head-bands\n6. Toys, including activity toys, and childcare articles, shall not be placed on the market, if any of their rubber or plastic components that come into direct as well as prolonged or short-term repetitive contact with the human skin or the oral cavity, under normal or reasonably foreseeable conditions of use, contain more than 0,5 mg/kg (0,00005 % by weight of this component) of any of the listed PAHs.\n7. By way of derogation from paragraphs 5 and 6, these paragraphs shall not apply to articles placed on the market for the first time before 27 December 2015.\n8. By 27 December 2017, the Commission shall review the limit values in paragraphs 5 and 6 in the light of new scientific information, including migration of PAHs from the articles referred to therein, and information on alternative raw materials and, if appropriate, modify these paragraphs accordingly.\n______________\n(*) OJ L 263, 9.10.2007, p. 1.\n(**) OJ L 171, 9.7.2003, p. 1.\n(***) OJ L 124, 9.5.2002, p. 1."},"1. From 1 January 2010, extender oils shall not be placed on the market, or used for the production of tyres or parts of tyres if they contain:\n— more than 1 mg/kg (0,0001 % by weight) BaP, or,\n— more than 10 mg/kg (0,001 % by weight) of the sum of all listed PAHs.\nThe standard EN 16143:2013 (Petroleum products — Determination of content of Benzo(a)pyrene (BaP) and selected polycyclic aromatic hydrocarbons (PAH) in extender oils — Procedure using double LC cleaning and GC/MS analysis) shall be used as the test method for demonstrating conformity with the limits referred to in the first subparagraph.\nUntil 23 September 2016, the limits referred to in the first subparagraph may be regarded as kept, if the polycyclic aromatics (PCA) extract is less than 3 % by weight as measured by the Institute of Petroleum standard IP 346:1998 (Determination of PCA in unused lubricating base oils and asphaltene free petroleum fractions — Dimethyl sulphoxide extraction refractive index method), provided that compliance with the limits of BaP and of the listed PAHs, as well as the correlation of the measured values with the PCA extract, is measured by the manufacturer or importer every six months or after each major operational change, whichever is earlier.\n2. Furthermore, tyres and treads for retreading manufactured after 1 January 2010 shall not be placed on the market if they contain extender oils exceeding the limits indicated in paragraph 1.\nThese limits shall be regarded as kept, if the vulcanised rubber compounds do not exceed the limit of 0,35 % Bay protons as measured and calculated by ISO 21461 (Rubber vulcanised — Determination of aromaticity of oil in vulcanised rubber compounds).\n3. By way of derogation, paragraph 2 shall not apply to retreaded tyres if their tread does not contain extender oils exceeding the limits referred to in paragraph 1.\n4. For the purpose of this entry ‘tyres’ shall mean tyres for vehicles covered by:\n— Directive 2007/46/EC of the European Parliament and of the Council of 5 September 2007 establishing a framework for the approval of motor vehicles and their trailers (*),\n— Directive 2003/37/EC of the European Parliament and of the Council of 26 May 2003 on type-approval of agricultural or forestry tractors, their trailers and interchangeable towed machinery, together with their systems, components and separate technical units (**), and\n— Directive 2002/24/EC of the European Parliament and of the Council of 18 March 2002 relating to the type-approval of two or three-wheel motor vehicles and repealing Council Directive 92/61/EEC (***).\n5. Articles shall not be placed on the market for supply to the general public, if any of their rubber or plastic components that come into direct as well as prolonged or short-term repetitive contact with the human skin or the oral cavity, under normal or reasonably foreseeable conditions of use, contain more than 1 mg/kg (0,0001 % by weight of this component) of any of the listed PAHs.\nSuch articles include amongst others:\n— sport equipment such as bicycles, golf clubs, racquets\n— household utensils, trolleys, walking frames\n— tools for domestic use\n— clothing, footwear, gloves and sportswear\n— watch-straps, wrist-bands, masks, head-bands\n6. Toys, including activity toys, and childcare articles, shall not be placed on the market, if any of their rubber or plastic components that come into direct as well as prolonged or short-term repetitive contact with the human skin or the oral cavity, under normal or reasonably foreseeable conditions of use, contain more than 0,5 mg/kg (0,00005 % by weight of this component) of any of the listed PAHs.\n7. By way of derogation from paragraphs 5 and 6, these paragraphs shall not apply to articles placed on the market for the first time before 27 December 2015.\n8. By 27 December 2017, the Commission shall review the limit values in paragraphs 5 and 6 in the light of new scientific information, including migration of PAHs from the articles referred to therein, and information on alternative raw materials and, if appropriate, modify these paragraphs accordingly.\n______________\n(*) OJ L 263, 9.10.2007, p. 1.\n(**) OJ L 171, 9.7.2003, p. 1.\n(***) OJ L 124, 9.5.2002, p. 1.","1. Ab dem 1. Januar 2010 dürfen Weichmacheröle nicht für die Herstellung von Reifen oder Reifenbestandteilen in Verkehr gebracht oder verwendet werden, wenn\no sie mehr als 1 mg/kg (0,0001 Gew.-%) BaP enthalten oder\no der Gehalt aller aufgeführten PAK zusammen mehr als 10 mg/kg (0,001 Gew.-%) beträgt.\nDie Norm EN 16143:2013 (Mineralölerzeugnisse - Bestimmung des Gehaltes an Benzo[a]pyren (BaP) und ausgewählten polyzyklischen aromatischen Kohlenwasserstoffen (PAKs) in Extenderölen — Verfahren mittels doppelter LC-Vorreinigung und GC/MS-Analyse) ist als Prüfmethode für den Nachweis der Einhaltung der in Unterabsatz 1 genannten Grenzwerte zu verwenden.\nBis 23. September 2016 gelten die in Unterabsatz 1 genannten Grenzwerte als eingehalten, wenn der Extrakt an polyzyklischen aromatischen Verbindungen weniger als 3 Gew.-% beträgt — gemessen gemäß der Norm IP 346:1998 des Institute of Petroleum (Bestimmung der polyzyklischen aromatischen Verbindungen in unbenutzten Schmierölen und asphaltenfreien Erdölfraktionen — Dimethylsulfoxid-Extraktion-Brechungsindex-Methode) —, sofern die Einhaltung der Grenzwerte für BaP und für die aufgeführten PAK sowie die Korrelation der Messwerte mit dem Extrakt an polyzyklischen aromatischen Verbindungen vom Hersteller oder Importeur alle sechs Monate oder nach jeder größeren Änderung der Betriebsverfahren durch Messung überprüft werden, wobei jeweils der frühere Zeitpunkt maßgeblich ist.\n2. Außerdem dürfen nach dem 1. Januar 2010 hergestellte Reifen und Profile für die Runderneuerung nicht in Verkehr gebracht werden, wenn sie Weichmacheröle enthalten, die die in Absatz 1 angegebenen Grenzwerte überschreiten.\nDiese Grenzwerte gelten als eingehalten, wenn die vulkanisierte Gummimasse den Grenzwert von 0,35 % HBay — gemessen und berechnet gemäß der ISO-Norm 21461 (Vulkanisierter Gummi — Bestimmung der Aromatizität von Öl in vulkanisierter Gummimasse) — nicht überschreitet.\n3. Ausgenommen von Absatz 2 sind runderneuerte Reifen, wenn ihr Profil keine Weichmacheröle enthält, die die in Absatz 1 angegebenen Grenzwerte überschreiten.\n4. „Reifen“ im Sinne dieses Eintrags sind Reifen für Fahrzeuge, die unter folgende Richtlinien fallen:\no Richtlinie 2007/46/EG des Europäischen Parlaments und des Rates vom 5. September 2007 zur Schaffung eines Rahmens für die Genehmigung von Kraftfahrzeugen und Kraftfahrzeuganhängern (****);\no Richtlinie 2003/37/EG des Europäischen Parlaments und des Rates vom 26. Mai 2003 über die Typgenehmigung für land- oder forstwirtschaftliche\nZugmaschinen, ihre Anhänger und die von ihnen gezogenen auswechselbaren Maschinen sowie für Systeme, Bauteile und selbstständige technische Einheiten dieser Fahrzeuge (*****) und\no Richtlinie 2002/24/EG des Europäischen Parlaments und des Rates vom 18. März 2002 über die Typgenehmigung für zweirädrige oder dreirädrige Kraftfahrzeuge und zur Aufhebung der Richtlinie 92/61/EWG des Rates (******).\n5. Erzeugnisse dürfen nicht für die allgemeine Öffentlichkeit in Verkehr gebracht werden, wenn einer ihrer Bestandteile aus Kunststoff oder Gummi, der bei normaler oder vernünftigerweise vorhersehbarer Verwendung unmittelbar, länger oder wiederholt für kurze Zeit mit der menschlichen Haut oder der Mundhöhle in Berührung kommt, mehr als 1 mg/kg (0,0001 Massenprozent w/w dieses Bestandteils) eines der aufgeführten PAK enthält. Zu diesen Erzeugnissen zählen unter anderem:\n— Sportgeräte wie Fahrräder, Golfschläger, Schläger,\n— Haushaltsgeräte, mit Rädern versehene Wagen, Laufhilfen,\n— Werkzeuge für den privaten Gebrauch,\n— Bekleidung, Schuhe, Handschuhe und Sportkleidung,\n— Uhrenarmbänder, Armbänder, Masken, Stirnbänder.\n6. Spielzeug, einschließlich Aktivitätsspielzeug, und Artikel für Säuglinge und Kleinkinder werden nicht in Verkehr gebracht, wenn einer ihrer Bestandteile aus Kunststoff oder Gummi, der bei normaler oder vernünftigerweise vorhersehbarer Verwendung unmittelbar, länger oder wiederholt für kurze Zeit mit der menschlichen Haut oder der Mundhöhle in Berührung kommt, mehr als 0,5 mg/kg (0,00005 Massenprozent w/w dieses Bestandteils) eines der aufgeführten PAK enthält.\n7. Davon abweichend gelten die Absätze 5 und 6 nicht für Erzeugnisse, die vor dem 27. Dezember 2015 erstmals in Verkehr gebracht wurden.\n8. Bis zum 27. Dezember 2017 überprüft die Kommission die Grenzwerte gemäß den Absätzen 5 und 6 im Lichte neuer wissenschaftlicher Erkenntnisse, auch über die Migration von PAK aus den darin genannten Erzeugnissen, sowie über alternative Rohstoffe und ändert diese Absätze gegebenenfalls entsprechend.\n______________\n(****) ABl. L 263 vom 9.10.2007, S. 1.\n(*****) ABl. L 171 vom 9.7.2003, S. 1.\n(******) ABl. L 124 vom 9.5.2002, S. 1.","1.自2010年1月1日起，增塑剂油不得投放市场或用于制造轮胎或轮胎组件，如果它们含有\n-超过1 mg / kg（0.0001％重量）的BaP或\n-所有列出的多环芳烃的含量合计超过10毫克/千克（0.001％重量）。\n标准EN 16143：2013（矿物油产品，增量油中苯并[a]（（BaP）和选定的多环芳烃（PAHs）的含量测定，采用双LC预清洗和GC / MS分析的方法）应被用作证明符合第一项所述限值的测试方法。\n直到2016年9月23日，如果多环芳族化合物的提取物重量少于3％，则认为符合第1项规定的限值-根据研究所的IP 346：1998标准石油的测定（未使用的润滑油和不含沥青质的石油馏分中多环芳族化合物的测定-二甲基亚砜萃取折光率法）-但制造商或进口商必须每六个月或在每次重大操作变更后（以较早者为准）测量BaP和所列多环芳烃的限值是否符合规定，以及测量值与五环芳烃提取物的关联性。\n2.此外，2010年1月1日之后制造的轮胎和胎面翻新轮胎，如果其所含的增塑剂油超过第1项规定的极限值，则不得投放市场。\n如果硫化橡胶混合物不超过0.35％HBay极限值，则认为符合这些极限值-根据ISO标准21461（硫化橡胶-硫化橡胶混合物中油的芳香性测定）进行测量和计算）。\n3.如果翻新轮胎的胎面不含任何超过第1项规定的极限值的软化油，则从第2项中排除。\n4.在本文中，“轮胎”是指应遵循以下准则的车辆轮胎：\n-2007年9月5日欧洲议会和理事会关于建立批准机动车及其挂车的框架的第2007/46 / EC号指令（****）；\n-欧洲议会和理事会于2003年5月26日发布的关于农业或林业应用类型批准的指令2003/37 / EC，关于农业或林业拖拉机、其拖车和可互换的牵引机械，以及其系统、部件和独立的技术单元的类型认证(**)，以及\n-2002年3月18日欧洲议会和理事会的指令2002/24 / EC，有关两轮或三轮机动车的型式批准，并废除了理事会指令92/61 / EEC（******） 。\n5.如果物品的任何塑料或橡胶成分在正常或合理可预见的使用下直接，长期或反复短期与人的皮肤或口腔接触，而所列的多环芳烃之一超过1毫克/千克（0.0001质量％w / w，该组分），则不得将其投放市场。这些产品包括：\n-运动器材，例如自行车，高尔夫俱乐部，俱乐部，\n-家用电器，带轮手推车，助行器，\n-私人使用的工具，\n-服装，鞋子，手套和运动服，\n-手表皮带，手镯，口罩，头巾。\n6.如果玩具，包括活动玩具以及婴幼儿用品，如果其塑料或橡胶成分中的任何一种在正常或合理可预见的使用下被直接，长时间或反复短期使用，则不得投放市场。人体皮肤或口腔接触，含有超过0.5 mg / kg（该组分的0.00005质量％w / w）的所列PAH之一。\n7.尽管如此，第5项和第6项不适用于2015年12月27日之前首次投放市场的产品。\n8.在2017年12月27日之前，委员会应根据新的科学信息，包括其中提及的物品中多环芳烃的迁移，以及关于替代原料的信息，审查第5和第6项中的限值，并酌情对这些条款进行相应的修改。\n______________\n(*) OJ L 263, 9.10.2007, p. 1.\n(**) OJ L 171, 9.7.2003, p. 1.\n(***) OJ L 124, 9.5.2002, p. 1."]
[null,{"$f":"IF($B$1=\"English\",C1714,IF($B$1=\"Deutsch\",D1714,IF($B$1=\"中文\",E1714,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used as substances or in mixtures, individually or in any combination of the phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material, in toys and childcare articles.\n2. Shall not be placed on the market in toys or childcare articles, individually or in any combination of the first three phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material.\nIn addition, DIBP shall not be placed on the market after 7 July 2020 in toys or childcare articles, individually or in any combination with the first three phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material.\n3. Shall not be placed on the market after 7 July 2020 in articles, individually or in any combination of the phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material in the article.\n4. Paragraph 3 shall not apply to:\n(a) articles exclusively for industrial or agricultural use, or for use exclusively in the open air, provided that no plasticised material comes into contact with human mucous membranes or into prolonged contact with human skin;\n(b) aircraft, placed on the market before 7 January 2024, or articles, whenever placed on the market, for use exclusively in the maintenance or repair of those aircraft, where those articles are essential for the safety and airworthiness of the aircraft;\n(c) motor vehicles within the scope of Directive 2007/46/EC, placed on the market before 7 January 2024, or articles, whenever placed on the market, for use exclusively in the maintenance or repair of those vehicles, where the vehicles cannot function as intended without those articles;\n(d) articles placed on the market before 7 July 2020;\n(e) measuring devices for laboratory use, or parts thereof;\n(f) materials and articles intended to come into contact with food within the scope of Regulation (EC) No 1935/2004 or Commission Regulation (EU) No 10/2011 (*);\n(g) medical devices within the scope of Directives 90/385/EEC, 93/42/EEC or 98/79/EC, or parts thereof;\n(h) electrical and electronic equipment within the scope of Directive 2011/65/EU;\n(i) the immediate packaging of medicinal products within the scope of Regulation (EC) No 726/2004, Directive 2001/82/EC or Directive 2001/83/EC;\n(j) toys and childcare articles covered by paragraphs 1 or 2.\n5. For the purposes of paragraphs 1, 2, 3 and 4(a),\n(a) ‘plasticised material’ means any of the following homogeneous materials:\n- polyvinyl chloride (PVC), polyvinylidene chloride (PVDC),polyvinyl acetate (PVA), polyurethanes,\n- any other polymer (including, inter alia, polymer foams and rubber material) except silicone rubber and natural latex coatings,\n- surface coatings, non-slip coatings, finishes, decals, printed designs,\n- adhesives, sealants, paints and inks.\n(b) ‘prolonged contact with human skin’ means continuous contact of more than 10 minutes duration or intermittent contact over a period of 30 minutes, per day.\n(c) ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.\n6. For the purposes of paragraph 4(b), ‘aircraft’ means one of the following:\n(a) a civil aircraft produced in accordance with a type certificate issued under Regulation (EC) No 216/2008 or with a design approval issued under the national regulations of a contracting State of the International Civil Aviation Organisation (ICAO), or for which a certificate of airworthiness has been issued by an ICAO contracting State under Annex 8 to the Convention on International Civil Aviation, signed on December 7, 1944 , in Chicago;\n(b) a military aircraft.\n\n----------------------------\n(*) Commission Regulation (EU) No 10/2011 of 14 January 2011 on plastic materials and articles intended to come into contact with food (OJ L 12, 15.1.2011, p. 1)."},"1. Shall not be used as substances or in mixtures, individually or in any combination of the phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material, in toys and childcare articles.\n2. Shall not be placed on the market in toys or childcare articles, individually or in any combination of the first three phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material.\nIn addition, DIBP shall not be placed on the market after 7 July 2020 in toys or childcare articles, individually or in any combination with the first three phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material.\n3. Shall not be placed on the market after 7 July 2020 in articles, individually or in any combination of the phthalates listed in column 1 of this entry, in a concentration equal to or greater than 0,1 % by weight of the plasticised material in the article.\n4. Paragraph 3 shall not apply to:\n(a) articles exclusively for industrial or agricultural use, or for use exclusively in the open air, provided that no plasticised material comes into contact with human mucous membranes or into prolonged contact with human skin;\n(b) aircraft, placed on the market before 7 January 2024, or articles, whenever placed on the market, for use exclusively in the maintenance or repair of those aircraft, where those articles are essential for the safety and airworthiness of the aircraft;\n(c) motor vehicles within the scope of Directive 2007/46/EC, placed on the market before 7 January 2024, or articles, whenever placed on the market, for use exclusively in the maintenance or repair of those vehicles, where the vehicles cannot function as intended without those articles;\n(d) articles placed on the market before 7 July 2020;\n(e) measuring devices for laboratory use, or parts thereof;\n(f) materials and articles intended to come into contact with food within the scope of Regulation (EC) No 1935/2004 or Commission Regulation (EU) No 10/2011 (*);\n(g) medical devices within the scope of Directives 90/385/EEC, 93/42/EEC or 98/79/EC, or parts thereof;\n(h) electrical and electronic equipment within the scope of Directive 2011/65/EU;\n(i) the immediate packaging of medicinal products within the scope of Regulation (EC) No 726/2004, Directive 2001/82/EC or Directive 2001/83/EC;\n(j) toys and childcare articles covered by paragraphs 1 or 2.\n5. For the purposes of paragraphs 1, 2, 3 and 4(a),\n(a) ‘plasticised material’ means any of the following homogeneous materials:\n- polyvinyl chloride (PVC), polyvinylidene chloride (PVDC),polyvinyl acetate (PVA), polyurethanes,\n- any other polymer (including, inter alia, polymer foams and rubber material) except silicone rubber and natural latex coatings,\n- surface coatings, non-slip coatings, finishes, decals, printed designs,\n- adhesives, sealants, paints and inks.\n(b) ‘prolonged contact with human skin’ means continuous contact of more than 10 minutes duration or intermittent contact over a period of 30 minutes, per day.\n(c) ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.\n6. For the purposes of paragraph 4(b), ‘aircraft’ means one of the following:\n(a) a civil aircraft produced in accordance with a type certificate issued under Regulation (EC) No 216/2008 or with a design approval issued under the national regulations of a contracting State of the International Civil Aviation Organisation (ICAO), or for which a certificate of airworthiness has been issued by an ICAO contracting State under Annex 8 to the Convention on International Civil Aviation, signed on December 7, 1944 , in Chicago;\n(b) a military aircraft.\n\n----------------------------\n(*) Commission Regulation (EU) No 10/2011 of 14 January 2011 on plastic materials and articles intended to come into contact with food (OJ L 12, 15.1.2011, p. 1).","1. Dürfen nicht als Stoffe oder in Gemischen einzeln oder in einer Kombination der in Spalte 1 aufgeführten Phthalate verwendet werden, wenn diese Konzentration mindestens 0,1 Gewichtsprozent des weichmacherhaltigen Materials in Spielzeug und Babyartikeln entspricht.\n2. Dürfen nicht in Spielzeug und Babyartikeln auf den Markt gebracht werden, wenn die Konzentration eines der in Spalte 1 aufgeführten Phthalate oder einer Kombination daraus mindestens 0,1 Gewichtsprozent des weichmacherhaltigen Materials ausmacht.\nFerner darf DIPB nach dem 7. Juli 2020 nicht in Spielzeug und Babyartikeln in Verkehr gebracht werden, wenn die Konzentration eines oder mehrerer der in Spalte 1 dieses Eintrags aufgeführten Phthalate mindestens 0,1 Gewichtsprozent des weichmacherhaltigen Materials ausmacht.\n3. Dürfen nach dem 7. Juli 2020 nicht in Erzeugnissen in Verkehr gebracht werden, wenn die Konzentration eines oder einer Kombination mehrerer der in Spalte 1 aufgeführten Phthalate mindestens 0,1 Gewichtsprozent eines im Erzeugnis enthaltenen weichmacherhaltigen Materials ausmacht.\n4. Absatz 3 gilt nicht für\na) Erzeugnisse, die ausschließlich für die industrielle oder landwirtschaftliche Verwendung oder für die Verwendung im Freien bestimmt sind, sofern kein weichmacherhaltiges Material mit menschlichen Schleimhäuten oder für längere Zeit mit der menschlichen Haut in Berührung kommt;\nb) Luftfahrzeuge, die vor dem 7. Januar 2024 in Verkehr gebracht wurden, oder Erzeugnisse — unabhängig vom Zeitpunkt des Inverkehrbringens —, die ausschließlich für die Wartung und Reparatur dieser Luftfahrzeuge bestimmt sind, wenn diese Erzeugnisse für die Sicherheit und Lufttüchtigkeit des Luftfahrzeugs unverzichtbar sind:\nc) Kraftfahrzeuge, die in den Geltungsbereich der Richtlinie 2007/46/EG fallen und vor dem 7. Januar 2024 in Verkehr gebracht wurden, oder Erzeugnisse, die ausschließlich für die Wartung und Reparatur dieser Kraftfahrzeuge verwendet werden, unabhängig davon, wann sie in den Verkehr gebracht wurden, wenn die Kraftfahrzeuge ihre beabsichtigte Funktion ohne diese Erzeugnisse nicht erfüllen können;\nd) Erzeugnisse, die vor dem 7. Juli 2020 in Verkehr gebracht wurden;\ne) Messgeräte für den Laborgebrauch oder Teile davon;\nf) Materialien und Gegenstände, die dazu bestimmt sind, mit Lebensmitteln in Berührung zu kommen und in den Anwendungsbereich der Verordnung (EG) Nr. 1935/2004 oder der Verordnung (EU) Nr. 10/2011 der Kommission (*1) fallen;\ng) medizinische Geräte, die in den Anwendungsbereich der Richtlinien 90/385/EWG, 93/42/EWG oder 98/79/EG fallen und Teile davon;\nh) Elektro- und Elektronikgeräten, die in den Anwendungsbereich der Richtlinie 2011/65/EU fallen.\ni) Primärverpackungen von Arzneimitteln, die in den Anwendungsbereich der Verordnung (EG) Nr. 726/2004, der Richtlinie 2001/82/EG oder der Richtlinie 2001/83/EG fallen;\nj) Spielzeug und Babyartikel, die unter die Absätze 1 oder 2 fallen.\n5. Für die Zwecke der Absätze 1, 2, 3 und 4 Buchstabe a gelten folgende Begriffsbestimmungen:\na) ‚weichmacherhaltiges Material‘ bezeichnet alle folgenden homogenen Materialien:\n-Polyvinylchlorid (PVC), Polyvinylidenchlorid (PVDC), Polyvinylacetat (PVA), Polyurethane\n-und alle anderen Polymere (unter anderem Polymerschaum und Kautschuk) außer Silikonkautschuk und natürliche Latexbeschichtungen,\n-Oberflächenbeschichtungen, rutschhemmende Beschichtungen, Verkleidungen, Klebeschichten, aufgedruckte Muster,\n-Kleber, Dichtungsmassen, Tinten und Farben;\nb) ‚für längere Zeit mit den menschlichen Haut in Berührung kommen‘ bezeichnet einen dauerhaften Kontakt von 10 Minuten oder wiederholte Berührungen über einen Zeitraum von 30 Minuten pro Tag;\nc) ‚Babyartikel‘ bezeichnet jedes Erzeugnis, das dazu bestimmt ist, den Schlaf, die Entspannung, die Hygiene, das Füttern und das Saugen von Kindern zu erleichtern.\n6. ‚Luftfahrzeug‘ bezeichnet für die Zwecke des Absatzes 4 Buchstabe b Folgendes:\na) ein ziviles Luftfahrzeug, das entsprechend einer nach der Verordnung (EU) Nr. 216/2008 ausgestellten Musterzulassung oder einer nach den nationalen Vorschriften eines Vertragsstaats der Internationalen Zivilluftfahrtorganisation ICAO erteilten Konstruktionsgenehmigung produziert worden ist, oder für das ein Lufttüchtigkeitszeugnis von einem ICAO-Vertragsstaat nach Anhang 8 des am 7. Dezember 1944 in Chicago unterzeichneten Abkommens über die internationale Zivilluftfahrt ausgestellt worden ist;\nb) ein Militärluftfahrzeug\n(*1) Verordnung (EU) Nr. 10/2011 der Kommission vom 14. Januar 2011 über Materialien und Gegenstände aus Kunststoff, die dazu bestimmt sind, mit Lebensmitteln in Berührung zu kommen (ABl. L 12 vom 15.1.2011, S. 1).\n\n","1.当浓度等于或大于塑化材料的0.1％的重量，不得作为物质或混合物，单独或以本条目第1项所列邻苯二甲酸盐的任何组合，在玩具和儿童护理用品中使用。\n2.当浓度等于或高于塑化材料重量的0.1%，不得在玩具或儿童护理用品中单独或与本条目第1项所列的前三种邻苯二甲酸盐的任何组合投放市场。\n此外，2020年7月7日之后，当浓度等于或高于塑化材料重量的0.1%，DIBP不得单独或与本条目第1项所列前三种邻苯二甲酸盐的任何组合投放市场。\n3.当浓度等于或高于该物品中塑化材料的0.1%，不得在2020年7月7日之后在物品中单独或与本条目第1项所列邻苯二甲酸盐的任何组合投放市场。\n4. 第3项不适用于以下情况\n(a)专门用于工业或农业的物品，或专门在户外使用的物品，条件是塑化材料不与人体粘膜接触或与人体皮肤长时间接触。\n(b)2024年1月7日前投放市场的飞机，或无论何时投放市场的、专门用于维护或修理这些飞机的物品，而这些物品对飞机的安全和适航性至关重要。\n(c)在2024年1月7日之前投放市场的第2007/46/EC号指令范围内的机动车，或在任何时候投放市场的专门用于维护或修理这些车辆的物品，若没有这些物品，这些车辆就无法正常运行。\n(d) 2020年7月7日前投放市场的物品。\n(e) 用于实验室的测量装置，或其部件。\n(f)(EC)第1935/2004号条例或(EU)第10/2011号委员会条例(*)范围内的拟与食品接触的材料和物品。\n(g) 第90/385/EEC、93/42/EEC或98/79/EC号指令范围内的医疗设备，或其组成部分。\n(h) 第2011/65/EU号指令范围内的电气和电子设备。\n(i)(EC)第726/2004号条例、第2001/82/EC号指令或第2001/83/EC号指令范围内的医药产品的直接包装。\n(j) 第1项或第2项所涉及的玩具和儿童护理用品。\n5. 就第1、2、3和4(a)款而言。\n(a) '塑化材料'是指以下任何一种均质材料。\n- 聚氯乙烯（PVC），聚偏二氯乙烯（PVDC），聚醋酸乙烯（PVA），聚氨酯。\n-任何其他聚合物（除其他外，包括聚合物泡沫和橡胶材料），但硅橡胶和天然乳胶涂料除外。\n- 表面涂层、防滑涂层、饰面、贴花、印刷设计。\n- 粘合剂、密封剂、油漆和油墨。\n(b) '与人体皮肤的长时间接触'是指每天持续10分钟以上的接触或30分钟内的间歇性接触。\n(c) '儿童护理用品'指任何旨在促进睡眠、放松、卫生、喂养儿童或儿童吸吮的产品。\n6. 就第4(b)段而言，'飞机'是指下列之一。\n(a) 根据(EC)216/2008号条例颁发的型号证书或根据国际民用航空组织(ICAO)缔约国的国家法规颁发的设计批准书生产的民用飞机，或根据1944年12月7日在芝加哥签署的《国际民用航空公约》附件8由ICAO缔约国颁发的适航证书。\n(b) 一架军用飞机。\n\n----------------------------\n(*) 2011年1月14日欧盟委员会条例（EU）第10/2011号，关于拟与食品接触的塑料材料和物品（OJ L 12, 15.1.2011, p. 1）。"]
[null,{"$f":"IF($B$1=\"English\",C1715,IF($B$1=\"Deutsch\",D1715,IF($B$1=\"中文\",E1715,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles which can be placed in the mouth by children.\n2. Such toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n(3. Regulation (EU) No 326/2015: paragraph 3 is deleted.)\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children."},"1. Shall not be used as substances or in mixtures, in concentrations greater than 0,1 % by weight of the plasticised material, in toys and childcare articles which can be placed in the mouth by children.\n2. Such toys and childcare articles containing these phthalates in a concentration greater than 0,1 % by weight of the plasticised material shall not be placed on the market.\n(3. Regulation (EU) No 326/2015: paragraph 3 is deleted.)\n4. For the purpose of this entry ‘childcare article’ shall mean any product intended to facilitate sleep, relaxation, hygiene, the feeding of children or sucking on the part of children.","1. Dürfen nicht als Stoffe oder in Gemischen in Konzentrationen von mehr als 0,1 Gew.-% des weichmacherhaltigen Materials in Spielzeug und Babyartikeln verwendet werden, die von Kindern in den Mund genommen werden können.\n2. Solche Spielzeuge und Babyartikel, die diese Phthalate in Konzentrationen von mehr als 0,1 Gew.-% des weichmacherhaltigen Materials enthalten, dürfen nicht in Verkehr gebracht werden.\n3. wegefallen\n4. Für die Zwecke dieses Eintrags bezeichnet der Begriff „Babyartikel“ jedes Erzeugnis, das dazu bestimmt ist, den Schlaf, die Entspannung, die Hygiene, das Füttern und das Saugen von Kindern zu erleichtern.","1.不得用作纯物质或用于玩具和儿童用品中，在塑性材料中重量百分比浓度不大于0.1%。\n2.玩具和儿童用品，如果使用了含邻苯二甲酸盐的浓度大于0.1％的塑性材料料，不得投放市场。\n(3. (欧盟)第326/2015号条例：第3段被删除。)\n4.对于这个项目，“儿童用品”，是指帮助促进睡眠，放松，卫生护理，喂养或吸吮的产品。"]
[null,{"$f":"IF($B$1=\"English\",C1716,IF($B$1=\"Deutsch\",D1716,IF($B$1=\"中文\",E1716,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market after 27 June 2010, for supply to the general public, as a constituent of paints, paint strippers, cleaning agents, self-shining emulsions or floor sealants in concentrations equal to or greater than 0,1 % by weight."},"Shall not be placed on the market after 27 June 2010, for supply to the general public, as a constituent of paints, paint strippers, cleaning agents, self-shining emulsions or floor sealants in concentrations equal to or greater than 0,1 % by weight.","Darf nach dem 27. Juni 2010 nicht zur Abgabe an die breite Öffentlichkeit in Farben, Abbeizmitteln, Reinigungsmitteln, selbstglänzenden Emulsionen oder Fußbodenversiegelungsmitteln in einer Konzentration von ≥ 0,1 Gew.-% in Verkehr gebracht werden.","作为油漆、油漆去除剂、清洁剂、自发光乳液或地板密封剂的组分，重量百分比大于等于0.1%的，  2010-06-27日起不得投放市场销售给公众。"]
[null,{"$f":"IF($B$1=\"English\",C1717,IF($B$1=\"Deutsch\",D1717,IF($B$1=\"中文\",E1717,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of spray paints or spray cleaners in aerosol dispensers in concentrations equal to or greater than 3 % by weight.\n2. Spray paints and spray cleaners in aerosol dispensers containing DEGBE and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that paints other than spray paints containing DEGBE in concentrations equal to or greater than 3 % by weight of that are placed on the market for supply to the general public are visibly, legibly and indelibly marked by 27 December 2010 as follows:\n‘Do not use in paint spraying equipment’."},"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of spray paints or spray cleaners in aerosol dispensers in concentrations equal to or greater than 3 % by weight.\n2. Spray paints and spray cleaners in aerosol dispensers containing DEGBE and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that paints other than spray paints containing DEGBE in concentrations equal to or greater than 3 % by weight of that are placed on the market for supply to the general public are visibly, legibly and indelibly marked by 27 December 2010 as follows:\n‘Do not use in paint spraying equipment’.","1. Darf nach dem 27. Juni 2010 nicht zur Abgabe an die breite Öffentlichkeit in Spritzfarben oder Reinigungssprays in Aerosolpackungen in einer\nKonzentration von ≥ 3 Gew.-% erstmalig in Verkehr gebracht werden.\n2. Nach dem 27. Dezember 2010 dürfen DEGBE-haltige Spritzfarben und Reinigungssprays in Aerosolpackungen, die den Anforderungen unter Absatz 1 nicht entsprechen, nicht mehr zur Abgabe an die breite Öffentlichkeit in Verkehr gebracht werden.\n3. Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften über die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte DEGBE-haltige Farben, die nicht zum Verspritzen bestimmt sind, in einer Konzentration von 3 Gew.- % oder mehr ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n„Darf nicht in Farbspritzausrüstung verwendet werden“.\n\n","1.作为喷漆或喷雾清洁剂的组分在气溶胶喷罐中的浓度质量百分比大于3%时，不得在2010年6月27日以后首次投放市场销售给普通公众。\n2.喷漆或喷雾清洁剂如含DEGBE并且不符合本条第1款的规定，2010年12月27日后不得投放市场销售给普通公众。\n3.不影响其它关于物质和配制品的分类、包装和标签等方面的公共规定，供应商应在投放市场之前确保，销售给普通公众的涂料（除喷漆外）若含DEGBE质量百分比大于等于3%，从2010年12月27日起其包装上应该清晰易见且永久的标记有以下文字：“不得在涂料喷涂设备中使用”"]
[null,{"$f":"IF($B$1=\"English\",C1718,IF($B$1=\"Deutsch\",D1718,IF($B$1=\"中文\",E1718,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market after 27 December 2010, as a constituent of mixtures in concentrations equal to or greater than 0,1 % by weight of MDI for supply to the general public, unless suppliers shall ensure before the placing on the market that the packaging:\n(a) contains protective gloves which comply with the requirements of Council Directive 89/686/EEC (*);\n(b) is marked visibly, legibly and indelibly as follows, and without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures:\n‘— Persons already sensitised to diisocyanates may develop allergic reactions when using this product.\n— Persons suffering from asthma, eczema or skin problems should avoid contact,\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nincluding dermal contact, with this product.\n— This product should not be used under conditions of poor ventilation unless a protective mask with an appropriate gas filter (i.e. type A1 according to standard EN 14387) is used.’\n2. By way of derogation, paragraph 1(a) shall not apply to hot melt adhesives.\n______________\n(*) OJ L 399, 30.12.1989, p. 18."},"1. Shall not be placed on the market after 27 December 2010, as a constituent of mixtures in concentrations equal to or greater than 0,1 % by weight of MDI for supply to the general public, unless suppliers shall ensure before the placing on the market that the packaging:\n(a) contains protective gloves which comply with the requirements of Council Directive 89/686/EEC (*);\n(b) is marked visibly, legibly and indelibly as follows, and without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures:\n‘— Persons already sensitised to diisocyanates may develop allergic reactions when using this product.\n— Persons suffering from asthma, eczema or skin problems should avoid contact,\nAnnankatu 18, P.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | Fax +358 9 68618210 | echa.europa.eu\nincluding dermal contact, with this product.\n— This product should not be used under conditions of poor ventilation unless a protective mask with an appropriate gas filter (i.e. type A1 according to standard EN 14387) is used.’\n2. By way of derogation, paragraph 1(a) shall not apply to hot melt adhesives.\n______________\n(*) OJ L 399, 30.12.1989, p. 18.","1. Darf nach dem 27. Dezember 2010 nicht zur Abgabe an die breite Öffentlichkeit in Gemischen, die diesen Stoff in einer Konzentration von ≥ 0,1 Gew.-% MDI enthalten, in Verkehr gebracht werden; es sei denn, der Lieferant gewährleistet vor dem Inverkehrbringen, dass die Verpackung\na) Schutzhandschuhe enthält, die den Anforderungen der Richtlinie 89/686/EWG des Rates entsprechen (*******);\nb) unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen ist:\n„— Bei Personen, die bereits für Diisocyanate sensibilisiert sind, kann der Umgang mit diesem Produkt allergische Reaktionen auslösen.\n— Bei Asthma, ekzematösen Hauterkrankungen oder Hautproblemen Kontakt, einschließlich Hautkontakt, mit dem Produkt vermeiden.\n— Das Produkt nicht bei ungenügender Lüftung verwenden oder Schutzmaske mit entsprechendem Gasfilter (Typ A1 nach EN 14387) tragen.“\n2. Absatz 1 Buchstabe a gilt nicht für Heißklebstoffe.\n______________\n(*******) ABl. L 399 vom 30.12.1989, S. 18.\n\n","1.配制品中含有二苯基甲烷二异氰酸酯(MDI)的重量百分比大于等于0,1%的，2010年12月27日之后不得投放市场供应给普通大众，除非供应商投放市场之前应确保：\na)包装中附有符合委员会指令89/686/EEC要求的防护手套\nb)在不违背理事会其他关于物质和配制品分类、标签和包装法规的前提下，包装上应使用清晰、明显、永久性标识标记如下：\n-对二异氰酸酯很敏感的人在使用本产品时，会引起过敏反应。\n-有哮喘，湿疹或皮肤问题的人应避免接触该产品，包括皮肤接触。\n-不要在通风不足的情况下使用该产品，除非佩戴含有气体过滤器的防护面罩（根据标准EN14387，A1型）。\n2. 作为豁免条款，1(a)不适用于热熔粘合剂。\n______________\n(*) OJ L 399, 30.12.1989, p. 18."]
[null,{"$f":"IF($B$1=\"English\",C1719,IF($B$1=\"Deutsch\",D1719,IF($B$1=\"中文\",E1719,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of neoprene-based contact adhesives in concentrations equal to or greater than 0,1 % by weight in package sizes greater than 350 g.\n2. Neoprene-based contact adhesives containing cyclohexane and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that neoprene-based contact adhesives containing cyclohexane in concentrations equal to or greater than 0,1 % by weight that are placed on the market for supply to the general public after 27 December 2010 are visibly, legibly and indelibly marked as follows:\n‘— This product is not to be used under conditions of poor ventilation.\n— This product is not to be used for carpet laying.’."},"1. Shall not be placed on the market for the first time after 27 June 2010, for supply to the general public, as a constituent of neoprene-based contact adhesives in concentrations equal to or greater than 0,1 % by weight in package sizes greater than 350 g.\n2. Neoprene-based contact adhesives containing cyclohexane and not conforming to paragraph 1 shall not be placed on the market for supply to the general public after 27 December 2010.\n3. Without prejudice to other Community legislation concerning the classification, packaging and labelling of substances and mixtures, suppliers shall ensure before the placing on the market that neoprene-based contact adhesives containing cyclohexane in concentrations equal to or greater than 0,1 % by weight that are placed on the market for supply to the general public after 27 December 2010 are visibly, legibly and indelibly marked as follows:\n‘— This product is not to be used under conditions of poor ventilation.\n— This product is not to be used for carpet laying.’.","1. Darf nach dem 27. Juni 2010 zur Abgabe an die breite Öffentlichkeit in Kontaktklebstoffen auf Neoprenbasis nicht in einer Konzentration von ≥ 0,1 Gew.-% in Packungsgrößen von mehr als 350 g erstmalig in Verkehr gebracht werden.\n2. Cyclohexanhaltige Kontaktklebstoffe auf Neoprenbasis, die den Anforderungen unter Absatz 1 nicht entsprechen, dürfen nach dem 27. Dezember 2010 nicht mehr zur Abgabe an die breite Öffentlichkeit in Verkehr gebracht werden.\n3. Unbeschadet anderer gemeinschaftlicher Rechtsvorschriften für die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen muss der Lieferant vor dem Inverkehrbringen gewährleisten, dass zur Abgabe an die breite Öffentlichkeit in Verkehr gebrachte Kontaktklebstoffe auf Neoprenbasis, die Cyclohexan in einer Konzentration von 0,1 Gew.-% oder mehr enthalten, ab dem 27. Dezember 2010 gut sichtbar, leserlich und unverwischbar mit folgender Aufschrift versehen sind:\n„— Dieses Produkt darf nicht bei ungenügender Lüftung verarbeitet werden.\n— Dieses Produkt darf nicht zum Verlegen von Teppichböden verwendet werden.“\n\n","1.作为氯丁橡胶接触粘合剂的成分，其浓度大于等于0.1%（重量百分比）销售包装超过350克，不得投放市场销售给普通大众。\n2.含有环己烷的氯丁橡胶接触粘合剂，如不符合本条第1款的规定，2010年12月27日之后不得投放市场销售给普通大众。\n3.如2010年12月27日之后销售该物质浓度大于等于0.1%的含有环己烷的氯丁橡胶接触粘合剂，在不违反委员会的其它关于物质和配制品分类、包装和标签法规的前提下，供应商必须保证粘合剂以不可磨损的方式，标记以下文字：\n—此产品不得在通风不良时使用。 \n—该产品不能用于地毯铺设。"]
[null,{"$f":"IF($B$1=\"English\",C1720,IF($B$1=\"Deutsch\",D1720,IF($B$1=\"中文\",E1720,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall not be:\n(a) placed on the market for the first time for supply to the general public or to professionals after 6 December 2010;\n(b) placed on the market for supply to the general public or to professionals after 6 December 2011;\n(c) used by professionals after 6 June 2012.\nFor the purposes of this entry:\n(i) ‘professional’ means any natural or legal person, including workers and self-employed workers undertaking paint stripping in the course of their professional activity outside an industrial installation;\n(ii) ‘industrial installation’ means a facility used for paint stripping activities.\n2. By way of derogation from paragraph 1, Member States may allow on their territories and for certain activities the use, by specifically trained professionals, of paint strippers containing dichloromethane and may allow the placing on the market of such paint strippers for supply to those professionals.\nMember States making use of this derogation shall define appropriate provisions for the protection of the health and safety of those professionals using paint strippers containing dichloromethane and shall inform the Commission thereof.\nThose provisions shall include a requirement that a professional shall hold a certificate that is accepted by the Member State in which that professional operates, or provide other documentary evidence to that effect, or be otherwise approved by that Member State, so as to demonstrate proper training and competence to safely use paint strippers containing dichloromethane.\nThe Commission shall prepare a list of the Member States which have made use of the derogation in this paragraph and make it publicly available over the Internet.\n\n3. A professional benefiting from the derogation referred to in paragraph 2 shall operate only in Member States which have made use of that derogation. The training referred to in paragraph 2 shall cover as a minimum:\n(a) awareness, evaluation and management of risks to health, including information on existing substitutes or processes, which under their conditions of use are less hazardous to the health and safety of workers;\n(b) use of adequate ventilation;\n(c) use of appropriate personal protective equipment that complies with Directive 89/686/EEC.\nEmployers and self-employed workers shall preferably replace dichloromethane with a chemical agent or process which, under its conditions of use, presents no risk, or a lower risk, to the health and safety of workers.\nProfessional shall apply all relevant safety measures in practice, including the use of personal protective equipment.\n4. Without prejudice to other Community legislation on workers protection, paint strippers containing dichloromethane in concentrations equal to or greater than 0,1 % by weight may be used in industrial installations only if the following minimum conditions are met:\n(a) effective ventilation in all processing areas, in particular for the wet processing and the drying of stripped articles: local exhaust ventilation at strip tanks supplemented by forced ventilation in those areas, so as to minimise exposure and to ensure compliance, where technically feasible, with relevant occupational exposure limits;\n(b) measures to minimise evaporation from strip tanks comprising: lids for covering strip tanks except during loading and unloading; suitable loading and unloading arrangements for strip tanks; and wash tanks with water or brine to remove excess solvent after unloading;\n(c) measures for the safe handling of dichloromethane in strip tanks comprising: pumps and pipework for transferring paint stripper to and from strip tanks; and suitable arrangements for safe cleaning of tanks and removal of sludge;\n(d) personal protective equipment that complies with Directive 89/686/EEC comprising: suitable protective gloves, safety goggles and protective clothing; and appropriate respiratory protective equipment where compliance with relevant occupational exposure limits cannot be otherwise achieved;\n(e) adequate information, instruction and training for operators in the use of such equipment.\n5. Without prejudice to other Community provisions concerning the classification, labelling and packaging of substances and mixtures, by 6 December 2011 paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall be visibly, legibly and indelibly marked as follows:\n‘Restricted to industrial use and to professionals approved in certain EU Member States — verify where use is allowed.’"},"1. Paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall not be:\n(a) placed on the market for the first time for supply to the general public or to professionals after 6 December 2010;\n(b) placed on the market for supply to the general public or to professionals after 6 December 2011;\n(c) used by professionals after 6 June 2012.\nFor the purposes of this entry:\n(i) ‘professional’ means any natural or legal person, including workers and self-employed workers undertaking paint stripping in the course of their professional activity outside an industrial installation;\n(ii) ‘industrial installation’ means a facility used for paint stripping activities.\n2. By way of derogation from paragraph 1, Member States may allow on their territories and for certain activities the use, by specifically trained professionals, of paint strippers containing dichloromethane and may allow the placing on the market of such paint strippers for supply to those professionals.\nMember States making use of this derogation shall define appropriate provisions for the protection of the health and safety of those professionals using paint strippers containing dichloromethane and shall inform the Commission thereof.\nThose provisions shall include a requirement that a professional shall hold a certificate that is accepted by the Member State in which that professional operates, or provide other documentary evidence to that effect, or be otherwise approved by that Member State, so as to demonstrate proper training and competence to safely use paint strippers containing dichloromethane.\nThe Commission shall prepare a list of the Member States which have made use of the derogation in this paragraph and make it publicly available over the Internet.\n\n3. A professional benefiting from the derogation referred to in paragraph 2 shall operate only in Member States which have made use of that derogation. The training referred to in paragraph 2 shall cover as a minimum:\n(a) awareness, evaluation and management of risks to health, including information on existing substitutes or processes, which under their conditions of use are less hazardous to the health and safety of workers;\n(b) use of adequate ventilation;\n(c) use of appropriate personal protective equipment that complies with Directive 89/686/EEC.\nEmployers and self-employed workers shall preferably replace dichloromethane with a chemical agent or process which, under its conditions of use, presents no risk, or a lower risk, to the health and safety of workers.\nProfessional shall apply all relevant safety measures in practice, including the use of personal protective equipment.\n4. Without prejudice to other Community legislation on workers protection, paint strippers containing dichloromethane in concentrations equal to or greater than 0,1 % by weight may be used in industrial installations only if the following minimum conditions are met:\n(a) effective ventilation in all processing areas, in particular for the wet processing and the drying of stripped articles: local exhaust ventilation at strip tanks supplemented by forced ventilation in those areas, so as to minimise exposure and to ensure compliance, where technically feasible, with relevant occupational exposure limits;\n(b) measures to minimise evaporation from strip tanks comprising: lids for covering strip tanks except during loading and unloading; suitable loading and unloading arrangements for strip tanks; and wash tanks with water or brine to remove excess solvent after unloading;\n(c) measures for the safe handling of dichloromethane in strip tanks comprising: pumps and pipework for transferring paint stripper to and from strip tanks; and suitable arrangements for safe cleaning of tanks and removal of sludge;\n(d) personal protective equipment that complies with Directive 89/686/EEC comprising: suitable protective gloves, safety goggles and protective clothing; and appropriate respiratory protective equipment where compliance with relevant occupational exposure limits cannot be otherwise achieved;\n(e) adequate information, instruction and training for operators in the use of such equipment.\n5. Without prejudice to other Community provisions concerning the classification, labelling and packaging of substances and mixtures, by 6 December 2011 paint strippers containing dichloromethane in a concentration equal to or greater than 0,1 % by weight shall be visibly, legibly and indelibly marked as follows:\n‘Restricted to industrial use and to professionals approved in certain EU Member States — verify where use is allowed.’","1. Farbabbeizer, die Dichlormethan (DCM) in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, dürfen\na) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2010 nicht mehr erstmalig in Verkehr gebracht werden;\nb) zur Abgabe an die breite Öffentlichkeit oder gewerbliche Verwender nach dem 6. Dezember 2011 nicht mehr in Verkehr gebracht werden;\nc) nach dem 6. Juni 2012 nicht mehr von gewerblichen Verwendern benutzt werden.\nFür die Zwecke dieses Eintrags bezeichnet der Ausdruck\ni) „gewerblicher Verwender“ eine natürliche oder juristische Person, einschließlich Angestellte und Selbstständige, die im Zuge ihrer beruflichen Tätigkeit außerhalb einer Industrieanlage Abbeizarbeiten durchführt;\nii) „Industrieanlage“ eine Anlage, die zum Abbeizen von Farbe genutzt wird.\n2. Abweichend von Absatz 1 können die Mitgliedstaaten in ihren Hoheitsgebieten für bestimmte Tätigkeiten die Verwendung von DCM-haltigen Farbabbeizern durch speziell geschulte gewerbliche Verwender und das Inverkehrbringen solcher Farbabbeizer zur Abgabe an diese gewerblichen Verwender gestatten.\nMitgliedstaaten, die von dieser Ausnahmeregelung Gebrauch machen, legen angemessene Bestimmungen zur Gewährleistung des Gesundheitsschutzes und der Sicherheit für gewerbliche Verwender fest, die DCM-haltige Farbabbeizer verwenden, und unterrichten die Kommission darüber.\nDiese Bestimmungen enthalten die Anforderung, dass ein gewerblicher Verwender über einen Sachkundenachweis verfügen muss, der in dem Mitgliedstaat, in dem er tätig ist, anerkannt wird, oder andere diesbezügliche Nachweisdokumente vorlegen oder eine anderweitige Zulassung desselben Mitgliedstaats besitzen muss, damit nachgewiesen werden kann, dass der gewerbliche Verwender im Umgang mit DCM-haltigen Farbabbeizern ordnungsgemäß geschult wurde und qualifiziert ist, sicher mit ihnen umzugehen.\nDie Kommission erstellt ein Verzeichnis der Mitgliedstaaten, die von der in diesem Absatz genannten Ausnahmeregelung Gebrauch machen, und veröffentlicht dieses Verzeichnis im Internet.\n3. Ein gewerblicher Verwender, der von der in Absatz 2 genannten Ausnahmeregelung Gebrauch macht, darf nur in Mitgliedstaaten tätig werden, die diese Ausnahmeregelung anwenden. Die in Absatz 2 genannte Schulung muss mindestens folgende Bereiche abdecken:\na) Kenntnis, Bewertung und Beherrschung der Gesundheitsrisiken, einschließlich Unterrichtung über bestehende Ersatzstoffe oder Verfahren, die unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender weniger gefährlich sind;\nb) Verwendung ausreichender Belüftung;\nc) Verwendung geeigneter persönlichen Schutzausrüstungen gemäß der Richtlinie 89/686/EWG.\nArbeitgeber und Selbstständige ersetzen DCM vorrangig durch einen chemischen Arbeitsstoff oder ein Verfahren, der bzw. das unter den jeweiligen Verwendungsbedingungen für die Gesundheit und Sicherheit der Verwender nicht oder weniger gefährlich ist.\nDer gewerbliche Verwender setzt alle einschlägigen Sicherheitsmaßnahmen in die Praxis um, einschließlich der Verwendung einer persönlichen Schutzausrüstung.\n4. Unbeschadet anderer Arbeitnehmerschutzvorschriften der Gemeinschaft dürfen Farbabbeizer, die DCM in einer Konzentration von 0,1 Gewichtsprozent\noder mehr enthalten, in Industrieanlagen nur verwendet werden, wenn mindestens folgende Bedingungen erfüllt sind:\na) wirksame Belüftung in allen Arbeitsräumen, insbesondere bei der Nassbehandlung und der Trocknung abgebeizter Gegenstände: lokale Absauganlagen\nan Abbeizbehältnissen, die durch Zwangsbelüftungsanlagen in diesen Bereichen ergänzt werden, um die Exposition zu minimieren und die maßgeblichen Arbeitsplatzgrenzwerte, soweit technisch möglich, einzuhalten;\nb) Maßnahmen zur weitestgehenden Verringerung der Verdampfung aus Abbeizbehältnissen, die Folgendes umfassen: Abdeckungen für Abbeizbehältnisse,\naußer bei der Beladung und Entladung; angemessene Vorkehrungen für die Beladung und Entladung der Abbeizbehältnisse; Reinigungsbehälter, mit Wasser oder Lauge gefüllt, um nach der Entladung das überschüssige Lösemittel vom Abbeizgut zu entfernen;\nc) Maßnahmen für die sichere Handhabung von DCM enthaltenden Abbeizbehältnissen, die Folgendes umfassen: Pumpen und Rohrleitungen für die Überleitung des Abbeizmittels aus den und in die Behältnisse; angemessene Vorkehrungen für die sichere Reinigung der Behältnisse und die Beseitigung von Schlämmen;\nd) persönliche Schutzausrüstungen gemäß der Richtlinie 89/686/EWG, die Folgendes umfassen: geeignete Schutzhandschuhe, Schutzbrillen und Schutzkleidung; geeignete Atemschutzgeräte, für den Fall, dass die Arbeitsplatzgrenzwerte nicht anderweitig eingehalten werden können;\ne) angemessene Informationen, Anweisungen und Übungen zur Verwendung solcher Ausrüstungsgegenstände für die Verwender.\n5. Unbeschadet anderer gemeinschaftlicher Bestimmungen für die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen müssen\nFarbabbeizer, die Dichlormethan in einer Konzentration von 0,1 Gewichtsprozent oder mehr enthalten, ab dem 6. Dezember 2011 gut sichtbar, leserlich\nund unverwischbar mit folgender Aufschrift versehen sein:\n„Nur für die industrielle Verwendung und für gewerbliche Verwender, die über eine Zulassung in bestimmten EU-Mitgliedstaaten verfügen. Überprüfen\nSie, in welchem Mitgliedstaat die Verwendung genehmigt ist.“","1.二氯甲烷（DCM）含量大于等于0.1（重量百分比）的脱漆剂，不得： (a)在2010年12月6日以后将不再有新产品首次投放市场，销售给普通大众或专业用户；\n(b)在2011年12月6日以后将不再投放市场，销售给广大市民或专业用户；\n(c)在2012年12月6以后，专业用户也不得使用。\n以下是关于这条款的一些注释：\n(i)“专业用户”是指自然人或法人，包括雇员及个体经营人士，他们不是在工业装置上进行脱漆作业；\n(ii)“工业装置”是指用于脱漆的设备。\n2.作为第1款的豁免条款，成员国可以允许在他们国家范围内，在由经过专门培训的专业人员从事的某些特定的工作中使用含DCM脱漆剂；也允许将这类脱漆剂投放市场销售给专业人员。\n各成员国在应用这一豁免时，应同时制定法规，以确保专业人员使用含DCM的脱漆剂时的健康与安全，并通知委员会。 \n这些规定包括专业用户必须持有成员国认可的能力证书，或提交其他有关有效的证明文件，以证明专业人员用户已经过适当的培训，有能力安全地使用含DCM的脱漆剂。\n委员会应准备一份应用该豁免的成员国名单，并公布在互联网上\n3.专业人员只能在应用该豁免的成员国内参考第2段应用该豁免。第2段中提及的培训应该至少包括：\n(a)告知健康风险，如何评估和管理风险，包括现有的替代产品，以及能够降低对员工健康和安全危害的工艺；\n(b) 充分通风换气；\n(c) 使用合适的符合89/686/EEC指令的个人防护用品。\n雇员或个体劳动者应优先考虑用对员工健康和安全无风险或者低风险的化学品或者工艺替代DCM。\n专业人员在操作时应确保所有的安全措施，包括个人防护用品。\n4.在不违反其它劳动保护法规的前提下，含DCM浓度重量百分比大于等于0.1%的脱漆剂，只有在符合以下条件下，可以用在工业装置中：\n(a)在所有加工区域，尤其是湿式加工和脱机物品烘干区域，确保有效通风：所有上述区域的强制通风外加脱漆槽的局部排风，以尽可能减少曝露。\n(b)采取措施尽可能减少脱漆剂挥发，包括：除了上下料，其它时间脱漆槽必须加盖；妥善安排脱漆槽的上下料过程；下料后，用水或盐水清洗脱漆槽，除去多余的溶剂\n(c)采取措施安全处理脱漆槽中的DCM，包括：转移脱漆剂进入、排出脱漆槽的泵和管路（防止泄露）；清理脱漆槽和去除污泥时合理安排\n(d)符合89/686/EEC指令的劳动防护用品，包括：合适的防护手套，安全眼镜，防护服；如果采取措施也不能够符合相关的职业危害曝露限值的话，还需要采用合时的呼吸保护设备。\n(e)为使用该设备的员工提供充分的信息，培训和指导。\n5．在不违背理事会其他关于物质和配制品分类、标签和包装法规的前提下，在2011年12月6日之后，含DCM质量百分比大于等于0.1%的脱漆剂应使用清晰、明显、永久性标识标记如下：‘仅限于在特定的欧盟成员国内用于工业用途或仅供专业人士使用 – 请核实是否允许使用’。"]
[null,{"$f":"IF($B$1=\"English\",C1721,IF($B$1=\"Deutsch\",D1721,IF($B$1=\"中文\",E1721,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market or used as a substance or constituent of mixtures in a concentration, equal to or greater than 0,1 % by weight for grouting applications after 5 November 2012."},"Shall not be placed on the market or used as a substance or constituent of mixtures in a concentration, equal to or greater than 0,1 % by weight for grouting applications after 5 November 2012.","Darf nach dem 5. November 2012 weder als Stoff noch in Gemischen in Konzentrationen von ≥ 0,1 Gew.-% für Abdichtungsanwendungen wie beispielsweise\nInjektion, Verpressung, Verfugung oder Verguss in Verkehr gebracht oder verwendet werden.","当物质或制剂中该成分浓度大于等于0.1%，在2012年11月5日之后不得投放市场或者用于注浆"]
[null,{"$f":"IF($B$1=\"English\",C1722,IF($B$1=\"Deutsch\",D1722,IF($B$1=\"中文\",E1722,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be used in articles or any parts thereof in concentrations greater than 0,1 mg/kg.\nArticles or any parts thereof containing DMF in concentrations greater than 0,1 mg/kg shall not be placed on the market."},"Shall not be used in articles or any parts thereof in concentrations greater than 0,1 mg/kg.\nArticles or any parts thereof containing DMF in concentrations greater than 0,1 mg/kg shall not be placed on the market.","Darf nicht in Erzeugnissen oder Bestandteilen davon in Konzentrationen von über 0,1 mg/kg verwendet werden.\n\nErzeugnisse oder deren Bestandteile, die DMF in einer Konzentration von über 0,1 mg/kg enthalten, dürfen nicht in den Verkehr gebracht werden.","在任何物品或者部件中含量不得超过0,1mg/kg。\n\nDMF的含量超过0,1mg/kg的任何产品或部件，不得投放市场."]
[null,{"$f":"IF($B$1=\"English\",C1723,IF($B$1=\"Deutsch\",D1723,IF($B$1=\"中文\",E1723,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be manufactured, placed on the market or used as substances or in mixtures after 10 October 2017 if the concentration of mercury in the mixtures is equal to or greater than 0,01 % by weight.\n\n2. Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight."},"1. Shall not be manufactured, placed on the market or used as substances or in mixtures after 10 October 2017 if the concentration of mercury in the mixtures is equal to or greater than 0,01 % by weight.\n\n2. Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight.","1. Darf nach dem 10. Oktober 2017 weder als Stoff noch in Gemischen hergestellt, in Verkehr gebracht oder verwendet werden, wenn die Quecksilberkonzentration in den Gemischen 0,01 Gewichtsprozent beträgt oder übersteigt.\n2. Erzeugnisse oder deren Bestandteile, die einen oder mehrere dieser Stoffe enthalten, dürfen nach dem 10. Oktober 2017 nicht in Verkehr gebracht werden, wenn die Quecksilberkonzentration in den Erzeugnissen bzw. deren Bestandteilen 0,01 Gewichtsprozent beträgt oder übersteigt.\n\n","1.当汞在配制品中浓度大于等于0.01％（重量），在2017年10月10日后不得生产或者投放市场。\n2.当产品或其组件中汞的浓度大于等于0.01％（重量），该产品获组件在2017年10月10日之后不得投放市场"]
[null,{"$f":"IF($B$1=\"English\",C1724,IF($B$1=\"Deutsch\",D1724,IF($B$1=\"中文\",E1724,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market or used in any individual part of jewellery articles if the concentration of lead (expressed as metal) in such a part is equal to or greater than 0,05 % by weight.\n2. For the purposes of paragraph 1:\n(i) ‘jewellery articles’ shall include jewellery and imitation jewellery articles and hair accessories, including:\n(a) bracelets, necklaces and rings;\n(b) piercing jewellery;\n(c) wrist watches and wrist-wear;\n(d) brooches and cufflinks;\n(ii) ‘any individual part’ shall include the materials from which the jewellery is made, as well as the individual components of the jewellery articles.\n3. Paragraph 1 shall also apply to individual parts when placed on the market or used for jewellery-making.\n4. By way of derogation, paragraph 1 shall not apply to:\n(a) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Council Directive 69/493/EEC (*);\n(b) internal components of watch timepieces inaccessible to consumers;\n(c) non-synthetic or reconstructed precious and semiprecious stones (CN code 7103, as established by Regulation (EEC) No 2658/87), unless they have been treated with lead or its compounds or mixtures containing these substances;\n(d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of minerals melted at a temperature of at least 500 °C.\n\n5. By way of derogation, paragraph 1 shall not apply to jewellery articles placed on the market for the first time before 9 October 2013 and jewellery articles produced before 10 December 1961.\n6. By 9 October 2017, the Commission shall re-evaluate this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 1 and, if appropriate, modify this entry accordingly.\n7. Shall not be placed on the market or used in articles supplied to the general public, if the concentration of lead (expressed as metal) in those articles or accessible parts thereof is equal to or greater than 0,05 % by weight, and those articles or accessible parts thereof may, during normal or reasonably foreseeable conditions of use, be placed in the mouth by children.\nThat limit shall not apply where it can be demonstrated that the rate of lead release from such an article or any such accessible part of an article, whether coated or uncoated, does not exceed 0,05 μg/cm² per hour (equivalent to 0,05 μg/g/h), and, for coated articles, that the coating is sufficient to ensure that this release rate is not exceeded for a period of at least two years of normal or reasonably foreseeable conditions of use of the article.\nFor the purposes of this paragraph, it is considered that an article or accessible part of an article may be placed in the mouth by children if it is smaller than 5 cm in one dimension or has a detachable or protruding part of that size.\n8. By way of derogation, paragraph 7 shall not apply to:\n(a) jewellery articles covered by paragraph 1;\n(b) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Directive 69/493/ EEC;\n(c) non-synthetic or reconstructed precious and semi-precious stones (CN code 7103 as established by Regulation (EEC) No 2658/ 87) unless they have been treated with lead or its compounds or mixtures containing these substances;\n(d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of mineral melted at a temperature of at least 500 ° C;\n(e) keys and locks, including padlocks;\n(f) musical instruments;\n(g) articles and parts of articles comprising brass alloys, if the concentration of lead (expressed as metal) in the brass alloy does not exceed 0,5 % by weight;\n(h) the tips of writing instruments;\n(i) religious articles;\n(j) portable zinc-carbon batteries and button cell batteries;\n(k) articles within the scope of:\n(i) Directive 94/62/EC;\n(ii) Regulation (EC) No 1935/2004;\n(iii) Directive 2009/48/EC of the European Parliament and of the Council (**);\n(iv) Directive 2011/65/EU of the European Parliament and of the Council (***)\n9. By 1 July 2019, the Commission shall re-evaluate paragraphs 7 and 8(e), (f), (i) and (j) of this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 7, including the requirement on coating integrity, and, if appropriate, modify this entry accordingly.\n10. By way of derogation paragraph 7 shall not apply to articles placed on the market for the first time before 1 June 2016.\n______________\n(*) OJ L 326, 29.12.1969, p. 36.\n(**) Directive 2009/48/EC of the European Parliament and of the Council of 18 June 2009 on the safety of toys (OJ L 170, 30.6.2009, p. 1).\n(***) Directive 2011/65/EU of the European Parliament and of the Council of 8 June 2011 on the restriction of the use of certain hazardous substances in electrical and electronic equipment (OJ L 174, 1.7.2011, p. 88)."},"1. Shall not be placed on the market or used in any individual part of jewellery articles if the concentration of lead (expressed as metal) in such a part is equal to or greater than 0,05 % by weight.\n2. For the purposes of paragraph 1:\n(i) ‘jewellery articles’ shall include jewellery and imitation jewellery articles and hair accessories, including:\n(a) bracelets, necklaces and rings;\n(b) piercing jewellery;\n(c) wrist watches and wrist-wear;\n(d) brooches and cufflinks;\n(ii) ‘any individual part’ shall include the materials from which the jewellery is made, as well as the individual components of the jewellery articles.\n3. Paragraph 1 shall also apply to individual parts when placed on the market or used for jewellery-making.\n4. By way of derogation, paragraph 1 shall not apply to:\n(a) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Council Directive 69/493/EEC (*);\n(b) internal components of watch timepieces inaccessible to consumers;\n(c) non-synthetic or reconstructed precious and semiprecious stones (CN code 7103, as established by Regulation (EEC) No 2658/87), unless they have been treated with lead or its compounds or mixtures containing these substances;\n(d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of minerals melted at a temperature of at least 500 °C.\n\n5. By way of derogation, paragraph 1 shall not apply to jewellery articles placed on the market for the first time before 9 October 2013 and jewellery articles produced before 10 December 1961.\n6. By 9 October 2017, the Commission shall re-evaluate this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 1 and, if appropriate, modify this entry accordingly.\n7. Shall not be placed on the market or used in articles supplied to the general public, if the concentration of lead (expressed as metal) in those articles or accessible parts thereof is equal to or greater than 0,05 % by weight, and those articles or accessible parts thereof may, during normal or reasonably foreseeable conditions of use, be placed in the mouth by children.\nThat limit shall not apply where it can be demonstrated that the rate of lead release from such an article or any such accessible part of an article, whether coated or uncoated, does not exceed 0,05 μg/cm² per hour (equivalent to 0,05 μg/g/h), and, for coated articles, that the coating is sufficient to ensure that this release rate is not exceeded for a period of at least two years of normal or reasonably foreseeable conditions of use of the article.\nFor the purposes of this paragraph, it is considered that an article or accessible part of an article may be placed in the mouth by children if it is smaller than 5 cm in one dimension or has a detachable or protruding part of that size.\n8. By way of derogation, paragraph 7 shall not apply to:\n(a) jewellery articles covered by paragraph 1;\n(b) crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Directive 69/493/ EEC;\n(c) non-synthetic or reconstructed precious and semi-precious stones (CN code 7103 as established by Regulation (EEC) No 2658/ 87) unless they have been treated with lead or its compounds or mixtures containing these substances;\n(d) enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of mineral melted at a temperature of at least 500 ° C;\n(e) keys and locks, including padlocks;\n(f) musical instruments;\n(g) articles and parts of articles comprising brass alloys, if the concentration of lead (expressed as metal) in the brass alloy does not exceed 0,5 % by weight;\n(h) the tips of writing instruments;\n(i) religious articles;\n(j) portable zinc-carbon batteries and button cell batteries;\n(k) articles within the scope of:\n(i) Directive 94/62/EC;\n(ii) Regulation (EC) No 1935/2004;\n(iii) Directive 2009/48/EC of the European Parliament and of the Council (**);\n(iv) Directive 2011/65/EU of the European Parliament and of the Council (***)\n9. By 1 July 2019, the Commission shall re-evaluate paragraphs 7 and 8(e), (f), (i) and (j) of this entry in the light of new scientific information, including the availability of alternatives and the migration of lead from the articles referred to in paragraph 7, including the requirement on coating integrity, and, if appropriate, modify this entry accordingly.\n10. By way of derogation paragraph 7 shall not apply to articles placed on the market for the first time before 1 June 2016.\n______________\n(*) OJ L 326, 29.12.1969, p. 36.\n(**) Directive 2009/48/EC of the European Parliament and of the Council of 18 June 2009 on the safety of toys (OJ L 170, 30.6.2009, p. 1).\n(***) Directive 2011/65/EU of the European Parliament and of the Council of 8 June 2011 on the restriction of the use of certain hazardous substances in electrical and electronic equipment (OJ L 174, 1.7.2011, p. 88).","1. Dürfen nicht in Verkehr gebracht oder in einem einzelnen Teil einer Schmuckware verwendet werden, wenn der Bleigehalt (in Metall) des betreffenden Teils 0,05 % oder mehr des Gewichts beträgt.\n2. Für die Zwecke des Absatzes 1 bezeichnet der Ausdruck:\ni) „Schmuckwaren“ Schmuck und Fantasieschmuck sowie Haarschmuck, einschließlich:\na) Armbänder, Halsketten und Ringe,\nb) Piercingschmuck,\nc) Armbanduhren und Armschmuck,\nd) Broschen und Manschettenknöpfe;\nii) „in einem einzelnen Teil“ auch die Materialien, aus denen der Schmuck hergestellt wurde, sowie die einzelnen Bestandteile der Schmuckwaren.\n3. Absatz 1 gilt auch für einzelne Teile, die für die Schmuckherstellung in Verkehr gebracht oder verwendet werden.\n4. Absatz 1 gilt jedoch nicht für:\na) Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/ EWG des Rates (***********),\nb) Einbauteile von Armband- und Taschenuhren sowie Zeitmessern, die für Verbraucher nicht zugänglich sind,\nc) nicht synthetische oder rekonstituierte Edel- und Schmucksteine (KN-Code 7103 gemäß Verordnung (EWG) Nr. 2658/87), sofern sie nicht mit Blei oder Bleiverbindungen oder Gemischen, die diese Stoffe enthalten, behandelt wurden,\nd) Email, definiert als verglasbare Gemische aus dem Schmelzen, Verglasen oder Sintern von Mineralien bei Temperaturen von mindestens 500 °C.\n5. Absatz 1 gilt jedoch nicht für Schmuckwaren, die vor dem 9. Oktober 2013 erstmals in Verkehr gebracht, und Schmuckwaren, die vor dem 10. Dezember 1961 hergestellt wurden.\n6. Bis zum 9. Oktober 2017 nimmt die Kommission eine Neubewertung der Absätze 1 bis 5 dieses Eintrags im Lichte neuer wissenschaftlicher Erkenntnisse vor; dabei wird auch die Verfügbarkeit von Alternativen und die Migration von Blei aus den in Absatz 1 genannten Erzeugnissen berücksichtigt und dieser Eintrag gegebenenfalls entsprechend geändert.\n7. Dürfen nicht in Verkehr gebracht oder in Erzeugnissen, die zur Abgabe an die breite Öffentlichkeit bestimmt sind, verwendet werden, wenn der Bleigehalt (in Metall) des betreffenden Erzeugnisses oder der zugänglichen Teile davon 0,05 % oder mehr des Gewichts beträgt und diese Erzeugnisse bzw. die zugänglichen Teile davon unter normalen oder vernünftigerweise vorhersehbaren Verwendungsbedingungen von Kindern in den Mund genommen werden könnten. Dieser Grenzwert gilt nicht, wenn die Freisetzungsrate von Blei aus einem solchen Erzeugnis oder den zugänglichen Teilen eines Erzeugnisses, seien sie beschichtet oder nicht, 0,05 μg/cm2 pro Stunde (entspricht 0,05 μg/g/h) nachweislich nicht überschreitet und — bei beschichteten Erzeugnissen — die Beschichtung ausreicht, damit diese Rate für einen Zeitraum von mindestens zwei Jahren bei normalen oder vernünftigerweise vorhersehbaren Bedingungen der Verwendung des Erzeugnisses nicht überschritten wird. Für die Zwecke dieses Absatzes gilt, dass ein Erzeugnis oder ein zugänglicher Teil eines Erzeugnisses von Kindern in den Mund genommen werden kann, wenn eines der Maße weniger als 5 cm beträgt oder wenn das Erzeugnis bzw. der Teil desselben ein abnehmbares oder hervorstehendes Teil dieser Größe aufweist.\n8. Absatz 7 gilt jedoch nicht für:\na) Schmuckwaren gemäß Absatz 1;\nb) Kristallglas gemäß Anhang I (Kristallglasarten 1, 2, 3 und 4) der Richtlinie 69/493/EWG;\nc) nicht synthetische oder rekonstituierte Edel- und Schmucksteine (KN-Code 7103 gemäß der Verordnung (EWG) Nr. 2658/87), sofern sie nicht mit Blei oder Bleiverbindungen oder Gemischen, die diese Stoffe enthalten, behandelt wurden;\nd)Email, definiert als verglasbare Gemische aus dem Schmelzen, Verglasen oder Sintern von Mineralien bei Temperaturen von mindestens 500 °C;\ne) Schlüssel und Schlösser einschließlich Vorhängeschlössern;\nf) Musikinstrumente;\ng) Erzeugnisse und Teile von Erzeugnissen, die Messinglegierungen enthalten, sofern der Bleigehalt (in Metall) im Messing 0,5 % des Gewichts nicht überschreitet;\nh) die Spitzen von Schreibgeräten;\ni) Devotionalien;\nj) Zink-Kohle-Gerätebatterien und Knopfzellen;\nk) Erzeugnisse im Anwendungsbereich der: i) Richtlinie 94/62/EG; ii) Verordnung (EG) Nr. 1935/2004; iii) Richtlinie 2009/48/EG des Europäischen Parlaments und des Rates(*); iv) Richtlinie 2011/65/EU des Europäischen Parlaments und des Rates(**).\n9. Bis zum 1. Juli 2019 nimmt die Kommission eine Neubewertung von Absatz 7 und Absatz 8 Buchstaben e, f, i und j dieses Eintrags im Lichte neuer wissenschaftlicher Erkenntnisse vor; dabei werden auch die Verfügbarkeit von Alternativen und die Migration von Blei aus den in Absatz 7 genannten Erzeugnissen sowie die Anforderungen an die Unversehrtheit der Beschichtung berücksichtigt, und dieser Eintrag wird gegebenenfalls entsprechend geändert.\n10. Absatz 7 gilt jedoch nicht für Erzeugnisse, die vor dem 1. Juni 2016 erstmals in Verkehr gebracht wurden.\n______________\n(*) Richtlinie 2009/48/EG des Europäischen Parlaments und des Rates vom 18. Juni 2009 über die Sicherheit von Spielzeug (ABl. L 170 vom 30.6.2009, S. 1).\n(**) Richtlinie 2011/65/EU des Europäischen Parlaments und des Rates vom 8. Juni 2011 zur Beschränkung der Verwendung bestimmter gefährlicher Stoffe in Elektro- und Elektronikgeräten (ABl. L 174 vom 1.7.2011, S. 88).\n(***********) ABl. L 326 vom 29.12.1969, S. 36.","1.如果零件中的铅含量（以金属计）占重量的0.05％或以上，该零件不得投放市场或用做任何珠宝首饰的单个零件。 \n2.对于第1条：\ni)珠宝首饰”应该包括珠宝及仿制首饰和发饰，包括：\na)手镯，项链和戒指，\nb)穿孔饰品，\nc)手表和手镯，\nd)胸针和袖扣;\nii)“单个零件”应该包括制造珠宝首饰的材料，以及首饰的单个部件。\n3.第1段也适用于那些在市场上销售的或用于珠宝制作的单个零件。\n4.第1段不适用于：\na)根据69/493/EEC（*）指令附件I（水晶玻璃类型1，2，3和4）中的定义的水晶玻璃；\nb)手表和怀表以及钟表中消费者接触不到的内部零件；\nc)非合成或再造的宝石和首饰宝石（按照法规（EEC）2658/87，CN代码7103），除非他们在加工过程中使用了含铅或铅化合物或者其它含铅配制品；\nd)搪瓷，被定义为在至少500℃的高温下，矿物被熔化，烧结或瓷化后形成的配制品。\n5)第1段不适用于已在2013年10月9日前已经投放市场的珠宝首饰和在1961年12月10日之前已制造好的珠宝首饰。\n6)在2017年10月9日之前，委员会会依据当时的科技能力对这个项目进行重新评估，包括替代品的可用性和在第一条中提到的珠宝首饰中铅的迁出情况，从而进行相应地修改。\n7.如果这些物品或其可接触部分的铅浓度（以金属表示）等于或大于0.05%（重量），并且这些物品或其可接触部分在正常或合理可预见的使用条件下可能被儿童放入口中，则不得投放市场或用于向公众提供的物品。\n如能证明从此类物品或物品的任何此类可接触部分（无论有无涂层）的铅释放率不超过每小时0.05μg/cm²（相当于0.05μg/h），且对于有涂层的物品，涂层足以确保在该物品的正常或可合理预见的使用条件下至少两年内不超过这一释放率，则该限制不适用。\n就本段而言，如果物品或物品的可接触部分在一个尺寸上小于5厘米，或有该尺寸的可拆卸或突出部分，则被认为可以被儿童放入口中。\n8. 作为减损，第7款不应适用于\n(a) 第1款所涵盖的珠宝制品。\n(b) 第69/493/EEC号指令附件一（第1、2、3和4类）中定义的水晶玻璃。\n(c) 非合成或重建的宝石和半宝石（根据(EEC)第2658/87号条例规定的CN代码7103），除非它们已经用铅或其化合物或含有这些物质的混合物处理过。\n(d) 搪瓷，定义为矿物在至少500摄氏度的温度下熔化、玻璃化或烧结而形成的可玻璃化的混合物。\n(e) 钥匙和锁具，包括挂锁。\n(f) 乐器。\n(g) 由黄铜合金组成的物品和物品的部件，如果铅（以金属表示）在黄铜合金中的浓度不超过0.5％（重量）。\n(h) 书写工具的尖端。\n(i) 宗教用品。\n(j) 便携式碳锌电池和扣式电池。\n(k) 符合下列规定的物品\n(i) 第94/62/EC号指令。\n(ii) 第1935/2004号条例（EC）。\n(iii) 欧洲议会和理事会的第2009/48/EC号指令（**）。\n(iv) 欧洲议会和理事会的第2011/65/EU号指令(***)\n9. 在2019年7月1日之前，委员会应根据新的科学信息，包括替代品的可得性和第7款所述物品中铅的迁移情况，包括对涂层完整性的要求，重新评估本条目第7款和第8款(e)、(f)、(i)和(j)项，并酌情对本条目进行相应修改。\n10. 作为减损，第7款不适用于2016年6月1日前首次投放市场的物品。\n______________\n(*) OJ L 326, 29.12.1969, p. 36.\n(**) 欧洲议会和理事会2009年6月18日关于玩具安全的第2009/48/EC号指令（OJ L 170, 30.6.2009, p. 1）。\n(***) 欧洲议会和理事会2011年6月8日关于限制在电气和电子设备中使用某些有害物质的指令2011/65/EU（OJ L 174，1.7.2011，第88页）。"]
[null,{"$f":"IF($B$1=\"English\",C1725,IF($B$1=\"Deutsch\",D1725,IF($B$1=\"中文\",E1725,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market or used, as a substance or as a constituent of mixtures in a concentration equal to or greater than 1 % by weight, where the substance or the mixture is placed on the market for use or used as an air freshener or deodoriser in toilets, homes, offices or other indoor public areas."},"Shall not be placed on the market or used, as a substance or as a constituent of mixtures in a concentration equal to or greater than 1 % by weight, where the substance or the mixture is placed on the market for use or used as an air freshener or deodoriser in toilets, homes, offices or other indoor public areas.","Darf als Stoff oder Bestandteil von Gemischen in einer Konzentration von 1 Gewichtsprozent oder mehr nicht in Verkehr gebracht oder verwendet werden, wenn der Stoff oder das Gemisch zur Verwendung als Lufterfrischer oder Deodorant in Toiletten, Privathaushalten, Büros oder anderen öffentlich zugänglichen Innenräumen in Verkehr gebracht oder als solche verwendet wird.","当其浓度以重量计等于或大于1%，不得作为物质或混合物的成分投放市场或使用，用于在厕所、家庭、办公室或其他室内公共场所作为空气清新剂或除臭剂。"]
[null,{"$f":"IF($B$1=\"English\",C1726,IF($B$1=\"Deutsch\",D1726,IF($B$1=\"中文\",E1726,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market in thermal paper in a concentration equal to or greater than 0,02 % by weight after 2 January 2020."},"Shall not be placed on the market in thermal paper in a concentration equal to or greater than 0,02 % by weight after 2 January 2020.","Darf in Thermopapier in einer Konzentration von ≥ 0,02 Gew.-% nach dem 2. Januar 2020 nicht in Verkehr gebracht werden.","2020年1月2日之后，不得在热敏纸中以等于或大于0.02%的重量浓度投放市场。"]
[null,{"$f":"IF($B$1=\"English\",C1727,IF($B$1=\"Deutsch\",D1727,IF($B$1=\"中文\",E1727,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020"},"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020","Gestrichen nach VERORDNUNG (EU) 2020/2096 vom 15. Dezember 2020","根据2020年12月15日发布的法规2020/2096/EU删除"]
[null,{"$f":"IF($B$1=\"English\",C1728,IF($B$1=\"Deutsch\",D1728,IF($B$1=\"中文\",E1728,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020"},"Deleted according to REGULATION (EU) 2020/2096 of 15 December 2020","Gestrichen nach VERORDNUNG (EU) 2020/2096 vom 15. Dezember 2020","根据2020年12月15日发布的法规2020/2096/EU删除"]
[null,{"$f":"IF($B$1=\"English\",C1729,IF($B$1=\"Deutsch\",D1729,IF($B$1=\"中文\",E1729,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Shall not be placed on the market to the general public after 9 May 2019 in windscreen washing or defrosting fluids, in a concentration equal to or greater than 0,6 % by weight."},"Shall not be placed on the market to the general public after 9 May 2019 in windscreen washing or defrosting fluids, in a concentration equal to or greater than 0,6 % by weight.","Darf nach dem 9. Mai 2019 nicht in Scheibenwaschflüssigkeiten oder Scheibenfrostschutzmitteln in einer Konzentration von 0,6 Gew.-% oder mehr für die allgemeine Öffentlichkeit in den Verkehr gebracht werden.","在2019年5月9日之后，当挡风玻璃清洗液或除霜液中浓度等于或高于0.6%（重量），不得向公众投放。"]
[null,{"$f":"IF($B$1=\"English\",C1730,IF($B$1=\"Deutsch\",D1730,IF($B$1=\"中文\",E1730,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market in wash-off cosmetic products in a concentration equal to or greater than 0,1 % by weight of either substance, after 31 January 2020.\n2. For the purposes of this entry, “wash-off cosmetic products” means cosmetic products as defined in Article 2(1)(a) of Regulation (EC) No 12"},"1. Shall not be placed on the market in wash-off cosmetic products in a concentration equal to or greater than 0,1 % by weight of either substance, after 31 January 2020.\n2. For the purposes of this entry, “wash-off cosmetic products” means cosmetic products as defined in Article 2(1)(a) of Regulation (EC) No 12","1. Darf nach dem 31. Januar 2020 in abwaschbaren kosmetischen Mitteln nicht in einer Konzentration von 0,1 Gewichtsprozent oder höher in den Verkehr gebracht werden.\n2. Für die Zwecke dieses Eintrags bezeichnet ‚abwaschbare kosmetische Mittel‘ kosmetische Mittel im Sinne von Artikel 2 Absatz 1 Buchstabe a der Verordnung (EG) Nr. 1223/2009, die unter normalen Anwendungsbedingungen nach dem Auftragen mit Wasser abgewaschen werden.“\n\n","1.在2020年1月31日之后，不得将浓度等于或大于0.1%（以重量计）的含两种物质的水洗型化妆品投放市场。\n2. 在本条目中，\"水洗化妆品 \"是指(EC)12号法规第2(1)(a)条中定义的化妆品。"]
[null,{"$f":"IF($B$1=\"English\",C1731,IF($B$1=\"Deutsch\",D1731,IF($B$1=\"中文\",E1731,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market as a substance on its own or in mixtures in a concentration equal to or greater than 0,3 % after 9 May 2020 unless manufacturers, importers and downstream users have included in the relevant chemical safety reports and safety data sheets, Derived No-Effect Levels (DNELs) relating to exposure of workers of 14,4 mg/m3 for exposure by inhalation and 4,8 mg/kg/day for dermal exposure.\n2. Shall not be manufactured, or used, as a substance on its own or in mixtures in a concentration equal to or greater than 0,3 % after 9 May 2020 unless manufacturers and downstream users take the appropriate risk management measures and provide the appropriate operational conditions to ensure that exposure of workers is below the DNELs specified in paragraph 1.\n3. By way of derogation from paragraphs 1 and 2, the obligations laid down therein shall apply from 9 May 2024 in relation to placing on the market for use, or use, as a solvent or reactant in the process of coating wires."},"1. Shall not be placed on the market as a substance on its own or in mixtures in a concentration equal to or greater than 0,3 % after 9 May 2020 unless manufacturers, importers and downstream users have included in the relevant chemical safety reports and safety data sheets, Derived No-Effect Levels (DNELs) relating to exposure of workers of 14,4 mg/m3 for exposure by inhalation and 4,8 mg/kg/day for dermal exposure.\n2. Shall not be manufactured, or used, as a substance on its own or in mixtures in a concentration equal to or greater than 0,3 % after 9 May 2020 unless manufacturers and downstream users take the appropriate risk management measures and provide the appropriate operational conditions to ensure that exposure of workers is below the DNELs specified in paragraph 1.\n3. By way of derogation from paragraphs 1 and 2, the obligations laid down therein shall apply from 9 May 2024 in relation to placing on the market for use, or use, as a solvent or reactant in the process of coating wires.","1. Darf nach dem 9. Mai 2020 nicht als Stoff oder in Gemischen in Konzentrationen von ≥ 0,3 % in den Verkehr gebracht werden, es sei denn, die Hersteller, Importeure und nachgeschalteten Anwender haben DNEL-Werte für die NMP-Exposition von Arbeitnehmern von 14,4 mg/m3 bei Inhalation und von 4,8 mg/kg/Tag bei Aufnahme über die Haut in die einschlägigen Stoffsicherheitsberichte und Sicherheitsdatenblätter aufgenommen.\n2. Darf nach dem 9. Mai 2020 nicht als Stoff oder in Gemischen in Konzentrationen von ≥ 0,3 % hergestellt oder verwendet werden, es sei denn, Hersteller und nachgeschaltete Anwender treffen geeignete Risikomanagementmaßnahmen und sorgen für angemessene Verwendungsbedingungen, die gewährleisten, dass die Exposition von Arbeitnehmern unter den in Absatz 1 angegebenen DNEL-Werten liegt.\n3. Abweichend von den Absätzen 1 und 2 gelten die darin vorgesehenen Auflagen für die Verwendung oder für das Inverkehrbringen zur Verwendung als Lösungsmittel oder Reaktant im Drahtbeschichtungsprozess ab dem 9. Mai 2024.","1. 2020年5月9日之后，不得作为一种物质单独或在混合物中以等于或大于0.3%的浓度投放市场，除非制造商、进口商和下游用户在相关的化学安全报告和安全数据表中列入与工人接触有关的衍生无效应水平（DNELs），即吸入接触为14.4mg/m3，皮肤接触为4.8mg/kg/day。\n2. 2020年5月9日之后，不得制造或使用浓度等于或大于0.3%的物质，除非制造商和下游用户采取适当的风险管理措施，并提供适当的操作条件，确保工人的接触低于第1款规定的DNEL。\n3. 作为对第1款和第2款的减损，其中规定的义务应从2024年5月9日起适用于在市场上投放和使用，或作为溶剂或反应物在电线涂层过程中使用。"]
[null,{"$f":"IF($B$1=\"English\",C1732,IF($B$1=\"Deutsch\",D1732,IF($B$1=\"中文\",E1732,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market after 1 November 2020 in any of the following:\n(a) clothing or related accessories;\n(b) textiles other than clothing which, under normal or reasonably foreseeable conditions of use, come into contact with human skin to an extent similar to clothing;\n(c) footwear;\nif the clothing, related accessory, textile other than clothing or footwear is for use by consumers and the substance is present in a concentration, measured in homogeneous material, equal to or greater than that specified for that substance in Appendix 12.\n2. By way of derogation, in relation to the placing on the market of formaldehyde [CAS No 50-00-0] in jackets, coats or upholstery, the relevant concentration for the purposes of paragraph 1 shall be 300 mg/kg during the period between 1 November 2020 and 1 November 2023. The concentration specified in Appendix 12 shall apply thereafter.\n3. Paragraph 1 shall not apply to:\n(a) clothing, related accessories or footwear, or parts of clothing, related accessories or footwear, made exclusively of natural leather, fur or hide;\n(b) non-textile fasteners and non-textile decorative attachments;\n(c) second-hand clothing, related accessories, textiles other than clothing or footwear\n(d) wall-to-wall carpets and textile floor coverings for indoor use, rugs and runners.\n4. Paragraph 1 shall not apply to clothing, related accessories, textiles other than clothing, or footwear within the scope of Regulation (EU) 2016/425 of the European Parliament\nand of the Council1 or Regulation (EU) 2017/745 of the European Parliament and of the Council2.\n5. Paragraph 1(b) shall not apply to disposable textiles. ‘Disposable textiles’ means textiles that are designed to be used only once or for a limited time and are not intended for subsequent use for the same or a similar purpose.\n6. Paragraphs 1 and 2 shall apply without prejudice to the application of any stricter restrictions set out in this Annex or in other applicable Union legislation.\n7. The Commission shall review the exemption in paragraph 3(d) and, if appropriate, modify that point accordingly."},"1. Shall not be placed on the market after 1 November 2020 in any of the following:\n(a) clothing or related accessories;\n(b) textiles other than clothing which, under normal or reasonably foreseeable conditions of use, come into contact with human skin to an extent similar to clothing;\n(c) footwear;\nif the clothing, related accessory, textile other than clothing or footwear is for use by consumers and the substance is present in a concentration, measured in homogeneous material, equal to or greater than that specified for that substance in Appendix 12.\n2. By way of derogation, in relation to the placing on the market of formaldehyde [CAS No 50-00-0] in jackets, coats or upholstery, the relevant concentration for the purposes of paragraph 1 shall be 300 mg/kg during the period between 1 November 2020 and 1 November 2023. The concentration specified in Appendix 12 shall apply thereafter.\n3. Paragraph 1 shall not apply to:\n(a) clothing, related accessories or footwear, or parts of clothing, related accessories or footwear, made exclusively of natural leather, fur or hide;\n(b) non-textile fasteners and non-textile decorative attachments;\n(c) second-hand clothing, related accessories, textiles other than clothing or footwear\n(d) wall-to-wall carpets and textile floor coverings for indoor use, rugs and runners.\n4. Paragraph 1 shall not apply to clothing, related accessories, textiles other than clothing, or footwear within the scope of Regulation (EU) 2016/425 of the European Parliament\nand of the Council1 or Regulation (EU) 2017/745 of the European Parliament and of the Council2.\n5. Paragraph 1(b) shall not apply to disposable textiles. ‘Disposable textiles’ means textiles that are designed to be used only once or for a limited time and are not intended for subsequent use for the same or a similar purpose.\n6. Paragraphs 1 and 2 shall apply without prejudice to the application of any stricter restrictions set out in this Annex or in other applicable Union legislation.\n7. The Commission shall review the exemption in paragraph 3(d) and, if appropriate, modify that point accordingly.","1. Dürfen nach dem 1. November 2020 in Folgendem nicht mehr in Verkehr gebracht werden:\na) Kleidung oder damit in Bezug stehendem Zubehör,\nb) anderen Textilien, die bei normaler oder vernünftigerweise vorhersehbarer Verwendung in einem ähnlichen Maße wie Kleidung mit der menschlichen Haut in Berührung kommen,\nc) Schuhwaren, wenn die Kleidung, das damit in Bezug stehende Zubehör, die anderen Textilien oder die Schuhwaren für die Nutzung durch Verbraucher vorgesehen sind und der Stoff in einer in homogenem Material gemessenen Konzentration vorhanden ist, die gleich der für diesen Stoff in Anlage 12 angegebenen ist oder darüber liegt.\n2. Abweichend von dieser Bestimmung liegt für das Inverkehrbringen von Formaldehyd [CAS-Nr. 50-00-0] in Jacken, Mänteln oder Polsterungen die entsprechende Konzentration im Sinne von Nummer 1 im Zeitraum vom 1. November 2020 bis 1. November 2023 bei 300 mg/kg. Danach gilt die in Anlage 12 angegebene Konzentration.\n3. Nummer 1 gilt nicht für\na) Kleidung, damit in Bezug stehendes Zubehör, Schuhwaren oder Teile von Kleidung, damit in Bezug stehendem Zubehör oder Schuhwaren, die ausschließlich aus Naturleder, Pelzen oder Häuten bestehen,\nb) nicht textile Verschlüsse und nicht textile Zierelemente,\nc) gebrauchte Kleidung, damit in Bezug stehendes Zubehör, andere Textilien oder Schuhwaren,\nd) Teppichböden und textile Fußbodenbeläge zur Verwendung in Innenräumen; Teppiche und Läufer.\n4. Nummer 1 gilt nicht für Kleidung, damit in Bezug stehendes Zubehör, andere Textilien oder Schuhwaren im Anwendungsbereich der Verordnung (EU) 2016/425 des Europäischen Parlaments und des Rates (*) oder der Verordnung (EU) 2017/745 des Europäischen Parlaments und des Rates (**).\n5. Nummer 1 Buchstabe b gilt nicht für Einwegtextilien. „Einwegtextilien“ sind Textilien, die nur für den einmaligen oder kurzzeitigen Gebrauch und nicht für eine spätere Verwendung zum gleichen oder zu einem ähnlichen Zweck vorgesehen sind.\n6. Die Nummern 1 und 2 gelten unbeschadet der Anwendung strengerer Beschränkungen, die in diesem Anhang oder in anderen einschlägigen Rechtsvorschriften der Union festgelegt sind.\n7. Die Kommission überprüft die Ausnahme in Nummer 3 Buchstabe d und ändert diesen Punkt gegebenenfalls entsprechend.\n\n______________\n(*) Verordnung (EU) 2016/425 des Europäischen Parlaments und des Rates vom 9. März 2016 über persönliche Schutzausrüstungen und zur Aufhebung der Richtlinie 89/686/EWG des Rates (ABl. L 81 vom 31.3.2016, S. 51).\n(**) Verordnung (EU) 2017/745 des Europäischen Parlaments und des Rates vom 5. April 2017 über Medizinprodukte, zur Änderung der Richtlinie 2001/83/EG, der Verordnung (EG) Nr. 178/2002 und der Verordnung (EG) Nr. 1223/2009 und zur Aufhebung der Richtlinien 90/385/EWG und 93/42/EWG des Rates (ABl. L 117 vom 5.5.2017, S. 1).\n\n","1. 不得在2020年11月1日之后在市场上投放以下任何一种产品。\n(a) 服装或相关配件。\n(b) 除服装外，在正常或可合理预见的使用条件下，与人体皮肤接触程度类似于服装的纺织品。\n(c) 鞋类。\n如果该服装、相关配件、除服装以外的纺织品或鞋类是供消费者使用的，并且该物质在同质材料中的测量浓度等于或大于附录12中为该物质规定的浓度。\n2. 作为减损，就夹克、大衣或室内装饰品中的甲醛[CAS No 50-00-0]投放市场而言，在2020年11月1日至2023年11月1日期间，第1项的相关浓度应为300毫克/千克。此后，附录12中规定的浓度将适用。\n3. 第1款不应适用于\n(a) 完全由天然皮革、毛皮或兽皮制成的服装、相关配件或鞋类，或服装、相关配件或鞋类的部件。\n(b) 非纺织品紧固件和非纺织品装饰性附件。\n(c) 二手服装、相关配件、服装或鞋类以外的纺织品\n(d) 墙到墙的地毯和室内用的纺织品地板覆盖物、地毯和滑道。\n4. 第1项不适用于欧洲议会和理事会第2016/425号条例（EU）范围内的服装、相关配件、除服装外的纺织品或鞋类。\n和理事会1或欧洲议会和理事会2的(EU)2017/745号条例范围内的服装、相关配件、服装以外的纺织品或鞋类。\n5. 第1（b）项不适用于一次性纺织品。一次性纺织品 \"是指旨在只使用一次或在有限的时间内使用，并且不打算在以后用于相同或类似目的的纺织品。\n6. 第1和第2项的适用不应影响本附件或其他适用的欧盟立法中规定的任何更严格的限制的适用。\n7. 委员会应审查第3(d)项中的豁免，并在适当时对其进行相应修改。"]
[null,{"$f":"IF($B$1=\"English\",C1733,IF($B$1=\"Deutsch\",D1733,IF($B$1=\"中文\",E1733,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market for supply to the general public after 2 January 2021 individually or in any combination, in a concentration equal to or greater than 2 ppb by weight of the mixtures containing organic solvents, in spray products.\n2. For the purpose of this entry, “spray products” means aerosol dispensers, pump sprays, trigger sprays, marketed for proofing or impregnation spray applications.\n3. Without prejudice to the implementation of other Union provisions concerning the classification, packaging and labelling of substances and mixtures, the packaging of spray products containing (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) silanetriol and/or TDFAs combined with organic solvents as referred to in paragraph 1 and placed on the market for professional use shall be marked clearly and indelibly: “for professional users only” and “Fatal if inhaled” with the pictogram GHS06.\n4. Section 2.3 of Safety Data Sheets shall contain the following information: “mixtures of (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) silanetriol and/or any of its mono-, di- or tri-O-(alkyl) derivatives in a concentration equal to or greater than 2 ppb and organic solvents in spray products, are for professional users only and marked ‘Fatal if inhaled’”.\n5. Organic solvents referred to in paragraph 1, 3, and 4 include organic solvents used as aerosol propellants."},"1. Shall not be placed on the market for supply to the general public after 2 January 2021 individually or in any combination, in a concentration equal to or greater than 2 ppb by weight of the mixtures containing organic solvents, in spray products.\n2. For the purpose of this entry, “spray products” means aerosol dispensers, pump sprays, trigger sprays, marketed for proofing or impregnation spray applications.\n3. Without prejudice to the implementation of other Union provisions concerning the classification, packaging and labelling of substances and mixtures, the packaging of spray products containing (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) silanetriol and/or TDFAs combined with organic solvents as referred to in paragraph 1 and placed on the market for professional use shall be marked clearly and indelibly: “for professional users only” and “Fatal if inhaled” with the pictogram GHS06.\n4. Section 2.3 of Safety Data Sheets shall contain the following information: “mixtures of (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) silanetriol and/or any of its mono-, di- or tri-O-(alkyl) derivatives in a concentration equal to or greater than 2 ppb and organic solvents in spray products, are for professional users only and marked ‘Fatal if inhaled’”.\n5. Organic solvents referred to in paragraph 1, 3, and 4 include organic solvents used as aerosol propellants.","1. Darf nach dem 2. Januar 2021 in Sprühprodukten zur Abgabe an die breite Öffentlichkeit weder einzeln noch in beliebiger Kombination bei einer Konzentration von 2 ppb oder höher bezogen auf das Gewicht der organische Lösungsmittel enthaltenden Gemische in Verkehr gebracht werden.\n2. ‚Sprühprodukte‘ im Sinne dieses Eintrags sind Aerosolpackungen, Pumpsprays, Triggersprays, die für abdichtende oder imprägnierende Sprühanwendungen in Verkehr gebracht werden.\n3. Unbeschadet der Durchführung anderer Unionsvorschriften über die Einstufung, Verpackung und Kennzeichnung von Stoffen und Gemischen ist die Verpackung von Sprühprodukten, die, wie in Absatz 1 aufgeführt, (3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoroctyl)-silantriol und/oder TDFAs in Verbindung mit organischen Lösungsmitteln enthalten und zur gewerblichen Verwendung in Verkehr gebracht werden, deutlich lesbar und dauerhaft wie folgt zu kennzeichnen: ‚nur für gewerbliche Verwender‘ und ‚Lebensgefahr bei Einatmen‘ mit dem Piktogramm GHS06.\n4. In Abschnitt 2.3 des Sicherheitsdatenblatts sind folgende Angaben aufzunehmen: ‚Gemische aus (3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoroctyl)-silantriol und/oder einem seiner Mono-, Di- oder Tri-O-(Alkyl)-Derivate in einer Konzentration von 2 ppb oder höher sowie aus organischen Lösungsmitteln in Sprühprodukten sind nur für gewerbliche Verwender bestimmt und gekennzeichnet mit ‚Lebensgefahr bei Einatmen‘.‘\n5. Zu den in den Absätzen 1, 3 und 4 genannten Lösungsmitteln gehören auch Lösungsmittel, die als Aerosoltreibmittel verwendet werden.","1.在2021年1月2日之后，对于有机溶剂（单独或以任何组合形式）重量浓度为2ppb或以上的喷雾产品，不得向公众供应或向市场投放。\n2.就本条目而言，\"喷雾产品\"是指市场上用于打样或浸渍喷雾的气溶胶分配器、泵式喷雾器、触发式喷雾器。\n3.在不影响执行欧盟关于物质和混合物分类、包装和标签的其他规定的情况下，含有（3,3,4,4,5,5,6,6,7,8,8,8-十三氟辛基）硅烷三醇和/或TDFAs及第1项所述的有机溶剂的喷雾产品，在投放市场用于专业用途时，应保证包装标签清晰、可读和不可磨损，并注明\"仅供专业人员使用 \"、\"吸入后可致死 \"、GHS06标志。\n4.安全数据表的第2、3项应包含以下信息：喷雾产品含有有机溶剂和浓度等于或大于2ppb（3,3,4,4,5,5,6,6,7,8,8,8-十三氟辛基）硅烷三醇及其任意单、双或三-邻-（烷基）衍生物的混合物，应注明“仅适用于专业使用者”和“吸入即致命'\"。\n5.第1、3、4项中提到的有机溶剂包括作为气雾剂推进剂的有机溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C1734,IF($B$1=\"Deutsch\",D1734,IF($B$1=\"中文\",E1734,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be used as substances on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) after 24 August 2023, unless:\n(a) the concentration of diisocyanates individually and in combination is less than 0,1 % by weight, or\n(b) the employer or self-employed ensures that industrial or professional user(s) have successfully completed training on the safe use of diisocyanates prior to the use of the substance(s) or mixture(s).\n2. Shall not be placed on the market as substances on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) after 24 February 2022, unless:\n(a) the concentration of diisocyanates individually and in combination is less than 0,1 % by weight, or\n(b) the supplier ensures that the recipient of the substance(s) or mixture(s) is provided with information on the requirements referred to in point (b) of paragraph 1 and the following statement is placed on the packaging, in a manner that is visibly distinct from the rest of the label information: “As from 24 August 2023 adequate training is required before industrial or professional use”.\n3. For the purpose of this entry “industrial and professional user(s)” means any worker or self-employed worker handling diisocyanates on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) or supervising these tasks.\n4. The training referred to in point (b) of paragraph 1 shall include the instructions for the control of dermal and inhalation exposure to diisocyanates at the workplace without prejudice to any national occupational exposure limit value or other appropriate risk management measures at national level. Such training shall be conducted by an expert on occupational safety and health with competence acquired by relevant vocational training. That training shall cover as a minimum:\n(a) the training elements in point (a) of paragraph 5 for all industrial and professional use(s).\n(b) the training elements in points (a) and (b) of paragraph 5 for the following uses:\n— handling open mixtures at ambient temperature (including foam tunnels);\n— spraying in a ventilated booth;\n— application by roller;\n— application by brush;\n— application by dipping and pouring;\n— mechanical post treatment (e.g. cutting) of not fully cured articles which are not warm anymore;\n— cleaning and waste;\n— any other uses with similar exposure through the dermal and/or inhalation route;\n(c) the training elements in points (a), (b) and (c) of paragraph 5 for the following uses:\n— handling incompletely cured articles (e.g. freshly cured, still warm);\n— foundry applications;\n— maintenance and repair that needs access to equipment;\n— open handling of warm or hot formulations (> 45 °C);\n— spraying in open air, with limited or only natural ventilation (includes large industry working halls) and spraying with high energy (e.g. foams, elastomers);\n— and any other uses with similar exposure through the dermal and/or inhalation route.\n5. Training elements:\n(a) general training, including on-line training, on:\n— chemistry of diisocyanates;\n— toxicity hazards (including acute toxicity);\n— exposure to diisocyanates;\n— occupational exposure limit values;\n— how sensitisation can develop;\n— odour as indication of hazard;\n— importance of volatility for risk;\n— viscosity, temperature, and molecular weight of diisocyanates;\n— personal hygiene;\n— personal protective equipment needed, including practical instructions for its correct use and its limitations;\n— risk of dermal contact and inhalation exposure;\n— risk in relation to application process used;\n— skin and inhalation protection scheme;\n— ventilation;\n— cleaning, leakages, maintenance;\n— discarding empty packaging;\n— protection of bystanders;\n— identification of critical handling stages;\n— specific national code systems (if applicable);\n— behaviour-based safety;\n— certification or documented proof that training has been successfully completed\n(b) intermediate level training, including on-line training, on:\n— additional behaviour-based aspects;\n— maintenance;\n— management of change;\n— evaluation of existing safety instructions;\n— risk in relation to application process used;\n— certification or documented proof that training has been successfully completed\n(c) advanced training, including on-line training, on:\n— any additional certification needed for the specific uses covered;\n— spraying outside a spraying booth;\n— open handling of hot or warm formulations (> 45 °C);\n— certification or documented proof that training has been successfully completed\n6. The training shall comply with the provisions set by the Member State in which the industrial or professional user(s) operate. Member States may implement or continue to apply their own national requirements for the use of the substance(s) or mixture(s), as long as the minimum requirements set out in paragraphs 4 and 5 are met.\n7. The supplier referred to in point (b) of paragraph 2 shall ensure that the recipient is provided with training material and courses pursuant to paragraphs 4 and 5 in the official language(s) of the Member State(s) where the substance(s) or mixture(s) are supplied. The training shall take into consideration the specificity of the products supplied, including composition, packaging, and design.\n8. The employer or self-employed shall document the successful completion of the training referred to in paragraphs 4 and 5. The training shall be renewed at least every five years.\n9. Member States shall include in their reports pursuant to Article 117(1) the following information:\n(a) any established training requirements and other risk management measures related to the industrial and professional uses of diisocyanates foreseen in national law;\n(b) the number of cases of reported and recognised occupational asthma and occupational respiratory and dermal diseases in relation to diisocyanates;\n(c) national exposure limits for diisocyanates, if there are any;\n(d) information about enforcement activities related to this restriction.\n10. This restriction shall apply without prejudice to other Union legislation on the protection of safety and health of workers at the workplace."},"1. Shall not be used as substances on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) after 24 August 2023, unless:\n(a) the concentration of diisocyanates individually and in combination is less than 0,1 % by weight, or\n(b) the employer or self-employed ensures that industrial or professional user(s) have successfully completed training on the safe use of diisocyanates prior to the use of the substance(s) or mixture(s).\n2. Shall not be placed on the market as substances on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) after 24 February 2022, unless:\n(a) the concentration of diisocyanates individually and in combination is less than 0,1 % by weight, or\n(b) the supplier ensures that the recipient of the substance(s) or mixture(s) is provided with information on the requirements referred to in point (b) of paragraph 1 and the following statement is placed on the packaging, in a manner that is visibly distinct from the rest of the label information: “As from 24 August 2023 adequate training is required before industrial or professional use”.\n3. For the purpose of this entry “industrial and professional user(s)” means any worker or self-employed worker handling diisocyanates on their own, as a constituent in other substances or in mixtures for industrial and professional use(s) or supervising these tasks.\n4. The training referred to in point (b) of paragraph 1 shall include the instructions for the control of dermal and inhalation exposure to diisocyanates at the workplace without prejudice to any national occupational exposure limit value or other appropriate risk management measures at national level. Such training shall be conducted by an expert on occupational safety and health with competence acquired by relevant vocational training. That training shall cover as a minimum:\n(a) the training elements in point (a) of paragraph 5 for all industrial and professional use(s).\n(b) the training elements in points (a) and (b) of paragraph 5 for the following uses:\n— handling open mixtures at ambient temperature (including foam tunnels);\n— spraying in a ventilated booth;\n— application by roller;\n— application by brush;\n— application by dipping and pouring;\n— mechanical post treatment (e.g. cutting) of not fully cured articles which are not warm anymore;\n— cleaning and waste;\n— any other uses with similar exposure through the dermal and/or inhalation route;\n(c) the training elements in points (a), (b) and (c) of paragraph 5 for the following uses:\n— handling incompletely cured articles (e.g. freshly cured, still warm);\n— foundry applications;\n— maintenance and repair that needs access to equipment;\n— open handling of warm or hot formulations (> 45 °C);\n— spraying in open air, with limited or only natural ventilation (includes large industry working halls) and spraying with high energy (e.g. foams, elastomers);\n— and any other uses with similar exposure through the dermal and/or inhalation route.\n5. Training elements:\n(a) general training, including on-line training, on:\n— chemistry of diisocyanates;\n— toxicity hazards (including acute toxicity);\n— exposure to diisocyanates;\n— occupational exposure limit values;\n— how sensitisation can develop;\n— odour as indication of hazard;\n— importance of volatility for risk;\n— viscosity, temperature, and molecular weight of diisocyanates;\n— personal hygiene;\n— personal protective equipment needed, including practical instructions for its correct use and its limitations;\n— risk of dermal contact and inhalation exposure;\n— risk in relation to application process used;\n— skin and inhalation protection scheme;\n— ventilation;\n— cleaning, leakages, maintenance;\n— discarding empty packaging;\n— protection of bystanders;\n— identification of critical handling stages;\n— specific national code systems (if applicable);\n— behaviour-based safety;\n— certification or documented proof that training has been successfully completed\n(b) intermediate level training, including on-line training, on:\n— additional behaviour-based aspects;\n— maintenance;\n— management of change;\n— evaluation of existing safety instructions;\n— risk in relation to application process used;\n— certification or documented proof that training has been successfully completed\n(c) advanced training, including on-line training, on:\n— any additional certification needed for the specific uses covered;\n— spraying outside a spraying booth;\n— open handling of hot or warm formulations (> 45 °C);\n— certification or documented proof that training has been successfully completed\n6. The training shall comply with the provisions set by the Member State in which the industrial or professional user(s) operate. Member States may implement or continue to apply their own national requirements for the use of the substance(s) or mixture(s), as long as the minimum requirements set out in paragraphs 4 and 5 are met.\n7. The supplier referred to in point (b) of paragraph 2 shall ensure that the recipient is provided with training material and courses pursuant to paragraphs 4 and 5 in the official language(s) of the Member State(s) where the substance(s) or mixture(s) are supplied. The training shall take into consideration the specificity of the products supplied, including composition, packaging, and design.\n8. The employer or self-employed shall document the successful completion of the training referred to in paragraphs 4 and 5. The training shall be renewed at least every five years.\n9. Member States shall include in their reports pursuant to Article 117(1) the following information:\n(a) any established training requirements and other risk management measures related to the industrial and professional uses of diisocyanates foreseen in national law;\n(b) the number of cases of reported and recognised occupational asthma and occupational respiratory and dermal diseases in relation to diisocyanates;\n(c) national exposure limits for diisocyanates, if there are any;\n(d) information about enforcement activities related to this restriction.\n10. This restriction shall apply without prejudice to other Union legislation on the protection of safety and health of workers at the workplace.","1. Dürfen nach dem 24. August 2023 weder als Stoff noch als Bestandteil in anderen Stoffen oder Gemischen industriell oder gewerblich verwendet werden, es sei denn,\na) die Konzentration von Diisocyanaten einzeln und in Kombination beträgt weniger als 0,1 Gew.-% oder\nb) der Arbeitgeber oder Selbstständige stellt sicher, dass industrielle oder gewerbliche Anwender vor der Verwendung des/der Stoffe(s) oder Gemische(s) erfolgreich eine Schulung zur sicheren Verwendung von Diisocyanaten abgeschlossen haben.\n2. Dürfen nach dem 24. Februar 2022 weder als Stoff noch als Bestandteil in anderen Stoffen oder Gemischen für die industrielle oder gewerbliche Verwendung in Verkehr gebracht werden es sein denn,\na) die Konzentration von Diisocyanaten einzeln und in Kombination beträgt weniger als 0,1 Gew.-% oder\nb) der Lieferant stellt sicher, dass der Abnehmer des/der Stoffe(s) oder Gemische(s) von den Anforderungen nach Absatz 1 Buchstabe b Kenntnis hat, und dass auf der Verpackung die folgende Erklärung deutlich von den übrigen Angaben auf dem Etikett unterscheidbar angebracht ist: ab dem 24. August 2023 muss vor der industriellen oder gewerblichen Verwendung eine angemessene Schulung erfolgen.\n3. Für die Zwecke dieses Eintrags bezeichnet der Ausdruck ,industrielle(r) oder gewerblicher Anwender' jeden Arbeitnehmer oder Selbstständigen, der Diisocyanate als Stoffe oder als Bestandteil in anderen Stoffen oder in Gemischen für die industrielle und gewerbliche Verwendung handhabt oder die Handhabung überwacht\n4. Die in Absatz 1 Buchstabe b erwähnte Schulung beinhaltet Anleitungen zur Kontrolle der Exposition am Arbeitsplatz gegenüber Diisocyanaten durch Hautkontakt und Einatmen; nationale Arbeitsplatzgrenzwerte oder andere angemessene Risikomanagementmaßnahmen auf nationaler Ebene bleiben davon unberührt. Diese Schulung wird von einem Experten auf dem Gebiet der Sicherheit und des Gesundheitsschutzes am Arbeitsplatz durchgeführt, der seine Kenntnisse im Rahmen einer entsprechenden Ausbildung erlangt hat. Die Schulung muss zumindest Folgendes abdecken:\na) die in Absatz 5 Buchstabe a genannten Schulungsbestandteile für alle industriellen und gewerblichen Verwendungen;\nb) die in Absatz 5 Buchstaben a und b genannten Schulungsbestandteile für folgende Verwendungen:\n- Handhabung offener Gemische bei Raumtemperatur (inklusive in Schaumtunneln);\n- Sprühen in einer belüfteten Spritzkabine;\n- Auftragen mit einer Rolle;\n- Auftragen mit einem Pinsel;\n- Auftragen durch Tauchen und Gießen;\n- mechanische Nachbehandlung (z.B. Schneiden) nicht vollständig getrockneter abgekühlter Erzeugnisse;\n- Reinigung und Abfallentsorgung;\n- jede sonstige Verwendung, bei der eine ähnliche Exposition durch Hautkontakt und/oder Einatmen besteht;\nc) die in Absatz 5 Buchstaben a, b und c genannten Schulungsbestandteile für folgende Verwendungen:\n- Handhabung unvollständig getrockneter Erzeugnisse (z.B frisch getrocknet, noch warm);\n- Gießereianwendungen;\n- Wartungs- und Reparaturarbeiten, für die Zugang zu Ausrüstung erforderlich ist;\n- offene Handhabung warmer oder heißer Formulierungen (> 45°C);\n- Sprühen unter freiem Himmel, mit eingeschränkter oder ausschließlich natürlicher Belüftung (auch in großen Industriehallen) und Sprühen mit hoher Energie (z.B Schaum, Elastomere)\n- und jede weitere Verwendung, bei der es zu einer ähnlichen Exposition durch Hautkontakt und/oder Einatmen kommt.\n5. Schulungsbestandteile:\na) allgemeine Schulung einschließlich Online-Schulung zu:\n- chemischen Eigenschaften der Diisocyanate;\n- Toxizität (einschließlich akuter Toxizität);\n- Exposition gegenüber Diisocyanaten;\n- Arbeitsplatzgrenzwerten;\n- Ursachen von Sensibilisierung;\n- Geruch als Indikator für Gefahren;\n- Risikorelevanz der Flüchtigkeit;\n- Viskosität, Temperatur und Molekulargewicht von Diisocyanaten;\n- persönlicher Hygiene;\n- erforderlicher persönlicher Schutzausrüstung einschließlich praktischer Anweisungen bezüglich ihrer sachgemäßen Verwendung und ihrer Grenzen;\n- Risiko einer Exposition durch Hautkontakt und Einatmen;\n- Risiko in Bezug auf den eingesetzten Anwendungsprozess;\n- Maßnahmen zum Hautschutz und zum Schtz beim Einatmen;\n- Belüftung;\n- Reinigung, Leckage, Wartung;\n- Entsorgung leerer Verpackungen;\n- Schutz umstehender Personen;\n- Erkennen der wesentlichen Handhabungsetappen;\n- spezifischen nationalen Codesystemen (sofern vorhanden);\n- sicherheitsförderndem Verhalten;\n- Bescheinigungen oder dokumentierten Nachweisen über den erfolgreichen Abschluss einer Schulung;\nb) Aufbauschulung einschließlich Online-Schulung zu:\n- weiteren verhaltensbezogenen Aspekten;\n- Instandhaltung;\n- Änderungsmanagement;\n- Bewertung bestehender Sicherheitsanweisungen;\n- Risiko in Bezug auf den eingesetzten Anwendungsprozess;\n- Bescheinigungen oder dokumentierten Nachweisen über den erfolgreichen Abschluss einer Schulung;\nc) Fortgeschrittenenschulung einschließlich Online-Schulung zu:\n- jeder weiteren für die spezifische Verwendung erforderlichen Zertifizierung;\n- Sprühen außerhalb einer Spritzkabine;\n- offener Handhabung heißer oder warmer Formulierungen (> 45°C);\n- Bescheinigungen oder dokumentierten Nachweisen über den erfolgreichen Abschluss einer Schulung;\nc) Fortgeschrittenenschulung einschließlich Online-Schulung zu:\n- jeder weiteren für die spezifische Verwendung erforderlichen Zertifizierung;\n- Sprühen außerhalb einer Spritzkabine;\n- offener Handhabung heißer oder warmer Formulierungen (> 45°C);\n- Bescheinigungen oder dokumentierten nachweisen über den erfolgreichen Abschluss einer Schulung;\n6. Die Schulung soll den Regeln des Mitgliedstaats entsprechen, in dem der/die industrielle(n) oder gewerblich(n) Anwender tätig ist/sind: mitgliedstaaten können ihre eigenen nationalen Anforderungen für die Verwendung des/der Stoffe(s) oder Gemische(s) umsetzen oder weiterhin anwenden, sofern die Mindestanforderungen nach den Absätzen 4 und 5 erfüllt sind.\n7. Der in Absatz 2 Buchstabe b genannte Lieferant stellt sicher, dass dem Abnehmer Schulungsmaterialien und Schulungen nach den Absätzen 4 und 5 in der/den Amtssprache(n) des/der Mitgliedstaats/n zur Verfügung gestellt werden, in den/in die der/die Stoff(e) oder das/die Gemische(e) geliefert wird/werden. Die Besonderheiten der gelieferten Produkte, einschließlich Zusammensetzung, Verpackung und Design, werden in der Schulung berücksichtigt.\n8. Der Arbeitgeber oder Selbstständige dokumentiert den erfolgreichen Abschluss der nach den Absätzen 4 und 5 vorgesehenen Schulung. Die Schulung muss mindestens alle fünf Jahre wiederholt werden.\n9. Die gemäß Artikel 117 Absatz 1 vorzulegenden Berichte der Mitgliedstaaten enthalten unter anderem die folgenden Informationen:\na) Alle eingeführten Schulungsanforderungen und andere Risikomanagementmaßnahmen bezüglich industrieller und gewerblicher Verwendungen von Diisocyanaten, die gemäß den antionalen Rechtsvorschriften vorgesehen sind;\nb) die Zahl der gemeldeten und anerkannten Fälle von Berufsasthma und berufsbedingten Atemwegs- und Hauterkrankungen, die mit Diisocyanaten im Zusammenhang stehen;\nc) nationale Expositionsgrenzwerte bei Diisocyanaten, sofern vorhanden;\nd) Informationen über Vollzugsmaßnahmen im Zusammenhang mit dieser Beschränkung.\n10. Diese Beschränkung gilt unbeschadet anderer Rechtsvorschriften der Union über die Sicherheit und den Gesundheitsschutz der Arbeitnehmern am Arbeitsplatz.\n\n","1.2023年8月24日之后，不得作为单独的物质、作为其他物质的成分或以混合物形式，作为工业和专业用途投放市场，除非：\n(a)二异氰酸酯的单独和组合浓度（重量）低于0.1%；\n(b)或雇主/自营职业者确保工业或专业用户在使用该物质或混合物之前已成功完成关于安全使用二异氰酸酯的培训。\n2.在2022年2月24日之后，不得作为单独的物质、作为其他物质的成分或以混合物形式，作为工业和专业用途投放市场，除非：\n(a)二异氰酸酯的单独和组合浓度低于0.1%（重量）；\n(b)或供应商确保向该物质或混合物的接收者提供关于第1项(b)条要求的信息，并在包装上以明显区别于其他标签信息的方式作出以下说明：\"从2023年8月24日起，在工业或专业使用前需要进行充分的培训\"。\n3.在本条目中，\"工业和专业用户\"是指出于工业和专业用途，对二异氰酸酯自行处理、作为其他物质的成分或混合物使用的任何工人或自营职业者，以及对这些工作进行监督的管理者。\n4.在不影响任何国家职业接触限值或国家一级其他适当的风险管理措施的情况下，第1项(b)条提及的培训应包括对工作场所控制皮肤和吸入接触二异氰酸酯的说明。这种培训应由具有相关职业培训能力的职业安全和健康专家进行。这种培训应至少包括：\n(a)第5项(a)条关于所有工业和专业用途的培训内容；\n(b)针对以下用途的第5项(a)和(b)条的培训内容：\n- 在环境温度下处理开放式混合物（包括泡沫隧道）\n- 在通风的喷房中进行喷涂\n- 使用滚筒\n- 使用刷子\n- 浸泡和浇注\n- 在降温后对未完全固化的物品进行机械性的后期处理（如切割）\n- 清洁和废料处理\n- 通过皮肤和/或吸入途径产生类似接触的任何其他用途\n(c) 第5项(a)、(b)和(c)点的培训内容，用于以下用途：\n- 处理未完全固化的物品（例如，刚固化的、未降温的）\n- 在铸造厂的应用\n- 对需要接触设备的维护和修理\n- 露天处理温热或高温的制剂（>45 °C）。\n- 在露天、有限或只有自然通风的情况下进行喷涂（包括大型工业工作车间）和高能量的喷涂（如泡沫、弹性体）\n- 以及任何其他通过皮肤和/或吸入途径有类似接触的用途。\n5. 培训内容：\n(a) 一般培训，包括在线培训，内容包括\n- 二异氰酸酯的化学成分\n- 毒性危害（包括急性毒性）\n- 二异氰酸酯的接触方式\n- 职业性接触限值\n- 敏感化是如何形成的\n- 气味作为危险的标志\n- 挥发性对风险的重要性\n- 二异氰酸酯的粘度、温度和分子量\n- 个人卫生\n- 所需的个人防护设备，包括正确使用的实用说明及其限制\n- 皮肤接触和吸入的风险\n- 与所使用的应用过程有关的风险\n- 皮肤和吸入保护方案\n- 通风\n- 清洁、泄漏、维护\n- 空包装丢弃\n- 对旁观者的保护\n- 关键处理阶段的识别\n- 具体的国家规范系统（如果适用）\n- 基于行为的安全\n- 已成功完成培训的证书或文件证明\n(b) 中级培训，包括在线培训，内容包括：\n- 基于行为的其他方面\n- 维护\n- 应变管理\n- 对现有安全指示的评估\n- 与所使用的应用程序有关的风险\n- 顺利完成培训的证明或文件证明\n(c) 高级培训，包括在线培训，内容包括：\n- 涵盖的具体用途所需的任何额外认证\n- 在喷漆室外进行喷漆\n- 公开处理高温或温热配方（>45℃）\n- 已成功完成培训的证书或文件证明\n6. 培训应符合工业或专业用户所在成员国的规定。只要符合第4和第5项规定的最低要求，成员国可以实施或继续实施其本国对该物质或混合物的使用要求。\n7.第2项(b)条中提到的供应商应确保根据第4项和第5项，以供应该物质或混合物的成员国的官方语言向接受者提供培训材料和课程。培训应考虑到所供应产品的特殊性，包括成分、包装和设计。\n8.雇主或自营职业者应记录成功完成第4和第5项所述培训的情况。培训应至少每五年更新一次。\n9.成员国应在其根据第117条第1款提交的报告中包括以下信息\n(a)国家法律中规定的与二异氰酸酯的工业和专业用途有关的任何既定培训要求和其他风险管理措施\n(b)与二异氰酸酯有关的已报告和已确认的职业性哮喘和职业性呼吸道及皮肤病的病例数\n(c) 国家对二异氰酸酯的接触限制，如果有的话\n(d) 与该限制有关的执法活动的信息\n10.本限制不应影响欧盟关于保护工人在工作场所的安全和健康的其他立法。"]
[null,{"$f":"IF($B$1=\"English\",C1735,IF($B$1=\"Deutsch\",D1735,IF($B$1=\"中文\",E1735,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0 % by weight"},"0 % by weight","0 Gew.%","0 %（按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1736,IF($B$1=\"Deutsch\",D1736,IF($B$1=\"中文\",E1736,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,0001 % by weight"},"0,0001 % by weight","0,0001 Gew.%","0.0001 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1737,IF($B$1=\"Deutsch\",D1737,IF($B$1=\"中文\",E1737,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,0003 % by weight"},"0,0003 % by weight","0,0003 Gew.%","0.0003 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1738,IF($B$1=\"Deutsch\",D1738,IF($B$1=\"中文\",E1738,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,0005 % by weight"},"0,0005 % by weight","0,0005 Gew.%","0.0005 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1739,IF($B$1=\"Deutsch\",D1739,IF($B$1=\"中文\",E1739,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,003 % by weight"},"0,003 % by weight","0,003 Gew.%","0.003 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1740,IF($B$1=\"Deutsch\",D1740,IF($B$1=\"中文\",E1740,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,005 % by weight"},"0,005 % by weight","0,005 Gew.%","0.005 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1741,IF($B$1=\"Deutsch\",D1741,IF($B$1=\"中文\",E1741,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,01 % by weight"},"0,01 % by weight","0,01 Gew.%","0.01 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1742,IF($B$1=\"Deutsch\",D1742,IF($B$1=\"中文\",E1742,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,02 % by weight"},"0,02 % by weight","0,02 Gew.%","0.02 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1743,IF($B$1=\"Deutsch\",D1743,IF($B$1=\"中文\",E1743,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,05 % by weight"},"0,05 % by weight","0,05 Gew.%","0.05 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1744,IF($B$1=\"Deutsch\",D1744,IF($B$1=\"中文\",E1744,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % by weight"},"0,1 % by weight","0,1 Gew.%","0.1 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1745,IF($B$1=\"Deutsch\",D1745,IF($B$1=\"中文\",E1745,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 % by weight \n(Repro. Tox: 0,3 % by weight)"},"0,1 % by weight \n(Repro. Tox: 0,3 % by weight)","0,1 Gew.% (Repro. Tox: 0,3 Gew.%)","0.1 % （按重量计）\n（生殖毒性：0.3 % 按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1746,IF($B$1=\"Deutsch\",D1746,IF($B$1=\"中文\",E1746,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mg/kg"},"0,1 mg/kg","0,1 mg/kg","0.1 mg/kg"]
[null,{"$f":"IF($B$1=\"English\",C1747,IF($B$1=\"Deutsch\",D1747,IF($B$1=\"中文\",E1747,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,3 % by weight"},"0,3 % by weight","0,3 Gew.%","0.3 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1748,IF($B$1=\"Deutsch\",D1748,IF($B$1=\"中文\",E1748,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,6 % by weight"},"0,6 % by weight","0,6 Gew.%","0.6 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1749,IF($B$1=\"Deutsch\",D1749,IF($B$1=\"中文\",E1749,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1 % by weight"},"1 % by weight","1 Gew.%","1 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1750,IF($B$1=\"Deutsch\",D1750,IF($B$1=\"中文\",E1750,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2 ppb"},"2 ppb","2 ppb","2 ppb"]
[null,{"$f":"IF($B$1=\"English\",C1751,IF($B$1=\"Deutsch\",D1751,IF($B$1=\"中文\",E1751,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3 % by weight"},"3 % by weight","3 Gew.%","3 % （按重量计）"]
[null,{"$f":"IF($B$1=\"English\",C1752,IF($B$1=\"Deutsch\",D1752,IF($B$1=\"中文\",E1752,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit values according to Appendix 12"},"Limit values according to Appendix 12","Grenzwerte entsprechend der Anlage 12","根据附录12规定的极限值"]
[null,{"$f":"IF($B$1=\"English\",C1753,IF($B$1=\"Deutsch\",D1753,IF($B$1=\"中文\",E1753,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated Substance"},"Regulated Substance","Reglementierte Inhaltsstoffe","受管制物质"]
[null,{"$f":"IF($B$1=\"English\",C1754,IF($B$1=\"Deutsch\",D1754,IF($B$1=\"中文\",E1754,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS No."},"CAS No.","CAS-Nummer","CAS号码"]
[null,{"$f":"IF($B$1=\"English\",C1755,IF($B$1=\"Deutsch\",D1755,IF($B$1=\"中文\",E1755,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Date of inclusion"},"Date of inclusion","Aufnahmedatum","纳入日期"]
[null,{"$f":"IF($B$1=\"English\",C1756,IF($B$1=\"Deutsch\",D1756,IF($B$1=\"中文\",E1756,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Restriction conditions; to see more text please press \"Show extract\""},"Restriction conditions; to see more text please press \"Show extract\"","Beschränkungsbedingunen: um mehr Text zu sehen bitte '' Auszug anzeigen'' drücken","限制条件；要看更多的文字，请按 \"显示摘要\""]
[null,{"$f":"IF($B$1=\"English\",C1757,IF($B$1=\"Deutsch\",D1757,IF($B$1=\"中文\",E1757,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Examples occurence"},"Examples occurence","Beispiele Vorkommen","出现的例子"]
[null,{"$f":"IF($B$1=\"English\",C1758,IF($B$1=\"Deutsch\",D1758,IF($B$1=\"中文\",E1758,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Annex XIV requirements"},"Annex XIV requirements","Annex XIV Bestimmungen","附件XIV的要求"]
[null,{"$f":"IF($B$1=\"English\",C1759,IF($B$1=\"Deutsch\",D1759,IF($B$1=\"中文\",E1759,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"SCIP-ID"},"SCIP-ID","SCIP-ID","在SCIP(物品或复杂物体（产品）中的高关注物质数据系统)中的编号（ID）"]
[null,{"$f":"IF($B$1=\"English\",C1760,IF($B$1=\"Deutsch\",D1760,IF($B$1=\"中文\",E1760,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration (specify unit)"},"Concentration (specify unit)","Konzentration [Einheit angeben]","浓度[指定单位] "]
[null,{"$f":"IF($B$1=\"English\",C1761,IF($B$1=\"Deutsch\",D1761,IF($B$1=\"中文\",E1761,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Part name of the specific part (in case of complex parts), regulated substance is contained."},"Part name of the specific part (in case of complex parts), regulated substance is contained.","Name des spezifischen Bauteils (bei zusammengesetzen Bauteilen), in dem der gegulierte Inhaltsstoff enthalten ist. ","含有受管制物质的特定部件（如果是复杂部件）的部件名称"]
[null,{"$f":"IF($B$1=\"English\",C1762,IF($B$1=\"Deutsch\",D1762,IF($B$1=\"中文\",E1762,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TARIC Code "},"TARIC Code ","TARIC Code ","TARIC码"]
[null,{"$f":"IF($B$1=\"English\",C1763,IF($B$1=\"Deutsch\",D1763,IF($B$1=\"中文\",E1763,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Kommentare","评论"]
[null,{"$f":"IF($B$1=\"English\",C1764,IF($B$1=\"Deutsch\",D1764,IF($B$1=\"中文\",E1764,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry included (E), changed (C)"},"Entry included (E), changed (C)","Eintrag aufgenommen E, geändert (C)","包括的条目(E)，改变的条目©"]
[null,{"$f":"IF($B$1=\"English\",C1765,IF($B$1=\"Deutsch\",D1765,IF($B$1=\"中文\",E1765,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1330-43-4, (anhydrous)\n12179-04-3, (pentahydrate)\n1303-96-4, (decahydrate)"},"1330-43-4, (anhydrous)\n12179-04-3, (pentahydrate)\n1303-96-4, (decahydrate)","1330-43-4, (wasserfrei)\n12179-04-3, (Pentahydrat)\n1303-96-4, (Decahydrat)","1330-43-4, (无水)\n12179-04-3, (五水)\n1303-96-4, (十水)"]
[null,{"$f":"IF($B$1=\"English\",C1766,IF($B$1=\"Deutsch\",D1766,IF($B$1=\"中文\",E1766,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Triethyl arsenate"},"Triethyl arsenate","Triethylarsenat","砷酸三乙酯"]
[null,{"$f":"IF($B$1=\"English\",C1767,IF($B$1=\"Deutsch\",D1767,IF($B$1=\"中文\",E1767,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium dichromate\ndihydrat and anhydrid"},"Sodium dichromate\ndihydrat and anhydrid","Natriumdichromat\n[dihydrat und anhydrid]","重铬酸钠\n二水和无水"]
[null,{"$f":"IF($B$1=\"English\",C1768,IF($B$1=\"Deutsch\",D1768,IF($B$1=\"中文\",E1768,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diarsenic Pentaoxide"},"Diarsenic Pentaoxide","Diarsenpentaoxid","五氧化二砷"]
[null,{"$f":"IF($B$1=\"English\",C1769,IF($B$1=\"Deutsch\",D1769,IF($B$1=\"中文\",E1769,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diarsenic Trioxide"},"Diarsenic Trioxide","Diarsentrioxid","三氧化二砷"]
[null,{"$f":"IF($B$1=\"English\",C1770,IF($B$1=\"Deutsch\",D1770,IF($B$1=\"中文\",E1770,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyl phthalate (DBP)"},"Dibutyl phthalate (DBP)","Dibutylphthalat (DBP)","邻苯二甲酸二丁酯 (DBP)"]
[null,{"$f":"IF($B$1=\"English\",C1771,IF($B$1=\"Deutsch\",D1771,IF($B$1=\"中文\",E1771,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(tributyltin) oxide (TBTO)"},"Bis(tributyltin) oxide (TBTO)","Bis(tributylzinn)oxid (TBTO)","三丁基氧化锡  (TBTO)"]
[null,{"$f":"IF($B$1=\"English\",C1772,IF($B$1=\"Deutsch\",D1772,IF($B$1=\"中文\",E1772,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead hydrogen arsenate"},"Lead hydrogen arsenate","Bleihydrogenarsenat","砷酸氢铅"]
[null,{"$f":"IF($B$1=\"English\",C1773,IF($B$1=\"Deutsch\",D1773,IF($B$1=\"中文\",E1773,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene"},"Anthracene","Anthracen","蒽"]
[null,{"$f":"IF($B$1=\"English\",C1774,IF($B$1=\"Deutsch\",D1774,IF($B$1=\"中文\",E1774,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzyl butyl phthalate (BBP)"},"Benzyl butyl phthalate (BBP)","Benzylbutylphthalat (BBP)","邻苯二甲酸丁基苄酯（BBP）"]
[null,{"$f":"IF($B$1=\"English\",C1775,IF($B$1=\"Deutsch\",D1775,IF($B$1=\"中文\",E1775,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4’-Diaminodiphenylmethan (MDA)"},"4,4’-Diaminodiphenylmethan (MDA)","4,4'-Methylendianilin (MDA)","4,4'-二氨基二苯甲烷 (MDA)"]
[null,{"$f":"IF($B$1=\"English\",C1776,IF($B$1=\"Deutsch\",D1776,IF($B$1=\"中文\",E1776,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-tert-butyl-2,4,6-trinitro-m-xylene (musk xylene)"},"5-tert-butyl-2,4,6-trinitro-m-xylene (musk xylene)","5-tert-Butyl-2,4,6-trinitro-m-xylol (Xylolmoschus)","5-叔丁基-2,4,6-三硝基-间二甲苯（麝香二甲苯）"]
[null,{"$f":"IF($B$1=\"English\",C1777,IF($B$1=\"Deutsch\",D1777,IF($B$1=\"中文\",E1777,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C10-13, chloro (Short Chain Chlorinated Paraffins)"},"Alkanes, C10-13, chloro (Short Chain Chlorinated Paraffins)","Alkane, C10-13, Chlor (kurzkettige chlorierte Paraffine)","Alkanes, C10-13, chloro (Short Chain Chlorinated Paraffins)"]
[null,{"$f":"IF($B$1=\"English\",C1778,IF($B$1=\"Deutsch\",D1778,IF($B$1=\"中文\",E1778,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromocyclododecane (HBCDD) and all major diastereoisomeric identified compounds: "},"Hexabromocyclododecane (HBCDD) and all major diastereoisomeric identified compounds: ","Hexabromcyclododecan (HBCDD) und alle größeren identifizierten diastereoisomeren Verbindungen: \n\n\n","六溴环十二烷（HBCDD）和所有主要的非对映异构体化合物"]
[null,{"$f":"IF($B$1=\"English\",C1779,IF($B$1=\"Deutsch\",D1779,IF($B$1=\"中文\",E1779,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromocyclododecane"},"Hexabromocyclododecane","Hexabromocyclododecan","六溴环十二烷"]
[null,{"$f":"IF($B$1=\"English\",C1780,IF($B$1=\"Deutsch\",D1780,IF($B$1=\"中文\",E1780,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,5,6,9,10-hexabromocyclododecane"},"1,2,5,6,9,10-hexabromocyclododecane","1,2,5,6,9,10-Hexabromocyclododecan","1,2,5,6,9,10-六溴环十二烷"]
[null,{"$f":"IF($B$1=\"English\",C1781,IF($B$1=\"Deutsch\",D1781,IF($B$1=\"中文\",E1781,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"alpha-hexabromocyclododecane"},"alpha-hexabromocyclododecane","α-Hexabromcyclododecan","α-六溴环十二烷"]
[null,{"$f":"IF($B$1=\"English\",C1782,IF($B$1=\"Deutsch\",D1782,IF($B$1=\"中文\",E1782,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"beta-hexabromocyclododecane"},"beta-hexabromocyclododecane","β-Hexabromcyclododecan","β-六溴环十二烷"]
[null,{"$f":"IF($B$1=\"English\",C1783,IF($B$1=\"Deutsch\",D1783,IF($B$1=\"中文\",E1783,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"gamma-hexabromocyclododecane"},"gamma-hexabromocyclododecane","γ-Hexabromcyclododecan","γ-六溴环十二烷"]
[null,{"$f":"IF($B$1=\"English\",C1784,IF($B$1=\"Deutsch\",D1784,IF($B$1=\"中文\",E1784,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris (2-chloroethyl) phosphate"},"Tris (2-chloroethyl) phosphate","Tris(2-chlorethyl)phosphat","磷酸三(2-氯乙基)酯"]
[null,{"$f":"IF($B$1=\"English\",C1785,IF($B$1=\"Deutsch\",D1785,IF($B$1=\"中文\",E1785,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Coal tar pitch, high temperature"},"Coal tar pitch, high temperature","Pech, Kohlenteer, Hochtemperatur","煤焦油沥青，高温"]
[null,{"$f":"IF($B$1=\"English\",C1786,IF($B$1=\"Deutsch\",D1786,IF($B$1=\"中文\",E1786,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisobutyl phthalate (DIBP)"},"Diisobutyl phthalate (DIBP)","Diisobutylphthalat","邻苯二甲酸二异丁酯（DIBP）"]
[null,{"$f":"IF($B$1=\"English\",C1787,IF($B$1=\"Deutsch\",D1787,IF($B$1=\"中文\",E1787,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead sulfochromate yellow (C.I. Pigment Yellow 34)"},"Lead sulfochromate yellow (C.I. Pigment Yellow 34)","Bleisulfochromatgelb (C.I. Pigment Gelb 34)","铅铬黄（ C.I.颜料黄 34）"]
[null,{"$f":"IF($B$1=\"English\",C1788,IF($B$1=\"Deutsch\",D1788,IF($B$1=\"中文\",E1788,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead chromate"},"Lead chromate","Bleichromat","铬酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1789,IF($B$1=\"Deutsch\",D1789,IF($B$1=\"中文\",E1789,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead chromate molybdate sulfate red (C.I. Pigment Red 104)"},"Lead chromate molybdate sulfate red (C.I. Pigment Red 104)","Bleichromatmolybdatsulfatrot (C.I. Pigment Rot 104)","钼铬红(C.I.颜料红 104)"]
[null,{"$f":"IF($B$1=\"English\",C1790,IF($B$1=\"Deutsch\",D1790,IF($B$1=\"中文\",E1790,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4 - Dinitrotoluene (2,4-DNT)"},"2,4 - Dinitrotoluene (2,4-DNT)","2,4-Dinitrotoluol","2,4 - 二硝基甲苯 (2,4-DNT)"]
[null,{"$f":"IF($B$1=\"English\",C1791,IF($B$1=\"Deutsch\",D1791,IF($B$1=\"中文\",E1791,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene-low"},"Anthracene oil, anthracene-low","Anthracenöl, Anthracenfrei","蒽油、蒽-低含量"]
[null,{"$f":"IF($B$1=\"English\",C1792,IF($B$1=\"Deutsch\",D1792,IF($B$1=\"中文\",E1792,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene paste, anthracene  fraction\n"},"Anthracene oil, anthracene paste, anthracene  fraction\n","Anthracenöl, Anthracenpaste, Anthracenfraktion","蒽油、蒽糊、蒽馏分"]
[null,{"$f":"IF($B$1=\"English\",C1793,IF($B$1=\"Deutsch\",D1793,IF($B$1=\"中文\",E1793,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene paste, distn. Lights"},"Anthracene oil, anthracene paste, distn. Lights","Anthracenöl, Anthracenpaste, leichte Destillate","蒽油、蒽糊、 轻馏分 "]
[null,{"$f":"IF($B$1=\"English\",C1794,IF($B$1=\"Deutsch\",D1794,IF($B$1=\"中文\",E1794,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil, anthracene paste"},"Anthracene oil, anthracene paste","Anthracenöl, Anthracenpaste","蒽油、蒽糊"]
[null,{"$f":"IF($B$1=\"English\",C1795,IF($B$1=\"Deutsch\",D1795,IF($B$1=\"中文\",E1795,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oil"},"Anthracene oil","Anthracenöl","蒽油"]
[null,{"$f":"IF($B$1=\"English\",C1796,IF($B$1=\"Deutsch\",D1796,IF($B$1=\"中文\",E1796,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acrylamide"},"Acrylamide","Acrylamid","丙烯酰胺 "]
[null,{"$f":"IF($B$1=\"English\",C1797,IF($B$1=\"Deutsch\",D1797,IF($B$1=\"中文\",E1797,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetraboron disodium heptaoxide, hydrate"},"Tetraboron disodium heptaoxide, hydrate","Tetrabordinatriumheptaoxid, Hydrat","水合四硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1798,IF($B$1=\"Deutsch\",D1798,IF($B$1=\"中文\",E1798,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichloroethylene"},"Trichloroethylene","Trichlorethen","三氯乙烯"]
[null,{"$f":"IF($B$1=\"English\",C1799,IF($B$1=\"Deutsch\",D1799,IF($B$1=\"中文\",E1799,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium chromate"},"Sodium chromate","Natriumchromat","重铬酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1800,IF($B$1=\"Deutsch\",D1800,IF($B$1=\"中文\",E1800,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium tetraborate, anhydrous"},"Disodium tetraborate, anhydrous","Dinatriumtetraborat, wasserfrei","无水四硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1801,IF($B$1=\"Deutsch\",D1801,IF($B$1=\"中文\",E1801,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium chromate"},"Potassium chromate","Kaliumchromat","铬酸钾"]
[null,{"$f":"IF($B$1=\"English\",C1802,IF($B$1=\"Deutsch\",D1802,IF($B$1=\"中文\",E1802,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium dichromate"},"Potassium dichromate","Kaliumdichromat","重铬酸钾"]
[null,{"$f":"IF($B$1=\"English\",C1803,IF($B$1=\"Deutsch\",D1803,IF($B$1=\"中文\",E1803,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid"},"Boric acid","Borsäure","硼酸"]
[null,{"$f":"IF($B$1=\"English\",C1804,IF($B$1=\"Deutsch\",D1804,IF($B$1=\"中文\",E1804,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid"},"Boric acid","Borsäure","硼酸"]
[null,{"$f":"IF($B$1=\"English\",C1805,IF($B$1=\"Deutsch\",D1805,IF($B$1=\"中文\",E1805,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid, crude natural"},"Boric acid, crude natural","Borsäure \n[crude natural]","硼酸，天然粗品"]
[null,{"$f":"IF($B$1=\"English\",C1806,IF($B$1=\"Deutsch\",D1806,IF($B$1=\"中文\",E1806,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium dichromate"},"Ammonium dichromate","Ammoniumdichromat","重铬酸铵"]
[null,{"$f":"IF($B$1=\"English\",C1807,IF($B$1=\"Deutsch\",D1807,IF($B$1=\"中文\",E1807,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acids generated from chromium trioxide and their oligomers [The group contains: Chromic acid, Chromic acid, Oligomers of chromic acid and dichromic acid]"},"Acids generated from chromium trioxide and their oligomers [The group contains: Chromic acid, Chromic acid, Oligomers of chromic acid and dichromic acid]","Säuren gebildet aus Chromtrioxid und ihre Oligomere ","由三氧化铬及其低聚物形成的酸 "]
[null,{"$f":"IF($B$1=\"English\",C1808,IF($B$1=\"Deutsch\",D1808,IF($B$1=\"中文\",E1808,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromic acid"},"Chromic acid","Chromsäure","铬酸"]
[null,{"$f":"IF($B$1=\"English\",C1809,IF($B$1=\"Deutsch\",D1809,IF($B$1=\"中文\",E1809,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Oligomers of chromic acid and dichromic acid"},"Oligomers of chromic acid and dichromic acid","Oligomere der Chromsäure und der Dichromsäure","铬酸和重铬酸的低聚物"]
[null,{"$f":"IF($B$1=\"English\",C1810,IF($B$1=\"Deutsch\",D1810,IF($B$1=\"中文\",E1810,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichromic acid"},"Dichromic acid","Dichromsäure","重铬酸"]
[null,{"$f":"IF($B$1=\"English\",C1811,IF($B$1=\"Deutsch\",D1811,IF($B$1=\"中文\",E1811,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) diacetate"},"Cobalt(II) diacetate","Kobalt(II)-diacetat","二乙酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C1812,IF($B$1=\"Deutsch\",D1812,IF($B$1=\"中文\",E1812,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) dinitrate"},"Cobalt(II) dinitrate","Kobalt(II)-dinitrat","二硝酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C1813,IF($B$1=\"Deutsch\",D1813,IF($B$1=\"中文\",E1813,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) carbonate"},"Cobalt(II) carbonate","Kobalt(II)-karbonat","碳酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C1814,IF($B$1=\"Deutsch\",D1814,IF($B$1=\"中文\",E1814,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) sulphate"},"Cobalt(II) sulphate","Kobalt(II)-sulfat","硫酸钴（II）"]
[null,{"$f":"IF($B$1=\"English\",C1815,IF($B$1=\"Deutsch\",D1815,IF($B$1=\"中文\",E1815,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium trioxide"},"Chromium trioxide","Chromtrioxid","三氧化铬"]
[null,{"$f":"IF($B$1=\"English\",C1816,IF($B$1=\"Deutsch\",D1816,IF($B$1=\"中文\",E1816,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Ethoxyethanol (ethylene glycol monoethyl ether; EGEE)"},"2-Ethoxyethanol (ethylene glycol monoethyl ether; EGEE)","2-Ethoxyethanol","2-乙氧基乙醇（乙二醇单乙基醚；EGEE）"]
[null,{"$f":"IF($B$1=\"English\",C1817,IF($B$1=\"Deutsch\",D1817,IF($B$1=\"中文\",E1817,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyethanol (ethylene glycol monomethyl ether; EGME)"},"2-Methoxyethanol (ethylene glycol monomethyl ether; EGME)","2-Methoxyethanol","2-甲氧基乙醇（乙二醇单甲基醚；EGME）"]
[null,{"$f":"IF($B$1=\"English\",C1818,IF($B$1=\"Deutsch\",D1818,IF($B$1=\"中文\",E1818,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Strontium chromate"},"Strontium chromate","Strontiumchromat","铬酸锶"]
[null,{"$f":"IF($B$1=\"English\",C1819,IF($B$1=\"Deutsch\",D1819,IF($B$1=\"中文\",E1819,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydrazine"},"Hydrazine","Hydrazin","肼 "]
[null,{"$f":"IF($B$1=\"English\",C1820,IF($B$1=\"Deutsch\",D1820,IF($B$1=\"中文\",E1820,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt dichloride\n\nCobalt dichloride was originally added to the candidate list as a SVHC substance on 28.10.2008. The entry was supplemented on 20.06.2011 by the reprotoxic properties."},"Cobalt dichloride\n\nCobalt dichloride was originally added to the candidate list as a SVHC substance on 28.10.2008. The entry was supplemented on 20.06.2011 by the reprotoxic properties.","Kobaltdichlorid \n\nKobaltdichlorid wurde ursprünglich als SVHC-Stoff am 28.10.2008 in die Kandidatenliste aufgenommen. Der Eintrag wurde am 20.06.2011 um die fortpflanzungsgefährdenden Eigenschaften ergänzt.","二氯化钴\n\n二氯化钴最初于2008年10月28日作为高危物质被列入候选名单。该条目在2011年6月20日被补充为生殖毒性物质。"]
[null,{"$f":"IF($B$1=\"English\",C1821,IF($B$1=\"Deutsch\",D1821,IF($B$1=\"中文\",E1821,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-ethoxyethyl acetate (2-EEA)"},"2-ethoxyethyl acetate (2-EEA)","2-Ethoxyethylacetat (2-EEA)","乙二醇乙醚醋酸酯 (2-EEA)"]
[null,{"$f":"IF($B$1=\"English\",C1822,IF($B$1=\"Deutsch\",D1822,IF($B$1=\"中文\",E1822,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,3-trichloropropane"},"1,2,3-trichloropropane","1,2,3-Trichlorpropan","1,2,3-三氯丙烷"]
[null,{"$f":"IF($B$1=\"English\",C1823,IF($B$1=\"Deutsch\",D1823,IF($B$1=\"中文\",E1823,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl esters, C7-rich"},"1,2-Benzenedicarboxylic acid, di-C6-8-branched alkyl esters, C7-rich","1,2-Benzoldicarbonsäure, Di-C6-8-verzweigte Alkylester, C7-reich (DIHP)","邻苯二甲酸二C6-8支链烷基酯(富C7) "]
[null,{"$f":"IF($B$1=\"English\",C1824,IF($B$1=\"Deutsch\",D1824,IF($B$1=\"中文\",E1824,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C7-11 -branched and linear alkyl esters\n(DHNUP)"},"1,2-Benzenedicarboxylic acid, di-C7-11 -branched and linear alkyl esters\n(DHNUP)","1,2-Benzoldicarbonsäure, Di-C7-11-verzweigte und lineare Alkylester (DHNUP)","1,2-苯二甲酸，二-C7-11-支链和直链烷基酯\n(DHNUP)"]
[null,{"$f":"IF($B$1=\"English\",C1825,IF($B$1=\"Deutsch\",D1825,IF($B$1=\"中文\",E1825,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Methyl-2-pyrrolidon (NMP)"},"1-Methyl-2-pyrrolidon (NMP)","1-Methyl-2-pyrrolidon (NMP)","1-甲基-2-吡咯烷酮 (NMP)"]
[null,{"$f":"IF($B$1=\"English\",C1826,IF($B$1=\"Deutsch\",D1826,IF($B$1=\"中文\",E1826,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead diarsenate"},"Trilead diarsenate","Tribleidiarsenat","砷酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1827,IF($B$1=\"Deutsch\",D1827,IF($B$1=\"中文\",E1827,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Zirconia Aluminosilicate Refractory Ceramic Fibres\n\nRefractory zirconium-aluminosilicate ceramic fibres are fibres listed under index number 650-017-00-8 in Annex VI, Part 3, Table 3.1 of Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on the classification, labelling and packaging of substances and mixtures and meet the three following conditions:\n\na. The oxides of aluminium, silicon and zirconium are the main components that occur (in the fibres) in variable concentration ranges\n\nb. The fibres have a length-weighted mean geometric diameter minus twice the geometric standard deviation of 6 or less micrometers (µm)\n\nc. The content of alkali and alkaline earth metal oxides (Na2O+K2O+CaO+MgO+BaO) is less than or equal to 18% by weight."},"Zirconia Aluminosilicate Refractory Ceramic Fibres\n\nRefractory zirconium-aluminosilicate ceramic fibres are fibres listed under index number 650-017-00-8 in Annex VI, Part 3, Table 3.1 of Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on the classification, labelling and packaging of substances and mixtures and meet the three following conditions:\n\na. The oxides of aluminium, silicon and zirconium are the main components that occur (in the fibres) in variable concentration ranges\n\nb. The fibres have a length-weighted mean geometric diameter minus twice the geometric standard deviation of 6 or less micrometers (µm)\n\nc. The content of alkali and alkaline earth metal oxides (Na2O+K2O+CaO+MgO+BaO) is less than or equal to 18% by weight.","Zirconium-Aluminiumsilikat-Keramikfasern, feuerfest\nFeuerfeste Zirconium-Aluminiumsilikat-Keramikfasern sind Fasern, die unter der Index-Nummer 650-017-00-8 in Anhang VI, Teil 3, Tabelle 3.1 der Verordnung (EG) Nr. 1272/2008 des Europäischen Parlaments und des Rates vom 16. Dezember 2008 über die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen erfasst sind und die drei folgenden Bedingungen erfüllen:\n\na. Die Oxide von Aluminium, Silizium und Zirconium sind die Hauptkomponenten, die (in den Fasern) in variablen Konzentrationsbereichen vorkommen\n\nb. Die Fasern haben einen längengewichteten mittleren geometrischen Durchmesser abzüglich der zweifachen geometrischen Standardabweichung von 6 oder weniger Mikrometern (µm)\n\nc. Der Gehalt an Alkali- und Erdalkalimetalloxiden (Na2O+K2O+CaO+MgO+BaO) liegt unter oder ist gleich 18 Gewichtsprozent","氧化锆硅酸铝耐火陶瓷纤维\n\n耐火锆硅酸盐陶瓷纤维是指2008年12月16日欧洲议会和理事会关于物质和混合物分类、标签和包装的(EC)1272/2008号法规附件六第三部分表3.1中索引号650-017-00-8所列的纤维，并符合以下三个条件。\n\na. 铝、硅和锆的氧化物是（在纤维中）以不同浓度范围出现的主要成分\n\nb. 纤维的长度加权平均几何直径减去两倍的几何标准偏差为6微米或以下\n\nc. 碱和碱土金属氧化物（Na2O+K2O+CaO+MgO+BaO）的含量按重量计算小于或等于18%。"]
[null,{"$f":"IF($B$1=\"English\",C1828,IF($B$1=\"Deutsch\",D1828,IF($B$1=\"中文\",E1828,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aluminosilicate refractory ceramic fibres"},"Aluminosilicate refractory ceramic fibres","Feuerfeste Zirconium-Aluminiumsilikat-Keramikfasern","硅酸铝耐火陶瓷纤维"]
[null,{"$f":"IF($B$1=\"English\",C1829,IF($B$1=\"Deutsch\",D1829,IF($B$1=\"中文\",E1829,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenolphthalein"},"Phenolphthalein","Phenolphthalein","酚酞"]
[null,{"$f":"IF($B$1=\"English\",C1830,IF($B$1=\"Deutsch\",D1830,IF($B$1=\"中文\",E1830,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentazinc chromate octahydroxide"},"Pentazinc chromate octahydroxide","Pentazinkchromat-octahydroxid","锌黄"]
[null,{"$f":"IF($B$1=\"English\",C1831,IF($B$1=\"Deutsch\",D1831,IF($B$1=\"中文\",E1831,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde, oligomeric reaction products with aniline\ntechnical MDA"},"Formaldehyde, oligomeric reaction products with aniline\ntechnical MDA","Formaldehyd, oligomeres Reaktionsprodukt mit Anilin\ntechnisches MDA","甲醛，与苯胺的低聚反应产物\n工业用MDA"]
[null,{"$f":"IF($B$1=\"English\",C1832,IF($B$1=\"Deutsch\",D1832,IF($B$1=\"中文\",E1832,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium hydroxyoctaoxodizincatedichromate(1-)"},"Potassium hydroxyoctaoxodizincatedichromate(1-)","Kaliumhydroxyoctaoxo-dizinkat-dichromat","氢氧化铬酸锌钾(1-)"]
[null,{"$f":"IF($B$1=\"English\",C1833,IF($B$1=\"Deutsch\",D1833,IF($B$1=\"中文\",E1833,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N-Dimethylacetamide (DMAC)"},"N,N-Dimethylacetamide (DMAC)","N,N-Dimethylacetamid (DMAC)","N,N-二甲基乙酰胺 (DMAC)"]
[null,{"$f":"IF($B$1=\"English\",C1834,IF($B$1=\"Deutsch\",D1834,IF($B$1=\"中文\",E1834,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Calcium arsenate"},"Calcium arsenate","Calciumarsenat","砷酸钙"]
[null,{"$f":"IF($B$1=\"English\",C1835,IF($B$1=\"Deutsch\",D1835,IF($B$1=\"中文\",E1835,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichromium tris(chromate)"},"Dichromium tris(chromate)","Dichromtris(chromat)","二铬 三铬（铬酸盐）"]
[null,{"$f":"IF($B$1=\"English\",C1836,IF($B$1=\"Deutsch\",D1836,IF($B$1=\"中文\",E1836,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead diazide, Lead azide"},"Lead diazide, Lead azide","Bleidiazid, \nBleiazid","迭氮化铅"]
[null,{"$f":"IF($B$1=\"English\",C1837,IF($B$1=\"Deutsch\",D1837,IF($B$1=\"中文\",E1837,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead dipicrate"},"Lead dipicrate","Bleidipikrat","三硝基苯酚铅"]
[null,{"$f":"IF($B$1=\"English\",C1838,IF($B$1=\"Deutsch\",D1838,IF($B$1=\"中文\",E1838,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead 2,4,6-trinitro-m-phenylene dioxide (lead styphnate)"},"Lead 2,4,6-trinitro-m-phenylene dioxide (lead styphnate)","Bleistyphnat","2,4,6-三硝基间苯二甲酸铅(苯乙烯酸铅)"]
[null,{"$f":"IF($B$1=\"English\",C1839,IF($B$1=\"Deutsch\",D1839,IF($B$1=\"中文\",E1839,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Arsenic acid"},"Arsenic acid","Arsensäure","亚砷酸"]
[null,{"$f":"IF($B$1=\"English\",C1840,IF($B$1=\"Deutsch\",D1840,IF($B$1=\"中文\",E1840,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl) ether (Diglyme)"},"Bis(2-methoxyethyl) ether (Diglyme)","Bis(2-methoxyethyl)ether","双(2-甲氧基乙基)醚(Diglyme)"]
[null,{"$f":"IF($B$1=\"English\",C1841,IF($B$1=\"Deutsch\",D1841,IF($B$1=\"中文\",E1841,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl)phthalate"},"Bis(2-methoxyethyl)phthalate","Bis(2-methoxyethyl)phthalat","双（2-甲氧基乙基）邻苯二甲酸酯"]
[null,{"$f":"IF($B$1=\"English\",C1842,IF($B$1=\"Deutsch\",D1842,IF($B$1=\"中文\",E1842,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyanilin (o-Anisidine)"},"2-Methoxyanilin (o-Anisidine)","2-Methoxyanilin (o-Anisidin)","2-甲氧基苯胺(邻氨基苯酚)"]
[null,{"$f":"IF($B$1=\"English\",C1843,IF($B$1=\"Deutsch\",D1843,IF($B$1=\"中文\",E1843,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1,1,3,3-tetramethylbutyl)phenol\n4-tert-Octylphenol"},"4-(1,1,3,3-tetramethylbutyl)phenol\n4-tert-Octylphenol","4-(1,1,3,3-Tetramethylbutyl)phenol\n4-tert-Octylphenol","4-(1,1,3,3-四甲基丁基)苯酚\n4-叔辛基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C1844,IF($B$1=\"Deutsch\",D1844,IF($B$1=\"中文\",E1844,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aluminosilicate Refractory Ceramic Fibres\n\nRefractory aluminosilicate ceramic fibres are fibres listed under index number 650-017-00-8 in Annex VI, Part 3, Table 3.1 of Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on the classification, labelling and packaging of substances and mixtures and meet the following three conditions:\n\na. The oxides of aluminium and silicon are the main components that occur (in the fibres) in variable concentration ranges\n\nb. The fibres have a length-weighted mean geometric diameter minus twice the geometric standard deviation of 6 or less micrometers (µm)\n\nc. The content of alkali and alkaline earth metal oxides (Na2O+K2O+CaO+MgO+BaO) is less than or equal to 18% by weight."},"Aluminosilicate Refractory Ceramic Fibres\n\nRefractory aluminosilicate ceramic fibres are fibres listed under index number 650-017-00-8 in Annex VI, Part 3, Table 3.1 of Regulation (EC) No 1272/2008 of the European Parliament and of the Council of 16 December 2008 on the classification, labelling and packaging of substances and mixtures and meet the following three conditions:\n\na. The oxides of aluminium and silicon are the main components that occur (in the fibres) in variable concentration ranges\n\nb. The fibres have a length-weighted mean geometric diameter minus twice the geometric standard deviation of 6 or less micrometers (µm)\n\nc. The content of alkali and alkaline earth metal oxides (Na2O+K2O+CaO+MgO+BaO) is less than or equal to 18% by weight.","Aluminiumsilikat-Keramikfasern, feuerfest\nFeuerfeste Aluminiumsilikat-Keramikfasern sind Fasern, die unter der Index-Nummer 650-017-00-8 in Anhang VI, Teil 3, Tabelle 3.1 der Verordnung (EG) Nr. 1272/2008 des Europäischen Parlaments und des Rates vom 16. Dezember 2008 über die Einstufung, Kennzeichnung und Verpackung von Stoffen und Gemischen erfasst sind und die drei folgenden Bedingungen erfüllen:\n\na. Die Oxide von Aluminium und Silizium sind die Hauptkomponenten, die (in den Fasern) in variablen Konzentrationsbereichen vorkommen\n\nb. Die Fasern haben einen längengewichteten mittleren geometrischen Durchmesser abzüglich der zweifachen geometrischen Standardabweichung von 6 oder weniger Mikrometern (µm)\n\nc. Der Gehalt an Alkali- und Erdalkalimetalloxiden (Na2O+K2O+CaO+MgO+BaO) liegt unter oder ist gleich 18 Gewichtsprozent","硅酸铝耐火陶瓷纤维\n\n硅酸铝耐火陶瓷纤维是指2008年12月16日欧洲议会和理事会关于物质和混合物分类、标签和包装的(EC)1272/2008号法规附件六第三部分表3.1中索引号650-017-00-8所列的纤维，并满足以下三个条件。\n\na.铝和硅的氧化物是（在纤维中）以不同浓度范围出现的主要成分\n\nb.纤维的长度加权平均几何直径减去两倍的几何标准偏差为6微米或以下\n\nc.碱和碱土金属氧化物（Na2O+K2O+CaO+MgO+BaO）的含量按重量计算小于或等于18%。"]
[null,{"$f":"IF($B$1=\"English\",C1845,IF($B$1=\"Deutsch\",D1845,IF($B$1=\"中文\",E1845,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aluminosilicate refractory ceramic fibres"},"Aluminosilicate refractory ceramic fibres","Feuerfeste Aluminiumsilikat-Keramikfasern ","硅酸铝耐火陶瓷纤维"]
[null,{"$f":"IF($B$1=\"English\",C1846,IF($B$1=\"Deutsch\",D1846,IF($B$1=\"中文\",E1846,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dichloroethane"},"1,2-dichloroethane","1,2-Dichlorethan","1,2-二氯乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1847,IF($B$1=\"Deutsch\",D1847,IF($B$1=\"中文\",E1847,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2'-dichloro-4,4'-methylenedianiline (MOCA)"},"2,2'-dichloro-4,4'-methylenedianiline (MOCA)","2,2'-Dichlor-4,4'-methylendianilin","2,2'-二氯-4,4'-亚甲基苯胺 (MOCA)"]
[null,{"$f":"IF($B$1=\"English\",C1848,IF($B$1=\"Deutsch\",D1848,IF($B$1=\"中文\",E1848,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formamide"},"Formamide","Formamid","甲酰胺"]
[null,{"$f":"IF($B$1=\"English\",C1849,IF($B$1=\"Deutsch\",D1849,IF($B$1=\"中文\",E1849,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N,N',N'-tetramethyl-4,4'-methylenedianiline\n(Michler’s base)"},"N,N,N',N'-tetramethyl-4,4'-methylenedianiline\n(Michler’s base)","N,N,N',N'-Tetramethyl-4,4'-methylendianilin (Michler's Base)","4,4'-(对二甲氨基)二苯基甲烷(米氏碱)"]
[null,{"$f":"IF($B$1=\"English\",C1850,IF($B$1=\"Deutsch\",D1850,IF($B$1=\"中文\",E1850,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diboron trioxide"},"Diboron trioxide","Dibortrioxid","三氧化二硼"]
[null,{"$f":"IF($B$1=\"English\",C1851,IF($B$1=\"Deutsch\",D1851,IF($B$1=\"中文\",E1851,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead(II) bis(methanesulfonate)"},"Lead(II) bis(methanesulfonate)","Blei(II)bis(methansulfonat)","铅（II）二（甲磺酸）"]
[null,{"$f":"IF($B$1=\"English\",C1852,IF($B$1=\"Deutsch\",D1852,IF($B$1=\"中文\",E1852,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-bis(dimethylamino)-4''-(methylamino)trityl alcohol\nThe substance is proposed only where it contains Michler’s ketone (EC Number: 202-027-5) or/and Michler’s\nbase (EC Number: 202-959-2) ≥ 0.1% (wt/wt)"},"4,4'-bis(dimethylamino)-4''-(methylamino)trityl alcohol\nThe substance is proposed only where it contains Michler’s ketone (EC Number: 202-027-5) or/and Michler’s\nbase (EC Number: 202-959-2) ≥ 0.1% (wt/wt)","4,4'-Bis(dimethylamino)-4''-(methylamino)tritylalkohol\n[mit ≥ 0.1% Michler's Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","4,4'-二[(二甲氨基)苯基]-4-甲氨基苯甲醇\n仅指含有米氏酮（EC编号：202-027-5）或/和米氏碱（EC编号：202-959-2）≥0.1%（质量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C1853,IF($B$1=\"Deutsch\",D1853,IF($B$1=\"中文\",E1853,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-\nbis(dimethylamino)benzophenone (Michler’s ketone)"},"4,4'-\nbis(dimethylamino)benzophenone (Michler’s ketone)","4,4'-Bis(dimethylamino)benzophenon\n(Michler's Keton)","4,4'-二(N,N-二甲氨基)二苯甲酮（米氏酮）"]
[null,{"$f":"IF($B$1=\"English\",C1854,IF($B$1=\"Deutsch\",D1854,IF($B$1=\"中文\",E1854,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[4-[[4-anilino-1-naphthyl][4-\n(dimethylamino)phenyl]methylene]cyclohexa-2,5-dien-1-ylidene]\ndimethylammonium chloride (C.I. Basic Blue 26)"},"[4-[[4-anilino-1-naphthyl][4-\n(dimethylamino)phenyl]methylene]cyclohexa-2,5-dien-1-ylidene]\ndimethylammonium chloride (C.I. Basic Blue 26)","[4-[[4-Anilino-1-naphthyl][4-(dimethylamino)phenyl]methylen]cyclohexa-2,5-dien-1-yliden] dimethylammonium chlorid\n(C.I. Basic Blue 26) [mit ≥ 0.1% Michler's Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","[4 - [[4 - 苯胺基-1 - 萘基] [4 - （二甲基氨基）苯基]亚甲基]环己-2,5 - 二烯-1 - 亚基]二甲基氯化铵（碱性蓝26) "]
[null,{"$f":"IF($B$1=\"English\",C1855,IF($B$1=\"Deutsch\",D1855,IF($B$1=\"中文\",E1855,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[4-[4,4'-Bis(dimethylamino) benzhydryliden]cyclohexa-2,5-dien-1-yliden]dimethylammonium chlorid\n(C.I. Basic Violet 3) [mit ≥ 0.1% Michler's Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]"},"[4-[4,4'-Bis(dimethylamino) benzhydryliden]cyclohexa-2,5-dien-1-yliden]dimethylammonium chlorid\n(C.I. Basic Violet 3) [mit ≥ 0.1% Michler's Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","[4-[4,4'-Bis(dimethylamino) benzhydryliden]cyclohexa-2,5-dien-1-yliden]dimethylammonium chlorid\n(C.I. Basic Violet 3) [mit ≥ 0.1% Michler's Keton (EG-Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","[4 - [4,4' - 双（二甲氨基）二苯亚甲基]环己-2,5 - 二烯-1 - 亚基]二甲基氯化铵（CI碱性紫3）[含≥0.1％ 米氏酮（EG-Nr.202-027-5）或者米氏碱（EC 202-959-2）]"]
[null,{"$f":"IF($B$1=\"English\",C1856,IF($B$1=\"Deutsch\",D1856,IF($B$1=\"中文\",E1856,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-bis(2-methoxyethoxy)ethane (Triglyme)"},"1,2-bis(2-methoxyethoxy)ethane (Triglyme)","1,2-Bis(2-methoxyethoxy)ethan\n(TEGDME; triglyme)","1,2-双(2-甲氧基乙氧基)乙烷 (三甘醇二甲醚 )"]
[null,{"$f":"IF($B$1=\"English\",C1857,IF($B$1=\"Deutsch\",D1857,IF($B$1=\"中文\",E1857,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1, 2-dimethoxyethane (EGDME)"},"1, 2-dimethoxyethane (EGDME)","1,2-Dimethoxyethan; Ethylenglycoldimethylether (EGDME)","1, 2-二甲氧基乙烷 (EGDME)"]
[null,{"$f":"IF($B$1=\"English\",C1858,IF($B$1=\"Deutsch\",D1858,IF($B$1=\"中文\",E1858,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinane-2,4,6-trione"},"1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinane-2,4,6-trione","1,3,5-Tris(oxiran-2-ylmethyl)-1,3,5-triazinan-2,4,6-trion (TGIC)","1,3,5-三缩水甘油-S-三嗪三酮"]
[null,{"$f":"IF($B$1=\"English\",C1859,IF($B$1=\"Deutsch\",D1859,IF($B$1=\"中文\",E1859,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-tris-[(2S and 2R)-2,3-epoxypropyl]-1,3,5-triazine-2,4,6-(1H, 3H, 5H)-\ntrione)"},"1,3,5-tris-[(2S and 2R)-2,3-epoxypropyl]-1,3,5-triazine-2,4,6-(1H, 3H, 5H)-\ntrione)","1,3,5-Tris[(2S und 2R)-2,3-epoxypropyl]-1,3,5-triazin-2,4,6-(1H,3H,5H)-trion (β-TGIC)","1,3,5-三-[(2S和2R)-2,3-环氧丙基]-1,3,5-三嗪-2,4,6-(1H, 3H, 5H)- 三酮)"]
[null,{"$f":"IF($B$1=\"English\",C1860,IF($B$1=\"Deutsch\",D1860,IF($B$1=\"中文\",E1860,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"α,α-Bis[4-(dimethylamino)phenyl]-4\n(phenylamino)naphthalene-1-methanol (C.I. Solvent Blue 4)"},"α,α-Bis[4-(dimethylamino)phenyl]-4\n(phenylamino)naphthalene-1-methanol (C.I. Solvent Blue 4)","alpha,alpha-Bis[4-(dimethylamino)phenyl]-4-(phenylamino)naphthalin-1-methanol (C.I. Solvent Blue 4) [mit ≥ 0.1% Michler's Keton (EG- Nr. 202-027-5) oder Michler's Base (EG-Nr. 202-959-2)]","α，α-双[4 - （二甲基氨基）苯基] -4（苯基氨基）萘-1 - 甲醇（溶剂蓝4）"]
[null,{"$f":"IF($B$1=\"English\",C1861,IF($B$1=\"Deutsch\",D1861,IF($B$1=\"中文\",E1861,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexahydromethylphthalic anhydride\n\nincluding cis- and trans- stereo isomeric forms and all possible combinations of the isomers"},"Hexahydromethylphthalic anhydride\n\nincluding cis- and trans- stereo isomeric forms and all possible combinations of the isomers","Hexahydromethylphthalsäureanhydrid\n\n[einschließlich cis- und trans- stereoisomerer Formen und alle möglichen Kombinationen der Isomere]","甲基六氢邻苯二甲酸酐\n\n包括顺式和反式立体异构体以及异构体的所有可能组合"]
[null,{"$f":"IF($B$1=\"English\",C1862,IF($B$1=\"Deutsch\",D1862,IF($B$1=\"中文\",E1862,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexahydromethylphthalic anhydride"},"Hexahydromethylphthalic anhydride","Hexahydromethylphthalsäureanhydrid","甲基六氢邻苯二甲酸酐"]
[null,{"$f":"IF($B$1=\"English\",C1863,IF($B$1=\"Deutsch\",D1863,IF($B$1=\"中文\",E1863,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexahydro-4-methylphthalic anhydride"},"Hexahydro-4-methylphthalic anhydride","Hexahydro-4-methylphthalsäureanhydrid","4-甲基六氢苯酐"]
[null,{"$f":"IF($B$1=\"English\",C1864,IF($B$1=\"Deutsch\",D1864,IF($B$1=\"中文\",E1864,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexahydro-1-methylphthalic anhydride"},"Hexahydro-1-methylphthalic anhydride","Hexahydro-1-methylphthalsaeureanhydrid ","六氢-1 - 甲基邻苯二甲酸酐"]
[null,{"$f":"IF($B$1=\"English\",C1865,IF($B$1=\"Deutsch\",D1865,IF($B$1=\"中文\",E1865,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexahydro-3-methylphthalic anhydride"},"Hexahydro-3-methylphthalic anhydride","Hexahydro-3-methylphthalsäureanhydrid","甲基六氢邻苯二甲酸酐"]
[null,{"$f":"IF($B$1=\"English\",C1866,IF($B$1=\"Deutsch\",D1866,IF($B$1=\"中文\",E1866,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C1867,IF($B$1=\"Deutsch\",D1867,IF($B$1=\"中文\",E1867,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead dioxide phosphonate"},"Trilead dioxide phosphonate","Tribleidioxidphosphonat","二碱式亚磷酸铅 "]
[null,{"$f":"IF($B$1=\"English\",C1868,IF($B$1=\"Deutsch\",D1868,IF($B$1=\"中文\",E1868,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pyrochlore, antimony lead yellow"},"Pyrochlore, antimony lead yellow","Pyrochlor, Antimonbleigelb","烧绿石，黄锑铅"]
[null,{"$f":"IF($B$1=\"English\",C1869,IF($B$1=\"Deutsch\",D1869,IF($B$1=\"中文\",E1869,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfurous acid, lead salt, dibasic"},"Sulfurous acid, lead salt, dibasic","Schweflige Säure, Bleisalz, dibasisch","亚硫酸，硝酸铅，二碱式亚磷酸铅 "]
[null,{"$f":"IF($B$1=\"English\",C1870,IF($B$1=\"Deutsch\",D1870,IF($B$1=\"中文\",E1870,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetralead trioxide sulphate"},"Tetralead trioxide sulphate","Tetrableitrioxidsulfat","三碱式硫酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1871,IF($B$1=\"Deutsch\",D1871,IF($B$1=\"中文\",E1871,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetraethyllead"},"Tetraethyllead","Tetraethylblei","四乙基铅"]
[null,{"$f":"IF($B$1=\"English\",C1872,IF($B$1=\"Deutsch\",D1872,IF($B$1=\"中文\",E1872,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead bis(carbonate) dihydroxide [Basic lead carbonate]"},"Trilead bis(carbonate) dihydroxide [Basic lead carbonate]","Tribleibis(carbonat)dihydroxid","氢氧化三铅（双碳酸酯）[碱性碳酸铅]"]
[null,{"$f":"IF($B$1=\"English\",C1873,IF($B$1=\"Deutsch\",D1873,IF($B$1=\"中文\",E1873,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tricosafluorododecanoic acid"},"Tricosafluorododecanoic acid","Tricosafluordodecansäure","全氟十二烷酸"]
[null,{"$f":"IF($B$1=\"English\",C1874,IF($B$1=\"Deutsch\",D1874,IF($B$1=\"中文\",E1874,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-Methylacetamide"},"N-Methylacetamide","N-Methylacetamid","N-甲基乙酰胺"]
[null,{"$f":"IF($B$1=\"English\",C1875,IF($B$1=\"Deutsch\",D1875,IF($B$1=\"中文\",E1875,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-Pentyl-isopentyl phthalate"},"N-Pentyl-isopentyl phthalate","N-Pentyl-isopentylphthalat","邻苯二甲酸二异戊酯"]
[null,{"$f":"IF($B$1=\"English\",C1876,IF($B$1=\"Deutsch\",D1876,IF($B$1=\"中文\",E1876,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"o-Aminoazotoluene [4-o-Tolylazo-o-toluidine]"},"o-Aminoazotoluene [4-o-Tolylazo-o-toluidine]","o-Aminoazotoluol (4-o-Tolylazo-o-toluidin)","邻氨基偶氮甲苯"]
[null,{"$f":"IF($B$1=\"English\",C1877,IF($B$1=\"Deutsch\",D1877,IF($B$1=\"中文\",E1877,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Orange lead [Lead tetroxide]"},"Orange lead [Lead tetroxide]","Orangemennige (Bleitetraoxid)"," 四氧化三铅"]
[null,{"$f":"IF($B$1=\"English\",C1878,IF($B$1=\"Deutsch\",D1878,IF($B$1=\"中文\",E1878,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"o-Toluidine"},"o-Toluidine","o-Toluidin","邻甲基苯胺"]
[null,{"$f":"IF($B$1=\"English\",C1879,IF($B$1=\"Deutsch\",D1879,IF($B$1=\"中文\",E1879,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentalead tetraoxide sulphate"},"Pentalead tetraoxide sulphate","Pentableitetraoxidsulfat","氧化铅与硫酸铅的复合物"]
[null,{"$f":"IF($B$1=\"English\",C1880,IF($B$1=\"Deutsch\",D1880,IF($B$1=\"中文\",E1880,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentacosafluorotridecanoic acid"},"Pentacosafluorotridecanoic acid","Pentacosafluortridecansäure","全氟十三酸"]
[null,{"$f":"IF($B$1=\"English\",C1881,IF($B$1=\"Deutsch\",D1881,IF($B$1=\"中文\",E1881,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dinoseb(ISO); 6-sec-butyl-2,4-dinitrophenol"},"Dinoseb(ISO); 6-sec-butyl-2,4-dinitrophenol","Dinoseb (6-sec-Butyl-2,4-dinitrophenol)","地乐酚(ISO); 6-仲丁基-2,4-二硝基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C1882,IF($B$1=\"Deutsch\",D1882,IF($B$1=\"中文\",E1882,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioxobis(stearato)trilead"},"Dioxobis(stearato)trilead","Dioxobis(stearato)triblei","双(十八酸基)二氧代三铅"]
[null,{"$f":"IF($B$1=\"English\",C1883,IF($B$1=\"Deutsch\",D1883,IF($B$1=\"中文\",E1883,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acetic acid, lead salt, basic"},"Acetic acid, lead salt, basic","Essigsäure, Bleisalz, basisch","醋酸，油酸铅，碱式碳酸铜 "]
[null,{"$f":"IF($B$1=\"English\",C1884,IF($B$1=\"Deutsch\",D1884,IF($B$1=\"中文\",E1884,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fatty acids, C16-18, lead salts"},"Fatty acids, C16-18, lead salts","Fettsäuren, C16-18-, Bleisalze","脂肪酸，C16-18-，硝酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1885,IF($B$1=\"Deutsch\",D1885,IF($B$1=\"中文\",E1885,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Furan"},"Furan","Furan","呋喃"]
[null,{"$f":"IF($B$1=\"English\",C1886,IF($B$1=\"Deutsch\",D1886,IF($B$1=\"中文\",E1886,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Henicosafluoroundecanoic acid"},"Henicosafluoroundecanoic acid","Henicosafluorundecansäure","全氟十一烷酸"]
[null,{"$f":"IF($B$1=\"English\",C1887,IF($B$1=\"Deutsch\",D1887,IF($B$1=\"中文\",E1887,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptacosafluorotetradecanoic acid"},"Heptacosafluorotetradecanoic acid","Heptacosafluortetradecansäure","全氟代十四酸"]
[null,{"$f":"IF($B$1=\"English\",C1888,IF($B$1=\"Deutsch\",D1888,IF($B$1=\"中文\",E1888,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicic acid, lead salt"},"Silicic acid, lead salt","Kieselsäure, Bleisalz","硅酸，铅盐"]
[null,{"$f":"IF($B$1=\"English\",C1889,IF($B$1=\"Deutsch\",D1889,IF($B$1=\"中文\",E1889,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicic acid (H2Si2O5), barium salt (1:1), lead-doped [Silicic acid,\nbarium salt, lead-doped]\n[with lead content (Pb) above the applicable general concentration limit for'reproductive toxicity' repr. 1A (CLP) or category 1 (DSD); the substance belongs to a group entry of lead compounds with index number 082-001-00-6 in CLP Regulation (EC) No 1272/2008]"},"Silicic acid (H2Si2O5), barium salt (1:1), lead-doped [Silicic acid,\nbarium salt, lead-doped]\n[with lead content (Pb) above the applicable general concentration limit for'reproductive toxicity' repr. 1A (CLP) or category 1 (DSD); the substance belongs to a group entry of lead compounds with index number 082-001-00-6 in CLP Regulation (EC) No 1272/2008]","Kieselsäure (H2Si2O5), Bariumsalz (1:1), Blei-dotiert\n[mit Bleigehalt (Pb) oberhalb des anwendbaren allgemeinen Konzentrationsgrenzwertes für 'Reproduktionstoxizität' Repr. 1A (CLP) oder Kategorie 1 (DSD); der Stoff gehört zu einem Gruppeneintrag von Bleiverbindungen mit der Indexnummer 082-001-00-6 in der CLP-Verordnung (EG) Nr. 1272/2008]","硅酸 (H2Si2O5), 钡盐 (1:1), 掺铅\n[铅含量(Pb)超过适用“生殖毒性”报告的一般浓度限制Repr. 1A（CLP）或类别1（DSD）；该物质属于CLP法规(EC) No 1272/2008中索引号为082-001-00-6的先导化合物组条目]"]
[null,{"$f":"IF($B$1=\"English\",C1890,IF($B$1=\"Deutsch\",D1890,IF($B$1=\"中文\",E1890,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methoxyacetic acid (MAA)"},"Methoxyacetic acid (MAA)","Methoxyessigsäure","甲氧基乙酸 (MAA)"]
[null,{"$f":"IF($B$1=\"English\",C1891,IF($B$1=\"Deutsch\",D1891,IF($B$1=\"中文\",E1891,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methyloxirane [Propylene oxide]"},"Methyloxirane [Propylene oxide]","Methyloxiran (Propylenoxid)","甲基环氧乙烷[环氧丙烷]"]
[null,{"$f":"IF($B$1=\"English\",C1892,IF($B$1=\"Deutsch\",D1892,IF($B$1=\"中文\",E1892,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material ","0,1 Massen%, jedoch Verbot bei Neuentwicklung von Materialien oder bei Material-Änderungen ","0.1％（质量百分比），但禁止用于新开发的材料或材料变更。"]
[null,{"$f":"IF($B$1=\"English\",C1893,IF($B$1=\"Deutsch\",D1893,IF($B$1=\"中文\",E1893,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N-dimethylformamide"},"N,N-dimethylformamide","N,N-Dimethylformamid","N,N-二甲基甲酰胺"]
[null,{"$f":"IF($B$1=\"English\",C1894,IF($B$1=\"Deutsch\",D1894,IF($B$1=\"中文\",E1894,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisopentylphthalate (DIPP)"},"Diisopentylphthalate (DIPP)","Diisopentylphthalat (DIPP)","邻苯二甲酸二异戊酯 (DIPP)"]
[null,{"$f":"IF($B$1=\"English\",C1895,IF($B$1=\"Deutsch\",D1895,IF($B$1=\"中文\",E1895,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dimethyl sulphate"},"Dimethyl sulphate","Dimethylsulfat","硫酸二甲酯"]
[null,{"$f":"IF($B$1=\"English\",C1896,IF($B$1=\"Deutsch\",D1896,IF($B$1=\"中文\",E1896,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide sulfate"},"Lead oxide sulfate","Bleisulfat, basisch","石灰浆 "]
[null,{"$f":"IF($B$1=\"English\",C1897,IF($B$1=\"Deutsch\",D1897,IF($B$1=\"中文\",E1897,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead titanium trioxide"},"Lead titanium trioxide","Bleititantrioxid","钛酸铅 "]
[null,{"$f":"IF($B$1=\"English\",C1898,IF($B$1=\"Deutsch\",D1898,IF($B$1=\"中文\",E1898,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead titanium zirconium oxide"},"Lead titanium zirconium oxide","Bleititanzirkonoxid","钛酸铅锆镧"]
[null,{"$f":"IF($B$1=\"English\",C1899,IF($B$1=\"Deutsch\",D1899,IF($B$1=\"中文\",E1899,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cyclohexane-1,2-dicarboxylic anhydride\nall possible combinations of the cis- and trans-isomers"},"Cyclohexane-1,2-dicarboxylic anhydride\nall possible combinations of the cis- and trans-isomers","Cyclohexan-1,2-dicarbonsäureanhydrid\n\nund alle möglichen Kombinationen an cis- und trans-Isomeren ","六氢甲基邻苯二甲酸酐\n所有可能的顺式和反式异构体的组合"]
[null,{"$f":"IF($B$1=\"English\",C1900,IF($B$1=\"Deutsch\",D1900,IF($B$1=\"中文\",E1900,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cyclohexane-1,2-dicarboxylic anhydride"},"Cyclohexane-1,2-dicarboxylic anhydride","Cyclohexan-1,2-dicarbonsäureanhydrid [1]","六氢甲基邻苯二甲酸酐"]
[null,{"$f":"IF($B$1=\"English\",C1901,IF($B$1=\"Deutsch\",D1901,IF($B$1=\"中文\",E1901,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"cis-cyclohexane-1,2-dicarboxylic anhydride"},"cis-cyclohexane-1,2-dicarboxylic anhydride","cis-Cyclohexan-1,2-dicarbonsäureanhydrid [2]","顺式-环己烷-1,2-二羧酸酐"]
[null,{"$f":"IF($B$1=\"English\",C1902,IF($B$1=\"Deutsch\",D1902,IF($B$1=\"中文\",E1902,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"trans-cyclohexane-1,2-dicarboxylic anhydride"},"trans-cyclohexane-1,2-dicarboxylic anhydride","trans-Cyclohexan-1,2-discarbonsäureanhydrid [3] ","反式-环己烷-1,2-二羧酸酐"]
[null,{"$f":"IF($B$1=\"English\",C1903,IF($B$1=\"Deutsch\",D1903,IF($B$1=\"中文\",E1903,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"C,C'-azodi(formamide) (ADCA)\n"},"C,C'-azodi(formamide) (ADCA)\n","Diazen-1,2-dicarboxamid \nC,C'-azodi(formamid) (ACDA)\n","C,C'-偶氮二甲酰胺  (ADCA)\n"]
[null,{"$f":"IF($B$1=\"English\",C1904,IF($B$1=\"Deutsch\",D1904,IF($B$1=\"中文\",E1904,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyltin dichloride"},"Dibutyltin dichloride","Dibutylzinndichlorid (DBTC)","二丁基二氯化锡"]
[null,{"$f":"IF($B$1=\"English\",C1905,IF($B$1=\"Deutsch\",D1905,IF($B$1=\"中文\",E1905,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diethyl sulphate"},"Diethyl sulphate","Diethylsulfat","硫酸二乙酯"]
[null,{"$f":"IF($B$1=\"English\",C1906,IF($B$1=\"Deutsch\",D1906,IF($B$1=\"中文\",E1906,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(pentabromophenyl)ether (decabromodiphenyl ether; decaBDE)"},"Bis(pentabromophenyl)ether (decabromodiphenyl ether; decaBDE)","Bis(pentabromphenyl)ether\n(Dekabromdiphenylether; DecaBDE)","十溴联苯醚（decaBDE）"]
[null,{"$f":"IF($B$1=\"English\",C1907,IF($B$1=\"Deutsch\",D1907,IF($B$1=\"中文\",E1907,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead bis(tetrafluoroborate)"},"Lead bis(tetrafluoroborate)","Bleibis(tetrafluoroborat)","四氟硼酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1908,IF($B$1=\"Deutsch\",D1908,IF($B$1=\"中文\",E1908,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead cyanamidate"},"Lead cyanamidate","Bleicyanoamidat","氨基氰铅盐"]
[null,{"$f":"IF($B$1=\"English\",C1909,IF($B$1=\"Deutsch\",D1909,IF($B$1=\"中文\",E1909,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead dinitrate"},"Lead dinitrate","Bleidinitrat","硝酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1910,IF($B$1=\"Deutsch\",D1910,IF($B$1=\"中文\",E1910,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead monoxide [Lead oxide]"},"Lead monoxide [Lead oxide]","Bleimonoxid (Bleioxid)","一氧化铅 [氧化铅]"]
[null,{"$f":"IF($B$1=\"English\",C1911,IF($B$1=\"Deutsch\",D1911,IF($B$1=\"中文\",E1911,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3-Ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidine"},"3-Ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidine","3-Ethyl-2-methyl-2-(3-methylbutyl)-1,3-oxazolidin","3-乙基-2-甲基-2-(3-甲基丁基)-1,3-恶唑烷"]
[null,{"$f":"IF($B$1=\"English\",C1912,IF($B$1=\"Deutsch\",D1912,IF($B$1=\"中文\",E1912,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-Methylenedi-o-toluidine"},"4,4'-Methylenedi-o-toluidine","4,4'-Methylendi-o-toluidin","4,4'-二氨基-3,3'-二甲基联苯基甲烷"]
[null,{"$f":"IF($B$1=\"English\",C1913,IF($B$1=\"Deutsch\",D1913,IF($B$1=\"中文\",E1913,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-oxydianiline and its salts"},"4,4'-oxydianiline and its salts","4,4'-Oxydianilin und seine Salze","4,4'-二氨基二苯醚及其盐"]
[null,{"$f":"IF($B$1=\"English\",C1914,IF($B$1=\"Deutsch\",D1914,IF($B$1=\"中文\",E1914,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-oxydianiline"},"4,4'-oxydianiline","4,4'-Oxydianilin","4,4'-二氨基二苯醚"]
[null,{"$f":"IF($B$1=\"English\",C1915,IF($B$1=\"Deutsch\",D1915,IF($B$1=\"中文\",E1915,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated \n[covering well-defined\nsubstances and UVCB substances, polymers and homologues]"},"4-(1,1,3,3-tetramethylbutyl)phenol, ethoxylated \n[covering well-defined\nsubstances and UVCB substances, polymers and homologues]","4-(1,1,3,3-Tetramethylbutyl)phenol, ethoxyliert \n[deckt wohldefinierte Stoffe, UVCB-Stoffe, Polymere und Homologe ab]","4-(1,1,3,3-四甲基丁基)苯酚，乙氧基化物 \n[包括定义明确的物质和UVCB物质、聚合物和同系物] "]
[null,{"$f":"IF($B$1=\"English\",C1916,IF($B$1=\"Deutsch\",D1916,IF($B$1=\"中文\",E1916,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(oxy-1,2-ethanediyl), α-[(1,1,3,3-tetramethylbutyl)phenyl]-ω-hydroxy-"},"Poly(oxy-1,2-ethanediyl), α-[(1,1,3,3-tetramethylbutyl)phenyl]-ω-hydroxy-","Poly(oxy-1,2-ethanediyl), α-[(1,1,3,3-tetramethylbutyl)phenyl]-ω-hydroxy-","聚(氧基-1,2-乙二基), α-[(1,1,3,3-四甲基丁基)苯基]-ω-羥基-"]
[null,{"$f":"IF($B$1=\"English\",C1917,IF($B$1=\"Deutsch\",D1917,IF($B$1=\"中文\",E1917,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polyethylene glycol p-(1,1,3,3-tetramethylbutyl)phenyl ether"},"Polyethylene glycol p-(1,1,3,3-tetramethylbutyl)phenyl ether","Polyethylene glycol p-(1,1,3,3-tetramethylbutyl)phenyl ether","聚(氧基-1,2-乙二基), α-[(1,1,3,3-四甲基丁基)苯基]-ω-羥基-"]
[null,{"$f":"IF($B$1=\"English\",C1918,IF($B$1=\"Deutsch\",D1918,IF($B$1=\"中文\",E1918,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"20-[4-(1,1,3,3-tetramethylbutyl)phenoxy]-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"20-[4-(1,1,3,3-tetramethylbutyl)phenoxy]-3,6,9,12,15,18-hexaoxaicosan-1-ol","20-[4-(1,1,3,3-tetramethylbutyl)phenoxy]-3,6,9,12,15,18-hexaoxaicosan-1-ol","20-[(1,1,3,3-四甲基丁基)苯氧基]-3,6,9,12,15,18-六氧核糖核酸-1-ol"]
[null,{"$f":"IF($B$1=\"English\",C1919,IF($B$1=\"Deutsch\",D1919,IF($B$1=\"中文\",E1919,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethanol "},"2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethanol ","2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethanol ","2-[4-(1,1,3,3-四甲基丁基)苯氧基] 乙醇 "]
[null,{"$f":"IF($B$1=\"English\",C1920,IF($B$1=\"Deutsch\",D1920,IF($B$1=\"中文\",E1920,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethoxy]ethanol"},"2-[2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethoxy]ethanol","2-[2-[4-(1,1,3,3-tetramethylbutyl)phenoxy]ethoxy]ethanol","2-[2-[4-(1,1,3,3-四甲基丁基)苯氧基]乙氧基]乙醇，2-{2-[4-(2,4,4-三甲基戊烷-2-基)苯氧基]乙氧基}乙醇"]
[null,{"$f":"IF($B$1=\"English\",C1921,IF($B$1=\"Deutsch\",D1921,IF($B$1=\"中文\",E1921,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Aminoazobenzene"},"4-Aminoazobenzene","4-Aminoazobenzol","4-阿基苯甲酯"]
[null,{"$f":"IF($B$1=\"English\",C1922,IF($B$1=\"Deutsch\",D1922,IF($B$1=\"中文\",E1922,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biphenyl-4-ylamine"},"Biphenyl-4-ylamine","4-Aminobiphenyl","4-氨基联苯酚酯"]
[null,{"$f":"IF($B$1=\"English\",C1923,IF($B$1=\"Deutsch\",D1923,IF($B$1=\"中文\",E1923,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-methyl-m-phenylenediamine [Toluene-2,4-diamine]"},"4-methyl-m-phenylenediamine [Toluene-2,4-diamine]","4-Methyl-m-phenylendiamin (2,4-Toluoldiamin)","正丙基溴"]
[null,{"$f":"IF($B$1=\"English\",C1924,IF($B$1=\"Deutsch\",D1924,IF($B$1=\"中文\",E1924,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched and linear: substances with a linear and/or\nbranched alkyl chain with a carbon number of 9 covalently bound in position\n4 to phenol, covering also UVCB- and well-defined substances which include\nany of the individual isomers or a combination thereof"},"4-Nonylphenol, branched and linear: substances with a linear and/or\nbranched alkyl chain with a carbon number of 9 covalently bound in position\n4 to phenol, covering also UVCB- and well-defined substances which include\nany of the individual isomers or a combination thereof","4-Nonylphenol, verzweigt und linear [Stoffe mit einer linearen und/oder verzweigten Alkylkette von 9 kovalent gebundenen C-Atomen in Position 4 zu Phenol, inklusive UVCB- und wohldefinierten Stoffen, individuellen Isomeren oder einer Kombination davon]","4-壬基酚，支链和直链：具有直链和(或)支链的碳原子数为9 烷基链在4号位置共价与苯酚结合的物质，也包括UVCB-和明确定义的物质，其中包括任何单独的异构体或其组合"]
[null,{"$f":"IF($B$1=\"English\",C1925,IF($B$1=\"Deutsch\",D1925,IF($B$1=\"中文\",E1925,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1-Ethyl-1,3-dimethylpentyl)phenol"},"4-(1-Ethyl-1,3-dimethylpentyl)phenol","4-(1-Ethyl-1,3-dimethylpentyl)phenol","4-(1-乙基-1,3-二甲基戊基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C1926,IF($B$1=\"Deutsch\",D1926,IF($B$1=\"中文\",E1926,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-nonyl-, branched"},"Phenol, 4-nonyl-, branched","Phenol, 4-nonyl-, verzweigt","酚，4-壬基-，支链的"]
[null,{"$f":"IF($B$1=\"English\",C1927,IF($B$1=\"Deutsch\",D1927,IF($B$1=\"中文\",E1927,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-(1-methyloctyl)phenol "},"p-(1-methyloctyl)phenol ","p-(1-methyloctyl)phenol ","对-(1-甲基辛基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C1928,IF($B$1=\"Deutsch\",D1928,IF($B$1=\"中文\",E1928,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-(1,1-dimethylheptyl)phenol "},"p-(1,1-dimethylheptyl)phenol ","p-(1,1-dimethylheptyl)phenol ","对-(1,1-二甲基庚基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C1929,IF($B$1=\"Deutsch\",D1929,IF($B$1=\"中文\",E1929,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-nonylphenol"},"p-nonylphenol","p-nonylphenol","对壬基酚"]
[null,{"$f":"IF($B$1=\"English\",C1930,IF($B$1=\"Deutsch\",D1930,IF($B$1=\"中文\",E1930,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1-Ethyl-1,4-dimethylpentyl)phenol "},"4-(1-Ethyl-1,4-dimethylpentyl)phenol ","4-(1-Ethyl-1,4-dimethylpentyl)phenol ","4-(1-乙基-1,4-二甲基戊基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C1931,IF($B$1=\"Deutsch\",D1931,IF($B$1=\"中文\",E1931,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1-ethyl-1-methylhexyl)phenol "},"4-(1-ethyl-1-methylhexyl)phenol ","4-(1-ethyl-1-methylhexyl)phenol ","4-(1-乙基-1-甲基己基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C1932,IF($B$1=\"Deutsch\",D1932,IF($B$1=\"中文\",E1932,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-isononylphenol"},"p-isononylphenol","p-isononylphenol","对异壬基酚"]
[null,{"$f":"IF($B$1=\"English\",C1933,IF($B$1=\"Deutsch\",D1933,IF($B$1=\"中文\",E1933,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, nonyl-, branched"},"Phenol, nonyl-, branched","Phenol, nonyl-, verzweigt","苯酚，壬基，支链的"]
[null,{"$f":"IF($B$1=\"English\",C1934,IF($B$1=\"Deutsch\",D1934,IF($B$1=\"中文\",E1934,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Isononylphenol"},"Isononylphenol","Isononylphenol","异壬基酚"]
[null,{"$f":"IF($B$1=\"English\",C1935,IF($B$1=\"Deutsch\",D1935,IF($B$1=\"中文\",E1935,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(3-ethylheptan-2-yl)phenol "},"4-(3-ethylheptan-2-yl)phenol ","4-(3-ethylheptan-2-yl)phenol ","4-(2,6-二甲基-2-庚基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C1936,IF($B$1=\"Deutsch\",D1936,IF($B$1=\"中文\",E1936,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1,1,5-Trimethylhexyl)phenol"},"4-(1,1,5-Trimethylhexyl)phenol","4-(1,1,5-Trimethylhexyl)phenol","4-(1,1,5-Trimethylhexyl)phenol"]
[null,{"$f":"IF($B$1=\"English\",C1937,IF($B$1=\"Deutsch\",D1937,IF($B$1=\"中文\",E1937,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol "},"Nonylphenol ","Nonylphenol ","壬基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C1938,IF($B$1=\"Deutsch\",D1938,IF($B$1=\"中文\",E1938,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"6-Methoxy-m-toluidine [p-cresidine]"},"6-Methoxy-m-toluidine [p-cresidine]","6-Methoxy-m-toluidin (p-Cresidin)","6-甲氧基间甲苯胺[对甲苯胺]"]
[null,{"$f":"IF($B$1=\"English\",C1939,IF($B$1=\"Deutsch\",D1939,IF($B$1=\"中文\",E1939,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[Phthalato(2-)]dioxotrilead"},"[Phthalato(2-)]dioxotrilead","[Phthalato(2-)]dioxotriblei"," [1,2-苯二羧酸根合]二氧化三铅"]
[null,{"$f":"IF($B$1=\"English\",C1940,IF($B$1=\"Deutsch\",D1940,IF($B$1=\"中文\",E1940,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid dipentylester, branched and linear"},"1,2-Benzenedicarboxylic acid dipentylester, branched and linear","1,2-Benzoldicarbonsäure, Dipentylester, verzweigt und linear","1,2-苯二甲酸，支链和直链"]
[null,{"$f":"IF($B$1=\"English\",C1941,IF($B$1=\"Deutsch\",D1941,IF($B$1=\"中文\",E1941,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-diethoxyethane"},"1,2-diethoxyethane","1,2-Diethoxyethan","1,2-二乙氧基乙烷"]
[null,{"$f":"IF($B$1=\"English\",C1942,IF($B$1=\"Deutsch\",D1942,IF($B$1=\"中文\",E1942,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-bromopropane; n-propyl bromide"},"1-bromopropane; n-propyl bromide","1-Brompropan (n-Propylbromid)","1-溴丙烷; 正丙基溴"]
[null,{"$f":"IF($B$1=\"English\",C1943,IF($B$1=\"Deutsch\",D1943,IF($B$1=\"中文\",E1943,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentadecafluorooctanoic Acid (PFOA)"},"Pentadecafluorooctanoic Acid (PFOA)","Pentadecafluoroktansäure (PFOA)","全氟辛酸（PFOA）"]
[null,{"$f":"IF($B$1=\"English\",C1944,IF($B$1=\"Deutsch\",D1944,IF($B$1=\"中文\",E1944,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dipentyl phthalate (DPP)"},"Dipentyl phthalate (DPP)","Dipentylphthalat (DPP)","邻苯二甲酸二戊酯（DPP）"]
[null,{"$f":"IF($B$1=\"English\",C1945,IF($B$1=\"Deutsch\",D1945,IF($B$1=\"中文\",E1945,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C1946,IF($B$1=\"Deutsch\",D1946,IF($B$1=\"中文\",E1946,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium oxide"},"Cadmium oxide","Cadmiumoxid","氧化镉"]
[null,{"$f":"IF($B$1=\"English\",C1947,IF($B$1=\"Deutsch\",D1947,IF($B$1=\"中文\",E1947,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium pentadecafluorooctanoate (APFO)"},"Ammonium pentadecafluorooctanoate (APFO)","Ammonium Pentadecafluoroktanoat (APFO)","全氟辛酸铵 （APFO）"]
[null,{"$f":"IF($B$1=\"English\",C1948,IF($B$1=\"Deutsch\",D1948,IF($B$1=\"中文\",E1948,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched and linear, ethoxylated \n[substances with a linear and/or branched alkyl chain with a\ncarbon number of 9 covalently bound in position 4 to phenol, ethoxylated covering UVCB- and well-defined\nsubstances, polymers and homologues, which include any of the individual isomers and/or combinations thereof]"},"4-Nonylphenol, branched and linear, ethoxylated \n[substances with a linear and/or branched alkyl chain with a\ncarbon number of 9 covalently bound in position 4 to phenol, ethoxylated covering UVCB- and well-defined\nsubstances, polymers and homologues, which include any of the individual isomers and/or combinations thereof]","4-Nonylphenol, verzweigt und linear, ethoxyliert \n[Stoffe mit einer linearen und/oder verzweigten Alkylkette von 9 kovalent gebundenen C-Atomen in Position 4 zu Phenol, ethoxyliert inklusive UVCB- und wohldefinierten Stoffen, Polymere und Homologe, die beliebige individuelle Isomere oder einer Kombination davon beinhalten]","4-壬基酚，支链和直链，乙氧基化物 \n[具有直链和(或)支链的碳原子数为9的烷基链在4号位置共价与苯酚结合的物质，也包括乙氧基化UVCB-和明确定义的物质，其中包括任何单独的异构体或其组合]"]
[null,{"$f":"IF($B$1=\"English\",C1949,IF($B$1=\"Deutsch\",D1949,IF($B$1=\"中文\",E1949,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated "},"Nonylphenol, ethoxylated ","Nonylphenol, ethoxyliert ","乙氧基化壬基酚"]
[null,{"$f":"IF($B$1=\"English\",C1950,IF($B$1=\"Deutsch\",D1950,IF($B$1=\"中文\",E1950,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated   (15-EO) "},"Nonylphenol, ethoxylated   (15-EO) ","Nonylphenol, ethoxyliert  (15-EO) (9016-45-9) ","乙氧基化壬基酚   (15-EO) "]
[null,{"$f":"IF($B$1=\"English\",C1951,IF($B$1=\"Deutsch\",D1951,IF($B$1=\"中文\",E1951,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated  (10-EO)"},"Nonylphenol, ethoxylated  (10-EO)","Nonylphenol, ethoxyliert (10-EO) (9016-45-9)","壬基酚，乙氧基化 (10-EO)"]
[null,{"$f":"IF($B$1=\"English\",C1952,IF($B$1=\"Deutsch\",D1952,IF($B$1=\"中文\",E1952,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (8-EO) "},"Nonylphenol, ethoxylated (8-EO) ","Nonylphenol, ethoxyliert (8-EO) (9016-45-9)","壬基酚，乙氧基化 (8-EO) "]
[null,{"$f":"IF($B$1=\"English\",C1953,IF($B$1=\"Deutsch\",D1953,IF($B$1=\"中文\",E1953,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol,  ethoxylated  (6,5-EO)"},"Nonylphenol,  ethoxylated  (6,5-EO)","Nonylphenol, ethoxyliert (6,5-EO) (9016-45-9)","乙氧基化壬基酚  (6,5-EO)"]
[null,{"$f":"IF($B$1=\"English\",C1954,IF($B$1=\"Deutsch\",D1954,IF($B$1=\"中文\",E1954,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, ethoxylated \n[1 - 2.5 moles ethoxylated]"},"4-Nonylphenol, ethoxylated \n[1 - 2.5 moles ethoxylated]","4-Nonylphenol,ethoxyliert\n[1 - 2.5 moles ethoxylated]","4-壬基酚，乙氧基化 \n[1-2.5 mol 乙氧基化物]"]
[null,{"$f":"IF($B$1=\"English\",C1955,IF($B$1=\"Deutsch\",D1955,IF($B$1=\"中文\",E1955,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[2-(4-nonylphenoxy)ethoxy]ethanol"},"2-[2-(4-nonylphenoxy)ethoxy]ethanol","2-[2-(4-nonylphenoxy)ethoxy]ethanol","2-[2-(4-壬基苯氧基)乙氧基]乙醇"]
[null,{"$f":"IF($B$1=\"English\",C1956,IF($B$1=\"Deutsch\",D1956,IF($B$1=\"中文\",E1956,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol "},"20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol ","20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol ","20-(4-壬基苯氧基)-3,6,9,12,15,18-六氧核糖核酸-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C1957,IF($B$1=\"Deutsch\",D1957,IF($B$1=\"中文\",E1957,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol"},"26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol","26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol","26-(4-壬基苯氧基)-3,6,9,12,15,18,21,24- 八氧六环素-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C1958,IF($B$1=\"Deutsch\",D1958,IF($B$1=\"中文\",E1958,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, branched, ethoxylated t"},"Nonylphenol, branched, ethoxylated t","Nonylphenol, verzweigt, ethoxyliert","壬基酚，支链，乙氧基化 "]
[null,{"$f":"IF($B$1=\"English\",C1959,IF($B$1=\"Deutsch\",D1959,IF($B$1=\"中文\",E1959,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, branched, ethoxylated  [1 - 2.5 mol ethoxylated]"},"Nonylphenol, branched, ethoxylated  [1 - 2.5 mol ethoxylated]","Nonylphenol, verzweigt, ethoxyliert [1 - 2.5 mol ethoxyliert]","壬基酚，支链，乙氧基化  [1-2.5 mol 乙氧基化物]"]
[null,{"$f":"IF($B$1=\"English\",C1960,IF($B$1=\"Deutsch\",D1960,IF($B$1=\"中文\",E1960,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol"},"2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol","2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol","2-[2-[2-[2-(4-基苯氧基)乙氧基]乙氧基]乙氧基]乙醇"]
[null,{"$f":"IF($B$1=\"English\",C1961,IF($B$1=\"Deutsch\",D1961,IF($B$1=\"中文\",E1961,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched, ethoxylated  [1 - 2.5 mol ethoxylated]"},"4-Nonylphenol, branched, ethoxylated  [1 - 2.5 mol ethoxylated]","4-Nonylphenol, verzweigt, ethoxyliert [1 - 2.5 mol ethoxyliert]","4-壬基酚，支链，乙氧基化  [1-2.5 mol 乙氧基化物]"]
[null,{"$f":"IF($B$1=\"English\",C1962,IF($B$1=\"Deutsch\",D1962,IF($B$1=\"中文\",E1962,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-Nonylphenol hexaethoxylate"},"p-Nonylphenol hexaethoxylate","p-Nonylphenol hexaethoxylate","p-壬基酚六乙氧基化物 "]
[null,{"$f":"IF($B$1=\"English\",C1963,IF($B$1=\"Deutsch\",D1963,IF($B$1=\"中文\",E1963,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Isononylphenol, ethoxylated"},"Isononylphenol, ethoxylated","Isononylphenol, ethoxyliert ","异壬基酚，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C1964,IF($B$1=\"Deutsch\",D1964,IF($B$1=\"中文\",E1964,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(oxy-1,2-ethanediyl), a-(nonylphenyl)-w-hydroxy-(CAS 9016-45-9) "},"Poly(oxy-1,2-ethanediyl), a-(nonylphenyl)-w-hydroxy-(CAS 9016-45-9) ","Poly(oxy-1,2-ethanediyl), a-(nonylphenyl)-w-hydroxy-(CAS 9016-45-9) ","聚(氧-1,2-乙二醇), a-(壬基苯基)-w-羟基-(CAS 9016-45-9) "]
[null,{"$f":"IF($B$1=\"English\",C1965,IF($B$1=\"Deutsch\",D1965,IF($B$1=\"中文\",E1965,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-t-Nonylphenol-diethoxylate"},"4-t-Nonylphenol-diethoxylate","4-t-Nonylphenol-diethoxylate","4-壬基酚-二乙氧基化物"]
[null,{"$f":"IF($B$1=\"English\",C1966,IF($B$1=\"Deutsch\",D1966,IF($B$1=\"中文\",E1966,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanol, 2-(4-nonylphenoxy)-"},"Ethanol, 2-(4-nonylphenoxy)-","Ethanol, 2-(4-nonylphenoxy)-","乙醇, 2-(4-基苯氧基)-"]
[null,{"$f":"IF($B$1=\"English\",C1967,IF($B$1=\"Deutsch\",D1967,IF($B$1=\"中文\",E1967,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-"},"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-","3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-","3,6,9,12-四氧杂环丁烷-1-醇, 14-(4-基苯氧基y)-"]
[null,{"$f":"IF($B$1=\"English\",C1968,IF($B$1=\"Deutsch\",D1968,IF($B$1=\"中文\",E1968,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (EO = 4)"},"Nonylphenol, ethoxylated (EO = 4)","Nonylphenol, ethoxyliert (EO = 4)","壬基酚，乙氧基化 (EO = 4)"]
[null,{"$f":"IF($B$1=\"English\",C1969,IF($B$1=\"Deutsch\",D1969,IF($B$1=\"中文\",E1969,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (polymer) "},"Nonylphenol, ethoxylated (polymer) ","Nonylphenol, ethoxyliert (polymer) ","壬基酚，乙氧基化 (聚合物) "]
[null,{"$f":"IF($B$1=\"English\",C1970,IF($B$1=\"Deutsch\",D1970,IF($B$1=\"中文\",E1970,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol"},"2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol","2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol","2-{2-[4-(3,6-二甲基庚烷-3-基)苯氧基]乙氧基}乙醇"]
[null,{"$f":"IF($B$1=\"English\",C1971,IF($B$1=\"Deutsch\",D1971,IF($B$1=\"中文\",E1971,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol"},"2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol","2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol","2-[4-(3,6-二甲基庚烷-3-基)苯氧基]乙氧基"]
[null,{"$f":"IF($B$1=\"English\",C1972,IF($B$1=\"Deutsch\",D1972,IF($B$1=\"中文\",E1972,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenolpolyglycolether"},"Nonylphenolpolyglycolether","Nonylphenolpolyglycolether","壬基酚聚乙二醇醚"]
[null,{"$f":"IF($B$1=\"English\",C1973,IF($B$1=\"Deutsch\",D1973,IF($B$1=\"中文\",E1973,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, branched"},"Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, branched","Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, verzweigt","聚(氧-1,2-乙二醇)，α-(壬基苯基)-ω-羟基-，支链的"]
[null,{"$f":"IF($B$1=\"English\",C1974,IF($B$1=\"Deutsch\",D1974,IF($B$1=\"中文\",E1974,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol,branched, ethoxylated"},"4-Nonylphenol,branched, ethoxylated","4-Nonylphenol, verzweigt, ethoxyliert","4-壬基酚，支链，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C1975,IF($B$1=\"Deutsch\",D1975,IF($B$1=\"中文\",E1975,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol "},"23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol ","23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol ","23-(壬基苯氧基)-O-(2-叠氮乙基)七聚乙二醇"]
[null,{"$f":"IF($B$1=\"English\",C1976,IF($B$1=\"Deutsch\",D1976,IF($B$1=\"中文\",E1976,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol"},"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol","26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol","26-(壬基苯氧基)-3,6,9,12,15,18,21,24- 八氧六环素-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C1977,IF($B$1=\"Deutsch\",D1977,IF($B$1=\"中文\",E1977,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol"},"14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol","14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol","14-(壬基苯氧基)-3,6,9,12-四氧杂环丁烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C1978,IF($B$1=\"Deutsch\",D1978,IF($B$1=\"中文\",E1978,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (EO = 10)"},"Nonylphenol, ethoxylated (EO = 10)","Nonylphenol, ethoxyliert (EO = 10)","壬基酚，乙氧基化 (EO = 10)"]
[null,{"$f":"IF($B$1=\"English\",C1979,IF($B$1=\"Deutsch\",D1979,IF($B$1=\"中文\",E1979,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trixylyl phosphate"},"Trixylyl phosphate","Trixylylphosphat","磷酸三(二甲苯)酯"]
[null,{"$f":"IF($B$1=\"English\",C1980,IF($B$1=\"Deutsch\",D1980,IF($B$1=\"中文\",E1980,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)"},"Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)","Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)","3,3'-((1,1'-联苯)-4,4'-二基双(偶氮))双(4-氨基萘-1-磺酸)二氯化萘 (C.I. 刚果红  28)"]
[null,{"$f":"IF($B$1=\"English\",C1981,IF($B$1=\"Deutsch\",D1981,IF($B$1=\"中文\",E1981,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"imidazolidine-2-thione (2-imidazoline-2-thiol)"},"imidazolidine-2-thione (2-imidazoline-2-thiol)","Imidazolidin-2-thion","咪唑啉-2-硫酮(2-咪唑啉-2-硫醇)"]
[null,{"$f":"IF($B$1=\"English\",C1982,IF($B$1=\"Deutsch\",D1982,IF($B$1=\"中文\",E1982,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium sulphide"},"Cadmium sulphide","Cadmiumsulfid","硫化镉"]
[null,{"$f":"IF($B$1=\"English\",C1983,IF($B$1=\"Deutsch\",D1983,IF($B$1=\"中文\",E1983,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dihexyl phthalate"},"Dihexyl phthalate","Dihexylphthalat","邻苯二甲酸二己酯"]
[null,{"$f":"IF($B$1=\"English\",C1984,IF($B$1=\"Deutsch\",D1984,IF($B$1=\"中文\",E1984,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead di(acetate)"},"Lead di(acetate)","Bleidi(acetat)","二醋酸铅"]
[null,{"$f":"IF($B$1=\"English\",C1985,IF($B$1=\"Deutsch\",D1985,IF($B$1=\"中文\",E1985,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo] -\n5-hydroxy-6-(phenylazo)naphthalene-2,7-disulphonate (C.I. Direct Black 38)"},"Disodium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo] -\n5-hydroxy-6-(phenylazo)naphthalene-2,7-disulphonate (C.I. Direct Black 38)","Dinatrium-4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo]-5-hydroxy-6-(phenylazo)naphthalin-2,7-disulfonat (C.I. Direct Red 38)","二钠 4-氨基-3-[[4'-[(2,4-二氨基苯基)偶氮][1,1'-二苯基]-4-基]偶氮] -\n5-羟基-6-(苯基偶氮)萘-2,7-二磺酸钠  (C.I. 直接黑 38)"]
[null,{"$f":"IF($B$1=\"English\",C1986,IF($B$1=\"Deutsch\",D1986,IF($B$1=\"中文\",E1986,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perborate; perboric acid, sodium salt"},"Sodium perborate; perboric acid, sodium salt","Natriumperborat; Perborsäure, Natriumsalz","过硼酸钠；过硼酸，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C1987,IF($B$1=\"Deutsch\",D1987,IF($B$1=\"中文\",E1987,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perboric acid (H3BO2(O2)), monosodium salt, trihydrate"},"Perboric acid (H3BO2(O2)), monosodium salt, trihydrate","Perboric acid (H3BO2(O2)), monosodium salt, trihydrate","高硼酸（H3BO2(O2)），单钠盐，三水合物"]
[null,{"$f":"IF($B$1=\"English\",C1988,IF($B$1=\"Deutsch\",D1988,IF($B$1=\"中文\",E1988,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)"},"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)","Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)","硼酸盐(2-), 四羟基双[μ-(过氧-κO1:κO2)]双-, 钠 (1:2)"]
[null,{"$f":"IF($B$1=\"English\",C1989,IF($B$1=\"Deutsch\",D1989,IF($B$1=\"中文\",E1989,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perboric acid, sodium salt"},"Perboric acid, sodium salt","Perboric acid, sodium salt","高硼酸，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C1990,IF($B$1=\"Deutsch\",D1990,IF($B$1=\"中文\",E1990,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perborate"},"Sodium perborate","Sodium perborate","过硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1991,IF($B$1=\"Deutsch\",D1991,IF($B$1=\"中文\",E1991,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)"},"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)","Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)","硼酸盐(2-), 四羟基双[μ-(过氧-κO1:κO2)]双-, 钠 (1:2)，水合物 (1:2:6)"]
[null,{"$f":"IF($B$1=\"English\",C1992,IF($B$1=\"Deutsch\",D1992,IF($B$1=\"中文\",E1992,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium peroxometaborate"},"Sodium peroxometaborate","Natriumperoxometaborat","过硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C1993,IF($B$1=\"Deutsch\",D1993,IF($B$1=\"中文\",E1993,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium chloride"},"Cadmium chloride","Cadmiumchlorid","氯化镉"]
[null,{"$f":"IF($B$1=\"English\",C1994,IF($B$1=\"Deutsch\",D1994,IF($B$1=\"中文\",E1994,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear"},"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear","1,2-Benzoldicarbonsäure, Dihexylester, verzweigt und linear","1,2-苯二甲酸，支链和直链"]
[null,{"$f":"IF($B$1=\"English\",C1995,IF($B$1=\"Deutsch\",D1995,IF($B$1=\"中文\",E1995,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of DOTE und MOTE)"},"Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of DOTE und MOTE)","Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of DOTE und MOTE)","十一烷酸酯和2-乙基己基-10-乙基-4-[[2-[(2-乙基己基)氧]-2-氧代乙基]硫]-4-辛基-7-氧代-8-氧-3,5-二硫-4-十一烷酸酯（DOTE和MOTE的反应质量)"]
[null,{"$f":"IF($B$1=\"English\",C1996,IF($B$1=\"Deutsch\",D1996,IF($B$1=\"中文\",E1996,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium fluoride"},"Cadmium fluoride","Cadmiumfluorid","氟化镉"]
[null,{"$f":"IF($B$1=\"English\",C1997,IF($B$1=\"Deutsch\",D1997,IF($B$1=\"中文\",E1997,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium sulphate"},"Cadmium sulphate","Cadmiumsulfat","硫酸镉"]
[null,{"$f":"IF($B$1=\"English\",C1998,IF($B$1=\"Deutsch\",D1998,IF($B$1=\"中文\",E1998,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate (DEHP)"},"Bis(2-ethylhexyl)phthalate (DEHP)","Bis(2-ethylhexyl)phthalat (DEHP)","邻苯二甲酸二(2-乙基)己酯  (DEHP)"]
[null,{"$f":"IF($B$1=\"English\",C1999,IF($B$1=\"Deutsch\",D1999,IF($B$1=\"中文\",E1999,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-\ndithia-4-stannatetradecanoate (DOTE)"},"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-\ndithia-4-stannatetradecanoate (DOTE)","2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoat (DOTE)","二正辛基-双（巯乙酸2-乙基己酯）锡（DOTE）"]
[null,{"$f":"IF($B$1=\"English\",C2000,IF($B$1=\"Deutsch\",D2000,IF($B$1=\"中文\",E2000,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)"},"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)","2-Benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)","2-苯并三唑-2-基-4,6-二叔丁基苯酚（UV-320）"]
[null,{"$f":"IF($B$1=\"English\",C2001,IF($B$1=\"Deutsch\",D2001,IF($B$1=\"中文\",E2001,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)"},"2-(2H-benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)","2-(2H-Benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)","2-（2H-苯并三唑-2-基）-4,6-二叔戊基苯酚（ UV-328）"]
[null,{"$f":"IF($B$1=\"English\",C2002,IF($B$1=\"Deutsch\",D2002,IF($B$1=\"中文\",E2002,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-\nmethyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-\ndimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]\n[covering any of the individual isomers of [1] and [2] or\nany combination thereof]"},"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-\nmethyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-\ndimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]\n[covering any of the individual isomers of [1] and [2] or\nany combination thereof]","5-sec-Butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxan [1], \n\n5-sec-Butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxan [2]\n\n[Die einzelnen Stereoisomere von [1] und [2] sowie alle möglichen Kombinationen sind durch diesen Eintrag abgedeckt]","[1] 5-二级丁基-2-(2,4-二甲基环己-3-烯-1-基)-5-甲基-1,3-二氧六环  [2] 5-二级丁基-2-(4,6-二甲基环己-3-烯-1-基)-5-甲基-1,3-二氧六环  [包含以上[1]和[2]任何异构体或组合]"]
[null,{"$f":"IF($B$1=\"English\",C2003,IF($B$1=\"Deutsch\",D2003,IF($B$1=\"中文\",E2003,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane"},"Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane","Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane","以下物质的反应质量：5-[(2R)-丁烷-2-基]-2-[(1R,2R)-2,4-二甲基环己基-3-烯-1-基]-5-甲基-1,3-二恶烷，5-[(2R)-丁烷-2-基]-2-[(1R,2S)-2,4-二甲基环己基-3-烯-1-基]-5-甲基-1,3-二恶烷，5-[(2R)-丁烷-2-基]-2-[(1S,2R)-2,4-二甲基环己基-3-烯-1-基]-5-甲基-1,3-二恶烷，5-[(2R)-丁烷-2-基]-2-[(1S,2S)-2,4-二甲基环己基-3-烯-1-基]-5-甲基-1,3-二恶烷， 5-[(2S)-丁烷-2-基]-2-[(1S,2R)-2,4-二甲基环己基-3-烯-1-基]-5-甲基-1,3-二恶烷 ，5-[(2S)-丁烷-2-基l]-2-[(1S,2S)-2,4甲基环己基-3-烯-1-基]-5-甲基-1,3-二恶烷 "]
[null,{"$f":"IF($B$1=\"English\",C2004,IF($B$1=\"Deutsch\",D2004,IF($B$1=\"中文\",E2004,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane"},"2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane","2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane","2-(2,4-二甲基环己烯-3-基）-5-甲基-（1-甲基丙基）-1,3-二恶烷"]
[null,{"$f":"IF($B$1=\"English\",C2005,IF($B$1=\"Deutsch\",D2005,IF($B$1=\"中文\",E2005,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane "},"Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane ","Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane ","5-二级丁基-2-(4,6-二甲基环己-3-烯-1-基)-5-甲基-1,3-二氧六环 和 5-二级丁基-2-(2,4-二甲基环己-3-烯-1-基)-5-甲基-1,3-二氧六环 的反应质量"]
[null,{"$f":"IF($B$1=\"English\",C2006,IF($B$1=\"Deutsch\",D2006,IF($B$1=\"中文\",E2006,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-二恶烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-, 顺式"]
[null,{"$f":"IF($B$1=\"English\",C2007,IF($B$1=\"Deutsch\",D2007,IF($B$1=\"中文\",E2007,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二恶烷, 2-[(1S,2S)-2,4-二甲基-3-环己烯-1-基]-5-methyl-5-(1-甲基丙基)-, 反式"]
[null,{"$f":"IF($B$1=\"English\",C2008,IF($B$1=\"Deutsch\",D2008,IF($B$1=\"中文\",E2008,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二恶烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-基]-5-methyl-5-(1-甲基丙基)-, 反式"]
[null,{"$f":"IF($B$1=\"English\",C2009,IF($B$1=\"Deutsch\",D2009,IF($B$1=\"中文\",E2009,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-","1,3-二恶烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-,反式相对构型"]
[null,{"$f":"IF($B$1=\"English\",C2010,IF($B$1=\"Deutsch\",D2010,IF($B$1=\"中文\",E2010,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-二恶烷, 2-[(1R,2S)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-, 顺式"]
[null,{"$f":"IF($B$1=\"English\",C2011,IF($B$1=\"Deutsch\",D2011,IF($B$1=\"中文\",E2011,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二恶烷, 2-[(1R,2S)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-, 反式"]
[null,{"$f":"IF($B$1=\"English\",C2012,IF($B$1=\"Deutsch\",D2012,IF($B$1=\"中文\",E2012,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- "},"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- ","1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- ","1,3-二恶烷, 2-[(1S,2R)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-, 顺式"]
[null,{"$f":"IF($B$1=\"English\",C2013,IF($B$1=\"Deutsch\",D2013,IF($B$1=\"中文\",E2013,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二恶烷,  2-[(1S,2R)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-, 反式"]
[null,{"$f":"IF($B$1=\"English\",C2014,IF($B$1=\"Deutsch\",D2014,IF($B$1=\"中文\",E2014,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-二恶烷,  2-[(1S,2S)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-, 顺式"]
[null,{"$f":"IF($B$1=\"English\",C2015,IF($B$1=\"Deutsch\",D2015,IF($B$1=\"中文\",E2015,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-"},"1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","1,3-二恶烷, 2-(2,4-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基)-"]
[null,{"$f":"IF($B$1=\"English\",C2016,IF($B$1=\"Deutsch\",D2016,IF($B$1=\"中文\",E2016,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane"},"5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-仲丁酯-2-(4,6-二甲基环己-3-烯-1-基)-5-甲基-1,3-二恶烷"]
[null,{"$f":"IF($B$1=\"English\",C2017,IF($B$1=\"Deutsch\",D2017,IF($B$1=\"中文\",E2017,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane"},"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-二级丁基-2-(2,4-二甲基环己-3-烯-1-基)-5-甲基-1,3-二氧六环"]
[null,{"$f":"IF($B$1=\"English\",C2018,IF($B$1=\"Deutsch\",D2018,IF($B$1=\"中文\",E2018,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-","1,3-二恶烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-基]-5-甲基-5-(1-甲基丙基))-, 顺式相对构型"]
[null,{"$f":"IF($B$1=\"English\",C2019,IF($B$1=\"Deutsch\",D2019,IF($B$1=\"中文\",E2019,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters \nwith ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)"},"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters \nwith ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)","1,2-Benzoldicarbonsäure, Di-C6-10-alkylester; 1,2-Benzoldicarbonsäure, gemischte Decyl- und Hexyl- und Octyldiester mit ≥ 0,3% Dihexylphthalat (EG Nr. 201-559-5)","邻苯二甲酸二（C6-C6）烷基酯：(癸基，己基，辛基）酯 与1，2-邻苯二甲酸的复合物且邻苯二甲酸二己酯含量≥ 0.3% (EC编码: 201-559-5)"]
[null,{"$f":"IF($B$1=\"English\",C2020,IF($B$1=\"Deutsch\",D2020,IF($B$1=\"中文\",E2020,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters"},"1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters","1,2-Benzoldicarbonsäure, gemischte Decyl- und Hexyl- und Octyldiester ","1,2-苯二甲酸，混合癸基和己基及辛基二酯"]
[null,{"$f":"IF($B$1=\"English\",C2021,IF($B$1=\"Deutsch\",D2021,IF($B$1=\"中文\",E2021,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C6-10-alkyl esters"},"1,2-Benzenedicarboxylic acid, di-C6-10-alkyl esters","1,2-Benzoldicarbonsäure, Di-C6-10-alkylester","1,2-苯二甲酸 ，双C6-10-烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C2022,IF($B$1=\"Deutsch\",D2022,IF($B$1=\"中文\",E2022,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorononan-1-oic-acid and its sodium and ammonium salts"},"Perfluorononan-1-oic-acid and its sodium and ammonium salts","Perfluornonan-1-säure und seine Narium- und Ammoniumsalze\n","全氟萘烷-1-酸及其钠盐和铵盐"]
[null,{"$f":"IF($B$1=\"English\",C2023,IF($B$1=\"Deutsch\",D2023,IF($B$1=\"中文\",E2023,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorononan-1-oic acid"},"Perfluorononan-1-oic acid","Perfluornonan-1-säure","全氟萘烷-1-酸"]
[null,{"$f":"IF($B$1=\"English\",C2024,IF($B$1=\"Deutsch\",D2024,IF($B$1=\"中文\",E2024,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"perfluorononan-1-oic acid sodium salts"},"perfluorononan-1-oic acid sodium salts","Natrium perfluornonanoat","全氟萘烷-1-酸钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2025,IF($B$1=\"Deutsch\",D2025,IF($B$1=\"中文\",E2025,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"perfluorononan-1-oic acid ammonium salts"},"perfluorononan-1-oic acid ammonium salts","Ammonium perfluornonanoat","全氟萘烷-1-酸铵盐"]
[null,{"$f":"IF($B$1=\"English\",C2026,IF($B$1=\"Deutsch\",D2026,IF($B$1=\"中文\",E2026,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nitrobenzene"},"Nitrobenzene","Nitrobenzol","硝基苯 "]
[null,{"$f":"IF($B$1=\"English\",C2027,IF($B$1=\"Deutsch\",D2027,IF($B$1=\"中文\",E2027,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)"},"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)","2-(2H-Benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)","2-(2’-羟基-3’-仲-丁基-5’-叔-丁基苯基) 苯並三唑 (UV-350)"]
[null,{"$f":"IF($B$1=\"English\",C2028,IF($B$1=\"Deutsch\",D2028,IF($B$1=\"中文\",E2028,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-propanesultone"},"1,3-propanesultone","1,3-Propansulton","1,3-丙基磺酸内酯"]
[null,{"$f":"IF($B$1=\"English\",C2029,IF($B$1=\"Deutsch\",D2029,IF($B$1=\"中文\",E2029,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)"},"2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)","2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)","2,4-二叔丁基-6-(5-氯苯三唑-2-基)苯酚(UV-327)"]
[null,{"$f":"IF($B$1=\"English\",C2030,IF($B$1=\"Deutsch\",D2030,IF($B$1=\"中文\",E2030,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[def]chrysene (Benzo[a]pyrene)"},"Benzo[def]chrysene (Benzo[a]pyrene)","Benzo[a]pyren (Benzo[def]chrysen)","苯并[def]屈 (苯并[a]芘)"]
[null,{"$f":"IF($B$1=\"English\",C2031,IF($B$1=\"Deutsch\",D2031,IF($B$1=\"中文\",E2031,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Heptylphenol, branched and linear (4-HPbl)"},"4-Heptylphenol, branched and linear (4-HPbl)","4-Heptylphenol, verzweigt und linear\n(4-HPbl)\n\n[Substanzen mit einer linearen und/oder verzweigten Alkylkette mit einer Kohlenstoffzahl von 7, die überwiegend in Position 4 kovalent an Phenol gebunden ist, wobei auch UVCB- und genau definierte Substanzen eingeschlossen sind, die eines der einzelnen Isomere oder eine Kombination davon enthalten]","4-庚基酚，支链和直链 - （4-HPbl）"]
[null,{"$f":"IF($B$1=\"English\",C2032,IF($B$1=\"Deutsch\",D2032,IF($B$1=\"中文\",E2032,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, heptyl derivs."},"Phenol, heptyl derivs.","Phenol, heptyl derivs.","酚类，庚基衍生物"]
[null,{"$f":"IF($B$1=\"English\",C2033,IF($B$1=\"Deutsch\",D2033,IF($B$1=\"中文\",E2033,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-heptylphenol "},"4-heptylphenol ","4-heptylphenol ","4-庚基苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C2034,IF($B$1=\"Deutsch\",D2034,IF($B$1=\"中文\",E2034,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1-diethylpropyl)- "},"Phenol, 4-(1,1-diethylpropyl)- ","Phenol, 4-(1,1-diethylpropyl)- ","酚，4-(1,1-二乙基丙基)-"]
[null,{"$f":"IF($B$1=\"English\",C2035,IF($B$1=\"Deutsch\",D2035,IF($B$1=\"中文\",E2035,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1-dimethylpentyl)-"},"Phenol, 4-(1,1-dimethylpentyl)-","Phenol, 4-(1,1-dimethylpentyl)-","酚，4-(1,1-二甲基戊基)-"]
[null,{"$f":"IF($B$1=\"English\",C2036,IF($B$1=\"Deutsch\",D2036,IF($B$1=\"中文\",E2036,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,2,2-trimethylbutyl)-"},"Phenol, 4-(1,2,2-trimethylbutyl)-","Phenol, 4-(1,2,2-trimethylbutyl)-","酚，4-(1,2,2-三甲基丁基)-"]
[null,{"$f":"IF($B$1=\"English\",C2037,IF($B$1=\"Deutsch\",D2037,IF($B$1=\"中文\",E2037,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,2-dimethylpentyl)-"},"Phenol, 4-(1,2-dimethylpentyl)-","Phenol, 4-(1,2-dimethylpentyl)-","酚，4-(1,2-二甲基戊基)-"]
[null,{"$f":"IF($B$1=\"English\",C2038,IF($B$1=\"Deutsch\",D2038,IF($B$1=\"中文\",E2038,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,3,3-trimethylbutyl)- "},"Phenol, 4-(1,3,3-trimethylbutyl)- ","Phenol, 4-(1,3,3-trimethylbutyl)- ","酚，4-(1,3,3-三甲基丁基)-"]
[null,{"$f":"IF($B$1=\"English\",C2039,IF($B$1=\"Deutsch\",D2039,IF($B$1=\"中文\",E2039,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,3-dimethylpentyl)-"},"Phenol, 4-(1,3-dimethylpentyl)-","Phenol, 4-(1,3-dimethylpentyl)-","酚，4-(1,3-二甲基戊基)-"]
[null,{"$f":"IF($B$1=\"English\",C2040,IF($B$1=\"Deutsch\",D2040,IF($B$1=\"中文\",E2040,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,4-dimethylpentyl)-"},"Phenol, 4-(1,4-dimethylpentyl)-","Phenol, 4-(1,4-dimethylpentyl)-","酚，4-(1,4-二甲基戊基)-"]
[null,{"$f":"IF($B$1=\"English\",C2041,IF($B$1=\"Deutsch\",D2041,IF($B$1=\"中文\",E2041,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-"},"Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-","Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-","酚，4-(1-乙基-2,2-二甲基丙基)-"]
[null,{"$f":"IF($B$1=\"English\",C2042,IF($B$1=\"Deutsch\",D2042,IF($B$1=\"中文\",E2042,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-"},"Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-","Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-","酚，4-(1-乙基-1,2-二甲基丙烷)-"]
[null,{"$f":"IF($B$1=\"English\",C2043,IF($B$1=\"Deutsch\",D2043,IF($B$1=\"中文\",E2043,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethylpentyl)-"},"Phenol, 4-(1-ethylpentyl)-","Phenol, 4-(1-ethylpentyl)-","酚，4-(1-乙基戊基)-"]
[null,{"$f":"IF($B$1=\"English\",C2044,IF($B$1=\"Deutsch\",D2044,IF($B$1=\"中文\",E2044,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-methylhexyl)-"},"Phenol, 4-(1-methylhexyl)-","Phenol, 4-(1-methylhexyl)-","酚，4-(1-甲基己基)-"]
[null,{"$f":"IF($B$1=\"English\",C2045,IF($B$1=\"Deutsch\",D2045,IF($B$1=\"中文\",E2045,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-propylbutyl)-"},"Phenol, 4-(1-propylbutyl)-","Phenol, 4-(1-propylbutyl)-","酚，4-(1-丙基丁基)-"]
[null,{"$f":"IF($B$1=\"English\",C2046,IF($B$1=\"Deutsch\",D2046,IF($B$1=\"中文\",E2046,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(3-ethylpentyl)- "},"Phenol, 4-(3-ethylpentyl)- ","Phenol, 4-(3-ethylpentyl)- ","酚，4-(3-乙基戊基)-"]
[null,{"$f":"IF($B$1=\"English\",C2047,IF($B$1=\"Deutsch\",D2047,IF($B$1=\"中文\",E2047,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(3-methylhexyl)- "},"Phenol, 4-(3-methylhexyl)- ","Phenol, 4-(3-methylhexyl)- ","酚，4-(3-甲基己基)-"]
[null,{"$f":"IF($B$1=\"English\",C2048,IF($B$1=\"Deutsch\",D2048,IF($B$1=\"中文\",E2048,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(4-methylhexyl)-"},"Phenol, 4-(4-methylhexyl)-","Phenol, 4-(4-methylhexyl)-","酚，4-(4-甲基己基)-"]
[null,{"$f":"IF($B$1=\"English\",C2049,IF($B$1=\"Deutsch\",D2049,IF($B$1=\"中文\",E2049,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(5-methylhexyl)-"},"Phenol, 4-(5-methylhexyl)-","Phenol, 4-(5-methylhexyl)-","酚，4-(5-甲基己基)-"]
[null,{"$f":"IF($B$1=\"English\",C2050,IF($B$1=\"Deutsch\",D2050,IF($B$1=\"中文\",E2050,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-"},"Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-","Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-","酚，4-(2-甲基-1-(1-甲基乙基)丙基)-"]
[null,{"$f":"IF($B$1=\"English\",C2051,IF($B$1=\"Deutsch\",D2051,IF($B$1=\"中文\",E2051,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(2,3-dimethylpentan-2-yl)phenol "},"4-(2,3-dimethylpentan-2-yl)phenol ","4-(2,3-dimethylpentan-2-yl)phenol ","4-(2,3-二甲基戊烷-2-基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C2052,IF($B$1=\"Deutsch\",D2052,IF($B$1=\"中文\",E2052,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(3-methylhexan-3-yl)phenol"},"4-(3-methylhexan-3-yl)phenol","4-(3-methylhexan-3-yl)phenol","4-(3-甲基己烷-3-基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2053,IF($B$1=\"Deutsch\",D2053,IF($B$1=\"中文\",E2053,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-tert-heptyl-"},"Phenol, 4-tert-heptyl-","Phenol, 4-tert-heptyl-","酚，4-叔庚醇"]
[null,{"$f":"IF($B$1=\"English\",C2054,IF($B$1=\"Deutsch\",D2054,IF($B$1=\"中文\",E2054,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1,3-trimethylbutyl)-"},"Phenol, 4-(1,1,3-trimethylbutyl)-","Phenol, 4-(1,1,3-trimethylbutyl)-","酚，4-(1,1,3-三甲基丁基)-"]
[null,{"$f":"IF($B$1=\"English\",C2055,IF($B$1=\"Deutsch\",D2055,IF($B$1=\"中文\",E2055,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1,2,2-tetramethylpropyl)- "},"Phenol, 4-(1,1,2,2-tetramethylpropyl)- ","Phenol, 4-(1,1,2,2-tetramethylpropyl)- ","酚，4-(1,1,2,2-四甲基丙基)-"]
[null,{"$f":"IF($B$1=\"English\",C2056,IF($B$1=\"Deutsch\",D2056,IF($B$1=\"中文\",E2056,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethyl-3-methylbutyl)-"},"Phenol, 4-(1-ethyl-3-methylbutyl)-","Phenol, 4-(1-ethyl-3-methylbutyl)-","酚，4-(1-乙基-3-甲基丁基)-"]
[null,{"$f":"IF($B$1=\"English\",C2057,IF($B$1=\"Deutsch\",D2057,IF($B$1=\"中文\",E2057,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-(1,1-dimethylpropyl)phenol"},"p-(1,1-dimethylpropyl)phenol","p-(1,1-dimethylpropyl)phenol\n4-tert-Pentylphenol (PTAP)","对-(1,1-二甲基丙基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2058,IF($B$1=\"Deutsch\",D2058,IF($B$1=\"中文\",E2058,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"},"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts","Nonadecafluorodecansäure (PFDA) und ihre Natrium- und Ammonium-Salze\nNonadecafluordecansäure\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat","全氟癸酸（PFDA）及其钠盐和铵盐"]
[null,{"$f":"IF($B$1=\"English\",C2059,IF($B$1=\"Deutsch\",D2059,IF($B$1=\"中文\",E2059,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decanoic acid, nonadecafluoro-, sodium salt "},"Decanoic acid, nonadecafluoro-, sodium salt ","Decansäure, Nonadecafluoro-, Natriumsalz","癸酸，非全氟，钠盐 "]
[null,{"$f":"IF($B$1=\"English\",C2060,IF($B$1=\"Deutsch\",D2060,IF($B$1=\"中文\",E2060,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonadecafluorodecanoic acid"},"Nonadecafluorodecanoic acid","Nonadecafluordecansäure","十一氟癸酸"]
[null,{"$f":"IF($B$1=\"English\",C2061,IF($B$1=\"Deutsch\",D2061,IF($B$1=\"中文\",E2061,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammoniumnonadecafluordecanoat"},"Ammoniumnonadecafluordecanoat","Ammoniumnonadecafluordecanoat","十四烷铵"]
[null,{"$f":"IF($B$1=\"English\",C2062,IF($B$1=\"Deutsch\",D2062,IF($B$1=\"中文\",E2062,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"sodium nonadecafluorodecanoate "},"sodium nonadecafluorodecanoate ","Natriumnonadecafluordecanoat","非全氟癸酸钠 "]
[null,{"$f":"IF($B$1=\"English\",C2063,IF($B$1=\"Deutsch\",D2063,IF($B$1=\"中文\",E2063,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexane-1-sulphonic acid and its salts"},"Perfluorohexane-1-sulphonic acid and its salts","Perfluorhexan-1-sulfonsäure und ihre Salze\n(PFHxS)","全氟己烷-1-磺酸及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C2064,IF($B$1=\"Deutsch\",D2064,IF($B$1=\"中文\",E2064,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium perfluorohexane-1-sulphonate"},"Potassium perfluorohexane-1-sulphonate","Potassium perfluorohexane-1-sulphonate","全氟己烷-1-磺酸钾"]
[null,{"$f":"IF($B$1=\"English\",C2065,IF($B$1=\"Deutsch\",D2065,IF($B$1=\"中文\",E2065,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexane-1-sulphonic acid"},"Perfluorohexane-1-sulphonic acid","Perfluorohexane-1-sulphonic acid","全氟己烷-1-磺酸"]
[null,{"$f":"IF($B$1=\"English\",C2066,IF($B$1=\"Deutsch\",D2066,IF($B$1=\"中文\",E2066,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)"},"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)","Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)","十三氟己烷磺酸与2,2'-亚氨基二乙醇的化合物(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2067,IF($B$1=\"Deutsch\",D2067,IF($B$1=\"中文\",E2067,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium perfluorohexane-1-sulphonate"},"Ammonium perfluorohexane-1-sulphonate","Ammonium perfluorohexane-1-sulphonate","全氟己烷-1-磺酸铵"]
[null,{"$f":"IF($B$1=\"English\",C2068,IF($B$1=\"Deutsch\",D2068,IF($B$1=\"中文\",E2068,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，镓盐（9CI）"]
[null,{"$f":"IF($B$1=\"English\",C2069,IF($B$1=\"Deutsch\",D2069,IF($B$1=\"中文\",E2069,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","双(4-甲基苯基)苯基锍，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2070,IF($B$1=\"Deutsch\",D2070,IF($B$1=\"中文\",E2070,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，钪（3+）盐salt (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C2071,IF($B$1=\"Deutsch\",D2071,IF($B$1=\"中文\",E2071,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，钕（3+）盐 (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C2072,IF($B$1=\"Deutsch\",D2072,IF($B$1=\"中文\",E2072,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟，钇（3+）盐 (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C2073,IF($B$1=\"Deutsch\",D2073,IF($B$1=\"中文\",E2073,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)"},"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)","Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)","锍，(硫代-4,1-苯)双[二苯基-，与1,1,2,2,3,3,4,4,5,5,6,6,三氟-1-己烷磺酸的盐(1:2)"]
[null,{"$f":"IF($B$1=\"English\",C2074,IF($B$1=\"Deutsch\",D2074,IF($B$1=\"中文\",E2074,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic"},"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","碘鎓，双[4-(1,1-二甲基丙基)苯基]-，与1,1,2,2,3,3,4,4,5,5,6,6-三氟-1-己烷磺酸的盐"]
[null,{"$f":"IF($B$1=\"English\",C2075,IF($B$1=\"Deutsch\",D2075,IF($B$1=\"中文\",E2075,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三[4-(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6-三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2076,IF($B$1=\"Deutsch\",D2076,IF($B$1=\"中文\",E2076,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，锂盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C2077,IF($B$1=\"Deutsch\",D2077,IF($B$1=\"中文\",E2077,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，锌盐"]
[null,{"$f":"IF($B$1=\"English\",C2078,IF($B$1=\"Deutsch\",D2078,IF($B$1=\"中文\",E2078,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","碘鎓，双[4-(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2079,IF($B$1=\"Deutsch\",D2079,IF($B$1=\"中文\",E2079,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt","1-己烷磺酸，1，1，2，2，3，3，4，4，5，5，6，6，6-三氟-，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2080,IF($B$1=\"Deutsch\",D2080,IF($B$1=\"中文\",E2080,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)"},"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","碘鎓，双[(1,1-二甲基乙基)苯基]-，与1,1,2,2,3,3,4,4,5,5,6,6-三氟-1-己烷磺酸的盐(1:1) (9CI)"]
[null,{"$f":"IF($B$1=\"English\",C2081,IF($B$1=\"Deutsch\",D2081,IF($B$1=\"中文\",E2081,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","(4-甲基苯基)二苯基锍，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-1-己烷磺酸盐(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2082,IF($B$1=\"Deutsch\",D2082,IF($B$1=\"中文\",E2082,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","锍， [4-[(2-甲基-1-氧代-2-丙烯-1-基)氧基]苯基]二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2083,IF($B$1=\"Deutsch\",D2083,IF($B$1=\"中文\",E2083,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"},"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate","Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate","锍，[4-[(2-甲基-1-氧代-2-丙烯基)氧]苯基]二苯基，与1，1，2，2，3，3，4，4，5，5，6，6，6-十三氟-1-己烷磺酸（1:1）的盐，与2-乙基三环[3.3.1.13,7]癸-2-基2-甲基-2-丙烯酸酯、3-羟基三环[3.3.1.13,7]癸-1-基2-甲基-2-丙烯酸酯和四氢-2-氧代-3-呋喃基2-甲基-2-丙烯酸酯的聚合物"]
[null,{"$f":"IF($B$1=\"English\",C2084,IF($B$1=\"Deutsch\",D2084,IF($B$1=\"中文\",E2084,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，铯盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2085,IF($B$1=\"Deutsch\",D2085,IF($B$1=\"中文\",E2085,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","二苯醚[k,n][1,4,7,10,13]四氧杂环十五烷，19-[4-(1,1-二甲基乙基)苯基]-6,7,9,10,12,13-六氢-，1,1,2,2,3,3,4,4,5,5,6,6-三氟-1-己烷磺酸酯 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2086,IF($B$1=\"Deutsch\",D2086,IF($B$1=\"中文\",E2086,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","乙铵, N-[4-[[4-(二乙基氨基)苯基][4-(乙基氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-乙基-, 1,1,2,2,3,3,4,4,5,5,6,6-三氟-1-己烷磺酸酯 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2087,IF($B$1=\"Deutsch\",D2087,IF($B$1=\"中文\",E2087,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","甲胺素, N-[4-[[4-(二甲基氨基)苯基][4-(乙基氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-甲基-, 1,1,2,3,4,4,5,5,6,6-三氟-1-己烷磺酸酯 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2088,IF($B$1=\"Deutsch\",D2088,IF($B$1=\"中文\",E2088,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","甲胺素, N-[4-[[4-(二甲基氨基)苯基][4-(苯基氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-甲基-, 1,1,2,3,4,4,5,6,6-三氟-1-己烷磺酸酯 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2089,IF($B$1=\"Deutsch\",D2089,IF($B$1=\"中文\",E2089,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","β-环糊精，与1,1,2,2,3,3,4,4,5,6,6,6-三氟-1-己烷磺酸离子(1-)(1:1)混合"]
[null,{"$f":"IF($B$1=\"English\",C2090,IF($B$1=\"Deutsch\",D2090,IF($B$1=\"中文\",E2090,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","γ-环糊精，与1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-1-己烷磺酸离子的组合(1-)(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2091,IF($B$1=\"Deutsch\",D2091,IF($B$1=\"中文\",E2091,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三苯基锍，1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸钠 (1：1)"]
[null,{"$f":"IF($B$1=\"English\",C2092,IF($B$1=\"Deutsch\",D2092,IF($B$1=\"中文\",E2092,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","喹啉, 1-(羧甲基)-4-[2-[4-[4-(2,2-二苯基乙烯基)苯基]-1,2,3,3a,4,8b-六氢环戊[b]吲哚-7-基]乙烯基]-, 1,1,2,2,3,3,4,5,6,6-十三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2093,IF($B$1=\"Deutsch\",D2093,IF($B$1=\"中文\",E2093,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","碘鎓，二苯基，1,1,2,3,4,5,6,6-三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2094,IF($B$1=\"Deutsch\",D2094,IF($B$1=\"中文\",E2094,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","甲胺，N,N,N-三甲基-，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐（1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2095,IF($B$1=\"Deutsch\",D2095,IF($B$1=\"中文\",E2095,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，与2-甲基-2-丙胺（1:1）的组合"]
[null,{"$f":"IF($B$1=\"English\",C2096,IF($B$1=\"Deutsch\",D2096,IF($B$1=\"中文\",E2096,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，与吡咯烷 (1:1)的组合"]
[null,{"$f":"IF($B$1=\"English\",C2097,IF($B$1=\"Deutsch\",D2097,IF($B$1=\"中文\",E2097,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","乙胺，N,N,N-三乙基，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐（1：1）"]
[null,{"$f":"IF($B$1=\"English\",C2098,IF($B$1=\"Deutsch\",D2098,IF($B$1=\"中文\",E2098,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid"},"1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid","1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid","1-丁铵，N,N,N-三丁基-，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐"]
[null,{"$f":"IF($B$1=\"English\",C2099,IF($B$1=\"Deutsch\",D2099,IF($B$1=\"中文\",E2099,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"California Proposition 65 (Reiter 16) "},"California Proposition 65 (Reiter 16) ","California Proposition 65 (Reiter 16) ","加利福尼亚州第65号提案（第16个产品）"]
[null,{"$f":"IF($B$1=\"English\",C2100,IF($B$1=\"Deutsch\",D2100,IF($B$1=\"中文\",E2100,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Safe Drinking Water and Toxic Enforcement Act of 1986, as amended (also known as California Proposition 65)"},"Safe Drinking Water and Toxic Enforcement Act of 1986, as amended (also known as California Proposition 65)","Safe Drinking Water and Toxic Enforcement Act of 1986, as amended (also known as California Proposition 65)","1986年安全饮用水和毒性强制法案（修正案）（也称加利福尼亚州第65号提案）"]
[null,{"$f":"IF($B$1=\"English\",C2101,IF($B$1=\"Deutsch\",D2101,IF($B$1=\"中文\",E2101,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The supplier must inform Bosch if any substance on the California Proposition 65 List is contained in a product or"},"The supplier must inform Bosch if any substance on the California Proposition 65 List is contained in a product or","The supplier must inform Bosch if any substance on the California Proposition 65 List is contained in a product or","出现下述情况时供应商必须通知博世：加利福尼亚65号提案清单中的任何物质以任何浓度包含在产品或"]
[null,{"$f":"IF($B$1=\"English\",C2102,IF($B$1=\"Deutsch\",D2102,IF($B$1=\"中文\",E2102,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"spare part or mixture in any concentration. The supplier is obliged to track the Proposition 65 List regularly "},"spare part or mixture in any concentration. The supplier is obliged to track the Proposition 65 List regularly ","spare part or mixture in any concentration. The supplier is obliged to track the Proposition 65 List regularly ","备件或配制品中。供应商有义务（在OEHHA网站上）定期追踪65号提案清单，"]
[null,{"$f":"IF($B$1=\"English\",C2103,IF($B$1=\"Deutsch\",D2103,IF($B$1=\"中文\",E2103,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(on OEHHA website) and to inform Bosch purchasing contact immediately if he gets information "},"(on OEHHA website) and to inform Bosch purchasing contact immediately if he gets information ","(on OEHHA website) and to inform Bosch purchasing contact immediately if he gets information ","并在收到信息后立即通知博世采购联系人"]
[null,{"$f":"IF($B$1=\"English\",C2104,IF($B$1=\"Deutsch\",D2104,IF($B$1=\"中文\",E2104,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"that any substance on the Proposition 65 List may be included in supplied material."},"that any substance on the Proposition 65 List may be included in supplied material.","that any substance on the Proposition 65 List may be included in supplied material.","在供应给博世的材料中可能含有65号提案清单中的某种或某些物质。"]
[null,{"$f":"IF($B$1=\"English\",C2105,IF($B$1=\"Deutsch\",D2105,IF($B$1=\"中文\",E2105,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Proposition 65 List:"},"Proposition 65 List:","Proposition 65 List:","65号提案清单："]
[null,{"$f":"IF($B$1=\"English\",C2106,IF($B$1=\"Deutsch\",D2106,IF($B$1=\"中文\",E2106,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Name of contained Substances"},"Name of contained Substances","Name of contained Substances","所含物质的名称"]
[null,{"$f":"IF($B$1=\"English\",C2107,IF($B$1=\"Deutsch\",D2107,IF($B$1=\"中文\",E2107,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS-Number"},"CAS-Number","CAS-Number","CAS编号"]
[null,{"$f":"IF($B$1=\"English\",C2108,IF($B$1=\"Deutsch\",D2108,IF($B$1=\"中文\",E2108,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient [mass%]"},"Concentration of ingredient [mass%]","Concentration of ingredient [mass%]","成分浓度[质量％]"]
[null,{"$f":"IF($B$1=\"English\",C2109,IF($B$1=\"Deutsch\",D2109,IF($B$1=\"中文\",E2109,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Designation of the material that contains the declared substance"},"Designation of the material that contains the declared substance","Designation of the material that contains the declared substance","指定包含申报物质的材料"]
[null,{"$f":"IF($B$1=\"English\",C2110,IF($B$1=\"Deutsch\",D2110,IF($B$1=\"中文\",E2110,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三苯基(苯甲基)磷酸盐, 1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-1-己烷磺酸酯 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2111,IF($B$1=\"Deutsch\",D2111,IF($B$1=\"中文\",E2111,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","1-己烷磺酸，1,1,2,2,3,3,4,4,5,5,6,6,6-三氟-，与N,N-二乙基乙胺的组合（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C2112,IF($B$1=\"Deutsch\",D2112,IF($B$1=\"中文\",E2112,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-isopropylidenediphenol (Bisphenol A)"},"4,4'-isopropylidenediphenol (Bisphenol A)","4,4'-isopropylidendiphenol\n(Bisphenol A)","4,4’-异丙基二苯酚（双酚A）"]
[null,{"$f":"IF($B$1=\"English\",C2113,IF($B$1=\"Deutsch\",D2113,IF($B$1=\"中文\",E2113,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction products of 1,3,4-thiadiazolidine-2,5-dithione,\nformaldehyde and 4-heptylphenol, branched and linear (RP-HP)\n[with ≥0.1% w/w 4-heptylphenol, branched and linear (4-HPbl)1]"},"Reaction products of 1,3,4-thiadiazolidine-2,5-dithione,\nformaldehyde and 4-heptylphenol, branched and linear (RP-HP)\n[with ≥0.1% w/w 4-heptylphenol, branched and linear (4-HPbl)1]","Reaktionsprodukt aus 1,3,4-Thiadiazolidin-2,5-dithion, Formaldehyd und 4-Heptylphenol, verzweigt und linear (RP-HP) \nmit ≥ 0,1% w/w 4-Heptylphenol, verzweigt und linear (4-HPbl)","1,3,4-噻二唑烷-2,5-二硫酮，甲醛，支链和线性的4-庚基苯酚 （RP-HP）[与≥0.1% w/w的4-庚基苯酚，支链和直链(4-HPbl)1] 的反应产物。"]
[null,{"$f":"IF($B$1=\"English\",C2114,IF($B$1=\"Deutsch\",D2114,IF($B$1=\"中文\",E2114,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs."},"Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs.","Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs.","1,3,4-噻二唑烷-2,5-二硫酮、甲醛、苯酚庚基衍生物的反应产物"]
[null,{"$f":"IF($B$1=\"English\",C2115,IF($B$1=\"Deutsch\",D2115,IF($B$1=\"中文\",E2115,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine"},"Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine","Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine","甲醛，与支链和直链庚基苯酚、二硫化碳和肼的反应产物"]
[null,{"$f":"IF($B$1=\"English\",C2116,IF($B$1=\"Deutsch\",D2116,IF($B$1=\"中文\",E2116,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium carbonate"},"Cadmium carbonate","Cadmiumcarbonat","碳酸镉"]
[null,{"$f":"IF($B$1=\"English\",C2117,IF($B$1=\"Deutsch\",D2117,IF($B$1=\"中文\",E2117,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium hydroxide, Cd(OH)2\n"},"Cadmium hydroxide, Cd(OH)2\n","Cadmiumhydroxid","氢氧化镉, Cd(OH)2\n"]
[null,{"$f":"IF($B$1=\"English\",C2118,IF($B$1=\"Deutsch\",D2118,IF($B$1=\"中文\",E2118,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium nitrate"},"Cadmium nitrate","Cadmiumnitrat","硝酸镉"]
[null,{"$f":"IF($B$1=\"English\",C2119,IF($B$1=\"Deutsch\",D2119,IF($B$1=\"中文\",E2119,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benz[a]anthracene"},"Benz[a]anthracene","Benz[a]anthracen","苯并[a]蒽"]
[null,{"$f":"IF($B$1=\"English\",C2120,IF($B$1=\"Deutsch\",D2120,IF($B$1=\"中文\",E2120,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chrysen"},"Chrysen","Chrysen","屈"]
[null,{"$f":"IF($B$1=\"English\",C2121,IF($B$1=\"Deutsch\",D2121,IF($B$1=\"中文\",E2121,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,6,7,8,9,14,15,16,17,17,18,18-\nDodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane\nPlus”TM) [covering any of its individual anti- and syn-isomers or any combination\nthereof]"},"1,6,7,8,9,14,15,16,17,17,18,18-\nDodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane\nPlus”TM) [covering any of its individual anti- and syn-isomers or any combination\nthereof]","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-dien (“Dechloran Plus”TM) \n[deckt alle individuellen anti- und syn-Isomere oder Kombinationen daraus ab]","1,6,7,8,9,14,15,16,17,17,18,18- 十二氯五环[12.2.1.16,9.02,13.05,10]辛十-7,15-二烯(“Dechlorane Plus”TM)涵盖其任何单独的反和同分异构体或其任何组合] "]
[null,{"$f":"IF($B$1=\"English\",C2122,IF($B$1=\"Deutsch\",D2122,IF($B$1=\"中文\",E2122,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene"},"(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-十二氯五环[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]十八碳烯-7,15-二烯"]
[null,{"$f":"IF($B$1=\"English\",C2123,IF($B$1=\"Deutsch\",D2123,IF($B$1=\"中文\",E2123,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene"},"1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene","1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene","1,6,7,8,9,14,15,16,17,17,18,18-十二氯五环[12.2.1.16,9.02,13.05,10]十八碳烯-7,15-二烯"]
[null,{"$f":"IF($B$1=\"English\",C2124,IF($B$1=\"Deutsch\",D2124,IF($B$1=\"中文\",E2124,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene"},"(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-十二氯五环[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]十八碳烯-7,15-二烯"]
[null,{"$f":"IF($B$1=\"English\",C2125,IF($B$1=\"Deutsch\",D2125,IF($B$1=\"中文\",E2125,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene"},"rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","相对构型-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-十二氯-1,4,4a,5,6,6a,7,10,10a,11,12,12a-十二氢-1,4:7,10-二甲基二苯醚[a,e]环辛烯"]
[null,{"$f":"IF($B$1=\"English\",C2126,IF($B$1=\"Deutsch\",D2126,IF($B$1=\"中文\",E2126,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene"},"rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","相对构型-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-十二氯-1,4,4a,5,6,6a,7,10,10a,11,12,12a-十二氢-1,4:7,10-二甲基二苯醚[a,e]环辛烯"]
[null,{"$f":"IF($B$1=\"English\",C2127,IF($B$1=\"Deutsch\",D2127,IF($B$1=\"中文\",E2127,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)"},"Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)","Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)","苯-1,2,4-三羧酸1,2酸酐（偏苯三酸酐）(TMA)"]
[null,{"$f":"IF($B$1=\"English\",C2128,IF($B$1=\"Deutsch\",D2128,IF($B$1=\"中文\",E2128,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dicyclohexyl phthalate (DCHP)"},"Dicyclohexyl phthalate (DCHP)","Dicyclohexylphthalat (DCHP)","邻苯二甲酸二环己酯 (DCHP)"]
[null,{"$f":"IF($B$1=\"English\",C2129,IF($B$1=\"Deutsch\",D2129,IF($B$1=\"中文\",E2129,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octamethylcyclotetrasiloxane (D4)"},"Octamethylcyclotetrasiloxane (D4)","Oktamethylcyclotetrasiloxan (D4)","八甲基环四硅氧烷（D4）"]
[null,{"$f":"IF($B$1=\"English\",C2130,IF($B$1=\"Deutsch\",D2130,IF($B$1=\"中文\",E2130,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decamethylcyclopentasiloxane (D5)"},"Decamethylcyclopentasiloxane (D5)","Dekamethylcyclopentasiloxan (D5)","十甲基环戊硅氧烷 (D5)"]
[null,{"$f":"IF($B$1=\"English\",C2131,IF($B$1=\"Deutsch\",D2131,IF($B$1=\"中文\",E2131,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dodecamethylcyclohexasiloxane (D6)"},"Dodecamethylcyclohexasiloxane (D6)","Dodekamethylcyclohexasiloxan (D6)","十二甲基环己硅氧烷 (D6)"]
[null,{"$f":"IF($B$1=\"English\",C2132,IF($B$1=\"Deutsch\",D2132,IF($B$1=\"中文\",E2132,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Blei","铅"]
[null,{"$f":"IF($B$1=\"English\",C2133,IF($B$1=\"Deutsch\",D2133,IF($B$1=\"中文\",E2133,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium octaborate"},"Disodium octaborate","Dinatriumoctaborat","八硼酸二钠"]
[null,{"$f":"IF($B$1=\"English\",C2134,IF($B$1=\"Deutsch\",D2134,IF($B$1=\"中文\",E2134,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[ghi]perylene"},"Benzo[ghi]perylene","Benzo[ghi]perylen","苯并[ghi]苝"]
[null,{"$f":"IF($B$1=\"English\",C2135,IF($B$1=\"Deutsch\",D2135,IF($B$1=\"中文\",E2135,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Terphenyl hydrogenated"},"Terphenyl hydrogenated","Terphenyl, hydriert","氢化三联苯"]
[null,{"$f":"IF($B$1=\"English\",C2136,IF($B$1=\"Deutsch\",D2136,IF($B$1=\"中文\",E2136,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethylenediamine (EDA)"},"Ethylenediamine (EDA)","Ethylendiamin (EDA)","乙二胺 (EDA)"]
[null,{"$f":"IF($B$1=\"English\",C2137,IF($B$1=\"Deutsch\",D2137,IF($B$1=\"中文\",E2137,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anything to declare? Please select"},"Anything to declare? Please select","Anything to declare? Please select","任何物质需要申报？"]
[null,{"$f":"IF($B$1=\"English\",C2138,IF($B$1=\"Deutsch\",D2138,IF($B$1=\"中文\",E2138,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7439-92-1 and its compounds"},"7439-92-1 and its compounds","7439-92-1 und seine Verbindungen","7439-92-1 及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C2139,IF($B$1=\"Deutsch\",D2139,IF($B$1=\"中文\",E2139,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7440-43-9 and its compounds"},"7440-43-9 and its compounds","7440-43-9 und seine Verbindungen","7440-43-9 及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C2140,IF($B$1=\"Deutsch\",D2140,IF($B$1=\"中文\",E2140,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7439-97-6 and its compounds"},"7439-97-6 and its compounds","7439-97-6 und seine Verbindungen","7439-97-6 及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C2141,IF($B$1=\"Deutsch\",D2141,IF($B$1=\"中文\",E2141,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1333-82-0 and its compounds"},"1333-82-0 and its compounds","1333-82-0 und seine Verbindungen","1333-82-0 及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C2142,IF($B$1=\"Deutsch\",D2142,IF($B$1=\"中文\",E2142,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-bis(4'-hydroxyphenyl)-4-methylpentane"},"2,2-bis(4'-hydroxyphenyl)-4-methylpentane","2,2-Bis(4'-hydroxyphenyl)-4-methylpentan","2，2-双(4’-羟基苯基)-4-甲基戊烷"]
[null,{"$f":"IF($B$1=\"English\",C2143,IF($B$1=\"Deutsch\",D2143,IF($B$1=\"中文\",E2143,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[k]fluoranthene"},"Benzo[k]fluoranthene","Benzo[k]fluoranthen","苯并[k]氟烷"]
[null,{"$f":"IF($B$1=\"English\",C2144,IF($B$1=\"Deutsch\",D2144,IF($B$1=\"中文\",E2144,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluoranthene"},"Fluoranthene","Fluoranthene","荧光素"]
[null,{"$f":"IF($B$1=\"English\",C2145,IF($B$1=\"Deutsch\",D2145,IF($B$1=\"中文\",E2145,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenanthrene"},"Phenanthrene","Phenanthrene","菲"]
[null,{"$f":"IF($B$1=\"English\",C2146,IF($B$1=\"Deutsch\",D2146,IF($B$1=\"中文\",E2146,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pyrene"},"Pyrene","Pyrene","芘"]
[null,{"$f":"IF($B$1=\"English\",C2147,IF($B$1=\"Deutsch\",D2147,IF($B$1=\"中文\",E2147,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,7,7-trimethyl-3-(phenylmethylene)bicyclo[2.2.1]heptan-2-one "},"1,7,7-trimethyl-3-(phenylmethylene)bicyclo[2.2.1]heptan-2-one ","1,7,7-Trimethyl-3-(phenylmethylen)bicyclo[2.2.1]heptan-2-on ","1，7，7-三甲基-3-(苯基亚甲基)双环[2 . 2 . 1]庚-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2148,IF($B$1=\"Deutsch\",D2148,IF($B$1=\"中文\",E2148,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyethylacetat"},"2-Methoxyethylacetat","2-methoxyethyl acetate","2-甲氧基乙基乙酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2149,IF($B$1=\"Deutsch\",D2149,IF($B$1=\"中文\",E2149,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"},"Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)","Tris(4-Nonylphenyl, verzweigt und linear) phosphit (TNPP) mit >= 0,1% Gew./Gew. 4-Nonylphenol, verzweigt und linear (4-NP)","三(4-壬基苯基，支化和线性)亚磷酸酯(TNPP)，含≥ 0.1% w/w的4-壬基苯酚，支化和线性(4-NP)"]
[null,{"$f":"IF($B$1=\"English\",C2150,IF($B$1=\"Deutsch\",D2150,IF($B$1=\"中文\",E2150,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(nonylphenyl) phosphite"},"Tris(nonylphenyl) phosphite","Tris(nonylphenyl) phosphite","亚磷酸三(壬基苯基)酯"]
[null,{"$f":"IF($B$1=\"English\",C2151,IF($B$1=\"Deutsch\",D2151,IF($B$1=\"中文\",E2151,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"tris(4-nonylphenyl, branched) phosphite"},"tris(4-nonylphenyl, branched) phosphite","tris(4-nonylphenyl, branched) phosphite","三(4-壬基苯基，支链)亚磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2152,IF($B$1=\"Deutsch\",D2152,IF($B$1=\"中文\",E2152,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-nonyl-, phosphite (3:1)"},"Phenol, 4-nonyl-, phosphite (3:1)","Phenol, 4-nonyl-, phosphite (3:1)","4-壬基苯酚，亚磷酸酯(3:1)"]
[null,{"$f":"IF($B$1=\"English\",C2153,IF($B$1=\"Deutsch\",D2153,IF($B$1=\"中文\",E2153,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, p-isononyl-, phosphite (3:1)"},"Phenol, p-isononyl-, phosphite (3:1)","Phenol, p-isononyl-, phosphite (3:1)","苯酚，对异壬基-，亚磷酸酯(3:1)"]
[null,{"$f":"IF($B$1=\"English\",C2154,IF($B$1=\"Deutsch\",D2154,IF($B$1=\"中文\",E2154,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, p-sec-nonyl-, phosphite"},"Phenol, p-sec-nonyl-, phosphite","Phenol, p-sec-nonyl-, phosphite","苯酚，对仲壬基-，亚磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2155,IF($B$1=\"Deutsch\",D2155,IF($B$1=\"中文\",E2155,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides (covering any of their individual isomers and combinations thereof)"},"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides (covering any of their individual isomers and combinations thereof)","2,3,3,3-Tetrafluor-2-(heptafluorpropoxy)propionsäure, ihre Salze und ihre Acylhalide \n[die eines ihrer einzelnen Isomere und Kombinationen davon abdecken]","2，3，3，3-四氟-2-(七氟丙氧基)丙酸、其盐和其酰卤(涵盖其任何单独的异构体及其组合)"]
[null,{"$f":"IF($B$1=\"English\",C2156,IF($B$1=\"Deutsch\",D2156,IF($B$1=\"中文\",E2156,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride"},"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride","2，3，3，3-四氟-2-(七氟丙氧基)丙酰氟"]
[null,{"$f":"IF($B$1=\"English\",C2157,IF($B$1=\"Deutsch\",D2157,IF($B$1=\"中文\",E2157,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid"},"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid","2，3，3，3-四氟-2-(七氟丙氧基)丙酸"]
[null,{"$f":"IF($B$1=\"English\",C2158,IF($B$1=\"Deutsch\",D2158,IF($B$1=\"中文\",E2158,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate"},"Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate","Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate","2，3，3，3-四氟-2-(七氟丙氧基)丙酸钾"]
[null,{"$f":"IF($B$1=\"English\",C2159,IF($B$1=\"Deutsch\",D2159,IF($B$1=\"中文\",E2159,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate"},"Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","2，3，3，3-四氟-2-(七氟丙氧基)丙酸铵"]
[null,{"$f":"IF($B$1=\"English\",C2160,IF($B$1=\"Deutsch\",D2160,IF($B$1=\"中文\",E2160,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-"},"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-","Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-","丙酸，2，3，3，3-四氟-2-(七氟丙氧基)-(+)-"]
[null,{"$f":"IF($B$1=\"English\",C2161,IF($B$1=\"Deutsch\",D2161,IF($B$1=\"中文\",E2161,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-"},"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-","Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-","丙酸，2，3，3，3-四氟-2-(七氟丙氧基)-(-)-"]
[null,{"$f":"IF($B$1=\"English\",C2162,IF($B$1=\"Deutsch\",D2162,IF($B$1=\"中文\",E2162,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-tert-butylphenol"},"4-tert-butylphenol","4-tert-Butylphenol","4-叔丁基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2163,IF($B$1=\"Deutsch\",D2163,IF($B$1=\"中文\",E2163,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisohexyl phthalat"},"Diisohexyl phthalat","Diisohexyl phthalate","邻苯二甲酸二异己酯"]
[null,{"$f":"IF($B$1=\"English\",C2164,IF($B$1=\"Deutsch\",D2164,IF($B$1=\"中文\",E2164,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon"},"2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon","2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone","2-苄基-2-(二甲氨基)-4’-吗啉代联苯"]
[null,{"$f":"IF($B$1=\"English\",C2165,IF($B$1=\"Deutsch\",D2165,IF($B$1=\"中文\",E2165,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorobutane sulfonic acid (PFBS) and its salts "},"Perfluorobutane sulfonic acid (PFBS) and its salts ","Perfluorbutansulfonsäure (PFBS) und seine Salze","全氟丁烷磺酸(PFBS)及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C2166,IF($B$1=\"Deutsch\",D2166,IF($B$1=\"中文\",E2166,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-one"},"2-methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-one","2-Methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-on","2-甲基-1-(4-甲基噻吩基)-2-吗啉代丙-1-酮"]
[null,{"$f":"IF($B$1=\"English\",C2167,IF($B$1=\"Deutsch\",D2167,IF($B$1=\"中文\",E2167,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-(2-methoxyethoxy)ethyl) ether"},"Bis(2-(2-methoxyethoxy)ethyl) ether","Bis(2-(2-methoxyethoxy)ethyl)ether ","双(2-(2-甲氧基乙氧基)乙基)醚"]
[null,{"$f":"IF($B$1=\"English\",C2168,IF($B$1=\"Deutsch\",D2168,IF($B$1=\"中文\",E2168,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"},"Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety","Dioctylzinndilaurat, Stannan-, Dioctylbis(coco-acyloxy)derivate und alle anderen Stannan-, Dioctylbis(fettacyloxy)derivate, wobei C12 die vorherrschende Kohlenstoffzahl der Fettacyloxyeinheit ist","二月桂酸二辛基锡，锡烷，二辛基-，双(可可酰氧基)衍生物。、以及任何其他锡烷、二辛基-、双(脂肪酰氧基)衍生物。其中C12是脂肪酰氧基部分的主要碳数"]
[null,{"$f":"IF($B$1=\"English\",C2169,IF($B$1=\"Deutsch\",D2169,IF($B$1=\"中文\",E2169,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioctyltin dilaurate"},"Dioctyltin dilaurate","Dioctylzinndilaurat","二月桂酸二辛锡"]
[null,{"$f":"IF($B$1=\"English\",C2170,IF($B$1=\"Deutsch\",D2170,IF($B$1=\"中文\",E2170,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"dioctyltin dilaurate; stannane, dioctyl-, bis(coco acyloxy) derivs."},"dioctyltin dilaurate; stannane, dioctyl-, bis(coco acyloxy) derivs.","Stannan, Dioctylbis(coco-acyloxy)derivate und","二月桂酸二辛锡；二辛基锡烷，双(可可酰氧基)衍生物。"]
[null,{"$f":"IF($B$1=\"English\",C2171,IF($B$1=\"Deutsch\",D2171,IF($B$1=\"中文\",E2171,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Stannane, dioctyl-, bis(coco acyloxy) derivs."},"Stannane, dioctyl-, bis(coco acyloxy) derivs.","alle anderen Stannan-, Dioctylbis(fettacyloxy)derivate, wobei C12 die vorherrschende Kohlenstoffzahl der Fettacyloxyeinheit","锡烷，二辛基-，双(可可酰氧基)衍生物。"]
[null,{"$f":"IF($B$1=\"English\",C2172,IF($B$1=\"Deutsch\",D2172,IF($B$1=\"中文\",E2172,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017"},"included in Annex 14\n- \nlast application date: 21. März 2016\n- \nsunset date:  21. September 2017","aufgenommen in Anhang 14\n- Antragsschluss: \n21. März 2016\n\n- Ablauftermin:  \n21. September 2017","包括在附录14\n-申请截止日期: 2016年3月21日\n-过期: 2017年9月21日"]
[null,{"$f":"IF($B$1=\"English\",C2173,IF($B$1=\"Deutsch\",D2173,IF($B$1=\"中文\",E2173,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CN-RoHS (tab 14) Applicable for Products in Compliance Management Catalogue"},"CN-RoHS (tab 14) Applicable for Products in Compliance Management Catalogue","CN-RoHS (tab 14) Applicable for Products in Compliance Management Catalogue","CN-RoHS (tab 14)达标管理目录限用物质应用例外清单"]
[null,{"$f":"IF($B$1=\"English\",C2174,IF($B$1=\"Deutsch\",D2174,IF($B$1=\"中文\",E2174,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated substances"},"Regulated substances","Regulated substances","管制物质"]
[null,{"$f":"IF($B$1=\"English\",C2175,IF($B$1=\"Deutsch\",D2175,IF($B$1=\"中文\",E2175,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS number"},"CAS number","CAS number","CAS号"]
[null,{"$f":"IF($B$1=\"English\",C2176,IF($B$1=\"Deutsch\",D2176,IF($B$1=\"中文\",E2176,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value [mass% in homogeneous material]"},"Limit value [mass% in homogeneous material]","Limit value [mass% in homogeneous material]","限值 [均一材质重量% ]"]
[null,{"$f":"IF($B$1=\"English\",C2177,IF($B$1=\"Deutsch\",D2177,IF($B$1=\"中文\",E2177,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of substance [mass% in homogeneous material]"},"Concentration of substance [mass% in homogeneous material]","Concentration of substance [mass% in homogeneous material]","物质含量 [均一材质重量%]"]
[null,{"$f":"IF($B$1=\"English\",C2178,IF($B$1=\"Deutsch\",D2178,IF($B$1=\"中文\",E2178,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Exception claimed? If so, which one?"},"Exception claimed? If so, which one?","Exception claimed? If so, which one?","豁免吗? 如果是，哪一项"]
[null,{"$f":"IF($B$1=\"English\",C2179,IF($B$1=\"Deutsch\",D2179,IF($B$1=\"中文\",E2179,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Designation of the material that contains the regulated substance"},"Designation of the material that contains the regulated substance","Designation of the material that contains the regulated substance","含有管制物质的材料的名称"]
[null,{"$f":"IF($B$1=\"English\",C2180,IF($B$1=\"Deutsch\",D2180,IF($B$1=\"中文\",E2180,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included ( E )\n- changed ( C )"},"Entry\n- included ( E )\n- changed ( C )","Entry\n- included ( E )\n- changed ( C )","输入\n-包括（E）\n-更改（C） "]
[null,{"$f":"IF($B$1=\"English\",C2181,IF($B$1=\"Deutsch\",D2181,IF($B$1=\"中文\",E2181,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"test report enclosed (optional)"},"test report enclosed (optional)","test report enclosed (optional)","附实验报告(可选)"]
[null,{"$f":"IF($B$1=\"English\",C2182,IF($B$1=\"Deutsch\",D2182,IF($B$1=\"中文\",E2182,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"method of measurement"},"method of measurement","method of measurement","测量方法"]
[null,{"$f":"IF($B$1=\"English\",C2183,IF($B$1=\"Deutsch\",D2183,IF($B$1=\"中文\",E2183,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited substances (P)"},"Prohibited substances (P)","Prohibited substances (P)","禁用物质 (P)"]
[null,{"$f":"IF($B$1=\"English\",C2184,IF($B$1=\"Deutsch\",D2184,IF($B$1=\"中文\",E2184,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Lead","铅"]
[null,{"$f":"IF($B$1=\"English\",C2185,IF($B$1=\"Deutsch\",D2185,IF($B$1=\"中文\",E2185,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C2186,IF($B$1=\"Deutsch\",D2186,IF($B$1=\"中文\",E2186,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury"},"Mercury","Mercury","汞"]
[null,{"$f":"IF($B$1=\"English\",C2187,IF($B$1=\"Deutsch\",D2187,IF($B$1=\"中文\",E2187,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium VI"},"Chromium VI","Chromium VI","六价铬"]
[null,{"$f":"IF($B$1=\"English\",C2188,IF($B$1=\"Deutsch\",D2188,IF($B$1=\"中文\",E2188,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated biphenyles (PBB)"},"Polybrominated biphenyles (PBB)","Polybrominated biphenyles (PBB)","多溴联苯 (PBB)"]
[null,{"$f":"IF($B$1=\"English\",C2189,IF($B$1=\"Deutsch\",D2189,IF($B$1=\"中文\",E2189,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated diphenyl ether (PBDE)"},"Polybrominated diphenyl ether (PBDE)","Polybrominated diphenyl ether (PBDE)","多溴联苯醚 (PBDE)"]
[null,{"$f":"IF($B$1=\"English\",C2190,IF($B$1=\"Deutsch\",D2190,IF($B$1=\"中文\",E2190,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7439-92-1 and its compounds"},"7439-92-1 and its compounds","7439-92-1 and its compounds","7439-92-1和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2191,IF($B$1=\"Deutsch\",D2191,IF($B$1=\"中文\",E2191,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7440-43-9 and its compounds"},"7440-43-9 and its compounds","7440-43-9 and its compounds","7440-43-9和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2192,IF($B$1=\"Deutsch\",D2192,IF($B$1=\"中文\",E2192,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7439-97-6 and its compounds"},"7439-97-6 and its compounds","7439-97-6 and its compounds","7439-97-6和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2193,IF($B$1=\"Deutsch\",D2193,IF($B$1=\"中文\",E2193,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1333-82-0 and its compounds"},"1333-82-0 and its compounds","1333-82-0 and its compounds","1333-82-0和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2194,IF($B$1=\"Deutsch\",D2194,IF($B$1=\"中文\",E2194,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material group"},"Material group","Material group","材料组 "]
[null,{"$f":"IF($B$1=\"English\",C2195,IF($B$1=\"Deutsch\",D2195,IF($B$1=\"中文\",E2195,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"List of Exemptions (12. March 2018) "},"List of Exemptions (12. March 2018) ","List of Exemptions (12. March 2018) ","豁免清单(2018.03.12) "]
[null,{"$f":"IF($B$1=\"English\",C2196,IF($B$1=\"Deutsch\",D2196,IF($B$1=\"中文\",E2196,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Annex 1 Compliance Management Catalogue of Electric Appliances and Electronic Products for Restriction Use Hazardous Substances   (The first batch) "},"Annex 1 Compliance Management Catalogue of Electric Appliances and Electronic Products for Restriction Use Hazardous Substances   (The first batch) ","Annex 1 Compliance Management Catalogue of Electric Appliances and Electronic Products for Restriction Use Hazardous Substances   (The first batch) ","附件 1 电器电子产品有害物质限制使用达标管理目录 （第一批）"]
[null,{"$f":"IF($B$1=\"English\",C2197,IF($B$1=\"Deutsch\",D2197,IF($B$1=\"中文\",E2197,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Annex II \nApplications Exempted From the Restriction in Product \nCompliance Management Catalogue (effective from 12. March 2019)"},"Annex II \nApplications Exempted From the Restriction in Product \nCompliance Management Catalogue (effective from 12. March 2019)","Annex II \nApplications Exempted From the Restriction in Product \nCompliance Management Catalogue (effective from 12. March 2019)","附件 2\n达标管理目录限用物质应用例外清单"]
[null,{"$f":"IF($B$1=\"English\",C2198,IF($B$1=\"Deutsch\",D2198,IF($B$1=\"中文\",E2198,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No."},"No.","No.","序号"]
[null,{"$f":"IF($B$1=\"English\",C2199,IF($B$1=\"Deutsch\",D2199,IF($B$1=\"中文\",E2199,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product name"},"Product name","Product name","产品名称"]
[null,{"$f":"IF($B$1=\"English\",C2200,IF($B$1=\"Deutsch\",D2200,IF($B$1=\"中文\",E2200,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Product range and definition"},"Product range and definition","Product range and definition","产品范围及定义"]
[null,{"$f":"IF($B$1=\"English\",C2201,IF($B$1=\"Deutsch\",D2201,IF($B$1=\"中文\",E2201,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Scope of application "},"Scope of application ","Scope of application ","适用范围说明"]
[null,{"$f":"IF($B$1=\"English\",C2202,IF($B$1=\"Deutsch\",D2202,IF($B$1=\"中文\",E2202,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"#"},"#","#","#"]
[null,{"$f":"IF($B$1=\"English\",C2203,IF($B$1=\"Deutsch\",D2203,IF($B$1=\"中文\",E2203,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Exemption"},"Exemption","Exemption","应用"]
[null,{"$f":"IF($B$1=\"English\",C2204,IF($B$1=\"Deutsch\",D2204,IF($B$1=\"中文\",E2204,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Restriction Limitation"},"Restriction Limitation","Restriction Limitation","限值要求"]
[null,{"$f":"IF($B$1=\"English\",C2205,IF($B$1=\"Deutsch\",D2205,IF($B$1=\"中文\",E2205,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Refrigerator "},"Refrigerator ","Refrigerator ","电冰箱"]
[null,{"$f":"IF($B$1=\"English\",C2206,IF($B$1=\"Deutsch\",D2206,IF($B$1=\"中文\",E2206,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A thermally insulated box consisting of one or multiple compartments that can be controlled at prescribed temperature, with appropriate volume and structure, is able to get the cooling capacity using natural or forced convection, and consumes one or many types of energy (volume ≤ 800 liters). "},"A thermally insulated box consisting of one or multiple compartments that can be controlled at prescribed temperature, with appropriate volume and structure, is able to get the cooling capacity using natural or forced convection, and consumes one or many types of energy (volume ≤ 800 liters). ","A thermally insulated box consisting of one or multiple compartments that can be controlled at prescribed temperature, with appropriate volume and structure, is able to get the cooling capacity using natural or forced convection, and consumes one or many types of energy (volume ≤ 800 liters). ","由一个或多个间室组 成且能够控制在规定的温 度下，具有适合的容积和 结构、使用自然对流或强 制对流、消耗一种或多种 能量以获取冷量的隔热箱 体（容积≤800 升）"]
[null,{"$f":"IF($B$1=\"English\",C2207,IF($B$1=\"Deutsch\",D2207,IF($B$1=\"中文\",E2207,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"From the point of installation, refrigerators can be divided into upright, portable, wallmounted, embedded, or other types. From the point of usage, refrigerators can be divided into refrigerator-freezer (cabinet), freezer (cabinet), refrigerator (cabinet), freezer, horizontal freezer, display cabinet, wine cabinet, etc. Methods for determination of linear dimensions of refrigerator and measurement of the volume can be found in GB / T 8059-2016 \"Household and similar refrigerating appliances\". "},"From the point of installation, refrigerators can be divided into upright, portable, wallmounted, embedded, or other types. From the point of usage, refrigerators can be divided into refrigerator-freezer (cabinet), freezer (cabinet), refrigerator (cabinet), freezer, horizontal freezer, display cabinet, wine cabinet, etc. Methods for determination of linear dimensions of refrigerator and measurement of the volume can be found in GB / T 8059-2016 \"Household and similar refrigerating appliances\". ","From the point of installation, refrigerators can be divided into upright, portable, wallmounted, embedded, or other types. From the point of usage, refrigerators can be divided into refrigerator-freezer (cabinet), freezer (cabinet), refrigerator (cabinet), freezer, horizontal freezer, display cabinet, wine cabinet, etc. Methods for determination of linear dimensions of refrigerator and measurement of the volume can be found in GB / T 8059-2016 \"Household and similar refrigerating appliances\". ","电冰箱从安装方式来看，包括驻 立式、便携式、挂壁式或嵌入式等多 种类型。按用途分包括冷藏冷冻箱 （柜） 、冷冻箱（柜）、冷藏箱（柜） 、 冰柜、卧式冷柜、展示柜、葡萄酒柜 等。其中，电冰箱线性尺寸的确定及 容 积 的 测 量 方 法 可 参 见 GB/T 8059-2016《家用和类似用途制冷器 具》。"]
[null,{"$f":"IF($B$1=\"English\",C2208,IF($B$1=\"Deutsch\",D2208,IF($B$1=\"中文\",E2208,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Air conditioner "},"Air conditioner ","Air conditioner ","空气 调节器"]
[null,{"$f":"IF($B$1=\"English\",C2209,IF($B$1=\"Deutsch\",D2209,IF($B$1=\"中文\",E2209,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"An equipment for directly providing processed air to confined space, room or area, including room air conditioner and unitary air conditioner (rated cooling capacity ≤14,000 watts). "},"An equipment for directly providing processed air to confined space, room or area, including room air conditioner and unitary air conditioner (rated cooling capacity ≤14,000 watts). ","An equipment for directly providing processed air to confined space, room or area, including room air conditioner and unitary air conditioner (rated cooling capacity ≤14,000 watts). ","一种向密闭空间、房 间或区域直接提供经过处 理的空气的设备。包括房 间空气调节器和单元式空 气调节机（额定制冷量≤ 14000 瓦） "]
[null,{"$f":"IF($B$1=\"English\",C2210,IF($B$1=\"Deutsch\",D2210,IF($B$1=\"中文\",E2210,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"An air conditioner mainly consists of refrigeration system, air circulation and purification devices for cooling and dehumidification, and/or heating and ventilating devices (they can be assembled in a box structure, or designed as a component system to be used together). Air conditioners include room air conditioners and unitary air conditioners (rated cooling capacity ≤ 14000 watts), where: 1) Room air conditioner mainly includes cooling system and air circulation and purifying devices for cooling and dehumidification, it can also include heating and ventilation devices (they can be assembled in a box structure or designed as a component system to be used together). From the point of structure, room air conditioners can be generally divided into all-inone, split-type, and multiconnected air conditioners, etc.; from the point of function, they can be divided into the types of cold air, heat pump, cold air dehumidification, cold air heat pump dehumidification, auxiliary heat pump electric heating, etc.; and from the point of cooling method, they can be divided into water cooling and air cooling types. 2) Unitary air conditioner mainly includes cooling system and air circulation and purification devices, it can also include heating, humidification and ventilation devices. From the point of function, unitary air conditioners can be divided into cooling only, heat pump, and constant temperature and humidity types; from the point of condenser cooling method, they can be divided into watercooled, and air-cooled types; from the point of heating method, it can be divided into electric heating, and heat pump heating types; from the point of structure, it can be divided into all-in-one, and split-type; from the point of air supplying, it can be divided into direct blow, and air duct types; from the point of air conditioning capacity regulating characteristics, they can be divided into constant capacity and variable capacity types."},"An air conditioner mainly consists of refrigeration system, air circulation and purification devices for cooling and dehumidification, and/or heating and ventilating devices (they can be assembled in a box structure, or designed as a component system to be used together). Air conditioners include room air conditioners and unitary air conditioners (rated cooling capacity ≤ 14000 watts), where: 1) Room air conditioner mainly includes cooling system and air circulation and purifying devices for cooling and dehumidification, it can also include heating and ventilation devices (they can be assembled in a box structure or designed as a component system to be used together). From the point of structure, room air conditioners can be generally divided into all-inone, split-type, and multiconnected air conditioners, etc.; from the point of function, they can be divided into the types of cold air, heat pump, cold air dehumidification, cold air heat pump dehumidification, auxiliary heat pump electric heating, etc.; and from the point of cooling method, they can be divided into water cooling and air cooling types. 2) Unitary air conditioner mainly includes cooling system and air circulation and purification devices, it can also include heating, humidification and ventilation devices. From the point of function, unitary air conditioners can be divided into cooling only, heat pump, and constant temperature and humidity types; from the point of condenser cooling method, they can be divided into watercooled, and air-cooled types; from the point of heating method, it can be divided into electric heating, and heat pump heating types; from the point of structure, it can be divided into all-in-one, and split-type; from the point of air supplying, it can be divided into direct blow, and air duct types; from the point of air conditioning capacity regulating characteristics, they can be divided into constant capacity and variable capacity types.","An air conditioner mainly consists of refrigeration system, air circulation and purification devices for cooling and dehumidification, and/or heating and ventilating devices (they can be assembled in a box structure, or designed as a component system to be used together). Air conditioners include room air conditioners and unitary air conditioners (rated cooling capacity ≤ 14000 watts), where: 1) Room air conditioner mainly includes cooling system and air circulation and purifying devices for cooling and dehumidification, it can also include heating and ventilation devices (they can be assembled in a box structure or designed as a component system to be used together). From the point of structure, room air conditioners can be generally divided into all-inone, split-type, and multiconnected air conditioners, etc.; from the point of function, they can be divided into the types of cold air, heat pump, cold air dehumidification, cold air heat pump dehumidification, auxiliary heat pump electric heating, etc.; and from the point of cooling method, they can be divided into water cooling and air cooling types. 2) Unitary air conditioner mainly includes cooling system and air circulation and purification devices, it can also include heating, humidification and ventilation devices. From the point of function, unitary air conditioners can be divided into cooling only, heat pump, and constant temperature and humidity types; from the point of condenser cooling method, they can be divided into watercooled, and air-cooled types; from the point of heating method, it can be divided into electric heating, and heat pump heating types; from the point of structure, it can be divided into all-in-one, and split-type; from the point of air supplying, it can be divided into direct blow, and air duct types; from the point of air conditioning capacity regulating characteristics, they can be divided into constant capacity and variable capacity types.","空气调节器主要包括制冷和除 湿用的制冷系统、空气循环和净化装 置和/或加热和通风装置组成（它们 可被组装在一个箱壳内或被设计成 一起使用的组件系统） 。 空气调节器包括房间空气调节 器和单元式空气调节机（额定制冷量 ≤14000 瓦） ，其中： 1）房间空气调节器主要包括制 冷和除湿用的制冷系统以及空气循 环和净化装置，还可包括加热和通风 装置(它们可被组装在一个箱壳内或 被设计成一起使用的组件系统)。 房间空气空调器一般可按结构 形式分为整体式、分体式和一拖多空 调器等；按功能分为冷风型、热泵型、冷风除湿型、冷风热泵除湿型、热泵 辅助电热型等；按冷却方式分为水冷 式和空气冷却式。 2）单元式空气调节机主要包括 制冷系统以及空气循环和净化装置， 还可以包括加热、加湿和通风装置。 单元式空气调节机按功能分为 单冷型、热泵型、恒温恒湿型；按冷 凝器的冷却方式分为水冷式、风冷 式；按加热方式分为电加热、热泵制 热；按结构型式分为整体型、分体型； 按送风型式分为直接吹出型、接风管 型；按空调机能力调节特性分为定容 型、非定容型。"]
[null,{"$f":"IF($B$1=\"English\",C2211,IF($B$1=\"Deutsch\",D2211,IF($B$1=\"中文\",E2211,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Washing machine "},"Washing machine ","Washing machine ","洗衣机"]
[null,{"$f":"IF($B$1=\"English\",C2212,IF($B$1=\"Deutsch\",D2212,IF($B$1=\"中文\",E2212,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"An appliance driven by electric power, and washes clothes (including drying function,) through mechanical actions (dry clothes capacity ≤ 10 kg).  "},"An appliance driven by electric power, and washes clothes (including drying function,) through mechanical actions (dry clothes capacity ≤ 10 kg).  ","An appliance driven by electric power, and washes clothes (including drying function,) through mechanical actions (dry clothes capacity ≤ 10 kg).  ","利用电能驱动，依靠 机械作用洗涤衣物（含兼 有干衣功能）的器具（干 衣量≤10 公斤）。"]
[null,{"$f":"IF($B$1=\"English\",C2213,IF($B$1=\"Deutsch\",D2213,IF($B$1=\"中文\",E2213,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The product range for washing machine with dry clothes capacity  ≤ 10 kg,  includes impeller type washing machine, drum type washing machine, agitator type washing machine, dehydration machine, etc.  "},"The product range for washing machine with dry clothes capacity  ≤ 10 kg,  includes impeller type washing machine, drum type washing machine, agitator type washing machine, dehydration machine, etc.  ","The product range for washing machine with dry clothes capacity  ≤ 10 kg,  includes impeller type washing machine, drum type washing machine, agitator type washing machine, dehydration machine, etc.  ","洗衣机的产品范围包括干衣量 ≤10 公斤的波轮式洗衣机、滚筒式 洗衣机、搅拌式洗衣机、脱水机等。"]
[null,{"$f":"IF($B$1=\"English\",C2214,IF($B$1=\"Deutsch\",D2214,IF($B$1=\"中文\",E2214,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Water heater"},"Water heater","Water heater","电热水器"]
[null,{"$f":"IF($B$1=\"English\",C2215,IF($B$1=\"Deutsch\",D2215,IF($B$1=\"中文\",E2215,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A device that turns electrical energy into thermal energy through electric heating elements such as electric heating pipe, electric heating membrane, and so on, to heat water to temperature below boiling point (with capacity≤ 500 ltr.), including water storage type electric water heater, instantaneous electric water heater, etc."},"A device that turns electrical energy into thermal energy through electric heating elements such as electric heating pipe, electric heating membrane, and so on, to heat water to temperature below boiling point (with capacity≤ 500 ltr.), including water storage type electric water heater, instantaneous electric water heater, etc.","A device that turns electrical energy into thermal energy through electric heating elements such as electric heating pipe, electric heating membrane, and so on, to heat water to temperature below boiling point (with capacity≤ 500 ltr.), including water storage type electric water heater, instantaneous electric water heater, etc.","通过电加热管、电热 膜等电加热元件将电能转 化为热能，并将热能传递 给水，使水加热至低于沸 点温度的器具（容量≤500 升）。包括储水式电热水 器、快热式电热水器等。"]
[null,{"$f":"IF($B$1=\"English\",C2216,IF($B$1=\"Deutsch\",D2216,IF($B$1=\"中文\",E2216,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electric water heaters include water storage type electric water heater, instantaneous electric water heater etc. (with capacity ≤ 500 ltr.), but does not include appliances and commercial vending machines with liquid heating capabilities such as coffee pots, egg boilers, stew pot, steamer, yogurt maker, hot water vending machine, etc. Where: 1) Storage type water heater refers to a fixed appliance that heats water and stores water in the container, and is equipped with water temperature control device.  2) Instantaneous water heater refers to an upright device that heats water when water flows "},"Electric water heaters include water storage type electric water heater, instantaneous electric water heater etc. (with capacity ≤ 500 ltr.), but does not include appliances and commercial vending machines with liquid heating capabilities such as coffee pots, egg boilers, stew pot, steamer, yogurt maker, hot water vending machine, etc. Where: 1) Storage type water heater refers to a fixed appliance that heats water and stores water in the container, and is equipped with water temperature control device.  2) Instantaneous water heater refers to an upright device that heats water when water flows ","Electric water heaters include water storage type electric water heater, instantaneous electric water heater etc. (with capacity ≤ 500 ltr.), but does not include appliances and commercial vending machines with liquid heating capabilities such as coffee pots, egg boilers, stew pot, steamer, yogurt maker, hot water vending machine, etc. Where: 1) Storage type water heater refers to a fixed appliance that heats water and stores water in the container, and is equipped with water temperature control device.  2) Instantaneous water heater refers to an upright device that heats water when water flows ","电热水器包括容量≤500 升的 储水式电热水器、快热式电热水器 等，但不包含咖啡壶、电水壶、煮蛋 器、炖锅、蒸锅、酸奶器、热水售卖 机等具备液体加热功能的液体加热 器具和商业售卖机。其中：1）储水 式热水器是指加热水并将水储存在 容器中，装有控制水温装置的固定式 器具。2）快热式热水器是指当水流 过器具时加热水的驻立式器具。"]
[null,{"$f":"IF($B$1=\"English\",C2217,IF($B$1=\"Deutsch\",D2217,IF($B$1=\"中文\",E2217,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Printer"},"Printer","Printer","打印机"]
[null,{"$f":"IF($B$1=\"English\",C2218,IF($B$1=\"Deutsch\",D2218,IF($B$1=\"中文\",E2218,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"An device that receives data from sources such as automatic data processing equipment, network, platform scanners, etc., and prints text, symbol, or image on the printing media through methods such as electrostatic, inkjet, dot matrix, or thermosimaging, etc. It also includes device whose main function is printing, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min)."},"An device that receives data from sources such as automatic data processing equipment, network, platform scanners, etc., and prints text, symbol, or image on the printing media through methods such as electrostatic, inkjet, dot matrix, or thermosimaging, etc. It also includes device whose main function is printing, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min).","An device that receives data from sources such as automatic data processing equipment, network, platform scanners, etc., and prints text, symbol, or image on the printing media through methods such as electrostatic, inkjet, dot matrix, or thermosimaging, etc. It also includes device whose main function is printing, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min).","从自动数据处理设 备、网络、平台式扫描仪 等来源接收数据，通过诸 如静电、喷墨、针打或热 成像等方法，在印刷（打 印）介质上打印正文、字 符或图像的设备。还包括 以打印功能为主，兼有其 他功能的设备。 （印刷幅面 ≤A3，且印刷速度≤60 张/ 分钟）。"]
[null,{"$f":"IF($B$1=\"English\",C2219,IF($B$1=\"Deutsch\",D2219,IF($B$1=\"中文\",E2219,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Printers include laser printer, inkjet printer, dot matrix printer, thermal printer and other equipment that work inline with computers or use cloud printing platform, to convert digital information into text and image and output the result in the form of hardcopy. It also includes devices whose main function is printing, but also has other functions. The printing format and speed shall be in according with the relevant existing standards and regulations. Printers do not include: 1) dot matrix printer with printing head pins ≥ 48; 2) designed only for printing media other than paper, such as cloth, plastic, metal, etc. 3) Needle printers, thermal printers and inkjet printers with a printing width of <110 mm "},"Printers include laser printer, inkjet printer, dot matrix printer, thermal printer and other equipment that work inline with computers or use cloud printing platform, to convert digital information into text and image and output the result in the form of hardcopy. It also includes devices whose main function is printing, but also has other functions. The printing format and speed shall be in according with the relevant existing standards and regulations. Printers do not include: 1) dot matrix printer with printing head pins ≥ 48; 2) designed only for printing media other than paper, such as cloth, plastic, metal, etc. 3) Needle printers, thermal printers and inkjet printers with a printing width of <110 mm ","Printers include laser printer, inkjet printer, dot matrix printer, thermal printer and other equipment that work inline with computers or use cloud printing platform, to convert digital information into text and image and output the result in the form of hardcopy. It also includes devices whose main function is printing, but also has other functions. The printing format and speed shall be in according with the relevant existing standards and regulations. Printers do not include: 1) dot matrix printer with printing head pins ≥ 48; 2) designed only for printing media other than paper, such as cloth, plastic, metal, etc. 3) Needle printers, thermal printers and inkjet printers with a printing width of <110 mm ","打印机包括激光打印机、喷墨打 印机、针式打印机、热打印机和其他 与计算机联机工作或利用云打印平 台，将数字信息转换成文字和图像并 以硬拷贝形式输出的设备，也包括以 打印功能为主，兼有其他功能设备。 其中印刷幅面和印刷速度按现 行有关标准和规定执行。 打印机不包括：1）打印头针数 ≥48 的针式打印机；2）设计上仅用 于打印介质是布、塑料、金属等纸以 外的设备；3）印刷幅宽<110 毫米的 针式打印机、热打印机和喷墨打印 机。"]
[null,{"$f":"IF($B$1=\"English\",C2220,IF($B$1=\"Deutsch\",D2220,IF($B$1=\"中文\",E2220,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Copier "},"Copier ","Copier ","复印机"]
[null,{"$f":"IF($B$1=\"English\",C2221,IF($B$1=\"Deutsch\",D2221,IF($B$1=\"中文\",E2221,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A device to obtain copies of the original writing, drawing, or printing material in the same size, magnified, or reduced in size. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, printing speed ≤ 60 sheets/min). "},"A device to obtain copies of the original writing, drawing, or printing material in the same size, magnified, or reduced in size. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, printing speed ≤ 60 sheets/min). ","A device to obtain copies of the original writing, drawing, or printing material in the same size, magnified, or reduced in size. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, printing speed ≤ 60 sheets/min). ","从书写、绘制或印刷 的原稿得到等倍、放大或 缩小的复印品的设备。还 包括以复印功能为主，兼 有其他功能的设备。 （印刷 幅面≤A3，且印刷速度≤ 60 张/分钟）。"]
[null,{"$f":"IF($B$1=\"English\",C2222,IF($B$1=\"Deutsch\",D2222,IF($B$1=\"中文\",E2222,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Copiers include electrostatic copier, ink jet copier, and devices that produce copies of the originals with a variety of different imaging processes. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min). Printing format and speed shall be in accordance with relevant "},"Copiers include electrostatic copier, ink jet copier, and devices that produce copies of the originals with a variety of different imaging processes. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min). Printing format and speed shall be in accordance with relevant ","Copiers include electrostatic copier, ink jet copier, and devices that produce copies of the originals with a variety of different imaging processes. It also includes device whose main function is copying, but also has other functions (printing format ≤ A3, and printing speed ≤ 60 sheets/min). Printing format and speed shall be in accordance with relevant ","复印机包括静电复印机、喷墨复 印机和其他用各种不同成像过程产 生原稿复印品的设备，还包括以复印 功能为主，兼有其他功能的设备（印 刷幅面≤A3，且印刷速度≤60 张/分 钟）。 其中印刷幅面和印刷速度按现 行有关标准和规定执行。"]
[null,{"$f":"IF($B$1=\"English\",C2223,IF($B$1=\"Deutsch\",D2223,IF($B$1=\"中文\",E2223,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fax machine "},"Fax machine ","Fax machine "," 传真机"]
[null,{"$f":"IF($B$1=\"English\",C2224,IF($B$1=\"Deutsch\",D2224,IF($B$1=\"中文\",E2224,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A telecommunication terminal device that converts static images of text, chart, and pictures to electrical signals, sends them out using scanning and photoelectric conversion technology, and receives copies in the form of recording, including equipment whose main function is fax, but also has other functions. "},"A telecommunication terminal device that converts static images of text, chart, and pictures to electrical signals, sends them out using scanning and photoelectric conversion technology, and receives copies in the form of recording, including equipment whose main function is fax, but also has other functions. ","A telecommunication terminal device that converts static images of text, chart, and pictures to electrical signals, sends them out using scanning and photoelectric conversion technology, and receives copies in the form of recording, including equipment whose main function is fax, but also has other functions. ","利用扫描和光电变换 技术，把文字、图表、相 片等静止图像变换成电信 号发送出去，接收时以记 录形式获取复制稿的通信 终端设备，包括以传真功 能为主，兼有其他功能的 设备。"]
[null,{"$f":"IF($B$1=\"English\",C2225,IF($B$1=\"Deutsch\",D2225,IF($B$1=\"中文\",E2225,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A fax machine has two functions: to send the original; and to receive and copy the original at the same time. It includes laser, inkjet, thermal imaging, as well as multifunction fax machine which integrates two or more of the faxing, printing, scanning, or copying functions. "},"A fax machine has two functions: to send the original; and to receive and copy the original at the same time. It includes laser, inkjet, thermal imaging, as well as multifunction fax machine which integrates two or more of the faxing, printing, scanning, or copying functions. ","A fax machine has two functions: to send the original; and to receive and copy the original at the same time. It includes laser, inkjet, thermal imaging, as well as multifunction fax machine which integrates two or more of the faxing, printing, scanning, or copying functions. ","传真机同时具有发送原稿和接 收并复制原稿两种功能。包括激光传 真机、喷墨传真机、热成像传真机， 以及具有传真、打印、扫描或复印等 多功能中两个或两个以上功能的多 功能一体机等。"]
[null,{"$f":"IF($B$1=\"English\",C2226,IF($B$1=\"Deutsch\",D2226,IF($B$1=\"中文\",E2226,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TV set "},"TV set ","TV set ","电视机"]
[null,{"$f":"IF($B$1=\"English\",C2227,IF($B$1=\"Deutsch\",D2227,IF($B$1=\"中文\",E2227,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A receiving device to be used to display TV signals; an electronic product powered by electricity, designed to receive, display, and play analog and/or digital color TV broadcasting signals transmitted through ground, cable, satellite, or network.  TV sets also includes display equipment whose main function is for displaying television signals although it is not equipped with TV tuner (LNB).  "},"A receiving device to be used to display TV signals; an electronic product powered by electricity, designed to receive, display, and play analog and/or digital color TV broadcasting signals transmitted through ground, cable, satellite, or network.  TV sets also includes display equipment whose main function is for displaying television signals although it is not equipped with TV tuner (LNB).  ","A receiving device to be used to display TV signals; an electronic product powered by electricity, designed to receive, display, and play analog and/or digital color TV broadcasting signals transmitted through ground, cable, satellite, or network.  TV sets also includes display equipment whose main function is for displaying television signals although it is not equipped with TV tuner (LNB).  ","用于信号显示的电视 接收装置，被设计用来接 收、显示、播放由地面、 有线、卫星或网络传输的 模拟和/或数字彩色电视 广播信号的，由电源供电 的电子产品。"]
[null,{"$f":"IF($B$1=\"English\",C2228,IF($B$1=\"Deutsch\",D2228,IF($B$1=\"中文\",E2228,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Including cathode-ray tube (black-and-white, color) televisions, LCD TVs, OLED TVs, rear-projection TVs, mobile TV receiving terminals and other TV tuner (tunnels) for receiving signals and restoring images and audio terminal device. Also it includes a device with main function of the display apparatus TV, even though without a television tuner (high frequency head). "},"Including cathode-ray tube (black-and-white, color) televisions, LCD TVs, OLED TVs, rear-projection TVs, mobile TV receiving terminals and other TV tuner (tunnels) for receiving signals and restoring images and audio terminal device. Also it includes a device with main function of the display apparatus TV, even though without a television tuner (high frequency head). ","Including cathode-ray tube (black-and-white, color) televisions, LCD TVs, OLED TVs, rear-projection TVs, mobile TV receiving terminals and other TV tuner (tunnels) for receiving signals and restoring images and audio terminal device. Also it includes a device with main function of the display apparatus TV, even though without a television tuner (high frequency head). ","包括阴极射线管（黑白、彩色） 电视机、液晶电视机、OLED 电视机、 背投电视机、移动电视接收终端及其 他含有电视调谐器（高频头）的用于 接收信号并还原出图像及伴音的终 端设备。也包括虽不具备电视调谐器 （高频头），但其主要功能为电视的 显示设备。"]
[null,{"$f":"IF($B$1=\"English\",C2229,IF($B$1=\"Deutsch\",D2229,IF($B$1=\"中文\",E2229,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monitor "},"Monitor ","Monitor ","监视器"]
[null,{"$f":"IF($B$1=\"English\",C2230,IF($B$1=\"Deutsch\",D2230,IF($B$1=\"中文\",E2230,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"An image output device which converts video signals to optic image signal, and to display the image of the processed data by way of illustration, including cathode ray tubes (black and white, color) monitor, LCD monitor, etc. that is mainly composed of display components (no tuner). "},"An image output device which converts video signals to optic image signal, and to display the image of the processed data by way of illustration, including cathode ray tubes (black and white, color) monitor, LCD monitor, etc. that is mainly composed of display components (no tuner). ","An image output device which converts video signals to optic image signal, and to display the image of the processed data by way of illustration, including cathode ray tubes (black and white, color) monitor, LCD monitor, etc. that is mainly composed of display components (no tuner). ","将视频信号转换为光 图像信号，用图示的方法 显示已处理数据的图像输 出设备。包括阴极射线管 （黑白、彩色）监视器、 液晶监视器等由显示器件 为核心组成的图像输出设 备（不含高频头） 。"]
[null,{"$f":"IF($B$1=\"English\",C2231,IF($B$1=\"Deutsch\",D2231,IF($B$1=\"中文\",E2231,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"From the point of material, monitor can be divided into CRT, DLP, LCD, LED, OLED, etc.; from the point of usage, they can be divided into security monitor, supervision monitor, radio and broadcasting monitor, computer monitor, and so on.  "},"From the point of material, monitor can be divided into CRT, DLP, LCD, LED, OLED, etc.; from the point of usage, they can be divided into security monitor, supervision monitor, radio and broadcasting monitor, computer monitor, and so on.  ","From the point of material, monitor can be divided into CRT, DLP, LCD, LED, OLED, etc.; from the point of usage, they can be divided into security monitor, supervision monitor, radio and broadcasting monitor, computer monitor, and so on.  ","监视器按材质可分为 CRT、DLP、 LCD、LED、OLED 等，按照用途可分 为安防监视器、监控监视器、广电监 视器、电脑监视器等。"]
[null,{"$f":"IF($B$1=\"English\",C2232,IF($B$1=\"Deutsch\",D2232,IF($B$1=\"中文\",E2232,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Microcomputer "},"Microcomputer ","Microcomputer ","微型 计算机"]
[null,{"$f":"IF($B$1=\"English\",C2233,IF($B$1=\"Deutsch\",D2233,IF($B$1=\"中文\",E2233,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"An entity based on the hardware system of a microcomputer, configured with necessary external device and software, and is suitable for a single user, including desktop PC (including all-inone PC), portable PC, tablet, and pocket PC.  "},"An entity based on the hardware system of a microcomputer, configured with necessary external device and software, and is suitable for a single user, including desktop PC (including all-inone PC), portable PC, tablet, and pocket PC.  ","An entity based on the hardware system of a microcomputer, configured with necessary external device and software, and is suitable for a single user, including desktop PC (including all-inone PC), portable PC, tablet, and pocket PC.  ","适合单个用户的，在 微型计算机硬件系统的基 础上配置必要的外部设备 和软件构成的实体。包括 台式微型计算机（含一体 机） 、便携式微型计算机、 平板电脑和掌上电脑等。"]
[null,{"$f":"IF($B$1=\"English\",C2234,IF($B$1=\"Deutsch\",D2234,IF($B$1=\"中文\",E2234,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Microcomputers include desktop PC (including all-in one PC), portable PC, tablet, and pocket PC. Where: 1) Desktop PC refers to PCs that are specifically designed for use on fixed desks in the office or home. It does not include computer servers, workstations that are special suitable for computer work room, and industrial PCs that are special suitable for industrial control and other PCs that have significantly different characters with desktop PCs.  2) Portable PC refers to PC that is characterized by portability, and is equipped with built-in input and output devices (such as monitors, keyboard etc.), as well as battery module; 3) Tablet: PC that takes a plate structure, and uses touch screen as the main component of input and output, and can be used hand-held. 4) Pocket PC (PDA): a handheld computing device that is running on the embedded operating system and application, and is small, lightweight, easy to carry, practical, and inexpensive. "},"Microcomputers include desktop PC (including all-in one PC), portable PC, tablet, and pocket PC. Where: 1) Desktop PC refers to PCs that are specifically designed for use on fixed desks in the office or home. It does not include computer servers, workstations that are special suitable for computer work room, and industrial PCs that are special suitable for industrial control and other PCs that have significantly different characters with desktop PCs.  2) Portable PC refers to PC that is characterized by portability, and is equipped with built-in input and output devices (such as monitors, keyboard etc.), as well as battery module; 3) Tablet: PC that takes a plate structure, and uses touch screen as the main component of input and output, and can be used hand-held. 4) Pocket PC (PDA): a handheld computing device that is running on the embedded operating system and application, and is small, lightweight, easy to carry, practical, and inexpensive. ","Microcomputers include desktop PC (including all-in one PC), portable PC, tablet, and pocket PC. Where: 1) Desktop PC refers to PCs that are specifically designed for use on fixed desks in the office or home. It does not include computer servers, workstations that are special suitable for computer work room, and industrial PCs that are special suitable for industrial control and other PCs that have significantly different characters with desktop PCs.  2) Portable PC refers to PC that is characterized by portability, and is equipped with built-in input and output devices (such as monitors, keyboard etc.), as well as battery module; 3) Tablet: PC that takes a plate structure, and uses touch screen as the main component of input and output, and can be used hand-held. 4) Pocket PC (PDA): a handheld computing device that is running on the embedded operating system and application, and is small, lightweight, easy to carry, practical, and inexpensive. ","微型计算机包括台式微型计算 机（含一体机） 、便携式微型计算机、 平板电脑和掌上电脑等。其中： 1）台式微型计算机是指专门为 适合办公或家庭固定台面使用的微 型计算机。不包括专门为适合机房使 用的计算机服务器、工作站，以及专 门为适合工业控制使用的工业应用 计算机等与台式微型计算机有显著 区别特征的其他微型计算机； 2）便携式微型计算机是指以便 携性为特点，内置了输入输出设备 （如显示器、键盘等）,配备电池模 块的微型计算机； 3）平板电脑：采用板式结构、 以触摸屏幕作为主要输入输出部件 可手持使用的微型计算机； 4）掌上电脑（PDA）：是一种运 行在嵌入式操作系统和内嵌式应用 软件之上的、小巧、轻便、易带、实 用、价廉的手持式计算设备。"]
[null,{"$f":"IF($B$1=\"English\",C2235,IF($B$1=\"Deutsch\",D2235,IF($B$1=\"中文\",E2235,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mobile communication handset "},"Mobile communication handset ","Mobile communication handset ","移动通信 手持机"]
[null,{"$f":"IF($B$1=\"English\",C2236,IF($B$1=\"Deutsch\",D2236,IF($B$1=\"中文\",E2236,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A handheld mobile user terminal device supports at least one digital mobile communications technology (e.g., a cellular mobile communication technology GSM / GPRS, CDMA, TDSCDMA, WCDMA, CDMA2000, LTE and its follow-up  evolution and integration technology.) to send or receive phone calls or other sound, image, and data between two sites through electromagnetic wave of the cellular network. "},"A handheld mobile user terminal device supports at least one digital mobile communications technology (e.g., a cellular mobile communication technology GSM / GPRS, CDMA, TDSCDMA, WCDMA, CDMA2000, LTE and its follow-up  evolution and integration technology.) to send or receive phone calls or other sound, image, and data between two sites through electromagnetic wave of the cellular network. ","A handheld mobile user terminal device supports at least one digital mobile communications technology (e.g., a cellular mobile communication technology GSM / GPRS, CDMA, TDSCDMA, WCDMA, CDMA2000, LTE and its follow-up  evolution and integration technology.) to send or receive phone calls or other sound, image, and data between two sites through electromagnetic wave of the cellular network. ","至少支持一种数字移 动通信技术（如蜂窝移动 通信技术中 GSM/GPRS、 CDMA、TD-SCDMA、WCDMA、 CDMA2000、 LTE 及其后续演 进与融合技术等） ，通过蜂 窝网络发送或接收两地讲 话或其他声音、图像、数 据的手持式移动用户终端 设备。"]
[null,{"$f":"IF($B$1=\"English\",C2237,IF($B$1=\"Deutsch\",D2237,IF($B$1=\"中文\",E2237,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mobile communication handset does not include wearable products which have positioning, simple calling, and other functions.  "},"Mobile communication handset does not include wearable products which have positioning, simple calling, and other functions.  ","Mobile communication handset does not include wearable products which have positioning, simple calling, and other functions.  ","移动通信手持机不包括具有定 位、简单通话等功能的可穿戴产品。"]
[null,{"$f":"IF($B$1=\"English\",C2238,IF($B$1=\"Deutsch\",D2238,IF($B$1=\"中文\",E2238,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Telephone set "},"Telephone set ","Telephone set ","电话单机"]
[null,{"$f":"IF($B$1=\"English\",C2239,IF($B$1=\"Deutsch\",D2239,IF($B$1=\"中文\",E2239,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"A telephone set is a user terminal telecommunication device that converts voice into signals that can be transmitted to another device, and converts the received signal to voice. "},"A telephone set is a user terminal telecommunication device that converts voice into signals that can be transmitted to another device, and converts the received signal to voice. ","A telephone set is a user terminal telecommunication device that converts voice into signals that can be transmitted to another device, and converts the received signal to voice. ","电话单机是将声音转 换成可以传送到另一台设 备的信号，在接收信号后 又可将信号转换成声音的 用户终端通信设备。"]
[null,{"$f":"IF($B$1=\"English\",C2240,IF($B$1=\"Deutsch\",D2240,IF($B$1=\"中文\",E2240,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Telephone set includes ordinary PSTN telephone, internet telephone (IP telephone), and other user equipment that converts voice energy into electrical energy and vice versa. Of which: 1) Ordinary PSTN telephone: is the telephone connected to the PSTN public switched telephone network, including wireline telephone and cordless phone. 2) Internet telephone (IP telephone): user terminal equipment that makes and receives calls through the internet. "},"Telephone set includes ordinary PSTN telephone, internet telephone (IP telephone), and other user equipment that converts voice energy into electrical energy and vice versa. Of which: 1) Ordinary PSTN telephone: is the telephone connected to the PSTN public switched telephone network, including wireline telephone and cordless phone. 2) Internet telephone (IP telephone): user terminal equipment that makes and receives calls through the internet. ","Telephone set includes ordinary PSTN telephone, internet telephone (IP telephone), and other user equipment that converts voice energy into electrical energy and vice versa. Of which: 1) Ordinary PSTN telephone: is the telephone connected to the PSTN public switched telephone network, including wireline telephone and cordless phone. 2) Internet telephone (IP telephone): user terminal equipment that makes and receives calls through the internet. ","电话单机包括 PSTN 普通电话 机、网络电话机（IP 电话机）和其 他通信中实现声能与电能相互转换 的用户设备。其中：1）PSTN 普通电 话机：是联入 PSTN 公共交换电话网 络的电话机，包括固定电话和无绳电 话。2）网络电话机（IP 电话机）： 通过互联网实现呼叫和通话的用户 终端设备。"]
[null,{"$f":"IF($B$1=\"English\",C2241,IF($B$1=\"Deutsch\",D2241,IF($B$1=\"中文\",E2241,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hg （Mercury）"},"Hg （Mercury）","Hg （Mercury）","汞（Hg）"]
[null,{"$f":"IF($B$1=\"English\",C2242,IF($B$1=\"Deutsch\",D2242,IF($B$1=\"中文\",E2242,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in single capped (compact) fluorescent lamps for general lighting purposes"},"Mercury in single capped (compact) fluorescent lamps for general lighting purposes","Mercury in single capped (compact) fluorescent lamps for general lighting purposes","普通照明用的单端 (紧凑型) 荧光灯"]
[null,{"$f":"IF($B$1=\"English\",C2243,IF($B$1=\"Deutsch\",D2243,IF($B$1=\"中文\",E2243,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Per Lamp"},"Per Lamp","Per Lamp","每灯管中 汞含量"]
[null,{"$f":"IF($B$1=\"English\",C2244,IF($B$1=\"Deutsch\",D2244,IF($B$1=\"中文\",E2244,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"< 30 W"},"< 30 W","< 30 W","< 30 W"]
[null,{"$f":"IF($B$1=\"English\",C2245,IF($B$1=\"Deutsch\",D2245,IF($B$1=\"中文\",E2245,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" 2.5mg"}," 2.5mg"," 2.5mg"," 2.5mg"]
[null,{"$f":"IF($B$1=\"English\",C2246,IF($B$1=\"Deutsch\",D2246,IF($B$1=\"中文\",E2246,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≥ 30 W and < 50 W"},"≥ 30 W and < 50 W","≥ 30 W and < 50 W","≥ 30 W and < 50 W"]
[null,{"$f":"IF($B$1=\"English\",C2247,IF($B$1=\"Deutsch\",D2247,IF($B$1=\"中文\",E2247,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" 3.5mg"}," 3.5mg"," 3.5mg"," 3.5mg"]
[null,{"$f":"IF($B$1=\"English\",C2248,IF($B$1=\"Deutsch\",D2248,IF($B$1=\"中文\",E2248,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≥ 50 W and < 150 W"},"≥ 50 W and < 150 W","≥ 50 W and < 150 W","≥ 50 W and < 150 W"]
[null,{"$f":"IF($B$1=\"English\",C2249,IF($B$1=\"Deutsch\",D2249,IF($B$1=\"中文\",E2249,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" 5mg"}," 5mg"," 5mg"," 5mg"]
[null,{"$f":"IF($B$1=\"English\",C2250,IF($B$1=\"Deutsch\",D2250,IF($B$1=\"中文\",E2250,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≥ 150 W"},"≥ 150 W","≥ 150 W","≥ 150 W"]
[null,{"$f":"IF($B$1=\"English\",C2251,IF($B$1=\"Deutsch\",D2251,IF($B$1=\"中文\",E2251,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" 15mg"}," 15mg"," 15mg"," 15mg"]
[null,{"$f":"IF($B$1=\"English\",C2252,IF($B$1=\"Deutsch\",D2252,IF($B$1=\"中文\",E2252,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"with circular or square structural shape and\ntube diameter ≤ 17 mm"},"with circular or square structural shape and\ntube diameter ≤ 17 mm","with circular or square structural shape and\ntube diameter ≤ 17 mm","灯管为环形或方形，管直径≤17mm"]
[null,{"$f":"IF($B$1=\"English\",C2253,IF($B$1=\"Deutsch\",D2253,IF($B$1=\"中文\",E2253,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" 7mg"}," 7mg"," 7mg","7mg"]
[null,{"$f":"IF($B$1=\"English\",C2254,IF($B$1=\"Deutsch\",D2254,IF($B$1=\"中文\",E2254,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For special purposes"},"For special purposes","For special purposes","特殊用途的"]
[null,{"$f":"IF($B$1=\"English\",C2255,IF($B$1=\"Deutsch\",D2255,IF($B$1=\"中文\",E2255,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"< 30w and life time>= 20000h"},"< 30w and life time>= 20000h","< 30w and life time>= 20000h","功率＜30W 且寿命≥ 20000h"]
[null,{"$f":"IF($B$1=\"English\",C2256,IF($B$1=\"Deutsch\",D2256,IF($B$1=\"中文\",E2256,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3.5mg"},"3.5mg","3.5mg","3.5mg"]
[null,{"$f":"IF($B$1=\"English\",C2257,IF($B$1=\"Deutsch\",D2257,IF($B$1=\"中文\",E2257,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in Tri-band phosphor with double-capped linear fluorescent lamps for general lighting purposes"},"Mercury in Tri-band phosphor with double-capped linear fluorescent lamps for general lighting purposes","Mercury in Tri-band phosphor with double-capped linear fluorescent lamps for general lighting purposes","普通照明用，使用三基色荧光粉的双端直管型 荧光灯"]
[null,{"$f":"IF($B$1=\"English\",C2258,IF($B$1=\"Deutsch\",D2258,IF($B$1=\"中文\",E2258,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"normal lifetime and a tube diameter < 9 mm (e.g. T2)"},"normal lifetime and a tube diameter < 9 mm (e.g. T2)","normal lifetime and a tube diameter < 9 mm (e.g. T2)","正常使用寿命的、管直径＜9mm(T2)"]
[null,{"$f":"IF($B$1=\"English\",C2259,IF($B$1=\"Deutsch\",D2259,IF($B$1=\"中文\",E2259,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4mg"},"4mg","4mg","4mg"]
[null,{"$f":"IF($B$1=\"English\",C2260,IF($B$1=\"Deutsch\",D2260,IF($B$1=\"中文\",E2260,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"normal lifetime and a tube diameter ≥ 9 mm and ≤ 17 mm (e.g. T5)"},"normal lifetime and a tube diameter ≥ 9 mm and ≤ 17 mm (e.g. T5)","normal lifetime and a tube diameter ≥ 9 mm and ≤ 17 mm (e.g. T5)","正常使用寿命的、9mm≤管直径≤17mm (T5)"]
[null,{"$f":"IF($B$1=\"English\",C2261,IF($B$1=\"Deutsch\",D2261,IF($B$1=\"中文\",E2261,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3mg"},"3mg","3mg","3mg"]
[null,{"$f":"IF($B$1=\"English\",C2262,IF($B$1=\"Deutsch\",D2262,IF($B$1=\"中文\",E2262,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"normal lifetime and a tube diameter > 17 mm and ≤ 28 mm (e.g. T8)"},"normal lifetime and a tube diameter > 17 mm and ≤ 28 mm (e.g. T8)","normal lifetime and a tube diameter > 17 mm and ≤ 28 mm (e.g. T8)","正常使用寿命的、17mm＜管直径≤28mm(T8)"]
[null,{"$f":"IF($B$1=\"English\",C2263,IF($B$1=\"Deutsch\",D2263,IF($B$1=\"中文\",E2263,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"normal lifetime and a tube diameter > 28 mm (e.g. T12)"},"normal lifetime and a tube diameter > 28 mm (e.g. T12)","normal lifetime and a tube diameter > 28 mm (e.g. T12)","正常使用寿命的、管直径＞28mm(T12)"]
[null,{"$f":"IF($B$1=\"English\",C2264,IF($B$1=\"Deutsch\",D2264,IF($B$1=\"中文\",E2264,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"long lifetime (≥ 25 000 h)"},"long lifetime (≥ 25 000 h)","long lifetime (≥ 25 000 h)","长寿命 (≥25000h)"]
[null,{"$f":"IF($B$1=\"English\",C2265,IF($B$1=\"Deutsch\",D2265,IF($B$1=\"中文\",E2265,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5mg"},"5mg","5mg","5mg"]
[null,{"$f":"IF($B$1=\"English\",C2266,IF($B$1=\"Deutsch\",D2266,IF($B$1=\"中文\",E2266,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in other fluorescent lamps"},"Mercury in other fluorescent lamps","Mercury in other fluorescent lamps","其它荧光灯每灯管中汞含量 "]
[null,{"$f":"IF($B$1=\"English\",C2267,IF($B$1=\"Deutsch\",D2267,IF($B$1=\"中文\",E2267,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Linear halophosphate lamps with tube > 28 mm (e.g. T10 and T12)"},"Linear halophosphate lamps with tube > 28 mm (e.g. T10 and T12)","Linear halophosphate lamps with tube > 28 mm (e.g. T10 and T12)","管径>28 mm（T10 和 T12）、使用卤磷酸钙荧 光粉的的直管型荧光灯"]
[null,{"$f":"IF($B$1=\"English\",C2268,IF($B$1=\"Deutsch\",D2268,IF($B$1=\"中文\",E2268,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10 mg"},"10 mg","10 mg","10 mg"]
[null,{"$f":"IF($B$1=\"English\",C2269,IF($B$1=\"Deutsch\",D2269,IF($B$1=\"中文\",E2269,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Non-linear halophosphate lamps (all diameters)"},"Non-linear halophosphate lamps (all diameters)","Non-linear halophosphate lamps (all diameters)","其它使用卤磷酸钙荧光粉的非直管型荧光灯 (所有管径)"]
[null,{"$f":"IF($B$1=\"English\",C2270,IF($B$1=\"Deutsch\",D2270,IF($B$1=\"中文\",E2270,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"15 mg"},"15 mg","15 mg","15 mg"]
[null,{"$f":"IF($B$1=\"English\",C2271,IF($B$1=\"Deutsch\",D2271,IF($B$1=\"中文\",E2271,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9)"},"Non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9)","Non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9)","管直径＞17mm 的非直管型三基色荧光粉荧光 灯 (T9)"]
[null,{"$f":"IF($B$1=\"English\",C2272,IF($B$1=\"Deutsch\",D2272,IF($B$1=\"中文\",E2272,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"15mg"},"15mg","15mg","15mg"]
[null,{"$f":"IF($B$1=\"English\",C2273,IF($B$1=\"Deutsch\",D2273,IF($B$1=\"中文\",E2273,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lamps for other general lighting and special purposes (e.g. induction lamps)"},"Lamps for other general lighting and special purposes (e.g. induction lamps)","Lamps for other general lighting and special purposes (e.g. induction lamps)","其他普通照明用或特殊用途荧光灯(例如感应 灯)"]
[null,{"$f":"IF($B$1=\"English\",C2274,IF($B$1=\"Deutsch\",D2274,IF($B$1=\"中文\",E2274,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes"},"Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes","Mercury in cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes"," 特殊用途的冷阴极荧光灯和外置电极荧光灯 (CCFL 和 EEFL)"]
[null,{"$f":"IF($B$1=\"English\",C2275,IF($B$1=\"Deutsch\",D2275,IF($B$1=\"中文\",E2275,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Short length (≤ 500 mm)"},"Short length (≤ 500 mm)","Short length (≤ 500 mm)","长度短(长度≤500mm)的灯 "]
[null,{"$f":"IF($B$1=\"English\",C2276,IF($B$1=\"Deutsch\",D2276,IF($B$1=\"中文\",E2276,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Medium length (> 500 mm and ≤ 1 500 mm)"},"Medium length (> 500 mm and ≤ 1 500 mm)","Medium length (> 500 mm and ≤ 1 500 mm)","长度中等(500mm＜长度≤1500mm)的灯"]
[null,{"$f":"IF($B$1=\"English\",C2277,IF($B$1=\"Deutsch\",D2277,IF($B$1=\"中文\",E2277,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Long length (> 1 500 mm)"},"Long length (> 1 500 mm)","Long length (> 1 500 mm)","长度长(长度＞1500mm)的灯"]
[null,{"$f":"IF($B$1=\"English\",C2278,IF($B$1=\"Deutsch\",D2278,IF($B$1=\"中文\",E2278,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"13mg"},"13mg","13mg","13mg"]
[null,{"$f":"IF($B$1=\"English\",C2279,IF($B$1=\"Deutsch\",D2279,IF($B$1=\"中文\",E2279,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"other low pressure discharge lamps (per lamp)"},"other low pressure discharge lamps (per lamp)","other low pressure discharge lamps (per lamp)"," 其他低气压放电灯 "]
[null,{"$f":"IF($B$1=\"English\",C2280,IF($B$1=\"Deutsch\",D2280,IF($B$1=\"中文\",E2280,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury (per lamp) ≤ 15mg"},"Mercury (per lamp) ≤ 15mg","Mercury (per lamp) ≤ 15mg","每灯管中汞含量≤15mg "]
[null,{"$f":"IF($B$1=\"English\",C2281,IF($B$1=\"Deutsch\",D2281,IF($B$1=\"中文\",E2281,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner) in lamps with improved colour rendering index Ra > 60"},"High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner) in lamps with improved colour rendering index Ra > 60","High Pressure Sodium (vapour) lamps for general lighting purposes not exceeding (per burner) in lamps with improved colour rendering index Ra > 60","显色指数改善型（Ra＞60）普通照明用高压钠 （蒸气）灯"]
[null,{"$f":"IF($B$1=\"English\",C2282,IF($B$1=\"Deutsch\",D2282,IF($B$1=\"中文\",E2282,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury (per lamp)"},"Mercury (per lamp)","Mercury (per lamp)","每灯管中汞含量 "]
[null,{"$f":"IF($B$1=\"English\",C2283,IF($B$1=\"Deutsch\",D2283,IF($B$1=\"中文\",E2283,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P ≤155W"},"P ≤155W","P ≤155W","P ≤155W"]
[null,{"$f":"IF($B$1=\"English\",C2284,IF($B$1=\"Deutsch\",D2284,IF($B$1=\"中文\",E2284,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"30mg"},"30mg","30mg","30mg"]
[null,{"$f":"IF($B$1=\"English\",C2285,IF($B$1=\"Deutsch\",D2285,IF($B$1=\"中文\",E2285,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"155W＜P≤405W"},"155W＜P≤405W","155W＜P≤405W","155W＜P≤405W"]
[null,{"$f":"IF($B$1=\"English\",C2286,IF($B$1=\"Deutsch\",D2286,IF($B$1=\"中文\",E2286,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"40mg"},"40mg","40mg","40mg"]
[null,{"$f":"IF($B$1=\"English\",C2287,IF($B$1=\"Deutsch\",D2287,IF($B$1=\"中文\",E2287,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"P＞405W"},"P＞405W","P＞405W","P＞405W"]
[null,{"$f":"IF($B$1=\"English\",C2288,IF($B$1=\"Deutsch\",D2288,IF($B$1=\"中文\",E2288,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"other High Pressure Sodium (vapour) lamps"},"other High Pressure Sodium (vapour) lamps","other High Pressure Sodium (vapour) lamps","其它普通照明用高压钠（蒸气）灯"]
[null,{"$f":"IF($B$1=\"English\",C2289,IF($B$1=\"Deutsch\",D2289,IF($B$1=\"中文\",E2289,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"25mg"},"25mg","25mg","25mg"]
[null,{"$f":"IF($B$1=\"English\",C2290,IF($B$1=\"Deutsch\",D2290,IF($B$1=\"中文\",E2290,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in High Pressure Mercury (vapour) lamps (HPMV)"},"Mercury in High Pressure Mercury (vapour) lamps (HPMV)","Mercury in High Pressure Mercury (vapour) lamps (HPMV)","高压汞(蒸汽)灯(HPMV)"]
[null,{"$f":"IF($B$1=\"English\",C2291,IF($B$1=\"Deutsch\",D2291,IF($B$1=\"中文\",E2291,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use, until\nDecember 31,2020"},"No limitation of use, until\nDecember 31,2020","No limitation of use, until\nDecember 31,2020","无限值要求，截至时间 为2020年12月31日"]
[null,{"$f":"IF($B$1=\"English\",C2292,IF($B$1=\"Deutsch\",D2292,IF($B$1=\"中文\",E2292,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in metal halide lamps (MH)"},"Mercury in metal halide lamps (MH)","Mercury in metal halide lamps (MH)","金属卤化物灯 (MH)"]
[null,{"$f":"IF($B$1=\"English\",C2293,IF($B$1=\"Deutsch\",D2293,IF($B$1=\"中文\",E2293,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No limitation of use"},"No limitation of use","No limitation of use","无限值要求"]
[null,{"$f":"IF($B$1=\"English\",C2294,IF($B$1=\"Deutsch\",D2294,IF($B$1=\"中文\",E2294,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in other discharge lamps for special purposes not specifically mentioned in this\nAnnex"},"Mercury in other discharge lamps for special purposes not specifically mentioned in this\nAnnex","Mercury in other discharge lamps for special purposes not specifically mentioned in this\nAnnex","本文件中未提及的其它特殊用途的放电灯中的汞"]
[null,{"$f":"IF($B$1=\"English\",C2295,IF($B$1=\"Deutsch\",D2295,IF($B$1=\"中文\",E2295,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury in hand crafted luminous discharge tubes (HLDTs) used for signs, decorative or architectural and specialist lighting and light-artwork,\n(a) 20 mg per electrode pair + 0,3 mg per tube length in cm, for outdoor applications and indoor applications exposed to temperatures below 20 °C;\n(b)15 mg per electrode pair + 0,24 mg, for all other indoor application"},"Mercury in hand crafted luminous discharge tubes (HLDTs) used for signs, decorative or architectural and specialist lighting and light-artwork,\n(a) 20 mg per electrode pair + 0,3 mg per tube length in cm, for outdoor applications and indoor applications exposed to temperatures below 20 °C;\n(b)15 mg per electrode pair + 0,24 mg, for all other indoor application","Mercury in hand crafted luminous discharge tubes (HLDTs) used for signs, decorative or architectural and specialist lighting and light-artwork,\n(a) 20 mg per electrode pair + 0,3 mg per tube length in cm, for outdoor applications and indoor applications exposed to temperatures below 20 °C;\n(b)15 mg per electrode pair + 0,24 mg, for all other indoor application","用于标志、装饰、建筑、专业照明和灯光艺术 的手工制作发光放电管(HLDTs)\n(a) 用于温度低于20℃的户外及室内时， 20mg/电极对 + 0.3mg/灯管长度(cm）\n(b)用于其他的室内环境时， 15mg/电极对 + 0.24mg/灯管长度(cm)"]
[null,{"$f":"IF($B$1=\"English\",C2296,IF($B$1=\"Deutsch\",D2296,IF($B$1=\"中文\",E2296,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury / per tube length\nin cm:\n80mg"},"Mercury / per tube length\nin cm:\n80mg","Mercury / per tube length\nin cm:\n80mg","汞含量 ≤ 80mg"]
[null,{"$f":"IF($B$1=\"English\",C2297,IF($B$1=\"Deutsch\",D2297,IF($B$1=\"中文\",E2297,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury used as a cathode sputtering inhibitor in DC plasma displays"},"Mercury used as a cathode sputtering inhibitor in DC plasma displays","Mercury used as a cathode sputtering inhibitor in DC plasma displays","直流等离子体显示器中作为阴极溅射抑制剂"]
[null,{"$f":"IF($B$1=\"English\",C2298,IF($B$1=\"Deutsch\",D2298,IF($B$1=\"中文\",E2298,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"with a content ≤ 30 mg"},"with a content ≤ 30 mg","with a content ≤ 30 mg","汞含量 ≤ 30 mg"]
[null,{"$f":"IF($B$1=\"English\",C2299,IF($B$1=\"Deutsch\",D2299,IF($B$1=\"中文\",E2299,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pb （lead）"},"Pb （lead）","Pb （lead）","铅（Pb）"]
[null,{"$f":"IF($B$1=\"English\",C2300,IF($B$1=\"Deutsch\",D2300,IF($B$1=\"中文\",E2300,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in glass of cathode ray tubes"},"Lead in glass of cathode ray tubes","Lead in glass of cathode ray tubes","阴极射线管用玻璃"]
[null,{"$f":"IF($B$1=\"English\",C2301,IF($B$1=\"Deutsch\",D2301,IF($B$1=\"中文\",E2301,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in glass of fluorescent tubes"},"Lead in glass of fluorescent tubes","Lead in glass of fluorescent tubes","荧光灯管用玻璃"]
[null,{"$f":"IF($B$1=\"English\",C2302,IF($B$1=\"Deutsch\",D2302,IF($B$1=\"中文\",E2302,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"not exceeding 0,2 % by weight"},"not exceeding 0,2 % by weight","not exceeding 0,2 % by weight","≤0.2%（重量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C2303,IF($B$1=\"Deutsch\",D2303,IF($B$1=\"中文\",E2303,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in steel for machining purposes and in galvanised steel"},"Lead as an alloying element in steel for machining purposes and in galvanised steel","Lead as an alloying element in steel for machining purposes and in galvanised steel","用于加工的钢合金和镀锌钢（铅作为合金元 素）"]
[null,{"$f":"IF($B$1=\"English\",C2304,IF($B$1=\"Deutsch\",D2304,IF($B$1=\"中文\",E2304,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"containing up to 0,35 %\nlead by weight"},"containing up to 0,35 %\nlead by weight","containing up to 0,35 %\nlead by weight","≤0.35%（重量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C2305,IF($B$1=\"Deutsch\",D2305,IF($B$1=\"中文\",E2305,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in aluminium containing"},"Lead as an alloying element in aluminium containing","Lead as an alloying element in aluminium containing","铝合金（铅作为合金元素)"]
[null,{"$f":"IF($B$1=\"English\",C2306,IF($B$1=\"Deutsch\",D2306,IF($B$1=\"中文\",E2306,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"up to 0,4 % lead by weight）"},"up to 0,4 % lead by weight）","up to 0,4 % lead by weight）","≤0.4%（重量百分比） "]
[null,{"$f":"IF($B$1=\"English\",C2307,IF($B$1=\"Deutsch\",D2307,IF($B$1=\"中文\",E2307,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element in Copper alloy"},"Lead as an alloying element in Copper alloy","Lead as an alloying element in Copper alloy","铜合金（铅作为合金元素）"]
[null,{"$f":"IF($B$1=\"English\",C2308,IF($B$1=\"Deutsch\",D2308,IF($B$1=\"中文\",E2308,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"containing up to 4 % lead\nby weight"},"containing up to 4 % lead\nby weight","containing up to 4 % lead\nby weight","≤4%（重量百分比） "]
[null,{"$f":"IF($B$1=\"English\",C2309,IF($B$1=\"Deutsch\",D2309,IF($B$1=\"中文\",E2309,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in high melting temperature type solders (i.e. lead- based alloys containing 85 % by weight or more lead)"},"Lead in high melting temperature type solders (i.e. lead- based alloys containing 85 % by weight or more lead)","Lead in high melting temperature type solders (i.e. lead- based alloys containing 85 % by weight or more lead)","高熔点焊料 (如铅含量超过 85%（重量百分 比）的铅基合金焊料)"]
[null,{"$f":"IF($B$1=\"English\",C2310,IF($B$1=\"Deutsch\",D2310,IF($B$1=\"中文\",E2310,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission, and network management for telecommunications"},"Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission, and network management for telecommunications","Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission, and network management for telecommunications","用于服务器、存储器和存储列阵系统的焊料； 用于交换、信号发送和传输，以及电信网络管 理的网络基础设施设备内焊料"]
[null,{"$f":"IF($B$1=\"English\",C2311,IF($B$1=\"Deutsch\",D2311,IF($B$1=\"中文\",E2311,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g.piezoelectronic devices, or in a glass or ceramic matrix compound"},"Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g.piezoelectronic devices, or in a glass or ceramic matrix compound","Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g.piezoelectronic devices, or in a glass or ceramic matrix compound","陶瓷及玻璃：用于除介电陶瓷电容以外的电子 电气元器件 (例如，压电器件、玻璃和陶瓷的 复合材料)"]
[null,{"$f":"IF($B$1=\"English\",C2312,IF($B$1=\"Deutsch\",D2312,IF($B$1=\"中文\",E2312,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher"},"Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher","Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher","介电陶瓷电容：用于连接≥交流 125V 或直流 250V"]
[null,{"$f":"IF($B$1=\"English\",C2313,IF($B$1=\"Deutsch\",D2313,IF($B$1=\"中文\",E2313,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC"},"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC","Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC","介电陶瓷电容：用于连接＜交流 125V 或直流 250V"]
[null,{"$f":"IF($B$1=\"English\",C2314,IF($B$1=\"Deutsch\",D2314,IF($B$1=\"中文\",E2314,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors’"},"Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors’","Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors’","用于集成电路或分立半导体中的锆钛酸铅 (PZT)介电陶瓷电容"]
[null,{"$f":"IF($B$1=\"English\",C2315,IF($B$1=\"Deutsch\",D2315,IF($B$1=\"中文\",E2315,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in bearing shells and bushes for refrigerant-containing compressors for heating, ventilation, air conditioning and\nrefrigeration (HVACR) applications"},"Lead in bearing shells and bushes for refrigerant-containing compressors for heating, ventilation, air conditioning and\nrefrigeration (HVACR) applications","Lead in bearing shells and bushes for refrigerant-containing compressors for heating, ventilation, air conditioning and\nrefrigeration (HVACR) applications","暖通空调 (HVACR) 设备压缩机轴承外壳及轴 衬"]
[null,{"$f":"IF($B$1=\"English\",C2316,IF($B$1=\"Deutsch\",D2316,IF($B$1=\"中文\",E2316,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead used in C-press compliant pin connector\nsystems used in spare parts"},"Lead used in C-press compliant pin connector\nsystems used in spare parts","Lead used in C-press compliant pin connector\nsystems used in spare parts","C-顺应针连接器系统（仅作为备用部件）"]
[null,{"$f":"IF($B$1=\"English\",C2317,IF($B$1=\"Deutsch\",D2317,IF($B$1=\"中文\",E2317,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead used in other than C-press compliant pin connector systems"},"Lead used in other than C-press compliant pin connector systems","Lead used in other than C-press compliant pin connector systems","除 C-顺应针连接器系统外的连接器系统 "]
[null,{"$f":"IF($B$1=\"English\",C2318,IF($B$1=\"Deutsch\",D2318,IF($B$1=\"中文\",E2318,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as a coating material for the thermal conduction module C-ring used in spare parts"},"Lead as a coating material for the thermal conduction module C-ring used in spare parts","Lead as a coating material for the thermal conduction module C-ring used in spare parts","环形导热模块的表面涂层（仅作为备用部 件）"]
[null,{"$f":"IF($B$1=\"English\",C2319,IF($B$1=\"Deutsch\",D2319,IF($B$1=\"中文\",E2319,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in white glasses used for optical applications"},"Lead in white glasses used for optical applications","Lead in white glasses used for optical applications","光学白玻璃"]
[null,{"$f":"IF($B$1=\"English\",C2320,IF($B$1=\"Deutsch\",D2320,IF($B$1=\"中文\",E2320,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors\nwith a lead content of more than 80 % and less than 85 % by weight"},"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors\nwith a lead content of more than 80 % and less than 85 % by weight","Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors\nwith a lead content of more than 80 % and less than 85 % by weight","微处理器的针脚与封装体连接所使用的、含两 种以上元素的焊料铅含量占 80%~85%（重量百 分比） "]
[null,{"$f":"IF($B$1=\"English\",C2321,IF($B$1=\"Deutsch\",D2321,IF($B$1=\"中文\",E2321,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit flip chip packages"},"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit flip chip packages","Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit flip chip packages","集成电路倒装芯片封装中半导体芯片及载体 之间形成可靠联接的焊料"]
[null,{"$f":"IF($B$1=\"English\",C2322,IF($B$1=\"Deutsch\",D2322,IF($B$1=\"中文\",E2322,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in linear incandescent lamps with silicate coated tubes"},"Lead in linear incandescent lamps with silicate coated tubes","Lead in linear incandescent lamps with silicate coated tubes","带硅酸盐套管的线型白炽灯"]
[null,{"$f":"IF($B$1=\"English\",C2323,IF($B$1=\"Deutsch\",D2323,IF($B$1=\"中文\",E2323,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead halide as radiant agent in high intensity discharge (HID) lamps used for professional reprography applications"},"Lead halide as radiant agent in high intensity discharge (HID) lamps used for professional reprography applications","Lead halide as radiant agent in high intensity discharge (HID) lamps used for professional reprography applications","用于专业复印设备的高强度放电灯(HID)中用 作发光剂的卤化铅"]
[null,{"$f":"IF($B$1=\"English\",C2324,IF($B$1=\"Deutsch\",D2324,IF($B$1=\"中文\",E2324,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as activator in the fluorescent powder of discharge lamps when used as speciality\nlamps for diazoprinting reprography,lithography, insect traps, photochemical and curing processes containing phosphors such as SMS（(Sr，Ba)2MgSi2O7:Pb）"},"Lead as activator in the fluorescent powder of discharge lamps when used as speciality\nlamps for diazoprinting reprography,lithography, insect traps, photochemical and curing processes containing phosphors such as SMS（(Sr，Ba)2MgSi2O7:Pb）","Lead as activator in the fluorescent powder of discharge lamps when used as speciality\nlamps for diazoprinting reprography,lithography, insect traps, photochemical and curing processes containing phosphors such as SMS（(Sr，Ba)2MgSi2O7:Pb）"," 用于重氮复印、平板印刷、捕虫器、光化学和 固化过程的特种灯所用的荧光粉如 SMS（ （Sr, Ba）2MgSi2O7:Pb） ，铅作为荧光粉中的催化剂"]
[null,{"$f":"IF($B$1=\"English\",C2325,IF($B$1=\"Deutsch\",D2325,IF($B$1=\"中文\",E2325,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"lead by weight ≤ 1 %"},"lead by weight ≤ 1 %","lead by weight ≤ 1 %","铅含量≤1 %（重量百分 比）"]
[null,{"$f":"IF($B$1=\"English\",C2326,IF($B$1=\"Deutsch\",D2326,IF($B$1=\"中文\",E2326,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)"},"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)","Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)","仿日晒放电灯所用含有磷元素的荧光粉如 BSP (BaSi2O5:Pb)，铅作为荧光粉中的催化剂, 铅含量≤1 %（重量百分 比）"]
[null,{"$f":"IF($B$1=\"English\",C2327,IF($B$1=\"Deutsch\",D2327,IF($B$1=\"中文\",E2327,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact energy saving lamps (ESL)"},"Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact energy saving lamps (ESL)","Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact energy saving lamps (ESL)","超小型节能灯(ESL)主汞齐组分 PbBiSn-Hg 和 PbInSn-Hg，以及辅助汞齐组分 PbSn-Hg 中 的铅"]
[null,{"$f":"IF($B$1=\"English\",C2328,IF($B$1=\"Deutsch\",D2328,IF($B$1=\"中文\",E2328,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCDs)"},"Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCDs)","Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCDs)","液晶显示器中连接前后平板荧光灯基质的玻璃中的氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C2329,IF($B$1=\"Deutsch\",D2329,IF($B$1=\"中文\",E2329,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in finishes of fine pitch components other than connectors with a pitch of 0,65 mm and less"},"Lead in finishes of fine pitch components other than connectors with a pitch of 0,65 mm and less","Lead in finishes of fine pitch components other than connectors with a pitch of 0,65 mm and less","用于引脚间距≤0.65mm 的细间距元器件 (不 包括连接器类)表面处理"]
[null,{"$f":"IF($B$1=\"English\",C2330,IF($B$1=\"Deutsch\",D2330,IF($B$1=\"中文\",E2330,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors"},"Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors","Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors","通孔盘状和平面阵列的多层陶瓷电容中焊料"]
[null,{"$f":"IF($B$1=\"English\",C2331,IF($B$1=\"Deutsch\",D2331,IF($B$1=\"中文\",E2331,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in surface conduction electron emitter displays (SED) used in structural elements, notably in the seal frit and frit ring"},"Lead oxide in surface conduction electron emitter displays (SED) used in structural elements, notably in the seal frit and frit ring","Lead oxide in surface conduction electron emitter displays (SED) used in structural elements, notably in the seal frit and frit ring","表面传导式电子发射显示器 (SED) 构件所用 的氧化铅，特别是密封玻璃和玻璃环"]
[null,{"$f":"IF($B$1=\"English\",C2332,IF($B$1=\"Deutsch\",D2332,IF($B$1=\"中文\",E2332,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in the glass envelope of black light blue lamps"},"Lead oxide in the glass envelope of black light blue lamps","Lead oxide in the glass envelope of black light blue lamps","黑光灯的玻璃泡壳中的氧化铅"]
[null,{"$f":"IF($B$1=\"English\",C2333,IF($B$1=\"Deutsch\",D2333,IF($B$1=\"中文\",E2333,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers"},"Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers","Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers","大功率扬声器（特指连续几小时运转在声功率 125 分贝以上）中传感器的焊料中的铅合金"]
[null,{"$f":"IF($B$1=\"English\",C2334,IF($B$1=\"Deutsch\",D2334,IF($B$1=\"中文\",E2334,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead bound in 4 categories crystal glass"},"Lead bound in 4 categories crystal glass","Lead bound in 4 categories crystal glass","以下 4 类水晶玻璃："]
[null,{"$f":"IF($B$1=\"English\",C2335,IF($B$1=\"Deutsch\",D2335,IF($B$1=\"中文\",E2335,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1． PbO >=30% (by weight), Density ≥3.00, Refractive ≥1.545"},"1． PbO >=30% (by weight), Density ≥3.00, Refractive ≥1.545","1． PbO >=30% (by weight), Density ≥3.00, Refractive ≥1.545","1．氧化铅含量≥30%（重量百分比），密度≥ 3.00，折射率≥1.545；"]
[null,{"$f":"IF($B$1=\"English\",C2336,IF($B$1=\"Deutsch\",D2336,IF($B$1=\"中文\",E2336,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2．PbO≥24%（by weight）, Density≥2.90，Refractive≥1.545；"},"2．PbO≥24%（by weight）, Density≥2.90，Refractive≥1.545；","2．PbO≥24%（by weight）, Density≥2.90，Refractive≥1.545；","2．氧化铅含量≥24%（重量百分比），密度≥ 2.90，折射率≥1.545；"]
[null,{"$f":"IF($B$1=\"English\",C2337,IF($B$1=\"Deutsch\",D2337,IF($B$1=\"中文\",E2337,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.45，Refractive≥1.520；"},"3. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.45，Refractive≥1.520；","3. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.45，Refractive≥1.520；","3. 氧化铅、氧化锌、氧化钡、氧化钾单一含量或含量总和≥10%（重量百分比），密度≥ 2.45，折射率≥1.520；"]
[null,{"$f":"IF($B$1=\"English\",C2338,IF($B$1=\"Deutsch\",D2338,IF($B$1=\"中文\",E2338,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.40，Surface hardness to Vickers hardness\n550±20。"},"4. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.40，Surface hardness to Vickers hardness\n550±20。","4. PbO 、ZnO 、BaO 、K2O singaly or together≥10%（by weight），Density≥2.40，Surface hardness to Vickers hardness\n550±20。","4. 氧化铅、氧化钡、氧化钾单一含量或含量 总和≥10%（重量百分比） ，密度≥2.40，表面 硬度达到维氏硬度 550±20。"]
[null,{"$f":"IF($B$1=\"English\",C2339,IF($B$1=\"Deutsch\",D2339,IF($B$1=\"中文\",E2339,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in soldering materials in mercury free flat fluorescent lamps (which, e.g. are used for liquid crystal displays, design or industrial lighting)"},"Lead in soldering materials in mercury free flat fluorescent lamps (which, e.g. are used for liquid crystal displays, design or industrial lighting)","Lead in soldering materials in mercury free flat fluorescent lamps (which, e.g. are used for liquid crystal displays, design or industrial lighting)","用于无汞平面荧光灯 (例如：用于液晶显示 器、设计或工业照明) 的焊料"]
[null,{"$f":"IF($B$1=\"English\",C2340,IF($B$1=\"Deutsch\",D2340,IF($B$1=\"中文\",E2340,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes"},"Lead oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes","Lead oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes","用于氩和氪激光管窗组件密封玻璃料中的氧 化铅"]
[null,{"$f":"IF($B$1=\"English\",C2341,IF($B$1=\"Deutsch\",D2341,IF($B$1=\"中文\",E2341,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in solders for the soldering of thin copper wires of 100 μm diameter and less in power transformers"},"Lead in solders for the soldering of thin copper wires of 100 μm diameter and less in power transformers","Lead in solders for the soldering of thin copper wires of 100 μm diameter and less in power transformers","电源变压器中直径≤100µm 的细铜线所用焊 料"]
[null,{"$f":"IF($B$1=\"English\",C2342,IF($B$1=\"Deutsch\",D2342,IF($B$1=\"中文\",E2342,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in cermet-based trimmer\npotentiometer elements"},"Lead in cermet-based trimmer\npotentiometer elements","Lead in cermet-based trimmer\npotentiometer elements","金属陶瓷质的微调电位器"]
[null,{"$f":"IF($B$1=\"English\",C2343,IF($B$1=\"Deutsch\",D2343,IF($B$1=\"中文\",E2343,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body"},"Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body","Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body","基于硼酸锌玻璃体的高压二极管的电镀层"]
[null,{"$f":"IF($B$1=\"English\",C2344,IF($B$1=\"Deutsch\",D2344,IF($B$1=\"中文\",E2344,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as a thermal stabiliser in polyvinyl chloride (PVC) used as base material in amperometric, potentiometric and conductometric electrochemical sensors which are used in in-vitro diagnostic medical devices for the analysis of blood and other body fluids and body gases. "},"Lead as a thermal stabiliser in polyvinyl chloride (PVC) used as base material in amperometric, potentiometric and conductometric electrochemical sensors which are used in in-vitro diagnostic medical devices for the analysis of blood and other body fluids and body gases. ","Lead as a thermal stabiliser in polyvinyl chloride (PVC) used as base material in amperometric, potentiometric and conductometric electrochemical sensors which are used in in-vitro diagnostic medical devices for the analysis of blood and other body fluids and body gases. ","用于电子电气元器件的焊料和最终表面材料， 以及点火模块和其他电气和电子发动机控制 系统（由于技术原因，必须直接安装在曲轴箱 或手持内燃机汽缸内的）中使用的印刷电路板 表面材料"]
[null,{"$f":"IF($B$1=\"English\",C2345,IF($B$1=\"Deutsch\",D2345,IF($B$1=\"中文\",E2345,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cd（Cadmium）"},"Cd（Cadmium）","Cd（Cadmium）","和镉（Cd）"]
[null,{"$f":"IF($B$1=\"English\",C2346,IF($B$1=\"Deutsch\",D2346,IF($B$1=\"中文\",E2346,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"one shot pellet type thermal cut-offs"},"one shot pellet type thermal cut-offs","one shot pellet type thermal cut-offs","一次性的球型热熔断体"]
[null,{"$f":"IF($B$1=\"English\",C2347,IF($B$1=\"Deutsch\",D2347,IF($B$1=\"中文\",E2347,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"electrical contacts"},"electrical contacts","electrical contacts","电触点"]
[null,{"$f":"IF($B$1=\"English\",C2348,IF($B$1=\"Deutsch\",D2348,IF($B$1=\"中文\",E2348,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound\npressure levels of 100 dB (A) and more"},"Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound\npressure levels of 100 dB (A) and more","Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound\npressure levels of 100 dB (A) and more","用于位于声压级≥100 分贝的大功率场声器 音圈上的电导体的电气或机械焊点"]
[null,{"$f":"IF($B$1=\"English\",C2349,IF($B$1=\"Deutsch\",D2349,IF($B$1=\"中文\",E2349,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"thick film pastes used on aluminium bonded beryllium oxide"},"thick film pastes used on aluminium bonded beryllium oxide","thick film pastes used on aluminium bonded beryllium oxide","氧化铍与铝键合用厚膜浆料中的镉和氧化镉"]
[null,{"$f":"IF($B$1=\"English\",C2350,IF($B$1=\"Deutsch\",D2350,IF($B$1=\"中文\",E2350,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"colour converting II-VI LEDs for use in solid state illumination or display systems "},"colour converting II-VI LEDs for use in solid state illumination or display systems ","colour converting II-VI LEDs for use in solid state illumination or display systems ","用于固态照明或显示系统中的彩色转换 II-VI 族发光二极管（LEDs）"]
[null,{"$f":"IF($B$1=\"English\",C2351,IF($B$1=\"Deutsch\",D2351,IF($B$1=\"中文\",E2351,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium < 10 μg Cd per square millimeter of light-emitting area"},"Cadmium < 10 μg Cd per square millimeter of light-emitting area","Cadmium < 10 μg Cd per square millimeter of light-emitting area","每平方毫米发光区域镉含量＜10µg"]
[null,{"$f":"IF($B$1=\"English\",C2352,IF($B$1=\"Deutsch\",D2352,IF($B$1=\"中文\",E2352,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium in cadmium-based semiconductor nanocrystal quantum dots for low energy conversion in display lighting applications\n"},"Cadmium in cadmium-based semiconductor nanocrystal quantum dots for low energy conversion in display lighting applications\n","Cadmium in cadmium-based semiconductor nanocrystal quantum dots for low energy conversion in display lighting applications\n","用于显示照明应用中的低能级转换镉基半导 体纳米晶体量子点中的镉"]
[null,{"$f":"IF($B$1=\"English\",C2353,IF($B$1=\"Deutsch\",D2353,IF($B$1=\"中文\",E2353,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"< 0.2 μg Cd per square\nmillimeter of screen display area"},"< 0.2 μg Cd per square\nmillimeter of screen display area","< 0.2 μg Cd per square\nmillimeter of screen display area","每平方毫米屏幕显示区 域镉含量＜0.2µg"]
[null,{"$f":"IF($B$1=\"English\",C2354,IF($B$1=\"Deutsch\",D2354,IF($B$1=\"中文\",E2354,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"photoresistors for analogue optocouplers applied in professional audio equipment"},"photoresistors for analogue optocouplers applied in professional audio equipment","photoresistors for analogue optocouplers applied in professional audio equipment","与业的声频设备中使用的模拟光耦合器中的 光敏电阻器中的镉"]
[null,{"$f":"IF($B$1=\"English\",C2355,IF($B$1=\"Deutsch\",D2355,IF($B$1=\"中文\",E2355,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cr VI （Hexavalent chromium）"},"Cr VI （Hexavalent chromium）","Cr VI （Hexavalent chromium）","六价铬(Cr6+)"]
[null,{"$f":"IF($B$1=\"English\",C2356,IF($B$1=\"Deutsch\",D2356,IF($B$1=\"中文\",E2356,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexavalent chromium as an anticorrosion agent of the carbon steel cooling system in absorption refrigerators"},"Hexavalent chromium as an anticorrosion agent of the carbon steel cooling system in absorption refrigerators","Hexavalent chromium as an anticorrosion agent of the carbon steel cooling system in absorption refrigerators","吸收式电冰箱中作为碳钢冷却系统防腐剂 "]
[null,{"$f":"IF($B$1=\"English\",C2357,IF($B$1=\"Deutsch\",D2357,IF($B$1=\"中文\",E2357,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexavalent chromium ≤ 0,75 % by weight in the cooling solution"},"Hexavalent chromium ≤ 0,75 % by weight in the cooling solution","Hexavalent chromium ≤ 0,75 % by weight in the cooling solution","冷却液中六价铬的含量 ≤0.75%（重量百分比）"]
[null,{"$f":"IF($B$1=\"English\",C2358,IF($B$1=\"Deutsch\",D2358,IF($B$1=\"中文\",E2358,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pb（lead） and Cd（Cadmium）"},"Pb（lead） and Cd（Cadmium）","Pb（lead） and Cd（Cadmium）","铅（Pb）和镉（Cd）"]
[null,{"$f":"IF($B$1=\"English\",C2359,IF($B$1=\"Deutsch\",D2359,IF($B$1=\"中文\",E2359,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium and lead in filter glasses and glasses used for reflectance standards"},"Cadmium and lead in filter glasses and glasses used for reflectance standards","Cadmium and lead in filter glasses and glasses used for reflectance standards","滤光玻璃和标准反射玻璃 "]
[null,{"$f":"IF($B$1=\"English\",C2360,IF($B$1=\"Deutsch\",D2360,IF($B$1=\"中文\",E2360,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and cadmium in printing inks for the application of enamels on glasses, such as borosilicate and soda lime glasses"},"Lead and cadmium in printing inks for the application of enamels on glasses, such as borosilicate and soda lime glasses","Lead and cadmium in printing inks for the application of enamels on glasses, such as borosilicate and soda lime glasses","用于硼硅玻璃表面瓷釉上的印刷油墨 "]
[null,{"$f":"IF($B$1=\"English\",C2361,IF($B$1=\"Deutsch\",D2361,IF($B$1=\"中文\",E2361,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C2362,IF($B$1=\"Deutsch\",D2362,IF($B$1=\"中文\",E2362,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Change history"},"Change history","Änderungsprotokoll","变更历史"]
[null,{"$f":"IF($B$1=\"English\",C2363,IF($B$1=\"Deutsch\",D2363,IF($B$1=\"中文\",E2363,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Section"},"Section","Bereich","条款"]
[null,{"$f":"IF($B$1=\"English\",C2364,IF($B$1=\"Deutsch\",D2364,IF($B$1=\"中文\",E2364,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comment"},"Comment","Bemerkung","注释"]
[null,{"$f":"IF($B$1=\"English\",C2365,IF($B$1=\"Deutsch\",D2365,IF($B$1=\"中文\",E2365,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Version"},"Version","Version","版本"]
[null,{"$f":"IF($B$1=\"English\",C2366,IF($B$1=\"Deutsch\",D2366,IF($B$1=\"中文\",E2366,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4 declarable substances added (25.06.2020)"},"4 declarable substances added (25.06.2020)","4 declarable substances added (25.06.2020)","添加4种申报物质（25.06.2020）"]
[null,{"$f":"IF($B$1=\"English\",C2367,IF($B$1=\"Deutsch\",D2367,IF($B$1=\"中文\",E2367,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"List of exemptions and expiry dates  updated"},"List of exemptions and expiry dates  updated","List of exemptions and expiry dates  updated","更新豁免和有效期清单"]
[null,{"$f":"IF($B$1=\"English\",C2368,IF($B$1=\"Deutsch\",D2368,IF($B$1=\"中文\",E2368,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n\n- sunset date:\n21. Mai 2015"},"included in Annex 14\n- \nlast application date:\n21. November 2013\n\n- sunset date:\n21. Mai 2015","aufgenommen in Anhang 14\n- Antragsschluss:\n21. November 2013\n- Ablauftermin:\n21. Mai 2015","包括在附录14\n-申请截止日期:2013年11月21日\n\n- 过期:2015年3月21日"]
[null,{"$f":"IF($B$1=\"English\",C2369,IF($B$1=\"Deutsch\",D2369,IF($B$1=\"中文\",E2369,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015"},"included in Annex 14\n- \nlast application date:\n21. November 2013\n- sunset date:\n21. Mai 2015","aufgenommen in Anhang 14\n- Antragsschluss:\n21. November 2013\n- Ablauftermin:\n21. Mai 2015","包括在附录14\n-申请截止日期:2013年11月21日\n- 过期:2015年3月21日"]
[null,{"$f":"IF($B$1=\"English\",C2370,IF($B$1=\"Deutsch\",D2370,IF($B$1=\"中文\",E2370,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n"},"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss:\n21. August 2013\n- Ablauftermin:\n21. Februar 2015\n","包括在附录14和17\n-申请截止日期:2013年8月21日\n- 过期:2015年2月21日"]
[null,{"$f":"IF($B$1=\"English\",C2371,IF($B$1=\"Deutsch\",D2371,IF($B$1=\"中文\",E2371,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: \n21. Februar 2013\n- \nsunset date:\n21. August 2014"},"included in Annex 14\n- \nlast application date: \n21. Februar 2013\n- \nsunset date:\n21. August 2014","aufgenommen in Anhang 14\n- Antragsschluss: \n21. Februar 2013\n- Ablauftermin:\n21. August 2014","包括在附录14\n-申请截止日期:2013年2月21日\n-过期:2015年8月21日"]
[null,{"$f":"IF($B$1=\"English\",C2372,IF($B$1=\"Deutsch\",D2372,IF($B$1=\"中文\",E2372,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date:\n21. Februar 2014\n- \nsunset date:\n21. August 2015"},"included in Annex 14\n- \nlast application date:\n21. Februar 2014\n- \nsunset date:\n21. August 2015","aufgenommen in Anhang 14\n- Antragsschluss:\n21. Februar 2014\n- Ablauftermin:\n21. August 2015","包括在附录14\n-申请截止日期:2014年2月21日\n-过期:2015年8月21日"]
[null,{"$f":"IF($B$1=\"English\",C2373,IF($B$1=\"Deutsch\",D2373,IF($B$1=\"中文\",E2373,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: 4. April 2019\n- \nsunset date: 4. Oktober 2020"},"included in Annex 14\n- \nlast application date: 4. April 2019\n- \nsunset date: 4. Oktober 2020","aufgenommen in Anhang 14\n- Antragsschluss: \n4. April 2019\n- Ablauftermin: \n4. Oktober 2020","包括在附录14\n-申请截止日期:2019年4月4日\n- 过期:2020年10月4日"]
[null,{"$f":"IF($B$1=\"English\",C2374,IF($B$1=\"Deutsch\",D2374,IF($B$1=\"中文\",E2374,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: \n21. August 2013\n- \nsunset date:\n21. Februar 2015"},"included in Annex 14\n- \nlast application date: \n21. August 2013\n- \nsunset date:\n21. Februar 2015","aufgenommen in Anhang 14\n- Antragsschluss: \n21. August 2013\n- Ablauftermin:\n21. Februar 2015","包括在附录14\n-申请截止日期:2013年8月21日\n-过期:2015年2月21日"]
[null,{"$f":"IF($B$1=\"English\",C2375,IF($B$1=\"Deutsch\",D2375,IF($B$1=\"中文\",E2375,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: 4. April 2019\n- \nsunset date: 4. Oktober 2020"},"included in Annex 14\n- \nlast application date: 4. April 2019\n- \nsunset date: 4. Oktober 2020","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss: 4. April 2019\n- Ablauftermin: 4. Oktober 2020","包括在附录14\n-申请截止日期:2019年4月4日\n-过期:2020年10月4日"]
[null,{"$f":"IF($B$1=\"English\",C2376,IF($B$1=\"Deutsch\",D2376,IF($B$1=\"中文\",E2376,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CN-ELV (tab 17) GB/T30512-2014"},"CN-ELV (tab 17) GB/T30512-2014","CN-ELV (tab 17) GB/T30512-2014","CN-ELV (tab 17) GB/T30512-2014"]
[null,{"$f":"IF($B$1=\"English\",C2377,IF($B$1=\"Deutsch\",D2377,IF($B$1=\"中文\",E2377,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated substances"},"Regulated substances","Regulated substances","管制物质"]
[null,{"$f":"IF($B$1=\"English\",C2378,IF($B$1=\"Deutsch\",D2378,IF($B$1=\"中文\",E2378,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS number"},"CAS number","CAS number","CAS编号"]
[null,{"$f":"IF($B$1=\"English\",C2379,IF($B$1=\"Deutsch\",D2379,IF($B$1=\"中文\",E2379,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value [mass% in homogeneous material]"},"Limit value [mass% in homogeneous material]","Limit value [mass% in homogeneous material]","限值 [均质材料中的质量% ]"]
[null,{"$f":"IF($B$1=\"English\",C2380,IF($B$1=\"Deutsch\",D2380,IF($B$1=\"中文\",E2380,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of substance [mass% in homogeneous material]"},"Concentration of substance [mass% in homogeneous material]","Concentration of substance [mass% in homogeneous material]","物质含量 [均质材料中的质量%]"]
[null,{"$f":"IF($B$1=\"English\",C2381,IF($B$1=\"Deutsch\",D2381,IF($B$1=\"中文\",E2381,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Exception claimed? If so, which one?"},"Exception claimed? If so, which one?","Exception claimed? If so, which one?","是否可以豁免？如果可以，符合豁免清单中的哪一条?"]
[null,{"$f":"IF($B$1=\"English\",C2382,IF($B$1=\"Deutsch\",D2382,IF($B$1=\"中文\",E2382,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Designation of the material that contains the regulated substance"},"Designation of the material that contains the regulated substance","Designation of the material that contains the regulated substance","含有管制物质的材料名称"]
[null,{"$f":"IF($B$1=\"English\",C2383,IF($B$1=\"Deutsch\",D2383,IF($B$1=\"中文\",E2383,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included ( E )\n- changed ( C )"},"Entry\n- included ( E )\n- changed ( C )","Entry\n- included ( E )\n- changed ( C )","录入记录\n-首次录入(E)\n-更新(C)"]
[null,{"$f":"IF($B$1=\"English\",C2384,IF($B$1=\"Deutsch\",D2384,IF($B$1=\"中文\",E2384,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"test report enclosed (optional)"},"test report enclosed (optional)","test report enclosed (optional)","附测试报告（可选项）"]
[null,{"$f":"IF($B$1=\"English\",C2385,IF($B$1=\"Deutsch\",D2385,IF($B$1=\"中文\",E2385,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"method of measurement"},"method of measurement","method of measurement","检测方法"]
[null,{"$f":"IF($B$1=\"English\",C2386,IF($B$1=\"Deutsch\",D2386,IF($B$1=\"中文\",E2386,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibited substances (P)"},"Prohibited substances (P)","Prohibited substances (P)","禁用物质 (P)"]
[null,{"$f":"IF($B$1=\"English\",C2387,IF($B$1=\"Deutsch\",D2387,IF($B$1=\"中文\",E2387,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Lead","铅"]
[null,{"$f":"IF($B$1=\"English\",C2388,IF($B$1=\"Deutsch\",D2388,IF($B$1=\"中文\",E2388,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C2389,IF($B$1=\"Deutsch\",D2389,IF($B$1=\"中文\",E2389,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury"},"Mercury","Mercury","汞"]
[null,{"$f":"IF($B$1=\"English\",C2390,IF($B$1=\"Deutsch\",D2390,IF($B$1=\"中文\",E2390,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium VI"},"Chromium VI","Chromium VI","六价铬"]
[null,{"$f":"IF($B$1=\"English\",C2391,IF($B$1=\"Deutsch\",D2391,IF($B$1=\"中文\",E2391,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated biphenyles (PBB)"},"Polybrominated biphenyles (PBB)","Polybrominated biphenyles (PBB)","多溴联苯 (PBB)"]
[null,{"$f":"IF($B$1=\"English\",C2392,IF($B$1=\"Deutsch\",D2392,IF($B$1=\"中文\",E2392,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polybrominated diphenyl ether (PBDE)"},"Polybrominated diphenyl ether (PBDE)","Polybrominated diphenyl ether (PBDE)","多溴联苯醚 (PBDE)"]
[null,{"$f":"IF($B$1=\"English\",C2393,IF($B$1=\"Deutsch\",D2393,IF($B$1=\"中文\",E2393,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7439-92-1 and its compounds"},"7439-92-1 and its compounds","7439-92-1 and its compounds","7439-92-1和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2394,IF($B$1=\"Deutsch\",D2394,IF($B$1=\"中文\",E2394,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7440-43-9 and its compounds"},"7440-43-9 and its compounds","7440-43-9 and its compounds","7440-43-9和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2395,IF($B$1=\"Deutsch\",D2395,IF($B$1=\"中文\",E2395,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7439-97-6 and its compounds"},"7439-97-6 and its compounds","7439-97-6 and its compounds","7439-97-6和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2396,IF($B$1=\"Deutsch\",D2396,IF($B$1=\"中文\",E2396,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1333-82-0 and its compounds"},"1333-82-0 and its compounds","1333-82-0 and its compounds","1333-82-0和它的混合物"]
[null,{"$f":"IF($B$1=\"English\",C2397,IF($B$1=\"Deutsch\",D2397,IF($B$1=\"中文\",E2397,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material group"},"Material group","Material group","材料组 "]
[null,{"$f":"IF($B$1=\"English\",C2398,IF($B$1=\"Deutsch\",D2398,IF($B$1=\"中文\",E2398,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Material group"},"Material group","Material group","材料组 "]
[null,{"$f":"IF($B$1=\"English\",C2399,IF($B$1=\"Deutsch\",D2399,IF($B$1=\"中文\",E2399,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"List of Exemptions (2014) "},"List of Exemptions (2014) ","List of Exemptions (2014) ","豁免清单 (2014) "]
[null,{"$f":"IF($B$1=\"English\",C2400,IF($B$1=\"Deutsch\",D2400,IF($B$1=\"中文\",E2400,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"GB/T30512-2014 \nAnnex A\n Exemption of prohibited substances"},"GB/T30512-2014 \nAnnex A\n Exemption of prohibited substances","GB/T30512-2014 \nAnnex A\n Exemption of prohibited substances","GB/T30512-2014 \n附录A\n禁用物质的豁免"]
[null,{"$f":"IF($B$1=\"English\",C2401,IF($B$1=\"Deutsch\",D2401,IF($B$1=\"中文\",E2401,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Materials and components "},"Materials and components ","Materials and components ","材料及零部件"]
[null,{"$f":"IF($B$1=\"English\",C2402,IF($B$1=\"Deutsch\",D2402,IF($B$1=\"中文\",E2402,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Scope and expiry date of the exemption "}," Scope and expiry date of the exemption "," Scope and expiry date of the exemption ","豁免范围和期限"]
[null,{"$f":"IF($B$1=\"English\",C2403,IF($B$1=\"Deutsch\",D2403,IF($B$1=\"中文\",E2403,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead as an alloying element"},"Lead as an alloying element","Lead as an alloying element","合金铅"]
[null,{"$f":"IF($B$1=\"English\",C2404,IF($B$1=\"Deutsch\",D2404,IF($B$1=\"中文\",E2404,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Steel and galvanized steel for machining (Lead ≤0.35%)"},"1. Steel and galvanized steel for machining (Lead ≤0.35%)","1. Steel and galvanized steel for machining (Lead ≤0.35%)","1. 机械加工用钢材和镀锌钢（铅≤0.35%）"]
[null,{"$f":"IF($B$1=\"English\",C2405,IF($B$1=\"Deutsch\",D2405,IF($B$1=\"中文\",E2405,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2. Aluminum material (Lead≤0.4%)"},"2. Aluminum material (Lead≤0.4%)","2. Aluminum material (Lead≤0.4%)","2. 铝材（铅≤0.4%）"]
[null,{"$f":"IF($B$1=\"English\",C2406,IF($B$1=\"Deutsch\",D2406,IF($B$1=\"中文\",E2406,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3. Copper alloy (Lead ≤4%)"},"3. Copper alloy (Lead ≤4%)","3. Copper alloy (Lead ≤4%)","3. 铜合金（铅≤4%）"]
[null,{"$f":"IF($B$1=\"English\",C2407,IF($B$1=\"Deutsch\",D2407,IF($B$1=\"中文\",E2407,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4(a) Bearing bush and shaft sleeve "},"4(a) Bearing bush and shaft sleeve ","4(a) Bearing bush and shaft sleeve ","4(a). 轴瓦和轴套"]
[null,{"$f":"IF($B$1=\"English\",C2408,IF($B$1=\"Deutsch\",D2408,IF($B$1=\"中文\",E2408,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4(b) Bearing bush and shaft sleeve of engine, transmission and air conditioning compressor "},"4(b) Bearing bush and shaft sleeve of engine, transmission and air conditioning compressor ","4(b) Bearing bush and shaft sleeve of engine, transmission and air conditioning compressor ","4(b). 发动机、变速器和空调压缩机的轴瓦和轴套"]
[null,{"$f":"IF($B$1=\"English\",C2409,IF($B$1=\"Deutsch\",D2409,IF($B$1=\"中文\",E2409,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and lead compounds for parts"},"Lead and lead compounds for parts","Lead and lead compounds for parts","部件用铅和铅化合物"]
[null,{"$f":"IF($B$1=\"English\",C2410,IF($B$1=\"Deutsch\",D2410,IF($B$1=\"中文\",E2410,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5. Storage battery"},"5. Storage battery","5. Storage battery","5. 蓄电池"]
[null,{"$f":"IF($B$1=\"English\",C2411,IF($B$1=\"Deutsch\",D2411,IF($B$1=\"中文\",E2411,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"6. Damper"},"6. Damper","6. Damper","6. 减震器"]
[null,{"$f":"IF($B$1=\"English\",C2412,IF($B$1=\"Deutsch\",D2412,IF($B$1=\"中文\",E2412,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"7. Flexible brake hoses, fuel hoses, flexible ventilation ducting, elastomer / metal parts for chassis and elastomer sulfurizing reagent and stabilizer for engine mounting (Lead≤0.5%)"},"7. Flexible brake hoses, fuel hoses, flexible ventilation ducting, elastomer / metal parts for chassis and elastomer sulfurizing reagent and stabilizer for engine mounting (Lead≤0.5%)","7. Flexible brake hoses, fuel hoses, flexible ventilation ducting, elastomer / metal parts for chassis and elastomer sulfurizing reagent and stabilizer for engine mounting (Lead≤0.5%)","7. 制动软管、燃油软管、通风软管、底盘用弹性体/金属件以及发动机悬置用的弹性体硫化剂和稳定剂（铅≤0.5%）"]
[null,{"$f":"IF($B$1=\"English\",C2413,IF($B$1=\"Deutsch\",D2413,IF($B$1=\"中文\",E2413,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"8. Elastomeric adhesive on the power assembly (Lead ≤0.5%) "},"8. Elastomeric adhesive on the power assembly (Lead ≤0.5%) ","8. Elastomeric adhesive on the power assembly (Lead ≤0.5%) ","8. 动力总成上的弹性体粘合剂（铅≤0.5%）"]
[null,{"$f":"IF($B$1=\"English\",C2414,IF($B$1=\"Deutsch\",D2414,IF($B$1=\"中文\",E2414,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"9. Welding flux for circuit boards and other electric parts"},"9. Welding flux for circuit boards and other electric parts","9. Welding flux for circuit boards and other electric parts","9. 电路板及其他电气部件用焊料"]
[null,{"$f":"IF($B$1=\"English\",C2415,IF($B$1=\"Deutsch\",D2415,IF($B$1=\"中文\",E2415,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"10. Valve seat "},"10. Valve seat ","10. Valve seat ","10. 气门阀座"]
[null,{"$f":"IF($B$1=\"English\",C2416,IF($B$1=\"Deutsch\",D2416,IF($B$1=\"中文\",E2416,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"11. Electrical components with leaded glass or ceramic matrix composites except for bulb glass and enamel layer of sparking plug"},"11. Electrical components with leaded glass or ceramic matrix composites except for bulb glass and enamel layer of sparking plug","11. Electrical components with leaded glass or ceramic matrix composites except for bulb glass and enamel layer of sparking plug","11. 灯泡玻璃和火花塞釉层除外的具有含铅玻璃或陶瓷基复合材料的电气元件"]
[null,{"$f":"IF($B$1=\"English\",C2417,IF($B$1=\"Deutsch\",D2417,IF($B$1=\"中文\",E2417,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"12. Pyrotechnic primer "},"12. Pyrotechnic primer ","12. Pyrotechnic primer ","12. 烟火起爆剂"]
[null,{"$f":"IF($B$1=\"English\",C2418,IF($B$1=\"Deutsch\",D2418,IF($B$1=\"中文\",E2418,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"13. Lead-coated steel plate for automotive fuel tank "},"13. Lead-coated steel plate for automotive fuel tank ","13. Lead-coated steel plate for automotive fuel tank ","13. 汽车油箱用镀铅钢板"]
[null,{"$f":"IF($B$1=\"English\",C2419,IF($B$1=\"Deutsch\",D2419,IF($B$1=\"中文\",E2419,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"14. Wheel counterbalance "},"14. Wheel counterbalance ","14. Wheel counterbalance ","14. 车轮平衡块"]
[null,{"$f":"IF($B$1=\"English\",C2420,IF($B$1=\"Deutsch\",D2420,IF($B$1=\"中文\",E2420,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"15. Carbon brush for electric machine "},"15. Carbon brush for electric machine ","15. Carbon brush for electric machine ","15. 电机碳刷"]
[null,{"$f":"IF($B$1=\"English\",C2421,IF($B$1=\"Deutsch\",D2421,IF($B$1=\"中文\",E2421,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"16. Copper in the friction materials of brake lining (Lead ≤0.5%) "},"16. Copper in the friction materials of brake lining (Lead ≤0.5%) ","16. Copper in the friction materials of brake lining (Lead ≤0.5%) ","16. 制动衬片摩擦材料中的铜（铅≤0.5%）"]
[null,{"$f":"IF($B$1=\"English\",C2422,IF($B$1=\"Deutsch\",D2422,IF($B$1=\"中文\",E2422,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexavalent chromium"},"Hexavalent chromium","Hexavalent chromium","六价铬"]
[null,{"$f":"IF($B$1=\"English\",C2423,IF($B$1=\"Deutsch\",D2423,IF($B$1=\"中文\",E2423,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"17. Anticorrosive paint "},"17. Anticorrosive paint ","17. Anticorrosive paint ","17. 防腐涂料"]
[null,{"$f":"IF($B$1=\"English\",C2424,IF($B$1=\"Deutsch\",D2424,IF($B$1=\"中文\",E2424,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"18. Chassis is assembled with corrosion prevention coating of bolts and nuts and other parts "},"18. Chassis is assembled with corrosion prevention coating of bolts and nuts and other parts ","18. Chassis is assembled with corrosion prevention coating of bolts and nuts and other parts ","18. 底盘装配用螺栓螺母等零件的防腐镀层"]
[null,{"$f":"IF($B$1=\"English\",C2425,IF($B$1=\"Deutsch\",D2425,IF($B$1=\"中文\",E2425,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"19. Heat absorption air conditioning in motor caravan"},"19. Heat absorption air conditioning in motor caravan","19. Heat absorption air conditioning in motor caravan","19. 旅居车内的吸热式空调"]
[null,{"$f":"IF($B$1=\"English\",C2426,IF($B$1=\"Deutsch\",D2426,IF($B$1=\"中文\",E2426,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury"},"Mercury","Mercury","汞"]
[null,{"$f":"IF($B$1=\"English\",C2427,IF($B$1=\"Deutsch\",D2427,IF($B$1=\"中文\",E2427,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"20. Electric-discharge lamp for headlamp"},"20. Electric-discharge lamp for headlamp","20. Electric-discharge lamp for headlamp","20. 前照灯用放电灯"]
[null,{"$f":"IF($B$1=\"English\",C2428,IF($B$1=\"Deutsch\",D2428,IF($B$1=\"中文\",E2428,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"21. Fluorescent tube of instrument board display"},"21. Fluorescent tube of instrument board display","21. Fluorescent tube of instrument board display","21. 仪表板显示器荧光管"]
[null,{"$f":"IF($B$1=\"English\",C2429,IF($B$1=\"Deutsch\",D2429,IF($B$1=\"中文\",E2429,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C2430,IF($B$1=\"Deutsch\",D2430,IF($B$1=\"中文\",E2430,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"22. Battery for electric vehicle"},"22. Battery for electric vehicle","22. Battery for electric vehicle","22. 电动车辆用电池"]
[null,{"$f":"IF($B$1=\"English\",C2431,IF($B$1=\"Deutsch\",D2431,IF($B$1=\"中文\",E2431,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bromide flame-retardant"},"Bromide flame-retardant","Bromide flame-retardant","溴化阻燃剂"]
[null,{"$f":"IF($B$1=\"English\",C2432,IF($B$1=\"Deutsch\",D2432,IF($B$1=\"中文\",E2432,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"23. Decabromodiphenyl ether"},"23. Decabromodiphenyl ether","23. Decabromodiphenyl ether","23. 十溴联苯醚"]
[null,{"$f":"IF($B$1=\"English\",C2433,IF($B$1=\"Deutsch\",D2433,IF($B$1=\"中文\",E2433,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2434,IF($B$1=\"Deutsch\",D2434,IF($B$1=\"中文\",E2434,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42551},"2016-06-30","2016-06-30","2016年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2435,IF($B$1=\"Deutsch\",D2435,IF($B$1=\"中文\",E2435,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2436,IF($B$1=\"Deutsch\",D2436,IF($B$1=\"中文\",E2436,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2437,IF($B$1=\"Deutsch\",D2437,IF($B$1=\"中文\",E2437,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2438,IF($B$1=\"Deutsch\",D2438,IF($B$1=\"中文\",E2438,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2439,IF($B$1=\"Deutsch\",D2439,IF($B$1=\"中文\",E2439,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2440,IF($B$1=\"Deutsch\",D2440,IF($B$1=\"中文\",E2440,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":41820},"2014-06-30","2014-06-30","2014年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2441,IF($B$1=\"Deutsch\",D2441,IF($B$1=\"中文\",E2441,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":42185},"2015-06-30","2015-06-30","2015年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2442,IF($B$1=\"Deutsch\",D2442,IF($B$1=\"中文\",E2442,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":41820},"2014-06-30","2014-06-30","2014年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2443,IF($B$1=\"Deutsch\",D2443,IF($B$1=\"中文\",E2443,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":41820},"2014-06-30","2014-06-30","2014年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2444,IF($B$1=\"Deutsch\",D2444,IF($B$1=\"中文\",E2444,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":41820},"2014-06-30","2014-06-30","2014年6月30日"]
[null,{"$f":"IF($B$1=\"English\",C2445,IF($B$1=\"Deutsch\",D2445,IF($B$1=\"中文\",E2445,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"From the implementation date of this Standard, nickel-cadmium battery is only allowed to be the spare parts of those vehicles which have entered into the market before this date."},"From the implementation date of this Standard, nickel-cadmium battery is only allowed to be the spare parts of those vehicles which have entered into the market before this date.","From the implementation date of this Standard, nickel-cadmium battery is only allowed to be the spare parts of those vehicles which have entered into the market before this date.","本标准实施之日起，镍镉电池只允许作为该日期之前上市车辆的备件进入市场"]
[null,{"$f":"IF($B$1=\"English\",C2446,IF($B$1=\"Deutsch\",D2446,IF($B$1=\"中文\",E2446,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Note 1: The content limits in parentheses are all in mass percentage. \nNote 2: The exemption deadline in the table is that – for the new certificated models, the exemption deadline shall be postponed for 2 years, from the exemption deadline of producing automobiles."},"Note 1: The content limits in parentheses are all in mass percentage. \nNote 2: The exemption deadline in the table is that – for the new certificated models, the exemption deadline shall be postponed for 2 years, from the exemption deadline of producing automobiles.","Note 1: The content limits in parentheses are all in mass percentage. \nNote 2: The exemption deadline in the table is that – for the new certificated models, the exemption deadline shall be postponed for 2 years, from the exemption deadline of producing automobiles.","注： 1.括号中的含量限值均为质量百分数。 2.表中的豁免期限为新认证车型的豁免期限，在生产车的豁免期限顺延2年。"]
[null,{"$f":"IF($B$1=\"English\",C2447,IF($B$1=\"Deutsch\",D2447,IF($B$1=\"中文\",E2447,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C2448,IF($B$1=\"Deutsch\",D2448,IF($B$1=\"中文\",E2448,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Content of the delivered material. Exact designation of the material supplied (e.g. Battery, screw made of material xyz or cutting steel made of material 11SMN30, reference to IMDS ID, CDX material"},"Content of the delivered material. Exact designation of the material supplied (e.g. Battery, screw made of material xyz or cutting steel made of material 11SMN30, reference to IMDS ID, CDX material","Inhalt des gelieferten Materials. Genau Benennung des gelieferten Materials (z.B. Batterie, Schraube aus Werkstoff xyz oder Automatenstahl aus Werkstoff 11SMN30, Referenz zu IMDSID, CDX-Werkstoff)","交付材料的组成。供应的材料的确切名称（例如电池、由某某材料制成的螺钉或由11SMN30 材料制成的切割钢，参考 IMDS ID、CDX 材料）"]
[null,{"$f":"IF($B$1=\"English\",C2449,IF($B$1=\"Deutsch\",D2449,IF($B$1=\"中文\",E2449,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"[2]\nValid for vehicles type-approved from 1 October 2022 and spare parts for these vehicles"},"[2]\nValid for vehicles type-approved from 1 October 2022 and spare parts for these vehicles","[2]\nAb dem 1. Oktober 2022 typgenehmigte Fahrzeuge und Ersatzteile für diese Fahrzeuge","[2]\n适用于2022年10月1日起通过型式认证的车辆以及这些车辆的备件"]
[null,{"$f":"IF($B$1=\"English\",C2450,IF($B$1=\"Deutsch\",D2450,IF($B$1=\"中文\",E2450,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated Substances"},"Regulated Substances","Regulated Substances","管制物质"]
[null,{"$f":"IF($B$1=\"English\",C2451,IF($B$1=\"Deutsch\",D2451,IF($B$1=\"中文\",E2451,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS number"},"CAS number","CAS number","CAS 号码"]
[null,{"$f":"IF($B$1=\"English\",C2452,IF($B$1=\"Deutsch\",D2452,IF($B$1=\"中文\",E2452,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limits"},"Limits","Limits","限值标准"]
[null,{"$f":"IF($B$1=\"English\",C2453,IF($B$1=\"Deutsch\",D2453,IF($B$1=\"中文\",E2453,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration"},"Concentration","Concentration","含量"]
[null,{"$f":"IF($B$1=\"English\",C2454,IF($B$1=\"Deutsch\",D2454,IF($B$1=\"中文\",E2454,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Typical uses"},"Typical uses","Typical uses","典型使用"]
[null,{"$f":"IF($B$1=\"English\",C2455,IF($B$1=\"Deutsch\",D2455,IF($B$1=\"中文\",E2455,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included (E)\n- changed (C) \n"},"Entry\n- included (E)\n- changed (C) \n","Entry\n- included (E)\n- changed (C) \n","录入记录\n-首次录入(E)\n-更新(C)\n"]
[null,{"$f":"IF($B$1=\"English\",C2456,IF($B$1=\"Deutsch\",D2456,IF($B$1=\"中文\",E2456,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4,6-Tris(tert-butyl)phenol (2,4,6-TTBP)"},"2,4,6-Tris(tert-butyl)phenol (2,4,6-TTBP)","2,4,6-Tris(tert-butyl)phenol (2,4,6-TTBP)","2,4,6-三(叔丁基)苯酚(2,4,6-TTBP)"]
[null,{"$f":"IF($B$1=\"English\",C2457,IF($B$1=\"Deutsch\",D2457,IF($B$1=\"中文\",E2457,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decabromodiphenyl ether (DecaBDE)"},"Decabromodiphenyl ether (DecaBDE)","Decabromodiphenyl ether (DecaBDE)","十溴联苯(DecaBDE)"]
[null,{"$f":"IF($B$1=\"English\",C2458,IF($B$1=\"Deutsch\",D2458,IF($B$1=\"中文\",E2458,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, isopropylated phosphate (3:1) (PIP 3:1)"},"Phenol, isopropylated phosphate (3:1) (PIP 3:1)","Phenol, isopropylated phosphate (3:1) (PIP 3:1)","苯酚，异丙基磷酸酯 (3:1) (PIP 3:1)"]
[null,{"$f":"IF($B$1=\"English\",C2459,IF($B$1=\"Deutsch\",D2459,IF($B$1=\"中文\",E2459,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorothiophenol (PCTP)"},"Pentachlorothiophenol (PCTP)","Pentachlorothiophenol (PCTP)","五氯硫酚(PCTP)"]
[null,{"$f":"IF($B$1=\"English\",C2460,IF($B$1=\"Deutsch\",D2460,IF($B$1=\"中文\",E2460,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorobutadiene (HCBD)"},"Hexachlorobutadiene (HCBD)","Hexachlorobutadiene (HCBD)","六氯丁二烯 (HCBD)"]
[null,{"$f":"IF($B$1=\"English\",C2461,IF($B$1=\"Deutsch\",D2461,IF($B$1=\"中文\",E2461,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≤ 0.3% by weight"},"≤ 0.3% by weight","≤ 0.3% by weight","质量小于等于0.3%"]
[null,{"$f":"IF($B$1=\"English\",C2462,IF($B$1=\"Deutsch\",D2462,IF($B$1=\"中文\",E2462,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0 % by weight"},"0 % by weight","0 % by weight","质量0 % "]
[null,{"$f":"IF($B$1=\"English\",C2463,IF($B$1=\"Deutsch\",D2463,IF($B$1=\"中文\",E2463,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0 % by weight"},"0 % by weight","0 % by weight","质量0 %"]
[null,{"$f":"IF($B$1=\"English\",C2464,IF($B$1=\"Deutsch\",D2464,IF($B$1=\"中文\",E2464,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≤ 1% by weight"},"≤ 1% by weight","≤ 1% by weight","质量小于等于1%"]
[null,{"$f":"IF($B$1=\"English\",C2465,IF($B$1=\"Deutsch\",D2465,IF($B$1=\"中文\",E2465,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0 % by weight"},"0 % by weight","0 % by weight","质量0 % "]
[null,{"$f":"IF($B$1=\"English\",C2466,IF($B$1=\"Deutsch\",D2466,IF($B$1=\"中文\",E2466,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"an antioxidant in fuel additives and fuel injector cleaners as well as an additive in oil and lubricants"},"an antioxidant in fuel additives and fuel injector cleaners as well as an additive in oil and lubricants","an antioxidant in fuel additives and fuel injector cleaners as well as an additive in oil and lubricants","燃油添加剂和喷油器清洁剂中的抗氧化剂，以及机油和润滑剂中的添加剂"]
[null,{"$f":"IF($B$1=\"English\",C2467,IF($B$1=\"Deutsch\",D2467,IF($B$1=\"中文\",E2467,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a flame retardant with applications in wire and cable rubber casings, textiles, electronic equipment casings, building and construction materials, and imported articles such as aerospace and automotive parts"},"a flame retardant with applications in wire and cable rubber casings, textiles, electronic equipment casings, building and construction materials, and imported articles such as aerospace and automotive parts","a flame retardant with applications in wire and cable rubber casings, textiles, electronic equipment casings, building and construction materials, and imported articles such as aerospace and automotive parts","一种阻燃剂，应用于电线电缆橡胶外壳、纺织品、电子设备外壳、建筑材料以及航空航天和汽车零部件等进口产品"]
[null,{"$f":"IF($B$1=\"English\",C2468,IF($B$1=\"Deutsch\",D2468,IF($B$1=\"中文\",E2468,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a flame retardant in plastics and as a functional fluid in aircraft and industrial machinery"},"a flame retardant in plastics and as a functional fluid in aircraft and industrial machinery","a flame retardant in plastics and as a functional fluid in aircraft and industrial machinery","塑料中的阻燃剂，用作飞机和工业机械中的功能流体"]
[null,{"$f":"IF($B$1=\"English\",C2469,IF($B$1=\"Deutsch\",D2469,IF($B$1=\"中文\",E2469,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" a substance with applications in the rubber industry"}," a substance with applications in the rubber industry"," a substance with applications in the rubber industry","一种应用在橡胶工业中的物质"]
[null,{"$f":"IF($B$1=\"English\",C2470,IF($B$1=\"Deutsch\",D2470,IF($B$1=\"中文\",E2470,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a solvent in rubber manufacturing and in hydraulic, heat transfer or transformer fluid"},"a solvent in rubber manufacturing and in hydraulic, heat transfer or transformer fluid","a solvent in rubber manufacturing and in hydraulic, heat transfer or transformer fluid","橡胶制造和液压、传热或变压器流体中的溶剂"]
[null,{"$f":"IF($B$1=\"English\",C2471,IF($B$1=\"Deutsch\",D2471,IF($B$1=\"中文\",E2471,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 17"},"included in Annex 17","aufgenommen in Anhang 17","包括在附录17"]
[null,{"$f":"IF($B$1=\"English\",C2472,IF($B$1=\"Deutsch\",D2472,IF($B$1=\"中文\",E2472,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: \n21. Oktober 2014\n- \nsunset date:  \n21. April 2016"},"included in Annex 14\n- \nlast application date: \n21. Oktober 2014\n- \nsunset date:  \n21. April 2016","aufgenommen in Anhang 14\n- Antragsschluss: \n21. Oktober 2014\n\n- Ablauftermin: \n21. April 2016","包括在附录14\n-申请截止日期:2014年10月21日\n-过期: 2016年4月21日"]
[null,{"$f":"IF($B$1=\"English\",C2473,IF($B$1=\"Deutsch\",D2473,IF($B$1=\"中文\",E2473,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: \n21. März 2016\n- \nsunset date:  \n21. September 2017"},"included in Annex 14\n- \nlast application date: \n21. März 2016\n- \nsunset date:  \n21. September 2017","aufgenommen in Anhang 14\n- Antragsschluss: \n21. März 2016\n\n- Ablauftermin: \n 21. September 2017","包括在附录14\n-申请截止日期:2016年3月21日\n-过期: 2017年9月21日"]
[null,{"$f":"IF($B$1=\"English\",C2474,IF($B$1=\"Deutsch\",D2474,IF($B$1=\"中文\",E2474,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nlast application date: 22. Juli 2017 \n- \nsunset date: 22. Januar 2019"},"included in Annex 14\n- \nlast application date: 22. Juli 2017 \n- \nsunset date: 22. Januar 2019","aufgenommen in Anhang 14\n- Antragsschluss: \n22. Juli 2017 \n- Ablauftermin: \n22. Januar 2019","包括在附录14\n-申请截止日期:  2017 年7月22日\n-过期: 2019年1月22日"]
[null,{"$f":"IF($B$1=\"English\",C2475,IF($B$1=\"Deutsch\",D2475,IF($B$1=\"中文\",E2475,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020","aufgenommen in Anhang 14\n- Antragsschluss: \n4. Januar 2019\n- Ablauftermin: \n4. Juli 2020","包括在附录14\n-申请截止日期:2019年1月4日\n-过期: 2020年7月4日"]
[null,{"$f":"IF($B$1=\"English\",C2476,IF($B$1=\"Deutsch\",D2476,IF($B$1=\"中文\",E2476,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017"},"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss: \n22. Februar 2016\n\n- Ablauftermin: \n22. August 2017","包括在附录14和17\n-申请截止日期：2016年2月22日\n-过期: 2017年8月22日"]
[null,{"$f":"IF($B$1=\"English\",C2477,IF($B$1=\"Deutsch\",D2477,IF($B$1=\"中文\",E2477,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Juli 2017\n- \nsunset date: 22. Januar 2019"},"included in Annex 14 and Annex 17\n- \nlast application date: 22. Juli 2017\n- \nsunset date: 22. Januar 2019","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss:  \n22. Juli 2017              \n- Ablauftermin: \n22. Januar 2019","包括在附录14和17\n-申请截止日期：2017年7月22日\n-过期: 2019年1月22日"]
[null,{"$f":"IF($B$1=\"English\",C2478,IF($B$1=\"Deutsch\",D2478,IF($B$1=\"中文\",E2478,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Juli 2017\n- \nsunset date: 22. Januar 2019"},"included in Annex 14 and Annex 17\n- \nlast application date: 22. Juli 2017\n- \nsunset date: 22. Januar 2019","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss: \n22. Juli 2017\n- Ablauftermin: \n22. Januar 2019","包括在附录14和17\n-申请截止日期：2017年7月22日\n-过期: 2019年1月22日"]
[null,{"$f":"IF($B$1=\"English\",C2479,IF($B$1=\"Deutsch\",D2479,IF($B$1=\"中文\",E2479,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017"},"included in Annex 14 and Annex 17\n- \nlast application date: 22. Februar 2016\n- \nsunset date: 22. August 2017","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss: 22. Februar 2016*\n- Ablauftermin: 22. August 2017**","包括在附录14和17\n-申请截止日期：2016年2月22日\n-过期: 2017年8月22日"]
[null,{"$f":"IF($B$1=\"English\",C2480,IF($B$1=\"Deutsch\",D2480,IF($B$1=\"中文\",E2480,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date: 22. Mai 2016\n- \nsunset date:  22. November 2017"},"included in Annex 14 and Annex 17\n- \nlast application date: 22. Mai 2016\n- \nsunset date:  22. November 2017","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss: \n22. Mai 2016\n\n- Ablauftermin:  \n22. November 2017","包括在附录14和17\n-申请截止日期：2016年2月22日\n-过期: 2017年8月22日"]
[null,{"$f":"IF($B$1=\"English\",C2481,IF($B$1=\"Deutsch\",D2481,IF($B$1=\"中文\",E2481,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14\n- \nLast application date: 4. Juli 2019\n-\nsunset date: 4. Januar 2021"},"included in Annex 14\n- \nLast application date: 4. Juli 2019\n-\nsunset date: 4. Januar 2021","aufgenommen in Anhang 14\n- Antragsschluss: \n4. Juli 2019\n- Ablauftermin: \n4. Januar 2021","包括在附录14\n-申请截止日期：2019年7月4日\n-过期: 2021年1月4日"]
[null,{"$f":"IF($B$1=\"English\",C2482,IF($B$1=\"Deutsch\",D2482,IF($B$1=\"中文\",E2482,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020"},"included in Annex 14 \n- \nlast application date: 4. Januar 2019\n- \nsunset date: 4. Juli 2020","aufgenommen in Anhang 14\n- Antragsschluss: 4. Januar 2019\n- Ablauftermin: 4. Juli 2020","包括在附录14\n-申请截止日期：2019年1月4日\n-过期: 2020年7月4日"]
[null,{"$f":"IF($B$1=\"English\",C2483,IF($B$1=\"Deutsch\",D2483,IF($B$1=\"中文\",E2483,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nLast application date: 04. Juli 2019\n- \nsunset date: 04. Januar 2021\n\n"},"included in Annex 14 and Annex 17\n- \nLast application date: 04. Juli 2019\n- \nsunset date: 04. Januar 2021\n\n","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss: \n04. Juli 2019\n- Ablauftermin: \n04. Januar 2021\n\n","包括在附录14和17\n-申请截止日期：2019年7月4日\n-过期: 2021年1月4日\n\n"]
[null,{"$f":"IF($B$1=\"English\",C2484,IF($B$1=\"Deutsch\",D2484,IF($B$1=\"中文\",E2484,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\nSunset date: 27.05.2023"},"Included in Annex 14\n\n- Last application date: 27.11.2021\nSunset date: 27.05.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.11.2021\n- Ablauftermin: \n27.05.2023","包括在附录14\n\n- 申请截止日期：2021年11月27日\n- 过期: 2023年5月27日"]
[null,{"$f":"IF($B$1=\"English\",C2485,IF($B$1=\"Deutsch\",D2485,IF($B$1=\"中文\",E2485,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n- Sunset date: 27.02.2023"},"Included in Annex 14\n\n- Last application date: 27.08.2021\n- Sunset date: 27.02.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.08.2021\n- Ablauftermin: \n27.02.2023","包括在附录14\n\n- 申请截止日期：2021年8月27日\n- 过期: 2023年2月27日"]
[null,{"$f":"IF($B$1=\"English\",C2486,IF($B$1=\"Deutsch\",D2486,IF($B$1=\"中文\",E2486,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023"},"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.11.2021\n- Ablauftermin: \n27.05.2023","包括在附录14\n\n- 申请截止日期：2021年11月27日\n- 过期: 2023年5月27日"]
[null,{"$f":"IF($B$1=\"English\",C2487,IF($B$1=\"Deutsch\",D2487,IF($B$1=\"中文\",E2487,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023"},"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.08.2021\n- Ablauftermin: \n27.02.2023","包括在附录14\n\n- 申请截止日期：2021年8月27日\n- 过期: 2023年2月27日"]
[null,{"$f":"IF($B$1=\"English\",C2488,IF($B$1=\"Deutsch\",D2488,IF($B$1=\"中文\",E2488,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.05.2022\n- Ablauftermin: \n27.11.2023","包括在附录14\n\n- 申请截止日期：2022年5月27日\n- 过期: 2023年11月27日"]
[null,{"$f":"IF($B$1=\"English\",C2489,IF($B$1=\"Deutsch\",D2489,IF($B$1=\"中文\",E2489,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.02.2022\n- Sunset date: 27.08.2023"},"Included in Annex 14\n\n- Last application date: 27.02.2022\n- Sunset date: 27.08.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.02.2022\n- Ablauftermin: \n27.08.2023","包括在附录14\n\n- 申请截止日期：2022年2月27日\n- 过期: 2023年8月27日"]
[null,{"$f":"IF($B$1=\"English\",C2490,IF($B$1=\"Deutsch\",D2490,IF($B$1=\"中文\",E2490,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Triethyl arsenate is used, among other things, in semiconductor production."},"Triethyl arsenate is used, among other things, in semiconductor production.","Triethylarsenat wird unter anderem in der Halbleiterherstellung verwendet.","砷酸三乙酯用于半导体生产等。"]
[null,{"$f":"IF($B$1=\"English\",C2491,IF($B$1=\"Deutsch\",D2491,IF($B$1=\"中文\",E2491,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Applications for sodium dichromates include the production of vitamin K, colour stains (wood preservatives), the production of essential oils and perfumes, the production of coloured glass and ceramic glazes, the production of other chromium compounds, the production of inorganic chromate pigments and anti-corrosion coatings for metals. "},"Applications for sodium dichromates include the production of vitamin K, colour stains (wood preservatives), the production of essential oils and perfumes, the production of coloured glass and ceramic glazes, the production of other chromium compounds, the production of inorganic chromate pigments and anti-corrosion coatings for metals. ","Zu den Verwendungsgebieten der Natriumdichromate zählen die Vitamin-K-Herstellung, Farbbeize (Holzschutz), die Herstellung von ätherischen Ölen und Parfümen, die Herstellung von farbigem Glas und Keramikglasuren, die Herstellung anderer Chromverbindungen, die Herstellung anorganischer Chromatpigmente sowie Antikorrosionsbeschichtungen für Metalle. ","重铬酸钠的应用包括生产维生素K、着色剂(木材防腐剂)、生产精油和香水、生产彩色玻璃和陶瓷釉、生产其他铬化合物、生产无机铬酸盐颜料和金属防腐涂层。"]
[null,{"$f":"IF($B$1=\"English\",C2492,IF($B$1=\"Deutsch\",D2492,IF($B$1=\"中文\",E2492,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diarsenic Pentaoxide is used as a decolorizing agent for glass and enamel, as a refining and oxidizing agent in the production of special glass and lead crystal, as a starting material for elemental arsenic, arsenic alloys and arsenic-containing semiconductors and as a cytostatic agent. The material is also used in metallurgical investigations. "},"Diarsenic Pentaoxide is used as a decolorizing agent for glass and enamel, as a refining and oxidizing agent in the production of special glass and lead crystal, as a starting material for elemental arsenic, arsenic alloys and arsenic-containing semiconductors and as a cytostatic agent. The material is also used in metallurgical investigations. ","  Diarsentrioxid wird als Entfärbungsmittel für Glas und Emaille, als Raffinations- und Oxidierungsmittel bei der Herstellung von Spezialglas und Bleikristall, als Ausgangsmaterial für elementares Arsen, Arsenlegierungen und arsenhaltige Halbleiter und als Zytostatikum verwendet. Außerdem wird der Stoff in metallurgischen Untersuchungen verwendet. ","二砷五氧化物用作玻璃和搪瓷的脱色剂，在生产特殊玻璃和铅晶体时用作精炼剂和氧化剂，用作元素砷、砷合金和含砷半导体的原料和细胞生长抑制剂。这种材料也用于冶金研究。"]
[null,{"$f":"IF($B$1=\"English\",C2493,IF($B$1=\"Deutsch\",D2493,IF($B$1=\"中文\",E2493,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diarsene trioxide is used as a decolorizing agent for glass and enamel, as a refining and oxidizing agent in the production of special glass and lead crystal, as a starting material for elemental arsenic, arsenic alloys and arsenic-containing semiconductors and as a cytostatic agent. The material is also used in metallurgical investigations. "},"Diarsene trioxide is used as a decolorizing agent for glass and enamel, as a refining and oxidizing agent in the production of special glass and lead crystal, as a starting material for elemental arsenic, arsenic alloys and arsenic-containing semiconductors and as a cytostatic agent. The material is also used in metallurgical investigations. ","  Diarsentrioxid wird als Entfärbungsmittel für Glas und Emaille, als Raffinations- und Oxidierungsmittel bei der Herstellung von Spezialglas und Bleikristall, als Ausgangsmaterial für elementares Arsen, Arsenlegierungen und arsenhaltige Halbleiter und als Zytostatikum verwendet. Außerdem wird der Stoff in metallurgischen Untersuchungen verwendet. ","三氧化二砷被用作玻璃和搪瓷的脱色剂，生产特殊玻璃和铅晶体时用作精炼剂和氧化剂，用作元素砷、砷合金和含砷半导体的原料以及细胞生长抑制剂。这种材料也用于冶金研究。"]
[null,{"$f":"IF($B$1=\"English\",C2494,IF($B$1=\"Deutsch\",D2494,IF($B$1=\"中文\",E2494,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutyl phthalate is used in cosmetic products (e.g. nail polish), in adhesives, in cellophane packaging for food and in children's toys."},"Dibutyl phthalate is used in cosmetic products (e.g. nail polish), in adhesives, in cellophane packaging for food and in children's toys.","Dibutylphthalat wird in Kosmetikprodukten (z. B. Nagellack), in Klebstoff, in Zellophanverpackungen für Nahrungsmittel und in Kinderspielzeug verwendet.","邻苯二甲酸二丁酯用于化妆品(如指甲油)、粘合剂、食品玻璃纸包装和儿童玩具。"]
[null,{"$f":"IF($B$1=\"English\",C2495,IF($B$1=\"Deutsch\",D2495,IF($B$1=\"中文\",E2495,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(tributyltin) oxide is used in antimicrobial products such as special paints, special coatings, polyurethane foams, upholstered furniture, down or special textiles. "},"Bis(tributyltin) oxide is used in antimicrobial products such as special paints, special coatings, polyurethane foams, upholstered furniture, down or special textiles. ","  Bis(tributylzinn)oxid wird unter anderem in antimikrobiellen Produkten wie Spezialfarben, Spezialbeschichtungen, Polyurethan-Schäumen, Polstermöbeln, Daunen oder Spezialtextilien eingesetzt. ","二(三丁基锡)氧化物用于抗菌产品，如特殊油漆、特殊涂料、聚氨酯泡沫、装饰家具、羽绒或特殊纺织品。"]
[null,{"$f":"IF($B$1=\"English\",C2496,IF($B$1=\"Deutsch\",D2496,IF($B$1=\"中文\",E2496,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead hydrogen arsenate has been used as a biocide in the past. Today, the material is used in the production of glass, plastic products, lead batteries, electrical appliances, paints, mortars, electronic products, fertilizers, cosmetics and textiles. "},"Lead hydrogen arsenate has been used as a biocide in the past. Today, the material is used in the production of glass, plastic products, lead batteries, electrical appliances, paints, mortars, electronic products, fertilizers, cosmetics and textiles. ","  Bleihydrogenarsenat wurde in der Vergangenheit als Biozid verwendet. Heute findet man den Stoff bei der Herstellung von Glas, in Kunststoffprodukten, in Bleiakkus, in Elektrogeräten, in Farben, in Mörtel, in Elektronikprodukten, in Düngemitteln sowie in Kosmetikprodukten und in Textilien. ","砷酸氢铅过去用作生物杀灭剂。如今，这种材料被用于生产玻璃、塑料制品、铅电池、电器、油漆、砂浆、电子产品、肥料、化妆品和纺织品。"]
[null,{"$f":"IF($B$1=\"English\",C2497,IF($B$1=\"Deutsch\",D2497,IF($B$1=\"中文\",E2497,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The use of anthracene in the EU is restricted to the manufacture of pyrotechnic and pharmaceutical products and to its use for research purposes. "},"The use of anthracene in the EU is restricted to the manufacture of pyrotechnic and pharmaceutical products and to its use for research purposes. ","  Die Verwendung von Anthracen ist in der EU beschränkt auf die Herstellung von pyrotechnischen Erzeugnissen und pharmazeutischen Produkten sowie auf die Verwendung für Forschungszwecke. ","蒽在欧盟的使用仅限于烟火和医药产品的制造及其研究目的。"]
[null,{"$f":"IF($B$1=\"English\",C2498,IF($B$1=\"Deutsch\",D2498,IF($B$1=\"中文\",E2498,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzyl butyl phthalate is used as a plasticizer for PVC and other polymers to improve extensibility and mobility. It is used for floor coverings, but also for sealants, adhesives, paints, coatings and inks. Consumer products such as sealants, adhesives, car care products, food packaging materials and cosmetics may contain benzyl butyl phthalate. "},"Benzyl butyl phthalate is used as a plasticizer for PVC and other polymers to improve extensibility and mobility. It is used for floor coverings, but also for sealants, adhesives, paints, coatings and inks. Consumer products such as sealants, adhesives, car care products, food packaging materials and cosmetics may contain benzyl butyl phthalate. ","Benzylbutylphthalat wird als Weichmacher für PVC und andere Polymere zur Verbesserung von Dehnbarkeit und Beweglichkeit verwendet. Es wird für Bodenbeläge, aber auch für Dichtungsmittel, Kleber, Farben, Beschichtungen und Tinten verwendet. Verbraucherprodukte wie Dichtungsmittel, Kleber, Autopflegeprodukte, Verpackungsmaterial für Lebensmittel und Kosmetika können Benzylbutylphthalat enthalten. ","邻苯二甲酸苄丁酯被用作聚氯乙烯和其他聚合物的增塑剂，以提高延展性和流动性。它用于地板覆盖物，也用于密封剂、粘合剂、油漆、涂料和油墨。密封剂、粘合剂、汽车护理产品、食品包装材料和化妆品等消费品可能含有邻苯二甲酸苄丁酯。"]
[null,{"$f":"IF($B$1=\"English\",C2499,IF($B$1=\"Deutsch\",D2499,IF($B$1=\"中文\",E2499,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"MDA is used as an amine component in two-component systems."},"MDA is used as an amine component in two-component systems.","MDA wird unter anderem als Amin-Komponente in Zweikomponentensystemen eingesetzt. ","在双组分体系中，丙二醛（MDA）被用作胺组分。"]
[null,{"$f":"IF($B$1=\"English\",C2500,IF($B$1=\"Deutsch\",D2500,IF($B$1=\"中文\",E2500,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Musk xylene is used in cosmetic products and detergents as a fragrance or scent enhancer. "},"Musk xylene is used in cosmetic products and detergents as a fragrance or scent enhancer. ","Xylolmoschus findet in Kosmetikprodukten und Waschmitteln als Duftstoff beziehungsweise Duftverstärker Verwendung. ","二甲苯麝香用于化妆品和洗涤剂中，作为香味或气味增强剂。"]
[null,{"$f":"IF($B$1=\"English\",C2501,IF($B$1=\"Deutsch\",D2501,IF($B$1=\"中文\",E2501,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C10-13, chloro are used in the production of rubber products, textile coatings, sealants, adhesives and paints."},"Alkanes, C10-13, chloro are used in the production of rubber products, textile coatings, sealants, adhesives and paints.","Kurzkettige Chlorparaffine werden für die Herstellung von Gummierzeugnissen, Beschichtungen von Textilien, Dichtungsmittel, Kleber und Farben verwendet. ","C10-13氯代烷烃用于生产橡胶产品、纺织涂料、密封剂、 粘合剂和油漆。"]
[null,{"$f":"IF($B$1=\"English\",C2502,IF($B$1=\"Deutsch\",D2502,IF($B$1=\"中文\",E2502,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromocyclodododecane is used in the production of styrene-containing polymers and in the textile industry due to its flame-retardant properties. These flame-retardant polymers are mainly used as insulating material, packaging material and in electrical appliances. Textiles coated with HBCDD can be found, for example, in car interiors, mattresses, upholstered furniture, curtains, roller blinds and wallpaper."},"Hexabromocyclodododecane is used in the production of styrene-containing polymers and in the textile industry due to its flame-retardant properties. These flame-retardant polymers are mainly used as insulating material, packaging material and in electrical appliances. Textiles coated with HBCDD can be found, for example, in car interiors, mattresses, upholstered furniture, curtains, roller blinds and wallpaper.","Hexabromcyclododecan wird wegen seiner flammenhemmenden Eigenschaften bei der Herstellung von styrolhaltigen Polymeren und in der Textilindustrie eingesetzt. Die schwerentflammbaren Polymere finden vor allem als Dämmstoff, als Verpackungsmaterial und in Elektrogeräten Verwendung. Mit HBCDD beschichtete Textilien findet man unter anderem als Autoinnenverkleidung sowie in Matratzen, Polstermöbeln, Vorhängen, Rollos und Tapeten.","六溴环十二烷由于其阻燃特性，被用于生产含苯乙烯的聚合物和纺织工业。这些阻燃聚合物主要用作绝缘材料、包装材料和电器产品。涂有六溴环十二烷的纺织品可用于汽车内饰、床垫、装饰家具、窗帘、卷帘和墙纸。"]
[null,{"$f":"IF($B$1=\"English\",C2503,IF($B$1=\"Deutsch\",D2503,IF($B$1=\"中文\",E2503,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(2-chloroethyl)phosphate is mainly used as a softener additive and viscosity regulator with flame retardant properties for acrylic resins, polyurethane, polyvinyl chloride and other polymers. Other applications include adhesives, coatings, fire resistant paints and lacquers. The main industries using TCEP are the furniture, textile and construction industries."},"Tris(2-chloroethyl)phosphate is mainly used as a softener additive and viscosity regulator with flame retardant properties for acrylic resins, polyurethane, polyvinyl chloride and other polymers. Other applications include adhesives, coatings, fire resistant paints and lacquers. The main industries using TCEP are the furniture, textile and construction industries.","Tris(2-chloroethyl)phosphat wird hauptsächlich als ein Weichmittelzusatz und Viskositätsregler mit flammhemmenden Eigenschaften für Acrylharze, Polyurethan, Polyvinylchlorid und andere Polymere verwendet. Andere Anwendungsbereiche sind Klebemittel, Beschichtungen, feuerbeständige Farben und Lacke. Die Industriezweige, die TCEP hauptsächlich verwenden, sind die Möbel-, Textil- und Bauindustrie.","磷酸三(2-氯乙基)酯主要用作丙烯酸树脂、聚氨酯、聚氯乙烯等 聚合物的软化剂添加剂和具有阻燃性能的粘度调节剂。其他应用包括粘合剂、涂料、防火涂料和清漆。使用TCEP的主要工业是家具、纺织和建筑工业。"]
[null,{"$f":"IF($B$1=\"English\",C2504,IF($B$1=\"Deutsch\",D2504,IF($B$1=\"中文\",E2504,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Coal tar pitch, high temperature is mainly used in the production of electrodes for industrial applications. Smaller quantities are intended for specific applications such as high performance corrosion protection, special purpose paving, production of other materials and the production of clay targets."},"Coal tar pitch, high temperature is mainly used in the production of electrodes for industrial applications. Smaller quantities are intended for specific applications such as high performance corrosion protection, special purpose paving, production of other materials and the production of clay targets.","Pech, Kohlenteer, Hochtemperatur wird hauptsächlich bei der Produktion von Elektroden für industrielle Anwendungen verwendet. Geringere Mengen sind bestimmt für spezifische Verwendungen wie beispielsweise als ein Hochleistungskorrosionsschutz, spezielle Zweckpflasterung, Herstellung von anderen Stoffen und die Produktion von Tontargets.","煤焦油沥青，高温主要用于生产工业应用的电极。少量用于特殊应用，如高性能防腐、特殊用途铺路、生产其他材料和生产粘土靶。"]
[null,{"$f":"IF($B$1=\"English\",C2505,IF($B$1=\"Deutsch\",D2505,IF($B$1=\"中文\",E2505,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisobutyl phthalate is used both as a plasticizer for cellulose nitrate, cellulose ether, polyacrylate and polyacetate dispersions and as a gelling aid in combination with other plasticizers. Diisobutyl phthalate-containing polymers are used for plastics, paints, adhesives, explosives and nail polishes."},"Diisobutyl phthalate is used both as a plasticizer for cellulose nitrate, cellulose ether, polyacrylate and polyacetate dispersions and as a gelling aid in combination with other plasticizers. Diisobutyl phthalate-containing polymers are used for plastics, paints, adhesives, explosives and nail polishes.","Diisobutylphthalat wird sowohl als Weichmacher für Cellulosenitrat, Celluloseether, Polyacrylat und Polyacetatdispersionen verwendet, als auch als eine Gelierhilfe in der Kombination mit anderen Weichmachern. Diisobutylphthalat-haltige Polymere werden für Kunststoffe, Lacke, Kleber, Explosivstoffe und Nagelpoliermittel verwendet. ","邻苯二甲酸二异丁酯既可用作硝酸纤维素、纤维素醚、聚丙烯酸酯和聚乙酸酯分散体的增塑剂，也可与其他增塑剂结合用作胶凝助剂。含邻苯二甲酸二异丁酯的聚合物用于塑料、油漆、粘合剂、炸药和指甲油。"]
[null,{"$f":"IF($B$1=\"English\",C2506,IF($B$1=\"Deutsch\",D2506,IF($B$1=\"中文\",E2506,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead sulphochromate yellow (Colour Index Pigment Yellow 34) is used as a colouring, painting and coating material in industries such as the rubber, plastics and paint, coating and lacquer industry. Applications include the production of agricultural equipment, vehicles and aircraft as well as painting roads and take-off and landing strips. "},"Lead sulphochromate yellow (Colour Index Pigment Yellow 34) is used as a colouring, painting and coating material in industries such as the rubber, plastics and paint, coating and lacquer industry. Applications include the production of agricultural equipment, vehicles and aircraft as well as painting roads and take-off and landing strips. ","Bleisulfochromatgelb (Colour Index Pigment Gelb 34) wird verwendet als ein Färbe-, Anstrich- und Beschichtungsstoff in Branchen wie der Gummi-, Kunststoff- und Farben-, Beschichtungs- und Lackindustrie. Die Anwendungen umfassen die Produktion von landwirtschaftlichen Geräten, Fahrzeugen und Flugzeugen sowie das Anstreichen von Straßen und Start- und Landestreifen. ","硫化铅黄(颜色指数颜料黄34)在橡胶、塑料和油漆、涂料和漆工业中用作着色、涂漆和涂层材料。应用领域包括农业设备、车辆和飞机的生产，以及道路和起降跑道的涂装。"]
[null,{"$f":"IF($B$1=\"English\",C2507,IF($B$1=\"Deutsch\",D2507,IF($B$1=\"中文\",E2507,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead chromate is used for the production of pigments and dyes, as a pigmenting or coating material in industrial and marine paint products or for the embalming/reproduction of artificial products. Other potential uses include cleaning and bleaching agents, light-sensitive materials and for the production of pyrotechnic powders. "},"Lead chromate is used for the production of pigments and dyes, as a pigmenting or coating material in industrial and marine paint products or for the embalming/reproduction of artificial products. Other potential uses include cleaning and bleaching agents, light-sensitive materials and for the production of pyrotechnic powders. ","Bleichromat wird für die Herstellung von Pigmenten und Farbstoffen verwendet, als ein Pigmentier- oder Beschichtungsstoff in industriellen und maritimen Anstreichprodukten oder für die Einbalsamierung/Wiederherstellung von Kunstprodukten. Weitere potenzielle Verwendungen umfassen die Verwendung als Reinigungs- und Bleichmittel, lichtempfindliche Materialien und für die Herstellung von pyrotechnischem Pulver. ","铬酸铅用于生产颜料和染料，在工业和海洋涂料产品中作为颜料或涂层材料，或用于人造产品的防腐/复制。其他潜在用途包括清洁剂和漂白剂、光敏材料以及烟火粉末的生产。"]
[null,{"$f":"IF($B$1=\"English\",C2508,IF($B$1=\"Deutsch\",D2508,IF($B$1=\"中文\",E2508,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead chromate molybdate sulphate red (Colour Index Pigment Red 104) is used as a dye, paint and coating material in industries such as the rubber, plastics and paint, coating and lacquer industry. Applications include the production of agricultural equipment, vehicles and aircraft as well as painting roads and take-off and landing strips. "},"Lead chromate molybdate sulphate red (Colour Index Pigment Red 104) is used as a dye, paint and coating material in industries such as the rubber, plastics and paint, coating and lacquer industry. Applications include the production of agricultural equipment, vehicles and aircraft as well as painting roads and take-off and landing strips. ","Bleichromatmolybdatsulfatrot (Colour Index Pigment Rot 104) wird verwendet als Färbe-, Anstrich- und Beschichtungsstoff in Branchen wie der Gummi-, Kunststoff- und Farben-, Beschichtungs- und Lackindustrie. Die Anwendungen umfassen die Produktion von landwirtschaftlichen Geräten, Fahrzeugen und Flugzeugen sowie das Anstreichen von Straßen und Start- und Landestreifen. ","铬酸铅钼酸盐硫酸盐红(颜色指数颜料红104)在橡胶、塑料和油漆、涂料和漆工业中用作染料、油漆和涂料材料。应用领域包括农业设备、车辆和飞机的生产，以及道路和起降跑道的涂装。"]
[null,{"$f":"IF($B$1=\"English\",C2509,IF($B$1=\"Deutsch\",D2509,IF($B$1=\"中文\",E2509,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4-dinitrotoluene is used in the production of toluene diisocyanate, which is used in the manufacture of flexible polyurethane foams. The material is also used as a gelling plasticizer for the production of explosive mixtures (e.g. airbags in cars)."},"2,4-dinitrotoluene is used in the production of toluene diisocyanate, which is used in the manufacture of flexible polyurethane foams. The material is also used as a gelling plasticizer for the production of explosive mixtures (e.g. airbags in cars).","2,4-Dinitrotoluol wird bei der Produktion von Toluendiisocyanat verwendet, das für die Herstellung von flexiblen Polyurethanschäumen eingesetzt wird. Der Stoff wird ebenfalls verwendet als Gelier-Plastifizierungsmittel für die Herstellung von Sprengstoffgemischen (z. B. Airbags in Autos). ","2，4-二硝基甲苯用于生产甲苯二异氰酸酯，甲苯二异氰酸酯用于制造软质聚氨酯泡沫。该材料还被用作生产爆炸性混合物(如汽车安全气囊)的胶凝增塑剂。"]
[null,{"$f":"IF($B$1=\"English\",C2510,IF($B$1=\"Deutsch\",D2510,IF($B$1=\"中文\",E2510,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection.","Anthracenöle werden hauptsächlich bei der Herstellung von anderen Stoffen wie beispielsweise Anthracen und Carbon-Black verwendet. Sie können auch als Reduktionsmittel in Hochöfen, als Komponenten in Bunkeröl, zur Imprägnierung, zur Abdichtung und als Korrosionsschutz verwendet werden.","蒽油主要用于生产蒽和炭黑等其他物质。它们也可用作高炉中的还原剂、燃料油中的组分，用于浸渍、密封和防腐蚀。"]
[null,{"$f":"IF($B$1=\"English\",C2511,IF($B$1=\"Deutsch\",D2511,IF($B$1=\"中文\",E2511,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection.","Anthracenöle werden hauptsächlich bei der Herstellung von anderen Stoffen wie beispielsweise Anthracen und Carbon-Black verwendet. Sie können auch als Reduktionsmittel in Hochöfen, als Komponenten in Bunkeröl, zur Imprägnierung, zur Abdichtung und als Korrosionsschutz verwendet werden. ","蒽油主要用于生产蒽和炭黑等其他物质。它们也可用作高炉中的还原剂、燃料油中的组分，用于浸渍、密封和防腐蚀。"]
[null,{"$f":"IF($B$1=\"English\",C2512,IF($B$1=\"Deutsch\",D2512,IF($B$1=\"中文\",E2512,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection.","Anthracenöle werden hauptsächlich bei der Herstellung von anderen Stoffen wie beispielsweise Anthracen und Carbon-Black verwendet. Sie können auch als Reduktionsmittel in Hochöfen, als Komponenten in Bunkeröl, zur Imprägnierung, zur Abdichtung und als Korrosionsschutz verwendet werden. ","蒽油主要用于生产蒽和炭黑等其他物质。它们也可用作高炉中的还原剂、燃料油中的组分，用于浸渍、密封和防腐蚀。"]
[null,{"$f":"IF($B$1=\"English\",C2513,IF($B$1=\"Deutsch\",D2513,IF($B$1=\"中文\",E2513,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection.","Anthracenöle werden hauptsächlich bei der Herstellung von anderen Stoffen wie beispielsweise Anthracen und Carbon-Black verwendet. Sie können auch als Reduktionsmittel in Hochöfen, als Komponenten in Bunkeröl, zur Imprägnierung, zur Abdichtung und als Korrosionsschutz verwendet werden. ","蒽油主要用于生产蒽和炭黑等其他物质。它们也可用作高炉中的还原剂、燃料油中的组分，用于浸渍、密封和防腐蚀。"]
[null,{"$f":"IF($B$1=\"English\",C2514,IF($B$1=\"Deutsch\",D2514,IF($B$1=\"中文\",E2514,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection."},"Anthracene oils are mainly used in the production of other substances such as anthracene and carbon black. They can also be used as reducing agents in blast furnaces, as components in bunker oil, for impregnation, sealing and corrosion protection.","Anthracenöle werden hauptsächlich bei der Herstellung von anderen Stoffen wie beispielsweise Anthracen und Carbon-Black verwendet. Sie können auch als Reduktionsmittel in Hochöfen, als Komponenten in Bunkeröl, zur Imprägnierung, zur Abdichtung und als Korrosionsschutz verwendet werden. ","蒽油主要用于生产蒽和炭黑等其他物质。它们也可用作高炉中的还原剂、燃料油中的成分，用于浸渍、密封和防腐蚀。"]
[null,{"$f":"IF($B$1=\"English\",C2515,IF($B$1=\"Deutsch\",D2515,IF($B$1=\"中文\",E2515,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acrylamide is used almost exclusively for the synthesis of polyacrylamides, which are then used in various applications, especially in waste water treatment and paper processing. Among the minor uses of acrylamide are the preparation of polyacrylamides for research purposes and their use as a cementing agent in civil engineering."},"Acrylamide is used almost exclusively for the synthesis of polyacrylamides, which are then used in various applications, especially in waste water treatment and paper processing. Among the minor uses of acrylamide are the preparation of polyacrylamides for research purposes and their use as a cementing agent in civil engineering.","Acrylamid wird nahezu ausschließlich für die Synthese von Polyacrylamiden verwendet, welche dann in verschiedenen Anwendungen, insbesondere in der Abwasserbehandlung und Papierverarbeitung, verwendet werden. Zu den geringeren Verwendungen von Acrylamid gehören die Zubereitung von Polyacrylamiden für Forschungszwecke und die Verwendung als Zementierstoff im Tiefbau.","丙烯酰胺几乎只用于合成聚丙烯酰胺，从而用于各种用途，特别是废水处理和纸张加工。丙烯酰胺的其他用途包括出于研究目的的聚丙烯酰胺制备、在土木工程中用作固化剂。"]
[null,{"$f":"IF($B$1=\"English\",C2516,IF($B$1=\"Deutsch\",D2516,IF($B$1=\"中文\",E2516,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium tetraborate and tetrabic sodium heptaoxide form the same compounds in aqueous solution. Applications include a wide range of applications such as detergents, glass and glass fibers, ceramics, industrial fluids, metallurgy, adhesives, flame retardants, personal care products, biocides and fertilizers. "},"Disodium tetraborate and tetrabic sodium heptaoxide form the same compounds in aqueous solution. Applications include a wide range of applications such as detergents, glass and glass fibers, ceramics, industrial fluids, metallurgy, adhesives, flame retardants, personal care products, biocides and fertilizers. ","Dinatriumtetraborat und Tetrabordinatriumheptaoxid bilden in wässriger Lösung dieselben Verbindungen. Zu den Verwendungen gehören eine Vielzahl von Anwendungen, z. B. in Wasch- und Reinigungsmitteln, in Glas und Glasfasern, Keramik, Industrieflüssigkeiten, Metallurgie, Klebstoffen, Flammschutzmitteln, Körperpflegeprodukten, Bioziden und Düngemitteln. ","四硼酸二钠和七氧化四钠在水溶液中形成相同的化合物，广泛应用于洗涤剂、玻璃和玻璃纤维、陶瓷、工业流体、冶金、粘合剂、阻燃剂、个人护理产品、生物杀灭剂和肥料。"]
[null,{"$f":"IF($B$1=\"English\",C2517,IF($B$1=\"Deutsch\",D2517,IF($B$1=\"中文\",E2517,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trichloroethene is used in the production of organic chlorine and fluorine compounds. It is also used for cleaning and degreasing metal parts or as a solvent in adhesives. "},"Trichloroethene is used in the production of organic chlorine and fluorine compounds. It is also used for cleaning and degreasing metal parts or as a solvent in adhesives. ","Trichlorethen wird bei der Herstellung organischer Chlor- und Fluor-Verbindungen verwendet. Außerdem wird es zum Reinigen und Entfetten von Metallteilen oder als Lösungsmittel in Klebstoffen benutzt. ","三氯乙烯用于生产有机氯和氟化合物。它也用于清洗和脱脂金属零件或作为粘合剂中的溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C2518,IF($B$1=\"Deutsch\",D2518,IF($B$1=\"中文\",E2518,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium chromate is used, for example, in chromium metal production, in the production of chlorates, in the coating of metals, as an analytical agent in the laboratory and in tanning leather and paints. "},"Sodium chromate is used, for example, in chromium metal production, in the production of chlorates, in the coating of metals, as an analytical agent in the laboratory and in tanning leather and paints. ","Natriumchromat wird beispielsweise in der Chrommetallherstellung, bei der Herstellung von Chloraten, in der Beschichtung von Metallen, als analytisches Agens im Labor sowie beim Gerben von Leder und in Farben verwendet. ","铬酸钠用于如铬金属生产、氯酸盐生产、金属涂层、实验室分析试剂以及制革和油漆。"]
[null,{"$f":"IF($B$1=\"English\",C2519,IF($B$1=\"Deutsch\",D2519,IF($B$1=\"中文\",E2519,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium tetraborate and tetrabic sodium heptaoxide form the same compounds in aqueous solution. Applications include a wide range of applications such as detergents, glass and glass fibers, ceramics, industrial fluids, metallurgy, adhesives, flame retardants, personal care products, biocides and fertilizers."},"Disodium tetraborate and tetrabic sodium heptaoxide form the same compounds in aqueous solution. Applications include a wide range of applications such as detergents, glass and glass fibers, ceramics, industrial fluids, metallurgy, adhesives, flame retardants, personal care products, biocides and fertilizers.","Dinatriumtetraborat und Tetrabordinatriumheptaoxid bilden in wässriger Lösung dieselben Verbindungen. Zu den Verwendungen gehören eine Vielzahl von Anwendungen, z. B. in Wasch- und Reinigungsmitteln, in Glas und Glasfasern, Keramik, Industrieflüssigkeiten, Metallurgie, Klebstoffen, Flammschutzmitteln, Körperpflegeprodukten, Bioziden und Düngemitteln.","四硼酸二钠和七氧化四钠在水溶液中形成相同的化合物，广泛应用于洗涤剂、玻璃和玻璃纤维、陶瓷、工业流体、冶金、粘合剂、阻燃剂、个人护理产品、生物杀灭剂和肥料。"]
[null,{"$f":"IF($B$1=\"English\",C2520,IF($B$1=\"Deutsch\",D2520,IF($B$1=\"中文\",E2520,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium chromate is used as a corrosion inhibitor in the treatment and coating of metals, for the production of reagents, chemicals and textiles, as a dye in the production of ceramics, glass and cement, in the production of pigments and inks and as an analytical agent in the laboratory. "},"Potassium chromate is used as a corrosion inhibitor in the treatment and coating of metals, for the production of reagents, chemicals and textiles, as a dye in the production of ceramics, glass and cement, in the production of pigments and inks and as an analytical agent in the laboratory. ","Kaliumchromat wird als Korrosionshemmer bei der Behandlung und Beschichtung von Metallen, zur Herstellung von Reagenzien, Chemikalien und Textilien, als Farbstoff bei der Keramik-, Glas- und Zementherstellung, bei der Herstellung von Pigmenten/Tinten und im Labor als analytisches Agens eingesetzt. ","铬酸钾在金属处理和涂层、试剂、化学品和纺织品生产中用作缓蚀剂，在陶瓷、玻璃和水泥生产中用作染料，在颜料和油墨生产中用作染料，在实验室中用作分析试剂。"]
[null,{"$f":"IF($B$1=\"English\",C2521,IF($B$1=\"Deutsch\",D2521,IF($B$1=\"中文\",E2521,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium dichromate is used for chromium metal production and as a corrosion inhibitor in the treatment and coating of metals. It is also used as a textile etchant, as an analytical agent in the laboratory, for cleaning laboratory glassware, in the manufacture of other reagents and as an oxidizing agent in photolithography."},"Potassium dichromate is used for chromium metal production and as a corrosion inhibitor in the treatment and coating of metals. It is also used as a textile etchant, as an analytical agent in the laboratory, for cleaning laboratory glassware, in the manufacture of other reagents and as an oxidizing agent in photolithography.","Kaliumdichromat wird für die Chrommetallherstellung und als Korrosionshemmer bei der Behandlung und Beschichtung von Metallen verwendet. Ferner findet es Anwendung als Textilbeizmittel, als analytisches Agens im Labor, zur Reinigung von Laborglasgeräten, bei der Herstellung anderer Reagenzien und als Oxidationsmittel in der Fotolithografie.","重铬酸钾用于生产金属铬，作为金属处理和涂层中的缓蚀剂。它还被用作纺织品蚀刻剂、实验室的分析试剂、实验室玻璃器皿的清洗、其他试剂的制造以及光刻中的氧化剂。"]
[null,{"$f":"IF($B$1=\"English\",C2522,IF($B$1=\"Deutsch\",D2522,IF($B$1=\"中文\",E2522,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid is used in a wide variety of applications due to its flame-retardant, antiseptic and preservative properties which influence consistency. It is used in detergents and cleaning agents, adhesives, toys, industrial fluids, brake fluids, glass, ceramics, flame retardants, paints, disinfectants, cosmetics, food additives, fertilizers, insecticides and other products."},"Boric acid is used in a wide variety of applications due to its flame-retardant, antiseptic and preservative properties which influence consistency. It is used in detergents and cleaning agents, adhesives, toys, industrial fluids, brake fluids, glass, ceramics, flame retardants, paints, disinfectants, cosmetics, food additives, fertilizers, insecticides and other products.","Borsäure wird aufgrund ihrer konsistenzbeeinflussenden, flammhemmenden, antiseptischen und konservierenden Eigenschaften mannigfaltig eingesetzt. Sie ist Bestandteil in Wasch- und Reinigungsmitteln, Klebstoffen, Spielsachen, Industrieflüssigkeiten, Bremsflüssigkeiten, Glas, Keramik, Flammschutzmitteln, Farben, Desinfektionsmitteln, Kosmetika, Lebensmittelzusatzstoffen, Düngemitteln, Insektiziden und anderen Produkten. ","硼酸因其影响稠度的阻燃、防腐和防腐性能而被广泛应用。它用于洗涤剂和清洁剂、粘合剂、玩具、工业液体、制动液、玻璃、陶瓷、阻燃剂、油漆、消毒剂、化妆品、食品添加剂、肥料、杀虫剂和其他产品。"]
[null,{"$f":"IF($B$1=\"English\",C2523,IF($B$1=\"Deutsch\",D2523,IF($B$1=\"中文\",E2523,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium dichromate is mainly used as an oxidizing agent. Other well-known applications are in the manufacture of light-sensitive screens and as a pickling agent in the manufacture of textiles. Among the minor uses appear to be metal treatment and use as a laboratory analytical agent."},"Ammonium dichromate is mainly used as an oxidizing agent. Other well-known applications are in the manufacture of light-sensitive screens and as a pickling agent in the manufacture of textiles. Among the minor uses appear to be metal treatment and use as a laboratory analytical agent.","Ammoniumdichromat wird hauptsächlich als Oxidationsmittel verwendet. Weitere bekannte Verwendungen finden sich bei der Herstellung lichtempfindlicher Bildschirme und als Beizmittel bei der Herstellung von Textilien. Zu den geringfügigen Verwendungen scheinen die Metallbehandlung und die Nutzung als laboranalytisches Agens zu gehören.","重铬酸铵主要用作氧化剂。其他熟知的应用是制造光敏屏和在纺织品制造中作为酸洗剂。次要用途包括金属处理和用作实验室分析试剂。"]
[null,{"$f":"IF($B$1=\"English\",C2524,IF($B$1=\"Deutsch\",D2524,IF($B$1=\"中文\",E2524,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acids generated from chromium trioxide and their oligomers are mainly used in metal finishing such as electroplating (e.g. hard chromium plating and decorative coating), conversion layers and brighteners. They are also used as fixing agents in water-based wood preservatives. Smaller uses can be found, for example, in the production of pigments and paints/lacquers, in the production of catalysts and cleaning agents and as oxidizing agents."},"Acids generated from chromium trioxide and their oligomers are mainly used in metal finishing such as electroplating (e.g. hard chromium plating and decorative coating), conversion layers and brighteners. They are also used as fixing agents in water-based wood preservatives. Smaller uses can be found, for example, in the production of pigments and paints/lacquers, in the production of catalysts and cleaning agents and as oxidizing agents.","Aus Chromtrioxid erzeugte Säuren und ihre Oligomere finden hauptsächlich Verwendung in der Metallveredelung wie Galvanoplastik (z. B. Hartverchromen und Dekorationsbeschichtung), Konversionsschichten und Aufheller. Sie werden auch als Fixiermittel in Holzkonservierungsmitteln auf Wasserbasis verwendet. Geringere Verwendungen finden sich z. B. bei der Herstellung von Pigmenten und Farben/Lacken, bei der Herstellung von Katalysatoren und Reinigungsmitteln und als Oxidationsmittel. ","由三氧化铬及其低聚物生成的酸主要用于金属表面处理，如电镀(如镀硬铬和装饰涂层)、转化层和增白剂。它们也用作水基木材防腐剂中的固定剂。也少见于生产颜料和油漆/清漆、催化剂和清洁剂，以及作为氧化剂。"]
[null,{"$f":"IF($B$1=\"English\",C2525,IF($B$1=\"Deutsch\",D2525,IF($B$1=\"中文\",E2525,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) diacetate is mainly used in the production of catalysts or as a catalyst. Lower uses include the production of other chemicals, including pigments, surface treatments, in alloys, dyes, rubber adhesion promoters and as feed additives."},"Cobalt(II) diacetate is mainly used in the production of catalysts or as a catalyst. Lower uses include the production of other chemicals, including pigments, surface treatments, in alloys, dyes, rubber adhesion promoters and as feed additives.","Kobalt(II)-diacetat wird hauptsächlich bei der Herstellung von Katalysatoren oder als Katalysator verwendet. Zu den geringeren Verwendungen gehören die Herstellung von anderen Chemikalien, unter anderem die Herstellung von Pigmenten, Oberflächenbehandlungen, in Legierungen, Farbstoffen, Gummihaftvermittlern und als Futterzusatz.","二乙酸钴主要用于生产催化剂或作为催化剂。较少用于生产其他化学品，包括颜料、表面处理、合金、染料、橡胶粘合促进剂和饲料添加剂。"]
[null,{"$f":"IF($B$1=\"English\",C2526,IF($B$1=\"Deutsch\",D2526,IF($B$1=\"中文\",E2526,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt (II) dinitrate is mainly used in the production of other chemicals and in the production of catalysts. Other possible applications are surface treatment and batteries."},"Cobalt (II) dinitrate is mainly used in the production of other chemicals and in the production of catalysts. Other possible applications are surface treatment and batteries.","Kobalt(II)-dinitrat wird hauptsächlich bei der Herstellung von anderen Chemikalien und bei der Herstellung von Katalysatoren verwendet. Weitere mögliche Verwendungen sind Oberflächenbehandlung und Batterien. ","二硝酸钴主要用于生产其他化学品和催化剂。其他可能的应用是表面处理和电池。"]
[null,{"$f":"IF($B$1=\"English\",C2527,IF($B$1=\"Deutsch\",D2527,IF($B$1=\"中文\",E2527,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) carbonate is mainly used in the production of catalysts. Smaller uses can be found as feed additive, in the production of other chemicals, in the production of pigments and as adhesive in primer frits."},"Cobalt(II) carbonate is mainly used in the production of catalysts. Smaller uses can be found as feed additive, in the production of other chemicals, in the production of pigments and as adhesive in primer frits.","Kobalt(II)-karbonat wird hauptsächlich bei der Herstellung von Katalysatoren verwendet. Geringere Verwendungen finden sich als Futterzusatz, bei der Herstellung von anderen Chemikalien, bei der Herstellung von Pigmenten und als Klebstoff in Grundierungsfritten. ","碳酸钴主要用于生产催化剂。在饲料添加剂、其他化学品的生产、颜料的生产以及底漆熔块的粘合剂等方面，可以找到较小的用途。"]
[null,{"$f":"IF($B$1=\"English\",C2528,IF($B$1=\"Deutsch\",D2528,IF($B$1=\"中文\",E2528,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt(II) sulphate is mainly used in the manufacture of other chemicals and pigments and possibly catalysts and desiccants. Other applications include surface treatments (e.g. electroplating), corrosion protection, decolourisation (of glass and ceramic goods), in batteries, animal feed additives and soil fertilisers."},"Cobalt(II) sulphate is mainly used in the manufacture of other chemicals and pigments and possibly catalysts and desiccants. Other applications include surface treatments (e.g. electroplating), corrosion protection, decolourisation (of glass and ceramic goods), in batteries, animal feed additives and soil fertilisers.","Kobalt(II)-sulfat wird hauptsächlich bei der Herstellung von anderen Chemikalien und Pigmenten sowie möglicherweise Katalysatoren und Trockenmittel verwendet. Weitere Verwendungen umfassen Oberflächenbehandlungen (z. B. Galvanoplastik), Korrosionsschutz, Entfärben (von Glas- und Keramikwaren), in Batterien, Tierfutterzusätze und Bodendüngemittel. ","硫酸钴主要用于制造其他化学品和颜料，也可能用于制造催化剂和干燥剂。其他应用包括表面处理(如电镀)、防腐、脱色(玻璃和陶瓷制品)、电池、动物饲料添加剂和土壤肥料。"]
[null,{"$f":"IF($B$1=\"English\",C2529,IF($B$1=\"Deutsch\",D2529,IF($B$1=\"中文\",E2529,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium trioxide is mainly used in metal finishing such as electroplating (e.g. hard chromium plating and decorative coating), conversion coatings and brighteners. It is also used as a fixing agent in water-based wood preservatives. Smaller uses are, for example, in the production of pigments and paints/lacquers, in the production of catalysts and cleaning agents and as oxidizing agents."},"Chromium trioxide is mainly used in metal finishing such as electroplating (e.g. hard chromium plating and decorative coating), conversion coatings and brighteners. It is also used as a fixing agent in water-based wood preservatives. Smaller uses are, for example, in the production of pigments and paints/lacquers, in the production of catalysts and cleaning agents and as oxidizing agents.","Chromtrioxid findet hauptsächlich Verwendung in der Metallveredelung wie Galvanoplastik (z. B. Hartverchromen und Dekorationsbeschichtung), Konversionsschichten und Aufheller. Es wird auch als Fixiermittel in Holzkonservierungsmitteln auf Wasserbasis verwendet. Geringere Verwendungen finden sich zum Beispiel bei der Herstellung von Pigmenten und Farben/Lacken, bei der Herstellung von Katalysatoren und Reinigungsmitteln und als Oxidationsmittel. ","三氧化铬主要用于金属表面处理，如电镀(如镀硬铬和装饰涂层)、转化膜和光亮剂。它也用作水基木材防腐剂中的固定剂。例如，较小的用途是生产颜料和油漆/清漆，生产催化剂和清洁剂以及作为氧化剂。"]
[null,{"$f":"IF($B$1=\"English\",C2530,IF($B$1=\"Deutsch\",D2530,IF($B$1=\"中文\",E2530,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Ethoxyethanol is mainly used as a chemical intermediate. It is less used as a solvent or laboratory chemical."},"2-Ethoxyethanol is mainly used as a chemical intermediate. It is less used as a solvent or laboratory chemical.","2-Ethoxyethanol wird hauptsächlich als chemisches Zwischenprodukt verwendet. Weniger Verwendung findet es als Lösungsmittel oder Laborchemikalie. ","2-乙氧基乙醇主要用作化学中间体。它较少用作溶剂或实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2531,IF($B$1=\"Deutsch\",D2531,IF($B$1=\"中文\",E2531,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyethanol is mainly used as a chemical intermediate. It is less used as a solvent or laboratory chemical. "},"2-Methoxyethanol is mainly used as a chemical intermediate. It is less used as a solvent or laboratory chemical. ","2-Methoxyethanol wird hauptsächlich als chemisches Zwischenprodukt verwendet. Weniger Verwendung findet es als Lösungsmittel oder Laborchemikalie. ","2-甲氧基乙醇主要用作化学中间体。它较少用作溶剂或实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2532,IF($B$1=\"Deutsch\",D2532,IF($B$1=\"中文\",E2532,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Strontium chromate is mainly used as a corrosion inhibitor in coating mixtures used in the aerospace, steel and aluminum strip coating and automotive coating sectors."},"Strontium chromate is mainly used as a corrosion inhibitor in coating mixtures used in the aerospace, steel and aluminum strip coating and automotive coating sectors.","Strontiumchromat wird hauptsächlich als Korrosionsinhibitor in Beschichtungsmischungen verwendet, die im Luft- und Raumfahrtsektor, im Bandbeschichtungssektor von Stahl und Aluminium und im Fahrzeugbeschichtungssektor Anwendung finden. ","铬酸锶主要用作航空航天、钢带和铝带涂层以及汽车涂层行业中涂层混合物的缓蚀剂。"]
[null,{"$f":"IF($B$1=\"English\",C2533,IF($B$1=\"Deutsch\",D2533,IF($B$1=\"中文\",E2533,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hydrazine is mainly used as an intermediate in the production of hydrazine derivatives, as a monomer in polymerisations, as a corrosion inhibitor in water treatment and for metal reduction and chemical refinement. Hydrazine is also used as fuel for spacecraft and as fuel for military (emergency) power units."},"Hydrazine is mainly used as an intermediate in the production of hydrazine derivatives, as a monomer in polymerisations, as a corrosion inhibitor in water treatment and for metal reduction and chemical refinement. Hydrazine is also used as fuel for spacecraft and as fuel for military (emergency) power units.","Hydrazin findet hauptsächlich Verwendung als Zwischenprodukt bei der Herstellung von Hydrazinderivaten, als Monomer in Polymerisationen, als Korrosionsinhibitor bei der Wasseraufbereitung sowie zur Metallreduktion und Veredelung von Chemikalien. Außerdem wird Hydrazin als Treibstoff für Raumfahrzeuge und als Brennstoff für militärische (Not-) Energieaggregate verwendet.","肼主要用作肼衍生物生产中的中间体、聚合中的单体、水处理中的缓蚀剂以及金属还原和化学精炼。肼也用作航天器的燃料和军事(应急)动力装置的燃料。"]
[null,{"$f":"IF($B$1=\"English\",C2534,IF($B$1=\"Deutsch\",D2534,IF($B$1=\"中文\",E2534,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt dichloride is mainly used as an intermediate in the production of other cobalt compounds, in tire adhesion additives, organic textile dyes and drying agents for paints. It is also used in surface treatment processes, for example in water treatment / corrosion-inhibiting chemicals, as a colorant or for decolorizing in the production of inorganic pigments & frits, glass and ceramics, in varistors and magnets, and in moisture meters."},"Cobalt dichloride is mainly used as an intermediate in the production of other cobalt compounds, in tire adhesion additives, organic textile dyes and drying agents for paints. It is also used in surface treatment processes, for example in water treatment / corrosion-inhibiting chemicals, as a colorant or for decolorizing in the production of inorganic pigments & frits, glass and ceramics, in varistors and magnets, and in moisture meters.","Kobaltdichlorid findet hauptsächlich Anwendung als Zwischenprodukt bei der Herstellung von weiteren Kobaltverbindungen, in Reifenhaftungszusätzen, organischen Textilfarbstoffen und Trocknungsmitteln für Anstriche. Außerdem wird es in Verfahren zur Oberflächenbehandlung eingesetzt, so zum Beispiel bei der Wasseraufbereitung / korrosionshemmende Chemikalie, als Farbstoff oder zum Entfärben bei der Herstellung von anorganischen Pigmenten & Fritten, Glas und Keramik, in Varistoren und Magneten sowie in Feuchtigkeitsmessgeräten.","二氯化钴主要用作生产其他钴化合物的中间体、轮胎粘合添加剂、有机纺织染料和油漆干燥剂。它也用于表面处理工艺，例如水处理/腐蚀抑制化学品，作为着色剂或用于无机颜料和玻璃料、玻璃和陶瓷、变阻器和磁铁以及湿度计生产中的脱色。"]
[null,{"$f":"IF($B$1=\"English\",C2535,IF($B$1=\"Deutsch\",D2535,IF($B$1=\"中文\",E2535,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ECHA has not yet received registration for 2-ethoxyethyl acetate. It can therefore be concluded that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past, the substance was mainly used as a solvent in coatings and in the chemical industry, but also as an intermediate in the production of cyanoacrylate adhesives. "},"ECHA has not yet received registration for 2-ethoxyethyl acetate. It can therefore be concluded that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past, the substance was mainly used as a solvent in coatings and in the chemical industry, but also as an intermediate in the production of cyanoacrylate adhesives. ","Bisher hat die ECHA noch keine Registrierung über 2-Ethoxyethylacetat erhalten. Daraus ist zu schließen, dass der Stoff in der EU nicht in Mengen über 1 Tonne/Jahr hergestellt oder importiert wird. In der Vergangenheit fand der Stoff hauptsächlich Verwendung als Lösungsmittel in Beschichtungen und in der chemischen Industrie, aber auch als Zwischenprodukt bei der Herstellung von Cyanoacrylat-Klebstoffen. ","ECHA尚未收到2-乙氧基乙酸乙酯的注册。因此可以得出结论，该物质在欧盟的生产或进口数量不超过1吨每年。该物质曾主要用作涂料和化学工业中的溶剂，但也用作氰基丙烯酸酯粘合剂生产中的中间体。"]
[null,{"$f":"IF($B$1=\"English\",C2536,IF($B$1=\"Deutsch\",D2536,IF($B$1=\"中文\",E2536,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,3-trichloropropane is mainly used as an intermediate in the production of chlorinated solvents and agricultural products. It is also used as a monomer. In the past, 1,2,3-trichloropropane was used as solvent, paint and varnish remover and degreasing agent."},"1,2,3-trichloropropane is mainly used as an intermediate in the production of chlorinated solvents and agricultural products. It is also used as a monomer. In the past, 1,2,3-trichloropropane was used as solvent, paint and varnish remover and degreasing agent.","1,2,3-Trichloropropan findet hauptsächlich Verwendung als Zwischenprodukt bei der Herstellung von chlorierten Lösungsmitteln und Agrarprodukten. Es wird auch verwendet als Monomer. In der Vergangenheit wurde 1,2,3-Trichloropropan als Lösungsmittel, Farb- und Lackentferner sowie als Entfettungsmittel verwendet. ","1，2，3-三氯丙烷主要用作氯化溶剂和农产品生产的中间体。它也用作单体。过去使用1，2，3-三氯丙烷作为溶剂、脱漆剂和脱脂剂。"]
[null,{"$f":"IF($B$1=\"English\",C2537,IF($B$1=\"Deutsch\",D2537,IF($B$1=\"中文\",E2537,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ECHA has not yet received registration for DIHP. Thus, it appears that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past, it was mainly used as a plasticizer in PVC and sealants, coatings and possibly in printing inks."},"ECHA has not yet received registration for DIHP. Thus, it appears that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past, it was mainly used as a plasticizer in PVC and sealants, coatings and possibly in printing inks.","Die ECHA hat bisher keine Registrierung für DIHP erhalten. Somit scheint es, dass der Stoff in der EU nicht in Mengen über 1 Tonne/Jahr hergestellt oder importiert wird. In der Vergangenheit wurden der hauptsächlich als Weichmacher in PVC und Dichtungsmitteln, Beschichtungen und möglicherweise in Druckfarben verwendet. ","ECHA尚未收到DIHP登记。因此，欧盟生产或进口该物质的数量似乎不超过1吨每年。它曾主要用作聚氯乙烯和密封剂、涂料中的增塑剂，也可能用于印刷油墨。"]
[null,{"$f":"IF($B$1=\"English\",C2538,IF($B$1=\"Deutsch\",D2538,IF($B$1=\"中文\",E2538,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ECHA has not yet received registration for DHNUP. Thus, it appears that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past it was mainly used as a plasticizer in PVC, foam, adhesives and coatings."},"ECHA has not yet received registration for DHNUP. Thus, it appears that the substance is not produced or imported in the EU in quantities above 1 tonne/year. In the past it was mainly used as a plasticizer in PVC, foam, adhesives and coatings.","Für DHNUP hat die ECHA bisher keine Registrierung erhalten. Somit scheint es, dass der Stoff in der EU nicht in Mengen über 1 Tonne/Jahr hergestellt oder importiert wird. In der Vergangenheit wurde er hauptsächlich als Weichmacher in PVC, Schaumstoff, Klebstoffen und Beschichtungen verwendet.","ECHA尚未收到DHNUP的登记。因此，欧盟生产或进口的物质数量似乎不超过1吨每年。它曾主要用作聚氯乙烯、泡沫、粘合剂和涂料中的增塑剂。"]
[null,{"$f":"IF($B$1=\"English\",C2539,IF($B$1=\"Deutsch\",D2539,IF($B$1=\"中文\",E2539,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Methyl-2-pyrrolidon findet hauptsächlich Anwendung als Lösungsmittel in Beschichtungen, Reinigungsmitteln, für die Herstellung elektronischer Geräte sowie auch in der Halbleiterindustrie, bei der petrochemischen Verarbeitung, in Arzneimitteln und in Agrochemikalien. "},"1-Methyl-2-pyrrolidon findet hauptsächlich Anwendung als Lösungsmittel in Beschichtungen, Reinigungsmitteln, für die Herstellung elektronischer Geräte sowie auch in der Halbleiterindustrie, bei der petrochemischen Verarbeitung, in Arzneimitteln und in Agrochemikalien. ","1-Methyl-2-pyrrolidon findet hauptsächlich Anwendung als Lösungsmittel in Beschichtungen, Reinigungsmitteln, für die Herstellung elektronischer Geräte sowie auch in der Halbleiterindustrie, bei der petrochemischen Verarbeitung, in Arzneimitteln und in Agrochemikalien. ","1-methyl-2-pyrrolidone is mainly used as a solvent in coatings, cleaning agents, for the manufacture of electronic devices and also in the semiconductor industry, in petrochemical processing, in pharmaceuticals and in agrochemicals."]
[null,{"$f":"IF($B$1=\"English\",C2540,IF($B$1=\"Deutsch\",D2540,IF($B$1=\"中文\",E2540,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trilead diarsenate is found in complex raw materials for the production of copper, lead and a number of precious metals. The trible diarsenate contained in the raw materials is converted into calcium arsenate and diarsene trioxide in the metallurgical refining process. While most of the calcium arsenate is apparently disposed of as waste, the diarsene trioxide is still used. "},"Trilead diarsenate is found in complex raw materials for the production of copper, lead and a number of precious metals. The trible diarsenate contained in the raw materials is converted into calcium arsenate and diarsene trioxide in the metallurgical refining process. While most of the calcium arsenate is apparently disposed of as waste, the diarsene trioxide is still used. ","Tribleidiarsenat kommt in komplexen Rohstoffen für die Herstellung von Kupfer, Blei und einer Reihe von Edelmetallen vor. Das in den Rohstoffen enthaltene Tribleidiarsenat wird im metallurgischen Veredelungsprozess in Calciumarsenat und Diarsentrioxid umgewandelt. Während der größte Teil des Calciumarsenats anscheindend als Abfall entsorgt wird, wird das Diarsentrioxid weiter verwendet. ","在生产铜、铅和一些贵金属的复杂原料中发现了三铅二砷。在冶金精炼过程中，原料中含有的三溴二砷酸盐转化为砷酸钙和三氧化二砷。虽然大多数砷酸钙显然是作为废物处理的，但三氧化二砷仍在使用。"]
[null,{"$f":"IF($B$1=\"English\",C2541,IF($B$1=\"Deutsch\",D2541,IF($B$1=\"中文\",E2541,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Refractory ceramic fibres are used for high-temperature insulation, almost exclusively in industrial applications (insulation of industrial furnaces and equipment, equipment for the automotive and aerospace industries) and for fire protection (buildings and industrial process equipment)."},"Refractory ceramic fibres are used for high-temperature insulation, almost exclusively in industrial applications (insulation of industrial furnaces and equipment, equipment for the automotive and aerospace industries) and for fire protection (buildings and industrial process equipment).","Feuerfeste Keramikfasern finden Anwendung bei der Hochtemperaturisolierung, fast ausschließlich in Industrieapplikationen (Isolierung von Industrieöfen und -ausrüstungen, Ausrüstungen für die Automobilindustrie, Luft- und Raumfahrtindustrie) und beim Feuerschutz (Gebäude und industrielle Prozessausrüstungen).","耐火陶瓷纤维用于高温绝缘，几乎只用于工业应用(工业炉和设备的绝缘、汽车和航空工业的设备)和防火(建筑和工业加工设备)。"]
[null,{"$f":"IF($B$1=\"English\",C2542,IF($B$1=\"Deutsch\",D2542,IF($B$1=\"中文\",E2542,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenolphthalein is mainly used for laboratory purposes (pH indicator solutions). It is less used in pharmaceutical preparations and in some special applications (e.g. pH indicator paper, invisible inks)."},"Phenolphthalein is mainly used for laboratory purposes (pH indicator solutions). It is less used in pharmaceutical preparations and in some special applications (e.g. pH indicator paper, invisible inks).","Phenolphthalein wird hauptsächlich für Laborzwecke (pH-Indikatorlösungen) verwendet. Weniger Verwendung findet es in pharmazeutischen Zubereitungen und in einigen Spezialapplikationen (z. B. pH-Indikatorpapier, unsichtbare Tinten).","酚酞主要用于实验室目的(pH指示剂溶液)。它较少用于药物制剂和一些特殊应用(如酸碱度指示纸、隐形油墨)。"]
[null,{"$f":"IF($B$1=\"English\",C2543,IF($B$1=\"Deutsch\",D2543,IF($B$1=\"中文\",E2543,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentazinc chromate octahydroxide is mainly used in coatings for the automotive and aerospace industries."},"Pentazinc chromate octahydroxide is mainly used in coatings for the automotive and aerospace industries.","Pentazinkchromat-octahydroxid findet hauptsächlich Verwendung in Beschichtungen im Fahrzeugwesen und in der Luft- und Raumfahrtindustrie.","八氢五锌铬酸盐主要用于汽车和航空工业的涂料。"]
[null,{"$f":"IF($B$1=\"English\",C2544,IF($B$1=\"Deutsch\",D2544,IF($B$1=\"中文\",E2544,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Technical MDA is mainly used in the production of other materials. Less use as ion exchange resins in nuclear power plants, as hardeners for epoxy resins, e.g. for the manufacture of rollers, pipes and moulds, and adhesives. "},"Technical MDA is mainly used in the production of other materials. Less use as ion exchange resins in nuclear power plants, as hardeners for epoxy resins, e.g. for the manufacture of rollers, pipes and moulds, and adhesives. ","Technisches MDA findet hauptsächlich Verwendung bei der Herstellung von anderen Stoffen. Weniger Verwendung als Ionenaustauschharze in Kernkraftwerken, als Härter für Epoxidharze, z. B. für die Herstellung von Rollen, Rohren und Formen sowie Klebstoffe. ","技术MDA主要用于其他材料的生产。在核电厂中较少用作离子交换树脂、环氧树脂的硬化剂，例如用于制造辊子、管道和模具以及粘合剂。"]
[null,{"$f":"IF($B$1=\"English\",C2545,IF($B$1=\"Deutsch\",D2545,IF($B$1=\"中文\",E2545,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium hydroxyoctaoxodizincatedichromate(1-) is mainly used in coatings in the aerospace industry as well as in the coating of steel and aluminium strips and vehicle coatings."},"Potassium hydroxyoctaoxodizincatedichromate(1-) is mainly used in coatings in the aerospace industry as well as in the coating of steel and aluminium strips and vehicle coatings.","Kaliumhydroxyoctaoxo-dizinkat-dichromat findet hauptsächlich Verwendung in Beschichtungen in der Luft- und Raumfahrtindustrie sowie in der Beschichtung von Stahl- und Aluminiumbändern und Fahrzeugbeschichtung.","羟基八氧代二氰基二氢钾(1-)主要用于航空航天工业的涂料，以及钢和铝带的涂料和车辆涂料。"]
[null,{"$f":"IF($B$1=\"English\",C2546,IF($B$1=\"Deutsch\",D2546,IF($B$1=\"中文\",E2546,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N-dimethylacetamide is used as a solvent, mainly in the manufacture of various fabrics and in the manufacture of fibers for clothing and other applications. It is also used as a reagent and in products such as industrial coatings and paints, insulating paper, polyimide films, stripping agents and ink removers. "},"N,N-dimethylacetamide is used as a solvent, mainly in the manufacture of various fabrics and in the manufacture of fibers for clothing and other applications. It is also used as a reagent and in products such as industrial coatings and paints, insulating paper, polyimide films, stripping agents and ink removers. ","N,N-Dimethylacetamid wird verwendet als Lösungsmittel, hauptsächlich bei der Herstellung verschiedener Stoffe und bei der Herstellung von Fasern für Kleidung und bei anderen Applikationen. Er wird auch eingesetzt als Reagens und in Produkten wie Industrielacken und -farben, Isolierpapier, Polyimidfolien, Abbeizmitteln und Tintenentfernern. ","N，N-二甲基乙酰胺用作溶剂，主要用于制造各种织物和制造服装和其他用途的纤维。它还用作试剂，用于工业涂料和油漆、绝缘纸、聚酰亚胺薄膜、剥离剂和油墨去除剂等产品。"]
[null,{"$f":"IF($B$1=\"English\",C2547,IF($B$1=\"Deutsch\",D2547,IF($B$1=\"中文\",E2547,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Calcium arsenate is present in complex raw materials (which themselves are by-products of metallurgical processes), which are mainly used for copper and lead refining. The material is used to deposit nickel from molten metal and to produce diarsene trioxide. However, most of the substance appears to be disposed of as waste."},"Calcium arsenate is present in complex raw materials (which themselves are by-products of metallurgical processes), which are mainly used for copper and lead refining. The material is used to deposit nickel from molten metal and to produce diarsene trioxide. However, most of the substance appears to be disposed of as waste.","Calciumarsenat ist in komplexen Rohstoffen vorhanden (die selber Nebenprodukte aus metallurgischen Prozessen sind), die hauptsächlich für die Kupfer- und Bleiraffination Verwendung finden. Der Stoff wird eingesetzt, um Nickel aus geschmolzenem Metall abzuscheiden und Diarsentrioxid herzustellen. Jedoch wird der größte Teil des Stoffes anscheinend als Abfall entsorgt. ","砷酸钙存在于复杂的原料中(它们本身是冶金过程的副产品)，主要用于铜和铅的精炼。这种材料用于从熔融金属中沉积镍并生产三氧化二砷。然而，大多数物质似乎是作为废物处理的。"]
[null,{"$f":"IF($B$1=\"English\",C2548,IF($B$1=\"Deutsch\",D2548,IF($B$1=\"中文\",E2548,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichrom tris(chromate) is mainly used in mixtures for metal surface treatment in the aerospace, steel and aluminium coating sectors. "},"Dichrom tris(chromate) is mainly used in mixtures for metal surface treatment in the aerospace, steel and aluminium coating sectors. ","Dichromtris(chromat) findet hautsächlich Verwendung in Gemischen bei der Metalloberflächenbehandlung in der Luft- und Raumfahrt sowie in den Stahl- und Aluminiumbeschichtungssektoren. ","重铬酸盐三(铬酸盐)主要用于航空航天、钢铁和铝涂层行业的金属表面处理混合物。"]
[null,{"$f":"IF($B$1=\"English\",C2549,IF($B$1=\"Deutsch\",D2549,IF($B$1=\"中文\",E2549,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead diazide is mainly used as a detonator or amplifier in detonators for both civil and military applications and as a detonator in pyrotechnic devices."},"Lead diazide is mainly used as a detonator or amplifier in detonators for both civil and military applications and as a detonator in pyrotechnic devices.","Bleidiazid findet hauptsächlich Verwendung als Zünder oder Verstärker in Detonatoren sowohl für zivile als auch militärische Verwendungen sowie als Zünder in pyrotechnischen Vorrichtungen.","二叠氮化铅主要用作民用和军用雷管中的雷管或放大器，以及烟火装置中的雷管。"]
[null,{"$f":"IF($B$1=\"English\",C2550,IF($B$1=\"Deutsch\",D2550,IF($B$1=\"中文\",E2550,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No registration for lead dipicrate has been submitted to ECHA. As with lead diazide and lead styphnate, the substance is an explosive. It may be used in small quantities in detonator mixtures together with the other two lead compounds mentioned."},"No registration for lead dipicrate has been submitted to ECHA. As with lead diazide and lead styphnate, the substance is an explosive. It may be used in small quantities in detonator mixtures together with the other two lead compounds mentioned.","Bei der ECHA wurde keine Registrierung für Bleidipikrat eingereicht. Bei dem Stoff handelt es sich wie bei Bleidiazid und Bleistyphnat um einen Explosivstoff. Es kann sein, dass er zusammen mit den beiden anderen genannten Bleiverbindungen in geringen Mengen in Detonator-Gemischen verwendet wird.","尚未向ECHA提交二碳酸铅的登记。与二叠氮铅和斯蒂芬酸铅一样，这种物质是一种爆炸物。它可与上述另外两种铅化合物一起少量用于雷管混合物中。"]
[null,{"$f":"IF($B$1=\"English\",C2551,IF($B$1=\"Deutsch\",D2551,IF($B$1=\"中文\",E2551,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead styphnate is mainly used as an initial explosive for small calibre and rifle ammunition. Other common applications include ammunition pyrotechnics, ammunition-operated devices such as bolt-firing devices and detonators for civil use. "},"Lead styphnate is mainly used as an initial explosive for small calibre and rifle ammunition. Other common applications include ammunition pyrotechnics, ammunition-operated devices such as bolt-firing devices and detonators for civil use. ","Bleistyphnat findet hauptsächlich Verwendung als Initialsprengstoff für Kleinkaliber- und Gewehrmunition. Weitere übliche Verwendungen finden sich in der Munitionspyrotechnik, munitionsbetriebenen Vorrichtungen wie Bolzensetzgeräte und Detonatoren für zivile Verwendungen. ","斯蒂芬酸铅主要用作小口径和步枪弹药的初始炸药。其他常见的应用包括弹药烟火、弹药操纵装置，如民用的螺栓点火装置和雷管。 "]
[null,{"$f":"IF($B$1=\"English\",C2552,IF($B$1=\"Deutsch\",D2552,IF($B$1=\"中文\",E2552,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Arsenic acid is mainly used to remove gas bubbles from ceramic glass melt (clarifying agent) and is used in the manufacture of laminated printed circuit boards. To a lesser extent, the substance is also used in the production of semiconductors and as a laboratory chemical. "},"Arsenic acid is mainly used to remove gas bubbles from ceramic glass melt (clarifying agent) and is used in the manufacture of laminated printed circuit boards. To a lesser extent, the substance is also used in the production of semiconductors and as a laboratory chemical. ","Arsensäure wird hauptsächlich benutzt, um Gasblasen aus Keramikglasschmelze zu entfernen (Klärmittel), und findet Verwendung bei der Herstellung von laminierten Leiterplatten. In geringerem Umfang wird der Stoff auch bei der Herstellung von Halbleitern und als Laborchemikalie verwendet. ","砷酸主要用于去除陶瓷玻璃熔体中的气泡(澄清剂)，并用于制造层压印刷电路板。在较小的程度上，这种物质也用于半导体生产和作为实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2553,IF($B$1=\"Deutsch\",D2553,IF($B$1=\"中文\",E2553,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-methoxyethyl)ether is primarily used as a reactive solvent or as a process chemical in a wide range of applications. It is also used for battery electrolytes and possibly in other products such as sealants, adhesives, fuels and car care products. "},"Bis(2-methoxyethyl)ether is primarily used as a reactive solvent or as a process chemical in a wide range of applications. It is also used for battery electrolytes and possibly in other products such as sealants, adhesives, fuels and car care products. ","Bis(2-methoxyethyl)ether findet vorrangig Verwendung als reaktives Lösungsmittel oder als Prozesschemikalie in einem breiten Spektrum von Applikationen. Ebenfalls wird es verwendet für Batterie-Elektrolyte und möglicherweise in anderen Produkten wie Dichtstoffe, Klebemittel, Treibstoffe und Autopflegemittel. ","双(2-甲氧基乙基)醚主要用作反应性溶剂或广泛应用的过程化学品。它也用于电池电解液，也可能用于其他产品，如密封剂、粘合剂、燃料和汽车护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C2554,IF($B$1=\"Deutsch\",D2554,IF($B$1=\"中文\",E2554,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No registration for bis(2-methoxyethyl)phthalate has been submitted to ECHA. It therefore appears that the substance is not produced or imported into the EU in quantities over 1 tonne per year. The main uses in the past have been as plasticizers in polymeric materials and paints, lacquers and paints, including printing inks. "},"No registration for bis(2-methoxyethyl)phthalate has been submitted to ECHA. It therefore appears that the substance is not produced or imported into the EU in quantities over 1 tonne per year. The main uses in the past have been as plasticizers in polymeric materials and paints, lacquers and paints, including printing inks. ","Bei der ECHA wurde keine Registrierung für Bis(2-methoxyethyl)phthalat eingereicht. Daher scheint es, dass der Stoff in der EU nicht in Mengen über 1t/Jahr hergestellt oder in die EU eingeführt wird. Die Hauptverwendungszwecke in der Vergangenheit erfolgten als Weichmacher in polymeren Werkstoffen und Farben, Lacken und Anstrichmitteln, einschließlich Druckfarben. ","没有向ECHA提交邻苯二甲酸二(2-甲氧基乙基)酯的登记。因此，该物质在欧盟的生产或进口量似乎不超过每年1吨。过去的主要用途是在聚合材料和涂料、天然漆和油漆(包括印刷油墨)中作为增塑剂。"]
[null,{"$f":"IF($B$1=\"English\",C2555,IF($B$1=\"Deutsch\",D2555,IF($B$1=\"中文\",E2555,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyaniline is mainly used in the production of paints (e.g. azo and naphthol dyes) for tattooing and for dyeing paper, polymers and aluminium foil."},"2-Methoxyaniline is mainly used in the production of paints (e.g. azo and naphthol dyes) for tattooing and for dyeing paper, polymers and aluminium foil.","2-Methoxyanilin wird hauptsächlich bei der Herstellung von Farben (z. B. Azo- und Naphtholfarben) zum Tätowieren und zum Färben von Papier, Polymeren und Aluminiumfolie verwendet.","2-甲氧基苯胺主要用于生产纹身和纸张、聚合物和铝箔染色用的油漆(如偶氮和萘酚染料)。"]
[null,{"$f":"IF($B$1=\"English\",C2556,IF($B$1=\"Deutsch\",D2556,IF($B$1=\"中文\",E2556,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(1,1,3,3-tetramethylbutyl)phenol is mainly used in the production of polymer mixtures, phenolic resins and ethoxylate surfactants. It is also used as a component in adhesives, coatings, inks and rubber products."},"4-(1,1,3,3-tetramethylbutyl)phenol is mainly used in the production of polymer mixtures, phenolic resins and ethoxylate surfactants. It is also used as a component in adhesives, coatings, inks and rubber products.","4-(1,1,3,3-Tetramethylbutyl)phenol wird hauptsächlich bei der Herstellung von Polymer-Gemischen, Phenolische Harze und Ethoxylat-Tensiden verwendet. Weiter findet er Verwendung als Komponente bei Klebstoffen, Beschichtungen, Tinten und Gummierzeugnissen.","4-(1，1，3，3-四甲基丁基)苯酚主要用于生产聚合物混合物、酚醛树脂和乙氧基化表面活性剂。它还被用作粘合剂、涂料、油墨和橡胶制品的成分。"]
[null,{"$f":"IF($B$1=\"English\",C2557,IF($B$1=\"Deutsch\",D2557,IF($B$1=\"中文\",E2557,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Refractory ceramic fibres are used for high-temperature insulation, almost exclusively in industrial applications (insulation of industrial furnaces and equipment, equipment for the automotive and aerospace industries) and for fire protection (buildings and industrial process equipment)."},"Refractory ceramic fibres are used for high-temperature insulation, almost exclusively in industrial applications (insulation of industrial furnaces and equipment, equipment for the automotive and aerospace industries) and for fire protection (buildings and industrial process equipment).","Feuerfeste Keramikfasern finden Anwendung bei der Hochtemperaturisolierung, fast ausschließlich in Industrieapplikationen (Isolierung von Industrieöfen und -ausrüstungen, Ausrüstungen für die Automobilindustrie, Luft- und Raumfahrtindustrie) und beim Feuerschutz (Gebäude und industrielle Prozessausrüstungen).","耐火陶瓷纤维用于高温绝缘，几乎只用于工业应用(工业炉和设备的绝缘、汽车和航空工业的设备)和防火(建筑和工业加工设备)。"]
[null,{"$f":"IF($B$1=\"English\",C2558,IF($B$1=\"Deutsch\",D2558,IF($B$1=\"中文\",E2558,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dichloroethane is mainly used in the production of other substances (e.g. vinyl chloride). It is partly used as a solvent in the chemical and pharmaceutical industries and in laboratories. "},"1,2-dichloroethane is mainly used in the production of other substances (e.g. vinyl chloride). It is partly used as a solvent in the chemical and pharmaceutical industries and in laboratories. ","1,2-Dichlorethan wird hauptsächlich bei der Herstellung von weiteren Stoffen (z. B. Vinylchlorid) verwendet. Teilweise wird es als Lösungsmittel in der chemischen und pharmazeutischen Industrie sowie in Laboren verwendet. ","1，2-二氯乙烷主要用于生产其他物质(如氯乙烯)。它在化学和制药工业以及实验室中被部分用作溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C2559,IF($B$1=\"Deutsch\",D2559,IF($B$1=\"中文\",E2559,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2'-dichloro-4,4'-methylenedianiline is mainly used as a hardener in resins and in the manufacture of polymer products such as polyurethane and also for the manufacture of other substances. The material can still be used in construction and art."},"2,2'-dichloro-4,4'-methylenedianiline is mainly used as a hardener in resins and in the manufacture of polymer products such as polyurethane and also for the manufacture of other substances. The material can still be used in construction and art.","2,2'-Dichlor-4,4'-methylendianilin wird hauptsächlich als Härter bei Harzen und bei der Herstellung von Polymer-Erzeugnissen wie z. B. Polyurethan und auch für die Herstellung von anderen Stoffen verwendet. Der Stoff kann weiterhin im Bauwesen und in der Kunst verwendet werden.","2，2 '-二氯-4，4 '-亚甲基二苯胺主要用作树脂中的硬化剂，用于制造聚氨酯等聚合物产品，也用于制造其他物质。该材料仍可用于建筑和艺术。"]
[null,{"$f":"IF($B$1=\"English\",C2560,IF($B$1=\"Deutsch\",D2560,IF($B$1=\"中文\",E2560,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used as an intermediate in the manufacture of agrochemicals, pharmaceuticals and industrial chemicals. Less often used as solvent and laboratory reagent for quality control in forensic laboratories, hospitals, pharmaceutical companies, food and beverage manufacturers and research laboratories. The fabric also seems to be used as a plasticizer."},"Mainly used as an intermediate in the manufacture of agrochemicals, pharmaceuticals and industrial chemicals. Less often used as solvent and laboratory reagent for quality control in forensic laboratories, hospitals, pharmaceutical companies, food and beverage manufacturers and research laboratories. The fabric also seems to be used as a plasticizer.","  Wird hauptsächlich als Zwischenprodukt bei der Herstellung von agrochemischen Erzeugnissen, Arzneimitteln und Industriechemikalien verwendet. Seltener verwendet als Lösungsmittel und als Laborreagenz zum Zweck der Qualitätskontrolle in forensischen Laboren, Krankenhäusern, Pharmazieunternehmen, bei Lebensmittel- und Getränkeherstellern und in Forschungslaboren. Der Stoff scheint auch als Weichmacher verwendet zu werden.","主要用作制造农用化学品、药品和工业化学品的中间体。在法医实验室、医院、制药公司、食品和饮料制造商以及研究实验室中，较少用作质量控制的溶剂和实验室试剂。这种织物似乎也被用作增塑剂。"]
[null,{"$f":"IF($B$1=\"English\",C2561,IF($B$1=\"Deutsch\",D2561,IF($B$1=\"中文\",E2561,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as an intermediate in the production of dyes and other substances."},"Used as an intermediate in the production of dyes and other substances.","Wird als Zwischenprodukt bei der Herstellung von Farbstoffen und anderen Stoffen verwendet.","用作生产染料和其他物质的中间体。"]
[null,{"$f":"IF($B$1=\"English\",C2562,IF($B$1=\"Deutsch\",D2562,IF($B$1=\"中文\",E2562,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Broadly used, e.g. in glass and glass fibers, frits, ceramics, flame retardants, catalysts, industrial fluids, metallurgy, nuclear energy, electrical equipment, adhesives, paints/lacquers, film development solutions, detergents and cleaners, reagents, biocides and insecticides."},"Broadly used, e.g. in glass and glass fibers, frits, ceramics, flame retardants, catalysts, industrial fluids, metallurgy, nuclear energy, electrical equipment, adhesives, paints/lacquers, film development solutions, detergents and cleaners, reagents, biocides and insecticides.","Wird breit verwendet, z. B. in Glas und Glasfasern, Fritten, Keramik, Flammschutzmitteln, Katalysatoren, industriellen Flüssigkeiten, im Hüttenwesen, im Kernenergiebereich, in elektrischen Geräten, Klebstoffen, Farben/Lacken, Filmentwicklungslösungen, Wasch- und Reinigungsmitteln, Reagenzien, Bioziden und Insektiziden. ","广泛应用于玻璃和玻璃纤维、熔块、陶瓷、阻燃剂、催化剂、工业流体、冶金、核能、电气设备、粘合剂、油漆/清漆、薄膜显影溶液、洗涤剂和清洁剂、试剂、生物杀灭剂和杀虫剂。"]
[null,{"$f":"IF($B$1=\"English\",C2563,IF($B$1=\"Deutsch\",D2563,IF($B$1=\"中文\",E2563,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used in (electrolytic and electroless) electroplating processes for electronic components (such as printed circuit boards). The material also seems to be used for batteries for special applications."},"Mainly used in (electrolytic and electroless) electroplating processes for electronic components (such as printed circuit boards). The material also seems to be used for batteries for special applications.","Wird hauptsächlich bei (elektrolytischen und stromlosen) Galvanisierungsverfahren für elektronische Komponenten (wie Leiterplatten) verwendet. Der Stoff scheint auch für Batterien für spezielle Anwendungsgebiete verwendet zu werden. ","主要用于电子元件(如印刷电路板)的(电解和无电)电镀工艺。这种材料似乎也用于特殊用途的电池。"]
[null,{"$f":"IF($B$1=\"English\",C2564,IF($B$1=\"Deutsch\",D2564,IF($B$1=\"中文\",E2564,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used to formulate writing inks and potentially other inks and to dye a wide variety of materials."},"Used to formulate writing inks and potentially other inks and to dye a wide variety of materials.","Wird zur Formulierung von Schreibtinten und potenziell auch anderen Tinten sowie zum Färben verschiedenster Materialien verwendet.","用于配制书写油墨和其他潜在油墨，并对各种材料进行染色。"]
[null,{"$f":"IF($B$1=\"English\",C2565,IF($B$1=\"Deutsch\",D2565,IF($B$1=\"中文\",E2565,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as an intermediate in the production of triphenylmethane dyes and other substances. Other potential uses as an additive (photosensitizer) in paints and pigments, in dry film products and as a process chemical in the production of electronic circuit boards."},"Used as an intermediate in the production of triphenylmethane dyes and other substances. Other potential uses as an additive (photosensitizer) in paints and pigments, in dry film products and as a process chemical in the production of electronic circuit boards.","Wird als Zwischenprodukt bei der Herstellung von Triphenylmethanfarbstoffen und anderen Stoffen verwendet. Andere potenzielle Verwendungen als Zusatzstoff (Photosensibilisator) in Farben und Pigmenten, in Trockenfilmprodukten und als Prozesschemikalie bei der Produktion elektronischer Leiterplatten. ","用作生产三苯甲烷染料和其他物质的中间体。其他潜在用途包括在油漆和颜料、干膜产品中作为添加剂(光敏剂)，以及生产电子电路板时作为加工化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2566,IF($B$1=\"Deutsch\",D2566,IF($B$1=\"中文\",E2566,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used to formulate paints, detergents and coatings and to dye paper, packaging, textiles, plastic products and other types of products. Also used in diagnostic and analytical applications."},"Used to formulate paints, detergents and coatings and to dye paper, packaging, textiles, plastic products and other types of products. Also used in diagnostic and analytical applications.","Wird zur Formulierung von Farben, Reinigungsmitteln und Beschichtungen sowie zum Färben von Papier, Verpackungen, Textilien, Kunststoffprodukten und anderen Arten von Erzeugnissen verwendet. Findet auch in diagnostischen und analytischen Anwendungen Verwendung. ","用于配制油漆、洗涤剂和涂料，以及给纸张、包装、纺织品、塑料制品和其他类型的产品染色。也用于诊断和分析应用。"]
[null,{"$f":"IF($B$1=\"English\",C2567,IF($B$1=\"Deutsch\",D2567,IF($B$1=\"中文\",E2567,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used in paper dyeing and in inks in printer cartridges and ballpoint pens. Also used for dyeing dried flowers, as a marker to increase the visibility of liquids and for dyeing in microbiological and clinical laboratories."},"Mainly used in paper dyeing and in inks in printer cartridges and ballpoint pens. Also used for dyeing dried flowers, as a marker to increase the visibility of liquids and for dyeing in microbiological and clinical laboratories.","Wird hauptsächlich beim Papierfärben und in Tinten in Druckerpatronen und Kugelschreibern verwendet. Findet auch beim Färben von Trockenblumen, als Marker zur Erhöhung der Sichtbarkeit von Flüssigkeiten sowie beim Färben in mikrobiologischen und klinischen Labors Verwendung. ","主要用于纸张染色以及打印机墨盒和圆珠笔中的墨水。也用于干花染色，作为标记增加液体的可见度，并用于微生物和临床实验室的染色。"]
[null,{"$f":"IF($B$1=\"English\",C2568,IF($B$1=\"Deutsch\",D2568,IF($B$1=\"中文\",E2568,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used as a solvent or processing aid in the production and formulation of industrial chemicals. Less often used in brake fluids and for repairing motor vehicles."},"Mainly used as a solvent or processing aid in the production and formulation of industrial chemicals. Less often used in brake fluids and for repairing motor vehicles.","Wird hauptsächlich als Lösungsmittel oder als Verarbeitungshilfsstoff bei der Herstellung und Formulierung von Industriechemikalien verwendet. Seltener verwendet in Bremsflüssigkeiten und zur Reparatur von Motorfahrzeugen. ","主要用作工业化学品生产和配方中的溶剂或加工助剂。少用于制动液和汽车修理。"]
[null,{"$f":"IF($B$1=\"English\",C2569,IF($B$1=\"Deutsch\",D2569,IF($B$1=\"中文\",E2569,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used as a solvent or processing aid in the production and formulation of industrial chemicals and as an electrolyte solvent in lithium batteries."},"Mainly used as a solvent or processing aid in the production and formulation of industrial chemicals and as an electrolyte solvent in lithium batteries.","Wird hauptsächlich als Lösungsmittel oder als Verarbeitungshilfsstoff bei der Herstellung und Formulierung von Industriechemikalien sowie als Elektrolytlösemittel in Lithiumbatterien verwendet.","主要用作工业化学品生产和配方中的溶剂或加工助剂，以及锂电池中的电解质溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C2570,IF($B$1=\"Deutsch\",D2570,IF($B$1=\"中文\",E2570,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used as hardener in resins and coatings. Also used in coatings for the printed circuit board industry, electrical insulation materials, resin casting systems, composite boards, screen printing coatings, tools, adhesives, lining materials and stabilizers for plastics."},"Mainly used as hardener in resins and coatings. Also used in coatings for the printed circuit board industry, electrical insulation materials, resin casting systems, composite boards, screen printing coatings, tools, adhesives, lining materials and stabilizers for plastics.","Wird hauptsächlich als Härter in Harzen und Beschichtungen verwendet. Findet auch in Lacken für die Leiterplattenindustrie, Elektroisoliermaterial, Harzgusssystemen, Verbundplatten, Siebdruckbeschichtungen, Werkzeugen, Klebstoffen, Auskleidungsmaterial und Stabilisatoren für Kunststoffe Verwendung. ","主要用作树脂和涂料的硬化剂。也用于印刷电路板行业的涂料、电绝缘材料、树脂浇铸系统、复合板、丝网印刷涂料、工具、粘合剂、衬里材料和塑料稳定剂。"]
[null,{"$f":"IF($B$1=\"English\",C2571,IF($B$1=\"Deutsch\",D2571,IF($B$1=\"中文\",E2571,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly used as solder resist in the EU. Also used in electrical insulation materials, resin casting systems, composite panels, screen printing, coatings, tools, adhesives, lining materials and stabilizers for plastics. "},"Mainly used as solder resist in the EU. Also used in electrical insulation materials, resin casting systems, composite panels, screen printing, coatings, tools, adhesives, lining materials and stabilizers for plastics. ","Wird in der EU hauptsächlich als Lötstopplack verwendet. Findet auch in Elektroisoliermaterial, Harzgusssystemen, Verbundplatten, im Siebdruck, in Beschichtungen, Werkzeugen, Klebstoffen, Auskleidungsmaterial und Stabilisatoren für Kunststoffe Verwendung. ","在欧盟主要用作阻焊剂。也用于电绝缘材料、树脂浇铸系统、复合板、丝网印刷、涂料、工具、粘合剂、衬里材料和塑料稳定剂。"]
[null,{"$f":"IF($B$1=\"English\",C2572,IF($B$1=\"Deutsch\",D2572,IF($B$1=\"中文\",E2572,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"It is mainly used for formulating printing inks and writing inks, for dyeing paper and in mixtures, such as windscreen washes. "},"It is mainly used for formulating printing inks and writing inks, for dyeing paper and in mixtures, such as windscreen washes. ","  Wird hauptsächlich zur Formulierung von Druckfarben und Schreibtinten, zum Färben von Papier und in Gemischen, wie beispielsweise Scheibenwaschmitteln, verwendet. ","主要用于配制印刷油墨和书写油墨，用于纸张染色和混合，如挡风玻璃清洗。 "]
[null,{"$f":"IF($B$1=\"English\",C2573,IF($B$1=\"Deutsch\",D2573,IF($B$1=\"中文\",E2573,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of polyester and alkyd resins and plasticizers for thermoplastic polymers. The anhydrides are also used as curing agents for epoxy resins and chain crosslinkers for thermoplastic polymers."},"Production of polyester and alkyd resins and plasticizers for thermoplastic polymers. The anhydrides are also used as curing agents for epoxy resins and chain crosslinkers for thermoplastic polymers.","Herstellung von Polyester und Alkydharzen sowie Weichmachern für thermoplastische Polymere. Die Anhydride werden auch als Härter für Epoxidharze und Kettenvernetzer für thermoplastische Polymere verwendet.","聚酯和醇酸树脂以及热塑性聚合物增塑剂的生产。酸酐也用作环氧树脂的固化剂和热塑性聚合物的链交联剂。"]
[null,{"$f":"IF($B$1=\"English\",C2574,IF($B$1=\"Deutsch\",D2574,IF($B$1=\"中文\",E2574,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of PVC; Use in plastic products"},"Production of PVC; Use in plastic products","Herstellung von PVC;\nVerwendung in Kunststofferzeugnissen ","聚氯乙烯生产；用于塑料产品"]
[null,{"$f":"IF($B$1=\"English\",C2575,IF($B$1=\"Deutsch\",D2575,IF($B$1=\"中文\",E2575,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use in coatings, paints, thinners, paint removers, inks and toners "},"Use in coatings, paints, thinners, paint removers, inks and toners ","Verwendung in Beschichtungsmitteln, Farben, Verdünnern, Farbentfernern, Tinten und Tonern ","用于涂料、油漆、稀释剂、脱漆剂、油墨和调色剂"]
[null,{"$f":"IF($B$1=\"English\",C2576,IF($B$1=\"Deutsch\",D2576,IF($B$1=\"中文\",E2576,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of PVC; Use of lead reinforced plastic materials in building interiors "},"Production of PVC; Use of lead reinforced plastic materials in building interiors ","Herstellung von PVC;\nVerwendung von bleiverstärkten Kunststoffmaterialien in Gebäudeinnenteilen ","聚氯乙烯生产；铅增强塑料材料在建筑内部的应用"]
[null,{"$f":"IF($B$1=\"English\",C2577,IF($B$1=\"Deutsch\",D2577,IF($B$1=\"中文\",E2577,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of PVC; Use in plastic products and in electric batteries and accumulators "},"Production of PVC; Use in plastic products and in electric batteries and accumulators ","Herstellung von PVC;\nVerwendung in Kunststofferzeugnissen sowie in elektrischen Batterien und Akkumulatoren ","聚氯乙烯生产；用于塑料制品、电池和蓄电池"]
[null,{"$f":"IF($B$1=\"English\",C2578,IF($B$1=\"Deutsch\",D2578,IF($B$1=\"中文\",E2578,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fuel additives and fuel mixtures "},"Fuel additives and fuel mixtures ","Kraftstoffzusätze und Kraftstoffmischungen ","燃料添加剂和燃料混合物"]
[null,{"$f":"IF($B$1=\"English\",C2579,IF($B$1=\"Deutsch\",D2579,IF($B$1=\"中文\",E2579,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of PTC ceramics "},"Production of PTC ceramics ","Herstellung von PTC-Keramik ","PTC陶瓷的生产"]
[null,{"$f":"IF($B$1=\"English\",C2580,IF($B$1=\"Deutsch\",D2580,IF($B$1=\"中文\",E2580,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products"},"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products","Herstellung von fluorierten Polymeren und fluorierten Telomeren;\nZusatzstoff und Komponente in Verbraucher- und Industrieprodukten","氟化聚合物和氟化调聚物的制备；\n消费品和工业产品中的添加剂和成分"]
[null,{"$f":"IF($B$1=\"English\",C2581,IF($B$1=\"Deutsch\",D2581,IF($B$1=\"中文\",E2581,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate and laboratory reagent"},"Intermediate and laboratory reagent","Zwischenprodukt und Laborreagenz","中间体和实验室试剂"]
[null,{"$f":"IF($B$1=\"English\",C2582,IF($B$1=\"Deutsch\",D2582,IF($B$1=\"中文\",E2582,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizers in plastics "},"Plasticizers in plastics ","Weichmacher in Kunststoffen ","塑料中的增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C2583,IF($B$1=\"Deutsch\",D2583,IF($B$1=\"中文\",E2583,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No information available "},"No information available ","Es liegen keine Angaben vor ","无可用信息"]
[null,{"$f":"IF($B$1=\"English\",C2584,IF($B$1=\"Deutsch\",D2584,IF($B$1=\"中文\",E2584,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of lead-acid batteries;\nProduction of crystal glass and ceramics;\nProduction of rubber protection;\nExplosives production;\nUsed to repair televisions,\ncomputer monitors and other devices with cathode ray tubes;\nUse in adsorbents, paints and pigments"},"Production of lead-acid batteries;\nProduction of crystal glass and ceramics;\nProduction of rubber protection;\nExplosives production;\nUsed to repair televisions,\ncomputer monitors and other devices with cathode ray tubes;\nUse in adsorbents, paints and pigments","Herstellung von Blei-Säure-Batterien;\nHerstellung von Kristallglas und Keramik;\nHerstellung von Gummischutz;\nSprengstoffherstellung;\nVerwendung bei der Reparatur von Fernsehgeräten,\nComputermonitoren und anderen Geräten mit Kathodenstrahlröhren;\nVerwendung in Adsorptionsmitteln, Farben und Pigmenten","生产铅酸电池；\n生产水晶玻璃和陶瓷；\n生产橡胶保护；\n生产炸药；\n用于修理电视，\n带有阴极射线管的计算机显示器和其他设备；\n用于吸附剂、油漆和颜料"]
[null,{"$f":"IF($B$1=\"English\",C2585,IF($B$1=\"Deutsch\",D2585,IF($B$1=\"中文\",E2585,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate and laboratory reagent"},"Intermediate and laboratory reagent","Zwischenprodukt und Laborreagenz","中间体和实验室试剂"]
[null,{"$f":"IF($B$1=\"English\",C2586,IF($B$1=\"Deutsch\",D2586,IF($B$1=\"中文\",E2586,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of plastic products;\nUse in electric batteries and accumulators;\nUse of lead-reinforced plastic materials in building interiors"},"Production of plastic products;\nUse in electric batteries and accumulators;\nUse of lead-reinforced plastic materials in building interiors","Herstellung von Kunststoffprodukten;\nVerwendung in elektrischen Batterien und Akkumulatoren;\nVerwendung von bleiverstärkten Kunststoffmaterialien in Gebäudeinnenteilen","生产塑料产品；\n用于电池和蓄电池；\n铅增强塑料材料在建筑内部的应用"]
[null,{"$f":"IF($B$1=\"English\",C2587,IF($B$1=\"Deutsch\",D2587,IF($B$1=\"中文\",E2587,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizers in PVC, sealants and printing inks"},"Plasticizers in PVC, sealants and printing inks","Weichmacher in PVC, in Dichtungsmitteln und Druckfarben","聚氯乙烯、密封剂和印刷油墨中的增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C2588,IF($B$1=\"Deutsch\",D2588,IF($B$1=\"中文\",E2588,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of plastic products, including compounding and conversion;\nmanufacture of bulk chemicals (including petroleum products)"},"Production of plastic products, including compounding and conversion;\nmanufacture of bulk chemicals (including petroleum products)","Herstellung von Kunststoffprodukten, einschließlich Compoundierung und Konversion;\nHerstellung von Massenchemikalien (einschließlich Mineralölprodukten)","塑料产品的生产，包括复合和转化；\n散装化学品(包括石油产品)的制造"]
[null,{"$f":"IF($B$1=\"English\",C2589,IF($B$1=\"Deutsch\",D2589,IF($B$1=\"中文\",E2589,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of plastic products, including compounding and conversion;\nUse of lead-reinforced plastic materials in building interiors"},"Production of plastic products, including compounding and conversion;\nUse of lead-reinforced plastic materials in building interiors","Herstellung von Kunststoffprodukten, einschließlich Compoundierung und Konversion;\nVerwendung von bleiverstärkten Kunststoffmaterialien in Gebäudeinnenteilen","塑料产品的生产，包括复合和转化；\n铅增强塑料材料在建筑内部的应用"]
[null,{"$f":"IF($B$1=\"English\",C2590,IF($B$1=\"Deutsch\",D2590,IF($B$1=\"中文\",E2590,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of fine chemicals;\nManufacture of computers, electronic and optical products;\nUse as laboratory reagent and intermediate"},"Production of fine chemicals;\nManufacture of computers, electronic and optical products;\nUse as laboratory reagent and intermediate","Herstellung von Feinchemikalien;\nHerstellung von Computern, elektronischen und optischen Produkten;\nVerwendung als Laborreagenz und Zwischenprodukt","精细化学品生产；\n计算机、电子和光学产品的制造；\n用作实验室试剂和中间体"]
[null,{"$f":"IF($B$1=\"English\",C2591,IF($B$1=\"Deutsch\",D2591,IF($B$1=\"中文\",E2591,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of plastic products, including compounding and conversion;\nUse of lead reinforced plastic materials in building interiors"},"Production of plastic products, including compounding and conversion;\nUse of lead reinforced plastic materials in building interiors","Herstellung von Kunststoffprodukten, einschließlich Compoundierung und Konversion;\nVerwendung von bleiverstärkten Kunststoffmaterialien in Gebäudeinnenteilen ","塑料产品的生产，包括复合和转化；\n铅增强塑料材料在建筑内部的应用"]
[null,{"$f":"IF($B$1=\"English\",C2592,IF($B$1=\"Deutsch\",D2592,IF($B$1=\"中文\",E2592,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No information available"},"No information available","Es liegen keine Angaben vor ","无可用信息"]
[null,{"$f":"IF($B$1=\"English\",C2593,IF($B$1=\"Deutsch\",D2593,IF($B$1=\"中文\",E2593,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products"},"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products","Herstellung von fluorierten Polymeren und fluorierten Telomeren;\nZusatzstoff und Komponente in Verbraucher- und Industrieprodukten ","氟化聚合物和氟化调聚物的制备；\n消费品和工业产品中的添加剂和成分"]
[null,{"$f":"IF($B$1=\"English\",C2594,IF($B$1=\"Deutsch\",D2594,IF($B$1=\"中文\",E2594,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products"},"Preparation of fluorinated polymers and fluorinated telomers;\nAdditives and components in consumer and industrial products","Herstellung von fluorierten Polymeren und fluorierten Telomeren;\nZusatzstoff und Komponente in Verbraucher- und Industrieprodukten ","氟化聚合物和氟化调聚物的制备；\n消费品和工业产品中的添加剂和成分"]
[null,{"$f":"IF($B$1=\"English\",C2595,IF($B$1=\"Deutsch\",D2595,IF($B$1=\"中文\",E2595,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Stone, gypsum, cement, glass and ceramic products"},"Stone, gypsum, cement, glass and ceramic products","Stein-, Gips-, Zement-, Glas- und Keramikerzeugnisse ","石材、石膏、水泥、玻璃和陶瓷产品"]
[null,{"$f":"IF($B$1=\"English\",C2596,IF($B$1=\"Deutsch\",D2596,IF($B$1=\"中文\",E2596,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For coating glass bulbs;\nFormulation (mixing) of mixtures and/or new packaging"},"For coating glass bulbs;\nFormulation (mixing) of mixtures and/or new packaging","Zur Beschichtung von Glaslampenkolben;\nFormulierung (Mischen) von Gemischen und/oder Neuverpackungen ","用于涂覆玻璃灯泡；\n混合物和/或新包装的配方(混合)"]
[null,{"$f":"IF($B$1=\"English\",C2597,IF($B$1=\"Deutsch\",D2597,IF($B$1=\"中文\",E2597,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of chemicals and chemical products for industrial use;\nProduction of cleaning agents or detergents;\nManufacture of food products, manufacture of fabricated metal products.\n\nDisinfectants (for private use), corrosive descaling agents, including products for ovens and stoves, disinfectants for use on surfaces in contact with food, industrial cleaning agents for ultrafiltration membranes or reverse osmosis, cleaning agents for floors and walls in the industrial sector, cleaning agents for wheels and tyres, pH regulator, corrosion inhibitors.>br>\nBasic chemical for the production of biocides.\n\nAdditives for motor fuels, bleaching agents for housings, cationic electrocoating, etching liquids, pesticides."},"Manufacture of chemicals and chemical products for industrial use;\nProduction of cleaning agents or detergents;\nManufacture of food products, manufacture of fabricated metal products.\n\nDisinfectants (for private use), corrosive descaling agents, including products for ovens and stoves, disinfectants for use on surfaces in contact with food, industrial cleaning agents for ultrafiltration membranes or reverse osmosis, cleaning agents for floors and walls in the industrial sector, cleaning agents for wheels and tyres, pH regulator, corrosion inhibitors.>br>\nBasic chemical for the production of biocides.\n\nAdditives for motor fuels, bleaching agents for housings, cationic electrocoating, etching liquids, pesticides.","Herstellung von Chemikalien und chemischen Produkten für industrielle Zwecke;\nHerstellung von Reinigungs- oder Waschmittel;\nHerstellung von Nahrungsmitteln, Herstellung von Metallerzeugnissen.\n\nDesinfektionsmittel (für private Zwecke), korrosive Entkalkungsmittel, einschließlich Produkte für Öfen und Herde, Desinfektionsmittel zur Verwendung auf Oberflächen im Kontakt mit Lebensmitteln, industrielles Reinigungsmittel für Ultrafiltrationsmembranen oder Umkehrosmose, Reinigungsmittel für Böden und Wände im industriellen Bereich, Reinigungsmittel für Räder und Reifen, pH-Regulator, Korrosionsschutzmittel.>br>\nBasischemikalie zur Herstellung von Bioziden.\n\nZusatzstoffe für Motorenkraftstoffe, Bleichmittel für Gehäuse, kationische Elektrobeschichtung, Ätzflüssigkeiten, Schädlingsbekämpfungsmittel.","工业用化学品和化学产品的制造；\n清洁剂的生产；\n食品制造，金属制品制造。\n\n消毒剂(私人使用)、腐蚀性除垢剂，包括烤箱和炉灶产品、用于接触食物表面的消毒剂、用于超滤膜或反渗透的工业清洁剂、工业部门地板和墙壁清洁剂、车轮和轮胎清洁剂、酸碱度调节剂、缓蚀剂。> br >\n生产生物杀灭剂的基本化学品。\n\n发动机燃料添加剂、外壳漂白剂、阳离子电泳涂料、蚀刻液、杀虫剂。"]
[null,{"$f":"IF($B$1=\"English\",C2598,IF($B$1=\"Deutsch\",D2598,IF($B$1=\"中文\",E2598,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate for the production of propylene oxide;\nCellulose modifier;\nApplications in coatings;\nLubricant;\nUse as fuel;\nAgrochemical use;\nDetergent;\nDe-icing and antifreeze;\nfunctional fluid;\nWater treatment chemicals"},"Intermediate for the production of propylene oxide;\nCellulose modifier;\nApplications in coatings;\nLubricant;\nUse as fuel;\nAgrochemical use;\nDetergent;\nDe-icing and antifreeze;\nfunctional fluid;\nWater treatment chemicals","Zwischenprodukt für die Herstellung von Propylenoxid;\nZellulose-Modifikator;\nVerwendungen in Beschichtungen;\nSchmiermittel;\nVerwendung als Kraftstoff;\nAgrochemische Verwendung;\nReinigungsmittel;\nEnteisungs- und Frostschutzamittel;\nFunktionsflüssigkeit;\nChemikalien zur Wasserbehandlung ","生产环氧丙烷的中间体；\n纤维素改性剂；\n涂料中的应用；\n润滑剂；\n用作燃料；\n农用化学品的使用；\n洗涤剂；\n除冰和防冻；\n功能流体；\n水处理化学品"]
[null,{"$f":"IF($B$1=\"English\",C2599,IF($B$1=\"Deutsch\",D2599,IF($B$1=\"中文\",E2599,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of synthetic/artificial leather in polyurethane;\nProduction of printed circuit boards in the electronics sector;\nReagent and catalyst for syntheses in organic chemistry;\nSolvents in syntheses and for crystallization in the pharmaceutical industry;\nCleaning solution in the textile industry;\nSelective absorption (e.g. acetylene extraction in ethylene streams);\nManufacture of electrical distributors and circuits"},"Production of synthetic/artificial leather in polyurethane;\nProduction of printed circuit boards in the electronics sector;\nReagent and catalyst for syntheses in organic chemistry;\nSolvents in syntheses and for crystallization in the pharmaceutical industry;\nCleaning solution in the textile industry;\nSelective absorption (e.g. acetylene extraction in ethylene streams);\nManufacture of electrical distributors and circuits","Fertigung von synthetischem/künstlichem Leder aus Polyurethan;\nHerstellung von Leiterplatten im Elektronikbereich;\nReagenz und Katalysator für Synthesen in der organischen Chemie;\nLösemittel in Synthesen und zur Kristallisierung in der Pharmaindustrie;\nReinigungslösung in der Textilindustrie;\nSelektive Absorption (z. B. Acetylenextraktion in Ethenströmen);\nHerstellung von elektrischen Verteilern und Schaltkreisen ","生产聚氨酯合成革/人造革；\n生产电子产业中的印刷电路板；\n有机化学合成用试剂和催化剂；\n制药工业中合成和结晶用的溶剂；\n纺织行业的清洗液；\n选择性吸收(例如乙烯流中的乙炔萃取)；\n配电装置和电路的制造"]
[null,{"$f":"IF($B$1=\"English\",C2600,IF($B$1=\"Deutsch\",D2600,IF($B$1=\"中文\",E2600,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizers and surface conditioners in fuels;\nPlasticizers for plastics"},"Plasticizers and surface conditioners in fuels;\nPlasticizers for plastics","Weichmacher und Oberflächenkonditionierer in Treibstoffen;\nWeichmacher für Kunststoffe ","燃料中的增塑剂和表面调节剂；\n塑料增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C2601,IF($B$1=\"Deutsch\",D2601,IF($B$1=\"中文\",E2601,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate product as methylating agent"},"Intermediate product as methylating agent","Zwischenprodukt als Methylierungsmittel","作为甲基化试剂的中间产物"]
[null,{"$f":"IF($B$1=\"English\",C2602,IF($B$1=\"Deutsch\",D2602,IF($B$1=\"中文\",E2602,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of plastic products, including compounding and conversion"},"Production of plastic products, including compounding and conversion","Herstellung von Kunststoffprodukten, einschließlich Compoundierung und Konversion ","塑料产品的生产，包括复合和转化"]
[null,{"$f":"IF($B$1=\"English\",C2603,IF($B$1=\"Deutsch\",D2603,IF($B$1=\"中文\",E2603,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Semiconductors in machines, apparatus and mechanical devices as well as electrical/electronic products"},"Semiconductors in machines, apparatus and mechanical devices as well as electrical/electronic products","Halbleiter in Maschinen, Apparaten und mechanischen Geräten sowie elektrischen/elektronischen Erzeugnissen ","机器、仪器和机械设备以及电气/电子产品中的半导体"]
[null,{"$f":"IF($B$1=\"English\",C2604,IF($B$1=\"Deutsch\",D2604,IF($B$1=\"中文\",E2604,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of computers, electronic and optical products, intermediate products"},"Manufacture of computers, electronic and optical products, intermediate products","Herstellung von Computern, elektronischen und optischen Produkten, Zwischenprodukt ","计算机、电子和光学产品、中间产品的制造"]
[null,{"$f":"IF($B$1=\"English\",C2605,IF($B$1=\"Deutsch\",D2605,IF($B$1=\"中文\",E2605,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Industrial use: Hardener for epoxy resins, intermediate in chemical synthesis or chemical process, monomer in the production of resins;\nCyclohexane-1,2-dicarboxylic anhydride (HHPA): Preparation of alkyd resins, plasticizers, insect repellents, rust inhibitors"},"Industrial use: Hardener for epoxy resins, intermediate in chemical synthesis or chemical process, monomer in the production of resins;\nCyclohexane-1,2-dicarboxylic anhydride (HHPA): Preparation of alkyd resins, plasticizers, insect repellents, rust inhibitors","Industrielle Verwendung: Härter für Epoxidharze, Zwischenprodukt bei der chemischen Synthese oder beim chemischen Prozess, Monomer bei der Herstellung von Harzen;\nCyclohexan-1,2-dicarbonsäureanhydrid (HHPA): Herstellung von Alkydharzen, Weichmachern, Insektenschutzmitteln, Rostinhibitoren","工业用途：环氧树脂的固化剂，化学合成或化学工艺中的中间体，生产树脂的单体。\n环己烷-1,2-二羧酸酐（HHPA）：醇酸树脂的制备、增塑剂、驱虫剂、防锈剂"]
[null,{"$f":"IF($B$1=\"English\",C2606,IF($B$1=\"Deutsch\",D2606,IF($B$1=\"中文\",E2606,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"blowing agent, aging and bleaching agent, foaming agent, catalyst, insulating material, building material, cement filler, dye, additive, bleaching agent in photography"},"blowing agent, aging and bleaching agent, foaming agent, catalyst, insulating material, building material, cement filler, dye, additive, bleaching agent in photography","Blähmittel, Alterungs- und Bleichmittel, Schäumungsmittel, Katalysator, Isoliermaterial, Baumaterial, Zementfüller, Farbstoff, Zusatzstoff, Bleichmittel bei der Fotografie ","发泡剂、老化和漂白剂、发泡剂、催化剂、绝缘材料、建筑材料、水泥填料、染料、添加剂、摄影漂白剂"]
[null,{"$f":"IF($B$1=\"English\",C2607,IF($B$1=\"Deutsch\",D2607,IF($B$1=\"中文\",E2607,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Additive in rubber, stabilizer in PVC plastics, catalyst in the production of polyurethanes and silicones; use in insulations and coatings, food packaging, T-shirts, polyurethane gloves, sanitary towels, medical devices, cellophane packaging and soft toys, PVC plastics (water pipes, packaging material, textile products), silicone rubber (sealants, dental products, paper coatings), polyurethanes (foams)."},"Additive in rubber, stabilizer in PVC plastics, catalyst in the production of polyurethanes and silicones; use in insulations and coatings, food packaging, T-shirts, polyurethane gloves, sanitary towels, medical devices, cellophane packaging and soft toys, PVC plastics (water pipes, packaging material, textile products), silicone rubber (sealants, dental products, paper coatings), polyurethanes (foams).","  Zusatzstoff in Kautschuk, Stabilisator in PVC-Kunststoffen, Katalysator bei der Herstellung von Polyurethanen und Silikonen;Verwendung in Isolierungen und Beschichtungen, Lebensmittelverpackungen, T-Shirts, Polyurethan-Handschuhen, Hygienebinden, medizinischen Geräten, Cellophan-Verpackungen und Plüschtieren, PVC-Kunststoffen (Wasserleitungen, Verpackungsmaterial, Textilprodukte), Silikonkautschuk (Dichtungsmittel, Dentalprodukte, Papierbeschichtungen), Polyurethanen (Schaumkunststoffe, Kleb-/Dichtstoffe), Glas (Beschichtungen), Isolierungen in elektronischen Erzeugnissen und Kabeln, Entwurmungsmitteln für Geflügel ","橡胶中的添加剂、聚氯乙烯塑料中的稳定剂、聚氨酯和硅酮生产中的催化剂；用于绝缘和涂料、食品包装、t恤、聚氨酯手套、卫生巾、医疗器械、玻璃纸包装和毛绒玩具、聚氯乙烯塑料(水管、包装材料、纺织品)、硅橡胶(密封剂、牙科产品、纸涂层)、聚氨酯(泡沫)。"]
[null,{"$f":"IF($B$1=\"English\",C2608,IF($B$1=\"Deutsch\",D2608,IF($B$1=\"中文\",E2608,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Production of fine chemicals;\nReactant in polymer synthesis;\nIntermediate product as methylating agent"},"Production of fine chemicals;\nReactant in polymer synthesis;\nIntermediate product as methylating agent","Herstellung von Feinchemikalien;\nReaktant bei der Polymersynthese;\nZwischenprodukt als Methylierungsmittel","精细化学品生产；\n聚合物合成中的反应物；\n作为甲基化试剂的中间产物"]
[null,{"$f":"IF($B$1=\"English\",C2609,IF($B$1=\"Deutsch\",D2609,IF($B$1=\"中文\",E2609,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Additive in flame retardants, plastics/polymers and textiles"},"Additive in flame retardants, plastics/polymers and textiles","Additiv in Flammschutzmitteln, Kunststoffen/Polymeren und Textilien","阻燃剂、塑料/聚合物和纺织品中的添加剂"]
[null,{"$f":"IF($B$1=\"English\",C2610,IF($B$1=\"Deutsch\",D2610,IF($B$1=\"中文\",E2610,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use with automated and manual electrolytic lead plating"},"Use with automated and manual electrolytic lead plating","Verwendung bei automatisiertem und manuellem elektrolytischen Verbleien","与自动和手动电镀铅一起使用"]
[null,{"$f":"IF($B$1=\"English\",C2611,IF($B$1=\"Deutsch\",D2611,IF($B$1=\"中文\",E2611,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No information available "},"No information available ","Es liegen keine Angaben vor ","无可用信息 "]
[null,{"$f":"IF($B$1=\"English\",C2612,IF($B$1=\"Deutsch\",D2612,IF($B$1=\"中文\",E2612,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of explosives;Manufacture of lead nitrate;Manufacture of weapons and ammunition;\nProduction of pigments and fine chemicals;\nUse in coatings, paints, thinners, paint removers, fillers, fillers, fillers, mortar, modelling clay, finger paints;\nIntermediate;\nlaboratory chemicals "},"Manufacture of explosives;Manufacture of lead nitrate;Manufacture of weapons and ammunition;\nProduction of pigments and fine chemicals;\nUse in coatings, paints, thinners, paint removers, fillers, fillers, fillers, mortar, modelling clay, finger paints;\nIntermediate;\nlaboratory chemicals ","  Herstellung von Sprengstoffen;Herstellung von Bleidinitrat;Herstellung von Waffen und Munition;\nHerstellung von Pigmenten und Feinchemikalien;\nVerwendung in Beschichtungsmitteln, Farben, Verdünnern, Farbentfernern, Füllstoffen, Spachtelmassen, Mörtel, Modellierton, Fingerfarben;\nZwischenprodukt;\nLaborchemikalien ","爆炸物制造；硝酸铅的制造；制造武器和弹药；\n颜料和精细化学品的生产；\n用于涂料、油漆、稀释剂、脱漆剂、填料、填充剂、砂浆、造型粘土、指纹漆；\n中间物质；\n实验室化学品"]
[null,{"$f":"IF($B$1=\"English\",C2613,IF($B$1=\"Deutsch\",D2613,IF($B$1=\"中文\",E2613,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use for the production of lead oxide; production of lead-acid batteries;\nProduction of crystal glass and ceramics;\nProduction of rubber protection;\nExplosives production;\nUse as intermediate product"},"Use for the production of lead oxide; production of lead-acid batteries;\nProduction of crystal glass and ceramics;\nProduction of rubber protection;\nExplosives production;\nUse as intermediate product","Verwendung zur Herstellung von Bleioxid;Herstellung von Blei-Säure-Batterien;\nHerstellung von Kristallglas und Keramik;\nHerstellung von Gummischutz;\nSprengstoffherstellung;\nVerwendung als Zwischenprodukt ","用于生产氧化铅；生产铅酸电池；\n生产水晶玻璃和陶瓷；\n生产橡胶保护；\n生产炸药；\n用作中间产品"]
[null,{"$f":"IF($B$1=\"English\",C2614,IF($B$1=\"Deutsch\",D2614,IF($B$1=\"中文\",E2614,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No information available "},"No information available ","Es liegen keine Angaben vor ","无可用信息"]
[null,{"$f":"IF($B$1=\"English\",C2615,IF($B$1=\"Deutsch\",D2615,IF($B$1=\"中文\",E2615,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"intermediate "},"intermediate ","Zwischenprodukt ","中间物质"]
[null,{"$f":"IF($B$1=\"English\",C2616,IF($B$1=\"Deutsch\",D2616,IF($B$1=\"中文\",E2616,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"intermediate"},"intermediate","Zwischenprodukt ","中间物质"]
[null,{"$f":"IF($B$1=\"English\",C2617,IF($B$1=\"Deutsch\",D2617,IF($B$1=\"中文\",E2617,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Emulsifier for emulsion polymerization;\nTextile and leather auxiliaries;\nPesticide formulations;\nVeterinary products;\nWater-based paints\nIntermediate for the preparation of octylphenol ether sulfates;\nIn the construction industry\nas a pore generator/foaming agent for concrete;\nas mould release agent on building sites and in the production of precast concrete parts as well as an aid for the cleaning of machines;\nas a component (emulsifier) of bitumen/wax emulsions for painting/sealing in the construction industry or when covering concrete surfaces;\n\nas metalworking fluids;\nas oil for lubrication or for hydraulic equipment"},"Emulsifier for emulsion polymerization;\nTextile and leather auxiliaries;\nPesticide formulations;\nVeterinary products;\nWater-based paints\nIntermediate for the preparation of octylphenol ether sulfates;\nIn the construction industry\nas a pore generator/foaming agent for concrete;\nas mould release agent on building sites and in the production of precast concrete parts as well as an aid for the cleaning of machines;\nas a component (emulsifier) of bitumen/wax emulsions for painting/sealing in the construction industry or when covering concrete surfaces;\n\nas metalworking fluids;\nas oil for lubrication or for hydraulic equipment","Emulgator für Emulsionspolymerisation;\nTextil- und Lederhilfsmittel;\nPestizidformulierungen;\nVeterinärmedizinische Produkte;\nWasserbasierte Anstrichfarben\nZwischenprodukt für die Herstellung von Octylphenolethersulfaten;\nIn der Bauindustrie\n\n    als Porenbildner/Schäumungsmittel für Beton;\n    als Formentrennmittel auf Baustellen und bei der Betonfertigteilherstellung sowie als Hilfsmittel für das Reinigen von Maschinen;\n    als Bestandteil (Emulgator) von Bitumen-/Wachsemulsionen zum Anstrich/Abdichten in der Bauindustrie bzw. beim Abdecken von Betonoberflächen;\n\nals Metallbearbeitungsflüssigkeiten;\nals Öl zur Schmierung oder für hydraulische Geräte","乳液聚合用乳化剂；\n纺织和皮革助剂；\n农药制剂；\n兽医产品；\n水性涂料\n制备辛基酚醚硫酸盐的中间体；\n在建筑行业\n作为混凝土的造孔剂/起泡剂；\n作为建筑工地和预制混凝土部件生产中的脱模剂，以及作为机器清洗的助剂；\n作为沥青/蜡乳液的组分(乳化剂),用于建筑行业的油漆/密封或覆盖混凝土表面；\n\n作为金属加工液；\n作为润滑油或液压设备的油"]
[null,{"$f":"IF($B$1=\"English\",C2618,IF($B$1=\"Deutsch\",D2618,IF($B$1=\"中文\",E2618,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"intermediate "},"intermediate ","Zwischenprodukt ","中间物质"]
[null,{"$f":"IF($B$1=\"English\",C2619,IF($B$1=\"Deutsch\",D2619,IF($B$1=\"中文\",E2619,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No information available "},"No information available ","Es liegen keine Angaben vor ","无可用信息"]
[null,{"$f":"IF($B$1=\"English\",C2620,IF($B$1=\"Deutsch\",D2620,IF($B$1=\"中文\",E2620,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate product in the production of sulfur dyes "},"Intermediate product in the production of sulfur dyes ","Zwischenprodukt bei der Herstellung von Schwefelfarbstoffen ","硫化染料生产的中间产品"]
[null,{"$f":"IF($B$1=\"English\",C2621,IF($B$1=\"Deutsch\",D2621,IF($B$1=\"中文\",E2621,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Industrial application of coatings or inks;\nAdhesives for the production of tires and rubber products;\nIntermediate in the production of ethoxylates and plastic stabilizer;\nFormulation of adhesives, paints "},"Industrial application of coatings or inks;\nAdhesives for the production of tires and rubber products;\nIntermediate in the production of ethoxylates and plastic stabilizer;\nFormulation of adhesives, paints ","Industrielle Anwendung von Beschichtungen oder Tinten;\nHaftkleber bei der Herstellung von Reifen und Gummiprodukten;\nZwischenprodukt bei der Herstellung von Ethoxylaten und Kunststoffstabilisator;\nFormulierung von Klebstoffen, Anstrichfarben ","涂料或油墨的工业应用；\n轮胎和橡胶产品生产用粘合剂；\n乙氧基化物和塑料稳定剂生产的中间体；\n粘合剂、油漆的配方"]
[null,{"$f":"IF($B$1=\"English\",C2622,IF($B$1=\"Deutsch\",D2622,IF($B$1=\"中文\",E2622,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"intermediate"},"intermediate","Zwischenprodukt ","中间物质"]
[null,{"$f":"IF($B$1=\"English\",C2623,IF($B$1=\"Deutsch\",D2623,IF($B$1=\"中文\",E2623,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of plastic products, including compounding and conversion; use of lead reinforced plastic materials in building interiors "},"Manufacture of plastic products, including compounding and conversion; use of lead reinforced plastic materials in building interiors ","Herstellung von Kunststoffprodukten, einschließlich Compoundierung und Konversion; Verwendung von bleiverstärkten Kunststoffmaterialien in Gebäudeinnenteilen ","塑料产品的制造，包括复合和转化；铅增强塑料材料在建筑内部的应用"]
[null,{"$f":"IF($B$1=\"English\",C2624,IF($B$1=\"Deutsch\",D2624,IF($B$1=\"中文\",E2624,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Laboratory chemical for analytical purposes "},"Laboratory chemical for analytical purposes ","Laborchemikalie für analytische Zwecke ","分析用途的实验室化学品"]
[null,{"$f":"IF($B$1=\"English\",C2625,IF($B$1=\"Deutsch\",D2625,IF($B$1=\"中文\",E2625,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvents in various formulations such as paints, inks and cleaning fluids;\nUse for glycol ethers, including hydraulic and brake fluids, antifreeze and chemical intermediates"},"Solvents in various formulations such as paints, inks and cleaning fluids;\nUse for glycol ethers, including hydraulic and brake fluids, antifreeze and chemical intermediates","Lösemittel in verschiedenen Formulierungen wie Anstrichfarben, Tinten und Reinigungsflüssigkeiten;\nVerwendung für Glykolether, einschließlich Hydraulik- und Bremsflüssigkeiten, Frostschutzmittel und chemische Zwischenprodukte ","各种配方中的溶剂，如油漆、油墨和清洗液；\n用于乙二醇醚，包括液压油和制动液、防冻剂和化学中间体"]
[null,{"$f":"IF($B$1=\"English\",C2626,IF($B$1=\"Deutsch\",D2626,IF($B$1=\"中文\",E2626,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of bulk chemicals (including petroleum products); industrial solvent for steam degreasing "},"Manufacture of bulk chemicals (including petroleum products); industrial solvent for steam degreasing ","Herstellung von Massenchemikalien (einschließlich Mineralölprodukten); industrielles Lösemittel für Dampfentfettung ","批量化学品(包括石油产品)的制造；蒸汽脱脂用工业溶剂"]
[null,{"$f":"IF($B$1=\"English\",C2627,IF($B$1=\"Deutsch\",D2627,IF($B$1=\"中文\",E2627,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PFOA is used as a process aid in the production of fluoropolymers. These are used in various industries, such as textiles, the paper industry and electroplating.\nMany products contain residues of PFOA such as textiles, carpets, upholstered furniture, paper, leather, printing ink, cleaning and care products for carpets, sealants, floor wax, paints, impregnating agents, fire-fighting foam, surface-treated carpeting and ski wax. PFOA is also found as an impurity in perfluorooctylsulfonyl fluoride (POSF) based substances."},"PFOA is used as a process aid in the production of fluoropolymers. These are used in various industries, such as textiles, the paper industry and electroplating.\nMany products contain residues of PFOA such as textiles, carpets, upholstered furniture, paper, leather, printing ink, cleaning and care products for carpets, sealants, floor wax, paints, impregnating agents, fire-fighting foam, surface-treated carpeting and ski wax. PFOA is also found as an impurity in perfluorooctylsulfonyl fluoride (POSF) based substances.","Verwendet wird PFOA als Prozesshilfsstoff in der Herstellung von Fluorpolymeren. Diese werden in verschiedenen Industriezweigen verwendet, wie z. B. im Textilbereich, der Papierindustrie und in der Galvanik.\nViele Produkte enthalten Reste von PFOA wie z. B. Textilstoffe, Teppiche, Polstermöbel, Papier, Leder, Druckerfarbe, Reinigungsmittel und Pflegemittel für Teppiche, Dichtungsmittel, Bodenwachs, Farben, Imprägnierungsmittel, Feuerlöschschaum, oberflächenbehandelte Auslegeware und Ski Wachs. Als Verunreinigung ist PFOA auch in Perfluoroctylsulfonylfluorid (POSF) basierten Stoffen zu finden.","PFOA在含氟聚合物的生产中用作加工助剂。他们用于各种行业，如纺织、造纸和电镀。\n许多产品含有PFOA残留物，如纺织品、地毯、装饰家具、纸张、皮革、油墨、地毯清洁和护理产品、密封剂、地板蜡、油漆、浸渍剂、消防泡沫、表面处理地毯和滑雪蜡。PFOA也是全氟辛基磺酰氟(POSF)基物质中的一种杂质。"]
[null,{"$f":"IF($B$1=\"English\",C2628,IF($B$1=\"Deutsch\",D2628,IF($B$1=\"中文\",E2628,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dipentyl phthalate is mainly used as a plasticizer in polyvinyl chloride (PVC), but DPP is also found in electrodes for membranes. DPP is used as a solvent in personal care products, printing inks, paints, nitrocellulose and synthetic resin paints and in the manufacture of adhesives and rubber."},"Dipentyl phthalate is mainly used as a plasticizer in polyvinyl chloride (PVC), but DPP is also found in electrodes for membranes. DPP is used as a solvent in personal care products, printing inks, paints, nitrocellulose and synthetic resin paints and in the manufacture of adhesives and rubber.","Dipentylphthtalat wird hauptsächlich als Weichmacher in Polyvinylchlorid (PVC) verwendet, jedoch findet man DPP ebenfalls in Elektroden für Membranen. Eingesetzt wird DPP als Lösungsmittel in Körperpflegeprodukten, Druckerfarben, Farben, Nitrozellulose und Kunstharzlacken und in der Herstellung von Klebstoffen und Gummi. ","邻苯二甲酸二戊酯主要用作聚氯乙烯(PVC)中的增塑剂，但DPP也存在于膜的电极中。在个人护理产品、印刷油墨、油漆、硝化纤维和合成树脂油漆以及粘合剂和橡胶的制造中，二氯苯酚被用作溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C2629,IF($B$1=\"Deutsch\",D2629,IF($B$1=\"中文\",E2629,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Electrodes in nickel-cadmium accumulators; coatings of metals (corrosion protection);\n\nas an alloying component, for example in electrical contacts and solders"},"Electrodes in nickel-cadmium accumulators; coatings of metals (corrosion protection);\n\nas an alloying component, for example in electrical contacts and solders","Elektroden in Nickel-Cadmium Akkumulatoren; Beschichtungen von Metallen (Korrosionsschutz);\n\nals Legierungsbestandteil zum Beispiel in elektrischen Kontakten und Loten","镍镉蓄电池中的电极；金属涂层(防腐蚀)；\n\n作为合金成分，例如在电触点和焊料中"]
[null,{"$f":"IF($B$1=\"English\",C2630,IF($B$1=\"Deutsch\",D2630,IF($B$1=\"中文\",E2630,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Raw material for the production of electrodes, alloys, pigments, catalysts and metal coatings; heat stabilizer in polymers; ceramic glazes and glass components; laboratory chemicals."},"Raw material for the production of electrodes, alloys, pigments, catalysts and metal coatings; heat stabilizer in polymers; ceramic glazes and glass components; laboratory chemicals.","Rohstoff für die Produktion von Elektroden, Legierungen, Pigmenten, Katalysatoren und Beschichtung von Metallen; Hitzestabilisator in Polymeren; Keramikglasuren und Glasbestandteil; Laborchemikalien. ","生产电极、合金、颜料、催化剂和金属涂层的原材料；聚合物中的热稳定剂:陶瓷釉料和玻璃部件；实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2631,IF($B$1=\"Deutsch\",D2631,IF($B$1=\"中文\",E2631,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"APFO is used as a process aid in the production of fluoropolymers. These are used in various industries, such as textiles, the paper industry and electroplating.\nMany products contain residues of APFO such as textiles, carpets, upholstered furniture, paper, leather, printing ink, cleaning and care products for carpets, sealants, floor wax, paints, impregnating agents, fire-fighting foam, surface-treated carpeting and ski wax."},"APFO is used as a process aid in the production of fluoropolymers. These are used in various industries, such as textiles, the paper industry and electroplating.\nMany products contain residues of APFO such as textiles, carpets, upholstered furniture, paper, leather, printing ink, cleaning and care products for carpets, sealants, floor wax, paints, impregnating agents, fire-fighting foam, surface-treated carpeting and ski wax.","Verwendet wird APFo als Prozesshilfsstoff in der Herstellung von Fluorpolymeren. Diese werden in verschiedenen Industriezweigen verwendet, wie z. B. im Textilbereich, der Papierindustrie und in der Galvanik.\nViele Produkte enthalten Reste von APFO wie z.B. Textilstoffe, Teppiche, Polstermöbel, Papier, Leder, Druckerfarbe, Reinigungsmittel und Pflegemittel für Teppiche, Dichtungsmittel, Bodenwachs, Farben, Imprägnierungsmittel, Feuerlöschschaum, oberflächenbehandelte Auslegeware und Ski Wachs. ","APFO在含氟聚合物的生产中用作加工助剂。这些被用于各种行业，如纺织、造纸和电镀。\n许多产品含有APFO残留物，如纺织品、地毯、装饰家具、纸张、皮革、油墨、地毯清洁和护理产品、密封剂、地板蜡、油漆、浸渍剂、消防泡沫、表面处理地毯和滑雪蜡。"]
[null,{"$f":"IF($B$1=\"English\",C2632,IF($B$1=\"Deutsch\",D2632,IF($B$1=\"中文\",E2632,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formulation component in mining; component in paints, varnishes, cleaning agents, adhesives and surface treatment agents; process chemical for emulsion polymerization "},"Formulation component in mining; component in paints, varnishes, cleaning agents, adhesives and surface treatment agents; process chemical for emulsion polymerization ","Formulierungsbestandteil im Bergbau; Bestandteil in Farben, Lacken, Reinigungsmitteln, Klebstoffen und Mitteln zur Oberflächenbehandlung; Prozesschemikalie zur Emulsionspolymerisation ","采矿中的配方成分；油漆、清漆、清洁剂、粘合剂和表面处理剂中的成分；乳液聚合过程化学品"]
[null,{"$f":"IF($B$1=\"English\",C2633,IF($B$1=\"Deutsch\",D2633,IF($B$1=\"中文\",E2633,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use as lubricant, hydraulic fluid, grease, release agent use in polyurethane, PVC, TPE, coatings and textiles\nFlame retardants in plastics production\nUse as plasticizer"},"Use as lubricant, hydraulic fluid, grease, release agent use in polyurethane, PVC, TPE, coatings and textiles\nFlame retardants in plastics production\nUse as plasticizer","Verwendung als Schmiermittel, hydraulische Flüssigkeit, Fett, Trennmittel>br>Verwendung in Polyurethan, PVC, TPE sowie in Beschichtungen und Textilien\nFlammschutzmittel in der Kunststoffproduktion\nVerwendung als Weichmacher ","用作润滑剂、液压油、润滑脂、脱模剂，用于聚氨酯、聚氯乙烯、热塑性弹性体、涂料和纺织品\n塑料生产中的阻燃剂\n用作增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C2634,IF($B$1=\"Deutsch\",D2634,IF($B$1=\"中文\",E2634,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dyes for textiles and paper\npH indicator\nAdditive for agar culture media (for biological staining of histological samples)\nGelling agent for polyvinyl alcohol"},"Dyes for textiles and paper\npH indicator\nAdditive for agar culture media (for biological staining of histological samples)\nGelling agent for polyvinyl alcohol","Färbemittel für Textilien und Papier\npH-Indikator\nZusatz für Agarnährböden (zur biologischen Färbung histologischer Proben)\nGeliermittel für Polyvinylalkohol ","纺织品和纸张用染料\n酸碱度指示器\n琼脂培养基添加剂(用于组织样品的生物染色)\n聚乙烯醇胶凝剂"]
[null,{"$f":"IF($B$1=\"English\",C2635,IF($B$1=\"Deutsch\",D2635,IF($B$1=\"中文\",E2635,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of rubber products and tyres\nProduction of masterbatches\nPreparation of predispersed imidazolidine-2-thione\nUse as vulcanizing agent\nFor repackaging "},"Manufacture of rubber products and tyres\nProduction of masterbatches\nPreparation of predispersed imidazolidine-2-thione\nUse as vulcanizing agent\nFor repackaging ","  Herstellung von Gummiwaren und Reifen\nHerstellung von Masterbatches\nHerstellung von vordispergiertem Imidazolidin-2-thion\nVerwendung als Vulkanisierungsmittel\nZur Wiederverpackung ","橡胶产品和轮胎的制造\n母料生产\n预分散咪唑烷-2-硫酮的制备\n用作硫化剂\n用于重新包装"]
[null,{"$f":"IF($B$1=\"English\",C2636,IF($B$1=\"Deutsch\",D2636,IF($B$1=\"中文\",E2636,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component for the production of organic and inorganic cadmium compounds\nComponent for the preparation of inorganic pigments\nLaboratory chemical (intermediate, perfumes, perfumes, cosmetics, personal care products)\nComponent for the production of photovoltaic modules\nAdditive for the production of frits and glasses\nAdditive for the production of electronic components"},"Component for the production of organic and inorganic cadmium compounds\nComponent for the preparation of inorganic pigments\nLaboratory chemical (intermediate, perfumes, perfumes, cosmetics, personal care products)\nComponent for the production of photovoltaic modules\nAdditive for the production of frits and glasses\nAdditive for the production of electronic components","  Bestandteil zur Herstellung von organischen und anorganischen Cadmiumverbindungen\nBestandteil zur Herstellung von anorganischen Pigmenten\nLaborchemikalie (Zwischenprodukt, Parfüme, Düfte, Kosmetik, Personal-Care-Produkte)\nBestandteil zur Herstellung von Photovoltaikmodulen\nAdditiv zur Herstellung von Fritten und Gläsern\nAdditiv zur Herstellung von elektronischen Bestandteilen ","用于生产有机和无机镉化合物的组件\n用于制备无机颜料的组分\n实验室化学品(中间体、香水、香水、化妆品、个人护理产品)\n用于生产光伏模块的组件\n用于生产玻璃料和玻璃的添加剂\n用于生产电子元件的添加剂"]
[null,{"$f":"IF($B$1=\"English\",C2637,IF($B$1=\"Deutsch\",D2637,IF($B$1=\"中文\",E2637,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizer for cellulose and vinylplastics"},"Plasticizer for cellulose and vinylplastics","Weichmacher für Cellulose und Vinylplastik","纤维素和乙烯基塑料增塑剂"]
[null,{"$f":"IF($B$1=\"English\",C2638,IF($B$1=\"Deutsch\",D2638,IF($B$1=\"中文\",E2638,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use as intermediate product\nUse as a laboratory chemical\nFor the production of coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling compounds"},"Use as intermediate product\nUse as a laboratory chemical\nFor the production of coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling compounds","Verwendung als Zwischenprodukt\nVerwendung als Laborchemikalie\nZur Herstellung von Beschichtungen und Farben, Verdünnungsmittel, Farbentferner, Füllmittel, Kitte, Pflaster, Modelliermassen ","用作中间产品\n用作实验室化学品\n用于生产涂料和油漆、稀释剂、脱漆剂、填料、腻子、灰泥、模型化合物"]
[null,{"$f":"IF($B$1=\"English\",C2639,IF($B$1=\"Deutsch\",D2639,IF($B$1=\"中文\",E2639,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dyes for textiles, leather and paper, plastics, wood and biological materials\nIngredient for the preparation of aqueous inks\nUse in hair dyes"},"Dyes for textiles, leather and paper, plastics, wood and biological materials\nIngredient for the preparation of aqueous inks\nUse in hair dyes","Färbemittel für Textilien, Leder und Papier, Kunststoff, Holz und biologische Materialen\nBestandteil zur Herstellung wässriger Tinten\n>Verwendung in Haarfärbemitteln","纺织品、皮革和纸、塑料、木材和生物材料用染料\n用于制备水性油墨的成分\n用于染发剂"]
[null,{"$f":"IF($B$1=\"English\",C2640,IF($B$1=\"Deutsch\",D2640,IF($B$1=\"中文\",E2640,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products"},"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products","Bleichmittel in Wasch- und Geschirrspülmittel\nReinigungsmittel\nVerwendung in kosmetischen Produkten  ","洗涤剂和餐具洗涤剂中的漂白剂\n清洁剂\n用于化妆品"]
[null,{"$f":"IF($B$1=\"English\",C2641,IF($B$1=\"Deutsch\",D2641,IF($B$1=\"中文\",E2641,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products "},"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products ","Bleichmittel in Wasch- und Geschirrspülmittel\nReinigungsmittel\nVerwendung in kosmetischen Produkten ","洗涤剂和餐具洗涤剂中的漂白剂\n清洁剂\n用于化妆品"]
[null,{"$f":"IF($B$1=\"English\",C2642,IF($B$1=\"Deutsch\",D2642,IF($B$1=\"中文\",E2642,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component for the production of organic and inorganic cadmium compounds\nStarting material in electroplating and electroplating\nComponent for the production of photovoltaic modules\nlaboratory chemical\nFungicide"},"Component for the production of organic and inorganic cadmium compounds\nStarting material in electroplating and electroplating\nComponent for the production of photovoltaic modules\nlaboratory chemical\nFungicide","Bestandteil zur Herstellung von organischen und anorganischen Cadmiumverbindungen\nAusgangsstoff in der Elektroplattierung und Galvanik\nBestandteil zur Herstellung von Photovoltaikmodulen\nLaborchemikalie\nFungizid ","用于生产有机和无机镉化合物的组件\n电镀和电镀的原材料\n用于生产光伏模块的组件\n实验室化学品\n杀真菌剂"]
[null,{"$f":"IF($B$1=\"English\",C2643,IF($B$1=\"Deutsch\",D2643,IF($B$1=\"中文\",E2643,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizer in polymers, insulating primer, sealing material, engine oil stabilizer, transmission lubricant for motor vehicles"},"Plasticizer in polymers, insulating primer, sealing material, engine oil stabilizer, transmission lubricant for motor vehicles","Weichmacher in Polymeren, Isoliergrund, Dichtungsmaterial, Motorölstabilisator, Getriebeschmiermittel für Kraftfahrzeuge","聚合物中的增塑剂、绝缘底漆、密封材料、机油稳定剂、汽车变速器润滑剂"]
[null,{"$f":"IF($B$1=\"English\",C2644,IF($B$1=\"Deutsch\",D2644,IF($B$1=\"中文\",E2644,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PVC heat stabilizer\nUse in plastics processing\nIndustrial use"},"PVC heat stabilizer\nUse in plastics processing\nIndustrial use","Wärmestabilisator von PVC\nVerwendung in der Kunststoffverarbeitung\nIndustrielle Verwedung ","聚氯乙烯热稳定剂\n用于塑料加工\n工业用途"]
[null,{"$f":"IF($B$1=\"English\",C2645,IF($B$1=\"Deutsch\",D2645,IF($B$1=\"中文\",E2645,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Research\nManufacture of glass\nHigh Temperature Dry Film Lubricant\nOptical electronics\nSolar cells"},"Research\nManufacture of glass\nHigh Temperature Dry Film Lubricant\nOptical electronics\nSolar cells","Forschung\nHerstellung von Glas\nHoch-Temperatur Trockenfilm-Schmiermittel\noptische Elektronik\nSolarzellen","研究\n玻璃制造\n高温干膜润滑剂\n光电子学\n太阳能电池"]
[null,{"$f":"IF($B$1=\"English\",C2646,IF($B$1=\"Deutsch\",D2646,IF($B$1=\"中文\",E2646,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component for the production of inorganic cadmium compounds\nStarting material for the surface treatment of metals\nLaboratory Chemical"},"Component for the production of inorganic cadmium compounds\nStarting material for the surface treatment of metals\nLaboratory Chemical","Bestandteil zur Herstellung von anorganischen Cadmiumverbindungen\nAusgangsstoff für die Oberflächenbehandlung von Metallen\nLaborchemikalie","用于生产无机镉化合物的组件\n金属表面处理的原材料\n实验室化学"]
[null,{"$f":"IF($B$1=\"English\",C2647,IF($B$1=\"Deutsch\",D2647,IF($B$1=\"中文\",E2647,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate is mainly used as a plasticizer in polymer products (mainly PVC) to increase the mobility of the product.\nConsumer exposure occurs through the respiratory tract through building materials (wallpaper, floor coverings), furniture and car interiors, through skin contact with shoes, rainwear, PVC gloves, artificial leather in furniture and car seats as well as toys and through ingestion of some baby and child products and food contact materials"},"Bis(2-ethylhexyl)phthalate is mainly used as a plasticizer in polymer products (mainly PVC) to increase the mobility of the product.\nConsumer exposure occurs through the respiratory tract through building materials (wallpaper, floor coverings), furniture and car interiors, through skin contact with shoes, rainwear, PVC gloves, artificial leather in furniture and car seats as well as toys and through ingestion of some baby and child products and food contact materials","Bis(2-ethylhexyl)phthalat wird hauptsächlich als Weichmacher in Polymerprodukten (hauptsächlich PVC) zur Erhöhung der Beweglichkeit des Produktes verwendet.\nDie Verbraucherexposition erfolgt über die Atemwege durch Baumaterialien (Tapeten, Bodenbeläge), Möbel und Autoinnenverkleidungen, durch Hautkontakt mit Schuhen, Regenbekleidung, PVC-Handschuhen, Kunstleder in Möbeln und Fahrzeugsitzen sowie Spielzeug und durch Verschlucken mancher Baby- und Kinderprodukte sowie Lebensmittelkontaktmaterial.","邻苯二甲酸二(2-乙基己基)酯主要用作聚合物产品(主要是聚氯乙烯)的增塑剂，以增加产品的流动性。\n消费者通过呼吸道接触建筑材料(墙纸、地板覆盖物)、家具和汽车内饰，通过皮肤接触鞋子、雨衣、聚氯乙烯手套、家具和汽车座椅中的人造革以及玩具，并通过摄入一些婴儿和儿童产品以及食物接触材料"]
[null,{"$f":"IF($B$1=\"English\",C2648,IF($B$1=\"Deutsch\",D2648,IF($B$1=\"中文\",E2648,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Starting material for the preparation of \"Reaction mass of\" 2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates and 2-ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates (\"\"Reaction mass of\"\" DOTE and MOTE)\nUse in plastics processing\nIndustrial use"},"Starting material for the preparation of \"Reaction mass of\" 2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates and 2-ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates (\"\"Reaction mass of\"\" DOTE and MOTE)\nUse in plastics processing\nIndustrial use","Ausgangsstoff zur Herstellung von \"Reaction mass of\" 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (\"Reaction mass of\" DOTE und MOTE)\nVerwendung in der Kunststoffverarbeitung\nIndustrielle Verwedung ","制备“2-乙基己基-10-乙基-4，4-二辛基-7-氧代-8-氧杂-3，5-二噻-4-锡酸酯和2-乙基己基-10-乙基-4-[[2-[(2-乙基己基)氧基]-2-氧代乙基]硫]-4-辛基-7-氧代-8-氧杂-3，5-二噻-4-锡酸酯的反应物料”(“DOTE和MOTE的反应物料”)\n用于塑料加工\n工业用途"]
[null,{"$f":"IF($B$1=\"English\",C2649,IF($B$1=\"Deutsch\",D2649,IF($B$1=\"中文\",E2649,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV stabilizer;\nUV absorbents;\nUV-protective agents"},"UV stabilizer;\nUV absorbents;\nUV-protective agents","UV-Stabilisator;\nUV-Absorptionsmittel;\nUV-Schutzmittel ","紫外线稳定剂；\n紫外线吸收剂；\n紫外线防护剂"]
[null,{"$f":"IF($B$1=\"English\",C2650,IF($B$1=\"Deutsch\",D2650,IF($B$1=\"中文\",E2650,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV stabilizer;\nUV absorbents;\nUV-protective agents"},"UV stabilizer;\nUV absorbents;\nUV-protective agents","UV-Stabilisator;\nUV-Absorptionsmittel;\nUV-Schutzmittel","紫外线稳定剂；\n紫外线吸收剂；\n紫外线防护剂"]
[null,{"$f":"IF($B$1=\"English\",C2651,IF($B$1=\"Deutsch\",D2651,IF($B$1=\"中文\",E2651,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"This group of substances is mainly used in fragrances."},"This group of substances is mainly used in fragrances.","Diese Gruppe von Stoffen findet hauptsächlich in Duftstoffen Verwendung.","这组物质主要用于香水。"]
[null,{"$f":"IF($B$1=\"English\",C2652,IF($B$1=\"Deutsch\",D2652,IF($B$1=\"中文\",E2652,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"in plasticisers, lubricants, coating agents, building materials, cable components, polymer films, PVC components and artists' supplies (e.g. in modelling clay and in finger paints)"},"in plasticisers, lubricants, coating agents, building materials, cable components, polymer films, PVC components and artists' supplies (e.g. in modelling clay and in finger paints)","in Weichmacher, Schmiermittel, Beschichtungsmittel, Baustoffe, Kabelbestandteile, Polymerfolien, PVC-Komponenten und Künstlerbedarf (z.B. in Modellierton und in Fingerfarben) ","增塑剂、润滑剂、涂层剂、建筑材料、电缆组件、聚合物薄膜、聚氯乙烯组件和艺术家用品(如造型粘土和指纹漆)"]
[null,{"$f":"IF($B$1=\"English\",C2653,IF($B$1=\"Deutsch\",D2653,IF($B$1=\"中文\",E2653,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Processing aid in the manufacture of fluoropolymers; lubricant in oils; wetting agent for fire-fighting foam; cleaning agent; antifouling in textiles; surface agent in polishes; sealant; in liquid crystal display panels."},"Processing aid in the manufacture of fluoropolymers; lubricant in oils; wetting agent for fire-fighting foam; cleaning agent; antifouling in textiles; surface agent in polishes; sealant; in liquid crystal display panels.","Prozesshilfsstoff in der Herstellung von Fluorpolymeren; Schmiermittel in Ölen; Netzmittel für Feuerlöschschaum; Reinigungsmittel; Antifouling in Textilien; Oberflächenagenz in Poliermittel; Abdichtungsmittel; in Flüssigkristalldisplay-Paneelen","含氟聚合物制造中的加工助剂；油中的润滑剂；消防泡沫润湿剂；清洁剂；纺织品防污；抛光剂中的表面活性剂；密封剂；用于液晶显示面板。"]
[null,{"$f":"IF($B$1=\"English\",C2654,IF($B$1=\"Deutsch\",D2654,IF($B$1=\"中文\",E2654,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of other substances"},"Manufacture of other substances","Herstellung anderer Stoffe ","其他物质的制造"]
[null,{"$f":"IF($B$1=\"English\",C2655,IF($B$1=\"Deutsch\",D2655,IF($B$1=\"中文\",E2655,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV stabilizer in coatings, plastics, rubber and cosmetics "},"UV stabilizer in coatings, plastics, rubber and cosmetics ","UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika ","涂料、塑料、橡胶和化妆品中的紫外线稳定剂"]
[null,{"$f":"IF($B$1=\"English\",C2656,IF($B$1=\"Deutsch\",D2656,IF($B$1=\"中文\",E2656,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate for the production of fine and bulk chemicals, electrolyte for lithium ion batteries "},"Intermediate for the production of fine and bulk chemicals, electrolyte for lithium ion batteries ","Zwischenprodukt für die Herstellung von Fein- und Bulkchemikalien, Elektrolyt für Lithiumionenbatterien ","精细和批量化学品生产的中间体，锂离子电池电解液"]
[null,{"$f":"IF($B$1=\"English\",C2657,IF($B$1=\"Deutsch\",D2657,IF($B$1=\"中文\",E2657,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika "},"UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika ","UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika ","涂层、塑料、橡胶和化妆品中的紫外稳定剂"]
[null,{"$f":"IF($B$1=\"English\",C2658,IF($B$1=\"Deutsch\",D2658,IF($B$1=\"中文\",E2658,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[a]pyrene is not registered. The substance is not normally manufactured, but can be an ingredient or contamination of another substance. "},"Benzo[a]pyrene is not registered. The substance is not normally manufactured, but can be an ingredient or contamination of another substance. ","Benzo[a]pyren ist nicht registriert. Der Stoff wird normalerweise nicht hergestellt, sondern kann ein Bestandteil oder eine Verunreinigung eines anderen Stoffes sein. ","苯并[a]芘未注册。这种物质通常不生产，但可能是另一种物质的成分或污染物。"]
[null,{"$f":"IF($B$1=\"English\",C2659,IF($B$1=\"Deutsch\",D2659,IF($B$1=\"中文\",E2659,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomer for the preparation of polymers"},"Monomer for the preparation of polymers","Monomer zur Herstellung von Polymeren","用于制备聚合物的单体"]
[null,{"$f":"IF($B$1=\"English\",C2660,IF($B$1=\"Deutsch\",D2660,IF($B$1=\"中文\",E2660,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the manufacture of chemicals and plastic products "},"For the manufacture of chemicals and plastic products ","Zur Herstellung von Chemikalien und Erzeugnissen aus Plastik ","用于制造化学品和塑料产品"]
[null,{"$f":"IF($B$1=\"English\",C2661,IF($B$1=\"Deutsch\",D2661,IF($B$1=\"中文\",E2661,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"e.g. as corrosion inhibitor, lubricant, softener "},"e.g. as corrosion inhibitor, lubricant, softener ","u.a. als Korrosionsinhibitor, Schmiermittel, Weichmacher ","例如作为腐蚀抑制剂、润滑剂、软化剂"]
[null,{"$f":"IF($B$1=\"English\",C2662,IF($B$1=\"Deutsch\",D2662,IF($B$1=\"中文\",E2662,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PFHxS is a known contamination in the production of PFOS. It can also be used as a replacement for PFOS"},"PFHxS is a known contamination in the production of PFOS. It can also be used as a replacement for PFOS","PFHxS ist eine bekannte Verunreinigung bei der Herstellung von PFOS. Es kann auch als Ersatz für PFOS eingesetzt werden","PFHxS是生产PFOS时的一种已知污染，也可作为PFOS的替代物"]
[null,{"$f":"IF($B$1=\"English\",C2663,IF($B$1=\"Deutsch\",D2663,IF($B$1=\"中文\",E2663,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the production of epoxy and epoxy hardeners (industrial and professional applications), coating material, for the production of polymers such as polycarbonates and PVC; use in thermal paper (industrial, professional and consumer)"},"For the production of epoxy and epoxy hardeners (industrial and professional applications), coating material, for the production of polymers such as polycarbonates and PVC; use in thermal paper (industrial, professional and consumer)","Zur Herstellung von Epoxiden und Expoxid Härtern (industrielle und professionelle Anwendungen), Beschichtungsmaterial, Zur Herstellung von Polymeren, wie z.B. Polycarbonaten und PVC; Verwendung in Thermopapier (industriell, professionell und Verbraucher)","用于生产环氧树脂和环氧树脂硬化剂(工业和专业应用)、涂料，用于生产聚合物，如聚碳酸酯和聚氯乙烯；用于热敏纸(工业、专业和消费者)"]
[null,{"$f":"IF($B$1=\"English\",C2664,IF($B$1=\"Deutsch\",D2664,IF($B$1=\"中文\",E2664,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in greases, lubricating greases and lubricating oils."},"Used in greases, lubricating greases and lubricating oils.","Wird in Fetten, Schmierfetten und Schmierölen eingesetzt.","用于润滑脂、润滑脂和润滑油。"]
[null,{"$f":"IF($B$1=\"English\",C2665,IF($B$1=\"Deutsch\",D2665,IF($B$1=\"中文\",E2665,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a pH regulator and in drinking water treatment products, laboratory chemicals, cosmetics and care products."},"Used as a pH regulator and in drinking water treatment products, laboratory chemicals, cosmetics and care products.","Wird als pH Regulator und in Trinkwasseraufbereitungsprodukten, Laborchemikalien, Kosmetika und Pflegeprodukten verwendet.","用作酸碱度调节剂，用于饮用水处理产品、实验室化学品、化妆品和护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C2666,IF($B$1=\"Deutsch\",D2666,IF($B$1=\"中文\",E2666,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The substance is used in the manufacture of electrical, electronic and optical equipment and in laboratory chemicals. "},"The substance is used in the manufacture of electrical, electronic and optical equipment and in laboratory chemicals. ","Der Stoff wird bei der Herstellung von elektrischer, elektronischer und optischer Ausrüstung und in Laborchemikalien verwendet. ","该物质用于制造电气、电子和光学设备以及实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2667,IF($B$1=\"Deutsch\",D2667,IF($B$1=\"中文\",E2667,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in the manufacture of glass, ceramic and porcelain products and in laboratory chemicals. "},"Used in the manufacture of glass, ceramic and porcelain products and in laboratory chemicals. ","Wird bei der Herstellung von Produkten aus Glas, Keramik und Porzellan und in Laborchemikalien verwendet. ","用于制造玻璃、陶瓷和瓷器产品以及实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C2668,IF($B$1=\"Deutsch\",D2668,IF($B$1=\"中文\",E2668,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Is not normally produced, but is a component or contamination of other substances."},"Is not normally produced, but is a component or contamination of other substances.","Wird normalerweise nicht produziert, sondern ist ein Bestandteil oder eine Verunreinigung anderer Stoffe.","不是正常生产的，而是其他物质的成分或污染。"]
[null,{"$f":"IF($B$1=\"English\",C2669,IF($B$1=\"Deutsch\",D2669,IF($B$1=\"中文\",E2669,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Is not normally produced, but is a component or contamination of other substances."},"Is not normally produced, but is a component or contamination of other substances.","Wird normalerweise nicht produziert, sondern ist ein Bestandteil oder eine Verunreinigung anderer Stoffe.","不是正常生产的，而是其他物质的成分或污染。"]
[null,{"$f":"IF($B$1=\"English\",C2670,IF($B$1=\"Deutsch\",D2670,IF($B$1=\"中文\",E2670,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as flame retardant in adhesives, sealants and binders."},"Used as flame retardant in adhesives, sealants and binders.","Wird als Flammschutzmittel in Kleb- und Dichtstoffen sowie in Bindemitteln eingesetzt. ","用作粘合剂、密封剂和粘合剂中的阻燃剂。"]
[null,{"$f":"IF($B$1=\"English\",C2671,IF($B$1=\"Deutsch\",D2671,IF($B$1=\"中文\",E2671,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in the manufacture of esters and polymers."},"Used in the manufacture of esters and polymers.","Herstellung von Estern und Polymeren","用于制造酯和聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C2672,IF($B$1=\"Deutsch\",D2672,IF($B$1=\"中文\",E2672,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in plastisol, PVC, rubber and plastic articles. A further use is also as a phlegmatiser and dispersing agent for formulations of organic peroxides."},"Used in plastisol, PVC, rubber and plastic articles. A further use is also as a phlegmatiser and dispersing agent for formulations of organic peroxides.","Plastisol, PVC, Kautschuk, Kunststoffe sowie Phlegmatisierungsmittel und Dispergiermittel zur Herstellung organischer Peroxide","用于塑料溶胶、聚氯乙烯、橡胶和塑料制品。另一个用途是作为有机过氧化物制剂的减敏剂和分散剂。"]
[null,{"$f":"IF($B$1=\"English\",C2673,IF($B$1=\"Deutsch\",D2673,IF($B$1=\"中文\",E2673,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in washing and cleaning products, polishes and waxes and cosmetics and personal care products."},"Used in washing and cleaning products, polishes and waxes and cosmetics and personal care products.","Wasch- und Reinigungsmittel, Polituren, Wachse, Kosmetika und Körperpflegeprodukte","用于洗涤和清洁产品、抛光剂和蜡、化妆品和个人护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C2674,IF($B$1=\"Deutsch\",D2674,IF($B$1=\"中文\",E2674,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products, textile treatment products and dyes."},"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products, textile treatment products and dyes.","Wasch- und Reinigungsmittel, Polituren, Wachse, Kosmetika, Körperpflegeprodukte, Textilbehandlungsmittel und Farbstoffe","用于洗涤和清洁产品、抛光剂和蜡、化妆品和个人护理产品、纺织品处理产品和染料。"]
[null,{"$f":"IF($B$1=\"English\",C2675,IF($B$1=\"Deutsch\",D2675,IF($B$1=\"中文\",E2675,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products."},"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products.","Wasch- und Reinigungsmittel, Polituren, Wachse, Kosmetika und Körperpflegeprodukte","用于洗涤和清洁产品，抛光剂和蜡，化妆品和个人护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C2676,IF($B$1=\"Deutsch\",D2676,IF($B$1=\"中文\",E2676,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in metals, welding and soldering products, metal surface treatment products, and polymers."},"Used in metals, welding and soldering products, metal surface treatment products, and polymers.","Metalle, Karosserie- und Lötprodukte, Metalloberflächenbehandlungsprodukte und Polymere","用于金属、焊接和钎焊产品、金属表面处理产品和聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C2677,IF($B$1=\"Deutsch\",D2677,IF($B$1=\"中文\",E2677,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in anti-freeze products, heat transfer fluids, lubricants and greases, and washing and cleaning products."},"Used in anti-freeze products, heat transfer fluids, lubricants and greases, and washing and cleaning products.","Frostschutzmittel, Wärmeträgerflüssigkeiten, Gleit- und Schmiermittel, Wasch- und Reinigungsmittel","用于防冻产品、传热流体、润滑剂和油脂以及洗涤和清洁产品。"]
[null,{"$f":"IF($B$1=\"English\",C2678,IF($B$1=\"Deutsch\",D2678,IF($B$1=\"中文\",E2678,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Not registered under REACH. Normally not produced intentionally but rather occurs as a constituent or impurity in other substances."},"Not registered under REACH. Normally not produced intentionally but rather occurs as a constituent or impurity in other substances.","Wird nicht absichtlich hergestellt, ist jedoch als Bestandteil oder Verunreinigung in anderen Stoffen","未在REACH下注册。通常不是有意产生的，而是作为其他物质的成分或杂质出现的。"]
[null,{"$f":"IF($B$1=\"English\",C2679,IF($B$1=\"Deutsch\",D2679,IF($B$1=\"中文\",E2679,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a plastic additive, solvent, in coatings/inks, in adhesives and sealants, and heat transfer fluids."},"Used as a plastic additive, solvent, in coatings/inks, in adhesives and sealants, and heat transfer fluids.","Kunststoffadditive, Lösemittel, Anstrichmittel, Tinten, Klebstoffe, Dichtungsmittel, Wärmeträgerflüssigkeiten","用作塑料添加剂、溶剂、涂料/油墨、粘合剂和密封剂以及传热流体。"]
[null,{"$f":"IF($B$1=\"English\",C2680,IF($B$1=\"Deutsch\",D2680,IF($B$1=\"中文\",E2680,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, pH regulators and water treatment products."},"Used in adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, pH regulators and water treatment products.","Klebstoffe, Dichtungsmittel, Anstrichmittel, Kitt, Füllmaterial, Mörtel, Modeliermasse, pH-Regulierer, Wasseraufbereitungsmittel","用于粘合剂和密封剂、涂料产品、填料、腻子、灰泥、造型粘土、酸碱度调节剂和水处理产品。"]
[null,{"$f":"IF($B$1=\"English\",C2681,IF($B$1=\"Deutsch\",D2681,IF($B$1=\"中文\",E2681,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C2682,IF($B$1=\"Deutsch\",D2682,IF($B$1=\"中文\",E2682,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Binder for refractory material"},"Binder for refractory material","Bindemittel für feuerfestes Material","耐火材料粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C2683,IF($B$1=\"Deutsch\",D2683,IF($B$1=\"中文\",E2683,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Binder for refractory material"},"Binder for refractory material","Bindemittel für feuerfestes Material","耐火材料粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C2684,IF($B$1=\"Deutsch\",D2684,IF($B$1=\"中文\",E2684,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Binder for refractory material"},"Binder for refractory material","Bindemittel für feuerfestes Material","耐火材料粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C2685,IF($B$1=\"Deutsch\",D2685,IF($B$1=\"中文\",E2685,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a transported intermediate for the manufacture of fine chemicals."},"Used as a transported intermediate for the manufacture of fine chemicals.","Als transportiertes Zwischenprodukt bei der Herstellung von Feinchemikalien","用作制造精细化学品的运输中间体。"]
[null,{"$f":"IF($B$1=\"English\",C2686,IF($B$1=\"Deutsch\",D2686,IF($B$1=\"中文\",E2686,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV filters in sunscreen and other cosmetics"},"UV filters in sunscreen and other cosmetics","UV-Filter in Sonnencreme und anderen Kosmetika","防晒霜和其他化妆品中的紫外线过滤器"]
[null,{"$f":"IF($B$1=\"English\",C2687,IF($B$1=\"Deutsch\",D2687,IF($B$1=\"中文\",E2687,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvent  for  gums,  resins,  waxes,  and  oils  and  in  the \nmanufacture of semiconductors, textile printing and photographic films. paints, lacquers, stains, inks, surface coatings, \nsilk-screen  printing,  photographic  and  photo  lithographic  processes,  semiconductors,  textile, \nleather, hydraulic fluids, jet fuel, varnishes, paper, acetate adhesives, nitrocellulose, cellulose \nacetate,  gums,  resins,  waxes,  and  oils,  textile  printing  and  dry-cleaning.  Technical  functions \ninclude solvent, drying retarder, and anti-icing additive, viscosity decreasing agent.\n"},"Solvent  for  gums,  resins,  waxes,  and  oils  and  in  the \nmanufacture of semiconductors, textile printing and photographic films. paints, lacquers, stains, inks, surface coatings, \nsilk-screen  printing,  photographic  and  photo  lithographic  processes,  semiconductors,  textile, \nleather, hydraulic fluids, jet fuel, varnishes, paper, acetate adhesives, nitrocellulose, cellulose \nacetate,  gums,  resins,  waxes,  and  oils,  textile  printing  and  dry-cleaning.  Technical  functions \ninclude solvent, drying retarder, and anti-icing additive, viscosity decreasing agent.\n","Lösemittel für Gummi, Harze, Wachse und Öle und zur Herstellung von Halbleitern, Textildrucken und fotografischen Filmen verwendet. Einsatzmöglichkeiten in Farben, Lacken, Beizen, Druckfarben, Oberflächenbeschichtungen, Siebdruck, fotografischen und fotolithografischen Verfahren, Halbleitern, Textilien, Leder, Hydraulikflüssigkeiten, Düsentreibstoff, Papier, Acetatkleber, Nitrocellulose, Celluloseacetat, Textildruck und in der chemischer Reinigung.","树胶、树脂、蜡和油的溶剂，半导体、纺织品印刷和摄影胶片制造。油漆、清漆、着色剂、油墨、表面涂层、丝网印刷、照相和光刻工艺、半导体、纺织品、皮革、液压油、喷气燃料、清漆、纸张、醋酸纤维粘合剂、硝化纤维、纤维素醋酸盐、树胶、树脂、蜡和油、纺织品印花和干洗。技术功能包括溶剂、干燥延迟剂、防冰添加剂、降粘剂。\n"]
[null,{"$f":"IF($B$1=\"English\",C2688,IF($B$1=\"Deutsch\",D2688,IF($B$1=\"中文\",E2688,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Primarily used as an antioxidant to stabilise polymers."},"Primarily used as an antioxidant to stabilise polymers.","TNPP wird hauptsächlich als Antioxidans zur Stabilisierung von Polymeren verwendet.","主要用作抗氧化剂来稳定聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C2689,IF($B$1=\"Deutsch\",D2689,IF($B$1=\"中文\",E2689,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Processing aid in the production of fluorinated polymers."},"Processing aid in the production of fluorinated polymers.","Verarbeitungshilfe bei der Herstellung von fluorierten Polymeren.","氟化聚合物生产中的加工助剂。"]
[null,{"$f":"IF($B$1=\"English\",C2690,IF($B$1=\"Deutsch\",D2690,IF($B$1=\"中文\",E2690,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly \nused in the phenolic/epoxy resin industry and is only used as an intermediate /in polymers\nUsed in coating products, polymers, adhesives, sealants and for the synthesis of other substances.\n"},"Mainly \nused in the phenolic/epoxy resin industry and is only used as an intermediate /in polymers\nUsed in coating products, polymers, adhesives, sealants and for the synthesis of other substances.\n","Hauptsächlich Einsatz in der Phenol-/Epoxidharzindustrie als Zwischenprodukt in Polymeren. Verwendung in Beschichtungsmaterial, Polymeren, Klebstoffen, Dicht-stoffen und zur Synthese anderer Stoffe.","主要用于酚醛/环氧树脂行业，仅用作中间体/聚合物\n用于涂料产品、聚合物、粘合剂、密封剂和其他物质的合成。\n"]
[null,{"$f":"IF($B$1=\"English\",C2691,IF($B$1=\"Deutsch\",D2691,IF($B$1=\"中文\",E2691,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisohexyl phthalate is a component (the branched form) of 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear (EC 271-093-5; CAS 68515-50-4). There are indications for potential use of the substances in the same types of applications (e.g. as sealant, plasticiser in polymers etc)."},"Diisohexyl phthalate is a component (the branched form) of 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear (EC 271-093-5; CAS 68515-50-4). There are indications for potential use of the substances in the same types of applications (e.g. as sealant, plasticiser in polymers etc).","Diisohexyl phthalat ist in verzweigter Form Bestandteil von 1,2-Benzoldicarbonsäure Diehexylester, verzweigt und linear (EG-Nr. 271-093-5, CAS-Nr. 68515-50-4). Die Verwendungsbereiche sind deshalb vergleichbar (Weichmacher in Polymeren, Dich-tungsmaterial usw.).","邻苯二甲酸二异己酯是1，2-苯二甲酸二己酯的一种组分(支化形式)，支化和线性的(EC 271-093-5；CAS 68515-50-4)。有迹象表明这些物质可能用于相同类型的应用(如密封剂、聚合物中的增塑剂等)。"]
[null,{"$f":"IF($B$1=\"English\",C2692,IF($B$1=\"Deutsch\",D2692,IF($B$1=\"中文\",E2692,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone is used\nfor the production of printing inks and surface coating based on based on acrylates polymerized by UV radiation.\n"},"2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone is used\nfor the production of printing inks and surface coating based on based on acrylates polymerized by UV radiation.\n","2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon wird zur Herstellung von Druckfarben und Oberflächenbeschichtungen auf Basis von durch UV-Strahlung po-lymerisierten Acrylaten verwendet.","使用2-苄基-2-二甲氨基-4’-吗啉代联苯酮用于生产基于通过紫外线辐射聚合的丙烯酸酯的印刷油墨和表面涂层。\n"]
[null,{"$f":"IF($B$1=\"English\",C2693,IF($B$1=\"Deutsch\",D2693,IF($B$1=\"中文\",E2693,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a catalyst/ additive/reactant in polymer manufacture and in chemical synthesis. It is also used as a flame retardant in polycarbonate (for electronic equipment)."},"Used as a catalyst/ additive/reactant in polymer manufacture and in chemical synthesis. It is also used as a flame retardant in polycarbonate (for electronic equipment).","Wird als Katalysator in der Polymerherstellung und in der chemischen Synthese sowie als Flammschutzmittel in Polycarbonat (bei elektroni-schen Geräten) verwendet.","在聚合物制造和化学合成中用作催化剂/添加剂/反应物。它也用作聚碳酸酯中的阻燃剂(用于电子设备)。"]
[null,{"$f":"IF($B$1=\"English\",C2694,IF($B$1=\"Deutsch\",D2694,IF($B$1=\"中文\",E2694,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methyl-1- (4-methylthiophenyl) -2-morpholinopropan-1-one is used as a photoinitiator in the manufacture of formulations and (outer) packaging, coatings, adhesives, printing inks, fiber sizes."},"2-Methyl-1- (4-methylthiophenyl) -2-morpholinopropan-1-one is used as a photoinitiator in the manufacture of formulations and (outer) packaging, coatings, adhesives, printing inks, fiber sizes.","2-Methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-on wird als Photoinitiator bei der Herstellung von Formulierungen und (Um-)Verpackungen, Beschichtungen, Klebstoffen, Druckfarben, Faserschlichten verwendet.","2-甲基-1-(4-甲基噻吩基)-2-吗啉代-1-酮在制剂和(外包装)、涂料、粘合剂、印刷油墨、纤维胶料的制造中用作光引发剂。"]
[null,{"$f":"IF($B$1=\"English\",C2695,IF($B$1=\"Deutsch\",D2695,IF($B$1=\"中文\",E2695,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-(2-methoxyethoxy)ethyl)ether is used in inks and toners as a solvent or extractant. Industrial use as a gas absorption liquid, solvent in synthesis reactions or as an extractant."},"Bis(2-(2-methoxyethoxy)ethyl)ether is used in inks and toners as a solvent or extractant. Industrial use as a gas absorption liquid, solvent in synthesis reactions or as an extractant.","Bis(2-(2-methoxyethoxy)ethyl)ether wird in Tinten und Toner als Lösemittel oder Extraktionsmittel verwendet. Industrielle Verwendung als Gasabsorptionsflüssigkeit, Lösungsmittel in Synthesereaktionen oder als Extraktionsmittel.","双(2-(2-甲氧基乙氧基)乙基)醚在油墨和调色剂中用作溶剂或萃取剂。工业上用作气体吸收液体、合成反应中的溶剂或萃取剂。"]
[null,{"$f":"IF($B$1=\"English\",C2696,IF($B$1=\"Deutsch\",D2696,IF($B$1=\"中文\",E2696,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The main ingredient dioctyltin dilaurate is used in adhesives and sealants and in the manufacture of plastic and rubber tyres"},"The main ingredient dioctyltin dilaurate is used in adhesives and sealants and in the manufacture of plastic and rubber tyres","Der Hauptbestandteil Dioctylzinndilaurat wird in Kleb- und Dichtstoffen sowie bei der Herstellung von Kunststoff- und Gummireifen verwendet","二月桂酸二辛酯的主要成分用于粘合剂和密封剂以及塑料和橡胶轮胎的制造"]
[null,{"$f":"IF($B$1=\"English\",C2697,IF($B$1=\"Deutsch\",D2697,IF($B$1=\"中文\",E2697,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Yes with exception"},"Yes with exception","Ja, mit Ausnahme","是的，含豁免项"]
[null,{"$f":"IF($B$1=\"English\",C2698,IF($B$1=\"Deutsch\",D2698,IF($B$1=\"中文\",E2698,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Yes with declaration"},"Yes with declaration","Ja, mit Deklaration","是的，需要申报"]
[null,{"$f":"IF($B$1=\"English\",C2699,IF($B$1=\"Deutsch\",D2699,IF($B$1=\"中文\",E2699,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nothing to declare"},"Nothing to declare","Nicht zu deklarieren","不申报"]
[null,{"$f":"IF($B$1=\"English\",C2700,IF($B$1=\"Deutsch\",D2700,IF($B$1=\"中文\",E2700,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N2580 (Bosch group) Excel file:"},"N2580 (Bosch group) Excel file:","N2580 (Bosch group) Excel file:","N2580 (博世集团) Excel 文件:"]
[null,{"$f":"IF($B$1=\"English\",C2701,IF($B$1=\"Deutsch\",D2701,IF($B$1=\"中文\",E2701,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Suppliers/Partners may choose make N2580 declarations by using either: the Bosch-PT specific declaration sheet, or the Compliance Data Exchange (CDX)"},"Suppliers/Partners may choose make N2580 declarations by using either: the Bosch-PT specific declaration sheet, or the Compliance Data Exchange (CDX)","Lieferanten/Partner können für die N2580 Deklaration entweder - die Bosch-PT spezifische Lieferantenerklärung über Inhaltstoffe verwenden, oder Compliance Data Exchange (CDX)","供应商/合作伙伴可以选择使用博世-PT特定申报单 或合规数据交换(CDX)进行N2580申报"]
[null,{"$f":"IF($B$1=\"English\",C2702,IF($B$1=\"Deutsch\",D2702,IF($B$1=\"中文\",E2702,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PT-specific requirements, instructions, and the CDX login are found by scrolling to “Specific quality documents/Power Tools” linked here:"},"PT-specific requirements, instructions, and the CDX login are found by scrolling to “Specific quality documents/Power Tools” linked here:","Die PT-spezifischen Anforderungen, Schulungsmaterial und der CDX Login sind im Bereich “Spezifische Regelungen Qualität/Power Tools” zu finden, unter: ","PT特定的要求、说明和CDX登录信息可参见“特定质量文件/电动工具”，可以找到PT特定的要求、说明和CDX登录信息，链接如下："]
[null,{"$f":"IF($B$1=\"English\",C2703,IF($B$1=\"Deutsch\",D2703,IF($B$1=\"中文\",E2703,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Information for business partners | Bosch Global"},"Information for business partners | Bosch Global","Informationen für Geschäftspartner | Bosch Global","商业伙伴信息 | 博世全球"]
[null,{"$f":"IF($B$1=\"English\",C2704,IF($B$1=\"Deutsch\",D2704,IF($B$1=\"中文\",E2704,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"https://www.bosch.com/company/supply-chain/information-for-business-partners/#quality-regulations-and-standards"},"https://www.bosch.com/company/supply-chain/information-for-business-partners/#quality-regulations-and-standards","https://www.bosch.com/de/unternehmen/supply-chain/informationen-fuer-geschaeftspartner/","https://www.bosch.com/company/supply-chain/information-for-business-partners/#quality-regulations-and-standards"]
[null,{"$f":"IF($B$1=\"English\",C2705,IF($B$1=\"Deutsch\",D2705,IF($B$1=\"中文\",E2705,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"},"Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)","Phenol, Alkylierungsprodukte (hauptsächlich in para-Position) mit C12-reichen verzweigten Alkylketten aus der Oligomerisierung, die alle einzelnen Isomere und/oder Kombinationen davon umfasst (PDDP)","具有来自低聚的富含 C12的支链烷基链的烷基化产物 （主要在对位）苯酚，包括所有单独的异构体和/或它们的组合 (PDDP) "]
[null,{"$f":"IF($B$1=\"English\",C2706,IF($B$1=\"Deutsch\",D2706,IF($B$1=\"中文\",E2706,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, dodecyl-, branched"},"Phenol, dodecyl-, branched","Phenol, dodecyl-, branched","十二烷基苯酚，支链"]
[null,{"$f":"IF($B$1=\"English\",C2707,IF($B$1=\"Deutsch\",D2707,IF($B$1=\"中文\",E2707,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, (tetrapropenyl) derivatives"},"Phenol, (tetrapropenyl) derivatives","Phenol, (tetrapropenyl) derivatives","（四丙烯基）苯酚，衍生物"]
[null,{"$f":"IF($B$1=\"English\",C2708,IF($B$1=\"Deutsch\",D2708,IF($B$1=\"中文\",E2708,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-dodecyl, branched"},"Phenol, 4-dodecyl, branched","Phenol, 4-dodecyl, branched","4-十二烷基苯酚，支链"]
[null,{"$f":"IF($B$1=\"English\",C2709,IF($B$1=\"Deutsch\",D2709,IF($B$1=\"中文\",E2709,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-isododecylphenol"},"4-isododecylphenol","4-isododecylphenol","4-异十二烷基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2710,IF($B$1=\"Deutsch\",D2710,IF($B$1=\"中文\",E2710,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, tetrapropylene-"},"Phenol, tetrapropylene-","Phenol, tetrapropylene-","四丙烯苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2711,IF($B$1=\"Deutsch\",D2711,IF($B$1=\"中文\",E2711,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-isododecyl-"},"Phenol, 4-isododecyl-","Phenol, 4-isododecyl-","4-十二烷基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2712,IF($B$1=\"Deutsch\",D2712,IF($B$1=\"中文\",E2712,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"orthoboric acid, sodium salt"},"orthoboric acid, sodium salt","Orthoborsäure, Natriumsalz ","原硼酸，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2713,IF($B$1=\"Deutsch\",D2713,IF($B$1=\"中文\",E2713,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"boric acid (H3BO3), sodium salt, hydrate"},"boric acid (H3BO3), sodium salt, hydrate","boric acid (H3BO3), sodium salt, hydrate","硼酸 (H3BO3)，钠盐，水合物 "]
[null,{"$f":"IF($B$1=\"English\",C2714,IF($B$1=\"Deutsch\",D2714,IF($B$1=\"中文\",E2714,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid (H3BO3), disodium salt"},"Boric acid (H3BO3), disodium salt","Boric acid (H3BO3), disodium salt","硼酸 (H3BO3)，二钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2715,IF($B$1=\"Deutsch\",D2715,IF($B$1=\"中文\",E2715,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trisodium orthoborate"},"Trisodium orthoborate","Trisodium orthoborate","原硼酸三钠"]
[null,{"$f":"IF($B$1=\"English\",C2716,IF($B$1=\"Deutsch\",D2716,IF($B$1=\"中文\",E2716,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid, sodium salt"},"Boric acid, sodium salt","Boric acid, sodium salt","硼酸，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2717,IF($B$1=\"Deutsch\",D2717,IF($B$1=\"中文\",E2717,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Orthoboric acid, sodium salt"},"Orthoboric acid, sodium salt","Orthoboric acid, sodium salt","原硼酸，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2718,IF($B$1=\"Deutsch\",D2718,IF($B$1=\"中文\",E2718,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid (H3BO3), sodium salt (1:1) "},"Boric acid (H3BO3), sodium salt (1:1) ","Boric acid (H3BO3), sodium salt (1:1) ","硼酸 (H3BO3)，钠盐(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2719,IF($B$1=\"Deutsch\",D2719,IF($B$1=\"中文\",E2719,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Medium-chain chlorinated paraffins (MCCP)"},"Medium-chain chlorinated paraffins (MCCP)","Mittelkettige Chlorparaffine (MCCP) (UVCB-Stoffe bestehend aus mehr als oder gleich 80 % linearen Chloralkanen mit Kohlenstoffkettenlängen im Bereich von C14 bis C17)","中链氯化石蜡 (MCCP)"]
[null,{"$f":"IF($B$1=\"English\",C2720,IF($B$1=\"Deutsch\",D2720,IF($B$1=\"中文\",E2720,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C14-16, chloro"},"Alkanes, C14-16, chloro","Alkanes, C14-16, chloro","烷烃，C14-16，氯"]
[null,{"$f":"IF($B$1=\"English\",C2721,IF($B$1=\"Deutsch\",D2721,IF($B$1=\"中文\",E2721,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C14-17, chloro"},"Alkanes, C14-17, chloro","Alkanes, C14-17, chloro","烷烃，C14-17，氯"]
[null,{"$f":"IF($B$1=\"English\",C2722,IF($B$1=\"Deutsch\",D2722,IF($B$1=\"中文\",E2722,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"di-, tri- and tetrachlorotetradecane "},"di-, tri- and tetrachlorotetradecane ","di-, tri- and tetrachlorotetradecane ","二，三和四氯十四烷"]
[null,{"$f":"IF($B$1=\"English\",C2723,IF($B$1=\"Deutsch\",D2723,IF($B$1=\"中文\",E2723,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetradecane, chloro derivs."},"Tetradecane, chloro derivs.","Tetradecane, chloro derivs.","十四烷，氯衍生物"]
[null,{"$f":"IF($B$1=\"English\",C2724,IF($B$1=\"Deutsch\",D2724,IF($B$1=\"中文\",E2724,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"glutaral"},"glutaral","Glutaral","戊二醛 "]
[null,{"$f":"IF($B$1=\"English\",C2725,IF($B$1=\"Deutsch\",D2725,IF($B$1=\"中文\",E2725,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-(1-methylpropylidene)bisphenol"},"4,4'-(1-methylpropylidene)bisphenol","4,4'-(1-Methylpropyliden)bisphenol","4,4'-(1-甲基亚丙基)双酚 "]
[null,{"$f":"IF($B$1=\"English\",C2726,IF($B$1=\"Deutsch\",D2726,IF($B$1=\"中文\",E2726,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"},"2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers","2-(4-tert-Butylbenzyl)propionaldehyd und seine einzelnen Stereoisomere","2-(4-叔丁基苄基)丙醛及其立体异构体 "]
[null,{"$f":"IF($B$1=\"English\",C2727,IF($B$1=\"Deutsch\",D2727,IF($B$1=\"中文\",E2727,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2R)-3-(4-tert-butylphenyl)-2-methylpropanal "},"(2R)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2R)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2R)-3-(4-叔丁基苯基)-2-甲基丙醛  "]
[null,{"$f":"IF($B$1=\"English\",C2728,IF($B$1=\"Deutsch\",D2728,IF($B$1=\"中文\",E2728,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(4-tert-butylbenzyl)propionaldehyde"},"2-(4-tert-butylbenzyl)propionaldehyde","2-(4-tert-butylbenzyl)propionaldehyde","2-(4-叔丁基苄基)丙醛 "]
[null,{"$f":"IF($B$1=\"English\",C2729,IF($B$1=\"Deutsch\",D2729,IF($B$1=\"中文\",E2729,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2S)-3-(4-tert-butylphenyl)-2-methylpropanal "},"(2S)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2S)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2S)-3-(4-叔丁基苯基)-2-甲基丙醛  "]
[null,{"$f":"IF($B$1=\"English\",C2730,IF($B$1=\"Deutsch\",D2730,IF($B$1=\"中文\",E2730,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"},"2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)","2,2-双(溴甲基)丙烷-1,3-二醇(BMP)； 2,2-二甲基丙-1-醇，三溴衍生物/3-溴-2,2-双(溴甲基)-1-丙醇(TBNPA)； 2,3-二溴-1-丙醇(2,3-DBPA) "]
[null,{"$f":"IF($B$1=\"English\",C2731,IF($B$1=\"Deutsch\",D2731,IF($B$1=\"中文\",E2731,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) "},"2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) ","2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) ","2,2-二甲基丙-1-醇，三溴衍生物(TBNPA)"]
[null,{"$f":"IF($B$1=\"English\",C2732,IF($B$1=\"Deutsch\",D2732,IF($B$1=\"中文\",E2732,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)"},"3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)","3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)","3-溴-2,2-双(溴甲基)-1-丙醇(TBNPA)"]
[null,{"$f":"IF($B$1=\"English\",C2733,IF($B$1=\"Deutsch\",D2733,IF($B$1=\"中文\",E2733,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-bis(bromomethyl)propane-1,3-diol (BMP)"},"2,2-bis(bromomethyl)propane-1,3-diol (BMP)","2,2-bis(bromomethyl)propane-1,3-diol (BMP)","2,2-双(溴甲基)丙烷-1,3-二醇(BMP)"]
[null,{"$f":"IF($B$1=\"English\",C2734,IF($B$1=\"Deutsch\",D2734,IF($B$1=\"中文\",E2734,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3-dibromo-1-propanol (2,3-DBPA) "},"2,3-dibromo-1-propanol (2,3-DBPA) ","2,3-dibromo-1-propanol (2,3-DBPA) ","2,3-二溴-1-丙醇 (2,3-DBPA) "]
[null,{"$f":"IF($B$1=\"English\",C2735,IF($B$1=\"Deutsch\",D2735,IF($B$1=\"中文\",E2735,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,4-dioxane"},"1,4-dioxane","1,4-Dioxan","1,4-二恶烷 "]
[null,{"$f":"IF($B$1=\"English\",C2736,IF($B$1=\"Deutsch\",D2736,IF($B$1=\"中文\",E2736,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Preparation of lubricant additive materials and of fuel system cleaners."},"Preparation of lubricant additive materials and of fuel system cleaners.","Verwendung als chemisches Zwischenprodukt. Herstellung von Schmiermitteladditivmaterialien und von Kraftstoffsystemreinigern in benzin- und dieselbetriebenen Straßenfahrzeugen und Schiffsdieselmotoren. Herstellung von Chemikalien, Gummiprodukten und Kunststoffprodukten.","润滑油添加剂材料和燃油系统清洁剂的制备。"]
[null,{"$f":"IF($B$1=\"English\",C2737,IF($B$1=\"Deutsch\",D2737,IF($B$1=\"中文\",E2737,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Not registered under REACH. May be used as solvent and corrosion inhibitor. "},"Not registered under REACH. May be used as solvent and corrosion inhibitor. ","nicht unter REACH registriert, daher liegen keine Informationen zu Verwendungen vor. \nBegrenzte Informationen über die Verwendung als Lösungsmittel und Korrosionsinhibitor.","未在 REACH 下注册。可用作溶剂和缓蚀剂。"]
[null,{"$f":"IF($B$1=\"English\",C2738,IF($B$1=\"Deutsch\",D2738,IF($B$1=\"中文\",E2738,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Flame retardants, plasticising additives in plastics, sealants, rubber and textiles"},"Flame retardants, plasticising additives in plastics, sealants, rubber and textiles","Verwendung als Flammschutzmittel und als sekundäre Weichmacheradditive in Kunststoffen, Dichtstoffen, Gummi und Textilien. Additive in Kühl- und Schmiermitteln in Maschinen und Herstellung von Metallprodukten.","塑料、密封剂、橡胶和纺织品中的阻燃剂、增塑添加剂"]
[null,{"$f":"IF($B$1=\"English\",C2739,IF($B$1=\"Deutsch\",D2739,IF($B$1=\"中文\",E2739,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biocides, leather tanning, x-ray film processing, cosmetics."},"Biocides, leather tanning, x-ray film processing, cosmetics.","Verwendung als Biozid, bei der Ledergerbung, Röntgenfilmverarbeitung und in der Kosmetikindustrie.","杀菌剂、皮革鞣制、X 光胶片处理、化妆品。"]
[null,{"$f":"IF($B$1=\"English\",C2740,IF($B$1=\"Deutsch\",D2740,IF($B$1=\"中文\",E2740,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Not registered under REACH. May be used in manufacture of phenolic and polycarbonate resin. "},"Not registered under REACH. May be used in manufacture of phenolic and polycarbonate resin. ","nicht unter REACH registriert, daher liegen keine Informationen zu Verwendungen vor. Mögliche Verwendung: Herstellung von Phenol- und Polycarbonatharzen. Freisetzung aus Harzauskleidungen bei der Verwendung als Korrosionsinhibitoren zur Beschichtung von Dosen in der Lebensmittelindustrie.","未在 REACH 下注册。 可用于制造酚醛树脂和聚碳酸酯树脂。 "]
[null,{"$f":"IF($B$1=\"English\",C2741,IF($B$1=\"Deutsch\",D2741,IF($B$1=\"中文\",E2741,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cleaning agents, cosmetics, in scented articles, polishes and wax blends."},"Cleaning agents, cosmetics, in scented articles, polishes and wax blends.","Duftstoff in der Kosmetikindustrie sowie in Wasch- und Reinigungsmitteln, Polituren und Wachsmischungen","清洁剂、化妆品、香味物品、抛光剂和蜡混合物。"]
[null,{"$f":"IF($B$1=\"English\",C2742,IF($B$1=\"Deutsch\",D2742,IF($B$1=\"中文\",E2742,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate."},"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate.","In der Polymerproduktion zur Herstellung von Kunststoffprodukten","TBNPA：塑料制品的聚合物生产制造，包括复合和转化以及作为中间体。 "]
[null,{"$f":"IF($B$1=\"English\",C2743,IF($B$1=\"Deutsch\",D2743,IF($B$1=\"中文\",E2743,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate."},"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate.","In der Polymerproduktion zur Herstellung von Kunststoffprodukten","TBNPA：塑料制品的聚合物生产制造，包括复合和转化以及作为中间体。 "]
[null,{"$f":"IF($B$1=\"English\",C2744,IF($B$1=\"Deutsch\",D2744,IF($B$1=\"中文\",E2744,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"BMP: manufacture of polymer resins and in one component foam (OCPF) application."},"BMP: manufacture of polymer resins and in one component foam (OCPF) application.","an Industriestandorten als reaktives Flammschutzmittel-Zwischenprodukt bei der Herstellung von Polymerharzen verwendet","BMP：聚合物树脂的制造和单组分泡沫 (OCPF) 应用。 "]
[null,{"$f":"IF($B$1=\"English\",C2745,IF($B$1=\"Deutsch\",D2745,IF($B$1=\"中文\",E2745,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"DBPA: registered as an intermediate."},"DBPA: registered as an intermediate.","als Zwischenprodukt bei der Herstellung von Feinchemikalien und Chemikalien einschließlich der Herstellung von Massenchemikalien im großen Maßstab verwendet","DBPA：注册为中间体。"]
[null,{"$f":"IF($B$1=\"English\",C2746,IF($B$1=\"Deutsch\",D2746,IF($B$1=\"中文\",E2746,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvent."},"Solvent.","Lösungsmittel bei der Synthese von Chemikalien","溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C2747,IF($B$1=\"Deutsch\",D2747,IF($B$1=\"中文\",E2747,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TSCA (Sec. 6(h))"},"TSCA (Sec. 6(h))","TSCA (Sec. 6(h))","TSCA 第 6(h)项"]
[null,{"$f":"IF($B$1=\"English\",C2748,IF($B$1=\"Deutsch\",D2748,IF($B$1=\"中文\",E2748,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TSCA (Sec. 5 (a)(2)"},"TSCA (Sec. 5 (a)(2)","TSCA (Sec. 5 (a)(2)","TSCA 第 5 (a)(2)款"]
[null,{"$f":"IF($B$1=\"English\",C2749,IF($B$1=\"Deutsch\",D2749,IF($B$1=\"中文\",E2749,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorobutadiene (HCBD)"},"Hexachlorobutadiene (HCBD)","Hexachlorobutadiene (HCBD)","六氯丁二烯 (HCBD)"]
[null,{"$f":"IF($B$1=\"English\",C2750,IF($B$1=\"Deutsch\",D2750,IF($B$1=\"中文\",E2750,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoyl fluoride, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-."},"Octanoyl fluoride, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-.","Octanoyl fluoride, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-.","2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-十五氟辛酰氟 。"]
[null,{"$f":"IF($B$1=\"English\",C2751,IF($B$1=\"Deutsch\",D2751,IF($B$1=\"中文\",E2751,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (PFOA)."},"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (PFOA).","Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (PFOA).","2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-十五氟辛酸（PFOA）。"]
[null,{"$f":"IF($B$1=\"English\",C2752,IF($B$1=\"Deutsch\",D2752,IF($B$1=\"中文\",E2752,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, silver (+) salt (1:1)."},"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, silver (+) salt (1:1).","Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, silver (+) salt (1:1).","2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-十五氟辛酸银 (+) 盐 (1:1)。"]
[null,{"$f":"IF($B$1=\"English\",C2753,IF($B$1=\"Deutsch\",D2753,IF($B$1=\"中文\",E2753,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, sodium salt (1:1)."},"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, sodium salt (1:1).","Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, sodium salt (1:1).","2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-十五氟辛酸钠盐 (1:1)。"]
[null,{"$f":"IF($B$1=\"English\",C2754,IF($B$1=\"Deutsch\",D2754,IF($B$1=\"中文\",E2754,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, potassium salt (1:1)."},"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, potassium salt (1:1).","Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, potassium salt (1:1).","2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-十五氟辛酸钾盐 (1:1)。"]
[null,{"$f":"IF($B$1=\"English\",C2755,IF($B$1=\"Deutsch\",D2755,IF($B$1=\"中文\",E2755,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, ammonium salt (1:1) (APFO)."},"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, ammonium salt (1:1) (APFO).","Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, ammonium salt (1:1) (APFO).","2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-十五氟辛酸铵盐 (1:1) (APFO)。"]
[null,{"$f":"IF($B$1=\"English\",C2756,IF($B$1=\"Deutsch\",D2756,IF($B$1=\"中文\",E2756,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-8-iodo-."},"Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-8-iodo-.","Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-8-iodo-.","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-十七氟-8-碘-辛烷 。"]
[null,{"$f":"IF($B$1=\"English\",C2757,IF($B$1=\"Deutsch\",D2757,IF($B$1=\"中文\",E2757,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-."},"1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-.","1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-.","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-十七氟-1-癸醇。"]
[null,{"$f":"IF($B$1=\"English\",C2758,IF($B$1=\"Deutsch\",D2758,IF($B$1=\"中文\",E2758,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-.heneicosafluoro-"},"1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-.heneicosafluoro-","1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-.heneicosafluoro-","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12- 二十四氟-1-十二醇。 "]
[null,{"$f":"IF($B$1=\"English\",C2759,IF($B$1=\"Deutsch\",D2759,IF($B$1=\"中文\",E2759,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-."},"Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-.","Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-.","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-十七氟-10-碘-癸烷。"]
[null,{"$f":"IF($B$1=\"English\",C2760,IF($B$1=\"Deutsch\",D2760,IF($B$1=\"中文\",E2760,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-12-iodo-."},"Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-12-iodo-.","Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-12-iodo-.","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-二十三氟-12-碘-十二烷。"]
[null,{"$f":"IF($B$1=\"English\",C2761,IF($B$1=\"Deutsch\",D2761,IF($B$1=\"中文\",E2761,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester."},"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester.","2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester.","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-二十四氟十二烷基酯-2-丙烯酸。"]
[null,{"$f":"IF($B$1=\"English\",C2762,IF($B$1=\"Deutsch\",D2762,IF($B$1=\"中文\",E2762,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester"},"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-十七氟癸酯-2-丙烯酸"]
[null,{"$f":"IF($B$1=\"English\",C2763,IF($B$1=\"Deutsch\",D2763,IF($B$1=\"中文\",E2763,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodo-."},"Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodo-.","Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodo-.","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-五氟-14-碘-十四烷。"]
[null,{"$f":"IF($B$1=\"English\",C2764,IF($B$1=\"Deutsch\",D2764,IF($B$1=\"中文\",E2764,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Tetradecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-."},"1-Tetradecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-.","1-Tetradecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-.","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-五氟-1-十四烷醇,。"]
[null,{"$f":"IF($B$1=\"English\",C2765,IF($B$1=\"Deutsch\",D2765,IF($B$1=\"中文\",E2765,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexadecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluoro-."},"1-Hexadecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluoro-.","1-Hexadecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluoro-.","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14, 14,15,15,16,16,16-九十四氟-1-十六醇。 "]
[null,{"$f":"IF($B$1=\"English\",C2766,IF($B$1=\"Deutsch\",D2766,IF($B$1=\"中文\",E2766,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodo-."},"Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodo-.","Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodo-.","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-九十四氟-16-碘-十六烷。"]
[null,{"$f":"IF($B$1=\"English\",C2767,IF($B$1=\"Deutsch\",D2767,IF($B$1=\"中文\",E2767,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (2:1)"},"Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (2:1)","Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (2:1)","2,2'-亚氨基双-乙醇 与 α-氟-ω-[2-(膦酰氧基)乙基]聚 (二氟亚甲基) 的化合物 (2:1)"]
[null,{"$f":"IF($B$1=\"English\",C2768,IF($B$1=\"Deutsch\",D2768,IF($B$1=\"中文\",E2768,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanol, 2,2'-iminobis-, compd. with .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoropoly(difluoromethylene)] (1:1)"},"Ethanol, 2,2'-iminobis-, compd. with .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoropoly(difluoromethylene)] (1:1)","Ethanol, 2,2'-iminobis-, compd. with .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoropoly(difluoromethylene)] (1:1)","2,2'-亚氨基双-乙醇与 α, α-[膦基双(氧-2,1-乙二基)]双[ω-氟聚(二氟亚甲基)] 的化合物(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2769,IF($B$1=\"Deutsch\",D2769,IF($B$1=\"中文\",E2769,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-, lithium salt (1:1) "},"Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-, lithium salt (1:1) ","Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-, lithium salt (1:1) ","α-[2-[(2-羧乙基)硫代]乙基]-ω-氟-聚(二氟亚甲基)，锂盐  (1:1) "]
[null,{"$f":"IF($B$1=\"English\",C2770,IF($B$1=\"Deutsch\",D2770,IF($B$1=\"中文\",E2770,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(difluoromethylene), .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-, ammonium salt (1:1)"},"Poly(difluoromethylene), .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-, ammonium salt (1:1)","Poly(difluoromethylene), .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-, ammonium salt (1:1)","α，α'-[膦基双(氧-2，1-乙二基)]双[ω-氟-聚(二氟亚甲基)，铵盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2771,IF($B$1=\"Deutsch\",D2771,IF($B$1=\"中文\",E2771,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:1) "},"Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:1) ","Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:1) ","α-氟-ω-[2-(膦酰氧基)乙基]聚(二氟亚甲基)，铵盐  (1:1) "]
[null,{"$f":"IF($B$1=\"English\",C2772,IF($B$1=\"Deutsch\",D2772,IF($B$1=\"中文\",E2772,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:2)"},"Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:2)","Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:2)","α-氟-ω-[2-(膦酰氧基)乙基]聚(二氟亚甲基)，铵盐  (1:2) "]
[null,{"$f":"IF($B$1=\"English\",C2773,IF($B$1=\"Deutsch\",D2773,IF($B$1=\"中文\",E2773,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (1:1)"},"Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (1:1)","Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (1:1)","2,2'-亚氨基双-乙醇与 α-氟-ω-[2-(膦酰氧基)乙基]聚 (二氟亚甲基)的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C2774,IF($B$1=\"Deutsch\",D2774,IF($B$1=\"中文\",E2774,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(oxy-1,2-ethanediyl), .alpha.-hydro-.omega.-hydroxy-, ether with .alpha.-fluoro-.omega.-(2-hydroxyethyl)poly(difluoromethylene) (1:1)"},"Poly(oxy-1,2-ethanediyl), .alpha.-hydro-.omega.-hydroxy-, ether with .alpha.-fluoro-.omega.-(2-hydroxyethyl)poly(difluoromethylene) (1:1)","Poly(oxy-1,2-ethanediyl), .alpha.-hydro-.omega.-hydroxy-, ether with .alpha.-fluoro-.omega.-(2-hydroxyethyl)poly(difluoromethylene) (1:1)","α-氢-ω-羟基聚氧乙烯与α-氟-ω-(2-羟乙基)聚(二氟亚甲基) (1:1)的醚化物"]
[null,{"$f":"IF($B$1=\"English\",C2775,IF($B$1=\"Deutsch\",D2775,IF($B$1=\"中文\",E2775,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Propanesulfonic acid, 2-methyl-, 2-[[1-oxo-3-[(.gamma.-.omega.-perfluoro- C4-16-alkyl)thio]propyl]amino] derivs., sodium salts"},"1-Propanesulfonic acid, 2-methyl-, 2-[[1-oxo-3-[(.gamma.-.omega.-perfluoro- C4-16-alkyl)thio]propyl]amino] derivs., sodium salts","1-Propanesulfonic acid, 2-methyl-, 2-[[1-oxo-3-[(.gamma.-.omega.-perfluoro- C4-16-alkyl)thio]propyl]amino] derivs., sodium salts","2-甲基-1-丙磺酸，2-[[1-氧代-3-[(γ-ω-全氟-C4-16-烷基)硫代]丙基]氨基]衍生物，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C2776,IF($B$1=\"Deutsch\",D2776,IF($B$1=\"中文\",E2776,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alcohols, C8-14, .gamma.-.omega.-perfluoro."},"Alcohols, C8-14, .gamma.-.omega.-perfluoro.","Alcohols, C8-14, .gamma.-.omega.-perfluoro.","C8-14，γ-ω-全氟醇类。"]
[null,{"$f":"IF($B$1=\"English\",C2777,IF($B$1=\"Deutsch\",D2777,IF($B$1=\"中文\",E2777,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Thiols, C8-20, .gamma.-.omega.-perfluoro, telomers with acrylamide."},"Thiols, C8-20, .gamma.-.omega.-perfluoro, telomers with acrylamide.","Thiols, C8-20, .gamma.-.omega.-perfluoro, telomers with acrylamide.","C8-20，γ-ω-全氟硫醇与丙烯酰胺的调聚物。"]
[null,{"$f":"IF($B$1=\"English\",C2778,IF($B$1=\"Deutsch\",D2778,IF($B$1=\"中文\",E2778,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-"},"Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","三氯(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-十七氟癸基)硅烷"]
[null,{"$f":"IF($B$1=\"English\",C2779,IF($B$1=\"Deutsch\",D2779,IF($B$1=\"中文\",E2779,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicic acid (H4SiO4), sodium salt (1:2), reaction products with chlorotrimethylsilane and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol."},"Silicic acid (H4SiO4), sodium salt (1:2), reaction products with chlorotrimethylsilane and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol.","Silicic acid (H4SiO4), sodium salt (1:2), reaction products with chlorotrimethylsilane and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol.","硅酸 (H4SiO4)，钠盐 (1:2)，与三甲基氯硅烷和 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-十七氟-1-癸醇 的反应产物。"]
[null,{"$f":"IF($B$1=\"English\",C2780,IF($B$1=\"Deutsch\",D2780,IF($B$1=\"中文\",E2780,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Thiols, C4-20, .gamma.-.omega.-perfluoro, telomers with acrylamide and acrylic acid, sodium salts."},"Thiols, C4-20, .gamma.-.omega.-perfluoro, telomers with acrylamide and acrylic acid, sodium salts.","Thiols, C4-20, .gamma.-.omega.-perfluoro, telomers with acrylamide and acrylic acid, sodium salts.","C4-20，γ-ω-全氟硫醇，丙烯酰胺和丙烯酸的调聚物，钠盐。 "]
[null,{"$f":"IF($B$1=\"English\",C2781,IF($B$1=\"Deutsch\",D2781,IF($B$1=\"中文\",E2781,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Propanaminium, 3-amino-N-(carboxymethyl)-N,N-dimethyl-, N-[2-[(.gamma.-.omega.-perfluoro-C4-20-a lkyl)thio]acetyl] derivs., inner salts."},"1-Propanaminium, 3-amino-N-(carboxymethyl)-N,N-dimethyl-, N-[2-[(.gamma.-.omega.-perfluoro-C4-20-a lkyl)thio]acetyl] derivs., inner salts.","1-Propanaminium, 3-amino-N-(carboxymethyl)-N,N-dimethyl-, N-[2-[(.gamma.-.omega.-perfluoro-C4-20-a lkyl)thio]acetyl] derivs., inner salts.","3-氨基-N-(羧甲基)-N，N-二甲基-1-丙胺，N-[2-[(γ-ω-全氟-C4-20-烷基)硫代]乙酰]衍生物, 内盐。 "]
[null,{"$f":"IF($B$1=\"English\",C2782,IF($B$1=\"Deutsch\",D2782,IF($B$1=\"中文\",E2782,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Examples of occurrence"},"Examples of occurrence","Beispiele Vorkommen","物质常见用途示例"]
[null,{"$f":"IF($B$1=\"English\",C2783,IF($B$1=\"Deutsch\",D2783,IF($B$1=\"中文\",E2783,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Bemerkungen","备注"]
[null,{"$f":"IF($B$1=\"English\",C2784,IF($B$1=\"Deutsch\",D2784,IF($B$1=\"中文\",E2784,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included ( E )\n- changed ( C )"},"Entry\n- included ( E )\n- changed ( C )","Eintrag\n- aufgenommen ( E )\n- geändert ( C )","录入记录\n-首次录入(E)\n-更新(C)"]
[null,{"$f":"IF($B$1=\"English\",C2785,IF($B$1=\"Deutsch\",D2785,IF($B$1=\"中文\",E2785,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C2786,IF($B$1=\"Deutsch\",D2786,IF($B$1=\"中文\",E2786,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Comments"},"Comments","Bemerkungen","备注"]
[null,{"$f":"IF($B$1=\"English\",C2787,IF($B$1=\"Deutsch\",D2787,IF($B$1=\"中文\",E2787,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Entry\n- included ( E )\n- changed ( C )"},"Entry\n- included ( E )\n- changed ( C )","Eintrag\n- aufgenommen ( E )\n- geändert ( C )","录入记录\n-首次录入(E)\n-更新(C)"]
[null,{"$f":"IF($B$1=\"English\",C2788,IF($B$1=\"Deutsch\",D2788,IF($B$1=\"中文\",E2788,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Examples occurence"},"Examples occurence","Examples occurence","物质常见用途示例"]
[null,{"$f":"IF($B$1=\"English\",C2789,IF($B$1=\"Deutsch\",D2789,IF($B$1=\"中文\",E2789,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Linear and branched perfluorocarboxylic acids of the formula CnF2n+1-C(= O)OH where n = 8, 9, 10, 11, 12, or 13 (C9-C14 PFCAs),including their salts, and any combinations thereof;\nPFNA - Perfluorononan-1-oic acid (C9-PFCA) \nPFDA - Nonadecafluorodecanoic acid (C10-PFCA) \nPFUnDA - Henicosafluoroundecanoic acid (C11-PFCA) \nPFDoDA - Tricosafluorododecanoic acid (C12-PFCA) \nPFTrDA - Pentacosafluorotridecanoic acid (C13-PFCA) \nPFTDA - Heptacosafluorotetradecanoic acid (C14-PFCA)"},"Linear and branched perfluorocarboxylic acids of the formula CnF2n+1-C(= O)OH where n = 8, 9, 10, 11, 12, or 13 (C9-C14 PFCAs),including their salts, and any combinations thereof;\nPFNA - Perfluorononan-1-oic acid (C9-PFCA) \nPFDA - Nonadecafluorodecanoic acid (C10-PFCA) \nPFUnDA - Henicosafluoroundecanoic acid (C11-PFCA) \nPFDoDA - Tricosafluorododecanoic acid (C12-PFCA) \nPFTrDA - Pentacosafluorotridecanoic acid (C13-PFCA) \nPFTDA - Heptacosafluorotetradecanoic acid (C14-PFCA)","Lineare und verzweigte perfluorierte Carbonsäuren mit der Formel CnF2n+1-C(= O)OH, wobei n = 8, 9, 10, 11, 12 oder 13 (C9-C14-PFCA) ist,einschließlich ihrer Salze und etwaiger Kombinationen davon.\nPFNA - Perfluorononan-1-oic acid (C9-PFCA) \nPFDA - Nonadecafluorodecanoic acid (C10-PFCA) \nPFUnDA - Henicosafluoroundecanoic acid (C11-PFCA) \nPFDoDA - Tricosafluorododecanoic acid (C12-PFCA) \nPFTrDA - Pentacosafluorotridecanoic acid (C13-PFCA) \nPFTDA - Heptacosafluorotetradecanoic acid (C14-PFCA) ","分子式 CnF2n+1-C(=O)OH 的直链和支链全氟羧酸，其中 n=8、9、10、11、12 或 13（C9-C14 PFCA），包括它们的盐类，以及它们的任何组合；\nPFNA - 全氟壬烷-1-油酸 (C9-PFCA)\nPFDA - 十九氟癸酸 (C10-PFCA)\nPFUnDA - 二十碳氟十一烷酸 (C11-PFCA)\nPFDoDA - 三氟十二烷酸 (C12-PFCA)\nPFTrDA - 五十二碳氟十三烷酸 (C13-PFCA)\nPFTDA - 七氟十四烷酸 (C14-PFCA) "]
[null,{"$f":"IF($B$1=\"English\",C2790,IF($B$1=\"Deutsch\",D2790,IF($B$1=\"中文\",E2790,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1.Shall not be manufactured, or placed on the market as substances on their own from 25 February 2023.\n\n2.Shall not, from 25 February 2023, be used in, or placed on the market in:\n(a)another substance, as a constituent;\n(b)a mixture;\n(c)an article,except\n\n if the concentration in the substance, the mixture, or the article is below 25 ppb for the sum of C9-C14 PFCAs and their salts or 260 ppb for the sum of C9-C14 PFCA-related substances.\n\n3 By way of derogation to paragraph 2, the concentration limit shall be 10 ppm for the sum of C9-C14 PFCAs, their salts and C9-C14 PFCA related substances, where they are present in a substance to be used as a transported isolated intermediate, provided that the conditions in points (a) to (f) of Article 18(4) of this Regulation are met for the manufacturing of fluorochemicals with a perfluoro carbon chain length equal to or shorter than 6 atoms. The Commission shall review this limit no later than 25 August 2023.\n\n4.Paragraph 2 shall apply from 4 July 2023to:\n(i)textiles for oil- and water-repellency for the protection of workers from dangerous liquids that comprise risks to their health and safety;\n(ii)the manufacture of polytetrafluoroethylene (PTFE) and polyvinylidene fluoride (PVDF) for the production of:\n— high performance, corrosion resistant gas filter membranes, water filter membranes and membranes for medical textiles;\n— industrial waste heat exchanger equipment;\n— industrial sealants capable of preventing leakage of volatile organic compounds and PM 2,5 particulates\n\n5.By way of derogation to paragraph 2, the use of C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall be allowed until 4 July 2025for:\n(i)photolithography or etch processes in semiconductor manufacturing;\n(ii)photographic coatings applied to films;\n(iii)invasive and implantable medical devices;\n(iv)fire-fighting foam for liquid fuel vapour suppression and liquid fuel fire (Class B fires) already installed in systems, including both mobile and fixed systems, subject to the following conditions:\n— fire-fighting foam that contains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall not be used for training;\n— fire-fighting foam that contains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall not be used for testing unless all releases are contained;\n— from 1 January 2023, uses of fire-fighting foam that con¬tains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall only be allowed to sites where all releases can be contained;\n— fire-fighting foam stockpiles that contain or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related sub¬stances shall be managed in accordance with Article 5 of Regulation (EU) 2019/1021. \n\n6.Paragraph 2(c) shall not apply to articles placed on the market before 25 February 2023.\n\n7.Paragraph 2 shall not apply to the can coating for  pressurised metered-dose inhalers until 25 August 2028.\n\n8.Paragraph 2 (c) shall apply from 31 December 2023to:\n(a)semiconductors on their own;\n(b)semiconductors incorporated in  semi-finished and  finished electronic equipment.\n\n9.Paragraph 2(c) shall apply from 31  December 2030to semiconductors  used in  spare or  replacement parts  for  finished electronic equipment placed on  the  market before 31  December 2023.\n\n10.Until 25  August  2024,  the  concentration limit referred to  in paragraph 2  shall  be 2 000ppb  for  the  sum  of  C9-C14 PFCAs  in fluoroplastics and  fluoroelastomers that contain perfluoroalkoxy groups. From 25  August  2024,  the  concentration limit  shall  be  100 ppb for  the  sum of  C9-C14 PFCAs, in  fluoroplastics and fluoroelastomers that contain perfluoroalkoxy groups. All emissions of C9-C14 PFCAs  during  the  manufacture  and  use  of  fluoroplastics and fluoroelastomers that contain perfluoroalkoxy groups shall be avoided and,  if  not  possible, reduced as  far  as  technically and  practically possible. This  derogation  shall not  apply to  articles referred to  in paragraph 2(c).  The  Commission shall  review this  derogation  no  later than 25 August 2024.\n\n11.The concentration limit referred to in paragraph 2 shall be 1  000ppb for the sum of C9-C14 PFCAs, where these are present in PTFE micro powders produced by ionising irradiation or by thermal degradation, as  well  as  in  mixtures and  articles for  industrial  and professional uses containing PTFE micro powders. All emissions of C9-C14 PFCAs  during  the  manufacture and  use  of  PTFE micro powders shall be  avoided and,  if  not  possible, reduced as  far  as technically and  practically possible. The  Commission shall review this derogation no later than 25 August 2024.\n\n12.For the purposes of this entry, C9-C14 PFCA-related substances are  substances that, based on  their molecular structure, are considered to  have  the  potential  to degrade or  be  transformed  to C9-C14 PFCAs.’\n"},"1.Shall not be manufactured, or placed on the market as substances on their own from 25 February 2023.\n\n2.Shall not, from 25 February 2023, be used in, or placed on the market in:\n(a)another substance, as a constituent;\n(b)a mixture;\n(c)an article,except\n\n if the concentration in the substance, the mixture, or the article is below 25 ppb for the sum of C9-C14 PFCAs and their salts or 260 ppb for the sum of C9-C14 PFCA-related substances.\n\n3 By way of derogation to paragraph 2, the concentration limit shall be 10 ppm for the sum of C9-C14 PFCAs, their salts and C9-C14 PFCA related substances, where they are present in a substance to be used as a transported isolated intermediate, provided that the conditions in points (a) to (f) of Article 18(4) of this Regulation are met for the manufacturing of fluorochemicals with a perfluoro carbon chain length equal to or shorter than 6 atoms. The Commission shall review this limit no later than 25 August 2023.\n\n4.Paragraph 2 shall apply from 4 July 2023to:\n(i)textiles for oil- and water-repellency for the protection of workers from dangerous liquids that comprise risks to their health and safety;\n(ii)the manufacture of polytetrafluoroethylene (PTFE) and polyvinylidene fluoride (PVDF) for the production of:\n— high performance, corrosion resistant gas filter membranes, water filter membranes and membranes for medical textiles;\n— industrial waste heat exchanger equipment;\n— industrial sealants capable of preventing leakage of volatile organic compounds and PM 2,5 particulates\n\n5.By way of derogation to paragraph 2, the use of C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall be allowed until 4 July 2025for:\n(i)photolithography or etch processes in semiconductor manufacturing;\n(ii)photographic coatings applied to films;\n(iii)invasive and implantable medical devices;\n(iv)fire-fighting foam for liquid fuel vapour suppression and liquid fuel fire (Class B fires) already installed in systems, including both mobile and fixed systems, subject to the following conditions:\n— fire-fighting foam that contains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall not be used for training;\n— fire-fighting foam that contains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall not be used for testing unless all releases are contained;\n— from 1 January 2023, uses of fire-fighting foam that con¬tains or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related substances shall only be allowed to sites where all releases can be contained;\n— fire-fighting foam stockpiles that contain or may contain C9-C14 PFCAs, their salts and C9-C14 PFCA-related sub¬stances shall be managed in accordance with Article 5 of Regulation (EU) 2019/1021. \n\n6.Paragraph 2(c) shall not apply to articles placed on the market before 25 February 2023.\n\n7.Paragraph 2 shall not apply to the can coating for  pressurised metered-dose inhalers until 25 August 2028.\n\n8.Paragraph 2 (c) shall apply from 31 December 2023to:\n(a)semiconductors on their own;\n(b)semiconductors incorporated in  semi-finished and  finished electronic equipment.\n\n9.Paragraph 2(c) shall apply from 31  December 2030to semiconductors  used in  spare or  replacement parts  for  finished electronic equipment placed on  the  market before 31  December 2023.\n\n10.Until 25  August  2024,  the  concentration limit referred to  in paragraph 2  shall  be 2 000ppb  for  the  sum  of  C9-C14 PFCAs  in fluoroplastics and  fluoroelastomers that contain perfluoroalkoxy groups. From 25  August  2024,  the  concentration limit  shall  be  100 ppb for  the  sum of  C9-C14 PFCAs, in  fluoroplastics and fluoroelastomers that contain perfluoroalkoxy groups. All emissions of C9-C14 PFCAs  during  the  manufacture  and  use  of  fluoroplastics and fluoroelastomers that contain perfluoroalkoxy groups shall be avoided and,  if  not  possible, reduced as  far  as  technically and  practically possible. This  derogation  shall not  apply to  articles referred to  in paragraph 2(c).  The  Commission shall  review this  derogation  no  later than 25 August 2024.\n\n11.The concentration limit referred to in paragraph 2 shall be 1  000ppb for the sum of C9-C14 PFCAs, where these are present in PTFE micro powders produced by ionising irradiation or by thermal degradation, as  well  as  in  mixtures and  articles for  industrial  and professional uses containing PTFE micro powders. All emissions of C9-C14 PFCAs  during  the  manufacture and  use  of  PTFE micro powders shall be  avoided and,  if  not  possible, reduced as  far  as technically and  practically possible. The  Commission shall review this derogation no later than 25 August 2024.\n\n12.For the purposes of this entry, C9-C14 PFCA-related substances are  substances that, based on  their molecular structure, are considered to  have  the  potential  to degrade or  be  transformed  to C9-C14 PFCAs.’\n","1.Dürfen ab dem 25. Februar 2023 nicht mehr als Stoffe selbst hergestellt oder in Verkehr gebracht werden.\n\n2.Dürfen ab dem 25. Februar 2023 nicht mehr verwendet oder in Verkehr gebracht werden\na)als Bestandteil eines anderen Stoffs,\nb)in einem Gemisch,\nc)in einem Erzeugnis,außer wenn die Konzentration im Stoff, im Gemisch oder in dem Erzeugnis weniger als 25 ppb für die Summe der C9-C14-PFCA und ihrer Salze oder 260 ppb für die Summe der C9-C14-PFCA-verwandten Stoffe beträgt.\n\n3.Abweichend von Absatz 2 beträgt der Konzentrationsgrenzwert für die Summe der C9-C14-PFCA, ihrer Salze und C9-C14-PFCA-verwandter Stoffe 10 ppm, wenn sie in einem Stoff vorhanden sind, der als transportiertes isoliertes Zwischenprodukt verwendet werden soll, sofern die Bedingungen des Artikels 18 Absatz 4 Buchstaben a bis f dieser Verordnung für die Herstellung von Fluorchemikalien mit einer Länge der Perfluorkohlenstoffkette von höchstens 6 Atomen erfüllt sind. Die Kommission überprüft diesen Grenzwert spätestens am 25. August 2023.\n\n4.Absatz 2 gilt ab dem 4. Juli 2023für\ni)öl- und wasserabweisende Textilien zum Schutz von Arbeitnehmern vor gefährlichen Flüssigkeiten, die Risiken für ihre Gesundheit und Sicherheit darstellen;\nii)die Herstellung von Polytetrafluorethylen (PTFE) und Polyvinyli¬denfluorid (PVDF) für die Herstellung von\n— hochleistungsfähigen, korrosionsbeständigen Gasfiltermembra¬nen, Wasserfiltermembranen und Membranen für medizinische Textilien,\n— industriellen Abwärmetauschern\n,— industriellen Dichtungsmassen, die das Austreten von flüchtigen organischen Verbindungen sowie von PM 2,5-Feinstaub verhin¬dern können.\n\n5.Abweichend von Absatz 2 ist die Verwendung von C9-C14-PFCA, ihren Salzen und C9-C14-PFCA-verwandten Stoffen bis zum 4. Juli 2025zulässig für\ni)fotolithografische oder Ätzverfahren bei der Halbleiterherstellung,\nii)fotografische Beschichtungen von Filmen,\niii)invasive und implantierbare Medizinprodukte,\niv)Feuerlöschschaum zur Bekämpfung von Dämpfen aus Flüssigbrennstoffen und Bränden von Flüssigbrennstoffen (Brandklasse B), der bereits in — mobile wie auch ortsfeste — Systeme eingefüllt ist, wobei folgende Bedingungen gelten:\n— Feuerlöschschaum, der C9-C14-PFCA, ihre Salze und C9-C14-PFCA-verwandte Stoffe enthält oder enthalten könnte, darf nicht für Ausbildungszwecke verwendet werden;\n— Feuerlöschschaum, der C9-C14-PFCA, ihre Salze und C9-C14-PFCA-verwandte Stoffe enthält oder enthalten könnte, darf nicht für Tests verwendet werden, es sei denn, alle Freiset¬zungen werden aufgefangen;\n— ab dem 1. Januar 2023 sind Verwendungen von Feuerlösch¬schaum, der C9-C14-PFCA, ihre Salze und C9-C14-PFCA-ver¬wandte Stoffe enthält oder enthalten könnte, nur an Standorten zulässig, an denen alle Freisetzungen aufgefangen werden kön¬nen;\n— Bestände von Feuerlöschschaum, der C9-C14-PFCA, ihre Salze und C9-C14-PFCA-verwandte Stoffe enthält oder enthalten könnte, sind im Einklang mit Artikel 5 der Verordnung (EU) 2019/1021 zu bewirtschaften. \n\n6.Absatz 2  Buchstabe c  gilt  nicht für  Erzeugnisse, die  vor  dem 25. Februar 2023in Verkehr gebracht wurden.\n7.Absatz 2 gilt bis zum 25. August 2028nicht für die Beschichtung der Dosen von Druckgas-Dosierinhalatoren.\n8.Absatz 2 Buchstabe c gilt ab dem 31. Dezember 2023für \na)Halbleiter an sich;\nb)Halbleiter, die in elektronische Halbfertig- und Fertiggeräte eingebaut sind.\n9.Absatz 2 Buchstabe c gilt ab dem 31. Dezember 2030für Halbleiter, die in Ersatzteilen für elektronische Fertiggeräte verwendet werden, die vor dem 31. Dezember 2023 in Verkehr gebracht wurden.\n10.Bis zum 25. August 2024 beträgt der Konzentrationsgrenzwert gemäß Absatz 2  für  die  Summe der  C9-C14-PFCA in  Fluorkunststoffen  und Fluorelastomeren,  die  Perfluoroalkoxy-Gruppen enthalten, 2 000ppb.  Ab dem 25. August 2024beträgt der Konzentrationsgrenzwert für die Summe der  C9-C14-PFCA  in  Fluorkunststoffen  und Fluorelastomeren,  die Perfluoroalkoxy-Gruppen enthalten,  100  ppb. Jegliche Emissionen von C9-C14-PFCA  bei  der  Herstellung  und  Verwendung von  Fluorkunststoffen und  Fluorelastomeren,  die  Perfluoroalkoxy-Gruppen enthalten, sind  zu vermeiden bzw.  —  falls  nicht möglich  —  soweit technisch und  praktisch durchführbar zu  verringern.  Diese Ausnahmeregelung gilt  nicht für  die  in Absatz 2  Buchstabe c  genannten  Erzeugnisse. Die  Kommission überprüft diese Ausnahmeregelung spätestens am 25. August 2024.\n11.Der Konzentrationsgrenzwert gemäß Absatz 2 beträgt 1 000ppb für  die  Summe der  C9-C14-PFCA, wenn diese in  PTFE-Mikropulvern enthalten sind, die  durch ionisierende Bestrahlung oder thermischen Abbau hergestellt  werden, sowie  in  Gemischen  und  Erzeugnissen für industrielle  und  gewerbliche  Zwecke,  die  PTFE-Mikropulver enthalten. Jegliche  Emissionen von C9-C14-PFCA bei  der  Herstellung  und Verwendung von  PTFE-Mikropulver sind  zu  vermeiden bzw.  —  falls nicht möglich  —  soweit technisch  und  praktisch durchführbar zu verringern.  Die Kommission überprüft  diese Ausnahmeregelung spätestens am 25. August 2024.\n12.Für  die  Zwecke  dieses Eintrags bezeichnet „C9-C14-PFCA- verwandte Stoffe“  Stoffe,  die  aufgrund ihrer Molekularstruktur potenziell zu   C9-C14-PFCA abgebaut oder in   C9-C14-PFCA umgewandelt werden.","1. 自 2023 年 2 月 25 日起，不得再作为物质制造或投放 市场。\n\n2. 2023 年 2 月 25 日起不得再以以下形式使用或投放市场：\na) 作为另一种物质的一部分，\nb) 在混合物中，\nc) 在物品中，\n除非该物质、混合物或物品中 C9-C14-PFCAs 及其盐类总和低于 25 ppb，或 C9-C14-PFCAs 相关物质总和低于 260 ppb .\n\n3. 作为对第 2 段的豁免，如果 C9-C14-FCAs及其盐类和 C9-C14-PFCAs 相关物质存在于用作可转移的分离中间体 的物质中，它们的总含量限值为 10 ppm，前提是满足本条例第 18(4) 款 a 至 f 项关于生产全氟化碳链长度不超过 6 个原子的氟化物的条件。委员会最迟将在 2023 年 8 月 25 日之前审查这一限值。\n\n4. 第 2 段自 2023 年 7 月 4 日起适用于以下情形：\ni)防油防水纺织品，以保护工人免受对其健康和安全构成风险的危险液体；\nii) 聚四氟乙烯 (PTFE) 和聚偏二氟乙烯 (PVDF) 的生产，用于生产：\n-高性能、耐腐蚀的气体过滤膜、水过滤膜和医用纺织品膜，\n-工业废热交换器,\n-可防止挥发性有机化合物和 PM2.5 细粉尘逸出的工业 密封剂。\n\n5. 作为对第 2 段的豁免，在 2025 年 7 月 4 日之前，允许C9-C14-PFCAs及其盐类和 C9-C14-PFCAs 相关物质使用在以下情形：\ni)半导体制造中的光刻或蚀刻工艺，\nii)胶片上的照相涂层，\niii)切入式和植入式医疗器械，\niv)用于扑灭液体燃料蒸气和液体燃料火灾(B级火灾)的灭火泡沫，该泡沫已经填充在移动式和固定式的系统中，其中适用以下条件：\n- 含有或可能含有 C9-C14-PFCAs及其盐类和 C9-C14-PFCAs 相关物质的消防泡沫不得用于培训目的；\n- 含有或可能含有 C9-C14-PFCAs及其盐类和 C9-C14-PFCAs相关物质的消防泡沫不得用于测试，除非所有释放物都能够被集中收集；\n- 从 2023 年 1 月 1 日起，只允许在含有或可能含有 C9-C14-PFCAs及其盐类和 C9-C14-PFCAs 相关物质的灭火泡沫中使用含有所有释放物都能够被集中收集的场所；\n- 含有或可能含有 C9-C14-PFCAs及其盐类和 C9-C14-PFCAs 相关物质的消防泡沫库存必须根据法规 (EU) 2019/1021 第 5 条进行管理。\n\n6、第2款c项不适用于2023年2月25日之前投放市场的产品。\n\n7. 在 2028 年 8 月 25 日之前，第 2 段不适用于加压式计量吸入器的罐体涂层。\n\n8. 第 2 款 c 项应自 2023 年 12 月 31 日起适用于\na) 半导体本身；\nb) 内置于半成品和成品电子设备中的半导体。\n\n9、第2款c款自2030年12月31日起适用于2023年12月31日之前投放市场的成品电子设备的备件中使用的半导体。\n\n10、截至2024年8月25日，含全氟烷氧基的氟塑料和含氟弹性体中C9-C14-PFCAs含量总和，按照第2段的规定，限值为2000ppb。从 2024 年 8 月 25 日起，含全氟烷氧基的氟塑料和氟弹性体中 C9-C14-PFCAs 含量总和的限值为 100 ppb。在生产和使用含有全氟烷氧基的氟塑料和氟弹性体时，应避免C9-C14-PFCAs的任何排放，如果无法避免，则从技术上和实践上尽可能减少其排放。此豁免不适用于第 2(c) 项 中提及的产品。委员会最迟将在 2024 年 8 月 25 日之前审查这一豁免项。\n\n11. 根据第 2 段，在通过电离辐射或热降解产生的 PTFE 微粉中，以及工业和商业用途的含有聚四氟乙烯微粉的配置品和物品中，C9-C14-PFCA 含量总和的限值为 1,000 ppb。在生产和使用PTFE 微粉过程中，应避免C9-C14-PFCA 的任何排放，如果无法避免，则从技术上和实践上尽可能减少其排放。此豁免不适用于第 2(c) 项 中提及的产品。委员会最迟将在 2024 年 8 月 25 日之前审查这一豁免项。\n\n12. 就本条目而言，“C9-C14-PFCA 相关物质”是指由于其分子结构而可能降解为 C9-C14-PFCA 或转化为 C9-C14-PFCA 的物质。"]
[null,{"$f":"IF($B$1=\"English\",C2791,IF($B$1=\"Deutsch\",D2791,IF($B$1=\"中文\",E2791,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"25 ppb for single substance, sum value 260 ppb"},"25 ppb for single substance, sum value 260 ppb","25 ppb für einzelne Substanz, Gesamtwert 260 ppb","单一物质 25 ppb，总量 260 ppb "]
[null,{"$f":"IF($B$1=\"English\",C2792,IF($B$1=\"Deutsch\",D2792,IF($B$1=\"中文\",E2792,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Asbestos, all mineral groups"},"Asbestos, all mineral groups","Asbest, alle Mineralgruppen","石棉，所有矿物组"]
[null,{"$f":"IF($B$1=\"English\",C2793,IF($B$1=\"Deutsch\",D2793,IF($B$1=\"中文\",E2793,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mercury and ist compounds"},"Mercury and ist compounds","Quecksilber und seine Verbindungen","汞及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C2794,IF($B$1=\"Deutsch\",D2794,IF($B$1=\"中文\",E2794,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ozon depleting substances\nz.B.: CFC, Halone"},"Ozon depleting substances\nz.B.: CFC, Halone","Ozonabbauende Stoffe \nz.B.: FCKW, Halone","破坏臭氧层物质，如：氟利昂，哈龙等"]
[null,{"$f":"IF($B$1=\"English\",C2795,IF($B$1=\"Deutsch\",D2795,IF($B$1=\"中文\",E2795,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Greenhouse gases\nz.B.  carbon dioxide (CO2), Methane (CH4), nitrous oxide (N2O), hydrofluorocarbons (HFCs), perfluorocarbons (PFCs), and sulfur hexafluoride (SF6), Nitrogen trifluoride (NF3). "},"Greenhouse gases\nz.B.  carbon dioxide (CO2), Methane (CH4), nitrous oxide (N2O), hydrofluorocarbons (HFCs), perfluorocarbons (PFCs), and sulfur hexafluoride (SF6), Nitrogen trifluoride (NF3). ","Treibhausgase\nz.B.  Kohlendioxid (CO2), Methan (CH4), Distickstoffmonoxid (N2O), Fluorkohlenwasserstoffe (FKW), Perfluorierte Kohlenwasserstoffe (PFC),  Schwefelhexafluorid (SF6), Stickstofftrifluorid (NF3). ","温室气体\n如： 二氧化碳 (CO2)、甲烷 (CH4)、一氧化二氮 (N2O)、氢氟烃 (HFCs)、全氟化碳 (PFCs) 和六氟化硫 (SF6)、三氟化氮 (NF3)。 "]
[null,{"$f":"IF($B$1=\"English\",C2796,IF($B$1=\"Deutsch\",D2796,IF($B$1=\"中文\",E2796,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Radioactive substances"},"Radioactive substances","Radioaktive Stoffe","放射性物质"]
[null,{"$f":"IF($B$1=\"English\",C2797,IF($B$1=\"Deutsch\",D2797,IF($B$1=\"中文\",E2797,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biocides"},"Biocides","Biozide","杀菌剂"]
[null,{"$f":"IF($B$1=\"English\",C2798,IF($B$1=\"Deutsch\",D2798,IF($B$1=\"中文\",E2798,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Endosulfan and its isomers"},"Endosulfan and its isomers","Endosulfan and its isomers","硫丹及其异构体"]
[null,{"$f":"IF($B$1=\"English\",C2799,IF($B$1=\"Deutsch\",D2799,IF($B$1=\"中文\",E2799,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Endosulfan alpha-isomer"},"Endosulfan alpha-isomer","Endosulfan alpha-isomer"," 硫丹 α 异构体 "]
[null,{"$f":"IF($B$1=\"English\",C2800,IF($B$1=\"Deutsch\",D2800,IF($B$1=\"中文\",E2800,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Endosulfan"},"Endosulfan","Endosulfan","硫丹"]
[null,{"$f":"IF($B$1=\"English\",C2801,IF($B$1=\"Deutsch\",D2801,IF($B$1=\"中文\",E2801,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Endosulfan beta-isomer"},"Endosulfan beta-isomer","Endosulfan beta-isomer","硫丹β-异构体"]
[null,{"$f":"IF($B$1=\"English\",C2802,IF($B$1=\"Deutsch\",D2802,IF($B$1=\"中文\",E2802,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptabromodiphenyl ether (Group)"},"Heptabromodiphenyl ether (Group)","Heptabromodiphenyl ether (Group)","  七溴二苯醚（组）"]
[null,{"$f":"IF($B$1=\"English\",C2803,IF($B$1=\"Deutsch\",D2803,IF($B$1=\"中文\",E2803,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl ether, heptabromo derivative"},"Diphenyl ether, heptabromo derivative","Diphenyl ether, heptabromo derivative"," 二苯醚，七溴衍生物"]
[null,{"$f":"IF($B$1=\"English\",C2804,IF($B$1=\"Deutsch\",D2804,IF($B$1=\"中文\",E2804,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromocyclododecane (HBCDD)"},"Hexabromocyclododecane (HBCDD)","Hexabromocyclododecane (HBCDD)"," 六溴环十二烷 (HBCDD) "]
[null,{"$f":"IF($B$1=\"English\",C2805,IF($B$1=\"Deutsch\",D2805,IF($B$1=\"中文\",E2805,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"gamma-hexabromocyclododecane"},"gamma-hexabromocyclododecane","gamma-hexabromocyclododecane","γ-六溴环十二烷"]
[null,{"$f":"IF($B$1=\"English\",C2806,IF($B$1=\"Deutsch\",D2806,IF($B$1=\"中文\",E2806,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"beta-hexabromocyclododecane"},"beta-hexabromocyclododecane","beta-hexabromocyclododecane"," β-六溴环十二烷 "]
[null,{"$f":"IF($B$1=\"English\",C2807,IF($B$1=\"Deutsch\",D2807,IF($B$1=\"中文\",E2807,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromocyclododecane"},"Hexabromocyclododecane","Hexabromocyclododecane","六溴环十二烷 "]
[null,{"$f":"IF($B$1=\"English\",C2808,IF($B$1=\"Deutsch\",D2808,IF($B$1=\"中文\",E2808,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,5,6,9,10-hexabromocyclodecane"},"1,2,5,6,9,10-hexabromocyclodecane","1,2,5,6,9,10-hexabromocyclodecane","1,2,5,6,9,10-六溴环癸烷"]
[null,{"$f":"IF($B$1=\"English\",C2809,IF($B$1=\"Deutsch\",D2809,IF($B$1=\"中文\",E2809,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"alpha-hexabromocyclododecane"},"alpha-hexabromocyclododecane","alpha-hexabromocyclododecane"," α-六溴环十二烷 "]
[null,{"$f":"IF($B$1=\"English\",C2810,IF($B$1=\"Deutsch\",D2810,IF($B$1=\"中文\",E2810,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromodiphenyl ether (group)"},"Hexabromodiphenyl ether (group)","Hexabromodiphenyl ether (group)","六溴二苯醚（组） "]
[null,{"$f":"IF($B$1=\"English\",C2811,IF($B$1=\"Deutsch\",D2811,IF($B$1=\"中文\",E2811,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl ether, hexabromo derivative"},"Diphenyl ether, hexabromo derivative","Diphenyl ether, hexabromo derivative","二苯醚，六溴衍生物"]
[null,{"$f":"IF($B$1=\"English\",C2812,IF($B$1=\"Deutsch\",D2812,IF($B$1=\"中文\",E2812,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,3-tribromo-4-(2,4,5-tribromophenoxy)benzene"},"1,2,3-tribromo-4-(2,4,5-tribromophenoxy)benzene","1,2,3-tribromo-4-(2,4,5-tribromophenoxy)benzene"," 1,2,3-三溴-4-(2,4,5-三溴苯氧基)苯"]
[null,{"$f":"IF($B$1=\"English\",C2813,IF($B$1=\"Deutsch\",D2813,IF($B$1=\"中文\",E2813,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorocyclohexanes, including lindane"},"Hexachlorocyclohexanes, including lindane","Hexachlorocyclohexanes, including lindane"," 六氯环己烷，包括林丹"]
[null,{"$f":"IF($B$1=\"English\",C2814,IF($B$1=\"Deutsch\",D2814,IF($B$1=\"中文\",E2814,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"γ-HCH or γ-BHC"},"γ-HCH or γ-BHC","γ-HCH or γ-BHC","γ-HCH（六氯环己烷） or γ-BHC（六氯化苯）"]
[null,{"$f":"IF($B$1=\"English\",C2815,IF($B$1=\"Deutsch\",D2815,IF($B$1=\"中文\",E2815,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"BHC or HCH"},"BHC or HCH","BHC or HCH","六氯化苯BHC  或 六氯环己烷HCH（俗称六六六）"]
[null,{"$f":"IF($B$1=\"English\",C2816,IF($B$1=\"Deutsch\",D2816,IF($B$1=\"中文\",E2816,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1α,2β,3α,4β,5α,6β)-1,2,3,4,5,6-hexachlorocyclohexane"},"(1α,2β,3α,4β,5α,6β)-1,2,3,4,5,6-hexachlorocyclohexane","(1α,2β,3α,4β,5α,6β)-1,2,3,4,5,6-hexachlorocyclohexane","(1α,2β,3α,4β,5α,6β)-1,2,3,4,5,6-六氯环己烷"]
[null,{"$f":"IF($B$1=\"English\",C2817,IF($B$1=\"Deutsch\",D2817,IF($B$1=\"中文\",E2817,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1α,2α,3β,4α,5β,6β)-1,2,3,4,5,6-hexachlorocyclohexane"},"(1α,2α,3β,4α,5β,6β)-1,2,3,4,5,6-hexachlorocyclohexane","(1α,2α,3β,4α,5β,6β)-1,2,3,4,5,6-hexachlorocyclohexane"," (1α,2α,3β,4α,5β,6β)-1,2,3,4,5,6-六氯环己烷"]
[null,{"$f":"IF($B$1=\"English\",C2818,IF($B$1=\"Deutsch\",D2818,IF($B$1=\"中文\",E2818,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentabromodiphenyl ether (group)"},"Pentabromodiphenyl ether (group)","Pentabromodiphenyl ether (group)"," 五溴二苯醚（组）"]
[null,{"$f":"IF($B$1=\"English\",C2819,IF($B$1=\"Deutsch\",D2819,IF($B$1=\"中文\",E2819,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl ether, pentabromo derivative"},"Diphenyl ether, pentabromo derivative","Diphenyl ether, pentabromo derivative"," 二苯醚，五溴衍生物"]
[null,{"$f":"IF($B$1=\"English\",C2820,IF($B$1=\"Deutsch\",D2820,IF($B$1=\"中文\",E2820,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-tribromo-2-(3,4-dibromophenoxy)benzene"},"1,3,5-tribromo-2-(3,4-dibromophenoxy)benzene","1,3,5-tribromo-2-(3,4-dibromophenoxy)benzene"," 1,3,5-三溴-2-(3,4-二溴苯氧基)苯"]
[null,{"$f":"IF($B$1=\"English\",C2821,IF($B$1=\"Deutsch\",D2821,IF($B$1=\"中文\",E2821,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2,3-tribromo-4-(2,4-dibromophenoxy)benzene"},"1,2,3-tribromo-4-(2,4-dibromophenoxy)benzene","1,2,3-tribromo-4-(2,4-dibromophenoxy)benzene"," 1,2,3-三溴-4-(2,4-二溴苯氧基)苯"]
[null,{"$f":"IF($B$1=\"English\",C2822,IF($B$1=\"Deutsch\",D2822,IF($B$1=\"中文\",E2822,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenol and its salts and esters"},"Pentachlorophenol and its salts and esters","Pentachlorophenol and its salts and esters"," 五氯苯酚及其盐类和酯类"]
[null,{"$f":"IF($B$1=\"English\",C2823,IF($B$1=\"Deutsch\",D2823,IF($B$1=\"中文\",E2823,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acetic acid, 2,2-dichloro-, 2,3,4,5,6-pentachlorophenyl ester"},"Acetic acid, 2,2-dichloro-, 2,3,4,5,6-pentachlorophenyl ester","Acetic acid, 2,2-dichloro-, 2,3,4,5,6-pentachlorophenyl ester","2,2-二氯-,2,3,4,5,6-五氯苯基 乙酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2824,IF($B$1=\"Deutsch\",D2824,IF($B$1=\"中文\",E2824,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Carbonic acid, 1,1-dimethylethyl pentachlorophenyl ester"},"Carbonic acid, 1,1-dimethylethyl pentachlorophenyl ester","Carbonic acid, 1,1-dimethylethyl pentachlorophenyl ester","1,1-二甲基乙基五氯苯基 碳酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2825,IF($B$1=\"Deutsch\",D2825,IF($B$1=\"中文\",E2825,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Acetic acid, 2,2,2-trichloro-, 2,3,4,5,6-pentachlorophenyl ester"},"Acetic acid, 2,2,2-trichloro-, 2,3,4,5,6-pentachlorophenyl ester","Acetic acid, 2,2,2-trichloro-, 2,3,4,5,6-pentachlorophenyl ester","2,2,2-三氯-，2,3,4,5,6-五氯苯 乙酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2826,IF($B$1=\"Deutsch\",D2826,IF($B$1=\"中文\",E2826,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substance group"},"Substance group","Stoffgruppe","物质组"]
[null,{"$f":"IF($B$1=\"English\",C2827,IF($B$1=\"Deutsch\",D2827,IF($B$1=\"中文\",E2827,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenol"},"Pentachlorophenol","Pentachlorophenol","五氯苯酚"]
[null,{"$f":"IF($B$1=\"English\",C2828,IF($B$1=\"Deutsch\",D2828,IF($B$1=\"中文\",E2828,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium pentachlorophenolate"},"Sodium pentachlorophenolate","Sodium pentachlorophenolate"," 五氯酚钠 "]
[null,{"$f":"IF($B$1=\"English\",C2829,IF($B$1=\"Deutsch\",D2829,IF($B$1=\"中文\",E2829,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenyl laurate"},"Pentachlorophenyl laurate","Pentachlorophenyl laurate","五氯苯月桂酸酯"]
[null,{"$f":"IF($B$1=\"English\",C2830,IF($B$1=\"Deutsch\",D2830,IF($B$1=\"中文\",E2830,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium pentachlorophenolate"},"Potassium pentachlorophenolate","Potassium pentachlorophenolate"," 五氯酚钾"]
[null,{"$f":"IF($B$1=\"English\",C2831,IF($B$1=\"Deutsch\",D2831,IF($B$1=\"中文\",E2831,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N2-benzyl pentachlorophenyl N2-carboxy-L-(2-aminoglutaramate)"},"N2-benzyl pentachlorophenyl N2-carboxy-L-(2-aminoglutaramate)","N2-benzyl pentachlorophenyl N2-carboxy-L-(2-aminoglutaramate)"," N2-苄基五氯苯基 N2-羧基-L-(2-氨基戊二酸)"]
[null,{"$f":"IF($B$1=\"English\",C2832,IF($B$1=\"Deutsch\",D2832,IF($B$1=\"中文\",E2832,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perchlorophenyl N-(benzyloxycarbonyl)-L-isoleucinate"},"Perchlorophenyl N-(benzyloxycarbonyl)-L-isoleucinate","Perchlorophenyl N-(benzyloxycarbonyl)-L-isoleucinate"," N-(苄氧基羰基)-L-异亮氨酸全氯苯基酯"]
[null,{"$f":"IF($B$1=\"English\",C2833,IF($B$1=\"Deutsch\",D2833,IF($B$1=\"中文\",E2833,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perchlorophenyl S-benzyl-N-(benzyloxycarbonyl)-L-cysteinate"},"Perchlorophenyl S-benzyl-N-(benzyloxycarbonyl)-L-cysteinate","Perchlorophenyl S-benzyl-N-(benzyloxycarbonyl)-L-cysteinate"," 全氯苯基 S-苄基-N-(苄氧基羰基)-L-半胱氨酸 "]
[null,{"$f":"IF($B$1=\"English\",C2834,IF($B$1=\"Deutsch\",D2834,IF($B$1=\"中文\",E2834,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenyl N-[[(4-methoxyphenyl)methoxy]carbonyl]-L-serinate"},"Pentachlorophenyl N-[[(4-methoxyphenyl)methoxy]carbonyl]-L-serinate","Pentachlorophenyl N-[[(4-methoxyphenyl)methoxy]carbonyl]-L-serinate","五氯苯基 N-[[(4-甲氧基苯基)甲氧基]羰基]-L-丝氨酸"]
[null,{"$f":"IF($B$1=\"English\",C2835,IF($B$1=\"Deutsch\",D2835,IF($B$1=\"中文\",E2835,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limits"},"Limits","Grenzwerte","限值"]
[null,{"$f":"IF($B$1=\"English\",C2836,IF($B$1=\"Deutsch\",D2836,IF($B$1=\"中文\",E2836,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibition of use, limits and exemptions according specific regulation "},"Prohibition of use, limits and exemptions according specific regulation ","Verwendungsverbot, Grenzwerte und Ausnahmen durch spezifische Regelungen","根据特定法规，禁止使用、限制和豁免"]
[null,{"$f":"IF($B$1=\"English\",C2837,IF($B$1=\"Deutsch\",D2837,IF($B$1=\"中文\",E2837,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- thermal insulations\n- friction coatings\n- seals\n- building materials"},"- thermal insulations\n- friction coatings\n- seals\n- building materials","- Isolationen\n'- Dichtungen\n'- Reibbeläge, Bremsbeläge","- 隔热材料\n- 摩擦涂层\n- 密封件\n- 建筑材料 "]
[null,{"$f":"IF($B$1=\"English\",C2838,IF($B$1=\"Deutsch\",D2838,IF($B$1=\"中文\",E2838,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"electrical contacts"},"electrical contacts","- elektrische Kontakte","- 电触点 "]
[null,{"$f":"IF($B$1=\"English\",C2839,IF($B$1=\"Deutsch\",D2839,IF($B$1=\"中文\",E2839,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- coolants\n- firefighting agents\n- cleaning agents"},"- coolants\n- firefighting agents\n- cleaning agents","- Kühlmitttel\n'- Löschmittel\n'- Reinigungsmittel","- 冷却剂\n- 灭火剂\n- 清洁剂"]
[null,{"$f":"IF($B$1=\"English\",C2840,IF($B$1=\"Deutsch\",D2840,IF($B$1=\"中文\",E2840,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- coolants\n- firefighting agents\n- cleaning agents"},"- coolants\n- firefighting agents\n- cleaning agents","- Kühlmitttel\n'- Löschmittel\n'- Reinigungsmittel","- 冷却剂\n- 灭火剂\n- 清洁剂"]
[null,{"$f":"IF($B$1=\"English\",C2841,IF($B$1=\"Deutsch\",D2841,IF($B$1=\"中文\",E2841,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Contamination in steel or other metals"},"Contamination in steel or other metals","- Verunreinigungen in Stahl","- 钢或其他金属的污染"]
[null,{"$f":"IF($B$1=\"English\",C2842,IF($B$1=\"Deutsch\",D2842,IF($B$1=\"中文\",E2842,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Liquids, packaging, coatings on products to which substances have been added/treated to prevent infestation by harmful organisms such as algae, fungi, bacteria, in order to preserve the original properties such as paints, liquids, plastics, sealants and adhesives, binders."},"Liquids, packaging, coatings on products to which substances have been added/treated to prevent infestation by harmful organisms such as algae, fungi, bacteria, in order to preserve the original properties such as paints, liquids, plastics, sealants and adhesives, binders.","Flüssigkeiten, Verpackungen, Beschichtungen auf Produkten, die mit Substanzen versetzt/behandelt sind, die einem Befall durch Schadorganismen wie Algen, Pilze, Bakterien, um die ursprünglichen Eigenschaften wie Farben, Flüssigkeiten, Kunststoffe, Dichtungs- und Klebkitten, Bindemitteln zu erhalten.","液体、包装、产品涂层，已添加/处理物质以防止有害生物（如藻类、真菌、细菌）的侵扰，防止油漆、液体、塑料、密封剂和粘合剂、粘合剂等变质。"]
[null,{"$f":"IF($B$1=\"English\",C2843,IF($B$1=\"Deutsch\",D2843,IF($B$1=\"中文\",E2843,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Prohibition of use, exemption for ionization chamber smoke detector"},"Prohibition of use, exemption for ionization chamber smoke detector","Verwendungsverbot, Ausnahme für Ionisationsrauchmelder","禁止使用，电离室烟雾探测器可豁免"]
[null,{"$f":"IF($B$1=\"English\",C2844,IF($B$1=\"Deutsch\",D2844,IF($B$1=\"中文\",E2844,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Asbestos Convention 1986 (No. 162), \n'- EU-REACh Annex XVII \n'- International Maritime Organization"},"- Asbestos Convention 1986 (No. 162), \n'- EU-REACh Annex XVII \n'- International Maritime Organization","- Asbestos Convention 1986 (No. 162), \n'- EU-REACh Annex XVII \n'- International Maritime Organization","- 1986 年石棉公约（第 162 号），\n'- 欧盟 REACh 附件 XVII\n'- 国际海事组织 "]
[null,{"$f":"IF($B$1=\"English\",C2845,IF($B$1=\"Deutsch\",D2845,IF($B$1=\"中文\",E2845,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Minamata Convention 1. Januar 2018 \n'- EU Mercury regulation  2017/852\n'- EU RoHS\n'- EU ELV\n"},"- Minamata Convention 1. Januar 2018 \n'- EU Mercury regulation  2017/852\n'- EU RoHS\n'- EU ELV\n","- Minamata Convention 1. Januar 2018 \n'- EU Mercury regulation  2017/852\n'- EU RoHS\n'- EU ELV\n","- 水俣公约 1. 2018 年 1 月\n'- 欧盟汞法规 2017/852\n'- 欧盟 RoHS\n'- 欧盟 ELV \n"]
[null,{"$f":"IF($B$1=\"English\",C2846,IF($B$1=\"Deutsch\",D2846,IF($B$1=\"中文\",E2846,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Montreal Protocol 1987\n'- EU 1005/2009"},"- Montreal Protocol 1987\n'- EU 1005/2009","- Montral Protocol 1987\n'- EU 1005/2009","- 1987 年蒙特利尔议定书\n'- 欧盟 1005/2009 （关于破坏臭氧层物质的欧盟法规）"]
[null,{"$f":"IF($B$1=\"English\",C2847,IF($B$1=\"Deutsch\",D2847,IF($B$1=\"中文\",E2847,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Kyoto Protokoll 16 February 2005 incl. Doha Annex\n'- EU 2021/1119, 401/2009, 2018/1999 (‘European Climate Law’)"},"- Kyoto Protokoll 16 February 2005 incl. Doha Annex\n'- EU 2021/1119, 401/2009, 2018/1999 (‘European Climate Law’)","- Kyoto Protokoll 16 February 2005 incl. Doha Annex\n'- EU 2021/1119, 401/2009, 2018/1999 (‘European Climate Law’)","- 《京都议定书》 2005 年 2 月 16 日，包括《多哈附件》\n'- EU 2021/1119、401/2009、2018/1999（“欧洲气候法”） "]
[null,{"$f":"IF($B$1=\"English\",C2848,IF($B$1=\"Deutsch\",D2848,IF($B$1=\"中文\",E2848,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EU Biocid Regulation EC 528/2012"},"EU Biocid Regulation EC 528/2012","EU Biocid Regulation EC 528/2012","欧盟杀菌剂法规 EC 528/2012"]
[null,{"$f":"IF($B$1=\"English\",C2849,IF($B$1=\"Deutsch\",D2849,IF($B$1=\"中文\",E2849,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"- Stockholm Convention\n' EU POP Regulation EU 2019/1021 "},"- Stockholm Convention\n' EU POP Regulation EU 2019/1021 ","- Stockholm Convention\n' EU POP Regulation EU 2019/1021 ","-斯德哥尔摩公约\n' 欧盟 POP（持久性有机污染物） 法规 EU 2019/1021 "]
[null,{"$f":"IF($B$1=\"English\",C2850,IF($B$1=\"Deutsch\",D2850,IF($B$1=\"中文\",E2850,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N-Dimethylformamid"},"N,N-Dimethylformamid","N,N-Dimethylformamid","N,N-二甲基甲酰胺"]
[null,{"$f":"IF($B$1=\"English\",C2851,IF($B$1=\"Deutsch\",D2851,IF($B$1=\"中文\",E2851,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market as a substance on its own, as a constituent of other\nsubstances, or in mixtures in a concentration equal to or greater than 0,3 % after 12\nDecember 2023 unless manufacturers, importers and downstream users have included in\nthe relevant chemical safety reports and safety data sheets, Derived No-Effect Levels\n(DNELs) relating to exposure of workers of 6 mg/m 3 for exposure by inhalation and 1,1\nmg/kg/day for dermal exposure.\n2. Shall not be manufactured, or used, as a substance on its own, as a constituent of other\nsubstances, or in mixtures in a concentration equal to or greater than 0,3 % after 12\nDecember 2023 unless manufacturers and downstream users take the appropriate risk\nmanagement measures and provide the appropriate operational conditions to ensure that\nexposure of workers is below the DNELs specified in paragraph 1.\n3. By way of derogation from paragraphs 1 and 2, the obligations laid down therein shall\napply from 12 December 2024 in relation to placing on the market for use, or use, as a\nsolvent in direct or transfer polyurethane coating processes of textiles and paper material or\nthe production of polyurethane membranes, and from 12 December 2025 in relation to\nplacing on the market for use, or use, as a solvent in the dry and wet spinning processes of\nsynthetic fibres."},"1. Shall not be placed on the market as a substance on its own, as a constituent of other\nsubstances, or in mixtures in a concentration equal to or greater than 0,3 % after 12\nDecember 2023 unless manufacturers, importers and downstream users have included in\nthe relevant chemical safety reports and safety data sheets, Derived No-Effect Levels\n(DNELs) relating to exposure of workers of 6 mg/m 3 for exposure by inhalation and 1,1\nmg/kg/day for dermal exposure.\n2. Shall not be manufactured, or used, as a substance on its own, as a constituent of other\nsubstances, or in mixtures in a concentration equal to or greater than 0,3 % after 12\nDecember 2023 unless manufacturers and downstream users take the appropriate risk\nmanagement measures and provide the appropriate operational conditions to ensure that\nexposure of workers is below the DNELs specified in paragraph 1.\n3. By way of derogation from paragraphs 1 and 2, the obligations laid down therein shall\napply from 12 December 2024 in relation to placing on the market for use, or use, as a\nsolvent in direct or transfer polyurethane coating processes of textiles and paper material or\nthe production of polyurethane membranes, and from 12 December 2025 in relation to\nplacing on the market for use, or use, as a solvent in the dry and wet spinning processes of\nsynthetic fibres."," 1. Darf nach dem 12. Dezember 2023 nicht als Stoff, als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von ≥ 0,3 % in Verkehr gebracht werden, es sei denn, die Hersteller, Importeure und nachgeschalteten Anwender haben DNEL-Werte für die Exposition von Arbeitnehmern von 6 mg/m3 bei Inhalation und von 1,1 mg/kg/Tag bei Aufnahme über die Haut in die einschlägigen Stoffsicherheitsberichte und Sicherheitsdatenblätter aufgenommen.\n2. Darf nach dem 12. Dezember 2023 nicht als Stoff, als Bestandteil anderer Stoffe oder in Gemischen in Konzentrationen von ≥ 0,3 % hergestellt oder verwendet werden, es sei denn, die Hersteller und nachgeschalteten Anwender treffen geeignete Risikomanagementmaßnahmen und sorgen für angemessene Verwendungsbedingungen, die gewährleisten, dass die Exposition von Arbeitnehmern unter den in Absatz 1 angegebenen DNEL-Werten liegt.\n3. Abweichend von den Absätzen 1 und 2 gelten die darin festgelegten Verpflichtungen für das Inverkehrbringen zur Verwendung oder für die Verwendung als Lösungsmittel für das Beschichten von Textilien und Papiermaterialien mit Polyurethan im direkten oder im Transferverfahren oder für die Herstellung von Polyurethanmembranen ab dem 12. Dezember 2024 und für das Inverkehrbringen zur Verwendung oder für die Verwendung als Lösungsmittel für das Trocken- und Nassspinnen synthetischer Fasern ab dem 12. Dezember 2025.","1.2023年12月12日起，DMF不得单独作为物质、作为其他物质的成分或以浓度等于或大于0.3%的混合物形式投放市场，除非制造商、进口商和下游用户已在相关化学品安全报告和安全数据表中，列出与工人接触相关的衍生无影响水平(DNEL)吸入接触限值为6mg/m3，皮肤接触限值为1.1mg/kg/天。\n2.2023年12月12日起，不得制造或使用DMF纯物质、含DMF成分的物质或DMF浓度等于或大于0.3%的混合物，除非制造商和下游用户采取适当的风险管理措施并提供适当的操作条件，以确保工人的接触低于第 1 段规定的DNEL。\n3.作为对第1段和第2段的豁免，DMF投放市场使用，或作为溶剂，用作纺织品和纸张材料的直接或转移聚氨酯涂层工艺或生产聚氨酯膜时，限制起始日期延后至2024年12月12日；DMF投放市场用作合成纤维的干法和湿法纺丝工艺中溶剂，限制起始日期延长至2025年12月12日。"]
[null,{"$f":"IF($B$1=\"English\",C2852,IF($B$1=\"Deutsch\",D2852,IF($B$1=\"中文\",E2852,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"tris(2-methoxyethoxy)vinylsilane"},"tris(2-methoxyethoxy)vinylsilane","tris(2-methoxyethoxy)vinylsilane","乙烯基-三(2-甲氧 基乙氧基)硅烷"]
[null,{"$f":"IF($B$1=\"English\",C2853,IF($B$1=\"Deutsch\",D2853,IF($B$1=\"中文\",E2853,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261"},"S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261","S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261","S-(三环[5.2.1.0'2，6]癸-3-烯-8(或9)-基) O-(异丙基或异丁基或 2-乙基己基) O-(异丙基或异丁基或2-乙基己基)二硫代磷酸酯\nX4261"]
[null,{"$f":"IF($B$1=\"English\",C2854,IF($B$1=\"Deutsch\",D2854,IF($B$1=\"中文\",E2854,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol"},"6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol","6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol","2,2'-亚甲基双-(4-甲基-6-叔丁基苯酚) (DBMC)"]
[null,{"$f":"IF($B$1=\"English\",C2855,IF($B$1=\"Deutsch\",D2855,IF($B$1=\"中文\",E2855,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"},"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)","(±)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚-2-酮，包括任何单独的异构体和/或其组合(4-MBC) "]
[null,{"$f":"IF($B$1=\"English\",C2856,IF($B$1=\"Deutsch\",D2856,IF($B$1=\"中文\",E2856,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(3E)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚烷-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2857,IF($B$1=\"Deutsch\",D2857,IF($B$1=\"中文\",E2857,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3E,4S)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚烷-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2858,IF($B$1=\"Deutsch\",D2858,IF($B$1=\"中文\",E2858,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3Z,4R)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚烷-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2859,IF($B$1=\"Deutsch\",D2859,IF($B$1=\"中文\",E2859,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one"},"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one","(±)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2860,IF($B$1=\"Deutsch\",D2860,IF($B$1=\"中文\",E2860,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,4S)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2861,IF($B$1=\"Deutsch\",D2861,IF($B$1=\"中文\",E2861,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3E,4R)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2862,IF($B$1=\"Deutsch\",D2862,IF($B$1=\"中文\",E2862,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3Z,4S)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]双环[2.2.1]庚-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C2863,IF($B$1=\"Deutsch\",D2863,IF($B$1=\"中文\",E2863,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material ","0,1 Massen%, jedoch Verbot bei Neuentwicklung von Materialien oder bei Material-Änderungen ","\n0.1质量-%，但禁止用于新材料开发或材料变更 "]
[null,{"$f":"IF($B$1=\"English\",C2864,IF($B$1=\"Deutsch\",D2864,IF($B$1=\"中文\",E2864,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material ","0,1 Massen%, jedoch Verbot bei Neuentwicklung von Materialien oder bei Material-Änderungen ","\n0.1质量-%，但禁止用于新材料开发或材料变更 "]
[null,{"$f":"IF($B$1=\"English\",C2865,IF($B$1=\"Deutsch\",D2865,IF($B$1=\"中文\",E2865,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material ","0,1 Massen%, jedoch Verbot bei Neuentwicklung von Materialien oder bei Material-Änderungen ","\n0.1质量-%，但禁止用于新材料开发或材料变更 "]
[null,{"$f":"IF($B$1=\"English\",C2866,IF($B$1=\"Deutsch\",D2866,IF($B$1=\"中文\",E2866,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material "},"0,1 mass-%, however prohibited for new developments of materials or in case of changes to the material ","0,1 Massen%, jedoch Verbot bei Neuentwicklung von Materialien oder bei Material-Änderungen ","\n0.1质量-%，但禁止用于新材料开发或材料变更 "]
[null,{"$f":"IF($B$1=\"English\",C2867,IF($B$1=\"Deutsch\",D2867,IF($B$1=\"中文\",E2867,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rubbers, plastics, sealants"},"Rubbers, plastics, sealants","Kautschuk, Kunststoff, Dichtstoffe","橡胶、塑料、密封剂"]
[null,{"$f":"IF($B$1=\"English\",C2868,IF($B$1=\"Deutsch\",D2868,IF($B$1=\"中文\",E2868,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lubricants, greases"},"Lubricants, greases","Schmierstoffe, Fette","润滑剂、润滑脂 "]
[null,{"$f":"IF($B$1=\"English\",C2869,IF($B$1=\"Deutsch\",D2869,IF($B$1=\"中文\",E2869,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rubbers, lubricants, adhesives, inks, fuels, gaskets"},"Rubbers, lubricants, adhesives, inks, fuels, gaskets","Kautschuk, Schmiermittel, Klebstoffe, Tinten, Kraftstoffe, Dichtungen","橡胶、润滑剂、粘合剂、油墨、燃料、垫圈"]
[null,{"$f":"IF($B$1=\"English\",C2870,IF($B$1=\"Deutsch\",D2870,IF($B$1=\"中文\",E2870,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cosmetics"},"Cosmetics","Kosmetik","化妆品"]
[null,{"$f":"IF($B$1=\"English\",C2871,IF($B$1=\"Deutsch\",D2871,IF($B$1=\"中文\",E2871,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-(hydroxymethyl)acrylamide"},"N-(hydroxymethyl)acrylamide","N-(hydroxymethyl)acrylamide","N-(羟甲基)丙烯酰胺"]
[null,{"$f":"IF($B$1=\"English\",C2872,IF($B$1=\"Deutsch\",D2872,IF($B$1=\"中文\",E2872,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"This substance is used in formulation or re-packing, at industrial sites and in manufacturing."},"This substance is used in formulation or re-packing, at industrial sites and in manufacturing.","Dieser Stoff wird bei der Formulierung oder Umverpackung, an Industriestandorten und in der Fertigung verwendet.","该物质用于配制或重新包装，在工业场所和制造中使用。"]
[null,{"$f":"IF($B$1=\"English\",C2873,IF($B$1=\"Deutsch\",D2873,IF($B$1=\"中文\",E2873,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"USA TSCA (sec 5(a)(2) sec. 6(h)) (Tab 18)"},"USA TSCA (sec 5(a)(2) sec. 6(h)) (Tab 18)","USA TSCA (sec 5(a)(2) sec. 6(h)) (Tab 18)","美国 TSCA法案 (条款 5(a)(2) 条款 6(h)) (表18)"]
[null,{"$f":"IF($B$1=\"English\",C2874,IF($B$1=\"Deutsch\",D2874,IF($B$1=\"中文\",E2874,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PFAS World (based on US Maine PFAS) (Tab 19)"},"PFAS World (based on US Maine PFAS) (Tab 19)","PFAS World (based on US Maine PFAS) (Reiter 19)","全氟和多氟烷基物质PFAS全球（基于美国缅因州PFAS法规）（表 19）"]
[null,{"$f":"IF($B$1=\"English\",C2875,IF($B$1=\"Deutsch\",D2875,IF($B$1=\"中文\",E2875,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"In July 2021, Public Law c. 477,"},"In July 2021, Public Law c. 477,","In July 2021, Public Law c. 477,","2021年7月，公共法律 c. 477,"]
[null,{"$f":"IF($B$1=\"English\",C2876,IF($B$1=\"Deutsch\",D2876,IF($B$1=\"中文\",E2876,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(LD 1503, 130th Legislature) was enacted by the Maine Legislature. This new law requires manufacturers"},"(LD 1503, 130th Legislature) was enacted by the Maine Legislature. This new law requires manufacturers","(LD 1503, 130th Legislature) was enacted by the Maine Legislature. This new law requires manufacturers","（LD 1503，第 130 届立法机关）由缅因州立法机关颁布。 这项新法律要求有意添加 PFAS 的产品制造商"]
[null,{"$f":"IF($B$1=\"English\",C2877,IF($B$1=\"Deutsch\",D2877,IF($B$1=\"中文\",E2877,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"of products with intentionally added PFAS to report the intentionally added presence of PFAS in those"},"of products with intentionally added PFAS to report the intentionally added presence of PFAS in those","of products with intentionally added PFAS to report the intentionally added presence of PFAS in those","从 2023 年 1 月 1 日起向商务部报告这些产品中有意添加 PFAS的情况。"]
[null,{"$f":"IF($B$1=\"English\",C2878,IF($B$1=\"Deutsch\",D2878,IF($B$1=\"中文\",E2878,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"products to the Department beginning January 1, 2023."},"products to the Department beginning January 1, 2023.","products to the Department beginning January 1, 2023."," "]
[null,{"$f":"IF($B$1=\"English\",C2879,IF($B$1=\"Deutsch\",D2879,IF($B$1=\"中文\",E2879,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bosch suppliers must inform Bosch if any substance (intentionally or not intentionally) of the Main Law"},"Bosch suppliers must inform Bosch if any substance (intentionally or not intentionally) of the Main Law","Bosch suppliers must inform Bosch if any substance (intentionally or not intentionally) of the Main Law","如果产品或备件或混合物中有任何浓度的EPA主要法律相关清单中的任何物质（有意或无意），"]
[null,{"$f":"IF($B$1=\"English\",C2880,IF($B$1=\"Deutsch\",D2880,IF($B$1=\"中文\",E2880,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"related list from EPA in a product or spare part or mixture in any concentration. The supplier is obliged to"},"related list from EPA in a product or spare part or mixture in any concentration. The supplier is obliged to","related list from EPA in a product or spare part or mixture in any concentration. The supplier is obliged to","博世供应商必须通知博世。供应商有义务跟踪EPA列表（下面的链接），"]
[null,{"$f":"IF($B$1=\"English\",C2881,IF($B$1=\"Deutsch\",D2881,IF($B$1=\"中文\",E2881,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"track the EPA list (link below) and to inform Bosch purchasing contact immediately if he gets information"},"track the EPA list (link below) and to inform Bosch purchasing contact immediately if he gets information","track the EPA list (link below) and to inform Bosch purchasing contact immediately if he gets information","并在获悉供应材料中可能包含EPA列表中的任何物质时立即通知博世采购联系人。"]
[null,{"$f":"IF($B$1=\"English\",C2882,IF($B$1=\"Deutsch\",D2882,IF($B$1=\"中文\",E2882,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"that any substance on the EPA list may be included in the supplied material."},"that any substance on the EPA list may be included in the supplied material.","that any substance on the EPA list may be included in the supplied material."," "]
[null,{"$f":"IF($B$1=\"English\",C2883,IF($B$1=\"Deutsch\",D2883,IF($B$1=\"中文\",E2883,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"EPA PFAS Master List of PFAS Substances V2: "},"EPA PFAS Master List of PFAS Substances V2: ","EPA PFAS Master List of PFAS Substances: ","EPA PFAS Master List of PFAS Substances: "]
[null,{"$f":"IF($B$1=\"English\",C2884,IF($B$1=\"Deutsch\",D2884,IF($B$1=\"中文\",E2884,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab 19: PFAS World (based on US Maine PFAS)"},"Tab 19: PFAS World (based on US Maine PFAS)","Register 19: PFAS World (based on US Maine PFAS)","表19：全氟和多氟烷基物质PFAS全球（基于美国缅因州PFAS法规）"]
[null,{"$f":"IF($B$1=\"English\",C2885,IF($B$1=\"Deutsch\",D2885,IF($B$1=\"中文\",E2885,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Automotive aftermarket select ‘Remains in/on Bosch Product and GB AA automotive’"},"Automotive aftermarket select ‘Remains in/on Bosch Product and GB AA automotive’","Automotive-Handelsware wählen Sie ' Verbleibt in/auf Bosch Produkt und GB AA Automotive'","汽车售后事业部AA选择“保留在博世产品中/上和 GB AA 汽车”"]
[null,{"$f":"IF($B$1=\"English\",C2886,IF($B$1=\"Deutsch\",D2886,IF($B$1=\"中文\",E2886,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"All other select ‘Bosch reference list’"},"All other select ‘Bosch reference list’","Alle anderen wählen 'Bosch Referenzliste'.","所有其他选择“Bosch reference list（博世参考列表）”"]
[null,{"$f":"IF($B$1=\"English\",C2887,IF($B$1=\"Deutsch\",D2887,IF($B$1=\"中文\",E2887,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Antimony"},"Antimony","Antimony","锑"]
[null,{"$f":"IF($B$1=\"English\",C2888,IF($B$1=\"Deutsch\",D2888,IF($B$1=\"中文\",E2888,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bauxite"},"Bauxite","Bauxite","铝土矿"]
[null,{"$f":"IF($B$1=\"English\",C2889,IF($B$1=\"Deutsch\",D2889,IF($B$1=\"中文\",E2889,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Baryte "},"Baryte ","Baryte ","重晶石"]
[null,{"$f":"IF($B$1=\"English\",C2890,IF($B$1=\"Deutsch\",D2890,IF($B$1=\"中文\",E2890,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beryllium"},"Beryllium","Beryllium","铍"]
[null,{"$f":"IF($B$1=\"English\",C2891,IF($B$1=\"Deutsch\",D2891,IF($B$1=\"中文\",E2891,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bismuth"},"Bismuth","Bismuth","铋"]
[null,{"$f":"IF($B$1=\"English\",C2892,IF($B$1=\"Deutsch\",D2892,IF($B$1=\"中文\",E2892,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Borate"},"Borate","Borate","硼酸盐"]
[null,{"$f":"IF($B$1=\"English\",C2893,IF($B$1=\"Deutsch\",D2893,IF($B$1=\"中文\",E2893,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cobalt"},"Cobalt","Cobalt","钴"]
[null,{"$f":"IF($B$1=\"English\",C2894,IF($B$1=\"Deutsch\",D2894,IF($B$1=\"中文\",E2894,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Coking Coal"},"Coking Coal","Coking Coal","焦煤"]
[null,{"$f":"IF($B$1=\"English\",C2895,IF($B$1=\"Deutsch\",D2895,IF($B$1=\"中文\",E2895,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluorite (CaF2) / Fluorspar "},"Fluorite (CaF2) / Fluorspar ","Fluorite (CaF2) / Fluorspar ","萤石 (CaF2) / 氟石"]
[null,{"$f":"IF($B$1=\"English\",C2896,IF($B$1=\"Deutsch\",D2896,IF($B$1=\"中文\",E2896,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gallium "},"Gallium ","Gallium ","镓"]
[null,{"$f":"IF($B$1=\"English\",C2897,IF($B$1=\"Deutsch\",D2897,IF($B$1=\"中文\",E2897,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Germanium"},"Germanium","Germanium","锗"]
[null,{"$f":"IF($B$1=\"English\",C2898,IF($B$1=\"Deutsch\",D2898,IF($B$1=\"中文\",E2898,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hafnium"},"Hafnium","Hafnium","铪"]
[null,{"$f":"IF($B$1=\"English\",C2899,IF($B$1=\"Deutsch\",D2899,IF($B$1=\"中文\",E2899,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Indium "},"Indium ","Indium ","铟"]
[null,{"$f":"IF($B$1=\"English\",C2900,IF($B$1=\"Deutsch\",D2900,IF($B$1=\"中文\",E2900,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lithium"},"Lithium","Lithium","锂"]
[null,{"$f":"IF($B$1=\"English\",C2901,IF($B$1=\"Deutsch\",D2901,IF($B$1=\"中文\",E2901,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Magnesium"},"Magnesium","Magnesium","镁"]
[null,{"$f":"IF($B$1=\"English\",C2902,IF($B$1=\"Deutsch\",D2902,IF($B$1=\"中文\",E2902,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Natural Graphite"},"Natural Graphite","Natural Graphite","天然石墨"]
[null,{"$f":"IF($B$1=\"English\",C2903,IF($B$1=\"Deutsch\",D2903,IF($B$1=\"中文\",E2903,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Natural Rubber"},"Natural Rubber","Natural Rubber","天然橡胶"]
[null,{"$f":"IF($B$1=\"English\",C2904,IF($B$1=\"Deutsch\",D2904,IF($B$1=\"中文\",E2904,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Niobium"},"Niobium","Niobium","铌"]
[null,{"$f":"IF($B$1=\"English\",C2905,IF($B$1=\"Deutsch\",D2905,IF($B$1=\"中文\",E2905,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphate rock "},"Phosphate rock ","Phosphate rock ","磷矿"]
[null,{"$f":"IF($B$1=\"English\",C2906,IF($B$1=\"Deutsch\",D2906,IF($B$1=\"中文\",E2906,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphorus"},"Phosphorus","Phosphorus","磷"]
[null,{"$f":"IF($B$1=\"English\",C2907,IF($B$1=\"Deutsch\",D2907,IF($B$1=\"中文\",E2907,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Scandium"},"Scandium","Scandium","钪"]
[null,{"$f":"IF($B$1=\"English\",C2908,IF($B$1=\"Deutsch\",D2908,IF($B$1=\"中文\",E2908,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silicon metal"},"Silicon metal","Silicon metal","硅 金属"]
[null,{"$f":"IF($B$1=\"English\",C2909,IF($B$1=\"Deutsch\",D2909,IF($B$1=\"中文\",E2909,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Strontium"},"Strontium","Strontium","锶"]
[null,{"$f":"IF($B$1=\"English\",C2910,IF($B$1=\"Deutsch\",D2910,IF($B$1=\"中文\",E2910,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tantalum (coltan)"},"Tantalum (coltan)","Tantalum (coltan)","鉭（鈳鉭鐵礦）"]
[null,{"$f":"IF($B$1=\"English\",C2911,IF($B$1=\"Deutsch\",D2911,IF($B$1=\"中文\",E2911,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" Tungstene"}," Tungstene"," Tungstene","钨 "]
[null,{"$f":"IF($B$1=\"English\",C2912,IF($B$1=\"Deutsch\",D2912,IF($B$1=\"中文\",E2912,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Vanadium"},"Vanadium","Vanadium","钒"]
[null,{"$f":"IF($B$1=\"English\",C2913,IF($B$1=\"Deutsch\",D2913,IF($B$1=\"中文\",E2913,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Platinum"},"Platinum","Platinum","铂"]
[null,{"$f":"IF($B$1=\"English\",C2914,IF($B$1=\"Deutsch\",D2914,IF($B$1=\"中文\",E2914,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Palladium"},"Palladium","Palladium","钯"]
[null,{"$f":"IF($B$1=\"English\",C2915,IF($B$1=\"Deutsch\",D2915,IF($B$1=\"中文\",E2915,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rhodium"},"Rhodium","Rhodium","铑"]
[null,{"$f":"IF($B$1=\"English\",C2916,IF($B$1=\"Deutsch\",D2916,IF($B$1=\"中文\",E2916,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ruthenium"},"Ruthenium","Ruthenium","钌"]
[null,{"$f":"IF($B$1=\"English\",C2917,IF($B$1=\"Deutsch\",D2917,IF($B$1=\"中文\",E2917,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iridium"},"Iridium","Iridium","铱"]
[null,{"$f":"IF($B$1=\"English\",C2918,IF($B$1=\"Deutsch\",D2918,IF($B$1=\"中文\",E2918,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Osmium"},"Osmium","Osmium","锇"]
[null,{"$f":"IF($B$1=\"English\",C2919,IF($B$1=\"Deutsch\",D2919,IF($B$1=\"中文\",E2919,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Yttrium"},"Yttrium","Yttrium","钇"]
[null,{"$f":"IF($B$1=\"English\",C2920,IF($B$1=\"Deutsch\",D2920,IF($B$1=\"中文\",E2920,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Terbium"},"Terbium","Terbium","铽"]
[null,{"$f":"IF($B$1=\"English\",C2921,IF($B$1=\"Deutsch\",D2921,IF($B$1=\"中文\",E2921,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dysprosium"},"Dysprosium","Dysprosium","镝"]
[null,{"$f":"IF($B$1=\"English\",C2922,IF($B$1=\"Deutsch\",D2922,IF($B$1=\"中文\",E2922,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Holmium"},"Holmium","Holmium","钬"]
[null,{"$f":"IF($B$1=\"English\",C2923,IF($B$1=\"Deutsch\",D2923,IF($B$1=\"中文\",E2923,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Erbium"},"Erbium","Erbium","铒"]
[null,{"$f":"IF($B$1=\"English\",C2924,IF($B$1=\"Deutsch\",D2924,IF($B$1=\"中文\",E2924,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Thulium"},"Thulium","Thulium","铥"]
[null,{"$f":"IF($B$1=\"English\",C2925,IF($B$1=\"Deutsch\",D2925,IF($B$1=\"中文\",E2925,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ytterbium "},"Ytterbium ","Ytterbium ","镱"]
[null,{"$f":"IF($B$1=\"English\",C2926,IF($B$1=\"Deutsch\",D2926,IF($B$1=\"中文\",E2926,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lutetium"},"Lutetium","Lutetium","镥"]
[null,{"$f":"IF($B$1=\"English\",C2927,IF($B$1=\"Deutsch\",D2927,IF($B$1=\"中文\",E2927,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Europium"},"Europium","Europium","铕"]
[null,{"$f":"IF($B$1=\"English\",C2928,IF($B$1=\"Deutsch\",D2928,IF($B$1=\"中文\",E2928,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gadolinium"},"Gadolinium","Gadolinium","钆"]
[null,{"$f":"IF($B$1=\"English\",C2929,IF($B$1=\"Deutsch\",D2929,IF($B$1=\"中文\",E2929,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lanthanum"},"Lanthanum","Lanthanum","镧"]
[null,{"$f":"IF($B$1=\"English\",C2930,IF($B$1=\"Deutsch\",D2930,IF($B$1=\"中文\",E2930,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cerium"},"Cerium","Cerium","铈"]
[null,{"$f":"IF($B$1=\"English\",C2931,IF($B$1=\"Deutsch\",D2931,IF($B$1=\"中文\",E2931,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Praseodymium"},"Praseodymium","Praseodymium","镨"]
[null,{"$f":"IF($B$1=\"English\",C2932,IF($B$1=\"Deutsch\",D2932,IF($B$1=\"中文\",E2932,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Neodymium"},"Neodymium","Neodymium","钕"]
[null,{"$f":"IF($B$1=\"English\",C2933,IF($B$1=\"Deutsch\",D2933,IF($B$1=\"中文\",E2933,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Promethium"},"Promethium","Promethium","钷"]
[null,{"$f":"IF($B$1=\"English\",C2934,IF($B$1=\"Deutsch\",D2934,IF($B$1=\"中文\",E2934,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Samarium "},"Samarium ","Samarium ","钐 "]
[null,{"$f":"IF($B$1=\"English\",C2935,IF($B$1=\"Deutsch\",D2935,IF($B$1=\"中文\",E2935,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Flame retardants\n• Lead-acid batteries"},"• Flame retardants\n• Lead-acid batteries","• Flame retardants\n• Lead-acid batteries","• 阻燃剂 \n• 铅酸电池"]
[null,{"$f":"IF($B$1=\"English\",C2936,IF($B$1=\"Deutsch\",D2936,IF($B$1=\"中文\",E2936,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Aluminium production"},"• Aluminium production","• Aluminium production","• 鋁生產"]
[null,{"$f":"IF($B$1=\"English\",C2937,IF($B$1=\"Deutsch\",D2937,IF($B$1=\"中文\",E2937,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Fillers\n• Chemicals "},"• Fillers\n• Chemicals ","• Fillers\n• Chemicals ","•填料 \n• 化学品"]
[null,{"$f":"IF($B$1=\"English\",C2938,IF($B$1=\"Deutsch\",D2938,IF($B$1=\"中文\",E2938,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Copper-beryllium alloy"},"• Copper-beryllium alloy","• Copper-beryllium alloy","• 铜铍合金"]
[null,{"$f":"IF($B$1=\"English\",C2939,IF($B$1=\"Deutsch\",D2939,IF($B$1=\"中文\",E2939,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Low-melting alloys\n• Metallurgical additives "},"• Low-melting alloys\n• Metallurgical additives ","• Low-melting alloys\n• Metallurgical additives ","• 低熔点合金 \n• 冶金添加剂"]
[null,{"$f":"IF($B$1=\"English\",C2940,IF($B$1=\"Deutsch\",D2940,IF($B$1=\"中文\",E2940,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Glass and fibreglass applications\n• Ceramics\n• Permanent magnets"},"• Glass and fibreglass applications\n• Ceramics\n• Permanent magnets","• Glass and fibreglass applications\n• Ceramics\n• Permanent magnets","• 玻璃和玻璃纤维应用 \n• 陶瓷\n• 鋁生產"]
[null,{"$f":"IF($B$1=\"English\",C2941,IF($B$1=\"Deutsch\",D2941,IF($B$1=\"中文\",E2941,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Rechargeable battery electrodes\n• Superalloys\n• Hardfacing\n• High speed steel\n• Other alloys \n• Catalysts\n• Magnets"},"• Rechargeable battery electrodes\n• Superalloys\n• Hardfacing\n• High speed steel\n• Other alloys \n• Catalysts\n• Magnets","• Rechargeable battery electrodes\n• Superalloys\n• Hardfacing\n• High speed steel\n• Other alloys \n• Catalysts\n• Magnets","•充电电池电极 \n• 高温合金 \n• 堆焊 \n• 高速钢 \n• 其他合金\n• 催化劑\n• 磁鐵"]
[null,{"$f":"IF($B$1=\"English\",C2942,IF($B$1=\"Deutsch\",D2942,IF($B$1=\"中文\",E2942,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Steel Production\n• Carbon fibres\n• Battery electrode"},"• Steel Production\n• Carbon fibres\n• Battery electrode","• Steel Production\n• Carbon fibres\n• Battery electrode","• 钢铁生产 \n• 碳纤维 \n• 电池电极"]
[null,{"$f":"IF($B$1=\"English\",C2943,IF($B$1=\"Deutsch\",D2943,IF($B$1=\"中文\",E2943,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Aluminium production\n• Steel and iron making"},"• Aluminium production\n• Steel and iron making","• Aluminium production\n• Steel and iron making","• 铝生产 \n• 鋼鐵製造"]
[null,{"$f":"IF($B$1=\"English\",C2944,IF($B$1=\"Deutsch\",D2944,IF($B$1=\"中文\",E2944,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Semiconductors\n• Integrated Circuits\n• Sensors\n• Alloys\n• Batteries\n• Magnets"},"• Semiconductors\n• Integrated Circuits\n• Sensors\n• Alloys\n• Batteries\n• Magnets","• Semiconductors\n• Integrated Circuits\n• Sensors\n• Alloys\n• Batteries\n• Magnets","• 半导体\n• 集成电路\n• 传感器\n• 合金\n• 电池\n• 磁铁"]
[null,{"$f":"IF($B$1=\"English\",C2945,IF($B$1=\"Deutsch\",D2945,IF($B$1=\"中文\",E2945,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Fibre optics\n• Infrared optics \n• Satellite solar cells\n• Polymerisation catalysts"},"• Fibre optics\n• Infrared optics \n• Satellite solar cells\n• Polymerisation catalysts","• Fibre optics\n• Infrared optics \n• Satellite solar cells\n• Polymerisation catalysts","• 光纤\n• 红外光学\n• 衛星太陽能電池\n• 聚合催化劑"]
[null,{"$f":"IF($B$1=\"English\",C2946,IF($B$1=\"Deutsch\",D2946,IF($B$1=\"中文\",E2946,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Superalloys\n• Nuclear control rods\n• Refractory ceramics"},"• Superalloys\n• Nuclear control rods\n• Refractory ceramics","• Superalloysv\n• Nuclear control rods\n• Refractory ceramics","• 高温合金\n• 核控制棒\n• 耐火陶瓷"]
[null,{"$f":"IF($B$1=\"English\",C2947,IF($B$1=\"Deutsch\",D2947,IF($B$1=\"中文\",E2947,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Flat panel displays\n• Low melting-point alloys\n• Compound Semiconductors\n• LEDs"},"• Flat panel displays\n• Low melting-point alloys\n• Compound Semiconductors\n• LEDs","• Flat panel displays\n• Low melting-point alloys\n• Compound Semiconductors\n• 引領","• 平板显示器\n• 低熔点合金\n• 化合物半导体\n• LED"]
[null,{"$f":"IF($B$1=\"English\",C2948,IF($B$1=\"Deutsch\",D2948,IF($B$1=\"中文\",E2948,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Lithium-Ion batteries (battery grade)\n• Photovoltaic cells and photonics\n• Solders"},"• Lithium-Ion batteries (battery grade)\n• Photovoltaic cells and photonics\n• Solders","• Lithium-Ion batteries (battery grade)\n• Photovoltaic cells and photonics\n• Solders","• 鋰離子電池（電池級）\n• 光伏電池和光子學\n• 焊料"]
[null,{"$f":"IF($B$1=\"English\",C2949,IF($B$1=\"Deutsch\",D2949,IF($B$1=\"中文\",E2949,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Aluminium alloys "},"• Aluminium alloys ","• Aluminium alloys ","• 铝合金"]
[null,{"$f":"IF($B$1=\"English\",C2950,IF($B$1=\"Deutsch\",D2950,IF($B$1=\"中文\",E2950,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Batteries (battery grade)\n• Refractories for steelmaking"},"• Batteries (battery grade)\n• Refractories for steelmaking","• Batteries (battery grade)\n• Refractories for steelmaking","• 電池（電池級）\n• 炼钢用耐火材料"]
[null,{"$f":"IF($B$1=\"English\",C2951,IF($B$1=\"Deutsch\",D2951,IF($B$1=\"中文\",E2951,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Rubber electrical insulators "},"• Rubber electrical insulators ","• Rubber electrical insulators ","• 橡胶电绝缘体"]
[null,{"$f":"IF($B$1=\"English\",C2952,IF($B$1=\"Deutsch\",D2952,IF($B$1=\"中文\",E2952,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Steels\n• Superalloys \n• Capacitors\n• Superconducting\n• Magnets"},"• Steels\n• Superalloys \n• Capacitors\n• Superconducting\n• Magnets","• Steels\n• Superalloys \n• Capacitors\n• Superconducting\n• Magnets","• 钢材\n• 高温合金\n• 電容器\n• 超導\n• 磁鐵”"]
[null,{"$f":"IF($B$1=\"English\",C2953,IF($B$1=\"Deutsch\",D2953,IF($B$1=\"中文\",E2953,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" • Phosphorus production"}," • Phosphorus production"," • Phosphorus production","• 磷生产"]
[null,{"$f":"IF($B$1=\"English\",C2954,IF($B$1=\"Deutsch\",D2954,IF($B$1=\"中文\",E2954,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":" • Steel production"}," • Steel production"," • Steel production","• 钢铁生产"]
[null,{"$f":"IF($B$1=\"English\",C2955,IF($B$1=\"Deutsch\",D2955,IF($B$1=\"中文\",E2955,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Solid oxide fuel cells\n• Aluminium-scandium alloys\n• 3D printing"},"• Solid oxide fuel cells\n• Aluminium-scandium alloys\n• 3D printing","• Solid oxide fuel cells\n• Aluminium-scandium alloys\n• 3D printing","• 固体氧化物燃料电池\n• 铝钪合金\n• 3D打印"]
[null,{"$f":"IF($B$1=\"English\",C2956,IF($B$1=\"Deutsch\",D2956,IF($B$1=\"中文\",E2956,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Semiconductors\n• Silicones\n• Photovoltaics\n• Electronic components"},"• Semiconductors\n• Silicones\n• Photovoltaics\n• Electronic components","• Semiconductors\n• Silicones\n• Photovoltaics\n• Electronic components","• 半导体\n• 有机硅\n• 光伏\n• 電子元器件"]
[null,{"$f":"IF($B$1=\"English\",C2957,IF($B$1=\"Deutsch\",D2957,IF($B$1=\"中文\",E2957,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Ceramic capacitors\n• PTC thermistors\n• Aluminium alloys"},"• Ceramic capacitors\n• PTC thermistors\n• Aluminium alloys","• Ceramic capacitors\n• PTC thermistors\n• 鋁合金”","•陶瓷电容器\n• PTC热敏电阻\n• Aluminium alloys"]
[null,{"$f":"IF($B$1=\"English\",C2958,IF($B$1=\"Deutsch\",D2958,IF($B$1=\"中文\",E2958,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Capacitors\n• Superalloys\n• Sputtering targets "},"• Capacitors\n• Superalloys\n• Sputtering targets ","• Capacitors\n• Superalloys\n• Sputtering targets ","•电容器 \n• 高温合金 \n• 溅射靶材"]
[null,{"$f":"IF($B$1=\"English\",C2959,IF($B$1=\"Deutsch\",D2959,IF($B$1=\"中文\",E2959,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Hard metals (tungsten carbide)\n• Alloy steel"},"• Hard metals (tungsten carbide)\n• Alloy steel","• Hard metals (tungsten carbide)\n• Alloy steel","• 硬质合金（碳化钨）\n • 合金钢"]
[null,{"$f":"IF($B$1=\"English\",C2960,IF($B$1=\"Deutsch\",D2960,IF($B$1=\"中文\",E2960,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• High-strength low-alloy (HSLA) steels\n• Special steels\n• Chemical catalysts"},"• High-strength low-alloy (HSLA) steels\n• Special steels\n• Chemical catalysts","• High-strength low-alloy (HSLA) steels\n• Special steels\n• Chemical catalysts","• 高强度低合金 (HSLA) 钢 \n• 特种钢\n• 化學催化劑\""]
[null,{"$f":"IF($B$1=\"English\",C2961,IF($B$1=\"Deutsch\",D2961,IF($B$1=\"中文\",E2961,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Chemical and automotive catalysts\n• Fuel cells\n• Electronic applications"},"• Chemical and automotive catalysts\n• Fuel cells\n• Electronic applications","• Chemical and automotive catalysts\n• Fuel cells\n• Electronic applications","• 化学和汽车催化剂 \n• 燃料电池 \n• 电子应用"]
[null,{"$f":"IF($B$1=\"English\",C2962,IF($B$1=\"Deutsch\",D2962,IF($B$1=\"中文\",E2962,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Phosphors Lighting "},"• Phosphors Lighting ","• Phosphors Lighting "," • 荧光灯"]
[null,{"$f":"IF($B$1=\"English\",C2963,IF($B$1=\"Deutsch\",D2963,IF($B$1=\"中文\",E2963,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Computers Magnets\n• Phosphors Lighting "},"• Computers Magnets\n• Phosphors Lighting ","• Computers Magnets\n• Phosphors Lighting ","• 电脑磁铁 \n• 磷光体照明"]
[null,{"$f":"IF($B$1=\"English\",C2964,IF($B$1=\"Deutsch\",D2964,IF($B$1=\"中文\",E2964,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Computers Magnets\n• Audio Systems Magnets"},"• Computers Magnets\n• Audio Systems Magnets","• Computers Magnets\n• Audio Systems Magnets","• 电脑磁铁 \n• 音响系统磁铁"]
[null,{"$f":"IF($B$1=\"English\",C2965,IF($B$1=\"Deutsch\",D2965,IF($B$1=\"中文\",E2965,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Magnets"},"• Magnets","• Magnets","• 磁铁 "]
[null,{"$f":"IF($B$1=\"English\",C2966,IF($B$1=\"Deutsch\",D2966,IF($B$1=\"中文\",E2966,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Glass Fibre Optics "},"• Glass Fibre Optics ","• Glass Fibre Optics ","• 玻璃光纤"]
[null,{"$f":"IF($B$1=\"English\",C2967,IF($B$1=\"Deutsch\",D2967,IF($B$1=\"中文\",E2967,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Lightweight portable x-ray machine for medical use"},"• Lightweight portable x-ray machine for medical use","• Lightweight portable x-ray machine for medical use","• 医用轻型便携式X光机"]
[null,{"$f":"IF($B$1=\"English\",C2968,IF($B$1=\"Deutsch\",D2968,IF($B$1=\"中文\",E2968,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Memory devices\n• Tunable lasers"},"• Memory devices\n• Tunable lasers","• Memory devices\n• Tunable lasers","• 存储设备 \n• 可调激光器"]
[null,{"$f":"IF($B$1=\"English\",C2969,IF($B$1=\"Deutsch\",D2969,IF($B$1=\"中文\",E2969,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Catalyst for cracking hydrocarbons in oil refineries"},"• Catalyst for cracking hydrocarbons in oil refineries","• Catalyst for cracking hydrocarbons in oil refineries","• 炼油厂裂解碳氢化合物的催化剂"]
[null,{"$f":"IF($B$1=\"English\",C2970,IF($B$1=\"Deutsch\",D2970,IF($B$1=\"中文\",E2970,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Phosphors Lighting "},"• Phosphors Lighting ","• Phosphors Lighting ","• 荧光灯"]
[null,{"$f":"IF($B$1=\"English\",C2971,IF($B$1=\"Deutsch\",D2971,IF($B$1=\"中文\",E2971,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Phosphors\n• Magnets"},"• Phosphors\n• Magnets","• Phosphors\n• Magnets","•荧光粉 \n• 磁铁"]
[null,{"$f":"IF($B$1=\"English\",C2972,IF($B$1=\"Deutsch\",D2972,IF($B$1=\"中文\",E2972,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• FCC Catalysts\n• Batteries\n• Alloys"},"• FCC Catalysts\n• Batteries\n• Alloys","• FCC Catalysts\n• Batteries\n• Alloys","• FCC 催化剂 \n• 电池 \n• 合金"]
[null,{"$f":"IF($B$1=\"English\",C2973,IF($B$1=\"Deutsch\",D2973,IF($B$1=\"中文\",E2973,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Mischmetal alloy\n• Flat-screen TVs\n• Low-energy light bulbs"},"• Mischmetal alloy\n• Flat-screen TVs\n• Low-energy light bulbs","• Mischmetal alloy\n• Flat-screen TVs\n• Low-energy light bulbs","•混合稀土合金 \n• 平面电视 \n• 节能灯泡"]
[null,{"$f":"IF($B$1=\"English\",C2974,IF($B$1=\"Deutsch\",D2974,IF($B$1=\"中文\",E2974,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Computers Magnets\n• Audio Systems Magnets"},"• Computers Magnets\n• Audio Systems Magnets","• Computers Magnets\n• Audio Systems Magnets","• 电脑磁铁 \n• 音响系统磁铁"]
[null,{"$f":"IF($B$1=\"English\",C2975,IF($B$1=\"Deutsch\",D2975,IF($B$1=\"中文\",E2975,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Magnets\n• Batteries"},"• Magnets\n• Batteries","• Magnets\n• Batteries","•磁铁 \n• 电池"]
[null,{"$f":"IF($B$1=\"English\",C2976,IF($B$1=\"Deutsch\",D2976,IF($B$1=\"中文\",E2976,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Atomic batteries"},"• Atomic batteries","• Atomic batteries","• 原子电池"]
[null,{"$f":"IF($B$1=\"English\",C2977,IF($B$1=\"Deutsch\",D2977,IF($B$1=\"中文\",E2977,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Magnets\n• Batteries"},"• Magnets\n• Batteries","• Magnets\n• Batteries","•磁铁 \n• 电池"]
[null,{"$f":"IF($B$1=\"English\",C2978,IF($B$1=\"Deutsch\",D2978,IF($B$1=\"中文\",E2978,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2979,IF($B$1=\"Deutsch\",D2979,IF($B$1=\"中文\",E2979,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2980,IF($B$1=\"Deutsch\",D2980,IF($B$1=\"中文\",E2980,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2981,IF($B$1=\"Deutsch\",D2981,IF($B$1=\"中文\",E2981,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2982,IF($B$1=\"Deutsch\",D2982,IF($B$1=\"中文\",E2982,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2983,IF($B$1=\"Deutsch\",D2983,IF($B$1=\"中文\",E2983,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2984,IF($B$1=\"Deutsch\",D2984,IF($B$1=\"中文\",E2984,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2985,IF($B$1=\"Deutsch\",D2985,IF($B$1=\"中文\",E2985,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2986,IF($B$1=\"Deutsch\",D2986,IF($B$1=\"中文\",E2986,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2987,IF($B$1=\"Deutsch\",D2987,IF($B$1=\"中文\",E2987,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2988,IF($B$1=\"Deutsch\",D2988,IF($B$1=\"中文\",E2988,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2989,IF($B$1=\"Deutsch\",D2989,IF($B$1=\"中文\",E2989,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2990,IF($B$1=\"Deutsch\",D2990,IF($B$1=\"中文\",E2990,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2991,IF($B$1=\"Deutsch\",D2991,IF($B$1=\"中文\",E2991,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2992,IF($B$1=\"Deutsch\",D2992,IF($B$1=\"中文\",E2992,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2993,IF($B$1=\"Deutsch\",D2993,IF($B$1=\"中文\",E2993,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2994,IF($B$1=\"Deutsch\",D2994,IF($B$1=\"中文\",E2994,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• RB Defined"},"• RB Defined","• RB Defined","• RB Defined"]
[null,{"$f":"IF($B$1=\"English\",C2995,IF($B$1=\"Deutsch\",D2995,IF($B$1=\"中文\",E2995,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2996,IF($B$1=\"Deutsch\",D2996,IF($B$1=\"中文\",E2996,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2997,IF($B$1=\"Deutsch\",D2997,IF($B$1=\"中文\",E2997,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C2998,IF($B$1=\"Deutsch\",D2998,IF($B$1=\"中文\",E2998,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C2999,IF($B$1=\"Deutsch\",D2999,IF($B$1=\"中文\",E2999,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3000,IF($B$1=\"Deutsch\",D3000,IF($B$1=\"中文\",E3000,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3001,IF($B$1=\"Deutsch\",D3001,IF($B$1=\"中文\",E3001,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain "]
[null,{"$f":"IF($B$1=\"English\",C3002,IF($B$1=\"Deutsch\",D3002,IF($B$1=\"中文\",E3002,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain  "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain  ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain  ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain  "]
[null,{"$f":"IF($B$1=\"English\",C3003,IF($B$1=\"Deutsch\",D3003,IF($B$1=\"中文\",E3003,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3004,IF($B$1=\"Deutsch\",D3004,IF($B$1=\"中文\",E3004,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3005,IF($B$1=\"Deutsch\",D3005,IF($B$1=\"中文\",E3005,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3006,IF($B$1=\"Deutsch\",D3006,IF($B$1=\"中文\",E3006,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3007,IF($B$1=\"Deutsch\",D3007,IF($B$1=\"中文\",E3007,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3008,IF($B$1=\"Deutsch\",D3008,IF($B$1=\"中文\",E3008,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3009,IF($B$1=\"Deutsch\",D3009,IF($B$1=\"中文\",E3009,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3010,IF($B$1=\"Deutsch\",D3010,IF($B$1=\"中文\",E3010,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3011,IF($B$1=\"Deutsch\",D3011,IF($B$1=\"中文\",E3011,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3012,IF($B$1=\"Deutsch\",D3012,IF($B$1=\"中文\",E3012,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3013,IF($B$1=\"Deutsch\",D3013,IF($B$1=\"中文\",E3013,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3014,IF($B$1=\"Deutsch\",D3014,IF($B$1=\"中文\",E3014,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3015,IF($B$1=\"Deutsch\",D3015,IF($B$1=\"中文\",E3015,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3016,IF($B$1=\"Deutsch\",D3016,IF($B$1=\"中文\",E3016,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3017,IF($B$1=\"Deutsch\",D3017,IF($B$1=\"中文\",E3017,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3018,IF($B$1=\"Deutsch\",D3018,IF($B$1=\"中文\",E3018,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3019,IF($B$1=\"Deutsch\",D3019,IF($B$1=\"中文\",E3019,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3020,IF($B$1=\"Deutsch\",D3020,IF($B$1=\"中文\",E3020,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3021,IF($B$1=\"Deutsch\",D3021,IF($B$1=\"中文\",E3021,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3022,IF($B$1=\"Deutsch\",D3022,IF($B$1=\"中文\",E3022,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3023,IF($B$1=\"Deutsch\",D3023,IF($B$1=\"中文\",E3023,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3024,IF($B$1=\"Deutsch\",D3024,IF($B$1=\"中文\",E3024,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3025,IF($B$1=\"Deutsch\",D3025,IF($B$1=\"中文\",E3025,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022"},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products \n• French Decree no. 2022-748 of 29 April 2022","• 欧盟生态设计指令（指令 2009/125/EC）\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法\n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3026,IF($B$1=\"Deutsch\",D3026,IF($B$1=\"中文\",E3026,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"NOTES"},"NOTES","NOTES","注释"]
[null,{"$f":"IF($B$1=\"English\",C3027,IF($B$1=\"Deutsch\",D3027,IF($B$1=\"中文\",E3027,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Platinum group metals (PGM)"},"Platinum group metals (PGM)","Platinum group metals (PGM)","铂族金属 (PGM)"]
[null,{"$f":"IF($B$1=\"English\",C3028,IF($B$1=\"Deutsch\",D3028,IF($B$1=\"中文\",E3028,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heavy-group rare earth elements (HREE)"},"Heavy-group rare earth elements (HREE)","Heavy-group rare earth elements (HREE)","重稀土元素 (HREE)"]
[null,{"$f":"IF($B$1=\"English\",C3029,IF($B$1=\"Deutsch\",D3029,IF($B$1=\"中文\",E3029,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Light-group rare earth elements (LREE)"},"Light-group rare earth elements (LREE)","Light-group rare earth elements (LREE)","轻稀土元素 (LREE)"]
[null,{"$f":"IF($B$1=\"English\",C3030,IF($B$1=\"Deutsch\",D3030,IF($B$1=\"中文\",E3030,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tab 12: Critical Raw Materials (EU)\n(high economic importance)"},"Tab 12: Critical Raw Materials (EU)\n(high economic importance)","Tab 12: Critical Raw Materials (EU)\n(high economic importance)","表12：关键原材料法案（欧盟）\n(具有高度经济重要性"]
[null,{"$f":"IF($B$1=\"English\",C3031,IF($B$1=\"Deutsch\",D3031,IF($B$1=\"中文\",E3031,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"MADSL exceeded"},"MADSL exceeded","MADSL überschritten"," 超过 MADSL"]
[null,{"$f":"IF($B$1=\"English\",C3032,IF($B$1=\"Deutsch\",D3032,IF($B$1=\"中文\",E3032,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used to formulate writing inks and potentially other inks and to dye a wide variety of materials."},"Used to formulate writing inks and potentially other inks and to dye a wide variety of materials.","Wird zur Formulierung von Schreibtinten und potenziell auch anderen Tinten sowie zum Färben verschiedenster Materialien verwendet.","用于配制书写墨水和其他可能的墨水，以及对多种材料进行染色"]
[null,{"$f":"IF($B$1=\"English\",C3033,IF($B$1=\"Deutsch\",D3033,IF($B$1=\"中文\",E3033,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025","aufgenommen in Anhang 14\n- Antragsschluss: \n01.11.2023\n\n- Ablauftermin:  \n01.05.2025\n","列入附件 14 \n\n- 最后申请日期：2023 年 11 月 1 日 \n- 日落日期：2025年5月1日"]
[null,{"$f":"IF($B$1=\"English\",C3034,IF($B$1=\"Deutsch\",D3034,IF($B$1=\"中文\",E3034,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025","Aufgenommen in Annex XIV;\n- Antragsschluss: 01.11.2023\n- Ablauftermin: 01.05.2025","列入附件 14 \n\n- 最后申请日期：2023 年 11 月 1 日 \n- 日落日期：2025年5月1日"]
[null,{"$f":"IF($B$1=\"English\",C3035,IF($B$1=\"Deutsch\",D3035,IF($B$1=\"中文\",E3035,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (8-EO)"},"Nonylphenol, ethoxylated (8-EO)","Nonylphenol, ethoxylated (8-EO)","壬基酚，乙氧基化 (8-EO)"]
[null,{"$f":"IF($B$1=\"English\",C3036,IF($B$1=\"Deutsch\",D3036,IF($B$1=\"中文\",E3036,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol"},"26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol","26-(4-Nonylphenoxy)-3,6,9,12,15,18,21,24- octaoxahexacosan -1-ol"," 26-(4-壬基苯氧基)-3,6,9,12,15,18,21,24-八氧杂六聚糖-1-醇 "]
[null,{"$f":"IF($B$1=\"English\",C3037,IF($B$1=\"Deutsch\",D3037,IF($B$1=\"中文\",E3037,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (6,5-EO)"},"Nonylphenol, ethoxylated (6,5-EO)","Nonylphenol, ethoxylated (6,5-EO)","壬基苯酚，乙氧基化 (6,5-EO) "]
[null,{"$f":"IF($B$1=\"English\",C3038,IF($B$1=\"Deutsch\",D3038,IF($B$1=\"中文\",E3038,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, branched, ethoxylated"},"Nonylphenol, branched, ethoxylated","Nonylphenol, branched, ethoxylated","壬基酚，支链，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C3039,IF($B$1=\"Deutsch\",D3039,IF($B$1=\"中文\",E3039,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, ethoxylated"},"4-Nonylphenol, ethoxylated","4-Nonylphenol, ethoxylated"," 4-壬基苯酚，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C3040,IF($B$1=\"Deutsch\",D3040,IF($B$1=\"中文\",E3040,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","20-(4-nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"," 20-(4-壬基苯氧基)-3,6,9,12,15,18-六氧二十烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3041,IF($B$1=\"Deutsch\",D3041,IF($B$1=\"中文\",E3041,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (10-EO)"},"Nonylphenol, ethoxylated (10-EO)","Nonylphenol, ethoxylated (10-EO)","壬基酚，乙氧基化 (10-EO)"]
[null,{"$f":"IF($B$1=\"English\",C3042,IF($B$1=\"Deutsch\",D3042,IF($B$1=\"中文\",E3042,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated"},"Nonylphenol, ethoxylated","Nonylphenol, ethoxylated","壬基酚，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C3043,IF($B$1=\"Deutsch\",D3043,IF($B$1=\"中文\",E3043,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-, branched"},"Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-, branched","Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-, branched","歧化-α-(壬基苯基)-ω-羟基-(聚环氧乙烷)"]
[null,{"$f":"IF($B$1=\"English\",C3044,IF($B$1=\"Deutsch\",D3044,IF($B$1=\"中文\",E3044,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, branched"},"Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, branched","Poly (oxy-1,2-ethanediyl), alpha -(nonylphenyl)-omega-hydroxy-, branched","歧化-α-(壬基苯基)-ω-羟基-(聚环氧乙烷)"]
[null,{"$f":"IF($B$1=\"English\",C3045,IF($B$1=\"Deutsch\",D3045,IF($B$1=\"中文\",E3045,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol"},"2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol","2-[2-[2-[2-(4-nonylphenoxy)ethoxy]ethoxy]ethoxy]ethanol","2-[2-[2-[2-(4-壬基苯氧基)乙氧基]乙氧基]乙氧基]乙醇"]
[null,{"$f":"IF($B$1=\"English\",C3046,IF($B$1=\"Deutsch\",D3046,IF($B$1=\"中文\",E3046,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (15-EO)"},"Nonylphenol, ethoxylated (15-EO)","Nonylphenol, ethoxylated (15-EO)","壬基酚，乙氧基化 (15-EO)"]
[null,{"$f":"IF($B$1=\"English\",C3047,IF($B$1=\"Deutsch\",D3047,IF($B$1=\"中文\",E3047,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[2-(4-nonylphenoxy)ethoxy]ethanol"},"2-[2-(4-nonylphenoxy)ethoxy]ethanol","2-[2-(4-nonylphenoxy)ethoxy]ethanol","2-[2-(4-壬基苯氧基)乙氧基]乙醇"]
[null,{"$f":"IF($B$1=\"English\",C3048,IF($B$1=\"Deutsch\",D3048,IF($B$1=\"中文\",E3048,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched, ethoxylated"},"4-Nonylphenol, branched, ethoxylated","4-Nonylphenol, branched, ethoxylated","4-壬基苯酚，支链，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C3049,IF($B$1=\"Deutsch\",D3049,IF($B$1=\"中文\",E3049,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Nonylphenol, branched, ethoxylated"},"4-Nonylphenol, branched, ethoxylated","4-Nonylphenol, branched, ethoxylated","4-壬基苯酚，支链，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C3050,IF($B$1=\"Deutsch\",D3050,IF($B$1=\"中文\",E3050,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"17-(4-nonylphenoxy)-3,6,9,12,15-pentaoxaheptadecan-1-ol"},"17-(4-nonylphenoxy)-3,6,9,12,15-pentaoxaheptadecan-1-ol","17-(4-nonylphenoxy)-3,6,9,12,15-pentaoxaheptadecan-1-ol","17-(4-壬基苯氧基)-3,6,9,12,15-五氧杂十七烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3051,IF($B$1=\"Deutsch\",D3051,IF($B$1=\"中文\",E3051,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Isononylphenol, ethoxylated"},"Isononylphenol, ethoxylated","Isononylphenol, ethoxylated","异壬基苯酚，乙氧基化"]
[null,{"$f":"IF($B$1=\"English\",C3052,IF($B$1=\"Deutsch\",D3052,IF($B$1=\"中文\",E3052,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (polymer)"},"Nonylphenol, ethoxylated (polymer)","Nonylphenol, ethoxylated (polymer)","壬基苯酚，乙氧基化（聚合物）"]
[null,{"$f":"IF($B$1=\"English\",C3053,IF($B$1=\"Deutsch\",D3053,IF($B$1=\"中文\",E3053,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (EO = 4)"},"Nonylphenol, ethoxylated (EO = 4)","Nonylphenol, ethoxylated (EO = 4)","壬基酚，乙氧基化 (EO = 4)"]
[null,{"$f":"IF($B$1=\"English\",C3054,IF($B$1=\"Deutsch\",D3054,IF($B$1=\"中文\",E3054,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenol, ethoxylated (EO = 10)"},"Nonylphenol, ethoxylated (EO = 10)","Nonylphenol, ethoxylated (EO = 10)","壬基酚，乙氧基化 (EO = 10)"]
[null,{"$f":"IF($B$1=\"English\",C3055,IF($B$1=\"Deutsch\",D3055,IF($B$1=\"中文\",E3055,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-t-Nonylphenol-diethoxylate"},"4-t-Nonylphenol-diethoxylate","4-t-Nonylphenol-diethoxylate","4-叔壬基酚二乙氧基化物"]
[null,{"$f":"IF($B$1=\"English\",C3056,IF($B$1=\"Deutsch\",D3056,IF($B$1=\"中文\",E3056,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-"},"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-","3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-","3,6,9,12-四氧四烷-1-醇，14-(4-壬基苯氧基)-"]
[null,{"$f":"IF($B$1=\"English\",C3057,IF($B$1=\"Deutsch\",D3057,IF($B$1=\"中文\",E3057,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(nonylphenoxy)ethanol"},"2-(nonylphenoxy)ethanol","2-(nonylphenoxy)ethanol","2-(壬基苯氧基)乙醇"]
[null,{"$f":"IF($B$1=\"English\",C3058,IF($B$1=\"Deutsch\",D3058,IF($B$1=\"中文\",E3058,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol"},"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol","26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol","辛基酚聚醚-9"]
[null,{"$f":"IF($B$1=\"English\",C3059,IF($B$1=\"Deutsch\",D3059,IF($B$1=\"中文\",E3059,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"44-(nonylphenoxy)-3,6,9,12,15,18,21,24,27,30,33,36,39,42-tetradecaoxatetratetracontanol"},"44-(nonylphenoxy)-3,6,9,12,15,18,21,24,27,30,33,36,39,42-tetradecaoxatetratetracontanol","44-(nonylphenoxy)-3,6,9,12,15,18,21,24,27,30,33,36,39,42-tetradecaoxatetratetracontanol","44-(壬基苯氧基)-3,6,9,12,15,18,21,24,27,30,33,36,39,42-十四氧四十四烷醇"]
[null,{"$f":"IF($B$1=\"English\",C3060,IF($B$1=\"Deutsch\",D3060,IF($B$1=\"中文\",E3060,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"20-(isononylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"20-(isononylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","20-(isononylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","20-(异壬基苯氧基)-3,6,9,12,15,18-六氧杂二十烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3061,IF($B$1=\"Deutsch\",D3061,IF($B$1=\"中文\",E3061,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-, branched"},"3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-, branched","3,6,9,12-Tetraoxatetradecan-1-ol, 14-(4-nonylphenoxy)-, branched","3,6,9,12-四氧十四烷-1-醇, 14-(4-壬基苯氧基)-, 支链"]
[null,{"$f":"IF($B$1=\"English\",C3062,IF($B$1=\"Deutsch\",D3062,IF($B$1=\"中文\",E3062,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-"},"Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-","Poly(oxy-1,2-ethanediyl), α-(nonylphenyl)-ω-hydroxy-","聚（氧-1,2-乙二基），α-（壬基苯基）-ω-羟基-"]
[null,{"$f":"IF($B$1=\"English\",C3063,IF($B$1=\"Deutsch\",D3063,IF($B$1=\"中文\",E3063,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,6,9,12,15,18,21,24,27-Nonaoxanonacosan-1-ol, 29-(isononylphenoxy)-"},"3,6,9,12,15,18,21,24,27-Nonaoxanonacosan-1-ol, 29-(isononylphenoxy)-","3,6,9,12,15,18,21,24,27-Nonaoxanonacosan-1-ol, 29-(isononylphenoxy)-","壬基酚聚氧乙烯醚"]
[null,{"$f":"IF($B$1=\"English\",C3064,IF($B$1=\"Deutsch\",D3064,IF($B$1=\"中文\",E3064,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,6,9,12,15-Pentaoxaheptadecan-1-ol, 17-(nonylphenoxy)-"},"3,6,9,12,15-Pentaoxaheptadecan-1-ol, 17-(nonylphenoxy)-","3,6,9,12,15-Pentaoxaheptadecan-1-ol, 17-(nonylphenoxy)-","17-壬基苯氧基-3,6,9,12,15-五氧杂-十七(碳)-1醇"]
[null,{"$f":"IF($B$1=\"English\",C3065,IF($B$1=\"Deutsch\",D3065,IF($B$1=\"中文\",E3065,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol"},"2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol","2-{2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethoxy}ethanol","3,6,3-壬基酚二氧化物"]
[null,{"$f":"IF($B$1=\"English\",C3066,IF($B$1=\"Deutsch\",D3066,IF($B$1=\"中文\",E3066,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol"},"2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol","2-[4-(3,6-dimethylheptan-3-yl)phenoxy]ethanol","3,6,3-壬基酚一氧化物"]
[null,{"$f":"IF($B$1=\"English\",C3067,IF($B$1=\"Deutsch\",D3067,IF($B$1=\"中文\",E3067,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonylphenolpolyglycolether"},"Nonylphenolpolyglycolether","Nonylphenolpolyglycolether","壬基酚聚乙二醇醚"]
[null,{"$f":"IF($B$1=\"English\",C3068,IF($B$1=\"Deutsch\",D3068,IF($B$1=\"中文\",E3068,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(4-nonylphenoxy)ethanol"},"2-(4-nonylphenoxy)ethanol","2-(4-nonylphenoxy)ethanol","2-(4-壬基苯氧基)乙醇"]
[null,{"$f":"IF($B$1=\"English\",C3069,IF($B$1=\"Deutsch\",D3069,IF($B$1=\"中文\",E3069,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"29-(nonylphenoxy)-3,6,9,12,15,18,21,24,27-nonaoxanonacosanol"},"29-(nonylphenoxy)-3,6,9,12,15,18,21,24,27-nonaoxanonacosanol","29-(nonylphenoxy)-3,6,9,12,15,18,21,24,27-nonaoxanonacosanol","壬基酚聚醚-10"]
[null,{"$f":"IF($B$1=\"English\",C3070,IF($B$1=\"Deutsch\",D3070,IF($B$1=\"中文\",E3070,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol"},"23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol","23-(nonylphenoxy)-3,6,9,12,15,18,21-heptaoxatricosan-1-ol","23-壬基苯氧基-3,6,9,12,15,18,21-七氧杂二十三烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3071,IF($B$1=\"Deutsch\",D3071,IF($B$1=\"中文\",E3071,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"20-(nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol"},"20-(nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","20-(nonylphenoxy)-3,6,9,12,15,18-hexaoxaicosan-1-ol","壬基酚聚醚-7"]
[null,{"$f":"IF($B$1=\"English\",C3072,IF($B$1=\"Deutsch\",D3072,IF($B$1=\"中文\",E3072,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-[2-(nonylphenoxy)ethoxy]ethanol"},"2-[2-(nonylphenoxy)ethoxy]ethanol","2-[2-(nonylphenoxy)ethoxy]ethanol","2-[2-(壬基苯氧基)乙氧基]乙醇"]
[null,{"$f":"IF($B$1=\"English\",C3073,IF($B$1=\"Deutsch\",D3073,IF($B$1=\"中文\",E3073,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol"},"26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol","26-(nonylphenoxy)-3,6,9,12,15,18,21,24-octaoxahexacosan-1-ol","辛基酚聚醚-9"]
[null,{"$f":"IF($B$1=\"English\",C3074,IF($B$1=\"Deutsch\",D3074,IF($B$1=\"中文\",E3074,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(isononylphenoxy)ethanol"},"2-(isononylphenoxy)ethanol","2-(isononylphenoxy)ethanol","2-(异壬基苯氧基)乙醇"]
[null,{"$f":"IF($B$1=\"English\",C3075,IF($B$1=\"Deutsch\",D3075,IF($B$1=\"中文\",E3075,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol"},"14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol","14-(nonylphenoxy)-3,6,9,12-tetraoxatetradecan-1-ol","14-(壬基苯氧基)-3,6,9,12-四氧乙酸十四烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3076,IF($B$1=\"Deutsch\",D3076,IF($B$1=\"中文\",E3076,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trixylyl phosphate"},"Trixylyl phosphate","Trixylylphosphat","磷酸三甲苯酯"]
[null,{"$f":"IF($B$1=\"English\",C3077,IF($B$1=\"Deutsch\",D3077,IF($B$1=\"中文\",E3077,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)"},"Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)","Dinatrium-3,3'-((1,1'-biphenyl)-4,4'-diylbis(azo))bis(4-aminonaphthalin-1-sulfonat) (C.I. Direct Red 28)","3,3'-[[1,1'-联苯]-4,4'-基双(偶氮)]双(4-氨基萘-1-磺酸)二钠（刚果红）"]
[null,{"$f":"IF($B$1=\"English\",C3078,IF($B$1=\"Deutsch\",D3078,IF($B$1=\"中文\",E3078,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Imidazolidine-2-thione (2-imidazoline-2-thiol)"},"Imidazolidine-2-thione (2-imidazoline-2-thiol)","Imidazolidin-2-thion","咪唑啉-2-硫酮（2-咪唑啉-2-硫醇）"]
[null,{"$f":"IF($B$1=\"English\",C3079,IF($B$1=\"Deutsch\",D3079,IF($B$1=\"中文\",E3079,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium sulphide"},"Cadmium sulphide","Cadmiumsulfid"," \t硫化镉"]
[null,{"$f":"IF($B$1=\"English\",C3080,IF($B$1=\"Deutsch\",D3080,IF($B$1=\"中文\",E3080,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dihexyl phthalate"},"Dihexyl phthalate","Dihexylphthalat","邻苯二甲酸二己酯"]
[null,{"$f":"IF($B$1=\"English\",C3081,IF($B$1=\"Deutsch\",D3081,IF($B$1=\"中文\",E3081,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead di(acetate)"},"Lead di(acetate)","Bleidi(acetat)","二（醋酸）铅"]
[null,{"$f":"IF($B$1=\"English\",C3082,IF($B$1=\"Deutsch\",D3082,IF($B$1=\"中文\",E3082,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo] -\n5-hydroxy-6-(phenylazo)naphthalene-2,7-disulphonate (C.I. Direct Black 38)"},"Disodium 4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo] -\n5-hydroxy-6-(phenylazo)naphthalene-2,7-disulphonate (C.I. Direct Black 38)","Dinatrium-4-amino-3-[[4'-[(2,4-diaminophenyl)azo][1,1'-biphenyl]-4-yl]azo]-5-hydroxy-6-(phenylazo)naphthalin-2,7-disulfonat (C.I. Direct Red 38)","4-氨基-3-[[4'-[(2,4-二氨基苯基)偶氮基][1,1'-联苯基]-4-醇]偶氮] -5-羟基-6-(苯基偶氮)萘-2,7-二磺酸二钠（直接黑38）"]
[null,{"$f":"IF($B$1=\"English\",C3083,IF($B$1=\"Deutsch\",D3083,IF($B$1=\"中文\",E3083,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perborate; perboric acid, sodium salt"},"Sodium perborate; perboric acid, sodium salt","Natriumperborat; Perborsäure, Natriumsalz","过硼酸钠； 过硼酸，钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3084,IF($B$1=\"Deutsch\",D3084,IF($B$1=\"中文\",E3084,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perboric acid (H3BO2(O2)), monosodium salt, trihydrate"},"Perboric acid (H3BO2(O2)), monosodium salt, trihydrate","Perboric acid (H3BO2(O2)), monosodium salt, trihydrate","过硼酸(H3BO2(O2))，单钠盐，三水合物（三水合过硼酸钠）"]
[null,{"$f":"IF($B$1=\"English\",C3085,IF($B$1=\"Deutsch\",D3085,IF($B$1=\"中文\",E3085,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)"},"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)","Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium (1:2)","硼酸(2-), 四羟基双[μ-(过氧羟基-κO1:κO2)]二钠 (1:2)"]
[null,{"$f":"IF($B$1=\"English\",C3086,IF($B$1=\"Deutsch\",D3086,IF($B$1=\"中文\",E3086,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perboric acid, sodium salt"},"Perboric acid, sodium salt","Perboric acid, sodium salt","过硼酸钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3087,IF($B$1=\"Deutsch\",D3087,IF($B$1=\"中文\",E3087,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perborate"},"Sodium perborate","Sodium perborate","过硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C3088,IF($B$1=\"Deutsch\",D3088,IF($B$1=\"中文\",E3088,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)"},"Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)","Borate(2-), tetrahydroxybis[μ-(peroxy-κO1:κO2)]di-, sodium, hydrate (1:2:6)","硼酸(2-), 四羟基双[μ-(过氧羟基-κO1:κO2)]二钠盐水合物 (1:2:6)"]
[null,{"$f":"IF($B$1=\"English\",C3089,IF($B$1=\"Deutsch\",D3089,IF($B$1=\"中文\",E3089,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium peroxometaborate"},"Sodium peroxometaborate","Sodium peroxometaborate","過氧偏硼酸鈉"]
[null,{"$f":"IF($B$1=\"English\",C3090,IF($B$1=\"Deutsch\",D3090,IF($B$1=\"中文\",E3090,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium chloride"},"Cadmium chloride","Cadmiumchlorid","氯化镉"]
[null,{"$f":"IF($B$1=\"English\",C3091,IF($B$1=\"Deutsch\",D3091,IF($B$1=\"中文\",E3091,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear"},"1,2-Benzenedicarboxylic acid, dihexyl ester, branched and linear","1,2-Benzoldicarbonsäure, Dihexylester, verzweigt und linear","1,2-苯二甲酸己酯支链和支链"]
[null,{"$f":"IF($B$1=\"English\",C3092,IF($B$1=\"Deutsch\",D3092,IF($B$1=\"中文\",E3092,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of  DOTE und MOTE)"},"Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of  DOTE und MOTE)","Reaction mass of 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (Reaction mass of DOTE und MOTE)","二正辛基-双（巯乙酸2-乙基己酯）锡和\n单辛基-三（2-乙基己基巯基乙酸酯）锡的反应产物（DOTE和 MOTE的反应产物）"]
[null,{"$f":"IF($B$1=\"English\",C3093,IF($B$1=\"Deutsch\",D3093,IF($B$1=\"中文\",E3093,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium fluoride"},"Cadmium fluoride","Cadmiumfluorid","氟化镉"]
[null,{"$f":"IF($B$1=\"English\",C3094,IF($B$1=\"Deutsch\",D3094,IF($B$1=\"中文\",E3094,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium sulphate"},"Cadmium sulphate","Cadmiumsulfat","硫酸镉"]
[null,{"$f":"IF($B$1=\"English\",C3095,IF($B$1=\"Deutsch\",D3095,IF($B$1=\"中文\",E3095,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate (DEHP)"},"Bis(2-ethylhexyl)phthalate (DEHP)","Bis(2-ethylhexyl)phthalat (DEHP)","双（2-乙基己基）邻苯二甲酸酯 (DEHP)"]
[null,{"$f":"IF($B$1=\"English\",C3096,IF($B$1=\"Deutsch\",D3096,IF($B$1=\"中文\",E3096,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-\ndithia-4-stannatetradecanoate (DOTE)"},"2-ethylhexyl 10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-\ndithia-4-stannatetradecanoate (DOTE)","2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoat (DOTE)","二正辛基-双（巯乙酸2-乙基己酯）锡（DOTE）"]
[null,{"$f":"IF($B$1=\"English\",C3097,IF($B$1=\"Deutsch\",D3097,IF($B$1=\"中文\",E3097,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)"},"2-benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)","2-Benzotriazol-2-yl-4,6-di-tert-butylphenol (UV-320)","2-苯并三唑-2-基-4,6-二叔丁基苯酚（紫外线吸收剂UV-320）"]
[null,{"$f":"IF($B$1=\"English\",C3098,IF($B$1=\"Deutsch\",D3098,IF($B$1=\"中文\",E3098,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)"},"2-(2H-benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)","2-(2H-Benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328)","2-（2H-苯并三唑-2-基）-4,6-二叔戊基苯酚\n（紫外线吸收剂 UV-328）"]
[null,{"$f":"IF($B$1=\"English\",C3099,IF($B$1=\"Deutsch\",D3099,IF($B$1=\"中文\",E3099,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-\nmethyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-\ndimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]\n[covering any of the individual isomers of [1] and [2] or\nany combination thereof]"},"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-\nmethyl-1,3-dioxane [1], 5-sec-butyl-2-(4,6-\ndimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane [2]\n[covering any of the individual isomers of [1] and [2] or\nany combination thereof]","5-sec-Butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxan [1], \n\n5-sec-Butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxan [2]\n\n[Die einzelnen Stereoisomere von [1] und [2] sowie alle möglichen Kombinationen sind durch diesen Eintrag abgedeckt]","5-仲丁基-2-(2,4-二甲基环己基-3-烯-1-醇)-5-甲基-1,3-二氧杂环[1], 5-仲丁基-2-(4,6-二甲基环己基-3-烯-1-醇)-5-甲基-1,3-二氧杂环[2]\n[包括[1] 和[2]的各异构体及此等异构体的任何组合]"]
[null,{"$f":"IF($B$1=\"English\",C3100,IF($B$1=\"Deutsch\",D3100,IF($B$1=\"中文\",E3100,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane"},"Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane","Reaction mass of 5-[(2R)-butan-2-yl]-2-[(1R,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1R,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2R)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2R)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane and 5-[(2S)-butan-2-yl]-2-[(1S,2S)-2,4-dimethylcyclohex-3-en-1-yl]-5-methyl-1,3-dioxane","反应物质5-[(2R)-丁-2-醇]-2-[(1R,2R)-2,4-二甲基环己基-3-烯-1-醇]-5-甲基-1,3-二氧杂环、5-[(2R)-丁-2-醇]-2-[(1R,2S)-2,4-二甲基环己基-3-烯-1-醇]-5-甲基-1,3-二氧杂环、5-[(2R)-丁-2-醇]-2-[(1S,2R)-2,4-二甲基环己基-3-烯-1-yl]-5-甲基-1,3-二氧杂环 、5-[(2R)-丁-2-醇]-2-[(1S,2S)-2,4-二甲基环己基-3-烯-1-醇]-5-甲基-1,3-二氧杂环、5-[(2S)-丁-2-醇]-2-[(1S,2R)-2,4-二甲基环己基-3-烯-1-醇]-5-甲基-1,3-二氧杂环和5-[(2S)-丁-2-醇]-2-[(1S,2S)-2,4-二甲基环己基-3-烯-1-醇]-5-甲基-1,3-二氧杂环"]
[null,{"$f":"IF($B$1=\"English\",C3101,IF($B$1=\"Deutsch\",D3101,IF($B$1=\"中文\",E3101,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane"},"2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane","2-(2,4-Dimethylcyclohex-3-ene-1-yl)-5-methyl-(1-methylpropyl)-1,3-dioxane","卡拉花醛"]
[null,{"$f":"IF($B$1=\"English\",C3102,IF($B$1=\"Deutsch\",D3102,IF($B$1=\"中文\",E3102,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane "},"Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane ","Reaction mass of 5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane and 5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane ","5-仲丁基-2-(2,4-二甲基环己基-3-烯-1-醇)-5-甲基-1,3-二氧杂环和 5-仲丁基-2-(4,6-二甲基环己基-3-烯-1-醇)-5-甲基-1,3-二氧杂环的反应产物"]
[null,{"$f":"IF($B$1=\"English\",C3103,IF($B$1=\"Deutsch\",D3103,IF($B$1=\"中文\",E3103,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-二噁烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-, 顺式-"]
[null,{"$f":"IF($B$1=\"English\",C3104,IF($B$1=\"Deutsch\",D3104,IF($B$1=\"中文\",E3104,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二噁烷, 2-[(1S,2S)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-,反式-"]
[null,{"$f":"IF($B$1=\"English\",C3105,IF($B$1=\"Deutsch\",D3105,IF($B$1=\"中文\",E3105,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二噁烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-,反式-"]
[null,{"$f":"IF($B$1=\"English\",C3106,IF($B$1=\"Deutsch\",D3106,IF($B$1=\"中文\",E3106,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-rel-","1,3-二噁烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-,反式-rel-"]
[null,{"$f":"IF($B$1=\"English\",C3107,IF($B$1=\"Deutsch\",D3107,IF($B$1=\"中文\",E3107,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-二噁烷, 2-[(1R,2S)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-, 顺式-"]
[null,{"$f":"IF($B$1=\"English\",C3108,IF($B$1=\"Deutsch\",D3108,IF($B$1=\"中文\",E3108,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1R,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二噁烷, 2-[(1R,2S)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-, 反式-"]
[null,{"$f":"IF($B$1=\"English\",C3109,IF($B$1=\"Deutsch\",D3109,IF($B$1=\"中文\",E3109,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- "},"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- ","1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis- ","1,3-二噁烷, 2-[(1S,2R)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-, 顺式- "]
[null,{"$f":"IF($B$1=\"English\",C3110,IF($B$1=\"Deutsch\",D3110,IF($B$1=\"中文\",E3110,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-"},"1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-Dioxane, 2-[(1S,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, trans-","1,3-二噁烷, 2-[(1S,2R)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-, 反式-"]
[null,{"$f":"IF($B$1=\"English\",C3111,IF($B$1=\"Deutsch\",D3111,IF($B$1=\"中文\",E3111,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-"},"1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-Dioxane, 2-[(1S,2S)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-","1,3-二噁烷, 2-[(1S,2S)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-, 顺式-"]
[null,{"$f":"IF($B$1=\"English\",C3112,IF($B$1=\"Deutsch\",D3112,IF($B$1=\"中文\",E3112,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-"},"1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","1,3-Dioxane, 2-(2,4-dimethyl-3-cyclohexen-1-yl)-5-methyl-5-(1-methylpropyl)-","1,3-二噁烷, 2-(2,4-二甲基-3-环己烯-1-醇)-5-甲基-5-(1-甲基丙基)-"]
[null,{"$f":"IF($B$1=\"English\",C3113,IF($B$1=\"Deutsch\",D3113,IF($B$1=\"中文\",E3113,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane"},"5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-sec-butyl-2-(4,6-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-仲丁基-2-(4,6-二甲基环己基-3-烯-1-醇)-5-甲基-1,3-二氧杂环"]
[null,{"$f":"IF($B$1=\"English\",C3114,IF($B$1=\"Deutsch\",D3114,IF($B$1=\"中文\",E3114,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane"},"5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-sec-butyl-2-(2,4-dimethylcyclohex-3-en-1-yl)-5-methyl-1,3-dioxane","5-仲丁基-2-(2,4-二甲基环己基-3-烯-1-醇)-5-甲基-1,3-二氧杂环"]
[null,{"$f":"IF($B$1=\"English\",C3115,IF($B$1=\"Deutsch\",D3115,IF($B$1=\"中文\",E3115,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-"},"1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-","1,3-Dioxane, 2-[(1R,2R)-2,4-dimethyl-3-cyclohexen-1-yl]-5-methyl-5-(1-methylpropyl)-, cis-rel-","1,3-二噁烷, 2-[(1R,2R)-2,4-二甲基-3-环己烯-1-醇]-5-甲基-5-(1-甲基丙基)-,"]
[null,{"$f":"IF($B$1=\"English\",C3116,IF($B$1=\"Deutsch\",D3116,IF($B$1=\"中文\",E3116,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters \nwith ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)"},"1,2-benzenedicarboxylic acid, di-C6-10-alkyl esters or mixed decyl and hexyl and octyl diesters \nwith ≥ 0.3% of dihexyl phthalate (EC No. 201-559-5)","1,2-Benzoldicarbonsäure, Di-C6-10-alkylester; 1,2-Benzoldicarbonsäure, gemischte Decyl- und Hexyl- und Octyldiester mit ≥ 0,3% Dihexylphthalat (EG Nr. 201-559-5)","邻苯二甲酸二(C6-C10)烷基酯，或癸基、己基、辛基酯混合物 \n含0.3%或以上的邻苯二甲酸二己酯（EC号：201-559-5）"]
[null,{"$f":"IF($B$1=\"English\",C3117,IF($B$1=\"Deutsch\",D3117,IF($B$1=\"中文\",E3117,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters"},"1,2-Benzenedicarboxylic acid, mixed decyl and hexyl and octyl diesters","1,2-Benzoldicarbonsäure, gemischte Decyl- und Hexyl- und Octyldiester ","1,2-苯二甲酸，混合癸基、己基、辛基酯"]
[null,{"$f":"IF($B$1=\"English\",C3118,IF($B$1=\"Deutsch\",D3118,IF($B$1=\"中文\",E3118,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-Benzenedicarboxylic acid, di-C6-10-alkyl esters"},"1,2-Benzenedicarboxylic acid, di-C6-10-alkyl esters","1,2-Benzoldicarbonsäure, Di-C6-10-alkylester","邻苯二甲酸二(C6-C10)烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3119,IF($B$1=\"Deutsch\",D3119,IF($B$1=\"中文\",E3119,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorononan-1-oic-acid and its sodium and ammonium salts"},"Perfluorononan-1-oic-acid and its sodium and ammonium salts","Perfluornonan-1-säure und seine Narium- und Ammoniumsalze\n","全氟壬酸及其钠盐和铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3120,IF($B$1=\"Deutsch\",D3120,IF($B$1=\"中文\",E3120,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorononan-1-oic acid"},"Perfluorononan-1-oic acid","Perfluornonan-1-säure","全氟壬酸"]
[null,{"$f":"IF($B$1=\"English\",C3121,IF($B$1=\"Deutsch\",D3121,IF($B$1=\"中文\",E3121,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"perfluorononan-1-oic acid sodium salts"},"perfluorononan-1-oic acid sodium salts","Natrium perfluornonanoat","全氟壬酸钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3122,IF($B$1=\"Deutsch\",D3122,IF($B$1=\"中文\",E3122,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"perfluorononan-1-oic acid ammonium salts"},"perfluorononan-1-oic acid ammonium salts","Ammonium perfluornonanoat","全氟壬酸铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3123,IF($B$1=\"Deutsch\",D3123,IF($B$1=\"中文\",E3123,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nitrobenzene"},"Nitrobenzene","Nitrobenzol","硝基苯"]
[null,{"$f":"IF($B$1=\"English\",C3124,IF($B$1=\"Deutsch\",D3124,IF($B$1=\"中文\",E3124,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)"},"2-(2H-benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)","2-(2H-Benzotriazol-2-yl)-4-(tert-butyl)-6-(sec-butyl)phenol (UV-350)","2-(2'-羟基-3'-异丁基-5'-叔丁基苯基)苯并三唑（UV-350）"]
[null,{"$f":"IF($B$1=\"English\",C3125,IF($B$1=\"Deutsch\",D3125,IF($B$1=\"中文\",E3125,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-propanesultone"},"1,3-propanesultone","1,3-Propansulton","1,3-丙烷磺内酯"]
[null,{"$f":"IF($B$1=\"English\",C3126,IF($B$1=\"Deutsch\",D3126,IF($B$1=\"中文\",E3126,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)"},"2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)","2,4-Di-tert-butyl-6-(5-chlorbenzotriazol-2-yl)phenol (UV-327)","2,4-二-叔丁基-6-(5-氯代苯并三唑-2-基)苯酚（UV-327）"]
[null,{"$f":"IF($B$1=\"English\",C3127,IF($B$1=\"Deutsch\",D3127,IF($B$1=\"中文\",E3127,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[def]chrysene (Benzo[a]pyrene)"},"Benzo[def]chrysene (Benzo[a]pyrene)","Benzo[a]pyren (Benzo[def]chrysen)","苯并[def]屈（苯并[a]芘）"]
[null,{"$f":"IF($B$1=\"English\",C3128,IF($B$1=\"Deutsch\",D3128,IF($B$1=\"中文\",E3128,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-Heptylphenol, branched and linear (4-HPbl)"},"4-Heptylphenol, branched and linear (4-HPbl)","4-Heptylphenol, verzweigt und linear\n(4-HPbl)\n\n[Substanzen mit einer linearen und/oder verzweigten Alkylkette mit einer Kohlenstoffzahl von 7, die überwiegend in Position 4 kovalent an Phenol gebunden ist, wobei auch UVCB- und genau definierte Substanzen eingeschlossen sind, die eines der einzelnen Isomere oder eine Kombination davon enthalten]","4-庚基苯酚，支链和直链 (4-HPbl)"]
[null,{"$f":"IF($B$1=\"English\",C3129,IF($B$1=\"Deutsch\",D3129,IF($B$1=\"中文\",E3129,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, heptyl derivs."},"Phenol, heptyl derivs.","Phenol, heptyl derivs.","酚，庚基衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3130,IF($B$1=\"Deutsch\",D3130,IF($B$1=\"中文\",E3130,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-heptylphenol "},"4-heptylphenol ","4-heptylphenol ","4-庚基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3131,IF($B$1=\"Deutsch\",D3131,IF($B$1=\"中文\",E3131,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1-diethylpropyl)- "},"Phenol, 4-(1,1-diethylpropyl)- ","Phenol, 4-(1,1-diethylpropyl)- ","4-(叔丁氧基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C3132,IF($B$1=\"Deutsch\",D3132,IF($B$1=\"中文\",E3132,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1-dimethylpentyl)-"},"Phenol, 4-(1,1-dimethylpentyl)-","Phenol, 4-(1,1-dimethylpentyl)-","4-(1,1-二甲基丙基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3133,IF($B$1=\"Deutsch\",D3133,IF($B$1=\"中文\",E3133,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,2,2-trimethylbutyl)-"},"Phenol, 4-(1,2,2-trimethylbutyl)-","Phenol, 4-(1,2,2-trimethylbutyl)-","4-(1,2,2-三甲基丁基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3134,IF($B$1=\"Deutsch\",D3134,IF($B$1=\"中文\",E3134,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,2-dimethylpentyl)-"},"Phenol, 4-(1,2-dimethylpentyl)-","Phenol, 4-(1,2-dimethylpentyl)-","4-(1,2-二甲基戊基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3135,IF($B$1=\"Deutsch\",D3135,IF($B$1=\"中文\",E3135,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,3,3-trimethylbutyl)- "},"Phenol, 4-(1,3,3-trimethylbutyl)- ","Phenol, 4-(1,3,3-trimethylbutyl)- "," 4-(1,3,3-三甲基丁基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C3136,IF($B$1=\"Deutsch\",D3136,IF($B$1=\"中文\",E3136,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,3-dimethylpentyl)-"},"Phenol, 4-(1,3-dimethylpentyl)-","Phenol, 4-(1,3-dimethylpentyl)-","4-(1,3-二甲基戊基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3137,IF($B$1=\"Deutsch\",D3137,IF($B$1=\"中文\",E3137,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,4-dimethylpentyl)-"},"Phenol, 4-(1,4-dimethylpentyl)-","Phenol, 4-(1,4-dimethylpentyl)-","4-(1,4-二甲基戊基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3138,IF($B$1=\"Deutsch\",D3138,IF($B$1=\"中文\",E3138,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-"},"Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-","Phenol, 4-(1-ethyl-2,2-dimethylpropyl)-","4-(1-乙基-2,2-二甲基丙基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3139,IF($B$1=\"Deutsch\",D3139,IF($B$1=\"中文\",E3139,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-"},"Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-","Phenol, 4-(1-ethyl-1,2-dimethylpropyl)-","4-(1-乙基-1,2-二甲基丙基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3140,IF($B$1=\"Deutsch\",D3140,IF($B$1=\"中文\",E3140,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethylpentyl)-"},"Phenol, 4-(1-ethylpentyl)-","Phenol, 4-(1-ethylpentyl)-","4-(1-乙基戊基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3141,IF($B$1=\"Deutsch\",D3141,IF($B$1=\"中文\",E3141,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-methylhexyl)-"},"Phenol, 4-(1-methylhexyl)-","Phenol, 4-(1-methylhexyl)-","4-(1-甲基己基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3142,IF($B$1=\"Deutsch\",D3142,IF($B$1=\"中文\",E3142,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-propylbutyl)-"},"Phenol, 4-(1-propylbutyl)-","Phenol, 4-(1-propylbutyl)-"," 4-(1-丙基丁基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3143,IF($B$1=\"Deutsch\",D3143,IF($B$1=\"中文\",E3143,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(3-ethylpentyl)- "},"Phenol, 4-(3-ethylpentyl)- ","Phenol, 4-(3-ethylpentyl)- ","4-(3-乙基戊基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C3144,IF($B$1=\"Deutsch\",D3144,IF($B$1=\"中文\",E3144,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(3-methylhexyl)- "},"Phenol, 4-(3-methylhexyl)- ","Phenol, 4-(3-methylhexyl)- ","4-(3-甲基己基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C3145,IF($B$1=\"Deutsch\",D3145,IF($B$1=\"中文\",E3145,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(4-methylhexyl)-"},"Phenol, 4-(4-methylhexyl)-","Phenol, 4-(4-methylhexyl)-","4-(4-甲基己基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3146,IF($B$1=\"Deutsch\",D3146,IF($B$1=\"中文\",E3146,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(5-methylhexyl)-"},"Phenol, 4-(5-methylhexyl)-","Phenol, 4-(5-methylhexyl)-","4-(5-甲基己基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3147,IF($B$1=\"Deutsch\",D3147,IF($B$1=\"中文\",E3147,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-"},"Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-","Phenol, 4-[2-methyl-1-(1-methylethyl)propyl]-","4-[2-甲基-1-(1-甲基乙基)丙基]苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3148,IF($B$1=\"Deutsch\",D3148,IF($B$1=\"中文\",E3148,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(2,3-dimethylpentan-2-yl)phenol "},"4-(2,3-dimethylpentan-2-yl)phenol ","4-(2,3-dimethylpentan-2-yl)phenol ","4-(2,3-二甲基戊烷-2-醇)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C3149,IF($B$1=\"Deutsch\",D3149,IF($B$1=\"中文\",E3149,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-(3-methylhexan-3-yl)phenol"},"4-(3-methylhexan-3-yl)phenol","4-(3-methylhexan-3-yl)phenol","4-(3-甲基己烷-3-醇)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3150,IF($B$1=\"Deutsch\",D3150,IF($B$1=\"中文\",E3150,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-tert-heptyl-"},"Phenol, 4-tert-heptyl-","Phenol, 4-tert-heptyl-","4-叔庚基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3151,IF($B$1=\"Deutsch\",D3151,IF($B$1=\"中文\",E3151,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1,3-trimethylbutyl)-"},"Phenol, 4-(1,1,3-trimethylbutyl)-","Phenol, 4-(1,1,3-trimethylbutyl)-","4-(1,1,3-三甲基丁基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3152,IF($B$1=\"Deutsch\",D3152,IF($B$1=\"中文\",E3152,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1,1,2,2-tetramethylpropyl)- "},"Phenol, 4-(1,1,2,2-tetramethylpropyl)- ","Phenol, 4-(1,1,2,2-tetramethylpropyl)- ","4-(1,1,2,2-四甲基丙基)苯酚 "]
[null,{"$f":"IF($B$1=\"English\",C3153,IF($B$1=\"Deutsch\",D3153,IF($B$1=\"中文\",E3153,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-(1-ethyl-3-methylbutyl)-"},"Phenol, 4-(1-ethyl-3-methylbutyl)-","Phenol, 4-(1-ethyl-3-methylbutyl)-","4-(1-乙基-3-甲基丁基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3154,IF($B$1=\"Deutsch\",D3154,IF($B$1=\"中文\",E3154,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"p-(1,1-dimethylpropyl)phenol"},"p-(1,1-dimethylpropyl)phenol","p-(1,1-dimethylpropyl)phenol\n4-tert-Pentylphenol (PTAP)","p-(1,1-二甲基丙基)苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3155,IF($B$1=\"Deutsch\",D3155,IF($B$1=\"中文\",E3155,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts"},"Nonadecafluorodecanoic acid (PFDA) and its sodium and ammonium salts","Nonadecafluorodecansäure (PFDA) und ihre Natrium- und Ammonium-Salze\nNonadecafluordecansäure\nAmmoniumnonadecafluordecanoat\nNatriumnonadecafluordecanoat","十九氟癸酸 (PFDA) 及其钠盐和铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3156,IF($B$1=\"Deutsch\",D3156,IF($B$1=\"中文\",E3156,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonadecafluorodecanoic acid"},"Nonadecafluorodecanoic acid","Nonadecafluordecansäure","十九氟癸酸"]
[null,{"$f":"IF($B$1=\"English\",C3157,IF($B$1=\"Deutsch\",D3157,IF($B$1=\"中文\",E3157,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammoniumnonadecafluordecanoat"},"Ammoniumnonadecafluordecanoat","Ammoniumnonadecafluordecanoat","十九氟癸酸铵"]
[null,{"$f":"IF($B$1=\"English\",C3158,IF($B$1=\"Deutsch\",D3158,IF($B$1=\"中文\",E3158,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"sodium nonadecafluorodecanoate "},"sodium nonadecafluorodecanoate ","Natriumnonadecafluordecanoat","十九氟癸酸钠"]
[null,{"$f":"IF($B$1=\"English\",C3159,IF($B$1=\"Deutsch\",D3159,IF($B$1=\"中文\",E3159,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexane-1-sulphonic acid and its salts"},"Perfluorohexane-1-sulphonic acid and its salts","Perfluorhexan-1-sulfonsäure und ihre Salze\n(PFHxS)","全氟己烷-1-磺酸及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C3160,IF($B$1=\"Deutsch\",D3160,IF($B$1=\"中文\",E3160,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium perfluorohexane-1-sulphonate"},"Potassium perfluorohexane-1-sulphonate","Potassium perfluorohexane-1-sulphonate","1-全氟己烷磺酸钾"]
[null,{"$f":"IF($B$1=\"English\",C3161,IF($B$1=\"Deutsch\",D3161,IF($B$1=\"中文\",E3161,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexane-1-sulphonic acid"},"Perfluorohexane-1-sulphonic acid","Perfluorohexane-1-sulphonic acid","全氟己烷-1-磺酸"]
[null,{"$f":"IF($B$1=\"English\",C3162,IF($B$1=\"Deutsch\",D3162,IF($B$1=\"中文\",E3162,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)"},"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)","Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)","十三氟己烷磺酸，与 2,2'-亚氨基二乙醇 (1:1) 的化合物"]
[null,{"$f":"IF($B$1=\"English\",C3163,IF($B$1=\"Deutsch\",D3163,IF($B$1=\"中文\",E3163,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium perfluorohexane-1-sulphonate"},"Ammonium perfluorohexane-1-sulphonate","Ammonium perfluorohexane-1-sulphonate","全氟己烷-1-磺酸铵"]
[null,{"$f":"IF($B$1=\"English\",C3164,IF($B$1=\"Deutsch\",D3164,IF($B$1=\"中文\",E3164,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟镓盐（9CI）"]
[null,{"$f":"IF($B$1=\"English\",C3165,IF($B$1=\"Deutsch\",D3165,IF($B$1=\"中文\",E3165,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","双(4-甲基苯基)苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-乙烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3166,IF($B$1=\"Deutsch\",D3166,IF($B$1=\"中文\",E3166,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟- 钪(3+)盐(3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3167,IF($B$1=\"Deutsch\",D3167,IF($B$1=\"中文\",E3167,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-钕(3+) 盐(3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3168,IF($B$1=\"Deutsch\",D3168,IF($B$1=\"中文\",E3168,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-钇(3+) 盐 (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3169,IF($B$1=\"Deutsch\",D3169,IF($B$1=\"中文\",E3169,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)"},"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)","Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)","(硫代-4,1-亚苯基)双[二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍盐 (1:2)"]
[null,{"$f":"IF($B$1=\"English\",C3170,IF($B$1=\"Deutsch\",D3170,IF($B$1=\"中文\",E3170,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic"},"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","双[4-(1,1-二甲基丙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸碘"]
[null,{"$f":"IF($B$1=\"English\",C3171,IF($B$1=\"Deutsch\",D3171,IF($B$1=\"中文\",E3171,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三[4-(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3172,IF($B$1=\"Deutsch\",D3172,IF($B$1=\"中文\",E3172,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 锂盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3173,IF($B$1=\"Deutsch\",D3173,IF($B$1=\"中文\",E3173,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 锌盐"]
[null,{"$f":"IF($B$1=\"English\",C3174,IF($B$1=\"Deutsch\",D3174,IF($B$1=\"中文\",E3174,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","双[4-(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸碘(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3175,IF($B$1=\"Deutsch\",D3175,IF($B$1=\"中文\",E3175,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3176,IF($B$1=\"Deutsch\",D3176,IF($B$1=\"中文\",E3176,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)"},"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","双[(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-乙烷磺酸碘盐(1:1) (9CI)"]
[null,{"$f":"IF($B$1=\"English\",C3177,IF($B$1=\"Deutsch\",D3177,IF($B$1=\"中文\",E3177,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," (4-甲基苯基)二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3178,IF($B$1=\"Deutsch\",D3178,IF($B$1=\"中文\",E3178,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","[4-[(2-甲基-1-氧代-2-丙烯-1-醇)氧基]苯基]二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3179,IF($B$1=\"Deutsch\",D3179,IF($B$1=\"中文\",E3179,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"},"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate","Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"," [4-[(2-甲基-1-氧代-2-丙烯基)氧基]苯基]二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍(1:1), 与 2-乙基三环[3.3.1.13,7]癸-2-醇 2-甲基-2-丙烯酸酯, 3-氢氧三环[3.3.1.13,7]癸-1-醇2-甲基-2-丙烯酸酯和四氢-2-氧代-3-呋喃基 2-甲基-2-丙烯酸酯的聚合物"]
[null,{"$f":"IF($B$1=\"English\",C3180,IF($B$1=\"Deutsch\",D3180,IF($B$1=\"中文\",E3180,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 铯盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3181,IF($B$1=\"Deutsch\",D3181,IF($B$1=\"中文\",E3181,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","二苯并[k,n][1,4,7,10,13]四噁噻环十五烷, 19-[4-(1,1-二甲基乙基)苯基]-6,7,9,10,12,13-六氢-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3182,IF($B$1=\"Deutsch\",D3182,IF($B$1=\"中文\",E3182,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","乙铵, N-[4-[[4-(二乙氨基)苯基][4-(乙氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-乙基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3183,IF($B$1=\"Deutsch\",D3183,IF($B$1=\"中文\",E3183,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","N-[4-[[4-(二甲基氨基)苯基][4-(乙氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-甲基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸甲胺 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3184,IF($B$1=\"Deutsch\",D3184,IF($B$1=\"中文\",E3184,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," N-[4-[[4-(二甲基氨基)苯基][4-(苯氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-甲基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸甲胺 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3185,IF($B$1=\"Deutsch\",D3185,IF($B$1=\"中文\",E3185,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","β-环糊精，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸离子(1-)的化合物(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3186,IF($B$1=\"Deutsch\",D3186,IF($B$1=\"中文\",E3186,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","γ-环糊精，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸离子(1-)的化合物(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3187,IF($B$1=\"Deutsch\",D3187,IF($B$1=\"中文\",E3187,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," 三苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3188,IF($B$1=\"Deutsch\",D3188,IF($B$1=\"中文\",E3188,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," 1-(羧甲基)-4-[2-[4-[4-(2,2-二苯基乙烯基)苯基]-1,2,3,3a,4,8b-六氢环五[b]吲哚-7-基]乙烯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸 喹啉(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3189,IF($B$1=\"Deutsch\",D3189,IF($B$1=\"中文\",E3189,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," 二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸碘 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3190,IF($B$1=\"Deutsch\",D3190,IF($B$1=\"中文\",E3190,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","N,N,N-三甲基甲胺-, 与 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3191,IF($B$1=\"Deutsch\",D3191,IF($B$1=\"中文\",E3191,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 与 2-甲基-2-丙酰胺的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3192,IF($B$1=\"Deutsch\",D3192,IF($B$1=\"中文\",E3192,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-,与吡咯烷的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3193,IF($B$1=\"Deutsch\",D3193,IF($B$1=\"中文\",E3193,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","N,N,N-三乙基-乙铵, 与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3194,IF($B$1=\"Deutsch\",D3194,IF($B$1=\"中文\",E3194,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid"},"1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid","1-Butanaminium, N,N,N-tributyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid","1-丁氨基, N,N,N-三丁基-, 与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐"]
[null,{"$f":"IF($B$1=\"English\",C3195,IF($B$1=\"Deutsch\",D3195,IF($B$1=\"中文\",E3195,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三苯基(苯甲基)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3196,IF($B$1=\"Deutsch\",D3196,IF($B$1=\"中文\",E3196,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 与三乙胺的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3197,IF($B$1=\"Deutsch\",D3197,IF($B$1=\"中文\",E3197,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-isopropylidenediphenol (Bisphenol A)"},"4,4'-isopropylidenediphenol (Bisphenol A)","4,4'-isopropylidendiphenol\n(Bisphenol A)","2,2-双对羟苯基丙烷 (双酚A)"]
[null,{"$f":"IF($B$1=\"English\",C3198,IF($B$1=\"Deutsch\",D3198,IF($B$1=\"中文\",E3198,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction products of 1,3,4-thiadiazolidine-2,5-dithione,\nformaldehyde and 4-heptylphenol, branched and linear (RP-HP)\n[with ≥0.1% w/w 4-heptylphenol, branched and linear (4-HPbl)1]"},"Reaction products of 1,3,4-thiadiazolidine-2,5-dithione,\nformaldehyde and 4-heptylphenol, branched and linear (RP-HP)\n[with ≥0.1% w/w 4-heptylphenol, branched and linear (4-HPbl)1]","Reaktionsprodukt aus 1,3,4-Thiadiazolidin-2,5-dithion, Formaldehyd und 4-Heptylphenol, verzweigt und linear (RP-HP) \nmit ≥ 0,1% w/w 4-Heptylphenol, verzweigt und linear (4-HPbl)","1,3,4-噻二唑-2,5-二硫酮, 甲醛和4-庚基苯酚, 支链和直链 (RP-HP)的反应产物\n[含≥0.1% 重量百分比的 4-庚基苯酚, 支链和直链 (4-HPbl)1]"]
[null,{"$f":"IF($B$1=\"English\",C3199,IF($B$1=\"Deutsch\",D3199,IF($B$1=\"中文\",E3199,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs."},"Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs.","Reaction product of 1,3,4-thiadiazolidine-2,5-dithione, formaldehyde and phenol, heptyl derivs.","1,3,4-噻二唑-2,5-二硫酮, 甲醛和庚基苯酚衍生物的反应产物"]
[null,{"$f":"IF($B$1=\"English\",C3200,IF($B$1=\"Deutsch\",D3200,IF($B$1=\"中文\",E3200,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine"},"Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine","Formaldehyde, reaction products with branched and linear heptylphenol, carbon disulfide and hydrazine","甲醛与支链和直链庚基苯酚、二硫化碳和联氨的反应产物"]
[null,{"$f":"IF($B$1=\"English\",C3201,IF($B$1=\"Deutsch\",D3201,IF($B$1=\"中文\",E3201,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium carbonate"},"Cadmium carbonate","Cadmiumcarbonat","碳酸镉"]
[null,{"$f":"IF($B$1=\"English\",C3202,IF($B$1=\"Deutsch\",D3202,IF($B$1=\"中文\",E3202,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium hydroxide, Cd(OH)2\n"},"Cadmium hydroxide, Cd(OH)2\n","Cadmiumhydroxid","氢氧化镉，Cd(OH)2\n"]
[null,{"$f":"IF($B$1=\"English\",C3203,IF($B$1=\"Deutsch\",D3203,IF($B$1=\"中文\",E3203,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium nitrate"},"Cadmium nitrate","Cadmiumnitrat","硝酸镉"]
[null,{"$f":"IF($B$1=\"English\",C3204,IF($B$1=\"Deutsch\",D3204,IF($B$1=\"中文\",E3204,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benz[a]anthracene"},"Benz[a]anthracene","Benz[a]anthracen","苯并(a)蒽"]
[null,{"$f":"IF($B$1=\"English\",C3205,IF($B$1=\"Deutsch\",D3205,IF($B$1=\"中文\",E3205,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chrysene"},"Chrysene","Chrysen","稠二萘"]
[null,{"$f":"IF($B$1=\"English\",C3206,IF($B$1=\"Deutsch\",D3206,IF($B$1=\"中文\",E3206,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,6,7,8,9,14,15,16,17,17,18,18-\nDodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane\nPlus”TM) [covering any of its individual anti- and syn-isomers or any combination\nthereof]"},"1,6,7,8,9,14,15,16,17,17,18,18-\nDodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene (“Dechlorane\nPlus”TM) [covering any of its individual anti- and syn-isomers or any combination\nthereof]","1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-dien (“Dechloran Plus”TM) \n[deckt alle individuellen anti- und syn-Isomere oder Kombinationen daraus ab]","1,6,7,8,9,14,15,16,17,17,18,18-十二氯代五环[12.2.1.16,9.02,13.05,10]十八-7,15-二烯 (“得克隆”TM) [包括其所有反式异构体和同分异构体及其任意组合]"]
[null,{"$f":"IF($B$1=\"English\",C3207,IF($B$1=\"Deutsch\",D3207,IF($B$1=\"中文\",E3207,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene"},"(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5R,6R,9S,10S,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-十二氯代五环[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]十八-7,15-二烯"]
[null,{"$f":"IF($B$1=\"English\",C3208,IF($B$1=\"Deutsch\",D3208,IF($B$1=\"中文\",E3208,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene"},"1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene","1,6,7,8,9,14,15,16,17,17,18,18-dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene","1,6,7,8,9,14,15,16,17,17,18,18-十二氯代五环[12.2.1.16,9.02,13.05,10]十八-7,15-二烯"]
[null,{"$f":"IF($B$1=\"English\",C3209,IF($B$1=\"Deutsch\",D3209,IF($B$1=\"中文\",E3209,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene"},"(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]octadeca-7,15-diene","(1S,2S,5S,6S,9R,10R,13R,14R)-1,6,7,8,9,14,15,16,17,17,18,18-十二氯代五环[12.2.1.1⁶,⁹.0²,¹³.0⁵,¹⁰]十八-7,15-二烯"]
[null,{"$f":"IF($B$1=\"English\",C3210,IF($B$1=\"Deutsch\",D3210,IF($B$1=\"中文\",E3210,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene"},"rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","rel-(1R,4S,4aS,6aR,7R,10S,10aS,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-十二氯-1,4,4a,5,6,6a,7,10,10a,11,12,12a-十二氢-1,4:7,10-二亚甲基二苯唑[a,e]环辛烯"]
[null,{"$f":"IF($B$1=\"English\",C3211,IF($B$1=\"Deutsch\",D3211,IF($B$1=\"中文\",E3211,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene"},"rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-1,4:7,10-dimethanodibenzo[a,e]cyclooctene","rel-(1R,4S,4aS,6aS,7S,10R,10aR,12aR)-1,2,3,4,7,8,9,10,13,13,14,14-十二氯-1,4,4a,5,6,6a,7,10,10a,11,12,12a-十二氢-1,4:7,10-二亚甲基二苯唑[a,e]环辛烯"]
[null,{"$f":"IF($B$1=\"English\",C3212,IF($B$1=\"Deutsch\",D3212,IF($B$1=\"中文\",E3212,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)"},"Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)","Benzene-1,2,4-tricarboxylic acid 1,2 anhydride (trimellitic anhydride) (TMA)","苯-1,2,4-三甲酸 1,2 酸酐 (偏苯三酸酐) (TMA)"]
[null,{"$f":"IF($B$1=\"English\",C3213,IF($B$1=\"Deutsch\",D3213,IF($B$1=\"中文\",E3213,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dicyclohexyl phthalate (DCHP)"},"Dicyclohexyl phthalate (DCHP)","Dicyclohexylphthalat (DCHP)","邻苯二甲酸二环己酯(DCHP)"]
[null,{"$f":"IF($B$1=\"English\",C3214,IF($B$1=\"Deutsch\",D3214,IF($B$1=\"中文\",E3214,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octamethylcyclotetrasiloxane (D4)"},"Octamethylcyclotetrasiloxane (D4)","Oktamethylcyclotetrasiloxan (D4)","八甲基环四硅氧烷 (D4)"]
[null,{"$f":"IF($B$1=\"English\",C3215,IF($B$1=\"Deutsch\",D3215,IF($B$1=\"中文\",E3215,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decamethylcyclopentasiloxane (D5)"},"Decamethylcyclopentasiloxane (D5)","Dekamethylcyclopentasiloxan (D5)"," 十甲基环五硅氧烷(D5)"]
[null,{"$f":"IF($B$1=\"English\",C3216,IF($B$1=\"Deutsch\",D3216,IF($B$1=\"中文\",E3216,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dodecamethylcyclohexasiloxane (D6)"},"Dodecamethylcyclohexasiloxane (D6)","Dodekamethylcyclohexasiloxan (D6)"," 十二甲基环六硅氧烷(D6)"]
[null,{"$f":"IF($B$1=\"English\",C3217,IF($B$1=\"Deutsch\",D3217,IF($B$1=\"中文\",E3217,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Blei","铅"]
[null,{"$f":"IF($B$1=\"English\",C3218,IF($B$1=\"Deutsch\",D3218,IF($B$1=\"中文\",E3218,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Disodium octaborate"},"Disodium octaborate","Dinatriumoctaborat","氧化硼钠"]
[null,{"$f":"IF($B$1=\"English\",C3219,IF($B$1=\"Deutsch\",D3219,IF($B$1=\"中文\",E3219,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[ghi]perylene"},"Benzo[ghi]perylene","Benzo[ghi]perylen","苯并(G,H,I)苝"]
[null,{"$f":"IF($B$1=\"English\",C3220,IF($B$1=\"Deutsch\",D3220,IF($B$1=\"中文\",E3220,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Terphenyl hydrogenated"},"Terphenyl hydrogenated","Terphenyl, hydriert","氢化三联苯"]
[null,{"$f":"IF($B$1=\"English\",C3221,IF($B$1=\"Deutsch\",D3221,IF($B$1=\"中文\",E3221,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethylenediamine (EDA)"},"Ethylenediamine (EDA)","Ethylendiamin (EDA)","乙二胺(EDA)"]
[null,{"$f":"IF($B$1=\"English\",C3222,IF($B$1=\"Deutsch\",D3222,IF($B$1=\"中文\",E3222,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-bis(4'-hydroxyphenyl)-4-methylpentane"},"2,2-bis(4'-hydroxyphenyl)-4-methylpentane","2,2-Bis(4'-hydroxyphenyl)-4-methylpentan","4,4'-(1,3-二甲基丁基)二苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3223,IF($B$1=\"Deutsch\",D3223,IF($B$1=\"中文\",E3223,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[k]fluoranthene"},"Benzo[k]fluoranthene","Benzo[k]fluoranthen","苯并[k]荧蒽"]
[null,{"$f":"IF($B$1=\"English\",C3224,IF($B$1=\"Deutsch\",D3224,IF($B$1=\"中文\",E3224,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fluoranthene"},"Fluoranthene","Fluoranthene","荧蒽"]
[null,{"$f":"IF($B$1=\"English\",C3225,IF($B$1=\"Deutsch\",D3225,IF($B$1=\"中文\",E3225,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenanthrene"},"Phenanthrene","Phenanthrene","菲"]
[null,{"$f":"IF($B$1=\"English\",C3226,IF($B$1=\"Deutsch\",D3226,IF($B$1=\"中文\",E3226,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pyrene"},"Pyrene","Pyrene","芘"]
[null,{"$f":"IF($B$1=\"English\",C3227,IF($B$1=\"Deutsch\",D3227,IF($B$1=\"中文\",E3227,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,7,7-trimethyl-3-(phenylmethylene)bicyclo[2.2.1]heptan-2-one "},"1,7,7-trimethyl-3-(phenylmethylene)bicyclo[2.2.1]heptan-2-one ","1,7,7-Trimethyl-3-(phenylmethylen)bicyclo[2.2.1]heptan-2-on ","3-亚苄基樟脑 "]
[null,{"$f":"IF($B$1=\"English\",C3228,IF($B$1=\"Deutsch\",D3228,IF($B$1=\"中文\",E3228,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methoxyethyl acetate"},"2-Methoxyethyl acetate","2-methoxyethyl acetate","乙二醇甲醚乙酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3229,IF($B$1=\"Deutsch\",D3229,IF($B$1=\"中文\",E3229,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)"},"Tris(4-nonylphenyl, branched and linear) phosphite (TNPP) with ≥ 0.1% w/w of 4-nonylphenol, branched and linear (4-NP)","Tris(4-Nonylphenyl, verzweigt und linear) phosphit (TNPP) mit >= 0,1% Gew./Gew. 4-Nonylphenol, verzweigt und linear (4-NP)","三(4-壬苯基, 支链和直链) 亚磷酸盐 (TNPP) ，含≥ 0.1%重量百分比的4-壬基酚，支链和直链 (4-NP)"]
[null,{"$f":"IF($B$1=\"English\",C3230,IF($B$1=\"Deutsch\",D3230,IF($B$1=\"中文\",E3230,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tris(nonylphenyl) phosphite"},"Tris(nonylphenyl) phosphite","Tris(nonylphenyl) phosphite","三(壬基酚)亚磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3231,IF($B$1=\"Deutsch\",D3231,IF($B$1=\"中文\",E3231,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"tris(4-nonylphenyl, branched) phosphite"},"tris(4-nonylphenyl, branched) phosphite","tris(4-nonylphenyl, branched) phosphite","三(-壬苯基支链)亚磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3232,IF($B$1=\"Deutsch\",D3232,IF($B$1=\"中文\",E3232,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-nonyl-, phosphite (3:1)"},"Phenol, 4-nonyl-, phosphite (3:1)","Phenol, 4-nonyl-, phosphite (3:1)","4-壬基-亚磷酸苯酚 (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3233,IF($B$1=\"Deutsch\",D3233,IF($B$1=\"中文\",E3233,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, p-isononyl-, phosphite (3:1)"},"Phenol, p-isononyl-, phosphite (3:1)","Phenol, p-isononyl-, phosphite (3:1)","p-异壬基-亚磷酸苯酚 (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3234,IF($B$1=\"Deutsch\",D3234,IF($B$1=\"中文\",E3234,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, p-sec-nonyl-, phosphite"},"Phenol, p-sec-nonyl-, phosphite","Phenol, p-sec-nonyl-, phosphite","p-仲壬基-亚磷酸苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3235,IF($B$1=\"Deutsch\",D3235,IF($B$1=\"中文\",E3235,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides (covering any of their individual isomers and combinations thereof)"},"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid, its salts and its acyl halides (covering any of their individual isomers and combinations thereof)","2,3,3,3-Tetrafluor-2-(heptafluorpropoxy)propionsäure, ihre Salze und ihre Acylhalide \n[die eines ihrer einzelnen Isomere und Kombinationen davon abdecken]","2,3,3,3-四氟-2-(七氟丙氧基)丙酸，及其盐和酰基卤化物（包括其所有异构体及其组合）"]
[null,{"$f":"IF($B$1=\"English\",C3236,IF($B$1=\"Deutsch\",D3236,IF($B$1=\"中文\",E3236,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride"},"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionyl fluoride","2,3,3,3-四氟-2-(七氟丙氧基)丙酰氟"]
[null,{"$f":"IF($B$1=\"English\",C3237,IF($B$1=\"Deutsch\",D3237,IF($B$1=\"中文\",E3237,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid"},"2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid","2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionic acid","2,3,3,3-四氟-2-(七氟丙氧基)丙酸"]
[null,{"$f":"IF($B$1=\"English\",C3238,IF($B$1=\"Deutsch\",D3238,IF($B$1=\"中文\",E3238,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate"},"Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate","Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propionate","2,3,3,3-四氟-2-(七氟丙氧基)丙酸钾"]
[null,{"$f":"IF($B$1=\"English\",C3239,IF($B$1=\"Deutsch\",D3239,IF($B$1=\"中文\",E3239,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate"},"Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","Ammonium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","2,3,3,3-四氟-2-(七氟丙氧基)丙酸胺"]
[null,{"$f":"IF($B$1=\"English\",C3240,IF($B$1=\"Deutsch\",D3240,IF($B$1=\"中文\",E3240,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-"},"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-","Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (+)-","丙酸，2,3,3,3-四氟-2-(七氟丙氧基)-, (+)-"]
[null,{"$f":"IF($B$1=\"English\",C3241,IF($B$1=\"Deutsch\",D3241,IF($B$1=\"中文\",E3241,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-"},"Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-","Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, (-)-","丙酸， 2,3,3,3-四氟-2-(七氟丙氧基)-, (-)-"]
[null,{"$f":"IF($B$1=\"English\",C3242,IF($B$1=\"Deutsch\",D3242,IF($B$1=\"中文\",E3242,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-tert-butylphenol"},"4-tert-butylphenol","4-tert-Butylphenol","4-叔丁基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3243,IF($B$1=\"Deutsch\",D3243,IF($B$1=\"中文\",E3243,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisohexyl phthalat"},"Diisohexyl phthalat","Diisohexyl phthalate","邻苯二甲酸双-4-甲基-2-戊酯"]
[null,{"$f":"IF($B$1=\"English\",C3244,IF($B$1=\"Deutsch\",D3244,IF($B$1=\"中文\",E3244,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon"},"2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon","2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone","2-苄基-2-二甲基氨基-1-(4-吗啉苯基)丁酮"]
[null,{"$f":"IF($B$1=\"English\",C3245,IF($B$1=\"Deutsch\",D3245,IF($B$1=\"中文\",E3245,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorobutane sulfonic acid (PFBS) and its salts "},"Perfluorobutane sulfonic acid (PFBS) and its salts ","Perfluorbutansulfonsäure (PFBS) und seine Salze","全氟丁磺酸（PFBS）及其盐 "]
[null,{"$f":"IF($B$1=\"English\",C3246,IF($B$1=\"Deutsch\",D3246,IF($B$1=\"中文\",E3246,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate"},"Potassium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate","Potassium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate","1,1,2,2,3,3,4,4,4-全氟丁基-1-磺酸钾"]
[null,{"$f":"IF($B$1=\"English\",C3247,IF($B$1=\"Deutsch\",D3247,IF($B$1=\"中文\",E3247,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonic acid"},"1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonic acid","1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonic acid","1,1,2,2,3,3,4,4,4-全氟丁基-1-磺酸"]
[null,{"$f":"IF($B$1=\"English\",C3248,IF($B$1=\"Deutsch\",D3248,IF($B$1=\"中文\",E3248,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"bis(4-t-butylphenyl)iodonium perfluorobutanesulfonate"},"bis(4-t-butylphenyl)iodonium perfluorobutanesulfonate","bis(4-t-butylphenyl)iodonium perfluorobutanesulfonate","双(4-叔丁基苯基)碘鎓全氟-1-丁磺酸"]
[null,{"$f":"IF($B$1=\"English\",C3249,IF($B$1=\"Deutsch\",D3249,IF($B$1=\"中文\",E3249,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"tetrabutyl-phosphonium nonafluoro-butane-1-sulfonate"},"tetrabutyl-phosphonium nonafluoro-butane-1-sulfonate","tetrabutyl-phosphonium nonafluoro-butane-1-sulfonate","全氟丁基磺酸四丁基磷"]
[null,{"$f":"IF($B$1=\"English\",C3250,IF($B$1=\"Deutsch\",D3250,IF($B$1=\"中文\",E3250,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"dimethyl(phenyl)sulfanium perfluorobutanesulfonate"},"dimethyl(phenyl)sulfanium perfluorobutanesulfonate","dimethyl(phenyl)sulfanium perfluorobutanesulfonate","二甲基(苯基)全氟丁磺酸锍"]
[null,{"$f":"IF($B$1=\"English\",C3251,IF($B$1=\"Deutsch\",D3251,IF($B$1=\"中文\",E3251,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate"},"Ammonium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate","Ammonium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonate","全氟丁基磺酸铵"]
[null,{"$f":"IF($B$1=\"English\",C3252,IF($B$1=\"Deutsch\",D3252,IF($B$1=\"中文\",E3252,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Triphenylsulfanium perfluorobutane sulfonate"},"Triphenylsulfanium perfluorobutane sulfonate","Triphenylsulfanium perfluorobutane sulfonate","三苯基全氟丁磺酸锍"]
[null,{"$f":"IF($B$1=\"English\",C3253,IF($B$1=\"Deutsch\",D3253,IF($B$1=\"中文\",E3253,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N,N-triethylethanaminium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate"},"N,N,N-triethylethanaminium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","N,N,N-triethylethanaminium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","N,N,N-三乙基乙铵 1,1,2,2,3,3,4,4,4-全氟丁基-1-磺酸盐"]
[null,{"$f":"IF($B$1=\"English\",C3254,IF($B$1=\"Deutsch\",D3254,IF($B$1=\"中文\",E3254,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"magnesium perfluorobutanesulfonate"},"magnesium perfluorobutanesulfonate","magnesium perfluorobutanesulfonate","全氟丁基磺酸镁"]
[null,{"$f":"IF($B$1=\"English\",C3255,IF($B$1=\"Deutsch\",D3255,IF($B$1=\"中文\",E3255,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"lithium perfluorobutanesulfonate"},"lithium perfluorobutanesulfonate","lithium perfluorobutanesulfonate","全氟丁基磺酸锂"]
[null,{"$f":"IF($B$1=\"English\",C3256,IF($B$1=\"Deutsch\",D3256,IF($B$1=\"中文\",E3256,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"morpholinium perfluorobutanesulfonate"},"morpholinium perfluorobutanesulfonate","morpholinium perfluorobutanesulfonate","全氟丁基磺酸吗啉"]
[null,{"$f":"IF($B$1=\"English\",C3257,IF($B$1=\"Deutsch\",D3257,IF($B$1=\"中文\",E3257,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-(4-butoxy-1-naphthalenyl)tetrahydrothiophenium 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate"},"1-(4-butoxy-1-naphthalenyl)tetrahydrothiophenium 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate","1-(4-butoxy-1-naphthalenyl)tetrahydrothiophenium 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate","1-(4-丁氧基-1-萘基)四氢噻吩嗡 1,1,2,2,3,3,4,4,4-全氟-1-丁磺酸盐"]
[null,{"$f":"IF($B$1=\"English\",C3258,IF($B$1=\"Deutsch\",D3258,IF($B$1=\"中文\",E3258,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-one"},"2-methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-one","2-Methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-on","2-甲基-1-(4-甲硫基苯)-2-吗啉基-1-丙酮"]
[null,{"$f":"IF($B$1=\"English\",C3259,IF($B$1=\"Deutsch\",D3259,IF($B$1=\"中文\",E3259,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-vinylimidazole"},"1-vinylimidazole","1-vinylimidazole","1-乙烯基咪唑"]
[null,{"$f":"IF($B$1=\"English\",C3260,IF($B$1=\"Deutsch\",D3260,IF($B$1=\"中文\",E3260,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-methylimidazole"},"2-methylimidazole","2-methylimidazole","2-甲基咪唑"]
[null,{"$f":"IF($B$1=\"English\",C3261,IF($B$1=\"Deutsch\",D3261,IF($B$1=\"中文\",E3261,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butyl 4-hydroxybenzoate"},"Butyl 4-hydroxybenzoate","Butyl 4-hydroxybenzoate","对羟基苯甲酸苯甲酯"]
[null,{"$f":"IF($B$1=\"English\",C3262,IF($B$1=\"Deutsch\",D3262,IF($B$1=\"中文\",E3262,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibutylbis(pentane-2,4-dionato-O,O')tin"},"Dibutylbis(pentane-2,4-dionato-O,O')tin","Dibutylbis(pentane-2,4-dionato-O,O')tin","二丁基双(2,4-戊二酸根合-O,O')锡"]
[null,{"$f":"IF($B$1=\"English\",C3263,IF($B$1=\"Deutsch\",D3263,IF($B$1=\"中文\",E3263,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-(2-methoxyethoxy)ethyl) ether"},"Bis(2-(2-methoxyethoxy)ethyl) ether","Bis(2-(2-methoxyethoxy)ethyl)ether ","双(2-(2-甲氧基乙氧基)乙基)酯"]
[null,{"$f":"IF($B$1=\"English\",C3264,IF($B$1=\"Deutsch\",D3264,IF($B$1=\"中文\",E3264,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety"},"Dioctyltin dilaurate, stannane, dioctyl-, bis(coco acyloxy) derivs., and any other stannane, dioctyl-, bis(fatty acyloxy) derivs. wherein C12 is the predominant carbon number of the fatty acyloxy moiety","Dioctylzinndilaurat, Stannan-, Dioctylbis(coco-acyloxy)derivate und alle anderen Stannan-, Dioctylbis(fettacyloxy)derivate, wobei C12 die vorherrschende Kohlenstoffzahl der Fettacyloxyeinheit ist","二月桂酸二正辛基锡，锡烷，二辛基-双（可可酰氧基）衍生物及其他锡烷；二辛基-双（脂肪酰氧基）衍生物，其中C12是脂肪酰氧基部分的主要碳原子数"]
[null,{"$f":"IF($B$1=\"English\",C3265,IF($B$1=\"Deutsch\",D3265,IF($B$1=\"中文\",E3265,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dioctyltin dilaurate"},"Dioctyltin dilaurate","Dioctylzinndilaurat","二月桂酸二正辛基锡"]
[null,{"$f":"IF($B$1=\"English\",C3266,IF($B$1=\"Deutsch\",D3266,IF($B$1=\"中文\",E3266,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"dioctyltin dilaurate; stannane, dioctyl-, bis(coco acyloxy) derivs."},"dioctyltin dilaurate; stannane, dioctyl-, bis(coco acyloxy) derivs.","Stannan, Dioctylbis(coco-acyloxy)derivate und","二月桂酸二正辛基锡，锡烷，二辛基-双（可可酰氧基）衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3267,IF($B$1=\"Deutsch\",D3267,IF($B$1=\"中文\",E3267,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Stannane, dioctyl-, bis(coco acyloxy) derivs."},"Stannane, dioctyl-, bis(coco acyloxy) derivs.","alle anderen Stannan-, Dioctylbis(fettacyloxy)derivate, wobei C12 die vorherrschende Kohlenstoffzahl der Fettacyloxyeinheit","锡烷，二辛基-双（可可酰氧基）衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3268,IF($B$1=\"Deutsch\",D3268,IF($B$1=\"中文\",E3268,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)"},"Phenol, alkylation products (mainly in para position) with C12-rich branched alkyl chains from oligomerisation, covering any individual isomers and/ or combinations thereof (PDDP)","Phenol, Alkylierungsprodukte (hauptsächlich in para-Position) mit C12-reichen verzweigten Alkylketten aus der Oligomerisierung, die alle einzelnen Isomere und/oder Kombinationen davon umfasst (PDDP)","苯酚，与富含C12支链的甲基链进行烷基化反应（主要为对位）生产的产物，包含各异构体和/或其组合（PDDP）"]
[null,{"$f":"IF($B$1=\"English\",C3269,IF($B$1=\"Deutsch\",D3269,IF($B$1=\"中文\",E3269,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, dodecyl-, branched"},"Phenol, dodecyl-, branched","Phenol, dodecyl-, branched","支链十二烷基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3270,IF($B$1=\"Deutsch\",D3270,IF($B$1=\"中文\",E3270,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, (tetrapropenyl) derivatives"},"Phenol, (tetrapropenyl) derivatives","Phenol, (tetrapropenyl) derivatives","（四丙烯基）苯酚衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3271,IF($B$1=\"Deutsch\",D3271,IF($B$1=\"中文\",E3271,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-dodecyl, branched"},"Phenol, 4-dodecyl, branched","Phenol, 4-dodecyl, branched","支链4-十二烷基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3272,IF($B$1=\"Deutsch\",D3272,IF($B$1=\"中文\",E3272,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-isododecylphenol"},"4-isododecylphenol","4-isododecylphenol","4-十二烷基苯酚异构体"]
[null,{"$f":"IF($B$1=\"English\",C3273,IF($B$1=\"Deutsch\",D3273,IF($B$1=\"中文\",E3273,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, tetrapropylene-"},"Phenol, tetrapropylene-","Phenol, tetrapropylene-","四烯丙基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3274,IF($B$1=\"Deutsch\",D3274,IF($B$1=\"中文\",E3274,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, 4-isododecyl-"},"Phenol, 4-isododecyl-","Phenol, 4-isododecyl-","4-十二烷基苯酚异构体"]
[null,{"$f":"IF($B$1=\"English\",C3275,IF($B$1=\"Deutsch\",D3275,IF($B$1=\"中文\",E3275,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"orthoboric acid, sodium salt"},"orthoboric acid, sodium salt","Orthoborsäure, Natriumsalz ","正硼酸钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3276,IF($B$1=\"Deutsch\",D3276,IF($B$1=\"中文\",E3276,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"boric acid (H3BO3), sodium salt, hydrate"},"boric acid (H3BO3), sodium salt, hydrate","boric acid (H3BO3), sodium salt, hydrate","硼酸（H3BO3）钠盐水合物"]
[null,{"$f":"IF($B$1=\"English\",C3277,IF($B$1=\"Deutsch\",D3277,IF($B$1=\"中文\",E3277,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid (H3BO3), disodium salt"},"Boric acid (H3BO3), disodium salt","Boric acid (H3BO3), disodium salt","硼酸（H3BO3）二钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3278,IF($B$1=\"Deutsch\",D3278,IF($B$1=\"中文\",E3278,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Trisodium orthoborate"},"Trisodium orthoborate","Trisodium orthoborate","正硼酸三钠"]
[null,{"$f":"IF($B$1=\"English\",C3279,IF($B$1=\"Deutsch\",D3279,IF($B$1=\"中文\",E3279,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid, sodium salt"},"Boric acid, sodium salt","Boric acid, sodium salt","硼酸钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3280,IF($B$1=\"Deutsch\",D3280,IF($B$1=\"中文\",E3280,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Orthoboric acid, sodium salt"},"Orthoboric acid, sodium salt","Orthoboric acid, sodium salt","正硼酸钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3281,IF($B$1=\"Deutsch\",D3281,IF($B$1=\"中文\",E3281,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boric acid (H3BO3), sodium salt (1:1) "},"Boric acid (H3BO3), sodium salt (1:1) ","Boric acid (H3BO3), sodium salt (1:1) ","硼酸（H3BO3）钠盐(1:1) "]
[null,{"$f":"IF($B$1=\"English\",C3282,IF($B$1=\"Deutsch\",D3282,IF($B$1=\"中文\",E3282,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Medium-chain chlorinated paraffins (MCCP)"},"Medium-chain chlorinated paraffins (MCCP)","Mittelkettige Chlorparaffine (MCCP) (UVCB-Stoffe bestehend aus mehr als oder gleich 80 % linearen Chloralkanen mit Kohlenstoffkettenlängen im Bereich von C14 bis C17)","中链氯化石蜡"]
[null,{"$f":"IF($B$1=\"English\",C3283,IF($B$1=\"Deutsch\",D3283,IF($B$1=\"中文\",E3283,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C14-16, chloro"},"Alkanes, C14-16, chloro","Alkanes, C14-16, chloro","烷烃，C14-16，氯"]
[null,{"$f":"IF($B$1=\"English\",C3284,IF($B$1=\"Deutsch\",D3284,IF($B$1=\"中文\",E3284,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C14-17, chloro"},"Alkanes, C14-17, chloro","Alkanes, C14-17, chloro","烷烃，C14-17，氯"]
[null,{"$f":"IF($B$1=\"English\",C3285,IF($B$1=\"Deutsch\",D3285,IF($B$1=\"中文\",E3285,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"di-, tri- and tetrachlorotetradecane "},"di-, tri- and tetrachlorotetradecane ","di-, tri- and tetrachlorotetradecane ","二、三、四-氯代十四烷 "]
[null,{"$f":"IF($B$1=\"English\",C3286,IF($B$1=\"Deutsch\",D3286,IF($B$1=\"中文\",E3286,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetradecane, chloro derivs."},"Tetradecane, chloro derivs.","Tetradecane, chloro derivs.","十四烷氯代衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3287,IF($B$1=\"Deutsch\",D3287,IF($B$1=\"中文\",E3287,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"glutaral"},"glutaral","Glutaral","戊二醛"]
[null,{"$f":"IF($B$1=\"English\",C3288,IF($B$1=\"Deutsch\",D3288,IF($B$1=\"中文\",E3288,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-(1-methylpropylidene)bisphenol"},"4,4'-(1-methylpropylidene)bisphenol","4,4'-(1-Methylpropyliden)bisphenol","2,2-二(4-羟基苯基)丁烷"]
[null,{"$f":"IF($B$1=\"English\",C3289,IF($B$1=\"Deutsch\",D3289,IF($B$1=\"中文\",E3289,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers"},"2-(4-tert-butylbenzyl)propionaldehyde and its individual stereoisomers","2-(4-tert-Butylbenzyl)propionaldehyd und seine einzelnen Stereoisomere","铃兰醛及其立体异构体"]
[null,{"$f":"IF($B$1=\"English\",C3290,IF($B$1=\"Deutsch\",D3290,IF($B$1=\"中文\",E3290,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2R)-3-(4-tert-butylphenyl)-2-methylpropanal "},"(2R)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2R)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2R)-3-(4-叔丁基苯基)-2-甲基丙醛 "]
[null,{"$f":"IF($B$1=\"English\",C3291,IF($B$1=\"Deutsch\",D3291,IF($B$1=\"中文\",E3291,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(4-tert-butylbenzyl)propionaldehyde"},"2-(4-tert-butylbenzyl)propionaldehyde","2-(4-tert-butylbenzyl)propionaldehyde","铃兰醛"]
[null,{"$f":"IF($B$1=\"English\",C3292,IF($B$1=\"Deutsch\",D3292,IF($B$1=\"中文\",E3292,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2S)-3-(4-tert-butylphenyl)-2-methylpropanal "},"(2S)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2S)-3-(4-tert-butylphenyl)-2-methylpropanal ","(2S)-3-(4-叔丁基苯基)-2-甲基丙醛 "]
[null,{"$f":"IF($B$1=\"English\",C3293,IF($B$1=\"Deutsch\",D3293,IF($B$1=\"中文\",E3293,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)"},"2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)","2,2-bis(bromomethyl)propane-1,3-diol (BMP); 2,2-dimethylpropan-1-ol, tribromo derivative/3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA); 2,3-dibromo-1-propanol (2,3-DBPA)","2,2-双(溴甲基)-1,3-丙二醇(BMP); 2,2-二甲基-1-丙醇, 三溴衍生物/3-溴-2,2-双(溴甲基)-1-丙醇 (TBNPA); 2,3-二溴-1-丙醇(2,3-DBPA)"]
[null,{"$f":"IF($B$1=\"English\",C3294,IF($B$1=\"Deutsch\",D3294,IF($B$1=\"中文\",E3294,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) "},"2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) ","2,2-dimethylpropan-1-ol, tribromo derivative (TBNPA) ","2,2-二甲基-1-丙醇, 三溴衍生物 (TBNPA) "]
[null,{"$f":"IF($B$1=\"English\",C3295,IF($B$1=\"Deutsch\",D3295,IF($B$1=\"中文\",E3295,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)"},"3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)","3-bromo-2,2-bis(bromomethyl)-1-propanol (TBNPA)","3-溴-2,2-双(溴甲基)-1-丙醇(TBNPA)"]
[null,{"$f":"IF($B$1=\"English\",C3296,IF($B$1=\"Deutsch\",D3296,IF($B$1=\"中文\",E3296,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2-bis(bromomethyl)propane-1,3-diol (BMP)"},"2,2-bis(bromomethyl)propane-1,3-diol (BMP)","2,2-bis(bromomethyl)propane-1,3-diol (BMP)","2,2-双(溴甲基)丙烷-1,3-diol (BMP)"]
[null,{"$f":"IF($B$1=\"English\",C3297,IF($B$1=\"Deutsch\",D3297,IF($B$1=\"中文\",E3297,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3-dibromo-1-propanol (2,3-DBPA) "},"2,3-dibromo-1-propanol (2,3-DBPA) ","2,3-dibromo-1-propanol (2,3-DBPA) ","2,3-二溴-1-丙醇 (2,3-DBPA) "]
[null,{"$f":"IF($B$1=\"English\",C3298,IF($B$1=\"Deutsch\",D3298,IF($B$1=\"中文\",E3298,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,4-dioxane"},"1,4-dioxane","1,4-Dioxan","1,4-二氧六环"]
[null,{"$f":"IF($B$1=\"English\",C3299,IF($B$1=\"Deutsch\",D3299,IF($B$1=\"中文\",E3299,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"tris(2-methoxyethoxy)vinylsilane"},"tris(2-methoxyethoxy)vinylsilane","tris(2-methoxyethoxy)vinylsilane","三(2-甲氧基乙氧基)乙烯基硅烷"]
[null,{"$f":"IF($B$1=\"English\",C3300,IF($B$1=\"Deutsch\",D3300,IF($B$1=\"中文\",E3300,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261"},"S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261","S-(tricyclo(5.2.1.0'2,6)deca-3-en-8(or 9)-yl O-(isopropyl or isobutyl or 2-ethylhexyl) O-(isopropyl or isobutyl or 2-ethylhexyl) phosphorodithioate\nX4261","S-(三环(5.2.1.0'2,6)十-3-烯-8(或 9)-基O-(异丙基或异丁基或 2-乙基己基) O-(异丙基或异丁基或 2-乙基己基) 磷酸二乙酯\nX4261"]
[null,{"$f":"IF($B$1=\"English\",C3301,IF($B$1=\"Deutsch\",D3301,IF($B$1=\"中文\",E3301,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol"},"6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol","6,6'-di-tert-butyl-2,2'-methylenedi-p-cresol","6,6'-二叔丁基-2,2'-亚甲基二-p-甲酚"]
[null,{"$f":"IF($B$1=\"English\",C3302,IF($B$1=\"Deutsch\",D3302,IF($B$1=\"中文\",E3302,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)"},"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one covering any of the individual isomers and/or combinations thereof (4-MBC)","(±)-1,7,7-三甲基-3-[(4-甲基苯基)亚甲基]二环[2.2.1]庚-2-酮，包括各异构体和/或其组合 (4-MBC)"]
[null,{"$f":"IF($B$1=\"English\",C3303,IF($B$1=\"Deutsch\",D3303,IF($B$1=\"中文\",E3303,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(3E)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(3E)-1,7,7-三甲基-3-(4-亚苯基亚甲基)二环[2.2.1]庚-2-酮 "]
[null,{"$f":"IF($B$1=\"English\",C3304,IF($B$1=\"Deutsch\",D3304,IF($B$1=\"中文\",E3304,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3E,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3E,4S)-1,7,7-三甲基-3-(4- 亚苯基亚甲基)二环[2.2.1]庚-2-酮 "]
[null,{"$f":"IF($B$1=\"English\",C3305,IF($B$1=\"Deutsch\",D3305,IF($B$1=\"中文\",E3305,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3Z,4R)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3Z,4R)-1,7,7-三甲基-3-(4-亚苯基亚甲基)二环[2.2.1]庚-2-酮 "]
[null,{"$f":"IF($B$1=\"English\",C3306,IF($B$1=\"Deutsch\",D3306,IF($B$1=\"中文\",E3306,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one"},"(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one","(±)-1,7,7-trimethyl-3-[(4-methylphenyl)methylene]bicyclo[2.2.1]heptan-2-one","(±)-1,7,7-三甲基-3-[(4-甲苯基)亚甲基]二环[2.2.1]庚-2-酮"]
[null,{"$f":"IF($B$1=\"English\",C3307,IF($B$1=\"Deutsch\",D3307,IF($B$1=\"中文\",E3307,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,4S)-1,7,7-trimethyl-3-(4-methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,4S)-1,7,7-三甲基-3-(4-亚苯基亚甲基)二环[2.2.1]庚-2-酮 "]
[null,{"$f":"IF($B$1=\"English\",C3308,IF($B$1=\"Deutsch\",D3308,IF($B$1=\"中文\",E3308,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3E,4R)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1S,3E,4R)-1,7,7-三甲基-3-(4-亚苯基亚甲基)二环[2.2.1]庚-2-酮 "]
[null,{"$f":"IF($B$1=\"English\",C3309,IF($B$1=\"Deutsch\",D3309,IF($B$1=\"中文\",E3309,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one "},"(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3Z,4S)-1,7,7-trimethyl-3-(4- methylbenzylidene)bicyclo[2.2.1]heptan-2-one ","(1R,3Z,4S)-1,7,7-三甲基-3-(4-亚苯基亚甲基)二环[2.2.1]庚-2-酮 "]
[null,{"$f":"IF($B$1=\"English\",C3310,IF($B$1=\"Deutsch\",D3310,IF($B$1=\"中文\",E3310,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1'-[ethane-1,2-diylbisoxy]bis[2,4,6-tribromobenzene"},"1,1'-[ethane-1,2-diylbisoxy]bis[2,4,6-tribromobenzene","1,1'-[ethane-1,2-diylbisoxy]bis[2,4,6-tribromobenzene","1,1'-[乙烷-1,2-二基二氧基]双[2,4,6-三溴苯"]
[null,{"$f":"IF($B$1=\"English\",C3311,IF($B$1=\"Deutsch\",D3311,IF($B$1=\"中文\",E3311,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol"},"2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol","2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol","2,2',6,6'-四溴-4,4'-异亚丙基双酚"]
[null,{"$f":"IF($B$1=\"English\",C3312,IF($B$1=\"Deutsch\",D3312,IF($B$1=\"中文\",E3312,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-sulphonyldiphenol"},"4,4'-sulphonyldiphenol","4,4'-sulphonyldiphenol","4,4'-磺酰基双酚"]
[null,{"$f":"IF($B$1=\"English\",C3313,IF($B$1=\"Deutsch\",D3313,IF($B$1=\"中文\",E3313,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Barium diboron tetraoxide"},"Barium diboron tetraoxide","Barium diboron tetraoxide","偏硼酸钡"]
[null,{"$f":"IF($B$1=\"English\",C3314,IF($B$1=\"Deutsch\",D3314,IF($B$1=\"中文\",E3314,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl) tetrabromophthalate covering any of the individual isomers and/or combinations thereof"},"Bis(2-ethylhexyl) tetrabromophthalate covering any of the individual isomers and/or combinations thereof","Bis(2-ethylhexyl) tetrabromophthalate covering any of the individual isomers and/or combinations thereof","双(2-乙基己基)四硼己酯包括各异构体和/或其组合"]
[null,{"$f":"IF($B$1=\"English\",C3315,IF($B$1=\"Deutsch\",D3315,IF($B$1=\"中文\",E3315,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl) tetrabromophthalate"},"Bis(2-ethylhexyl) tetrabromophthalate","Bis(2-ethylhexyl) tetrabromophthalate","双(2-乙基己基)四硼己酯"]
[null,{"$f":"IF($B$1=\"English\",C3316,IF($B$1=\"Deutsch\",D3316,IF($B$1=\"中文\",E3316,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Isobutyl 4-hydroxybenzoate"},"Isobutyl 4-hydroxybenzoate","Isobutyl 4-hydroxybenzoate","尼泊金异丁酯"]
[null,{"$f":"IF($B$1=\"English\",C3317,IF($B$1=\"Deutsch\",D3317,IF($B$1=\"中文\",E3317,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Melamine"},"Melamine","Melamine","三聚氰胺"]
[null,{"$f":"IF($B$1=\"English\",C3318,IF($B$1=\"Deutsch\",D3318,IF($B$1=\"中文\",E3318,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluoroheptanoic acid and its salts"},"Perfluoroheptanoic acid and its salts","Perfluoroheptanoic acid and its salts","全氟庚酸及其盐"]
[null,{"$f":"IF($B$1=\"English\",C3319,IF($B$1=\"Deutsch\",D3319,IF($B$1=\"中文\",E3319,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium perfluoroheptanoate"},"Ammonium perfluoroheptanoate","Ammonium perfluoroheptanoate","全氟庚酸铵"]
[null,{"$f":"IF($B$1=\"English\",C3320,IF($B$1=\"Deutsch\",D3320,IF($B$1=\"中文\",E3320,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"potassium perfluoroheptanoate"},"potassium perfluoroheptanoate","potassium perfluoroheptanoate","全氟庚酸鉀"]
[null,{"$f":"IF($B$1=\"English\",C3321,IF($B$1=\"Deutsch\",D3321,IF($B$1=\"中文\",E3321,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluoroheptanoic acid"},"Perfluoroheptanoic acid","Perfluoroheptanoic acid","全氟庚酸"]
[null,{"$f":"IF($B$1=\"English\",C3322,IF($B$1=\"Deutsch\",D3322,IF($B$1=\"中文\",E3322,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perfluoroheptanoate"},"Sodium perfluoroheptanoate","Sodium perfluoroheptanoate","全氟庚酸鈉"]
[null,{"$f":"IF($B$1=\"English\",C3323,IF($B$1=\"Deutsch\",D3323,IF($B$1=\"中文\",E3323,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"reaction mass of 2,2,3,3,5,5,6,6-octafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)morpholine and 2,2,3,3,5,5,6,6-octafluoro-4-(heptafluoropropyl)morpholine"},"reaction mass of 2,2,3,3,5,5,6,6-octafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)morpholine and 2,2,3,3,5,5,6,6-octafluoro-4-(heptafluoropropyl)morpholine","reaction mass of 2,2,3,3,5,5,6,6-octafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)morpholine and 2,2,3,3,5,5,6,6-octafluoro-4-(heptafluoropropyl)morpholine","reaction mass of 2,2,3,3,5,5,6,6-octafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)morpholine and 2,2,3,3,5,5,6,6-octafluoro-4-(heptafluoropropyl)morpholine"]
[null,{"$f":"IF($B$1=\"English\",C3324,IF($B$1=\"Deutsch\",D3324,IF($B$1=\"中文\",E3324,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in articles, by professional workers (widespread uses), in formulation or re-packing, at industrial sites and in manufacturing."},"Used in articles, by professional workers (widespread uses), in formulation or re-packing, at industrial sites and in manufacturing.","Wird in Artikeln, von Fachleuten (weit verbreitete Verwendung), bei der Formulierung oder Umverpackung, in Industrieanlagen und in der Fertigung verwendet.","由专业人员用于（广泛使用于）工业场所及生产中的各种物品、配方、再包装。"]
[null,{"$f":"IF($B$1=\"English\",C3325,IF($B$1=\"Deutsch\",D3325,IF($B$1=\"中文\",E3325,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3326,IF($B$1=\"Deutsch\",D3326,IF($B$1=\"中文\",E3326,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3327,IF($B$1=\"Deutsch\",D3327,IF($B$1=\"中文\",E3327,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3328,IF($B$1=\"Deutsch\",D3328,IF($B$1=\"中文\",E3328,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use as lubricant, hydraulic fluid, grease, release agent use in polyurethane, PVC, TPE, coatings and textiles\nFlame retardants in plastics production\nUse as plasticizer"},"Use as lubricant, hydraulic fluid, grease, release agent use in polyurethane, PVC, TPE, coatings and textiles\nFlame retardants in plastics production\nUse as plasticizer","Verwendung als Schmiermittel, hydraulische Flüssigkeit, Fett, Trennmittel>br>Verwendung in Polyurethan, PVC, TPE sowie in Beschichtungen und Textilien\nFlammschutzmittel in der Kunststoffproduktion\nVerwendung als Weichmacher ","用作润滑剂、液压液、油脂及聚氨酯/PVC/TPE/涂层/纺织品的脱模剂\n塑料生产中的阻燃剂\n用作塑化剂"]
[null,{"$f":"IF($B$1=\"English\",C3329,IF($B$1=\"Deutsch\",D3329,IF($B$1=\"中文\",E3329,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dyes for textiles and paper\npH indicator\nAdditive for agar culture media (for biological staining of histological samples)\nGelling agent for polyvinyl alcohol"},"Dyes for textiles and paper\npH indicator\nAdditive for agar culture media (for biological staining of histological samples)\nGelling agent for polyvinyl alcohol","Färbemittel für Textilien und Papier\npH-Indikator\nZusatz für Agarnährböden (zur biologischen Färbung histologischer Proben)\nGeliermittel für Polyvinylalkohol ","纺织品和纸张染色剂\npH指示剂\n（用于组织样本生物染色用）琼脂培养基添加剂\n聚乙烯醇凝胶剂"]
[null,{"$f":"IF($B$1=\"English\",C3330,IF($B$1=\"Deutsch\",D3330,IF($B$1=\"中文\",E3330,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of rubber products and tyres\nProduction of masterbatches\nPreparation of predispersed imidazolidine-2-thione\nUse as vulcanizing agent\nFor repackaging "},"Manufacture of rubber products and tyres\nProduction of masterbatches\nPreparation of predispersed imidazolidine-2-thione\nUse as vulcanizing agent\nFor repackaging ","  Herstellung von Gummiwaren und Reifen\nHerstellung von Masterbatches\nHerstellung von vordispergiertem Imidazolidin-2-thion\nVerwendung als Vulkanisierungsmittel\nZur Wiederverpackung ","橡胶产品和轮胎生产\n母胶生产\n配制预分散型2-硫代咪唑烷酮\n用作硫化剂\n用于再包装 "]
[null,{"$f":"IF($B$1=\"English\",C3331,IF($B$1=\"Deutsch\",D3331,IF($B$1=\"中文\",E3331,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component for the production of organic and inorganic cadmium compounds\nComponent for the preparation of inorganic pigments\nLaboratory chemical (intermediate, perfumes, perfumes, cosmetics, personal care products)\nComponent for the production of photovoltaic modules\nAdditive for the production of frits and glasses\nAdditive for the production of electronic components"},"Component for the production of organic and inorganic cadmium compounds\nComponent for the preparation of inorganic pigments\nLaboratory chemical (intermediate, perfumes, perfumes, cosmetics, personal care products)\nComponent for the production of photovoltaic modules\nAdditive for the production of frits and glasses\nAdditive for the production of electronic components","  Bestandteil zur Herstellung von organischen und anorganischen Cadmiumverbindungen\nBestandteil zur Herstellung von anorganischen Pigmenten\nLaborchemikalie (Zwischenprodukt, Parfüme, Düfte, Kosmetik, Personal-Care-Produkte)\nBestandteil zur Herstellung von Photovoltaikmodulen\nAdditiv zur Herstellung von Fritten und Gläsern\nAdditiv zur Herstellung von elektronischen Bestandteilen ","生产有机和无机镉化合物的成分\n配制无机颜料的成分\n实验室化学品（中间体、香精、香料、化妆品、个人护理产品）\n生产光伏组件的成分\n生产玻璃原料和玻璃用添加剂\n生产电子元件用添加剂"]
[null,{"$f":"IF($B$1=\"English\",C3332,IF($B$1=\"Deutsch\",D3332,IF($B$1=\"中文\",E3332,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizer for cellulose and vinylplastics"},"Plasticizer for cellulose and vinylplastics","Weichmacher für Cellulose und Vinylplastik","纤维素和乙烯基塑料用塑化剂"]
[null,{"$f":"IF($B$1=\"English\",C3333,IF($B$1=\"Deutsch\",D3333,IF($B$1=\"中文\",E3333,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Use as intermediate product\nUse as a laboratory chemical\nFor the production of coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling compounds"},"Use as intermediate product\nUse as a laboratory chemical\nFor the production of coatings and paints, thinners, paint removers, fillers, putties, plasters, modelling compounds","Verwendung als Zwischenprodukt\nVerwendung als Laborchemikalie\nZur Herstellung von Beschichtungen und Farben, Verdünnungsmittel, Farbentferner, Füllmittel, Kitte, Pflaster, Modelliermassen ","用作中间产品\n用作实验室化学品\n用于生产涂料、油漆、稀释剂、脱漆剂、填充剂、油灰、灰泥、印模膏"]
[null,{"$f":"IF($B$1=\"English\",C3334,IF($B$1=\"Deutsch\",D3334,IF($B$1=\"中文\",E3334,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dyes for textiles, leather and paper, plastics, wood and biological materials\nIngredient for the preparation of aqueous inks\nUse in hair dyes"},"Dyes for textiles, leather and paper, plastics, wood and biological materials\nIngredient for the preparation of aqueous inks\nUse in hair dyes","Färbemittel für Textilien, Leder und Papier, Kunststoff, Holz und biologische Materialen\nBestandteil zur Herstellung wässriger Tinten\n>Verwendung in Haarfärbemitteln","纺织品、皮革、纸张、塑料、木料和生物材料用染料\n制备水性墨水的成分\n用于染发"]
[null,{"$f":"IF($B$1=\"English\",C3335,IF($B$1=\"Deutsch\",D3335,IF($B$1=\"中文\",E3335,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products"},"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products","Bleichmittel in Wasch- und Geschirrspülmittel\nReinigungsmittel\nVerwendung in kosmetischen Produkten  ","清洁剂和餐具洗涤剂用漂白剂\n清洁剂\n用于化妆品"]
[null,{"$f":"IF($B$1=\"English\",C3336,IF($B$1=\"Deutsch\",D3336,IF($B$1=\"中文\",E3336,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\nSunset date: 27.05.2023"},"Included in Annex 14\n\n- Last application date: 27.11.2021\nSunset date: 27.05.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.11.2021\n- Ablauftermin: \n27.05.2023","在附件14中\n\n- 上次申请日期：2021年11月27日\n受管制起始日期：2023年5月27日"]
[null,{"$f":"IF($B$1=\"English\",C3337,IF($B$1=\"Deutsch\",D3337,IF($B$1=\"中文\",E3337,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n- Sunset date: 27.02.2023"},"Included in Annex 14\n\n- Last application date: 27.08.2021\n- Sunset date: 27.02.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.08.2021\n- Ablauftermin: \n27.02.2023","在附件14中\n\n- 上次申请日期：2021年8月27日\n-受管制起始日期：2023年2月27日"]
[null,{"$f":"IF($B$1=\"English\",C3338,IF($B$1=\"Deutsch\",D3338,IF($B$1=\"中文\",E3338,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023"},"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.11.2021\n- Ablauftermin: \n27.05.2023","在附件14中\n\n- 上次申请日期：2021年11月27日\n-受管制起始日期：2023年5月27日"]
[null,{"$f":"IF($B$1=\"English\",C3339,IF($B$1=\"Deutsch\",D3339,IF($B$1=\"中文\",E3339,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium perborate monohydrate"},"Sodium perborate monohydrate","Natrium perborate monohydrate","一水过硼酸钠"]
[null,{"$f":"IF($B$1=\"English\",C3340,IF($B$1=\"Deutsch\",D3340,IF($B$1=\"中文\",E3340,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perboric acid (HBO(O2)), sodium\nsalt, tetrahydrate"},"Perboric acid (HBO(O2)), sodium\nsalt, tetrahydrate","Perboric acid (HBO(O2)), sodium\nsalt, tetrahydrate","过硼酸(HBO(O2))，钠\n盐，四水合物"]
[null,{"$f":"IF($B$1=\"English\",C3341,IF($B$1=\"Deutsch\",D3341,IF($B$1=\"中文\",E3341,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perboric acid, sodium salt,\ntetrahydrate"},"Perboric acid, sodium salt,\ntetrahydrate","Perboric acid, sodium salt,\ntetrahydrate","过硼酸，钠盐\n四水合物"]
[null,{"$f":"IF($B$1=\"English\",C3342,IF($B$1=\"Deutsch\",D3342,IF($B$1=\"中文\",E3342,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-(hydroxymethyl)acrylamide"},"N-(hydroxymethyl)acrylamide","N-(hydroxymethyl)acrylamide","N-羟甲基丙烯酰胺"]
[null,{"$f":"IF($B$1=\"English\",C3343,IF($B$1=\"Deutsch\",D3343,IF($B$1=\"中文\",E3343,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products "},"Bleaching agents in detergents and dishwashing detergents\ncleansers\nUse in cosmetic products ","Bleichmittel in Wasch- und Geschirrspülmittel\nReinigungsmittel\nVerwendung in kosmetischen Produkten ","清洁剂和餐具洗涤剂用漂白剂\n清洁剂\n用于化妆品 "]
[null,{"$f":"IF($B$1=\"English\",C3344,IF($B$1=\"Deutsch\",D3344,IF($B$1=\"中文\",E3344,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component for the production of organic and inorganic cadmium compounds\nStarting material in electroplating and electroplating\nComponent for the production of photovoltaic modules\nlaboratory chemical\nFungicide"},"Component for the production of organic and inorganic cadmium compounds\nStarting material in electroplating and electroplating\nComponent for the production of photovoltaic modules\nlaboratory chemical\nFungicide","Bestandteil zur Herstellung von organischen und anorganischen Cadmiumverbindungen\nAusgangsstoff in der Elektroplattierung und Galvanik\nBestandteil zur Herstellung von Photovoltaikmodulen\nLaborchemikalie\nFungizid ","生产有机和无机镉化合物的成分\n电镀原材料和电镀\n生产光伏组件的成分\n实验室化学品\n杀菌剂"]
[null,{"$f":"IF($B$1=\"English\",C3345,IF($B$1=\"Deutsch\",D3345,IF($B$1=\"中文\",E3345,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Plasticizer in polymers, insulating primer, sealing material, engine oil stabilizer, transmission lubricant for motor vehicles"},"Plasticizer in polymers, insulating primer, sealing material, engine oil stabilizer, transmission lubricant for motor vehicles","Weichmacher in Polymeren, Isoliergrund, Dichtungsmaterial, Motorölstabilisator, Getriebeschmiermittel für Kraftfahrzeuge","聚合物、绝缘底漆、密封材料、机油稳定剂、机动车传动润滑剂用塑化剂"]
[null,{"$f":"IF($B$1=\"English\",C3346,IF($B$1=\"Deutsch\",D3346,IF($B$1=\"中文\",E3346,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PVC heat stabilizer\nUse in plastics processing\nIndustrial use"},"PVC heat stabilizer\nUse in plastics processing\nIndustrial use","Wärmestabilisator von PVC\nVerwendung in der Kunststoffverarbeitung\nIndustrielle Verwedung ","PVC热稳定剂\n用于塑料加工\n工业用途"]
[null,{"$f":"IF($B$1=\"English\",C3347,IF($B$1=\"Deutsch\",D3347,IF($B$1=\"中文\",E3347,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Research\nManufacture of glass\nHigh Temperature Dry Film Lubricant\nOptical electronics\nSolar cells"},"Research\nManufacture of glass\nHigh Temperature Dry Film Lubricant\nOptical electronics\nSolar cells","Forschung\nHerstellung von Glas\nHoch-Temperatur Trockenfilm-Schmiermittel\noptische Elektronik\nSolarzellen","研究\n玻璃生产\n高温干膜润滑剂\n光学电子元件\n太阳能电池"]
[null,{"$f":"IF($B$1=\"English\",C3348,IF($B$1=\"Deutsch\",D3348,IF($B$1=\"中文\",E3348,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Component for the production of inorganic cadmium compounds\nStarting material for the surface treatment of metals\nLaboratory Chemical"},"Component for the production of inorganic cadmium compounds\nStarting material for the surface treatment of metals\nLaboratory Chemical","Bestandteil zur Herstellung von anorganischen Cadmiumverbindungen\nAusgangsstoff für die Oberflächenbehandlung von Metallen\nLaborchemikalie","无机镉化合物生产组分\n金属表面处理原材料\n实验室化学品"]
[null,{"$f":"IF($B$1=\"English\",C3349,IF($B$1=\"Deutsch\",D3349,IF($B$1=\"中文\",E3349,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-ethylhexyl)phthalate is mainly used as a plasticizer in polymer products (mainly PVC) to increase the mobility of the product.\nConsumer exposure occurs through the respiratory tract through building materials (wallpaper, floor coverings), furniture and car interiors, through skin contact with shoes, rainwear, PVC gloves, artificial leather in furniture and car seats as well as toys and through ingestion of some baby and child products and food contact materials"},"Bis(2-ethylhexyl)phthalate is mainly used as a plasticizer in polymer products (mainly PVC) to increase the mobility of the product.\nConsumer exposure occurs through the respiratory tract through building materials (wallpaper, floor coverings), furniture and car interiors, through skin contact with shoes, rainwear, PVC gloves, artificial leather in furniture and car seats as well as toys and through ingestion of some baby and child products and food contact materials","Bis(2-ethylhexyl)phthalat wird hauptsächlich als Weichmacher in Polymerprodukten (hauptsächlich PVC) zur Erhöhung der Beweglichkeit des Produktes verwendet.\nDie Verbraucherexposition erfolgt über die Atemwege durch Baumaterialien (Tapeten, Bodenbeläge), Möbel und Autoinnenverkleidungen, durch Hautkontakt mit Schuhen, Regenbekleidung, PVC-Handschuhen, Kunstleder in Möbeln und Fahrzeugsitzen sowie Spielzeug und durch Verschlucken mancher Baby- und Kinderprodukte sowie Lebensmittelkontaktmaterial.","双(2-乙基己基)己酯主要用作聚合物产品（主要是PVC）的塑化剂，用于增强产品的流动性。\n消费者可通过建筑材料（墙纸、地板）、家具、汽车内饰等产生呼吸道接触，通过鞋子、防水衣、PVC手套、家具和汽车座位上的人造革、玩具等发生皮肤接触，以及通过摄入某些婴幼儿产品和食品接触材料发生接触"]
[null,{"$f":"IF($B$1=\"English\",C3350,IF($B$1=\"Deutsch\",D3350,IF($B$1=\"中文\",E3350,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Starting material for the preparation of \"Reaction mass of\" 2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates and 2-ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates (\"\"Reaction mass of\"\" DOTE and MOTE)\nUse in plastics processing\nIndustrial use"},"Starting material for the preparation of \"Reaction mass of\" 2-ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates and 2-ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoates (\"\"Reaction mass of\"\" DOTE and MOTE)\nUse in plastics processing\nIndustrial use","Ausgangsstoff zur Herstellung von \"Reaction mass of\" 2-Ethylhexyl-10-ethyl-4,4-dioctyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate und 2-Ethylhexyl-10-ethyl-4-[[2-[(2-ethylhexyl)oxy]-2-oxoethyl]thio]-4-octyl-7-oxo-8-oxa-3,5-dithia-4-stannatetradecanoate (\"Reaction mass of\" DOTE und MOTE)\nVerwendung in der Kunststoffverarbeitung\nIndustrielle Verwedung ","配制甲基锡三(巯基乙酸异辛酯)和2-乙基己基-10-乙基-4-[[2-[(2-乙基己基)氧基]-2-氧代乙基]硫杂]-4-辛基-7-氧代-8-氧杂-3,5-二硫杂-4-十四锡酸酯反应物（即DOTE和MOTE反应物）的原材料\n用于塑料加工\n工业用途"]
[null,{"$f":"IF($B$1=\"English\",C3351,IF($B$1=\"Deutsch\",D3351,IF($B$1=\"中文\",E3351,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV stabilizer;\nUV absorbents;\nUV-protective agents"},"UV stabilizer;\nUV absorbents;\nUV-protective agents","UV-Stabilisator;\nUV-Absorptionsmittel;\nUV-Schutzmittel ","UV稳定剂；\nUV吸收剂\nUV保护剂"]
[null,{"$f":"IF($B$1=\"English\",C3352,IF($B$1=\"Deutsch\",D3352,IF($B$1=\"中文\",E3352,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV stabilizer;\nUV absorbents;\nUV-protective agents"},"UV stabilizer;\nUV absorbents;\nUV-protective agents","UV-Stabilisator;\nUV-Absorptionsmittel;\nUV-Schutzmittel","UV稳定剂；\nUV吸收剂\nUV保护剂"]
[null,{"$f":"IF($B$1=\"English\",C3353,IF($B$1=\"Deutsch\",D3353,IF($B$1=\"中文\",E3353,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"This group of substances is mainly used in fragrances."},"This group of substances is mainly used in fragrances.","Diese Gruppe von Stoffen findet hauptsächlich in Duftstoffen Verwendung.","该组物质主要用于香水。"]
[null,{"$f":"IF($B$1=\"English\",C3354,IF($B$1=\"Deutsch\",D3354,IF($B$1=\"中文\",E3354,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023"},"Included in Annex 14\n\n- Last application date: 27.11.2021\n- Sunset date: 27.05.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.11.2021\n- Ablauftermin: \n27.05.2023","在附件14中\n\n- 上次申请日期：2021年11月27日\n-受管制起始日期：2023年5月27日"]
[null,{"$f":"IF($B$1=\"English\",C3355,IF($B$1=\"Deutsch\",D3355,IF($B$1=\"中文\",E3355,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023"},"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.08.2021\n- Ablauftermin: \n27.02.2023","在附件14中\n\n- 上次申请日期：2021年8月27日\n\n-受管制起始日期：2023年2月27日"]
[null,{"$f":"IF($B$1=\"English\",C3356,IF($B$1=\"Deutsch\",D3356,IF($B$1=\"中文\",E3356,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025","aufgenommen in Anhang 14 \n- Antragsschluss: \n01.11.2023\n\n- Ablauftermin:  \n01.05.2025\n","在附件14中\n\n- 上次申请日期：2023年11月1日\n-受管制起始日期：2025年5月1日"]
[null,{"$f":"IF($B$1=\"English\",C3357,IF($B$1=\"Deutsch\",D3357,IF($B$1=\"中文\",E3357,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n"},"included in Annex 14 and Annex 17\n- \nlast application date:\n21. August 2013\n- \nsunset date:\n21. Februar 2015\n","aufgenommen in Anhang 14 und Anhang 17\n- Antragsschluss:\n21. August 2013\n- Ablauftermin:\n21. Februar 2015\n","在附件14和附件17中\n- \n上次申请日期：\n21.2013年8月\n- \n受管制起始日期：\n21.2015年2月\n"]
[null,{"$f":"IF($B$1=\"English\",C3358,IF($B$1=\"Deutsch\",D3358,IF($B$1=\"中文\",E3358,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025","aufgenommen in Anhang 14\n- Antragsschluss: \n01.11.2023\n\n- Ablauftermin:  \n01.05.2025\n","在附件14中\n\n- 上次申请日期：2023年11月1日\n-受管制起始日期：2025年5月1日"]
[null,{"$f":"IF($B$1=\"English\",C3359,IF($B$1=\"Deutsch\",D3359,IF($B$1=\"中文\",E3359,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.05.2022\n- Ablauftermin: \n27.11.2023","在附件14中\n\n- 上次申请日期：2022年5月27日\n-受管制起始日期：2023年11月27日"]
[null,{"$f":"IF($B$1=\"English\",C3360,IF($B$1=\"Deutsch\",D3360,IF($B$1=\"中文\",E3360,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.05.2022\n- Ablauftermin: \n27.11.2023","在附件14中\n\n- 上次申请日期：2022年5月27日\n-受管制起始日期：2023年11月27日"]
[null,{"$f":"IF($B$1=\"English\",C3361,IF($B$1=\"Deutsch\",D3361,IF($B$1=\"中文\",E3361,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.02.2022\n- Sunset date: 27.08.2023"},"Included in Annex 14\n\n- Last application date: 27.02.2022\n- Sunset date: 27.08.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.02.2022\n- Ablauftermin: \n27.08.2023","在附件14中\n\n- 上次申请日期：2022年2月27日\n-受管制起始日期：2023年8月27日"]
[null,{"$f":"IF($B$1=\"English\",C3362,IF($B$1=\"Deutsch\",D3362,IF($B$1=\"中文\",E3362,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"in plasticisers, lubricants, coating agents, building materials, cable components, polymer films, PVC components and artists' supplies (e.g. in modelling clay and in finger paints)"},"in plasticisers, lubricants, coating agents, building materials, cable components, polymer films, PVC components and artists' supplies (e.g. in modelling clay and in finger paints)","in Weichmacher, Schmiermittel, Beschichtungsmittel, Baustoffe, Kabelbestandteile, Polymerfolien, PVC-Komponenten und Künstlerbedarf (z.B. in Modellierton und in Fingerfarben) ","用于塑化剂、润滑剂、涂布剂、建筑材料、电缆组件、高分子膜、PVC组件及艺术用品（如雕塑黏土指画颜料）"]
[null,{"$f":"IF($B$1=\"English\",C3363,IF($B$1=\"Deutsch\",D3363,IF($B$1=\"中文\",E3363,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Processing aid in the manufacture of fluoropolymers; lubricant in oils; wetting agent for fire-fighting foam; cleaning agent; antifouling in textiles; surface agent in polishes; sealant; in liquid crystal display panels."},"Processing aid in the manufacture of fluoropolymers; lubricant in oils; wetting agent for fire-fighting foam; cleaning agent; antifouling in textiles; surface agent in polishes; sealant; in liquid crystal display panels.","Prozesshilfsstoff in der Herstellung von Fluorpolymeren; Schmiermittel in Ölen; Netzmittel für Feuerlöschschaum; Reinigungsmittel; Antifouling in Textilien; Oberflächenagenz in Poliermittel; Abdichtungsmittel; in Flüssigkristalldisplay-Paneelen","含氟聚合物生产用加工助剂，油中的润滑成分，消防泡沫中的润湿剂，清洁剂，纺织品防污剂，亮光剂中的表面活性剂，液晶显示面板的密封剂。"]
[null,{"$f":"IF($B$1=\"English\",C3364,IF($B$1=\"Deutsch\",D3364,IF($B$1=\"中文\",E3364,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023"},"Included in Annex 14\n\n- Last application date: 27.08.2021\n\n- Sunset date: 27.02.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.08.2021\n- Ablauftermin: \n27.02.2023","在附件14中\n\n- 上次申请日期：2021年8月27日\n\n-受管制起始日期：2023年2月27日"]
[null,{"$f":"IF($B$1=\"English\",C3365,IF($B$1=\"Deutsch\",D3365,IF($B$1=\"中文\",E3365,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of other substances"},"Manufacture of other substances","Herstellung anderer Stoffe ","其他物质的生产"]
[null,{"$f":"IF($B$1=\"English\",C3366,IF($B$1=\"Deutsch\",D3366,IF($B$1=\"中文\",E3366,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV stabilizer in coatings, plastics, rubber and cosmetics "},"UV stabilizer in coatings, plastics, rubber and cosmetics ","UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika ","涂料、塑料、橡胶和化妆品中的UV稳定剂 "]
[null,{"$f":"IF($B$1=\"English\",C3367,IF($B$1=\"Deutsch\",D3367,IF($B$1=\"中文\",E3367,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Intermediate for the production of fine and bulk chemicals, electrolyte for lithium ion batteries "},"Intermediate for the production of fine and bulk chemicals, electrolyte for lithium ion batteries ","Zwischenprodukt für die Herstellung von Fein- und Bulkchemikalien, Elektrolyt für Lithiumionenbatterien ","精细化妆品和散装化妆品生产用中间产品，锂离子电池电极 "]
[null,{"$f":"IF($B$1=\"English\",C3368,IF($B$1=\"Deutsch\",D3368,IF($B$1=\"中文\",E3368,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika "},"UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika ","UV-Stabilisator in Beschichtungen, Plastik, Gummi und Kosmetika ","涂层、塑料、胶粘剂和化妆品中的UV稳定剂 "]
[null,{"$f":"IF($B$1=\"English\",C3369,IF($B$1=\"Deutsch\",D3369,IF($B$1=\"中文\",E3369,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[a]pyrene is not registered. The substance is not normally manufactured, but can be an ingredient or contamination of another substance. "},"Benzo[a]pyrene is not registered. The substance is not normally manufactured, but can be an ingredient or contamination of another substance. ","Benzo[a]pyren ist nicht registriert. Der Stoff wird normalerweise nicht hergestellt, sondern kann ein Bestandteil oder eine Verunreinigung eines anderen Stoffes sein. ","苯并[a]芘未登记。该物质一般不生产，但可用于构成或掺入其他物质。 "]
[null,{"$f":"IF($B$1=\"English\",C3370,IF($B$1=\"Deutsch\",D3370,IF($B$1=\"中文\",E3370,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monomer for the preparation of polymers"},"Monomer for the preparation of polymers","Monomer zur Herstellung von Polymeren","用于制备聚合物的单体"]
[null,{"$f":"IF($B$1=\"English\",C3371,IF($B$1=\"Deutsch\",D3371,IF($B$1=\"中文\",E3371,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.05.2022\n- Ablauftermin: \n27.11.2023","在附件14中\n\n- 上次申请日期：2022年5月27日\n-受管制起始日期：2023年11月27日"]
[null,{"$f":"IF($B$1=\"English\",C3372,IF($B$1=\"Deutsch\",D3372,IF($B$1=\"中文\",E3372,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023"},"Included in Annex 14\n\n- Last application date: 27.05.2022\n- Sunset date: 27.11.2023","Aufgenommen in Annex 14\n- Antragsschluss: \n27.05.2022\n- Ablauftermin: \n27.11.2023","在附件14中\n\n- 上次申请日期：2022年5月27日\n-受管制起始日期：2023年11月27日"]
[null,{"$f":"IF($B$1=\"English\",C3373,IF($B$1=\"Deutsch\",D3373,IF($B$1=\"中文\",E3373,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the manufacture of chemicals and plastic products "},"For the manufacture of chemicals and plastic products ","Zur Herstellung von Chemikalien und Erzeugnissen aus Plastik ","用于生产化学品和塑料制品 "]
[null,{"$f":"IF($B$1=\"English\",C3374,IF($B$1=\"Deutsch\",D3374,IF($B$1=\"中文\",E3374,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"e.g. as corrosion inhibitor, lubricant, softener "},"e.g. as corrosion inhibitor, lubricant, softener ","u.a. als Korrosionsinhibitor, Schmiermittel, Weichmacher ","如用作阻蚀剂、润滑剂、软化剂 "]
[null,{"$f":"IF($B$1=\"English\",C3375,IF($B$1=\"Deutsch\",D3375,IF($B$1=\"中文\",E3375,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PFHxS is a known contamination in the production of PFOS. It can also be used as a replacement for PFOS"},"PFHxS is a known contamination in the production of PFOS. It can also be used as a replacement for PFOS","PFHxS ist eine bekannte Verunreinigung bei der Herstellung von PFOS. Es kann auch als Ersatz für PFOS eingesetzt werden","PFHxS已知为PFOS生产中的掺入物。也可用于替换PFOS"]
[null,{"$f":"IF($B$1=\"English\",C3376,IF($B$1=\"Deutsch\",D3376,IF($B$1=\"中文\",E3376,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"For the production of epoxy and epoxy hardeners (industrial and professional applications), coating material, for the production of polymers such as polycarbonates and PVC; use in thermal paper (industrial, professional and consumer)"},"For the production of epoxy and epoxy hardeners (industrial and professional applications), coating material, for the production of polymers such as polycarbonates and PVC; use in thermal paper (industrial, professional and consumer)","Zur Herstellung von Epoxiden und Expoxid Härtern (industrielle und professionelle Anwendungen), Beschichtungsmaterial, Zur Herstellung von Polymeren, wie z.B. Polycarbonaten und PVC; Verwendung in Thermopapier (industriell, professionell und Verbraucher)","用于生产环氧树脂和环氧固化剂（各种工业和专业应用）、涂料，生产聚碳酸酯和PVC等聚合物，用于热敏纸（工业、专业和消费用）"]
[null,{"$f":"IF($B$1=\"English\",C3377,IF($B$1=\"Deutsch\",D3377,IF($B$1=\"中文\",E3377,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in greases, lubricating greases and lubricating oils."},"Used in greases, lubricating greases and lubricating oils.","Wird in Fetten, Schmierfetten und Schmierölen eingesetzt.","用于油脂、润滑脂和润滑油。"]
[null,{"$f":"IF($B$1=\"English\",C3378,IF($B$1=\"Deutsch\",D3378,IF($B$1=\"中文\",E3378,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a pH regulator and in drinking water treatment products, laboratory chemicals, cosmetics and care products."},"Used as a pH regulator and in drinking water treatment products, laboratory chemicals, cosmetics and care products.","Wird als pH Regulator und in Trinkwasseraufbereitungsprodukten, Laborchemikalien, Kosmetika und Pflegeprodukten verwendet.","用作pH值调节剂、饮用水处理产品、实验室化学品、化妆品和护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C3379,IF($B$1=\"Deutsch\",D3379,IF($B$1=\"中文\",E3379,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The substance is used in the manufacture of electrical, electronic and optical equipment and in laboratory chemicals. "},"The substance is used in the manufacture of electrical, electronic and optical equipment and in laboratory chemicals. ","Der Stoff wird bei der Herstellung von elektrischer, elektronischer und optischer Ausrüstung und in Laborchemikalien verwendet. ","该物质用于生产电气、电子和光学设备，用作实验室化学品。 "]
[null,{"$f":"IF($B$1=\"English\",C3380,IF($B$1=\"Deutsch\",D3380,IF($B$1=\"中文\",E3380,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in the manufacture of glass, ceramic and porcelain products and in laboratory chemicals. "},"Used in the manufacture of glass, ceramic and porcelain products and in laboratory chemicals. ","Wird bei der Herstellung von Produkten aus Glas, Keramik und Porzellan und in Laborchemikalien verwendet. ","用于生产玻璃、陶瓷和瓷器产品，用作实验室化学品。 "]
[null,{"$f":"IF($B$1=\"English\",C3381,IF($B$1=\"Deutsch\",D3381,IF($B$1=\"中文\",E3381,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Is not normally produced, but is a component or contamination of other substances."},"Is not normally produced, but is a component or contamination of other substances.","Wird normalerweise nicht produziert, sondern ist ein Bestandteil oder eine Verunreinigung anderer Stoffe.","一般不生产，但可用于构成或掺入其他物质。"]
[null,{"$f":"IF($B$1=\"English\",C3382,IF($B$1=\"Deutsch\",D3382,IF($B$1=\"中文\",E3382,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Is not normally produced, but is a component or contamination of other substances."},"Is not normally produced, but is a component or contamination of other substances.","Wird normalerweise nicht produziert, sondern ist ein Bestandteil oder eine Verunreinigung anderer Stoffe.","一般不生产，但可用于构成或掺入其他物质。"]
[null,{"$f":"IF($B$1=\"English\",C3383,IF($B$1=\"Deutsch\",D3383,IF($B$1=\"中文\",E3383,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as flame retardant in adhesives, sealants and binders."},"Used as flame retardant in adhesives, sealants and binders.","Wird als Flammschutzmittel in Kleb- und Dichtstoffen sowie in Bindemitteln eingesetzt. ","用作胶粘剂、密封剂和粘合剂中的阻燃剂。"]
[null,{"$f":"IF($B$1=\"English\",C3384,IF($B$1=\"Deutsch\",D3384,IF($B$1=\"中文\",E3384,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025"},"Included in Annex 14\n\n- Last application date: 01.11.2023\n- Sunset date: 01.05.2025","Aufgenommen in Annex 14\n\n- Antragsschluss: 01.11.2023\n- Ablaufdatum: 01.05.2025","在附件14中\n\n- 上次申请日期：2023年11月1日\n-受管制起始日期：2025年5月1日"]
[null,{"$f":"IF($B$1=\"English\",C3385,IF($B$1=\"Deutsch\",D3385,IF($B$1=\"中文\",E3385,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in the manufacture of esters and polymers."},"Used in the manufacture of esters and polymers.","Herstellung von Estern und Polymeren","用于生产酯类和聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C3386,IF($B$1=\"Deutsch\",D3386,IF($B$1=\"中文\",E3386,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in plastisol, PVC, rubber and plastic articles. A further use is also as a phlegmatiser and dispersing agent for formulations of organic peroxides."},"Used in plastisol, PVC, rubber and plastic articles. A further use is also as a phlegmatiser and dispersing agent for formulations of organic peroxides.","Plastisol, PVC, Kautschuk, Kunststoffe sowie Phlegmatisierungsmittel und Dispergiermittel zur Herstellung organischer Peroxide","用于塑料溶胶、PVC、橡胶和塑料制品。还可用作有机过氧化物配方中的阻遏剂和分散剂。"]
[null,{"$f":"IF($B$1=\"English\",C3387,IF($B$1=\"Deutsch\",D3387,IF($B$1=\"中文\",E3387,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in washing and cleaning products, polishes and waxes and cosmetics and personal care products."},"Used in washing and cleaning products, polishes and waxes and cosmetics and personal care products.","Wasch- und Reinigungsmittel, Polituren, Wachse, Kosmetika und Körperpflegeprodukte","用于清洗和清洁产品、抛光剂和蜡类、化妆品及个人护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C3388,IF($B$1=\"Deutsch\",D3388,IF($B$1=\"中文\",E3388,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products, textile treatment products and dyes."},"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products, textile treatment products and dyes.","Wasch- und Reinigungsmittel, Polituren, Wachse, Kosmetika, Körperpflegeprodukte, Textilbehandlungsmittel und Farbstoffe","用于清洗和清洁产品、抛光剂和蜡类、化妆品和个人护理产品、纺织品处理产品和燃料。"]
[null,{"$f":"IF($B$1=\"English\",C3389,IF($B$1=\"Deutsch\",D3389,IF($B$1=\"中文\",E3389,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products."},"Used in washing and cleaning products, polishes and waxes, cosmetics and personal care products.","Wasch- und Reinigungsmittel, Polituren, Wachse, Kosmetika und Körperpflegeprodukte","用于清洗和清洁产品、抛光剂和蜡类、化妆品和个人护理产品。"]
[null,{"$f":"IF($B$1=\"English\",C3390,IF($B$1=\"Deutsch\",D3390,IF($B$1=\"中文\",E3390,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in metals, welding and soldering products, metal surface treatment products, and polymers."},"Used in metals, welding and soldering products, metal surface treatment products, and polymers.","Metalle, Karosserie- und Lötprodukte, Metalloberflächenbehandlungsprodukte und Polymere","用于金属、焊接和锡焊产品、金属表面处理产品及聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C3391,IF($B$1=\"Deutsch\",D3391,IF($B$1=\"中文\",E3391,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in anti-freeze products, heat transfer fluids, lubricants and greases, and washing and cleaning products."},"Used in anti-freeze products, heat transfer fluids, lubricants and greases, and washing and cleaning products.","Frostschutzmittel, Wärmeträgerflüssigkeiten, Gleit- und Schmiermittel, Wasch- und Reinigungsmittel","用于防冻产品、导热流体、润滑油和油脂，以及清洗和清洁产品。"]
[null,{"$f":"IF($B$1=\"English\",C3392,IF($B$1=\"Deutsch\",D3392,IF($B$1=\"中文\",E3392,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Not registered under REACH. Normally not produced intentionally but rather occurs as a constituent or impurity in other substances."},"Not registered under REACH. Normally not produced intentionally but rather occurs as a constituent or impurity in other substances.","Wird nicht absichtlich hergestellt, ist jedoch als Bestandteil oder Verunreinigung in anderen Stoffen","未根据REACH登记。一般不计划生产，但可构成或掺入其他物质。"]
[null,{"$f":"IF($B$1=\"English\",C3393,IF($B$1=\"Deutsch\",D3393,IF($B$1=\"中文\",E3393,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a plastic additive, solvent, in coatings/inks, in adhesives and sealants, and heat transfer fluids."},"Used as a plastic additive, solvent, in coatings/inks, in adhesives and sealants, and heat transfer fluids.","Kunststoffadditive, Lösemittel, Anstrichmittel, Tinten, Klebstoffe, Dichtungsmittel, Wärmeträgerflüssigkeiten","用作塑料添加剂、溶剂，用于涂料/墨水、胶粘剂和密封剂、导热流体。"]
[null,{"$f":"IF($B$1=\"English\",C3394,IF($B$1=\"Deutsch\",D3394,IF($B$1=\"中文\",E3394,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used in adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, pH regulators and water treatment products."},"Used in adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, pH regulators and water treatment products.","Klebstoffe, Dichtungsmittel, Anstrichmittel, Kitt, Füllmaterial, Mörtel, Modeliermasse, pH-Regulierer, Wasseraufbereitungsmittel","用于胶粘剂和密封剂、涂料产品、填充剂、油灰、灰泥、雕塑黏土、pH调节剂和水处理产品。"]
[null,{"$f":"IF($B$1=\"English\",C3395,IF($B$1=\"Deutsch\",D3395,IF($B$1=\"中文\",E3395,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"-"},"-","-","-"]
[null,{"$f":"IF($B$1=\"English\",C3396,IF($B$1=\"Deutsch\",D3396,IF($B$1=\"中文\",E3396,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Binder for refractory material"},"Binder for refractory material","Bindemittel für feuerfestes Material","耐火材料用粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C3397,IF($B$1=\"Deutsch\",D3397,IF($B$1=\"中文\",E3397,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Binder for refractory material"},"Binder for refractory material","Bindemittel für feuerfestes Material","耐火材料用粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C3398,IF($B$1=\"Deutsch\",D3398,IF($B$1=\"中文\",E3398,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Binder for refractory material"},"Binder for refractory material","Bindemittel für feuerfestes Material","耐火材料用粘合剂"]
[null,{"$f":"IF($B$1=\"English\",C3399,IF($B$1=\"Deutsch\",D3399,IF($B$1=\"中文\",E3399,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a transported intermediate for the manufacture of fine chemicals."},"Used as a transported intermediate for the manufacture of fine chemicals.","Als transportiertes Zwischenprodukt bei der Herstellung von Feinchemikalien","用作生产精细化学品的运输中间体。"]
[null,{"$f":"IF($B$1=\"English\",C3400,IF($B$1=\"Deutsch\",D3400,IF($B$1=\"中文\",E3400,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"UV filters in sunscreen and other cosmetics"},"UV filters in sunscreen and other cosmetics","UV-Filter in Sonnencreme und anderen Kosmetika","防晒霜和其他化妆品汇总的UV过滤成分"]
[null,{"$f":"IF($B$1=\"English\",C3401,IF($B$1=\"Deutsch\",D3401,IF($B$1=\"中文\",E3401,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvent  for  gums,  resins,  waxes,  and  oils  and  in  the \nmanufacture of semiconductors, textile printing and photographic films. paints, lacquers, stains, inks, surface coatings, \nsilk-screen  printing,  photographic  and  photo  lithographic  processes,  semiconductors,  textile, \nleather, hydraulic fluids, jet fuel, varnishes, paper, acetate adhesives, nitrocellulose, cellulose \nacetate,  gums,  resins,  waxes,  and  oils,  textile  printing  and  dry-cleaning.  Technical  functions \ninclude solvent, drying retarder, and anti-icing additive, viscosity decreasing agent.\n"},"Solvent  for  gums,  resins,  waxes,  and  oils  and  in  the \nmanufacture of semiconductors, textile printing and photographic films. paints, lacquers, stains, inks, surface coatings, \nsilk-screen  printing,  photographic  and  photo  lithographic  processes,  semiconductors,  textile, \nleather, hydraulic fluids, jet fuel, varnishes, paper, acetate adhesives, nitrocellulose, cellulose \nacetate,  gums,  resins,  waxes,  and  oils,  textile  printing  and  dry-cleaning.  Technical  functions \ninclude solvent, drying retarder, and anti-icing additive, viscosity decreasing agent.\n","Lösemittel für Gummi, Harze, Wachse und Öle und zur Herstellung von Halbleitern, Textildrucken und fotografischen Filmen verwendet. Einsatzmöglichkeiten in Farben, Lacken, Beizen, Druckfarben, Oberflächenbeschichtungen, Siebdruck, fotografischen und fotolithografischen Verfahren, Halbleitern, Textilien, Leder, Hydraulikflüssigkeiten, Düsentreibstoff, Papier, Acetatkleber, Nitrocellulose, Celluloseacetat, Textildruck und in der chemischer Reinigung.","树胶、树脂、蜡和油用溶剂，用于 \n生产半导体、纺织印花膜、油漆、涂料、染料、墨水、表面涂料、 \n丝网印刷、照相和光刻工艺、半导体、纺织品、 \n皮革、液压液、喷气燃料、清漆、纸张、醋酸胶、硝酸纤维、纤维素 \n醋酸纤维素、树胶、树脂、蜡、油类、纺织品印花和干洗。技术作用 \n包括溶剂、抗干燥剂、抗结冰添加剂、降粘剂。\n"]
[null,{"$f":"IF($B$1=\"English\",C3402,IF($B$1=\"Deutsch\",D3402,IF($B$1=\"中文\",E3402,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Primarily used as an antioxidant to stabilise polymers."},"Primarily used as an antioxidant to stabilise polymers.","TNPP wird hauptsächlich als Antioxidans zur Stabilisierung von Polymeren verwendet.","主要用作稳定聚合物的抗氧化剂。"]
[null,{"$f":"IF($B$1=\"English\",C3403,IF($B$1=\"Deutsch\",D3403,IF($B$1=\"中文\",E3403,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Processing aid in the production of fluorinated polymers."},"Processing aid in the production of fluorinated polymers.","Verarbeitungshilfe bei der Herstellung von fluorierten Polymeren.","生产含氟聚合物的加工助剂。"]
[null,{"$f":"IF($B$1=\"English\",C3404,IF($B$1=\"Deutsch\",D3404,IF($B$1=\"中文\",E3404,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mainly \nused in the phenolic/epoxy resin industry and is only used as an intermediate /in polymers\nUsed in coating products, polymers, adhesives, sealants and for the synthesis of other substances.\n"},"Mainly \nused in the phenolic/epoxy resin industry and is only used as an intermediate /in polymers\nUsed in coating products, polymers, adhesives, sealants and for the synthesis of other substances.\n","Hauptsächlich Einsatz in der Phenol-/Epoxidharzindustrie als Zwischenprodukt in Polymeren. Verwendung in Beschichtungsmaterial, Polymeren, Klebstoffen, Dicht-stoffen und zur Synthese anderer Stoffe.","主要 \n用于酚醛/环氧树脂工业，仅用作中间体/用于聚合物\n用于涂料产品、聚合物、胶粘剂、密封剂和其他物质的合成。\n"]
[null,{"$f":"IF($B$1=\"English\",C3405,IF($B$1=\"Deutsch\",D3405,IF($B$1=\"中文\",E3405,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diisohexyl phthalate is a component (the branched form) of 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear (EC 271-093-5; CAS 68515-50-4). There are indications for potential use of the substances in the same types of applications (e.g. as sealant, plasticiser in polymers etc)."},"Diisohexyl phthalate is a component (the branched form) of 1,2-benzenedicarboxylic acid, dihexyl ester, branched and linear (EC 271-093-5; CAS 68515-50-4). There are indications for potential use of the substances in the same types of applications (e.g. as sealant, plasticiser in polymers etc).","Diisohexyl phthalat ist in verzweigter Form Bestandteil von 1,2-Benzoldicarbonsäure Diehexylester, verzweigt und linear (EG-Nr. 271-093-5, CAS-Nr. 68515-50-4). Die Verwendungsbereiche sind deshalb vergleichbar (Weichmacher in Polymeren, Dich-tungsmaterial usw.).","邻苯二甲酸双-4-甲基-2-戊酯（支链）是1,2-苯二甲酸二己酯支链和直链（EC 271-093-5; CAS 68515-50-4）的成分。该物质可根据说明用于相同应用（如用作密封剂、聚合物塑化剂等）。"]
[null,{"$f":"IF($B$1=\"English\",C3406,IF($B$1=\"Deutsch\",D3406,IF($B$1=\"中文\",E3406,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone is used\nfor the production of printing inks and surface coating based on based on acrylates polymerized by UV radiation.\n"},"2-benzyl-2-dimethylamino-4'-morpholinobutyrophenone is used\nfor the production of printing inks and surface coating based on based on acrylates polymerized by UV radiation.\n","2-Benzyl-2-(dimethylamino)-4'-morpholinobutyrophenon wird zur Herstellung von Druckfarben und Oberflächenbeschichtungen auf Basis von durch UV-Strahlung po-lymerisierten Acrylaten verwendet.","2-苄基-2-二甲基氨基-1-(4-吗啉苯基)丁酮用于\n生产基于UV辐照聚合丙烯酸盐的印刷用油墨和表面涂料。\n"]
[null,{"$f":"IF($B$1=\"English\",C3407,IF($B$1=\"Deutsch\",D3407,IF($B$1=\"中文\",E3407,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Used as a catalyst/ additive/reactant in polymer manufacture and in chemical synthesis. It is also used as a flame retardant in polycarbonate (for electronic equipment)."},"Used as a catalyst/ additive/reactant in polymer manufacture and in chemical synthesis. It is also used as a flame retardant in polycarbonate (for electronic equipment).","Wird als Katalysator in der Polymerherstellung und in der chemischen Synthese sowie als Flammschutzmittel in Polycarbonat (bei elektroni-schen Geräten) verwendet.","用作聚合物生产和化学品合成中的催化剂/添加剂/反应物。此外，也可用作聚碳酸酯（电子设备用）的阻燃剂。"]
[null,{"$f":"IF($B$1=\"English\",C3408,IF($B$1=\"Deutsch\",D3408,IF($B$1=\"中文\",E3408,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Methyl-1- (4-methylthiophenyl) -2-morpholinopropan-1-one is used as a photoinitiator in the manufacture of formulations and (outer) packaging, coatings, adhesives, printing inks, fiber sizes."},"2-Methyl-1- (4-methylthiophenyl) -2-morpholinopropan-1-one is used as a photoinitiator in the manufacture of formulations and (outer) packaging, coatings, adhesives, printing inks, fiber sizes.","2-Methyl-1-(4-methylthiophenyl)-2-morpholinopropan-1-on wird als Photoinitiator bei der Herstellung von Formulierungen und (Um-)Verpackungen, Beschichtungen, Klebstoffen, Druckfarben, Faserschlichten verwendet.","2-甲基-1-(4-甲硫基苯)-2-吗啉基-1-丙酮在各种配方产品及（外）包装材料、涂层、胶粘剂、印刷用油墨、浸润剂生产中用作光引发剂。"]
[null,{"$f":"IF($B$1=\"English\",C3409,IF($B$1=\"Deutsch\",D3409,IF($B$1=\"中文\",E3409,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ECHA has no public registered data indicating whether or in which chemical products the substance might be used."},"ECHA has no public registered data indicating whether or in which chemical products the substance might be used.","Der ECHA liegen keine öffentlich registrierten Daten vor, aus denen hervorgeht, ob oder in welchen chemischen Produkten der Stoff verwendet werden könnte.","ECHA无公开登记数据说明可能化学产品中是否使用了该物质以及哪些化学品使用了该物质。"]
[null,{"$f":"IF($B$1=\"English\",C3410,IF($B$1=\"Deutsch\",D3410,IF($B$1=\"中文\",E3410,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ECHA has no public registered data indicating whether or in which chemical products the substance might be used."},"ECHA has no public registered data indicating whether or in which chemical products the substance might be used.","Der ECHA liegen keine öffentlich registrierten Daten vor, aus denen hervorgeht, ob oder in welchen chemischen Produkten der Stoff verwendet werden könnte.","ECHA无公开登记数据说明可能化学产品中是否使用了该物质以及哪些化学品使用了该物质。"]
[null,{"$f":"IF($B$1=\"English\",C3411,IF($B$1=\"Deutsch\",D3411,IF($B$1=\"中文\",E3411,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"This substance is used in the following products: cosmetics and personal care products and pharmaceuticals.\nOther release to the environment of this substance is likely to occur from: indoor use as processing aid"},"This substance is used in the following products: cosmetics and personal care products and pharmaceuticals.\nOther release to the environment of this substance is likely to occur from: indoor use as processing aid","Dieser Stoff wird in folgenden Produkten verwendet: Kosmetika und Körperpflegeprodukte sowie Arzneimittel.\nAndere Freisetzungen dieses Stoffes in die Umwelt sind wahrscheinlich durch: Verwendung in Innenräumen als Verarbeitungshilfsmittel","该物质用于以下产品：化妆品、个人护理产品和药品。\n该物质可能通过以下其他方式排放到环境中：室内用作加工助剂"]
[null,{"$f":"IF($B$1=\"English\",C3412,IF($B$1=\"Deutsch\",D3412,IF($B$1=\"中文\",E3412,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"This substance is used in the following products: adhesives and sealants."},"This substance is used in the following products: adhesives and sealants.","Dieser Stoff wird in folgenden Produkten verwendet: Klebstoffe und Dichtstoffe.","该物质用于以下产品：胶粘剂和密封剂。"]
[null,{"$f":"IF($B$1=\"English\",C3413,IF($B$1=\"Deutsch\",D3413,IF($B$1=\"中文\",E3413,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(2-(2-methoxyethoxy)ethyl)ether is used in inks and toners as a solvent or extractant. Industrial use as a gas absorption liquid, solvent in synthesis reactions or as an extractant."},"Bis(2-(2-methoxyethoxy)ethyl)ether is used in inks and toners as a solvent or extractant. Industrial use as a gas absorption liquid, solvent in synthesis reactions or as an extractant.","Bis(2-(2-methoxyethoxy)ethyl)ether wird in Tinten und Toner als Lösemittel oder Extraktionsmittel verwendet. Industrielle Verwendung als Gasabsorptionsflüssigkeit, Lösungsmittel in Synthesereaktionen oder als Extraktionsmittel.","双(2-(2-甲氧基乙氧基)乙基)酯作为溶剂或萃取剂用于墨水和墨粉。工业上用作气体吸收液、合成反应溶液或萃取剂。"]
[null,{"$f":"IF($B$1=\"English\",C3414,IF($B$1=\"Deutsch\",D3414,IF($B$1=\"中文\",E3414,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"The main ingredient dioctyltin dilaurate is used in adhesives and sealants and in the manufacture of plastic and rubber tyres"},"The main ingredient dioctyltin dilaurate is used in adhesives and sealants and in the manufacture of plastic and rubber tyres","Der Hauptbestandteil Dioctylzinndilaurat wird in Kleb- und Dichtstoffen sowie bei der Herstellung von Kunststoff- und Gummireifen verwendet","主要成分二月桂酸二正辛基锡用于胶粘剂和密封剂，以及用于塑料和橡胶轮胎的生产"]
[null,{"$f":"IF($B$1=\"English\",C3415,IF($B$1=\"Deutsch\",D3415,IF($B$1=\"中文\",E3415,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Preparation of lubricant additive materials and of fuel system cleaners."},"Preparation of lubricant additive materials and of fuel system cleaners.","Verwendung als chemisches Zwischenprodukt. Herstellung von Schmiermitteladditivmaterialien und von Kraftstoffsystemreinigern in benzin- und dieselbetriebenen Straßenfahrzeugen und Schiffsdieselmotoren. Herstellung von Chemikalien, Gummiprodukten und Kunststoffprodukten.","配制润滑剂添加剂材料及燃料系统清洁剂。"]
[null,{"$f":"IF($B$1=\"English\",C3416,IF($B$1=\"Deutsch\",D3416,IF($B$1=\"中文\",E3416,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Not registered under REACH. May be used as solvent and corrosion inhibitor. "},"Not registered under REACH. May be used as solvent and corrosion inhibitor. ","nicht unter REACH registriert, daher liegen keine Informationen zu Verwendungen vor. \nBegrenzte Informationen über die Verwendung als Lösungsmittel und Korrosionsinhibitor.","未根据REACH登记。可用作溶剂和阻蚀剂。 "]
[null,{"$f":"IF($B$1=\"English\",C3417,IF($B$1=\"Deutsch\",D3417,IF($B$1=\"中文\",E3417,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Flame retardants, plasticising additives in plastics, sealants, rubber and textiles"},"Flame retardants, plasticising additives in plastics, sealants, rubber and textiles","Verwendung als Flammschutzmittel und als sekundäre Weichmacheradditive in Kunststoffen, Dichtstoffen, Gummi und Textilien. Additive in Kühl- und Schmiermitteln in Maschinen und Herstellung von Metallprodukten.","阻燃剂、塑料用塑化添加剂、密封剂、橡胶和纺织品"]
[null,{"$f":"IF($B$1=\"English\",C3418,IF($B$1=\"Deutsch\",D3418,IF($B$1=\"中文\",E3418,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Biocides, leather tanning, x-ray film processing, cosmetics."},"Biocides, leather tanning, x-ray film processing, cosmetics.","Verwendung als Biozid, bei der Ledergerbung, Röntgenfilmverarbeitung und in der Kosmetikindustrie.","杀虫剂、皮革鞣制加工、x-射线胶片加工、化妆品。"]
[null,{"$f":"IF($B$1=\"English\",C3419,IF($B$1=\"Deutsch\",D3419,IF($B$1=\"中文\",E3419,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Not registered under REACH. May be used in manufacture of phenolic and polycarbonate resin. "},"Not registered under REACH. May be used in manufacture of phenolic and polycarbonate resin. ","nicht unter REACH registriert, daher liegen keine Informationen zu Verwendungen vor. Mögliche Verwendung: Herstellung von Phenol- und Polycarbonatharzen. Freisetzung aus Harzauskleidungen bei der Verwendung als Korrosionsinhibitoren zur Beschichtung von Dosen in der Lebensmittelindustrie.","未根据REACH登记。可用于上产酚醛树脂和聚碳酸酯树脂。 "]
[null,{"$f":"IF($B$1=\"English\",C3420,IF($B$1=\"Deutsch\",D3420,IF($B$1=\"中文\",E3420,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cleaning agents, cosmetics, in scented articles, polishes and wax blends."},"Cleaning agents, cosmetics, in scented articles, polishes and wax blends.","Duftstoff in der Kosmetikindustrie sowie in Wasch- und Reinigungsmitteln, Polituren und Wachsmischungen","清洁剂、化妆品、有香味的物品、抛光剂和蜡混合物。"]
[null,{"$f":"IF($B$1=\"English\",C3421,IF($B$1=\"Deutsch\",D3421,IF($B$1=\"中文\",E3421,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate."},"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate.","In der Polymerproduktion zur Herstellung von Kunststoffprodukten","TBNPA：聚合物塑料产品生产，包括复合、转化及作为中间体。"]
[null,{"$f":"IF($B$1=\"English\",C3422,IF($B$1=\"Deutsch\",D3422,IF($B$1=\"中文\",E3422,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate."},"TBNPA: polymer production manufacture of plastics products, including compounding and conversion and as an intermediate.","In der Polymerproduktion zur Herstellung von Kunststoffprodukten","TBNPA：聚合物塑料产品生产，包括复合、转化及作为中间体。"]
[null,{"$f":"IF($B$1=\"English\",C3423,IF($B$1=\"Deutsch\",D3423,IF($B$1=\"中文\",E3423,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"BMP: manufacture of polymer resins and in one component foam (OCPF) application."},"BMP: manufacture of polymer resins and in one component foam (OCPF) application.","an Industriestandorten als reaktives Flammschutzmittel-Zwischenprodukt bei der Herstellung von Polymerharzen verwendet","BMP：生产聚合物树脂，用于单组分泡沫（OCPF）应用。"]
[null,{"$f":"IF($B$1=\"English\",C3424,IF($B$1=\"Deutsch\",D3424,IF($B$1=\"中文\",E3424,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"DBPA: registered as an intermediate."},"DBPA: registered as an intermediate.","als Zwischenprodukt bei der Herstellung von Feinchemikalien und Chemikalien einschließlich der Herstellung von Massenchemikalien im großen Maßstab verwendet","DBPA：登记的中间体。"]
[null,{"$f":"IF($B$1=\"English\",C3425,IF($B$1=\"Deutsch\",D3425,IF($B$1=\"中文\",E3425,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Solvent."},"Solvent.","Lösungsmittel bei der Synthese von Chemikalien","溶剂。"]
[null,{"$f":"IF($B$1=\"English\",C3426,IF($B$1=\"Deutsch\",D3426,IF($B$1=\"中文\",E3426,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rubbers, plastics, sealants"},"Rubbers, plastics, sealants","Kautschuk, Kunststoff, Dichtstoffe","橡胶、塑料、密封剂"]
[null,{"$f":"IF($B$1=\"English\",C3427,IF($B$1=\"Deutsch\",D3427,IF($B$1=\"中文\",E3427,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lubricants, greases"},"Lubricants, greases","Schmierstoffe, Fette","润滑剂、油脂"]
[null,{"$f":"IF($B$1=\"English\",C3428,IF($B$1=\"Deutsch\",D3428,IF($B$1=\"中文\",E3428,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Rubbers, lubricants, adhesives, inks, fuels, gaskets"},"Rubbers, lubricants, adhesives, inks, fuels, gaskets","Kautschuk, Schmiermittel, Klebstoffe, Tinten, Kraftstoffe, Dichtungen","橡胶、润滑剂、胶粘剂、墨水、燃料、垫圈"]
[null,{"$f":"IF($B$1=\"English\",C3429,IF($B$1=\"Deutsch\",D3429,IF($B$1=\"中文\",E3429,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cosmetics"},"Cosmetics","Kosmetik","化妆品"]
[null,{"$f":"IF($B$1=\"English\",C3430,IF($B$1=\"Deutsch\",D3430,IF($B$1=\"中文\",E3430,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ECHA has no public registered data indicating whether or in which chemical products the substance might be used."},"ECHA has no public registered data indicating whether or in which chemical products the substance might be used.","ECHA has no public registered data indicating whether or in which chemical products the substance might be used.","ECHA无公开登记数据说明可能化学产品中是否使用了该物质以及哪些化学品使用了该物质。"]
[null,{"$f":"IF($B$1=\"English\",C3431,IF($B$1=\"Deutsch\",D3431,IF($B$1=\"中文\",E3431,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"While the substance itself is not registered under REACH, identification as an SVHC can be seen as a measure to avoid future regrettable substitution. "},"While the substance itself is not registered under REACH, identification as an SVHC can be seen as a measure to avoid future regrettable substitution. ","Auch wenn der Stoff selbst nicht im Rahmen von REACH registriert ist, kann die Identifizierung als besonders besorgniserregender Stoff als Maßnahme zur Vermeidung künftiger bedauerlicher Substitutionen angesehen werden. ","虽然该物质本身并未在REACH中登记，但可发现有将SVHC标识为一项测量指标，以避免以后可能发生的不当替换。 "]
[null,{"$f":"IF($B$1=\"English\",C3432,IF($B$1=\"Deutsch\",D3432,IF($B$1=\"中文\",E3432,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"As a reactive flame retardant and as an additive flame retardant in the manufacture of polymer resins, in products such as epoxy coated circuit boards, printed circuit boards, paper and textiles."},"As a reactive flame retardant and as an additive flame retardant in the manufacture of polymer resins, in products such as epoxy coated circuit boards, printed circuit boards, paper and textiles.","Als reaktives Flammschutzmittel und als additives Flammschutzmittel bei der Herstellung von Polymerharzen, in Produkten wie epoxidbeschichteten Leiterplatten, gedruckten Schaltungen, Papier und Textilien.","作为一种阻燃反应剂和添加剂，用于生产聚合物树脂、环氧树脂涂层电路板、打印电路板、纸张和纺织品等。"]
[null,{"$f":"IF($B$1=\"English\",C3433,IF($B$1=\"Deutsch\",D3433,IF($B$1=\"中文\",E3433,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"In the manufacture of: pulp, paper and paper products, textile, leather or fur and chemicals."},"In the manufacture of: pulp, paper and paper products, textile, leather or fur and chemicals.","Bei der Herstellung von: Zellstoff, Papier und Papierprodukten, Textilien, Leder oder Pelzen und Chemikalien.","用于生产：纸浆、纸张和纸产品、纺织品、皮革、毛皮和化学品。"]
[null,{"$f":"IF($B$1=\"English\",C3434,IF($B$1=\"Deutsch\",D3434,IF($B$1=\"中文\",E3434,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"In paints and coatings."},"In paints and coatings.","In Farben und Lacken..","用于油漆和涂料。"]
[null,{"$f":"IF($B$1=\"English\",C3435,IF($B$1=\"Deutsch\",D3435,IF($B$1=\"中文\",E3435,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"As a flame retardant and as a plasticiser for flexible polyvinylchloride and for use in wire and cable insulation, film and sheeting, carpet backing, coated fabrics, wall coverings and adhesives."},"As a flame retardant and as a plasticiser for flexible polyvinylchloride and for use in wire and cable insulation, film and sheeting, carpet backing, coated fabrics, wall coverings and adhesives.","Als Flammschutzmittel und als Weichmacher für flexibles Polyvinylchlorid und zur Verwendung in Draht- und Kabelisolierungen, Folien und Platten, Teppichrücken, beschichteten Geweben, Wandverkleidungen und Klebstoffen.","作为软质聚氯乙烯的阻燃剂和塑化，用于电线和电缆绝缘、薄膜和薄板、地毯底布、涂层布料、墙面材料及胶粘剂。"]
[null,{"$f":"IF($B$1=\"English\",C3436,IF($B$1=\"Deutsch\",D3436,IF($B$1=\"中文\",E3436,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"In the manufacture of substances and in the following products: coating products, fillers, putties, plasters, modelling clay and inks and toners."},"In the manufacture of substances and in the following products: coating products, fillers, putties, plasters, modelling clay and inks and toners.","Bei der Herstellung von Stoffen und in folgenden Produkten: Beschichtungsstoffe, Spachtelmassen, Kitte, Putze, Modelliermasse sowie Tinten und Toner.","用于生产以下物质及用于以下产品：涂料产品、填料、油灰、石膏、造型粘土以及油墨和调色剂。"]
[null,{"$f":"IF($B$1=\"English\",C3437,IF($B$1=\"Deutsch\",D3437,IF($B$1=\"中文\",E3437,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"In polymers and resins, coating products, adhesives and sealants, leather treatment products, laboratory chemicals."},"In polymers and resins, coating products, adhesives and sealants, leather treatment products, laboratory chemicals.","In Polymeren und Harzen, Beschichtungsprodukten, Klebstoffen und Dichtungsmitteln, Lederbehandlungsprodukten und Laborchemikalien.","聚合物和树脂、涂料产品、胶粘剂和密封剂、皮革处理产品、实验室化学品。"]
[null,{"$f":"IF($B$1=\"English\",C3438,IF($B$1=\"Deutsch\",D3438,IF($B$1=\"中文\",E3438,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"While the substance itself is not registered under REACH, identification as an SVHC can be seen as a measure to avoid future regrettable substitution."},"While the substance itself is not registered under REACH, identification as an SVHC can be seen as a measure to avoid future regrettable substitution.","Auch wenn der Stoff selbst nicht im Rahmen von REACH registriert ist, kann die Identifizierung als besonders besorgniserregender Stoff als Maßnahme zur Vermeidung künftiger bedauerlicher Substitutionen angesehen werden. ","虽然该物质本身并未在REACH中登记，但可发现有将SVHC标识为一项测量指标，以避免以后可能发生的不当替换。"]
[null,{"$f":"IF($B$1=\"English\",C3439,IF($B$1=\"Deutsch\",D3439,IF($B$1=\"中文\",E3439,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenol salts"},"Pentachlorophenol salts","Pentachlorophenol salts","五氯苯酚盐"]
[null,{"$f":"IF($B$1=\"English\",C3440,IF($B$1=\"Deutsch\",D3440,IF($B$1=\"中文\",E3440,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorophenol esters"},"Pentachlorophenol esters","Pentachlorophenol esters","五氯苯酚酯"]
[null,{"$f":"IF($B$1=\"English\",C3441,IF($B$1=\"Deutsch\",D3441,IF($B$1=\"中文\",E3441,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perchlorophenyl 5-oxo-L-prolinate"},"Perchlorophenyl 5-oxo-L-prolinate","Perchlorophenyl 5-oxo-L-prolinate","全氯苯基5-氧代-L-脯氨酸"]
[null,{"$f":"IF($B$1=\"English\",C3442,IF($B$1=\"Deutsch\",D3442,IF($B$1=\"中文\",E3442,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Zinc bis(pentachlorophenolate)"},"Zinc bis(pentachlorophenolate)","Zinc bis(pentachlorophenolate)","双（五氯酚）锌"]
[null,{"$f":"IF($B$1=\"English\",C3443,IF($B$1=\"Deutsch\",D3443,IF($B$1=\"中文\",E3443,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexane-1-sulphonic acid, its salts and related substances"},"Perfluorohexane-1-sulphonic acid, its salts and related substances","Perfluorohexane-1-sulphonic acid, its salts and related substances","全氟己烷-1-磺酸及其盐和相关物质"]
[null,{"$f":"IF($B$1=\"English\",C3444,IF($B$1=\"Deutsch\",D3444,IF($B$1=\"中文\",E3444,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟镓盐（9CI）"]
[null,{"$f":"IF($B$1=\"English\",C3445,IF($B$1=\"Deutsch\",D3445,IF($B$1=\"中文\",E3445,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium perfluorohexane-1-sulphonate"},"Potassium perfluorohexane-1-sulphonate","Potassium perfluorohexane-1-sulphonate","全氟己烷-1-磺酸钾"]
[null,{"$f":"IF($B$1=\"English\",C3446,IF($B$1=\"Deutsch\",D3446,IF($B$1=\"中文\",E3446,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟- 钪(3+)盐(3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3447,IF($B$1=\"Deutsch\",D3447,IF($B$1=\"中文\",E3447,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 锌盐"]
[null,{"$f":"IF($B$1=\"English\",C3448,IF($B$1=\"Deutsch\",D3448,IF($B$1=\"中文\",E3448,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 与三乙胺的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3449,IF($B$1=\"Deutsch\",D3449,IF($B$1=\"中文\",E3449,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3450,IF($B$1=\"Deutsch\",D3450,IF($B$1=\"中文\",E3450,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三苯基（苯甲基）-，1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3451,IF($B$1=\"Deutsch\",D3451,IF($B$1=\"中文\",E3451,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N,N-tributylbutan-1-aminium tridecafluorohexane-1-sulfonate"},"N,N,N-tributylbutan-1-aminium tridecafluorohexane-1-sulfonate","N,N,N-tributylbutan-1-aminium tridecafluorohexane-1-sulfonate","N,N,N-三丁基-1-丁氨十三氟乙烷-1-磺酸盐"]
[null,{"$f":"IF($B$1=\"English\",C3452,IF($B$1=\"Deutsch\",D3452,IF($B$1=\"中文\",E3452,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N,N,N-triethylethanaminium tridecafluorohexane-1-sulfonate"},"N,N,N-triethylethanaminium tridecafluorohexane-1-sulfonate","N,N,N-triethylethanaminium tridecafluorohexane-1-sulfonate","N,N,N-三乙基乙铵十三氟乙烷-1-磺酸盐"]
[null,{"$f":"IF($B$1=\"English\",C3453,IF($B$1=\"Deutsch\",D3453,IF($B$1=\"中文\",E3453,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. With pyrrolidine (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-,与吡咯烷的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3454,IF($B$1=\"Deutsch\",D3454,IF($B$1=\"中文\",E3454,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","乙铵, N-[4-[[4-(二乙氨基)苯基][4-(乙氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-乙基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3455,IF($B$1=\"Deutsch\",D3455,IF($B$1=\"中文\",E3455,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","N-[4-[[4-(二甲基氨基)苯基][4-(乙氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-甲基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸甲胺 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3456,IF($B$1=\"Deutsch\",D3456,IF($B$1=\"中文\",E3456,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," N-[4-[[4-(二甲基氨基)苯基][4-(苯氨基)-1-萘基]亚甲基]-2,5-环己二烯-1-亚基]-N-甲基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸甲胺 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3457,IF($B$1=\"Deutsch\",D3457,IF($B$1=\"中文\",E3457,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","β-环糊精，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸离子(1-)的化合物(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3458,IF($B$1=\"Deutsch\",D3458,IF($B$1=\"中文\",E3458,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)"},"Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-)(1:1)","γ-环糊精，与1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸离子(1-)的化合物(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3459,IF($B$1=\"Deutsch\",D3459,IF($B$1=\"中文\",E3459,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," 三苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3460,IF($B$1=\"Deutsch\",D3460,IF($B$1=\"中文\",E3460,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," 1-(羧甲基)-4-[2-[4-[4-(2,2-二苯基乙烯基)苯基]-1,2,3,3a,4,8b-六氢环五[b]吲哚-7-基]乙烯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸 喹啉(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3461,IF($B$1=\"Deutsch\",D3461,IF($B$1=\"中文\",E3461,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," 二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸碘 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3462,IF($B$1=\"Deutsch\",D3462,IF($B$1=\"中文\",E3462,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)"},"Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","Methanaminium, N,N,N-trimethyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","N,N,N-三甲基甲胺-, 与 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸的盐(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3463,IF($B$1=\"Deutsch\",D3463,IF($B$1=\"中文\",E3463,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 与 2-甲基-2-丙酰胺的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3464,IF($B$1=\"Deutsch\",D3464,IF($B$1=\"中文\",E3464,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","双[4-(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸碘(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3465,IF($B$1=\"Deutsch\",D3465,IF($B$1=\"中文\",E3465,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium perfluorohexane-1-sulphonate"},"Ammonium perfluorohexane-1-sulphonate","Ammonium perfluorohexane-1-sulphonate","全氟乙烷-1-磺酸铵"]
[null,{"$f":"IF($B$1=\"English\",C3466,IF($B$1=\"Deutsch\",D3466,IF($B$1=\"中文\",E3466,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)"},"Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)","Tridecafluorohexanesulphonic acid, compound with 2,2'-iminodiethanol (1:1)","十三氟乙烷磺酸，与 2,2'-亚氨基二乙醇的化合物 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3467,IF($B$1=\"Deutsch\",D3467,IF($B$1=\"中文\",E3467,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)"},"Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","双[(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-乙烷磺酸碘盐(1:1) (9CI)"]
[null,{"$f":"IF($B$1=\"English\",C3468,IF($B$1=\"Deutsch\",D3468,IF($B$1=\"中文\",E3468,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"," (4-甲基苯基)二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3469,IF($B$1=\"Deutsch\",D3469,IF($B$1=\"中文\",E3469,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","[4-[(2-甲基-1-氧代-2-丙烯-1-醇)氧基]苯基]二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍(1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3470,IF($B$1=\"Deutsch\",D3470,IF($B$1=\"中文\",E3470,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"},"Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate","Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1), polymer with 2-ethyltricyclo[3.3.1.13,7]dec-2-yl 2-methyl-2-propenoate, 3-hydroxytricyclo[3.3.1.13,7]dec-1-yl 2-methyl-2-propenoate and tetrahydro-2-oxo-3-furanyl 2-methyl-2-propenoate"," [4-[(2-甲基-1-氧代-2-丙烯基)氧基]苯基]二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍(1:1), 与 2-乙基三环[3.3.1.13,7]癸-2-醇 2-甲基-2-丙烯酸酯, 3-氢氧三环[3.3.1.13,7]癸-1-醇2-甲基-2-丙烯酸酯和四氢-2-氧代-3-呋喃基 2-甲基-2-丙烯酸酯的聚合物"]
[null,{"$f":"IF($B$1=\"English\",C3471,IF($B$1=\"Deutsch\",D3471,IF($B$1=\"中文\",E3471,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 铯盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3472,IF($B$1=\"Deutsch\",D3472,IF($B$1=\"中文\",E3472,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","二苯并[k,n][1,4,7,10,13]四噁噻环十五烷, 19-[4-(1,1-二甲基乙基)苯基]-6,7,9,10,12,13-六氢-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3473,IF($B$1=\"Deutsch\",D3473,IF($B$1=\"中文\",E3473,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-钕(3+) 盐(3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3474,IF($B$1=\"Deutsch\",D3474,IF($B$1=\"中文\",E3474,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","1-乙烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-钇(3+) 盐 (3:1)"]
[null,{"$f":"IF($B$1=\"English\",C3475,IF($B$1=\"Deutsch\",D3475,IF($B$1=\"中文\",E3475,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)"},"Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)","Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:2)","(硫代-4,1-亚苯基)双[二苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍盐 (1:2)"]
[null,{"$f":"IF($B$1=\"English\",C3476,IF($B$1=\"Deutsch\",D3476,IF($B$1=\"中文\",E3476,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic"},"Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","双[4-(1,1-二甲基丙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸碘"]
[null,{"$f":"IF($B$1=\"English\",C3477,IF($B$1=\"Deutsch\",D3477,IF($B$1=\"中文\",E3477,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","三[4-(1,1-二甲基乙基)苯基]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-己烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3478,IF($B$1=\"Deutsch\",D3478,IF($B$1=\"中文\",E3478,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)"},"1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","1-己烷磺酸, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-, 锂盐 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3479,IF($B$1=\"Deutsch\",D3479,IF($B$1=\"中文\",E3479,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)"},"Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","双(4-甲基苯基)苯基-, 1,1,2,2,3,3,4,4,5,5,6,6,6-十三氟-1-乙烷磺酸锍 (1:1)"]
[null,{"$f":"IF($B$1=\"English\",C3480,IF($B$1=\"Deutsch\",D3480,IF($B$1=\"中文\",E3480,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctane sulfonic acid and its derivatives (PFOS)\nPerfluorooctane sulfonates (PFOS) C8F17SO2X (X = OH, Metal salt (O-M+), halide, amide, and other derivatives including polymers)\n"},"Perfluorooctane sulfonic acid and its derivatives (PFOS)\nPerfluorooctane sulfonates (PFOS) C8F17SO2X (X = OH, Metal salt (O-M+), halide, amide, and other derivatives including polymers)\n","Perfluorooctane sulfonic acid and its derivatives (PFOS)\nPerfluorooctane sulfonates (PFOS) C8F17SO2X (X = OH, Metal salt (O-M+), halide, amide, and other derivatives including polymers)\n","全氟己烷磺酸及其衍生物(PFOS)\n全氟己烷磺酸 (PFOS) C8F17SO2X (X = OH,金属盐(O-M+), 卤化物、酰胺及其他衍生物，包括聚合物)\n"]
[null,{"$f":"IF($B$1=\"English\",C3481,IF($B$1=\"Deutsch\",D3481,IF($B$1=\"中文\",E3481,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctanoic acid (PFOA), its salts and PFOA-related substances"},"Perfluorooctanoic acid (PFOA), its salts and PFOA-related substances","Perfluorooctanoic acid (PFOA), its salts and PFOA-related substances","全氟辛酸 (PFOA)及其盐和PFOA相关物质"]
[null,{"$f":"IF($B$1=\"English\",C3482,IF($B$1=\"Deutsch\",D3482,IF($B$1=\"中文\",E3482,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecanol"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecanol","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecanol","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，16-二十九氟十六醇"]
[null,{"$f":"IF($B$1=\"English\",C3483,IF($B$1=\"Deutsch\",D3483,IF($B$1=\"中文\",E3483,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl dihydrogen phosphate"},"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl dihydrogen phosphate","4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl dihydrogen phosphate","4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，13，13，13-二十氟-2-羟基-12-（三氟甲基）二氢磷酸十三烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3484,IF($B$1=\"Deutsch\",D3484,IF($B$1=\"中文\",E3484,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl dihydrogen phosphate"},"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl dihydrogen phosphate","4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl dihydrogen phosphate","4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，15，15，15-二十四氟-2-羟基-14-（三氟甲基）二氢磷酸十五烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3485,IF($B$1=\"Deutsch\",D3485,IF($B$1=\"中文\",E3485,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl dihydrogen phosphate"},"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl dihydrogen phosphate","4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl dihydrogen phosphate","4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，17，17，17-二十八氟-2-羟基-16-（三氟甲基）二氢磷酸十七烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3486,IF($B$1=\"Deutsch\",D3486,IF($B$1=\"中文\",E3486,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodohexadecane"},"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodohexadecane","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodohexadecane","1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14-二十九氟-16-碘十六烷"]
[null,{"$f":"IF($B$1=\"English\",C3487,IF($B$1=\"Deutsch\",D3487,IF($B$1=\"中文\",E3487,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-nonadecafluoro-11-iodoundecane"},"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-nonadecafluoro-11-iodoundecane","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-nonadecafluoro-11-iodoundecane","1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9-十九氟-11-碘十一烷"]
[null,{"$f":"IF($B$1=\"English\",C3488,IF($B$1=\"Deutsch\",D3488,IF($B$1=\"中文\",E3488,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs."},"Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs.","Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs.","次膦酸，双（全氟-C6-12-烷基）衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3489,IF($B$1=\"Deutsch\",D3489,IF($B$1=\"中文\",E3489,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-(carboxylatomethyl)-1-(2-hydroxyethyl)-4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-oxodecyl)piperazinium"},"1-(carboxylatomethyl)-1-(2-hydroxyethyl)-4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-oxodecyl)piperazinium","1-(carboxylatomethyl)-1-(2-hydroxyethyl)-4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-oxodecyl)piperazinium","1-（羧基甲基）-1-（2-羟乙基）-4-（2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十九氟-1-氧代癸基）哌嗪"]
[null,{"$f":"IF($B$1=\"English\",C3490,IF($B$1=\"Deutsch\",D3490,IF($B$1=\"中文\",E3490,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Carboxylic acids, C7-13, perfluoro, ammonium salts"},"Carboxylic acids, C7-13, perfluoro, ammonium salts","Carboxylic acids, C7-13, perfluoro, ammonium salts","羧酸，C7-13，全氟，铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3491,IF($B$1=\"Deutsch\",D3491,IF($B$1=\"中文\",E3491,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-icosafluoro-11-(trifluoromethyl)dodecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-icosafluoro-11-(trifluoromethyl)dodecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-icosafluoro-11-(trifluoromethyl)dodecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，12，12，12-二十氟-11-（三氟甲基）甲基丙烯酸十二酯"]
[null,{"$f":"IF($B$1=\"English\",C3492,IF($B$1=\"Deutsch\",D3492,IF($B$1=\"中文\",E3492,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，14，14，14-二十四氟-13-（三氟甲基）甲基丙烯酸十四酯"]
[null,{"$f":"IF($B$1=\"English\",C3493,IF($B$1=\"Deutsch\",D3493,IF($B$1=\"中文\",E3493,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptadecafluoro-1-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]nonene"},"Heptadecafluoro-1-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]nonene","Heptadecafluoro-1-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]nonene","十七氟-1-[(2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟辛基）氧基]壬烯"]
[null,{"$f":"IF($B$1=\"English\",C3494,IF($B$1=\"Deutsch\",D3494,IF($B$1=\"中文\",E3494,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, γ-ω-perfluoro-C8-14-alkyl esters"},"2-Propenoic acid, γ-ω-perfluoro-C8-14-alkyl esters","2-Propenoic acid, γ-ω-perfluoro-C8-14-alkyl esters","2-丙烯酸，γ-ω-全氟-C8-14-烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3495,IF($B$1=\"Deutsch\",D3495,IF($B$1=\"中文\",E3495,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, perfluoro-C8-16-alkyl esters"},"2-Propenoic acid, perfluoro-C8-16-alkyl esters","2-Propenoic acid, perfluoro-C8-16-alkyl esters","2-丙烯酸，全氟-C8-16-烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3496,IF($B$1=\"Deutsch\",D3496,IF($B$1=\"中文\",E3496,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-(3-aminopropyl)-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide"},"N-(3-aminopropyl)-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide","N-(3-aminopropyl)-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide","N-（3-氨丙基）-2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟辛酰胺"]
[null,{"$f":"IF($B$1=\"English\",C3497,IF($B$1=\"Deutsch\",D3497,IF($B$1=\"中文\",E3497,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, pentadecafluoro-, branched"},"Octanoic acid, pentadecafluoro-, branched","Octanoic acid, pentadecafluoro-, branched","辛酸，十五氟-，支链"]
[null,{"$f":"IF($B$1=\"English\",C3498,IF($B$1=\"Deutsch\",D3498,IF($B$1=\"中文\",E3498,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octanoic acid, pentadecafluoro-, branched, ammonium salt"},"Octanoic acid, pentadecafluoro-, branched, ammonium salt","Octanoic acid, pentadecafluoro-, branched, ammonium salt","辛酸，十五氟-，支链，铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3499,IF($B$1=\"Deutsch\",D3499,IF($B$1=\"中文\",E3499,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkyl iodides, C6-18, perfluoro"},"Alkyl iodides, C6-18, perfluoro","Alkyl iodides, C6-18, perfluoro","烷基碘，C6-18，全氟"]
[null,{"$f":"IF($B$1=\"English\",C3500,IF($B$1=\"Deutsch\",D3500,IF($B$1=\"中文\",E3500,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Amides, C7-19, α-ω-perfluoro-N,N-bis(hydroxyethyl)"},"Amides, C7-19, α-ω-perfluoro-N,N-bis(hydroxyethyl)","Amides, C7-19, α-ω-perfluoro-N,N-bis(hydroxyethyl)","酰胺，C7-19，α-ω-全氟-N，N-双（羟乙基）"]
[null,{"$f":"IF($B$1=\"English\",C3501,IF($B$1=\"Deutsch\",D3501,IF($B$1=\"中文\",E3501,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fatty acids, C7-19, perfluoro"},"Fatty acids, C7-19, perfluoro","Fatty acids, C7-19, perfluoro","脂肪酸，C7-19，全氟"]
[null,{"$f":"IF($B$1=\"English\",C3502,IF($B$1=\"Deutsch\",D3502,IF($B$1=\"中文\",E3502,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl acrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl acrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl acrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，16，16，16-二十八氟-15-（三氟甲基）丙烯酸十六酯"]
[null,{"$f":"IF($B$1=\"English\",C3503,IF($B$1=\"Deutsch\",D3503,IF($B$1=\"中文\",E3503,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs., aluminum salts"},"Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs., aluminum salts","Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs., aluminum salts","次膦酸，双（全氟-C6-12-烷基）衍生物，铝盐"]
[null,{"$f":"IF($B$1=\"English\",C3504,IF($B$1=\"Deutsch\",D3504,IF($B$1=\"中文\",E3504,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1'-[oxybis[(1-methylethylene)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol]"},"1,1'-[oxybis[(1-methylethylene)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol]","1,1'-[oxybis[(1-methylethylene)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol]","1，1'-[氧基双[（1-甲基乙烯）氧基]]双[4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，15-二十五氟十五烷-2-醇]"]
[null,{"$f":"IF($B$1=\"English\",C3505,IF($B$1=\"Deutsch\",D3505,IF($B$1=\"中文\",E3505,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2-carboxylatoethyl)(dimethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl)amino]propyl]ammonium"},"(2-carboxylatoethyl)(dimethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl)amino]propyl]ammonium","(2-carboxylatoethyl)(dimethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl)amino]propyl]ammonium","（2-羧酸乙酯)（二甲基）[3-[（4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，15-二十五氟-2-羟基十五烷基）氨基]丙基]铵"]
[null,{"$f":"IF($B$1=\"English\",C3506,IF($B$1=\"Deutsch\",D3506,IF($B$1=\"中文\",E3506,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2-carboxylatoethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl)amino]propyl]dimethylammonium"},"(2-carboxylatoethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl)amino]propyl]dimethylammonium","(2-carboxylatoethyl)[3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl)amino]propyl]dimethylammonium","（2-羧酸乙酯)[3-[(4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，13-二十一氟-2-羟基十三烷基)氨基]丙基]二甲基铵"]
[null,{"$f":"IF($B$1=\"English\",C3507,IF($B$1=\"Deutsch\",D3507,IF($B$1=\"中文\",E3507,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"(2-carboxylatoethyl)(dimethyl)[[[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl]amino]propyl]mmonium"},"(2-carboxylatoethyl)(dimethyl)[[[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl]amino]propyl]mmonium","(2-carboxylatoethyl)(dimethyl)[[[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl]amino]propyl]mmonium","（2-羧酸乙酯）（二甲基）[[[4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，15，15，15-二十四氟-2-羟基-14-（三氟甲基）十五烷基]氨基]丙基]铵"]
[null,{"$f":"IF($B$1=\"English\",C3508,IF($B$1=\"Deutsch\",D3508,IF($B$1=\"中文\",E3508,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl phosphate"},"Diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl phosphate","Diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl phosphate","二胺3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸基磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3509,IF($B$1=\"Deutsch\",D3509,IF($B$1=\"中文\",E3509,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctylethyldimethylchlorosilane;Perfluorooctylethyldimethylchlorosilane"},"Perfluorooctylethyldimethylchlorosilane;Perfluorooctylethyldimethylchlorosilane","Perfluorooctylethyldimethylchlorosilane;Perfluorooctylethyldimethylchlorosilane","全氟辛基乙基二甲基氯硅烷；全氟辛基乙基二甲基氯硅烷"]
[null,{"$f":"IF($B$1=\"English\",C3510,IF($B$1=\"Deutsch\",D3510,IF($B$1=\"中文\",E3510,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl acrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl acrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl acrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，17，18，18，18-三十二氟-17-（三氟甲基）丙烯酸十八烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3511,IF($B$1=\"Deutsch\",D3511,IF($B$1=\"中文\",E3511,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，16，16，16-二十八氟-15-（三氟甲基）甲基丙烯酸十六烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3512,IF($B$1=\"Deutsch\",D3512,IF($B$1=\"中文\",E3512,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，17，18，18，18-三十二氟-17-（三氟甲基）甲基丙烯酸十八酯"]
[null,{"$f":"IF($B$1=\"English\",C3513,IF($B$1=\"Deutsch\",D3513,IF($B$1=\"中文\",E3513,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl dihydrogen phosphate"},"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl dihydrogen phosphate","4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl dihydrogen phosphate","4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，13-二十一氟-2-羟基十三烷基二氢磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3514,IF($B$1=\"Deutsch\",D3514,IF($B$1=\"中文\",E3514,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol"},"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol","1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoropentadecan-2-ol","1-[[3-（二甲氨基）丙基]氨基]-4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，15-二十五氟十五烷-2-醇"]
[null,{"$f":"IF($B$1=\"English\",C3515,IF($B$1=\"Deutsch\",D3515,IF($B$1=\"中文\",E3515,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluorotridecan-2-ol"},"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluorotridecan-2-ol","1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluorotridecan-2-ol","1-[[3-（二甲氨基）丙基]氨基]-4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，13-二十一氟十三烷-2-醇"]
[null,{"$f":"IF($B$1=\"English\",C3516,IF($B$1=\"Deutsch\",D3516,IF($B$1=\"中文\",E3516,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)pentadecan-2-ol"},"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)pentadecan-2-ol","1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)pentadecan-2-ol","1-[[3-（二甲氨基）丙基]氨基]-4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，15，15，15-二十四氟-14-（三氟甲基）十五烷-2-醇"]
[null,{"$f":"IF($B$1=\"English\",C3517,IF($B$1=\"Deutsch\",D3517,IF($B$1=\"中文\",E3517,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-12-(trifluoromethyl)tridecan-1-ol"},"1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-12-(trifluoromethyl)tridecan-1-ol","1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-12-(trifluoromethyl)tridecan-1-ol","1-[[3-（二甲氨基）丙基]氨基]-4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，13，13，13-二十氟-12-（三氟甲基）十三烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3518,IF($B$1=\"Deutsch\",D3518,IF($B$1=\"中文\",E3518,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，11-十七氟-2-羟基十一烷基磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3519,IF($B$1=\"Deutsch\",D3519,IF($B$1=\"中文\",E3519,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-henicosafluoro-2-hydroxytridecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，13-二十一氟-2-羟基十三烷基磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3520,IF($B$1=\"Deutsch\",D3520,IF($B$1=\"中文\",E3520,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，15-二十五氟-2-羟基十五烷基磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3521,IF($B$1=\"Deutsch\",D3521,IF($B$1=\"中文\",E3521,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonacosafluoro-2-hydroxyheptadecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonacosafluoro-2-hydroxyheptadecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonacosafluoro-2-hydroxyheptadecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，17，17，17-二十九氟-2-羟基十七烷基磷酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3522,IF($B$1=\"Deutsch\",D3522,IF($B$1=\"中文\",E3522,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，13，13，13-二十氟-2-羟基-12-（三氟甲基）磷酸十三烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3523,IF($B$1=\"Deutsch\",D3523,IF($B$1=\"中文\",E3523,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，15，15，15-二十四氟-2-羟基-14-（三氟甲基）磷酸十五烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3524,IF($B$1=\"Deutsch\",D3524,IF($B$1=\"中文\",E3524,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl phosphate"},"Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl phosphate","Diammonium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl phosphate","二胺4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，17，17，17-二十八氟-2-羟基-16-（三氟甲基）磷酸十七烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3525,IF($B$1=\"Deutsch\",D3525,IF($B$1=\"中文\",E3525,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Carbamic acid, [2-(sulfothio)ethyl]-, C-(γ-ω-perfluoro-C6-9-alkyl) esters, monosodium salts"},"Carbamic acid, [2-(sulfothio)ethyl]-, C-(γ-ω-perfluoro-C6-9-alkyl) esters, monosodium salts","Carbamic acid, [2-(sulfothio)ethyl]-, C-(γ-ω-perfluoro-C6-9-alkyl) esters, monosodium salts","氨基甲酸，[2-（磺硫基）乙基]-，C-(γ-ω-全氟-C6-9-烷基）酯，单钠盐"]
[null,{"$f":"IF($B$1=\"English\",C3526,IF($B$1=\"Deutsch\",D3526,IF($B$1=\"中文\",E3526,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)silane"},"Triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)silane","Triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)silane","三乙氧基（3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸基磷酸酯）硅烷"]
[null,{"$f":"IF($B$1=\"English\",C3527,IF($B$1=\"Deutsch\",D3527,IF($B$1=\"中文\",E3527,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctylethyltrichlorosilane;Perfluorooctylethyltrichlorosilane"},"Perfluorooctylethyltrichlorosilane;Perfluorooctylethyltrichlorosilane","Perfluorooctylethyltrichlorosilane;Perfluorooctylethyltrichlorosilane","全氟辛基乙基三氯硅烷；全氟辛基乙基三氯硅烷"]
[null,{"$f":"IF($B$1=\"English\",C3528,IF($B$1=\"Deutsch\",D3528,IF($B$1=\"中文\",E3528,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonadecafluoro-9-iodononane"},"Nonadecafluoro-9-iodononane","Nonadecafluoro-9-iodononane","十九氟-9-碘壬烷"]
[null,{"$f":"IF($B$1=\"English\",C3529,IF($B$1=\"Deutsch\",D3529,IF($B$1=\"中文\",E3529,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Icosafluoro-10-iodo-2-(trifluoromethyl)decane"},"Icosafluoro-10-iodo-2-(trifluoromethyl)decane","Icosafluoro-10-iodo-2-(trifluoromethyl)decane","二十氟-10-碘-2-（三氟甲基）癸烷"]
[null,{"$f":"IF($B$1=\"English\",C3530,IF($B$1=\"Deutsch\",D3530,IF($B$1=\"中文\",E3530,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecan-1-ol"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecan-1-ol","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecan-1-ol","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸烷-1-醇"]
[null,{"$f":"IF($B$1=\"English\",C3531,IF($B$1=\"Deutsch\",D3531,IF($B$1=\"中文\",E3531,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) hydrogen phosphate"},"Bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) hydrogen phosphate","Bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) hydrogen phosphate","双（3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸基磷酸酯）磷酸氢盐"]
[null,{"$f":"IF($B$1=\"English\",C3532,IF($B$1=\"Deutsch\",D3532,IF($B$1=\"中文\",E3532,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecanol"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecanol","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecanol","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-二十一氟十二醇"]
[null,{"$f":"IF($B$1=\"English\",C3533,IF($B$1=\"Deutsch\",D3533,IF($B$1=\"中文\",E3533,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl] hydrogen phosphate"},"Bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl] hydrogen phosphate","Bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl] hydrogen phosphate","双[3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-二十一氟十二烷基]磷酸氢盐"]
[null,{"$f":"IF($B$1=\"English\",C3534,IF($B$1=\"Deutsch\",D3534,IF($B$1=\"中文\",E3534,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-甲基丙烯酸十七氟癸酯"]
[null,{"$f":"IF($B$1=\"English\",C3535,IF($B$1=\"Deutsch\",D3535,IF($B$1=\"中文\",E3535,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iododecane"},"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iododecane","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iododecane","1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8-十七氟-10-癸基碘"]
[null,{"$f":"IF($B$1=\"English\",C3536,IF($B$1=\"Deutsch\",D3536,IF($B$1=\"中文\",E3536,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-henicosafluoro-12-iodododecane"},"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-henicosafluoro-12-iodododecane","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-henicosafluoro-12-iodododecane","1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10-二十一氟-12-碘十二烷"]
[null,{"$f":"IF($B$1=\"English\",C3537,IF($B$1=\"Deutsch\",D3537,IF($B$1=\"中文\",E3537,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-甲基丙烯酸二十一氟十二烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3538,IF($B$1=\"Deutsch\",D3538,IF($B$1=\"中文\",E3538,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Potassium perfluorooctanoate"},"Potassium perfluorooctanoate","Potassium perfluorooctanoate","全氟辛酸钾"]
[null,{"$f":"IF($B$1=\"English\",C3539,IF($B$1=\"Deutsch\",D3539,IF($B$1=\"中文\",E3539,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethyl perfluorooctanoate"},"Ethyl perfluorooctanoate","Ethyl perfluorooctanoate","全氟辛酸乙酯"]
[null,{"$f":"IF($B$1=\"English\",C3540,IF($B$1=\"Deutsch\",D3540,IF($B$1=\"中文\",E3540,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-tetracosafluoro-12-iodo-2-(trifluoromethyl)dodecane"},"1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-tetracosafluoro-12-iodo-2-(trifluoromethyl)dodecane","1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-tetracosafluoro-12-iodo-2-(trifluoromethyl)dodecane","1，1，1，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12-二十四氟-12-碘-2-（三氟甲基）十二烷"]
[null,{"$f":"IF($B$1=\"English\",C3541,IF($B$1=\"Deutsch\",D3541,IF($B$1=\"中文\",E3541,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octacosafluoro-14-iodo-2-(trifluoromethyl)tetradecane"},"Octacosafluoro-14-iodo-2-(trifluoromethyl)tetradecane","Octacosafluoro-14-iodo-2-(trifluoromethyl)tetradecane","二十八氟-14-碘-2-（三氟甲基）十四烷"]
[null,{"$f":"IF($B$1=\"English\",C3542,IF($B$1=\"Deutsch\",D3542,IF($B$1=\"中文\",E3542,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ammonium pentadecafluorooctanoate"},"Ammonium pentadecafluorooctanoate","Ammonium pentadecafluorooctanoate","十五氟辛酸铵"]
[null,{"$f":"IF($B$1=\"English\",C3543,IF($B$1=\"Deutsch\",D3543,IF($B$1=\"中文\",E3543,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-ethylheptadecafluorooctanesulphonamide"},"N-ethylheptadecafluorooctanesulphonamide","N-ethylheptadecafluorooctanesulphonamide","N-乙基全氟辛基磺酰胺"]
[null,{"$f":"IF($B$1=\"English\",C3544,IF($B$1=\"Deutsch\",D3544,IF($B$1=\"中文\",E3544,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，16-二十九氟十六烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3545,IF($B$1=\"Deutsch\",D3545,IF($B$1=\"中文\",E3545,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl methacrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl methacrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl methacrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，14-二十五氟十四烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3546,IF($B$1=\"Deutsch\",D3546,IF($B$1=\"中文\",E3546,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl acrylate"},"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl acrylate","4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl acrylate","4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，17，17，17-二十八氟-2-羟基-16-（三氟甲基）丙烯酸十七酯"]
[null,{"$f":"IF($B$1=\"English\",C3547,IF($B$1=\"Deutsch\",D3547,IF($B$1=\"中文\",E3547,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl acrylate"},"4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl acrylate","4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl acrylate","4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，15，15，15-二十四氟-2-羟基-14-（三氟甲基）丙烯酸十五酯"]
[null,{"$f":"IF($B$1=\"English\",C3548,IF($B$1=\"Deutsch\",D3548,IF($B$1=\"中文\",E3548,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl acrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl acrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl acrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-丙烯酸二十一氟十二烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3549,IF($B$1=\"Deutsch\",D3549,IF($B$1=\"中文\",E3549,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,4-bis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]benzenesulphonyl chloride"},"3,4-bis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]benzenesulphonyl chloride","3,4-bis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]benzenesulphonyl chloride","3，4-双[（2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟-1-氧辛基）氨基]苯磺酰氯"]
[null,{"$f":"IF($B$1=\"English\",C3550,IF($B$1=\"Deutsch\",D3550,IF($B$1=\"中文\",E3550,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-bromohenicosafluorodecane"},"1-bromohenicosafluorodecane","1-bromohenicosafluorodecane","1-溴全氟癸烷"]
[null,{"$f":"IF($B$1=\"English\",C3551,IF($B$1=\"Deutsch\",D3551,IF($B$1=\"中文\",E3551,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-12-iodododecane"},"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-12-iodododecane","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-12-iodododecane","1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12-二十五氟-12-碘十二烷"]
[null,{"$f":"IF($B$1=\"English\",C3552,IF($B$1=\"Deutsch\",D3552,IF($B$1=\"中文\",E3552,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonacosafluoro-1-iodotetradecane"},"Nonacosafluoro-1-iodotetradecane","Nonacosafluoro-1-iodotetradecane","二十九氟-1-碘十四烷"]
[null,{"$f":"IF($B$1=\"English\",C3553,IF($B$1=\"Deutsch\",D3553,IF($B$1=\"中文\",E3553,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentadecafluorooctyl fluoride"},"Pentadecafluorooctyl fluoride","Pentadecafluorooctyl fluoride","十五氟辛氟"]
[null,{"$f":"IF($B$1=\"English\",C3554,IF($B$1=\"Deutsch\",D3554,IF($B$1=\"中文\",E3554,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentadecafluorooctanoic acid"},"Pentadecafluorooctanoic acid","Pentadecafluorooctanoic acid","十五氟辛酸"]
[null,{"$f":"IF($B$1=\"English\",C3555,IF($B$1=\"Deutsch\",D3555,IF($B$1=\"中文\",E3555,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silver(1+) perfluorooctanoate"},"Silver(1+) perfluorooctanoate","Silver(1+) perfluorooctanoate","十五氟辛酸银（1+）"]
[null,{"$f":"IF($B$1=\"English\",C3556,IF($B$1=\"Deutsch\",D3556,IF($B$1=\"中文\",E3556,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sodium pentadecafluorooctanoate"},"Sodium pentadecafluorooctanoate","Sodium pentadecafluorooctanoate","十五氟辛酸钠"]
[null,{"$f":"IF($B$1=\"English\",C3557,IF($B$1=\"Deutsch\",D3557,IF($B$1=\"中文\",E3557,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Methyl perfluorooctanoate"},"Methyl perfluorooctanoate","Methyl perfluorooctanoate","十五氟辛酸甲酯"]
[null,{"$f":"IF($B$1=\"English\",C3558,IF($B$1=\"Deutsch\",D3558,IF($B$1=\"中文\",E3558,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Henicosafluoro-10-iododecane"},"Henicosafluoro-10-iododecane","Henicosafluoro-10-iododecane","二十一氟-10-癸基碘"]
[null,{"$f":"IF($B$1=\"English\",C3559,IF($B$1=\"Deutsch\",D3559,IF($B$1=\"中文\",E3559,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptadecafluoro-1-iodooctane"},"Heptadecafluoro-1-iodooctane","Heptadecafluoro-1-iodooctane","十七氟-1-碘辛烷"]
[null,{"$f":"IF($B$1=\"English\",C3560,IF($B$1=\"Deutsch\",D3560,IF($B$1=\"中文\",E3560,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctylethyltrimethoxysilane;Perfluorooctylethyltrimethoxysilane"},"Perfluorooctylethyltrimethoxysilane;Perfluorooctylethyltrimethoxysilane","Perfluorooctylethyltrimethoxysilane;Perfluorooctylethyltrimethoxysilane","全氟辛基乙基三甲氧基硅烷；全氟辛基乙基三甲氧基硅烷"]
[null,{"$f":"IF($B$1=\"English\",C3561,IF($B$1=\"Deutsch\",D3561,IF($B$1=\"中文\",E3561,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctylethyldichloromethyl silane;Perfluorooctylethyldichloromethyl silane"},"Perfluorooctylethyldichloromethyl silane;Perfluorooctylethyldichloromethyl silane","Perfluorooctylethyldichloromethyl silane;Perfluorooctylethyldichloromethyl silane","全氟辛基乙基二氯甲基硅烷；全氟辛基乙基二氯甲基硅烷"]
[null,{"$f":"IF($B$1=\"English\",C3562,IF($B$1=\"Deutsch\",D3562,IF($B$1=\"中文\",E3562,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Thiols, C8-20, γ-ω-perfluoro, telomers with acrylamide"},"Thiols, C8-20, γ-ω-perfluoro, telomers with acrylamide","Thiols, C8-20, γ-ω-perfluoro, telomers with acrylamide","硫醇，C8-20，γ-ω-全氟，丙烯酰胺调聚物"]
[null,{"$f":"IF($B$1=\"English\",C3563,IF($B$1=\"Deutsch\",D3563,IF($B$1=\"中文\",E3563,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chromium(3+) perfluorooctanoate"},"Chromium(3+) perfluorooctanoate","Chromium(3+) perfluorooctanoate","全氟辛酸铬（3+）"]
[null,{"$f":"IF($B$1=\"English\",C3564,IF($B$1=\"Deutsch\",D3564,IF($B$1=\"中文\",E3564,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Propanamide, 3-[(γ-ω-perfluoro-C4-10-alkyl)thio] derivs."},"Propanamide, 3-[(γ-ω-perfluoro-C4-10-alkyl)thio] derivs.","Propanamide, 3-[(γ-ω-perfluoro-C4-10-alkyl)thio] derivs.","丙酰胺，3-[（γ-ω-全氟-C4-10-烷基）硫代]衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3565,IF($B$1=\"Deutsch\",D3565,IF($B$1=\"中文\",E3565,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkyl iodides, C4-20, γ-ω-perfluoro"},"Alkyl iodides, C4-20, γ-ω-perfluoro","Alkyl iodides, C4-20, γ-ω-perfluoro","烷基碘，C4-20，γ-ω-全氟"]
[null,{"$f":"IF($B$1=\"English\",C3566,IF($B$1=\"Deutsch\",D3566,IF($B$1=\"中文\",E3566,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Fatty acids, C7-13, perfluoro"},"Fatty acids, C7-13, perfluoro","Fatty acids, C7-13, perfluoro","脂肪酸，C7-13，全氟"]
[null,{"$f":"IF($B$1=\"English\",C3567,IF($B$1=\"Deutsch\",D3567,IF($B$1=\"中文\",E3567,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl acrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl acrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl acrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-全氟癸基丙烯酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3568,IF($B$1=\"Deutsch\",D3568,IF($B$1=\"中文\",E3568,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodotetradecane"},"1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodotetradecane","1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodotetradecane","1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12-二十五氟-14-碘十四烷"]
[null,{"$f":"IF($B$1=\"English\",C3569,IF($B$1=\"Deutsch\",D3569,IF($B$1=\"中文\",E3569,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecene"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecene","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecene","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-全氟癸基乙烯"]
[null,{"$f":"IF($B$1=\"English\",C3570,IF($B$1=\"Deutsch\",D3570,IF($B$1=\"中文\",E3570,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorooctanoic anhydride"},"Perfluorooctanoic anhydride","Perfluorooctanoic anhydride","全氟辛酸酐"]
[null,{"$f":"IF($B$1=\"English\",C3571,IF($B$1=\"Deutsch\",D3571,IF($B$1=\"中文\",E3571,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-carboxyethylbis(2-hydroxyethyl)-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]propylammonium hydroxide"},"2-carboxyethylbis(2-hydroxyethyl)-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]propylammonium hydroxide","2-carboxyethylbis(2-hydroxyethyl)-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]propylammonium hydroxide","2-羧乙基双（2-羟乙基）-3-[（2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟-1-氧辛基）氨基]丙基氢氧化铵"]
[null,{"$f":"IF($B$1=\"English\",C3572,IF($B$1=\"Deutsch\",D3572,IF($B$1=\"中文\",E3572,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecanol"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecanol","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecanol","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，14-二十五氟十四醇"]
[null,{"$f":"IF($B$1=\"English\",C3573,IF($B$1=\"Deutsch\",D3573,IF($B$1=\"中文\",E3573,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"N-[3-[bis(2-hydroxyethyl)amino]propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide"},"N-[3-[bis(2-hydroxyethyl)amino]propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide","N-[3-[bis(2-hydroxyethyl)amino]propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide","N-[3-[双（2-羟乙基）氨基]丙基]-2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟辛酰胺"]
[null,{"$f":"IF($B$1=\"English\",C3574,IF($B$1=\"Deutsch\",D3574,IF($B$1=\"中文\",E3574,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl acrylate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl acrylate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl acrylate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，14，14，14-二十四氟-13-（三氟甲基）丙烯酸十四酯"]
[null,{"$f":"IF($B$1=\"English\",C3575,IF($B$1=\"Deutsch\",D3575,IF($B$1=\"中文\",E3575,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl dihydrogen phosphate"},"3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl dihydrogen phosphate","3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl dihydrogen phosphate","3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-二十一氟十二烷基二氢磷酸氢盐"]
[null,{"$f":"IF($B$1=\"English\",C3576,IF($B$1=\"Deutsch\",D3576,IF($B$1=\"中文\",E3576,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butanoic acid, 3,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-2-(trifluoromethyl)-"},"Butanoic acid, 3,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-2-(trifluoromethyl)-","Butanoic acid, 3,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-2-(trifluoromethyl)-","丁酸，3，3，4，4，4-五氟-2-[1，2，2，2-四氟-1-（三氟甲基）乙基]-2-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3577,IF($B$1=\"Deutsch\",D3577,IF($B$1=\"中文\",E3577,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,4,4,5,5,6,6,6-nonafluoro-3,3-bis(trifluoromethyl)-"},"Hexanoic acid, 2,2,4,4,5,5,6,6,6-nonafluoro-3,3-bis(trifluoromethyl)-","Hexanoic acid, 2,2,4,4,5,5,6,6,6-nonafluoro-3,3-bis(trifluoromethyl)-","己酸，2，2，4，4，5，5，6，6，6-九氟-3，3-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3578,IF($B$1=\"Deutsch\",D3578,IF($B$1=\"中文\",E3578,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,3,4,4,5,5,6,6,6-nonafluoro-2,3-bis(trifluoromethyl)-"},"Hexanoic acid, 2,3,4,4,5,5,6,6,6-nonafluoro-2,3-bis(trifluoromethyl)-","Hexanoic acid, 2,3,4,4,5,5,6,6,6-nonafluoro-2,3-bis(trifluoromethyl)-","己酸，2，3，4，4，5，5，6，6，6-九氟-2，3-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3579,IF($B$1=\"Deutsch\",D3579,IF($B$1=\"中文\",E3579,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,3,4,5,6,6,6-nonafluoro-4,5-bis(trifluoromethyl)-"},"Hexanoic acid, 2,2,3,3,4,5,6,6,6-nonafluoro-4,5-bis(trifluoromethyl)-","Hexanoic acid, 2,2,3,3,4,5,6,6,6-nonafluoro-4,5-bis(trifluoromethyl)-","己酸，2，2，3，3，4，5，6，6，6-九氟-4，5-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3580,IF($B$1=\"Deutsch\",D3580,IF($B$1=\"中文\",E3580,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,3,4,4,6,6,6-nonafluoro-5,5-bis(trifluoromethyl)-"},"Hexanoic acid, 2,2,3,3,4,4,6,6,6-nonafluoro-5,5-bis(trifluoromethyl)-","Hexanoic acid, 2,2,3,3,4,4,6,6,6-nonafluoro-5,5-bis(trifluoromethyl)-","己酸，2，2，3，3，4，4，6，6，6-九氟-5，5-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3581,IF($B$1=\"Deutsch\",D3581,IF($B$1=\"中文\",E3581,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,6,6,7,7,7-dodecafluoro-5-(trifluoromethyl)-"},"Heptanoic acid, 2,2,3,3,4,4,5,6,6,7,7,7-dodecafluoro-5-(trifluoromethyl)-","Heptanoic acid, 2,2,3,3,4,4,5,6,6,7,7,7-dodecafluoro-5-(trifluoromethyl)-","庚酸，2，2，3，3，4，4，5，6，6，7，7，7-十二氟-5-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3582,IF($B$1=\"Deutsch\",D3582,IF($B$1=\"中文\",E3582,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,3,3,4,4,5,5,6,6,7,7,7-dodecafluoro-2-(trifluoromethyl)-"},"Heptanoic acid, 2,3,3,4,4,5,5,6,6,7,7,7-dodecafluoro-2-(trifluoromethyl)-","Heptanoic acid, 2,3,3,4,4,5,5,6,6,7,7,7-dodecafluoro-2-(trifluoromethyl)-","庚酸，2，3，3，4，4，5，5，6，6，7，7，7-十二氟-2-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3583,IF($B$1=\"Deutsch\",D3583,IF($B$1=\"中文\",E3583,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-"},"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-","Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-","己酸，2，3，3，4，4，5，5，6，6，6-十氟-2-（1，1，2，2，2-五氟乙基）-"]
[null,{"$f":"IF($B$1=\"English\",C3584,IF($B$1=\"Deutsch\",D3584,IF($B$1=\"中文\",E3584,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ethanaminium, N,N,N-triethyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)"},"Ethanaminium, N,N,N-triethyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)","Ethanaminium, N,N,N-triethyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)","乙酰胆碱，N，N，N-三乙基-，2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟辛酸（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3585,IF($B$1=\"Deutsch\",D3585,IF($B$1=\"中文\",E3585,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-"},"Decanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","Decanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","癸酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟-"]
[null,{"$f":"IF($B$1=\"English\",C3586,IF($B$1=\"Deutsch\",D3586,IF($B$1=\"中文\",E3586,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Decenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluoro-"},"2-Decenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluoro-","2-Decenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluoro-","2-癸酸，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十六氟-"]
[null,{"$f":"IF($B$1=\"English\",C3587,IF($B$1=\"Deutsch\",D3587,IF($B$1=\"中文\",E3587,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphate)"},"1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphate)","1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphate)","1-癸醇，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟-，1-（二氢磷酸酯）"]
[null,{"$f":"IF($B$1=\"English\",C3588,IF($B$1=\"Deutsch\",D3588,IF($B$1=\"中文\",E3588,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,3,3,4,4,5,6,6,6-nonafluoro-2,5-bis(trifluoromethyl)-"},"Hexanoic acid, 2,3,3,4,4,5,6,6,6-nonafluoro-2,5-bis(trifluoromethyl)-","Hexanoic acid, 2,3,3,4,4,5,6,6,6-nonafluoro-2,5-bis(trifluoromethyl)-","己酸，2，3，3，4，4，5，6，6，6-九氟-2，5-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3589,IF($B$1=\"Deutsch\",D3589,IF($B$1=\"中文\",E3589,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Propanaminium,N,N,N-trimethyl-3- [(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl) amino]-, chloride (1:1)"},"1-Propanaminium,N,N,N-trimethyl-3- [(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl) amino]-, chloride (1:1)","1-Propanaminium,N,N,N-trimethyl-3- [(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl) amino]-, chloride (1:1)","1-丙铵，N，N，N-三甲基-3-[（2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟-1-氧辛基）氨基]-，氯化物（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3590,IF($B$1=\"Deutsch\",D3590,IF($B$1=\"中文\",E3590,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1-Propanesulfonic acid,3-[ethyl (2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-,sodium salt (1:1)"},"1-Propanesulfonic acid,3-[ethyl (2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-,sodium salt (1:1)","1-Propanesulfonic acid,3-[ethyl (2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-,sodium salt (1:1)","1-丙磺酸，3-[乙基（2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-十五氟-1-氧辛基）氨基]-，钠盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3591,IF($B$1=\"Deutsch\",D3591,IF($B$1=\"中文\",E3591,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phosphine, tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]-"},"Phosphine, tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]-","Phosphine, tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]-","磷化氢，三[4-(3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯）苯基]-"]
[null,{"$f":"IF($B$1=\"English\",C3592,IF($B$1=\"Deutsch\",D3592,IF($B$1=\"中文\",E3592,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Palladium, dichlorobis[tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phosphine-κP]-"},"Palladium, dichlorobis[tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phosphine-κP]-","Palladium, dichlorobis[tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phosphine-κP]-","钯，二氯双[三[4-（3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯）苯基]磷化氢-κP]-"]
[null,{"$f":"IF($B$1=\"English\",C3593,IF($B$1=\"Deutsch\",D3593,IF($B$1=\"中文\",E3593,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butanoic acid, 3,3,4,4,4-pentafluoro-2,2-bis(1,1,2,2,2-pentafluoroethyl)-"},"Butanoic acid, 3,3,4,4,4-pentafluoro-2,2-bis(1,1,2,2,2-pentafluoroethyl)-","Butanoic acid, 3,3,4,4,4-pentafluoro-2,2-bis(1,1,2,2,2-pentafluoroethyl)-","丁酸，3，3，4，4，4-五氟-2，2-双（1，1，2，2，2-五氟乙基）-"]
[null,{"$f":"IF($B$1=\"English\",C3594,IF($B$1=\"Deutsch\",D3594,IF($B$1=\"中文\",E3594,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,3,3,4,5,5,6,6,6-nonafluoro-2,4-bis(trifluoromethyl)-"},"Hexanoic acid, 2,3,3,4,5,5,6,6,6-nonafluoro-2,4-bis(trifluoromethyl)-","Hexanoic acid, 2,3,3,4,5,5,6,6,6-nonafluoro-2,4-bis(trifluoromethyl)-","己酸，2，3，3，4，5，5，6，6，6-九氟-2，4-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3595,IF($B$1=\"Deutsch\",D3595,IF($B$1=\"中文\",E3595,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 3,3,4,4,5,5,6,6,6-nonafluoro-2,2-bis(trifluoromethyl)-"},"Hexanoic acid, 3,3,4,4,5,5,6,6,6-nonafluoro-2,2-bis(trifluoromethyl)-","Hexanoic acid, 3,3,4,4,5,5,6,6,6-nonafluoro-2,2-bis(trifluoromethyl)-","己酸，3，3，4，4，5，5，6，6，6-九氟-2，2-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3596,IF($B$1=\"Deutsch\",D3596,IF($B$1=\"中文\",E3596,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,3,5,5,6,6,6-nonafluoro-4,4-bis(trifluoromethyl)-"},"Hexanoic acid, 2,2,3,3,5,5,6,6,6-nonafluoro-4,4-bis(trifluoromethyl)-","Hexanoic acid, 2,2,3,3,5,5,6,6,6-nonafluoro-4,4-bis(trifluoromethyl)-","己酸，2，2，3，3，5，5，6，6，6-九氟-4，4-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3597,IF($B$1=\"Deutsch\",D3597,IF($B$1=\"中文\",E3597,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,4,4,5,6,6,6-nonafluoro-3,5-bis(trifluoromethyl)-"},"Hexanoic acid, 2,2,3,4,4,5,6,6,6-nonafluoro-3,5-bis(trifluoromethyl)-","Hexanoic acid, 2,2,3,4,4,5,6,6,6-nonafluoro-3,5-bis(trifluoromethyl)-","己酸，2，2，3，4，4，5，6，6，6-九氟-3，5-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3598,IF($B$1=\"Deutsch\",D3598,IF($B$1=\"中文\",E3598,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,5,5,6,6,7,7,7-dodecafluoro-4-(trifluoromethyl)-"},"Heptanoic acid, 2,2,3,3,4,5,5,6,6,7,7,7-dodecafluoro-4-(trifluoromethyl)-","Heptanoic acid, 2,2,3,3,4,5,5,6,6,7,7,7-dodecafluoro-4-(trifluoromethyl)-","庚酸，2，2，3，3，4，5，5，6，6，7，7，7-十二氟-4-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3599,IF($B$1=\"Deutsch\",D3599,IF($B$1=\"中文\",E3599,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,4,4,5,5,6,6,7,7,7-dodecafluoro-3-(trifluoromethyl)-"},"Heptanoic acid, 2,2,3,4,4,5,5,6,6,7,7,7-dodecafluoro-3-(trifluoromethyl)-","Heptanoic acid, 2,2,3,4,4,5,5,6,6,7,7,7-dodecafluoro-3-(trifluoromethyl)-","庚酸，2，2，3，4，4，5，5，6，6，7，7，7-十二氟-3-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3600,IF($B$1=\"Deutsch\",D3600,IF($B$1=\"中文\",E3600,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Isooctanoic acid, pentadecafluoro-"},"Isooctanoic acid, pentadecafluoro-","Isooctanoic acid, pentadecafluoro-","异辛酸，十五氟-"]
[null,{"$f":"IF($B$1=\"English\",C3601,IF($B$1=\"Deutsch\",D3601,IF($B$1=\"中文\",E3601,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3602,IF($B$1=\"Deutsch\",D3602,IF($B$1=\"中文\",E3602,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Octadecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester"},"Octadecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","Octadecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","十八烷酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯"]
[null,{"$f":"IF($B$1=\"English\",C3603,IF($B$1=\"Deutsch\",D3603,IF($B$1=\"中文\",E3603,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanedioic acid, 3-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]-2-oxoethyl]-3-hydroxy-, 1,5-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester"},"Pentanedioic acid, 3-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]-2-oxoethyl]-3-hydroxy-, 1,5-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester","Pentanedioic acid, 3-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]-2-oxoethyl]-3-hydroxy-, 1,5-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester","戊二酸，3-[2-[（3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯）氧基]-2-氧基乙基]-3-羟基-，1，5-双（3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯）"]
[null,{"$f":"IF($B$1=\"English\",C3604,IF($B$1=\"Deutsch\",D3604,IF($B$1=\"中文\",E3604,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C4–10-alkyl)thio]methyl] derivatives, phosphates, ammonium salts"},"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C4–10-alkyl)thio]methyl] derivatives, phosphates, ammonium salts","1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C4–10-alkyl)thio]methyl] derivatives, phosphates, ammonium salts","1，3-丙二醇，2，2-双[[（γ-ω-全氟-C4–10-烷基）硫代]甲基]衍生物，磷酸盐，铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3605,IF($B$1=\"Deutsch\",D3605,IF($B$1=\"中文\",E3605,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C6–12-alkyl)thio]methyl] derivatives, phosphates, ammonium salts"},"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C6–12-alkyl)thio]methyl] derivatives, phosphates, ammonium salts","1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C6–12-alkyl)thio]methyl] derivatives, phosphates, ammonium salts","1，3-丙二醇，2，2-双[[（γ-ω-全氟-C6–12-烷基）硫代]甲基]衍生物，磷酸盐，铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3606,IF($B$1=\"Deutsch\",D3606,IF($B$1=\"中文\",E3606,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C10-20-alkyl)thio]methyl] derivs., phosphates, ammonium salts"},"1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C10-20-alkyl)thio]methyl] derivs., phosphates, ammonium salts","1,3-Propanediol, 2,2-bis[[(γ-ω-perfluoro-C10-20-alkyl)thio]methyl] derivs., phosphates, ammonium salts","1，3-丙二醇，2，2-双[[(γ-ω-全氟-C10-20-烷基）硫代]甲基]衍生物，磷酸盐，铵盐"]
[null,{"$f":"IF($B$1=\"English\",C3607,IF($B$1=\"Deutsch\",D3607,IF($B$1=\"中文\",E3607,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Oxirane, methyl-, polymer with oxirane, mono[2-hydroxy-3-[( γ-ω-perfluoro-C8-20-alkyl)thio]propyl] ethers"},"Oxirane, methyl-, polymer with oxirane, mono[2-hydroxy-3-[( γ-ω-perfluoro-C8-20-alkyl)thio]propyl] ethers","Oxirane, methyl-, polymer with oxirane, mono[2-hydroxy-3-[( γ-ω-perfluoro-C8-20-alkyl)thio]propyl] ethers","环氧乙烷，甲基-，环氧乙烷聚合物，单[2-羟基-3-[（γ-ω-全氟-C8-20-烷基）硫代]丙基]醚"]
[null,{"$f":"IF($B$1=\"English\",C3608,IF($B$1=\"Deutsch\",D3608,IF($B$1=\"中文\",E3608,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 4,4-bis[(γ-ω-perfluoro-C8-20-alkyl)thio]derivs., compds. with diethanolamine"},"Pentanoic acid, 4,4-bis[(γ-ω-perfluoro-C8-20-alkyl)thio]derivs., compds. with diethanolamine","Pentanoic acid, 4,4-bis[(γ-ω-perfluoro-C8-20-alkyl)thio]derivs., compds. with diethanolamine","戊酸，4，4-双[（-ω-全氟-C8-20-烷基）硫代]衍生物，二乙醇胺化合物"]
[null,{"$f":"IF($B$1=\"English\",C3609,IF($B$1=\"Deutsch\",D3609,IF($B$1=\"中文\",E3609,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethyl methacrylate, Me methacrylate and γ-ω-perfluoro-C8-14-alkyl acrylate"},"2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethyl methacrylate, Me methacrylate and γ-ω-perfluoro-C8-14-alkyl acrylate","2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethyl methacrylate, Me methacrylate and γ-ω-perfluoro-C8-14-alkyl acrylate","2-丙烯酸，2-甲基-，C10-16-烷基酯，2-甲基丙烯酸羟乙酯，甲基丙烯酸酯和γ-ω-全氟-C8-14-丙烯酸烷基酯聚合物"]
[null,{"$f":"IF($B$1=\"English\",C3610,IF($B$1=\"Deutsch\",D3610,IF($B$1=\"中文\",E3610,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, dodecyl ester, polymers with Bu (1-oxo-2-propenyl)carbamate and γ-ω-perfluoro-C8-14-alkyl acrylate"},"2-Propenoic acid, dodecyl ester, polymers with Bu (1-oxo-2-propenyl)carbamate and γ-ω-perfluoro-C8-14-alkyl acrylate","2-Propenoic acid, dodecyl ester, polymers with Bu (1-oxo-2-propenyl)carbamate and γ-ω-perfluoro-C8-14-alkyl acrylate","2-丙烯酸，十二烷基酯，丁基（1-含氧-2-丙烯基）氨基甲酸酯和γ-ω-全氟-C8-14-丙烯酸烷基酯聚合物"]
[null,{"$f":"IF($B$1=\"English\",C3611,IF($B$1=\"Deutsch\",D3611,IF($B$1=\"中文\",E3611,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, homopolymer"},"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, homopolymer","2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, homopolymer","2-丙烯酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯，均聚物；2-丙烯酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯，均聚物"]
[null,{"$f":"IF($B$1=\"English\",C3612,IF($B$1=\"Deutsch\",D3612,IF($B$1=\"中文\",E3612,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl 2-methyl-2-propenoate, methyl 2-methyl-2-propenoate,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-methyl-2-propenoate and 3,3,4,4,5,5,6,6, 7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate"},"2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl 2-methyl-2-propenoate, methyl 2-methyl-2-propenoate,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-methyl-2-propenoate and 3,3,4,4,5,5,6,6, 7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate","2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl 2-methyl-2-propenoate, methyl 2-methyl-2-propenoate,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-methyl-2-propenoate and 3,3,4,4,5,5,6,6, 7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate","2-丙烯酸，2-甲基-，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-二十一氟十二烷基酯，聚合物3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯 2-甲基-2-丙烯酸丁基酯，甲基 2-甲基-2-丙烯酸丁基酯，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，14-二十五氟十四烷基 2-甲基-2-丙烯酸丁基酯和3，3，4，4，5，5，6，6，7，7，8，8，8-十三氟辛酯2-甲基-2-丙烯酸丁基酯"]
[null,{"$f":"IF($B$1=\"English\",C3613,IF($B$1=\"Deutsch\",D3613,IF($B$1=\"中文\",E3613,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, polymer with 2-propenoic acid"},"2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, polymer with 2-propenoic acid","2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, polymer with 2-propenoic acid","2-丙烯酸，2-甲基-，2，2，3，3，4，4，5，5，6，6，7，7，8，8，8-全氟辛基丙烯酸酯，聚合物2-丙烯酸"]
[null,{"$f":"IF($B$1=\"English\",C3614,IF($B$1=\"Deutsch\",D3614,IF($B$1=\"中文\",E3614,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,4,5,5,6,6,6-nonafluoro-3,4-bis(trifluoromethyl)-"},"Hexanoic acid, 2,2,3,4,5,5,6,6,6-nonafluoro-3,4-bis(trifluoromethyl)-","Hexanoic acid, 2,2,3,4,5,5,6,6,6-nonafluoro-3,4-bis(trifluoromethyl)-","己酸，2，2，3，4，5，5，6，6，6-九氟-3，4-双（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3615,IF($B$1=\"Deutsch\",D3615,IF($B$1=\"中文\",E3615,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,3,4,5,5,6,6,6-decafluoro-4-(1,1,2,2,2-pentafluoroethyl)-"},"Hexanoic acid, 2,2,3,3,4,5,5,6,6,6-decafluoro-4-(1,1,2,2,2-pentafluoroethyl)-","Hexanoic acid, 2,2,3,3,4,5,5,6,6,6-decafluoro-4-(1,1,2,2,2-pentafluoroethyl)-","己酸，2，2，3，3，4，5，5，6，6，6-十氟-4-（1，1，2，2，2-五氟乙基）-"]
[null,{"$f":"IF($B$1=\"English\",C3616,IF($B$1=\"Deutsch\",D3616,IF($B$1=\"中文\",E3616,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,2,3,4,4,5,5,6,6,6-decafluoro-3-(1,1,2,2,2-pentafluoroethyl)-"},"Hexanoic acid, 2,2,3,4,4,5,5,6,6,6-decafluoro-3-(1,1,2,2,2-pentafluoroethyl)-","Hexanoic acid, 2,2,3,4,4,5,5,6,6,6-decafluoro-3-(1,1,2,2,2-pentafluoroethyl)-","己酸，2，2，3，4，4，5，5，6，6，6-十氟-3-（1，1，2，2，2-五氟乙基）-"]
[null,{"$f":"IF($B$1=\"English\",C3617,IF($B$1=\"Deutsch\",D3617,IF($B$1=\"中文\",E3617,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-(1,1,2,2,3,3,3-heptafluoropropyl)-"},"Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-(1,1,2,2,3,3,3-heptafluoropropyl)-","Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-(1,1,2,2,3,3,3-heptafluoropropyl)-","戊酸，2，3，3，4，4，5，5，5-八氟-2-(1，1，2，2，3，3，3-卜氟胺)-"]
[null,{"$f":"IF($B$1=\"English\",C3618,IF($B$1=\"Deutsch\",D3618,IF($B$1=\"中文\",E3618,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-"},"Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-","Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-","戊酸，2，3，3，4，4，5，5，5-八氟-2-[1，2，2，2-四氟-1-（三氟甲基）乙基]-"]
[null,{"$f":"IF($B$1=\"English\",C3619,IF($B$1=\"Deutsch\",D3619,IF($B$1=\"中文\",E3619,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,2,3,5,5,5-hexafluoro-3,4,4-tris(trifluoromethyl)-"},"Pentanoic acid, 2,2,3,5,5,5-hexafluoro-3,4,4-tris(trifluoromethyl)-","Pentanoic acid, 2,2,3,5,5,5-hexafluoro-3,4,4-tris(trifluoromethyl)-","戊酸，2，2，3，5，5，5-六氟-3，4，4-苯三甲酸三（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3620,IF($B$1=\"Deutsch\",D3620,IF($B$1=\"中文\",E3620,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,2,4,5,5,5-hexafluoro-3,3,4-tris(trifluoromethyl)-"},"Pentanoic acid, 2,2,4,5,5,5-hexafluoro-3,3,4-tris(trifluoromethyl)-","Pentanoic acid, 2,2,4,5,5,5-hexafluoro-3,3,4-tris(trifluoromethyl)-","戊酸，2，2，4，5，5，5-六氟-3，3，4-苯三甲酸三（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3621,IF($B$1=\"Deutsch\",D3621,IF($B$1=\"中文\",E3621,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,3,5,5,5-hexafluoro-2,4,4-tris(trifluoromethyl)-"},"Pentanoic acid, 2,3,3,5,5,5-hexafluoro-2,4,4-tris(trifluoromethyl)-","Pentanoic acid, 2,3,3,5,5,5-hexafluoro-2,4,4-tris(trifluoromethyl)-","戊酸，2，3，3，5，5，5-六氟-2，4，4-苯三甲酸三（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3622,IF($B$1=\"Deutsch\",D3622,IF($B$1=\"中文\",E3622,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,4,5,5,5-hexafluoro-2,3,4-tris(trifluoromethyl)-"},"Pentanoic acid, 2,3,4,5,5,5-hexafluoro-2,3,4-tris(trifluoromethyl)-","Pentanoic acid, 2,3,4,5,5,5-hexafluoro-2,3,4-tris(trifluoromethyl)-","戊酸，2，3，4，5，5，5-六氟-2，3，4-苯三甲酸三（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3623,IF($B$1=\"Deutsch\",D3623,IF($B$1=\"中文\",E3623,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,4,4,5,5,5-hexafluoro-2,3,3-tris(trifluoromethyl)-"},"Pentanoic acid, 2,4,4,5,5,5-hexafluoro-2,3,3-tris(trifluoromethyl)-","Pentanoic acid, 2,4,4,5,5,5-hexafluoro-2,3,3-tris(trifluoromethyl)-","戊酸，2，4，4，5，5，5-六氟-2，3，3-苯三甲酸三（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3624,IF($B$1=\"Deutsch\",D3624,IF($B$1=\"中文\",E3624,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 3,3,4,5,5,5-hexafluoro-2,2,4-tris(trifluoromethyl)-"},"Pentanoic acid, 3,3,4,5,5,5-hexafluoro-2,2,4-tris(trifluoromethyl)-","Pentanoic acid, 3,3,4,5,5,5-hexafluoro-2,2,4-tris(trifluoromethyl)-","戊酸，3，3，4，5，5，5-六氟-2，2，4-苯三甲酸三（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3625,IF($B$1=\"Deutsch\",D3625,IF($B$1=\"中文\",E3625,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,2,3,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-"},"Pentanoic acid, 2,2,3,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-","Pentanoic acid, 2,2,3,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-","戊酸，2，2，3，4，5，5，5-七氟-3-（1，1，2，2，2-五氟乙基）-4-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3626,IF($B$1=\"Deutsch\",D3626,IF($B$1=\"中文\",E3626,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,2,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-"},"Pentanoic acid, 2,2,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-","Pentanoic acid, 2,2,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-","戊酸，2，2，4，4，5，5，5-七氟-3-（1，1，2，2，2-五氟乙基）-3-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3627,IF($B$1=\"Deutsch\",D3627,IF($B$1=\"中文\",E3627,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-"},"Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-","Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-","戊酸，2，3，4，4，5，5，5-七氟-3-（1，1，2，2，2-五氟乙基）-2-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3628,IF($B$1=\"Deutsch\",D3628,IF($B$1=\"中文\",E3628,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,3,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-"},"Pentanoic acid, 2,3,3,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-","Pentanoic acid, 2,3,3,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-","戊酸，2，3，3，4，5，5，5-七氟-2-（1，1，2，2，2-五氟乙基）-4-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3629,IF($B$1=\"Deutsch\",D3629,IF($B$1=\"中文\",E3629,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-"},"Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-","Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-","戊酸，2，3，4，4，5，5，5-七氟-2-（1，1，2，2，2-五氟乙基）-3-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3630,IF($B$1=\"Deutsch\",D3630,IF($B$1=\"中文\",E3630,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 3,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-"},"Pentanoic acid, 3,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-","Pentanoic acid, 3,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-","戊酸，3，3，4，4，5，5，5-七氟-2-（1，1，2，2，2-五氟乙基）-2-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3631,IF($B$1=\"Deutsch\",D3631,IF($B$1=\"中文\",E3631,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentanoic acid, 3,4,4,5,5,5-hexafluoro-2,2,3-(trifluoromethyl)-"},"Pentanoic acid, 3,4,4,5,5,5-hexafluoro-2,2,3-(trifluoromethyl)-","Pentanoic acid, 3,4,4,5,5,5-hexafluoro-2,2,3-(trifluoromethyl)-","戊酸，3，4，4，5，5，5-六氟-2，2，3-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3632,IF($B$1=\"Deutsch\",D3632,IF($B$1=\"中文\",E3632,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butanoic acid, 4,4,4-trifluoro-2,2,3,3-tetrakis(trifluoromethyl)-"},"Butanoic acid, 4,4,4-trifluoro-2,2,3,3-tetrakis(trifluoromethyl)-","Butanoic acid, 4,4,4-trifluoro-2,2,3,3-tetrakis(trifluoromethyl)-","丁酸，4，4，4-三氟-2，2，3，3-四（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3633,IF($B$1=\"Deutsch\",D3633,IF($B$1=\"中文\",E3633,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butanoic acid, 2,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-3-(trifluoromethyl)-"},"Butanoic acid, 2,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-3-(trifluoromethyl)-","Butanoic acid, 2,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-3-(trifluoromethyl)-","丁酸，2，3，4，4，4-五氟-2-[1，2，2，2-四氟-1-（三氟甲基）乙基]-3-（三氟甲基）-"]
[null,{"$f":"IF($B$1=\"English\",C3634,IF($B$1=\"Deutsch\",D3634,IF($B$1=\"中文\",E3634,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Butanoic acid, 2,3,3,4,4,4-hexafluoro-2-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]-"},"Butanoic acid, 2,3,3,4,4,4-hexafluoro-2-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]-","Butanoic acid, 2,3,3,4,4,4-hexafluoro-2-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]-","丁酸，2，3，3，4，4，4-六氟-2-[2，2，2-三氟-1，1-双（三氟甲基）乙基]-"]
[null,{"$f":"IF($B$1=\"English\",C3635,IF($B$1=\"Deutsch\",D3635,IF($B$1=\"中文\",E3635,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2- pentafluoroethyl)-, ammonium salt (1:1)"},"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2- pentafluoroethyl)-, ammonium salt (1:1)","Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2- pentafluoroethyl)-, ammonium salt (1:1)","己酸，2，3，3，4，4，5，5，6，6，6-十氟-2-（1，1，2，2，2-五氟乙基）-铵盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3636,IF($B$1=\"Deutsch\",D3636,IF($B$1=\"中文\",E3636,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-, sodium salt (1:1)"},"Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-, sodium salt (1:1)","Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-, sodium salt (1:1)","己酸，2，3，3，4，4，5，5，6，6，6-十氟-2-（1，1，2，2，2-五氟乙基）-钠盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3637,IF($B$1=\"Deutsch\",D3637,IF($B$1=\"中文\",E3637,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, ammonium salt (1:1)"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, ammonium salt (1:1)","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, ammonium salt (1:1)","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-，铵盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3638,IF($B$1=\"Deutsch\",D3638,IF($B$1=\"中文\",E3638,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, iron salt (1:x)"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, iron salt (1:x)","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, iron salt (1:x)","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-，铁盐（1:x）"]
[null,{"$f":"IF($B$1=\"English\",C3639,IF($B$1=\"Deutsch\",D3639,IF($B$1=\"中文\",E3639,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, potassium salt (1:1)"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, potassium salt (1:1)","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, potassium salt (1:1)","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-钾盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3640,IF($B$1=\"Deutsch\",D3640,IF($B$1=\"中文\",E3640,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)- , sodium salt (1:1)"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)- , sodium salt (1:1)","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)- , sodium salt (1:1)","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-钠盐（1:1）"]
[null,{"$f":"IF($B$1=\"English\",C3641,IF($B$1=\"Deutsch\",D3641,IF($B$1=\"中文\",E3641,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, chromium salt (1:x)"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, chromium salt (1:x)","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, chromium salt (1:x)","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-，铬盐（1:x）"]
[null,{"$f":"IF($B$1=\"English\",C3642,IF($B$1=\"Deutsch\",D3642,IF($B$1=\"中文\",E3642,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, aluminum salt (3:1)"},"Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, aluminum salt (3:1)","Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, aluminum salt (3:1)","庚酸，2，2，3，3，4，4，5，5，6，7，7，7-十二氟-6-（三氟甲基）-，铝盐（3:1）"]
[null,{"$f":"IF($B$1=\"English\",C3643,IF($B$1=\"Deutsch\",D3643,IF($B$1=\"中文\",E3643,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(perfluorooctyl)phosphinic acid"},"Bis(perfluorooctyl)phosphinic acid","Bis(perfluorooctyl)phosphinic acid","双（全氟辛基）次膦酸"]
[null,{"$f":"IF($B$1=\"English\",C3644,IF($B$1=\"Deutsch\",D3644,IF($B$1=\"中文\",E3644,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Perfluorohexylperfluorooctyl phosphinate"},"Perfluorohexylperfluorooctyl phosphinate","Perfluorohexylperfluorooctyl phosphinate","全氟己基全氟辛基次膦酸酯"]
[null,{"$f":"IF($B$1=\"English\",C3645,IF($B$1=\"Deutsch\",D3645,IF($B$1=\"中文\",E3645,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-tricosafluoro-11-iodo-"},"Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-tricosafluoro-11-iodo-","Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-tricosafluoro-11-iodo-","十一烷，1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11-二十三氟-11-碘-"]
[null,{"$f":"IF($B$1=\"English\",C3646,IF($B$1=\"Deutsch\",D3646,IF($B$1=\"中文\",E3646,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15-hentriacontafluoro-15-iodo-"},"Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15-hentriacontafluoro-15-iodo-","Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15-hentriacontafluoro-15-iodo-","十五烷，1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15-三十一氟-15-碘-"]
[null,{"$f":"IF($B$1=\"English\",C3647,IF($B$1=\"Deutsch\",D3647,IF($B$1=\"中文\",E3647,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-heptacosafluoro-13-iodo-"},"Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-heptacosafluoro-13-iodo-","Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-heptacosafluoro-13-iodo-","十三烷，1，1，1，2，2，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13-二十七氟-13-碘-"]
[null,{"$f":"IF($B$1=\"English\",C3648,IF($B$1=\"Deutsch\",D3648,IF($B$1=\"中文\",E3648,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkyl iodides, C10-12, γ-ω-perfluoro"},"Alkyl iodides, C10-12, γ-ω-perfluoro","Alkyl iodides, C10-12, γ-ω-perfluoro","烷基碘，C10-12，γ-ω-全氟"]
[null,{"$f":"IF($B$1=\"English\",C3649,IF($B$1=\"Deutsch\",D3649,IF($B$1=\"中文\",E3649,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Dodecenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-"},"2-Dodecenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-","2-Dodecenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-","2-十二碳烯酸，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-二十碳氟-"]
[null,{"$f":"IF($B$1=\"English\",C3650,IF($B$1=\"Deutsch\",D3650,IF($B$1=\"中文\",E3650,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dodecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-"},"Dodecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","Dodecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","十二烷酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，12-二十一氟-"]
[null,{"$f":"IF($B$1=\"English\",C3651,IF($B$1=\"Deutsch\",D3651,IF($B$1=\"中文\",E3651,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, hexadecyl 2-propenoate, N-(hydroxymethyl)-2-propenamide, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate"},"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, hexadecyl 2-propenoate, N-(hydroxymethyl)-2-propenamide, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate","2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, hexadecyl 2-propenoate, N-(hydroxymethyl)-2-propenamide, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate","2-丙烯酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，11，11，12，12，12-二十一氟十二烷基酯，聚合物3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯2-丙烯酸丁基酯，十六烷基2-丙烯酸丁基酯，N-（羟甲基）-2-丙烯酰胺，十八基2-丙烯酸丁基酯，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，14-二十五氟十四烷基2-丙烯酸丁基酯和3，3，4，4，5，5，6，6，7，7，8，8，8-十三氟辛酯2-丙烯酸丁基酯"]
[null,{"$f":"IF($B$1=\"English\",C3652,IF($B$1=\"Deutsch\",D3652,IF($B$1=\"中文\",E3652,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-[(2-methyl-1-oxo-2-propenyl)oxy]poly(oxy-1, 2-ethanediyl), 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl 2-propenoate, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-tritriacontafluorooctadecyl 2-propenoate"},"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-[(2-methyl-1-oxo-2-propenyl)oxy]poly(oxy-1, 2-ethanediyl), 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl 2-propenoate, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-tritriacontafluorooctadecyl 2-propenoate","2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-[(2-methyl-1-oxo-2-propenyl)oxy]poly(oxy-1, 2-ethanediyl), 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl 2-propenoate, octadecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-tritriacontafluorooctadecyl 2-propenoate","2-丙烯酸，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，11，11，12，12，12-二十一氟十二烷基酯，聚合物3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，10-十七氟癸酯2-丙烯酸丁基酯，α-（2-甲基-1-含氧-2-丙烯基）-ω-[（2-甲基-1-含氧-2-丙烯基）氧基]聚（氧基-1，2-乙二醇），3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，16-二十九氟十六烷基2-丙烯酸丁基酯，十八烷基2-丙烯酸丁基酯，3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，14-二十五氟十四烷基2-烯酸丁基酯和3，3，4，4，5，5，6，6，7，7，8，8，9，9，10，10，11，11，12，12，13，13，14，14，15，15，16，16，17，17，18，18，18-十三氟辛酯2-丙烯酸丁基酯"]
[null,{"$f":"IF($B$1=\"English\",C3653,IF($B$1=\"Deutsch\",D3653,IF($B$1=\"中文\",E3653,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethylmethacrylate, Me methacrylate and perfluoro-C8-14-alkyl acrylate"},"2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethylmethacrylate, Me methacrylate and perfluoro-C8-14-alkyl acrylate","2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethylmethacrylate, Me methacrylate and perfluoro-C8-14-alkyl acrylate","2-丙烯酸，2-甲基-，C10-16-烷基酯，聚合物2-甲基丙烯酸羟乙酯，甲基丙烯酸酯和全氟-C8-14-丙烯酸烷基酯"]
[null,{"$f":"IF($B$1=\"English\",C3654,IF($B$1=\"Deutsch\",D3654,IF($B$1=\"中文\",E3654,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated Biphenyls (PCB)"},"Polychlorinated Biphenyls (PCB)","Polychlorinated Biphenyls (PCB)","多氯联苯（PCB）"]
[null,{"$f":"IF($B$1=\"English\",C3655,IF($B$1=\"Deutsch\",D3655,IF($B$1=\"中文\",E3655,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chloro-1,1'-biphenyl"},"Chloro-1,1'-biphenyl","Chloro-1,1'-biphenyl","氯-1，1 '-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3656,IF($B$1=\"Deutsch\",D3656,IF($B$1=\"中文\",E3656,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dichlorobiphenyl"},"Dichlorobiphenyl","Dichlorobiphenyl","二氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3657,IF($B$1=\"Deutsch\",D3657,IF($B$1=\"中文\",E3657,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrachloro(tetrachlorophenyl)benzene"},"Tetrachloro(tetrachlorophenyl)benzene","Tetrachloro(tetrachlorophenyl)benzene","四氯苯"]
[null,{"$f":"IF($B$1=\"English\",C3658,IF($B$1=\"Deutsch\",D3658,IF($B$1=\"中文\",E3658,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',4,4',6,6'-hexachlorobiphenyl"},"2,2',4,4',6,6'-hexachlorobiphenyl","2,2',4,4',6,6'-hexachlorobiphenyl","2，2'，4，4'，6，6'-六氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3659,IF($B$1=\"Deutsch\",D3659,IF($B$1=\"中文\",E3659,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3'-dichlorobiphenyl"},"3,3'-dichlorobiphenyl","3,3'-dichlorobiphenyl","3，3'-二氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3660,IF($B$1=\"Deutsch\",D3660,IF($B$1=\"中文\",E3660,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4',5-trichlorobiphenyl"},"2,4',5-trichlorobiphenyl","2,4',5-trichlorobiphenyl","2，4'，5-三氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3661,IF($B$1=\"Deutsch\",D3661,IF($B$1=\"中文\",E3661,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,3',4,4',5-pentachlorobiphenyl"},"2,3',4,4',5-pentachlorobiphenyl","2,3',4,4',5-pentachlorobiphenyl","2，3'，4，4'，5-五氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3662,IF($B$1=\"Deutsch\",D3662,IF($B$1=\"中文\",E3662,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',3,4,4',5'-hexachlorobiphenyl"},"2,2',3,4,4',5'-hexachlorobiphenyl","2,2',3,4,4',5'-hexachlorobiphenyl","2，2'，3，4，4'，5'-六氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3663,IF($B$1=\"Deutsch\",D3663,IF($B$1=\"中文\",E3663,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',3,4,4',5,5'-heptachlorobiphenyl"},"2,2',3,4,4',5,5'-heptachlorobiphenyl","2,2',3,4,4',5,5'-heptachlorobiphenyl","2，2'，3，4，4'，5，5'-七氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3664,IF($B$1=\"Deutsch\",D3664,IF($B$1=\"中文\",E3664,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',4,5,5'-pentachlorobiphenyl"},"2,2',4,5,5'-pentachlorobiphenyl","2,2',4,5,5'-pentachlorobiphenyl","2，2'，4，5，5'-五氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3665,IF($B$1=\"Deutsch\",D3665,IF($B$1=\"中文\",E3665,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4,6-Trichlorobiphenyl"},"2,4,6-Trichlorobiphenyl","2,4,6-Trichlorobiphenyl","2，4，6-三氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3666,IF($B$1=\"Deutsch\",D3666,IF($B$1=\"中文\",E3666,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',5,5'-tetrachlorobiphenyl"},"2,2',5,5'-tetrachlorobiphenyl","2,2',5,5'-tetrachlorobiphenyl","2，2'，5，5'-四氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3667,IF($B$1=\"Deutsch\",D3667,IF($B$1=\"中文\",E3667,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4,5-trichloro-1,1'-biphenyl"},"2,4,5-trichloro-1,1'-biphenyl","2,4,5-trichloro-1,1'-biphenyl","2，4，5-三氯-1，1'-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3668,IF($B$1=\"Deutsch\",D3668,IF($B$1=\"中文\",E3668,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3,3',4,4'-tetrachloro-1,1'-biphenyl"},"3,3',4,4'-tetrachloro-1,1'-biphenyl","3,3',4,4'-tetrachloro-1,1'-biphenyl","3，3'，4，4'-四氯-1,1’-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3669,IF($B$1=\"Deutsch\",D3669,IF($B$1=\"中文\",E3669,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',3,3',4,4',5-heptachlorobiphenyl"},"2,2',3,3',4,4',5-heptachlorobiphenyl","2,2',3,3',4,4',5-heptachlorobiphenyl","2，2'，3，3'，4，4'，5-七氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3670,IF($B$1=\"Deutsch\",D3670,IF($B$1=\"中文\",E3670,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4-PCB"},"2,4-PCB","2,4-PCB","2，4-PCB"]
[null,{"$f":"IF($B$1=\"English\",C3671,IF($B$1=\"Deutsch\",D3671,IF($B$1=\"中文\",E3671,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nonachloro-1,1'-biphenyl"},"Nonachloro-1,1'-biphenyl","Nonachloro-1,1'-biphenyl","九氯-1,1’-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3672,IF($B$1=\"Deutsch\",D3672,IF($B$1=\"中文\",E3672,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,1'-Biphenyl, chloro derivs."},"1,1'-Biphenyl, chloro derivs.","1,1'-Biphenyl, chloro derivs.","1，1'-联苯，氯衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3673,IF($B$1=\"Deutsch\",D3673,IF($B$1=\"中文\",E3673,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4,4'-dichlorobiphenyl"},"4,4'-dichlorobiphenyl","4,4'-dichlorobiphenyl","4，4'-二氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3674,IF($B$1=\"Deutsch\",D3674,IF($B$1=\"中文\",E3674,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Decachloro-1,1'-biphenyl"},"Decachloro-1,1'-biphenyl","Decachloro-1,1'-biphenyl","十氯-1,1’-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3675,IF($B$1=\"Deutsch\",D3675,IF($B$1=\"中文\",E3675,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-chlorobiphenyl"},"2-chlorobiphenyl","2-chlorobiphenyl","2-氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3676,IF($B$1=\"Deutsch\",D3676,IF($B$1=\"中文\",E3676,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"3-chlorobiphenyl"},"3-chlorobiphenyl","3-chlorobiphenyl","3-氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3677,IF($B$1=\"Deutsch\",D3677,IF($B$1=\"中文\",E3677,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"4-chlorobiphenyl"},"4-chlorobiphenyl","4-chlorobiphenyl","4-氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3678,IF($B$1=\"Deutsch\",D3678,IF($B$1=\"中文\",E3678,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,2',4,4'-tetrachlorobiphenyl"},"2,2',4,4'-tetrachlorobiphenyl","2,2',4,4'-tetrachlorobiphenyl","2，2'，4，4'-四氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3679,IF($B$1=\"Deutsch\",D3679,IF($B$1=\"中文\",E3679,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4,4'-trichlorobiphenyl"},"2,4,4'-trichlorobiphenyl","2,4,4'-trichlorobiphenyl","2，4，4'-三氯联苯"]
[null,{"$f":"IF($B$1=\"English\",C3680,IF($B$1=\"Deutsch\",D3680,IF($B$1=\"中文\",E3680,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachloro[1,1'-biphenyl]"},"Pentachloro[1,1'-biphenyl]","Pentachloro[1,1'-biphenyl]","五氯[1，1'-联苯]"]
[null,{"$f":"IF($B$1=\"English\",C3681,IF($B$1=\"Deutsch\",D3681,IF($B$1=\"中文\",E3681,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptachloro-1,1'-biphenyl"},"Heptachloro-1,1'-biphenyl","Heptachloro-1,1'-biphenyl","七氯-1，1'-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3682,IF($B$1=\"Deutsch\",D3682,IF($B$1=\"中文\",E3682,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated dibenzo-p-dioxins and dibenzofurans (PCDD/PCDF)"},"Polychlorinated dibenzo-p-dioxins and dibenzofurans (PCDD/PCDF)","Polychlorinated dibenzo-p-dioxins and dibenzofurans (PCDD/PCDF)","多氯二苯并二恶英和二联苯夫喃（PCDD/PCDF）"]
[null,{"$f":"IF($B$1=\"English\",C3683,IF($B$1=\"Deutsch\",D3683,IF($B$1=\"中文\",E3683,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polychlorinated naphthalenes"},"Polychlorinated naphthalenes","Polychlorinated naphthalenes","多氯化萘"]
[null,{"$f":"IF($B$1=\"English\",C3684,IF($B$1=\"Deutsch\",D3684,IF($B$1=\"中文\",E3684,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Naphthalene, chloro derivs."},"Naphthalene, chloro derivs.","Naphthalene, chloro derivs.","萘，氯衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3685,IF($B$1=\"Deutsch\",D3685,IF($B$1=\"中文\",E3685,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Polycyclic aromatic hydrocarbons (PAHs)"},"Polycyclic aromatic hydrocarbons (PAHs)","Polycyclic aromatic hydrocarbons (PAHs)","多环芳烃（PAHs）"]
[null,{"$f":"IF($B$1=\"English\",C3686,IF($B$1=\"Deutsch\",D3686,IF($B$1=\"中文\",E3686,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Indeno[1,2,3-cd]pyrene"},"Indeno[1,2,3-cd]pyrene","Indeno[1,2,3-cd]pyrene","茚并[1，2，3-cd]芘"]
[null,{"$f":"IF($B$1=\"English\",C3687,IF($B$1=\"Deutsch\",D3687,IF($B$1=\"中文\",E3687,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[def]chrysene"},"Benzo[def]chrysene","Benzo[def]chrysene","苯并[def]屈"]
[null,{"$f":"IF($B$1=\"English\",C3688,IF($B$1=\"Deutsch\",D3688,IF($B$1=\"中文\",E3688,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[k]fluoranthene"},"Benzo[k]fluoranthene","Benzo[k]fluoranthene","苯并[k]荧蒽"]
[null,{"$f":"IF($B$1=\"English\",C3689,IF($B$1=\"Deutsch\",D3689,IF($B$1=\"中文\",E3689,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Benzo[e]acephenanthrylene"},"Benzo[e]acephenanthrylene","Benzo[e]acephenanthrylene","苯并[e]醋菲烯"]
[null,{"$f":"IF($B$1=\"English\",C3690,IF($B$1=\"Deutsch\",D3690,IF($B$1=\"中文\",E3690,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrabromodiphenyl ether (group)"},"Tetrabromodiphenyl ether (group)","Tetrabromodiphenyl ether (group)","四溴二苯醚（基团）"]
[null,{"$f":"IF($B$1=\"English\",C3691,IF($B$1=\"Deutsch\",D3691,IF($B$1=\"中文\",E3691,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dibromo-4-(3,4-dibromophenoxy)benzene"},"1,2-dibromo-4-(3,4-dibromophenoxy)benzene","1,2-dibromo-4-(3,4-dibromophenoxy)benzene","1，2-二溴-4-（3，4-二溴苯氧基）苯"]
[null,{"$f":"IF($B$1=\"English\",C3692,IF($B$1=\"Deutsch\",D3692,IF($B$1=\"中文\",E3692,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dibromo-4-(2,6-dibromophenoxy)benzene"},"1,2-dibromo-4-(2,6-dibromophenoxy)benzene","1,2-dibromo-4-(2,6-dibromophenoxy)benzene","1，2-二溴-4-（2，6-二溴苯氧基）苯"]
[null,{"$f":"IF($B$1=\"English\",C3693,IF($B$1=\"Deutsch\",D3693,IF($B$1=\"中文\",E3693,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl ether, tetrabromo derivative"},"Diphenyl ether, tetrabromo derivative","Diphenyl ether, tetrabromo derivative","二苯醚，四溴衍生物"]
[null,{"$f":"IF($B$1=\"English\",C3694,IF($B$1=\"Deutsch\",D3694,IF($B$1=\"中文\",E3694,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,2-dibromo-4-(2,4-dibromophenoxy)benzene"},"1,2-dibromo-4-(2,4-dibromophenoxy)benzene","1,2-dibromo-4-(2,4-dibromophenoxy)benzene","1，2-二溴-4-（2，4-二溴苯氧基）苯"]
[null,{"$f":"IF($B$1=\"English\",C3695,IF($B$1=\"Deutsch\",D3695,IF($B$1=\"中文\",E3695,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1,3,5-tribromo-2-(4-bromophenoxy)benzene"},"1,3,5-tribromo-2-(4-bromophenoxy)benzene","1,3,5-tribromo-2-(4-bromophenoxy)benzene","1，3，5-三溴-2-（4-溴苯氧基）苯"]
[null,{"$f":"IF($B$1=\"English\",C3696,IF($B$1=\"Deutsch\",D3696,IF($B$1=\"中文\",E3696,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dicofol"},"Dicofol","Dicofol","三氯杀螨醇"]
[null,{"$f":"IF($B$1=\"English\",C3697,IF($B$1=\"Deutsch\",D3697,IF($B$1=\"中文\",E3697,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(pentabromophenyl) ether"},"Bis(pentabromophenyl) ether","Bis(pentabromophenyl) ether","双（五溴苯基）醚"]
[null,{"$f":"IF($B$1=\"English\",C3698,IF($B$1=\"Deutsch\",D3698,IF($B$1=\"中文\",E3698,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorobenzene"},"Hexachlorobenzene","Hexachlorobenzene","六氯苯"]
[null,{"$f":"IF($B$1=\"English\",C3699,IF($B$1=\"Deutsch\",D3699,IF($B$1=\"中文\",E3699,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlordecone"},"Chlordecone","Chlordecone","十氯酮"]
[null,{"$f":"IF($B$1=\"English\",C3700,IF($B$1=\"Deutsch\",D3700,IF($B$1=\"中文\",E3700,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dodecachloropentacyclo[5.2.1.02,6.03,9.05,8]decane"},"Dodecachloropentacyclo[5.2.1.02,6.03,9.05,8]decane","Dodecachloropentacyclo[5.2.1.02,6.03,9.05,8]decane","十二氯五环[5.2.1.02]癸烷"]
[null,{"$f":"IF($B$1=\"English\",C3701,IF($B$1=\"Deutsch\",D3701,IF($B$1=\"中文\",E3701,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aldrin"},"Aldrin","Aldrin","艾氏剂"]
[null,{"$f":"IF($B$1=\"English\",C3702,IF($B$1=\"Deutsch\",D3702,IF($B$1=\"中文\",E3702,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexabromo-1,1'-biphenyl"},"Hexabromo-1,1'-biphenyl","Hexabromo-1,1'-biphenyl","六溴-1，1'-联苯"]
[null,{"$f":"IF($B$1=\"English\",C3703,IF($B$1=\"Deutsch\",D3703,IF($B$1=\"中文\",E3703,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Clofenotane"},"Clofenotane","Clofenotane","滴滴涕"]
[null,{"$f":"IF($B$1=\"English\",C3704,IF($B$1=\"Deutsch\",D3704,IF($B$1=\"中文\",E3704,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Chlordane , pur"},"Chlordane , pur","Chlordane , pur","氯丹，纯"]
[null,{"$f":"IF($B$1=\"English\",C3705,IF($B$1=\"Deutsch\",D3705,IF($B$1=\"中文\",E3705,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dieldrin"},"Dieldrin","Dieldrin","狄氏剂"]
[null,{"$f":"IF($B$1=\"English\",C3706,IF($B$1=\"Deutsch\",D3706,IF($B$1=\"中文\",E3706,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Pentachlorobenzene"},"Pentachlorobenzene","Pentachlorobenzene","五氯苯"]
[null,{"$f":"IF($B$1=\"English\",C3707,IF($B$1=\"Deutsch\",D3707,IF($B$1=\"中文\",E3707,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Endrin"},"Endrin","Endrin","异狄氏剂"]
[null,{"$f":"IF($B$1=\"English\",C3708,IF($B$1=\"Deutsch\",D3708,IF($B$1=\"中文\",E3708,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Heptachlor"},"Heptachlor","Heptachlor","七氯"]
[null,{"$f":"IF($B$1=\"English\",C3709,IF($B$1=\"Deutsch\",D3709,IF($B$1=\"中文\",E3709,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Toxaphene"},"Toxaphene","Toxaphene","毒杀芬"]
[null,{"$f":"IF($B$1=\"English\",C3710,IF($B$1=\"Deutsch\",D3710,IF($B$1=\"中文\",E3710,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Alkanes, C10-13, chloro"},"Alkanes, C10-13, chloro","Alkanes, C10-13, chloro","烷烃，C10-13，氯"]
[null,{"$f":"IF($B$1=\"English\",C3711,IF($B$1=\"Deutsch\",D3711,IF($B$1=\"中文\",E3711,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Hexachlorobuta-1,3-diene"},"Hexachlorobuta-1,3-diene","Hexachlorobuta-1,3-diene","六氯-1，3-丁二烯"]
[null,{"$f":"IF($B$1=\"English\",C3712,IF($B$1=\"Deutsch\",D3712,IF($B$1=\"中文\",E3712,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde"},"Formaldehyde","Formaldehyd","甲醛"]
[null,{"$f":"IF($B$1=\"English\",C3713,IF($B$1=\"Deutsch\",D3713,IF($B$1=\"中文\",E3713,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0.1 ml/cbm (ppm) in wood-based materials"},"0.1 ml/cbm (ppm) in wood-based materials","0.1 ml/cbm (ppm) in Holzwerkstoffen","木质材料中0.1ml/cbm（ppm）"]
[null,{"$f":"IF($B$1=\"English\",C3714,IF($B$1=\"Deutsch\",D3714,IF($B$1=\"中文\",E3714,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"ChemVerbotsVGermany\n*The equilibrium concentration of formaldehyde in the air of a test room must be below 0.1 ml/cbm (ppm) with caused by coated and uncoated wood-based materials (chipboard, blockboard, veneer panels and fibreboard). Furniture must comply with the same limit in full body test."},"ChemVerbotsVGermany\n*The equilibrium concentration of formaldehyde in the air of a test room must be below 0.1 ml/cbm (ppm) with caused by coated and uncoated wood-based materials (chipboard, blockboard, veneer panels and fibreboard). Furniture must comply with the same limit in full body test.","Chemikalien-Verbotsverordnung Deutschland\nDie Gleichgewichtskonzentration von Formaldehyd in der Luft eines Prüfraums muss unter 0,1 ml/cbm (ppm) liegen, verursacht durch beschichtete und unbeschichtete Holzwerkstoffe (Spanplatten, Tischlerplatten, Furnierplatten und Faserplatten). Die Möbel müssen den gleichen Grenzwert im Ganzkörpertest einhalten.","德国化学品禁止规则\n*试验室中有涂层和无涂层的木质材料（刨花板、细木工板、胶合板和纤维板）散发在空气中的甲醛平衡浓度必须低于0.1ml/cbm（ppm）。家具在全身测试中必须符合相同的限制。"]
[null,{"$f":"IF($B$1=\"English\",C3715,IF($B$1=\"Deutsch\",D3715,IF($B$1=\"中文\",E3715,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"PFHxS, its salts and related substances"},"PFHxS, its salts and related substances","PFHxS, its salts and related substances","全氟己基磺酸(PFHxS)及其盐类，和其相关化合物"]
[null,{"$f":"IF($B$1=\"English\",C3716,IF($B$1=\"Deutsch\",D3716,IF($B$1=\"中文\",E3716,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"C9-C14 PFCAs and their salts"},"C9-C14 PFCAs and their salts","C9-C14 PFCAs and their salts","C9-C14 PFCA及其盐类"]
[null,{"$f":"IF($B$1=\"English\",C3717,IF($B$1=\"Deutsch\",D3717,IF($B$1=\"中文\",E3717,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Dechlorane plus (DP)“1,4:7,10-Dimethanodibenzo[a,e]cyclooctene, 1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-, which has the molecular formula C18H12Cl12”"},"Dechlorane plus (DP)“1,4:7,10-Dimethanodibenzo[a,e]cyclooctene, 1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-, which has the molecular formula C18H12Cl12”","Dechlorane plus (DP)“1,4:7,10-Dimethanodibenzo[a,e]cyclooctene, 1,2,3,4,7,8,9,10,13,13,14,14-dodecachloro-1,4,4a,5,6,6a,7,10,10a,11,12,12a-dodecahydro-, which has the molecular formula C18H12Cl12”","灭蚁灵加（DP）“1，4：7，10-二甲基二苯并[a，e]环辛烯，1，2，3，4，7，8，9，10，13，13，1,4，1,4-十二氯-1，4，4a，5，6，6a，7，10，10a，11，12，12a-十二氢-，分子式为C18 H12 Cl 12”"]
[null,{"$f":"IF($B$1=\"English\",C3718,IF($B$1=\"Deutsch\",D3718,IF($B$1=\"中文\",E3718,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"decabromodiphenyl ethane (DBDPE) “Benzene, 1,1′-(1,2-ethanediyl)bis [2,3,4,5,6- pentabromo-, which has the molecular formula C14H4Br10)”"},"decabromodiphenyl ethane (DBDPE) “Benzene, 1,1′-(1,2-ethanediyl)bis [2,3,4,5,6- pentabromo-, which has the molecular formula C14H4Br10)”","decabromodiphenyl ethane (DBDPE) “Benzene, 1,1′-(1,2-ethanediyl)bis [2,3,4,5,6- pentabromo-, which has the molecular formula C14H4Br10)”","十溴二苯乙烷（DBDPE）“苯，1，1'-（1，2-乙二基）双[2，3，4，5，6-五溴-，分子式为C14H4Br10）”"]
[null,{"$f":"IF($B$1=\"English\",C3719,IF($B$1=\"Deutsch\",D3719,IF($B$1=\"中文\",E3719,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Group"},"Group","Gruppe","组别"]
[null,{"$f":"IF($B$1=\"English\",C3720,IF($B$1=\"Deutsch\",D3720,IF($B$1=\"中文\",E3720,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≤ 25 ppb PFHxS\n≤ 1000 ppb PFHxS-related substances (sum)"},"≤ 25 ppb PFHxS\n≤ 1000 ppb PFHxS-related substances (sum)","≤ 25 ppb PFHxS\n≤ 1000 ppb PFHxS-related substances (sum)","≤ 25 ppb PFHxS\nPFHxS有关物质（总和）≤1000ppb"]
[null,{"$f":"IF($B$1=\"English\",C3721,IF($B$1=\"Deutsch\",D3721,IF($B$1=\"中文\",E3721,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"≤ 25 ppb, ≤ 260 ppb (sum)"},"≤ 25 ppb, ≤ 260 ppb (sum)","≤ 25 ppb, ≤ 260 ppb (sum)","≤ 25 ppb，≤ 260 ppb（总和）"]
[null,{"$f":"IF($B$1=\"English\",C3722,IF($B$1=\"Deutsch\",D3722,IF($B$1=\"中文\",E3722,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)"},"Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)","Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)","关于降低化学品相关风险的法令ORRChim（RO 2022）"]
[null,{"$f":"IF($B$1=\"English\",C3723,IF($B$1=\"Deutsch\",D3723,IF($B$1=\"中文\",E3723,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)"},"Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)","Ordinance on the reduction of risks related to chemicals ORRChim (RO 2022)","关于降低化学品相关风险的法令ORRChim（RO 2022）"]
[null,{"$f":"IF($B$1=\"English\",C3724,IF($B$1=\"Deutsch\",D3724,IF($B$1=\"中文\",E3724,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n"},"Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n","Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n","加拿大公报，第一部分，第156卷，第20号：《禁止特定有毒物质法规2022》\n"]
[null,{"$f":"IF($B$1=\"English\",C3725,IF($B$1=\"Deutsch\",D3725,IF($B$1=\"中文\",E3725,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n"},"Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n","Canada Gazette, Part I, Volume 156, Number 20: Prohibition of Certain Toxic Substances Regulations, 2022\n","加拿大公报，第一部分，第156卷，第20号：《禁止特定有毒物质法规2022》\n"]
[null,{"$f":"IF($B$1=\"English\",C3726,IF($B$1=\"Deutsch\",D3726,IF($B$1=\"中文\",E3726,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"By Substance groups:\nName and CAS of the contained substances"},"By Substance groups:\nName and CAS of the contained substances","Bei Substanzgruppen:\nName und CAS der enthaltenen Substanzen","By Substance groups:\nName and CAS of the contained substances"]
[null,{"$f":"IF($B$1=\"English\",C3727,IF($B$1=\"Deutsch\",D3727,IF($B$1=\"中文\",E3727,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Regulated Substances"},"Regulated Substances","Reglementierte Inhaltsstoffe ","管控的物质"]
[null,{"$f":"IF($B$1=\"English\",C3728,IF($B$1=\"Deutsch\",D3728,IF($B$1=\"中文\",E3728,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"CAS-Number"},"CAS-Number","CAS-Number","CAS编号"]
[null,{"$f":"IF($B$1=\"English\",C3729,IF($B$1=\"Deutsch\",D3729,IF($B$1=\"中文\",E3729,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limit value [mass-%]"},"Limit value [mass-%]","Grenzwert [Massen%]","限值 （质量%）"]
[null,{"$f":"IF($B$1=\"English\",C3730,IF($B$1=\"Deutsch\",D3730,IF($B$1=\"中文\",E3730,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient [mass%]"},"Concentration of ingredient [mass%]","Concentration of ingredient [mass%]","成分浓度[质量％]"]
[null,{"$f":"IF($B$1=\"English\",C3731,IF($B$1=\"Deutsch\",D3731,IF($B$1=\"中文\",E3731,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Designation of the material that contains the declared substance"},"Designation of the material that contains the declared substance","Designation of the material that contains the declared substance","指定包含申报物质的材料"]
[null,{"$f":"IF($B$1=\"English\",C3732,IF($B$1=\"Deutsch\",D3732,IF($B$1=\"中文\",E3732,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substance Presence"},"Substance Presence","Substanz Vorhanden","物质存在"]
[null,{"$f":"IF($B$1=\"English\",C3733,IF($B$1=\"Deutsch\",D3733,IF($B$1=\"中文\",E3733,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Aluminium"},"Aluminium","Aluminium","铝"]
[null,{"$f":"IF($B$1=\"English\",C3734,IF($B$1=\"Deutsch\",D3734,IF($B$1=\"中文\",E3734,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Capacitors\n• Electronics enclosure"},"• Capacitors\n• Electronics enclosure","• Capacitors\n• Electronics enclosure","• 电容器\n• 电子产品外壳"]
[null,{"$f":"IF($B$1=\"English\",C3735,IF($B$1=\"Deutsch\",D3735,IF($B$1=\"中文\",E3735,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• RB Defined"},"• RB Defined","• RB Defined","• 博世定义"]
[null,{"$f":"IF($B$1=\"English\",C3736,IF($B$1=\"Deutsch\",D3736,IF($B$1=\"中文\",E3736,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Arsenic"},"Arsenic","Arsenic","砷"]
[null,{"$f":"IF($B$1=\"English\",C3737,IF($B$1=\"Deutsch\",D3737,IF($B$1=\"中文\",E3737,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Metallurgy\n• Semi-conductors"},"• Metallurgy\n• Semi-conductors","• Metallurgy\n• Semi-conductors","• 冶金\n• 半导体"]
[null,{"$f":"IF($B$1=\"English\",C3738,IF($B$1=\"Deutsch\",D3738,IF($B$1=\"中文\",E3738,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3739,IF($B$1=\"Deutsch\",D3739,IF($B$1=\"中文\",E3739,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Boron"},"Boron","Boron","硼"]
[null,{"$f":"IF($B$1=\"English\",C3740,IF($B$1=\"Deutsch\",D3740,IF($B$1=\"中文\",E3740,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Metallurgy grade"},"• Metallurgy grade","• Metallurgy grade","• 冶金级"]
[null,{"$f":"IF($B$1=\"English\",C3741,IF($B$1=\"Deutsch\",D3741,IF($B$1=\"中文\",E3741,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3742,IF($B$1=\"Deutsch\",D3742,IF($B$1=\"中文\",E3742,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Copper"},"Copper","Copper","铜"]
[null,{"$f":"IF($B$1=\"English\",C3743,IF($B$1=\"Deutsch\",D3743,IF($B$1=\"中文\",E3743,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Feldspar (silikate)"},"Feldspar (silikate)","Feldspar (silikate)","长石（硅酸盐）"]
[null,{"$f":"IF($B$1=\"English\",C3744,IF($B$1=\"Deutsch\",D3744,IF($B$1=\"中文\",E3744,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Electrification across all strategic technologies"},"• Electrification across all strategic technologies","• Electrification across all strategic technologies","• 所有战略技术的电气化"]
[null,{"$f":"IF($B$1=\"English\",C3745,IF($B$1=\"Deutsch\",D3745,IF($B$1=\"中文\",E3745,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Glass\n• Ceramics"},"• Glass\n• Ceramics","• Glass\n• Ceramics","• 玻璃\n• 陶瓷"]
[null,{"$f":"IF($B$1=\"English\",C3746,IF($B$1=\"Deutsch\",D3746,IF($B$1=\"中文\",E3746,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3747,IF($B$1=\"Deutsch\",D3747,IF($B$1=\"中文\",E3747,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3748,IF($B$1=\"Deutsch\",D3748,IF($B$1=\"中文\",E3748,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Gold"},"Gold","Gold","金"]
[null,{"$f":"IF($B$1=\"English\",C3749,IF($B$1=\"Deutsch\",D3749,IF($B$1=\"中文\",E3749,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain \n• French Decree no. 2022-748 of 29 April 2022"},"• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain \n• French Decree no. 2022-748 of 29 April 2022","• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain \n• French Decree no. 2022-748 of 29 April 2022","• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain \n• French Decree no. 2022-748 of 29 April 2022"]
[null,{"$f":"IF($B$1=\"English\",C3750,IF($B$1=\"Deutsch\",D3750,IF($B$1=\"中文\",E3750,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Helium "},"Helium ","Helium ","氦"]
[null,{"$f":"IF($B$1=\"English\",C3751,IF($B$1=\"Deutsch\",D3751,IF($B$1=\"中文\",E3751,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Lead","铅"]
[null,{"$f":"IF($B$1=\"English\",C3752,IF($B$1=\"Deutsch\",D3752,IF($B$1=\"中文\",E3752,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Cryogenics manufacturing\n• Semiconductors manufacturing"},"• Cryogenics manufacturing\n• Semiconductors manufacturing","• Cryogenics manufacturing\n• Semiconductors manufacturing","• 低温制造\n• 半导体制造"]
[null,{"$f":"IF($B$1=\"English\",C3753,IF($B$1=\"Deutsch\",D3753,IF($B$1=\"中文\",E3753,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3754,IF($B$1=\"Deutsch\",D3754,IF($B$1=\"中文\",E3754,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3755,IF($B$1=\"Deutsch\",D3755,IF($B$1=\"中文\",E3755,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manganese "},"Manganese ","Manganese ","锰"]
[null,{"$f":"IF($B$1=\"English\",C3756,IF($B$1=\"Deutsch\",D3756,IF($B$1=\"中文\",E3756,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Mica"},"Mica","Mica","云母"]
[null,{"$f":"IF($B$1=\"English\",C3757,IF($B$1=\"Deutsch\",D3757,IF($B$1=\"中文\",E3757,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Steelmaking\n• Batteries"},"• Steelmaking\n• Batteries","• Steelmaking\n• Batteries","• 炼钢\n• 电池"]
[null,{"$f":"IF($B$1=\"English\",C3758,IF($B$1=\"Deutsch\",D3758,IF($B$1=\"中文\",E3758,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Electrical or thermal insulators"},"• Electrical or thermal insulators","• Electrical or thermal insulators","• 电绝缘体或热绝缘体"]
[null,{"$f":"IF($B$1=\"English\",C3759,IF($B$1=\"Deutsch\",D3759,IF($B$1=\"中文\",E3759,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3760,IF($B$1=\"Deutsch\",D3760,IF($B$1=\"中文\",E3760,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• RB Defined"},"• RB Defined","• RB Defined","• 博世定义"]
[null,{"$f":"IF($B$1=\"English\",C3761,IF($B$1=\"Deutsch\",D3761,IF($B$1=\"中文\",E3761,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Nickel"},"Nickel","Nickel","镍"]
[null,{"$f":"IF($B$1=\"English\",C3762,IF($B$1=\"Deutsch\",D3762,IF($B$1=\"中文\",E3762,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Batteries\n• Magnets"},"• Batteries\n• Magnets","• Batteries\n• Magnets","• 电池\n• 磁铁"]
[null,{"$f":"IF($B$1=\"English\",C3763,IF($B$1=\"Deutsch\",D3763,IF($B$1=\"中文\",E3763,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3764,IF($B$1=\"Deutsch\",D3764,IF($B$1=\"中文\",E3764,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tin (niobium / cassiterite)"},"Tin (niobium / cassiterite)","Tin (niobium / cassiterite)","锡（铌/锡石）"]
[null,{"$f":"IF($B$1=\"English\",C3765,IF($B$1=\"Deutsch\",D3765,IF($B$1=\"中文\",E3765,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Titanium metal"},"Titanium metal","Titanium metal","钛金属"]
[null,{"$f":"IF($B$1=\"English\",C3766,IF($B$1=\"Deutsch\",D3766,IF($B$1=\"中文\",E3766,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Superconducting magnets"},"• Superconducting magnets","• Superconducting magnets","• 超导磁体"]
[null,{"$f":"IF($B$1=\"English\",C3767,IF($B$1=\"Deutsch\",D3767,IF($B$1=\"中文\",E3767,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Lightweight high-strength alloys "},"• Lightweight high-strength alloys ","• Lightweight high-strength alloys ","• 轻质高强合金"]
[null,{"$f":"IF($B$1=\"English\",C3768,IF($B$1=\"Deutsch\",D3768,IF($B$1=\"中文\",E3768,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain "},"• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain ","• CD80015 - Bosch Supply Chain Management - Corporate Social Responsibility in the Supply Chain ","• CD80015 - 博世供应链管理 - 供应链企业社会责任"]
[null,{"$f":"IF($B$1=\"English\",C3769,IF($B$1=\"Deutsch\",D3769,IF($B$1=\"中文\",E3769,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products "},"• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• EU Ecodesign Directive (Directive 2009/125/EC)\n• EU Critical Raw Materials Act (March, 2023)\n• DIN EN 45558: General method to declare the use of critical raw materials in energy-related products ","• 欧盟生态设计指令（指令 2009/125/EC）\n• 欧盟关键原材料法案（2023 年 3 月）\n• DIN EN 45558：声明在能源相关产品中使用关键原材料的一般方法"]
[null,{"$f":"IF($B$1=\"English\",C3770,IF($B$1=\"Deutsch\",D3770,IF($B$1=\"中文\",E3770,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"recovered from manufacturing waste or post-consumer waste, present in permanent magnets incorporated in product"},"recovered from manufacturing waste or post-consumer waste, present in permanent magnets incorporated in product","Zurückgewonnen aus Produktionsabfällen oder Post-Verbraucher-Abfällen, die in Dauermagneten in Produkten enthalten sind","从制造废物或消费后废物中回收，存在于产品中的永磁体中"]
[null,{"$f":"IF($B$1=\"English\",C3771,IF($B$1=\"Deutsch\",D3771,IF($B$1=\"中文\",E3771,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Diphenyl(2,4,6-trimethylbenzoyl)phosphine oxide"},"Diphenyl(2,4,6-trimethylbenzoyl)phosphine oxide","Diphenyl(2,4,6-trimethylbenzoyl)phosphine oxide","二苯基(2,4,6-三甲基苯甲酰基)氧化膦"]
[null,{"$f":"IF($B$1=\"English\",C3772,IF($B$1=\"Deutsch\",D3772,IF($B$1=\"中文\",E3772,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bis(4-chlorophenyl) sulphone"},"Bis(4-chlorophenyl) sulphone","Bis(4-chlorophenyl) sulphone","双(4-氯苯基)砜"]
[null,{"$f":"IF($B$1=\"English\",C3773,IF($B$1=\"Deutsch\",D3773,IF($B$1=\"中文\",E3773,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Inks and toners, coating products, photo-chemicals, polymers, adhesives and sealants and fillers, putties, plasters, modelling clay "},"Inks and toners, coating products, photo-chemicals, polymers, adhesives and sealants and fillers, putties, plasters, modelling clay ","Tinten und Toner, Beschichtungsprodukte, Fotochemikalien, Polymere, Kleb- und Dichtstoffe sowie Spachtelmassen, Kitte, Putze, Modelliermasse","油墨和碳粉、涂料产品、光化学品、聚合物、粘合剂、密封剂和填料、腻子、灰泥、造型粘土"]
[null,{"$f":"IF($B$1=\"English\",C3774,IF($B$1=\"Deutsch\",D3774,IF($B$1=\"中文\",E3774,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of chemicals, plastic products and rubber products."},"Manufacture of chemicals, plastic products and rubber products.","Herstellung von Chemikalien, Kunststoff- und Gummierzeugnissen.","化学品、塑料制品和橡胶制品的制造"]
[null,{"$f":"IF($B$1=\"English\",C3775,IF($B$1=\"Deutsch\",D3775,IF($B$1=\"中文\",E3775,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Substance group"},"Substance group","Substanzgruppe","物质组"]
[null,{"$f":"IF($B$1=\"English\",C3776,IF($B$1=\"Deutsch\",D3776,IF($B$1=\"中文\",E3776,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"MOAH (Mineral Oil Hydrocarbons) with 1-7 aromatic Rings for printing inks"},"MOAH (Mineral Oil Hydrocarbons) with 1-7 aromatic Rings for printing inks","MOAH (Mineral Oil Hydrocarbons) with 1-7 aromatic Rings for printing inks","MOAH (Mineral Oil Hydrocarbons) with 1-7 aromatic Rings for printing inks"]
[null,{"$f":"IF($B$1=\"English\",C3777,IF($B$1=\"Deutsch\",D3777,IF($B$1=\"中文\",E3777,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"MOAH (Mineral Oil Hydrocarbons) with 3-7 aromatic Rings for printing inks"},"MOAH (Mineral Oil Hydrocarbons) with 3-7 aromatic Rings for printing inks","MOAH (Mineral Oil Hydrocarbons) with 3-7 aromatic Rings for printing inks","MOAH (Mineral Oil Hydrocarbons) with 3-7 aromatic Rings for printing inks"]
[null,{"$f":"IF($B$1=\"English\",C3778,IF($B$1=\"Deutsch\",D3778,IF($B$1=\"中文\",E3778,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Medium- chained chlorinated paraffins (MCCPs) –Alkanes, C14-17, chloro"},"Medium- chained chlorinated paraffins (MCCPs) –Alkanes, C14-17, chloro","Mittelkettige Chlorparaffine (MCCPs) -Alkane, C14-17, Chlor","中链氯化石蜡 (MCCP) – C14-17氯化烷烃"]
[null,{"$f":"IF($B$1=\"English\",C3779,IF($B$1=\"Deutsch\",D3779,IF($B$1=\"中文\",E3779,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Tetrabromobisphenol A (TBBP-A, flame retardant) (2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol)"},"Tetrabromobisphenol A (TBBP-A, flame retardant) (2,2',6,6'-tetrabromo-4,4'-isopropylidenediphenol)","Tetrabrombisphenol A (TBBP-A, Flammschutzmittel) (2,2',6,6'-Tetrabromo-4,4'-Isopropylidendiphenol)","四溴双酚 A（TBBP-A，阻燃剂）（2,2',6,6'-四溴-4,4'-异丙叉二苯酚）"]
[null,{"$f":"IF($B$1=\"English\",C3780,IF($B$1=\"Deutsch\",D3780,IF($B$1=\"中文\",E3780,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2006/66EC, 2008/98/EC, 2019/1020/EC and 2023/1542/EC"},"2006/66EC, 2008/98/EC, 2019/1020/EC and 2023/1542/EC","2006/66EC, 2008/98/EC, 2019/1020/EC and 2023/1542/EC","2006/66EC, 2008/98/EC, 2019/1020/EC and 2023/1542/EC"]
[null,{"$f":"IF($B$1=\"English\",C3781,IF($B$1=\"Deutsch\",D3781,IF($B$1=\"中文\",E3781,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,002 expressed as cadmium metal, for portable battery only"},"0,002 expressed as cadmium metal, for portable battery only","0,002 ausgedrückt als metallisches Cadmium, nur für Gerätebatterien","0.002 以金属镉计，仅适用于便携式电池"]
[null,{"$f":"IF($B$1=\"English\",C3782,IF($B$1=\"Deutsch\",D3782,IF($B$1=\"中文\",E3782,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,0005 expressed as merury metal"},"0,0005 expressed as merury metal","0,0005 ausgedrückt als metallisches Quecksilber","0.0005 以金属汞计"]
[null,{"$f":"IF($B$1=\"English\",C3783,IF($B$1=\"Deutsch\",D3783,IF($B$1=\"中文\",E3783,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead and its compounds"},"Lead and its compounds","Blei und seine Verbindungen","铅及其化合物"]
[null,{"$f":"IF($B$1=\"English\",C3784,IF($B$1=\"Deutsch\",D3784,IF($B$1=\"中文\",E3784,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Cadmium"},"Cadmium","Cadmium","镉"]
[null,{"$f":"IF($B$1=\"English\",C3785,IF($B$1=\"Deutsch\",D3785,IF($B$1=\"中文\",E3785,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Lead"},"Lead","Blei","铅"]
[null,{"$f":"IF($B$1=\"English\",C3786,IF($B$1=\"Deutsch\",D3786,IF($B$1=\"中文\",E3786,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"0,01 expressed as lead metal, for portable battery from 15.06.2024, not for portable zinc-air button cells until 15.06.2028"},"0,01 expressed as lead metal, for portable battery from 15.06.2024, not for portable zinc-air button cells until 15.06.2028","0,01 ausgedrückt als metallisches Blei, für Gerätebatterien ab 15.06.2024, nicht für Zink-Luft Knopfzellen bis 15.06.2028","0.01 以金属铅计，从2024年6月15日起适用于便携式电池，其中便携式锌-空气纽扣电池可豁免至2028年6月15日起执行。"]
[null,{"$f":"IF($B$1=\"English\",C3787,IF($B$1=\"Deutsch\",D3787,IF($B$1=\"中文\",E3787,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":2E-3},2E-3,2E-3,"0.002"]
[null,{"$f":"IF($B$1=\"English\",C3788,IF($B$1=\"Deutsch\",D3788,IF($B$1=\"中文\",E3788,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":4.0000000000000001E-3},4.0000000000000001E-3,4.0000000000000001E-3,"0.004"]
[null,{"$f":"IF($B$1=\"English\",C3789,IF($B$1=\"Deutsch\",D3789,IF($B$1=\"中文\",E3789,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"By Substance groups: Name of the contained substances"},"By Substance groups: Name of the contained substances","Bei Substanzgruppen: Name der enthaltenen Substanzen","按物质组别：所含物质名称"]
[null,{"$f":"IF($B$1=\"English\",C3790,IF($B$1=\"Deutsch\",D3790,IF($B$1=\"中文\",E3790,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"By Substance groups: CAS of the contained substances"},"By Substance groups: CAS of the contained substances","Bei Substanzgruppen: CAS der enthaltenen Substanzen","按物质组别：所含物质CAS号"]
[null,{"$f":"IF($B$1=\"English\",C3791,IF($B$1=\"Deutsch\",D3791,IF($B$1=\"中文\",E3791,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Silver"},"Silver","Silber","银色"]
[null,{"$f":"IF($B$1=\"English\",C3792,IF($B$1=\"Deutsch\",D3792,IF($B$1=\"中文\",E3792,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• Electronic"},"• Electronic","• Elektronisch","• 电子设备"]
[null,{"$f":"IF($B$1=\"English\",C3793,IF($B$1=\"Deutsch\",D3793,IF($B$1=\"中文\",E3793,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"• French Decree no. 2022-748 of 29 April 2022"},"• French Decree no. 2022-748 of 29 April 2022","• French Decree no. 2022-748 of 29 April 2022","• 2022 年 4 月 29 日第 2022-748 号法国法令"]
[null,{"$f":"IF($B$1=\"English\",C3794,IF($B$1=\"Deutsch\",D3794,IF($B$1=\"中文\",E3794,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Yes - all contained CRM declared"},"Yes - all contained CRM declared","Ja-alle enthaltenen CRM deklariert","是 – 所含的关键原材料均已申报"]
[null,{"$f":"IF($B$1=\"English\",C3795,IF($B$1=\"Deutsch\",D3795,IF($B$1=\"中文\",E3795,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"No - no CRM contained"},"No - no CRM contained","Nein-keine CRM enthalten","否 – 不含任何关键原材料   "]
[null,{"$f":"IF($B$1=\"English\",C3796,IF($B$1=\"Deutsch\",D3796,IF($B$1=\"中文\",E3796,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"11.a EU Packaging directive 94/62/EC"},"11.a EU Packaging directive 94/62/EC","11.a EU Packaging directive 94/62/EC","11.a EU Packaging directive 94/62/EC"]
[null,{"$f":"IF($B$1=\"English\",C3797,IF($B$1=\"Deutsch\",D3797,IF($B$1=\"中文\",E3797,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"11. b France Decree No. 2022-105"},"11. b France Decree No. 2022-105","11. b France Decree No. 2022-105","11. b France Decree No. 2022-105"]
[null,{"$f":"IF($B$1=\"English\",C3798,IF($B$1=\"Deutsch\",D3798,IF($B$1=\"中文\",E3798,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"MOSH (Mineral Oil Saturated Hydrocarbons) with 16-35 aromatic Rings for printing inks"},"MOSH (Mineral Oil Saturated Hydrocarbons) with 16-35 aromatic Rings for printing inks","MOSH (Mineral Oil Saturated Hydrocarbons) with 16-35 aromatic Rings for printing inks","MOSH (Mineral Oil Saturated Hydrocarbons) with 16-35 aromatic Rings for printing inks"]
[null,{"$f":"IF($B$1=\"English\",C3799,IF($B$1=\"Deutsch\",D3799,IF($B$1=\"中文\",E3799,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"11. b France Decree No. 2022-105"},"11. b France Decree No. 2022-105","11. b France Decree No. 2022-105","11. b France Decree No. 2022-105"]
[null,{"$f":"IF($B$1=\"English\",C3800,IF($B$1=\"Deutsch\",D3800,IF($B$1=\"中文\",E3800,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfuric acid, cadmium salt, hydrate (3:3:8)"},"Sulfuric acid, cadmium salt, hydrate (3:3:8)","Schwefelsäure, Cadmiumsalz, Hydrat (3:3:8)","硫酸, 镉盐, 水合物 (3:3:8)"]
[null,{"$f":"IF($B$1=\"English\",C3801,IF($B$1=\"Deutsch\",D3801,IF($B$1=\"中文\",E3801,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Sulfuric acid, cadmium salt (1:1), hydrate"},"Sulfuric acid, cadmium salt (1:1), hydrate","Schwefelsäure, Cadmiumsalz (1:1)","硫酸, 镉盐（1:1）水合物"]
[null,{"$f":"IF($B$1=\"English\",C3802,IF($B$1=\"Deutsch\",D3802,IF($B$1=\"中文\",E3802,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"cadmium chloride (CdCl2), hydrate (2:5)"},"cadmium chloride (CdCl2), hydrate (2:5)","Cadmiumchlorid (CdCl2), Hydrat (2:5)","氯化镉 (CdCl2)，水合物 (2:5)"]
[null,{"$f":"IF($B$1=\"English\",C3803,IF($B$1=\"Deutsch\",D3803,IF($B$1=\"中文\",E3803,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Formaldehyde\nCAS-Nr. 50-00-0\nEG-Nr. 200-001-8 \nand formaldehyde releasing substances\n "},"Formaldehyde\nCAS-Nr. 50-00-0\nEG-Nr. 200-001-8 \nand formaldehyde releasing substances\n ","Formaldehyd\nCAS-Nr. 50-00-0\nEG-Nr. 200-001-8\nund Formaldehydabspalter","甲醛\nCAS 编号 50-00-0\nEG-编号 200-001-8\n以及能释放出甲醛的物质"]
[null,{"$f":"IF($B$1=\"English\",C3804,IF($B$1=\"Deutsch\",D3804,IF($B$1=\"中文\",E3804,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Synthetic polymer microparticles:\npolymers that are solid and which fulfil both of the following conditions:\n(a) are contained in particles and constitute at least 1 % by weight of those particles; or\nbuild a continuous surface coating on particles;\n(b) at least 1 % by weight of the particles referred to in point (a) fulfil either of the\nfollowing conditions:\n(i) all dimensions of the particles are equal to or less than 5 mm;\n(ii) the length of the particles is equal to or less than 15 mm and their length to\ndiameter ratio is greater than 3.\nThe following polymers are excluded from this designation:\n(a) polymers that are the result of a polymerisation process that has taken place in\nnature, independently of the process through which they have been extracted, which are\nnot chemically modified substances;\n(b) polymers that are degradable as proved in accordance with Appendix 15;\n(c) polymers that have a solubility greater than 2 g/L as proved in accordance with\nAppendix 16;\n(d) polymers that do not contain carbon atoms in their chemical structure."},"Synthetic polymer microparticles:\npolymers that are solid and which fulfil both of the following conditions:\n(a) are contained in particles and constitute at least 1 % by weight of those particles; or\nbuild a continuous surface coating on particles;\n(b) at least 1 % by weight of the particles referred to in point (a) fulfil either of the\nfollowing conditions:\n(i) all dimensions of the particles are equal to or less than 5 mm;\n(ii) the length of the particles is equal to or less than 15 mm and their length to\ndiameter ratio is greater than 3.\nThe following polymers are excluded from this designation:\n(a) polymers that are the result of a polymerisation process that has taken place in\nnature, independently of the process through which they have been extracted, which are\nnot chemically modified substances;\n(b) polymers that are degradable as proved in accordance with Appendix 15;\n(c) polymers that have a solubility greater than 2 g/L as proved in accordance with\nAppendix 16;\n(d) polymers that do not contain carbon atoms in their chemical structure.","Synthetische Polymermikropartikel:\nfeste Polymere, die beide der folgenden Bedingungen erfüllen:\na) sie sind in Partikeln enthalten und machen mindestens 1 Gewichtsprozent dieser Partikel aus oder bilden eine kontinuierliche Oberflächenbeschichtung auf Partikeln;\nb) mindestens 1 Gewichtsprozent der unter Buchstabe a genannten Partikel erfüllt eine der folgenden Bedingungen:\ni) alle Dimensionen der Partikel sind gleich oder kleiner als 5 mm;\nii) die Länge der Partikel ist gleich oder kleiner als 15 mm und das Verhältnis von Länge zu Durchmesser ist größer als 3.\n\nDie folgenden Polymere sind von dieser Bezeichnung ausgenommen:\na) Polymere, die das Ergebnis eines Polymerisationsprozesses sind, der in der Natur stattgefunden hat, unabhängig von dem Verfahren, mit dem sie extrahiert wurden, und bei denen es sich nicht um chemisch veränderte Stoffe handelt;\nb) Polymere, die nachweislich gemäß Anlage 15 abbaubar sind;\nc) Polymere, die nachweislich gemäß Anlage 16 eine Löslichkeit über 2 g/l aufweisen;\nd) Polymere, die in ihrer chemischen Struktur keine Kohlenstoffatome enthalten..","合成高分子微粒：\n固体聚合物且满足以下两个条件：\n(a) 包含在颗粒中并占这些颗粒重量的至少 1%； 或在颗粒上形成连续的表面涂层；\n(b) (a)点中提及的至少1％重量比的颗粒满足以下条件之一：\n(i) 颗粒的所有尺寸均等于或小于 5 毫米；\n(ii)颗粒的长度等于或小于15毫米且其长径比大于3。\n以下聚合物不包括在该定义中：\n(a) 聚合物是自然界中发生的聚合过程的结果，与提取它们的过程无关，它们不是化学改性物质；\n(b) 根据附录 15 证明可降解的聚合物；\n(c) 根据附录 16 证明溶解度大于 2 g/L 的聚合物；\n(d) 化学结构中不含碳原子的聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C3805,IF($B$1=\"Deutsch\",D3805,IF($B$1=\"中文\",E3805,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market in articles, after 6 August 2026, if, under the test\nconditions specified in Appendix 14, the concentration of formaldehyde released from those\narticles exceeds:\n(a) 0,062 mg/m3 for furniture and wood-based articles;\n(b) 0,080 mg/m3 for articles other than furniture and wood-based articles.\nThe first subparagraph shall not apply to:\n(a) articles in which formaldehyde or formaldehyde releasing substances are exclusively\nnaturally present in the materials from which the articles are produced;\n(b) articles that are exclusively for outdoor use under foreseeable conditions;\n(c) articles in constructions, that are exclusively used outside the building shell and\nvapour barrier and that do not emit formaldehyde into indoor air;\n(d) articles exclusively for industrial or professional use unless formaldehyde released\nfrom them leads to exposure of the general public under foreseeable conditions of use;\n(e) articles for which the restriction laid down in entry 72 applies;\n(f) articles that are biocidal products within the scope of Regulation (EU) No 528/2012 of\nthe European Parliament and of the Council1;\n(g) devices within the scope of Regulation (EU) 2017/745;\n(h) personal protective equipment within the scope of Regulation (EU) 2016/425;\n(i) articles intended to come into contact directly or indirectly with food within the scope\nof Regulation (EC) No 1935/2004;\n(j) second-hand articles.\n2. Shall not be placed on the market in road vehicles after 6 August 2027 if, under the test\nconditions specified in Appendix 14, the concentration of formaldehyde in the interior of\nthose vehicles exceeds 0,062 mg/m3\n.\nThe first subparagraph shall not apply to:\n(a) road vehicles exclusively for industrial or professional use unless the concentration of\nformaldehyde in the interior of those vehicles leads to exposure of the general public\nunder foreseeable conditions of use;\n(b) second-hand vehicles."},"1. Shall not be placed on the market in articles, after 6 August 2026, if, under the test\nconditions specified in Appendix 14, the concentration of formaldehyde released from those\narticles exceeds:\n(a) 0,062 mg/m3 for furniture and wood-based articles;\n(b) 0,080 mg/m3 for articles other than furniture and wood-based articles.\nThe first subparagraph shall not apply to:\n(a) articles in which formaldehyde or formaldehyde releasing substances are exclusively\nnaturally present in the materials from which the articles are produced;\n(b) articles that are exclusively for outdoor use under foreseeable conditions;\n(c) articles in constructions, that are exclusively used outside the building shell and\nvapour barrier and that do not emit formaldehyde into indoor air;\n(d) articles exclusively for industrial or professional use unless formaldehyde released\nfrom them leads to exposure of the general public under foreseeable conditions of use;\n(e) articles for which the restriction laid down in entry 72 applies;\n(f) articles that are biocidal products within the scope of Regulation (EU) No 528/2012 of\nthe European Parliament and of the Council1;\n(g) devices within the scope of Regulation (EU) 2017/745;\n(h) personal protective equipment within the scope of Regulation (EU) 2016/425;\n(i) articles intended to come into contact directly or indirectly with food within the scope\nof Regulation (EC) No 1935/2004;\n(j) second-hand articles.\n2. Shall not be placed on the market in road vehicles after 6 August 2027 if, under the test\nconditions specified in Appendix 14, the concentration of formaldehyde in the interior of\nthose vehicles exceeds 0,062 mg/m3\n.\nThe first subparagraph shall not apply to:\n(a) road vehicles exclusively for industrial or professional use unless the concentration of\nformaldehyde in the interior of those vehicles leads to exposure of the general public\nunder foreseeable conditions of use;\n(b) second-hand vehicles.","1. Dürfen nach dem 6. August 2026 nicht mehr in Erzeugnissen in Verkehr gebracht werden, wenn unter den in Anlage 14 genannten Prüfbedingungen die Konzentration an Formaldehyd, das aus diesen Erzeugnissen freigesetzt wird, folgende Werte überschreitet:\n    a) 0,062 mg/m3 für Möbel und Erzeugnisse auf Holzwerkstoffbasis;\n    b) 0,080 mg/m3 für andere Erzeugnisse als Möbel und Erzeugnisse auf Holzwerkstoffbasis.\n    Unterabsatz 1 gilt nicht für\n    a) Erzeugnisse, bei denen Formaldehyd oder Formaldehydabspalter ausschließlich natürlich in den Materialien vorkommen, aus denen die Erzeugnisse hergestellt werden;\n    b) Erzeugnisse, die unter vorhersehbaren Bedingungen ausschließlich zur Verwendung im Freien bestimmt sind;\n    c) Erzeugnisse in Bauwerken, die ausschließlich außerhalb der Gebäudehülle und der Dampfsperre verwendet werden und von denen kein Formaldehyd in die Innenraumluft freigesetzt wird;\n    d) Erzeugnisse, die ausschließlich für die industrielle oder gewerbliche Verwendung bestimmt sind, außer wenn aus ihnen freigesetztes Formaldehyd unter vorhersehbaren Verwendungsbedingungen zu einer Exposition der breiten Öffentlichkeit führt;\n    e) Erzeugnisse, für die die Beschränkung gemäß Eintrag 72 gilt;\n    f) Erzeugnisse, die als Biozidprodukte der Verordnung (EU) Nr. 528/2012 des Europäischen Parlaments und des Rates unterliegen(*);\n    g) Produkte, die in den Geltungsbereich der Verordnung (EU) 2017/745 des Europäischen Parlaments und des Rates fallen;\n    h) persönliche Schutzausrüstungen im Rahmen der Verordnung (EU) 2016/425;\n    i) Gegenstände, die dazu bestimmt sind, mit Lebensmitteln unmittelbar oder mittelbar in Berührung zu kommen, die in den Anwendungsbereich der Verordnung (EG) Nr. 1935/2004 fallen;\n    j) gebrauchte Erzeugnisse.\n2. Dürfen nach dem 6. August 2027 nicht mehr in Straßenfahrzeugen in Verkehr gebracht werden, wenn unter den in Anlage 14 genannten Prüfbedingungen die Konzentration an Formaldehyd im Inneren dieser Fahrzeuge 0,062 mg/m3 überschreitet.\n    Unterabsatz 1 gilt nicht für\n    a) Straßenfahrzeuge, die ausschließlich für die industrielle oder gewerbliche Verwendung bestimmt sind, es sei denn, die Konzentration von Formaldehyd im Inneren dieser Fahrzeuge führt unter vorhersehbaren Verwendungsbedingungen zu einer Exposition der breiten Öffentlichkeit;\n    b) Gebrauchtfahrzeuge.","1. 2026 年 8 月 6 日后，如果在附录 14 规定的测试条件下，物品中释放的甲醛浓度超过：\n(a) 家具和木制品为 0.062 mg/m3；\n(b) 家具和木质制品以外的制品为 0.080 mg/m3。\n第一项不适用于：\n(a) 甲醛或释放甲醛的物质完全天然存在于生产该制品的材料中的制品；\n(b) 专门供在可预见条件下户外使用的物品；\n(c) 专门用于建筑物外壳和防潮层之外且不向室内空气释放甲醛的建筑制品；\n(d) 专门用于工业或专业用途的物品，除非其释放的甲醛在可预见的使用条件下导致公众接触；\n(e) 适用于第 72 条规定的限制的物品；\n(f) 属于欧洲议会和理事会 1 法规 (EU) No 528/2012 范围内的杀菌产品的物品；\n(g) 法规 (EU) 2017/745 范围内的设备；\n(h) 法规(EU) 2016/425 范围内的个人防护设备；\n(i) 法规 (EC) No 1935/2004 范围内的直接或间接接触食品的物品；\n(j) 二手物品。\n2. 2027 年 8 月 6 日之后，如果在附录 14 规定的测试条件下，道路车辆车内甲醛浓度超过 0.062 mg/m3，则不得投放市场。\n第一项不适用于：\n(a) 专门用于工业或专业用途的道路车辆，除非这些车辆内部的甲醛浓度导致公众在可预见的使用条件下接触甲醛；\n(b) 二手车。"]
[null,{"$f":"IF($B$1=\"English\",C3806,IF($B$1=\"Deutsch\",D3806,IF($B$1=\"中文\",E3806,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"1. Shall not be placed on the market as substances on their own or, where the synthetic\npolymer microparticles are present to confer a sought-after characteristic, in mixtures in a\nconcentration equal to or greater than 0,01 % by weight.\n2. For the purposes of this entry, the following definitions apply:\n(a) “particle” means a minute piece of matter, other than single molecules, with defined\nphysical boundaries;\n(b) “solid” means a substance or mixture other than a liquid or gas;\n(c) “gas” means a substance or mixture which at 50 °C has a vapour pressure greater\nthan 300 kPa (absolute), or is completely gaseous at 20 °C at a standard pressure of\n101,3 kPa;\n(d) “liquid” means a substance or mixture that meets any of the following conditions:\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\n(i) the substance or mixture at 50 °C has a vapour pressure of not more than 300 kPa,\nis not completely gaseous at 20 °C and at a standard pressure of 101,3 kPa, and has a\nmelting point or initial melting point of 20 °C or less at a standard pressure of 101,3\nkPa;\n(ii) the substance or mixture fulfils the criteria in the American Society for Testing and\nMaterials (ASTM) D 4359-90 Standard Test Method for Determining Whether a Material\nIs a Liquid or a Solid;\n(iii) the substance or mixture passes the fluidity test (penetrometer test) described in\nchapter 2.3.4 of Part 2 of Annex A to the European Agreement concerning the\nInternational Carriage of Dangerous Goods by Road (ADR) concluded at Geneva on 30\nSeptember 1957;\n(e) “make-up product” means any substance or mixture intended to be placed in contact\nwith specific external parts of the human body, namely the epidermis, eye brows and eye\nlashes, with a view to, exclusively or mainly, changing their appearance;\n3. Where the concentration of synthetic polymer microparticles covered by this entry cannot\nbe determined by available analytical methods or accompanying documentation, in order to\nverify the compliance with the concentration limit referred to in paragraph 1, only the\nparticles of at least the following size shall be taken into account:\n(a) 0,1 μm for any dimension, for particles where all dimensions are equal to or smaller\nthan 5 mm;\n(b) 0,3 μm in length, for particles that have a length that is equal to or smaller than 15\nmm and a length to diameter ratio greater than 3.\n4. Paragraph 1 shall not apply to the placing on the market of:\n(a) synthetic polymer microparticles, as substances on their own or in mixtures, for use\nat industrial sites;\n(b) medicinal products within the scope of Directive 2001/83/EC and veterinary medicinal\nproducts within the scope of Regulation (EU) 2019/6 of the European Parliament and of\nthe Council;\n(c) EU fertilising products within the scope of Regulation (EU) 2019/1009 of the European\nParliament and of the Council;\n(d) food additives within the scope of Regulation (EC) No 1333/2008 of the European\nParliament and of the Council;\n(e) in vitro diagnostic devices, including devices within the scope of Regulation (EU)\n2017/746 of the European Parliament and of the Council;\n(f) food within the meaning of Article 2 of Regulation (EC) No 178/2002, not covered by\npoint (d) of this paragraph, and feed as defined in Article 3(4) of that Regulation.\n5. Paragraph 1 shall not apply to the placing on the market of the following synthetic\npolymer microparticles, as substances on their own or in mixtures:\n(a) synthetic polymer microparticles which are contained by technical means so that\nreleases to the environment are prevented when used in accordance with the instructions\nfor use during the intended end use;\n(b) synthetic polymer microparticles the physical properties of which are permanently\nmodified during intended end use in such a way that the polymer no longer falls within\nthe scope of this entry;\n(c) synthetic polymer microparticles which are permanently incorporated into a solid\nmatrix during intended end use.\n6. Paragraph 1 shall apply as follows regarding the following uses:\n(a) from 17 October 2029 to synthetic polymer microparticles for use in the encapsulation\nof fragrances;\n(b) from 17 October 2027 for “rinse-off products” as defined in point (1)(a) of the\nPreamble to Annexes II to VI to Regulation (EC) No 1223/2009 unless such products are\ncovered by point (a) of this paragraph or contain synthetic polymer microparticles for use\nas an abrasive, i.e. namely to exfoliate, polish or clean (“microbeads”);\n(c) from 17 October 2035 for lip products as defined in point (1)(e) of the Preamble to\nAnnexes II to VI to Regulation (EC) No 1223/2009, nail products as defined in point\n(1)(g) of the Preamble to Annexes II to VI to that Regulation, and make-up products\nwithin the scope of that Regulation, unless such products are covered by points (a) or (b)\nof this paragraph or contain microbeads;\n(d) from 17 October 2029 for leave-on products, as defined in point (1)(b) of the\nPreamble to Annexes II to VI to Regulation (EC) No 1223/2009, unless such products are\ncovered by points (a) or (c) of this paragraph;\n(e) from 17 October 2028 for detergents, as defined in Article 2(1) of Regulation (EC) No\n648/2004, waxes, polishes and air care products, unless those products are covered by\npoint (a) of this paragraph or contain microbeads;\n(f) from 17 October 2029 for “devices”, within the scope of Regulation (EU) 2017/745 of\nthe European Parliament and of the Council, unless those devices contain microbeads;\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\n(g) from 17 October 2028 for “fertilising products”, as defined in Article 2, point (1), of\nRegulation (EU) 2019/1009, which do not fall within the scope of that Regulation;\n(h) from 17 October 2031 for plant protection products within the meaning of Article 2(1)\nof Regulation (EC) No 1107/2009 of the European Parliament and of the Council6 and\nseeds treated with those products, and biocidal products as defined in Article 3(1), point\n(a), of Regulation (EU) No 528/2012 of the European Parliament and of the Council7;\n(i) from 17 October 2028 for products for agricultural and horticultural uses not covered\nby points (g) or (h);\n(j) from 17 October 2031 for granular infill for use on synthetic sports surfaces.\n7. From 17 October 2025 suppliers of synthetic polymer microparticles referred to in\nparagraph 4, point (a), shall provide the following information:\n(a) instructions for use and disposal explaining to industrial downstream users how to\nprevent releases of synthetic polymer microparticles to the environment;\n(b) the following statement:\n“The synthetic polymer microparticles supplied is subject to conditions laid down by\nentry 78 of Annex XVII to Regulation (EC) No 1907/2006 of the European Parliament\nand of the Council”;\n(c) the information on quantity or, as applicable, concentration of synthetic polymer\nmicroparticles in the substance or mixture;\n(d) generic information on the identity of the polymers contained in the substance or\nmixture that enables manufacturers, industrial downstream users and other suppliers to\ncomply with their obligations laid down in paragraphs 11 and 12.\n8. From 17 October 2026 suppliers of products containing synthetic polymer microparticles\nreferred to in paragraph 4, point (e), and from 17 October 2025 suppliers of products\ncontaining synthetic polymer microparticles referred to in paragraph 4, point (d), and\nparagraph 5, shall provide instructions for use and disposal explaining to professional users\nand the general public how to prevent releases of synthetic polymer microparticles to the\nenvironment.\n9. From 17 October 2031 until 16 October 2035 suppliers of products referred to in\nparagraph 6, point (c), containing synthetic polymer microparticles shall provide the\nfollowing statement: “This product contains microplastics.” However, products placed on the\nmarket before 17 October 2031 are not required to bear that statement until 17 December\n2031.\n10. The information referred to in paragraphs 7, 8 and 9 shall be provided in the form of\nclearly visible, legible and indelible text or, where appropriate regarding the information in\nparagraphs 7 and 8, in the form of pictograms. The text or pictograms shall be placed on the\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\nlabel, the packaging, or the package leaflet of the products containing synthetic polymer\nmicroparticles or, regarding the information in paragraph 7, on the safety data sheet. In\naddition to the text or pictograms, suppliers may provide a digital tool that gives access to\nan electronic version of that information. Where instructions for use and disposal are\nprovided in accordance with paragraphs 7, 8 and 9 in the form of a text, they shall be in the\nofficial languages of the Member States where the substance or mixture is placed on the\nmarket, unless the Member States concerned provide otherwise.\n11. Starting from 2026 manufacturers and industrial downstream users of synthetic polymer\nmicroparticles in the form of pellets, flakes, and powders used as feedstock in plastic\nmanufacturing at industrial sites, and, starting from 2027, other manufacturers of synthetic\npolymer microparticles and other industrial downstream users using synthetic polymer\nmicroparticles at industrial sites shall submit the following information to the Agency by 31\nMay of each year:\n(a) a description of the uses of synthetic polymer microparticles in the previous calendar\nyear;\n(b) for each use of synthetic polymer microparticles, generic information on the identity\nof the polymers used;\n(c) for each use of synthetic polymer microparticles, an estimate of the quantity of\nsynthetic polymer microparticles released to the environment in the previous calendar\nyear, which shall include also the quantity of synthetic polymer microparticles released to\nthe environment during transportation.\n(d) for each use of synthetic polymer microparticles, a reference to the derogation laid\ndown in paragraph 4, point (a).\n12. From 2027, suppliers of products containing synthetic polymer microparticles refe rred to\nin paragraphs 4, points (b), (d) and (e), and paragraph 5, placed on the market for the first\ntime to professional users and the general public, shall submit the following information to\nthe Agency by 31 May of each year:\n(a) a description of the end uses for which the synthetic polymer microparticles were\nplaced on the market in the previous calendar year;\n(b) for each end use for which the synthetic polymer microparticles were placed on the\nmarket, generic information on the identity of the polymers placed on the market in the\nprevious calendar year;\n(c) for each end use for which the synthetic polymer microparticles were placed on the\nmarket, an estimate of the quantity of synthetic polymer microparticles released to the\nenvironment in the previous calendar year, which shall include also the quantity of\nsynthetic polymer microparticles released to the environment during transportation.\n(d) for each use of synthetic polymer microparticles, a reference to the applicable\nderogation or derogations laid down in paragraph 4, point (b), (d) or (e), or 5 point (a),\n(b) or (c).\n13. The Agency shall make the information submitted under paragraphs 11 and 12 available\nto the Member States.\n14. Manufacturers, importers and industrial downstream users of products containing\nsynthetic polymer microparticles shall provide specific information on the identity of\npolymers covered by this entry contained in those products and the function of those\npolymers in the products to competent authorities upon their request. The specific\ninformation on the polymer identity shall be sufficient to unequivocally identify polymers and\nshall at least include the information laid down in points 2.1 to 2.2.3 and points 2.3.5, 2.3.6\nand 2.3.7 of Annex VI, where applicable. If the information is not available to industrial\ndownstream users, they shall request it from their supplier within 7 days from the receipt of\nthe request from the competent authorities and shall inform the authorities of the request\nmade without delay. Having received the request referred to in the second subparagraph,\nthe suppliers shall provide the requested information within 30 days to the industrial\ndownstream user or directly to the competent authority requesting it. Where the supplier\nprovides the information to the industrial downstream user, the industrial downstream user\nshall forward that information to the competent authorities without delay. Where the\nsupplier provides the information directly to the authority, it shall without delay inform the\nindustrial downstream user concerned to that effect.\n15. Manufacturers, importers and industrial downstream users of products containing\npolymers claimed to be excluded from the designation of synthetic polymer microparticles on\ngrounds of degradability or solubility shall provide, without delay, information proving that\nthose polymers are degradable in accordance with Appendix 15 or soluble in accordance with\nAppendix 16, as applicable, to competent authorities upon their request.\n16. Paragraph 1 shall not apply to placing on the market of synthetic polymers\nmicroparticles, on their own or in mixtures, placed on the market before 17 October 2023.\nHowever, the first subparagraph shall not apply to the placing on the market of synthetic\npolymers microparticles for uses listed in paragraph 6."},"1. Shall not be placed on the market as substances on their own or, where the synthetic\npolymer microparticles are present to confer a sought-after characteristic, in mixtures in a\nconcentration equal to or greater than 0,01 % by weight.\n2. For the purposes of this entry, the following definitions apply:\n(a) “particle” means a minute piece of matter, other than single molecules, with defined\nphysical boundaries;\n(b) “solid” means a substance or mixture other than a liquid or gas;\n(c) “gas” means a substance or mixture which at 50 °C has a vapour pressure greater\nthan 300 kPa (absolute), or is completely gaseous at 20 °C at a standard pressure of\n101,3 kPa;\n(d) “liquid” means a substance or mixture that meets any of the following conditions:\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\n(i) the substance or mixture at 50 °C has a vapour pressure of not more than 300 kPa,\nis not completely gaseous at 20 °C and at a standard pressure of 101,3 kPa, and has a\nmelting point or initial melting point of 20 °C or less at a standard pressure of 101,3\nkPa;\n(ii) the substance or mixture fulfils the criteria in the American Society for Testing and\nMaterials (ASTM) D 4359-90 Standard Test Method for Determining Whether a Material\nIs a Liquid or a Solid;\n(iii) the substance or mixture passes the fluidity test (penetrometer test) described in\nchapter 2.3.4 of Part 2 of Annex A to the European Agreement concerning the\nInternational Carriage of Dangerous Goods by Road (ADR) concluded at Geneva on 30\nSeptember 1957;\n(e) “make-up product” means any substance or mixture intended to be placed in contact\nwith specific external parts of the human body, namely the epidermis, eye brows and eye\nlashes, with a view to, exclusively or mainly, changing their appearance;\n3. Where the concentration of synthetic polymer microparticles covered by this entry cannot\nbe determined by available analytical methods or accompanying documentation, in order to\nverify the compliance with the concentration limit referred to in paragraph 1, only the\nparticles of at least the following size shall be taken into account:\n(a) 0,1 μm for any dimension, for particles where all dimensions are equal to or smaller\nthan 5 mm;\n(b) 0,3 μm in length, for particles that have a length that is equal to or smaller than 15\nmm and a length to diameter ratio greater than 3.\n4. Paragraph 1 shall not apply to the placing on the market of:\n(a) synthetic polymer microparticles, as substances on their own or in mixtures, for use\nat industrial sites;\n(b) medicinal products within the scope of Directive 2001/83/EC and veterinary medicinal\nproducts within the scope of Regulation (EU) 2019/6 of the European Parliament and of\nthe Council;\n(c) EU fertilising products within the scope of Regulation (EU) 2019/1009 of the European\nParliament and of the Council;\n(d) food additives within the scope of Regulation (EC) No 1333/2008 of the European\nParliament and of the Council;\n(e) in vitro diagnostic devices, including devices within the scope of Regulation (EU)\n2017/746 of the European Parliament and of the Council;\n(f) food within the meaning of Article 2 of Regulation (EC) No 178/2002, not covered by\npoint (d) of this paragraph, and feed as defined in Article 3(4) of that Regulation.\n5. Paragraph 1 shall not apply to the placing on the market of the following synthetic\npolymer microparticles, as substances on their own or in mixtures:\n(a) synthetic polymer microparticles which are contained by technical means so that\nreleases to the environment are prevented when used in accordance with the instructions\nfor use during the intended end use;\n(b) synthetic polymer microparticles the physical properties of which are permanently\nmodified during intended end use in such a way that the polymer no longer falls within\nthe scope of this entry;\n(c) synthetic polymer microparticles which are permanently incorporated into a solid\nmatrix during intended end use.\n6. Paragraph 1 shall apply as follows regarding the following uses:\n(a) from 17 October 2029 to synthetic polymer microparticles for use in the encapsulation\nof fragrances;\n(b) from 17 October 2027 for “rinse-off products” as defined in point (1)(a) of the\nPreamble to Annexes II to VI to Regulation (EC) No 1223/2009 unless such products are\ncovered by point (a) of this paragraph or contain synthetic polymer microparticles for use\nas an abrasive, i.e. namely to exfoliate, polish or clean (“microbeads”);\n(c) from 17 October 2035 for lip products as defined in point (1)(e) of the Preamble to\nAnnexes II to VI to Regulation (EC) No 1223/2009, nail products as defined in point\n(1)(g) of the Preamble to Annexes II to VI to that Regulation, and make-up products\nwithin the scope of that Regulation, unless such products are covered by points (a) or (b)\nof this paragraph or contain microbeads;\n(d) from 17 October 2029 for leave-on products, as defined in point (1)(b) of the\nPreamble to Annexes II to VI to Regulation (EC) No 1223/2009, unless such products are\ncovered by points (a) or (c) of this paragraph;\n(e) from 17 October 2028 for detergents, as defined in Article 2(1) of Regulation (EC) No\n648/2004, waxes, polishes and air care products, unless those products are covered by\npoint (a) of this paragraph or contain microbeads;\n(f) from 17 October 2029 for “devices”, within the scope of Regulation (EU) 2017/745 of\nthe European Parliament and of the Council, unless those devices contain microbeads;\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\n(g) from 17 October 2028 for “fertilising products”, as defined in Article 2, point (1), of\nRegulation (EU) 2019/1009, which do not fall within the scope of that Regulation;\n(h) from 17 October 2031 for plant protection products within the meaning of Article 2(1)\nof Regulation (EC) No 1107/2009 of the European Parliament and of the Council6 and\nseeds treated with those products, and biocidal products as defined in Article 3(1), point\n(a), of Regulation (EU) No 528/2012 of the European Parliament and of the Council7;\n(i) from 17 October 2028 for products for agricultural and horticultural uses not covered\nby points (g) or (h);\n(j) from 17 October 2031 for granular infill for use on synthetic sports surfaces.\n7. From 17 October 2025 suppliers of synthetic polymer microparticles referred to in\nparagraph 4, point (a), shall provide the following information:\n(a) instructions for use and disposal explaining to industrial downstream users how to\nprevent releases of synthetic polymer microparticles to the environment;\n(b) the following statement:\n“The synthetic polymer microparticles supplied is subject to conditions laid down by\nentry 78 of Annex XVII to Regulation (EC) No 1907/2006 of the European Parliament\nand of the Council”;\n(c) the information on quantity or, as applicable, concentration of synthetic polymer\nmicroparticles in the substance or mixture;\n(d) generic information on the identity of the polymers contained in the substance or\nmixture that enables manufacturers, industrial downstream users and other suppliers to\ncomply with their obligations laid down in paragraphs 11 and 12.\n8. From 17 October 2026 suppliers of products containing synthetic polymer microparticles\nreferred to in paragraph 4, point (e), and from 17 October 2025 suppliers of products\ncontaining synthetic polymer microparticles referred to in paragraph 4, point (d), and\nparagraph 5, shall provide instructions for use and disposal explaining to professional users\nand the general public how to prevent releases of synthetic polymer microparticles to the\nenvironment.\n9. From 17 October 2031 until 16 October 2035 suppliers of products referred to in\nparagraph 6, point (c), containing synthetic polymer microparticles shall provide the\nfollowing statement: “This product contains microplastics.” However, products placed on the\nmarket before 17 October 2031 are not required to bear that statement until 17 December\n2031.\n10. The information referred to in paragraphs 7, 8 and 9 shall be provided in the form of\nclearly visible, legible and indelible text or, where appropriate regarding the information in\nparagraphs 7 and 8, in the form of pictograms. The text or pictograms shall be placed on the\nP.O. Box 400, FI-00121 Helsinki, Finland | Tel. +358 9 686180 | echa.europa.eu\nlabel, the packaging, or the package leaflet of the products containing synthetic polymer\nmicroparticles or, regarding the information in paragraph 7, on the safety data sheet. In\naddition to the text or pictograms, suppliers may provide a digital tool that gives access to\nan electronic version of that information. Where instructions for use and disposal are\nprovided in accordance with paragraphs 7, 8 and 9 in the form of a text, they shall be in the\nofficial languages of the Member States where the substance or mixture is placed on the\nmarket, unless the Member States concerned provide otherwise.\n11. Starting from 2026 manufacturers and industrial downstream users of synthetic polymer\nmicroparticles in the form of pellets, flakes, and powders used as feedstock in plastic\nmanufacturing at industrial sites, and, starting from 2027, other manufacturers of synthetic\npolymer microparticles and other industrial downstream users using synthetic polymer\nmicroparticles at industrial sites shall submit the following information to the Agency by 31\nMay of each year:\n(a) a description of the uses of synthetic polymer microparticles in the previous calendar\nyear;\n(b) for each use of synthetic polymer microparticles, generic information on the identity\nof the polymers used;\n(c) for each use of synthetic polymer microparticles, an estimate of the quantity of\nsynthetic polymer microparticles released to the environment in the previous calendar\nyear, which shall include also the quantity of synthetic polymer microparticles released to\nthe environment during transportation.\n(d) for each use of synthetic polymer microparticles, a reference to the derogation laid\ndown in paragraph 4, point (a).\n12. From 2027, suppliers of products containing synthetic polymer microparticles refe rred to\nin paragraphs 4, points (b), (d) and (e), and paragraph 5, placed on the market for the first\ntime to professional users and the general public, shall submit the following information to\nthe Agency by 31 May of each year:\n(a) a description of the end uses for which the synthetic polymer microparticles were\nplaced on the market in the previous calendar year;\n(b) for each end use for which the synthetic polymer microparticles were placed on the\nmarket, generic information on the identity of the polymers placed on the market in the\nprevious calendar year;\n(c) for each end use for which the synthetic polymer microparticles were placed on the\nmarket, an estimate of the quantity of synthetic polymer microparticles released to the\nenvironment in the previous calendar year, which shall include also the quantity of\nsynthetic polymer microparticles released to the environment during transportation.\n(d) for each use of synthetic polymer microparticles, a reference to the applicable\nderogation or derogations laid down in paragraph 4, point (b), (d) or (e), or 5 point (a),\n(b) or (c).\n13. The Agency shall make the information submitted under paragraphs 11 and 12 available\nto the Member States.\n14. Manufacturers, importers and industrial downstream users of products containing\nsynthetic polymer microparticles shall provide specific information on the identity of\npolymers covered by this entry contained in those products and the function of those\npolymers in the products to competent authorities upon their request. The specific\ninformation on the polymer identity shall be sufficient to unequivocally identify polymers and\nshall at least include the information laid down in points 2.1 to 2.2.3 and points 2.3.5, 2.3.6\nand 2.3.7 of Annex VI, where applicable. If the information is not available to industrial\ndownstream users, they shall request it from their supplier within 7 days from the receipt of\nthe request from the competent authorities and shall inform the authorities of the request\nmade without delay. Having received the request referred to in the second subparagraph,\nthe suppliers shall provide the requested information within 30 days to the industrial\ndownstream user or directly to the competent authority requesting it. Where the supplier\nprovides the information to the industrial downstream user, the industrial downstream user\nshall forward that information to the competent authorities without delay. Where the\nsupplier provides the information directly to the authority, it shall without delay inform the\nindustrial downstream user concerned to that effect.\n15. Manufacturers, importers and industrial downstream users of products containing\npolymers claimed to be excluded from the designation of synthetic polymer microparticles on\ngrounds of degradability or solubility shall provide, without delay, information proving that\nthose polymers are degradable in accordance with Appendix 15 or soluble in accordance with\nAppendix 16, as applicable, to competent authorities upon their request.\n16. Paragraph 1 shall not apply to placing on the market of synthetic polymers\nmicroparticles, on their own or in mixtures, placed on the market before 17 October 2023.\nHowever, the first subparagraph shall not apply to the placing on the market of synthetic\npolymers microparticles for uses listed in paragraph 6.","1. Dürfen nicht als solche oder, wenn die synthetischen Polymermikropartikel vorhanden sind, um eine gewünschte Eigenschaft zu verleihen, in Gemischen in einer Konzentration von 0,01 Gewichtsprozent oder mehr in Verkehr gebracht werden.\n2. Für die Zwecke dieses Eintrags gelten folgende Begriffsbestimmungen:\n    a) ‚Partikel‘ bezeichnet ein winziges Materialteilchen, ausgenommen einzelne Moleküle, mit definierten physischen Grenzen;\n    b) ‚Feststoff‘ bezeichnet einen anderen Stoff oder ein anderes Gemisch als eine Flüssigkeit oder ein Gas.\n    c) ‚Gas‘ bezeichnet einen Stoff oder ein Gemisch, der bzw. das bei 50 °C einen Dampfdruck von mehr als 300 kPa   (absolut) hat oder bei 20 °C und einem Standarddruck von 101,3 kPa vollständig gasförmig ist.\n    d) ‚Flüssigkeit‘ bezeichnet einen Stoff oder ein Gemisch, der bzw. das eine der folgenden Bedingungen erfüllt:\n    i) Der Stoff oder das Gemisch hat bei 50 °C einen Dampfdruck von nicht mehr als 300 kPa, ist bei 20 °C und einem Standarddruck von 101,3 kPa nicht vollständig gasförmig und hat einen Schmelzpunkt oder Schmelzbeginn von 20 °C oder weniger bei einem Standarddruck von 101,3 kPa;\n    ii) der Stoff oder das Gemisch erfüllt die Kriterien der Norm D 4359-90 ‚Standard Test Method For Determining Whether A Material Is A Liquid Or A Solid‘ der American Society for Testing and Materials (ASTM);\n    iii) der Stoff oder das Gemisch besteht die Prüfung zur Bestimmung des Fließverhaltens (Penetrometerverfahren) gemäß Anhang A Teil 2 Kapitel 2.3.4 des am 30. September 1957 in Genf geschlossenen Europäischen Übereinkommens über die internationale Beförderung gefährlicher Güter auf der Straße (ADR);\n    e) ‚Make-up-Produkt‘ bezeichnet jeden Stoff oder jedes Gemisch, der bzw. das dazu bestimmt ist, äußerlich mit bestimmten Teilen des menschlichen Körpers, nämlich Haut, Augenbrauen und Wimpern, in Berührung zu kommen, und zwar zu dem ausschließlichen oder überwiegenden Zweck, ihr Aussehen zu verändern.\n3. Kann die Konzentration der unter diesen Eintrag fallenden synthetischen Polymermikropartikel nicht anhand der verfügbaren Analysemethoden oder Begleitunterlagen bestimmt werden, so sind zur Überprüfung der Einhaltung des in Absatz 1 genannten Konzentrationsgrenzwerts nur die Partikel zu berücksichtigen, die mindestens die folgende Größe aufweisen:\n    a) 0,1 μm für eine Dimension bei Partikeln, bei denen alle Dimensionen gleich oder kleiner als 5 mm sind;\n    b) 0,3 μm für die Länge bei Partikeln mit einer Länge gleich oder kleiner als 15 mm und einem Verhältnis von Länge zu Durchmesser größer als 3.\n4. Absatz 1 gilt nicht für das Inverkehrbringen von\n    a) synthetischen Polymermikropartikeln als solche oder in Gemischen zur Verwendung in Industrieanlagen;\n    b) Arzneimitteln im Sinne der Richtlinie 2001/83/EG und Tierarzneimitteln im Sinne der Verordnung (EU) 2019/6 des Europäischen Parlaments und des Rates;\n    c) EU-Düngeprodukten im Sinne der Verordnung (EU) 2019/1009 des Europäischen Parlaments und des Rates;\n    d) Lebensmittelzusatzstoffen im Sinne der Verordnung (EG) Nr. 1333/2008 des Europäischen Parlaments und des Rates;\n    e) In-vitro-Diagnostika, einschließlich Produkte im Sinne der Verordnung (EU) 2017/746 des Europäischen Parlaments und des Rates;\n    f) Lebensmitteln im Sinne des Artikels 2 der Verordnung (EG) Nr. 178/2002, die nicht unter Buchstabe d des vorliegenden Absatzes fallen, und Futtermitteln im Sinne des Artikels 3 Nummer 4 der genannten Verordnung.\n5. Absatz 1 gilt nicht für das Inverkehrbringen der folgenden synthetischen Polymermikropartikel als solche oder in Gemischen:\n    a) synthetische Polymermikropartikel, die durch technische Mittel so eingeschlossen sind, dass eine Freisetzung in die Umwelt verhindert wird, wenn sie während der vorgesehenen Endanwendung vorschriftsmäßig verwendet werden;\n    b) synthetische Polymermikropartikel, deren physikalische Eigenschaften während der vorgesehenen Endanwendung dauerhaft so verändert werden, dass das Polymer nicht mehr in den Anwendungsbereich dieses Eintrags fällt;\n    c) synthetische Polymermikropartikel, die während der vorgesehenen Endverwendung dauerhaft in eine feste Matrix integriert werden.\n6. Absatz 1 gilt wie folgt für folgende Verwendungen:\n    a) ab dem 17. Oktober 2029 für synthetische Polymermikropartikel zur Verwendung bei der Verkapselung von Duftstoffen;\n    b) ab dem 17. Oktober 2027 für auszuspülende/abzuspülende Mittel im Sinne der Nummer 1 Buchstabe a der Präambel der Anhänge II bis VI der Verordnung (EG) Nr. 1223/2009, es sei denn, diese Mittel fallen unter Buchstabe a des vorliegenden Absatzes oder enthalten synthetische Polymermikropartikel zur Verwendung als Abrasivstoff, d. h. zum Peelen, Polieren oder Reinigen (im Folgenden ‚Mikroperlen‘);\n    c) ab dem 17. Oktober 2035 für Lippenmittel im Sinne der Nummer 1 Buchstabe e der Präambel der Anhänge II bis VI der Verordnung (EG) Nr. 1223/2009, für Nagelmittel im Sinne der Nummer 1 Buchstabe g der Präambel der Anhänge II bis VI der genannten Verordnung und für Make-up-Produkte, die in den Anwendungsbereich der genannten Verordnung fallen, es sei denn, diese Mittel und Produkte fallen unter Buchstabe a oder b des vorliegenden Absatzes oder enthalten Mikroperlen;\n    d) ab dem 17. Oktober 2029 für Mittel, die auf der Haut/in den Haaren verbleiben, im Sinne der Nummer 1 Buchstabe b der Präambel der Anhänge II bis VI der Verordnung (EG) Nr. 1223/2009, es sei denn, diese Mittel fallen unter Buchstabe a oder c des vorliegenden Absatzes;\n    e) ab dem 17. Oktober 2028 für Detergenzien im Sinne des Artikels 2 Absatz 1 der Verordnung (EG) Nr. 648/2004, Wachse, Poliermittel und Lufterfrischer, es sei denn, diese Mittel und Produkte fallen unter Buchstabe a des vorliegenden Absatzes oder enthalten Mikroperlen;\n    f) ab dem 17. Oktober 2029 für Produkte im Sinne der Verordnung (EU) 2017/745 des Europäischen Parlaments und des Rates, es sei denn, diese Produkte enthalten Mikroperlen;\n    g) ab dem 17. Oktober 2028 für Düngeprodukte im Sinne des Artikels 2 Nummer 1 der Verordnung (EU) 2019/1009, die nicht in den Anwendungsbereich der genannten Verordnung fallen;\n    h) ab dem 17. Oktober 2031 für Pflanzenschutzmittel im Sinne des Artikels 2 Nummer 1 der Verordnung (EG) Nr. 1107/2009 des Europäischen Parlaments und des Rates und mit diesen Produkten behandeltes Saatgut sowie Biozidprodukte im Sinne des Artikels 3 Absatz 1 Buchstabe a der Verordnung (EU) Nr. 528/2012 des Europäischen Parlaments und des Rates;\n    i) ab dem 17. Oktober 2028 für Produkte für landwirtschaftliche oder gartenbauliche Verwendungen, die nicht unter Buchstabe g oder h fallen;\n    j) ab dem 17. Oktober 2031 für Einstreugranulat für synthetische Sportböden.\n7. Ab dem 17. Oktober 2025 müssen Lieferanten synthetischer Polymermikropartikel im Sinne des Absatzes 4 Buchstabe a folgende Informationen bereitstellen:\n    a) Anweisungen für die Verwendung und Entsorgung für nachgeschaltete industrielle Anwender, in denen erläutert wird, wie die Freisetzung synthetischer Polymermikropartikel in die Umwelt verhindert werden kann;\n    b) den folgenden Hinweis: ‚Die gelieferten synthetischen Polymermikropartikel unterliegen den Bedingungen des Eintrags 78 in Anhang XVII der Verordnung (EG) Nr. 1907/2006 des Europäischen Parlaments und des Rates.‘;\n    c) Angaben zur Menge oder gegebenenfalls zur Konzentration synthetischer Polymermikropartikel im Stoff oder Gemisch;\n    d) allgemeine Informationen zur Identität der in dem Stoff oder Gemisch enthaltenen Polymere, die es den Herstellern, industriellen nachgeschalteten Anwendern und anderen Lieferanten ermöglichen, ihren Verpflichtungen gemäß den Absätzen 11 und 12 nachzukommen.\n8. Lieferanten von Produkten, die synthetische Polymermikropartikel im Sinne des Absatzes 4 Buchstabe e enthalten, müssen ab dem 17. Oktober 2026 und Lieferanten von Produkten, die synthetische Polymermikropartikel im Sinne des Absatzes 4 Buchstabe d und des Absatzes 5 enthalten, müssen ab dem 17. Oktober 2025 Anweisungen für die Verwendung und Entsorgung für gewerbliche Anwender und die breite Öffentlichkeit zur Verfügung stellen, in denen erläutert wird, wie die Freisetzung synthetischer Polymermikropartikel in die Umwelt verhindert werden kann.\n9. Ab dem 17. Oktober 2031 bis zum 16. Oktober 2035 müssen Lieferanten von Produkten im Sinne des Absatzes 6 Buchstabe c, die synthetische Polymermikropartikel enthalten, diese Produkte mit folgendem Hinweis versehen: ‚Dieses Produkt enthält Mikroplastik.‘ Produkte, die vor dem 17. Oktober 2031 in Verkehr gebracht wurden, müssen jedoch erst ab dem 17. Dezember 2031 mit diesem Hinweis versehen sein.\n10. Die Informationen gemäß den Absätzen 7, 8 und 9 müssen in Form von deutlich sichtbarem, lesbarem und unauslöschlichem Text bzw. die Informationen gemäß den Absätzen 7 und 8 gegebenenfalls in Form von Piktogrammen erfolgen. Der Text bzw. die Piktogramme muss bzw. müssen auf dem Etikett, der Verpackung oder in der Packungsbeilage der Produkte, die synthetische Polymermikropartikel enthalten, angegeben sein bzw. die Informationen gemäß Absatz 7 müssen sich im Sicherheitsdatenblatt befinden. Zusätzlich zu dem Text oder den Piktogrammen können Lieferanten ein digitales Instrument bereitstellen, das den Zugang zu einer elektronischen Version dieser Informationen ermöglicht.\n    Werden Anweisungen für die Verwendung und Entsorgung gemäß den Absätzen 7, 8 und 9 in Textform bereitgestellt, so sind sie in den Amtssprachen der Mitgliedstaaten abzufassen, in denen der Stoff oder das Gemisch in Verkehr gebracht wird, sofern dies von den betroffenen Mitgliedstaaten nicht anders geregelt wurde.\n11. Hersteller und nachgeschaltete industrielle Anwender von synthetischen Polymermikropartikeln in Form von Granulaten, Flocken und Pulvern, die als Ausgangsmaterial für die Kunststoffherstellung in industriellen Anlagen verwendet werden, bzw. andere Hersteller von synthetischen Polymermikropartikeln und andere nachgeschaltete industrielle Anwender, die synthetische Polymermikropartikel in industriellen Anlagen verwenden, müssen der Agentur ab dem Jahr 2026 bzw. ab dem Jahr 2027 bis zum 31. Mai jedes Jahres die folgenden Informationen vorlegen:\n    a) eine Beschreibung der Verwendungen von synthetischen Polymermikropartikeln im vorangegangenen Kalenderjahr;\n    b) für jede Verwendung synthetischer Polymermikropartikel allgemeine Informationen zur Identität der verwendeten Polymere;\n    c) für jede Verwendung synthetischer Polymermikropartikel eine Schätzung der Menge synthetischer Polymermikropartikel, die im vorangegangenen Kalenderjahr in die Umwelt freigesetzt wurden, einschließlich der Menge synthetischer Polymermikropartikel, die während des Transports in die Umwelt freigesetzt wurden;\n    d) für jede Verwendung von synthetischen Polymermikropartikeln einen Hinweis auf die Ausnahmeregelung gemäß Absatz 4 Buchstabe a.\n12. Ab dem Jahr 2027 müssen Lieferanten von Produkten, die synthetische Polymermikropartikel im Sinne des Absatzes 4 Buchstaben b, d und e sowie des Absatzes 5 enthalten und erstmals für gewerbliche Anwender und die breite Öffentlichkeit in Verkehr gebracht wurden, der Agentur bis zum 31. Mai jedes Jahres die folgenden Informationen vorlegen:\n    a) eine Beschreibung der Endverwendungen, für die die synthetischen Polymermikropartikel im vorangegangenen Kalenderjahr in Verkehr gebracht wurden;\n    b) für jede Endverwendung, für die die synthetischen Polymermikropartikel in Verkehr gebracht wurden, allgemeine Informationen über die Identität der im vorangegangenen Kalenderjahr in Verkehr gebrachten Polymere;\n    c) für jede Endverwendung, für die die synthetischen Polymermikropartikel in Verkehr gebracht wurden, eine Schätzung der Menge synthetischer Polymermikropartikel, die im vorangegangenen Kalenderjahr in die Umwelt freigesetzt wurden, einschließlich der Menge synthetischer Polymermikropartikel, die während des Transports in die Umwelt freigesetzt wurden;\n    d) für jede Verwendung von synthetischen Polymermikropartikeln einen Hinweis auf die geltende(n) Ausnahmeregelung(en) gemäß Absatz 4 Buchstabe b, d oder e oder Absatz 5 Buchstabe a, b oder c.\n 13. Die Agentur muss die gemäß den Absätzen 11 und 12 übermittelten Informationen den Mitgliedstaaten zur Verfügung stellen.\n 14. Hersteller, Importeure und nachgeschaltete industrielle Anwender von Produkten, die synthetische Polymermikropartikel enthalten, müssen den zuständigen Behörden auf deren Ersuchen spezifische Informationen über die Identität der unter diesen Eintrag fallenden Polymere, die in diesen Produkten enthalten sind, und über die Funktion dieser Polymere in den Produkten zur Verfügung stellen. Die spezifischen Informationen über die Identität der Polymere müssen ausreichen, um die Polymere eindeutig zu identifizieren, und mindestens die Angaben gemäß Anhang VI Nummern 2.1 bis 2.2.3 und Nummern 2.3.5, 2.3.6 und 2.3.7, sofern anwendbar, umfassen. Stehen die Informationen den nachgeschalteten industriellen Anwendern nicht zur Verfügung, so müssen sie diese innerhalb von sieben Tagen nach Eingang des Ersuchens der zuständigen Behörden bei ihrem Lieferanten anfordern und die Behörden unverzüglich darüber unterrichten.\n    Nach Eingang des Ersuchens gemäß Unterabsatz 2 müssen die Lieferanten die angeforderten Informationen innerhalb von 30 Tagen an den nachgeschalteten industriellen Anwender oder direkt an die zuständige Behörde, die die Informationen angefordert hat, übermitteln.\n    Stellt der Lieferant dem nachgeschalteten industriellen Anwender die Informationen zur Verfügung, so muss dieser sie unverzüglich an die zuständigen Behörden weiterleiten.\n    Stellt der Lieferant die Informationen direkt der Behörde zur Verfügung, so muss diese den betreffenden nachgeschalteten industriellen Anwender unverzüglich darüber unterrichten.\n15. Hersteller, Importeure und nachgeschaltete industrielle Anwender von Produkten, die Polymere enthalten, die aus Gründen der Abbaubarkeit oder Löslichkeit in Anspruch nehmen, von der Bezeichnung synthetischer Polymermikropartikel ausgenommen zu sein, müssen den zuständigen Behörden auf deren Ersuchen unverzüglich Informationen vorlegen, die belegen, dass diese Polymere abbaubar gemäß Anlage 15 bzw. löslich gemäß Anlage 16 sind.\n16. Absatz 1 gilt nicht für das Inverkehrbringen von synthetischen Polymermikropartikeln als solche oder in Gemischen, die vor dem 17. Oktober 2023 in Verkehr gebracht wurden.\n    Unterabsatz 1 gilt jedoch nicht für das Inverkehrbringen synthetischer Polymermikropartikel für die in Absatz 6 genannten Verwendungszwecke.","1.不得以单独物质的形式投放市场，或者当合成聚合物微粒被用于赋予混合物受欢迎的特性，且在混合物中的浓度等于或大于0.01%（以重量计）时不得投放市场。\n\n2.就本条目而言，以下定义适用：\n(a)“颗粒”是指除单分子之外的具有明确物理边界的微小物质；\n(b)“固体”是指液体或气体以外的物质或混合物；\n(c)“气体”是指在50℃时蒸气压大于300 kPa（绝对），或在20℃标准大气压101.3 kPa时完全气化的物质或混合物；\n(d)“液体”是指满足以下任一条件的物质或混合物：\n  (i)该物质或混合物在50℃时的蒸气压不超过300 kPa，在20℃标准大气压101.3 kPa时不完全气化，在标准大气压101.3 kPa下的熔点或初始熔点为20℃或更低；\n  (ii)该物质或混合物符合美国材料与试验协会(ASTM) D 4359-90 确定材料是液体还是固体的标准测试方法中的标准；\n  (iii)该物质或混合物通过了1957年9月30日在日内瓦缔结的《欧洲国际危险货物公路运输协定》(ADR)附件A第2部分第2.3.4章中所述的流动性测试（针入度测试）；\n(e)“化妆品”是指旨在与人体特定外部部分（即表皮、眉毛和睫毛）接触的任何物质或混合物，目的是专门或主要改变其外观；\n\n3.如果本条目涵盖的合成聚合物微粒的浓度无法通过现有的分析方法或随附文件确定，为了验证是否符合第1款中提到的浓度限值，仅应考虑至少具有以下尺寸的颗粒：\n(a)对于所有尺寸等于或小于5mm的颗粒，任意尺寸下限为0.1μm；\n(b)对于长度等于或小于15mm且长径比大于3的颗粒，长度下限为0.3μm。\n\n4.第1款不适用于投放市场的：\n(a)作为单独物质或用于混合物，在工业场所使用的合成聚合物微粒；\n(b)指令2001/83/EC范围内的医药产品以及欧洲议会和理事会法规 (EU) 2019/6范围内的兽药产品；\n(c)欧洲议会和理事会法规(EU) 2019/1009范围内的欧盟肥料产品；\n(d)欧洲议会和理事会(EC) No 1333/2008法规范围内的食品添加剂；\n(e)体外诊断设备，包括欧洲议会和理事会法规(EU) 2017/746范围内的设备；\n(f)法规(EC) No 178/2002第2条含义内、且本款(d)点未涵盖的食品，以及该法规第3(4)条定义的饲料。\n\n5.第1款不适用于将以下合成聚合物微粒作为单独物质或混合物投放市场：\n(a)通过技术手段，在预期最终使用过程中按照使用说明使用时可防止释放到环境中的合成聚合物微粒；\n(b)物理性质在预期最终使用过程中永久改变，使得聚合物不再落入本条目范围内的合成聚合物微粒；\n(c)在预期最终使用过程中被永久掺入固体基质中的合成聚合物微粒。\n\n6.第1款适用于下列用途：\n(a)自2029年10月17日起，适用于用于香料封装的合成聚合物微粒；\n(b)自2027年10月17日起，适用于法规 (EC) No 1223/2009附件II至VI序言第(1)(a)点中定义的“洗去类产品”，除非此类产品属于本款(a)点范围，或含有的合成聚合物微粒作为磨料使用，即用于去角质、抛光或清洁（“微珠”）；\n(c)自2035年10月17日起，适用于法规(EC) No 1223/2009附件II至VI前言第(1)(e)点定义的唇部产品，前言第(1)(g)点定义的美甲产品，以及该法规范围内的美妆产品，除非此类产品属于本款(a)或(b)点所涵盖的范围或含有微珠；\n(d)自2029年10月17日起，适用于法规(EC) No 1223/2009附件II至VI序言第(1)(b)点所定义驻留类产品，除非此类产品属于本款第(a)或(c)点所涵盖的范围；\n(e)自2028年10月17日起，适用于法规(EC) No 648/2004第2(1)条所定义的清洁剂，蜡、抛光剂和空气护理产品，除非这些产品属于本款(a)点所涵盖的范围或含有微珠；\n(f)自2029年10月17日起，适用于欧洲议会和理事会法规(EU) 2017/745范围内的“设备”，除非这些设备含有微珠；\n(g)自2028年10月17日起，适用于不属于法规(EU) 2019/1009第2条第(1)点定义范围的“肥料产品”；\n(h)自2031年10月17日起，适用于欧洲议会和理事会法规(EC) No 1107/2009第2(1)条含义内的植物保护产品，以及用这些产品处理过的种子，以及欧洲议会和理事会法规(EU) No 528/2012第3(1)条(a)点定义的生物杀灭剂产品；\n(i)自2028年10月17日起，适用于(g)或(h)点未涵盖的农业和园艺用途产品；\n(j)自2031年10月17日起，适用于合成材料运动场地面层上使用的颗粒填充物。\n\n7.自2025年10月17日起，第4款(a)点提到的合成聚合物微粒供应商应提供以下信息：\n(a)向工业下游用户解释如何防止合成聚合物微粒释放到环境中的使用和处置说明；\n(b)以下声明：“所提供的合成聚合物微粒须符合欧洲议会和理事会法规(EC) No 1907/2006附件XVII第78条规定的条件”；\n(c)有关物质或混合物中合成聚合物微粒的数量或浓度（如适用）的信息；\n(d)有关物质或混合物中所含聚合物特性的一般信息，使制造商、工业下游用户和其他供应商能够履行第11和12款规定的义务。\n\n8.自2026年10月17日起，含有第4款(e)点所述合成聚合物微粒产品的供应商，以及自2025年10月17日起，含有第4款(d)点和第5款所述合成聚合物微粒产品的供应商，应提供使用和处置说明，向专业用户和公众解释如何防止合成聚合物微粒释放到环境中。\n\n9.自2031年10月17日到2035年10月16日，第6款(c)点中提到的含有合成聚合物微粒产品的供应商应提供以下声明：“该产品含有微塑料。”2031年10月17日之前投放市场的产品在2031年12月17日之前无需附有该声明。\n\n10.第7、8和9款中提及的信息应以清晰可见、易读且不可磨灭的文本形式提供，或者在适用于第7款和第8款中的信息时，以象形图的形式提供。文字或象形图应放置在含有合成聚合物微粒产品的标签、包装或包装说明书上，或者就第7款的信息而言，应放置在安全数据表上。除了文本或象形图之外，供应商还可以提供数字工具来访问该信息的电子版本。\n如果按照第7、8和9款以文本形式提供使用和处置说明，则应使用该物质或混合物投放市场的成员国的官方语言，除非该成员国有关部门另有规定的。\n\n11.自2026年开始，在工业现场使用颗粒、薄片和粉末形式的合成聚合物微粒作为塑料制造原料的制造商和工业下游用户，以及自2027年开始，其他合成聚合物微粒制造商和其他在工业场所使用合成聚合物微粒的工业下游用户，应在每年5月31日之前向管理局提交以下信息：\n(a)上一日历年合成聚合物微粒用途的描述；\n(b)对于合成聚合物微粒的每次使用，有关所用聚合物特性的一般信息；\n(c)对于合成聚合物微粒的每次使用，估算上一日历年向环境释放的合成聚合物微粒的数量，其中还应包括运输过程中向环境释放的合成聚合物微粒的数量。\n(d)对于合成聚合物微粒的每次使用，参考第4款(a)点中规定的豁免。\n\n12.自2027年起，首次向专业用户和公众投放市场的第4款（b）、（d）和（e）点以及第5款中提到的含有合成聚合物微粒产品的供应商，应每年5月31日之前向管理局提交以下信息：\n(a)上一日历年合成聚合物微粒投放市场的最终用途的描述；\n(b)对于合成聚合物微粒投放市场的每种最终用途，有关上一日历年投放市场的聚合物特性的一般信息；\n(c)对于合成聚合物微粒投放市场的每种最终用途，估算上一日历年释放到环境中的合成聚合物微粒的数量，其中还应包括运输过程中释放到环境中的合成聚合物微粒的数量。\n(d)对于合成聚合物微粒的每次使用，提及第4款(b)、(d)或(e)点或第5款(a)、(b)或(c)点中规定的适用的一项或多项豁免。\n\n13.管理机构应向成员国提供根据第11和12款提交的信息。\n\n14.含有合成聚合物微粒的产品的制造商、进口商和工业下游用户应应主管当局的要求，提供有关这些产品中本条目所涵盖的聚合物的特性以及这些聚合物在产品中的功能的具体信息。有关聚合物特性的具体信息应足以明确识别聚合物，并应至少包括附件VI第2.1至2.2.3点以及第2.3.5、2.3.6和2.3.7点（如适用）中规定的信息。\n如果工业下游用户无法获得该信息，他们应在收到主管当局的请求后7天内向其供应商索取，并应立即将所提出的请求通知当局。\n供应商收到上述要求后，应在30天内向工业下游用户或直接向提出要求的主管机关提供所要求的信息。\n供应商向工业下游用户提供信息的，工业下游用户应及时将该信息转发给主管部门。如果供应商直接向主管部门提供信息，则应立即将此信息告知相关工业下游用户。\n\n15.含有声称因可降解性或溶解性而被排除在指定合成聚合物微粒范围之外的聚合物的产品的制造商、进口商和工业下游用户，应立即应主管当局要求，提供信息证明这些聚合物根据附录15是可降解的或根据附录16是可溶解（如适用）。\n\n16.第1款不适用于2023年10月17日之前投放市场的合成聚合物微粒以单独或是混合物的形式投放市场。\n然而，第一段不适用于第6段所列用途的合成聚合物微粒的投放市场。"]
[null,{"$f":"IF($B$1=\"English\",C3807,IF($B$1=\"Deutsch\",D3807,IF($B$1=\"中文\",E3807,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"a) 0,062 mg/m3 for furniture and wood-based articles;\n(b) 0,080 mg/m3 for articles other than furniture and wood-based articles"},"a) 0,062 mg/m3 for furniture and wood-based articles;\n(b) 0,080 mg/m3 for articles other than furniture and wood-based articles"," a) 0,062 mg/m3 für Möbel und Gegenstände auf Holzbasis;\n(b) 0,080 mg/m3 für andere Gegenstände als Möbel und Gegenstände auf Holzbasis","a) 家具和木制品为 0.062 mg/m3；\n(b) 家具和木质制品以外的制品为 0,080 mg/m3"]
[null,{"$f":"IF($B$1=\"English\",C3808,IF($B$1=\"Deutsch\",D3808,IF($B$1=\"中文\",E3808,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Included in Annex XIV:\nlast application date: 01.11.2023\nsunset date: 01.05.2025"},"Included in Annex XIV:\nlast application date: 01.11.2023\nsunset date: 01.05.2025","Included in Annex XIV:\nlast application date: 01.11.2023\nsunset date: 01.05.2025","包含在附件十四中：\n最后申请日期：2023 年 11 月 1 日\n日落日期：2025 年 5 月 1 日"]
[null,{"$f":"IF($B$1=\"English\",C3809,IF($B$1=\"Deutsch\",D3809,IF($B$1=\"中文\",E3809,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Monteponite (CdO)"},"Monteponite (CdO)","Monteponite (CdO)","蒙脱石 (CdO)"]
[null,{"$f":"IF($B$1=\"English\",C3810,IF($B$1=\"Deutsch\",D3810,IF($B$1=\"中文\",E3810,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Oligomerisation and alkylation reaction products of 2-phenylpropene and phenol"},"Oligomerisation and alkylation reaction products of 2-phenylpropene and phenol","Oligomerisierungs- und Alkylierungsreaktionsprodukte von 2-Phenylpropen und Phenol ","2-苯基丙烯与苯酚的低聚和烷基化反应产物"]
[null,{"$f":"IF($B$1=\"English\",C3811,IF($B$1=\"Deutsch\",D3811,IF($B$1=\"中文\",E3811,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Phenol, methylstyrenated"},"Phenol, methylstyrenated","Phenol, methylstyrolisiert","甲基苯乙烯化苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3812,IF($B$1=\"Deutsch\",D3812,IF($B$1=\"中文\",E3812,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Bumetrizole (UV-326)"},"Bumetrizole (UV-326)","Bumetrizol  (UV-326)","布美曲唑 (UV-326)"]
[null,{"$f":"IF($B$1=\"English\",C3813,IF($B$1=\"Deutsch\",D3813,IF($B$1=\"中文\",E3813,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(dimethylamino)-2-[(4-methylphenyl)methyl]-1-[4-(morpholin-4-yl)phenyl]butan-1-one"},"2-(dimethylamino)-2-[(4-methylphenyl)methyl]-1-[4-(morpholin-4-yl)phenyl]butan-1-one","2-(Dimethylamino)-2-[(4-methylphenyl)methyl]-1-[4-(morpholin-4-yl)phenyl]butan-1-on ","2-(二甲基氨基)-2-[(4-甲基苯基)甲基]-1-[4-(吗啉-4-基)苯基]丁-1-酮"]
[null,{"$f":"IF($B$1=\"English\",C3814,IF($B$1=\"Deutsch\",D3814,IF($B$1=\"中文\",E3814,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2-(2H-benzotriazol-2-yl)-4-(1,1,3,3-tetramethylbutyl)phenol (UV-329)"},"2-(2H-benzotriazol-2-yl)-4-(1,1,3,3-tetramethylbutyl)phenol (UV-329)","2-(2H-Benzotriazol-2-yl)-4-(1,1,3,3-tetramethylbutyl)phenol (UV-329)","2-(2H-苯并三唑-2-基)-4-(1,1,3,3-四甲基丁基)苯酚 (UV-329)"]
[null,{"$f":"IF($B$1=\"English\",C3815,IF($B$1=\"Deutsch\",D3815,IF($B$1=\"中文\",E3815,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"2,4,6-tri-tert-butylphenol"},"2,4,6-tri-tert-butylphenol","2,4,6-Tri-tert-butylphenol ","2,4,6-三叔丁基苯酚"]
[null,{"$f":"IF($B$1=\"English\",C3816,IF($B$1=\"Deutsch\",D3816,IF($B$1=\"中文\",E3816,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, inks and toners and polymers."},"Adhesives and sealants, coating products, fillers, putties, plasters, modelling clay, inks and toners and polymers.","Kleb- und Dichtstoffen, Beschichtungsprodukten, Füllstoffen, Kitten, Putzen, Modelliermasse, Tinten, Tonern und Polymeren","粘合剂和密封剂、涂料产品、填料、腻子、灰泥、造型粘土、油墨、墨粉和聚合物。"]
[null,{"$f":"IF($B$1=\"English\",C3817,IF($B$1=\"Deutsch\",D3817,IF($B$1=\"中文\",E3817,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Coating products, adhesives and sealants and washing and cleaning products."},"Coating products, adhesives and sealants and washing and cleaning products.","Beschichtungsprodukten, Kleb- und Dichtstoffen, Wasch- und Reinigungsmitteln","涂料产品、粘合剂和密封剂以及洗涤和清洁产品。"]
[null,{"$f":"IF($B$1=\"English\",C3818,IF($B$1=\"Deutsch\",D3818,IF($B$1=\"中文\",E3818,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Inks and toners, coating products."},"Inks and toners, coating products.","Tinten und Toner sowie in Beschichtungsprodukten","油墨和碳粉、涂料产品。"]
[null,{"$f":"IF($B$1=\"English\",C3819,IF($B$1=\"Deutsch\",D3819,IF($B$1=\"中文\",E3819,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Air care products, coating products, adhesives and sealants, lubricants and greases, polishes and waxes and washing and cleaning products."},"Air care products, coating products, adhesives and sealants, lubricants and greases, polishes and waxes and washing and cleaning products.","Luftpflegeprodukten, Beschichtungsprodukten, Kleb- und Dichtstoffen sowie in Schmiermitteln und Fette, Polituren und Wachse, Wasch- und Reinigungsmittel","空气护理产品、涂料产品、粘合剂和密封剂、润滑剂和油脂、抛光剂和蜡以及洗涤和清洁产品。"]
[null,{"$f":"IF($B$1=\"English\",C3820,IF($B$1=\"Deutsch\",D3820,IF($B$1=\"中文\",E3820,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Manufacture of another substance; formulation of mixtures and in fuel products."},"Manufacture of another substance; formulation of mixtures and in fuel products.","Herstellung eines anderen Stoffes, bei der Formulierung von Gemischen und in Kraftstoffprodukten","另一种物质的制造； 混合物和燃料产品的配方。"]
[null,{"$f":"IF($B$1=\"English\",C3821,IF($B$1=\"Deutsch\",D3821,IF($B$1=\"中文\",E3821,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Limits [mass %]\nor intentionally added\n\nExplanation: Limit related to mass in complete delivered component (Bosch SNR)"},"Limits [mass %]\nor intentionally added\n\nExplanation: Limit related to mass in complete delivered component (Bosch SNR)","Grenzwerte [Massen %]\noder absichtlich hinzugefügt\n\nErklärung: Grenzwert bezogen auf die Masse des gesamten gelieferten Bauteils (Bosch SNR)","限值[质量%]\n或有意添加\n\n说明：以完整交付组件（博世 SNR）的质量为基数的限值"]
[null,{"$f":"IF($B$1=\"English\",C3822,IF($B$1=\"Deutsch\",D3822,IF($B$1=\"中文\",E3822,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":"Concentration of ingredient [mass%]\n\nExplanation: Enter the total amount of the Concentration of ingredient in [mass%]"},"Concentration of ingredient [mass%]\n\nExplanation: Enter the total amount of the Concentration of ingredient in [mass%]","Konzentration des Inhaltsstoffs [Massen %]\n\nErklärung: Angabe der Gesamtmenge der Konzentration des Inhaltsstoffs in [Masse%] an.","成分浓度[质量%]\n\n说明： 输入该成分浓度的总量[质量%]"]
[null,{"$f":"IF($B$1=\"English\",C3823,IF($B$1=\"Deutsch\",D3823,IF($B$1=\"中文\",E3823,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3824,IF($B$1=\"Deutsch\",D3824,IF($B$1=\"中文\",E3824,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3825,IF($B$1=\"Deutsch\",D3825,IF($B$1=\"中文\",E3825,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3826,IF($B$1=\"Deutsch\",D3826,IF($B$1=\"中文\",E3826,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3827,IF($B$1=\"Deutsch\",D3827,IF($B$1=\"中文\",E3827,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3828,IF($B$1=\"Deutsch\",D3828,IF($B$1=\"中文\",E3828,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3829,IF($B$1=\"Deutsch\",D3829,IF($B$1=\"中文\",E3829,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3830,IF($B$1=\"Deutsch\",D3830,IF($B$1=\"中文\",E3830,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3831,IF($B$1=\"Deutsch\",D3831,IF($B$1=\"中文\",E3831,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3832,IF($B$1=\"Deutsch\",D3832,IF($B$1=\"中文\",E3832,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3833,IF($B$1=\"Deutsch\",D3833,IF($B$1=\"中文\",E3833,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3834,IF($B$1=\"Deutsch\",D3834,IF($B$1=\"中文\",E3834,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3835,IF($B$1=\"Deutsch\",D3835,IF($B$1=\"中文\",E3835,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3836,IF($B$1=\"Deutsch\",D3836,IF($B$1=\"中文\",E3836,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3837,IF($B$1=\"Deutsch\",D3837,IF($B$1=\"中文\",E3837,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3838,IF($B$1=\"Deutsch\",D3838,IF($B$1=\"中文\",E3838,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3839,IF($B$1=\"Deutsch\",D3839,IF($B$1=\"中文\",E3839,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3840,IF($B$1=\"Deutsch\",D3840,IF($B$1=\"中文\",E3840,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3841,IF($B$1=\"Deutsch\",D3841,IF($B$1=\"中文\",E3841,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3842,IF($B$1=\"Deutsch\",D3842,IF($B$1=\"中文\",E3842,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3843,IF($B$1=\"Deutsch\",D3843,IF($B$1=\"中文\",E3843,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3844,IF($B$1=\"Deutsch\",D3844,IF($B$1=\"中文\",E3844,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3845,IF($B$1=\"Deutsch\",D3845,IF($B$1=\"中文\",E3845,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3846,IF($B$1=\"Deutsch\",D3846,IF($B$1=\"中文\",E3846,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3847,IF($B$1=\"Deutsch\",D3847,IF($B$1=\"中文\",E3847,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3848,IF($B$1=\"Deutsch\",D3848,IF($B$1=\"中文\",E3848,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3849,IF($B$1=\"Deutsch\",D3849,IF($B$1=\"中文\",E3849,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3850,IF($B$1=\"Deutsch\",D3850,IF($B$1=\"中文\",E3850,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3851,IF($B$1=\"Deutsch\",D3851,IF($B$1=\"中文\",E3851,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3852,IF($B$1=\"Deutsch\",D3852,IF($B$1=\"中文\",E3852,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3853,IF($B$1=\"Deutsch\",D3853,IF($B$1=\"中文\",E3853,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3854,IF($B$1=\"Deutsch\",D3854,IF($B$1=\"中文\",E3854,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3855,IF($B$1=\"Deutsch\",D3855,IF($B$1=\"中文\",E3855,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3856,IF($B$1=\"Deutsch\",D3856,IF($B$1=\"中文\",E3856,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3857,IF($B$1=\"Deutsch\",D3857,IF($B$1=\"中文\",E3857,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3858,IF($B$1=\"Deutsch\",D3858,IF($B$1=\"中文\",E3858,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3859,IF($B$1=\"Deutsch\",D3859,IF($B$1=\"中文\",E3859,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3860,IF($B$1=\"Deutsch\",D3860,IF($B$1=\"中文\",E3860,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3861,IF($B$1=\"Deutsch\",D3861,IF($B$1=\"中文\",E3861,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3862,IF($B$1=\"Deutsch\",D3862,IF($B$1=\"中文\",E3862,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3863,IF($B$1=\"Deutsch\",D3863,IF($B$1=\"中文\",E3863,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3864,IF($B$1=\"Deutsch\",D3864,IF($B$1=\"中文\",E3864,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3865,IF($B$1=\"Deutsch\",D3865,IF($B$1=\"中文\",E3865,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3866,IF($B$1=\"Deutsch\",D3866,IF($B$1=\"中文\",E3866,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3867,IF($B$1=\"Deutsch\",D3867,IF($B$1=\"中文\",E3867,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3868,IF($B$1=\"Deutsch\",D3868,IF($B$1=\"中文\",E3868,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3869,IF($B$1=\"Deutsch\",D3869,IF($B$1=\"中文\",E3869,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3870,IF($B$1=\"Deutsch\",D3870,IF($B$1=\"中文\",E3870,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3871,IF($B$1=\"Deutsch\",D3871,IF($B$1=\"中文\",E3871,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3872,IF($B$1=\"Deutsch\",D3872,IF($B$1=\"中文\",E3872,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3873,IF($B$1=\"Deutsch\",D3873,IF($B$1=\"中文\",E3873,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3874,IF($B$1=\"Deutsch\",D3874,IF($B$1=\"中文\",E3874,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3875,IF($B$1=\"Deutsch\",D3875,IF($B$1=\"中文\",E3875,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3876,IF($B$1=\"Deutsch\",D3876,IF($B$1=\"中文\",E3876,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3877,IF($B$1=\"Deutsch\",D3877,IF($B$1=\"中文\",E3877,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3878,IF($B$1=\"Deutsch\",D3878,IF($B$1=\"中文\",E3878,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3879,IF($B$1=\"Deutsch\",D3879,IF($B$1=\"中文\",E3879,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3880,IF($B$1=\"Deutsch\",D3880,IF($B$1=\"中文\",E3880,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3881,IF($B$1=\"Deutsch\",D3881,IF($B$1=\"中文\",E3881,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3882,IF($B$1=\"Deutsch\",D3882,IF($B$1=\"中文\",E3882,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3883,IF($B$1=\"Deutsch\",D3883,IF($B$1=\"中文\",E3883,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3884,IF($B$1=\"Deutsch\",D3884,IF($B$1=\"中文\",E3884,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3885,IF($B$1=\"Deutsch\",D3885,IF($B$1=\"中文\",E3885,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3886,IF($B$1=\"Deutsch\",D3886,IF($B$1=\"中文\",E3886,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3887,IF($B$1=\"Deutsch\",D3887,IF($B$1=\"中文\",E3887,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3888,IF($B$1=\"Deutsch\",D3888,IF($B$1=\"中文\",E3888,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3889,IF($B$1=\"Deutsch\",D3889,IF($B$1=\"中文\",E3889,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3890,IF($B$1=\"Deutsch\",D3890,IF($B$1=\"中文\",E3890,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3891,IF($B$1=\"Deutsch\",D3891,IF($B$1=\"中文\",E3891,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3892,IF($B$1=\"Deutsch\",D3892,IF($B$1=\"中文\",E3892,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3893,IF($B$1=\"Deutsch\",D3893,IF($B$1=\"中文\",E3893,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3894,IF($B$1=\"Deutsch\",D3894,IF($B$1=\"中文\",E3894,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3895,IF($B$1=\"Deutsch\",D3895,IF($B$1=\"中文\",E3895,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3896,IF($B$1=\"Deutsch\",D3896,IF($B$1=\"中文\",E3896,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3897,IF($B$1=\"Deutsch\",D3897,IF($B$1=\"中文\",E3897,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3898,IF($B$1=\"Deutsch\",D3898,IF($B$1=\"中文\",E3898,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3899,IF($B$1=\"Deutsch\",D3899,IF($B$1=\"中文\",E3899,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3900,IF($B$1=\"Deutsch\",D3900,IF($B$1=\"中文\",E3900,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3901,IF($B$1=\"Deutsch\",D3901,IF($B$1=\"中文\",E3901,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3902,IF($B$1=\"Deutsch\",D3902,IF($B$1=\"中文\",E3902,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3903,IF($B$1=\"Deutsch\",D3903,IF($B$1=\"中文\",E3903,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3904,IF($B$1=\"Deutsch\",D3904,IF($B$1=\"中文\",E3904,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3905,IF($B$1=\"Deutsch\",D3905,IF($B$1=\"中文\",E3905,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3906,IF($B$1=\"Deutsch\",D3906,IF($B$1=\"中文\",E3906,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3907,IF($B$1=\"Deutsch\",D3907,IF($B$1=\"中文\",E3907,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3908,IF($B$1=\"Deutsch\",D3908,IF($B$1=\"中文\",E3908,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3909,IF($B$1=\"Deutsch\",D3909,IF($B$1=\"中文\",E3909,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3910,IF($B$1=\"Deutsch\",D3910,IF($B$1=\"中文\",E3910,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3911,IF($B$1=\"Deutsch\",D3911,IF($B$1=\"中文\",E3911,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3912,IF($B$1=\"Deutsch\",D3912,IF($B$1=\"中文\",E3912,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3913,IF($B$1=\"Deutsch\",D3913,IF($B$1=\"中文\",E3913,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3914,IF($B$1=\"Deutsch\",D3914,IF($B$1=\"中文\",E3914,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3915,IF($B$1=\"Deutsch\",D3915,IF($B$1=\"中文\",E3915,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3916,IF($B$1=\"Deutsch\",D3916,IF($B$1=\"中文\",E3916,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3917,IF($B$1=\"Deutsch\",D3917,IF($B$1=\"中文\",E3917,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3918,IF($B$1=\"Deutsch\",D3918,IF($B$1=\"中文\",E3918,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3919,IF($B$1=\"Deutsch\",D3919,IF($B$1=\"中文\",E3919,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3920,IF($B$1=\"Deutsch\",D3920,IF($B$1=\"中文\",E3920,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3921,IF($B$1=\"Deutsch\",D3921,IF($B$1=\"中文\",E3921,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3922,IF($B$1=\"Deutsch\",D3922,IF($B$1=\"中文\",E3922,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3923,IF($B$1=\"Deutsch\",D3923,IF($B$1=\"中文\",E3923,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3924,IF($B$1=\"Deutsch\",D3924,IF($B$1=\"中文\",E3924,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3925,IF($B$1=\"Deutsch\",D3925,IF($B$1=\"中文\",E3925,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3926,IF($B$1=\"Deutsch\",D3926,IF($B$1=\"中文\",E3926,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3927,IF($B$1=\"Deutsch\",D3927,IF($B$1=\"中文\",E3927,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3928,IF($B$1=\"Deutsch\",D3928,IF($B$1=\"中文\",E3928,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3929,IF($B$1=\"Deutsch\",D3929,IF($B$1=\"中文\",E3929,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3930,IF($B$1=\"Deutsch\",D3930,IF($B$1=\"中文\",E3930,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3931,IF($B$1=\"Deutsch\",D3931,IF($B$1=\"中文\",E3931,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3932,IF($B$1=\"Deutsch\",D3932,IF($B$1=\"中文\",E3932,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3933,IF($B$1=\"Deutsch\",D3933,IF($B$1=\"中文\",E3933,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3934,IF($B$1=\"Deutsch\",D3934,IF($B$1=\"中文\",E3934,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3935,IF($B$1=\"Deutsch\",D3935,IF($B$1=\"中文\",E3935,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3936,IF($B$1=\"Deutsch\",D3936,IF($B$1=\"中文\",E3936,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3937,IF($B$1=\"Deutsch\",D3937,IF($B$1=\"中文\",E3937,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3938,IF($B$1=\"Deutsch\",D3938,IF($B$1=\"中文\",E3938,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3939,IF($B$1=\"Deutsch\",D3939,IF($B$1=\"中文\",E3939,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3940,IF($B$1=\"Deutsch\",D3940,IF($B$1=\"中文\",E3940,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3941,IF($B$1=\"Deutsch\",D3941,IF($B$1=\"中文\",E3941,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3942,IF($B$1=\"Deutsch\",D3942,IF($B$1=\"中文\",E3942,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3943,IF($B$1=\"Deutsch\",D3943,IF($B$1=\"中文\",E3943,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3944,IF($B$1=\"Deutsch\",D3944,IF($B$1=\"中文\",E3944,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3945,IF($B$1=\"Deutsch\",D3945,IF($B$1=\"中文\",E3945,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3946,IF($B$1=\"Deutsch\",D3946,IF($B$1=\"中文\",E3946,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3947,IF($B$1=\"Deutsch\",D3947,IF($B$1=\"中文\",E3947,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3948,IF($B$1=\"Deutsch\",D3948,IF($B$1=\"中文\",E3948,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3949,IF($B$1=\"Deutsch\",D3949,IF($B$1=\"中文\",E3949,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3950,IF($B$1=\"Deutsch\",D3950,IF($B$1=\"中文\",E3950,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3951,IF($B$1=\"Deutsch\",D3951,IF($B$1=\"中文\",E3951,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3952,IF($B$1=\"Deutsch\",D3952,IF($B$1=\"中文\",E3952,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3953,IF($B$1=\"Deutsch\",D3953,IF($B$1=\"中文\",E3953,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3954,IF($B$1=\"Deutsch\",D3954,IF($B$1=\"中文\",E3954,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3955,IF($B$1=\"Deutsch\",D3955,IF($B$1=\"中文\",E3955,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3956,IF($B$1=\"Deutsch\",D3956,IF($B$1=\"中文\",E3956,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3957,IF($B$1=\"Deutsch\",D3957,IF($B$1=\"中文\",E3957,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3958,IF($B$1=\"Deutsch\",D3958,IF($B$1=\"中文\",E3958,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3959,IF($B$1=\"Deutsch\",D3959,IF($B$1=\"中文\",E3959,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3960,IF($B$1=\"Deutsch\",D3960,IF($B$1=\"中文\",E3960,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3961,IF($B$1=\"Deutsch\",D3961,IF($B$1=\"中文\",E3961,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3962,IF($B$1=\"Deutsch\",D3962,IF($B$1=\"中文\",E3962,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3963,IF($B$1=\"Deutsch\",D3963,IF($B$1=\"中文\",E3963,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3964,IF($B$1=\"Deutsch\",D3964,IF($B$1=\"中文\",E3964,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3965,IF($B$1=\"Deutsch\",D3965,IF($B$1=\"中文\",E3965,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3966,IF($B$1=\"Deutsch\",D3966,IF($B$1=\"中文\",E3966,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3967,IF($B$1=\"Deutsch\",D3967,IF($B$1=\"中文\",E3967,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3968,IF($B$1=\"Deutsch\",D3968,IF($B$1=\"中文\",E3968,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3969,IF($B$1=\"Deutsch\",D3969,IF($B$1=\"中文\",E3969,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3970,IF($B$1=\"Deutsch\",D3970,IF($B$1=\"中文\",E3970,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3971,IF($B$1=\"Deutsch\",D3971,IF($B$1=\"中文\",E3971,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3972,IF($B$1=\"Deutsch\",D3972,IF($B$1=\"中文\",E3972,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3973,IF($B$1=\"Deutsch\",D3973,IF($B$1=\"中文\",E3973,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3974,IF($B$1=\"Deutsch\",D3974,IF($B$1=\"中文\",E3974,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3975,IF($B$1=\"Deutsch\",D3975,IF($B$1=\"中文\",E3975,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3976,IF($B$1=\"Deutsch\",D3976,IF($B$1=\"中文\",E3976,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3977,IF($B$1=\"Deutsch\",D3977,IF($B$1=\"中文\",E3977,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3978,IF($B$1=\"Deutsch\",D3978,IF($B$1=\"中文\",E3978,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3979,IF($B$1=\"Deutsch\",D3979,IF($B$1=\"中文\",E3979,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]
[null,{"$f":"IF($B$1=\"English\",C3980,IF($B$1=\"Deutsch\",D3980,IF($B$1=\"中文\",E3980,IF($B$1=\"Japanese\",#REF!,\"F\"))))","v":0}]

{"sheet":"16_California_Proposition_65","index":22,"n_rows":11,"n_cols":10,"rows_kept":11,"cut":false,"hidden":true,"merged":[[11,0,11,4],[0,0,0,4],[2,0,2,3],[3,0,3,3],[4,0,4,3],[5,0,5,3],[6,0,6,3]]}
[{"$f":"Translator!B2099","v":"California Proposition 65 (Reiter 16) "},null,null,null,null,null,null,null,null,{"$f":"Translator!B26","v":"Yes"}]
[null,null,null,null,null,null,null,null,null,{"$f":"Translator!B27","v":"No"}]
[{"$f":"Translator!B2100","v":"Safe Drinking Water and Toxic Enforcement Act of 1986, as amended (also known as California Proposition 65)"}]
[{"$f":"Translator!B2101","v":"The supplier must inform Bosch if any substance on the California Proposition 65 List is contained in a product or"}]
[{"$f":"Translator!B2102","v":"spare part or mixture in any concentration. The supplier is obliged to track the Proposition 65 List regularly "}]
[{"$f":"Translator!B2103","v":"(on OEHHA website) and to inform Bosch purchasing contact immediately if he gets information "}]
[{"$f":"Translator!B2104","v":"that any substance on the Proposition 65 List may be included in supplied material."}]
[{"$f":"Translator!B2105","v":"Proposition 65 List:"},"https://oehha.ca.gov/proposition-65/proposition-65-list"]
[{"$f":"Translator!B2137","v":"Anything to declare? Please select"},"Ja"]
[]
[{"$f":"Translator!B2106","v":"Name of contained Substances"},{"$f":"Translator!B2107","v":"CAS-Number"},{"$f":"Translator!B2108","v":"Concentration of ingredient [mass%]"},{"$f":"Translator!B2109","v":"Designation of the material that contains the declared substance"},{"$f":"Translator!B3031","v":"MADSL exceeded"}]

{"sheet":"17_CN-ELV","index":23,"n_rows":44,"n_cols":12,"rows_kept":44,"cut":false,"hidden":true,"merged":[[0,0,0,11],[2,0,2,11],[9,0,9,11],[10,6,10,7],[43,6,43,7]]}
[{"$f":"Translator!B2376","v":"CN-ELV (tab 17) GB/T30512-2014"}]
[{"$f":"Translator!B2377","v":"Regulated substances"},{"$f":"Translator!B2378","v":"CAS number"},null,{"$f":"Translator!B2379","v":"Limit value [mass% in homogeneous material]"},{"$f":"Translator!B3789","v":"By Substance groups: Name of the contained substances"},{"$f":"Translator!B3790","v":"By Substance groups: CAS of the contained substances"},{"$f":"Translator!B2380","v":"Concentration of substance [mass% in homogeneous material]"},{"$f":"Translator!B2381","v":"Exception claimed? If so, which one?"},{"$f":"Translator!B2382","v":"Designation of the material that contains the regulated substance"},{"$f":"Translator!B2383","v":"Entry\n- included ( E )\n- changed ( C )"},{"$f":"Translator!B2384","v":"test report enclosed (optional)"},{"$f":"Translator!B2385","v":"method of measurement"}]
[{"$f":"Translator!B2386","v":"Prohibited substances (P)"}]
[{"$f":"Translator!B2387","v":"Lead"},{"$f":"Translator!B2393","v":"7439-92-1 and its compounds"},"P",0.1,null,null,null,null,null,"E2014"]
[{"$f":"Translator!B2388","v":"Cadmium"},{"$f":"Translator!B2394","v":"7440-43-9 and its compounds"},"P",0.01,null,null,null,null,null,"E2014"]
[{"$f":"Translator!B2389","v":"Mercury"},{"$f":"Translator!B2395","v":"7439-97-6 and its compounds"},"P",0.1,null,null,null,null,null,"E2014"]
[{"$f":"Translator!B2390","v":"Chromium VI"},{"$f":"Translator!B2396","v":"1333-82-0 and its compounds"},"P",0.1,null,null,null,null,null,"E2014"]
[{"$f":"Translator!B2391","v":"Polybrominated biphenyles (PBB)"},{"$f":"Translator!B2397","v":"Material group"},"P",0.1,null,null,null,null,null,"E2014"]
[{"$f":"Translator!B2392","v":"Polybrominated diphenyl ether (PBDE)"},{"$f":"Translator!B2398","v":"Material group"},"P",0.1,null,null,null,null,null,"E2014"]
[{"$f":"Translator!B2399","v":"List of Exemptions (2014) "}]
[null,null,null,null,null,null,{"$f":"Translator!B2400","v":"GB/T30512-2014 \nAnnex A\n Exemption of prohibited substances"}]
[]
[null,null,null,null,null,null,{"$f":"Translator!B2401","v":"Materials and components "},{"$f":"Translator!B2402","v":" Scope and expiry date of the exemption "}]
[null,null,null,null,null,null,{"$f":"Translator!B2403","v":"Lead as an alloying element"}]
[null,null,null,null,null,null,{"$f":"Translator!B2404","v":"1. Steel and galvanized steel for machining (Lead ≤0.35%)"}]
[null,null,null,null,null,null,{"$f":"Translator!B2405","v":"2. Aluminum material (Lead≤0.4%)"}]
[null,null,null,null,null,null,{"$f":"Translator!B2406","v":"3. Copper alloy (Lead ≤4%)"}]
[null,null,null,null,null,null,{"$f":"Translator!B2407","v":"4(a) Bearing bush and shaft sleeve "},{"$f":"Translator!B2433","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2408","v":"4(b) Bearing bush and shaft sleeve of engine, transmission and air conditioning compressor "},{"$f":"Translator!B2434","v":"2016-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2409","v":"Lead and lead compounds for parts"}]
[null,null,null,null,null,null,{"$f":"Translator!B2410","v":"5. Storage battery"}]
[null,null,null,null,null,null,{"$f":"Translator!B2411","v":"6. Damper"}]
[null,null,null,null,null,null,{"$f":"Translator!B2412","v":"7. Flexible brake hoses, fuel hoses, flexible ventilation ducting, elastomer / metal parts for chassis and elastomer sulfurizing reagent and stabilizer for engine mounting (Lead≤0.5%)"},{"$f":"Translator!B2435","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2413","v":"8. Elastomeric adhesive on the power assembly (Lead ≤0.5%) "},{"$f":"Translator!B2436","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2414","v":"9. Welding flux for circuit boards and other electric parts"}]
[null,null,null,null,null,null,{"$f":"Translator!B2415","v":"10. Valve seat "},{"$f":"Translator!B2437","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2416","v":"11. Electrical components with leaded glass or ceramic matrix composites except for bulb glass and enamel layer of sparking plug"}]
[null,null,null,null,null,null,{"$f":"Translator!B2417","v":"12. Pyrotechnic primer "},{"$f":"Translator!B2438","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2418","v":"13. Lead-coated steel plate for automotive fuel tank "},{"$f":"Translator!B2439","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2419","v":"14. Wheel counterbalance "},{"$f":"Translator!B2440","v":"2014-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2420","v":"15. Carbon brush for electric machine "},{"$f":"Translator!B2441","v":"2015-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2421","v":"16. Copper in the friction materials of brake lining (Lead ≤0.5%) "},{"$f":"Translator!B2442","v":"2014-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2422","v":"Hexavalent chromium"}]
[null,null,null,null,null,null,{"$f":"Translator!B2423","v":"17. Anticorrosive paint "},{"$f":"Translator!B2443","v":"2014-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2424","v":"18. Chassis is assembled with corrosion prevention coating of bolts and nuts and other parts "},{"$f":"Translator!B2444","v":"2014-06-30"}]
[null,null,null,null,null,null,{"$f":"Translator!B2425","v":"19. Heat absorption air conditioning in motor caravan"}]
[null,null,null,null,null,null,{"$f":"Translator!B2426","v":"Mercury"}]
[null,null,null,null,null,null,{"$f":"Translator!B2427","v":"20. Electric-discharge lamp for headlamp"}]
[null,null,null,null,null,null,{"$f":"Translator!B2428","v":"21. Fluorescent tube of instrument board display"}]
[null,null,null,null,null,null,{"$f":"Translator!B2429","v":"Cadmium"}]
[null,null,null,null,null,null,{"$f":"Translator!B2430","v":"22. Battery for electric vehicle"},{"$f":"Translator!B2445","v":"From the implementation date of this Standard, nickel-cadmium battery is only allowed to be the spare parts of those vehicles which have entered into the market before this date."}]
[null,null,null,null,null,null,{"$f":"Translator!B2431","v":"Bromide flame-retardant"}]
[null,null,null,null,null,null,{"$f":"Translator!B2432","v":"23. Decabromodiphenyl ether"}]
[null,null,null,null,null,null,{"$f":"Translator!B2446","v":"Note 1: The content limits in parentheses are all in mass percentage. \nNote 2: The exemption deadline in the table is that – for the new certificated models, the exemption deadline shall be postponed for 2 years, from the exemption deadline of producing automobiles."}]

{"sheet":"18_TSCA (Sec. 5(a)(2),Sec 6(h))","index":24,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,6]]}
[{"$f":"Translator!B2873","v":"USA TSCA (sec 5(a)(2) sec. 6(h)) (Tab 18)"}]
[{"$f":"Translator!B2450","v":"Regulated Substances"},{"$f":"Translator!B2451","v":"CAS number"},null,{"$f":"Translator!B2452","v":"Limits"},{"$f":"Translator!B2453","v":"Concentration"},{"$f":"Translator!B2788","v":"Examples occurence"},{"$f":"Translator!B2455","v":"Entry\n- included (E)\n- changed (C) \n"}]
[{"$f":"Translator!B2747","v":"TSCA (Sec. 6(h))"}]
[{"$f":"Translator!B2456","v":"2,4,6-Tris(tert-butyl)phenol (2,4,6-TTBP)"},"732-26-3","P",{"$f":"Translator!B2461","v":"≤ 0.3% by weight"},null,{"$f":"Translator!B2466","v":"an antioxidant in fuel additives and fuel injector cleaners as well as an additive in oil and lubricants"},"E2021"]
[{"$f":"Translator!B2457","v":"Decabromodiphenyl ether (DecaBDE)"},"1163-19-5","P",{"$f":"Translator!B2462","v":"0 % by weight"},null,{"$f":"Translator!B2467","v":"a flame retardant with applications in wire and cable rubber casings, textiles, electronic equipment casings, building and construction materials, and imported articles such as aerospace and automotive parts"},"E2021"]
[{"$f":"Translator!B2458","v":"Phenol, isopropylated phosphate (3:1) (PIP 3:1)"}," 68937-41-7","P",{"$f":"Translator!B2463","v":"0 % by weight"},null,{"$f":"Translator!B2468","v":"a flame retardant in plastics and as a functional fluid in aircraft and industrial machinery"},"E2021"]
[{"$f":"Translator!B2459","v":"Pentachlorothiophenol (PCTP)"},"133-49-3",null,{"$f":"Translator!B2464","v":"≤ 1% by weight"},null,{"$f":"Translator!B2469","v":" a substance with applications in the rubber industry"},"E2021"]
[{"$f":"Translator!B2460","v":"Hexachlorobutadiene (HCBD)"},"87-68-3","P",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,{"$f":"Translator!B2470","v":"a solvent in rubber manufacturing and in hydraulic, heat transfer or transformer fluid"},"E2021"]
[{"$f":"Translator!B2748","v":"TSCA (Sec. 5 (a)(2)"}]
[{"$f":"Translator!B2749","v":"Hexachlorobutadiene (HCBD)"},"87-68-3","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2750","v":"Octanoyl fluoride, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-."},"335-66-0","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2751","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (PFOA)."},"335-67-1","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2752","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, silver (+) salt (1:1)."},"335-93-3","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2753","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, sodium salt (1:1)."},"335-95-5","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2754","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, potassium salt (1:1)."},"2395-00-8","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2755","v":"Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, ammonium salt (1:1) (APFO)."},"3825-26-1","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2756","v":"Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-8-iodo-."},"507-63-1","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2757","v":"1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-."},"678-39-7","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2758","v":"1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-.heneicosafluoro-"},"865-86-1","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2759","v":"Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-."},"2043-53-0","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2760","v":"Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-12-iodo-."},"2043-54-1","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2761","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester."},"17741-60-5","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2762","v":"2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester"},"27905-45-9","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2763","v":"Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-14-iodo-."},"30046-31-2","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2764","v":"1-Tetradecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-."},"39239-77-5","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2765","v":"1-Hexadecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluoro-."},"60699-51-6","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2766","v":"Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodo-."},"65510-55-6","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2767","v":"Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (2:1)"},"65530-63-4","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2768","v":"Ethanol, 2,2'-iminobis-, compd. with .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoropoly(difluoromethylene)] (1:1)"},"65530-64-5","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2769","v":"Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-, lithium salt (1:1) "},"65530-69-0","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2770","v":"Poly(difluoromethylene), .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-, ammonium salt (1:1)"},"65530-70-3","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2771","v":"Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:1) "},"65530-71-4","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2772","v":"Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt (1:2)"},"65530-72-5","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2773","v":"Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (1:1)"},"65530-74-7","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2774","v":"Poly(oxy-1,2-ethanediyl), .alpha.-hydro-.omega.-hydroxy-, ether with .alpha.-fluoro-.omega.-(2-hydroxyethyl)poly(difluoromethylene) (1:1)"},"65545-80-4","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2775","v":"1-Propanesulfonic acid, 2-methyl-, 2-[[1-oxo-3-[(.gamma.-.omega.-perfluoro- C4-16-alkyl)thio]propyl]amino] derivs., sodium salts"},"68187-47-3","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2776","v":"Alcohols, C8-14, .gamma.-.omega.-perfluoro."},"68391-08-2","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2777","v":"Thiols, C8-20, .gamma.-.omega.-perfluoro, telomers with acrylamide."},"70969-47-0","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2778","v":"Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-"},"78560-44-8","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2779","v":"Silicic acid (H4SiO4), sodium salt (1:2), reaction products with chlorotrimethylsilane and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol."},"125476-71-3","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2780","v":"Thiols, C4-20, .gamma.-.omega.-perfluoro, telomers with acrylamide and acrylic acid, sodium salts."},"1078712-88-5","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]
[{"$f":"Translator!B2781","v":"1-Propanaminium, 3-amino-N-(carboxymethyl)-N,N-dimethyl-, N-[2-[(.gamma.-.omega.-perfluoro-C4-20-a lkyl)thio]acetyl] derivs., inner salts."},"1078715-61-3","D",{"$f":"Translator!$B$2465","v":"0 % by weight"},null,null,"E2021"]

{"sheet":"19_PFAS World","index":25,"n_rows":14293,"n_cols":6,"rows_kept":14293,"cut":false,"hidden":true,"merged":[[0,0,0,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,5],[6,0,6,5],[7,0,7,5],[8,0,8,5],[9,0,9,5],[10,0,10,5]]}
[{"$f":"Translator!B2874","v":"PFAS World (based on US Maine PFAS) (Tab 19)"}]
[]
[{"$f":"Translator!B2875","v":"In July 2021, Public Law c. 477,"}]
["An Act To Stop Perfluoroalkyl and Polyfluoroalkyl Substances Pollution"]
[{"$f":"Translator!B2876","v":"(LD 1503, 130th Legislature) was enacted by the Maine Legislature. This new law requires manufacturers"}]
[{"$f":"Translator!B2877","v":"of products with intentionally added PFAS to report the intentionally added presence of PFAS in those"}]
[{"$f":"Translator!B2878","v":"products to the Department beginning January 1, 2023."}]
[{"$f":"Translator!B2879","v":"Bosch suppliers must inform Bosch if any substance (intentionally or not intentionally) of the Main Law"}]
[{"$f":"Translator!B2880","v":"related list from EPA in a product or spare part or mixture in any concentration. The supplier is obliged to"}]
[{"$f":"Translator!B2881","v":"track the EPA list (link below) and to inform Bosch purchasing contact immediately if he gets information"}]
[{"$f":"Translator!B2882","v":"that any substance on the EPA list may be included in the supplied material."}]
[{"$f":"Translator!B2883","v":"EPA PFAS Master List of PFAS Substances V2: "}]
["https://comptox.epa.gov/dashboard/chemical-lists/PFASMASTERV2"]
[]
[{"$f":"Translator!B3727","v":"Regulated Substances"},{"$f":"Translator!B3728","v":"CAS-Number"},null,{"$f":"Translator!B3729","v":"Limit value [mass-%]"},{"$f":"Translator!B3730","v":"Concentration of ingredient [mass%]"},{"$f":"Translator!B3731","v":"Designation of the material that contains the declared substance"}]
["1,2-Propanediol, 3-(diethylamino)-, polymers with 5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexane, propylene glycol and reduced Me esters of reduced polymd. oxidized tetrafluoroethylene, 2-ethyl-1-hexanol-blocked, acetates (salts)","328389-90-8","D",0]
["Vinyl fluoride-Vinylidene fluoride-Tetrafluoroethylene copolymer","32802-40-7","D",0]
["chloromethyl 2,2-dichloro-1,1,2-trifluoroethyl ether","32776-56-0","D",0]
["Propanoic acid, 3-hydroxy-2-(hydroxymethyl)-2-methyl-, polymers with 5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexane and reduced Me esters of reduced polymd. oxidized tetrafluoroethylene, compds. with triethylamine","328389-91-9","D",0]
["Propanoic acid, 3-hydroxy-2-(hydroxymethyl)-2-methyl-, polymers with 1,4-cyclohexanedimethanol, 5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexan e and reduced Me esters of reduced polymd. oxidized tetrafluoroethylene, compds. with ¿","328390-05-2","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], alpha-hydro-omega-hydroxy-, polymer with 1,3-diisocyanatomethylbenzene, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-N-propyl-1-octanesulfonamide- and polypropylene glycol mono-Bu¿","330678-54-1","D",0]
["Cyanic acid, [2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]di-4,1-phenylene ester, homopolymer","32755-72-9","D",0]
["1-Iodopentadecafluoroheptane","335-58-0","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N-(2-hydroxyethyl)-N-methylbutane-1-sulphonamide","34454-97-2","D",0]
["1-Dodecanethiol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","34451-28-0","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,4-nonafluoro-N-(2-hydroxyethyl)butane-1-sulphonamide","34449-89-3","D",0]
["4-(2,2,3,3-Tetrafluoropropyl)morpholine","343331-58-8","D",0]
["2-Propenoic acid, dodecyl ester, polymers with(chloromethyl)ethenylbenzene, N-(hydroxymethyl)-2-propenamide and gamma-omega-perfluoro-C10-14-alkyl acrylates","330809-58-0","D",0]
["Phosphonium, tributyl(2-methoxypropyl)-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-N-methyl-1-butanesulfonamide (1:1)","332350-90-0","D",0]
["Phosphonium, triphenyl(phenylmethyl)-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-N-methyl-1-butanesulfonamide (1:1)","332350-93-3","D",0]
["N-Methyl-1-butanesulfonamide, 1,1,2,2,3,3,4,4,4-nonafluoro-, salts with benzene-chlorine-sulfurchloride reaction products","332912-47-7","D",0]
["2H-Perfluoro-5-methyl-3,6-dioxanonane","3330-14-1","D",0]
["Perfluoro-3-(1H-perfluoroethoxy)propane","3330-15-2","D",0]
["2H-Perfluoro(5,8-dimethyl-3,6,9-trioxadodecane)","3330-16-3","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymers with 2,3-dihydroxypropyl methacrylate, gamma-omega-perfluoro-C8-16-alkyl acrylate,polyethylene glycol methacrylate Me ether and polypropylene glycolmonomethacrylate","333784-44-4","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymers with maleicanhydride, 2-[[(2-mercaptoethoxy)carbonyl]amino]ethyl methacrylate, gamma-omega-perfluoro-C8-16-alkyl acrylate and stearyl methacrylate","333784-46-6","D",0]
["Perfluoro-2,3-dimethylpentane","335-14-8","D",0]
["potassium 1,2,2,3,3,4,5,5,6,6-decafluoro-4-(pentafluoroethyl)cyclohexanesulphonate","335-24-0","D",0]
["Perfluoro-1,3-dimethylcyclohexane","335-27-3","D",0]
["2-PROPANONE, HEXAFLUORO-, TRIHYDRATE","34202-69-2","D",0]
["1H,1H,11H-Eicosafluoro-1-undecanol","307-70-0","D",0]
["Potassium 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecanoate","307-71-1","D",0]
["Perfluorodecanedioic acid","307-78-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl acrylate","307-87-9","D",0]
["(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)di(4,1-phenylene) dicyanate","32728-27-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-[methyl[(nonafluorobutyl)sulfonyl]amino]ethyl ester, polymer with alpha-(1-oxo-2-propenyl)-omega-methoxypoly(oxy-1,2-ethanediyl) and 2-propenoic acid, graft (9CI)","335593-06-1","D",0]
["Octanoyl chloride, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","335-64-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluorooctane","335-65-9","D",0]
["1,8-Diiodoperfluorooctane","335-70-6","D",0]
["Bis(perfluorobutyryl)peroxide","336-64-1","D",0]
["Perfluorobutanoic anhydride","336-59-4","D",0]
["1,1,2,2-tetrachloro-3,3,4,4-tetrafluorocyclobutane","336-50-5","D",0]
["1-Ethoxy-2,2,3,3,3-pentafluoro-1-Propanol","337-28-0","D",0]
["3,3,4,4-Tetrafluoro-4-iodo-1-butene","33831-83-3","D",0]
["perfluoro-N,N-bis(perfluoroethyl)propylamine","338-81-8","D",0]
["1,2-dichloro-3,3,4,4,5,5,6,6-octafluorocyclohexene","336-19-6","D",0]
["Perfluorohexanedioic acid","336-08-3","D",0]
["1H,1H,7H-Dodecafluoro-1-heptanol","335-99-9","D",0]
["N-allyl-1,1,2,2,3,3,4,4,5,5,5-undecafluoropentane-1-sulphonamide","335-97-7","D",0]
["1-Decanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heneicosafluoro-","335-77-3","D",0]
["Perfluoroheptanesulphonyl fluoride","335-71-7","D",0]
["Perfluamine","338-83-0","D",0]
["Fluorocarbon FC 70","338-84-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymers with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol- and 2-hydroxyethyl acrylate-blocked 2,4-TDI-trimethylolpropane polymer, Memethacrylate and¿","339163-51-8","D",0]
["2,2,3,3,4,4,5,5,6-nonafluoro-6-(heptafluoropropyl)tetrahydro-2H-pyran","335-35-3","D",0]
["Perfluoropropanoic acid","422-64-0","D",0]
["1-Chloro-1,1,2,2,3,3,3-heptafluoropropane","422-86-6","D",0]
["1,3-Diiodoperfluoropropane","422-91-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecyl methacrylate","41123-44-8","D",0]
["1,1,2,2,3,3,4,4,4-nonafluoro-N-[(trifluoromethyl)sulfonyl]-1-Butanesulfonamide","39847-37-5","D",0]
["Bis(1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonyl)imide","39847-39-7","D",0]
["eledoisin perfluoroacetate","39877-24-2","D",0]
["1,4-Butanediol, polymer with 1,6-diisocyanatohexane, 2-ethyl-1-hexanol-and gamma-omega-perfluoro-C8-14-alc.-blocked","399026-30-3","D",0]
["6,6,7,7,8,8,8-heptafluoro-2-methylocta-3,5-dione","40002-62-8","D",0]
["Sodium perfluorooctanesulfonate","4021-47-0","D",0]
["Pent-4-en-2-yl perfluoro-2-propoxypropanoate","402570-09-6","D",0]
["3,4-Dichloro-1-methylbutyl perfluoro-2-(propoxy)propanoate","402570-10-9","D",0]
["3,4-Dichloro-perfluoro-1-methylbutyl perfluoro-2-propoxypropanoate","402570-11-0","D",0]
["Perfluoro(7-methyl)octanesulfonate potassium salt","40365-28-4","D",0]
["Perfluoro(butyltetrahydrofuran)","40464-54-8","D",0]
["1,1,2,2,3,3-Hexafluoro-1-[(trifluoroethenyl)oxy]-3-(trifluoromethoxy)propane","40573-09-9","D",0]
["Benzoic acid, 4-(1,1-dimethylethyl)-, ethenyl ester, polymer with ethene, 4-(ethenyloxy)-1-butanol, 1,1,2,3,3,3-hexafluoro-1-propene and 1,1,2,2-tetrafluoroethene","406207-51-0","D",0]
["Heptadecafluoro-N,N-bis(2-hydroxyethyl)octanesulphonamide","40630-61-3","D",0]
["N-Allylperfluorobutanesulfonamide","40630-65-7","D",0]
["1,1,1,3,3-Pentafluorobutane","406-58-6","D",0]
["(Perfluorocyclohexyl)methyl prop-2-enoate","40677-94-9","D",0]
["(1H,1H-Perfluoroethyl)(2H-perfluoroethyl)ether","406-78-0","D",0]
["2:2 Fluorotelomer iodide","40723-80-6","D",0]
["trifluoroacetic anhydride","407-25-0","D",0]
["Dichloro(methyl)(1,1,2,2-tetrafluoroethyl)silane","422-69-5","D",0]
["2,2,3,3,4,4,5-Heptafluorotetrahydro-5-(nonafluorobutyl)furan","335-36-4","D",0]
["Perfluorobutanoyl fluoride","335-42-2","D",0]
["2,2,3-Trichloroheptafluorobutane","335-44-4","D",0]
["Heptane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-hexadecafluoro-","335-57-9","D",0]
["[3,3,4,4-Tetrafluoro-4-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]butyl]trichlorosilane","413570-89-5","D",0]
["7H-Perfluoroheptanoyl chloride","41405-35-0","D",0]
["ethyl perfluoroheptanoate","41430-70-0","D",0]
["(7.alpha.,17.beta.)-17-(acetyloxy)-7-[9-[(4,4,5,5,5-pentafluoropentyl)thio]nonyl]-estr-4-en-3-one","415927-29-6","D",0]
["Sodium 2-[(perfluorooctyl)oxy]benzene-1-sulfonate","41674-07-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl acrylate","4180-26-1","D",0]
["(2,2,3,3,4,4,5,5,6,6,7,7,8,9,9,9-Hexadecafluoro-8-(trifluoromethyl)nonyl)oxirane","41925-33-1","D",0]
["octafluorotetrahydrothiophene 1,1-dioxide","42060-64-0","D",0]
["alpha,alpha,beta,beta-tetrafluoro-2-methylphenetole","42145-66-4","D",0]
["2-Propenoic acid, 2-hydroxyethyl ester, adduct with 5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexane (1:1), reaction products with ethoxylated reduced Me esters of reduced polymd. oxidized tetrafluoroethylene","421595-49-5","D",0]
["1,1,1,2-Tetrafluoro-2-chloropropane","421-73-8","D",0]
["1,3-Dichloro-1,1,2,2-tetrafluoropropane","422-00-4","D",0]
["3-Chloro-1,1,1,2,2-pentafluoropropane","422-02-6","D",0]
["2,2,3,3,3-pentafluoropropylamine","422-03-7","D",0]
["Pentafluoropropiononitrile","422-04-8","D",0]
["2:1 Fluorotelomer alcohol","422-05-9","D",0]
["pentafluoropropionaldehyde","422-06-0","D",0]
["1,3,3-Trichloro-1,1,2,2-tetrafluoropropane","422-54-8","D",0]
["1-Bromoheptafluoropropane","422-85-5","D",0]
["2-Propenethioic acid, 2-methyl-, S-[3,3,4,4,5,5,6,6,7,8,8,8-dodecafluoro-7-(trifluoromethyl)octyl] ester","30769-91-6","D",0]
["N-(2-Methylsulfinyl-1,1-dimethyl-ethyl)-N'-{2-methyl-4-[perfluoroisopropyl]phenyl}phthalamide","371771-07-2","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], .alpha.-[2-[ethyl[(perfluorooctyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","37338-48-0","D",0]
["1,1-Dichloro-1,2,2,2-tetrafluoroethane","374-07-2","D",0]
["3,3,4,4,4-Pentafluorobut-1-ene","374-27-6","D",0]
["pentadecafluorotriethylamine","359-70-6","D",0]
["perfluorohept-1-ene","355-63-5","D",0]
["dodecafluorocyclohexane","355-68-0","D",0]
["decafluorocyclohexene","355-75-9","D",0]
["1H,1H,5H-Perfluoropentanol","355-80-6","D",0]
["tris(2,2,3,3,4,4,5,5-octafluoropentyl) phosphate","355-86-2","D",0]
["1H,1H,5H-Perfluoropentyl methacrylate","355-93-1","D",0]
["tetrafluorosuccinyl chloride","356-15-0","D",0]
["1,2-Dichlorohexafluorocyclobutane","356-18-3","D",0]
["1,3-Dichloro-1,2,2,3,4,4-hexafluoro-cyclobutane","356-19-4","D",0]
["Methyl perfluorobutanoate","356-24-1","D",0]
["Heptafluorobutyraldehyde ethyl hemiacetal","356-26-3","D",0]
["Ethyl perfluorobutanoate","356-27-4","D",0]
["vinyl heptafluorobutyrate","356-28-5","D",0]
["1,1,2,3,3,4,4,5,6,6-Decafluorohexa-1,5-diene","356-35-4","D",0]
["Pentafluoropropanoic anhydride","356-42-3","D",0]
["Bis(pentafluoropropionyl) peroxide","356-45-6","D",0]
["Perfluoro-2-methyloxane","356-47-8","D",0]
["Perfluoro-5-(pentafluoroethyl)oxolane","356-48-9","D",0]
["1-cyano-2,2,3,3-tetrafluorocyclobutane","356-81-0","D",0]
["(E)-Perfluoro(4-methyl-2-pentene)","3709-71-5","D",0]
["1,2-Dibromo-1-Chloro-1,2,2-Trifluoroethane","354-51-8","D",0]
["Bromopentafluoroethane","354-55-2","D",0]
["Pentafluoroiodoethane","354-64-3","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with ethene and 1,1,2,2-tetrafluoroethene","35560-16-8","D",0]
["2,2,3,3,4,4,5,5,6,6-decafluoro-1-(trifluoromethyl)piperidine","359-71-7","D",0]
["1,3,3,3-Tetrafluoro-1-methoxy-2-(trifluoromethyl)-1-propene","360-53-2","D",0]
["Methyl 3,3,3-trifluoro-2-(trifluoromethyl)propionate","360-54-3","D",0]
["Perfluorobut-2-ene","360-89-4","D",0]
["tris[6,6,7,7,8,8,8-heptafluoro-2,2-di[2H3]methyl[1,1,1-2H3]octane-3,5-dionato-O,O']europium","36393-27-8","D",0]
["1H,1H,3H-Perfluorobutyl 2-methylacrylate","36405-47-7","D",0]
["(perfluoroethylene)bis[(perfluoromethyl)aminyl] dioxide","36525-64-1","D",0]
["Propane, 1,1,3,3-tetrabromo-1,2,2,3-tetrafluoro-","36567-29-0","D",0]
["ammonium 8-chlorohexadecafluoro-7-methyloctanoate","3658-57-9","D",0]
["Ammonium perfluoro(7-methyloctanoate)","3658-62-6","D",0]
["Ammonium octadecafluoro-9-(trifluoromethyl)decanoate","3658-63-7","D",0]
["3,3-Bis(trifluoromethyl)perfluoropentane","36591-89-6","D",0]
["1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonic anhydride","36913-91-4","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, oxidized, polymd., reduced, hydrolyzed, reaction products with ammonia","370097-12-4","D",0]
["Ethanol, 2,2¿,2¿¿-nitrilotris-, compds. with hydrolyzed reduced polymd. oxidized 1,1,2,3,3,3-hexafluoro-1-propene","370097-18-0","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoroocty ester, polymer with .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-hydroxypoly(oxy-1,2-ethanediyl) and .alpha.-(1-oxo-2-propenyl)-.omega.-hydroxypoly[oxy(methyl-1,2-ethanediyl)]","370100-90-6","D",0]
["7:2 Fluorotelomer dihydrogen phosphate","37013-72-2","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester, polymer with methyloxirane polymer with oxiranemono-2-propenoate, tert- Bu 2-ethylhexaneperoxoate-initiated","370873-97-5","D",0]
["2-Pentene, 1,1,1,2,3,4,5,5,5-nonafluoro-4-(trifluoromethyl)-, (Z)-","3709-70-4","D",0]
["1H,1H-Perfluoropropyl acrylate","356-86-5","D",0]
["1-(2,2,3,3,4,4,4-heptafluoro-1-oxobutyl)-1H-imidazole","32477-35-3","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymers withN-(1,1-dimethyl-3-oxobutyl)-2-propenamide, 2-ethylhexyl acrylate, gamma-omega-perfluoro-C8-16-alkyl acrylate, stearyl acrylate and vinyl chloride, ¿","325966-78-7","D",0]
["Methanaminium, N,N,N-trimethyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)","32609-65-7","D",0]
["Bis(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoyl) peroxide","32687-76-6","D",0]
["2-Propenoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester","307-98-2","D",0]
["Perfluorotetradecahydrophenanthrene","306-91-2","D",0]
["1-(Trifluoromethyl)perfluorodecalin","306-92-3","D",0]
["Perflunafene","306-94-5","D",0]
["Perfluoro-2-methyldecalin","306-95-6","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-[3-(dimethylamino)propyl], reaction products with acrylic acid (TSCA)","306973-44-4","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-hydro-omega-hydroxy-, polymer with 1,6-diisocyanatohexane, N-(hydroxyethyl)-N-methylperfluoro-C4-8-alkanesulfonamides-blocked","306975-84-8","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-[2-(methylamino)ethyl]-omega-[(1,1,3,3-tetramethylbutyl)phenoxy]-, N-[(perfluoro-C4-8-alkyl)sulfonyl] derivs.","306979-40-8","D",0]
["Perfluoro-1,2-dimethylcyclohexane","306-98-9","D",0]
["2-Methyl(nonafluorobutyl)sulfonylaminoethyl 2-propenoate telomer with 2-mercaptoethanol","306997-46-6","D",0]
["Perfluoroperhydrofluorene","307-08-4","D",0]
["1-chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexane","307-22-2","D",0]
["1-Octanol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","307-30-2","D",0]
["1-Chloroheptadecafluorooctane","307-33-5","D",0]
["Perfluorooctane","307-34-6","D",0]
["Perfluorodecane","307-45-9","D",0]
["Perfluoroundecane","307-49-3","D",0]
["Perfluorodecanesulphonyl fluoride","307-51-7","D",0]
["Perfluorododecane","307-59-5","D",0]
["Perfluorotetradecane","307-62-0","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, telomer with 2,2-dichloro-1,1,1-trifluoroethane and 1,1-difluoroethene (9CI)","321657-92-5","D",0]
["vinyl pentafluoropropionate","357-47-1","D",0]
["Hexane, 1,6-diisocyanato-, homopolymer, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-octanol-blocked","357624-15-8","D",0]
["2-Propenoic acid, 2-methyl-, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-methyl-2-propenoate, methyl 2-methyl-2-propenoate and 2-methylpropyl 2-methyl-2-propenoate","357924-15-3","D",0]
["Perfluorobutane-1-sulfonamidoethanol","34454-99-4","D",0]
["undecafluorocyclohexane","308-24-7","D",0]
["2,2,3,3,4,4,5,5,5-nonafluoropentyl acrylate","308-26-9","D",0]
["2-Propanol, 1-[4-(1-methylpropyl)phenoxy]-3-(2,2,3,3-tetrafluoropropoxy)-","308362-88-1","D",0]
["Iodonium, (3-methylphenyl)phenyl-, ar'-C12-13-branched alkyl derivs., (OC-6-11)-hexafluoroantimonates(1-)","309263-22-7","D",0]
["N,N-Diethyl-2H-perfluoropropanamine","309-88-6","D",0]
["Potassium perfluorocyclohexyl sulfonate","3107-18-4","D",0]
["Disodium 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl phosphate","3107-32-2","D",0]
["Ethanesulfonic acid, 2-(1-(difluoro((trifluoroethenyl)oxy)methyl)-1,2,2,2-tetrafluoroethoxy)-1,1,2,2-tetrafluoro-, polymer with tetrafluoroethene","31175-20-9","D",0]
["Ethanesulfonic acid, 1,1,2,2-tetrafluoro-2-[1,2,2-trifluoro-2-[(trifluoroethenyl)oxy]-1-(trifluomethyl)ethoxyl]-, sodium salt, polymer with tetrafluoroethene","31176-88-2","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N,N-bis(nonafluorobutyl)-1-butanamine","311-89-7","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,10,10,10-hexadecafluoro-9-(trifluoromethyl)decyl ester, homopolymer","31214-91-2","D",0]
["1,1,2,2-Tetrafluoro-3-(trimethylsilyl)-cyclobutane","312-81-2","D",0]
["octafluoronaphthalene","313-72-4","D",0]
["N-methyl-N-(1,1,2,2-tetrafluoroethyl)benzenesulphonamide","31375-11-8","D",0]
["N-Methylperfluorooctanesulfonamide","31506-32-8","D",0]
["N-Butylperfluorooctane-1-sulfonamide","31506-34-0","D",0]
["Tetrafluoroethene polymer with trifluoro(pentaflurorethoxy)ethene","31784-04-0","D",0]
["1-Decanaminium, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-N,N-bis(2-hydroxyethyl)-N-methyl-, iodide (1:1)","31841-41-5","D",0]
["Siloxanes and Silicones, di-Me, mono[3-[(2-methyl-1-oxo-2-propenyl)oxy]propyl group]-terminated, polymers with 2-[[[[5-[[[2-[[[[[5-[[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]carbonyl]amino]-2-","321371-84-0","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with methyloxirane polymer with oxirane mono-2-propenoate,tert-Bu 2-ethylhexaneperoxoate-initiated","393582-46-2","D",0]
["2-Propenoic acid, octahydro-4,7-methano-1H-indenyl ester, polymers with gamma-omega-perfluoro-C6-22-alkyl acrylate and polyethylene glycol methacrylate Meether, di-Me 2,2'-azobis[2-methylpropanoate]-initiated","393582-59-7","D",0]
["2-Propenoic acid, octadecyl ester, polymers with gamma-omega-perfluoro-C6-22-alkylacrylate","393819-33-5","D",0]
["Chlorodifluoromethane and chloropentafluoroethane mixture","39432-81-0","D",0]
["1,1,1,2,3,3-Hexafluoro-3-methoxypropane","382-34-3","D",0]
["1H,4H-Octafluorobutane","377-36-6","D",0]
["Perfluorobutanedioic acid","377-38-8","D",0]
["(2E)-4,4,5,5,6,6,6-Heptafluorohex-2-en-1-ol","37759-88-9","D",0]
["Diethyl tetrafluorosuccinate","377-71-9","D",0]
["2,2,3,3-tetrafluoro-3-(heptafluoropropoxy)propionic acid","378-03-0","D",0]
["1,4-dibromo-2-chloro-1,1,2-trifluorobutane ","378-13-2","D",0]
["Methyl 1H,1H-perfluoropropyl ether","378-16-5","D",0]
["2,2,3,3-Tetrafluorocyclobutanemethanol","378-17-6","D",0]
["Methyl pentafluoropropionate","378-75-6","D",0]
["Potassium perfluoropropanoate","378-76-7","D",0]
["Sodium perfluoropropanoate","378-77-8","D",0]
["Octafluoroadipoyl difluoride","37881-62-2","D",0]
["1-Butene, 1,1,2,3,3,4,4-heptafluoro-4-iodo-","378-82-5","D",0]
["Ammonium tricosafluorododecanoate","3793-74-6","D",0]
["Silver perfluorobutanoate","3794-64-7","D",0]
["(3-(Perfluorooctyl)sulphonylaminopropyl)trimethylammonium chloride","38006-74-5","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, telomer with 1-dodecanethiol, methyl 2-methyl-2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-hydroxypoly(oxy-¿","380843-06-1","D",0]
["1-Octanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-[2-(phosphonooxy)ethyl]-","3820-83-5","D",0]
["1,1-Bis(trifluoromethyl)ethene","382-10-5","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester","3934-23-4","D",0]
["Perfluoropentanoyl fluoride","375-62-2","D",0]
["Trichloro(1,1,2,2,3,3,4,4-octafluorobutyl)-silane","375-63-3","D",0]
["Perfluorobutanesulfonyl fluoride","375-72-4","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulphonic acid","375-73-5","D",0]
["Hexafluoroamylene glycol","376-90-9","D",0]
["Methyl 2,3,3,3-tetrafluoropropanoate","382-93-4","D",0]
["2-(N-Butylperfluorooctanesulfonamido)ethyl acrylate","383-07-3","D",0]
["Dichloromethyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","38436-16-7","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-iodononan-1-ol","38550-44-6","D",0]
["1-andecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-iodo-","38550-45-7","D",0]
["1-Tridecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro-2-iodo-","38550-46-8","D",0]
["Oxirane, 2-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heneicosafluoroandecyl)-","38565-54-7","D",0]
["1,1,1,3,3,3-hexafluoro[2-2H]propan-2-[2H]ol","38701-74-5","D",0]
["sodium N-ethyl-N-[(heptadecafluorooctyl)sulphonyl]glycinate","3871-50-9","D",0]
["Potassium perfluoropentanesulfonate","3872-25-1","D",0]
["Praseodymium(3+) (1Z)-2,2,3,3,4,4,4-heptafluoro-1-(4,7,7-trimethyl-3-oxo-2-bicyclo[2.2.1]heptanylidene)butan-1-olate","38832-94-9","D",0]
["1-Propanaminium, 3-[(carboxymethyl)[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-N,N,N-trimethyl-, inner salt","38850-52-1","D",0]
["1-Propanaminium, N-(2-hydroxyethyl)-N,N-dimethyl-3-[(3-sulfopropyl)[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-, inner salt","38850-58-7","D",0]
["1-Propanesulfonic acid, 3-[[3-(dimethylamino)propyl][(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-","38850-60-1","D",0]
["1,3-Bis(1,1,2,2-tetrafluoroethoxy)benzene","3914-19-0","D",0]
["Methylperfluoro-2,5,8-trimethyl-3,6,9-trioxadodecanoic acid","39187-47-8","D",0]
["Alcohols, C8-14, .alpha.-.omega.-perfluoro, ethoxylated, propoxylated","391895-07-1","D",0]
["Tris(2-(perfluorododecyl)ethyl)phosphate","393098-42-5","D",0]
["Tris(2-(perfluorotetradecanyl)ethyl)phosphate","393098-44-7","D",0]
["Perfluoroisobutene","382-21-8","D",0]
["1-Octanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-methyl-, reaction products with benzene-chlorine-sulfur chloride (S2Cl2) reaction products chlorides","182700-90-9","D",0]
["Ytterbium(3+) tris[(3Z)-6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-5-oxo-3-octen-3-olate]","18323-96-1","D",0]
["tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyloctane-3,5-dionato-O,O')holmium","18323-97-2","D",0]
["tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyloctane-3,5-dionato-O,O')dysprosium","18323-98-3","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), polymers with 1,1'-methylenebis[4-isocyanatobenzene] and polymethylenepolyphenylene isocyanate, 2-ethylhexyl esters, Me Et ketone oxime-blocked","178535-22-3","D",0]
["Siloxanes and Silicones, di-Me, 3-hydroxypropylmethyl, methylvinyl, [(ethenyldimethylsilyl)oxy]-terminated, ethers with trifluoro(trifluoromethyl)oxirane homopolymer 1,2,2,2-tetrafluoro-1-(hydroxymethyl) ethyltetrafluoro (trifluoromethyl) ethyl¿","174393-72-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers with delta-omega-perfluoro-C10-16-alkyl acrylate and vinyl acetate","174125-96-3","D",0]
["Perfluoro(1,1,9,9-tetrahydro-2,5-bis(trifluoromethyl)-3,6-dioxa-8-nonen-1-ol)","174082-85-0","D",0]
["1,1,1,3,3,3-Hexafluoropropane-2,2-diamine","1737-80-0","D",0]
["alpha,alpha,beta,beta-tetrafluoro-p-methylphenetole","1737-11-7","D",0]
["4,4,4-trifluoro-3-(trifluoromethyl)crotonic acid","1763-28-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecanoic acid","1765-48-6","D",0]
["Propanoic acid, 3-[(gamma-omega-perfluoro-C6-18-alkyl)thio] derivs.","176590-84-4","D",0]
["1H,1H-Heptafluorobutyl epoxide","1765-92-0","D",0]
["Perfluoro-N-[(trifluoromethyl)sulfonyl]butanesulfonamide sodium salt","176719-69-0","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 2-ethylhexyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propen-1-yl)-omega-methoxypoly(oxy¿","176741-19-8","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,methyloxirane polymer with oxirane mono-2-propenoate, alpha-(2-methyl-1-oxo-¿","176894-23-8","D",0]
["Siloxanes and Silicones, di-Me, vinyl group-terminated, polymers with 4-bromo-3,3,4,4-tetrafluoro-1-butene, 1,1-difluoroethene, 1,1,2,3,3,3-hexafluoro-1-propene and tetrafluoroethene","177473-71-1","D",0]
["Propanenitrile, 2,3,3,3-tetrafluoro-2-[1,1,2,2,3,3-hexafluoro-3-[(trifluoroethenyl)oxy]propoxy]-, polymer with tetrafluoroethene and trifluoro(trifluoromethoxy)ethene","177484-43-4","D",0]
["3-[(Perfluorooctane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide potassium","178094-69-4","D",0]
["3-[(Perfluoroheptane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide potassium salt","178094-70-7","D",0]
["1-Hexanesulfonamide, N-[3-(dimethyloxidoamino)propyl]-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, potassium salt (1:1)","178094-71-8","D",0]
["3-[(Perfluoropentane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide potassium salt","178094-72-9","D",0]
["3-[(Perfluorobutane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide potassium salt","178094-73-0","D",0]
["2-Propenamide, N-[(C1-20-alkyloxy)methyl]derivs., polymers with acryonitrile,.alpha.-fluoro-.omega.-[2-[(1-oxo-propenyl)oxy]ethyl] poly(difluoromethylene) and polyethylene-polypropylene glycol acrylate C1-20-alkyl ethers","182700-85-2","D",0]
["1,1,1,3,3-Pentafluoro-3-methoxy-2-(trifluoromethyl)propane","382-26-3","D",0]
["Perfluoro(N-methylmorpholine)","382-28-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(methoxymethyl)propane","382-30-9","D",0]
["1H,1H,3H-Perfluorobutanol","382-31-0","D",0]
["1-Decanamine, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","30670-30-5","D",0]
["Hexacosafluoro-13-(trifluoromethyl)tetradecanoic acid","18024-09-4","D",0]
["Decafluoro-5-(trifluoromethyl)hexanoyl fluoride","18017-31-7","D",0]
["1,6-Divinylperfluorohexane","1800-91-5","D",0]
["Perfluoromethylcyclopentane","1805-22-7","D",0]
["Sulfonic acids, C6-12-alkane, gamma-omega-perfluoro, ammonium salts","180582-79-0","D",0]
["6:2 Fluorotelomer sulfonate barium salt","1807944-82-6","D",0]
["1H,1H,2H,2H-Perfluorohexyl methacrylate","1799-84-4","D",0]
["Praseodymium, tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-3,5-octanedionato-betaO3,betaO5)-","17978-77-7","D",0]
["tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-3,5-octanedionato-O,O')neodymium","17978-76-6","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-[3-(dimethyloxidoamino)propyl]","179005-07-3","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-[3-(dimethyloxidoamino)propyl], potassium salts","179005-06-2","D",0]
["Fatty acids, linseed-oil, gamma-omega-perfluoro-C8-14-alkyl esters","178535-23-4","D",0]
["Propane, 1,1,1,2,2-pentafluoro-","1814-88-6","D",0]
["Sodium tributyl(2-methoxypropyl)phosphanium 4,4'-(1,1,1,3,3,3-hexafluoropropane-2,2-diyl)diphenolate (1/1/1)","181531-28-2","D",0]
["Alcohols, C1-20, reaction products with glycidol, gamma-omega-perfluoro C8-14 alcs.and N,N',2-tris(6-isocyanatohexyl)imidodicarbonic diamide","182700-79-4","D",0]
["2-Propenoic acid, C1-20-alkyl esters, polymers with .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene)","182700-81-8","D",0]
["2-Butenedioic acid (Z)-, di-C1-20-alkyl esters, polymer with acrylamide N-[(C1-10-alkyloxy)methyl]derivs.,.alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl] poly (difluoromethylene) and vinylchloride","182700-82-9","D",0]
["2-Butenedioic acid (Z)-, di-C1-20-alkyl esters, polymer with .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene), 2-hydroxyethyl acrylate and vinyl chloride","182700-83-0","D",0]
["2-Propenoic acid, C1-20-alkyl esters, polymers with .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and polyethylene-polypropylene glycol monoacrylate","182700-84-1","D",0]
["2-Iodoperfluorobutane","375-51-9","D",0]
["Boron, trifluoro(tetrahydrofuran)-, (T-4)-, polymer with 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane, ether with 2,2-dimethyl-1,3-propanediol (2:1), bis(hydrogen sulfate), diammonium salt","452080-67-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-methylpropyl ester, polymer with butyl 2-propenoate and 2,5-furandione, gamma-omega-perfluoro-C8-14-alkyl esters, tert-Bubenzenecarboperoxoate-initiated","459415-06-6","D",0]
["Propane, 1,1,1,3,3-pentafluoro-","460-73-1","D",0]
["1,1'-Oxybis(1,1,2,2,3,3,4,4,5,5,5-undecafluoropentane)","464-36-8","D",0]
["1,1,1-Trichloropentafluoropropane","4259-43-2","D",0]
["1H-Perfluoro-1,1-propanediol","422-63-9","D",0]
["Perfluoropropionyl fluoride","422-61-7","D",0]
["Perfluoropropionyl chloride","422-59-3","D",0]
["3-Chloro-1,1,1,2,2,3-hexafluoropropane","422-57-1","D",0]
["HCFC-225ca","422-56-0","D",0]
["1-Chloro-1,1,2,2,3,3-hexafluoropropane","422-55-9","D",0]
["Nonafluoro-1-iodobutane","423-39-2","D",0]
["Perfluoropropanesulfonic acid","423-41-6","D",0]
["Ammonium perfluoroundecanoate","4234-23-5","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","423-54-1","D",0]
["1-Bromoheptadecafluorooctane","423-55-2","D",0]
["N-(2-Hydroxyethyl)-N-propylperfluorooctanesulfonamide","4236-15-1","D",0]
["11:1 Fluorotelomer alcohol","423-65-4","D",0]
["2-(N-Ethyl-N-(perfluorooctylsulfonyl)amino)ethyl acrylate","423-82-5","D",0]
["N-allylheptadecafluorooctanesulphonamide","423-86-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononanoyl chloride","423-95-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-6-[(tridecafluorohexyl)oxy]hexane","424-20-4","D",0]
["vinyl perfluorovalerate","424-37-3","D",0]
["Diethyl perfluoroglutarate","424-40-8","D",0]
["1H,1H-Perfluoropropyl methacrylate","45115-53-5","D",0]
["2,2,2-trifluoroethyl trifluoroacetate","407-38-5","D",0]
["2,3,3,3-Tetrafluoro-2-(1,1,2,2-tetrafluoro-2-(fluorosulphonyl)ethoxy)propionyl fluoride","4089-57-0","D",0]
["8-Fluorosulfonylperfluoro(2,5-dimethyl-3,6-dioxaoctanoyl) fluoride","4089-58-1","D",0]
["ammonium 2-[2-[2-(aminosulphonyl)-1,1,2,2-tetrafluoroethoxy]-1,1,2,3,3,3-hexafluoropropoxy]-2,3,3,3-tetrafluoropropionate","4089-61-6","D",0]
["1-Chloro-1,1,2,2,3,3,4,4-octafluorobutane","423-31-4","D",0]
["Methyl perfluoro-2-[2-(3,3,3-trichloropropoxy)propoxy]propanoate","426264-19-9","D",0]
["Trichloro(1,1,2,3,3,3-hexafluoropropyl)silane","426-50-6","D",0]
["Ethyl perfluoropropionate","426-65-3","D",0]
["Trifluoro(trifluoromethyl)oxirane","428-59-1","D",0]
["Hexane, 1,6-diisocyanato-, homopolymer, alpha-fluoro-omega-(hydroxyethyl)poly(difluoromethylene)- and Me Et ketone oxime- and polyethylene glycol mono-Me ether-blocked","428842-38-0","D",0]
["tris[6,6,7,7,8,8,8-heptafluoro-2,2-di[(2H3)methyl](1,1,1-2H3)octane-3,5-dionato-O,O']praseodymium","42942-19-8","D",0]
["methylsilylidyne tris(trifluoroacetate)","429-72-1","D",0]
["Disulfide, bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)","42977-21-9","D",0]
["1,1,1,2,3-Pentafluoropropane","431-31-2","D",0]
["2,2,3,3-Tetrafluoropropanenitrile","431-32-3","D",0]
["1,1,1,2,3,3-hexafluoropropane","431-63-0","D",0]
["2-chloro-1,1,1,3,3,3-hexafluoropropane","431-87-8","D",0]
["1,1,1,2,3,3,3-Heptafluoropropane","431-89-0","D",0]
["Perfluorotrihexylamine","432-08-6","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)thio]propanoic acid lithium salt","433333-62-1","D",0]
["Iodononafluoro-t-butane","4459-18-1","D",0]
["1,1,2,2-Tetrafluoro-2-(1,2,2,2-tetrafluoroethoxy)ethane-1-sulfonyl fluoride","446312-61-4","D",0]
["3-Methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]-oxetane","449177-94-0","D",0]
["2,2,3,3-Tetrafluoropropyl methacrylate","45102-52-1","D",0]
["1H,1H-Perfluorobutyl acrylate","424-64-6","D",0]
["decafluorocyclopentane","376-77-2","D",0]
["1H,1H,5H-Perfluoropentyl acrylate","376-84-1","D",0]
["perfluoropent-1-ene","376-87-4","D",0]
["perfluoroglutaronitrile","376-89-6","D",0]
["1,6-Diiodoperfluorohexane","375-80-4","D",0]
["3,3,4,4,4-pentafluorobutan-2-ol","374-40-3","D",0]
["2,2-bis(Trifluoromethyl)perfluoropropane","374-51-6","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, polymers with 1,3-butanediol, 1,3-diisocyanatomethylbenzene and 2-ethyl-2-(hydroxymethyl)-1,3-propanediol","374551-53-8","D",0]
["Perfluorobutylcyclohexane","374-60-7","D",0]
["2-Propenoic acid, butyl ester, polymer with 2-ethylhexyl-2-propenoate, 2-hydroxyethyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl-2-propenoate, 4,4'-azobis[4-cyanopentanoic acid]-initiated","374623-78-6","D",0]
["1,1,2,2,3,4,4,5,5,6-Decafluoro-3,6-bis(trifluoromethyl)cyclohexane","374-77-6","D",0]
["2H-Tricosafluoro-5,8,11,14-tetrakis(trifluoromethyl)-3,6,9,12,15-pentaoxaoctadecane","37486-69-4","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, telomer with chlorotrifluoroethene, oxidized, reduced, Et ester","374931-83-6","D",0]
["Heptafluorobutyl iodide","374-98-1","D",0]
["2,2,3,3,4,4,4-heptafluorobutylamine","374-99-2","D",0]
["Heptafluorobutyronitrile","375-00-8","D",0]
["3:1 Fluorotelomer alcolhol","375-01-9","D",0]
["heptafluorobutyraldehyde","375-02-0","D",0]
["Heptafluoro-1-methoxypropane","375-03-1","D",0]
["3,3,4,4,5,5,5-heptafluoropentan-2-ol","375-14-4","D",0]
["Heptafluorobutyryl Chloride","375-16-6","D",0]
["Heptafluorobutyric-acid","375-22-4","D",0]
["1,1,1,3,4-pentachloro-2,2,3,4,4-pentafluorobutane","375-46-2","D",0]
["Perfluoro-1,4-diiodobutane","375-50-8","D",0]
["Perfluoropentanedioic acid","376-73-8","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propanenitrile","42532-60-5","D",0]
["Perfluoromethoxypropionyl fluoride","425-38-7","D",0]
["2,2,3,3-Tetrafluoro-1,4-butanediol","425-61-6","D",0]
["1,1,2,2-Tetrafluoro-1-methoxyethane","425-88-7","D",0]
["nonatetracontafluoro-24-iodotetracosane","39823-55-7","D",0]
["Perfluoropentanesulfonyl fluoride","375-81-5","D",0]
["Perfluoroheptanoyl fluoride","375-84-8","D",0]
["Perfluoroheptanoic acid","375-85-9","D",0]
["1-Bromopentadecafluoroheptane","375-88-2","D",0]
["dotetracontafluoroicosane","37589-57-4","D",0]
["Perfluoroheptanesulfonic acid","375-92-8","D",0]
["Perfluorononane","375-96-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-henicosafluorodecane","375-97-3","D",0]
["Perfluorotridecane","376-03-4","D",0]
["2-(N-Ethylperfluorooctanesulfonamido)ethyl methacrylate","376-14-7","D",0]
["1H,1H,9H-Hexadecafluoro-1-nonanol","376-18-1","D",0]
["perfluoronon-1-ene","376-22-7","D",0]
["1,3-Dioxole, 4,5-difluoro-2,2-bis(trifluoromethyl)-, polymer with 1,1,2,2-tetrafluoroethene","37626-13-4","D",0]
["Ammonium 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoate","376-34-1","D",0]
["Diethyl octafluorohexanedioate","376-50-1","D",0]
["Adiponitrile, perfluoro","376-53-4","D",0]
["3,3,4,4,5,5-Hexafluorodihydro-2H-pyran-2,6(3H)-dione","376-68-1","D",0]
["5H-Octafluoropentanoyl chloride","376-71-6","D",0]
["5H-Octafluoropentanoic acid","376-72-7","D",0]
["Perfluoroacetyl fluoride","354-34-7","D",0]
["Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","1835251-22-3","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","1244062-17-6","D",0]
["Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","250738-42-2","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","154478-87-2","D",0]
["Dotriacontane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","137338-41-1","D",0]
["Triacontane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","137338-40-0","D",0]
["3,6,9,12-Tetraoxadocosan-1-ol, 15,15,16,16,17, 17,18,18,19,19,20,20,21,21,22,22,22-heptadecafluorodimethyl-","88271-22-1","D",0]
["Undecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-nonadecafluoro-","191852-87-6","D",0]
["1,2-Undecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexa decafluoro-10-(trifluoromethyl)-, 1-(dihydrogen phosphate)","54009-73-3","D",0]
["1,2-Undecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10, 11,11,11-hexa decafluoro-10-(trifluoromethyl)-, 1-(dihydrogen phosphate), diammonium salt","63295-18-1","D",0]
["1,2-Undecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10, 11,11,11-hexa decafluoro-10-(trifluoromethyl)-, 1-(dihydrogen phosphate), compd. with 2,2¿-iminobis[ethanol] (1:2)","63295-19-2","D",0]
["2-Undecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)-, dihydrogen phosphate, diammonium salt","63295-23-8","D",0]
["Octacosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","137338-39-7","D",0]
["Hexacosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","133310-73-3","D",0]
["Tetracosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","117146-18-6","D",0]
["Heptadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","931415-52-0","D",0]
["Octadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","138472-76-1","D",0]
["Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","6145-05-7","D",0]
["Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","182130-15-0","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","182130-14-9","D",0]
["Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","1835250-47-9","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","182130-12-7","D",0]
["Tetracosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,17, 17,18,18,19,19,20,20,21,21,22,22,23,23,24, 24,24-tetratriacontafluoro-","100550-08-1","D",0]
["3,6,9,12,15,18,21,24-Octaoxatetratriacontan-1-ol, 27,27,28,28,29,29,30,30,31,31,32,32,33,33,34,34,34-heptadecafluoro-","88247-40-9","D",0]
["Acetic acid, 2-[[3,3,4,4,5,5,6,6,7,7,8,8,9,10,10, 10-hexadeca fluoro-1-[(phosphonooxy)methyl]-9-(trifluoromethyl) decyl]oxy]-, ammonium salt (1:2)","63295-24-9","D",0]
["Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(phenylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","1310480-28-4","D",0]
["Methanaminium, N-[4-[[4-(dimethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-methyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","1310480-27-3","D",0]
["Ethanaminium, N-[4-[[4-(diethylamino)phenyl][4-(ethylamino)-1-naphthalenyl]methylene]-2,5-cyclohexadien-1-ylidene]-N-ethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","1310480-24-0","D",0]
["1-Hexanesulfonyl fluoride, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","423-50-7","D",0]
["Potassium perfluorohexane-1-sulphonate","3871-99-6","D",0]
["Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","116177-54-9","D",0]
["3,6,9,12-Tetraoxadocosan-1-ol, 15,15,16,16,17, 17,18,18,19,19,20,20,21,21,22,22,22-heptadecafluoro-","55427-54-8","D",0]
["Ethanol, 2-[2-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluorodecyl)oxy]methylethoxy] methylethoxy]-","88243-12-3","D",0]
["Propanol, [2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10, 10-heptadecafluorodecyl)oxy]methylethoxy]-","88243-13-4","D",0]
["Ethanol, 2-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl)oxy]ethoxy]-","56900-98-2","D",0]
["Undecanal, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heneicosafluoro-","63967-42-0","D",0]
["Decanal, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-","335-73-9","D",0]
["Nonanal, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoro-","63967-40-8","D",0]
["2-Dodecenal, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-","864551-40-6","D",0]
["Dodecanal, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","864551-38-2","D",0]
["Decanal, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","135984-68-8","D",0]
["1-Undecanol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,11,11,11-heneicosafluoro-","307-46-0","D",0]
["1-Decanol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-nonadecafluoro-","307-37-9","D",0]
["1-Nonanol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoro-","423-56-3","D",0]
["1-Undecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)-","31200-97-2","D",0]
["9-Tetracosene, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","1244062-16-5","D",0]
["2-Undecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11, 11,11-heptadecafluoro-, dihydrogen phosphate, potassium salt","90179-37-6","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, 1-(dihydrogen phosphat), ammonium salt (1:2)","93857-45-5","D",0]
["1-Undecanol, 2-chloro-4,4,5,5,6,6,7,7,8,8,9,9,10, 11,11,11-hexadecafluoro-10-(trifluoromethyl)-, dihydrogen phosphate","63295-22-7","D",0]
["3,6,9,12,15,18,21-Heptaoxahentriacontan-1-ol, 24,24,25,25,26,26,27,27,28,28,29,29,30, 30,31,31,31-heptadecafluoropentamethyl-","88243-10-1","D",0]
["Phosphine, tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]-","325459-92-5","D",0]
["2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethyl methacrylate, Me methacrylate und alpha-omega-perfluoro-C8-14-alkylacrylate","125328-29-2","D",0]
["2-Propenoic acid, perfluoro-C8-16-alkyl esters","85681-64-7","D",0]
["Piperazinium, 1-(carboxymethyl)-1-(2-hydroxyethyl)-4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-oxodecyl)-, innersalt","71356-38-2","D",0]
["Pentanedioic acid, 3- [2- [(3, 3, 4, 4, 5, 5, 6, 6, 7, 7, 8, 8, 9, 9, 10, 10, 10- heptadecafluorodecyl ) oxy] - 2- oxoethyl] - 3- hydroxy- , 1, 5- bis(3, 3, 4, 4, 5, 5, 6, 6, 7, 7, 8, 8, 9, 9, 10, 10, 10- heptadecafluorodecyl ) ester","302911-86-0","D",0]
["Pentanoic acid, 3,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-","1882109-63-8","D",0]
["Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-","1882109-64-9","D",0]
["Pentanoic acid, 2,3,3,4,5,5,5-heptafluoro-2-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-","1882109-65-0","D",0]
["Pentanoic acid, 2,3,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-2-(trifluoromethyl)-","1882109-66-1","D",0]
["Pentanoic acid, 2,2,4,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-3-(trifluoromethyl)-","1882109-67-2","D",0]
["Pentanoic acid, 2,2,3,4,5,5,5-heptafluoro-3-(1,1,2,2,2-pentafluoroethyl)-4-(trifluoromethyl)-","1882109-68-3","D",0]
["Pentanoic acid, 3,3,4,5,5,5-hexafluoro-2,2,4-tris(trifluoromethyl)-","1882109-70-7","D",0]
["Pentanoic acid, 2,4,4,5,5,5-hexafluoro-2,3,3-tris(trifluoromethyl)-","1882109-71-8","D",0]
["Pentanoic acid, 2,3,4,5,5,5-hexafluoro-2,3,4- tris(trifluoromethyl)-","1882109-72-9","D",0]
["Pentanoic acid, 2,3,3,5,5,5-hexafluoro-2,4,4- tris(trifluoromethyl)-","1882109-73-0","D",0]
["Pentanoic acid, 2,2,4,5,5,5-hexafluoro-3,3,4-tris(trifluoromethyl)-","1882109-74-1","D",0]
["Pentanoic acid, 2,2,3,5,5,5-hexafluoro-3,4,4- tris(trifluoromethyl)-","1882109-75-2","D",0]
["Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2- [1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-","1882109-76-3","D",0]
["Pentanoic acid, 2,3,3,4,4,5,5,5-octafluoro-2- (1,1,2,2,3,3,3-heptafluoropropyl)-","1882109-77-4","D",0]
["Hexanoic acid, 2,2,3,4,4,5,5,6,6,6-decafluoro-3-(1,1,2,2,2-pentafluoroethyl)-","1882109-78-5","D",0]
["Hexanoic acid, 2,2,3,3,4,5,5,6,6,6-decafluoro-4- (1,1,2,2,2-pentafluoroethyl)-","1882109-79-6","D",0]
["Hexanoic acid, 2,3,3,4,4,5,6,6,6-nonafluoro-2,5- bis(trifluoromethyl)-","1882109-80-9","D",0]
["Hexanoic acid, 2,2,3,4,5,5,6,6,6-nonafluoro-3,4- bis(trifluoromethyl)-","1882109-81-0","D",0]
["Octanoic acid, pentadecafluoro-, branched","90480-55-0","D",0]
["Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","78560-44-8","D",0]
["3,6,9,12,15,18-Hexaoxaoctacosan-1-ol, 21,21,22, 22,23,23,24,24,25,25,26,26,27,27,28,28,28-heptadecafluoro hexamethyl-","88243-16-7","D",0]
["3,6,9,12,15,18-Hexaoxaoctacosan-1-ol, 21,21,22, 22,23,23,24,24,25,25,26,26,27,27,28,28,28-heptadecafluoropentamethyl-","88243-11-2","D",0]
["3,6,9,12,15,18-Hexaoxaoctacosan-1-ol, 21,21,22, 22,23,23,24,24,25,25,26,26,27,27,28,28,28-heptadecafluoro-","88247-39-6","D",0]
["3,6,9,12,15-Pentaoxapentacosan-1-ol, 18,18,19, 19,20,20,21,21,22,22,23,23,24,24,25,25,25-heptadecafluoropentamethyl-","88243-15-6","D",0]
["3,6,9,12-Tetraoxadocosan-1-ol, 15,15,16,16,17, 17,18,18,19,19,20,20,21,21,22,22,22-heptadecafluorotetramethyl-","88243-14-5","D",0]
["Octadecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester","99955-83-6","D",0]
["2-Pentadecanol, 1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)-","94159-82-7","D",0]
["2-Tridecanol, 1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro-","94159-80-5","D",0]
["2-Pentadecanol, 1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-","94159-79-2","D",0]
["2-Tridecanol, 1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-eicosafluoro-12-(trifluoromethyl)-","94159-83-8","D",0]
["1-Propanaminium, N-(2-carboxyethyl)-N,N-dimethyl-3-[[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl]amino]-, innersalt","93776-15-9","D",0]
["1-Propanaminium, N-(2-carboxyethyl)-3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro-2-hydroxytridecyl)amino]-N,N-dimethyl-, inner salt","93776-13-7","D",0]
["1-Propanaminium, N-(2-carboxyethyl)-N,N-dimethyl-3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl)amino]-, inner salt","93776-12-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-Dotriacontafluoro-17-(trifluoromethyl)octadecyl methacrylate","94158-65-3","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-Octacosafluoro-15-(trifluoromethyl)hexadecyl methacrylate","94158-64-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-Dotriacontafluoro-17-(trifluoromethyl)octadecyl acrylate","94158-63-1","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-Octacosafluoro-15-(trifluoromethyl)hexadecyl acrylate","91615-22-4","D",0]
["2-Propenoic acid, gamma-mu-perfluoro-C8-14-alkyl esters","85631-54-5","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","1996-88-9","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","27905-45-9","D",0]
["2-(Perfluorodecyl) ethyl methacrylate, 2- Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester","2144-54-9","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl acrylate","17741-60-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-Tetracosafluoro-13-(trifluoromethyl)tetradecyl methacrylate","74256-15-8","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-Icosafluoro-11-(trifluoromethyl)dodecyl methacrylate","74256-14-7","D",0]
["Beta-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-) (1:1)","1329995-45-0","D",0]
["Pyridinium, 1-[2-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]ethyl]-, chloride (1:1)","308-01-0","D",0]
["Pyridinium, 1-[2-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]ethyl]-, bromide (1:1)","331755-02-3","D",0]
["Piperazinium, 1-(2-hydroxyethyl)-1-methyl-4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)-, chloride (1:1)","103555-98-2","D",0]
["1-Propanaminium, N-(carboxymethyl)-N,N-dimethyl-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, inner salt","90179-39-8","D",0]
["1-Propanaminium, N-(2-carboxyethyl)-N,N-dimethyl-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, inner salt","5158-52-1","D",0]
["1-Propanesulfonic acid, 2-[[3-[(3,3,4,4,5,5,6,6, 7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-1-oxopropyl]amino]-2-methyl-","755698-73-8","D",0]
["Butanedioic acid, 2-sulfo-, 1,4-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester, sodium salt (1:1)","54950-06-0","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, 1-(hydrogen sulfate), ammonium salt (1:1)","63225-58-1","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(hydrogen sulfate), ammonium salt (1:1)","63225-57-0","D",0]
["1-Decansulfonsäure, 3,3,4,4,5,5,6,6,7,7,8,8,9, 9,10,10,10-heptadecafluoro-, potassium salt (1:1)","438237-73-1","D",0]
["1-Dodecanesulfonic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","120226-60-0","D",0]
["1-Decanesulfonic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","39108-34-4","D",0]
["2-Propenamide, telomer with 3,3,4,4,5,5,6,6,7,7, 8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-1-dodecanethiol","121913-10-8","D",0]
["2-Propenamide, telomer with 3,3,4,4,5,5,6,6,7,7, 8,8,9,9,10,10,10-heptadecafluoro-1-decanethiol","76830-13-2","D",0]
["1-Propanaminium, 3-[[2-[(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl)thio]acetyl] amino]-N,N,N-trimethyl-","704870-51-9","D",0]
["Glycine, N-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)sulfonyl]-N-propyl-, lithium salt","441765-18-0","D",0]
["Ethanaminium, N-(2-carboxyethyl)-2-[[(3,3,4,4, 5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl) sulfonyl]amino]-N,N-dimethyl-, inner salt","34695-31-3","D",0]
["Ethanaminium, N-(2-carboxyethyl)-2-[[(3,3,4,4, 5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro decyl)sulfonyl]amino]-N,N-dimethyl-, inner salt","34695-29-9","D",0]
["1-Propanaminium, N-(carboxymethyl)-3-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)sulfonyl]amino]-N,N-dimethyl-, inner salt","34455-35-1","D",0]
["1-Propanaminium, N-(carboxymethyl)-3-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)sulfonyl]amino]-N,N-dimethyl-, inner salt","34455-21-5","D",0]
["1-Propanaminium, 3-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)sulfonyl]amino]-N,N,N-trimethyl-, 4-methylbenzenesulfonate (1:1)","438237-77-5","D",0]
["1-Dodecanesulfonamide, N-[3-(dimethylamino) propyl]-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11, 11,12,12,12-heneicosafluoro-","34455-24-8","D",0]
["1-Decanesulfonamide, N-[3-(dimethylamino) propyl]-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","34455-23-7","D",0]
["1-Decanesulfonamide, N-[3-(dimethyloxido amino)propyl]-3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluoro-","80475-33-8","D",0]
["Octanamide, N-[3-(dimethyloxidoamino)propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","30295-53-5","D",0]
["2-Propenoic acid, 4,4,5,5,6,6,7,7,8,8,9,9,10,10, 11,11,11-heptadecafluoro-2-hydroxyundecyl ester","76962-34-0","D",0]
["1-Undecanol, 2-chloro-4,4,5,5,6,6,7,7,8,8,9,9, 10,11,11,11-hexadecafluoro-10-(trifluoromethyl)-, hydrogen phosphate","63295-26-1","D",0]
["1-Nonadecanol, 12,12,13,13,14,14,15,15,16, 16,17,17, 18,18,19,19,19-heptadecafluoro-, dihydrogen phosphate","2343-53-5","D",0]
["Phosphoric acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluorodecyl bis(3,3,4,4,5,5,6,6, 7,7,8,8,8-tridecafluorooctyl) ester","1578186-53-4","D",0]
["1,2-Undecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,11, 11,11-hexadecafluoro-10-(trifluoromethyl)-, 1,1-(hydrogen phosphate)","63295-20-5","D",0]
["Acetic acid, 2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10, 10-heptadecafluorodecyl)thio]-, lithium salt (1:1)","441765-12-4","D",0]
["Glycine, N-[3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-2-hydroxypropyl]-N-methyl-","93128-66-6","D",0]
["Butanoic acid, 4-[[3-(dimethylamino)propyl] amino]-2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11, 11,12,12,12-heneicosa fluorododecyl)thio]-4-oxo-","1383438-90-1","D",0]
["Butanoic acid, 4-[[3-(dimethylamino)propyl] amino]-2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) thio]-4-oxo-","1383438-89-8","D",0]
["1-Propanaminium, N-(carboxymethyl)-3-[[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12, 12,12-heneicosafluorododecyl) thio]acetyl] amino]-N,N-dimethyl-, inner salt","1513863-97-2","D",0]
["1-Propanaminium, N-(carboxymethyl)-3-[[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]acetyl] amino]-N,N-dimethyl-, inner salt","1513863-96-1","D",0]
["1-Propanaminium, N-ethyl-3-[[3-[(3,3,4,4,5, 5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) thio]-2-methyl-1-oxopropyl]amino]-N,N-dimethyl-, ethyl sulfate (1:1)","67333-62-4","D",0]
["1-Propanaminium, 3-[[2-[(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,11,11,12,12,12-heneicosafluorodo decyl)thio]acetyl]amino]-N,N,N-trimethyl-","1513864-01-1","D",0]
["1,2-Propanediol, 3-[(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl)oxy]-","121500-31-0","D",0]
["3,6,9,12,15-Pentaoxapentacosan-1-ol, 18,18, 19,19,20,20,21,21,22,22,23,23,24,24,25,25,25-heptadecafluoropentamethyl-, acetate","88243-09-8","D",0]
["3,6,9,12,15,18,21,24-Octaoxatetratriacontan-1-ol, 27,27,28,28,29,29,30,30,31,31,32,32,33,33,34,34,34-heptadecafluorooctamethyl-","88243-17-8","D",0]
["beta-Alanine, N-(2-carboxyethyl)-N-[6-[[(3,3,4,4, 5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro decyl)sulfonyl]amino]hexyl]-, dipotassium salt","98900-53-9","D",0]
["2-Propenoic acid, polymer with 2-ethenylnaphthalene and 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl 2-propenoate","934505-67-6","D",0]
["1-Propanaminium, N,N,N-trimethyl-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, iodide (1:1)","335-90-0","D",0]
["Glycine, N-ethyl-N-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)-, ammonium salt","138473-79-7","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-(14-hydroxy-3,6,9,12-tetraoxatetradec-1-yl)-","89932-71-8","D",0]
["Ethanaminium, N,N,N-trimethyl-2-[(2,2,3,3,4,4, 5,5,6,6,7,7,7-pentadecafluoro-1-oxooctyl)amino]-, chloride (1:1)","178766-44-4","D",0]
["Octanamide, N-[3-(dimethylamino)propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","376-23-8","D",0]
["1-Pentanaminium, N,N,N-trimethyl-5-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, iodide (1:1)","91707-61-8","D",0]
["1-Propanesulfonic acid, 2-[[3-[(3,3,4,4,5,5,6,6,7, 7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro dodecyl)sulfinyl]-1-oxopropyl]amino]-2-methyl-","1513864-11-3","D",0]
["Docosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","93454-71-8","D",0]
["Eicosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","90499-29-9","D",0]
["Nonadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","125635-85-0","D",0]
["Octadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","93454-70-7","D",0]
["Heptadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10-heneicosafluoro-","200817-54-5","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","41997-13-1","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with pyrrolidine (1:1)","1187817-57-7","D",0]
["Sulfonium, bis(4-methylphenyl)phenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","341548-85-4","D",0]
["Potassium N-ethyl-N- [(tridecafluorohexyl)sulfonyl]-","","D",0]
["1-Butanaminium, N,N,N-tributyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid","108427-54-9","D",0]
["Phosphonium, triphenyl(phenylmethyl)-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","1000597-52-3","D",0]
["Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","213740-81-9","D",0]
["Perfluorohexane-1-sulphonic acid","355-46-4","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-methyl-","68259-15-4","D",0]
["1-Hexanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-(2-hydroxyethyl)-","34455-03-3","D",0]
["1-Hexanesulfinic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt (2:1)","86525-30-6","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with 2,2'-iminobis[ethanol] (1:1)","70225-16-0","D",0]
["Ethanaminium, N,N,N-triethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","108427-55-0","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd.with 2-methyl-2-propanamine (1:1)","202189-84-2","D",0]
["Methanaminium, N,N,N-trimethyl-, salt with1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)","189274-31-5","D",0]
["Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","153443-35-7","D",0]
["Quinolinium, 1-(carboxymethyl)-4-[2-[4-[4-(2,2-diphenylethenyl)phenyl]-1,2,3,3a,4,8b-hexahydrocyclopent[b]indol-7-yl]ethenyl]-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","1462414-59-0","D",0]
["Sulfonium, triphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","144116-10-9","D",0]
["Gamma-Cyclodextrin, compd. with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid ion(1-) (1:1)","1329995-69-8","D",0]
["Eicosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8, 13,13,14,14,15,15,16,16,17,17,18,18,19,19,20,20,20-tetratriacontafluoro-","133299-41-9","D",0]
["1-Propanesulfonic acid, 2-[[3-[(3,3,4,4,5,5,6,6,7, 7,8,8,9,9,10,10,10-heptadecafluorodecyl) sulfinyl]-1-oxopropyl]amino]-2-methyl-","1513864-12-4","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)sulfinyl]-","1513864-19-1","D",0]
["1-Propanesulfonic acid, 2-[[3-[(3,3,4,4,5,5,6,6,7, 7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro dodecyl)thio]-1-oxopropyl]amino]-2-methyl-, sodium salt (1:1)","62880-98-2","D",0]
["1-Propanesulfonic acid, 2-[[3-[(3,3,4,4,5,5,6,6, 7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-1-oxopropyl]amino]-2-methyl-, sodium salt (1:1)","62880-96-0","D",0]
["1-Propanesulfonic acid, 2-[[3-[(3,3,4,4,5,5,6,6, 7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro dodecyl)thio]-1-oxopropyl] amino]-2-methyl-","690947-60-5","D",0]
["1-Undecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-nonadecafluoro-","87017-97-8","D",0]
["Ammonium perfluorohexane-1-sulphonate","68259-08-5","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, gallium salt (9CI)","341035-71-0","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, scandium(3+) salt (3:1)","350836-93-0","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, neodymium(3+) salt (3:1)","41184-65-0","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, yttrium(3+) salt (3:1)","41242-12-0","D",0]
["Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","421555-73-9","D",0]
["Iodonium, bis[4-(1,1-dimethylpropyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","421555-74-0","D",0]
["Sulfonium, tris[4-(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic","425670-70-8","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, zinc salt","70136-72-0","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, compd. with N,N-diethylethanamine (1:1)","72033-41-1","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, sodium salt (1:1)","82382-12-5","D",0]
["Iodonium, bis[(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1) (9CI)","866621-50-3","D",0]
["Sulfonium, (4-methylphenyl)diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","910606-39-2","D",0]
["Sulfonium, [4-[(2-methyl-1-oxo-2-propen-1-yl)oxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","911027-68-4","D",0]
["Sulfonium, [4-[(2-methyl-1-oxo-2-propenyl)oxy]phenyl]diphenyl-, salt with 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonic acid (1:1)....","911027-69-5","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, cesium salt (1:1)","92011-17-1","D",0]
["Dibenzo[k,n][1,4,7,10,13]tetraoxathiacyclopentadecinium, 19-[4-(1,1-dimethylethyl)phenyl]-6,7,9,10,12,13-hexahydro-, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-1-hexanesulfonate (1:1)","928049-42-7","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, lithium salt (1:1)","55120-77-9","D",0]
["octadecyl acrylate","4813-57-4","D",0]
["1,1,2,2-Tetrahydroperfluorohexadecyl acrylate","34362-49-7","D",0]
["Perfluorooctyl phosphonic acid","40143-78-0","D",0]
["1,5-Trisiloxanediol, 3-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-1,1,3,5,5-pentamethyl- (9CI)","165320-75-2","D",0]
["Butanoic acid, 4,4,4-trifluoro-2,2,3,3-tetrakis(trifluoromethyl)-","1882109-62-7","D",0]
["Ethanaminium, N,N,N-triethyl-,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)","98241-25-9","D",0]
["Butanoic acid, 2,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-3-(trifluoromethyl)-","1882109-61-6","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, chromium(3+) salt (3:1)","68141-02-6","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-pentacosafluoro-12-iodo-","307-60-8","D",0]
["Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-tricosafluoro-11-iodo-","307-50-6","D",0]
["Heptadecafluoro-1-iodooctane","507-63-1","D",0]
["Octanoyl fluoride, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","335-66-0","D",0]
["Phosphinic acid, P-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-P-(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)-","610800-34-5","D",0]
["Phosphinic acid, P,P-bis(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-","40143-79-1","D",0]
["Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs., aluminum salts","93062-53-4","D",0]
["Phosphinic acid, bis(perfluoro-C6-12-alkyl) derivs.","68412-69-1","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, 1,1'-anhydride","33496-48-9","D",0]
["Ethyl perfluorooctanoate","3108-24-5","D",0]
["Methyl perfluorooctanoate","376-27-2","D",0]
["Fatty acids, C7-13, perfluoro, ammonium salts","72968-38-8","D",0]
["Fatty acids, C7-19, perfluoro","91032-01-8","D",0]
["Fatty acids, C7-13, perfluoro","68333-92-6","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, aluminum salt(3:1)","15715-47-6","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, chromium salt(1:x)","15739-82-9","D",0]
["1,1,2,2-Tetrahydroperfluorotetradecyl acrylate","34395-24-9","D",0]
["1-Propanaminium, 3-[[4-[(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl)oxy]-1,4-dioxo-2-buten-1-yl]amino]-N,N,N-trimethyl-, iodide (1:1)","121912-26-3","D",0]
["2-Dodecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11, 12,12,12-nonadecafluoro-1-[(1-methylpropyl) amino]-","94817-80-8","D",0]
["2-Undecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11, 11,11-nonadecafluoro-1-[(1-methylpropyl) amino]-","94817-79-5","D",0]
["1-Undecanaminium, 4,4,5,5,6,6,7,7,8,8,9,9,10,10, 11,11,11-heptadecafluoro-2-hydroxy-N,N-bis(2-hydroxyethyl)-N-methyl-, iodide (1:1)","93776-18-2","D",0]
["1-Decanaminium, N,N-diethyl-3,3,4,4,5,5, 6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-2-hydroxy-N-methyl-, iodide (1:1)","99679-40-0","D",0]
["Butanoic acid, 2,3,3,4,4,4-hexafluoro-2-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]-","1882109-60-5","D",0]
["Poly[[1,3-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl )-1,3:1,3-disiloxanediylidene]-1,3-","161045-59-6","D",0]
["Silicic acid (H4SiO4), disodium salt, reaction products with chlorotrimethylsilane and 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol","125476-71-3","D",0]
["Trisiloxane, 3,3'-(3,3,4,4,5,5,6,6,7,7,8,8-dodecafluoro-1,10-decanediyl)bis[3-[(dimethylsilyl)oxy]-1,1,5,5-tetramethyl-, reaction products with 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-1-undecene","185701-89-7","D",0]
["Siloxanes and Silicones, di-Me, mono[3-[(2-methyl-1-oxo-2-propenyl)oxy]propyl group]-terminated, polymers with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol- and 2-hydroxyethyl acrylate-blocked 2,4-TDI-trimethylolpropane polymer,..","501098-09-5","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, telomer with 1-dodecanethiol, 2-ethylhexyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate and","321318-71-2","D",0]
["2-Propenoic acid, C16-18-alkyl esters, polymers with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl acrylate","160336-09-4","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl)-.omega.-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl)oxy]-","122402-79-3","D",0]
["Perfluoro compounds, C5-18","86508-42-1","D",0]
["Cyclotetrasiloxane, 2-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)-2,4,6,8-tetramethyl-, Si-[3-(oxiranylmethoxy)propyl] derivs.","206886-57-9","D",0]
["Poly(difluoromethylene), alpha-fluoro-omega-[2-sulphoethyl)-","80010-37-3","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-(phosphonooxy)ethyl)-","65530-61-2","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.¿-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-","65530-62-3","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-[[2-(trimethylammonio)ethyl]thio]ethyl]-, methyl sulfate","65530-57-6","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-[2-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]ethyl]-omega-hydroxy-","93480-00-3","D",0]
["Octanoic acid, pentadecafluoro-, mixed esters with 2,2'-[1,4-butanediylbis(oxymethylen)]bis[oxirane] and 2,2'-[1,6-hexanediylbis(oxymethylen)]bis[oxirane]","90480-57-2","D",0]
["Fatty acids, C6-18, perfluoro, ammonium salts","72623-77-9","D",0]
["Fatty acids, C7-13, perfluoro, compds. with ethylamine","69278-80-4","D",0]
["1,1,2,2-Tetrahydroperfluorooctadecyl acrylate","65150-93-8","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)- , sodium salt(1:1)","18017-22-6","D",0]
["tetradecafluorohexane","355-42-0","D",0]
["1,1,1,2,2,3,3,4,4,5,6,6,6-Tridecafluoro-5-iodohexane","355-44-2","D",0]
["perfluorohexadecane","355-49-7","D",0]
["Perfluorohexadecyl iodide","355-50-0","D",0]
["(Perfluoroethyl)methyl iodide","354-69-8","D",0]
["N,N-Bis(2-hydroxyethyl)perfluorobutanesulfonamide","34455-00-0","D",0]
["8:3 Fluorotelomer carboxylic acid","34598-33-9","D",0]
["4'-[2-(2,4-Di-tert-pentylphenoxy)butyramido]perfluoro-2'-hydroxybutyranilide","346-10-1","D",0]
["Perfluorobutane-1-sulfinic acid","34642-43-8","D",0]
["Europium tri[3-(heptafluoropropylhydroxymethylene)]-(+)-camphorate","34788-82-4","D",0]
["3-Cyclohexene-1-carboxylic acid, 6-[(di-2-propenylamino)carbonyl]-,(1R,6R)-rel-, reaction products with pentafluoroiodoethane-tetrafluoroethylene telomer","348137-34-8","D",0]
["3,3,4,4,5,5,6,6,6-nonafluorohexyl nitrate","34839-44-6","D",0]
["1,1,1-Trifluoro-2-(trifluoromethyl)pentane-2,4-diol","34844-48-9","D",0]
["Methanol, reaction products fluorinated 2,2,3,3-tetrafluorooxetane homopolymer-iodine reaction products-trichloroethenylsilane polymer","349660-50-0","D",0]
["(1,1,2,2-tetrafluoroethoxy)benzene","350-57-2","D",0]
["2-Propenoic acid, polymer with butyl-2-propenoate, 2-propenoic acid, 2-hydroxyethyl ester and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl-2-propenoate","350672-19-4","D",0]
["2-Propenoic acid, polymer with butyl-2-propenoate, 2-hydroxyethyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl-2-propenoate, compd. with 2-(dimethylamino)ethanol","350672-20-7","D",0]
["Acetic acid, trifluoro-, trianhydride with boric acid (H3BO3)","350-70-9","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)-benzaldehyde","35295-35-3","D",0]
["4-(1,1,2,2-Tetrafluoroethoxy)-benzaldehyde","35295-36-4","D",0]
["perfluorodecene","35328-43-9","D",0]
["Propane, 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]-, polymer with chlorotrifluoroethene and ethene","35397-13-8","D",0]
["Pentafluoroethane","354-33-6","D",0]
["1-chloro-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexane","355-41-9","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, potassium salt(1:1)","29457-73-6","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, iron salt (1:x)","61436-04-2","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-, ammoniumsalt (1:1)","19742-57-5","D",0]
["Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-, sodium salt (1:1)","1195164-59-0","D",0]
["Hexanoic acid, 2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2- pentafluoroethyl)-, ammonium salt(1:1)","13058-06-5","D",0]
["Perfluoromethylcyclohexane","355-02-2","D",0]
["Hexane, 1,6-diisocyanato-, homopolymer, 1,1,2,2,3,3,4,4,4,-nonafluoro-N-(2-hydroxyethyl)-N-methyl-1-butanesulfonamide- and stearyl alcohol-blocked","355009-66-4","D",0]
["Perfluoro-2-methyl-3-ethylpentane","354-97-2","D",0]
["undecafluorocyclohexanesulphonyl fluoride","355-03-3","D",0]
["Perfluoroisohexane","355-04-4","D",0]
["3,3,4,4,5,5,5-Heptafluoropent-1-ene","355-08-8","D",0]
["Perfluoro-2,3-dimethylbutane","354-96-1","D",0]
["Perflisobutane","354-92-7","D",0]
["Perfluoroethanesulfonic acid","354-88-1","D",0]
["Pentafluoro ethanesulfonyl fluoride","354-87-0","D",0]
["Trichloro(1,1,2,2-tetrafluoroethyl)silane","354-83-6","D",0]
["Pentafluoropropionamide","354-76-7","D",0]
["3,3,4,4,5,5,5-heptafluoropentan-2-one","355-17-9","D",0]
["2,3-Dichlorooctafluorobutane","355-20-4","D",0]
["1,4-Dichloro-1,1,2,2,3,3,4,4-octafluorobutane","355-24-8","D",0]
["Butane, decafluoro-","355-25-9","D",0]
["1H,1H-Perfluoro-1-pentanol","355-28-2","D",0]
["1H-Perfluorohexane","355-37-3","D",0]
["Perfluorohexanoyl fluoride","355-38-4","D",0]
["Pyridinium, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-,iodide (1:1)","25935-14-2","D",0]
["Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15-hentriacontafluoro-15-iodo","335-79-5","D",0]
["Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-heptacosafluoro-13-iodo-","376-04-5","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-10-iodo-","423-62-1","D",0]
["Nonane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-nonadecafluoro-9-iodo-","558-97-4","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, 1-(dihydrogen phosphat)","57678-05-4","D",0]
["Alkyl iodides, C10-12, gamma-omega-perfluoro","68390-33-0","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, polymer with 2-propenoic acid","53515-73-4","D",0]
["2-Propenoic acid, 2-methyl-,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecylester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-methyl-2-propenoate, methyl 2-methyl-2-¿","65104-45-2","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, homopolymer","74049-08-4","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, alpha-¿","116984-14-6","D",0]
["2-Propenoic acid, dodecyl ester, polymers with Bu (1-oxo-2-propenyl)carbamate und gamma-omega-perfluoro-C8-14-alkyl acrylate","144031-01-6","D",0]
["2-Propenoic acid, 2-methyl-, C10-16-alkyl esters, polymers with 2-hydroxyethyl methacrylate, Me methacrylate und gamma-omega-perfluoro-C8-14-alkylacrylate","129783-45-5","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, ¿","115592-83-1","D",0]
["2-Pentadecanol, 1,1'-[oxybis[(1-methyl-2,1-ethanediyl)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro- (9CI)","93776-00-2","D",0]
["1,2-andecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-,1-(dihydrogen phosphat), ammonium salt (1:2)","94200-45-0","D",0]
["Pentanoic acid, 4,4-bis[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs., compds.with diethanolamine","71608-61-2","D",0]
["Oxirane, 2-methyl-, polymer with oxirane, mono[2-hydroxy-3-[(gamma-omega-perfluoro-C8-20-alkyl)thio]propyl] ethers","183146-60-3","D",0]
["1,3-Propanediol, 2,2-bis[[(gamma-omega-perfluoro-C10-20-alkyl)thio]methyl] derivs.,phosphats, ammonium salts","148240-89-5","D",0]
["1,3-Propanediol, 2,2-bis[[(gamma-omega-perfluoro-C6-12-alkyl)thio]methyl] derivs.,phosphats, ammonium salts","148240-87-3","D",0]
["1,3-Propanediol, 2,2-bis[[(gamma-omega-perfluoro-C4-10-alkyl)thio]methyl] derivs.,phosphats, ammonium salts","148240-85-1","D",0]
["Carbamic acid, [2-(sulfothio)ethyl]-, C-(gamma-omega-perfluoro-C6-9-alkyl) esters,monosodium salts","95370-51-7","D",0]
["Thiols, C8-20, gamma-omega-perfluoro, telomers with acrylamide","70969-47-0","D",0]
["Propanamide, 3-[(gamma-omega-perfluoro-C4-10-alkyl)thio] derivs.","68187-42-8","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)trimethoxy-","83048-65-1","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-14-iodo-","307-63-1","D",0]
["Perfluorooctanoate","45285-51-6","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","335-67-1","D",0]
["Silane, triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","101947-16-4","D",0]
["Silane, chloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)dimethyl-","74612-30-9","D",0]
["Silane, dichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)methyl-","3102-79-2","D",0]
["Amides, C7-19, alpha-omega-perfluoro-N,N-bis(hydroxyethyl)","90622-99-4","D",0]
["Alkyl iodides, C4-20, gamma-omega-perfluoro","68188-12-5","D",0]
["Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-nonadecafluoro-11-iodo-","65510-56-7","D",0]
["Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-nonacosafluoro-16-iodo-","65510-55-6","D",0]
["Tetradecane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12- pentacosafluoro-14-iodo-","30046-31-2","D",0]
["Dodecane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-12-iodo-","2043-54-1","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","2043-53-0","D",0]
["Alkyl iodides, C6-18, perfluoro","90622-71-2","D",0]
["Decane, 1-bromo-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heneicosafluoro-","307-43-7","D",0]
["Tetradecane, 1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-octacosafluoro-14-iodo-2-(trifluoromethyl)-","3248-63-3","D",0]
["Dodecane, 1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12, 12-tetracosafluoro-12-iodo-2-(trifluoromethyl)-","3248-61-1","D",0]
["Decane, 1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-eicosafluoro-10-iodo-2-(trifluoromethyl)-","677-93-0","D",0]
["2-Propenoic acid, 2-methyl-,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl ester","6014-75-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl acrylate","16083-87-7","D",0]
["2-Propenoic acid,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl ester","52956-82-8","D",0]
["2-Propenoic acid, 2-methyl-,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecylester","4980-53-4","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-2-hydroxy-16-(trifluoromethyl)heptadecyl acrylate","16083-78-6","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, 1,1'-(hydrogen phosphat)","1895-26-7","D",0]
["2-Dodecenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-","70887-94-4","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","678-39-7","D",0]
["Hexanoic acid, 3,3,4,4,5,5,6,6,6-nonafluoro-2,2-bis(trifluoromethyl)-","1812247-17-8","D",0]
["Hexanoic acid, 2,3,3,4,5,5,6,6,6-nonafluoro-2,4-bis(trifluoromethyl)-","1812247-19-0","D",0]
["Hexanoic acid, 2,2,4,4,5,5,6,6,6-nonafluoro-3,3-bis(trifluoromethyl)-","1812247-20-3","D",0]
["Butanoic acid, 3,3,4,4,4-pentafluoro-2,2-bis(1,1,2,2,2-pentafluoroethyl)-","1882109-58-1","D",0]
["Butanoic acid, 3,3,4,4,4-pentafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-2-(trifluoromethyl)-","1882109-59-2","D",0]
["Oxirane, 2-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]methyl]-","114482-33-6","D",0]
["Ethanesulfonic acid, 2-[ethyl(2,2,3,3,4,4,5,5,6,6, 7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, potassium salt (1:1)","57670-46-9","D",0]
["1-Propanesulfonic acid, 3-[(3-aminopropyl) (2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-2-hydroxy-, sodium salt (1:1)","98900-76-6","D",0]
["Benzenesulfonic acid, 4-[[[3-(methylamino) propyl](2,2,3,3,4,4 ,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]methyl]-, sodium salt (1:1)","98900-75-5","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-[3-(trimethoxysilyl)propyl]-","98046-76-5","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-[dimethoxy[3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]propyl]silyl]-omega-[[dimethoxy[3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]propyl]silyl]oxy]-","154380-30-0","D",0]
["11,14,17,20,23,26,29,32-Octaoxaoctatetracontan-33-one, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","67549-47-7","D",0]
["1H,1H,2H,2H-Perfluorodecane-1-thiol","34143-74-3","D",0]
["1-Tridecanaminium, 2-(acetyloxy)-N-(carboxy methyl)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12, 12,13,13,13-heneicosafluoro-N,N-dimethyl-, inner salt","80244-66-2","D",0]
["1-Undecanaminium, 2-(acetyloxy)-N-(carboxy methyl)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-N,N-dimethyl-, inner salt","80234-03-3","D",0]
["1-Dodecanaminium, N-(carboxymethyl)-5,5,6,6, 7,7,8,8,9,9,10,10,11,11,12,12,12-heptadeca fluoro-N,N-dimethyl-","2089109-30-6","D",0]
["1-Dodecanaminium, N-(carboxymethyl)-3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-N,N-dimethyl-, inner salt","171184-04-6","D",0]
["1-Tetradecanaminium, N-(carboxymethyl)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-tricosafluoro-N,N-dimethyl-, inner salt","171184-17-1","D",0]
["1-Dodecanaminium, N-(carboxymethyl)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-nonadecafluoro-N,N-dimethyl-, inner salt","171184-16-0","D",0]
["1-Decanaminium, N-(carboxymethyl)-3,3,4,4,5,5, 6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-N,N-dimethyl-, inner salt","145441-32-3","D",0]
["1-Dodecanaminium, N-(carboxymethyl)-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-N,N-dimethyl-","2089109-27-1","D",0]
["1-Decanaminium, N-(carboxymethyl)-3,3,4,4,5,5, 6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-N,N-dimethyl-","2089109-26-0","D",0]
["Ethanaminium, N-ethyl-2-[[[[3-[[[3-[[[3-[[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadeca fluorodecyl)oxy]carbonyl]amino]methylphenyl] carbonimidoyl]amino]methylphenyl]carbonimidoyl]amino]methylphenyl]amino]carbonyl]oxy]-N,N-dimethyl-, ethyl ¿","100107-48-0","D",0]
["Ethanaminium, N-ethyl-2-[[[[3-[[[[3-[[[[3-[[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadeca fluorodecyl)oxy]carbonyl]amino]methylphenyl] amino]carbonyl]amino]methylphenyl]amino]carbonyl]amino]methylphenyl]amino]carbonyl]oxy]-N,N-dimethyl-, ethyl ¿","100155-23-5","D",0]
["Hexanoic acid, 2,2,3,3,5,5,6,6,6-nonafluoro-4,4-bis(trifluoromethyl)-","1192593-79-5","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","865-86-1","D",0]
["1-Tetradecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-","39239-77-5","D",0]
["1-Hexadecanol,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluoro-","60699-51-6","D",0]
["1-Dodecene,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","30389-25-4","D",0]
["1-Decene, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","21652-58-4","D",0]
["Pentanoic acid, 3,4,4,5,5,5-hexafluoro-2,2,3-(trifluoromethyl)-","1882109-69-4","D",0]
["Oxirane, 2-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl)-","38565-53-6","D",0]
["Tridecanoic acid, 27,27,28,28,29,29,30,30,31,31, 32,32,33,33,34,34,34-heptadecafluoro-3,6,9,12, 15,18,21,24-octaoxatetra triacont-1-yl ester","67535-33-5","D",0]
["Palladium, dichlorobis[tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phosphine-betaP]-","326475-46-1","D",0]
["Silver(1+) Perfluorooctanoate","335-93-3","D",0]
["Potassium Perfluorooctanoate","2395-00-8","D",0]
["Octanoic acid, pentadecafluoro-, sodium salt","335-95-5","D",0]
["ammonium pentadecafluorooctanoate","3825-26-1","D",0]
["Octanoic acid, pentadecafluoro-, branched, ammonium salt","90480-56-1","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)-","15166-06-0","D",0]
["2,3,3,4,4,5,5,6,6,6-decafluoro-2-(1,1,2,2,2-pentafluoroethyl)-hexanoic acid","35605-76-6","D",0]
["Isooctanoic acid, pentadecafluoro-","123116-17-6","D",0]
["2,3,3,4,4,5,5,6,6,7,7,7-dodecafluoro-2-(trifluoromethyl)-heptanoic acid","207678-51-1","D",0]
["2,2,3,4,4,5,5,6,6,7,7,7-dodecafluoro-3-(trifluoromethyl)-heptanoic acid","705240-04-6","D",0]
["2,2,3,3,4,4,5,6,6,7,7,7–dodecafluoro-5-(trifluoromethyl)-heptanoic acid","909009-42-3","D",0]
["2,2,3,3,4,5,5,6,6,7,7,7-dodecafluoro-4-(trifluoromethyl)-heptanoic acid","1144512-18-4","D",0]
["Hexanoic acid, 2,2,3,3,4,4,6,6,6-nonafluoro-5,5-bis(trifluoromethyl)-","1144512-34-4","D",0]
["Hexanoic acid, 2,2,3,4,4,5,6,6,6-nonafluoro-3,5-bis(trifluoromethyl)-","1144512-35-5","D",0]
["Hexanoic acid, 2,2,3,3,4,5,6,6,6-nonafluoro-4,5-bis(trifluoromethyl)-","1144512-36-6","D",0]
["1,2-Bis(perfluorobutyl)ethene","84551-43-9","D",0]
["Perfluoro-6-carboxyl-5-oxaheptanesulfonic acid","852157-01-8","D",0]
["12-H-Perfluorododecanoate","1696259-75-2","D",0]
["2,2,3-Trifluoro-3-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]propanoate","2127366-90-7","D",0]
["Docosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,20,20-hentetracontafluoro-22-iodo-","263756-45-2","D",0]
["2-Amino-1-[3,4,5-tris(1,1,2,2-tetrafluoroethoxy)phenyl]ethan-1-ol--hydrogen chloride (1/1)","70126-67-9","D",0]
["octafluorobutane-1,4-disulfonamide","87988-73-6","D",0]
["2-chloro-3,4,4,4-tetrafluoro-3-(trifluoromethyl)but-1-ene","235106-10-2","D",0]
["1,1,1,2-Tetrafluoro-2,2-dimethoxyethane","595543-28-5","D",0]
["2,3-Difluoro-2-(heptafluoropropyl)-3-(trifluoromethyl)oxirane","71917-16-3","D",0]
["1,3-bis(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)urea","1543-55-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,33,33,34,34,35,35,36,36,37,37,38,38,39,39,40,40,41,41,42,42,43,43,44,44,44-Pentacontafluorotetratetracontane","114221-78-2","D",0]
["6-Methoxyquinolin-4-yl nonafluorobutane-1-sulfonate","1161941-02-1","D",0]
["1-Methylethyl 2-chloro-4-fluoro-5-(2-methoxy-6-oxo-4-(pentafluoroethyl)-1(6H)-pyrimidinyl)benzoate","115784-92-4","D",0]
["5-(4-tert-Butylphenyl)-N-(2,2,3,3,4,4,4-heptafluorobutyl)-1,2-oxazole-3-carboxamide","922421-40-7","D",0]
["Perfluoro(dimethyldecalin)","54471-59-9","D",0]
["2-(Tridecafluorohexyl)-5,6-dihydro-2H-pyran-2-ol","1401315-55-6","D",0]
["1,2-bis(2-Octyldodecyl) 3-((perfluoropentyl)ethyl) 2-hydroxy-1,2,3-propanetricarboxylate","214334-16-4","D",0]
["Ethyl 3-methyl-5-(nonafluorobutyl)-1H-pyrazole-4-carboxylate","119403-58-6","D",0]
["[(1Z)-1,2-Difluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)ethenyl]benzene","854992-57-7","D",0]
["Perfluoro-2-ethoxypropanoic acid","267239-61-2","D",0]
["3-(Trimethoxysilyl)propyl pentadecafluorooctanoate","98046-77-6","D",0]
["1,1-Dichloro-2,2,3,3,4,4,5,5-octafluoro-1-(propylsulfanyl)pentane","141700-49-4","D",0]
["2-[(2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl)oxy]ethan-1-ol","169289-67-2","D",0]
["Methyl 3-(perfluorohexyl)propanoate","110260-75-8","D",0]
["5,5,5-Trifluoro-3-hydroxy-4-(trifluoromethyl)pentanoic acid","63979-48-6","D",0]
["Iron(6+) cyclopenta-1,3-diene-1,2,3,4,5-pentaide 4,4-dimethyl-5,5-bis(trifluoromethyl)oxolan-3-ide--carbon monooxide (1/1/1/2)","54657-46-4","D",0]
["N-(Carboxymethyl)-3-[[2-[(perfluorotetradecyl)ethylthio]acetyl]amino]-N,N-dimethyl-1-propanaminium","1513863-99-4","D",0]
["4:4 Fluorotelomer alcohol","3792-02-7","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, lithium salt (1:1)","131651-65-5","D",0]
["(3β,5α)-Cholestan-3-ol 2,3,3,4,4,5,5,6,6,7,7,8,8,8-tetradecafluorooctanoate","123613-18-3","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-[(1,1,2-trifluoro-2-propenyl)oxy]-","174082-80-5","D",0]
["Copolymer of octadecyl acrylate, 2,4,6-tris(allyloxy)triazine, 2-(3,5-dimethylpyrazole-1-carboxamido)ethyl methacrylate, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate","1620402-95-0","D",0]
["Chloro(3,3,4,4,5,5,5-heptafluoropentyl)propyl(3,3,3-trifluoropropyl)silane","608296-40-8","D",0]
["2-hydroxy-4-(2,2,3,3,3-pentafluoropropoxy)benzoic Acid","651331-92-9","D",0]
["5-Methyl-5-(2,2,3,3-tetrafluoropropoxy)hex-1-en-3-yne","72063-49-1","D",0]
["3-(Heptafluoropropyl)-1,2,4-oxadiazol-5(2H)-one","4314-49-2","D",0]
["4,4,4-Trifluoro-3-(trifluoromethyl)-3',4',5'-trimethoxycrotonophenone","35443-96-0","D",0]
["Perfluorobutyl acetate","209597-28-4","D",0]
["Butanamide, 2,2,3,3,4,4,4-heptafluoro-N-(phenylmethyl)-","560-02-1","D",0]
["1,1,2-Trifluoro-1-(trifluoromethoxy)ethane","84011-00-7","D",0]
["4-[(6-Methoxy-3-pyridazinyl)sulfamoyl]anilinium heptadecafluorononanoate","298703-33-0","D",0]
["N-(3,3,4,4,5,5,5-Heptafluoropent-1-en-2-yl)cyclohexanamine","921193-83-1","D",0]
["Perfluorobutanoate","45048-62-2","D",0]
["2,5-bis(heptafluoropropyl)-1,3,4-oxadiazole","647-79-0","D",0]
["3,3,3-Trifluoro-N-(4-nitrophenyl)-2-(trifluoromethyl)propanamide","294651-51-7","D",0]
["3-[(Perfluoro-1-oxoundecyl)amino]-N,N-dimethyl-N-[2-(1-methylethoxy)-2-oxoethyl]-1-propanaminium","1513863-86-9","D",0]
["2,5-Pyrrolediethanol, 1-methyl-alpha,alpha,alpha',alpha'-tetrakis(trifluoromethyl)-","102367-00-0","D",0]
["5,5,6,6,7,7,7-Heptafluoro-3-iodoheptan-1-ol","89621-93-2","D",0]
["5-Chloro-1,1,1-trifluoro-2-(trifluoromethyl)pentane-2,4-diol","101931-56-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorodecane","154478-86-1","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-1-(piperidin-1-yl)propan-1-one","176702-75-3","D",0]
["(7.alpha.,17β)-3-methoxy-7-[9-[(4,4,5,5,5-pentafluoropentyl)sulfinyl]nonyl]estra-1,3,5(10)-trien-17-ol","1221256-46-7","D",0]
["5-Methoxy-3,3-bis(trifluoromethyl)-1,2-dithiolane","62378-48-7","D",0]
["(1,2,2,2-Tetrafluoroethyl)benzene","56424-23-8","D",0]
["3-[(12,12,13,13,14,14,15,15,16,16,17,17,17-Tridecafluoroheptadecanoyl)oxy]-4-(trimethylazaniumyl)butanoate","142674-38-2","D",0]
["2-Butyl-2,3,3,4,4,5,5-heptafluorooxolane","76298-23-2","D",0]
["2-Propenoic acid, 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl ester, homopolymer","26246-67-3","D",0]
["3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butan-2-one","80553-01-1","D",0]
["2-bromo-2,3,3,3-tetrafluoropropanoyl chloride","6066-45-1","D",0]
["1,1,1,5,5,5-Hexafluoro-2,4-bis(trifluoromethyl)-2,3-pentadiene","13222-45-2","D",0]
["3-[(Carboxymethyl)sulfanyl]-4,4,5,5,6,6,6-heptafluorohexanoic acid","424-55-5","D",0]
["2,2,3,3,5,6-Hexafluoro-2,3-dihydro-1,4-dioxine","56625-38-8","D",0]
["3‐[Diethyl(3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10‐hexadecafluorodec‐2‐en‐1‐yl)azaniumyl]‐2,2‐dimethylpropyl phosphonate","67304-22-7","D",0]
["1-[[[[4-(2-(Perfluorobutyl)-1-ethyl)phenyl]methoxy]carbonyl]oxy]-2,5-pyrrolidinedione","825635-46-9","D",0]
["N-Ethyl-N-[2-[[2-[[2-[(3,4,5,6-tetrahydro-4,6-dioxo-1,3,5-triazin-2-yl)amino]ethyl]amino]ethyl]amino]ethyl]perfluorooctanesulfonamide","38006-65-4","D",0]
["2-[[1,1,1,3,3,3-hexafluoro-2-[3-(trifluoromethyl)phenyl]propan-2-yl]oxymethyl]oxirane","25056-12-6","D",0]
["4-[1,1,2,2-tetrafluoro-2-(4-hydroxyphenyl)ethyl]phenol","433719-69-8","D",0]
["2,3,4,5,7,7,8,8-Octafluorobicyclo[4.2.0]octa-1,3,5-triene","52196-63-1","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluorohexyl)sulfonyl]amino)-1-propanesulfonate","112972-61-9","D",0]
["8:2 Fluorotelomer sulfonamido N-monomethyl amine","90851-71-1","D",0]
["N-[3-(Dimethylamino)propyl]-N-[(heptadecafluorooctyl)sulfonyl]-beta-alanine","1432486-92-4","D",0]
["1,1,1,2,2,3,3-Heptafluoroundecane","1190430-20-6","D",0]
["(Perfluorobutyl) sulfonamido acetic acid","347872-22-4","D",0]
["6:2 Fluorotelomer sulfinyl amido sulfonic acid","1513864-10-2","D",0]
["Bis[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy](oxo)phosphanium","79339-01-8","D",0]
["2,4-dibromo-3,3,4,4-tetrafluorobut-1-ene","161958-58-3","D",0]
["N-Cyclooctyl-1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonamide","1456900-48-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-octylnonanamide","33496-55-8","D",0]
["1-bromo-3,3,4,4,4-pentafluorobutan-2-one","92737-01-4","D",0]
["1-[4-(1,1,2,2-Tetrafluoroethoxy)phenyl]piperazine","823197-44-0","D",0]
["Perfluoroundecanesulfonate","441296-91-9","D",0]
["1,1,1,2,3,3-Hexafluoro-2,3-bis(trifluoromethoxy)propane","95842-02-7","D",0]
["bis(Perfluoroethyl)sulfone","14930-22-4","D",0]
["Perfluoroheptanamide","2358-22-7","D",0]
["1,2,3,4,5-Pentafluoro-6-(pentafluoroethoxy)benzene","159752-92-8","D",0]
["3-Chloro-3,4,4,4-tetrafluoro-2-methylbutan-2-ol","94083-43-9","D",0]
["1,2,2,3,3,5,5,6,6,7,7-Undecafluorobicyclo[2.2.1]heptane","4934-61-6","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)phenol","129560-95-8","D",0]
["2,2,4,4,5,5,6,6,7,7,9,9-Dodecafluorodecane-1,10-diol","90177-97-2","D",0]
["Methyl 4,4,5,5,6,6,6-heptafluorohexanoate","2070-60-2","D",0]
["Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-, reaction products with chromium chloride hydroxide (CrCl2(OH)) (1:2)","70892-42-1","D",0]
["1H-1,2,4-Triazole, 3-(heptadecafluorooctyl)-5-methyl-","667873-26-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Octadecafluoro-2,3,4,5,6,7,8,9-octahydro-1H-trindene","33021-47-5","D",0]
["1,2-bis[di(propan-2-yloxy)phosphoryl]-3,3,4,4,5,5-hexafluorocyclopentene","41161-76-6","D",0]
["2-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)pyridine-4-carbonitrile","929211-36-9","D",0]
["Ethane, 1-bromo-2-chloro-1,1,2,2-tetrafluoro-","354-53-0","D",0]
["4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]-N-(prop-2-en-1-yl)benzamide","143906-91-6","D",0]
["3-[(Triethylsilyl)oxy]-4,4-bis(trifluoromethyl)cyclobut-2-en-1-one","89101-64-4","D",0]
["Sodium 4,8-dioxa-3H-perfluorononanoate","2250081-67-3","D",0]
["1-(Perfluoroethyl)decane","69125-77-5","D",0]
["Ammonium perfluorotridecanoate","4288-72-6","D",0]
["2-(2-Bromo-1,1,2,2-tetrafluoroethyl)bicyclo[2.2.1]heptane","627528-39-6","D",0]
["Methoxydipropyl(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)silane","608299-82-7","D",0]
["Methyl 4-[(heptafluoropropyl)sulfanyl]benzoate","85260-50-0","D",0]
["1,1,2,2-tetrafluoro-6,6-dimethylheptane-3,5-dione","59857-66-8","D",0]
["2,3,3,4,4,4-Hexafluorobut-1-ene-1,1-dithiol","919515-73-4","D",0]
["1-Bromo-2,3,3,3-tetrafluoropropene","666-32-0","D",0]
["Perfluoro-1-butanesulfinic acid ammonium","187480-45-1","D",0]
["2,2,3,3,4,4,4-heptafluoro-1,1-diphenylbutan-1-ol","559-54-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorotriacontane","766529-12-8","D",0]
["3-[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy]prop-1-ene","150771-44-1","D",0]
["1,1,1,2,2-Pentafluoro-2-[(pentafluoroethyl)selanyl]ethane","6123-61-1","D",0]
["Lithium 3-[ethyl[(perfluorobutyl)sulfonyl]amino]propanesulfonate","864069-41-0","D",0]
["{2-[Ethyl(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)amino]ethyl}phosphonic acid","57670-47-0","D",0]
["N,N-Diethyl-3,4,4,5,5,6,6,7,7,8,8,8-dodecafluorooct-2-en-1-amine","67490-96-4","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-N-methylnonan-1-amine","228569-93-5","D",0]
["Dichlorophenyl(3-(1,1,2,2-tetrafluoroethoxy)propyl)silane","731-21-5","D",0]
["1-(2,2,2-Trifluoroethoxy)nonafluorocyclohexene","2356-01-6","D",0]
["2-Decanol, 1-[bis(2-hydroxyethyl)amino]-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","53269-76-4","D",0]
["1,1,2,2-Tetrafluoro-3-(pentafluoroethyl)cyclobutane","67230-15-3","D",0]
["2,3,3,5,5,6,6,8,8,10,10,12,12,14,14,14-Hexadecafluoro-4,7,9,11,13-pentaoxatetradecanoic acid","919005-23-5","D",0]
["N,N-Dibutyl-N-methylbutan-1-aminium nonafluorobutane-1-sulfonate","124472-66-8","D",0]
["5,10,15,20-Tetrakis{2,3,5,6-tetrafluoro-4-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-henicosafluorododecyl)sulfanyl]phenyl}porphyrin","956790-67-3","D",0]
["Phenol, 2-amino-4-(heptafluoropropyl)-","61324-30-9","D",0]
["Fluoro[perfluoro-2-(perfluoro-2-sulfoethoxy)propoxy]acetic acid","2416366-19-1","D",0]
["N-[(5-bromo-2-propan-2-yloxyphenyl)methylideneamino]-2,2,3,3,4,4,4-heptafluorobutanamide","6162-95-4","D",0]
["N~1~,N~1~,N~2~-Trimethyl-N~2~-(2,2,3,3-tetrafluoropropyl)ethane-1,2-diamine","114309-91-0","D",0]
["1-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-trimethylmethanaminium benzenesulfonate (1:1)","167162-25-6","D",0]
["Heptane, 6,7-dichloro-1,1,2,2,3,3,4,4,5,5,6-undecafluoro-","538345-75-4","D",0]
["Methoxy(3,3,4,4,5,5,6,6,6-nonafluorohexyl)propyl(3,3,3-trifluoropropyl)silane","608300-17-0","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoro-2-hydroxyheptyl 2-methylprop-2-enoate","36915-03-4","D",0]
["1,2,3,4-Tetrafluoro-5-(1,1,1,2,4,4,5,5,5-nonafluoropent-2-en-3-yl)-6-(trifluoromethyl)benzene","129246-68-0","D",0]
["1,1,1,2,2,3,3,4,5,6,6,7,7,8,8,8-Hexadecafluorooct-4-ene","35844-81-6","D",0]
["1',2,2',2',3,3,3',3',4,4,4',4'-Dodecafluoro[1,1'-bi(cyclobutan)]-1-ene","68252-06-2","D",0]
["N,N'-1,4-Phenylenebis(perfluorobutanamide)","524726-49-6","D",0]
["2,2,3,3-Tetrafluoropropyl 4-(2H-tetrazol-5-yl)benzoate","651769-26-5","D",0]
["1-Iodo-4-(1,1,2,2-tetrafluoroethoxy)benzene","863323-03-9","D",0]
["3,3,4,4,5,5,5-Heptafluoropentan-2-amine","1446355-42-5","D",0]
["3-(4-Chlorophenyl)-6-(heptafluoropropyl)-1,4-dihydro-1,2,4,5-tetrazine","59872-89-8","D",0]
["2-Bromo-3,3,4,4,5,5,6,6,6-nonafluorohexan-1-ol","89807-84-1","D",0]
["1,1,1,2,5,6,6,6-Octafluoro-2,5-bis(trifluoromethyl)hex-3-ene","88562-40-7","D",0]
["Tris(1,1,1,3,3,3-hexafluoropropan-2-yl) phosphite","66470-81-3","D",0]
["N-(29-Hydroxy-3,6,9,12,15,18,21,24,27-nonaoxanonacos-1-yl)perfluorononanamide","83952-10-7","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)-2-[(trimethylsilyl)oxy]propanenitrile","41309-98-2","D",0]
["Ethyl perfluorodecanoate","33304-55-1","D",0]
["1-Methoxy-3-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-44-4","D",0]
["Propan-2-yl nonadecafluorodecanoate","71356-37-1","D",0]
["1,2,2,3,3,4,4,4a,5,5,6,6,7,7,8,8,8a-Heptadecafluorodecahydronaphthalene-1-carboxylic acid","172155-05-4","D",0]
["3-Ethoxy-3-pentyl-5,5-bis(trifluoromethyl)-1,2-dithiolane","62378-57-8","D",0]
["Trimethyl(1,1,2,2,3,3,4,4-octafluorobutyl)silane","62281-31-6","D",0]
["(1r,4r)-4-(Heptafluoropropyl)cyclohexane-1-carboxamide","88951-19-3","D",0]
["1,2,2,3,3,4,4,5-Octafluoro-6-oxabicyclo[3.1.0]hexane","710-70-3","D",0]
["Tricyclo[7.3.3.15,11]heptasiloxane-3,7-diol, 1,3,5,7,9,11,14-heptacyclopentyl-14-[[dimethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silyl]oxy]-","352538-84-2","D",0]
["1,2,2,3,4,4,5,6,6,7,8,8,9,9-Tetradecafluoro-10,10-bis(trifluoromethyl)tricyclo[3.3.1.13,7]decane","2280049-22-9","D",0]
["4-[5-(Heptafluoropropyl)-1H-1,2,4-triazol-3-yl]aniline","1692915-43-7","D",0]
["2-Propenoic acid, 4,4,5,5,6,6,7,7,7-nonafluoro-2-hydroxyheptyl ester, polymer with 2-methyl-2-[(1-oxo-2-propen-1-yl)amino]-1-propanesulfonic acid","910114-98-6","D",0]
["{Ethyl[(perfluorodecyl)sulfonyl]amino}acetic acid","61481-04-7","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorodocosane","133310-70-0","D",0]
["Heptafluoropropyl sulfurofluoridate","662-98-6","D",0]
["N-[6-(Heptafluoropropyl)-2-oxo-2H-pyran-3-yl]benzamide","860454-18-8","D",0]
["(5-Difluoromethylperfluoro-1-pentyl)methanesulfinic acid sodium","187480-48-4","D",0]
["4-Cyanophenyl 4-(tridecafluorohexyl)benzoate","74701-19-2","D",0]
["(3,3,4,4,5,5,5-Heptafluoropentyl) methoxybis(3,3,3-trifluoropropyl) silane","608300-52-3","D",0]
["HFE-134","1691-17-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-pentylnonanamide","33496-54-7","D",0]
["4-(Pentafluoroethyl)-1,3-thiazol","1824049-08-2","D",0]
["N-(Perfluorobutanoyl)glutamic acid 1-ethyl ester","88435-87-4","D",0]
["2-(Tridecafluorohexyl)oxirane","52835-17-3","D",0]
["Chlorosulfurous acid, 2,2,3,3-tetrafluoropropyl ester","110920-07-5","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propanamide","662-20-4","D",0]
["1,3-dibromo-1,4-dichloro-1,2,2,3,4,4-hexafluorobutane","124311-10-0","D",0]
["Perfluoro(3-methoxy-2-oxabicyclo[3.3.0]octane)","87744-08-9","D",0]
["2-Propenoic acid, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl ester, telomer with 3-mercapto-1,2-propanediol, polymer with 2-methyloxirane polymer with oxirane di-2-propenoate, and 2-methyloxirane polymer with oxirane mono-2-propenoa","1017237-78-3","D",0]
["Perfluoro-4-(fluorosulfonyl)butanoic acid","83071-25-4","D",0]
["Siloxanes and Silicones, di-Me, 3-hydroxypropyl Me, Me 11-oxo-11-[(.gamma.-.omega.-perfluoroalkyl)oxy]undecyl, ethoxylated","500218-22-4","D",0]
["Chlorotetrafluoropropane","134190-50-4","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[[(perfluoropropyl)sulfonyl]amino]-1-propanaminium","2089108-65-4","D",0]
["Perfluoro(3,3'-(piperazine-1,4-diyl)dipropanoic acid)","948014-40-2","D",0]
["[3,5-Bis(tridecafluorohexyl)phenyl](diphenyl)phosphane","874161-77-0","D",0]
["6-methyl-2-(1,2,2,2-tetrafluoroethyl)-1H-benzimidazole","41185-76-6","D",0]
["Perfluoro-3-methoxypropanoic anhydride","42566-65-4","D",0]
["Propyl perfluoroheptanoate","134638-94-1","D",0]
["8-(Perfluorotetradecyl)-3,6-dioxaoctanol","108026-36-4","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N'-phenylbutanehydrazide","77146-66-8","D",0]
["Bis(pentafluoroethyl)diazene","756-00-3","D",0]
["Sodium perfluoropentanesulfonate","630402-22-1","D",0]
["8-bromo-2,2,6-trimethyl-4,4-bis(trifluoromethyl)-1H-3,1-benzoxazine","76220-89-8","D",0]
["6-Azido-2,2,3,3,4,4,5,5-octafluoro-2,3,4,5-tetrahydropyridine","89516-72-3","D",0]
["ethyl 2-[2-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-4-methylphenyl]sulfanylacetate","63780-80-3","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, 2,3-dihydroxypropyl ethers, N-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]carbamates","933999-90-7","D",0]
["1,6-bis(trimethoxysilanylethyl)perfluorohexane","94403-04-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,10-Octadecafluoro-10-iododecane","89608-43-5","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propan-1-amine","182243-54-5","D",0]
["N-Ethylperfluorooctanamide","89685-57-4","D",0]
["2,4-Bis[3,4,4,4-tetrafluoro-3-(trifluoromethyl)butyl]-1lambda~6~,3lambda~6~-dithietane-1,1,3,3-tetrone","1346175-94-7","D",0]
["N-((2,3-Dimethyl-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-71-7","D",0]
["N,N'-bis(Perfluorononanoyl)1,12-dodecandiamine","204922-38-3","D",0]
["2-(Nonafluorobutyl)aniline","106877-28-5","D",0]
["8:2 fluorotelomer unsaturated carboxylic acid","161094-76-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-N'-[(E)-(4-nitrophenyl)methylene]heptanehydrazide","470677-20-4","D",0]
["3-[(3-{[(Perfluorooctyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","73469-65-5","D",0]
["Ethylcellulose perfluorobutyrate","52627-33-5","D",0]
["1,1,2,2-Tetrafluoro-2-(1,1,2,2-tetrafluoroethoxy)ethane-1-sulfinic acid","88239-67-2","D",0]
["Bis(pentafluoroethyl)triselane","51684-79-8","D",0]
["N-[3-Borono-4-(heptafluoropropyl)phenyl]glycinamide","174778-59-7","D",0]
["5-(Perfluoropropyl)-2,2-dimethyl-3,5-pentanedione strontium(2+) (2:1)","125009-58-7","D",0]
["3-[(Heptafluoropropyl)sulfanyl]benzoic acid","79865-60-4","D",0]
["2-Iodo-4-(tridecafluorohexyl)thiophene","1453469-60-7","D",0]
["Silver(1+) 1,1,1,2,3,3,3-heptafluoropropan-2-ide","22407-25-6","D",0]
["Acetic acid ethenyl ester, polymer with ethene, 3,3,4,4,5,5,6,6,6-nonafluoro-1-hexene and 1,1,2,2-tetrafluoroethene","283164-62-5","D",0]
["2‐(5,5,7,7,8,8,10,10,11,11,13,13,14,14,16,16,17,17,18,18,19,19,19‐Tricosafluoro‐2‐oxo‐3,6,9,12,15‐pentaoxa‐1‐azanonadecan‐1‐yl)ethyl 2‐methylprop‐2‐enoate","653573-81-0","D",0]
["2,2,3,3-Tetrafluoro-N,N-dimethylpropan-1-amine","813-87-6","D",0]
["1,5-Dideoxy-1,1,1,5,5,5-hexafluoro-2,4-di-C-fluoro-2,4-bis-O-(heptafluoropropyl)pent-3-ulose","67118-49-4","D",0]
["1,1,2,2,3,3,4,5,5,6-Decafluorocyclohexane","2691-98-7","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-hydroxy-1-(naphthalen-2-yl)hex-1-en-3-one","849798-42-1","D",0]
["Perfluoroheptanenitrile","62038-08-8","D",0]
["Tetradecafluorocycloheptane","355-59-9","D",0]
["Methyl 2,3,4,4,5,5,6,6,6-nonafluoro-2-hexenoate","88022-46-2","D",0]
["4-Methylbenzene-1-sulfonic acid--5,5,6,6,7,7,8,8,8-nonafluorooctan-1-ol (1/1)","162082-63-5","D",0]
["3,3,4,4,4‐Pentafluorobutanal","239437-47-9","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[[(perfluoropropyl)sulfonyl]amino]-1-propanaminium","2089109-08-8","D",0]
["1,1'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(4-chlorobenzene)","88964-96-9","D",0]
["1-Nitro-4-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]benzene","147395-05-9","D",0]
["N-[3-[[(Perfluorooctyl)sulfonyl]amino]propyl]-N,N-dimethyl-1-decanaminium bromide (1:1)","14513-26-9","D",0]
["Pentanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[2,2,3,3,4,4,5,5,5-nonafluoro- (9CI)","547727-86-6","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(morpholin-4-yl)butane-1-thione","1206684-15-2","D",0]
["1,1'-(2,2,3,4,4,4-Hexafluorobutane-1,3-diyl)dibenzene","89185-53-5","D",0]
["[(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)oxy]acetonitrile","62656-65-9","D",0]
["Dimethyl perfluorodecanedioate","4590-24-3","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl acetate","356-06-9","D",0]
["(2H-Perfluoropropyl)(1H,1H-perfluoroethyl)ether","993-95-3","D",0]
["2-[1,1,2-Trifluoro-2-[1,1,2,2-tetrafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)ethoxy]ethoxy]acetic acid","919005-35-9","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8, 8,8-heptadecafluorooctyl)sulfonyl]methylamino] ethyl ester, homopolymer","27119-23-9","D",0]
["1,2-bis(1,1,2,2-tetrafluoroethoxy)benzene","4063-48-3","D",0]
["5,5,5-Trifluoro-4,4-bis(trifluoromethyl)pentanenitrile","5634-47-9","D",0]
["1,1,1,2-tetrafluoro-4-iodo-2-(trifluoromethoxy)pentane","243139-56-2","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl prop-2-enoate","376-56-7","D",0]
["3,3,4,4,5,5,5-heptafluoropentanal","126015-32-5","D",0]
["3,3,4,4,5,5,6,6,6-nonafluorohexan-1-yl 2-chloroacrylate","701909-41-3","D",0]
["1,1,1,7,7,7-Hexafluoro-6-hydroxy-4-oxo-2,6-bis(trifluoromethyl)heptan-2-yl acetate","101952-35-6","D",0]
["Perfluoro-5-heptene-1-sulfonic acid","2089109-42-0","D",0]
["Propane, 1-[1-[difluoro[(1,2,2-trifluoroethenyl) oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2,3,3,3-heptafluoro-, homopolymer","98973-10-5","D",0]
["Carbamic acid, (1-(diethoxyphosphinyl)-2,2,2-trifluoro-1-(trifluoromethyl)ethyl)-, phenylmethyl ester","145430-03-1","D",0]
["Methyl difluoro[(heptadecafluorooctyl)oxy]acetate","121591-26-2","D",0]
["Propan-2-yl [1,1,1,3,3,3-hexafluoro-2-(4-sulfamoylanilino)propan-2-yl]carbamate","5226-23-3","D",0]
["(2Z)‐4,4,5,5,6,6,7,7,8,8,9,9,10,10,10‐Pentadecafluorodec‐2‐enoic acid","173441-56-0","D",0]
["4-(Heptafluoropropyl)quinoline","181059-73-4","D",0]
["(1R-trans)-N,N'-1,2-Cyclohexanediylbis(perfluorobutanamide)","133964-60-0","D",0]
["1,1,1,2,2,4,5,6,7,7,7-Undecafluoro-6-(trifluoromethyl)-4-hepten-3-one","143582-62-1","D",0]
["4-Chlorobenzenediazonium perfluorobutanoate perfluorobutanoic acid (1:1:1)","630-31-9","D",0]
["Benzenesulfonic acid, 4-[2-[4-[[2-(acetyloxy)ethyl]ethylamino]phenyl]diazenyl]-, 2,2,3,3,4,4,5,5-octafluoropentyl ester","302929-37-9","D",0]
["2,4,6-tris(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptoxy)-1,3,5-triazine","464-34-6","D",0]
["2-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)cyclopentan-1-ol","34844-38-7","D",0]
["3-Bromo-1,1,2,3,4,4,4-heptafluorobut-1-ene","140427-84-5","D",0]
["Ethyl 2-diazo-4,4,5,5,6,6,6-heptafluoro-3-oxohexanoate","15959-98-5","D",0]
["Methyl 3-(pentafluoroethyl)benzoate","64299-46-3","D",0]
["2-Methyl-2-[[1-oxo-3-[(3,3,4,4,5,5, 6,6,7,7,8,8,8-tridecafluorooctyl)thio]propyl]amino]-1-propanesulfonic acid magnesium salt (2:1)","68005-63-0","D",0]
["3-(iodomethyl)-4-(2,2,3,3,4,4,5,5,5-nonafluoropentyl)pyrrolidine-1-carbonitrile","231285-91-9","D",0]
["Hexafluoropropene, oligomeric reaction products with tetrafluoroethylene, telomers with pentafluoroethyl hypofluorite","161278-44-0","D",0]
["2:2 Fluorotelomer sulfonate","2485704-05-8","D",0]
["Difluoromethyl 1H,1H-perfluoropropyl ether","56860-81-2","D",0]
["Propanoic acid - 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptan-1-ol (1/1)","87925-97-1","D",0]
["Octafluoro-3-methoxyprop-1-ene","67641-44-5","D",0]
["2,2,3,3,3-Pentafluoro-1-(pyridin-2-yl)propan-1-ol","17556-46-6","D",0]
["1,1,1,2,3,3,3-Heptafluoropropan-2-yl benzoate","57024-21-2","D",0]
["N-[4-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)phenyl]-4-(trifluoromethyl)benzamide","1246525-60-9","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoic acid--N-methylmethanamine (1/1)","328065-54-9","D",0]
["1,2,2,3,3,4-Hexafluorobutane-1,4-disulfonyl difluoride","90127-84-7","D",0]
["1,1,2,2,3,3-Hexafluoropropyl sulfurofluoridate","105660-26-2","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononan-2-one","77893-60-8","D",0]
["1,1-Dichloro-1,2,2-trifluoro-2-(1,2,2,2-tetrafluoroethoxy)ethane","51410-36-7","D",0]
["4,4'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(2,6-difluorophenol)","114611-30-2","D",0]
["1-(Perfluoroheptyl)nonadecane","1980065-05-1","D",0]
["1,2,3,4,5-Pentafluoro-6-(heptadecafluorooctyl)benzene","54387-09-6","D",0]
["2,2,3,3-Tetrafluoro-3-iodopropanoyl fluoride","91095-98-6","D",0]
["Ethyl 2-bromo-3,3,3-trifluoro-2-(trifluoromethyl)propanoate","648-62-4","D",0]
["3,3′-Oxybis[2,2,3,3-tetrafluoropropanoyl fluoride]","1428-40-6","D",0]
["2-bromo-2,3,3,3-tetrafluoropropanoyl bromide","41874-81-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-(4-nitrophenyl)nonanamide","164796-46-7","D",0]
["2,2,3,3,5,5,6,6-Octafluorocyclohexane-1,4-dione","17222-07-0","D",0]
["3-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)benzoic acid","2396-20-5","D",0]
["HFC-245ea","24270-66-4","D",0]
["5-Ethoxy-3,3-bis(trifluoromethyl)-1,2-dithiolane","62378-51-2","D",0]
["{[(2,3,3,4,4,5,5-Heptafluorocyclopent-1-en-1-yl)oxy]methyl}benzene","66463-33-0","D",0]
["3-({3-[(2-Hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoroethyl)sulfonyl]amino)-1-propanesulfonate","2089108-92-7","D",0]
["3,3-Bis(trifluoromethyl)-3-hydroxypropionic acid","1547-36-0","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-[(4-sulfamoylphenyl)methyl]nonanamide","316827-33-5","D",0]
["(1E)-2,2,3,3,4,4,4-Heptafluoro-N-phenylbutan-1-imine","62765-24-6","D",0]
["Trimethyl{3-{4-[3,4,4,4-tetrafluoro-2-(perfluoroisopropyl)-1,3-bis(trifluoromethyl)-1-butenyloxy]phenylsulfonylamino}propyl}ammonium iodide","158658-62-9","D",0]
["1,1-diphenyl-3,3-bis(trifluoromethyl)-2,1-benzoxaphosphol-1-ium","77047-91-7","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-(2-fluorophenyl)nonanamide","344282-15-1","D",0]
["2,5-Bis(heptafluoropropyl)benzoxazole","61324-23-0","D",0]
["1,1,1,4,4,5,5,6,6,7,7,8,8,8-Tetradecafluorooct-2-ene","935476-95-2","D",0]
["(10E)-12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,19-Heptadecafluorononadec-10-en-1-ol","135131-50-9","D",0]
["10-H-Perfluorodecanoate","1696259-72-9","D",0]
["2,2,3,3-Tetrafluoro-3-{1,1,2,3,3,3-hexafluoro-2-[(trifluoroethenyl)oxy]propoxy}propanoic acid","946163-81-1","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-Heptacosafluoropentadec-1-ene","1270180-04-5","D",0]
["(3E)-5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluorodeca-1,3-diene","148626-04-4","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluorobutyl)sulfonyl]amino}-1-butanaminium","2089108-84-7","D",0]
["1,1,1,2,2,3,4,4-Octafluorobutane","119450-58-7","D",0]
["N-(Carboxymethyl)-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-N,N-dimethyloctanaminium","2089109-25-9","D",0]
["5-[2-(Ethenyloxy)ethoxy]-1,1,1,2,2,3,3,4,4-nonafluoropentane","572911-07-0","D",0]
["2-Chloro-N-{[4-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)phenyl]carbamoyl}benzamide","74702-99-1","D",0]
["HFE-356pcf2","50807-77-7","D",0]
["2-[3,3,4,4,5,5,5-Heptafluoro-2,2-bis(trifluoromethyl)pentyl]oxirane","119285-89-1","D",0]
["N,N′-[Phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-perfluoro-1-hexanesulfonamide] ammonium salt","118337-75-0","D",0]
["(1,1,2,3,3,3-Hexafluoropropoxy)acetic acid","919005-38-2","D",0]
["3-{3-[3-(1,1,2,2-Tetrafluoroethoxy)phenyl]propyl}aniline","89807-71-6","D",0]
["4-[(Perfluoro-1-ethyl-2-methyl-1-propen-1-yl)oxy]benzoic acid sodium salt","927408-18-2","D",0]
["2,2'-(5-Iodo-1,3-phenylene)bis(hexafluoropropan-2-ol)","53173-72-1","D",0]
["1,1,1,2,2,3,3-heptafluoro-5-iodononane","755-48-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,9,9,10,10,11,11,11-Icosafluoroundecane","777931-73-4","D",0]
["3-(2,2,3,3-Tetrafluoropropoxy)thiophene","144203-97-4","D",0]
["Methyl 3,3,4,4,5,5,6,6-octafluoro-2-oxohexanoate","74067-15-5","D",0]
["1,2-Decanediol, 5,5,6,6,7,7,8,8,9,9,10,10,10-tridecafluoro-","147274-18-8","D",0]
["1-Bromoperfluorobutane","375-48-4","D",0]
["2-Fluoro-2-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]acetic acid","919005-01-9","D",0]
["Methyl perfluoro-3,6-dioxaheptanoate","39187-41-2","D",0]
["4-(2,2,3,3-tetrafluoropropoxy)benzene-1,2-dicarbonitrile","121190-46-3","D",0]
["4-(1,1,2,2-tetrafluoroethoxy)phenol","85578-29-6","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-7-[(prop-2-en-1-yl)oxy]heptane","678-50-2","D",0]
["1,1,4,4,5,5,5-Heptafluoro-2-methoxy-3-(trifluoromethyl)pent-1-ene","67544-90-5","D",0]
["Methoxy(3,3,4,4,4-pentafluorobutyl)propyl(3,3,3-trifluoropropyl)silane","608300-04-5","D",0]
["1H-Imidazole, 4-(pentafluoroethyl)-","81769-52-0","D",0]
["Poly(difluoromethylene), .alpha.-[2-[[2-(dimethylamino)ethyl]thio]ethyl]-.omega.-fluoro-","65530-55-4","D",0]
["2-[(5-Chloro-1,1,2,2,3,3,4,4,5,5-decafluoropentyl)oxy]-1,1,2,2-tetrafluoroethane-1-sulfonic acid","2196242-85-8","D",0]
["Propanoic acid, 3-hydroxy-2-(hydroxymethyl)-2-methyl-, polymer with 2-ethyl-2-(hydroxymethyl)-1,3-propanediol and N,N',2-tris(6-isocyanatohexyl)imidodicarbonic diamide, reaction products with N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-","306975-56-4","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluoro-N-(26-hydroxy-3,6,9,12,15,18,21,24-octaoxahexacos-1-yl)-N-methyl-1-octanesulfonamide","594-99-0","D",0]
["Dimethyl (1,1,1,3,3,3-hexafluoro-2-methylpropan-2-yl)phosphonate","646-87-7","D",0]
["N-[3-(Dimethylamino)propyl]-2,2,3,3,4,4,5,5,5-nonafluoropentanamide","153339-13-0","D",0]
["1,1,1,2,2,3,3,4,4,13,13,14,14,15,15,16,16,16-Octadecafluoro-6,11-diiodohexadecane","13105-46-9","D",0]
["5,5,6,6,7,7,7-Heptafluoro-4,4-bis(trifluoromethyl)heptan-1-ol","110254-90-5","D",0]
["Phosphonic acid, [3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy]butyl]-","646029-85-8","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)propanoic anhydride","13049-92-8","D",0]
["Chlorodimethyl(3,3,4,4,4-pentafluorobutyl)silane","648-51-1","D",0]
["(Perfluorohexyl)methane","158118-02-6","D",0]
["11-Chloro-perfluoroundecanoate","1696260-07-7","D",0]
["3,5-Bis(1,1,2,2-tetrafluoroethoxy)benzeneethanamine, hydrochloride","70126-63-5","D",0]
["4,5-Bis(pentafluoroethyl)-1,2,3,4,5-trithiadiazolidine","87985-86-2","D",0]
["2-Tert-butyl-5-hydroxy-2-methyl-5-(1,1,2,2-tetrafluoroethyl)oxolan-3-one","6002-58-0","D",0]
["Nonafluoropentanamide","13485-61-5","D",0]
["2,2'-[(1,1,2,2-Tetrafluoroethane-1,2-diyl)bis(oxy)]bis(difluoroacetyl fluoride)","24647-19-6","D",0]
["(2E)-4,4,5,5,6,6,6-Heptafluorohex-2-ene","1081782-31-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(3-phenylpropyl)butanamide","77970-73-1","D",0]
["5,5,5-Trifluoro-4-hydroxy-2-methyl-4-(trifluoromethyl)pentyl 2-methylprop-2-enoate","853064-87-6","D",0]
["3,3,4,4,4-Pentafluoro-2-hydrazinyl-2-hydroxybutanehydrazide","89972-15-6","D",0]
["1-Chloro-1,1,2,2-tetrafluoro-2-(1,2,2,2-tetrafluoroethoxy)ethane","51410-37-8","D",0]
["5-(Heptafluoropropyl)-6-methylpyrimidine-2,4(1H,3H)-dione","145663-05-4","D",0]
["Chlorodiethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","608295-89-2","D",0]
["Perfluoropropanol","72301-80-5","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl formate","78689-20-0","D",0]
["3,6-Dihydro-1,3,6-trioxo[1]benzothiopyrano[2,3-e]isoindol-2-yl perfluorobutanesulfonate","639827-04-6","D",0]
["Perfluoro-1,6-hexanedisulfinic acid, sodium salt (1:2)","105198-07-0","D",0]
["Benzyl 8-[(4-cyanophenyl)amino]-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoro-8-oxooctanoate","1308677-07-7","D",0]
["5,5-Dimethoxy-2-phenyl-4,4-bis(trifluoromethyl)-4,5-dihydro-1,3-thiazole","65093-93-8","D",0]
["(4S)-4-Benzyl-2-(heptafluoropropyl)-4,5-dihydro-1,3-oxazole","1366341-52-7","D",0]
["2-((((Tridecafluorohexyl)sulfonyl)methyl)amino)ethyl methacrylate","2233599-90-9","D",0]
["7,7,8,8,9,9,10,10,11,11,12,12,12-Tridecafluoro-1-(1H-naphtho[2,3-d]imidazol-2-yl)dodecan-6-one","240121-57-7","D",0]
["4H-Pyran-4-one, 5,6-dihydro-6,6-bis(trifluoromethyl)-2-methyl-","102129-09-9","D",0]
["1-(4-chloronaphthalen-1-yl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-one","35554-25-7","D",0]
["1,1,2,2,2-Pentafluoro-N-(pentafluoroethane) - N-(trifluoromethane) ethaneamine","758-48-5","D",0]
["3,3,3',3'-Tetrakis(trifluoromethyl)-1,1'-spirobi[2,1-benzoxasilole]","70091-69-9","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1-(undecafluoropentyl)pyrrolidine","94718-24-8","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluorobutyl)sulfonyl]amino}-1-propanaminium","2089109-04-4","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(perfluorohexyl)sulfonyl]amino]propyl]-1-propanaminium","2089108-73-4","D",0]
["1,1,1,2,2,5,5,5-Octafluoro-4-(trifluoromethyl)pentan-3-one","61637-91-0","D",0]
["3-[(6,6,7,7,8,8,9,9,10,10,11,11,11-Tridecafluoroundecanoyl)oxy]-4-(trimethylazaniumyl)butanoate","142674-34-8","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-oxo-2,3-dihydropyrimidin-4-yl)butanamide","94720-20-4","D",0]
["2,5-Bis[(nonadecafluorononyl)oxy]benzene-1-sulfonic acid","76069-15-3","D",0]
["Methyl 4,4,5,5,6,6,7,7,7-nonafluoro-3-oxoheptanoate","89129-70-4","D",0]
["2,3,3,3-Tetrafluoro-2-methoxypropanoic acid","10186-64-8","D",0]
["1,1,2,2-Tetrafluoro-1,2-bis(trifluoromethoxy)ethane","378-11-0","D",0]
["2,2,3,3,4,4,5,5-Octafluorohexane-1,6-diyl bis(4-methylbenzene-1-sulfonate)","58191-47-2","D",0]
["4-Bromo-2,3,3,4,5,5,6,6-octafluoro-1-nitrocyclohex-1-ene","79150-80-4","D",0]
["6-(1,1-Difluoroethoxy)-1,1,1,2,2,3,3,4,4,5,5-undecafluorohexane","197963-86-3","D",0]
["2-Difluoromethoxy-2,2-difluoroacetic acid","75780-06-2","D",0]
["1-(2,2,3,3-Tetrafluoropropyl)piperidine","91461-54-0","D",0]
["2-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-(pentafluoroethyl)-3,3-bis(trifluoromethyl)oxirane","103697-21-8","D",0]
["1-Chloro-2-(difluoromethoxy)-1,1,2,2-tetrafluoroethane","32778-12-4","D",0]
["2-{[(2,2,3,3,3-Pentafluoro-1-phenylpropylidene)amino]oxy}acetamide","89040-78-8","D",0]
["4-(2-Chloroethoxy)-1,1,1,2,2,3,3-heptafluorobutane","679-53-8","D",0]
["Ethyl 4,4,5,5,6,6,6-heptafluoro-3-sulfanylhexanoate","377-64-0","D",0]
["Fatty acids, C18-unsatd., trimers, 2-[methyl[(1,1,2,2,3,3,4,4,5,5,5-undecafluoropentyl)sulfonyl]amino]ethyl esters","148240-81-7","D",0]
["4-Heptanone, 2,6-bis(trifluoromethyl)-2,6-dihydroxy-1,1,1,7,7,7-hexafluoro-, azine","101913-85-3","D",0]
["N-Methyl-N-[3-[(perfluorohexylsulfonyl)amino]propyl]acetamide","85520-95-2","D",0]
["2-(Perfluorotetradecyl)ethylsulfonic acid","1377603-17-2","D",0]
["Silsesquioxanes, 3-hydroxypropyl Me 3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]propyl 3-[(1,4,5,6-tetrahydro-4,6-dithioxo-1,3,5-triazin-2-yl)amino]propyl, ethoxy- and methoxy-terminated, ethers wit","1380516-78-8","D",0]
["N-(2,2,3,3,4,4,4-Heptafluorobutyl)-N'-methylthiourea","105412-23-5","D",0]
["1,1,1,2,3,3,4,4-Octafluoro-4-[1,1,2,2,3,4,4,4-octafluoro-3-(trifluoromethyl)butoxy]-2-(trifluoromethyl)butane","73309-73-6","D",0]
["(OC-6-21)-(4-Carboxylato-1,1,2,2,3,3,4,4-octafluorobutyl)pentafluoro-sulfate(1-)","722450-66-0","D",0]
["1,2,3,3,4-Pentafluoro-4-(trifluoromethyl)cyclobut-1-ene","105311-66-8","D",0]
["tris((Perfluoropropyl)methyl) borate","755-53-3","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl methanesulfonate","188534-35-2","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N-[2-methyl-1-(pyrrolidin-1-yl)propylidene]butane-1-sulfonamide","496949-61-2","D",0]
["1-(2,2,3,3-Tetrafluoropropyl)-1H-1,2,4-triazol-3-amine","937602-82-9","D",0]
["Copolymer of 1,1-difluoroethene, perfluoroethene, 1,1,2,2-tetrafluoro-3-iodopropoxyperfluoroethene and perfluoro(methoxyethene)","179765-14-1","D",0]
["(1,1,2,3,3,3-Hexafluoropropyl)cyclopropane","57915-70-5","D",0]
["2‐(5,5,7,7,8,8,10,10,11,11,13,13,14,14,15,15,16,16,16‐Nonadecafluoro‐2‐oxo‐3,6,9,12‐tetraoxa‐1‐azahexadecan‐1‐yl)ethyl 2‐methylprop‐2‐enoate","549549-24-8","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 1,1-difluoroethene, ethyl 2-propenoate and 1,1,2,3,3,3-hexafluoro-1-propene","1646594-71-9","D",0]
["Siloxanes and Silicones, di-Me, Bu group- and 3-[(2-methyl-1-oxo-2-propen-1-yl)oxy]propyl group-terminated, telomers with acrylic acid, di-Me, Me 3-mercaptopropyl siloxanes, Me acrylate, Me methacrylate and 2-[methyl[(perfluoro-c4-8-alkyl) ¿","1645852-10-3","D",0]
["Sulfonamides, C7-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with 1,3-bis(isocyanatomethyl)benzene","1645852-09-0","D",0]
["Poly[oxy(1,1,2,2-tetrafluoro-1,2-ethanediyl)], alpha-(2,2,2-trifluoroacetyl)-omega-[(2,2,2-trifluoroacetyl)oxy]-","1646599-55-4","D",0]
["1,2,2,3,3,4,5,5-Octafluoro-4-(trifluoromethyl)-Cyclopentanecarbonyl fluoride","1646599-70-3","D",0]
["2,3,3,3-tetrafluoropropanamide","1647-57-0","D",0]
["dichloromethyl[3-(1,1,2,2-tetrafluoroethoxy)propyl]silane","1692-54-2","D",0]
["3,3,4,4-tetrafluorohexa-1,5-diene","1763-21-9","D",0]
["Tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-3,5-octanedionate-O,O')europium","17631-68-4","D",0]
["1-Chloroheptafluorocyclopentene","1759-63-3","D",0]
["1,1,2,2-Tetrahydroperfluorobutyl acrylate","17527-31-0","D",0]
["Benzene, 1,3-diisocyanatomethyl-, polymers with hydrolyzed Me esters of reduced polymd. oxidized tetrafluoroethylene","175449-31-7","D",0]
["2-Propenoic acid, polymers with lauryl acrylate and 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl acrylate","1648534-82-0","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-[2-(methylamino)ethyl]-omega-hydroxy-, N-[(perfluoro-C4-8-alkyl)sulfonyl] derivs., C12-16-alkyl ethers","1648539-69-8","D",0]
["2-Propenoic acid, 2-(methylamino)ethyl ester, N-[(perfluoro-C4-8-alkyl)sulfonyl] derivs., polymers with propene","1648540-20-8","D",0]
["Perfluoro-9-(trifluoromethyl)decanoic acid","16486-94-5","D",0]
["Docosafluoro-11-(trifluoromethyl)dodecanoic acid","16486-96-7","D",0]
["Perfluorooctadecanoic acid","16517-11-6","D",0]
["Propane, 1,1,1,2,2,3,3-heptafluoro-3-((trifluoroethenyl)oxy)-, polymer with tetrafluoroethene and trifluoro(trifluoromethoxy)ethene","165178-32-5","D",0]
["Perfluorooctanesulfonamido ammonium iodide","1652-63-7","D",0]
["2,2-dichloro-1,1,1,3,3,3-hexafluoropropane","1652-80-8","D",0]
["1,1,3-Trichloro-1,2,2,3,3-pentafluoropropane","1652-81-9","D",0]
["ammonium 8-chlorotetradecafluorooctanoate","16557-94-1","D",0]
["Poly(oxy-1,2-ethanediyl), alpha,alpha',alpha''-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)silylidyne]tris[oxy(dimethylsilylene)-3,1-propanediyl]]tris[omega-methoxy-","165967-96-4","D",0]
["(Heptafluorobutanoyl)pivaloylmethane","17587-22-3","D",0]
["Sodium, di(perfluoroalkyl(C4-18))sulfonatobutanedioic acid","160994-59-2","D",0]
["Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-,reaction products with ammonia","160994-74-1","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, fluorinated","161075-00-9","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated","161075-02-1","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters, hydrolysed","161075-03-2","D",0]
["Sulfonamides, C7-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with 1,3-bis(isocyanatomethyl)benzene and N-butyl-1-butanamine","1645850-46-9","D",0]
["1,2-andecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-,1,1'-(hydrogen phosphat)","170004-70-3","D",0]
["Cyclohexanemethanol, 4-[(ethenyloxy)methyl]-, polymer with chlorotrifluoroethene, (ethenyloxy)cyclohexane, .alpha.-[[4-[(ethenyloxy)methyl]cyclohexyl]methyl]-.omega.-hydroxypoly(oxy-1,2-ethanediyl) and ethoxyethene (9CI)","170442-59-8","D",0]
["Methanol, reaction products with 1,1,1,2,2,3,4,5,5,6,6,7,7,7-tetradecafluoro-3-heptene","1708962-18-8","D",0]
["Methanol, reaction products with 1,1,1,2,3,4,4,5,5,6,6,7,7,7-tetradecafluoro-2-heptene","1708962-19-9","D",0]
["allyl heptafluorobutyrate","17165-55-8","D",0]
["Isoprene-Chlorotrifluoroethylene copolymer","172018-29-0","D",0]
["Ammonium perfluorononanesulfonate","17202-41-4","D",0]
["Tetrafluoroethylene-Formaldehyde copolymer","172074-62-3","D",0]
["Chlorotrifluoroethylene-Vinylmethyldiethoxysilane copolymer","172074-63-4","D",0]
["Vinyl chloride-2,2,3,3-Tetrafluoropropyl acrylate copolymer","172074-65-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, polymer with 2-methyl-2-[(1-oxo-2-propen-1-yl)amino]-1-propane sulfonic acid and 2,2,2-trifluoroethyl 2-propenoate","172083-53-3","D",0]
["4-Heptadecafluorooctanesulfonamidobenzenesulfonic acid sodium salt","172398-80-0","D",0]
["2-(Difluoromethylene)-4,4,5-trifluoro-5-(trifluoromethyl)-1,3-dioxolane","17256-52-9","D",0]
["6-H-Perfluorohexanoic acid","1726-50-7","D",0]
["Methyl 2,2,3,3,4,4-hexafluoro-4-iodobutanoate","17308-98-4","D",0]
["2-Propenoic acid, 2-(ethyl((nonafluorobutyl)sulfonyl)amino)ethyl ester","17329-79-2","D",0]
["Perfluoro-3,4-dimethylhexane","1735-48-4","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)toluene","1737-10-6","D",0]
["(2H-Perfluoroethyl)(1H,1H,3H-perfluoropropyl)ether","16627-68-2","D",0]
["pentafluoropropanol","28302-70-7","D",0]
["Perfluoro-6-(1,2-dibromoethoxy)hexanenitrile","283593-02-2","D",0]
["1-Chloro-1,2,2,2-tetrafluoroethane","2837-89-0","D",0]
["Vinyl chloride-1,1,5-Trihydroperfluoroamyl acrylate copolymer","28497-93-0","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C12 fraction","274918-10-4","D",0]
["Benzene, pentafluoro[1,2,2-trifluoro-2-[(trifluoroethenyl)oxy]-1-(trifluoromethyl)ethoxy]-, polymer with tetrafluoroethene and trifluoro(trifluoromethoxy)ethene","26658-70-8","D",0]
["2-(4H-Perfluorobutyl)-2-propanol","2673-15-6","D",0]
["Fluoroether E4","26738-51-2","D",0]
["Propanoic acid, ethenyl ester, polymer with 1,1-difluoroethene and 1,1,2,2-tetrafluoroethene","26779-98-6","D",0]
["1-Propene, polymer with tetrafluoroethene","27029-05-6","D",0]
["Sodium perfluoropentanoate","2706-89-0","D",0]
["Perfluoropentanoic acid","2706-90-3","D",0]
["Perfluoropentanesulfonic acid","2706-91-4","D",0]
["Propane, hexafluoro-","27070-61-7","D",0]
["2H-Perfluorofluoro-5,8,11,14,17,20,23-heptamethyl-3,6,9,12,15,18,21,24-octaoxaheptacosane","27120-63-4","D",0]
["phenylbis(trifluoroacetato-O)iodine","2712-78-9","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-hydroxy-4-nitrophenyl)butyramide","2712-83-6","D",0]
["1,1-dichloro-1,2,2,3,3,3-hexafluoropropane","2729-28-4","D",0]
["1,1-Dibromo-1,2,2,2-Tetrafluoroethane","27336-23-8","D",0]
["Siloxanes and Silicones, 3-[[2-[(2-aminoethyl)amino]ethyl]amino]propyl hydroxy, hydroxy 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl, hydroxy-terminated, formates (salts)","273737-91-0","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C3 fraction","274917-93-0","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C4 fraction","274917-94-1","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C5 fraction","274917-95-2","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C6 fraction","274917-96-3","D",0]
["Bis(3,5,6-trichloro-2,2,3,4,4,5,6,6-octafluoro-1-oxohexyl)peroxide","28285-49-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with 1-ethenyl-4-[(andecafluorohexenyl)oxy]benzene, graft(9CI)","167229-03-0","D",0]
["1-Iodo-1H,1H,2H,2H-perfluoroheptane","1682-31-1","D",0]
["2,3,3,3-Tetrafluoro-2-(perfluoroethoxy)propanoyl fluoride","1682-78-6","D",0]
["Ethanesulfonyl fluoride, 1,1,2,2-tetrafluoro-2-[(1,2,2-trifluoroethenyl)oxy]-, polymer with 1,1,2,2-tetrafluoroethene, hydrolyzed, lithium salts","1687740-67-5","D",0]
["2-Perfluorooctylsulfonyl-N-ethylaminoethyl alcohol","1691-99-2","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C13 fraction","274918-12-6","D",0]
["Ethanol, 2,2'-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)imino]bis-","27607-36-9","D",0]
["Ethanol, 2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)amino]-","27607-42-7","D",0]
["1-Nonanesulfonyl chloride, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-","27607-61-0","D",0]
["2,4,4,5,7,7,8,10,10,11,13,13,14,16,16,17,17,18,18,18-Icosafluoro-2,5,8,11,14-pentakis(trifluoromethyl)-3,6,9,12,15-pentaoxaoctadecan-1-ol","27617-34-1","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexane-1-sulphonyl chloride","27619-88-1","D",0]
["1-Decanesulfonyl chloride, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","27619-90-5","D",0]
["1-Dodecanesulfonyl chloride,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","27619-91-6","D",0]
["Perfluoro-2,5,8-trimethyl-3,6,9-trioxadodecanoyl fluoride","27639-98-1","D",0]
["Hexanedioic acid, dimethyl ester, polymers with 2,2-bis(bromomethyl)-1,3-propanediol-ethanethiol-tetrafluoroethylene telomer reaction products","277752-44-0","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, potassium salt","2795-39-3","D",0]
["1,1-dimethyl-3-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]urea","27954-37-6","D",0]
["tetrafluorobenzene","28016-01-5","D",0]
["1,1-Dichloro-2,3,3,3-tetrafluoroprop-1-ene","2804-55-9","D",0]
["Potassium perfluorodecanesulfonate","2806-16-8","D",0]
["alpha,alpha,beta,beta-tetrafluoro-2-methyl-4-nitrophenetole","28202-30-4","D",0]
["alpha,alpha,beta,beta-tetrafluoro-o-nitrophenetole","28202-31-5","D",0]
["4-(1,1,2,2-Tetrafluoroethoxy)nitrobenzene","28202-32-6","D",0]
["o-sec-butyl-alpha,alpha,beta,beta-tetrafluorophenetole","28202-34-8","D",0]
["Siloxanes and Silicones, hydrogen gamma-omega-perfluoro-C6-10-alkyl","160965-19-5","D",0]
["1-(1,3-Dimethylbutoxy)-2-(perfluorohexyl)ethane","210896-25-6","D",0]
["Butanoic acid, 2,2,3,3,4,4-hexafluoro-4-[(trifluoroethenyl) oxy]-, sodium salt, polymer with 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]propane and tetrafluoroethene","211697-45-9","D",0]
["Fatty acids, C7-19, perfluoro, ammonium salts","212013-54-2","D",0]
["2-Propenoic acid, gamma-omega-perfluoro-C8-20-alkyl esters","212013-58-6","D",0]
["2-Propenoic acid, esters, 2-methyl-, C18-22-alkyl esters, polymers with cyclohexyl methacrylate, .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and 2-hydroxyethyl methacrylate-5-isocyanato-1-(isocyanatomethyl)-1,3,3-¿","212013-59-7","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 2-ethylhexyl 2-propenoate,(2-methyl-1-oxo-2-propenyl)-methoxypoly( oxy-1,2-ethanediyl),(2-methyl-1-oxo-2-propenyl)-(2-methyl-1-oxo-2-propenyl)oxypoly(oxy-1,2-ethanediyl ) and ¿","200358-70-9","D",0]
["Propanoyl fluoride, 2,3,3,3-tetrafluoro-2-(1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy)-, polymer with trifluoro(trifluoromethyl)oxirane, reaction products with 3-(ethenyldimethylsilyl)-N-methylbenzenamine","185701-88-6","D",0]
["1,4-Dibromo-1,1,2,2-tetrafluorobutane","18599-20-7","D",0]
["2-Vinyl(1-bromoperfluoroethane)","18599-22-9","D",0]
["Ammonium hexadecafluorononanoate","1868-86-6","D",0]
["Ethyl N-ethyl-N-((heptadecafluorooctyl)sulfonyl)glycinate","1869-77-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with 2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate, sodium salt","1878204-24-0","D",0]
["Perfluoro-N-(perfluoroethyl)sulfonylethanesulfonamide  compd. with N,N-diethylethanamine (1:1)","188596-18-1","D",0]
["1,3,3,4,4,5,5-Heptafluoro-Cyclopentene","1892-03-1","D",0]
["2-Propenoic acid, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl ester","1893-52-3","D",0]
["N-ethylsulfonylglycine, perfluoroalkyl (C5-10), potassium salt","190605-64-2","D",0]
["tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyloctane-3,5-dionato-O,O')lanthanum","19106-89-9","D",0]
["Methyl 4-trifluoroethenoxy-2,2,3,3,4,4-hexafluorobutanoate","19190-61-5","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-5-[(trifluoroethenyl)oxy]pentanenitrile","19237-73-1","D",0]
["1-Propanol, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-[(1,1,2-trifluoro-2-propen-1-yl)oxy]propoxy]-, polymer with 1,1,1,2,2,3,3-heptafluoro-3-[(1,2,2-trifluoroethenyl)oxy]propane and 1,1,2,2-tetrafluoroethene","192575-94-3","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexene","19430-93-4","D",0]
["Bis(4-tert-butylphenyl)iodanium nonafluorobutane-1-sulfonate","194999-85-4","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], alpha-(2-methyl-1-oxo-2-propenyl)-omega-hydroxy-, polymer with alpha-fluoro-omega-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and alpha-(2-methyl-1-oxo-2-propenyl)-omega-methoxypoly(oxy-1,2-¿","195158-89-5","D",0]
["2-[(Bicyclo[2.2.1]hept-5-en-2-yl)methyl]-1,1,1,3,3,3-hexafluoropropan-2-ol","196314-61-1","D",0]
["bis[2-[ethyl[(heptadecafluorooctyl)sulphonyl]amino]ethyl] (4-methyl-1,3-phenylene)biscarbamate","21055-88-9","D",0]
["N,N-Dimethyl-3-{[(pentadecafluoroheptyl)sulfonyl]amino}-1-propanamine N-oxide","178094-74-1","D",0]
["N,N-dimethyl-3-[(perfluoropentane-1-sulfonyl)amino]propan-1-amine N-oxide","178094-75-2","D",0]
["3-[(Perfluorobutane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide","178094-76-3","D",0]
["Siloxanes and Silicones, Me hydrogen, Me 3,3,4,4,5,5,6,6,6-nonafluorohexyl","178233-65-3","D",0]
["2-Propenoic acid, C12-14-alkyl esters, polymers with Bu (1-oxo-2-propenyl)carbamate and delta-omega-perfluoro-C6-12-alkyl acrylate","178233-67-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl methacrylate","1841-46-9","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate andmethyloxirane polymer with oxirane mono-2-propenoate (9CI)","200413-68-9","D",0]
["2-Propenoic acid, 2-methyl-, polymer with butyl 2-methyl-2-propenoate,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, 2-hydroxyethyl 2-methyl-2-propenoate and methyl 2-methyl-2-propenoate","200513-42-4","D",0]
["4-Methyl-alpha,alpha-bis(trifluoromethyl)benzenemethanol","2010-61-9","D",0]
["Sodium perfluoroheptanoate","20109-59-5","D",0]
["2-Propenoic acid, 2-methyl-, hexadecyl ester, polymers with 2-hydroxyethylmethacrylate, gamma-omega-perfluoro-C10-16-alkyl acrylate and stearyl methacrylate","203743-03-7","D",0]
["3,3,4,4,5,5,6,6-Octafluoro-6-iodohex-1-ene","203929-12-8","D",0]
["4:2 Fluorotelomer alcohol","2043-47-2","D",0]
["Nonane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","2043-52-9","D",0]
["1H,1H,2H,2H-Perfluorohexyl iodide","2043-55-2","D",0]
["4,5-Dichloro-1,1,1,3,3,4,5,5-octafluoropentan-2-one","20474-89-9","D",0]
["Perfluoro(2-methyl-3-oxahexanoyl) fluoride","2062-98-8","D",0]
["2,2,3,3-Tetrafluoropropionamide","2069-86-5","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]-, polymer with 1,1-dichlorethene","207004-58-8","D",0]
["Perfluoro-4-methyl-2-pentene","2070-70-4","D",0]
["(1-Propanamine, 2-(trimethoxysilyl)-, reaction products with reduced methanol-peroxidized poly(tetrafluoroethylene)","207574-77-4","D",0]
["1-Butanol, 4-(ethenyloxy)-, polymer with 1-chloro-1,2,2-trifluoroethene and ethoxyethene, hydrogen butanedioate","207691-69-8","D",0]
["Oxirane, methyl-, polymer with oxirane, mono(4,4,5,5,6,6,7,7,8,8,9,9,10,10-heptadecafluoro-1-methyl undecyl)ether","208721-05-5","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, ion(1-), 1-(4-butoxy-1-naphthalenyl)tetrahydrothiophenium","209482-18-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers with gamma-omega-perfluoro-C10-16-alkyl acrylate and vinyl acetate, acetates","196316-34-4","D",0]
["alpha,alpha,beta,beta-tetrafluoro-m-nitrophenetole","1644-21-9","D",0]
["Hexafluoroisopropylideneimine","1645-75-6","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-(3-chloro-2-hydroxypropyl)-N-methyl","1645842-67-6","D",0]
["Siloxanes and Silicones, di-Me, Bu group- and 3-[(2-methyl-1-oxo-2-propen-1-yl)oxy]propyl group-terminated, telomer with acrylic acid, di-Me, Me 3-mercaptopropyl siloxanes, Me acrylate, Me methacrylate and 2-[methyl[(perfluoro-C4-8-alkyl)¿","1645845-44-8","D",0]
["Siloxanes and Silicones, di-Me, polymers with 3-[(2-aminoethyl)amino)propyl silsesquioxanes, hydroxy-terminated, reaction products with 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-1-octanesulfonyl fluoride","1645848-42-5","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters","161075-12-3","D",0]
["1,1,2,2-Tetrafluoro-2-(trifluoromethoxy)-N,N-bis(trifluoromethyl)ethanamine","160228-75-1","D",0]
["Benzoic acid, 2,3,4,5-tetrachloro-6-[[(3-hydroxyphenyl)amino]carbonyl]-, perfluoro-C6-8-alkanesulfonates (esters), monopotassium salts","160305-97-5","D",0]
["1-Propanaminium, 3-amino-N-(2-carboxyethyl)-N,N-dimethyl-, N-(delta-.omega.-perfluoro-beta-hydroxy-C12-18-alkyl) derivs., inner salts","160336-10-7","D",0]
["2-Propenoic acid, butyl ester, polymers with 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl acrylate","160336-17-4","D",0]
["Butanoic acid, 4-[[3-(dimethylamino)propyl]amino]-4-oxo-, 2 (or 3)-[(gamma-omega-perfluoro-C3-14-alkyl)thio] derivs.","160336-21-0","D",0]
["Alkyl iodides, C1-24, perfluoro","160402-15-3","D",0]
["Quaternary ammonium compoands, bis(hydroxyethyl)methyl(delta-omega-perfluoro-beta-hydroxy-C10-14-alkyl), iodides","160402-26-6","D",0]
["Chloroethylene-vinylformic acid-perfluoroalkyl(ethyl) copolymer","160476-36-8","D",0]
["Phosphoric acid, mono(perfluoro-C10-18-alkyl) esters, diammonium salts","160498-33-9","D",0]
["(+/-)-2-amino-4,4,4-trifluoro-3-(trifluoromethyl)butyric acid","16063-80-2","D",0]
["3,5,7,7-Tetrachloro-2,2,3,4,4,5,6,6,7-nonafluoroheptanoic acid","16069-78-6","D",0]
["1,2-Benzenedicarboxylic acid, bis(gamma-omega-perfluoro-1-methyl-C5-20-alkyl)esters","160709-28-4","D",0]
["2-Propenoic acid, esters, 2-methyl-, 2-ethylhexyl ester, polymers with 2-[[(heptadecafluorooctyl)sulfonyl]amino]ethyl methacrylate N-C1-3-alkyl derivs.","160709-33-1","D",0]
["Iodoperfluoroalkane(C5-14)","160738-69-2","D",0]
["nickel(II) trifluoroacetate","16083-14-0","D",0]
["1-Nonanol, 4,4,5,5,6,6,7,7,8,9,9,9-dodecafluoro-2-iodo-8-(trifluoromethyl)-","16083-62-8","D",0]
["1-Decanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluoro-2-iodo-","16083-64-0","D",0]
["Perfluoro(4-methyl-3,6-dioxaoct-7-ene)sulfonyl fluoride","16090-14-5","D",0]
["Perfluoro(2-propoxypropyl vinyl ether)","1644-11-7","D",0]
["2,2'-(1,4-Phenylene)bis(hexafluoropropan-2-ol)","1992-15-0","D",0]
["[(2,2,3,3-tetrafluoropropoxy)methyl]oxirane","19932-26-4","D",0]
["1,1'-[(1,1,2,2-tetrafluoroethylene)bis(oxy)]bis[1,2,2-trifluoroethylene]","1998-53-4","D",0]
["Diphosphoric acid, polymers with ethoxylated reduced Me esters of reduced polymd. oxidized tetrafluoroethylene","200013-65-6","D",0]
["Dichloro-3-(perfluoro-2-propoxy)propylmethylsilane","20006-68-2","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl 2-methylprop-2-enoate","17526-97-5","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced and hydrolyzed","161075-14-5","D",0]
["Perfluoroalkyl(C4-23) iodide","161075-23-6","D",0]
["Alanine, 2-methyl-N-(1-oxo-2-propenyl)-, perfluoro-.omega.-[(perfluoro-C1-8-alkyl)oxy]-C3-12-alkyl esters","161075-35-0","D",0]
["Alcohols, C12-26-secondary, .gamma.-.omega.-perfluoro, ethoxylated  (2-Perfluoroalkyl(C9-23)-1-methylethyl polyoxyethylene ether)","161075-39-4","D",0]
["1,3-Dioxole, 2,2,4-trifluoro-5-(trifluoromethoxy) polymer with tetrafluoroethene","161611-79-6","D",0]
["Perfluoropropyl trifluorovinyl ether","1623-05-8","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, ethoxylated","162492-15-1","D",0]
["Alcohols, C8-14, perfluoro, reaction products with di-Me, Me hydrogen siloxanes and polyethylene glycol mono-Me ether Basic information","162567-79-5","D",0]
["2-Propenoic acid, butyl ester, reaction product with poly(oxy-1,2-ethanediyl), .alpha.-methyl-.omega.-hydroxy-, and N-ethyl-N-2-hydroxyethyl perfluoroctane sulfonamide","162568-17-4","D",0]
["Hexanedioic acid, polymers with 1,3-butanediol, 1,4-butanediol, di-Et malonate, 1,6-diisocyanatohexane, ethoxylated reduced Me esters of reduced polymd. oxidized tetrafluoroethylene, 1,6-hexanediol, 1,1'-methylenebis[isocyanatobenzene],¿","1627515-87-0","D",0]
["Hexanenitrile, 2,2,3,3,4,4,5,5,6,6-decafluoro-6-[(trifluoroethenyl)oxy]-, polymer with tetrafluoroethene and trifluoro(trifluoromethoxy)ethene","163336-49-0","D",0]
["2-Propenoic acid, 2-ethylhexyl ester, polymer with 1,1-dichloroethene and .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]pol y(difluoromethylene)","163440-88-8","D",0]
["Poly(difluoromethylene), .alpha.-hydro-.omega.-(2,2-dichloro-2-fluoroethyl)-","163440-89-9","D",0]
["Butane, 1-ethoxy-1,1,2,2,3,3,4,4,4-nonafluoro-","163702-05-4","D",0]
["Propane, 2-(ethoxydifluoromethyl)-1,1,1,2,3,3,3-heptafluoro-","163702-06-5","D",0]
["Butane, 1,1,1,2,2,3,3,4,4-nonafluoro-4-methoxy","163702-07-6","D",0]
["Propane, 2-(difluoromethoxymethyl)-1,1,1,2,3,3,3-heptafluoro-","163702-08-7","D",0]
["Perfluoro(2,7-dimethyl-3,6-dioxasuberoyl) fluoride","1644-10-6","D",0]
["2-(Perfluoropropoxy)-1H,1H-perfluoropropanol","26537-88-2","D",0]
["2-Propenoic acid, esters, 2-methyl-, 2-ethylhexyl ester, polymer with 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-hexadecafluoro-2-hydroxy-10-(trifluoromethyl)undecyl 2-propenoate","26570-69-4","D",0]
["Oxirane, tetrafluoro-, homopolymer","26591-06-0","D",0]
["Decafluorobis(trifluoromethyl)cyclohexane","26637-68-3","D",0]
["Tetrafluoroethylene-perfluoro(sulfinoethoxypropoxytrifluoroethylene) copolymer","26654-97-7","D",0]
["Vinyl fluoride-Hexafluoropropylene copolymer","25120-58-5","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methylaniline","238098-26-5","D",0]
["Propanedioic acid, mono(gamma-omega-perfluoro-C8-12-alkyl) derivs., di-me esters","238420-68-3","D",0]
["Propanedioic acid, mono(gamma-omega-perfluoro-C8-12-alkyl) derivs., bis[4-(ethenyloxy)butyl] esters","238420-80-9","D",0]
["Propanoyl fluoride, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-, polymer with trifluoro(trifluoromethyl)oxirane, reaction products with 3,3'-(3,3,4,4,5,5,6,6,7,7,8,8-...","241148-23-2","D",0]
["Pentadecafluoro-2-iodoheptane","24394-25-0","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-2-hydroxy-10-(trifluoromethyl)undecyl acrylate","24407-09-8","D",0]
["Heptafluoropropan-2-ol","24427-67-6","D",0]
["N-Methyl-N-(2-hydroxyethyl)perfluorooctanesulfonamide","24448-09-7","D",0]
["3-chloro-2,2,3,3-tetrafluoropropanoyl chloride","24503-62-6","D",0]
["Pentafluoro(1,2,2-trifluoro-2-((trifluorovinyl)oxy)-1-(trifluoromethyl)ethoxy)benzene","24520-19-2","D",0]
["2-Propenoic acid, 2-methyl-, 2-(diethylamino)ethyl ester, polymers withglycidyl methacrylate and gamma-omega-perfluoro-C6-20-alkyl acrylate, acetates(salts)","247047-61-6","D",0]
["N-allyl-N-ethylheptadecafluorooctanesulphonamide","24924-36-5","D",0]
["Ethene, 1,1-difluoro-, homopolymer","24937-79-9","D",0]
["Ethene, chlorotrifluoro-, polymer with chloroethene","24937-97-1","D",0]
["Oxirane, 2,2,3-trifluoro-3-(trifluoromethyl)-, homopolymer","25038-02-2","D",0]
["Ethene, tetrafluoro-, polymer with ethene","25038-71-5","D",0]
["Ethene, 1-chloro-1,2,2-trifluoro-, polymer with 1,1,2,2-tetrafluoroethene","25038-89-5","D",0]
["Ethene, tetrafluoro-, polymer with trifluoro(trifluoromethoxy)ethene","26425-79-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, reaction products with 5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexane and Me Etketone oxime, polymers with gamma-omega-perfluoro-C8-20-alkyl acrylate and stearylacrylate","221455-57-8","D",0]
["2-Propenoic acid, gamma-omega-perfluoro-C8-20-alkyl ester, polymers withacrylonitrile, polyethylene glycol dimethacrylate and polyethylene glycolmethacrylate Me ether","221455-61-4","D",0]
["2-Propenoic acid, 2-methyl-, oxiranylmethyl ester, polymers with acrylicacid-glycidyl Ph ether-TDI reaction product, gamma-omega-perfluoro-C8-20-alkylacrylate and stearyl acrylate","221455-62-5","D",0]
["2-Propenoic acid, 2-hydroxyethyl ester, polymers with gamma-omega-perfluoro-C8-20-alkyl acrylate and stearyl acrylate","221455-63-6","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymers with 2-hydroxyethyl methacrylate-5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexane-Me Et ketone oxime reaction product, gamma-omega-perfluoro-C8-20-alkyl acrylate and¿","221455-64-7","D",0]
["Acetic acid, trifluoro-, thallium(3+) salt","23586-53-0","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene ...","25190-89-0","D",0]
["N-Methylperfluorooctanesulfonamidoethyl acrylate","25268-77-3","D",0]
["Propane, 1,1,2,2,3,3-hexafluoro-1-[(trifluoroethenyl)oxy]-3-(trifluoromethoxy)-, polymer with 1,1-difluoroethene and tetrafluoroethene","252846-11-0","D",0]
["Pentafluoroiodoethane-tetrafluoroethylene telomer","25398-32-7","D",0]
["1-Nonene, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-","25431-45-2","D",0]
["p-(pentadecafluoroheptyl)benzenesulphonyl chloride","25444-35-3","D",0]
["N,N,N,-Triethylethanaminium 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","25628-08-4","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,isooctadecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-methoxypoly(oxy-1,2-ethanediyl),¿","256488-93-4","D",0]
["Ethene, tetrafluoro-, polymer with 1,1-difluoroethene","25684-76-8","D",0]
["Isobutylene-Tetrafluoroethylene copolymer","25684-89-3","D",0]
["Perfluoro(2-(2-phenoxypropoxy)propanoyl) fluoride","25711-77-7","D",0]
["Methanol, telomer with 1,1,2,2-tetrafluoroethene","25971-78-2","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-{[1,1,1,2,3,3-hexafluoro-3-({1,1,1,2,3,3-hexafluoro-3-[(trifluoroethenyl)oxy]propan-2-yl}oxy)propan-2-yl]oxy}propane","2599-84-0","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymers withN-(hydroxymethyl)-2-propenamide, gamma-omega-perfluoro-C8-16-alkyl acrylate andstearyl acrylate","260794-06-7","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymers with N-(hydroxymethyl)-2-propenamide, perfluoro-C8-16-alkyl acrylate, stearyl acrylate and vinyl chloride","260794-09-0","D",0]
["Polymer of tetrafluoroethylene-vinylacetate","26299-59-2","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 2-ethylhexyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, isooctadecyl 2-propenoate, 2-methyloxirane polymer withoxirane mono-2-propenoate, and alpha..","263260-98-6","D",0]
["Hexafluoropropene oxide trimer","2641-34-1","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with tetrafluoroethene","25067-11-2","D",0]
["3-[(Perfluorodecane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide","200636-64-2","D",0]
["4-Hydroxyphenyl nonafluorobutane-1-sulfonate","1463426-93-8","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(pentafluorophenyl)butanamide","60839-98-7","D",0]
["1-(Dimethylamino)-3-(perfluorohexyl)propan-2-ol","80233-98-3","D",0]
["Bis(perfluorohexyl) phosphinic acid erbium(3+) salt","500776-73-8","D",0]
["Acrylates/Perfluorohexylethyl methacrylate Copolymer is a copolymer of perfluorohexylethyl methacrylate, and one or more monomers consisting of acrylic acid, methoacrylic acid, or one of their simple esters","1557087-30-5","D",0]
["N-[4-(Heptafluoropropyl)phenyl]acetamide","199530-73-9","D",0]
["perfluoro[2-(2-methoxypropoxy)propanoic acid]","2479-73-4","D",0]
["14:2 Fluorotelomer sulfonamido propyl betaine","278598-47-3","D",0]
["12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,19-Heptadecafluorononadecan-1-ol","1512-02-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,20,20,21,21,21-Hentetracontafluorohenicosyl 2-methylprop-2-enoate","132405-54-0","D",0]
["HG–03","173350-37-3","D",0]
["Potassium perfluorodecanoate","51604-85-4","D",0]
["Copolymer of methyl perfluoro-3-(1-methyl-2-vinyloxyethoxy)propanoate and perfluoroethene (having 1,000 or more of number average molecular weight also insoluble in water, fat-soluble solvent, universally applicable solvent, acid and alkali)","509072-42-8","D",0]
["1,1,1,2,2,5,5,5-Octafluoro-4-(trifluoromethyl)pentane","90278-01-6","D",0]
["5,5'-(1,1,2,2,3,3-hexafluoropropane-1,3-diyl)bis(2h-tetrazole)","7401-42-5","D",0]
["1-(4-Chlorophenyl)-2,2,3,3,3-pentafluoropropan-1-one","781-97-5","D",0]
["1,1,2,2-Tetrafluoro-1,4-diiodobutane","755-95-3","D",0]
["Nonafluoropentanoyl bromide","159623-35-5","D",0]
["1-fluoro-1,3-bis(1,1,1,2,3,3,3-heptafluoropropan-2-yl)thiazirene","17886-82-7","D",0]
["Trimethyl[(2,2,3,3,3-pentafluoropropanoyl)oxy]stannane","876171-27-6","D",0]
["N,N'-(3,4-Dioxocyclobut-1-ene-1,2-diyl)bis(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonamide)","1234571-87-9","D",0]
["1,1,1,2,3,3-Hexafluoropropan-2-yl but-2-enoate","135771-94-7","D",0]
["4,4'-Bis(2-bromo-1,1,2,2-tetrafluoroethoxy)-1,1'-biphenyl","134130-29-3","D",0]
["2,2,3,3-Tetrafluoro-3-(pentafluorophenoxy)propanoic acid","88388-84-5","D",0]
["Phenol, 4,4'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis-, dipotassium salt","25088-69-1","D",0]
["Vinyl fluoride-Vinylidene fluoride-Chlorotrifluoroethylene copolymer","25101-38-6","D",0]
["Ethene, chlorotrifluoro-, polymer with ethene","25101-45-5","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1-chloro-1,2,2-trifluoroethene and 1,1-difluoroethene","25101-47-7","D",0]
["1-Butanol, 4-(ethenyloxy)-, polymer with 1,1,2,2-tetrafluoroethene","25120-52-9","D",0]
["2-(Perfluorododecyl)ethane-1-thiol","79840-60-1","D",0]
["4,4,5,5,6,6-Hexafluoro-2-phenyl-1lambda~6~,3lambda~6~-dithiane-1,1,3,3-tetrone","152192-93-3","D",0]
["2-(1,1,1,3,3,3-hexafluoropropan-2-ylidene)-3,4-dihydronaphthalen-1(2h)-one","35474-71-6","D",0]
["Ethene, tetrafluoro-, polymer with 1,1-difluoroethene and 1-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2,3,3,3-heptafluoropropane","349118-39-4","D",0]
["2,5-Bis(pentadecafluoroheptyl)-1,3,4-oxadiazole","1555-24-4","D",0]
["Bis(2-chloro-3,3,4,4,5,5-hexafluoro-1-cyclopenten-1-yl)mercury","49771-65-5","D",0]
["2,2,3,3,5,5,6,6-Octafluoro-4-(nonafluorocyclopentyl)morpholine","94718-25-9","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Tricosafluorotridec-1-ene","1270180-02-3","D",0]
["1-[4'-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutane-1-sulfonyl)-5'-methyl[2',3'-dihydro[2,3'-bifuran]]-2'-yl]ethan-1-one","771491-82-8","D",0]
["(4,4,5,5,6,6,6-Heptafluoro-2-iodohex-2-en-1-yl)(trimethyl)silane","89608-30-0","D",0]
["4-(Hydroxymethyl)-2,2-bis(trifluoromethyl)-1,3-oxazolidin-5-one","150582-54-0","D",0]
["2,2,3,3-Tetrafluoro-N-(2,2,3,3-tetrafluoropropyl)propan-1-amine","78650-56-3","D",0]
["4-Ethyl-2-(heptafluoropropyl)pyrimidine-5-carboxylic acid","914201-17-5","D",0]
["1-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-iodocyclohexane","4316-00-1","D",0]
["2,2,4,4-Tetrachloro-6,6-bis(2,2,3,3-tetrafluoropropoxy)-1,3,5,2lambda~5~,4lambda~5~,6lambda~5~-triazatriphosphinine","65601-40-3","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, compd. with piperidine (1:1)","71463-74-6","D",0]
["Icosafluorododecahydroacenaphthylene","307-07-3","D",0]
["2,2,3,3,4,4-Hexafluorobutyl 2-methylprop-2-enoate","45168-50-1","D",0]
["N-Cyclopropyl-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanamide","6395-49-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Octadecafluoro-1,9-diiodononane","22116-95-6","D",0]
["Ammonium bis(N-ethyl-2-perfluorooctylsulfonaminoethyl)phosphate","30381-98-7","D",0]
["2-Propenoic acid, 2-methyl-, polymers with 2-ethylhexyl methacrylate, N-(hydroxymethyl)-2-propenamide and 2-[methyl[(gamma-omega-perfluoro-C8-14-alkyl)sulfonyl]amino]ethyl acrylate","304012-61-1","D",0]
["Copolymer of 1,1-difluoroethylene-perfluoroethylene-chlorotrifluoroethylene (a number-average molecular weight is not less than 1,000 and polymer is insoluble in water, fat-soluble solvent, usual solvent, acid and alkali)","30421-59-1","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctylamine","30556-86-6","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,2-trifluoro-1-(trifluoromethyl)ethyl ester","3063-94-3","D",0]
["3-Ethoxy-1,1,1,2,3,4,4,5,5,6,6,6-dodecafluoro-2-(trifluoromethyl)-hexane","297730-93-9","D",0]
["S-((Perfluoro-7-(methyl)octyl)ethyl) thiomethacrylate","28506-33-4","D",0]
["Sevoflurane","28523-86-6","D",0]
["Perfluorodimethylcyclobutane","28677-00-1","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, homopolymer, syndiotactic (9CI)","287391-07-5","D",0]
["(Perfluorocyclohexyl)methanol","28788-68-3","D",0]
["trichloroheptafluorobutane","28984-80-7","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, homopolymer","29014-57-1","D",0]
["ammonium heptadecafluorooctanesulfonate","29081-56-9","D",0]
["Propane, 1,1,1,2,2,3,3-heptafluoro-3-[(1,2,2-trifluoroethenyl)oxy]-, polymer with ethene and 1,1,2,2-tetrafluoroethene","29087-71-6","D",0]
["Lithium heptadecafluorooctanesulfonate","29457-72-5","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, potassium salt (1:1)","29420-49-3","D",0]
["N-(4-(1,1,1,3,3,3-Hexafluoro-2-hydroxy-propan-2-yl)phenyl)-N-(2,2,2-trifluoroethyl)benzenesulfonamide","293754-55-9","D",0]
["Perfluoro(3-oxapent-4-ene)sulfonyl fluoride","29514-94-1","D",0]
["2-Methyl-3,3,4,4-tetrafluoro-2-butanol","29553-26-2","D",0]
["Bis(2-{ethyl[(perfluorooctyl)sulfonyl]amino}ethyl) hydrogen phosphate","2965-52-8","D",0]
["Perfluorononanesulfonate potassium","29359-39-5","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethoxy)propionyl fluoride","2927-83-5","D",0]
["2-[2,4-Bis(1,1-dimethylpropyl)phenoxy]-N-[4-[(2,2,3,3,4,4,4-heptafluoro-1-oxobutyl)amino]-3-hydroxyphenyl]-Hexanamide","2923-93-5","D",0]
["Potassium perfluoroundecanoate","30377-53-8","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C7 fraction","274917-97-4","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C8 fraction","274918-01-3","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C9 fraction","274918-02-4","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C10 fraction","274918-03-5","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, decarboxylated, C11 fraction","274918-09-1","D",0]
["1,1,3-Trihydroperfluoropropyl acrylate-Styrene copolymer","28501-21-5","D",0]
["Perfluoroeicosyl iodide","29809-34-5","D",0]
["Perfluorooctadecyl iodide","29809-35-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,20,20,21,21,22,22-pentatetracontafluoro-22-iododocosane","29809-36-7","D",0]
["sodium 1-(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl) 2-sulphonatobenzoate","29811-19-6","D",0]
["Vinyl 1H,1H,3H-perfluoropropyl ether","29819-80-5","D",0]
["2-(N-Ethylperfluorooctanesulfonamido)acetic acid","2991-50-6","D",0]
["Potassium N-ethyl-N-[(heptadecafluorooctyl)sulphonyl]glycinate","2991-51-7","D",0]
["Ammonium 2-(N-ethylperfluorooctanesulfonamido)acetate","2991-52-8","D",0]
["(6H-Perfluorohexyl)methyl acrylate","2993-85-3","D",0]
["Perfluoro-1,2-dimethylcyclobutane","2994-71-0","D",0]
["1,2-Benzenedicarboxylic acid, 4,4'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis-","3016-76-0","D",0]
["Perfluoro-2,7-dimethyloctane","3021-63-4","D",0]
["[3-(Heptadecafluorooctylsulfonylamino)propyl]dimethylamine N-oxide","30295-51-3","D",0]
["1-Hexanesulfonamide, N-[3-(dimethyloxidoamino)propyl]-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","30295-56-8","D",0]
["Perfluoro-3-ethyl-2,4-dimethyl-2-pentene","30320-26-4","D",0]
["Perfluoro(3-isopropyl-4-methyl-2-pentene)","30320-27-5","D",0]
["Perfluorobutanesulfonamide","30334-69-1","D",0]
["ethyl perfluorononan-1-oate","30377-52-7","D",0]
["sodium undecafluorohexanoate","2923-26-4","D",0]
["Sodium 2,2,3,3-tetrafluoropropionate","22898-01-7","D",0]
["Ammonium 2-(perfluorohexyl)ethyl hydrogen phosphate","2353-52-8","D",0]
["1,2-dichloro-1,1,2-trifluoro-2-(trifluoromethoxy)ethane","2356-53-8","D",0]
["Perfluorooctylsulfonylpropylaminoethyl acrylate","2357-60-0","D",0]
["2-Propenoic acid, butyl ester, polymer with ethenyl chloroacetate, ethyl 2-propenoate, 2,2,3,3,4,4,5,5-octafluoropentyl 2-propenoate and 2,2,3,3-tetrafluoropropyl 2-propenoate (9CI)","235775-84-5","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymers with N,N-dimethyl-2-propenamide, gamma-omega-perfluoro-C8-20-alkyl acrylate and vinylchloride","221455-67-0","D",0]
["2-Propenoic acid, reaction products with N-[3-(dimethylamino)propyl]-1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonamide","212335-64-3","D",0]
["1,2,2,2-Tetrafluoroethanesulfonyl fluoride","2127-74-4","D",0]
["Butyl acrylate modified ethylene and chlorotrifluoroethylene, polymer","213188-00-2","D",0]
["Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, salt with perfluoro-1-octanesulfonic acid (1:1)","213740-80-8","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,methyloxirane polymer with oxirane mono-2-propenoate butyl ether, and 2-propenoic acid (9CI)","214002-95-6","D",0]
["1,1,1,2,2-pentafluoro-6,6-dimethylheptane-3,5-dione","2145-68-8","D",0]
["1,1,2,3,4,4,4-heptafluoro-3-(trifluoromethyl)but-1-ene","21581-82-8","D",0]
["Hexafluoroisopropyl acrylate","2160-89-6","D",0]
["2,4,6-tris(pentadecafluoroheptyl)-1,3,5-triazine","21674-38-4","D",0]
["Siloxanes and Silicones, di-Me, mono[3-[(2-methyl-1-oxo-2-propen-1-yl)oxy]propyl group]-terminated, polymers with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl methacrylate,3a,4,7,7a,-hexahydro-4,7-methano-1H-indenyl acrylate¿","218286-10-3","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 2-ethylhexyl-2-propenoate, 2-[(heptadecafluorooctyl)sulfonyl]propylamino]ethyl-2-propenoate and .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-hydroxypoly[oxy(methyl-1,2-ethanediyl)]","218448-95-4","D",0]
["2-Propenoic acid, 2-ethylhexyl ester, polymer with 2-[[(heptadecafluorooctyl)sulfonyl]propylamino]ethyl, 2-propenoate and .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-hydroxypoly(oxy-1,2-ethanediyl)","218448-99-8","D",0]
["Dimethyl 2-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-1,3-propanedioate","220075-01-4","D",0]
["Sulfonium, dimethylphenyl-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonic acid(1:1)","220133-51-7","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, telomer with chlorotrifluoroethene, oxidized, reduced, Et ester, hydrolyzed","220182-27-4","D",0]
["1-Octadecanamine, reaction products with Et esters of reduced polymd. oxidized tetrafluoroethylene","220207-10-3","D",0]
["Glycine, N,N-bis[2-hydroxy-3-(2-propen-1-yloxy)propyl]-, sodium salt(1:1), reaction products with ammonium hydroxide and 1,1,1,2,2-pentafluoro-2-iodoethane-tetrafluoroethylene telomer","220459-70-1","D",0]
["tetrabutyl-phosphonium nonafluoro-butane-1-sulfonate","220689-12-3","D",0]
["Ammonium 2,2,3,3,4,4,5,5-octafluorovalerate","22715-45-3","D",0]
["(E)-1,3,3,3-Tetrafluoroprop-1-ene","29118-24-9","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[2-[ethyl[(heptadecafluorooctyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","29117-08-6","D",0]
["Polymer(ethylene/tetrafluoroethylene/propylene)","29697-44-7","D",0]
["Siloxanes and Silicones, 3-aminopropyl ethoxy, ethoxy(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl), polymers with 3-aminopropyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silsesquioxanes, hydrolyzed, formates (salts)","297175-70-3","D",0]
["Copper, [C,C,C,C-tetrakis(pentadecafluoroheptyl)-29H,31H-phthalocyaninato(2-)-N29,N30,N31,N32]-","29763-53-9","D",0]
["Propane, 1,1,1,2,2,3,3-heptafluoro-3-((trifluoroethenyl)oxy)-, polym...","26655-00-5","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymers with N-(hydroxymethyl)-2-propenamide, gamma-omega-perfluoro-C8-20-alkyl acrylate andvinyl chloride","221455-71-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, reaction products with 5-isocyanato-1-(isocyanatomethyl)-1,3,3-trimethylcyclohexane and Me Etketone oxime, polymers with 2-ethylhexyl acrylate, 2-hydroxyethyl acrylate..","221455-72-7","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with gamma-omega-perfluoro-C8-20-alkyl acrylate","221455-73-8","D",0]
["Sodium perfluorobutanoate","2218-54-4","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with poly(Bu acrylate) and polyethylene-polypropylene glycol mono-Bu ether","222716-67-8","D",0]
["2,3,3,3-Tetrafluoro-2-(2,3,4,5,6-pentafluorophenoxy)-propanoyl fluoride","22304-57-0","D",0]
["1-Propanamine, 3-(triethoxysilyl)-, reaction products with Et esters of reduced polymd. oxidized poly(tetrafluoroethylene)","223557-70-8","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, polymers with 5-amino-1,3,3-trimethylcyclohexanemethanamine, carbonic acid, 1,6-diisocyanatohexane,1,6-hexanediol, 1,1'-methylenbis[4-isocyanatocyclohexane] andtrimethylolpropane","223586-53-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymers with gamma-omega-perfluoro-C8-20-alkyl acrylate and polyethylene glycol monomethacrylate","224790-87-8","D",0]
["2-Propenoic acid, gamma-omega-perfluoro-C8-20-alkyl esters, polymers withpolyethylene glycol monomethacrylate and polypropylene glycolmonomethacrylate","224790-97-0","D",0]
["N,N',N''-(Phosphinylidynetris(oxyethane-2,1-diyl))tris(N-ethylheptadecafluorooctane-1-sulphonamide)","2250-98-8","D",0]
["1,2,3,3,3-Pentafluoropropene","2252-83-7","D",0]
["1,1,1,2,2,3,3-Heptafluoropropane","2252-84-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl methacrylate","2261-99-6","D",0]
["N-Butylheptadecafluoro-N-(2-hydroxyethyl)octanesulphonamide","2263-09-4","D",0]
["1,3-Bis[4-(ethenyloxy)butyl] 2-(perfluorohexyl)ethylpropanedioate","226409-30-9","D",0]
["N-Propylperfluorooctanesulfonamide","2266-83-3","D",0]
["1,1,1,3-Tetrachlorotetrafluoropropane","2268-46-4","D",0]
["Silane, triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)-","146090-84-8","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-methyl-N-[(3-octadecyl-2-oxo-5-oxazolidinyl)methyl]","306974-19-6","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-(hydroxyethyl)-N-methyl, reaction products with 12-hydroxyoctadecanoic acid and 2,4-TDI, ammonium salts","306973-47-7","D",0]
["Pyridinium, 1-[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-, inner salt","254889-10-6","D",0]
["Siloxanes and Silicones, di-Me, mono[3-[(2-methyl-1-oxo-2-propen-1-yl)oxy]propyl group]-terminated, polymers with 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl acrylate and stearyl methacrylate","306974-28-7","D",0]
["Sulfonic acids, C6-8-alkane, perfluoro, compds. with polyethylene-polypropylene glycol bis(2-aminopropyl) ether","306974-45-8","D",0]
["Fatty acids, C18-unsatd., dimers, 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl esters","306974-63-0","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-[3-(dimethylamino)propyl], reaction products with acrylic acid","192662-29-6","D",0]
["2-Propenoic acid, 2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethyl ester, polymer with 2-[methyl[(nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-omega-hydroxypoly(oxy-1,2-ethanediyl), alpha-(2-methyl-1-oxo ¿","68586-13-0","D",0]
["1,1,1,3-Tetramethyl-3,3-bis(1,1,2,2,3,3,6,6,6-nonafluorohexyl)disiloxane","122179-35-5","D",0]
["1202381-95-0 (name too long)","1202381-95-0","D",0]
["Potassium 1,1,2,2-tetrafluoro-2-(pentafluoroethoxy)ethane-1-sulfonate","117205-07-9","D",0]
["Perfluoro(2-ethoxyethanesulfonic acid)","113507-82-7","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymers with N-(hydroxymethyl)-2-propenamide, 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl methacrylate, stearyl methacrylate and vinylidene chloride","306975-85-9","D",0]
["1-Hexadecanaminium, N,N-dimethyl-N-[2-[(2-methyl-1-oxo-propen-1-yl)oxy]ethyl]-, bromide (1:1), polymers with Bu acrylate, Bu methacrylate and 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl acrylate","306976-25-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-methylpropyl ester, polymer with 2,4-diisocyanato-1-methylbenzene, 2-ethyl-2-(hydroxymethyl)-1,3-propanediol and 2-propenoic acid, N-ethyl-N-(hydroxyethyl)perfluoro-C4-8-alkanesulfonamides-blocked","306976-55-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, telomer with 2-[ethyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl methacrylate and 1-octanethiol, N-oxides","306977-10-6","D",0]
["2-Propenoic acid, 2-methyl-, 3-(trimethoxysilyl)propyl ester, polymers with acrylic acid, 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl acrylate and propylene glycol monoacrylate, hydrolyzed, compds. with 2,2'-(methylimino)bis[ethanol]","306977-58-2","D",0]
["2-Propenoic acid, butyl ester, polymers with acrylamide, 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl acrylate and vinylidene chloride","306978-04-1","D",0]
["Hexane, 1,6-diisocyanato-, homopolymer, N-(hydroxyethyl)-N-methylperfluoro-C4-8-alkanesulfonamides- and stearyl alc.-blocked","306978-65-4","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N,N'-[1,6-hexanediylbis[(2-oxo-3,5-oxazolidinediyl)methylene]]bis[N-methyl-","306980-27-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl ester, polymers with polyethylene glycol acrylate Me ether","504396-13-8","D",0]
["Siloxanes and Silicones, di-Me, 3-hydroxypropyl group-terminated, reaction products with Me Et ketone oxime, 2-mercaptoethanol, 2-[methyl[(perfluoro-C3-8-alkyl)sulfonyl]amino]ethyl acrylate, polymethylenepolyphenylene isocyanate and polypropylene ¿","507225-08-3","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl ester, polymer with octadecyl 2-propenoate and 2-propenoic acid","67906-71-2","D",0]
["Hexane, 1-(ethenylsulfinyl)-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","680187-85-3","D",0]
["Triethoxy(1,1,2,2,3,3,6,6,6-nonafluorohexyl)silane","102390-98-7","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10¿","1094598-90-9","D",0]
["2-Propenoic acid, 2-methyl-, polymers with 2-(dimethylamino)ethylmethacrylate, Me methacrylate, gamma-omega-perfluoro-C8-16-alkyl acrylate undvinylpyrrolidone¿","1223402-68-3","D",0]
["2-Propenoic acid, polymer with butyl 2-propenoate und 2,5-furundione, gamma-omega-perfluoro-C8-14-alkyl esters, tert-Bu 2-ethylhexaneperoxoate-initiated,compds. with 2-(dimethylamino)ethanol","1264198-78-8","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, reactionproducts with [(trimethylsilyl)oxy]-modified silica","254889-67-3","D",0]
["Benzene, 1-nitro-4-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","171561-95-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymer with 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate, 2 ¿","68797-76-2","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[[[5-[[[4-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]butoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl ester, telomer with butyl 2-propenoate, 2-[[(1,1,2,2,3,3,4,4,5 ¿","70900-40-2","D",0]
["1-Hexanesulfonamide, N-[3-(dimethylamino)propyl]-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, acetate (1:1)","73772-33-5","D",0]
["1-Hexanesulfonamide, N-[3-(dimethylamino)propyl]-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-[2-[2-(2-hydroxyethoxy)ethoxy]ethyl]-","73772-34-6","D",0]
["Benzene, 1-chloro-4-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","76848-59-4","D",0]
["1H-Benzimidazolium, 1,3-diethyl-2-methyl-5-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-, 4-methylbenzenesulfonate (1:1)","76848-68-5","D",0]
["Thiophene, 2-[2-[(tridecafluorohexyl)sulfonyl]ethenyl]-","86525-43-1","D",0]
["Furan, 2-[2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethenyl]-","86525-48-6","D",0]
["Benzene, 1-methyl-4-[2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethenyl]-","86525-51-1","D",0]
["Benzene, 1-methoxy-4-[2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethenyl]-","86525-52-2","D",0]
["Thiophene, 2-[1-(phenylthio)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-48-9","D",0]
["Furan, 2-[1-(phenylthio)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-49-0","D",0]
["Benzene, 1-methyl-4-[1-(phenylthio)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-50-3","D",0]
["Thiophene, 2-[1-(nitromethyl)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-55-8","D",0]
["Furan, 2-[1-(nitromethyl)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-56-9","D",0]
["2,4-Pentanedione, 3-[1-(2-thienyl)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-63-8","D",0]
["2,4-Pentanedione, 3-[1-(2-furanyl)-2-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]ethyl]-","89863-64-9","D",0]
["Isoxazolidine, 4-(4-methoxyphenyl)-2-methyl-5-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","93416-31-0","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-[4,7-dimethyl-4-[[(1-methylpropylidene)amino]oxy]-3,5-dioxa-6-aza-4-silanon-6-en-1-yl]-N-ethyl","944578-05-6","D",0]
["Hexane, 1-(ethenylsulfonyl)-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","680187-86-4","D",0]
["Benzoic acid, 4-[2,2,2-trifluoro-1-hydroxy-1-(trifluoromethyl)ethyl]-","16261-80-6","D",0]
["N-(2-Bromo-4,4,5,5-tetrafluoro-3-oxo-1-phenylpent-1-en-1-yl)hypobromous amide","143674-86-6","D",0]
["3,4,4,4-Tetrafluoro-1-iodo-3-(trifluoromethyl)-1-butene","243139-61-9","D",0]
["7,7,8,8,9,9,10,10,10-Nonafluoro-5-iododecan-2-one","109574-82-5","D",0]
["Acetic acid--2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptan-1-ol (1/1)","87925-96-0","D",0]
["2-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)oxy]ethan-1-ol","54949-99-4","D",0]
["1-Heptanol, 4,4,5,5,6,6,7,7,7-nonafluoro-","83310-97-8","D",0]
["Butane, 1,1,1,2-tetrafluoro-4-iodo-2-(trifluoromethyl)-","99324-96-6","D",0]
["1,1'-Plumbanediylbis(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyloctane-3,5-dione)","21600-78-2","D",0]
["1,1,2,2-Tetrafluoro-1,2-dihydroacenaphthylene","21846-40-2","D",0]
["4,5,5,5-Tetrafluoro-4-(heptafluoropropoxy)pentanoic acid","243128-40-7","D",0]
["5-[1,2,2,2-Tetrafluoro-1-(heptafluoropropoxy)ethyl]furan-2(5H)-one","143327-96-2","D",0]
["2-(Chlorodifluoromethyl)-1,1,1,3,3,3-hexafluoropropane","1559-48-4","D",0]
["Octafluoro-1-Pentanol","39660-55-4","D",0]
["1-(Prop-1-en-2-yl)-2-(2,2,3,3,4,4,5,5,6,6,6-undecafluorohexyl)benzene","676273-93-1","D",0]
["2-{[4-(Heptafluoropropyl)phenyl]methyl}oxirane","144006-68-8","D",0]
["(Perfluoropropyl)chloromethyl-2,4-difluorophenylmethanol","92737-03-6","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecyl)sulfonyl]propanoic acid","54207-74-8","D",0]
["n-(2-chloroethyl)-2,2,3,3,4,4,4-heptafluorobutanamide","4314-29-8","D",0]
["N-Ethenyl-heptadecafluoro-N-methyl-1-octanesulfonamide","87988-66-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodoheptadecane","129838-39-7","D",0]
["3-Chloro-4-[4-(1,1,2,3,3,3-hexafluoropropoxy)phenoxy]aniline","83660-69-9","D",0]
["Benzyl (1,1,1,3,3,3-hexafluoropropan-2-ylidene)carbamate","128229-95-8","D",0]
["4H,4H-Decafluoroheptane-3,5-dione","38007-33-9","D",0]
["1-(Anthracen-2-yl)-4,4,5,5,5-pentafluoropentane-1,3-dione","819060-51-0","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propen-1-yl)- ¿","68227-94-1","D",0]
["2-Propenoic acid, ethyl ester, polymer with 4-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]butyl 2-propenoate, 4-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]butyl 2-propenoate, alpha-(2-methyl-1-oxo ¿","68228-00-2","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-(phenylmethyl)-","68298-09-9","D",0]
["2-Propenoic acid, 2-methyl-, 4-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]butyl ester, telomer with butyl 2-propenoate, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2 ¿","68299-39-8","D",0]
["Methyl perfluorooctadecanoate","16753-33-6","D",0]
["Ethyl 2,2,3,4,4,4-hexafluorobutanoate","5200-38-4","D",0]
["1-Octene, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, polymer with ethene and 1,1,2,2-tetrafluoroethene","69288-57-9","D",0]
["Perfluoropropanamine","105579-92-8","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl phosphate","1411713-84-2","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-tridecafluoro-2-methyldec-3-yn-2-ol","82721-70-8","D",0]
["1‐Bromo‐1‐chloro‐2‐(difluoromethoxy)‐1,2,2‐trifluoroethane","31702-61-1","D",0]
["2-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]ethan-1-ol","104568-28-7","D",0]
["2-Pentynoic acid, 4,4,5,5,5-pentafluoro-, ethyl ester","129922-54-9","D",0]
["2,3,5,6-Tetrafluoro-4-[(pentafluoroethyl)sulfanyl]pyridine","162147-73-1","D",0]
["Cyclopentene, 1-methoxyheptafluoro-","1759-60-0","D",0]
["bis(2,2,3,3,4,4,5,5-octafluoropentyl) 3-methylpentanedioate","376-94-3","D",0]
["3,3,4,4,5,5,6,6-Octafluorooctane-1,8-diamine","94403-06-2","D",0]
["Triethoxy{3-[(heptadecafluorooctyl)oxy]propyl}silane","88101-78-4","D",0]
["4-(2-Ethoxyphenyl)-5-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]-2,4-dihydro-3H-1,2,4-triazole-3-thione","7168-26-5","D",0]
["1,2,2,3,3,4,5,5,6,6-Decafluor-4-pentafluorethylcyclohexanesulfonic acid","646-83-3","D",0]
["Hexanamide, 2-[2,4-bis(1,1-dimethylpropyl)phenoxy]-N-[3-hydroxy-4-[(octafluoro-1-oxopentyl)amino]phenyl]-","83003-52-5","D",0]
["N-(2-Hydroxyethoxy)ethyl-N-propylperfluorooctanesulfonamide","102579-26-0","D",0]
["1-(ethoxymethyl)-3-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)urea","27942-17-2","D",0]
["1,1,2,2-tetrafluoropropane","40723-63-5","D",0]
["Poly(difluoromethylen), alpha-(2-hydroxyethyl)-omega-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]- (9CI)","761418-87-5","D",0]
["(1E)-1,2,3,3,4,4,5,5,6,6,6-Undecafluoro-1-methoxyhex-1-ene","62949-64-8","D",0]
["2-(4,4,5,5,6,6,6-heptafluorohexyl)propanedioic Acid","244022-64-8","D",0]
["Perfluorocyclohexane sulfonic acid","2106-55-0","D",0]
["N,N-Diethyl-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptanethioamide","61906-64-7","D",0]
["Diphenylbis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)stannane","96325-94-9","D",0]
["Poly( oxy-1 ; 2-ethanedilyl), alpha-methyl--[(4, 4, 5, 5, 6, 6, 7, 7, 8, 8, 9, 9-tridecafluoro-2-hydroxynonyl) oxy]-","1227060-33-4","D",0]
["Poly[1,4-phenylene(1,1,2,2-tetrafluoro-1,2-ethanediyl)]","25669-37-8","D",0]
["Propanamide, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-N-[3-(,4,6,8-tetramethylcyclotetrasiloxan-2-yl)propyl]- (9CI)","173524-60-2","D",0]
["Propanamide, N-[3-(ethenyldimethylsilyl)phenyl]-2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-N-methyl- (9CI)","185438-14-6","D",0]
["Propanenitrile, 3,3'-[[4-[[2-bromo-4-nitro-6-(trifluoromethyl)phenyl]azo]phenyl]imino]bis- (9CI)","246871-16-9","D",0]
["Propanoyl fluoride, 2,2'-[(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis(oxy)]bis[2,3,3,3-tetrafluoro-, polymer with trifluoro(trifluoromethyl)oxirane, reaction produts with 3-(ethenyldimethylsilyl)-N-methylbenzenamine","166242-54-2","D",0]
["Siloxanes and Silicones, di-Me, Me 3,3,3-trifluoropropyl, hydroxy- and vinyl group-terminated","110475-04-2","D",0]
["Siloxanes and Silicones, di-Me, Me 3,3,3-trifluoropropyl, Me vinyl,hydroxy- and vinyl group-terminated","133649-92-0","D",0]
["Siloxanes and Silicones, Me 3,3,3-trifluoropropyl","63148-56-1","D",0]
["Siloxanes and Silicones, Me 3,3,3-trifluoropropyl, ((ethenyldimethylsilyl)oxy)-terminated","68037-88-7","D",0]
["Siloxanes and Silicones, Me 3,3,3-trifluoropropyl, hydroxy-terminated","68607-77-2","D",0]
["Siloxanes and Silicones, Me 3,3,3-trifluoropropyl, Me vinyl, hydroxy-terminated","68952-02-3","D",0]
["Siloxanes and Silicones, Me hydrogen, Me 3,3,3-trifluoropropyl","67923-24-4","D",0]
["Siloxanes and Silicones, Me Ph, Me 3,3,3-trifluoropropyl","1643944-25-5","D",0]
["Tetrachlorotrifluoropropane","29470-95-9","D",0]
["Trans-1,3,3,3-tetrafluoropropene","1645-83-6","D",0]
["1-Bromo-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzene","2396-22-7","D",0]
["N-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl)Maleimide","852527-40-3","D",0]
["N-[5-(Heptafluoropropyl)[1,1'-biphenyl]-2-yl]benzamide","748785-00-4","D",0]
["1-Propene, 1-chloro-3,3,3-trifluoro-, (1E)-","102687-65-0","D",0]
["1H-Indene, 5-[4'-[difluoro(3,4,5-trifluorophenoxy)methyl]-2,3',5'-trifluoro[1,1'-biphenyl]-4-yl]-2,3-dihydro-2-propyl-","1357385-67-1","D",0]
["2,2,2-Trifluoroethanol","75-89-8","D",0]
["2,2,2-Trifluoroethyl acrylate","407-47-6","D",0]
["Phenol, 4,4'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis-, reaction products with benzene, chlorine and sulfur chloride (S2Cl2)","921213-47-0","D",0]
["HG–21","249932-26-1","D",0]
["Octan-2-yl heptafluorobutanoate","560-01-0","D",0]
["1-Chloro-1-(difluoromethoxy)-1,2,2,2-tetrafluoroethane","57041-64-2","D",0]
["Methyl 3-(chlorosulfanyl)-2,2,3,3-tetrafluoropropanoate","77705-95-4","D",0]
["Perfluoro-1-ethyl-2-methylcyclohexane","96009-78-8","D",0]
["5-Methyl-2-(1,2,2,2-tetrafluoroethyl)pyridine","16876-49-6","D",0]
["1,1,2,2,3,3-Hexafluoro-2,3-dihydro-1H-indene","2338-64-9","D",0]
["(Pentafluoroethyl)(diphenyl)phosphane","20157-74-8","D",0]
["2,2,3-Trifluoro-3-(heptafluoropropoxy)propanoic acid","824393-42-2","D",0]
["4-methyl-6-(2,2,3,3,4,4,5,5-octafluoropentoxy)pyrimidin-2-amine","5483-61-4","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","71864-97-6","D",0]
["1H,5H-Perfluoropentane","755-23-7","D",0]
["1,3-Bis(1,1,2,2-tetrafluoroethoxy)propane","138845-14-4","D",0]
["Ethyl 4-[(nonafluorobutyl)sulfanyl]benzoate","1262679-06-0","D",0]
["Perfluoro-1-propanol","53520-89-1","D",0]
["N,N-Diethyl-1,1,2,2,2-pentafluoroethan-1-amine","61881-20-7","D",0]
["1,1,1,5,5,6,6,7,7,8,8,8-dodecafluorooctane-2,4-dione","261503-40-6","D",0]
["Copolymer of chloroethene, octadecan-1-yl acrylate, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-yl methacrylate","1620760-72-6","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-[(4-sulfamoylphenyl)methyl]butanamide","165618-97-3","D",0]
["3-[{3-[(Carboxymethyl)(perfluorodecanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["Benzene, 1-fluoro-4-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","149652-30-2","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with 2-ethyl-1-hexanol and polymethylenepolyphenylene isocyanate","160901-25-7","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with 2-ethyl-1-hexanol, Me Et ketone oxime and polymethylenepolyphenylene isocyanate","160901-26-8","D",0]
["Fatty acids, C18-unsatd., trimers, 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl esters","161074-58-4","D",0]
["9-Octadecenoic acid (9Z)-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","167289-73-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with 1,1-dichloroethene, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, ¿","112311-93-0","D",0]
["2-Propenoic acid, 2-methyl-, octadecyl ester, polymer with 1,1-dichloroethene, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, ¿","112328-98-0","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, ...","119973-84-1","D",0]
["Siloxanes und Silicones, di-Me, 3-hydroxypropyl group-terminated,polymers with 2-butyne-1,4-diol-gamma-omega-perfluoro C10-20 thiol reactionproduct und 1,6-diisocyanato-2,2,4(or 2,4,4)-trimethylhexane","127133-54-4","D",0]
["Silane, trichloro(heptadecafluorodecyl)-","146443-00-7","D",0]
["1-Decanesulfonic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, ammonium salt (1:1)","149724-40-3","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers withBu acrylate, gamma-omega-perfluoro-C8-14-alkyl acrylate und polyethylene glycolmonomethacrylate","150409-17-9","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers withacrylonitrile, gamma-omega-perfluoro-C8-14-alkyl acrylate, polyethylene glycolmonomethacrylate und styrene","150409-18-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers withMe methacrylate, gamma-omega-perfluoro-C8-14-alkyl acrylate, polyethylene glycolmonomethacrylate und stearyl methacrylate","150409-19-1","D",0]
["Silane, diethoxy(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)methyl-","152992-46-6","D",0]
["Imidodicarbonic diamide, N,N',2-tris(6-isocyanatohexyl)-, reaction productswith glycidol, hydrolyzed ethylene-pentafluoroiodoethane-tetrafluoroethylene telomer reaction product and stearyl alc.","162491-88-5","D",0]
["Trisiloxane, 3-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-1,1,1,3,5,5,5-heptamethyl-","163921-85-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymers with N-(hydroxymethyl)-2-methyl-2-propenamide and gamma-omega-perfluoro-C10-16-alkylacrylate","200295-54-1","D",0]
["2-Propenoic acid, 2-methyl-, butyl ester, polymers with 2-ethylhexylmethacrylate, N-(hydroxymethyl)-2-methyl-2-propenamide and gamma-omega-perfluoro-C10-14-alkyl methacrylate","200295-55-2","D",0]
["Alkenes, C8-14 alpha, gamma-omega-perfluoro","210432-72-7","D",0]
["Butanedioic acid, 2-methylen-, 4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl) ester","230295-05-3","D",0]
["2-Propenoic acid, 2-methyl-,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecylester, polymer with N-(butoxymethyl)-2-methyl-2-propenamide, dodecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-¿","247109-50-8","D",0]
["2-Propen-1-ol, reaction products with 1,1,1,2,2-pentafluoro-2-iodoethane-tetrafluoroethylene telomer, dehydroiodinated, reaction products withepichlorohydrin and triethylenetetramine","464178-90-3","D",0]
["2-Propenoic acid, delta-omega-perfluoro-C9-15-alkyl esters","671756-62-0","D",0]
["Fatty acids, C18-unsatd., trimers, 2-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl esters","148240-80-6","D",0]
["1,1'-Peroxybis(2,2,3,3,4,4,5,5-octafluorocyclopentan-1-ol)","106813-72-3","D",0]
["1-Aziridinepropionic acid, 2,2,3,3,3-pentafluoropropyl ester","24116-27-6","D",0]
["1,1,1,2,2,3,3,4,4,12,12,13,13,14,14,15,15,15-Octadecafluoro-6,10-diiodopentadecane","40735-25-9","D",0]
["1,1'-Peroxybis(2,2,3,3,4,4,5,5,6,6-decafluorocyclohexan-1-ol)","106813-73-4","D",0]
["Allyl perfluoroisopropyl ether","15242-17-8","D",0]
["Butanedioic acid, monopolyisobutylene derivs.,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","253683-00-0","D",0]
["1-Tridecanaminium, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro-2-hydroxy-N,N-bis(2-hydroxyethyl)-N-methyl-, iodide (1:1)","93776-17-1","D",0]
["2H-Pyran, 2,2,3,3,4,4,5,5,6-nonafluorotetrahydro-6-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-nonadecafluorononyl)-","68155-54-4","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8- heptadecafluoro-, ion(1-)","45298-90-6","D",0]
["Imidodicarbonic diamide, N,N',2-tris(6-isocyanatohexyl)-, reaction products with3-chloro-1,2-propanediol, ethylene, iodoethane and tetrafluoroethylene","254889-72-0","D",0]
["Methanol, reaction products with 1,6-diisocyanatohexane, ethylene, ethyleneoxide, iodoethane and tetrafluoroethylene","254889-79-7","D",0]
["2-Propenoic acid, reaction products with acetic acid (gamma-omega-perfluoro-C8-10-alkyl)thio derivs. Bu esters und polyethylenimine","1374418-39-9","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymers with gamma-omega-perfluoro-C8-16-alkyl methacrylate, stearyl methacrylate und tridecylmethacrylate","1221681-75-9","D",0]
["Butanoic acid, 3-oxo-, 2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl ester,polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate¿","1430799-96-4","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10¿","1429174-38-8","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymers with 2-(methyl((perfluoro-C4-8-alkyl)sulfonyl)amino)ethyl acrylate and vinylidene chloride","306975-62-2","D",0]
["1-Hexanesulfonyl bromide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","111393-39-6","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N,N-dimethyl-","1270179-82-2","D",0]
["1-Hexanesulfonamide, N,N-diethyl-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","1270179-93-5","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-methyl-N-(2-oxiranylmethyl)","129813-71-4","D",0]
["â-Alanine, N-[3-(dimethylamino)propyl]-N-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","141607-32-1","D",0]
["1-Hexanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-methyl-","1427176-17-7","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N,N-bis(2-methoxyethyl)-","1427176-20-2","D",0]
["Benzenamine, 4-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","147029-28-5","D",0]
["1,1,2,2-Tetrafluoro-3-iodopropane","679-87-8","D",0]
["4,4-bis(Trifluoromethyl)-4-fluoropropanoic acid","243139-62-0","D",0]
["2,4,6-Tris(undecafluoropentyl)-1,3,5-triazine","23790-50-3","D",0]
["2‐{[2‐(Acetyloxy)‐3-(perfluorohexyl)propyl]dimethylazaniumyl}acetate","80234-02-2","D",0]
["1-Chloro-1,1,2,2-tetrafluoro-2-(pentafluoro-lambda~6~-sulfanyl)ethane","646-63-9","D",0]
["(1E)-4,4,5,5,6,6,6-Heptafluoro-1-iodo-3,3-bis(trifluoromethyl)-1-hexene","126681-21-8","D",0]
["1-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methylbenzene","51114-10-4","D",0]
["1,3-Dinitro-5-{[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)oxy]methyl}benzene","138528-18-4","D",0]
["1-[1,2,2,2-tetrafluoro-1-(heptafluoropropoxy)ethoxy]propan-2-one","851224-03-8","D",0]
["Perfluorononanoate","72007-68-2","D",0]
["4-{2-[3,4-Bis(methoxycarbonyl)phenyl]-1,1,1,3,3,3-hexafluoropropan-2-yl}benzene-1,2-dicarboxylic acid","136403-85-5","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluoropentyl)sulfonyl]amino)-1-propanesulfonate","2089108-90-5","D",0]
["p-((1,1,2,2-Tetrafluoroethyl)thio)aniline","713-63-3","D",0]
["Hexakis(2,2,3,3,4,4,4‐heptafluorobutoxy)‐ 1,3,5,2lambda5,4lambda5,6lambda5‐ triazatriphosphinine","470-73-5","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-methylnon-2-ene","112343-55-2","D",0]
["1,4-Bis(perfluoropropyl)butane","377-06-0","D",0]
["3,3,4,4,5,5,6,6,6‐Nonafluorohexanoic acid","70887-89-7","D",0]
["1,2,2,3,3,4-Hexafluorobutane","114810-02-5","D",0]
["3-[(12,12,13,13,14,14,15,15,15-Nonafluoropentadecanoyl)oxy]-4-(trimethylazaniumyl)butanoate","142674-37-1","D",0]
["N-[(4-Bromophenyl)(perfluorobutyl)-λ4-sulfanylidene]acetamide","1178899-27-8","D",0]
["Perfluoro-8-methoxyoctanesulfonic acid","914070-83-0","D",0]
["3,3,4,4,5,5,6,6,7,7-Decafluoro-1,2-dithiepane","24345-54-8","D",0]
["Triphenyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)phosphanium iodide","94190-73-5","D",0]
["1-Chloro-1,1,2,3,3,4,4-heptafluoro-4-iodo-2-(trifluoromethyl)butane","677-90-7","D",0]
["2-[2,2,2-Trifluoro-1-(trifluoromethyl)ethyl]benzothiazole","66172-01-8","D",0]
["5,6-Dichloro-2-(pentafluoroethyl)-1H-imidazo[4,5-b]pyrazine","53338-41-3","D",0]
["2,3,3,3-Tetrafluoro-2-(fluorosulfonyl)propanoyl fluoride","754-41-6","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-N-[(4-sulfamoylphenyl)methyl]pentanamide","165618-98-4","D",0]
["Methyl 4,4,5,5,6,6,6-heptafluoro-3,3-dihydroxyhexanoate","89148-14-1","D",0]
["Ethyl 2-acetyl-3,3,4,4,5,5,5-heptafluoropentanoate","189237-57-8","D",0]
["Methyl 3,3,4,4,5,5,6,6,6-nonafluoro-2-oxohexanoate","74067-16-6","D",0]
["1,1,1,2,2,3,3,4,5,6,6,6-Dodecafluorohexane","142347-11-3","D",0]
["Perfluoro-2-(trifluoromethoxy)ethanesulfonyl fluoride","139747-75-4","D",0]
["Perfluoro-2(1-propoxy)perfluoropropanamide","13140-35-7","D",0]
["1,2,3,4,5-Pentafluoro-6-(nonafluorobutyl)benzene","19108-38-4","D",0]
["N-[3-(N,N-Dimethyl-N-oxidoamino)propyl]-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-N-methyloctanesulfonamide","80475-34-9","D",0]
["2-[4-(Bromomethyl)phenyl]-1,1,1,3,3,3-hexafluoropropan-2-ol","202134-57-4","D",0]
["2,2-Difluoro-3-(nonafluorobutoxy)propanoic acid","824393-39-7","D",0]
["1-Chloro-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-hexadecafluorooctane","423-53-0","D",0]
["7-H-Perfluoroheptanoate","69681-35-2","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reaction products with ethylenediamine","161075-06-5","D",0]
["Propane, 1,3-dibromo-2-chloro-1,1,2,3,3-pentafluoro-","422-79-7","D",0]
["Borate(1-), tris(1,1,1,3,3,3-hexafluoro-2-propanolato)hydro-, sodium (1:1), (T-4)-","139494-68-1","D",0]
["1,1,1,2,3,3-Hexafluoropentane","57915-69-2","D",0]
["12:2 Fluorotelomer sulfonamido betaine","278598-45-1","D",0]
["1,1,1,4,5,5,5-Heptafluoro-2,3,4-tris(trifluoromethyl)pent-2-ene","90141-43-8","D",0]
["4,4'-[(3,3,4,4,5,5-Hexafluoro-1-cyclopentene-1,2-diyl)bis(5-methyl-4,2-thienediyl)]diphenol","156686-73-6","D",0]
["N,N'-bis(Perfluorobutanoyl)1,6-hexanediamine","123665-83-8","D",0]
["3-Amino-2,4,4,5,5,6,6-heptafluorocyclohex-2-en-1-one","1551-64-0","D",0]
["5-(Heptafluoropropyl)-3-methoxy-1-methyl-1H-1,2,4-triazole","714975-34-5","D",0]
["Perfluoroalkylethyl acrylates (C6-C14)","85361-54-5","D",0]
["Nonadecafluorodecanoic acid, sodium salt","3830-45-3","D",0]
["Ammonium nonadecafluorodecanoate","3108-42-7","D",0]
["Ammonium salts of perfluorononan-1-oic-acid","4149-60-4","D",0]
["Iodonium, bis(4-dodecylphenyl)-, branched and linear, hexafluoroantimonate(1-)","96195-78-7","D",0]
["bis(2-hydroxyethyl)ammonium bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl) phosphate","94231-56-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-henicosafluoroundecyl acrylate","94231-57-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-icosafluoro-11-(vinyloxy)undecane","94231-58-0","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl dihydrogen phosphate","94231-59-1","D",0]
["butan-2-one O,O',O''-[[3-(1,1,2,2-tetrafluoroethoxy)propyl]silylidyne]trioxime","94232-71-0","D",0]
["triethoxy[3-(1,1,2,2-tetrafluoroethoxy)propyl]silane","94232-72-1","D",0]
["3-chloro-1,1,1,5,5,5-hexamethyl-3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)trisiloxane","94237-06-6","D",0]
["1,1,5,5,5-hexamethyl-3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-3-[(trimethylsilyl)oxy]trisiloxane","94237-07-7","D",0]
["methoxydimethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","94237-08-8","D",0]
["2-[[[dimethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silyl]oxy]methyl]-2-[[(1-oxoallyl)oxy]methyl]-1,3-propanediyl diacrylate","94237-11-3","D",0]
["2-[[[[3-(acryloyloxy)-2,2-bis[(acryloyloxy)methyl]propoxy]methyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silyl]oxy]methyl]-2-[(acryloyloxy)methyl]propane-1,3-diyl diacrylate","94237-12-4","D",0]
["2-[(acryloyloxy)methyl]-2-[[[bis[3-(acryloyloxy)-2,2-bis[(acryloyloxy)methyl]propoxy](3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silyl]oxy]methyl]propane-1,3-diyl diacrylate","94237-13-5","D",0]
["1,1-dichloro-3,3,3-trimethyl-1-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)disiloxane","94237-17-9","D",0]
["bis(2-hydroxyethyl)ammonium bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-nonacosafluorohexadecyl) phosphate","94291-75-5","D",0]
["bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-tritriacontafluorooctadecyl] hydrogen phosphate, compound with 2,2'-iminodiethanol (1:1)","94291-76-6","D",0]
["bis[3,3,4,4,5,5,6,6,7,7,8,8,9,10,10,10-hexadecafluoro-9-(trifluoromethyl)decyl] hydrogen phosphate, compound with 2,2'-iminodiethanol (1:1)","94291-77-7","D",0]
["bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-icosafluoro-11-(trifluoromethyl)dodecyl] hydrogen phosphate, compound with 2,2'-iminodiethanol (1:1)","94291-78-8","D",0]
["(Z)-Octadec-9-enyl (5-(((2-(((perfluorooctyl)sulphonyl)methylamino)ethoxy)carbonyl)amino)-o-tolyl)carbamate","94313-84-5","D",0]
["5-fluoro-5,7,7-tris(trifluoromethyl)-6-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]-1,4-dioxepane","94333-56-9","D",0]
["Propyl perfluorononanoate","99156-01-1","D",0]
["Nonafluoropentanoyl chloride","375-60-0","D",0]
["Hexafluoroacetone hydrate","10543-95-0","D",0]
["1-[4-(Heptafluoropropyl)-1H-pyrrol-3-yl]ethan-1-one","121103-97-7","D",0]
["Pentafluoropropanoic acid--piperazine (1/1)","1690-94-4","D",0]
["2-Propenoic acid, 2-methyl-, octadecyl ester, polymer with 1,1-dichloroethene, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,¿","112310-55-1","D",0]
["Thiocyanic acid, .gamma.-.omega.-perfluoro-C4-20-alkyl esters","97553-95-2","D",0]
["cyclo-hexachloro[mu-N-methyl-[N-(perfluorooctylsulphonyl)]glycinato-O1:O1']]di-mu-hydroxytrichromium","97298-47-0","D",0]
["2-Butenoic acid, 4-oxo-4-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyandecyl)amino]-, (Z)- (9CI)","97259-81-9","D",0]
["Alkenes, C8-14 alpha-,delta-omega-perfluoro-","97659-47-7","D",0]
["Ethanol, 2-(methylamino)-, N-(gamma-omega-perfluoro-C8-14-beta-alkenyl) derivs.","97660-44-1","D",0]
["Bis(1H,1H,6H-perfluorohexyl)-2-sulfobutanedioate sodium salt","98151-22-5","D",0]
["5-{[1,1,1,4,5,5,5-Heptafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-4-(trifluoromethyl)pent-2-en-2-yl]oxy}benzene-1,3-dicarboxylic acid","97220-62-7","D",0]
["Calcium perfluoroundecanoate","97163-17-2","D",0]
[".alpha.-[2-Hydroxy-3-[.alpha.-perfluoroisopropylpoly(degree of polymerization 7-15)(difluoromethylene)]propyl]-.omega.-methoxy-poly(degree of polymerization 1-25)(oxyethylene)","96353-69-4","D",0]
["2-Propenoic acid, 2-fluoro-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","96250-52-1","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)propyl 2-fluoroprop-2-enoate","96250-49-6","D",0]
["1,3-Benzenedicarboxylic acid, 5-[(heptadecafluorononenyl)oxy]-","96210-37-6","D",0]
["Betaines, N-(hydroxyethyl)-N-methyl-N-(2-sulfoethyl)-N-(1,1,2-trihydroperfluoro-C8-14-2-alkenyl)","98219-29-5","D",0]
["Oxirane, mono[[(beta-omega-perfluoro-omega-hydro-C2-4-alkyl)oxy]methyl] derivs.","98561-39-8","D",0]
["Alcohols, C3-7, beta-omega-perfluoro-omega-hydro, reaction products with 3a,4,7,7a-tetrahydro-1,3-isobenzofurandione","98561-40-1","D",0]
["Alcohols, C3-7, beta-omega-perfluoro-omega-hydro, reaction products with 3a,4,7,7a-tetrahydromethyl-4,7-methanoisobenzofuran-1,3-dione","98561-41-2","D",0]
["1-Butanol, 4-(ethenyloxy)-, polymer with 1-chloro-1,2,2-trifluoroethene and ethoxyethene","98728-78-0","D",0]
["Sodium Perfluorononanesulfonate","98789-57-2","D",0]
["Sulfonamides, C7-8-alkane, perfluoro, N-methyl-N-[2-[(1-oxo-2-propenyl)oxy]ethyl], polymers with 2-ethoxyethyl acrylate, glycidyl methacrylate and N,N,N-trimethyl-2-[(2-methyl-1-oxo-2-propenyl)oxy]ethanaminium chloride","98999-57-6","D",0]
["N-[3-(Dimethylamino)propyl]-4-[[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-buten-1-yl]oxy]benzenesulfonamide","220288-28-8","D",0]
["1-Bromo-2,2,3,3,4,4-hexafluorocyclobutyl acetate","714-43-2","D",0]
["Perfluoro-1-(tetrafluoroiodo)-1-octyne","1424379-21-4","D",0]
["1,1,1,2,4,4,5,5,6,6,7,7-Dodecafluoro-2-(trifluoromethyl)heptan-3-one","680-07-9","D",0]
["Bis(perfluorooctyl) phosphinic acid methyl ester","610800-37-8","D",0]
["Methanaminium, N,N,N-trimethyl-, 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate (1:1)","25628-17-5","D",0]
["2,2,3,3-Tetrafluoropropyl 3,3,3-trifluoropropanoate","63296-99-1","D",0]
["4,6-Dichloro-2-(heptafluoropropyl)pyrimidine","1023815-51-1","D",0]
["Perfluoro-2-[2-[(ethenyl)oxy]propoxy]ethanesulfinic acid sodium","187480-43-9","D",0]
["[N(E),S(S)]-N-(4-methylphenyl)methyleneperfluorobutanesulfinamide","1612778-39-8","D",0]
["4-(Difluoromethyl)-1,2,3,3,4,5,5,6,6-nonafluorocyclohex-1-ene","116487-62-8","D",0]
["(3S)-1,1,1,2,2-Pentafluorododecan-3-ol","307531-78-8","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-icosafluorodecane-1-sulfonic acid","2274731-07-4","D",0]
["1,1,2,2-Tetrafluorononane-3,5-dione","59857-64-6","D",0]
["1-Bromo-4-(2,2,3,3,4,4,4-heptafluorobutoxy)benzene","1365808-49-6","D",0]
["6-(2,2,3,3-Tetrafluoropropoxy)-1,3-benzothiazol-2-amine","1855907-41-3","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecanenitrile","26649-26-3","D",0]
["(Perfluoropropyl)phenylmethanol","785-93-3","D",0]
["Perfluoro-2-[3-(methoxy)propoxy]acetic acid","919005-51-9","D",0]
["Phosphonic acid, mono[2,2-bis[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]methyl]-3-hydroxypropyl] ester","138655-68-2","D",0]
["2-Chloro-6-(difluoromethoxy)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)aniline","1262665-50-8","D",0]
["3-[(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)sulfanyl]benzoic acid","88489-75-2","D",0]
["2,2,3,3,3-Pentafluoro-N-propylpropanamide","62243-62-3","D",0]
["1-(3-chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-one","35443-98-2","D",0]
["1,1,2,2-Tetrafluoroethan-1-ol","130953-44-5","D",0]
["2-Bromo-3,3,4,4,5,5,6,6,6-nonafluorohex-1-ene","59665-23-5","D",0]
["N-[3-(Dimethylamino)propyl]perfluoro-4-(methyl)cyclohexanecarboxamide N-oxide","200636-86-8","D",0]
["Benzene, 1,1'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis[3-nitro-","64465-34-5","D",0]
["Benzyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","147224-19-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-N~1~,N~1~,N~8~,N~8~-tetrakis(trifluoromethyl)octane-1,8-diamine","141496-31-3","D",0]
["1,1,1,3,3,3-hexafluoro-2-(3-nitrophenyl)propan-2-ol","2402-65-5","D",0]
["Bis(heptafluoroisopropyl)mercury","756-88-7","D",0]
["3-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-sulfonyl)propan-1-ol","106104-73-8","D",0]
["(1,1,2,2-Tetrafluoro-1,2-ethanediyl)bis[dimethylphenylsilane","79035-75-9","D",0]
["3-(Nonafluorobutyl)quinoxalin-2(1H)-one","89995-30-2","D",0]
["(1z,6z)-2,2,3,3,4,4,5,5-octafluorohexanediimidamide","678-57-9","D",0]
["5-Chloro-2-(heptafluoropropyl)benzimidazole","6866-58-6","D",0]
["2,4-Dinitro-N-[4-(1,1,2,2-tetrafluoroethoxy)phenyl]-6-(trifluoromethyl)-benzenamine","79930-77-1","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with (2-bromo-1,1,2,2-tetrafluoroethoxy)trifluoroethene, 1,1-difluoroethene, ethene, tetrafluoroethene and trifluoro(trifluoromethoxy)ethene (9CI)","149935-00-2","D",0]
["1-[3-Methylidene-4-(2,2,3,3,4,4,5,5,5-nonafluoropentyl)pyrrolidin-1-yl]ethan-1-one","31164-13-3","D",0]
["4-Cyanophenyl 4-(undecafluoropentyl)benzoate","88951-06-8","D",0]
["Perfluorotetradecanesulfonate","343629-46-9","D",0]
["Octafluoro-4-(heptafluoropropyl)morpholine","1704-69-4","D",0]
["Pentafluoroethyl trifluoromethanesulfonate","74501-94-3","D",0]
["1-(Heptafluoropropyl)-4-methylisoquinoline","70414-16-3","D",0]
["3,6-Octanediol, 1,2,2,7,7,8-hexafluoro-1,8-bis(heptafluoropropoxy)-","185697-78-3","D",0]
["1-bromo-3-(1,1,2,2-tetrafluoroethoxy)benzene","527751-45-7","D",0]
["1-(4-Methylphenyl)-2,2-bis(trifluoromethyl)aziridine","64030-45-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(1-phenylpropan-2-yl)butanamide","90582-01-7","D",0]
["N-(4-Bromophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","308-67-8","D",0]
["4,5,6-Tris(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-1,2,3-triazine","116392-95-1","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl hydrogen phosphate","1158182-59-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5-undecafluoro-7-iodododecane","1980063-53-3","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-iodo-7,7-dimethyloctane","1464148-69-3","D",0]
["4-[(2-Chloro-4-nitrophenyl)diazenyl]-N-(2,2,3,3-tetrafluoropropyl)aniline","327972-10-1","D",0]
["4,4-Bis(trifluoromethyl)-3-(trimethylsilyl)oxetan-2-one","88237-30-3","D",0]
["Bis(2-(methyl((nonafluorobutyl)sulfonyl)amino)ethyl) octadecanedioate","890406-75-4","D",0]
["5,6-Bis(pentafluoroethyl)-1,2,3,4,5,6-tetrathiadiazinane","87985-88-4","D",0]
["2-Propenoic acid, 2-methyl-, 3-(trimethoxysilyl)propyl ester, polymer with ethenylbenzene, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl 2-propenoate and 2-hydroxyethyl 2-propenoate","95590-48-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-(diethylamino)ethyl ester, polymer with  .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(diflluoromethylene), acetate (salt)","500701-62-2","D",0]
["2,2-Bis(trifluoromethyl)oxirane","31898-68-7","D",0]
["(7a,17b)-7-(9-((4,4,5,5,5-Pentafluoropentyl)thio)nonyl)-estra-1,3,5(10)-triene-3,17-diol 17-acetate","875573-69-6","D",0]
["N-(2,2,3,3,4,4,4-Heptafluorobutanoyl)-2-methylalanine","880353-20-8","D",0]
["Thiobenzyl N-heptafluorobutyrylanthranilate","82422-25-1","D",0]
["1,2,3,3,3-Pentafluoro-1-[(1,2,3,3,3-pentafluoroprop-1-en-1-yl)oxy]prop-1-ene","3823-94-7","D",0]
["4,6-Nonanedione, 2,8-bis(trifluoromethyl)-2,8-dihydroxy-1,1,1,9,9,9-hexafluoro-","101832-24-0","D",0]
["5-(Tridecafluorohexyl)uridine","58671-32-2","D",0]
["3,3,4,4,5,5,6,6,7,7-Decafluorooctyl 2-methylprop-2-enoate","61915-92-2","D",0]
["Siloxanes and Silicones, di-Me, Me hydrogen, Me 3-(2-oxiranylmethoxy)propyl, Me 2-phenylpropyl, Me 3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]propyl, [[dimethyl[3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,","1382351-49-6","D",0]
["1,1'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(4-bromobenzene)","88964-95-8","D",0]
["2-(2-Bromo-1,1,2,2-tetrafluoroethoxy)-2,3,3,3-tetrafluoropropanoyl fluoride","87000-86-0","D",0]
["N-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]benzenamine","2002-95-1","D",0]
["1,3,3,4,4-Pentafluoro-2-(1,2,2,2-tetrafluoroethyl)cyclobut-1-ene","61898-36-0","D",0]
["Heptanamide, 2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoro-N-phenyl-","315237-99-1","D",0]
["Ethyl 2,2,3,3-tetrafluoro-3-phenylpropanoate","14160-54-4","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-(methanesulfinyl)hexane","357604-65-0","D",0]
["2-(Heptafluoropropyl)oxirane","51035-20-2","D",0]
["1,1,1,5,5,5-Hexafluoro-2,4-bis(trifluoromethyl)pentane-2,4-diol","503169-49-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-1-(thiophen-2-yl)nonane-1,3-dione","171520-40-4","D",0]
["1,6-Dibromo-2,3,5-trichloro-1,1,2,3,4,4,5,6,6-nonafluorohexane","85131-86-8","D",0]
["2-Methoxyethyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","340034-67-5","D",0]
["Perfluoro-(2-n-propyl)pyran","74948-35-9","D",0]
["1-(3,3,4,4,4-Pentafluorobut-1-yn-1-yl)cyclohexan-1-ol","95540-96-8","D",0]
["1-Bromo-1,1,2,2,4,5,5,7,8,8,10,11,11,13,13,14,14,14-octadecafluoro-4,7,10-tris(trifluoromethyl)-3,6,9,12-tetraoxatetradecane","1482416-51-2","D",0]
["1-(3,5-Dibromophenyl)-2,2,3,3,4,4,4-heptafluorobutan-1-one","79851-20-0","D",0]
["3H-Perfluoro-2-butene","22692-37-1","D",0]
["3-[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propane-2-sulfonyl]benzoic acid","88489-83-2","D",0]
["2,2,3,3-Tetrafluoropropyl nonafluorobutane-1-sulfonate","66959-14-6","D",0]
["1-[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy]-3-(2-nitro-1H-imidazol-1-yl)propan-2-ol","104290-39-3","D",0]
["S-Propan-2-yl pentafluoropropanethioate","62243-63-4","D",0]
["1-Decanol, 7,7,8,8,9,9,10,10,10-nonafluoro-5-iodo-","116486-78-3","D",0]
["Perfluoro-2-methylheptane","153273-32-6","D",0]
["Perfluorohexadecanesulfonic acid","81735-29-7","D",0]
["Perfluoro-N-methyl-decahydroquinoline","86714-33-2","D",0]
["2-methyl-1-(1,1,2,2-tetrafluoroethyl)benzimidazole","42379-52-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,8,8-Pentadecafluoro-10-iododecane","49676-71-3","D",0]
["5:2 Fluorotelomer carboxylic acid","889944-77-8","D",0]
["Bis(2-chloro-2,3,3,3-tetrafluoro-1-oxopropyl)peroxide","422312-38-7","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)propanenitrile","382-17-2","D",0]
["N-[4-(Pentafluoroethoxy)phenyl]pyridine-4-carboxamide","62315-15-5","D",0]
["1,1,1-trifluoroethane","420-46-2","D",0]
["N-Propylperfluorooctane sulfonamidoethanol polyoxyethylene","52550-45-5","D",0]
["Polyethylene oxide, mono(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) ether","52550-44-4","D",0]
["3,3,4,4,4-Pentafluorobutyl methacrylate","52519-51-4","D",0]
["Sodium 4-{perfluoro[4-ethyl-3,4-dimethylhex-2-en-2-yl]oxy}benzene-1-sulfonate","52584-45-9","D",0]
["2-(Perfluorobutyl)ethyl acrylate","52591-27-2","D",0]
["Potassium p-(2,2,2-trifluoro-1-(p-hydroxyphenyl)-1-(trifluoromethyl)ethyl)phenolate","52870-69-6","D",0]
["(1H,1H-Perfluoro-12-methyltridecyl)oxirane","54009-78-8","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, hydrogen phosphat, compd. with 2,2'-iminobis[ethanol](1:1) (9CI)","57677-98-2","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, hydrogenphosphat, compd. with 2,2'-iminobis[ethanol] (1:1) (9CI)","57677-97-1","D",0]
["Bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) hydrogen phosphate","57677-95-9","D",0]
["Potassium 2,3,4,5-tetrachloro-6-(((3-(((heptadecafluorooctyl)sulphonyl)oxy)phenyl)amino)carbonyl)benzoate","57589-85-2","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene, 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","57570-64-6","D",0]
["(Perfluoro-9-methyldecyl)ethyl acrylate","52956-81-7","D",0]
["3,3-Dichloro-1,1,1,2-tetrafluoropropane","53063-54-0","D",0]
["1,3-Bis(2-(perfluoro-7-methyloctyl)-1-ethylsulfanyl)propan-2-yl {4-methyl-3-[(2-methylaziridine-1-carbonyl)amino]phenyl}carbamate","53122-42-2","D",0]
["3,5,7,9,9-Pentachloro-2,2,3,4,4,5,6,6,7,8,8,9-dodecafluorononanoic acid","53281-25-7","D",0]
["3,5,7,9,11,11-Hexachloro-2,2,3,4,4,5,6,6,7,8,8,9,10,10,11-pentadecafluoroundecanoic acid","53281-37-1","D",0]
["Trimethyl-3-((perfluorobutylsulphonyl)amino)propylammonium chloride","53518-00-6","D",0]
["6:2 fluorotelomer carboxylic acid","53826-12-3","D",0]
["3-(Perfluorononyl)-1,2-propanediol-1-phosphate","54009-74-4","D",0]
["2-Butenedioic acid (2Z)-, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester","54950-04-8","D",0]
["2:2 Fluorotelomer alcohol","54949-74-5","D",0]
["Copolymer of fluoroethene, perfluoroethene and perfluoropropene","54733-33-4","D",0]
["1,4-Bis((perfluorohexyl)ethyl) sulphonatosuccinate sodium","54950-05-9","D",0]
["2,4,6-tris(nonadecafluorononyl)-1,3,5-triazine","57101-59-4","D",0]
["Proline, 1-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)sulfonyl]-, lithium salt (9CI)","503431-63-8","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,isooctadecyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propenyl)-.omega-methoxypoly(oxy-1,2-ethanediyl) and ¿","503448-36-0","D",0]
["Bis((perfluorobutyl)ethyl) 2-[(carboxymethyl)thio]butanedioate lithium salt","503534-33-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with alpha-(2-methyl-1-oxo-2-propenyl)-omega-methoxypoly(oxy-1,2-ethanediyl), tert-Bu 2-ethylhexaneperoxoate-initiated","503621-60-1","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with alpha-(2-methyl-1-oxo-2-propenyl)-omega-methoxypoly(oxy-1,2-ethanediyl), di-Me 2,2'-azobis[2-methylpropanoate]-initiated","503621-79-2","D",0]
["2-Propenoic acid, polymer with butyl 2-propenoate and 2,5-furandione, gamma-omega-perfluoro-C8-14-alkyl esters, potassium salts, tert-Bubenzenecarboperoxoate-initiated","524729-93-9","D",0]
["(1H,1H-Perfluoro-14-methylpentadecyl)oxirane","54009-77-7","D",0]
["(Z)-1,2,3,3,3-pentafluoropropene","5528-43-8","D",0]
["1-Hexanesulfonyl chloride, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","55591-23-6","D",0]
["Morpholine, 2,2,3,3,5,5,6,6-octafluoro-4-(pentafluoroethyl)-","55716-11-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8-dodecafluoro-2-methyloctan-2-ol","55793-32-3","D",0]
["1,1,1,2,2,3,3,4,5,5,6,6,6-Tridecafluoro-4-(trifluoromethyl)-hexane","558-69-0","D",0]
["Potassium N-((heptadecafluorooctyl)sulphonyl)-N-propylglycinate","55910-10-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl acrylate","559-11-5","D",0]
["perfluorooct-1-ene","559-14-8","D",0]
["[(1,2,3,3,4,4,5,5,6,6,6-Undecafluorohex-1-en-1-yl)oxy]benzene","55937-49-0","D",0]
["Octafluorocyclopentene","559-40-0","D",0]
["(Perfluorobutyryl)-2-thenoylmethane","559-94-4","D",0]
["Ethene, tetrafluoro-, polymer with 1,1-difluoroethene and trifluoro(trifluoromethoxy)ethene","56357-87-0","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-[2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl]-omega-hydroxy-","56372-23-7","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoro-1-(pentafluoroethyl)piperidine","564-11-4","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-(tridecafluorohexyl)-omega-hydroxy-","56467-05-1","D",0]
["(2-chloro-1,1,2,2-tetrafluoroethoxy)trifluoroethylene","56672-52-7","D",0]
["Tetraethylammonium-heptadecafluorooctanesulphonate","56773-42-3","D",0]
["Fluoroether E-6","55154-18-2","D",0]
["Alkenes, C4-20 alpha-, gamma-omega-perfluoro","68155-04-4","D",0]
["Cyclohexanesulfonyl fluoride, nonafluorobis(trifluoromethyl)-","68156-00-3","D",0]
["Potassium 2,2,3,3,4,4,5,5,6¿nonafluoro¿1,6¿ bis(trifluoromethyl)cyclohexane¿1¿sulfonate","68156-01-4","D",0]
["decafluoro(pentafluoroethyl)cyclohexanesulphonyl fluoride","68156-06-9","D",0]
["Ammonium bis(2-(ethyl((pentadecafluoroheptyl)sulphonyl)amino)ethyl) phosphate","67939-97-3","D",0]
["4-[Methyl[(nonafluorobutyl)sulfonyl]amino]butyl methacrylate","67906-39-2","D",0]
["4-(Methyl((undecafluoropentyl)sulphonyl)amino)butyl methacrylate","67906-40-5","D",0]
["N-allyl-N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptane-1-sulphonamide","67906-41-6","D",0]
["Ammonium perfluorodecanesulfonate","67906-42-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl ester","67906-70-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-(ethyl((undecafluoropentyl)sulfonyl)amino)ethyl ester","67906-73-4","D",0]
["Benzenediazonium, 2-methoxy-4-(phenylamino)-, chloride (1:1), polymer with formaldehyde and hydrogen hexafluorophosphate(1-)","67907-00-0","D",0]
["Tetrafluorosuccinyl fluoride","679-13-0","D",0]
["1-Heptanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-[2-(phosphonooxy)ethyl]-","67923-61-9","D",0]
["2-(Ethyl((nonafluorobutyl)sulphonyl)amino)ethyl methacrylate","67939-33-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(nonafluorobutyl)sulfonyl]amino]ethyl ester, polymer with octadecyl 2-propenoate and 2-propenoic acid","67939-34-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(pentadecafluoroheptyl)sulfonyl]amino]ethyl ester","67939-36-0","D",0]
["1-Octanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-[3-(trichlorosilyl)propyl]-","67939-42-8","D",0]
["2-Propenoic acid, 2-methyl-, 4-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]butyl ester","67939-61-1","D",0]
["1-Pentanesulfonamide, N,N'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-1,1,2,2,3,3,4,4,5,5,5-undecafluoro-","67939-87-1","D",0]
["N-(3-(Dimethylamino)propyl)heptadecafluorooctanesulphonamide monohydrochloride","67939-88-2","D",0]
["2-(Ethyl((1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulphonyl)amino)ethyl dihydrogen phosphate","67939-89-3","D",0]
["1-Pentanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,5-undecafluoro-N-[2-(phosphonooxy)ethyl]-","67939-90-6","D",0]
["Bis(2-(ethyl(nonafluorobutanesulphonyl)amino)ethyl) hydrogen phosphate","67939-91-7","D",0]
["(1,1,2,2-tetrafluoroethoxy)ethylene","681-49-2","D",0]
["Ethene, 1-bromo-1,2,2-trifluoro-, homopolymer","55157-25-0","D",0]
["Poly(tetrafluoroethylene-co-vinylidene fluoride-co-propylene)","54675-89-7","D",0]
["Copolymer of ethylene/tetrafluoroethylene/3,3,3-trifluoro-2-(trifluoromethyl)-1-propene (a number-average molecular weight is not less than 1,000 and the polymer is insoluble in water, lipid soluble solvent, usual solvent, acid and alkali)","54302-05-5","D",0]
["Chlorotrifluoro ethylene, ethylene, hexafluoroisobutylene terpolymer","54302-04-4","D",0]
["[2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-dotriacontafluoro-16-(trifluoromethyl)heptadecyl]oxirane","54009-79-9","D",0]
["Diammonium 2-(ethyl((pentadecafluoroheptyl)sulphonyl)amino)ethyl phosphate","67939-98-4","D",0]
["N-(3-(Dimethylamino)propyl)perfluoroheptanesulfonamide hydrochloride","67940-02-7","D",0]
["Perfluoro-(2,5,8-trimethyl-3,6,9-trioxadodecanoic) acid potassium salt","67963-77-3","D",0]
["1-Hexanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-[2-(phosphonooxy)ethyl]-","67969-65-7","D",0]
["N-ethyl-N-[2-(phosphonooxy)ethyl]perfluorooctanesulfonamide diammonium salt","67969-69-1","D",0]
["Carbamic acid, N,N'-(4-methyl-1,3-phenylene)bis-, bis[2-[ethyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl] ester","68081-83-4","D",0]
["Perfluoro-13-methyltetradecanoic acid compd. with ethanamine","68052-68-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-hexacosafluoro-13-(trifluoromethyl)myristoyl fluoride","68025-62-7","D",0]
["2-(Methyl((pentadecafluoroheptyl)sulfonyl)amino)ethyl acrylate","68084-62-8","D",0]
["Perfluoroalkyl (C2-C8)ethyl mercaptan","68140-18-1","D",0]
["1,1,2,2-Tetrahydroperfluoroalkyl (C4-20) mercaptan","68140-19-2","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-docosafluoro-11-(trifluoromethyl)lauric acid, compound with ethylamine (1:1)","68015-87-2","D",0]
["Perfluoro-7-(trifluoromethyl)octanoic acid ethanamine","68015-86-1","D",0]
["Ethanaminium perfluoro-9-methyldecanoate","68015-85-0","D",0]
["2,2,3,3,4,4,5,6,6,6-Decafluoro-5-(trifluoromethyl)hexanoic acid - ethanamine (1:1)","68015-84-9","D",0]
["1-Chloro-1,2,2,3,3-pentafluoropropane","679-99-2","D",0]
["Propane, 3-chloro-1,1,2,2-tetrafluoro-","679-85-6","D",0]
["Thiols, C6-12, gamma-omega-perfluoro","68140-20-5","D",0]
["Thiols, C10-20, gamma-omega-perfluoro","68140-21-6","D",0]
["2-Propenoic acid, polymers with gamma-omega-perfluoro-C8-16-alkyl acrylate andstearyl acrylate","503297-86-7","D",0]
["1,1,2,2-Tetrahydroperfluoroeicosyl alcohol","65104-65-6","D",0]
["1,1,2,2-Tetrahydroperfluoroeicosyl methacrylate","65104-66-7","D",0]
["1,1,2,2-Tetrahydroperfluoro-1-octadecanol","65104-67-8","D",0]
["Perfluoro-2,5,8,11,14,17,20,23,26-nonamethyl-3,6,9,12,15,18,21,24,27-nonaoxatriacontan-1-oyl fluoride","65150-88-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16-tritriacontafluoro-18-iodooctadecane","65150-94-9","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1-chloro-1,2,2-trifluoroethene and 1,1,2,2-tetrafluoroethene","64155-70-0","D",0]
["Ammonium perfluoro-2-methyl-3-oxahexanoate","62037-80-3","D",0]
["methyl 2,2,3,3,4,4-hexafluoro-4-[1,2,2-trifluoro-2-[(trifluorovinyl)oxy]-1-(trifluoromethyl)ethoxy]butyrate","62361-02-8","D",0]
["1,1,1,3,3,5,5,5-Octafluoro-2,2,4,4-tetrakis(trifluoromethyl)pentane","62375-54-6","D",0]
["(1R,4S)-3-(2,2,3,3,4,4,4-Heptafluoro-1-hydroxybutylidene)-1,7,7-trimethylbicyclo[2.2.1]heptan-2-one","63180-06-3","D",0]
["1H,1H,2H,2H-Perfluorotetradecanol sulfate ammonium salt","63225-59-2","D",0]
["1,4-Bis(1H,1H,9H-perfluorononyl) sulfobutanedioate sodium","63367-17-9","D",0]
["1-Propene, polymer with 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]propane and tetrafluoroethene","63391-86-6","D",0]
["Methyl 2,2,3,3,4-pentafluoro-4-oxobutanoate","63425-24-1","D",0]
["1-Nonanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-, dihydrogenphosphat, diammonium salt (9CI)","63439-39-4","D",0]
["Phosphonic acid, P-[[4-[(heptadecafluorononen-1-yl)oxy]phenyl]methyl]-","63513-12-2","D",0]
["Copolymer of hexafluoropropene, perfluoro(ethoxyethene) and tetrafluoroethene","63654-40-0","D",0]
["Hexafluoropropene, 1-((trifluoroethenyl)oxy)heptafluoropropane, tetrafluoroethene polymer","63654-41-1","D",0]
["2-Pentene, 1,1,1,3,4,5,5,5-octafluoro-2,4-bis(trifluoromethyl)-","63703-15-1","D",0]
["Methyl perfluoro(3-(1-ethenyloxypropan-2-yloxy)propanoate)","63863-43-4","D",0]
["Propanoic acid, 3-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, methyl ester, polymer with tetrafluoroethene","63863-44-5","D",0]
["1-Iodoperfluoropentane","638-79-9","D",0]
["Chlorotetrafluoroethane","63938-10-3","D",0]
["perfluoroheptanal","63967-41-9","D",0]
["(Perfluorooctadecyl)ethyl 2-propenoate","65104-64-5","D",0]
["3-[[[4-[(Heptadecafluorononenyl)oxy]phenyl]sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium, iodide","59493-70-8","D",0]
["1-(3-(4-((Heptadecafluorononyl)oxy)-benzamido)propyl)-N,N,N-trimethylammonium iodide","59493-72-0","D",0]
["p-[(undecafluorohexenyl)oxy]benzenesulphonyl chloride","59493-82-2","D",0]
["Sodium 4-perfluorohexenyloxybenzenesulfonate","59493-84-4","D",0]
["p-Perfluorononenyloxybenzenesulfonyl chloride","59536-15-1","D",0]
["N-(2-Carboxyethyl)-N,N-dimethyl-3-[[(perfluorohexyl)ethylsulfonyl]amino]propanaminium","61798-69-4","D",0]
["Heptadecafluoro-N-(2-(phosphonooxy)ethyl)-N-propyloctanesulphonamide","64264-44-4","D",0]
["N-(2-aminoethyl)-2-[1-[difluoro[(trifluorovinyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoroethanesulphonamide","64346-90-3","D",0]
["Ethanesulfonamide, N-(2-aminoethyl)-2-[1-[difluoro[(1,2,2-trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoro-, polymer with 1,1,2,2-tetrafluoroethene","64346-91-4","D",0]
["3,3,4,4-Tetrafluoro-2-methylbutan-2-yl 2-methylprop-2-enoate","64375-26-4","D",0]
["Hexafluorobutyl methacrylate polymer","64376-86-9","D",0]
["1,8-Dibromo-1,1,2,2-tetrafluoro-Octane","64382-00-9","D",0]
["1,3-Butanediol, polymer with 1,3-diisocyanatomethylbenzene and 2-ethyl-2-(hydroxymethyl)-1,3-propanediol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-decanol- and Me Et ketone oxime-blocked","644965-83-3","D",0]
["2,2,3,3,4,5,5-Heptafluorotetrahydro-4-(1,1,2,2,3,3,4,4,4-nonafluorobutyl)furan","646-85-5","D",0]
["1,1,1-trifluoro-2-(trifluoromethyl)pent-4-en-2-ol","646-97-9","D",0]
["Octanenitrile, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","647-12-1","D",0]
["7H-Perfluoroheptanal","647-44-9","D",0]
["4,4,5,5,6,6,6-Heptafluoro-2-iodohexan-1-ol","647-84-7","D",0]
["Benzenesulfonic acid, 4-[(nonadecafluorodecenyl)oxy]-, sodium salt","64910-98-1","D",0]
["1-Butene, 4-bromo-3,3,4,4-tetrafluoro-, polymer with 1,1-difluoroeth...","65059-79-2","D",0]
["3,4-Dichloro-alpha,alpha-bis(trifluoromethyl)benzenemethanol","65072-48-2","D",0]
["Ethanesulfonic acid, 2-[1-[difluoro[(1,2,2-trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoro-, potassium salt (1:1), polymer with 1,1,2,2-tetrafluoroethene","65086-49-9","D",0]
["Ethanesulfonamide, N-butyl-2-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoro-, polymer with tetrafluoroethene","65104-43-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18-heptatriacontafluoro-20-iodoicosane","65104-63-4","D",0]
["3-(Heptadecafluorooctyl)-1,2,4-trioxolane","63967-43-1","D",0]
["2-Propenoic acid, 2-methyl-, cyclohexyl ester, polymers with maleicanhydride, gamma-omega-perfluoro-C8-20-alkyl acrylate and 2,4,6-tris(2-propenyloxy)-1,3,5-triazine","518045-14-2","D",0]
["4-(Perfluoro(4-ethyl-3,4-dimethylhex-2-en-2-yl)oxy)benzene-1-sulfonyl chloride","51947-19-4","D",0]
["p-[[4,4,5,5,5-pentafluoro-3-(pentafluoroethyl)-1,2,3-tris(trifluoromethyl)pent-1-enyl]oxy]-N-[3-(triethoxysilyl)propyl]benzenesulphonamide","52026-59-2","D",0]
["1-Propanaminium, N,N,N-trimethyl-3-[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-, chloride (1:1)","52166-82-2","D",0]
["Bis(nonafluorobutyl)phosphinic acid","52299-25-9","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with alpha-(2-methyl-1-oxo-2-propenyl)-omega-hydroxypoly(oxy-1,2-ethanediyl), tert-Bu 2-ethylhexaneperoxoate-initiated","503621-80-5","D",0]
["Propanoic acid, 3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-2-methyl-, lithium salt (1:1)","476304-39-9","D",0]
["2-Propenoic acid, 2-methyl-, 3-(trimethoxysilyl)propyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate¿","477529-30-9","D",0]
["((Perfluoro-9-methyldecyl)methyl)oxirane","47795-34-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers with gamma-omega-perfluoro-C8-14-alkyl acrylate, acetates, N-oxides","479029-28-2","D",0]
["2-Propeonic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl-, polymer with 2-methyloxirane, polymer with oxirane bis(2methyl2propenoate) and 2-methyloxirane polymer with oxirane mono(2methyl-2-propenoate)","479074-93-6","D",0]
["1,5-bis(2,3-epoxypropoxy)-2,2,3,3,4,4-hexafluoropentane","4798-39-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl methacrylate","48076-44-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl methacrylate","48077-33-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-henicosafluoroundecyl methacrylate","48077-86-7","D",0]
["N-(2-Hydroxyethyl)-perfluoro-1-butanesulfonamide, cmpd. with 2,2'-iminobis[ethanol] (1:1)","484022-20-0","D",0]
["4-(Nonafluorobutoxy)butanesulfonic acid ammonium salt","484023-69-0","D",0]
["2-Hydroxy-3-[(2-hydroxyethyl)[(nonafluorobutyl)sulfonyl]amino]propanesulfonic acid monoammonium salt","484023-82-7","D",0]
["2-Hydroxy-3-[ethyl[(nonafluorobutyl)sulfonyl]amino]propanesulfonic acid monoammonium salt","484023-83-8","D",0]
["Perfluorobutane-1-sulfonamidoethanolate ammonium salt","484024-67-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecyl acrylate","4998-38-3","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Et esters","502164-17-2","D",0]
["Perfluoro dimethylethylpentane","50285-18-2","D",0]
["Perfluoro(3-ethyl-2,3-dimethylpentane)","50285-19-3","D",0]
["(1R)-3-(2,2,3,3,4,4,4-heptafluoro-1-oxobutyl)-1,7,7-trimethylbicyclo[2.2.1]heptan-2-one","51800-99-8","D",0]
["Decanoyl chloride, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","64018-23-1","D",0]
["3,3,4,4,5,5,6,6,6-nonafluorohexanoyl chloride","64018-24-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl chloride","64018-25-3","D",0]
["Dodecanoyl chloride, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","64018-26-4","D",0]
["1,1,2,3,3-pentafluoro-3-[(trifluorovinyl)oxy]propene","64080-43-9","D",0]
["Bis(2-(perfluorododecyl)ethyl) hydrogen phosphate","57677-99-3","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with alpha-(2-methyl-1-oxo-2-propen-1-yl)-omega-hydroxypoly[oxy(methyl-1,2-ethanediyl)], tert-Bu 2-ethylhexaneperoxoate-initiated","503621-81-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with octahydro-4,7-methano-1H-indenyl 2-propenoate","504395-90-8","D",0]
["1-Hexanesulfonamide, N-[3-(dimethylamino)propyl]-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","50598-28-2","D",0]
["1-Octanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(phenylmethyl)-","50598-29-3","D",0]
["1,3-Dichloro-1,1,2,2,3-pentafluoropropane","507-55-1","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,8,8,8-dodecafluoro-7-(trifluoromethyl)octyl ester","50836-65-2","D",0]
["m-(1,1,2,2-tetrafluoroethoxy)phenyl isocyanate","50844-57-0","D",0]
["Silver pentafluoropropionate","509-09-1","D",0]
["2-Propenoic acid, esters, 2-methyl-, 2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethyl ester, polymer with butyl 2-propenoate","50937-96-7","D",0]
["2-Propanone, 1,1,1,3,3,3-hexafluoro-, polymer with ethene and 1,1,2,2-tetrafluoroethene","51023-51-9","D",0]
["Perfluorotetradecanedioic acid dihydrazide","5102-53-4","D",0]
["Benzenesulfonic acid, [[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]methyl]-, sodium salt (1:1)","51032-47-4","D",0]
["9-[(4,4,5,5,5-Pentafluoropentyl)sulfanyl]nonan-1-ol","511545-94-1","D",0]
["Ethoxy-1,1,2,2-tetrafluoroethane","512-51-6","D",0]
["2-Butenedioic acid(Z)-, mono(2,2,3,3-tetrafluoropropyl)ester, sodium salt, polymer with ethenylbenzene","51343-70-5","D",0]
["Perfluoro(dibutylmethylamine)","514-03-4","D",0]
["N-(Perfluoro-1-oxononyl)-N-methylglycine sodium salt","51588-53-5","D",0]
["Poly(oxy(trifluoro(trifluoromethyl)-1,2-ethanediyl)), alpha-(1-carboxy-1,2,2,2-tetrafluoroethyl)-omega-etrafluoro(trifluoromethyl)ethoxy)-","51798-33-5","D",0]
["3,3,4,4,5,5,6,6-octafluoroocta-1,7-diene","678-65-9","D",0]
["Hexafluoroglutaryl chloride","678-77-3","D",0]
["hexafluoroglutaryl difluoride","678-78-4","D",0]
["1H,1H,5H,5H-Perfluoro-1,5-pentanediol diacrylate","678-95-5","D",0]
["Perfluorohexadecanoic acid","67905-19-5","D",0]
["2-(Methyl((undecafluoropentyl)sulfonyl)amino)ethyl acrylate","67584-56-9","D",0]
["5-Iodoperfluoro-3-oxapentanesulfonyl fluoride","66137-74-4","D",0]
["1,1'-[oxybis(ethane-1,2-diyloxy)]bis[heptadecafluorononene]","66138-93-0","D",0]
["Ethene, 1-bromo-1,2,2-trifluoro-, telomer with tribromofluoromethane","66143-00-8","D",0]
["Butanoic acid, 2,2,3,3,4,4-hexafluoro-4-[(trifluoroethenyl)oxy]-, methyl ester, homopolymer, hydrolyzed","661476-43-3","D",0]
["1,1-dichloro-1,2,2-trifluoro-2-iodoethane  ","661-66-5","D",0]
["1,2-Dibromohexafluoropropane","661-95-0","D",0]
["1,2-Dichloro-1,1,2,3,3,3-hexafluoropropane","661-97-2","D",0]
["1,3-dichloro-1,1,2,2,3,3-hexafluoropropane","662-01-1","D",0]
["Heptafluorobutyramide","662-50-0","D",0]
["1,1,2,2,3,3,4,4-octafluoro-5-(vinyloxy)pentane","66396-73-4","D",0]
["N-[(Heptadecafluorooctyl)sulfonyl]-N-propylglycine","66551-19-7","D",0]
["1-(Perfluoroethoxy)perfluoropropane","66840-50-4","D",0]
["(Perfluorododecyl)ethylene","67103-05-3","D",0]
["Potassium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","67118-55-2","D",0]
["Potassium perfluoro(2-(2-propoxypropoxy)propanoate)","67118-57-4","D",0]
["Cyclohexanesulfonic acid, decafluoro(pentafluoroethyl)-, potassium salt (1:1)","67584-42-3","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-2-propen-1-yl-","67584-48-9","D",0]
["N-allyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptane-1-sulphonamide","67584-49-0","D",0]
["S-(3-(Ethoxycarbonylaminomethyl)-3-(perfluorohexyl)propyl)sulfurothioate sodium","67846-66-6","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-hydro-omega-hydroxy-, ether with alpha-fluoro-omega-(2-hydroxyethyl)poly(difluoromethylene) (1:1)","65545-80-4","D",0]
["2,3,3,3-Tetrafluoro-2-(nonafluorobutoxy)propanoyl fluoride","65566-03-2","D",0]
["2-Propenoic acid, 2-methyl-, 2-(diethylamino)ethyl ester, N-oxide, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and alpha-(2-methyl-1-oxo-2-propenyl)-omega-(nonylphenoxy)poly(oxy-1,2-ethanediyl)","65605-53-0","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-hydroxyethyl)-, dihydrogen 2-hydroxy-1,2,3-propanetricarboxylate","65605-56-3","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-hydroxyethyl)-, hydrogen 2-hydroxy-1,2,3-propanetricarboxylate","65605-57-4","D",0]
["hydroxybis(trifluoroacetato-O)indium","66027-94-9","D",0]
["2-Propenoic acid, 2-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl ester","67584-57-0","D",0]
["3-((Perfluoroheptyl)sulfonylamino)-N,N,N-trimethyl-1-propanaminium iodide","67584-58-1","D",0]
["2-(N-Methylperfluorobutanesulfonamido)ethyl methacrylate","67584-59-2","D",0]
["2-(Methyl((undecafluoropentyl)sulphonyl)amino)ethyl methacrylate","67584-60-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl ester","67584-61-6","D",0]
["Potassium N-ethyl-N-[(pentadecafluoroheptyl)sulphonyl]glycinate","67584-62-7","D",0]
["Ethyl N-ethyl-N-((nonafluorobutyl)sulfonyl)glycinate","67584-63-8","D",0]
["2-Propanol, 1,1,1,3,3,3-hexafluoro-, 2-(4-methylbenzenesulfonate)","67674-48-0","D",0]
["1-Chloro-1,1,2,2,3-pentafluoropropane","677-55-4","D",0]
["HFC-236cb","677-56-5","D",0]
["Heptafluoro-2-iodopropane","677-69-0","D",0]
["1,1,1,3,3,3-hexafluoropropane-2,2-diol","677-71-4","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propanoyl fluoride","677-84-9","D",0]
["1,2-Dichloro-4-iodoperfluorobutane","678-13-7","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)undecane-1,2-diol","67824-44-6","D",0]
["Dodecafluoropentane","678-26-2","D",0]
["Perfluorooctanedioic acid","678-45-5","D",0]
["Tetraethyl 4,4'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bisphthalate","67846-42-8","D",0]
["1-Heptanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-[3-(trichlorosilyl)propyl]-","67584-50-3","D",0]
["Methanesulfonic acid, 1,1,1-trifluoro-, calcium salt (2:1)","55120-75-7","D",0]
["Methanesulfonic acid, trifluoro-, compd. with N,N-dioctyl-1-octanamine (1:1)","82052-13-9","D",0]
["N-(2,3-Dihydro-2-oxo-1H-benzimidazol-5-yl)-3-oxo-2-[[2-(trifluoromethyl)phenyl]azo]butyramide","68134-22-5","D",0]
["Pentachlorotrifluoropropane","134237-31-3","D",0]
["2,2-Dichloro-1,1,1-trifluoroethane","306-83-2","D",0]
["Perfluoroindane","1736-47-6","D",0]
["Erbium, tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-3,5-octanedionato-betaO3,betaO5)-","17978-75-5","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)silanetriol","185911-29-9","D",0]
["N,N,N',N',N'',N''-Hexamethyl-1-(1,1,2,2,3,3,6,6,6-nonafluorohexyl)silanetriamine","186599-46-2","D",0]
["3-(Heptafluoroisopropoxy)propyltrimethoxysilane","19116-61-1","D",0]
["1H,1H,6H,6H-Perfluorohexane-1,6-diol diacrylate","2264-01-9","D",0]
["Tris(4-tert-butylphenyl)sulfonium perfluorobutanesulfonate","241806-75-7","D",0]
["(Perfluorocyclohexyl)methyl methacrylate","25965-83-7","D",0]
["1,1,1,2,2,3,4,4,5,5,5-Undecafluoro-3-(1,1,2,2,2-pentafluoroethyl)pentane","2690-05-3","D",0]
["Perfluoroethylcyclohexane","335-21-7","D",0]
["Perfluoro-1,3-diethylcyclohexane","335-23-9","D",0]
["1H,1H,6H,6H-Perfluoro-1,6-hexanediol","355-74-8","D",0]
["Undecafluoro(heptafluoropropyl)cyclohexane","374-59-4","D",0]
["Perfluoro-1,3,5-trimethylcyclohexane","374-76-5","D",0]
["Perfluorobutyrylamidine","375-19-9","D",0]
["Undecafluoro(1,1,1,2,3,3,3-heptafluoropropan-2-yl)cyclohexane","423-02-9","D",0]
["Perfluoromethyldecalin","51294-16-7","D",0]
["Trichloro(1,1,2,2,3,3,6,6,6-nonafluorohexyl)silane","78560-47-1","D",0]
["Siloxanes and Silicones, di-Me, Me 3,3,4,4,5,5,6,6,6-nonafluorohexyl-","882878-48-0","D",0]
["Methanesulfonamide, 1,1,1-trifluoro-N-((trifluoromethyl)sulfonyl)-, lithium salt","90076-65-6","D",0]
["Potassium N-ethyl-N-[(nonafluorobutyl)sulphonyl]glycinate","67584-51-4","D",0]
["Potassium N-ethyl-N-[(undecafluoropentyl)sulphonyl]glycinate","67584-52-5","D",0]
["Potassium N-ethyl-N-[(tridecafluorohexyl)sulphonyl]glycinate","67584-53-6","D",0]
["Perfluoroheptane sulfonamido amine","67584-54-7","D",0]
["2-(Methyl((nonafluorobutyl)sulphonyl)amino)ethyl acrylate","67584-55-8","D",0]
["3-Pyridinecarbonitrile, 4-methyl-2,6-bis((4-methylphenyl)amino)-5-((2-(trifluoromethyl)phenyl)azo)-","669005-94-1","D",0]
["2-[difluoro(3,4,5-trifluorophenoxy)methyl]-1,3-difluoro-5-[2-fluoro-4-(4-propylphenyl)phenyl]benzene","303186-36-9","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester","139322-97-7","D",0]
["4-(difluoro(3,4,5-trifluorophenoxy)methyl)-3,5-difluoro-4'-propyl-1,1'-biphenyl","303186-20-1","D",0]
["4-Chloro-alpha,alpha,alpha-trifluorotoluene","98-56-6","D",0]
["Benzamide, 3,3'-((2-chloro-5-methyl-1,4-phenylene)bis(imino(1-acetyl-2-oxo-2,1-ethanediyl)azo))bis(4-chloro-N-(2-(4-chlorophenoxy)-5-(trifluoromethyl)phenyl)-","57971-97-8","D",0]
["2-Propenoic acid, 2-methyl-, oxiranylmethyl ester, polymers with N-(butoxymethyl)-2-methyl-2-propenamide, N-(hydroxymethyl)-2-methyl-2-propenamide, .delta.-.omega.-perfluoro-C8-14-alkyl acrylate and stearyl acrylate","628723-87-5","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,2-trifluoroethyl ester, homopolymer","54802-79-8","D",0]
["2-Naphthalenecarboxamide, N,N'-(2,5-dichloro-1,4-phenylene)bis(4-((2-chloro-5-(trifluoromethyl)phenyl)azo)-3-hydroxy-","52238-92-3","D",0]
["2-Ethoxyethyl 2-(4-(3-chloro-5-trifluoromethyl-2-pyridyloxy)phenoxy)...","87237-48-7","D",0]
["2,4,6-Trimethyl-2,4,6-tris(3,3,3-trifluoropropyl)cyclotrisiloxane","2374-14-3","D",0]
["2,4,6,8-Tetramethyl-2,4,6,8-tetrakis(3,3,3-trifluoropropyl)cyclotetr...","429-67-4","D",0]
["Benzene, 1,3-bis(trifluoromethyl)-","402-31-3","D",0]
["Benzene, 1-[(trans,trans)-4'-propyl[1,1'-bicyclohexyl]-4-yl]-4-(trifluoromethoxy)-","133937-72-1","D",0]
["Bis(1,1,1,5,5,5-Hexafluoropentane-2,4-Dionato-O,O')Nickel","14949-69-0","D",0]
["Chloro-1,1,1-trifluoroethane","75-88-7","D",0]
["Cyclotetrasiloxane, 2-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)-2,4,6,8-tetramethyl- (9CI)","193425-63-7","D",0]
["Ethene, chlorotrifluoro-, polymer with 1,1-difluoroethene","9010-75-7","D",0]
["Lithium trifluoromethanesulphonate","33454-82-9","D",0]
["Poly(difluoromethylene), alpha-(cyclohexylmethyl)-omega-hydro-","65530-85-0","D",0]
["Sodium 2-((nonafluorobutylsulfonylamino)methyl)benzenesulfonate","68299-19-4","D",0]
["Benzenesulfonic acid, [[[(1,1,2,2,3,3,4,4,5,5,5-undecafluoropentyl)sulfonyl]amino]methyl]-, sodium salt (1:1)","68299-20-7","D",0]
["Benzenesulfonic acid, [[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]methyl]-, sodium salt (1:1)","68299-21-8","D",0]
["Benzenesulfonic acid, ar-[[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptyl)sulfonyl]amino]methyl]-, sodium salt (1:1)","68299-29-6","D",0]
["1-Heptanesulfonamide, N-butyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-(2-hydroxyethyl)-","68310-02-1","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], alpha-[2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]ethyl]-omega-hydroxy-","68259-38-1","D",0]
["1,1,1,2,2,3,3,4,5,5,5-Undecafluoro-4-iodopentane","68158-13-4","D",0]
["1,1-Difluoroethene, hexafluoropropene, 1-((trifluoroethenyl)oxy)heptafluoropropane, tetrafluoroethene polymer","68182-34-3","D",0]
["1,4-Butanediol, 2,3-bis[(gamma-omega-perfluoro-C6-20-alkyl)thio] derivs.","68187-24-6","D",0]
["Butanoic acid, 4-[[3-(dimethylamino)propyl]amino]-4-oxo-, 2(or 3)-[(gamma-omega-perfluoro-C6-20-alkyl)thio] derivs.","68187-25-7","D",0]
["1-Propanesulfonic acid, 2-methyl-, 2-[[1-oxo-3-[(.gamma.-.omega.-perfluoro-C4-16-alkyl)thio]propyl]amino]derivs.., sodium salts","68187-47-3","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene and 1,2,3,3,3-pentafluoro-1-propene","68214-23-3","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl ester, telomer with 2-[ethyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, 2-[ethyl[(1,1,2,2,3,3 ¿","68227-87-2","D",0]
["2-Propenoic acid, butyl ester, telomer with 2-(((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl)methylamino)ethyl 2-propenoate, 2-(methyl((1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl)amino)ethyl 2-propenoate, alpha-(2-methyl-1-oxo-2..","68227-96-3","D",0]
["2-Propenoic acid, 4-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptyl)sulfonyl]amino]butyl ester","68227-97-4","D",0]
["2-Propenoic acid, 4-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]butyl ester","68227-98-5","D",0]
["2-Propenoic acid, 4-[methyl[(1,1,2,2,3,3,4,4,5,5,5-undecafluoropentyl)sulfonyl]amino]butyl ester","68227-99-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene), 2-hydroxyethyl 2-methyl-2-propenoate and N-(hydroxymethyl)-2-propenamide","68239-43-0","D",0]
["1,1,2,2,3,3,4,4,5,5,5-undecafluoro-N-(4-hydroxybutyl)-N-methylpentane-1-sulphonamide","68239-72-5","D",0]
["1-Octanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(4-hydroxybutyl)-N-methyl-","68239-73-6","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-(4-hydroxybutyl)-N-methyl-","68239-74-7","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-(3-(trimethoxysilyl)propyl)heptane-1-sulphonamide","68239-75-8","D",0]
["1-Hexene, 3,3,4,4,5,5,6,6,6-nonafluoro-, polymer with ethene and tetrafluoroethene","68258-85-5","D",0]
["Perfluorononanesulfonyl fluoride","68259-06-3","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-(4-hydroxybutyl)-N-methylheptane-1-sulphonamide","68298-89-5","D",0]
["1-Hexanesulfonamide, N,N'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-","67939-92-8","D",0]
["Bis(2-{ethyl[(perfluoroheptyl)sulfonyl]amino}ethyl) hydrogen phosphate","67939-93-9","D",0]
["N,N',N''-(Phosphoryltris(oxyethylene))tris(N-ethyl-perfluoroheptane-1-sulphonamide)","67939-94-0","D",0]
["Trimethyl-3-(((nonafluorobutyl)sulphonyl)amino)propylammonium iodide","67939-95-1","D",0]
["2-(Methyl((pentadecafluoroheptyl)sulphonyl)amino)ethyl methacrylate","67939-96-2","D",0]
["Potassium decafluoro(trifluoromethyl)cyclohexanesulfonate","68156-07-0","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], .alpha.-[2-[ethyl[(pentadecafluoroheptyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","68259-39-2","D",0]
["2-Propenoic acid, 2-(ethyl((undecafluoropentyl)sulfonyl)amino)ethyl ester","68298-06-6","D",0]
["N-(Phenylmethyl)perfluorobutanesulfonamide","68298-07-7","D",0]
["1-Heptanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-(phenylmethyl)-","68298-10-2","D",0]
["3-([(Perfluorooctyl)sulfonyl]{3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}amino)-1-propanesulfonate","68298-11-3","D",0]
["N-(Methyl)nonafluorobutanesulfonamide","68298-12-4","D",0]
["Undecafluoro-N-methyl-1-pentanesulfonamide","68298-13-5","D",0]
["2-(Butyl((pentadecafluoroheptyl)sulphonyl)amino)ethyl acrylate","68298-60-2","D",0]
["2-Propenoic acid, 2-[butyl[(heptadecafluorooctyl)sulfonyl]amino]ethyl ester, telomer with 2-[butyl[(pentadecafluoroheptyl)sulfonyl]amino]ethyl 2-propenoate, methyloxirane polymer with oxirane di-2-propenoate, methyloxirane polymer with oxirane ¿","68298-62-4","D",0]
["2-[[[[5-[[[2-[ethyl[(heptadecafluorooctyl)sulphonyl]amino]ethoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl methacrylate","68298-72-6","D",0]
["2-[[[[5-[[[2-[ethyl[(pentadecafluoroheptyl)sulphonyl]amino]ethoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl methacrylate","68298-73-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[[[5-[[[2-[ethyl[(tridecafluorohexyl)sulfonyl]amino]ethoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl ester (9CI)","68298-74-8","D",0]
["2-[[[[5-[[[2-[ethyl[(undecafluoropentyl)sulphonyl]amino]ethoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl methacrylate","68298-75-9","D",0]
["2-[[[[5-[[[2-[ethyl[(nonafluorobutyl)sulphonyl]amino]ethoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl methacrylate","68298-76-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[[[5-[[[2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl ester, telomer with butyl 2-propenoate, 2-[[[[5-[[[2-[ethyl[ ¿","68298-78-2","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[2-[ethyl[(nonafluorobutyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","68298-79-3","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[2-[ethyl[(perfluoropentyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","68298-80-6","D",0]
["alpha-(2-(Ethyl((pentadecafluoroheptyl)sulfonyl)amino)ethyl)-omega-hydroxy poly(oxy-1,2-ethanediyl)","68298-81-7","D",0]
["Ammonium perfluoroheptanesulfonate","68259-07-4","D",0]
["2-[[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-icosafluoroundecyl)sulphonyl]methylamino]ethyl acrylate","66008-68-2","D",0]
["2-[[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl)sulphonyl]methylamino]ethyl acrylate","66008-69-3","D",0]
["2-[methyl[(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl)sulphonyl]amino]ethyl acrylate","66008-70-6","D",0]
["N-(Carboxymethyl)-N,N-dimethyl-3-(methyl((perfluorohexyl)ethylsulfonyl)amino)-1-propanaminium","66008-71-7","D",0]
["N-(2-Carboxyethyl)-N,N-dimethyl-3-[methyl[(perfluorohexyl)ethylsulfonyl]amino]-1-propanaminium","66008-72-8","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymer with .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene)","65605-58-5","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1,2,2,2-tetrafluoro-1-(fluorocarbonyl)ethyl]-.omega.-[tetrafluoro(trifluoromethyl)ethoxy]-","65208-35-7","D",0]
["1,1'-(2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene)bis(3,4-dimethylbenzene)","65294-20-4","D",0]
["4-[[3,4,4,4-Tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-buten-1-yl]oxy]benzoic acid","65439-50-1","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-hydroxyethyl)-, ester with 2,15-bis(carboxymethyl)-4,13-dioxo-3,14-dioxa-5,12-diazahexadecane-1,2,15,16-tetracarboxylic acid (6:1)","65530-58-7","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-hydroxyethyl)-, 2-hydroxy-1,2,3-propanetricarboxylate (3:1)","65530-59-8","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-hydroxyethyl)-","65530-60-1","D",0]
["Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (2:1)","65530-63-4","D",0]
["Ethanol, 2,2'-iminobis-, compd. with .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoropoly(difluoromethylene)] (1:1)","65530-64-5","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-[(1-oxooctadecyl)oxy]ethyl]-","65530-65-6","D",0]
["Poly(difluoromethylene), alpha-fluoro-omega-(2-((2-methyl-1-oxo-2-propen-1-yl)oxy)ethyl)-","65530-66-7","D",0]
["Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-, lithium salt (1:1)","65530-69-0","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-, ammonium salt","65530-70-3","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, monoammonium salt","65530-71-4","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, diammonium salt","65530-72-5","D",0]
["Ethanol, 2,2'-iminobis-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (1:1)","65530-74-7","D",0]
["Poly(difluoromethylene), .alpha.-ethenyl-.omega.-fluoro-","65530-75-8","D",0]
["Poly(difluoromethylene), alpha,omega-difluoro-","65530-82-7","D",0]
["Poly(difluoromethylene), .alpha.-[2-[(2-carboxyethyl)thio]ethyl]-.omega.-fluoro-  (Zonyl 7950)","65530-83-8","D",0]
["2-[methyl[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-pentacosafluorotridecyl)sulphonyl]amino]ethyl acrylate","66008-67-1","D",0]
["Ammonium perfluoropentanesulfonate","68259-09-6","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, ammonium salt","68259-10-9","D",0]
["Ammonium perfluoropentanoate","68259-11-0","D",0]
["Perfluorononanesulfonic acid","68259-12-1","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-Pentadecafluoro-N-methyl-1-heptanesulfonamide","68259-14-3","D",0]
["4-[methyl[(pentadecafluoroheptyl)sulphonyl]amino]butyl methacrylate","67906-38-1","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene) and N-(hydroxymethyl)-2-propenamide","65605-59-6","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene), 2-hydroxyethyl 2-methyl-2-propenoate and N-(hydroxymethyl)-2-propenamide","65605-60-9","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-3-[(2-methyl-1-oxo-2-propenyl)oxy]-, chloride, polymer with .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene), 2-hydroxyethyl 2-methyl-2-propenoate, N-(hydroxymeth...","65605-62-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with N,N-dimethyl-2-propenamide, alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene) and methyl 2-propenoate","65605-65-4","D",0]
["2-Propenoic acid, butyl ester, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene) and N-(hydroxymethyl)-2-propenamide","65605-66-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with butyl 2-propenoate, alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene) and N-(hydroxymethyl)-2-propenamide","65605-68-7","D",0]
["2-Propenoic acid, methyl ester, polymer with .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene)","65605-69-8","D",0]
["Perfluoroalkylethyl acrylate","65605-70-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with alpha-fluoro-omega-[2-[(1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene), N-(hydroxymethyl)-2-propenamide and (2,2,2-trifluoroethoxy)ethene","65605-71-2","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene), N-(hydroxymethyl)-2-propenamide and methyl 2-propenoate","65605-72-3","D",0]
["Poly(difluoromethylene), alpha-fluoro-omega-[2-[(1-oxo-2-propen-1-yl)oxy]ethyl]-, homopolymer","65605-73-4","D",0]
["2-Propenoic acid, 2-oxiranylmethyl ester, polymer with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]poly(difluoromethylene)","65605-74-5","D",0]
["Diethyl-methyl-[2-(2-methylprop-2-enoyloxy)ethyl]azanium,2-ethylhexyl 2-methylprop-2-enoate,2-hydroxyethyl 2-methylprop-2-enoate","65636-35-3","D",0]
["3,3,4,4,5,5,6,6,7,7,7-Undecafluoroheptane-1-sulphonyl chloride","65702-23-0","D",0]
["1-Undecanesulfonyl chloride, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-nonadecafluoro-","65702-24-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-Hexadecafluoro-2-iodo-10-(trifluoromethyl)undecan-1-ol","65726-35-4","D",0]
["Perfluorocyclohexanecarbonyl fluoride","6588-63-2","D",0]
["tripentacontafluoro-26-iodohexacosane","65975-15-7","D",0]
["Diisopropyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","356056-14-9","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, 1(dihydrogen phosphate)","57678-01-0","D",0]
["N-[3-(dimethylamino)propyl]-3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluoro-octane-1-sulfonamide","34455-22-6","D",0]
["Bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)tin oxide","324063-66-3","D",0]
["(prop-2-en-1-yl)tris(3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctyl)stannane","192212-66-1","D",0]
["tris(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)stannane","175354-32-2","D",0]
["4-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]butane-1thiol","36097-07-1","D",0]
["1H-Perfluorooct-1-yne","55756-24-6","D",0]
["1H,1H-Undecafluorohexylamine","355-34-0","D",0]
["(7E)-7H,8H-Hexacosafluorotetradec-7-ene","51249-67-3","D",0]
["3-perfluorohexyl-2-hydroxypropyl methacrylate","86994-47-0","D",0]
["N-Succinimidyl 4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononanoate","932710-51-5","D",0]
["bromotris(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)stannane","175354-31-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononyl iodide","34451-26-8","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononan-1-ol","80806-68-4","D",0]
["Chlorodimethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-noctyl)silane","102488-47-1","D",0]
["3-(Perfluoro-3-methylbutyl)-1,2-propenoxide 97%","54009-81-3","D",0]
["1H,1H-Tridecafluoro-1-iodoheptane","212563-43-4","D",0]
["Methyl Undecafluorohexanoate","424-18-0","D",0]
["Ethyl Perfluoroamyl Ketone","383177-55-7","D",0]
["(Perfluorohexyl)phenyliodonium Trifluoromethanesulfonate","77758-84-0","D",0]
["Phosphonic acid, P-¿(3,¿3,¿4,¿4,¿5,¿5,¿6,¿6,¿7,¿7,¿8,¿8,¿8-¿tridecafluorooctyl)¿-","252237-40-4","D",0]
["Ammonium Perfluorohexylethylsulfonate","59587-39-2","D",0]
["1-hexanol, 2,2,3,3,4,4,5,5,6,6,6-undecafluoro-","423-46-1","D",0]
["2-(Perfluoro-3-methylbutyl)ethyl methacrylate","65195-44-0","D",0]
["Perfluorododecanoic acid","307-55-1","D",0]
["Pentacosafluorotridecanoic acid","72629-94-8","D",0]
["Phosphonic acid, perfluoro-C6-12-alkyl derivs.","68412-68-0","D",0]
["undecafluorohexanoic acid","307-24-4","D",0]
["1-bromo-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexane","335-56-8","D",0]
["Thiocyanic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester","26650-09-9","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononyl methacrylate","1228350-17-1","D",0]
["1-Octanesulfonamide, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-N(2-hydroxyethyl)-N-methyl-","51619-73-9","D",0]
["Tris[4-(tridecafluorohexyl)phenyl]phosphine","193197-68-1","D",0]
["4-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)benzyl alcohol","356055-76-0","D",0]
["Tris[4-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)phenyl]phosphine","219985-31-6","D",0]
["1-Methyl-3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)imidazolium hexafluorophosphate","313475-50-2","D",0]
["N-[4-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)benzyloxycarbonyloxy] succinimide","556050-48-7","D",0]
["4,4,5,5,6,7,7,7-Octafluoro-2-hydroxy-6-(trifluoromethyl)heptyl methacrylate","16083-79-7","D",0]
["2-Chloro-4,6-bis[3-(perfluorohexyl)propyloxy]-1,3,5-triazine","916770-15-5","D",0]
["Bis(4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononyl) azodicarboxylate","452912-11-7","D",0]
["2,7-Bis(1H1H2H,2H-perfluorooctyl)-9-fluorenylmethoxycarbonyl chloride","932710-57-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-hydroxynonyl acrylate","127377-12-2","D",0]
["Perfluoroheptanoyl chloride","52447-22-0","D",0]
["2H,2H,3H,3H-Perfluorononanoic acid","27854-30-4","D",0]
["4,4,5,5,6,7,7,7-Octafluoro-2-hydroxy-6-(trifluoromethyl)heptyl acrylate","16083-76-4","D",0]
["N-(4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononyl)iodoacetamide","852527-50-5","D",0]
["N-(4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononyl)maleimide","852527-41-4","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononyl azide","852527-60-7","D",0]
["1-(Perfluorohexyl)octane","133331-77-8","D",0]
["Thionyl chloride, reaction products with ammonia and polymd. oxidized 1,1,2,3,3,3-hexafluoro-1-propene hydrolyzed high-boiling fraction non-aqueous phase","147129-88-2","D",0]
["Butyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","147224-18-8","D",0]
["1,2,3-Propanetricarboxylic acid, 1-sulfo-, C,C,C-tris[1-[(2,2,3,3,3-pentafluoropropoxy)methyl]propyl] ester, sodium salt (1:1)","1472634-24-4","D",0]
["2-{Methyl[(nonafluorobutyl)sulfonyl]amino}ethyl phosphate","147545-41-3","D",0]
["ammonium 2,2,3,3-tetrafluoropropionate","1428-27-9","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymer with 1-ethenyl-2-pyrrolidinone and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate, acetate","1334473-84-5","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1,2,2,2-tetrafluoro-1-(methoxycarbonyl)ethyl]-.omega.-[tetrafluoro(trifluoromethyl)ethoxy]-","134035-61-3","D",0]
["Perfluorooctane sulfonamido amine","13417-01-1","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, dimer","13429-24-8","D",0]
["Hexene, undecafluoro(4-sulfophenoxy)-, sodium salt","134344-15-3","D",0]
["Hexane, 1,6-diisocyanato-, homopolymer, gamma-omega-perfluoro-C6-20-alc.-blocked","135228-60-3","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl methacrylate","13695-31-3","D",0]
["Iodonium, diphenyl-, 4,4'-di-C10-13-alkyl derivs., (OC-6-11)-hexafluoroantimonates(1-)","1370442-66-2","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-[(trifluoroethenyl)oxy]butane","13782-76-8","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, fluorinated, reduced, 3-[2,4,6,8-tetramethyl-4,6,8-tris[3-(trimethoxysilyl)propyl] cyclotetrasiloxan-2-yl]propyl ethers","1378309-01-3","D",0]
["Ethanesulfonyl fluoride, 2-[1-[difluoro][(1,2,2-trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoro-, polymer with 1,1,2,2-tetrafluoroethene, hydrolyzed, potassium salts","1378928-76-7","D",0]
["Ethanesulfonyl fluoride, 2-(1-(difluoro((1,2,2-trifluoroethenyl)oxy)methyl)-1,2,2,2-tetrafluoroethoxy)-1,1,2,2-tetrafluoro-, polymer with 1,1,2,2-tetrafluoroethene, hydrolyzed","1378930-04-1","D",0]
["Propanoic acid, 3-[1-[difluoro[(1,2,2-trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, methyl ester, polymer with 1,1,2,2-tetrafluoroethene, hydrolyzed, potassium salts","1378930-30-3","D",0]
["Enflurane","13838-16-9","D",0]
["1,1'-[(difluoromethylene)bis(oxy)]bis[1,2,2-trifluoroethylene]","13845-92-6","D",0]
["1,1,2,2,3,3-Hexafluoro-1,3-bis((trifluorovinyl)oxy)propane","13846-22-5","D",0]
["Pentane, 1,1,1,2,2,3,4,5,5,5-decafluoro-","138495-42-8","D",0]
["Siloxanes and Silicones, 3-aminopropyl Me, di-Me, Me 3-mercaptopropyl, polymers with stearyl acrylate, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate, rel-(1R,2R,4R)-1,7,7-trimethylbicyclo[2.2.1]hept-2-yl methacrylate and vinyl chloride","1407491-30-8","D",0]
["Perfluoropentadecanoic acid","141074-63-7","D",0]
["Siloxanes and Silicones, di-Me, butyl- and 3-[(2-methyl-1-oxo-2-propenyl)oxy]propyl group-terminated, polymers with 2-[[(heptadecafluororoctyl)sulfonyl]methylamino]ethylacrylate and iso-Bu methacrylate","146632-08-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","80793-17-5","D",0]
["sodium hydrogen (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)phosphonate","1189052-95-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-chloroacrylate","96383-55-0","D",0]
["sodium 2-methyl-2-({3-[(3,3,4,4,5,5,6,6,7,7,8,8,8- tridecafluorooctyl)thio]propanoyl}amino)propane-1-sulfonate","62880-93-7","D",0]
["2-hydroxy-N,N,N-trimethyl-3-[(3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctyl)thio]propan-1-aminium chloride","88992-45-4","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)propene","1428-33-7","D",0]
["143336-91-8 (name too long)","143336-91-8","D",0]
["Perfluoro-N,N,N',N'-tetrakis(heptafluoropropyl)-1,6-hexanediamine","143356-32-5","D",0]
["Siloxanes und Silicones, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy Me, hydroxy Me, Me octyl, ethers with polyethylene glycol mono-Me ether","143372-54-7","D",0]
["tris(trifluoroacetato-O)iodine","14353-86-7","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.,.alpha.',.alpha.'',.alpha.'''-(oxydi-3,1,2-propanetriyl)tetrakis[.omega.-[(heptadecafluorononenyl)oxy]]-","143907-02-2","D",0]
["Sulfonium, triphenyl-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonic acid(1:1)","144317-44-2","D",0]
["1,3-Propanediol, 2,2-bis(bromomethyl)-, reaction products with ethanethiol-tetrafluoroethylene telomer","144468-31-5","D",0]
["1,3-Propanediol, 2,2-bis(bromomethyl)-, reaction products with ethanethiol-tetrafluoroethylene telomer, polymers with 1,6-diisocyanato-2,2,4(or 2,4,4)-trimethylhexane¿","144468-32-6","D",0]
["4,5-Dichloroperfluoro-3-oxapentanesulfonyl fluoride","144728-59-6","D",0]
["Perfluoro-1-(2-iodoethoxy)-2-propoxypropane","144938-16-9","D",0]
["Quaternary ammonium compounds, diethylmethyl(gamma-omega-perfluoro-C8-14-beta-alkenyl), tetraphenylborates","145477-02-7","D",0]
["Perfluoro(2-(2-propoxypropoxy)-1H,1H-propan-1-ol)","14548-74-4","D",0]
["Butyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","145510-89-0","D",0]
["Ethene, 1-(2-bromo-1,1,2,2-tetrafluoroethoxy)-1,2,2-trifluoro-, polymer with 1,1-difluoroethene, 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","145724-84-1","D",0]
["2,3,3,3-Tetrafluoro-2-{1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy}propan-1-ol","14620-81-6","D",0]
["Poly[oxy(1,1,2,2-tetrafluoro-1,2-ethanediyl)], .alpha.-(1,1-difluoro-2-hydroxyethyl)-.omega.-(1,1-difluoro-2-hydroxyethoxy)","146222-54-0","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,block, peroxidized adipoyl chloride-triethylene glycol polymer-initiated","146289-38-5","D",0]
["2-(((Heptadecafluorooctyl)sulfonyl)methylamino)ethyl methacrylate","14650-24-9","D",0]
["Perfluoro-n-undecanoic acid","2058-94-8","D",0]
["9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonadecafluoro-3-(2-hydroxyethyl)-5-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-nonadecafluoroundecyl)oxy]-4,6-dioxa-3-aza-5-phosphaheptadecan-1-ol 5-oxide","101896-22-4","D",0]
["Sulfuric acid, mono(gamma-mu-perfluoro-C8-14-alkyl) esters, ammonium salts","101940-12-9","D",0]
["Sodium perfluorobutanesulfinate","102061-82-5","D",0]
["Benzene, reaction products with chlorine and sulfur chloride (S2Cl2), hexafluoroantimonates(1-)","109037-75-4","D",0]
["Benzene, reaction products with chlorine and sulfur chloride (S2Cl2), hexafluorophosphates(1-)","109037-77-6","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, phosphat (3:1) (9CI)","106554-16-9","D",0]
["Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, salt with 1,1,2,2,2-pentafluoro-N-[(pentafluoroethyl)sulfonyl]ethanesulfonamide (1:1).","524067-96-7","D",0]
["Sulfonium, triphenyl-, salt with 1,1,2,2,3,3,4,4-octafluoro-1,4-butanedisulfonic acid (2:1).","848407-98-7","D",0]
["Propanoyl fluoride, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-, polymer with trifluoro(trifluoromethyl)oxirane, reaction products with 3-(ethenyldimethylsilyl)-N-methylbenzenamine and 2,4,6,8-tetramethylcycl¿","802935-59-7","D",0]
["Trisiloxane, 1,1,3,5,5-pentamethyl-3-[3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]butyl]-.","145782-39-4","D",0]
["3,8,11,14-Tetraoxa-2,4-disilaheptadecane, 4-[(dimethylsilyl)oxy]-10,12,12,13,15,15,16,16,17,17,17-undecafluoro-2,4-dimethyl-10,13-bis(trifluoromethyl)-.","133068-47-0","D",0]
["Propanoyl fluoride, 2,2'-[(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis(oxy)]bis[2,3,3,3-tetrafluoro-, polymer with trifluoro(trifluoromethyl)oxirane, reaction products with N-[3-(triethoxysilyl)propyl]-1,2-ethanediamine.","185701-90-0","D",0]
["Trisiloxane, 3-[(dimethylsilyl)oxy]-1,1,5,5-tetramethyl-3-(3,3,4,4,5,5,6,6,6-nonafluorohexyl)-.","178241-16-2","D",0]
["2,4,13,15-Tetrasilahexadecane, 4,13-bis[(dimethylsilyl)methyl]-7,7,8,8,9,9,10,10-octafluoro-2,4,13,15-tetramethyl-.","401510-99-4","D",0]
["Furan, tetrahydro-, polymer with 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane, monoester with [3-(carboxyamino)methyl]-3,5,5-trimethylcyclohexyl]carbamic acid mono[2-[(1-oxo-2-propenyl)oxy]ethyl] ester, 2,2,2-trifluoroethyl ether.","709670-53-1","D",0]
["Silsesquioxanes, 3,3,4,4,5,5,6,6,6-nonafluorohexyl, [(dimethylsilyl)oxy]-terminated.","507225-02-7","D",0]
["Silane, bis[(1,1-dimethyl-2-propynyl)oxy]methyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)-.","506417-14-7","D",0]
["1,1,1,2,3,3,3-heptafluoro-2-[(trifluorovinyl)oxy]propane","10372-98-2","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, polymer with octadecyl 2-methyl-2-propenoate","104242-01-5","D",0]
["Siloxanes and silicones, dimethyl, methyl 3-(1,1,2,2-tetrafluoroethoxy)propyl, methyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl-","104780-70-3","D",0]
["Perfluoroethyl vinyl ether","10493-43-3","D",0]
["1,2-Nonundiol, 4,4,5,5,6,6,7,7,8,9,9,9-dodecafluoro-8-(trifluoromethyl)-, 1-(dihydrogen phosphat)","105416-14-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ..","105656-07-3","D",0]
["1-Butene, 4-bromo-3,3,4,4-tetrafluoro-, polymer with ethene, 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","105656-63-1","D",0]
["3,7-bis(2-hydroxyethyl)-5-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-nonadecafluoroundecyl)oxy]-4,6-dioxa-3,7-diaza-5-phosphanonane-1,9-diol 5-oxide","101896-21-3","D",0]
["1,5-Trisiloxanediol, 1,1,3,5,5-pentamethyl-3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-.","1010387-03-7","D",0]
["Sulfonium, triphenyl-, 2,2'-oxybis[1,1,2,2-tetrafluoroethanesulfonate] (2:1).","848408-02-6","D",0]
["Iodonium, bis[4-(1,1-dimethylethyl)phenyl]-, 1,1,2,2,3,3,4,4-octafluoro-1,4-butanedisulfonate(2-) (2:1).","799274-55-8","D",0]
["Cyclotetrasiloxane, 2,4,6,8-tetramethyl-2-[3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]propyl]-.","756819-73-5","D",0]
["Propanoyl fluoride, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]-, polymer with 2,2,3-trifluoro-3-(trifluoromethyl)oxirane, reaction products with 3,3¿-(1,2-ethanediyl)bis[3-[(dimethylsilyl)oxy]-¿","913292-62-3","D",0]
["Siloxanes and Silicones, di-Me, Me 3,3,4,4,5,5,6,6,6-nonafluorohexyl, chloro-terminated.","908858-79-7","D",0]
["1,3,5,2,4,6-Triazatriphosphorine,2,2,4,4,6,6-hexahydrotris[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]tris(2,2,3,3,3-pentafluoropropoxy)-(9CI)","106796-59-2","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, polymer with ethenyltriethoxysilane (9CI)","106826-29-3","D",0]
["2-Propenoic acid, 2-methyl-, polymer with 2-(diethylamino)ethyl 2-methyl-2-propenoate, 2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate, acetate","1071022-26-8","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene, block","107221-31-8","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, polymer with 1,1-difluoroethene, ethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","107810-71-9","D",0]
["1,3-Propanediol, 2,2-bis(((gamma-omega-perfluoro-C6-12-alkyl)thio)methyl) derivs., polymers with 2,2-bis(((gamma-omega-perfluoro-C10-20-alkyl)thio)methyl)-1,3-propanediol,....","1078142-10-5","D",0]
["Thiols, C4-20, gamma-omega-perfluoro, telomers with acrylamide und acrylic acid, sodium salts","1078712-88-5","D",0]
["1-Propanaminium, 3-amino-N-(carboxymethyl)-N,N-dimethyl-, N-[2-[(.gamma.-.omega.-perfluoro-C4-20-alkyl)thio]acetyl] derivs., inner salts","1078715-61-3","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with (2-bromo-1,1,2,2-tetrafluoroethoxy)trifluoroethene, 1,1-difluoroethene and tetrafluoroethene","108144-05-4","D",0]
["Perfluorohexanesulfonate","108427-53-8","D",0]
["Cyclotetrasiloxane, 2,4,6,8-tetramethyl-2-[3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy] propoxy]propyl]-, Si -[3-(2-oxiranylmethoxy)propyl] derivs.","1005771-59-4","D",0]
["2-Perfluoroalkyl(C4-14)ethyl acrylate- benzyl methacrylate","100932-58-9","D",0]
["Acrinathrin","101007-06-1","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,3,3,3-pentafluoro-1-(pentafluoroethyl)-1-(trifluoromethyl)propyl ester, homopolymer","101061-04-5","D",0]
["1,1,1,3,3,4,4,4-Octafluoro-2-(trifluoromethyl)butan-2-yl 2-methylprop-2-enoate","101061-05-6","D",0]
["1-Butene, 1,1,2,3,3,4,4-heptafluoro-4-[(trifluoroethenyl)oxy]-, homopolymer","101182-89-2","D",0]
["1012783-71-9 (name too long)","1012783-71-9","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, acrylates","101316-90-9","D",0]
["2-Propenoic acid, 2-methyl-,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecylester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl...","105681-94-5","D",0]
["Trimethoxy(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","85857-16-5","D",0]
["Dimethoxymethyl(3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctyl)silane","85857-17-6","D",0]
["Alkyl iodides, C8-14, gamma-omega-perfluoro","85995-91-1","D",0]
["Ethaneperoxoic acid, reaction products with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl thiocyanate and3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl thiocyanate","182176-52-9","D",0]
["Pentane, 1,1,1,2,2,3,4,5,5,5-decafluoro-3-methoxy-4-(trifluoromethyl)-","132182-92-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-6-iodohexane","355-43-1","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1,1'-(hydrogen phosphat)","678-41-1","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphat)","57678-03-2","D",0]
["1,2-Heptadecanediol,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-16-(trifluoromethyl)-, 1-(dihydrogen phosphat),diammonium salt (9CI)","94200-52-9","D",0]
["1,2-Pentadecanediol,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)-, 1-(dihydrogen phosphat), diammonium salt (9CI)","94200-51-8","D",0]
["1,2-Tridecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-eicosafluoro-12-(trifluoromethyl)-, 1-(dihydrogen phosphat), diammoniumsalt (9CI)","94200-50-7","D",0]
["1,2-Heptadecanediol,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonacosafluoro-, 1-(dihydrogen phosphat), diammonium salt (9CI)","94200-48-3","D",0]
["1,2-Pentadecanediol,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-, 1-(dihydrogen phosphat), diammonium salt (9CI)","94200-47-2","D",0]
["1,2-Tridecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro-, 1-(dihydrogen phosphat), diammonium salt (9CI)","94200-46-1","D",0]
["1,2-Tridecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro-, 1-(dihydrogen phosphat)","94158-70-0","D",0]
["1,2-Heptadecanediol,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,17,17,17-octacosafluoro-16-(trifluoromethyl)-, 1-(dihydrogen phosphat)","63295-29-4","D",0]
["1,2-Pentadecanediol,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)-, 1-(dihydrogen phosphat)","63295-28-3","D",0]
["1,2-Tridecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-eicosafluoro-12-(trifluoromethyl)-, 1-(dihydrogen phosphat)","63295-27-2","D",0]
["Decanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","27854-31-5","D",0]
["2-Decenoic acid, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluoro-","70887-84-2","D",0]
["Dodecanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-","53826-13-4","D",0]
["Perfluorononan-1-oic acid","375-95-1","D",0]
["Perfluoromyristic acid","376-06-7","D",0]
["Nonadecafluorodecanoic acid","335-76-2","D",0]
["N-[3-(dimethylamino)propyl]-3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctanesulphonamide N-oxide","80475-32-7","D",0]
["3-Iodo-1,1,2,2-tetrafluoropropyl trifluorovinyl ether","106108-22-9","D",0]
["1-1-Difluoro(trifluoroethenyl)oxymethyl-1,2,2,2-tetrafluoroethoxy-1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propane polymer with tetrafluoroethene and 1,1,2,2-tetrafluoro-3-iodo-1-(trifluoroethenyl)oxypropane","106108-23-0","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-(1,1,2,2-tetrafluoro-3-iodopropoxy)propanoate","106394-03-0","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(1,1,2,2-tetrafluoro-3-iodopropoxy)-, sodium salt","106394-04-1","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2-tetrafluoro-3-iodopropoxy)propoxy]propanoate","106394-05-2","D",0]
["1H,1H-Tridecafluoroheptylamine","423-49-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptan-1-ol","375-82-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-ol","647-42-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-8-iodooctane","2043-57-4","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester","2144-53-8","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl acrylate","17527-29-6","D",0]
["Ammonium undecafluorohexanoate","21615-47-4","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooct-1-ene","25291-17-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctanesulphonyl chloride","27619-89-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctanesulphonic acid","27619-97-2","D",0]
["Carboxymethyldimethyl-3-[[(3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctyl)sulphonyl]amino]propylammonium hydroxide","34455-29-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-8-iodononane","38550-34-4","D",0]
["(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl)oxirane","38565-52-5","D",0]
["2-[methyl[(3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctyl)sulphonyl]amino]ethyl acrylate","49859-70-3","D",0]
["Silane, triethoxy(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-","51851-37-7","D",0]
["Potassium 3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctanesulphonate","59587-38-1","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro","68391-08-2","D",0]
["Dichloromethyl(3,3,4,4,5,5,6,6,7,7,8,8,8tridecafluorooctyl)silane","73609-36-6","D",0]
["Trichloro(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","78560-45-9","D",0]
["Perfluoro-2,5-dimethyl-3,6-dioxanonanoic acid","13252-14-7","D",0]
["Perfluoro-2,5,8,11,14-pentamethyl-3,6,9,12,15-pentaoxaoctadecanoyl fluoride","13252-15-8","D",0]
["Mercury bis(trifluoroacetate)","13257-51-7","D",0]
["Lithium bis[(pentafluoroethyl)sulfonyl]azanide","132843-44-8","D",0]
["2-(((Heptadecafluorooctyl)sulphonyl)propylamino)ethyl methacrylate","13285-40-0","D",0]
["alpha-fluoro-omega-(2-hydroxyethyl)poly(difluomethylene)","126927-97-7","D",0]
["Broflanilide","1207727-04-5","D",0]
["Poly[oxy(1,1,2,2,3,3-hexafluoro-1,3-propanediyl)], .alpha.-(2-carboxy-1,1,2,2-tetrafluoroethyl)-.omega.-(1,1,2,2,3,3,3-heptafluoropropoxy)-","120895-92-3","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoro-6-[(trifluoroethenyl)oxy]hexanenitrile","120903-40-4","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,block","121065-52-9","D",0]
["Noviflumuron","121451-02-3","D",0]
["3,5-dichloro-2-fluoro-4-(1,1,2,3,3,3-hexafluoropropoxy)aniline","121451-05-6","D",0]
["Borate(1-), tetrahydro-, sodium (1:1), reaction products with reduced polymd. oxidized tetrafluoroethylene, hydrolyzed, diallyl ethers, polymers with 2,4,6,8-tetramethylcyclotetrasiloxane, Si-(8,13-dioxo-4,7,12-trioxa-9-azapentadec¿","1214752-87-0","D",0]
["N,N'-bis(2-hydroxy-6,6,7,7-tetrafluoro-4-oxaheptyl)tetramethylethylenediaminium chloride","1220100-43-5","D",0]
["Perfluoro-3-[3-[3-(propoxy)propoxy]propoxy]propanoyl fluoride","122075-99-4","D",0]
["Perfluoro-3,7,11-trioxatetradecane","122076-00-0","D",0]
["2-Perfluoroalkyl(C4-14)ethyl acrylate-ethyl methacrylate-polyethylene glycol mono methacrylate copolymer","122304-67-0","D",0]
["Phosphoric acid, mixed esters with polyethylene glycol and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-octanol, ammonium salts","1224429-82-6","D",0]
["6,9,12,15-Tetraoxa-2-silaoctadecane, 2,2-dichloro-8,10,10,11,13,13,14,16,16,17,17,18,18,18-tetradecafluoro-8,11,14-tris(trifluoromethyl)-","122734-47-8","D",0]
["1,2-Dichloro-1,1,2,3,3,4,4-heptafluoro-4-[(1,2,2-trifluoroethenyl)oxy]butane","122857-45-8","D",0]
["Poly(difluoromethylene), .alpha.-[2-(acetyloxy)-3-[(carboxymethyl)dimethylammonio]propyl]-.omega.-fluoro-, inner salt","123171-68-6","D",0]
["Potassium trifluorotris(perfluoroethyl)phosphate","123215-04-3","D",0]
["Perfluoro(4a-(cyclohexylmethyl)decahydronaphthalene)","125061-94-1","D",0]
["Perfluoro-2-methyl-3-oxahexanoic acid","13252-13-6","D",0]
["N-(2-Carboxyethyl)-N,N-dimethyl-3-[(perfluoro-1-oxodecyl)amino]propanaminium","113933-98-5","D",0]
["Hexafluoroacetone-trifluoroethene-vinylidene fluoride copolymer","114502-89-5","D",0]
["4-(1H,1H-Perfluoropropyl)-1,3-dioxolan-2-one","114810-51-4","D",0]
["Cyclobutane, octafluoro-","115-25-3","D",0]
["Siloxanes and Silicones, di-Me, Me 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl","115340-95-9","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-iodo-6-(trifluoromethyl)aniline","1207315-39-6","D",0]
["Quaternary ammonium compounds, diethylmethyl(gamma-omega-perfluoro-C8-14-beta-alkenyl), Me sulfates","127133-57-7","D",0]
["2-Propenoic acid, 2-methyl-, polymers with Bu methacrylate, lauryl methacrylate and 2-[methyl[(perfluoro-C4-8-alkyl)sulfonyl]amino]ethyl methacrylate","127133-66-8","D",0]
["Hexane, 1,6-diisocyanato-, homopolymer, .alpha.-[1-[[[3-[[3-(dimethylamino)propyl]amino]propyl]amino]carbonyl]-1,2,2,2-tetrafluoroethyl]-.omega.-(1,1,2,2,3,3,3-heptafluoropropoxy)poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]]-blocked","1279108-20-1","D",0]
["Poly[oxy(1,1,2,2-tetrafluoro-1,2-ethanediyl)], alpha-(1,1-difluoro-2-methoxy-2-oxoethyl)-omega-(1,1-difluoro-2-methoxy-2-oxoethoxy)-","130030-19-2","D",0]
["[(Perfluoroheptanoyl)amino]-3-betaine","130114-31-7","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoic acid--ammonia (1/1)","13043-05-5","D",0]
["1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl acrylate","13057-08-4","D",0]
["1,4-Dichloro-2-(1,1,2,3,3,3-hexafluoropropoxy)-5-nitrobenzene","130841-23-5","D",0]
["Hexafluoroacetone sesquihydrate","13098-39-0","D",0]
["Poly(difluoromethylene), .alpha.-chloro-.omega.-(1-chloro-1-fluoroethyl)-","131324-06-6","D",0]
["Perfluoro-2-methyl-3-oxaoctanedioyl fluoride","13140-22-2","D",0]
["Perfluoro-2,5,8,11,14,17-hexamethyl-3,6,9,12,15,18-hexaoxaheneicosanoyl fluoride","13140-24-4","D",0]
["Perfluoro-2,5,8,11,14,17,20-heptamethyl-3,6,9,12,15,18,21-heptaoxatetracosanoyl fluoride","13140-25-5","D",0]
["Perfluoro-2,5,8,11,14,17,20,23-octamethyl-3,6,9,12,15,18,21,24-octaoxaheptacosanoyl fluoride","13140-26-6","D",0]
["Methyl perfluoro(2-propoxypropanoate)","13140-34-6","D",0]
["2-Methoxy-2H-perfluoropropane","13171-18-1","D",0]
["Dichlorotetrafluoroethane","1320-37-2","D",0]
["Hexafluoro-1,3-bis(trifluoromethyl)cyclobutane","13221-71-1","D",0]
["3-(Perfluoro-2-butyl)propane-1,2-diol","125070-38-4","D",0]
["2-Propanol, 1-[(2-dodecylhexadecyl)oxy]-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","160819-50-1","D",0]
["2-Propanol, 1,3-bis[(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl)thio]-","160819-47-6","D",0]
["Ethanesulfonic acid, 2-[(3,3,4,4,5,5,6,6,7,7,8,8,9, 9,10,10,10-heptadecafluorodecyl)thio]-, lithium salt (1:1)","441765-14-6","D",0]
["Propanoic acid, 3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluorodecyl)thio]-, lithium salt (1:1)","481050-04-8","D",0]
["Propanoic acid, 3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluorodecyl)thio]-","54207-62-4","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, 1-(dihydrogen phosphat), ammonium salt (1:1)","93776-21-7","D",0]
["1-Tridecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-tricosafluoro-","1545-59-1","D",0]
["1-Pentadecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-heptacosafluoro-","176676-70-3","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, lithium salt (1:1)","17125-58-5","D",0]
["Hexanoic acid, 2,3,4,4,5,5,6,6,6-nonafluoro-2,3-bis(trifluoromethyl)-","1812247-18-9","D",0]
["Octanamide, N-(3-aminopropyl)-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","85938-56-3","D",0]
["1-Octanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-","4151-50-2","D",0]
["Nonene, heptadecafluoro-1-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]- (9CI)","84029-60-7","D",0]
["1-Propanesulfonic acid, 3-[ethyl(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, sodium salt (1:1)","89685-61-0","D",0]
["1-Propanaminium, N,N,N-trimethyl-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, chloride (1:1)","53517-98-9","D",0]
["Benzenesulfonyl chloride, 3,4-bis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-","24216-05-5","D",0]
["Octanamide, N-[3-[bis(2-hydroxyethyl)amino]propyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","41358-63-8","D",0]
["1-Propanaminium, N-(2-carboxyethyl)-N,N-bis(2-hydroxyethyl)-3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]-, inner salt","39186-68-0","D",0]
["Diphosphoric acid, mono(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl) ester, compd. with 2,2¿,2¿¿-nitrilotris[ethanol] (1:3)","98005-85-7","D",0]
["Undecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","1835250-28-6","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","77117-48-7","D",0]
["Silane, tetrakis[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl)thio]ethyl]-","1189587-64-1","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)tris(1-methylethoxy)-","246234-80-0","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)trimethoxy-","123445-18-1","D",0]
["2-Propanol, 1-[(2-decyltetradecyl)oxy]-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","160819-49-8","D",0]
["2-Propanone, 1,1,1,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene, tetrafluoroethene and trifluoroethene","125128-66-7","D",0]
["8-(Ethenyloxy)-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","125660-00-6","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1,2,2,2-tetrafluoro-1-(hydroxymethyl)ethyl]-.omega.-[tetrafluoro(trifluoromethyl)ethoxy]-","126066-30-6","D",0]
["Ethanol, 2,2¿-[oxybis(2,1-ethanediyloxy)]bis-, ethers with ethoxylated reduced Me esters of reduced polymd. oxidized tetrafluoroethylene","1260733-08-1","D",0]
["Thieno[3,4-b]thiophene, homopolymer, 2-[1-[difluoro[(1,2,2-trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoroethanesulfonic acid-tetrafluoroethylene polymer-doped","1269217-82-4","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-,dihydrogen phosphat, diammonium salt (9CI)","93857-44-4","D",0]
["Phosphoric acid, mono(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl) mono(3,3,4, 4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl) ester","1578186-42-1","D",0]
["Phosphoric acid, mono(3,3,4,4,5,5,6,6,7,7,8,8,9, 9,10,10,11,11,12,12,12-heneicosafluorododecyl) mono(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl) ester","1158182-61-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluoro-1-(hydroxymethyl)decyl ester","146955-29-5","D",0]
["Phosphoric acid, mono(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,11,11,12,12,12-heneicosafluoro dodecyl) mono(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluorodecyl) ester","1158182-60-5","D",0]
["Diphosphoric acid, mono(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl) ester, compd. with 2-aminoethanol (1:3)","98005-84-6","D",0]
["Acetamide, N-[3-(dimethylamino)propyl]-2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12, 12,12-heneicosafluorododecyl) thio]-","1513863-92-7","D",0]
["1-Decanesulfonamide, 3,3,4,4,5,5,6,6,7,7,8,8,9, 9,10,10,10-heptadecafluoro-N-[3-(phosphorno oxy)propyl]-N-propyl-, sodium salt (1:2)","441765-20-4","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1,1',1''-phosphat","149790-22-7","D",0]
["Phosphoric acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10, 11,11,12,12,12-heneicosafluorododecylbis (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) ester","1578186-57-8","D",0]
["Phosphoric acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10, 11,11,12,12,12-heneicosafluorododecyl 3,3,4,4, 5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester","1578186-64-7","D",0]
["Phosphoric acid, bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl) 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester","1578186-56-7","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphat), ammonium salt (1:1)","93776-20-6","D",0]
["Acetamide, N-[3-(dimethylamino)propyl]-2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","1513863-91-6","D",0]
["Ethanaminium, 2-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl)thio]ethoxy]-N,N,N-trimethyl-, iodide (1:1)","71625-52-0","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-, chloride (1:1)","71940-07-3","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12, 12-heneicosafluorododecyl)sulfinyl]-","1513864-17-9","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","727351-53-3","D",0]
["2,5,8,11,14,17,20,23-Octaoxa-27-thiaheptatria contan-25-ol, 30,30,31,31,32,32,33,33,34,34,35, 35,36,36,37,37,37-heptadecafluoro-","121912-28-5","D",0]
["Sodium 1,1,2,2-Tetrafluoro-2-(1,2,2,2-tetrafluoroethoxy)ethane-1-sulfonate","1132933-86-8","D",0]
["(2R,4R)-1,1,2,3,3,4-Hexafluoro-2,4-bis(trifluoromethyl)cyclobutane","1583-98-8","D",0]
["Perfluoro(2-methylpent-2-ene)","1584-03-8","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with tetrafluoroethene, oxidized","158706-63-9","D",0]
["Perfluoro-5-(trifluoromethyl)hexanoic acid","15899-29-3","D",0]
["Perfluoro-6-methylheptanecarboxylic acid","15899-31-7","D",0]
["2-(Difluoroiodomethyl)-1,1,1,2,3,3,3-heptafluoropropane","1542-18-3","D",0]
["3-(Perfluoroethyl)propanol","148043-73-6","D",0]
["Fatty acids, C18-unsatd., trimers, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl esters","148240-79-3","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-(hydroxyethyl)-N-methyl, reaction products with 1,6-diisocyanatohexane homopolymer and ethylene glycol","148684-79-1","D",0]
["Bis(3-(perfluoroethyl)-1-(9-bromononyl)propyl) thioether","148757-89-5","D",0]
["2-Propenoic acid, 2-methyl-, C12-18-alkyl esters, polymer with .alpha.-fluoro-.omega.-[2-[(1-oxy-2-propenyl)oxy]ethyl]poly(difluoromethylene) and vinylidene chloride","148878-17-5","D",0]
["Perfluoroheptanedioic acid","14919-09-6","D",0]
["4-(Methyl((nonafluorobutyl)sulfonyl)amino)butyl prop-2-enoate","1492-87-1","D",0]
["2,3-Dichloro-1,1,1,2-tetrafluoropropane","149329-25-9","D",0]
["6:2 Fluorotelomer thioether propanoic acid","149339-57-1","D",0]
["4(perfluorooctyl)-2-butanol","149868-74-6","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene, ethene, 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","149935-01-3","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers withBu acrylate, gamma-omega-perfluoro-C8-14-alkyl acrylate und polyethylene glycolmonomethacrylate¿","150135-57-2","D",0]
["3:2 Fluorotelomer iodide","1513-88-8","D",0]
["Copoly[2,2-bis[4-(4-aminophenoxy)phenyl]propane, 2,2-bis[4-(4-aminophenoxy)phenyl]hexafluoropropane, 1,3-bis(3-aminopropyl)-1,1,3,3-tetramethyldisiloxane, tertphthaloyl chloride, isophthaloyl chloride] 1,3-Benzenedicarbonyl dichloride, polymer ¿","151402-74-3","D",0]
["Hexafluoro-2-methyl-2-propanol","1515-14-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,10,10,10-hexadecafluoro-9-(trifluoromethyl)decyl methacrylate","15166-00-4","D",0]
["(E)-Perfluoro-2-butene","1516-64-9","D",0]
["cis-Perfluoro-2,4-dimethylcyclobutane","1583-97-7","D",0]
["2,2,2-tris(Trifluoromethyl)ethanol","14117-17-0","D",0]
["2-Methyl-2-propenoic acid methyl ester, 2,2,3,3,3-pentafluoropropyl 2-methyl-2-propenoate-2,2,3,3-tetrafluoropropyl 2-methyl-2-propenoate copolymer","142033-27-0","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., fluorinated, reduced, 3-[tris[3-(trimethoxysilyl)propyl]silyl]propyl ethers","1422364-27-9","D",0]
["3,5,6-Trichloro-2,2,3,4,4,5,6,6-octafluorohexanoyl chloride","1422-98-6","D",0]
["2-Propenoic acid, 2-methyl-, octadecyl ester, polimer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, ¿","142636-88-2","D",0]
["4,4'-(2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene)diphenol","1478-61-1","D",0]
["trifluoro(1,1,2,2,3,4,4-heptafluorobut-3-enyl)oxirane","15453-10-8","D",0]
["Benzoic acid, ethenyl ester, polymer with propanoic acid, 2,2-dimethyl-, ethenyl ester, 1-butanol 4-(ethenyloxy)-, 1-propene, 2-methyl- and ethene, tetrafluoro-","154532-82-8","D",0]
["7H-Perfluoroheptanoic acid","1546-95-8","D",0]
["Magnesium, chloro-2-propen-1-yl-, reaction products with Me esters of fluorinated reduced polymd. oxidized tetrafluoroethylene and trimethoxysilane","1538576-70-3","D",0]
["Quaternary ammonium compoands, diethylmethyl(gamma-omega-perfluoro-C8-14-beta-alkenyl), tetrafluoroborates","153325-45-2","D",0]
["1H,1H,2H-Perfluorocyclopentane","15290-77-4","D",0]
["Bis(perfluoroethanesulfonyl)imide","152894-10-5","D",0]
["2-Propenoic acid, hexadecyl ester, polymer with .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and octadecyl 2-propenoate","152521-13-6","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymer withchloroethene and .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene)","152521-12-5","D",0]
["2,3,3,4,4,5,5-Heptafluoro-1-pentene","1547-26-8","D",0]
["2-Propenoic acid, 2-methyl-, butyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate, 2-hydroxyethyl 2-methyl-2-propenoate and methyl 2-methyl-2-propenoate,block (9CI)","154965-63-6","D",0]
["Trichloro(3-(1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethoxy)propyl)silane","15538-93-9","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,10,10,10-hexadecafluoro-9-(trifluoromethyl)decyl acrylate","15577-26-1","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, N-(3-isocyanatomethylphenyl)carbamates","1564254-27-8","D",0]
["2-Oxiranemethanol, polymers with reduced Me esters of reduced polymd. oxidized tetrafluoroethylene","156559-18-1","D",0]
["Perfluoro-9-methyldecanoyl fluoride","15720-98-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,8,8,8-Tetradecafluoro-7-(trifluoromethyl)octyl fluoride","15742-62-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-docosafluoro-11-(trifluoromethyl)dodecanoyl fluoride","15811-52-6","D",0]
["Thiols, C4-20, gamma-omega-perfluoro, reaction products withhexakis(methoxymethyl)melamine und vinyl tert-decanoate","151686-30-5","D",0]
["(2R,3R)-2,3-Dichloro-1,1,1,2,3,4,4,4-octafluorobutane","119450-81-6","D",0]
["3-[2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)propoxy]prop-1-ene","119511-16-9","D",0]
["Methyldichloro[3-[2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propoxy]propyl]silane","119511-19-2","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate, ¿","119973-85-2","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with 1-ethenyl-2-pyrrolidinone, 2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate, sodium salt","1206450-10-3","D",0]
["2-Propenoic acid, 2-methyl-, polymer with 2-hydroxyethyl 2-methyl-2-propenoate, alpha-(1-oxo-2-propen-1-yl)-omega-hydroxypoly(oxy-1,2-ethanediyl) and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate, sodium salt","1158951-86-0","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymer with 2-hydroxyethyl 2-propenoate, .alpha.-(2-methyl-1-oxo-2-propen-1-yl)-.omega.-methoxypoly(oxy-1,2-ethanediyl) and 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane polymer with¿","1092822-31-5","D",0]
["4,4'-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]bisbenzenamine","1095-78-9","D",0]
["N-(Carboxymethyl)-N-[3-[[(perfluorooctyl)sulfonyl]amino]propyl]-N,N-bis(2-hydroxy-3-sulfopropyl)ammonium chloride, trisodium","109669-84-3","D",0]
["Imidodicarbonic diamide, N,N¿,2-tris(6-isocyanatohexyl)-, reaction products with 3-chloro-1,2-propanediol and alpha-fluoro-omega-(2-hydroxyethyl)poly(difluoromethylene)","110053-43-5","D",0]
["Perfluoroalkyl(C4-C14)carbonyl aminohexanoic acid, ammonium salt","110070-82-1","D",0]
["alpha-[2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propylamino]ethyl]-omega-(4-sulfobutoxy)-poly(oxy-1,2-ethanediyl) sodium salt (1:1)","110494-69-4","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,octadecyl 2-propenoate,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12¿","110570-84-8","D",0]
["2-[[3-[(Perfluorooctyl)sulfonyl]propyl]amino]ethyl-2-propenoate","110570-90-6","D",0]
["2-Propenoic acid, 2-[[3-[(heptadecafluorooctyl)sulfonyl]propyl]amino]ethyl ester polymer with .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-hydroxypoly(oxy-1,2-ethanediyl)","110570-91-7","D",0]
["2-Propenoic acid, 2-[[3-[(heptadecafluorooctyl)sulfonyl]propyl]amino]ethyl ester polymer with .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-hydroxypoly[oxy(methyl-1,2-ethanediy)]","110570-92-8","D",0]
["5,5'-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]-bis(1,3-isobenzofurandione)","1107-00-2","D",0]
["An acrylate-perfluoroalkyl copolymer surfactant (3M Co.) (Fluorad FC 430)","11114-17-3","D",0]
["Ethanesulfonic acid, 1,1,2,2-tetrafluoro-2-((trifluoroethenyl)oxy)-, polymer with tetrafluoroethene","111173-25-2","D",0]
["(1Z)-1-Chloro-2,3,3,3-tetrafluoroprop-1-ene","111512-60-8","D",0]
["Tetraconazole","112281-77-3","D",0]
["Perfluoro(2-[(1-propoxypropan-2-yl)oxy]propanoyl) fluoride","112820-37-8","D",0]
["Oxetane, 2,2,3,3-tetrafluoro-, homopolymer, fluorinated","113114-19-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate und2-(phosphonooxy)ethyl 2-methyl-2-propenoate, block (9CI)","113150-11-1","D",0]
["N-(2-Carboxyethyl)-3-[(perfluoro-1-oxononyl)amino]-N,N-dimethyl-1-propanaminium","119131-05-4","D",0]
["3-Chloro-1,1,1,2-tetrafluoropropane","151771-09-4","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[[[[1,3,3-trimethyl-5-[[[[(1-methylpropylidene)amino]oxy]carbonyl]amino]cyclohexyl]methyl]amino]carbonyl]oxy]ethyl ester, polymer with alpha-fluoro-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene)","152286-23-2","D",0]
["Oxirane, methyl-, polymer with oxirane, mono(2-methyl-2-propenoate), octyl ether, polymer with alpha-fluoro-omega-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and alpha-(2-methyl-1-oxo-2-propenyl)-omega-hydroxypoly[oxy(methyl¿","152286-25-4","D",0]
["4,5-epoxy-1,1,2,3,3,4,5,5-octafluoropent-1-ene","15453-08-4","D",0]
["1,1'-isopropylidenebis[4-(1,1,2,2-tetrafluoroethoxy)benzene]","1544-19-0","D",0]
["1333523-10-6 (name too long)","1333523-10-6","D",0]
["Propane, 1,1,1,2,2,3,3-heptafluoro-3-[(1,2,2-trifluoroethenyl)oxy]-, polymer with 1-chloro-1,2,2-trifluoroethene and 1,1,2,2-tetrafluoroethene","116018-07-6","D",0]
["Ethene, 1,1,2,2-tetrafluoro-","116-14-3","D",0]
["Hexafluoropropene","116-15-4","D",0]
["N-Ethyl-N-(perfluoro-1-oxoheptyl)-glycine sodium salt","116537-74-7","D",0]
["4,4'-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]bis-benzoic acid","1171-47-7","D",0]
["1-[5-(Polyfluorophenyl)-4,5-dihydro-3-heteromonocycle]substituted-ethyl","1173693-36-1","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,2,3,3,4,4-octafluoro-4-(fluorosulfonyl)butoxy]propanoyl fluoride","117516-16-2","D",0]
["Lithium perfluoroheptanesulfonate","117806-54-9","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, reaction products with epichlorohydrin,polyethylene glycol mono-Me ether und N,N',2-tris(6-isocyanatohexyl)imidodicarbonic diamide","118102-37-7","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, reaction products with epichlorohydrin,tetrahydrofuran homopolymer und N,N',2-tris(6-isocyanatohexyl)imidodicarbonic diamide","118102-38-8","D",0]
["Disulfides, bis(gamma-omega-perfluoro-C6-20-alkyl)","118400-71-8","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with rel-(1R,2R,4R)-1,7,7-trimethylbicyclo[2.2.1]hept-2-yl 2-propenoate (9CI)","118570-85-7","D",0]
["Copolymer of octadecyl acrylate / chloroethene / docosyl acrylate / 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate / N-(hydroxymethyl)acrylamide","1187311-64-3","D",0]
["Perfluoro(methyl vinyl ether)","1187-93-5","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorononane","1190430-21-7","D",0]
["Acetic acid, 2,2-difluoro-2-[[2,2,4,5-tetrafluoro-5-(trifluoromethoxy)-1,3-dioxolan-4-yl]oxy]-, ammonium salt (1:1)","1190931-27-1","D",0]
["2,2-Difluoro-2-[[2,2,4,5-tetrafluoro-5-(trifluoromethoxy)-1,3-dioxolan-4-yl]oxy]acetic acid","1190931-41-9","D",0]
["Flupoxam","119126-15-7","D",0]
["Siloxanes and Silicones, Me hydrogen, [[7,9,9,10,12,12,13,13,14,14,14-undecafluoro-1,1-dimethyl-7,10-bis(trifluoromethyl)-5,8,11-trioxa-1-silatetradec-1-yl]oxy]-terminated.","1010423-83-2","D",0]
["heptadecafluoro-N-methylisooctanesulphonamide","93894-71-4","D",0]
["tetraethylammonium heptadecafluoroisooctanesulphonate","93894-70-3","D",0]
["Isooctanesulfonic acid, heptadecafluoro-, potassium salt","93894-68-9","D",0]
["diethyl[3-[[(heptadecafluoroisooctyl)sulphonyl]amino]propyl]methylammonium iodide","93894-72-5","D",0]
["magnesium heptadecafluoroisooctanesulphonate","93894-73-6","D",0]
["9-octadecenyl [5-[[[2-[[(heptadecafluoroisooctyl)sulphonyl]methylamino]ethoxy]carbonyl]amino]-2-methylphenyl]carbamate","93894-74-7","D",0]
["((Perfluorohexadecyl)methyl)oxirane","94158-68-6","D",0]
["((Perfluoro-11-methyldodecyl)ethyl) dihydrogen phosphate","94200-57-4","D",0]
["(Perfluoro-9-methyldecyl)ethyl dihydrogen phosphate","94200-56-3","D",0]
["16:2 Fluorotelomer dihydrogen phosphate","94200-55-2","D",0]
["14:2 Fluorotelomer dihydrogen phosphate","94200-54-1","D",0]
["Diammonium 3-(perfluoro-15-methylhexadecyl)-2-hydroxypropyl dihydrogen phosphate","94200-53-0","D",0]
["methyl trimethyl-2(or 3)-[[[4-[[4,4,5,5,5-pentafluoro-3-(pentafluoroethyl)-1,2,3-tris(trifluoromethyl)-1-pentenyl]oxy]phenyl]sulphonyl]amino]propylammonium sulphate","93951-33-8","D",0]
["bis(tridecafluorohexyl) disulphide","93962-52-8","D",0]
["methyl 4-(1,1,2,2-tetrafluoroethoxy)benzoate","93982-47-9","D",0]
["sodium 4-[[1,4,4,5,5,5-hexafluoro-1,2,3-tris(trifluoromethyl)-2-pentenyl]oxy]benzenesulphonate","94042-94-1","D",0]
["sodium 4-[[1,3,4,4,5,5,5-heptafluoro-2-[2,2,3,3,3-pentafluoro-1-(pentafluoroethyl)-1-(trifluoromethyl)propyl]-3-(trifluoromethyl)-1-pentenyl]oxy]benzenesulphonate","94042-95-2","D",0]
["trimethyl-3-[[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulphonyl]amino]propylammonium iodide","94088-80-9","D",0]
["Tetradecanoic acid, 1,1'-(methyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silylene) ester","94094-26-5","D",0]
["Pentanoic acid, 4,4-bis[(.gamma.-.omega.-perfluoro-C6-12-alkyl)thio] derivatives, compounds with diethanolamine","94095-37-1","D",0]
["Sodium 3-[[3-(dimethylamino)propyl][(perfluorooctyl)sulfonyl]amino]-2-hydroxypropanesulfonate","94133-90-1","D",0]
["3-((Perfluorooctylsulfonyl)-2-hydroxy-3-sulfopropylamino)-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium  monosodium hydroxide","94133-91-2","D",0]
["2,6-difluoro-N-[[[2-methyl-4-[2,2,2-trifluoro-1-hydroxy-1-(trifluoromethyl)ethyl]phenyl]amino]carbonyl]benzamide","94157-91-2","D",0]
["N-[[[2,5-dimethyl-4-[2,2,2-trifluoro-1-hydroxy-1-(trifluoromethyl)ethyl]phenyl]amino]carbonyl]-2,6-difluorobenzamide","94157-92-3","D",0]
["Diammonium 3-(perfluorohexadecyl)-2-hydroxypropyl dihydrogen phosphate","94200-49-4","D",0]
["bis(2-hydroxyethyl)ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl] phosphate","93776-30-8","D",0]
["bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl] hydrogen phosphate, compound with 2,2'-iminodiethanol (1:1)","93776-31-9","D",0]
["(2-Carboxylatoethyl)-3-((perfluoro-9-methyldecyl)-2-hydroxypropyl)aminopropyldimethylammonium","93777-12-9","D",0]
["Ammonium bis((perfluorotetradecyl)ethyl) phosphate","93777-13-0","D",0]
["diethyl[3-[[(heptadecafluorooctyl)sulphonyl]amino]propyl]methylammonium iodide","93803-06-6","D",0]
["Isooctanesulfonic acid, heptadecafluoro-, lithium salt","93894-67-8","D",0]
["(Perfluorooctyl)-2-hydroxypropyl dihydrogen phosphate","94158-69-7","D",0]
["Bis(2-hydroxyethyl)methyl[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-2-hydroxy-14-(trifluoromethyl)pentadecyl]ammonium iodide","94159-76-9","D",0]
["[bis(2-hydroxyethyl)][2-hydroxy-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-12-(trifluoromethyl)tridecan-1-yl]methylammonium iodide","94159-77-0","D",0]
["[(4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-2-hydroxy-10-(trifluoromethyl)undecyl]bis(2-hydroxyethyl)methylammonium iodide","94159-78-1","D",0]
["1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecan-2-ol","94159-81-6","D",0]
["1,2-andecanediol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-","94159-84-9","D",0]
["1-Aziridineethanol, alpha-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl)-","94159-85-0","D",0]
["2-andecanol, 1-(ethenyloxy)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-","94159-86-1","D",0]
["Glycine, N-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyandecyl)-N-methyl-, monopotassium salt (9CI)","94159-87-2","D",0]
["4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl)-2,2-dimethyl-1,3-dioxolane","94159-88-3","D",0]
["potassium N-[4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-2-hydroxy-10-(trifluoromethyl)undecyl]-N-methylaminoacetate","94159-89-4","D",0]
["4-[2,2,3,3,4,4,5,5,6,6,7,7,8,9,9,9-hexadecafluoro-8-(trifluoromethyl)nonyl]-2,2-dimethyl-1,3-dioxolane","94159-90-7","D",0]
["2-andecanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-1-phenoxy-","94159-91-8","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-1-phenoxy-10-(trifluoromethyl)undecan-2-ol","94159-92-9","D",0]
["Butanedioic acid, sulfo-, 1,4-bis(alpha-omega-perfluoro-C6-12-alkyl) esters, sodium salts","94166-88-8","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl dihydrogen phosphate","94200-42-7","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-nonacosafluoro-2-hydroxyheptadecyl dihydrogen phosphate","94200-43-8","D",0]
["3-(Perfluorohexadecyl)-2-hydroxypropyl dihydrogen phosphate","94200-44-9","D",0]
["butan-2-one O,O',O''-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silylidyne]oxime","94158-20-0","D",0]
["2-Oxepanone, homopolymer, decyl perfluoro-C8-14-alkyl esters, reactionproducts with 1H-imidazole-1-propanamine and TDI homopolymer","332076-33-2","D",0]
["2-Oxepanone, homopolymer, decyl perfluoro-C8-14-alkyl esters, reactionproducts with 1H-imidazole-1-propanamine, polyethylene glycol and TDIhomopolymer","332076-34-3","D",0]
["Betaines, (hydroxyethyl)methyl(gamma,omega-perfluoro-C8-14-beta-alkenyl)(2-sulfopropyl)","115340-82-4","D",0]
["Quaternary ammonium compounds, trimethyl(delta-omega-perfluoro-C8-14-beta-alkenyl), chlorides","115535-36-9","D",0]
["Benzenesulfonamide, 4-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)oxy]-","89932-76-3","D",0]
["Ethanethioic acid, S-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester","125640-21-3","D",0]
["8,10-Heptadecanedione,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-triacontafluoro-","36554-97-9","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)-, diethyl ester (9CI)","854095-13-9","D",0]
["2-Butenedioic acid, 1-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl) ester","152682-85-4","D",0]
["2,8,9-Trioxa-5-aza-1-silabicyclo[3.3.3]undecane, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-iododecyl)-","135587-17-6","D",0]
["Benzoic acid, 4-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)oxy]-","188034-84-6","D",0]
["2-Butenedioic acid (2Z)-, 1-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl) ester","229957-05-5","D",0]
["Benzenemethanol, 4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-alpha,alpha-diphenyl-","649561-66-0","D",0]
["Iodine, bis(acetato-betaO)[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]- (9CI)","882186-02-9","D",0]
["Phosphine, [4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]diphenyl-","462996-04-9","D",0]
["Phenol, 4-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","142623-70-9","D",0]
["2-Propenoic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl ester","15498-45-0","D",0]
["Decane, 10-(ethenylsulfonyl)-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","93345-48-3","D",0]
["Phosphinic acid, bis(heptadecafluorooctyl)-, sodium salt (9CI)","500776-69-2","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-, bis(1-methylethyl) ester (9CI)","90183-56-5","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(4-methylbenzenesulfonate)","113823-56-6","D",0]
["Phosphine, bis[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phenyl-","892154-91-5","D",0]
["2-Propenoic acid, 2-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)methylamino]ethyl ester","93491-54-4","D",0]
["Butanedioic acid, 2-methylen-, 1,4-bis(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl) ester","243977-25-5","D",0]
["2-Oxepanone, homopolymer, decyl perfluoro-C8-14-alkyl esters, reactionproducts with 1H-imidazole-1-propanamine, polyethylene-polypropyleneglycol and TDI homopolymer","332076-28-5","D",0]
["(dodecyl)trimethylammonium 2,2,3,3-tetrafluoropropionate","94158-60-8","D",0]
["2-andecanol, 1-[2-(2-butoxyethoxy)ethoxy]-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-","94158-61-9","D",0]
["1-[2-(2-butoxyethoxy)ethoxy]-4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)undecan-2-ol","94158-62-0","D",0]
["((Perfluorododecyl)methyl)oxirane","94158-66-4","D",0]
["((Perfluorotetradecyl)methyl)oxirane","94158-67-5","D",0]
["Benzene, 1-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)sulfonyl]-4-(hexyloxy)-","1161917-33-4","D",0]
["Benzene, 1-[chlorobis(4-methoxyphenyl)methyl]-4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","865758-36-7","D",0]
["Benzenemethanol, 4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-alpha,alpha-bis(4-methoxyphenyl)-","865758-47-0","D",0]
["Palladium, dichlorobis[tris[3-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phosphine-betaP]-","343343-17-9","D",0]
["2-Propenoic acid, 2-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)sulfonyl]methylamino]ethyl ester","48077-95-8","D",0]
["beta-D-Glucopyranosiduronic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl","864551-34-8","D",0]
["Carbonic acid, 2,5-dioxo-1-pyrrolidinyl [4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]methylester","556050-49-8","D",0]
["Thymidine, 5'-O-[[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]bis(4-methoxyphenyl)methyl]-, 3'-[2-cyanoethyl N,N-bis(1-methylethyl)phosphoramidite]","902456-09-1","D",0]
["Cytidine, N-benzoyl-2'-deoxy-5'-O-[[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]bis(4-methoxyphenyl)methyl]-, 3'-[2-cyanoethyl N,N-bis(1-methylethyl)phosphoramidite]","1401422-19-2","D",0]
["Guanosine, 2'-deoxy-5'-O-[[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl](4-methoxyphenyl)phenylmethyl]-N-(2-methyl-1-oxopropyl)-, 3'-[2-cyanoethyl N,N-bis(1-methylethyl)phosphoramidite]","1401422-22-7","D",0]
["Guanosine, 2'-deoxy-5'-O-[[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]bis(4-methoxyphenyl)methyl]-N-(2-methyl-1-oxopropyl)-, 3'-[2-cyanoethyl N,N-bis(1-methylethyl)phosphoramidite]","1401422-21-6","D",0]
["Octane, 1,1,1,2,3,3,4,4,5,5,6,6-dodecafluoro-8-iodo-2-(trifluoromethyl)-","18017-20-4","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,8,8,8-dodecafluoro-7-(trifluoromethyl)-","20015-46-7","D",0]
["2-Nonanol, 1-amino-4,4,5,5,6,6,7,7,8,9,9,9-dodecafluoro-8-(trifluoromethyl)-","58935-89-0","D",0]
["Oxirane, 2-[2,2,3,3,4,4,5,5,6,7,7,7-dodecafluoro-6-(trifluoromethyl)heptyl]-","24564-77-0","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,8,8,8-dodecafluoro-7-(trifluoromethyl)octyl ester","50836-66-3","D",0]
["2-Propenoic acid, 4,4,5,5,6,6,7,7,8,9,9,9-dodecafluoro-2-hydroxy-8-(trifluoromethyl)nonyl ester","16083-75-3","D",0]
["2-Propenoic acid, 2-methyl-, 4,4,5,5,6,6,7,7,8,9,9,9-dodecafluoro-2-hydroxy-8-(trifluoromethyl)nonyl ester","16083-81-1","D",0]
["Phenol, 4-bromo-2-[4,4,5,5,6,6,7,7,8,9,9,9-dodecafluoro-8-(trifluoromethyl)nonyl]-","610778-18-2","D",0]
["Bis((perfluoro-13-methyltetradecyl)ethyl) hydrogen phosphate","93776-29-5","D",0]
["Octanimidamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-hydroxy-","4314-38-9","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, 2-propen-1-ylester","20120-44-9","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, ethenyl ester","307-93-7","D",0]
["Pyridinium, 1-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)-, 1,1,1-trifluoromethanesulfonate (1:1)","25061-59-0","D",0]
["1-Decanaminium, N-(carboxymethyl)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluoro-N,N-dimethyl-, inner salt","171184-15-9","D",0]
["5-Tridecene, 7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-pentadecafluoro-","52717-05-2","D",0]
["lithium 2-(bis(4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluoro-2-hydroxynonyl)amino)ethane-1-sulfonate","1262880-17-0","D",0]
["(perfluorohexyl)hexadecane","133310-71-1","D",0]
["Methyl Perfluoroamyl Ketone","2708-07-8","D",0]
["6:2 fluorotelomer aldehyde","56734-81-7","D",0]
["6:2 fluorotelomer unsaturated aldehyde","69534-12-9","D",0]
["6:2 fluorotelomer unsaturated carboxylic acid","70887-88-6","D",0]
["2-Iodo-1-(perfluorohex-1-yl)octane","109574-84-7","D",0]
["Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-8-iodo-","10258-49-8","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","25291-12-7","D",0]
["Tridecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-","169331-74-2","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-","38787-57-4","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","25431-48-5","D",0]
["Pentadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","918-32-1","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","38787-66-5","D",0]
["Nonadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-","109856-51-1","D",0]
["Tricosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-","57325-44-7","D",0]
["2-Decene, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluoro-, (E)- (9CI)","89889-22-5","D",0]
["1-Nonanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-","755-02-2","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, butyl ester","307-96-0","D",0]
["Silsesquioxanes, 3-aminopropyl 3,3,4,4,5,5,6,6,6-nonafluorohexyl, hydroxy-terminated acetates","943344-69-2","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, ammonium salt","95144-12-0","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with chlorotrifluoroethene, 1,1-difluoroethene and tetrafluoroethene","95325-75-0","D",0]
["2-Methoxyperfluoro(2,5-di(propan-2-yl)oxolane)","957209-18-6","D",0]
["Methyl perfluoro-3-(3-methoxypropoxy)-3H-propanoate","958445-54-0","D",0]
["Sodium salts of perfluorononan-1-oic-acid","21049-39-8","D",0]
["6-Tetradecene, 8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentadecafluoro-","38787-60-9","D",0]
["Octanal, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","335-60-4","D",0]
["1,1-Octanediol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","31185-69-0","D",0]
["8-Heptadecene, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-","52717-06-3","D",0]
["2-Nonanone, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-","754-85-8","D",0]
["2-Nonanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-2-methyl-","92914-88-0","D",0]
["Decanoic acid, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluoro-","812-70-4","D",0]
["Octanoyl bromide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","222037-87-8","D",0]
["Octanimidamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","307-31-3","D",0]
["Nonanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluoro-","45291-33-6","D",0]
["Octanoic-1,2-13C2 acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","864071-08-9","D",0]
["Octanoic-1-13C acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (9CI)","864071-09-0","D",0]
["1-Octanaminium, N,N,N-trimethyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)","927835-01-6","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, potassium salt,hydrate (1:1:2)","98065-31-7","D",0]
["7-Hexadecene,1,1,1,2,2,3,3,4,4,5,5,6,6,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-triacontafluoro-, (E)- (9CI)","51249-68-4","D",0]
["Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-8-(2-propen-1-yloxy)-","812-72-6","D",0]
["Oxirane, 2-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)-","20084-49-5","D",0]
["1-Octanamine, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)-","3145-68-4","D",0]
["1-Decanol, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluoro-","25600-66-2","D",0]
["1,1,2,3,3,3-hexafluoro-2-(trifluoromethyl)propane-1-sulphonic anhydride","93894-52-1","D",0]
["[(2,2,3,4,4,4-hexafluorobutoxy)methyl]oxirane","93858-69-6","D",0]
["Bis((perfluoro-11-methyldodecyl)ethyl) hydrogen phosphate","93857-56-8","D",0]
["Bis((perfluoro-9-methyldecyl)ethyl) phosphate","93857-55-7","D",0]
["Bis((perfluorohexadecyl)ethyl) hydrogen phosphate","93857-54-6","D",0]
["trimethoxy[3-(1,1,2,2-tetrafluoroethoxy)propyl]silane","93804-21-8","D",0]
["1,1'-[oxybis[(isopropylene)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-icosafluoro-12-(trifluoromethyl)tridecan-2-ol","93776-04-6","D",0]
["1,1'-[oxybis(propyleneoxy)]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)undecan-2-ol]","93776-05-7","D",0]
["33,33,34,34,35,35,36,36,37,37,38,38,39,39,40,40,41,41,42,42,43,43,44,44,44-pentacosafluoro-2,5,8,11,14,17,20,23,26-decaoxatetratetracontan-31-ol","93776-06-8","D",0]
["2,5,8,11,14,17,20,23,26,29-Decaoxadotetracontan-31-ol,33,33,34,34,35,35,36,36,37,37,38,38,39,39,40,40,41,41,42,42,42-heneicosafluoro-","93776-07-9","D",0]
["2,5,8,11,14,17,20,23,26,29-Decaoxatetracontan-31-ol,33,33,34,34,35,35,36,36,37,37,38,38,39,39,40,40,40-heptadecafluoro-","93776-08-0","D",0]
["33,33,34,34,35,35,36,36,37,37,38,38,39,39,40,40,41,41,42,42,43,44,44,44-tetracosafluoro-43-(trifluoromethyl)-2,5,8,11,14,17,20,23,26,29-decaoxatetratetracontan-31-ol","93776-09-1","D",0]
["33,33,34,34,35,35,36,36,37,37,38,38,39,39,40,40,41,42,42,42-icosafluoro-41-(trifluoromethyl)-2,5,8,11,14,17,20,23,26,29-decaoxodotetracontan-31-ol","93776-10-4","D",0]
["33,33,34,34,35,35,36,36,37,37,38,38,39,40,40,40-hexadecafluoro-39-(trifluoromethyl)-2,5,8,11,14,17,20,23,26,29-decaoxatetracontan-31-ol","93776-11-5","D",0]
["1-Propanaminium, N-(2-carboxyethyl)-3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyandecyl)amino]-N,N-dimethyl-, inner salt","93776-14-8","D",0]
["Bis(2-hydroxyethyl)methyl(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-pentacosafluoro-2-hydroxypentadecyl)ammonium iodide","93776-16-0","D",0]
["bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl] hydrogen phosphate","93776-19-3","D",0]
["Ammonium bis(2-(perfluorododecyl)ethyl) phosphate","93776-22-8","D",0]
["ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-tritriacontafluorooctadecyl] phosphate","93776-23-9","D",0]
["ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,10,10,10-hexadecafluoro9-(trifluoromethyl)decyl] phosphate","93776-24-0","D",0]
["ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-icosafluoro-11-(trifluoromethyl)dodecyl] phosphate","93776-25-1","D",0]
["ammonium bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl) phosphate","93776-26-2","D",0]
["ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl] phosphate","93776-27-3","D",0]
["ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl] phosphate","93776-28-4","D",0]
["1,1,2,2,3,3,4,4-octafluoro-N-(2-hydroxyethyl)-N-methylbutane-1-sulphonamide","93894-53-2","D",0]
["Nonadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","25431-52-1","D",0]
["1,1-Dihydroperfluoroctylamine","307-29-9","D",0]
["Tricosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","57325-43-6","D",0]
["1-Octanamine, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, hydrochloride(1:1)","5678-75-1","D",0]
["Pentacosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodo-","2837-34-5","D",0]
["1-Pentene, 2,3,3,4,4,5,5-heptafluoro-, polymer with ethene and 1,1,2,2-tetrafluoroethene","94228-79-2","D",0]
["Ethenyl benzoate polymer with 2-butenoic acid, ethenyl 2,2-dimethylpropanoate, 4-(ethenyloxy)-1-butanol, 2-methyl-1-propene and 1,1,2,2-tetrafluoroethene, dihydrogen 1,2,4-benzenetricarboxylate, compd. with N,N-diethylethanamine","938155-33-0","D",0]
["N,N-bis(2-hydroxyethyl)-4-[[4,4,5,5,5-pentafluoro-3-(pentafluoroethyl)-1,2,3-tris(trifluoromethyl)pent-1-enyl]oxy]benzenesulphonamide","93819-97-7","D",0]
["(Perfluoro-13-methyltetradecyl)ethyl dihydrogen phosphate","93857-42-2","D",0]
["diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,18,18,18-dotriacontafluoro-17-(trifluoromethyl)octadecyl phosphate","93857-43-3","D",0]
["12:2 Fluorotelomer dihydrogen phosphate (ester), diammonium salt","93857-46-6","D",0]
["14:2 Fluorotelomer dihydrogen phosphate diammonium salt","93857-47-7","D",0]
["16:2 Fluorotelomer phosphate","93857-48-8","D",0]
["Diammonium (perfluoro-7-methyloctyl)ethyl phosphate","93857-49-9","D",0]
["Diammonium (perfluoro-9-methyldecyl)ethyl phosphate","93857-50-2","D",0]
["diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-tetracosafluoro-13-(trifluoromethyl)tetradecyl phosphate","93857-51-3","D",0]
["diammonium 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,16,16,16-octacosafluoro-15-(trifluoromethyl)hexadecyl phosphate","93857-52-4","D",0]
["Bis((perfluorotetradecyl)ethyl) hydrogen phosphate","93857-53-5","D",0]
["heptadecafluoroisooctanesulphonamide","93894-56-5","D",0]
["1,1,2,2,3,3,4,4-octafluorobutane-1-sulphonic anhydride","93894-55-4","D",0]
["1,1,2,2,3,3,4,4-octafluoro-N,N-bis(2-hydroxyethyl)butane-1-sulphonamide","93894-54-3","D",0]
["heptadecafluoroisooctanesulphonamide, compound with triethylamine(1:1)","93894-57-6","D",0]
["Isooctanesulfonamide, heptadecafluoro-N-(2-hydroxyethyl)-N-methyl-","93894-65-6","D",0]
["Isooctanesulfonamide, heptadecafluoro-N,N-bis(2-hydroxyethyl)-","93894-66-7","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","96497-21-1","D",0]
["Dodecane, 12-azido-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-","145876-00-2","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(hydrogen sulfate), potassium salt (1:1)","1262446-13-8","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-acetate","37858-04-1","D",0]
["Phosphonic acid, P-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-, diethyl ester","90146-96-6","D",0]
["Silanetriamine, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-N,N,N',N',N'',N''-hexamethyl-","186599-45-1","D",0]
["Hexacosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","176979-19-4","D",0]
["Hexacosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-12-iodo-","1257261-91-8","D",0]
["Octacosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","1257261-95-2","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)bis(1-methylethyl)-","356056-15-0","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-2-methyl-","136022-91-8","D",0]
["Silane, trichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)-","102488-49-3","D",0]
["1-Decene, 1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-iodo-,(Z)- (9CI)","56184-40-8","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)bis(1-methylethyl)-","356056-16-1","D",0]
["Docosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,15,15,16,16,17,17,18,18,19,19,20,20,21,21,22,22,22-tetratriacontafluoro-10,13-diiodo-","460744-98-3","D",0]
["Eicosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,14,14,15,15,16,16,17,17,18,18,19,19,20,20,20-triacontafluoro-9,12-diiodo-","25474-72-0","D",0]
["5-Tetradecene,1,1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-hexacosafluoro-, (E)- (9CI)","51249-69-5","D",0]
["Tetracosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,17,17,18,18,19,19,20,20,21,21,22,22,23,23,24,24,24-tetratriacontafluoro-10,15-diiodo-","959462-52-3","D",0]
["Heneicosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,14,14,15,15,16,16,17,17,18,18,19,19,20,20,21,21,21-tetratriacontafluoro-10,12-diiodo-","1254971-75-9","D",0]
["Silanamine, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-N,N,1,1-tetramethyl-","1221157-06-7","D",0]
["6-Tetradecene, 1,1,1,2,2,3,3,4,4,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-","53638-14-5","D",0]
["1,4-Butanediol, 2-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-","135440-42-5","D",0]
["8-Hexadecene,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-triacontafluoro-, (E)- (9CI)","35709-15-0","D",0]
["Heptacosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,18,18,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,27,27,27-dotetracontafluoro-12,16-diiodo-","784189-62-4","D",0]
["Benzenemethanamine, 4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","609816-23-1","D",0]
["Octanamide, N,N'-trimethylenbis[2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (8CI)","29680-98-6","D",0]
["1,3,5,2-Triazaphosphorine, 2,2-diazido-2,2-dihydro-4,6-bis(pentadecafluoroheptyl)- (9CI)","95215-99-9","D",0]
["Phosphinous amide, N-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)-P,P-bis(pentafluorophenyl)- (9CI)","518358-34-4","D",0]
["[1,1'-Biphenyl]-4-carboxylic acid, 4'-(2-methylbutyl)-,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, (S)- (9CI)","118826-52-1","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-(4-methoxyphenyl)-","103188-04-1","D",0]
["Tetracosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","1257261-94-1","D",0]
["Decanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-2-methyl-","136022-86-1","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)tripropoxy-","521084-64-0","D",0]
["Phosphonic acid, P-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","80220-63-9","D",0]
["1-Propanol, 3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","36880-07-6","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-, sodium salt (9CI)","92678-93-8","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-, compd. with N,N-diethylethanamine (1:1) (9CI)","92678-96-1","D",0]
["2-Dodecenal, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-eicosafluoro-,(2Z)-","1383918-01-1","D",0]
["Disiloxane, 1,3-bis(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-1,1,3,3-tetramethyl-","129498-18-6","D",0]
["Phosphonic acid, P-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)-","252237-39-1","D",0]
["3-Undecen-2-one, 4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-hexadecafluoro-, (Z)-(9CI)","136909-85-8","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-, dimethyl ester (9CI)","61726-43-0","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-isocyanato-","142010-50-2","D",0]
["Benzene, 1-bromo-4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","195324-88-0","D",0]
["Oxirane, 2-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-","52835-16-2","D",0]
["Decane, 10,10-diethoxy-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","133377-48-7","D",0]
["Benzene, 1-bromo-3-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","340157-97-3","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)-, dimethyl ester (9CI)","61726-45-2","D",0]
["Benzenemethanol, 4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","356055-77-1","D",0]
["Octacosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,27,27,28,28,28-dotetracontafluoro-12,17-diiodo-","1980064-30-9","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-octadecafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl]-.omega.-hydroxy-","104075-36-7","D",0]
["3,5-Dichloro-4-(1,1,2,2-tetrafluoroethoxy)aniline","104147-32-2","D",0]
["2-Propenoic acid, 2-[[(heptadecafluorooctyl)sulfonyl]propylamino]ethylester, copolymer with methyloxirane and oxiranemono-2-propenoate","104242-02-6","D",0]
["Carbamic acid, [3-[[[2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethoxy]carbonyl]amino]-4-methylphenyl]-, 2-[[(heptadecafluorooctyl)sulfonyl]propylamino]ethyl ester","104267-74-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-Nonacosafluorohexadec-1-ene","104564-28-5","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], .alpha.-hydro-.omega.-hydroxy-, ether with 2,2-bis(hydroxymethyl)-1,3-propanediol (4:1), polymer with 1,3-diisocyanatomethylbenzene, polyethylene glycol mono-Me ether- and 3,3,4,4,5,5,6,6,7,7,8,8,8-trid¿","1304012-00-7","D",0]
["1H-Tridecafluoro-3,3-dimethylhex-1-yne","261503-44-0","D",0]
["Triethoxy[5,5,6,6,7,7,7-heptafluoro-4,4bis(trifluoromethyl)heptyl]silane","130676-81-2","D",0]
["(Perfluorohexyl)trifluorooxirane","87375-53-9","D",0]
["Perfluorohexanoyl chloride","335-53-5","D",0]
["3,3,4,4,5,5,6,6,7,7,7-Undecafluoroheptan-2-ol","914637-05-1","D",0]
["Perfluorohexanoic Anhydride","308-13-4","D",0]
["Siloxanes and Silicones, di-Me, Bu group- and hydrogen-terminated, reaction products with 3-(ethenyldimethylsilyl)-N-methylbenzenamine and 2,2¿-[(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis(oxy)]bis[2,3,3,3-tetrafluoropropanoyl fluoride]-2,2,3-¿","1202381-96-1","D",0]
["Oxetane, 2,2,3,3-tetrafluoro-, homopolymer, fluorinated, reduced, bis(2,3-dihydroxypropyl) ethers.","1188330-60-0","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], .alpha.-hydro-.omega.-hydroxy-, polymer with 1,3-diisocyanatomethylbenzene, polyethylene glycol mono-Me ether- and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-octanol-blocked.","1304011-35-5","D",0]
["Sulfonium, (4-methylphenyl)diphenyl-, salt with 4,4,5,5,6,6-hexafluorodihydro-4H-1,3,2-dithiazine 1,1,3,3-tetraoxide (1:1).","862261-51-6","D",0]
["Borate(1-), tetrahydro-, sodium (1:1), reaction products with reduced polymd. oxidized tetrafluoroethylene, hydrolyzed, diallyl ethers, polymers with 3-[(dimethylsilyl)oxy]-1,1,3,5,5-pentamethyl-1-[2 -(trimethoxysilyl)ethyl]trisiloxane.","1072943-15-7","D",0]
["Sulfonium, triphenyl-, salt with 4,4,5,5,6,6-hexafluorodihydro-4H-1,3,2-dithiazine 1,1,3,3-tetraoxide (1:1).","808752-25-2","D",0]
["1-Octanesulfonyl fluoride, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-","307-35-7","D",0]
["Perfluorooctane sulfonic acid","1763-23-1","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl N,N-dibutyl-beta-alaninate","108196-44-7","D",0]
["Trimethyl(tridecafluorohexyl)silane","135841-49-5","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)phosphonic acid monoethyl ester","1189052-97-8","D",0]
["1-(Perfluorohexyl)docosane","825651-73-8","D",0]
["Reaction products with N-methylamine acetate, potassium hydroxide, .alpha.-fluoro-.omega.-iodopoly(perfluoroethylene)(n=4-8) and 2-propen-1-ol  (Unidyne DS 102)","104075-34-5","D",0]
["Hexacosane,1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,17,17,18,18,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,26-dotetracontafluoro-12,15-diiodo-","1980086-18-7","D",0]
["Silanediamine, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-N,N,N',N',1-pentamethyl-","186599-47-3","D",0]
["Phosphinic acid, P-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-","731858-13-2","D",0]
["2-Decenal, 3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluoro-, (2Z)-","142502-68-9","D",0]
["Phosphinic acid, P-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)-","731858-15-4","D",0]
["3-Methyl-3-[[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)oxy]methyl]-oxetane","475678-78-5","D",0]
["Propanyl fluoride, 2,2'-[(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis(oxy)bis[2,3,3,3-tetrafluoro-, polymer with trifluoro(trifluoromethyl)oxirane, hydrolyzed.","183905-82-0","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha., .alpha¿.-(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis[.omega.-(1,2,2,2-tetrafluoro-1-[(2-propenylamino)carbonyl]ethoxy]-.","162442-49-1","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha., .alpha¿.-(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis[.omega.-(1-carboxy-1,2,2,2-tetrafluoroethoxy)-.","132910-12-4","D",0]
["Propanyl fluoride, 2,2'-[(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis(oxy)bis[2,3,3,3-tetrafluoro-, polymer with trifluoro(trifluoromethyl)oxirane, reaction products with 2-propen-1-amine.","183905-83-1","D",0]
["Silanol, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)dimethyl-.","128194-56-9","D",0]
["Propanol fluoride, 2,2¿-[(1,1,2,2-tetrafluoro-1,2-ethanediyl)bis(oxy)]bis[2,3,3,3-tetrafluoro-, polymer with 2,2,3-trifluoro-3-(trifluoromethyl)oxirane, reaction products with 3-(ethenyldimethylsilyl)-N-methylbenzenamine and methylbis[(1-¿","917979-29-4","D",0]
["Siloxanes and silicones, Me hydrogen, [[dimethyl[3,3,4,4-tetrafluoro-4-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]butyl]silyl]oxy]-terminated.","166089-96-9","D",0]
["Silane, trichloro(12,12,13,13,14,14,15,15,15-nonafluoropentadecyl)-.","2301857-79-2","D",0]
["1-Pentadecene, 12,12,13,13,14,14,15,15,15-nonafluoro-.","631842-87-0","D",0]
["Siloxanes and Silicones, di-Me, 3,3,4,4,5,5,6,6-nonafluorohexyl group terminated.","2374700-01-1","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[tetrafluoro(trifluoromethyl)ethyl]-.omega.-[1,2,2,2-tetrafluoro-1-[[3-(trimethoxysilyl)propoxy]methyl]ethoxy]-.","211931-77-0","D",0]
["Siloxanes and silicones, di-Me, 3-hydroxypropyl Me, Me hydrogen, ethers with trifluoro(trifluoromethyl)oxirane homopolymer 1,2,2,2-tetrafluoro-1-(hydroxymethyl)ethyl tetrafluoro(trifluoromethyl)ethyl ether.","174393-73-8","D",0]
["Boron, trifluoro(tetrahydrofuran)-, (T-4)-, polymer with 3-methyl-3-((2,2,3,3,3-pentafluoropropoxy)methyl)oxetane, ether with 2,2-dimethyl-1,3-propanediol (2:1), polymer with alpha-hydro-omega-hydroxypoly(oxy-1,2-ethanediyl) and ¿","1029089-63-1","D",0]
["Lufenuron","103055-07-8","D",0]
["Perfluoro-2,9-dimethyldecane","103188-55-2","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], alpha-[1,2,2,2-tetrafluoro-1-[[(2-hydroxyethyl)amino]carbonyl]ethyl]-omega-[tetrafluoro(trifluoromethyl)ethoxy]-, ether with alpha-hydro-omega-hydroxypoly(oxy-1,2-ethanediyl) (2:1)","1033385-42-0","D",0]
["2-(Perfluorotetradecyl)ethanethiol","103119-64-8","D",0]
["N-[3-(Dimethylamino)propyl]perfluoroheptanamide","103831-28-3","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-[2-(2-hydroxyethoxy)ethyl]-","110388-02-8","D",0]
["1,3-Propanediol, 2,2-bis[[(gamma-omega-perfluoro-C10-20-alkyl)thio]methyl] derivs.,phosphats","148240-88-4","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, polymers with 1,6-diisocyanatohexane,ethylene glycol, glycidol and 2,4-TDI","253873-70-0","D",0]
["Thiocyanic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester","26650-10-2","D",0]
["Phosphinic acid, bis(heneicosafluorodecyl)- (9CI)","52299-27-1","D",0]
["1,3-Isobenzofurundione, polymer with alpha-fluoro-omega-(oxiranylmethyl)poly(difluoromethylen) und (phenoxymethyl)oxirane (9CI)","107097-76-7","D",0]
["2-Propenoic acid, 2-methyl-, C7-8-alkyl esters, polymers with 2-[methyl[(gamma-omega-perfluoro-C8-14-alkyl)sulfonyl]amino]ethyl acrylate","68988-54-5","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-¿","142636-90-6","D",0]
["2-Propenoic acid, 2-methyl-, phenylmethyl ester, polymer with 1,1-dichloroethene, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl 2-propenoate¿","142636-91-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers with gamma-omega-perfluoro-C10-16-alkyl acrylate and vinyl acetate","186397-57-9","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate,peroxidized adipoyl chloride-triethylene glycol polymer-initiated","193635-71-1","D",0]
["2-Propenoic acid, 2-methyl-, gamma-omega-perfluoro-C6-16-alkyl esters, polymerswith 1-(3,4-dichlorophenyl)-1H-pyrrole-2,5-dione and sodium 4-ethenylbenzenesulfonate (1:1)","202875-75-0","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, polymers with alpha-fluoro-omega-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylen), methanol, stearylacrylate, stearyl methacrylate, 2,4-TDI and vinyl chloride","376364-33-9","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) esters, polymers with N-(hydroxymethyl)-2-propenamide, gamma-omega-perfluoro-C8-18-alkyl acrylate andvinyl chloride","502135-45-7","D",0]
["2-Propenoic acid, 2-methyl-, oxiranylmethyl ester, polymers with .gamma.-.omega.-perfluoro-C6-16-alkyl acrylate and stearyl acrylate","503284-73-9","D",0]
["2-Propenoic acid, gamma-omega-perfluoro-C6-16-alkyl esters, polymers withacrylonitrile, N-(butoxymethyl)-2-propenamide, polyethylene glycoldimethacrylate and polyethylene glycol methacrylate Me ether","503287-56-7","D",0]
["2-Butenedioic acid, 2-methyl-, (2Z)-, polymers with gamma-omega-perfluoro-C8-16-alkyl acrylate, stearyl acrylate and styrene","503296-97-7","D",0]
["2-Propenoic acid, 2-methyl-, 1,4-butanediyl ester, polymers with C14-24-alkyl methacrylate, cyclohexyl methacrylate, 2-hydroxyethyl acrylate, gamma-omega-perfluoro-C6-16-alkyl acrylate and 2-[[[[[1,3,3-trimethyl-5¿","503299-29-4","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[[[[1,3,3-trimethyl-5-[[[[(1-methylpropylidene)amino]oxy]carbonyl]amino]cyclohexyl]methyl]amino]carbonyl]oxy]ethyl ester, polymers with 2-ethylhexyl acrylate, 2-hydroxyethylacrylate and¿","503299-50-1","D",0]
["Alkyl iodides, C8-20, gamma-omega-perfluoro, reaction products with potassiumacrylate","509086-57-1","D",0]
["2-Propenoic acid, 2-methyl-, cyclohexyl ester, polymers with maleicanhydride, gamma-omega-perfluoro-C6-16-alkyl acrylate and 2,4,6-tris(2-propenyloxy)-1,3,5-triazine","510732-38-4","D",0]
["2-Propenoic acid, 2-methyl-, octadecyl ester, polymers with gamma-omega-perfluoro-C8-14-alkyl acrylate","510732-48-6","D",0]
["2-Propenoic acid, 2-methyl-, polymers with ethylene dimethacrylate,ethylene oxide, nonadecyl acrylate, gamma-omega-perfluoro-C6-16-alkyl acrylate andpropylene oxide","510733-10-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, telomers with Et acrylate,1-octanethiol and gamma-omega-perfluoro-C6-16-alkyl acrylate","510734-75-5","D",0]
["2-Propenoic acid, gamma-omega-perfluoro-C8-16-alkyl esters, polymers with ethyleneand N-(hydroxymethyl)-2-propenamide","511271-18-4","D",0]
["1,3-Propanediol, 2,2-bis[[(gamma-omega-perfluoro-C6-12-alkyl)thio]methyl] derivs.,phosphats","148240-86-2","D",0]
["Phosphine, tris[3-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]-","342889-38-7","D",0]
["Benzene, 1-[chloro[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl]phenylmethyl]-4-methoxy-","865758-37-8","D",0]
["3-Pyridinecarboxylic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","331716-84-8","D",0]
["2-Butenedioic acid (2Z)-, 1,4-bis(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl) ester","234096-30-1","D",0]
["2-Butenedioic acid (2E)-, 1,4-bis(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl) ester","934166-50-4","D",0]
["Fatty acids, C9-15-unsatd., gamma-omega-perfluoro, Et esters, reaction products with(3-hydroxypropoxy)-terminated di-Me siloxanes, Me Et ketone oxime,polymethylenpolyphenylene isocyanate and polypropylene","510732-30-6","D",0]
["2-Propenoic acid, 2-methyl-, C7-18-alkyl esters, polymers with 2-[methyl[(gamma-omega-perfluoro-C8-14-alkyl)sulfonyl]amino]ethyl acrylate","68988-55-6","D",0]
["Siloxanes and Silicones, hydroxy Me, Me octyl, Me (gamma-omega-perfluoro C8-14-alkyl)oxy, ethers with polyethylene glycol mono-Me ether","170424-64-3","D",0]
["Amines, C12-14-tert-alkyl, compds. with gamma-omega-perfluoro-C6-12-alkyldihydrogen phosphat (1:1)","206009-80-5","D",0]
["Amines, C12-14-tert-alkyl, compds. with bis(gamma-omega-perfluoro-C6-12-alkyl)hydrogen phosphat (1:1)","206009-81-6","D",0]
["1,4-Butanediol, 2,3-bis[(gamma-omega-perfluoro-C6-20-alkyl)thio] derivs., polymerswith 1,6-diisocyanatotrimethylhexane and 2,2'-(methylimino)bis[ethanol]","68037-23-0","D",0]
["Sulfonic acids, C8-20-alkane, gamma-omega-perfluoro, compds. with triethylamine","297175-71-4","D",0]
["1-Propanol, 2,3-bis[(gamma-omega-perfluoro-C6-20-alkyl)thio] derivs.","70983-61-8","D",0]
["1,4-Butanediol, polymers with 2,3-bis[(gamma-omega-perfluoro-C6-20-alkyl)thio]-1,4-butanediol, C36-alkylene diisocyanate and 1,6-diisocyanato-2,2,4(or 2,4,4)-trimethylhexane","71205-28-2","D",0]
["Acetic acid, bis[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs.","71608-37-2","D",0]
["Acetic acid, bis[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs., Me esters","71608-39-4","D",0]
["Acetic acid, bis[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs., sodium salts","71608-40-7","D",0]
["Bicyclo[2.2.1]heptane-2,3-dicarboxylic acid, 5-[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs.","71608-43-0","D",0]
["Chromium, bis[(gamma-omega-perfluoro-C8-20-alkyl)thio]acetate chloro hydroxycomplexes","71608-44-1","D",0]
["Chromium, 4,4-bis[(gamma-omega-perfluoro-C8-20-alkyl)thio]pentanoate chlorohydroxy complexes","71608-45-2","D",0]
["Chromium, chloro hydroxy 5-[(gamma-omega-perfluoro-C8-20-alkyl)thio]bicyclo[2.2.1]heptane-2,3-dicarboxylate complexes","71608-46-3","D",0]
["4,7-Methanoisobenzofuran-1,3-dione, hexahydro-, 5-[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs.","71608-58-7","D",0]
["Propanamide, N-(1,1-dimethyl-3-oxobutyl)-, 3-[(gamma-omega-perfluoro-C6-20-alkyl)thio] derivs.","71608-63-4","D",0]
["Thiols, C4-20, gamma-omega-perfluoro, reaction products with methylatedformaldehyde-1,3,5-triazine-2,4,6-triamine polymer","113089-67-1","D",0]
["2-Propenoic acid, 2-methyl-, cyclohexyl ester, polymers with glycidylmethacrylate and gamma-omega-perfluoro-C6-16-alkyl acrylate","511271-19-5","D",0]
["1-Decene, 2-bromo-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","51249-65-1","D",0]
["Eicosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","1257261-93-0","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,13,13,14,14,14-hexacosafluoro-9-iodo-","53638-13-4","D",0]
["1-Decene, 2-chloro-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","110927-73-6","D",0]
["Docosane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","176979-18-3","D",0]
["Octanamide, N,N'-(1R,2R)-1,2-cyclohexanediylbis[2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro- (9CI)","864149-62-2","D",0]
["Hexadecanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester","111918-97-9","D",0]
["Methanesulfonic acid, 1,1,1-trifluoro-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester","17352-09-9","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-hydroxy-","15435-88-8","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester","886046-97-5","D",0]
["Benzeneethanamine, N-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctylidene)-","29723-33-9","D",0]
["2-Propenamide, N-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)-","424-01-1","D",0]
["Octanamide, N-butyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","37696-83-6","D",0]
["Benzoic acid, 4-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]-","129560-87-8","D",0]
["Octanamide, N-dodecyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","37696-86-9","D",0]
["Benzoic acid, 4-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)amino]-","73782-58-8","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-(2-hydroxypropyl)-","1407514-44-6","D",0]
["Benzoic acid, 4-hydroxy-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctylester","869308-35-0","D",0]
["1-Octanol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, 1-(4-methylbenzenesulfonate)","24962-65-0","D",0]
["Octanamide, N-[4-(dimethylamino)butyl]-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","118454-01-6","D",0]
["2-Butenedioic acid (2E)-, bis(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl) ester (9CI)","24120-18-1","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, (4-ethenylphenyl)methyl ester","230295-06-4","D",0]
["Octanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-N-[3-(triethoxysilyl)propyl]-","37043-12-2","D",0]
["1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexahydro-2,2,4,4,6,6-hexakis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]- (9CI)","186043-52-7","D",0]
["Octadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","176979-17-2","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymers with 2-[2-[2-(2-hydroxyethoxy)ethoxy]ethoxy]ethyl methacrylate, 14-hydroxy-3,6,9,12-tetraoxahexadec-1-yl methacrylate and gamma-omega-perfluoro-C6-16-alkyl acrylate","512179-48-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymers with gamma-omega-perfluoro-C8-16-alkyl acrylate and polyethylene glycol monoacrylate","515152-55-3","D",0]
["Alcohols, C8-14, gamma-omega-perfluoro, reaction products with epichlorohydrin andpropylene oxide, trimethylamine-quaternized","185630-70-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-[methyl[(gamma-omega-perfluoro-C8-14-alkyl)sulfonyl]amino]ethyl esters, reaction products with polyethylene glycolbis(2-mercaptoacetate)","68784-73-6","D",0]
["2-Propenoic acid, 2-methyl-, C4-8-alkyl esters, polymers with 2-[methyl[(gamma-omega-perfluoro-C8-14-alkyl)sulfonyl]amino]ethyl acrylate","68988-52-3","D",0]
["1-Dodecanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-, 1-(hydrogen sulfate), potassium salt (1:1)","1262446-14-9","D",0]
["Octanamide, N,N'-1,2-cyclohexanediylbis[2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-","305848-92-4","D",0]
["1,2-Benzenedicarboxylic acid, 3,4,5,6-tetrachloro-, 1,2-bis(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl) ester","2212-77-3","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluorononyl ester","1799-55-9","D",0]
["1-Propanaminium, N,N,N-tripropyl-, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanoate (1:1)","277749-00-5","D",0]
["2-Propenoic acid, 2-methyl-, 1,1,2,2,3,3,3-heptafluoropropyl ester, polymer with methyl 2-methyl-2-propenoate, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluorononyl 2-methyl-2-propenoate und 1,1,2,2,2-pentafluoroethyl2-methyl-2-propenoate","1017277-36-9","D",0]
["Decane, 10-bromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","21652-57-3","D",0]
["andecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","38550-35-5","D",0]
["Nonane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,9,9,9-octadecafluoro-8-iodo-","922524-04-7","D",0]
["1-Decyne, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-","55009-88-6","D",0]
["Dodecane, 12-bromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-","332136-76-2","D",0]
["Decane, 9,10-dibromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","51249-63-9","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","99325-00-5","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","92835-74-0","D",0]
["Hexadecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-10-iodo-","96791-81-0","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,12-docosafluoro-9-iodo-","641617-25-6","D",0]
["Tetradecane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,13,13,14,14,14-hexacosafluoro-","53638-09-8","D",0]
["Decane, 9,9,10-tribromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","59665-26-8","D",0]
["Dodecane, 11,12-dibromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-heneicosafluoro-","214358-54-0","D",0]
["5-(Pentafluorosulfanyl)perfluoropentyl sulfonic acid","2089109-32-8","D",0]
["HG’-03","485399-48-2","D",0]
["1-Propenylperfluoropropane","355-95-3","D",0]
["1,1,1,2,2,3,3,4,4,11,11,12,12,13,13,14,14,14-Octadecafluorotetradecane","1835252-03-3","D",0]
["3-Butyl-1-methyl-1H-imidazolium N,N-bis(perfluorobutanesulfonyl)amide","872345-66-9","D",0]
["1H-Benzimidazole, 5,6-dimethyl-2-(pentafluoroethyl)-","500799-98-4","D",0]
["4-Heptanone, 2,6-bis(trifluoromethyl)-2,6-dihydroxy-1,1,1,7,7,7-hexafluoro-, bis(triethylamine)salt","101913-86-4","D",0]
["1,1,3,5,5-Pentamethyl-1,5-bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)trisiloxane","521069-00-1","D",0]
["2-(Heptafluoropropyl)-4-methyl-5,7-dinitro-1H-benzimidazole","60167-95-5","D",0]
["1,2,4,5,5,6,6,7,7-Nonafluorocyclohepta-1,3-diene","89537-38-2","D",0]
["Perfluoroethanesulfonamide","78491-70-0","D",0]
["4,4,4-trifluoro-3-hydroxy-3-(trifluoromethyl)-1-[3-(trifluoromethyl)phenyl]butan-1-one","34844-16-1","D",0]
["4,4,4-trifluoro-1-(4-methoxyphenyl)-2-propyl-3-(trifluoromethyl)butane-1,3-diol","34848-36-7","D",0]
["1,1,3,3,4,4,4a,5,5,6,6,7,7,8,8,8a-Hexadecafluoro-2-(trifluoromethyl)decahydroisoquinoline","86714-34-3","D",0]
["[(1,2,2,2-Tetrafluoroethyl)sulfanyl]benzene","130612-76-9","D",0]
["1-(2H-Perfluoropropyl)ethanol","2711-81-1","D",0]
["3-(2,2,3,3,4,4,4-Heptafluorobutoxy)propanenitrile","1365808-34-9","D",0]
["Potassium trifluoro(pentafluoroethyl)borate(1-)","476639-90-4","D",0]
["Methyl 5H-perfluoropentanoate","54822-22-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,19,19,20,20,21,21,22,22,23,23,23-Docosafluorotricosane","1980076-48-9","D",0]
["2-(Perfluoro-7-methyloctyl)ethanol","31200-98-3","D",0]
["1,1,1-Trichloro-2,2,3,3,4,5,5,5-octafluoro-4-(trifluoromethyl)pentane","88639-55-8","D",0]
["Phenyl nonafluorobutane-1-sulfonate","25628-11-9","D",0]
["Ethyl [(2,2,3,3,4,4,4-heptafluorobutanimidoyl)oxy]acetate","4314-33-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-Heptacosafluorodocosane","1309378-06-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iododocosane","129838-43-3","D",0]
["2-bromo-3,4,4,5,5,5-hexafluoro-3-(trifluoromethyl)pent-1-ene","234096-31-2","D",0]
["Benzoic acid--2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptan-1-ol (1/1)","87926-00-9","D",0]
["Bis((perfluoroheptyl)methyl) phosphate ammonium","1555-33-5","D",0]
["3,3,4,4,5,5-hexafluoroheptane-2,6-diol","3726-32-7","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[[(perfluoroheptyl)sulfonyl]amino]-1-propanaminium","2089109-10-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-iodooctan-2-ol","89807-99-8","D",0]
["1,2,3,3,3-Pentafluoroprop-1-ene-1-sulfonyl fluoride","685-22-3","D",0]
["4-(2,2,3,3-Tetrafluoropropoxy)phenol","111915-33-4","D",0]
["N,N-Bis(trifluoromethyl)-2-bromotetrafluoroethylamine","2261-32-7","D",0]
["Perfluoro-p-methylcyclohexylsulfonic acid","742-73-4","D",0]
["3-Methylbutyl (1-(diphenylphosphinyl)-2,2,2-trifluoro-1-(trifluoromethyl)ethyl)carbamate","145430-08-6","D",0]
["3-(6,6,7,7,8,8,9,9,10,10,11,11,11-Tridecafluoroundecyl)benzene-1,2-diol","131545-70-5","D",0]
["N-Ethyl-N-[3-(trimethoxysilyl)propyl]perfluoro-1-butanesulfonamide","154380-33-3","D",0]
["1,1,1,2,2-Pentafluoro-2-[1,1,2,2-tetrafluoro-2-(pentafluoroethoxy)ethoxy]ethane","356-70-7","D",0]
["Perfluorobutyl formate","197218-56-7","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, sodium salt (1:2)","245331-02-6","D",0]
["Heptyl 2,3,3,4,4,5,5,6,6,7,7,8,8,8-tetradecafluorooctanoate","118663-63-1","D",0]
["Ethyl 3-(2-ethoxy-2-oxoethyl)-5-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl)-2-oxooxolane-3-carboxylate","674786-75-5","D",0]
["2,2,4,4,5,5-Hexafluoro-1,3-dioxolane","21297-65-4","D",0]
["1,3-Bis(tridecafluorohexyl)benzene","124389-29-3","D",0]
["2-(1,1,1,3,3,3-hexafluoropropan-2-ylidene)-1-phenyldecan-1-one","35444-13-4","D",0]
["(7E)-1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorohexadec-7-ene","152128-75-1","D",0]
["5,5,6,6,7,7,7-Heptafluoro-4,4-bis(trifluoromethyl)hept-1-ene","72487-68-4","D",0]
["3-[3,3,3-Trifluoro-2-hydroxy-2-(trifluoromethyl)propyl]bicyclo[2.2.1]heptan-2-yl 2-methylprop-2-enoate","824411-04-3","D",0]
["Lonaprisan","211254-73-8","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(4-(methylamino)phenyl)propan-2-ol","1481-11-4","D",0]
["1,1,2,2,3,3,4,4,5,5,6,7,8,9,9,9-Hexadecafluoro-7-nonene-1-sulfonic acid","2089109-53-3","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-(1-carboxy-1,2,2,2-tetrafluoroethyl)-.omega.-(1,1,2,2,3,3,3-heptafluoropropoxy)-","90317-74-1","D",0]
["2,2,3,3,3-pentafluoro-1,1-diphenylpropan-1-ol","337-33-7","D",0]
["5,5,6,6,7,7,8,8,8-Nonafluoro-3-iodo-2-methyloct-3-en-2-ol","144295-00-1","D",0]
["Sodium-2-(Perfluorohexyl)ethanethiolate","1248568-70-8","D",0]
["(E)-1-(4-Methoxyphenyl)-N-[4-(nonafluorobutyl)phenyl]methanimine","73603-85-7","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl 2-fluoroprop-2-enoate","119986-76-4","D",0]
["2-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-5-methylcyclohexan-1-ol","52450-55-2","D",0]
["(4S,5R)-4-(Propan-2-yl)-5-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-1,3-oxazolidin-2-one","871210-22-9","D",0]
["3-[2-(Pentafluoroethyl)phenyl]propanoic acid","1380390-10-2","D",0]
["Tris(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-3,5-octanedionato)gadolinium(III)","17631-67-3","D",0]
["17:2 Fluorotelomer alcohol","176676-71-4","D",0]
["N-{N-[4-(Morpholine-4-carbonyl)benzoyl]valyl}-1-(5,5,6,6,6-pentafluoro-2-methyl-4-oxohexan-3-yl)pyrrolidine-2-carboximidic acid","149859-17-6","D",0]
["PROPANE, 2,2,3,3-TETRAFLUORO-1,1,1-TRICH","422-51-5","D",0]
["3,3,5-Trifluoro-5-(trifluoromethyl)-1,2,4-trioxolane","120030-78-6","D",0]
["Ammonium perfluorobutanedioiate","126996-02-9","D",0]
["3,4,4,4-Tetrafluoro-3-(trifluoromethoxy)butan-1-ol","1378864-58-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,8-Tetradecafluorooctane","361532-17-4","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methylpropanoate","242812-05-1","D",0]
["Ethyl 3,3,4,4,5,5,6,6,6-nonafluoro-2-methylidenehexanoate","117374-41-1","D",0]
["1-(Perfluoroethyl)-2-(perfluoropropyl)ethene","887111-61-7","D",0]
["Benzoic acid--1,1,3,3,3-pentafluoro-2-(trifluoromethyl)propan-1-ol (1/1)","62619-31-2","D",0]
["{3,4,5-Tris[1,1,2-trifluoro-2-(heptafluoropropoxy)ethoxy]phenyl}methanol","1233312-87-2","D",0]
["N-[3-(Dimethylamino)propyl]-N-[(undecafluoropentyl)sulfonyl]-beta-alanine","1383438-83-2","D",0]
["1,1,2,2-Tetrafluorocyclopropane","3899-71-6","D",0]
["5-fluoro-2-methyl-6-(pentafluoroethyl)pyrimidin-4(1h)-one","1548-79-4","D",0]
["2,3,4,4,5,5,6,6,6-Nonafluorohex-2-enoyl fluoride","88022-45-1","D",0]
["Lithium(1+) perfluoro-8‐{[(perfluorooctanesulfonyl)azanidyl]sulfonyl}octane","226885-12-7","D",0]
["2,6-Difluoro-N-((2-methyl-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)benzamide","100341-24-0","D",0]
["1-Methyl-4-(pentafluoroethyl)benzene","117081-46-6","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]-N-2-propen-1-yl-propanamide","174080-50-3","D",0]
["Chlorodipropyl(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)silane","608296-18-0","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(propane-2-sulfonyl)benzoic acid","1355555-15-5","D",0]
["2,2-bis(Trifluoromethyl)propionic acid","45048-36-0","D",0]
["Heptadecafluorononanoic acid--N-methylmethanamine (1/1)","77032-24-7","D",0]
["Potassium 2,2,3-trifluoro-3-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]propanoate","1087271-46-2","D",0]
["Acetic acid, compounds, chloro-, sodium salt, reaction products with N-(3-aminopropyl)-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-1-octanesulfonamide and 3-chloro-2-hydroxy-1-propanesulfonic acid monosodium salt","512179-62-3","D",0]
["Sodium 3-[[(perfluorooctyl)sulfonyl]propylamino]propanesulfonate","95470-07-8","D",0]
["4-[4-(Heptadecafluorooctyl)phenoxy]butyl prop-2-enoate","649721-94-8","D",0]
["4,4,4-trifluoro-3-hydroxy-1-(4-nitrophenyl)-3-(trifluoromethyl)butan-1-one","34844-17-2","D",0]
["1,1,1,2,2,3,3,5,5,5-Decafluoro-4,4-bis(trifluoromethyl)pentane","29971-79-7","D",0]
["4-(1,2,2,2-Tetrafluoroethyl)aniline","1547146-29-1","D",0]
["3-(Perfluorobutanesulfonamido)-N,N,N-trimethylpropan-1-aminium","70225-21-7","D",0]
["Ethyl 4,4,5,5,6,6,6-heptafluoro-3-hydroxyhexanoate","2707-76-8","D",0]
["2-Propenoic acid, 2-methyl-, 3-chloro-2-hydroxypropyl ester, polymer with .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene)","101896-32-6","D",0]
["6,6-Bis(trifluoromethyl)-1,3,5-triazinane-2,4-dione","1619-99-4","D",0]
["4-{[(1E)-1,2,3,3,4,4,5,5,6,6,6-Undecafluorohex-1-en-1-yl]oxy}benzene-1-sulfonyl chloride","958825-16-6","D",0]
["Heptadecafluorononanoyl bromide","261503-42-8","D",0]
["N,N′-[1,6-Hexanediylbis[(2-oxo-3,5-oxazolidinediyl)methylene]]bis[N-methyl-perfluoro-1-octanesulfonamide]","116250-61-4","D",0]
["Nifluridide","61444-62-0","D",0]
["Tetradecyl perfluorobutanoate","7365-36-8","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoroheptanenitrile","26649-23-0","D",0]
["3,4-Bis(difluoromethylidene)-1,1,2,2-tetrafluorocyclobutane","711-40-0","D",0]
["N-{2-[(6-Ethoxy-1,3-benzothiazol-2-yl)amino]-1,1,1,3,3,3-hexafluoropropan-2-yl}acetamide","4598-21-4","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-hexadecafluorooctane-1-sulfonic acid","134615-57-9","D",0]
["5-Chloro-perfluoropentanoic acid","66443-79-6","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-hexylbutanamide","75668-28-9","D",0]
["Methyl 4-(pentadecafluoroheptyl)cyclohexane-1-carboxylate","88951-17-1","D",0]
["(4E)-1,1,1,2,4,5,6,7,7,7-Decafluoro-2,6-bis(trifluoromethyl)hept-4-en-3-one","134330-91-9","D",0]
["Sodium perfluorohex-5-enoate","45187-32-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-Nonacosafluorotetradecane","66577-33-1","D",0]
["2λ5,4λ5,6λ5-1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexakis[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]-","1383437-42-0","D",0]
["Chlorodiethyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","608295-76-7","D",0]
["2-bromo-2,3,3,3-tetrafluoropropanoic acid","13859-31-9","D",0]
["N,N-Dicyclohexyl-2,2,3,3,4,4,4-heptafluorobutanamide","386-84-5","D",0]
["3,3,4,4,4-Pentafluoro-2-methylidenebutanoyl chloride","824411-01-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluoro-13-octacosene","1151525-71-1","D",0]
["Oxirane, 2-[(ethenyloxy)methyl]-, polymer with 1-propene and 1,1,2,2-tetrafluoroethene","69492-03-1","D",0]
["Bis(perfluoro-1-methyl-ethoxyethyl) phosphinic acid","500776-74-9","D",0]
["3,4,5,6,7-Pentafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-benzofuran-1(3H)-one","1419865-31-8","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoro-2-hydroxyundecyl 2-methylprop-2-enoate","93706-76-4","D",0]
["Perfluoroisobutyric acid","335-10-4","D",0]
["Sodium (N-methylperfluorobutanesulfonamido)acetate","864069-37-4","D",0]
["Ethyl 4,4,5,5,6,6,6-heptafluoronorleucinate","63664-52-8","D",0]
["2,2,3,3,4,5,6,7-Octafluoro-2,3-dihydro-1H-inden-1-one","58161-61-8","D",0]
["1-Cyano-2,2,3,3,4,4,4-heptafluorobutyl dimethyl phosphate","56376-19-3","D",0]
["1,1,2,2-Tetrafluoro-2-(1,1,2,2-tetrafluoro-2-iodoethoxy)ethane-1-sulfonamide","148716-83-0","D",0]
["2,2'-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)azanediyl]di(ethan-1-ol)","27607-40-5","D",0]
["Sodium 2-[[3,4,5-tris(1,1,2,3,3,3-hexafluoropropoxy)benzoyl]amino]ethanesulfonate","75860-13-8","D",0]
["6-[(Nonadecafluorononyl)oxy]hexanoic acid","113560-31-9","D",0]
["Buprofezin-Flubendiamide mixt.","1235982-65-6","D",0]
["1,1,1,3,3,3-Hexafluoro-2-iodopropane","4141-91-7","D",0]
["2,4-Difluoro-3-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]azete","62888-44-2","D",0]
["Phenyltetrafluoroethyl ether","53998-02-0","D",0]
["2-Bromo-6-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-3,5,5-trimethylcyclohex-2-en-1-one","101564-48-1","D",0]
["2,2,2-Triethoxy-4,4,5,5-tetrakis(trifluoromethyl)-1,3,2lambda5-dioxaphospholane","1708-77-6","D",0]
["Ethyl 4,4,5,5,6,6,6-heptafluorohexanoate","424-66-8","D",0]
["1,2,4,5-Tetrafluoro-3-(heptafluoropropyl)benzene","153817-18-6","D",0]
["{[(3,3,4,4,5,5-Hexafluoropent-1-yn-1-yl)sulfanyl]methyl}benzene","201943-34-2","D",0]
["Perfluorodichlorooctane","178335-16-5","D",0]
["2-(1,1,2,2-Tetrafluoroethyl)-1,4,5,6-tetrahydropyrimidine","936224-58-7","D",0]
["2-Propen-1-ol, reaction products with 1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-6-iodohexane, dehydroiodinated, reaction products with epichlorohydrin-triethylenetetramine polymer","464178-94-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluorodecane","1287702-46-8","D",0]
["Sodium potassium (perfluorobutanesulfonamido)acetic acid","688361-68-4","D",0]
["2,2-Bis(trifluoromethyl)-1,2-dihydropyrimidine--hydrogen chloride (1/1)","59389-79-6","D",0]
["1-Methyl-N-(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)cyclopentane-1-carboxamide","1440968-23-9","D",0]
["Methacrylic acid, 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl ester, polymer with 2-(diethylamino)ethyl methacrylate","34438-59-0","D",0]
["3-(Tridecafluorohexyl)benzene-1-thiol","56285-78-0","D",0]
["Perfluoro-5-fluorocarbonyl-3-oxapentanesulfonyl fluoride","1169825-97-1","D",0]
["4-(3-Chlorophenyl)-5-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]-2,4-dihydro-3H-1,2,4-triazole-3-thione","7166-97-4","D",0]
["3-[[(Perfluoropropyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium iodide","1966131-52-1","D",0]
["1-Ethoxy-1,1,2,3,3,3-hexafluoro-2-(trifluoromethyl)propane--1-ethoxy-1,1,2,2,3,3,4,4,4-nonafluorobutane (1/1)","813458-04-7","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-(phenylsulfanyl)octan-2-ol","89807-96-5","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7-Tridecafluorooctan-1-ol","112708-16-4","D",0]
["Sodium perfluorohexylperfluorooctylphosphinate","2361298-14-6","D",0]
["2-Propanol, 1,1,1,3,3,3-hexafluoro-2-[[(2-methoxyethyl)amino]methyl]-","380609-16-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-methylpropan-2-yl prop-2-enoate","53038-41-8","D",0]
["N-Methyl-4-(nonafluorobutyl)aniline","1426840-85-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6-Dodecafluorohexane","86498-66-0","D",0]
["Ethyl [5-(heptafluoropropyl)-1-methyl-1H-pyrazol-3-yl]acetate","1428569-19-0","D",0]
["8-(Heptafluoropropyl)adenosine","147916-81-2","D",0]
["Bis(2,2,3,3-tetrafluoropropyl) 2,2,2-trifluoroethyl phosphate","79338-99-1","D",0]
["2-(1,1,2,2-Tetrafluoro-2-phenylethyl)aniline--hydrogen chloride (1/1)","61547-72-6","D",0]
["Sodium 2-[[3-[[(perfluorohexyl)sulfonyl]amino]propyl]amino]ethanesulfonate","80621-18-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-hydroxybutanimidamide","4314-37-8","D",0]
["Methyl (2E)-4,4,5,5,6,6,6-heptafluoro-2-methyl-2-hexenoate","88021-94-7","D",0]
["2-bromo-1,1,1,3,3,4,4,5,5,5-decafluoro-2-(trifluoromethyl)pentane","22528-67-2","D",0]
["Bis(1,1,1,2,3,3-hexafluoropropan-2-yl) but-2-enedioate","24120-21-6","D",0]
["2-Propanol-d, 1,1,1,3,3,3-hexafluoro-","38701-73-4","D",0]
["1,1,1,2,2,3,3,12,12,13,13,14,14,14-Tetradecafluorotetradecane","1835251-91-6","D",0]
["1-(Perfluoroheptyl)octadecane","1980076-71-8","D",0]
["2-Bromo-2-(bromomethyl)-1,1,1,3,3,3-hexafluoropropane","247220-90-2","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl 4-(3-phenoxybenzyl)piperazine-1-carboxylate","1416133-89-5","D",0]
["2-[3-[(Perfluoro-1-oxononyl)amino]propoxy]-N,N,N-trimethylethanaminium 4-methylbenzenesulfonate","85212-69-7","D",0]
["N~1~,N~1~,N'~1~,N'~1~-Tetraethyl-2,3,3,3-tetrafluoroprop-1-ene-1,1-diamine","216393-97-4","D",0]
["Siloxanes and silicones, dimethyl, methyl 3-(1,1,2,2-tetrafluoroethoxy)propyl, methyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl, hydroxy terminated","115340-94-8","D",0]
["4-Chloro-1,1,1-trifluoro-5-methyl-2-(trifluoromethyl)hex-2-ene","99903-41-0","D",0]
["1,1'-(1,2,3,3,4,4-Hexafluorocyclobutane-1,2-diyl)bis(4-bromobenzene)","918409-60-6","D",0]
["2-(Heptafluoropropyl)-9H-purin-6-amine","147916-77-6","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-(methanesulfonyl)butane","40630-22-6","D",0]
["3-Methylbutyl heptadecafluorononanoate","117374-32-0","D",0]
["4H-Perfluoropentanesulfonic acid","2089109-55-5","D",0]
["2,2,3-Trifluoro-3-(trifluoromethyl)-2,3-dihydro-1H-inden-1-one","60375-80-6","D",0]
["Cloflubicyne","224790-70-9","D",0]
["Chloro-4-(chlorotetrafluoroethyl)-1-(trifluoromethyl)benzene","72030-22-9","D",0]
["Undecanoyl chloride, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-","89373-67-1","D",0]
["2‐ [2-(Perfluorodecyl)ethylsulfanyl]acetic acid","1513863-88-1","D",0]
["4,4,5,5,5-Pentafluoro-1-phenylpent-1-en-3-ol","56184-56-6","D",0]
["4-[(Diphenylmethoxy)methyl]-2,2-bis(trifluoromethyl)-1,3-dioxolane","51125-55-4","D",0]
["1,1,1,2,2,3,3,4,4,7,7,8,8,8-Tetradecafluorooctane","343627-66-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorotriacontane","93454-75-2","D",0]
["3-(1,1,2,2-tetrafluoroethoxy)phenol","53997-99-2","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-amine","2809-92-9","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate","82682-08-4","D",0]
["Chloro(3,3,4,4,5,5,5-heptafluoropentyl)bis(3,3,3-trifluoropropyl)silane","608296-81-7","D",0]
["2-(Tridecafluorohexyl)aniline","139613-89-1","D",0]
["Pyrifluquinazon","337458-27-2","D",0]
["Perfluorotridecanoate","862374-87-6","D",0]
["Hexafluoropropene, oxidized, oligomers reduced, reaction products with methanol, reduced, reaction products with ethylene oxide","162492-13-9","D",0]
["(1E)-3,3,4,4,5,5,5-Heptafluoro-1-iodopent-1-ene","157430-71-2","D",0]
["2,3,3,3-Tetrafluoro-2-(perfluoropentoxy)propan-1-ol","78693-85-3","D",0]
["(2-methylphenyl) 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","42096-33-3","D",0]
["Dichlorotris[(1,1,1,3,3,3-hexafluoropropan-2-yl)oxy]-lambda~5~-phosphane","66559-58-8","D",0]
["Perfluoro-3,7-dimethyloctanoic acid","172155-07-6","D",0]
["2-(Tridecafluorohexyl)-1H-benzimidazole","119403-54-2","D",0]
["Ethyl perfluorododecanoate","158607-41-1","D",0]
["3-Octanone, 8-chloro-5,5,6,6,7,7,8,8-octafluoro-2,2-dimethyl-","119091-29-1","D",0]
["2-C-(Heptafluoropropyl)-α-D-ribofuranose","467220-81-1","D",0]
["2,3,3,3-Tetrafluoro-1-(2-hydroxyphenyl)propan-1-one","83505-20-8","D",0]
["Pentafluoropropanoyl bromide","64609-91-2","D",0]
["1-Ethyl-3-methylpyridin-1-ium nonafluorobutane-1-sulfonate","1015420-87-7","D",0]
["Octane, 1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-8-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]-","78522-74-4","D",0]
["1,2-Dibromoperfluoroheptane","678-32-0","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-[(prop-2-en-1-yl)oxy]hexane","188298-09-1","D",0]
["1-Chloro-1,1,2,2,4,5,5,5-octafluoro-4-(trifluoromethyl)pentan-3-one","42287-81-0","D",0]
["5,5,6,6,7,7,7-Heptafluoro-3-nitro-3-heptene","1422-67-9","D",0]
["[2-(Difluoromethyl)-2,3,3,3-tetrafluoropropyl]benzene","55012-43-6","D",0]
["1,1,2,2,3,5,6,7,8-Nonafluoro-4-methyl-1,2-dihydronaphthalene","65653-73-8","D",0]
["N,N'-(3,3'-Dichloro[1,1'-biphenyl]-4,4'-diyl)bis(heptafluorobutanimidic acid)","75042-09-0","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N,N-dimethyl-N-propyl-1-propanaminium bromide","163973-44-2","D",0]
["4-(Dimethylamino)-2-{[(perfluorobutyl)sulfonyl]amino}butanoic acid","2089109-96-4","D",0]
["tert-Butyl heptafluorobutanoate","425-24-1","D",0]
["Cyclohexane, 1,1,2,2,3,3,4,4,5,5,6-undecafluoro-6-iodo-","355-69-1","D",0]
["Decafluorocyclohexane","55101-67-2","D",0]
["Zonyl FSP(An anionic surfactant derived from linear perfluoroalkyl ethers of PEG phosphate ammonium salt (Du Pont) )","67479-86-1","D",0]
["4,4,5,5,6,6,6-Heptafluoro-3-(nitromethyl)hexanoic acid","7079-86-9","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Hexadecafluorododecane-1,12-diyl)bis(trichlorosilane)","445303-83-3","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-sulfonamide","29765-95-5","D",0]
["6,6,7,7-Tetrafluoro-2,3-diazabicyclo[3.2.0]hept-2-ene","87102-51-0","D",0]
["2'-Deoxy-5-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)uridine","79383-26-9","D",0]
["1,2,4-Trifluoro-3,5-bis(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-nitrobenzene","20017-51-0","D",0]
["5,5,6,6,7,7,8,8,9,9,9-Undecafluorononane-2,4-dione","75824-01-0","D",0]
["2-[Perfluoro-2-(propoxy)ethoxyethoxy]acetic acid","919005-44-0","D",0]
["1,1,1,2,3,3-Hexafluoro-3-(trifluoromethoxy)-2-(trifluoromethyl)propane","110719-85-2","D",0]
["Sodium 2‐{[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9‐hexadecafluorononyl)oxy]carbonyl}benzene‐1‐sulfonate","29811-20-9","D",0]
["Perfluorodecanoate","73829-36-4","D",0]
["Sodium N-(2-carboxylatoethyl)-3-[(2-carboxyethyl)[(perfluorohexyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","81190-42-3","D",0]
["N-(2-Methoxyethyl)-N-methyl-P,P-bis(perfluorobutyl)phosphinic amide","1609949-98-5","D",0]
["2-Pentanone, 4-chloro-5,5,5-trifluoro-4-(trifluoromethyl)-","101931-67-3","D",0]
["2-(Acryloyloxy)ethyl pentadecafluorooctanoate","14814-76-7","D",0]
["3,5-dichloro-4-(1,1,2,3,3,3-hexafluoropropoxy)aniline","108997-68-8","D",0]
["(1E)-1,2,3,3,3-Pentafluoro-1-(trifluoromethoxy)prop-1-ene","1621181-80-3","D",0]
["Methyl perfluorobutanesulfonate","6401-03-2","D",0]
["1,3-Propanedisulfonic acid, 1,1,2,2,3,3-hexafluoro-, lithium salt (1:2)","156000-47-4","D",0]
["2-Methyl-3-(pentafluoroethyl)non-2-en-4-yne","112678-68-9","D",0]
["2-(2,3,3,4,4,5,5-Heptafluoropentyl)oxolane","194348-01-1","D",0]
["D-Galactose 6-(1-(perfluorooctyl)-3-dodecyl hydrogen phosphate)","147695-19-0","D",0]
["2-(Heptafluoropropyl)-1-methoxy-4-methylbenzene","87461-66-3","D",0]
["(10E)-12,12,13,13,14,14,15,15,16,16,17,17,17-Tridecafluoroheptadec-10-en-1-ol","135131-53-2","D",0]
["Methoxydipropyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","608299-88-3","D",0]
["(1S,2R)-1-(Heptafluoropropyl)-2-iodocyclohexane","7589-44-8","D",0]
["[4-(2,2,3,3-Tetrafluoropropoxy)phenyl]hydrazine","175691-03-9","D",0]
["4,4'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(2-bromophenol)","189039-61-0","D",0]
["Pentafluorocyclopropane","872-58-2","D",0]
["2-(2,2,3,3-Tetrafluoropropoxy)ethan-1-ol","50997-68-7","D",0]
["1,1,2,2-Tetrafluoro-2-(2,2,2-trifluoroethoxy)ethane-1-sulfonic acid","113507-78-1","D",0]
["3,6-Dioxabicyclo[3.1.0]hexane, 1,2,2,4,4,5-hexafluoro-","680615-57-0","D",0]
["2,2-Difluoro-2-(2,3,3,4,4,5,5-heptafluorooxolan-2-yl)-1-(morpholin-4-yl)ethan-1-one","5190-45-4","D",0]
["2,2,4,5-Tetrafluoro-3,5-bis(trifluoromethyl)-2,5-dihydrofuran","90169-96-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-Heptacosafluoro-15-iodopentadecane","146983-96-2","D",0]
["1-[4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)phenyl]ethan-1-one","353273-22-0","D",0]
["2-(1,2,3,3,3-Pentafluoroprop-1-en-1-yl)oxolane","74727-27-8","D",0]
["2,2,3,3,4,4,4-Heptafluorobutanoyl nitrite","663-25-2","D",0]
["3-N,3-N,9-N,9-N-tetraethyl-3,9-bis(1,2,2,2-tetrafluoroethyl)-2,4,8,10-tetraoxaspiro[5.5]undecane-3,9-diamine","89752-23-8","D",0]
["Acetic acid--2,3,3,4,4-pentafluorocyclobut-1-en-1-ol (1/1)","61996-29-0","D",0]
["N-(Carboxymethyl)-3-{(carboxymethyl)[(nonafluorobutyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","2089109-88-4","D",0]
["2-[4-(Heptadecafluorooctyl)phenoxy]ethyl prop-2-enoate","649721-92-6","D",0]
["HFE-236ca12","78522-47-1","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-iododecane","40735-32-8","D",0]
["N-(6-Amino-1,3-dimethyl-2,4-dioxo-1,2,3,4-tetrahydropyrimidin-5-yl)-2,2,3,3,3-pentafluoropropanamide","288391-11-7","D",0]
["Trimethylsilyl 4,4,4-trifluoro-3-(trifluoromethyl)but-2-enoate","88237-43-8","D",0]
["5-(Undecafluoropentyl)-1H-imidazole","113934-18-2","D",0]
["hexafluoropentanedioic acid- piperazine(1:1)","1652-47-7","D",0]
["N-(Morpholin-4-ylmethyl)perfluorooctane-1-sulfonamide","100221-83-8","D",0]
["2,2-Difluoro-2-[1,1,2,2-tetrafluoro-2-(perfluoroethoxy)ethoxy]-N-[3-(trimethoxysilyl)propyl]acetamide","154380-35-5","D",0]
["2,2,3,4,4-Pentafluoro-4-(trifluoromethoxy)butanoic acid","919005-24-6","D",0]
["1-(3,3,4,4,5,5,5-Heptafluoro-1-iodopentyl)-2,8,9-trioxa-5-aza-1-silabicyclo[3.3.3]undecane","112330-85-5","D",0]
["3,4,4,5,5,6,6,6‐Octafluorohex‐2‐enal","864551-39-3","D",0]
["4-(2,2,3,3,4,4,5,5,5-Nonafluoropentyl)-1,3-dioxolan-2-one","912364-40-0","D",0]
["1,1,1,2,2,3,3-Heptafluorooctane","2708-54-5","D",0]
["(Nonafluorobutyl)carbonimidoyl","424-32-8","D",0]
["1,1,1,2,2,3,3,4,4,15,15,16,16,17,17,18,18,18-Octadecafluorooctadecane","1835251-99-4","D",0]
["Pentafluoroethoxybenzene","1644-22-0","D",0]
["[[4-[(Heptadecafluorononyl)oxy]phenyl]methyl]-phosphonic acid","63513-09-7","D",0]
["3-[2,2,3,3,4,4,5,5-octafluoro-1-(trifluoromethyl)cyclopentyl]propanoic Acid","243659-13-4","D",0]
["Prop-2-en-1-yl tridecafluoroheptanoate","53378-90-8","D",0]
["2-[3,3,3-trifluoro-2,2-bis(trifluoromethyl)propyl]oxirane","502482-28-2","D",0]
["2-(2-Amino-5-methyl-phenyl)-1,1,1,3,3,3-hexafluoro-propan-2-ol","1992-07-0","D",0]
["Decane-1,10-diyl bis(heptafluorobutanoate)","426-64-2","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptane-1,1-diol","812-87-3","D",0]
["1,1,1,3,3,3-Hexafluoro-2-nitropropane","13071-90-4","D",0]
["1-(4-Chlorophenyl)-2-ethyl-4,4,4-trifluoro-3-(trifluoromethyl)butane-1,3-diol","34848-31-2","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl nonafluorobutane-1-sulfonate","118334-96-6","D",0]
["Potassium perfluoropentanoate","336-23-2","D",0]
["3-Formyl-2,2-bis(trifluoromethyl)cyclopropane-1-carbonyl chloride","99903-47-6","D",0]
["Dichloro(pentafluorophenyl)(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","2400991-08-2","D",0]
["1-Chloro-3,3-bis(trifluoromethyl)-1,3-dihydro-1lambda~3~,2-benziodoxole","76215-48-0","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(trifluoromethyl)-, 1,1'-anhydride, reaction products with di-Et sulfate and potassium fluoride","1017237-71-6","D",0]
["1,1,1,3,3,4,4,6,6,6-Decafluoro-2,5-bis(trifluoromethyl)hexane-2,5-diol","652132-19-9","D",0]
["Sodium .alpha.-[2-[[(heptadecafluorooctyl)sulfonyl]propylamino]ethyl]-.omega.-(4-sulfonatobutoxy)poly(oxyethylene)","146245-94-5","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with ammonia, reduced","161308-17-4","D",0]
["Tetradecyl perfluorodecanoate","250237-67-3","D",0]
["4-Chloro-2,2-bis(trifluoromethyl)-2H-1,3-dioxole","89444-44-0","D",0]
["3,4-dibromo-1,1,1,2,2-pentafluorobutane","378-69-8","D",0]
["4-(2,3-Dimethylphenyl)-5-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]-2,4-dihydro-3H-1,2,4-triazole-3-thione","7167-31-9","D",0]
["3-[(Perfluoro-1-oxobutyl)amino]-N,N,N-trimethyl-1-propanaminium chloride","89148-25-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-9-docosene","118642-84-5","D",0]
["N,N,N-Triethyldecan-1-aminium heptadecafluorooctane-1-sulfonate","773895-92-4","D",0]
["2,2'-(1,1,2,2,3,3-Hexafluoropropane-1,3-diyl)bis(1H-benzimidazole)","1642-30-4","D",0]
["2-Bromo-4-(1,1,2,2-tetrafluoroethoxy)phenol","89227-92-9","D",0]
["1-Butanamine, 1,1,2,2,3,3,4,4,4-nonafluoro-N,N-bis(1,1,2,2,3,3,4,4,4-nonafluorobutyl)-, mixt. with 1,1,2,2,3,3,4,4,4-nonafluoro-N-(1,1,2,2,3,3,4,4,4-nonafluorobutyl)-N-(trifluoromethyl)-1-butanamine","51142-49-5","D",0]
["(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)(trimethoxy)-lambda~5~-phosphane","650-58-8","D",0]
["Triethylammonium perfluorooctane sulfonate","54439-46-2","D",0]
["Phosphite, tris(2,2,3,3-tetrafluoropropyl)-","2241-68-1","D",0]
["Pentafluoroethane-D1","87458-21-7","D",0]
["1,1,1,2,2,3,3-Heptafluoropentadecane","106873-69-2","D",0]
["1,1,1,2,3,3-Hexafluoro-3-(3,3,3-trifluoropropoxy)propane","845523-33-3","D",0]
["4,4-Bis(trifluoromethyl)-4,5-dihydro-1H-pyrazole-3-carbonitrile","61859-93-6","D",0]
["2-(2-Chloro-1,1,2-trifluoroethoxy)-1,1,1,2-tetrafluoroethane","51410-31-2","D",0]
["4,4-Dichloro-2,2,5,5-tetrafluoro-3-(trifluoromethyl)-1,3-oxazolidine","104550-51-8","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, 1,3,3a,4,7,7a-hexahydro-1,3-dioxo-4,7-methano-2H-isoindol-2-yl ester","307531-76-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorohexadecane","147492-59-9","D",0]
["3,5-Dimethyl-1-(2,2,3,3-tetrafluoropropyl)-1H-pyrazol-4-amine","1006486-98-1","D",0]
["3,4-Dibromo-2,2,5,5-tetrafluorooxolane","1070993-50-8","D",0]
["2-Chloro-3-iodo-5-(pentafluoroethyl)pyridine","1286743-96-1","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reduced, reaction products with ethylene oxide and methacrylic anhydride","162492-14-0","D",0]
["2-Ethylhexyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","340034-61-9","D",0]
["1,1,2,2-tetrafluoroethylether","2356-61-8","D",0]
["Chloro(nonafluoro)cyclopentane","376-76-1","D",0]
["Ethyl 4,4,5,5-tetrafluoro-3-hydroxypent-2-enoate","138709-59-8","D",0]
["Tris(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) phosphate","165325-62-2","D",0]
["Perfluoro-2,5-dimethyl-3,6-dioxanonanoic acid, sodium salt","67963-76-2","D",0]
["4-[[2,2,3,3-tetrafluoro-3-(trifluoromethoxy)propanoyl]amino]benzoate","6813-23-6","D",0]
["Ethyl 6-chloro-3,4,4,5,5,6,6-heptafluorohex-2-enoate","170502-20-2","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexane-1-sulfonamide","29765-93-3","D",0]
["1,1,2,3,3,4,4,5,5-Nonafluoro-5-[(trifluoroethenyl)oxy]pent-1-ene","122440-16-8","D",0]
["N-Butyl-N-[(nonafluorobutyl)sulfonyl]glycine","864069-45-4","D",0]
["Ethyl perfluoroundecanoate","41506-11-0","D",0]
["Quinolin-6-yl nonafluorobutane-1-sulfonate","920491-93-6","D",0]
["(1H,1H,2H,2H-perfluorooctyl)triacetoxysilane","1034681-41-8","D",0]
["Ethyl 5-chloro-2,2,3,3,4,4-hexafluoropentanoate","139265-07-9","D",0]
["Sodium N-[(nonafluorobutyl)sulfonyl]-N-propylglycinate","864069-35-2","D",0]
["2,2,2-trifluoroethyl perfluorobutanimidate","4078-29-9","D",0]
["3,3'-Bis(tridecafluorohexyl)-2,2'-bithiophene","630045-87-3","D",0]
["5-Chloro-1,1,1,2,2-pentafluoropentane","1024003-32-4","D",0]
["3,5,7,8-Tetrachloro-2,2,3,4,4,5,6,6,7,8,8-undecafluorooctanoic acid--cyclohexanamine (1/1)","2966-03-2","D",0]
["(1R,2S)-1-Iodo-2-(pentafluoroethyl)cyclohexane","38787-67-6","D",0]
["Bis(perfluoropentanoyl) peroxide","308-29-2","D",0]
["3-[(2-Carboxyethyl)[(perfluoropentyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","2089109-16-8","D",0]
["1,1,1,7-Tetrachloro-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptane","1550-21-6","D",0]
["[3-(2,2,3,3,4,4,4-heptafluorobutanoyloxy)-2,2-bis(2,2,3,3,4,4,4-heptafluorobutanoyloxymethyl)propyl] 2,2,3,3,4,4,4-heptafluorobutanoate","464-40-4","D",0]
["6H-Perfluorohex-1-ene","1767-94-8","D",0]
["N-(2-Bromo-4-nitrophenyl)-2,3,3,3-tetrafluoro-2-(trifluoromethyl)propanamide","105923-30-6","D",0]
["5-(Nonafluorobutyl)bicyclo[2.2.1]hept-2-ene","118777-97-2","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoro-3-methoxy-1-phenylheptan-1-one","105602-77-5","D",0]
["cis-Perfluorohydrindan","75262-87-2","D",0]
["Decane, 10-azido-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-","121177-79-5","D",0]
["3-(Butane-2-sulfonyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-57-2","D",0]
["N,N-Dimethyl-1H,1H,7H-perfluoroheptanamine","104312-38-1","D",0]
["tert-Butyl tridecafluoroheptaneperoxoate","83162-30-5","D",0]
["Ethyl (2-chloro-1,1,2,2-tetrafluoroethoxy)(difluoro)acetate","83865-06-9","D",0]
["1,1,3,4,4,4-Hexafluoro-3-(trifluoromethyl)but-1-ene","1840-17-1","D",0]
["1-Bromo-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-2-ol","89807-98-7","D",0]
["Nafion 117( A perfluorosulfonic acid cationic exchange membrane, probably a perfluoro(3,6-dioxa-4-methyl-7-octenesulfonic acid)-tetrafluoroethylene copolymer (Nicolet Inst. Corp.). -[O-CF2-CF(CF3)]n-OCF2-SO3H grafted to fluorocarbon chain )","66796-30-3","D",0]
["3,5-Dichloro-4-[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]aniline","105406-41-5","D",0]
["Butan-2-yl N-(2,2,3,3,4,4,4-heptafluorobutanoyl)-D-alaninate","93080-42-3","D",0]
["Sodium 3-(perfluoropropyl)propanoate","1207462-13-2","D",0]
["4‐Methyl‐1‐(1,1,2,2,2‐pentafluoroethyl)‐2,6,7‐trioxabicyclo[2.2.2]octane","31185-65-6","D",0]
["N-(((2,3-Dimethyl-4-((1,1,2,2-tetrafluoroethyl)thio)phenyl)amino)carbonyl)-2,6-difluorobenzamide","100279-93-4","D",0]
["N-Benzyl-2,2,3,3,3-pentafluoropropionamide","1799-75-3","D",0]
["2-(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptanoyl)cyclohexan-1-one","141478-89-9","D",0]
["(E)-1-[(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)oxy]-1-oxo-2-phenyl-1lambda~5~-diazene","88280-62-0","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol and 2-aminoethanol","161212-28-8","D",0]
["2'-Deoxy-5-(tridecafluorohexyl)uridine","144862-39-5","D",0]
["1-Benzoyl-3,5-bis(heptafluoropropyl)pyrazole","231953-37-0","D",0]
["Dimethyl (6,6,7,7,7-pentafluoro-2-oxoheptyl)phosphonate","62401-59-6","D",0]
["Perfluoroheptane sulfonic anhydride","140429-92-1","D",0]
["3,4,4-Trifluoro-3-(heptafluoropropyl)-1,2lambda~6~-oxathietane-2,2-dione","156465-44-0","D",0]
["2,2-Dichloro-4,4,6,6-tetrakis(2,2,3,3-tetrafluoropropoxy)-1,3,5,2lambda~5~,4lambda~5~,6lambda~5~-triazatriphosphinine","65601-42-5","D",0]
["2-(4-tert-Butylpyridin-2-yl)-1,1,1,3,3,3-hexafluoropropan-2-ol","87432-81-3","D",0]
["4-(1,1,2,3,3,3-Hexafluoropropoxy)-N-(2-phenoxyethyl)benzamide","909351-91-3","D",0]
["3-(Heptafluoropropyl)-4-nitro-5-phenylpyrazole","244187-06-2","D",0]
["Phosphonous acid, ethyl-, diethyl ester, compd. with 1,1,1,2,3,3,3-heptafluoro-2-iodopropane (1:1)","72220-43-0","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(1,2,2,2-tetrafluoro-1-iodoethoxy)propane","107432-46-2","D",0]
["1-Methyl-4-(nonadecafluorononyl)benzene","88950-99-6","D",0]
["7-Azido-1H,1H-perfluoroheptane","159707-40-1","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-sulfonate","425670-75-3","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[(heptadecafluorooctyl)sulfonyl] propylamino]ethyl]-ω-[2-[[(heptadecafluorooctyl)sulfonyl] propylamino]ethoxy]-","138570-74-8","D",0]
["2-[[(Heptadecafluorooctyl)sulfonyl]propylamino]ethyl [3-[[[2-[[(heptecafluorooctyl)sulfonyl]methylamino]ethoxy]carbonyl]amino]-4-methylphenyl]carbamate","99908-28-8","D",0]
["3-(2,2,3,3-Tetrafluoropropoxy)prop-1-ene","681-68-5","D",0]
["2-(Pentafluoroethyl)cyclohexanone","56734-75-9","D",0]
["1,1,1,2,5,5,5-Heptafluoro-4-methylpent-2-ene","90296-73-4","D",0]
["1,2,3,4,7,7-Hexachloro-5-(2,2,3,3-tetrafluorocyclobutyl)bicyclo[2.2.1]hept-2-ene","1890-47-7","D",0]
["Poly(oxy-1,2-ethanediyl), α-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-oxooctyl)-ω-hydroxy-","67296-32-6","D",0]
["5,5,6,6-Tetrafluorodecane-2,4,7,9-tetrone","63579-02-2","D",0]
["N-(Carboxylatomethyl)-3-[[[4-[(perfluorooctyl)oxy]phenyl]sulfonyl]amino]-N,N-dimethyl-1-propanaminium","89932-75-2","D",0]
["3-((3-((N-(2-Carboxyethyl)-perfluorobutyl)sulfonamido)propyl)-dimethylammonio)propanoate","2254560-13-7","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-phenylnonanamide","313366-93-7","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(propane-1-sulfinyl)benzoic acid","1355554-90-3","D",0]
["Tris(perfluoro(2-isopropoxyethyl))-methylsilane","104745-21-3","D",0]
["Formic acid--3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-ol (1/1)","53488-23-6","D",0]
["4-Chloro-2-fluoro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-90-3","D",0]
["4-(Nonafluorobutyl)benzonitrile","137052-16-5","D",0]
["Tridecyl perfluorobutanoate","959088-59-6","D",0]
["(1,1,2,2-Tetrafluoroethoxy)cyclohexane","456-63-3","D",0]
["(1S,4S)-3-(Heptafluorobutyryl)camphor","115224-00-5","D",0]
["Perfluoro-1,3-diisopropylcyclohexane","75169-51-6","D",0]
["3-[(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)oxy]-2-methylprop-1-ene","38471-83-9","D",0]
["\"Methoxy(3,3,4,4,5,5,6,6,7,7,8,8,8- tridecafluorooctyl)-silanediol\"","1531633-11-0","D",0]
["Methyl 2,2,3,3-tetrafluoropropionate","1893-38-5","D",0]
["N,N'-(Methylenedi-1,4-phenylene)bis(perfluorobutanamide)","124232-75-3","D",0]
["2,2,3,3,4,4-Hexafluoro-1-butanamine","605685-98-1","D",0]
["1-Chloro-2,2,3,3,4,4,5,5-octafluoro-1-isocyanatopentane","189244-65-3","D",0]
["Perfluorooctanesulfinic acid","647-29-0","D",0]
["N-ethyl-2-[[[[3-[[[[3-[[[[3-[[[2-[ethyl[(perfluorooctyl)sulfonyl]amino]ethoxy]carbonyl]amino]methylphenyl]amino]carbonyl]amino]methylphenyl]amino]carbonyl]amino]methylphenyl]amino]carbonyl]oxy]-N,N-dimethylethanaminium","100066-53-3","D",0]
["5-(Heptafluoropropyl)-1-methylisoquinoline","28439-77-2","D",0]
["Perfluoro-3-(pentafluoro-lambda6-sulfanyl)-1-propanesulfonic acid","2089109-31-7","D",0]
["Sodium 3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfanyl]propanoate","1254255-46-3","D",0]
["2-Pyrroleethanol, alpha,alpha-bis(trifluoromethyl)-1,5-dimethyl-","102367-04-4","D",0]
["3-[Perfluoro-2-(propoxy)ethoxy]propanoic acid","919005-43-9","D",0]
["N-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)-4-methoxybenzamide","40024-23-5","D",0]
["1-[(Phenylsulfonyl)oxy]-2,2-bis(trifluoromethyl)aziridine","55734-41-3","D",0]
["1,1,1,2,2-Pentafluorodecane","1024003-30-2","D",0]
["Polypropene-co-perfluoroethene-co-(vinyl butan-2-enoate)","852204-74-1","D",0]
["Poly[oxy(1,1,2,2,3,3,4,4,5,5-decafluoro-1,5-pentanediyl)], .alpha.-[5-[[2-(carboxymethyl)-1-oxooctadecyl]oxy]-1,1,2,2,3,3,4,4-octafluoropentyl]-.omega.-(nonafluorobutoxy)-","219795-01-4","D",0]
["4-(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)aniline","919289-98-8","D",0]
["3-Hydroxy-3-(1,1,2,2-tetrafluoroethyl)piperazin-2-one","89972-19-0","D",0]
["Perfluorodecahydro-2-sec-butylnaphthalene","119141-86-5","D",0]
["2-(2,3,3,4,4,5,5-Heptafluorocyclopent-1-en-1-yl)-3-methylthiophene","743457-67-2","D",0]
["N-Benzyl-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanamide","82970-41-0","D",0]
["1-Bromo-3-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethyl]benzene","64115-95-3","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl methyl{[3-(pyridin-4-yl)phenyl]methyl}carbamate","1416133-88-4","D",0]
["N-Bromo-2,2,2-trifluoroethanimidoyl fluoride","89554-90-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(1,2,3,4-tetrahydroquinolin-6-yl)propan-2-ol","65797-52-6","D",0]
["Acrylic acid, ester with 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-N-propyl-1-octanesulfonamide, polymer with acrylamide and styrene","30869-50-2","D",0]
["3-(Pentafluoroethyl)benzonitrile","1823246-09-8","D",0]
["2-(1-Adamantylamino)-1,1,1,3,3,3-hexafluoro-2-propanol, sesquihydrate","63765-69-5","D",0]
["1-Fluoro-4-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]benzene","26029-51-6","D",0]
["1-Chloroperfluoropentane","375-71-3","D",0]
["2-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)naphthalene","51114-14-8","D",0]
["Ethoxydimethyl (3,3,4,4,5,5,5-heptafluoropentyl) silane","608301-01-5","D",0]
["1,3-Bis(2-phenyl-1,3,4-oxadiazol-5-yl)perfluoropropane","5086-79-3","D",0]
["1,1,1,2,3,3,3-Heptafluoro-2-(1,1,2,2-tetrafluoro-2-iodoethoxy)propane","16005-38-2","D",0]
["2,2,3,3,4,4,4-heptafluoro-1-pyrrolidin-1-ylbutan-1-one","424-54-4","D",0]
["2-(2,2,3,3,3-Pentafluoropropanoyl)cyclohexan-1-one","2145-82-6","D",0]
["1-(Difluoromethyl)-3,3,4,4,5,5,6,6-octafluorocyclohex-1-ene","115880-31-4","D",0]
["2,2,3,3-Tetrafluoro-3-methoxypropanoic acid","93449-21-9","D",0]
["Heptadecafluorononanoic acid--aniline (1/1)","95682-67-0","D",0]
["Bis(2,2,3,3,4,4,5,5-octafluoropentyl) ethanedioate","866-11-5","D",0]
["6,6,7,7,8,8,9,9,9-Nonafluoro-3-methylnon-4-yn-3-ol","82721-69-5","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluoropentyl)sulfonyl]amino}propyl)-1-butanaminium","2089109-94-2","D",0]
["N-[2-(3,4-Dimethoxyphenyl)ethyl]-2,2,3,3,4,4,4-heptafluorobutanamide","13230-87-0","D",0]
["4'-Hydroxy[1,1'-biphenyl]-4-yl 2-[perfluoro-4-morpholinylmethyl]-perfluoropropanoate","304658-31-9","D",0]
["N-(Carboxylatomethyl)-N,N-dimethyl-3-[(perfluoro-1-oxododecyl)amino]propanaminium","1513863-82-5","D",0]
["1-Bromo-4-(1,2,2,3,3,3-hexafluoropropyl)benzene","189762-31-0","D",0]
["1-[3,5-Bis(nonafluorobutyl)-1H-pyrazol-1-yl]ethan-1-one","247170-28-1","D",0]
["4,4',5,5,5',5'-Hexafluoro-2,2,2',2'-tetrakis(trifluoromethyl)-4,4'-bi-1,3-dioxolane","139481-27-9","D",0]
["4-Methyl-2,2-bis(trifluoromethyl)-2H-pyrido[1,2-a][1,3,5]triazine","6334-38-9","D",0]
["1,1',1'',1'''-[(5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-pentadecafluoroundecane-1,3-diyl)diphosphoryl]tetraaziridine","23081-40-5","D",0]
["6-tert-Butyl-2-chloro-4,4-bis(trifluoromethyl)-1,3,2lambda~5~-dioxaphosphinan-2-one","102338-71-6","D",0]
["1-Benzyl-2-(heptafluoropropyl)-4,5-dihydro-1H-imidazole","1069085-51-3","D",0]
["1-Bromo-4-(tridecafluorohexyl)benzene","149068-56-4","D",0]
["Poly(1,1-difluoroethylene/1,1,3,3,3-pentafluoropropene/tetrafluoroethylene/trifluoromethyl trifluorovinyl ether)","259152-52-8","D",0]
["Perfluoro-2-methyl-3-(propan-2-yl)pentan-3-yl","93683-27-3","D",0]
["3,3,3-trifluoro-1-(2-methylaziridin-1-yl)-2-(trifluoromethyl)propan-1-one","50837-76-8","D",0]
["Chlorodiethyl(3,3,4,4,5,5,5-heptafluoropentyl)silane","608295-70-1","D",0]
["4,4-Bis(trifluoromethyl)bicyclo[3.2.0]hepta-2,6-diene","714-64-7","D",0]
["1,2,3-Trichloro-3,4,4,5,5-pentafluorocyclopent-1-ene","3824-97-3","D",0]
["Phenyl(tridecafluorohexyl)iodanium","74061-31-7","D",0]
["1,4-Bis(perfluorobutyl)butane","345944-97-0","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoroheptyl prop-2-enoate","443145-46-8","D",0]
["4-(Propan-2-yl)-2-(1,1,2,2-tetrafluoroethyl)-1,3-oxazol-5(2H)-one","51314-53-5","D",0]
["(4-Chlorophenyl)[4-(1,1,2,2-tetrafluoroethoxy)phenyl]methanone","334931-09-8","D",0]
["Allyl 2,2,3,3,4,4,5,5-octafluoropentyl ether","3108-07-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Nonadecafluorodecan-1-amine","307-36-8","D",0]
["5-(1,1,2,2-tetrafluoroethyl)-1H-1,2,4-triazole","1207091-13-1","D",0]
["1,1,1,3,3,3-hexafluoro-2-(iodomethyl)propane","883449-40-9","D",0]
["2,6-Difluoro-N-[{[2-fluoro-4-(1,1,2,2-tetrafluoroethanesulfinyl)phenyl]imino}(hydroxy)methyl]benzene-1-carboximidic acid","100341-42-2","D",0]
["(1,1,1,5,5,6,6,7,7,7-Decafluorohept-3-yn-2-ylidene)cyclopentane","139226-05-4","D",0]
["1,1,2,2,3,3,4,5,5,6-Decafluoro-4,6-dimethylcyclohexane","29917-43-9","D",0]
["2,2,3,3-Tetrafluoro-3-(methylsulfanyl)propanoic acid","77705-92-1","D",0]
["1,1,1,3,3,3-Hexafluoro-2-[5-(2-methyl-2-propanyl)-1,1-dioxido-3,3-bis(trifluoromethyl)-3H-2,1-benzoxathiol-7-yl]-2-propanol","84649-60-5","D",0]
["2-[(2,2,3,3-Tetrafluoropropyl)sulfanyl]phenol","90314-95-7","D",0]
["17-H-Perfluoroheptadecanoic acid","1870-13-9","D",0]
["Tetraethyl (3,3,4,4-tetrafluorocyclobut-1-ene-1,2-diyl)bis(phosphonate)","4545-92-0","D",0]
["1H,1H-Perfluorononylamine; 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluorononylamine","355-47-5","D",0]
["Dichloro(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)(pentafluorophenyl)silane","2400991-07-1","D",0]
["2-Propenoic acid, butyl ester, polymer with 2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate, 2-[methyl[(nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate, .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-hydroxypoly(oxy-1,4-butanediyl), .alph","68227-95-2","D",0]
["[2,2-Bis(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)ethenyl]benzene","63551-09-7","D",0]
["Ethyl 3,3,4,4-tetrafluorobutanoate","106693-03-2","D",0]
["1-Bromoperfluoroundecane","172155-03-2","D",0]
["Tecarfarin sodium","1004551-83-0","D",0]
["3,6,9,12,15,18,21,24,27,30-Decaoxatetratriacont-1-yl [(perfluorooctyl)sulfonyl]carbamate","64309-62-2","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-propoxyhexane","1193009-98-1","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.'-[sulfonylbis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-","65530-76-9","D",0]
["1-(Nitroethenyl)perfluorobutane","306935-66-0","D",0]
["10-H-Perfluorodecanoic acid","112823-28-6","D",0]
["6-(Heptafluoropropyl)pyridin-3-amine","317810-57-4","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-N-(2-hydroxyethyl)propanamide","137506-19-5","D",0]
["2'-Deoxy-5-(nonafluorobutyl)uridine","58671-35-5","D",0]
["1,1,2,3,3,3-Hexafluoro-2-iodopropyl sulfurofluoridate","77570-01-5","D",0]
["1,4-Bis(heptadecafluorooctyl)benzene","132877-69-1","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropane-2-sulfonyl)benzoic acid","88489-82-1","D",0]
["2,3,3,5,5-Pentakis(trifluoromethyl)-1,4,2-dioxazolidine","63527-91-3","D",0]
["Ethyl 3-[4-(dimethylamino)phenyl]-2-(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)prop-2-enoate","75988-12-4","D",0]
["5,5,6,6,6-Pentafluorohex-1-ene","106128-16-9","D",0]
["S-[3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butyl] ethanethioate","1097631-01-0","D",0]
["4,4,4-trifluoro-1-phenyl-3-(trifluoromethyl)but-2-en-1-one","35443-84-6","D",0]
["Surflon S 113  (perfluoroalkylcarboxylate)","76199-70-7","D",0]
["N'-(3-Acetyl-4-{3-[tert-butyl(heptafluoropropyl)amino]-2-hydroxypropoxy}phenyl)-N,N-diethylcarbamimidic acid--hydrogen iodide (1/1)","149825-34-3","D",0]
["Propane, chloropentafluoro-","134237-41-5","D",0]
["2-Chloro-1-(2-chloro-1,1-difluoroethoxy)-1,1-difluoroethane","38217-12-8","D",0]
["Tetrafluorosuccinonitrile","663-41-2","D",0]
["1,1,1,2,2-Pentafluoro-6-methylheptane-3,5-dione","2355-62-6","D",0]
["PROPANE, 1,1-DICHLORO-2,2,3,3-TETRAFLUOR","4071-01-6","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexanal","135984-67-7","D",0]
["3-(Butylsulfanyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-07-2","D",0]
["2-(Trimethoxysilyl)ethyl heptadecafluorononanoate","85857-19-8","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl nonafluorobutane-1-sulfonate","924894-08-6","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoropentane","158118-01-5","D",0]
["2-Fluoro-4,6-bis(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-1,3,5-triazine","10271-36-0","D",0]
["2-Chloro-6-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)aniline","1630969-89-9","D",0]
["N-(2-Carboxyethyl)-3-[(2-carboxyethyl)[(perfluoropropyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","1513864-24-8","D",0]
["6-(Nonafluorobutyl)-2-phenylpyrimidin-4(3H)-one","180748-44-1","D",0]
["2-Chloro-4-methoxyphenyl nonafluorobutane-1-sulfonate","1131890-97-5","D",0]
["2-Oxetanone, 4,4-bis(trifluoromethyl)-","1718-33-8","D",0]
["3-(4-Chlorophenyl)-6-(pentafluoroethyl)-1,4-dihydro-1,2,4,5-tetrazine","59872-88-7","D",0]
["(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)acetonitrile","75988-02-2","D",0]
["3-(Nonafluorobutyl)-5-phenyl-1H-pyrazole","204130-95-0","D",0]
["6-[(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptyl)oxy]-1,3,5-triazine-2,4-diamine","57338-65-5","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with methacrylic anhydride","161308-19-6","D",0]
["Bis-(1H,1H,7H-perfluoroheptyl) (1S,3R)-camphorate","2355-57-9","D",0]
["2,2,3,3,3-Pentafluoropropanoyl nitrite","664-16-4","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluoroheptanamide","130043-47-9","D",0]
["4,4'-(3,3,4,4-Tetrafluorocyclobut-1-ene-1,2-diyl)dianiline","169381-04-8","D",0]
["1H,1H,2H,2H-Perfluorohexyl bromide","38436-14-5","D",0]
["Nonanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[9-chloro-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro- (9CI)","548455-85-2","D",0]
["11-(Perfluorooctyl)undecyl methacrylate","3794-51-2","D",0]
["Bis(perfluoroheptyl) phosphinic acid","158986-67-5","D",0]
["2-Nitro-4-[(2,2,3,3-tetrafluoropropyl)sulfanyl]aniline","54058-62-7","D",0]
["1,1,1,3,3,3-Hexafluoro-2-{[fluoro(~2~H_2_)methyl]oxy}(~2~H)propane","1173021-96-9","D",0]
["(2Z)-3,4,4,5,5,6,6,7,7,8,8,9,9,9-Tetradecafluoro-2-iodonon-2-en-1-ol","1211961-38-4","D",0]
["2-Phenyl-4,4-bis(trifluoromethyl)quinazolin-1(4H)-ol","62457-67-4","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoroheptyl carbonochloridate","821806-42-2","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl Iodide","200112-75-0","D",0]
["bis(2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-1-oxopropyl)peroxide","56347-79-6","D",0]
["2-Propenoic acid, polymers, 2-methyl-, polymer with 2-(diethylamino)ethyl 2-methyl-2-propenoate, 2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate","1071022-25-7","D",0]
["3-({3-[(2-Hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoropentyl)sulfonyl]amino)-1-propanesulfonate","2089108-95-0","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-(1-carboxy-1,2,2,2-tetrafluoroethyl)-ω-[tetrafluoro(trifluoromethyl)ethoxy]-, ammonium salt (1:1)","83606-67-1","D",0]
["1(Perfluoroethyl)2-(perfluoropentyl)ethene","935477-04-6","D",0]
["Sulfonium, (thiodi-4,1-phenylene)bis[diphenyl-, (OC-6-11)-hexafluoroantimonate(1-) (1:2), mixt. with diphenyl[4-(phenylthio)phenyl]sulfonium (OC-6-11)-hexafluoroantimonate(1-) (1:1)","159120-95-3","D",0]
["1,3-Oxathiolane-4-acetic acid, 5-oxo-2,2-bis(trifluoromethyl)-","170996-97-1","D",0]
["Hexanediamide, 2,2,3,3,4,4,5,5-octafluoro-N1,N6-bis[4-(2-phenyldiazenyl)phenyl]-","547746-38-3","D",0]
["1-Chloro-8-iodoperfluorooctane","16486-98-9","D",0]
["2-Bromo-3,3,3-trifluoro-2-(trifluoromethyl)propanoyl bromide","677-79-2","D",0]
["Trichloro[4-(perfluorooctyl)phenyl]silane","753025-21-7","D",0]
["Phosphonic acid, [3-[ethyl[(heptadecafluorooctyl)sulfonyl]amino]propyl]-, diethyl ester","71463-80-4","D",0]
["{4-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl)oxy]-5-methoxy-2-nitrophenyl}methanol","853929-03-0","D",0]
["5,5,6,6,7,7,7-Heptafluoro-3-heptene","355-98-6","D",0]
["1-Butanesulfonamide, 1,1,2,2,3,3,4,4,4-nonafluoro-, ammonium salt (1:1)","131003-86-6","D",0]
["3-(1-Hydroxy-2,2,2-trifluoro-1-(trifluoromethyl)ethyl)-2,4-pentanedione","15700-73-9","D",0]
["Perfluoroethane-1-sulfinic acid","344324-36-3","D",0]
["2,6-Difluoro-N-((2-methyl-4-(1,1,2,2-tetrafluoroethylsulfanyl)phenyl)carbamoyl)benzamide","100279-02-5","D",0]
["3-(Pentafluoroethoxy)prop-1-ene","140899-22-5","D",0]
["N-(Pentafluoroethyl)-N-(trifluoromethyl)hypofluorous amide","680-19-3","D",0]
["Copolymer of perfluoro2-(1-methyl-2-vinyloxyethoxy)ethanesulfonyl fluoride and tetrafluoroethene","70073-44-8","D",0]
["bis(perfluorooctanoyl) peroxide","34434-27-0","D",0]
["Perfluorodecane amido amine oxide","70674-76-9","D",0]
["1h,1h-perfluorohexyl p-toluenesulfonate","355-77-1","D",0]
["5-[(2,2,3,3,4,4,4-Heptafluorobutoxy)methyl]-2,4(1H,3H)-pyrimidinedione","59727-25-2","D",0]
["4-[(Perfluorooctyl)oxy]benzenesulfonic acid sodium","124206-97-9","D",0]
["Bis[tetrafluoro-1-oxo-2-[(tridecafluorohexyl)oxy]propyl]peroxide","149264-55-1","D",0]
["4,4,4-Trifluoro-1-(thiophen-2-yl)-3-(trifluoromethyl)but-2-en-1-ol","100482-55-1","D",0]
["2,2,3,3-Tetrafluoropropyl 2,2,2-trifluoroethyl carbonate","1791423-48-7","D",0]
["1,1,1,2,2,3,3,5,5,5-Decafluoro-4-nitroso-4-(trifluoromethyl)pentane","67728-23-8","D",0]
["Butyl perfluorononanoate","117374-31-9","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, N-[3-(trimethoxysilyl)propyl]carbamates","1638852-33-1","D",0]
["4-(Heptafluoroisopropyl)toluene","2396-26-1","D",0]
["N,N-Diethyl-2-(1,2,2,2-tetrafluoroethyl)-1,3-dioxan-2-amine","89752-22-7","D",0]
["2-Iodo-1,1,2,2-tetrafluoroethyl chlorosulfate","192569-10-1","D",0]
["2-Hydroxy-N,N,N-trimethyl-3-[(perfluorobutyl)ethylthio]-1-propanaminium","1513864-16-8","D",0]
["Bis(1,1-dihydroperfluorobutyl) fumarate","24120-17-0","D",0]
["1,10-Bis(perfluoroethyl)decane","1835251-85-8","D",0]
["2,4,6-Tribromophenyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","189575-10-8","D",0]
["1-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)pent-1-yne","63369-95-9","D",0]
["Perfluoro-1-decanesulfonamide","4262-70-8","D",0]
["2-Perfluoroheptyl-5-phenyl-1,3,4-oxadiazole","5756-55-8","D",0]
["Ethyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","76145-88-5","D",0]
["2-Chloro-1,1,1,2,3,4,4,4-octafluorobutane","71342-62-6","D",0]
["3-Pentanol, 1,1,1,2,4,5,5,5-octafluoro-2,4-bis(trifluoromethyl)-, compd. with tetrahydrofuran (1:1)","6884-92-0","D",0]
["1-Chloro-1,2,2,3,3,4,4,4-octafluoro-1-iodobutane","65975-08-8","D",0]
["1-Bromo-3-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-48-8","D",0]
["[(4,4,5,5,6,6,6-Heptafluoro-2-iodohexyl)oxy](trimethyl)silane","89608-38-8","D",0]
["1,1,2,3,4,4-Hexafluoro-1,2,3,4-tetrakis(heptafluoropropoxy)butane","54208-66-1","D",0]
["N-(Carboxymethyl)-5,5,6,6,7,7,8,8,8-nonafluoro-N,N-dimethyloctan-1-aminium","2089109-28-2","D",0]
["1,1,2,2-Tetrafluoro-1,2-dinitroethane","356-16-1","D",0]
["3-(Ethanesulfonyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-44-7","D",0]
["2,2,3-Trifluoro-3-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy](1-14C)propanoic acid","2087970-37-2","D",0]
["[6-(2,2,3,3-Tetrafluoropropoxy)pyridin-3-yl]methanol","106341-50-8","D",0]
["2-Ethyl-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctanal","61314-65-6","D",0]
["Pentadecafluoroheptyl 2-methylprop-2-enoate","96724-20-8","D",0]
["4-(2-Bromo-2,3,3,3-tetrafluoropropanamido)butanoic acid","113360-58-0","D",0]
["2,2-Dibromo-4,4,5,5-tetrafluoro-1,3-bis(trifluoromethyl)imidazolidine","91539-76-3","D",0]
["Silver(1+) (3Z)‐6,6,7,7,8,8,8‐heptafluoro‐2,2‐ dimethyl‐5‐oxooct‐3‐en‐3‐olate","76121-99-8","D",0]
["2,2,3,3,4,4,5,5,6-Nonafluoro-6-(tridecafluorohexyl)oxane","64191-44-2","D",0]
["Copolymer of 2-(methacryloyloxy)ethyl(dimethyl)ammonium acetate, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-yl methacrylate","1621858-65-8","D",0]
["(2E)-1,1,1,2,3,4,4,5,5,6,6,7,7,8,8,8-Hexadecafluorooct-2-ene","31143-13-2","D",0]
["1-Methoxy-3-(1,1,2,2-tetrafluoroethoxy)benzene","478282-30-3","D",0]
["1,1,1,2,2,4,4-Heptafluoro-4-iodobutane","1810-11-3","D",0]
["Poly-1,1-difluoroethene-co-perfluoro(3-methoxypropoxy)ethene-co-tetrafluoroethene","355015-68-8","D",0]
["2-Propenoic acid, 2-(methylamino)ethyl ester, N-[(.gamma.-.omega.-perfluoro-C8-14-alkyl)sulfonyl] derivs., reaction products with polyethylene glycol bis(thioglycolate)","72480-32-1","D",0]
["2,2,3,3,3-Pentafluoropropan-1-amine--hydrogen chloride (1/1)","374-14-1","D",0]
["Methoxydimethyl(3,3,4,4,5,5,5-heptafluoropentyl)silane","608298-96-0","D",0]
["3,3,4,4,5,6,6,6-Octafluoro-5-(trifluoromethyl)hex-1-ene","139060-76-7","D",0]
["2-[(Heptadecafluorooctyl)sulfonyl]ethyl 2-propenoate","124576-86-9","D",0]
["Butanamide, N,N'-(1,1'-biphenyl)-4,4'-diylbis(2,2,3,3,4,4,4-heptafluoro-","75042-07-8","D",0]
["1,1,1,2,2,3,3-Heptafluoro-4,4-bis(trifluoromethyl)hexane","100646-00-2","D",0]
["Ethyl (2E)-2-[(S)-perfluorobutylsulfinylimino]acetate","1612778-42-3","D",0]
["1-Chloro-1,2,3,3,3-pentafluoroprop-1-ene","2804-49-1","D",0]
["1-Bromo-2-(2,2,3,3,4,4,4-heptafluoro-butoxy)-benzene","1365808-29-2","D",0]
["(2E)‐4,4,5,5,6,6,7,7,8,8,8‐Undecafluorooct‐2‐enoic  acid","875878-70-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluorooctane","1645298-12-9","D",0]
["1,1,1-Trifluoro-4-methyl-2-(trifluoromethyl)pent-4-en-2-ol","665-05-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18-tetratriacontafluorooctadecanoic acid","2274731-02-9","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)di(propan-2-yl)silane","356056-13-8","D",0]
["15H-Perfluoropentadecanoic acid","1895-14-3","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-iodopropyl)-","68379-37-3","D",0]
["bis(2,2,3,3,4,4,5,5-octafluoropentyl) benzene-1,2-dicarboxylate","572-94-1","D",0]
["3-Hydroxy-4-methyl-5,5-bis(trifluoromethyl)furan-2(5H)-one","825630-89-5","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, methacrylates","721399-22-0","D",0]
["2,2,3,3-Tetrafluoro-3-iodopropanenitrile","99643-24-0","D",0]
["Poly(difluoromethylene), .alpha.,.omega.-diethenyl-","402574-89-4","D",0]
["Pentapotassium 6,9,12-tris(carboxylatomethyl)-3-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)-3,6,9,12,15-pentaazaheptadecane-1,17-dioate","155286-99-0","D",0]
["5-(Heptafluoropropyl)-2-sulfanylidene-2,3-dihydropyrimidin-4(1H)-one","145663-11-2","D",0]
["N‐Propyl‐N‐[2‐(2‐{2‐[2‐(N‐propyl-perfluorooctanesulfonamido)ethoxy]ethoxy}ethoxy)ethyl]perfluorooctane‐1‐sulfonamide","86279-54-1","D",0]
["3-[(Nonafluorobutyl)sulfanyl]propan-1-ol","875628-33-4","D",0]
["1,2,4-Triazolo(4,3-b)pyridazine, 8-(p-fluorophenyl)-6-(pentafluoroethyl)-","73673-81-1","D",0]
["3,3,3-Trifluoro-2,2-bis(trifluoromethyl)propanoic acid","917951-63-4","D",0]
["3,4,4,5,5,6,6,6-Octafluoro-N,N-dimethylhex-2-en-1-amine","90292-36-7","D",0]
["Stannane, chlorotris(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-","181625-76-3","D",0]
["3-(1,1,2,3,3,3-Hexafluoropropyl)cyclohex-1-ene","57915-75-0","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethoxy)-2-(trifluoromethyl)propane","681-08-3","D",0]
["N,N'-bis(Perfluorobutanoyl)1,4-butanediamine","2967-59-1","D",0]
["1,1,1,2-Tetrafluoro-2-(fluoromethoxy)ethane","56885-27-9","D",0]
["1-Hydroxy-6:2 fluorotelomer sulfonic acid","2089110-01-8","D",0]
["1-Propanaminium, 3-[(carboxymethyl)[(1,1,2,2,3,3,3-heptafluoropropyl)sulfonyl]amino]-N,N-dimethyl-N-(3-sulfopropyl)-","2089109-79-3","D",0]
["4-Heptanone, 2,6-bis(trifluoromethyl)-2,6-dihydroxy-1,1,1,7,7,7-hexafluoro-, phenylhydrazone","101913-90-0","D",0]
["2,6-Dibromo-3,5-difluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridine","259875-80-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorohentriacontane","264229-79-0","D",0]
["Cyclopentanone, 2,5-bis(2,2,3,3,4,4,5,5,5-nonafluoro-1-oxopentyl)-","672956-74-0","D",0]
["2Z-1-(Methoxy-1-fluoropropenyl)perfluoropropane","90292-38-9","D",0]
["9H-Perfluorodecanesulfonic acid","2089109-60-2","D",0]
["Methyl 3,3,4,4-tetrafluoro-2-oxobutanoate","74067-13-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-[(prop-2-yn-1-yl)oxy]octane","1334419-24-7","D",0]
["1,1,1,3,5,5,6,6,7,7,7-Undecafluoro-2,4-bis(trifluoromethyl)hept-3-ene","500339-30-0","D",0]
["Pentafluoro(prop-1-en-1-yl)cyclopropane","499784-17-7","D",0]
["Potassium 2,2,3-trifluoro-3-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy](1-14-C)propanoate","2087970-38-3","D",0]
["2-Chloro-4-(2-chloro-1,1,2,2-tetrafluoroethoxy)phenol","89227-91-8","D",0]
["3-[[(Perfluorohexyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium chloride, sodium salt (1:1:1)","148026-38-4","D",0]
["1-(Pentafluoroethyl)naphthalene","117081-47-7","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoropentanal hydrate (1:1)","907607-08-3","D",0]
["2,3-difluoro-2-(tridecafluorohexyl)oxirane","1350637-14-7","D",0]
["Sodium 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9‐hexadecafluorononyl sulfate","29811-17-4","D",0]
["4-(Perfluorobutyl)-3,3-difluorobutanesulfonyl chloride","1225375-54-1","D",0]
["Nonadecafluorononan-1-ol","85758-72-1","D",0]
["2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Hexadecafluorononanenitrile","376-26-1","D",0]
["1,1-Dibromo-1,2,2,3,3,4,4,4-octafluorobutane","73533-18-3","D",0]
["1,2,3,4,5-Pentafluoro-6-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzene","17480-16-9","D",0]
["1,1,2,2-Tetrafluoropropan-1-ol","28106-65-2","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-1-phenylnonane-1,3-dione","99338-16-6","D",0]
["3-[(2-Carboxyethyl)[(perfluoro-1-sulfonyltridecyl)amino]-N-(carboxymethyl)-N,N-dimethyl- 1-propanaminium","2089109-20-4","D",0]
["Imidazolidine, 2-heptafluoropropyl-","31185-53-2","D",0]
["1,1,2,2,3,3-Hexafluorocyclobutane","55101-70-7","D",0]
["5,5,5-Trifluoro-4-(methoxymethoxy)-4-(trifluoromethyl)pent-1-ene","150669-66-2","D",0]
["3-(2-Chloro-4-fluorobenzamido)-2-fluoro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","862133-15-1","D",0]
["2,2-Dichloro-4,4,5,5-tetrafluoro-1,3-bis(trifluoromethyl)imidazolidine","91584-67-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluorononacosane","1980053-42-6","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], α-(3,3,4,4,5,5,6,6,7,7,8,8, 9,9,10,10,10-heptadecafluorodecyl)-ω-hydroxy-","58285-35-1","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(1,1,2,2-tetrafluoro-2-iodoethoxy)propane","81747-61-7","D",0]
["Propyl 2,2,3,3-tetrafluoropropyl carbonate","879496-52-3","D",0]
["2,2-Dichlorotrifluoroethyl 1,1,3-trichlorotetrafluoropropyl ether","61196-11-0","D",0]
["1-bromo-1h,1h,2h,2h-perfluorooctane","161583-34-2","D",0]
["3:3 Fluorotelomer carboxylic acid","356-02-5","D",0]
["5,5-Bis(trifluoromethyl)-4,5-dihydro-1H-pyrazole-4-carbonitrile","61859-92-5","D",0]
["2-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)-1,2,3,4-tetrahydronaphthalen-1-ol","34844-43-4","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide, chloroacetyl chloride and pyridine","162492-12-8","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1,6-hexanediamine","355-73-7","D",0]
["N,N,N-Tributyl-1-butanaminium 2-{2-[3,3-bis(trifluoromethyl)-1λ3,2-benziodoxol-1(3H)-yl]phenyl}-1,1,1,3,3,3-hexafluoro-2-propanolate","80559-53-1","D",0]
["Perfluorotetracosane","1766-41-2","D",0]
["3-Amino-3-[4-(1,1,2,2-tetrafluoroethoxy)phenyl]propanoic acid","773122-82-0","D",0]
["1,3-Propanediamine, N,N-dimethyl-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (2:1)","65530-79-2","D",0]
["Fatty acids, C18-unsatd., trimers, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl esters","148240-78-2","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.'-(thiodi-2,1-ethanediyl)bis[.omega.-fluoro-","65530-73-6","D",0]
["5-(Henicosafluorodecyl)-1H-imidazole","81769-57-5","D",0]
["1,1-Difluoro-1-(trifluoromethoxy)ethane","69948-27-2","D",0]
["3-(2,2,3,3,4,4,4-Heptafluorobutylidene)dihydro-2(3H)-furanone","89608-45-7","D",0]
["Perfluoro(4-isopropyltoluene)","20017-49-6","D",0]
["2,2,3,3,4,4-Hexafluoro-4-(heptafluoropropoxy)butanoic acid","1010786-64-7","D",0]
["2,2,3,3,4,4,5,5,6-Nonafluoro-6-iodooxane","827601-56-9","D",0]
["Ethyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-2-oxooctanoate","117516-21-9","D",0]
["5-(Pentafluoroethyl)-1,2-oxazol-3-amine","110234-44-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-Tricosafluoroheptacosane","1980054-34-9","D",0]
["4-Methyl-1,1,1-trifluoro-2-(trifluoromethyl)-2,4-pentanediol","101931-57-1","D",0]
["[(Tridecafluorohexyl)oxy]acetic acid","759414-86-3","D",0]
["Perfluoro-2,3-bis[2-(fluorosulfonyl)ethoxy]propanoyl fluoride","921204-31-1","D",0]
["1-(1-Azepanyl)-3-azido-2,2,3,3-tetrafluoro-1-propanone","1242614-42-1","D",0]
["Perfluoro(2,5,8,10-tetramethyl-3,6,9-trioxaundecanoic) acid","1212077-14-9","D",0]
["Perfluorodecahydro-1-isobutylnaphthalene","118945-65-6","D",0]
["1,1'-[Peroxybis(carbonyloxy)]bis(2,2,3,3,4,4,5,5-octafluoropentane)","188715-78-8","D",0]
["1,3-Dibromo-1,1,2,2,3,3-hexafluoropropane","4259-29-4","D",0]
["1,1,2,2,3,3,4,4,5-Nonafluoro-5-(pentafluoroethyl)-6,6-bis(trifluoromethyl)cyclohexane","144898-38-4","D",0]
["1-Bromo-3-(heptadecafluorooctyl)benzene","325459-90-3","D",0]
["2,2,3,3-Tetrafluorobutyl carbonate","156783-98-1","D",0]
["1,1,1-Trichloro-3,3,4,4,4-pentafluorobutan-2-one","87375-47-1","D",0]
["6,6,7,7,8,8,8-Heptafluoro-5,5-bis(trifluoromethyl)-1,3-octadiene","1429188-77-1","D",0]
["4,4,4-Trifluoro-3-hydroxy-1-{4-[4,4,4-trifluoro-1,3-dihydroxy-3-(trifluoromethyl)butyl]phenyl}-3-(trifluoromethyl)butan-1-one","101247-78-3","D",0]
["Octyl 2,2,3,3,3-pentafluoropropanoate","1867-95-4","D",0]
["1,1-bis(Trifluoromethyl)ethane","382-09-2","D",0]
["3-[[(Perfluoropropyl)sulfonyl]amino]propanesulfonic acid","2089108-61-0","D",0]
["Ethane,1-bromo-1,1,2,2-tetrafluoro-","354-07-4","D",0]
["1,1,3,3,4,5,6,7-Octafluoro-1,3-dihydro-2-benzofuran","122180-11-4","D",0]
["1,1,2,3,4,4,5,5,5-Nonafluoropent-2-ene","935476-71-4","D",0]
["4,4'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)di(benzene-1-thiol)","93129-79-4","D",0]
["(1s,4s)-4-(Heptafluoropropyl)cyclohexane-1-carboxamide","88951-18-2","D",0]
["N-(2-Hydroxyethyl)-4-[(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-en-1-yl)oxy]benzamide","144770-79-6","D",0]
["2‐{[2‐(Acetyloxy)‐3-(perfluorododecyl)propyl]dimethylazaniumyl}acetate","80244-67-3","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentyl 4-hydroxybenzoate","118841-84-2","D",0]
["Nonafluoromorpholine","378-94-9","D",0]
["N-[(Chlorocarbonyl)oxy]-2,2,3,3,4,4,4-heptafluorobutanimidamide","4368-74-5","D",0]
["1-Hexadecylpyridinium perfluoro-1-octanesulfonate","334529-63-4","D",0]
["2-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)propane-1,3-diol","25664-42-0","D",0]
["Sodium 2,2,3,3,4,4,5,5,6,6,7,7‐dodecafluoroheptyl  sulfate","29811-16-3","D",0]
["3-(Perfluorobutyl)propanoic acid","80705-13-1","D",0]
["(3,3,4,5,5,5-Hexafluoro-2,2-dimethylpentyl)benzene","89185-59-1","D",0]
["1,1'-(Piperazine-1,4-diyl)bis(heptafluorobutan-1-one)","120219-50-3","D",0]
["naphthalen-1-yl 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","32848-17-2","D",0]
["Imidazole perfluoropropionic acid salt","200705-90-4","D",0]
["1,3-Dichloro-1,1,3,4,4,4-hexafluorobutan-2-one","143425-67-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Nonadecafluoroheptacosane","117948-74-0","D",0]
["Bis(2,2,3,3,4,4,5,5-octafluoropentyl) bis{tris[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]silyl} orthosilicate","94048-09-6","D",0]
["Nonafluoro(nitroso)cyclopentane","91816-92-1","D",0]
["D-Galactose 6-(sodium 1-(perfluorooctyl)-3-dodecyl phosphate)","147684-10-4","D",0]
["2-Chloroperfluorohexane","1426-23-9","D",0]
["Perfluoro[1,2-13C2]dodecanoic acid","960315-52-0","D",0]
["1-[Bis(2-hydroxyethyl)amino]-4,4,5,5,6,6,6-heptafluorohexan-2-ol","189160-58-5","D",0]
["Phosphonium, tributyl(2-methoxypropyl)-, salt with 4,4'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis[phenol] (1:1)","126049-00-1","D",0]
["1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Hexacosafluorotridec-1-ene","66325-97-1","D",0]
["2,3,3,3-Tetrafluoro-N,N-dimethylprop-1-en-1-amine","41874-82-2","D",0]
["3,3,4,4-tetrafluorooxolane","374-33-4","D",0]
["Trimethoxy(pentadecafluoroheptyl)silane","84464-06-2","D",0]
["3-Methyl-4-(methylsulfanyl)phenyl pentafluoroethane-1-sulfonate","57728-77-5","D",0]
["3-Ethenyl-1,2,2-trifluoro-1-(trifluoromethyl)cyclobutane","925686-63-1","D",0]
["6-fluoro-2-(pentafluoroethyl)-1h-benzimidazole","5847-95-0","D",0]
["Ethane, 1,1,1,2-tetrafluoro-2-methoxy-, (S)-","156700-89-9","D",0]
["1,1,1,3,5,7,7-Heptachloro-2,2,3,4,4,5,6,6,7-nonafluoroheptane","53281-02-0","D",0]
["(1r,4r)-4-(Heptafluoropropyl)cyclohexane-1-carboxylic acid","88951-23-9","D",0]
["1,1,2,2,8,8,9,9-Octafluorononane-3,5,7-trione","425639-05-0","D",0]
["2-(Heptafluoropropyl)-1H-indole","123825-50-3","D",0]
["N-[4-(Nonafluorobutoxy)phenyl]pyridine-4-carboxamide--hydrogen chloride (1/1)","62315-29-1","D",0]
["1H,6H-Perfluorohexane","336-07-2","D",0]
["3-Chloro-4-(pentafluoroethyl)pyridine","1816286-90-4","D",0]
["4H-Perfluorobutanoic acid","679-12-9","D",0]
["1H,1H,2H-Perfluoro(4,7,10,13,16-pentamethyl-5,8,11,14,17-pentaoxaeicos-1-ene)","1212247-15-8","D",0]
["N'-{[4-(Dimethylamino)phenyl]methylidene}-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptanehydrazide","328016-16-6","D",0]
["3-[Hexyl[(perfluorododecyl)sulfonyl]amino]-2-hydroxypropyl hexatriacontanoate","141187-89-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-[(methylamino)methyl]propan-2-ol","380609-21-2","D",0]
["N-Benzoyl-3'-O-[(R)-(2-cyanoethoxy)(diisopropylamino)phosphino]-2'-deoxy-5'-O-{[4-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)phenyl][bis(4-methoxyphenyl)]methyl}adenosine","865758-44-7","D",0]
["Trimethylsilyl heptadecafluorononanoate","1244856-06-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-Nonacosafluorotriacontane","1228093-93-3","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(2-methylpropane-2-sulfinyl)benzoic acid","1355554-39-0","D",0]
["(1E)-3,4,4,4-Tetrafluoro-1-iodo-3-(trifluoromethyl)but-1-ene","24716-84-5","D",0]
["2,2-Dichlorotrifluoroethyl chlorodifluoromethyl ether","37136-24-6","D",0]
["perfluoro[2-(2-methoxypropoxy)propanoic acid]ammonium","510774-77-3","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)propanethioyl fluoride","62619-35-6","D",0]
["Allylperfluorobutanamide","24429-61-6","D",0]
["1,2-Ethanediyl bis(perfluorobutanesulfonate)","92982-03-1","D",0]
["2-(Heptafluoropropyl)-1,4-dimethoxybenzene","80790-98-3","D",0]
["Perfluorocarbons","308069-13-8","D",0]
["2-(Perfluorovinyloxy)perfluoroethanesulfonic acid sodium salt","26953-98-0","D",0]
["N-Methyl-4-[3,4,4,4-tetrafluoro-3-(trifluoromethyl)butane-1-sulfonyl]butan-1-amine","1353009-38-7","D",0]
["1,1,2,2,2-Pentafluoro-N,N-bis(trifluoromethyl)ethan-1-amine","815-28-1","D",0]
["Bis(2,2,3,3,4,4,4-heptafluorobutyl) phenylphosphonate","31430-72-5","D",0]
["2,2,3,3-Tetrafluoro-3-(1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy)propanoic acid","1071906-96-1","D",0]
["{[(2,2,3,3,4,4,4-Heptafluorobutyl)sulfanyl]methyl}benzene","200337-06-0","D",0]
["1-Chloro-1,1,3,3,4,4,4-heptafluorobutan-2-one","87375-46-0","D",0]
["2-(Heptafluoropropyl)cyclohexan-1-one","61282-91-5","D",0]
["1,1,1,3,3,5,5,7,7,9,9-Undecafluoro-2,4,6,8-tetraoxadecan-10-oyl fluoride","21703-47-9","D",0]
["1,1,2,2-Tetrafluoro-7-methyl-2,3-dihydro-1H-indene","922141-55-7","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorooctadecane","133310-68-6","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1-(pentafluoroethyl)pyrrolidine","78159-15-6","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]propoxy]-propanoic acid methyl ester","133609-46-8","D",0]
["1H,1H-Perfluorohexadecan-1-ol","216144-94-4","D",0]
["Ethyl 3-amino-4,4,5,5,5-pentafluoropent-2-enoate","72850-56-7","D",0]
["(S)-Perfluorobutanesulfinamide","1303994-31-1","D",0]
["1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexahydro-2,2,4,4,6,6-hexakis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8-tetradecafluorooctyl)oxy]-","186406-49-5","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,9,9,9-Heptadecafluorononyl 2-methylprop-2-enoate","140838-93-3","D",0]
["doravirine","1338225-97-0","D",0]
["PHENETHYLAMINE, N-ETHYL-alpha-METHYL-m-T","3239-44-9","D",0]
["cinacalcet","226256-56-0","D",0]
["1H-Indeno[5,4-f]quinoline-7-carboxamide, N-[2,5-bis(trifluoromethyl)phenyl]-2,4a,4b,5,6,6a,7,8,9,9a,9b,10,11,11a-tetradecahydro-4a,6a-dimethyl-2-oxo-, (4aR,4bS,6aS,7S,9aS,9bS,11aR)-","164656-23-9","D",0]
["2H-3,1-Benzoxazin-2-one, 6-chloro-4-(2-cyclopropylethynyl)-1,4-dihydro-4-(trifluoromethyl)-, (4S)-","154598-52-4","D",0]
["elexacaftor","2216712-66-0","D",0]
["Benzenesulfonamide, 4-[5-(4-methylphenyl)-3-(trifluoromethyl)-1H-pyrazol-1-yl]-","169590-42-5","D",0]
["cangrelor","163706-06-7","D",0]
["lomitapide","182431-12-5","D",0]
["voxilaprevir","1535212-07-7","D",0]
["vinflunine","162652-95-1","D",0]
["upadacitinib","1310726-60-3","D",0]
["enzalutamide","915087-33-1","D",0]
["fenfluramine","458-24-2","D",0]
["flecainide","54143-55-4","D",0]
["Benzenepropanamine, N-methyl-γ-[4-(trifluoromethyl)phenoxy]-","54910-89-3","D",0]
["3-Pyridinecarboxylic acid, 2-[[2-methyl-3-(trifluoromethyl)phenyl]amino]-","38677-85-9","D",0]
["fluphenazine","69-23-8","D",0]
["(1E)-5-Methoxy-1-[4-(trifluoromethyl)phenyl]-1-pentanone O-(2-aminoethyl)oxime","54739-18-3","D",0]
["fosaprepitant","172673-20-0","D",0]
["fosnetupitant","1703748-89-3","D",0]
["gemcitabine","95058-81-4","D",0]
["glecaprevir","1365970-03-1","D",0]
["ivosidenib","1448347-49-6","D",0]
["trifluoperazine","117-89-5","D",0]
["Ethanone, 1-(4-(4-(5-(2,6-difluorophenyl)-4,5-dihydro-3-isoxazolyl)-2-thiazolyl)-1-piperidinyl)-2-(5-methyl-3-(trifluoromethyl)-1H-pyrazol-1-yl)-","1003318-67-9","D",0]
["(2RS)-2-[4-(4-chloro­phenoxy)-2-(trifluoromethyl)phenyl]-1-(1H- 1,2,4-triazol-1-yl)propan-2-ol; mefentrifluconazole","1417782-03-6","D",0]
["Cyclopropanecarboxylic acid, 3-((1Z)-2-chloro-3,3,3-trifluoro-1-propenyl)-2,2-dimethyl-, (2-methyl(1,1'-biphenyl)-3-yl)methyl ester, (1R,3R)-rel-","82657-04-3","D",0]
["Bicalutamide","90357-06-5","D",0]
["maraviroc","376348-65-1","D",0]
["mefloquine","53230-10-7","D",0]
["netupitant","290297-26-6","D",0]
["N-[3-[3-(1H-imidazolyl)propoxy]phenyl]-4-methyl-3-[[4-(3-pyridinyl)-2-pyrimidinyl]amino]benzamide","641571-10-0","D",0]
["nilutamide","63612-50-0","D",0]
["nitisinone","104206-65-7","D",0]
["penfluridol","26864-56-2","D",0]
["ponatinib","943319-70-8","D",0]
["regorafenib","755037-03-7","D",0]
["rolapitant","552292-08-7","D",0]
["1H-Indole-7-carboxamide, 2,3-dihydro-1-(3-hydroxypropyl)-5-[(2R)-2-[[2-[2-(2,2,2-trifluoroethoxy)phenoxy]ethyl]amino]propyl]-","160970-54-7","D",0]
["siponimod","1230487-00-9","D",0]
["7-[(3R)-3-amino-1-oxo-4-(2,4,5-trifluorophenyl)buyl]-5,6,7,8-tetrahydro-3-trifluoromethyl)-1,4-triazolo[4,3-a]","486460-32-6","D",0]
["4-(4-((((4-CHLORO-3-(TRIFLUOROMETHYL)PHENYL)AMINO)CARBONYL)AMINO)PHENOXY)-N-METHYL-2-PYRIDINECARBOXAMIDE","284461-73-0","D",0]
["tafluprost","209860-87-7","D",0]
["telotristat","1033805-22-9","D",0]
["teriflunomide","163451-81-8","D",0]
["tezacaftor","1152311-62-0","D",0]
["tipranavir","174484-41-4","D",0]
["5-Heptenoic acid, 7-[(1R,2R,3R,5S)-3,5-dihydroxy-2-[(1E,3R)-3-hydroxy-4-[3-(trifluoromethyl)phenoxy]-1-buten-1-yl]cyclopentyl]-, 1-methylethyl ester, (5Z)-","157283-68-6","D",0]
["1H-Benzimidazole, 2-[[[3-methyl-4-(2,2,2-trifluoroethoxy)-2-pyridinyl]methyl]sulfinyl]-","103577-45-3","D",0]
["Polyfluorinated alkyl halide.","","D",0]
["Polyfluorinated alkyl polyamide.","","D",0]
["Perfluoroalkylsulfonamide salt (PROVISIONAL).","","D",0]
["Perfluoroalkyl acrylate copolymer (PROVISIONAL).","","D",0]
["Perfluoroalkyl acrylate copolymer latex (PROVISIONAL).","","D",0]
["Perfluoroalkyl ethanol and methyl alcohol adducts of toluene diisocyanate.","","D",0]
["Perfluoroalkyl ethylacrylate oligomer (PROVISIONAL).","","D",0]
["Perfluoroalkyl ethylmethacrylate copolymer - TSCA Accession Number 248567","","D",0]
["Perfluoroalkyl polyether (PROVISIONAL).","","D",0]
["Perfluoroalkyl substituted alkyl sulfonate.","","D",0]
["Perfluoroalkyl acrylate (PROVISIONAL).","","D",0]
["Perfluoroalkylacrylate copolymer (PROVISIONAL).","","D",0]
["Perfluoroalkylacrylate copolymer (PROVISIONAL).- TSCA Accession Number 158022","","D",0]
["Perfluoroalkylacrylate copolymer (PROVISIONAL).- TSCA Accession Number 164148","","D",0]
["Perfluoroalkylated polyamino acid (PROVISIONAL).","","D",0]
["Perfluoroalkylethyl acrylate copolymer (PROVISIONAL).","","D",0]
["Perfluoroalkylethyl amine (PROVISIONAL).","","D",0]
["Perfluoroalkylethyl ester (PROVISIONAL).- TSCA Accession Number 144582","","D",0]
["Perfluoroalkylethyl ester (PROVISIONAL).- TSCA Accession Number 169347","","D",0]
["Perfluoroalkylethyl methacrylate copolymer (PROVISIONAL).","","D",0]
["Perfluoroalkylethyl methacrylate copolymer, salt (PROVISIONAL).","","D",0]
["Perfluoroalkylethylacrylate copolymer (PROVISIONAL) - TSCA Accession Number 135058","","D",0]
["Perfluoroalkylethylacrylate copolymer (PROVISIONAL).- TSCA Accession Number 137587","","D",0]
["Perfluoroalkylethylacrylate copolymer (PROVISIONAL) - TSCA Accession Number 137667","","D",0]
["Polyfluorinated alkyl amine.","","D",0]
["4-Isoxazolecarboxamide, 5-methyl-N-[4-(trifluoromethyl)phenyl]-","75706-12-6","D",0]
["letermovir","917389-32-3","D",0]
["Perfluoroalkylsulfonamidoalkyl acrylate, polymer with acrylic acid derivatives (PROVISIONAL).","","D",0]
["Perfluorobutanesulfonamide and polyoxyalkylene containing polyurethane.","","D",0]
["Perfluoroelastomer (PROVISIONAL).- TSCA Accession Number 102659","","D",0]
["Perfluoroelastomer (PROVISIONAL).- TSCA Accession Number 102659","","D",0]
["Perfluoropolyamphiphile (PROVISIONAL).","","D",0]
["Perfluoropolyether ally ether (PROVISIONAL).","","D",0]
["Perfluoropolyether chlorosilane (PROVISIONAL).","","D",0]
["Perfluoropolyether compound (PROVISIONAL).","","D",0]
["Perfluoropolyether methoxysilane (PROVISIONAL).","","D",0]
["Perfluoropolyether modified organosilane (PROVISIONAL).","","D",0]
["Perfluoropolyether modified silane (PROVISIONAL).","","D",0]
["Perfluoropolyether-block-polytetrafluoroethylene (PROVISIONAL).","","D",0]
["PET+PTFE","","D",0]
["Basic Polymer: PFA","","D",0]
["Perfluoroethylene-propylene","","D",0]
["Phosphoric acid, mixed esters with partially fluorinated alcohol, ammonium salts (PROVISIONAL).","","D",0]
["Plastic: PI+PTFE","","D",0]
["PMMA-F","","D",0]
["Poly-.beta.-fluoroalkylethyl acrylate and alkyl acrylate (PROVISIONAL).","","D",0]
["Poly-.beta.-fluoroalkylethyl acrylate and polyoxyalkyl methacrylate (PROVISIONAL).","","D",0]
["Polyfluoralkyl ether.","","D",0]
["Metaflumizone","139968-49-3","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL).- TSCA Accession Number 274421","","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL) - TSCA Accession Number 264687","","D",0]
["Fluoroalkyl acrylate copolymer modified with polysiloxanes.- TSCA Accession Number 244441","","D",0]
["Fluorinated oligomer alcohol (PROVISIONAL).","","D",0]
["FFKO","","D",0]
["Caoutchouc: FKM","","D",0]
["Fluoralkyl acrylate copolymer.","","D",0]
["Fluorinated acrylate, polymer with alkyloxirane homopolymer monether with alkanediol mono(2-methyl-2-propenoate), tert-Bu 2-ethylhexaneperoxoate-initiated.","","D",0]
["Fluorinated acrylic alkylamino copolymer (PROVISIONAL).","","D",0]
["Fluorinated acrylic alkylamino copolymer.","","D",0]
["Fluorinated acrylic copolymer (PROVISIONAL) - TSCA Accession Number 138648","","D",0]
["Fluorinated acrylic copolymer (PROVISIONAL).- TSCA Accession Number 196704","","D",0]
["Fluorinated acrylic copolymer (PROVISIONAL) - TSCA Accession Number 255700","","D",0]
["Fluorinated acrylic copolymer (PROVISIONAL) - TSCA Accession Number 255846","","D",0]
["Fluorinated acrylic copolymer (PROVISIONAL).- TSCA Accession Number 265599","","D",0]
["Fluorinated acrylic ester copolymer (PROVISIONAL).","","D",0]
["Fluorinated acrylic ester polymer (PROVISIONAL).","","D",0]
["Fluorinated acrylic polymer with acrylate groups (PROVISIONAL).","","D",0]
["Fluorinated aliphatic isocyanate polymer (PROVISIONAL).","","D",0]
["Fluorinated alkenyl ether (PROVISIONAL).","","D",0]
["Fluorinated alkyl silane (PROVISIONAL).","","D",0]
["Fluorinated alkylsulfonamido acrylate copolymer (PROVISIONAL).","","D",0]
["Fluorinated alkylsulfonamido polymer (PROVISIONAL).","","D",0]
["Fluorinated alkylsulfonamidol urethane polymer (PROVISIONAL).","","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL).- TSCA Accession Number 264687","","D",0]
["Aromatic fluoroalkyl mixture complex.","","D",0]
["Aryl phosphonate ester of a perfluoropolyether (PROVISIONAL).","","D",0]
["Betaines, dimethyl (polyfluoro-hydro-alkyl) (PROVISIONAL).","","D",0]
["Perfluoro rubber","","D",0]
["Fluorinated organopolysilazane.","","D",0]
["Fluorinated phosphate (PROVISIONAL).","","D",0]
["Fluorinated polyalkyl alkoxy siloxanes (PROVISIONAL).","","D",0]
["Fluorinated polyalkyl silicones (PROVISIONAL).","","D",0]
["Fluorinated silane (PROVISIONAL).","","D",0]
["Fluorinated substituted urethane (PROVISIONAL).","","D",0]
["Fluorinated sulfonamide alcohol (PROVISIONAL).","","D",0]
["Fluorinated vinyl ether polymer (PROVISIONAL).","","D",0]
["Fluoro alkyl siloxane polymer (PROVISIONAL).","","D",0]
["Fluoro modified, polyether modified polyacrylate (PROVISIONAL).- TSCA Accession Number 256372","","D",0]
["Fluoro modified, polyether modified polyacrylate (PROVISIONAL).- TSCA Accession Number 262885","","D",0]
["Fluoro modified, polyether modified, and alkyl modified polymethylsiloxane (PROVISIONAL).","","D",0]
["Fluoro-modified acrylic copolymer.","","D",0]
["Fluoroacrylate copolymer (PROVISIONAL).","","D",0]
["Fluoroacrylate modified urethane (PROVISIONAL).","","D",0]
["Fluoroalkyl acrylate co-polymer (PROVISIONAL).","","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL) - TSCA Accession Number 274421","","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL).- TSCA Accession Number 235586","","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL) - TSCA Accession Number 234981","","D",0]
["Fluoroalkyl acrylate copolymer (PROVISIONAL).- TSCA Accession Number 253975","","D",0]
["Fluorinated amine oxide (PROVISIONAL).","","D",0]
["Aprepitant","170729-80-3","D",0]
["bendroflumethiazide","73-48-3","D",0]
["benfluorex","23602-78-0","D",0]
["1H-Pyrazole-3-carbonitrile, 5-amino-1-(2,6-dichloro-4-(trifluoromethyl)phenyl)-4-((trifluoromethyl)sulfinyl)-","120068-37-3","D",0]
["triflusulfuron-methyl","126535-15-7","D",0]
["trifloxystrobin","141517-21-7","D",0]
["Tefluthrin","79538-32-2","D",0]
["Pyroxsulam","422556-08-9","D",0]
["PYRIDALYL","179101-81-6","D",0]
["Picolinafen","137641-05-5","D",0]
["(RS)-N-[2-(1,3-dimethylbutyl)-3-thienyl]-1-methyl-3-(trifluoromethyl)pyrazole-4-carboxamide","183675-82-3","D",0]
["FLUOPYRAM","658066-35-4","D",0]
["flonicamid","158062-67-0","D",0]
["Flutolanil","66332-96-5","D",0]
["Flutianil(ISO); (2Z)-(]([2-fluoro-5-(trifluoromethyl)phenyl]thio)[)[3-(2-methoxyphenyl)-1,3-thiazolidin-2-ylidene]acetonitrile","958647-10-4","D",0]
["3-chloro-4-(chloromethyl)-1-[3-(trifluoromethyl)phenyl]pyrrolidin-2-one","61213-25-0","D",0]
["fluopicolide","239110-15-7","D",0]
["flazasulfuron","104040-78-0","D",0]
["Diflufenican","83164-33-4","D",0]
["Cyflumetofen","400882-07-7","D",0]
["benfluralin","1861-40-1","D",0]
["sulfoxaflor","946578-00-3","D",0]
["fluazinam","79622-59-6","D",0]
["tembotrione","335104-84-2","D",0]
["apalutamide","956104-40-8","D",0]
["Fluorinated copolymer (PROVISIONAL).","","D",0]
["Fluorinated ester.","","D",0]
["Fluorinated methacrylate monomer (PROVISIONAL).","","D",0]
["sodium trifluoroacetate","2923-18-4","D",0]
["Benzamide, N-(((4-(2-chloro-4-(trifluoromethyl)phenoxy)-2-fluorophenyl)amino)carbonyl)-2,6-difluoro-","101463-69-8","D",0]
["Benzeneacetic acid, .alpha.-(methoxymethylene)-2-[[[6-(trifluoromethyl)-2-pyridinyl]oxy]methyl]-, methyl ester, (.alpha.E)-","117428-22-5","D",0]
["Triflumizole","68694-11-1","D",0]
["prosulfuron","94125-34-5","D",0]
["Haloxyfop-P(R)-2-(](4-[3-chloro-5-(trifluoromethyl)-2-pyridyloxy]phenoxy)[)propanoic acid","95977-29-0","D",0]
["GAMMA-CYHALOTHRIN","76703-62-3","D",0]
["LAMBDA-CYHALOTHRIN","91465-08-6","D",0]
["Cyano-(3-phenoxyphenyl)methyl N-[2-chloro-4-(trifluoromethyl)phenyl]-D-valinate","102851-06-9","D",0]
["flufenacet","142459-58-3","D",0]
["(RS)-N-benzyl-2-(α,α,α,4-tetrafluoro-m-tolyoxy)butyramide","113614-08-7","D",0]
["2-(2,2-Difluoroethoxy)-N-(5,8-dimethoxy[1,2,4]triazolo[1,5-c]pyrimidin-2-yl)-6-(trifluoromethyl)benzenesulfonamide","219714-96-2","D",0]
["Cyflufenamid","180409-60-3","D",0]
["(2R)-2-(4-{[5-(trifluoromethyl)pyridin-2-yl]oxy}phenoxy)propanoic acid","83066-88-0","D",0]
["flumetralin","62924-70-3","D",0]
["Fluometuron","2164-17-2","D",0]
["Oxyfluorfen","42874-03-3","D",0]
["Chlorfenapyr","122453-73-0","D",0]
["flocoumafen","90035-08-8","D",0]
["4-Bromo-2-(4-chlorophenyl)-5-(trifluoromethyl)-1H-pyrrole-3-carbonitrile","122454-29-9","D",0]
["alpelisib","1217486-61-7","D",0]
["Perfluorinated organic peroxide (PROVISIONAL).","","D",0]
["Perfluorinated polyamine (PROVISIONAL).","","D",0]
["Perfluoro alkoxy acid fluoride derivative (PROVISIONAL).","","D",0]
["PAK+FEP+MF+PAI","","D",0]
["Modified fluoroalkyl urethane (PROVISIONAL).","","D",0]
["Modified perfluoropolyether salt (PROVISIONAL).","","D",0]
["Modified perfluoropolyoxyalkane (PROVISIONAL).","","D",0]
["Plastic: PA+PTFE","","D",0]
["Polyamide10T/X impact modified + Polytetrafluorethylene","","D",0]
["Polyamide 10T/X + Polytetrafluorethylene","","D",0]
["PA12-I+PTFE","","D",0]
["PA12+PTFE","","D",0]
["Basic Polymer: PA6+PA66-I+PTFE","","D",0]
["Polyamide6+Polyamide66+Polytetrafluorethylene","","D",0]
["Basic Polymer: PA6+PTFE","","D",0]
["Plastic: PA612+PTFE","","D",0]
["Basic Polymer: PA66+PA6+PTFE","","D",0]
["Plastic: PA66+PTFE","","D",0]
["Plastic: PA6T/66-I+PTFE","","D",0]
["Plastic: PA6T/66+PTFE","","D",0]
["Basic polymer:PA6T/XT+PTFE","","D",0]
["Plastic: Polyamide-imide + Perfluoro(ethylene-propylene)polymer + Melamine-formaldehyde copolymer + Polyacrylate","","D",0]
["Basic Polymer: PAI+FEP+PAK+MF","","D",0]
["Basic Polymer: PAI+FEP+PAK+MF","","D",0]
["Perfluorinated difunctional acid flouride (PROVISIONAL).","","D",0]
["Fluoroethylene vinyl copolymer (PROVISIONAL).","","D",0]
["Fluoroethylene-vinylether copolymer (PROVISIONAL).","","D",0]
["Fluoroolefin copolymer (PROVISIONAL).","","D",0]
["Modified fluorinated acrylic resin (PROVISIONAL).","","D",0]
["PAK+PAI+MF+FEP","","D",0]
["Plastic: Polyacrylate + Perfluoro(ethylene-propylene)polymer + Polyamide-imide + Melamine-formaldehyde copolymer","","D",0]
["Basic Polymer: PAK+MF+FEP+PAI","","D",0]
["Basic Polymer: PAK+MF+PAI+FEP","","D",0]
["Basic Polymer: PAK+PAI+FEP+MF","","D",0]
["Partially fluorinated alcohol substituted glycol (PROVISIONAL).","","D",0]
["Partially fluorinated alcohol, reaction products with phosphorus oxide (P2O5) (PROVISIONAL).","","D",0]
["Partially fluorinated alcohol, reaction products with phosphorus oxide (P2O5), amine salts.","","D",0]
["Partially fluorinated alcohol, reaction products with phosphorus oxide (P2O5), ammonium salts (PROVISIONAL).","","D",0]
["Partially fluorinated alkyl betaine (PROVISIONAL).","","D",0]
["Partially fluorinated amphiphilic condensation polymer (PROVISIONAL).","","D",0]
["Partially fluorinated borate ester (PROVISIONAL).","","D",0]
["Polytetrafluoroethylene + Polyamide","","D",0]
["PC+PTFE","","D",0]
["Poly(Cyclohexylene dimethylene Terephthalate) + Polytetrafluoroethylene","","D",0]
["PCTFE","","D",0]
["PE-F","","D",0]
["Polyehtylen+polytetrafluoroethylene","","D",0]
["Pefluoroalkylethylmethacrylate copolymer (PROVISIONAL).","","D",0]
["Perfluorinated alcohol (PROVISIONAL).","","D",0]
["Plastic: Polyamide-imide + Melamine-formaldehyde copolymer + Polyacrylate + Perfluoro(ethylene-propylene)polymer","","D",0]
["Isoflurane","26675-46-7","D",0]
["Halothane","151-67-7","D",0]
["Tritosulfuron","142469-14-5","D",0]
["Rubber, synthetic, fluoro","64706-30-5","D",0]
["FKM, fluoroelastomers","64706-30-65","D",0]
["Perfluoropolyether (PFPE)\ror Perfluoropolyether\rdicarboxylic acid,","76415-97-9","D",0]
["Glycine, N,N-bis[2-hydroxy-3-(2-propenyloxy)propyl]-, monosodium salt, reaction products with ammonium hydroxide and pentafluoroiodoethane-tetrafluoroethylene telomer","220459-70-12","D",0]
["1-Butanaminium, N,N,N-tributyl-, hexafluorophosphate(1-)","3109-63-5","D",0]
["Copolymer of perfluorohexylethyl methacrylate, 2-N,N-diethylaminoethyl methacrylate, 2-hydroxyethyl methacrylate, and 2,2'-ethylenedioxydiethyl dimethacrylate, malic acid salt","1225273-44-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymers with γ-ω-perfluoro-C8-14-alkyl acrylate, N-oxides","783306-31-0","D",0]
["PAK+PAI+MF+FEP","","D",0]
["Polyfluoroalkyl phosphoric acid salt (PROVISIONAL).- TSCA Accession Number 204230","","D",0]
["PTFE","","D",0]
["poly(tetrafluoroethylene-co-perfluoro(propylvinyl ether))","26655-005","D",0]
["Basic Polymer: PAI+PAK+FEP+MF","","D",0]
["Basic Polymer: PAI+PAK+MF+FEP","","D",0]
["Polyamide-imide + Polytetrafluoroethylene","","D",0]
["Isoxaflutole","141112-29-0","D",0]
["Chlorotrifluoroethylene","79-38-9","D",0]
["Vinylidene fluoride","75-38-7","D",0]
["Poly(oxy-1,2-ethanediyl), α-sulfo-ω-[(perfluoroalkyl)oxy]-, sodium salt","138226-34-3","D",0]
["3,3,3-trifluoropropene","677-21-4","D",0]
["Perfluoroalkylphosphonic acids (PFPAs)","1240600-40-1","D",0]
["Fluorotelomer alcohols (FTOHs) and fluorotelomer ethoxylates (FTEOs):6:2FTEOs","52440-44-4","D",0]
["Phosphoric acid, fluoro-C9-15-alkyl esters","223239-92-7","D",0]
["Glycine, N-Acetyl-N-[3-(trifluoromethyl)phenyl]valyl-","379685-96-8","D",0]
["2-(2-nitro-4-trifluoromethylphenylamino)ethanol","10442-83-8","D",0]
["2-bromo-3,3,3-trifluoroprop-1-ene","1514-82-5","D",0]
["Trans-1,1,1,4,4,4-hexafluorobut-2-ene","66711-86-2","D",0]
["2-Butene, 1,1,1,4,4,4-hexafluoro-, (2Z)-","692-49-9","D",0]
["1-Chloro-2,3,3,3-tetrafluoropropene","3110-38-1","D",0]
["Perfluorohexane (n- and iso-) FC-72/PF-5060","1064697-81-9","D",0]
["Reaction mass of 1,1,2,2,3,3,4,4,4-nonafluoro-N,N-bis(nonafluorobutyl)butan-1-amine and 1,1,2,2,3,3,4,4,4-nonafluoro-N-[1,1,2,3,3-hexafluoro-2-(trifluoromethyl)propyl]-N-(1,1,2,2,3,3,4,4,4-nonafluorobutyl)butan-1-amine","1064698-37-8","D",0]
["Hydrofluoric acid, reaction products with 4-(1-methylethyl)morpholine","1093615-61-2","D",0]
["Chlorodifluoromethane","75-45-6","D",0]
["D-Limonene","5989-27-5","D",0]
["SF-coat-AS-20280","2414599-48-9","D",0]
["SF-coat-SFE-X008","441049-46-2","D",0]
["Fluoroelastomer (PROVISIONAL).","","D",0]
["Trifluoroethene polymer with, 4-(ethenyloxy)-1-butanol, olefin copolymers and amine (PROVISIONAL).","","D",0]
["Urethane polymer modified with perfluoroalkylsulfonamide (PROVISIONAL).","","D",0]
["Urethane polymer modified with perfluoroalkylsulfonamide and polyethoxylate (PROVISIONAL).","","D",0]
["PTFE+PBT","","D",0]
["Polyfluorinated alkyl thio acrylamide.","","D",0]
["Polyfluorinated alkyl thio polyacrylamide.","","D",0]
["Polyfluorinated alkyl thio polyacrylic acid-acrylamide.","","D",0]
["Polyfluorinated alkyl thiol.","","D",0]
["Polyfluoro alkylether (PROVISIONAL).","","D",0]
["Polyfluoroacyl chloride (PROVISIONAL).","","D",0]
["Polyfluoroacyl peroxide (PROVISIONAL).","","D",0]
["Polyfluoroalkyl betaine (PROVISIONAL).","","D",0]
["Polyfluoroalkyl phosphoric acid (PROVISIONAL).","","D",0]
["Polyfluoroalkyl phosphoric acid salt (PROVISIONAL).- TSCA Accession Number 254649","","D",0]
["Polyfluoroalkyl phosphoric acid salt (PROVISIONAL).- TSCA Accession Number 221637","","D",0]
["Polyfluoroalkylproponic acid ethyl ester (PROVISIONAL).","","D",0]
["Polymer of perfluoroalkylethylacrylate, alkylaminomethacrylate, hydroxyalkylmethacrylate, organic acid salt.","","D",0]
["Polymer of perfluoroalkylethylmethacrylate, alkylacrylate, chloroethene, and urethane methacrylate.","","D",0]
["Polyperfluoro alkylene glycol, perfluoroalkoxy-and hydroxy alkyl amido perfluoroalkyl terminated (PROVISIONAL).","","D",0]
["Polyoxymethylene+Polytetrafluorethylene","","D",0]
["PPS+PTFE","","D",0]
["Basic polymer: PTFE","","D",0]
["PTFE-Fibre","","D",0]
["Polytetrafluoroethylene + Liquid Crystal Polymer","","D",0]
["Trifluoroethene polymer with 4-(ethenyloxy)-1-butanol, ethene, ethoxy- and olefin ethoxy copolymer (PROVISIONAL).","","D",0]
["Perfluoroalkylethylacrylate copolymer (PROVISIONAL) - TSCA Accession Number 152411","","D",0]
["Perfluoroalkylethylmethacrylate copolymer.","","D",0]
["Perfluoroalkylphosphate ammonium salt (PROVISIONAL).","","D",0]
["Polyfluorinated alkyl quaternary ammonium chloride.","","D",0]
["PTFE+PCT","","D",0]
["Polytetrafluoroethylene + Polyethylene terephthalate","","D",0]
["pLASTIC: PVDF","","D",0]
["Polyvinylidene fluoride, crosslinked","","D",0]
["Resin: Polyvinylformal","","D",0]
["Quaternary ammonium perfluoroalkyl carboxylate (PROVISIONAL).","","D",0]
["Reaction product of a fluorinated alcohol, epichlorohydrin, a diol and an isocyanate (PROVISIONAL).","","D",0]
["Reaction product of a fluorinated alcohol, epichlorohydrin, an alkyl glycol and an isocyanate (PROVISIONAL).","","D",0]
["Salt of perfluoro fatty acids (PROVISIONAL).","","D",0]
["Siloxane grafted fluoroelastomer.","","D",0]
["Siloxanes and Silicones, alkyl, alkyl propoxy ethyl, methyl octyl, alkyl polyfluorooctyl.","","D",0]
["Siloxanes and silicones, amino alkyl substituted alkyl hydroxyl, hydroxyl fluorinated alkyl, ester salts, reaction products with mixed metal oxides (PROVISIONAL).","","D",0]
["Siloxanes and Silicones, aminoalkyl fluorooctyl, hydroxy-terminatedsalt.","","D",0]
["Siloxanes and silicones, dimethyl, methylfluoroalkyl (PROVISIONAL).- TSCA Accession Number 46641","","D",0]
["Siloxanes and silicones, dimethyl, methylfluoroalkyl (PROVISIONAL).- TSCA Accession Number 99333","","D",0]
["Substituted perfluoroalkenyl ammonium salt (PROVISIONAL).","","D",0]
["Substituted tetrafluoroalkene.","","D",0]
["Tetrafluoro acrylates copolymer with polyoxy methyl derivatives (PROVISIONAL).","","D",0]
["Tetrafluoroethylene chlorotrifluoroethylene copolymer (PROVISIONAL).","","D",0]
["Basic Polymer: PTFE+PA","","D",0]
["Modified ethylene-tetrafluoro ethylene copolymer (PROVISIONAL).","","D",0]
["Modified fluorinated acrylate (PROVISIONAL).","","D",0]
["Modified fluorinated acrylate.","","D",0]
["Fluoropolymer (PROVISIONAL).","","D",0]
["Fluoroalkyl acrylate copolymer - TSCA Accession Number 272583","","D",0]
["Fluoroalkyl acrylate copolymer.- TSCA Accession Number 236238","","D",0]
["Fluoroalkyl acrylate copolymer - TSCA Accession Number 199350","","D",0]
["Fluoroalkyl acrylate copolymer - TSCA Accession Number 255653","","D",0]
["Fluoroalkyl acrylate copolymer - TSCA Accession Number 236238","","D",0]
["Fluoroalkyl methacrylate co-polymer (PROVISIONAL) - TSCA Accession Number 261826","","D",0]
["Fluoroalkyl methacrylate co-polymer (PROVISIONAL).- TSCA Accession Number 261826","","D",0]
["Fluoroalkyl methacrylate co-polymer (PROVISIONAL) - TSCA Accession Number 240392","","D",0]
["Fluoroalkyl methacrylate copolymer (PROVISIONAL).","","D",0]
["Fluoroalkyl methacrylate copolymer (PROVISIONAL).","","D",0]
["Fluoroalkyl methacrylate copolymer (PROVISIONAL) - TSCA Accession Number 268781","","D",0]
["Fluoroalkyl methacrylate copolymer.","","D",0]
["Fluoroalkyl methylacrylate copolymer.","","D",0]
["Fluoroalkyl substituted siloxanes (PROVISIONAL).","","D",0]
["Fluoroalkyl sulfonamide (PROVISIONAL).","","D",0]
["Fluoroalkyl sulfonamide derivative.","","D",0]
["Fluoroalkylacrylate copolymer (PROVISIONAL) - TSCA Accession Number 274352","","D",0]
["Fluoroalkylsiloxane hydrolyzate (PROVISIONAL).","","D",0]
["Fluorocarbon polymer (PROVISIONAL).","","D",0]
["Fluorochemical ester (PROVISIONAL).","","D",0]
["Basic Polymer: MF+PAK+PAI+FEP","","D",0]
["Plastic: PTFE+PA6","","D",0]
["Plastic: PTFE+PA612","","D",0]
["PTFE+PBT","","D",0]
["Perfluoroalkenyltrialkylammonium salt (PROVISIONAL).","","D",0]
["Fluoropolymeric sulfonic acid (PROVISIONAL).","","D",0]
["Fluoropolymeric sulfonic acid salt (PROVISIONAL).","","D",0]
["Fluorosilicone polymer (PROVISIONAL).","","D",0]
["Fluorosiloxane polymer (PROVISIONAL).","","D",0]
["Basic Duromer: Fluorosiloxane resin ( Compound of a polymeric network)","","D",0]
["FMACP","","D",0]
["FMQ","","D",0]
["Fluorinated polyacrylate","","D",0]
["Basic Rubber: FVMQ","","D",0]
["Basic Rubber: FZ","","D",0]
["FZ","","D",0]
["Hexafluoropropylene-perfluoro (alkyl vinyl ether)-tetrafluoroethylene copolymer (PROVISIONAL).","","D",0]
["Hydrofluorocarbon ethers (PROVISIONAL).","","D",0]
["Hydrofluoroolefin polymer with 1,1-difluoroethene (PROVISIONAL).","","D",0]
["Liquid Crystal Polymer + Polytetrafluoroethylene","","D",0]
["MF+FEP+PAI+PAK","","D",0]
["Plastic: Melamine-formaldehyde copolymer + Perfluoro(ethylene-propylene)polymer + Polyacrylate + Polyamide-imide","","D",0]
["Basic Polymer: MF+PAI+FEP+PAK","","D",0]
["Plastic: Melamine-formaldehyde copolymer + Polyamide-imide + Polyacrylate + Perfluoro(ethylene-propylene)polymer","","D",0]
["Basic Polymer: MF+PAK+FEP+PAI","","D",0]
["Ammonium salt of fluorinated alkoxyfluoropropanoic acid.","","D",0]
["1-Propanol, 2,3-bis[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]-","64493-46-5","D",0]
["Silver perfluoropentanoate","2795-30-4","D",0]
["Methyl 4-(heptadecafluorooctyl)benzoate","80791-12-4","D",0]
["Cyclohexyl pentafluoropropanoate","24262-73-5","D",0]
["Pentafluoroethylphosphonic acid","103305-01-7","D",0]
["5-Bromo-4,4,5,5-tetrafluoropentanoic acid","234443-22-2","D",0]
["3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8-Tetradecafluorooctyl)amino]phenol","89984-91-8","D",0]
["1-[2,2-Bis(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)ethenyl]naphthalene","58510-86-4","D",0]
["N-[6-(Pentafluoroethyl)pyridin-3-yl]acetamide","1580464-60-3","D",0]
["4,7-METHANOSELENOPHENE, OCTAHYDRO-2,2,3,","102489-70-3","D",0]
["1,1'-[Oxybis(1,1,2,3,3,3-hexafluoropropane-1,2-diyl)]bis(4-bromo-2-chloro-6-fluorobenzene)","161045-78-9","D",0]
["Poly(propene-co-tetrafluoroethene-co-3,3,3-trifluoroprop-1-ene)","28853-89-6","D",0]
["4'-Phenyl-4,4,4-trifluoro-3-trifluoromethylcrotonophenone","35444-06-5","D",0]
["Perfluoro-n-(1,2,3,4,5-13C5)nonanoic acid","960315-49-5","D",0]
["1-(1,1,2,2-Tetrafluoroethoxy)propane","380-48-3","D",0]
["1-(4-Bromophenyl)-4,4,4-trifluoro-2-methyl-3-(trifluoromethyl)butane-1,3-diol","34848-34-5","D",0]
["Cadmium bis(1,1,2,2,3,3,4,4,4-nonafluorobutan-1-ide)","93367-04-5","D",0]
["Flucybene","3289-22-3","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoro-, trimethylsilyl ester","1244856-04-9","D",0]
["4,4-Bis(trifluoromethyl)-2H,4H-1,3-benzodioxine","874280-19-0","D",0]
["N-{4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]phenyl}acetamide","111641-66-8","D",0]
["2-Chloro-3,3,4,4,5,5,6,6,6-nonafluorohex-1-ene","110927-72-5","D",0]
["3-[Ethyl(perfluoro-1-oxopentyl)amino]-2-hydroxypropyl heptanoate","141187-90-8","D",0]
["2-(1-Ethenoxy-perfluoropropan-2-yl)oxy-perfluoroethanesulfonyl fluoride","103381-09-5","D",0]
["Tetrafluoropropane-1,1,1,2-tetrol","112385-13-4","D",0]
["N-[4-(Heptadecafluorooctyl)phenyl]prop-2-enamide","649721-86-8","D",0]
["N-(2,4-Difluorophenyl)-1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonamide","23375-29-3","D",0]
["Perfluorovaleraldehyde","375-53-1","D",0]
["1-(1,2-Difluoroethenyl)perfluorohexane","7621-51-4","D",0]
["1‐(1,1,2,2,3,3,3‐Heptafluoropropyl)‐4‐methyl‐2,6,7‐trioxabicyclo[2.2.2]octane","31185-67-8","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorotridecanamide","1513863-80-3","D",0]
["1-Pentanone, 1-(9H-fluoren-2-yl)-2,2,3,3,4,4,5,5-octafluoro-, O-[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]oxime","848352-66-9","D",0]
["7-Chloroperfluoroheptanoyl chloride","662-62-4","D",0]
["2,4,6-Tris(1,1,2,2-tetrafluoro-2-iodoethyl)-1,3,5-triazine","649560-98-5","D",0]
["Dawn (fluorocarbon)","88152-93-6","D",0]
["2(3H)-Furanone, 5-(3-chloro-2,2,3,3-tetrafluoropropyl)dihydro-","462655-90-9","D",0]
["N11-Ethyl-N6-methyl-3-pentafluoroethyl-6,11-dihydro-5H-pyrido(2,3-b)(1,5)benzodiazepin-5-one","133626-89-8","D",0]
["3-Trifluoromethylperfluoro-2-pentanone","93830-92-3","D",0]
["1,1,1,2,2,3,3,4,4,5-Decafluorononane","126038-57-1","D",0]
["(Carboxymethyl)[3‐(perfluoropropanesulfonamido)propyl]dimethylazanium","2089109-21-5","D",0]
["2,3,3-Trifluoro-3-(trifluoromethoxy)propanoic acid","919005-18-8","D",0]
["Poly2-(N,N-diethylamino)ethyl methacrylate-co-(3,6-dioxaoctan-1,8-diyl dimethacrylate)-co-(2-hydroxyethyl methacrylate)-co-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-yl methacrylate)","863408-19-9","D",0]
["Carbon monoxide; cyclopenta-1,3-diene; 3-methyl-2,2-bis(trifluoromethyl)tetrahydrofuran-4-ide; tungsten","54657-29-3","D",0]
["1-(1-Chloro-2,2,2-trifluoroethoxy)-1,1,2,2-tetrafluoroethane","51410-33-4","D",0]
["3-(Tridecafluorohexyl)oxan-2-ol","169213-94-9","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentyl dihydrogen phosphate","39482-86-5","D",0]
["Poly(oxy-1,2-ethanediyl), α-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,11,11,11-nonadecafluoro-2-hydroxy-2-methylundecyl)-ω-hydroxy-","90168-35-7","D",0]
["2-(Difluoromethyl)-1,1,1,2,6,6,7,8,8,8-decafluoro-5-methyloctane","57915-74-9","D",0]
["2,2-Bis[(2,2,3,3-tetrafluoropropoxy)methyl]propane-1,3-diol","60285-71-4","D",0]
["[(Perfluorotetradecanoyl)amino]-3-betaine","1513863-83-6","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluoro-N-(2-phenylethyl)hexanamide","70414-01-6","D",0]
["Difluoromethyl 2H-perfluoropropyl ether","56860-85-6","D",0]
["2,4,6-Pyridinetriethanol, beta,beta,beta',beta',beta'',beta''-hexa(trifluoromethyl)-","102206-82-6","D",0]
["1-Ethoxy-4,4,5,5,6,6,6-heptafluoro-1-hexen-3-one","184783-37-7","D",0]
["7,7-Bis(trifluoromethyl)-1,3,5-cycloheptatriene","714-82-9","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-(1,1,2,2,3,3,3-heptafluoropropyl)-ω-[1,2,2,2-tetrafluoro-1-[[[3-(triethoxysilyl)propyl] amino]carbonyl]ethoxy]-","220864-26-6","D",0]
["2-Hydroxy-4-(2,2,3,3-tetrafluoropropoxy)benzoic acid","651331-94-1","D",0]
["Copper(1+) 1,1,2,2,2-pentafluoroethan-1-ide","60007-39-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodotriacontane","1257261-89-4","D",0]
["(7E)-1,4,5,5,6,6-Hexafluoro-7-(fluoromethylene)bicyclo[2.2.2]oct-2-ene","31503-75-0","D",0]
["N-[3-(Dimethyloxidoamino)propyl]-3H-perfluoro-4,8-dioxanonanamide","1204951-03-0","D",0]
["3-[Dimethyl(3-{[(perfluorobutyl)sulfonyl]amino}propyl)ammonio]propanoate","1513864-21-5","D",0]
["5-(Perfluoropropyl)-1-phenyl-1H-tetrazole","2712-85-8","D",0]
["(2S,3R)-2,3-Dichloro-1,1,1,2,3-pentafluoropropane","111512-55-1","D",0]
["Perfluorooctahydroquinolidizine","86714-38-7","D",0]
["Perfluoroundecanoate","196859-54-8","D",0]
["2H,2H,3H,3H-Perfluorooctanoate","1799325-94-2","D",0]
["Poly[oxy[methyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silylene]]","115287-18-8","D",0]
["2,3-Bis(heptafluoropropyl)quinoxaline","2559-75-3","D",0]
["3-Phenyl-5-(tridecafluorohexyl)-1,2,4-oxadiazole","146304-76-9","D",0]
["[(4-{3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propyl}-1,2-phenylene)bis(oxy)]bis(triethylsilane)","1637311-39-7","D",0]
["2,2-Bis(trifluoromethyl)-1,3-oxazol-5(2H)-one","72681-60-8","D",0]
["2,2,3,3,4,4,5-Heptafluorononanoic acid","498543-97-8","D",0]
["2,6-Difluoro-N-((3-methyl-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)benzamide","100341-27-3","D",0]
["N,N-Dibutyl-N-methylbutan-1-aminium heptadecafluorooctane-1-sulfonate","124472-68-0","D",0]
["(Heptafluoropropyl)benzene","378-98-3","D",0]
["Pentanoic acid, 4,4,5,5,5-pentafluoro-3-oxo-, ethyl ester","663-35-4","D",0]
["4-(1,1,2,2-tetrafluoroethoxy)aniline","713-62-2","D",0]
["1,1,1,2,4,4,4-Heptafluoro-3-(trifluoromethyl)but-2-ene","41004-33-5","D",0]
["Ethyl 2,2,3,3,4,4,4-heptafluorobutyl carbonate","1980034-03-4","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-[3-(trifluoromethyl)phenyl]butanamide","2059-15-6","D",0]
["5,5,6,6,7,7,7-Heptafluoroheptan-3-amine--hydrogen chloride (1/1)","2263-70-9","D",0]
["Ammonium 7:2 fluorotelomer phosphate diester","1895-79-0","D",0]
["Tetradecyl 2,3,3,3-tetrafluoropropanoate","88239-59-2","D",0]
["1-Tetradecanol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-heptacosafluoro-","15622-57-8","D",0]
["Methacrylic acid, ester with N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-1-octanesulfonamide, polymer with ethyl acrylate, methacrylamide and methyl methacrylate","30869-51-3","D",0]
["2,2'-(2,2,3,3-Tetrafluorobutane-1,4-diyl)bis(oxirane)","194877-37-7","D",0]
["Hexafluorodichlorobutene","11111-49-2","D",0]
["2,4,6-Tris(tridecafluorohexyl)-1,3,5-triazine","25761-65-3","D",0]
["Copolymer of ethene, 2,3,3,4,4,5,5-heptafluoropent-1-ene, perfluoropropene and perfluoroethene (having 1,000 or more of number average molecular weight also insoluble in water, lipophilic solvents, generally used solvents, acid and alkaline)","203572-45-6","D",0]
["Piperidinium perfluorononanoate","95682-66-9","D",0]
["2,3,3,4,4,4-Hexafluoro-1-(piperidin-1-yl)butan-1-one","62765-23-5","D",0]
["1,2-Dichlorotetrafluorocyclobutene-1","377-93-5","D",0]
["1,1,1-Trifluoro-4-methyl-6-phenyl-2-(trifluoromethyl)hexane-2,4-diol","101914-06-1","D",0]
["1,1'-(1,1,2,2-Tetrafluoroethane-1,2-diyl)di(pyrrolidin-2-one)","143697-60-3","D",0]
["Butane, 2-bromo-1,1,1,2,3,4,4,4-octafluoro-","2924-31-4","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Pentadecafluorononane-1-thiol","26166-99-4","D",0]
["1-Bromo-4-(2,2,3,3-tetrafluorocyclobutyl)benzene","885267-02-7","D",0]
["Perfluorodecahydro-2-n-butylnaphthalene","119107-96-9","D",0]
["6,6,6-trifluoro-5-hydroxy-2,2-dimethyl-5-(trifluoromethyl)hexan-3-one","34844-45-6","D",0]
["N-[3-(Dimethylamino)propyl]-perfluoropentadecanamide","1513863-81-4","D",0]
["Fluowet PL 80","141615-38-5","D",0]
["Mono(N-ethyl-2-perfluorooctylsulfonaminoethyl)hydrogen sulfate","2558-75-0","D",0]
["Lithium 4-[(2-hydroxyethyl)[(perfluorobutyl)sulfonyl]amino]butanesulfonate","864069-51-2","D",0]
["1-(4-(4-Fluorophenyl)-8-phenylpyrazolo(5,1-c)(1,2,4)triazin-3-yl)-2,2,3,3,3-pentafluoro-1-propanone","72307-48-3","D",0]
["1-(2,2,3,3-Tetrafluoropropyl)piperidine-4-carboxylic acid","937602-77-2","D",0]
["2-Chloro-2,3,3,3-tetrafluoropropanoyl chloride","6066-46-2","D",0]
["Methyl 5,5,6,6,7,7,8,8,9,9,9-undecafluoro-4-oxononanoate","1456734-51-2","D",0]
["1-Chloro-4-(1,1,2,2-tetrafluoroethoxy)benzene","75820-58-5","D",0]
["Perfluoro-4-methyl-3,6-dioxaoctane-sulfonyl fluoride","27744-59-8","D",0]
["(3,3,4,4,5,5,5-Heptafluoro-1-iodopentyl)(trimethyl)silane","89608-32-2","D",0]
["1-(1,1,2,2-Tetrafluoroethyl)-1H-imidazole","91047-49-3","D",0]
["2-{[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)oxy]methyl}oxirane","384828-82-4","D",0]
["3,3,4,4,4-Pentafluorobutyl thiocyanate","29640-25-3","D",0]
["Potassium 2-(perfluorobutanesulfonamido)ethanolate","688738-73-0","D",0]
["1-(1-Chloro-1,2,2,2-tetrafluoroethyl)-2,3,4,5,6-pentafluorobenzene","42900-92-5","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[[(perfluorooctyl)sulfonyl]amino]-1-propanaminium","2089108-69-8","D",0]
["Pentyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","183873-55-4","D",0]
["Monopotassium monoperfluorohexyl ethylphosphate","150033-28-6","D",0]
["4-(1,1,2,2,2-pentafluoroethoxy)phenol","658-46-8","D",0]
["4,4,5,5-tetrafluoro-1-phenylpentane-1,3-dione","59857-67-9","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl nitrite","677-88-3","D",0]
["Chloro(3,3,4,4,5,5,6,6,6-nonafluorohexyl)propyl(3,3,3-trifluoropropyl)silane","608296-47-5","D",0]
["Perfluoropentanamide","355-81-7","D",0]
["9-[2-(2-Methoxyethoxy)ethoxy]-9-[3-[(perfluoroheptyl)methoxy]propyl]-2,5,8,10,13,16-hexaoxa-9-silaheptadecane","154380-27-5","D",0]
["1H,1H,2H,2H-Perfluorododecyl acetate","37858-05-2","D",0]
["Copolymer of fluoroethene and perfluoroethene","25120-57-4","D",0]
["3-[[3-(Dimethylamino)-2-hydroxypropyl][(perfluorohexyl)sulfonyl]amino]-1-propanesulfonic acid","762193-45-3","D",0]
["N-[3-[[(Perfluorooctyl)sulfonyl]amino]propyl]-N,N-dimethylhexanaminium bromide","53518-01-7","D",0]
["5,5,6,6-Tetrafluorohexane-2,4-dione","59857-63-5","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluorobutyl)sulfonyl]amino}propyl)-1-butanaminium","2089109-93-1","D",0]
["N,N'-ditert-butyl-2,2,3,3,4,4-hexafluoropentanediamide","2262-87-5","D",0]
["1,1,1,4,4,5,5,5-Octafluoro-2-trifluoromethylpentane-3-thione","79272-22-3","D",0]
["3-Phenyl-1-(undecafluorocyclohexyl)prop-2-yn-1-one","106226-84-0","D",0]
["1-bromo-1,1,2,2-tetrafluorobutane","127117-30-0","D",0]
["7-Iodoperfluoro-3-oxaheptanesulfonyl fluoride","67990-76-5","D",0]
["Perfluorobut-1-ene","357-26-6","D",0]
["Lithium perfluoro({[1-(1,2-dichloro-1,2,2-trifluoroethoxy)propan-2-yl]oxy}methoxy)methanesulfonate","1383434-27-2","D",0]
["(Heptadecafluorooctyl)silane","762260-70-8","D",0]
["[1-(Difluoromethoxy)-1,2,2,2-tetrafluoroethoxy](difluoro)acetic acid","267901-01-9","D",0]
["Undecafluorohexanoic acid--hexan-1-amine (1/1)","565225-91-4","D",0]
["Poly(difluoromethylene), .alpha.-[2-[[2-[(carboxymethyl)dimethylammonio]ethyl]thio]ethyl]-.omega.-fluoro-, inner salt","65530-68-9","D",0]
["3-[[(Perfluorooctyl)sulfonyl]methylamino]-N,N,N-trimethyl-1-propanaminium sulfate (1:1)","153968-05-9","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl methyl carbonate","277332-95-3","D",0]
["Methyl cyano[2-(2,2,3,3-tetrafluoro-2,3-dihydro-1,4-benzodioxin-6-yl)hydrazinylidene]acetate","36865-53-9","D",0]
["(Perfluorooctyl)phenylmethanol","78960-85-7","D",0]
["Siloxanes and Silicones, di-Me, Me 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-nonadecafluorododecyl-","259725-95-6","D",0]
["2,2,3,3,4,4-Hexafluoropentane-1,5-diyl bis(4-methylbenzene-1-sulfonate)","632-01-9","D",0]
["(2E)-4,5,5,6,6,6-Hexafluoro-4-(trifluoromethyl)hex-2-enoic acid","239463-98-0","D",0]
["4,4,5,5,5-Pentafluoropentane-1-thiol","148757-88-4","D",0]
["2-(4-Chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)butanoic acid","99903-58-9","D",0]
["(2E)-4,4,5,5,5-Pentafluoropent-2-en-1-ol","148757-93-1","D",0]
["1-[(Perfluorohexyl)ethoxy]-3-[(perfluorohexyl)ethylthio]-2-propanol","155604-47-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,17,17,18,18,19,19,20,20,21,21,22,22,22-Hexacosafluorodocosane","1835255-18-9","D",0]
["Perfluoro-2-methoxyaceticacid","674-13-5","D",0]
["1,1,1,2,2,3,3-Heptafluoro-5-iodoundecane","23885-16-7","D",0]
["1-[4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)piperazin-1-yl]hexan-1-one","113584-36-4","D",0]
["N-Nitrosobis(2,2,3,3,4,4,4-heptafluorobutyl)amine","83329-16-2","D",0]
["4-{2-[2,4-Bis(2-methylbutan-2-yl)phenoxy]butanamido}-2-hydroxy-N-(nonafluorobutyl)benzamide","94705-65-4","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluoro-N,N,N-tripropylhexan-1-aminium iodide","649724-86-7","D",0]
["Sodium (2S)-3-carboxy-2-({2-hydroxy-3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfanyl]propyl}amino)propanoate","93128-61-1","D",0]
["Perfluorobutylcyclopentane","87744-21-6","D",0]
["4-Methyl-2,2-bis(trifluoromethyl)imidazolidine--water (1/1)","64038-68-2","D",0]
["3-(Perfluoroheptanesulfonamido)-N,N,N-trimethylpropan-1-aminium","70225-19-3","D",0]
["(3β,7β)-25,26,26,26,27,27,27-Heptafluorocholest-5-ene-3,7-diol","240129-42-4","D",0]
["5-Bromo-2-(heptafluoropropyl)pyridine","1816282-96-8","D",0]
["Octene-1-sulfonic acid, pentadecafluoro-, potassium salt (1:1)","12751-11-0","D",0]
["2,3,3,3-Tetrafluoro-1-phenylpropan-1-one","2267-65-4","D",0]
["2-(1,1,2,2,3,3,4,4,5,5,5-Undecafluoropentylsulfonylamino)acetic acid","647-43-8","D",0]
["Methyl 2-chloro-4-(pentafluoroethyl)pyridine-3-carboxylate","1580464-71-6","D",0]
["3-(6,6,7,7,8,8,9,9,9-Nonafluorononyl)-4'-octyl-2,2'-bithiophene","919079-95-1","D",0]
["Furan, 2-methyl-5-[2,2,2-trifluoro-1-(trifluoromethyl)ethoxy]-","184778-47-0","D",0]
["(Pentafluoroethyl)trimethylsilane","124898-13-1","D",0]
["2,2,3,3-Tetrafluoro-1,4-diazabicyclo[2.2.2]octane","106705-50-4","D",0]
["Potassium 2,2,3,3-tetrafluoropropanoate","71592-16-0","D",0]
["2,3,3,3-Tetrafluoroprop-1-ene-1,1-dithiol","919515-71-2","D",0]
["Propan-2-yl ethyl(heptafluoropropyl)phosphinate","77529-57-8","D",0]
["2-Fluoroethyl pentafluoropropanoate","61799-71-1","D",0]
["1-Propanaminium, 3-[[4-[(heptadecafluorononyl)oxy]benzoyl]amino]-N,N,N-trimethyl- (9CI)","59493-71-9","D",0]
["2-[4-(1,1,2,2-Tetrafluoro-2-phenylethyl)phenyl]propan-2-amine--hydrogen chloride (1/1)","40396-69-8","D",0]
["Methyl 4-{[1,1,1,4,5,5,5-heptafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-4-(trifluoromethyl)pent-2-en-2-yl]oxy}benzoate","66432-83-5","D",0]
["3,4,4,5,5,5-Hexafluoro-2-(trifluoromethyl)pent-2-enoic acid","673486-80-1","D",0]
["5-(Heptafluoropropyl)-1H-pyrrole-2-carbaldehyde","123825-52-5","D",0]
["4-Bromo-2,2,4,5,5-pentafluoro-1,3-dioxolane","139139-66-5","D",0]
["2-Chloro-3,3,4,4,5,5-hexafluorocyclopent-1-ene-1-carbonitrile","84439-71-4","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[(2-hydroxy-3-sulfopropyl)[(perfluoropentyl)sulfonyl]amino]-, inner salt","2089109-67-9","D",0]
["Ytterbium(3+) bis(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)(1,2,2,3,3,4,4,4-octafluorobutane-1-sulfonyl)methanide (methanesulfonyl)methanide tris(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)methanide (1/1/1/1)","293290-88-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,14,14,15,15,16,16,17,17,18,18,18-Docosafluorooctadecane","1835255-24-7","D",0]
["N-[3-(Dimethylamino)propyl]-perfluoroundecanamide","1513863-78-9","D",0]
["5-Chloro-2,2,3,3,4,6-hexafluoro-2,3-dihydropyridine","79150-77-9","D",0]
["4,4,5,5-Tetramethyl-2-[5-(tridecafluorohexyl)thiophen-2-yl]-1,3,2-dioxaborolane","1338083-27-4","D",0]
["2-Butene, 4-bromo-1,1,1-trifluoro-2-(trifluoromethyl)-","163773-91-9","D",0]
["Butanoic acid, heptafluoro-, (4-methoxyphenyl)methyl ester","87461-67-4","D",0]
["3-(Ethylsulfanyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355553-99-9","D",0]
["Potassium perfluoro-2-[2-(fluorosulfonyl)ethoxy]propanoate","647836-31-5","D",0]
["1-Butene, 3,3,4,4-tetrafluoro-4-[(1,2,2-trifluoroethenyl)oxy]-, homopolymer","122817-52-1","D",0]
["3,4-dichloro-2,2,3,4,4-pentafluorobutanoic acid","375-07-5","D",0]
["1-Undecanamine, 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-","139175-50-1","D",0]
["5-[(2,2,3,3-Tetrafluoropropoxy)methyl]cytidine","62012-64-0","D",0]
["4-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]phenol","892155-19-0","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with propylene oxide, chloroacetyl chloride and pyridine","161212-16-4","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl trifluoromethanesulfonate","171182-86-8","D",0]
["2,2,3,3,4,4,4-heptafluoro-n'-(2,2,3,3,4,4,4-heptafluorobutanoyl)butanehydrazide","648-19-1","D",0]
["4-[(2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl)oxy]phenol","129560-96-9","D",0]
["2-(heptafluoropropyl)-4,5-dihydro-1h-imidazole","4472-70-2","D",0]
["4-{3-[(2,2,3,3,3-Pentafluoropropyl)amino]propyl}benzene-1,2-diol","675589-36-3","D",0]
["2,4,5,6,7-Pentafluoro-2-(trifluoromethyl)-1-benzofuran-3(2H)-one","649727-96-8","D",0]
["2-Chloro-1,1,1,2,3,3-hexafluoro-3-(trichloromethoxy)propane","61136-57-0","D",0]
["4-[Tris(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silyl]benzoic acid","189077-31-4","D",0]
["1,1,2,2-tetrafluoro-7,7a-dihydro-2aH-cyclobuta[a]indene","74879-58-6","D",0]
["1,6-Dibromonaphthalen-2-yl heptafluorobutanoate","82126-64-5","D",0]
["Hentriacontafluorohexadecanoate anion","1214264-30-8","D",0]
["1-Bromo-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexane","355-36-2","D",0]
["6-Bromo-2,2,3,3-tetrafluoro-2,3-dihydro-1,4-benzodioxine","141872-90-4","D",0]
["2-Hydroxy-3-[(perfluoroheptyl)methoxy]propyl heneicosanoate","141187-88-4","D",0]
["3,4,4-Trifluoro-3-(pentafluoroethyl)-1,2l6-oxathietane-2,2-dione","108858-07-7","D",0]
["Trichloro(3,3,4,4,5,5,5-heptafluoropentyl)silane","866-24-0","D",0]
["3-(2,2-Dichloroethenyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylic acid","121618-20-0","D",0]
["3-Cyclohexene-1-carboxylic acid, 6-[(di-2-propen-1-ylamino)carbonyl]-, sodium salt (1:1), (1R,6R)-rel-, reaction products with 1,1,1,2,2-pentafluoro-2-iodoethane-tetrafluoroethylene telomer, ammonium salts","392286-82-7","D",0]
["2H-Perfluoropropanoic anhydride","337-83-7","D",0]
["Alkyl iodides, C4-18, .gamma.-.omega.-perfluoro","68390-32-9","D",0]
["1-(3,3,4,4,5,5,6,6-Octafluoro-1-iodohexyl)-2,8,9-trioxa-5-aza-1-silabicyclo[3.3.3]undecane","135587-12-1","D",0]
["2,2,5,5-Tetrakis(trifluoromethyl)-3-imidazoline","114611-60-8","D",0]
["1,1,1,2,2,3,3-Heptafluoro-5-nitroheptan-4-ol","355-90-8","D",0]
["Bis(2,2,3,3,4,4,4-heptafluoro-1-butyl) phosphate ammonium salt","2561-18-4","D",0]
["5-Hydroxy-3,7-bis{2,2,3,3-tetrafluoro-3-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]propyl}-4,5,6,7-tetrahydro-3H-2,8-benzodioxacycloundecine-1,9-dione","62478-08-4","D",0]
["Sulfate(1-), (5-carboxylato-1,1,2,2,3,3,4,4,5,5-decafluoropentyl)pentafluoro-, (OC-6-21)-","761370-26-7","D",0]
["Poly(chloroethene-co-(docosan-1-yl methacrylate)-co-(icosan-1-yl methacrylate)-co-(octadecyl methacrylate)-co-tetracosan-1-yl methacrylate)-co-3,3,4,4,5,5,6,6,7,7,8,8,8-tetradecafluorooctan-1-yl methacrylate","1392191-75-1","D",0]
["4-Chloro-5-methyl-3-(nonafluorobutyl)pyrazole","247220-82-2","D",0]
["3-[(Perfluoropentanesulfonyl)amino]propane-1-sulfonic acid","2089108-63-2","D",0]
["Perfluoro-3-methylheptane","153273-33-7","D",0]
["2,2'-[Methylenebis(oxy)]bis[1,1,1,3,3,3-hexafluororopane","194039-81-1","D",0]
["Heptafluoropropane-1-sulfonyl chloride","140681-08-9","D",0]
["Poly(oxy-1,2-ethanediyl), α-[1-[(diethylamino)methyl]-3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-nonadecafluoroundecyl]-ω-hydroxy-","90168-36-8","D",0]
["N-tert-Butyl-2,2,3,3,4,4,4-heptafluorobutanamide","99089-22-2","D",0]
["Acetic acid, cyano-, 2,2,2-trifluoro-1-(trifluoromethyl)ethyl ester","500116-88-1","D",0]
["Ethyl 2-acetyl-4,4,5,5,6,6,6-heptafluoro-3-oxohexanoate","115479-06-6","D",0]
["1-[3-(1,1,2,2-Tetrafluoroethoxy)phenyl]propan-2-amine--hydrogen chloride (1/1)","70126-65-7","D",0]
["Hexadecyl 2,3,3,3-tetrafluoropropanoate","88239-60-5","D",0]
["Phosphonic acid, P-[3,5,5,6,8,8,9,11,11,12,14,14,15,17,17,18,18,19,19,19-eicosafluoro-3,6,9,12,15-pentakis(trifluoromethyl)-4,7,10,13,16-pentaoxanonadec-1-yl]-, monoethyl ester","1198297-67-4","D",0]
["2,3,3,4,4,5,5-Heptafluoropentanoic acid","143467-04-3","D",0]
["Chlorodiethyl(3,3,4,4,4-pentafluorobutyl)silane","608295-57-4","D",0]
["2-Amino-1-[3,5-bis(1,1,2,2-tetrafluoroethoxy)phenyl]ethan-1-ol--hydrogen chloride (1/1)","70126-66-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-(4-methylpiperazin-1-yl)heptan-1-one","560092-29-7","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)-1,2-dimethylpyridin-1-ium","140160-19-6","D",0]
["Perfluorohexane sulfonic anhydride","109065-55-6","D",0]
["Cyclopent-1-en-1-yl nonafluorobutane-1-sulfonate","36839-94-8","D",0]
["1,1,1,2,3,4,4-Heptafluoro-4-[(trifluoroethenyl)oxy]but-2-ene","136132-94-0","D",0]
["2,2,3,3-Tetrafluoro-2,3,4,5,6,7-hexahydro-4,7-methano-1-benzothiophene","102489-65-6","D",0]
["Plastic: FEP+PAK+MF+PAI","","D",0]
["FEP+PAK+PAI+MF","","D",0]
["Tetrafluoroethylene-propylene copolymer","","D",0]
["Copolymer of fluoroolefin (PROVISIONAL).","","D",0]
["trifluoromethanesulphonic acid","1493-13-6","D",0]
["Methanesulfonic acid, 1,1,1-trifluoro-, potassium salt (1:1)","2926-27-4","D",0]
["2,2,4,4,6,6,8,8,10,10,12,12,14,14,14-Pentadecafluoro-3,5,7,9,11,13-hexaoxatetradecanoic acid C8 Po-PFECA","39492-92-7","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-4-(1,1,2,2,3,3,4,4,4-nonafluorobutoxy)-1-butanesulfonic acid 4:4 C8 PFESA","1237850-23-5","D",0]
["4:2 chlorinated polyfluorinated ether sulfonic acid (2-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutoxy)-1,1,2,2-tetrafluoroethanesulfonic acid) 4:2Cl-PFESA","737728-96-0","D",0]
["(Trifluoromethyl)-phosphonic acid","374-09-4","D",0]
["(Undecafluoropenty)lphosphonic acid","2109769-70-0","D",0]
["1,1,1-Trifluoro-N,N-bis(trifluoromethyl)methanamine","432-03-1","D",0]
["2-Oxepanone, polymer with n-decanol and heptadecafluorodecanol, reaction product with benzene, diisocyanatomethyl (PROVISIONAL).","","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, telomers with C18-26-alkyl acrylate, 1-dodecanethiol, N-(hydroxymethyl)-2-methyl-2-propenamide, polyfluorooctyl methacrylate and vinylidene chloride, 2,2¿-[1,2-diazenediylbis(1-methylethy¿","","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl esters, telomers with C18-26-alkyl acrylate, 1-dodecanethiol, N-(hydroxymethyl)-2-methyl-2-propenamide, polyfluorooctyl methacrylate, 2,2¿-[1,2-diazenediylbis(1-methylethylidene)]bis[4,5-dihydro-1H-¿","","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with poly(difluoromethylene), .omega.-(2-((1-oxo-2-propenyl)oxy)ethyl)- (PROVISIONAL).","","D",0]
["Basic Rubber: AFMU","","D",0]
["Alkane carboxylic acids esters with long chain fatty alcohol and fluorinated alkylsulfonamidoalkyl alcohol (PROVISIONAL).","","D",0]
["Alkenoic acid, polymer with alkyl alkenoate, alkylalkylalkenoate, alkenoic acid and tridecafluoro alkylalkenoate, compds. with alkylaminoalcanol.","","D",0]
["Alkyl acid fluoride (PROVISIONAL).","","D",0]
["Alkyl methacrylates, polymer with substituted carbomonocycle, hydroxymethyl acrylamide and fluorinatedalkyl acrylate (PROVISIONAL).","","D",0]
["Alkyl perfluorinated acryloyl ester (PROVISIONAL).","","D",0]
["Alkylene diisocyanate homopolymer, reaction product with substituted polyethylene glycol, perfluoroalkyl alcohol, methyl ethyl ketoxime and perfluoroalkylene glycol (PROVISIONAL).","","D",0]
["Alkylpolycarboxylic acid, derivative, tris(fluorinatedalkoxy)alkyl ester salt.","","D",0]
["FEP+PAI+PAK+MF","","D",0]
["4,4,4-Trifluoro-3-hydroxy-2-(propan-2-yl)-3-(trifluoromethyl)butanal","100482-86-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorooctacosane","250738-45-5","D",0]
["1,1,1,2,2,3,3,4,4,5-Decafluoropentane","51000-94-3","D",0]
["1,1,3,3,4,4,6,6,7,7,9,9,10,10,12,12,13,13,15,15-eicosafluoro-2,5,8,11,14-Pentaoxapentadecane","173350-38-4","D",0]
["Disubstituted tetrafluoroalkane.- TSCA Accession Number 62625","","D",0]
["Diethylene glycol, polymer with diisocyanatoalkane, polyethylene glycol monomethyl ether- and fluorinatedalkanol-blocked (PROVISIONAL).","","D",0]
["Copolymers of fluoroolefin and vinyl ethers (PROVISIONAL).- TSCA Accession Number 125601","","D",0]
["Disubstituted tetrafluoroalkane.- TSCA Accession Number 68101","","D",0]
["ECTFE","","D",0]
["Plastic: ETFE","","D",0]
["Copolymers of fluoroolefin and vinyl ethers (PROVISIONAL).- TSCA Accession Number 114831","","D",0]
["Copolymers of fluoroolefin and vinyl ethers (PROVISIONAL).- TSCA Accession Number 114795","","D",0]
["Copolymer of tetrafluoroethylene and perfluoroalkoxy ethene (PROVISIONAL).","","D",0]
["Copolymer of tetrafluoroethene and perfluorosulfonylvinylether (PROVISIONAL).","","D",0]
["Copolymer of perfluoroalkylsulfonamidoalkyl acrylate and alkyl acrylate modified fatty acid dimers (PROVISIONAL).","","D",0]
["Copolymer of perfluorinated and alkyl methacrylates.","","D",0]
["ETFEX","","D",0]
["Ethylene-tetrafluoroethylene copolymer (PROVISIONAL).","","D",0]
["Ethylene-tetrafluoroethylene-fluorinated alkene copolymer.","","D",0]
["Basic Polymer:FAA","","D",0]
["perfluoro(ethylene-propylene) plastic","","D",0]
["Basic Polymer: FEP+MF+PAI+PAK","","D",0]
["Plastic: FEP+MF+PAK+PAI","","D",0]
["FEP+PAI+MF+PAK","","D",0]
["Methyl 4,4,5,5,6,6,6-heptafluoro-2-methylidenehexanoate","88021-90-3","D",0]
["Bis(perfluorodecyl) phosphinic acid erbium(3+) salt","500776-91-0","D",0]
["2,2,3-Trifluoro-3-(1,1,2,2-tetrafluoroethyl)oxirane","50838-64-7","D",0]
["1-Bromo-4-(pentafluoroethoxy)benzene","56425-85-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl undec-10-enoate","156757-62-9","D",0]
["5-(1,2,2,2-Tetrafluoro)ethoxy-perfluoro-3-oxa-4-methylpentanesulfonic acid","749836-20-2","D",0]
["difluoromethyl 1,1,2 trifluroethylether","69948-24-9","D",0]
["N-(2-Bromo-4-nitrophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","111189-67-4","D",0]
["1,1,1,2,2,3,3,5,5,5-Decafluoro-4-iodo-4-(trifluoromethyl)pentane","102780-88-1","D",0]
["Perfluorotetradecanesulfonic acid","1379460-39-5","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(2-methylpropane-1-sulfonyl)benzoic acid","1355555-21-3","D",0]
["3,3,4,4,5,5,5-Heptafluoro-1-(3-methyl-1,3-benzothiazol-2(3H)-ylidene)-2-pentanone","41131-07-1","D",0]
["Perfluoro-3-ethenyloxy-1-propanesulfonyl fluoride","77416-84-3","D",0]
["Methoxydipropyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","608299-76-9","D",0]
["Perfluoro(2,5,8,11,14-pentamethyl-3,6,9,12,15-pentaoxaoctadecanoic) acid","52481-85-3","D",0]
["1-[3,5-Bis({[tert-butyl(dimethyl)silyl]oxy}methyl)phenyl]-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptan-1-one","1335496-60-0","D",0]
["3,4,4,5,5,6,6,6‐Octafluorohex‐2‐enoic acid","70887-90-0","D",0]
["(6-Chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexyl)benzene","904-75-6","D",0]
["2-Bromo-6-[(1,1,1,3,3,3-hexafluoropropan-2-yl)oxy]pyridin-3-amine","917924-01-7","D",0]
["2-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)cyclohexan-1-one","67535-66-4","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-methoxybutan-1-ol","377-52-6","D",0]
["1-{2-[(2,2-Dimethylaziridin-1-yl)(difluoro)methyl]-3,3,3-trifluoro-2-(trifluoromethyl)propyl}pyrrolidine","23252-36-0","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-phenylbutanethioamide","61881-12-7","D",0]
["Perfluorodecahydro-1-(perfluorobutyl)naphthalene","118914-93-5","D",0]
["1-Bromo-3-(2,2,3,3-tetrafluoropropoxy)benzene","958452-23-8","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide and methacrylic anhydride","161308-18-5","D",0]
["1,1,1,2,3,3-Hexafluoroheptane","57915-71-6","D",0]
["Benzenesulfonic acid--2,2,3,3-tetrafluoropropan-1-ol (1/1)","65675-12-9","D",0]
["N-Heptafluorobutyrylproline","56236-41-0","D",0]
["[1,1,1,2,2,3,3,4,4,14,14,15,15,16,16,17,17,17-Octadecafluoro-10-(4,4,5,5,6,6,7,7,7-nonafluoroheptyl)heptadec-9-en-8-yl]-lambda~2~-stannanyl","217805-03-3","D",0]
["[Ethyl(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)amino]methanesulfonic acid","94196-26-6","D",0]
["26-Hydroxy-3,6,9,12,15,18,21,24-octaoxahexacos-1-yl 3,4,5-tris(1,1,2,3,3,3-hexafluoropropoxy)benzoate","75860-11-6","D",0]
["2‐Chloro‐1‐(chlorodifluoromethoxy)‐1,1,2‐trifluoroethane","37031-53-1","D",0]
["3,3,4,4-tetrafluoro-1,6-diiodohexane","2163-06-6","D",0]
["S-(2,2,3,3,3-Pentafluoropropyl) ethanethioate","69531-84-6","D",0]
["2,3,3-Trifluoro-3-[perfluoro-3-(methoxy)propoxy]propanoic acid","919005-20-2","D",0]
["6-Bromo-1,1,2,2-tetrafluoro-2,3-dihydro-1H-indene","922141-62-6","D",0]
["3-Fluoropropyl nonafluorobutane-1-sulfonate","1346521-48-9","D",0]
["Sulfonium, [4-[2-(1,1-dimethylethoxy)-2-oxoethoxy]phenyl]diphenyl-, 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate (1:1)","857285-80-4","D",0]
["1-(Heptafluoropropyl)-4-methoxybenzene","97745-82-9","D",0]
["3,4-Dihydro-6-phenyl-4,4-bis(trifluoromethyl)-1,3,5-triazin-2(1H)-one","352317-57-8","D",0]
["2,5-Bis(1,1,2,2,2-pentafluoroethyl)-1,3,4-oxadiazole","891-87-2","D",0]
["Perfluoro-N-(hexanesulfonyl)hexane‐1‐sulfonamide","213342-85-9","D",0]
["3-methyl-4-(2,2,3,3,4,4,5,5,5-nonafluoropentyl)cyclopentane-1,1-dicarboxylic Acid","20116-32-9","D",0]
["Sodium 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoate","2264-25-7","D",0]
["Perfluoro(2-((6-chlorohexyl)oxy)ethanesulfonic acid)","756426-58-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodononadecane","129838-41-1","D",0]
["(Nonafluorobutyl)phosphonic acid","52299-24-8","D",0]
["1-[4-(1,1,2,2-Tetrafluoroethoxy)phenyl]ethan-1-one","101975-15-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-methylnonanamide","314053-71-9","D",0]
["1,1,1,2,3,3-Hexafluoro-4-(1,1,2,2-tetrafluoroethoxy)pentane","24556-39-6","D",0]
["Perftoran","99752-82-6","D",0]
["Methoxydipropyl(3,3,4,4,5,5,5-heptafluoropentyl)silane","608299-70-3","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl benzoate","10315-85-2","D",0]
["Perfluoropentanoic anhydride","308-28-1","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7-Tetradecafluoroheptane","19493-30-2","D",0]
["1-Nitro-3-(nonafluorobutyl)benzene","2398-76-7","D",0]
["Acetic acid--2-bromo-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-ol (1/1)","89807-82-9","D",0]
["Perfucol","105605-66-1","D",0]
["tert-Butyl (1,1,1,3,3,3-hexafluoropropan-2-ylidene)carbamate","52786-55-7","D",0]
["2,2,3-Trifluoro-3-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]propanoic acid","919005-12-2","D",0]
["5-(Heptafluoropropyl)-3-phenyl-1H-pyrazole","54864-78-7","D",0]
["2-Pentanol, 1,1,1-trifluoro-5-(triethoxysilyl)-2-(trifluoromethyl)-","753453-64-4","D",0]
["3,6-Diphenyl-4-[2,2,2-trifluoro-1-(trifluoromethyl)ethyl]pyridazine","62284-34-8","D",0]
["Octadecafluorodecahydroazulene","68697-63-2","D",0]
["O,O'-bis(2-Methylpropyl) ethylphosphonous acid compd. with perfluoro-3-iodopropane (1:1)","80392-02-5","D",0]
["2-[3-(2,4-Difluorophenyl)-3-hydroxy-4-(1H-1,2,4-triazol-1-yl)butan-2-yl]-4-[4-(2,2,3,3-tetrafluoropropoxy)phenyl]-2,4-dihydro-3H-1,2,4-triazol-3-one","155432-64-7","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-7-(2-methoxyethoxy)heptane","657349-05-8","D",0]
["But-3-en-2-yl 2-fluoro-2-(trifluoromethyl)hex-4-enoate","88071-33-4","D",0]
["Methyl 4-bromo-2,2,3,3,4,4-hexafluorobutanoate","128160-31-6","D",0]
["1-Cyclohexyl-5-[(1,1,1,3,3,3-hexafluoropropan-2-yl)oxy]pyrrolidin-2-one","88461-16-9","D",0]
["Methyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","154194-61-3","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium methanesulfonate","153163-64-5","D",0]
["perfluorooctyl methacrylate","15498-46-1","D",0]
["[(2,2,3,3-Tetrafluoropropane-1-sulfonyl)methyl]benzene","233761-83-6","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)propanedioic acid","36390-03-1","D",0]
["4-[(Heptadecafluorononyl)oxy]benzoic acid","58253-64-8","D",0]
["3H-perfluoro-3-[(3-methoxy-propoxy) propanoic acid], ammonium salt","958445-44-8","D",0]
["1-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzene","353272-53-4","D",0]
["Perfluoro-1-dodecanol, 1-(dihydrogen phosphate), sodium salt (1:2)","1260224-55-2","D",0]
["1,1,1,2-Tetrafluoro-4-iodo-2-(trifluoromethyl)nonane","756-92-3","D",0]
["3-chloro-2,2,3,3-tetrafluoropropanoyl fluoride","5930-66-5","D",0]
["5-Ethylidene-2,2-bis(trifluoromethyl)-1,3-dioxolan-4-one","825630-88-4","D",0]
["(Dichloromethyl)[3-(1,2,2,2-tetrafluoroethoxy)propyl]silane","92417-47-5","D",0]
["Poly(oxy-1,2-ethanediyl), α-[[4-[(nonadecafluorononyl)oxy]phenyl]methyl]-ω-[[4-[(nonadecafluorononyl)oxy]phenyl]methoxy]-","138226-36-5","D",0]
["Diethyl 2-[1-hydroxy-2,2,2-trifluoro-1-(trifluoromethyl)ethyl]malonate","680-08-0","D",0]
["Chlorosulfurous acid, 2,2,3,3,4,4,5,5-octafluoropentyl ester","254756-55-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,8,8,9,9,10,10,11,11,12,12,12-Docosafluorododecane","1835255-38-3","D",0]
["TRIS(1H,1H,2H,2H-PERFLUOROHEXYL)TIN BROMIDE","240497-37-4","D",0]
["6-tert-butyl-2,2-dimethyl-4,4-bis(trifluoromethyl)-3,1-benzoxathiine","84649-62-7","D",0]
["1-(2,2,3,3,4,4,4-Heptafluorobutoxy)-4-nitrobenzene","109230-68-4","D",0]
["2,3,3,4,4,5,5-Heptafluorooxolane-2-carboxamide","65578-60-1","D",0]
["4,4,5,5,5-Pentafluoro-2-(trifluoromethyl)pent-1-ene-1,3-dione","53352-88-8","D",0]
["1,1,2,2,3,3-Hexafluoro-1,3-bis(pentafluoroethoxy)propane","114636-26-9","D",0]
["5-tert-Butyl-7-(heptafluoropropyl)-2-phenylpyrazolo[1,5-a]pyrimidine","346637-99-8","D",0]
["3-[(Perfluoro-1-oxononyl)amino]-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium chloride","83579-63-9","D",0]
["1,2,3,4,5,5,6,6-Octafluorobicyclo[2.2.0]hex-2-ene","30301-52-1","D",0]
["3-[Chloro(dimethyl)silyl]propyl pentadecafluorooctanoate","20120-37-0","D",0]
["bis(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl) carbonate","866-05-7","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-sulfoethyl)-, ammonium salt","80010-38-4","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorohexadecane","106873-68-1","D",0]
["4,6,7-Trichloro-1,1,2,3,3,4,5,5,6,7,7-undecafluorohept-1-ene","755-13-5","D",0]
["Undecafluorohexanenitrile","23790-49-0","D",0]
["2,3,4,5,6,6,7,7-Octafluorocyclohepta-2,4-dien-1-one","92406-76-3","D",0]
["Lithium 3-[(2-hydroxyethyl)[(perfluorobutyl)sulfonyl]amino]propanesulfonate","864069-50-1","D",0]
["3,3-Bis[(2,2,3,3-tetrafluoropropoxy)methyl]oxetane","67416-37-9","D",0]
["N-((3-Chloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100279-10-5","D",0]
["5-Chloro-7-(dihydroxymethylidene)-3-(pentafluoroethyl)-3H-2-benzopyran-6,8(4H,7H)-dione","142689-09-6","D",0]
["Silane, (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-","469904-32-3","D",0]
["4-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)oxy]phenol","129560-98-1","D",0]
["Prop-2-en-1-yl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","84123-65-9","D",0]
["(Perfluorohexyl)ethyl 2-(hydroxymethyl)-2-propenoate","152238-55-6","D",0]
["2-Pentenoic acid, 4,4,5,5,5-pentafluoro-3-hydroxy-, ethyl ester","26717-86-2","D",0]
["1-(2-Chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-ol","100482-52-8","D",0]
["1,1,2,2,3,3,4,4-Octafluoropentane","40723-64-6","D",0]
["4-(Perfluorononyl)oxybenzenesulfonate sodium","91998-13-9","D",0]
["1-Nitro-2-(pentafluoroethyl)benzene","60979-15-9","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)propanoic acid--N-propylpropan-1-amine (1/1)","165951-17-7","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-1,4-bis[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]butane","23228-90-2","D",0]
["{[1,1,1,3,3,4,4,5,5,5-Decafluoro-2-(trifluoromethyl)pentan-2-yl]sulfanyl}benzene","102780-89-2","D",0]
["2-(Nonafluorobutyl)-1H-indene","1608112-37-3","D",0]
["4-Cyanophenyl 4-(pentadecafluoroheptyl)benzoate","88951-07-9","D",0]
["Bis(2,2,3,3,4,4,5,5-octafluoropentyl) but-2-enedioate","63137-87-1","D",0]
["2,2,3,3,5,5-Hexafluoro-4-(trifluoromethyl)oxolane","61340-70-3","D",0]
["Furan, tetrahydro-, polymer with 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane, mono[[(1-oxo-2-propen-1-yl)oxy]ethyl] ether","1043910-77-5","D",0]
["15,15,16,16,16-Pentafluorohexadecane-1-thiol","220414-16-4","D",0]
["5,6-Dibromo-2,2-bis(trifluoromethyl)-2H-1,3-benzodioxole","920507-89-7","D",0]
["1-(Difluoromethoxy)-1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethane","40891-98-3","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[[(perfluoroethyl)sulfonyl]amino]-1-propanaminium","2089109-07-7","D",0]
["2-Propanol, 3-(2-benzothiazolyl)-1,1,1-trifluoro-2-trifluoromethyl-","102071-71-6","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl heptafluorobutanoate","922168-41-0","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-[1-[[(6-aminohexyl)amino]carbonyl]-1,2,2,2-tetrafluoroethyl]-ω-(1,1,2,2,3,3,3-heptafluoropropoxy)-","1207376-64-4","D",0]
["Methyl 3,4,5-tris[1,1,2-trifluoro-2-(heptafluoropropoxy)ethoxy]benzoate","1233312-86-1","D",0]
["1,2,3,4,5-Pentafluoro-6-(1,1,2,2,3,3,3-heptafluoropropyl)cyclohexane","918409-18-4","D",0]
["Ethyl (2E)-4,4,5,5,6,6,6-heptafluorohex-2-enoate","37759-79-8","D",0]
["3-IMIDAZOLINE, 4-AMINO-2,2,5,5-TETRAKIS(","23757-42-8","D",0]
["1-Butene, 3,3,4,4,4-pentafluoro-, polymer with ethene and 1,1,2,2-tetrafluoroethene","460314-45-8","D",0]
["5-Ethenyl-perfluoro-3-oxapentanesulfonyl fluoride","84271-38-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,27,27,28,28,29,29,30,30,30-Pentacontafluoro-14,17-diiodotriacontane","114221-75-9","D",0]
["2-Propenoic acid, 2-methyl-, polymer with 2-hydroxyethyl 2-methyl-2-propenoate, α-(1-oxo-2-propen-1-yl)-ω-hydroxypoly(oxy-1,2-ethanediyl) and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate","1158951-85-9","D",0]
["2,3,3,3-Tetrafluoro-2-{1,1,2,2,3,3-hexafluoro-3-[(trifluoroethenyl)oxy]propoxy}propanenitrile","124709-43-9","D",0]
["Propyl perfluorohexanoate","134638-93-0","D",0]
["N-Ethyl-N-[(perfluoroethyl)sulfonyl]glycine","1003194-07-7","D",0]
["8,8,8-Trifluoro-7-hydroxy-6-(1-hydroxyethyl)-7-(trifluoromethyl)octanenitrile","101858-32-6","D",0]
["N,N'-(1,2-Phenylene)bis(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide)","24151-81-3","D",0]
["5:3 Fluorotelomer carboxylic acid","914637-49-3","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-(fluorosulfonyl)propanoate","663-78-5","D",0]
["Strontium 6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-5-oxooct-3-en-3-olate--water (1/2/1)","36885-30-0","D",0]
["3,3,3-Trifluoro-2-(phenylsulfanyl)-2-(trifluoromethyl)propanoyl chloride","69162-16-9","D",0]
["1-Ethenyl-4-{[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)oxy]methyl}benzene","117767-64-3","D",0]
["4-{(E)-[4-(Heptafluoropropyl)phenyl]diazenyl}-N,N-dimethylaniline","144499-72-9","D",0]
["1,1,1,4,4,5,6,6,6-Nonafluoro-2,2,5-tris(trifluoromethyl)hexan-3-one","88995-86-2","D",0]
["Cerium(3+) tris-[1,1,1,2,2,3,3-heptafluoro-7,7-dimethyl-6-oxo-4-octen-4-olate]","172424-98-5","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-1-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]-8-iodooctane","25080-25-5","D",0]
["[1,1,2,2-Tetrafluoro-2-(trifluoromethoxy)ethoxy]acetic acid","919005-40-6","D",0]
["Dichlorobis(1,1,2,2,3,3,6,6,6-nonafluorohexyl)silane","156323-66-9","D",0]
["imidodicarbonic diamide, N,N'2-tris(6-isocyanatohexyl)-, reaction products with ethylene glycol, alpha- fluoro-, omega-[2[(1-oxo- 2-propenyl)oxy]ethyl]poly(difluoromethylene), glycidol and 2,4-TDI","329201-80-1","D",0]
["5-Chloro-6-(2,2,3,3-tetrafluoropropoxy)pyridin-3-ol","1355067-28-5","D",0]
["Acetic acid--2,2,3,3,4,4,5,5-octafluoropentan-1-ol (1/1)","1422-69-1","D",0]
["(2E)-1,1,2,3,4,5,5,5-Octafluoro-1-iodo-4-(trifluoromethyl)-2-pentene","120695-78-5","D",0]
["Disodium perfluoro-3,5,7,10,13-pentaoxapentadecanedioate","88707-87-3","D",0]
["5-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]benzene-1,3-dicarbonyl dichloride","121699-18-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,7,7-Tetradecafluoro-8-[(prop-2-en-1-yl)oxy]octane","192998-90-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecanoyl Chloride","2248-93-3","D",0]
["N-Ethyl-3-[[(perfluorooctyl)sulfonyl]amino]-N,N-dimethylpropanaminium ethyl sulfate (1:1)","53518-05-1","D",0]
["N-{[2,5-Dichloro-4-(1,1,2,2-tetrafluoroethanesulfinyl)phenyl]carbamoyl}-2,6-difluorobenzene-1-carboximidic acid","100341-45-5","D",0]
["1,8-Octanediylbis-1,1'-(perfluorohexane)","959462-54-5","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol, reduced, reaction products with 1-chloro-2,3-epoxypropane","161212-24-4","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl diethylphosphinite","95932-53-9","D",0]
["2,2,3,3,4,4,5,5-octafluoropentanoyl Bromide","376-69-2","D",0]
["5-Chloro-3-(heptafluoropropyl)-5-(trifluoromethyl)-5H-1,4,2-dioxazole","88326-81-2","D",0]
["N-(Carboxylatomethyl)-N,N-dimethyl-4-[[perfluoro-1-ethyl-2-methyl-1-propen-1-yl]oxy]benzenaminium","927408-20-6","D",0]
["Potassium 4-[(perfluorooctyl)oxy]benzoate","89932-68-3","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-5-[(tridecafluorohexyl)oxy]pentan-1-amine","188630-32-2","D",0]
["Lithium 3-[(perfluorooctane-1-sulfonyl)(propyl)amino]propanoate","163973-26-0","D",0]
["5-Bromo-5'-(tridecafluorohexyl)-2,2'-bithiophene","327630-35-3","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2,2,3,3,4,4,4-heptafluorobutanoyl)-N-(2-hydroxy-2-phenylethyl)butanamide","55521-07-8","D",0]
["2H-Perfluoro(2-methylpentane)","30320-28-6","D",0]
["5-{[1,1,1,4,5,5,5-Heptafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-4-(trifluoromethyl)pent-2-en-2-yl]oxy}benzene-1,3-diamine","138781-42-7","D",0]
["19-Bromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluorononadecane","1597-70-2","D",0]
["Butanoic acid, 2,2,3,3,4,4,4-heptafluoro-, 2-[6,7-dihydro-3-methyl-2-[[[4-(2-phenyldiazenyl)phenyl]amino]carbonyl]-4(5H)-benzofuranylidene]hydrazide","890011-12-8","D",0]
["4,4,5,5,6,6,6-Heptafluoro-L-norleucine","148043-94-1","D",0]
["Perfluoro-1-octanesulfinic acid","187480-42-8","D",0]
["4-(Perfluorohexyl)-3,3-difluorobutanol 1-(dihydrogen phosphate) ammonium salt (1:2)","1025044-22-7","D",0]
["3-[(2-Carboxyethyl)[(perfluorobutyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","2089109-15-7","D",0]
["4-(1,2-Dichloro-1,2,2-trifluoroethoxy)-2,2,3,3,4,4-hexafluorobutanoic acid","86556-81-2","D",0]
["N'-[(4-Ethylphenyl)methylidene]-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptanehydrazide","445258-05-9","D",0]
["Cyclopropanecarboxylic acid, 2,2-bis(trifluoromethyl)-3-(3,3,3-trifluoro-2-     (trifluoromethyl)-1-propenyl)-, trans","99903-53-4","D",0]
["Perfluoro-5,5'-bis(trifluoromethyl)-1,1'-bicyclohexyl","105462-77-9","D",0]
["{[(2-Chloro-3,3,4,4-tetrafluorocyclobut-1-en-1-yl)oxy]methyl}benzene","18448-29-8","D",0]
["1,1,1,3,4,4,4-Heptafluoro-3-(heptafluoropropoxy)-2-(trifluoromethyl)butan-2-yl prop-2-enoate","1622868-66-9","D",0]
["2-[[(Perfluorooctyl)sulfonyl]oxy]-1H-benz[de]isoquinoline-1,3(2H)-dione","639827-02-4","D",0]
["2-({3-[3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butane-1-sulfonyl]propyl}amino)ethan-1-ol","1353009-40-1","D",0]
["1,1,1,2,2,3,3-heptafluoroheptan-4-ol","425-21-8","D",0]
["Dimethyl (2Z)-2,3,4-trifluoro-4-(trifluoromethyl)-2-pentenedioate","74032-60-3","D",0]
["10-Bromo-1,1,1,2,2,3,3,4,4-nonafluorodecane","457603-91-7","D",0]
["(5Z)-1,1,1,2,2,3,3,4,4-Nonafluoro-6-iododec-5-ene","107831-93-6","D",0]
["1-(Heptafluoropropyl)-4-iodobenzene","1417885-93-8","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-1,6-dimethoxyhexane","132182-96-8","D",0]
["(3,3,4,4,5,5,6,6-Octafluorooctane-1,8-diyl)bis(trichlorosilane)","193622-77-4","D",0]
["Perfluoro(4-methoxybutanoic acid)","863090-89-5","D",0]
["2-Buten-1-one, 1-(2-furyl)-4,4,4-trifluoro-3-trifluoromethyl-","35444-09-8","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-1-(pentafluorophenyl)pentan-1-one","1610931-27-5","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-omega.-(2-((2-methyl-1-oxo-2-propenyl)oxy)ethyl), copolymer with t-butyl-2-methylpropenoate and ethyleneiminyl-2-methylpropenoate","220713-85-9","D",0]
["2,2,3,3,4,4-Hexafluoro-1-(2-hydroxy-2-phenylethyl)cyclobutan-1-ol","100427-76-7","D",0]
["Ammonium 2‐{[difluoro(trifluoromethoxy)methoxy]difluoromethoxy}‐2,2‐difluoroacetate","919004-95-8","D",0]
["1-Cyclohexene-1-carbonitrile, 2-amino-3,3,4,4,5,5-hexafluoro-6-imino-","90408-50-7","D",0]
["Des-iodoflubendiamide","1016160-78-3","D",0]
["desflurane","57041-67-5","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-(((tridecafluorohexyl)sulfonyl)amino)propan-1-aminium","736877-37-5","D",0]
["6,6,7,7-Tetrafluoro-5-hydroxy-2,2-dimethyl-5-phenylheptan-3-one","5568-41-2","D",0]
["(2E)-1-Propenylperfluorohexane","80793-20-0","D",0]
["Perfluoro-10-dodecene-1-sulfonic acid","2089109-47-5","D",0]
["2-(o-Cyanophenoxy)-3'-hydroxy-4'-(perfluorobutyrylamino)tetradecananilide","117844-18-5","D",0]
["Ethyl 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoate","42287-85-4","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)benzoic acid","129590-24-5","D",0]
["2,6-Diphenyl-4,4-bis(trifluoromethyl)-1,4-dihydro-1,3,5-triazine","24337-46-0","D",0]
["[(2,2,3,3,4,4,5,5-Octafluoropentane-1-sulfonyl)methyl]benzene","201943-30-8","D",0]
["1-Diazonio-4-[(4S)-5-oxo-2,2-bis(trifluoromethyl)-1,3-oxazolidin-4-yl]but-1-en-2-olate","675605-29-5","D",0]
["5-(2,2,3,3,3-Pentafluoropropyl)-2,4(1H,3H)-pyrimidinedione","53489-96-6","D",0]
["3-(Tridecafluorohexyl)aniline","119534-79-1","D",0]
["Trimethoxy(tridecafluorohexyl)silane","84464-05-1","D",0]
["(Diethoxymethyl)(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","136790-31-3","D",0]
["1-Nitro-3-(tridecafluorohexyl)benzene","132782-24-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-phenyloctan-1-one","292863-75-3","D",0]
["(3,3,4,4,5,5,5-Heptafluoro-1-iodopent-1-ene-1,2-diyl)bis(trimethylsilane)","89608-41-3","D",0]
["4-((Henicosafluorodecyl)oxy)benzenesulfonic acid","786629-35-4","D",0]
["4-(Chlorosulfonyl)-1,1,2,2,3,3,4,4-octafluorobutane-1-sulfonic acid","709605-80-1","D",0]
["Triethylammonium perfluoroheptane sulfonate","72033-40-0","D",0]
["3-[4-(2,2,3,3-Tetrafluoropropoxy)phenyl]prop-2-enenitrile","123632-23-5","D",0]
["ethyl 2-ethoxy-2,3,3,3-tetrafluoropropanoate","10186-66-0","D",0]
["4-Chloro-2-(heptafluoropropyl)pyridine","1816283-32-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl octanoate","18770-62-2","D",0]
["(Perfluorohexadecyl)hexadecane","137338-42-2","D",0]
["1-Aziridinepropionic acid, 2,2,3,3,4,4,4-heptafluorobutyl ester","24160-20-1","D",0]
["2-chloro-1,1,1,3,3,3-hexafluoro-2-(trifluoromethyl)propane","4459-16-9","D",0]
["1,1-Dichloro-2,3,4,4,4-pentafluorobut-1-ene","141535-83-3","D",0]
["Amphetamine PFP","70363-72-3","D",0]
["5-Bromo-1,1,1,2,2,3,3-heptafluoropentane","355-94-2","D",0]
["1,1,1-trifluoro-4-iodo-2,2-bis(trifluoromethyl)butane","14115-45-8","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with ammonia, dehydrated","161308-23-2","D",0]
["1,1,1,3,3,3-Hexafluoro-2,2-di-4-tolylpropane","1095-77-8","D",0]
["Perfluorobicyclo-(4.4.0)-dec-1,6-ene","54939-04-7","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)propanoyl fluoride","382-22-9","D",0]
["Methyl 3-[(heptafluoropropyl)sulfanyl]benzoate","88489-61-6","D",0]
["Bis(heptafluoropropyl)phosphinic chloride","90403-29-5","D",0]
["5:3 Fluorotelomer betaine","171184-14-8","D",0]
["Butanedioic acid, 2,2,3,3-tetrafluoro-, 1,4-dimethyl ester","356-36-5","D",0]
["3-[[(Perfluorooctyl)sulfonyl]methylamino]-N,N,N-trimethylpropanaminium iodide","53518-02-8","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)benzonitrile","96308-32-6","D",0]
["1-Hexanesulfonamide, N-[3-(dimethylamino)propyl]-3,3,4,4,5,5,6,6,6-nonafluoro-","34455-17-9","D",0]
["1,2,5,5,6,6-Hexafluoro-3,4-dimethyl-1,3-cyclohexadiene","31462-68-7","D",0]
["Ethyl (1R,3S)-3-(2,2-dibromoethenyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylate","99903-49-8","D",0]
["5-(1,1,2,2-Tetrafluoroethoxy)-1,3-dihydro-2H-benzimidazole-2-thione","97963-60-5","D",0]
["Methyl 4,4,4-trifluoro-3-(trifluoromethyl)butanoate","674335-88-7","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-1-(4-methylphenyl)pentan-1-one","647-60-9","D",0]
["1,1,1,2,3,4,5,5,6,6,6-Undecafluoro-4-(trifluoromethyl)hex-2-ene","403855-46-9","D",0]
["Bis[2-[[(perfluorooctyl)sulfonyl]amino]ethyl] (4-methyl-1,3-phenylene)bis-carbamate","89946-29-2","D",0]
["7-Chloro-1,1,2,2-tetrafluoro-2,3-dihydro-1H-indene","922141-57-9","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)propanedioic acid","26564-96-5","D",0]
["1,1,2,2,3,3,4,4-octafluoro-5-iodo-5-(trifluoromethyl)cyclopentane","125112-67-6","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-1-phenylnon-1-en-3-one","89176-08-9","D",0]
["2‐(1,1,2,2,3,3,4,4,5,5,6,6,6‐Tridecafluorohexanesulfonamido)acetic acid","1003193-99-4","D",0]
["[(1,1,1,3,3,3-Hexafluoro-2-phenylpropan-2-yl)oxy](trimethyl)silane","131297-16-0","D",0]
["4H-1,3,2-Dithiazine, 4,4,5,5,6,6-hexafluorodihydro-, 1,1,3,3-tetraoxide, potassium salt (1:1)","588668-97-7","D",0]
["N-(2,2,3,3,3-Pentafluoro-1-phenylpropylidene)hydroxylamine","65686-80-8","D",0]
["Perfluorooctanesulfonamide lithium salt (1:1)","76752-79-9","D",0]
["Perfluorotetralin","2342-07-6","D",0]
["2,2,3,3-Tetrafluoroputrescine","356-56-9","D",0]
["1H,1H,2H,2H-Perfluorotetradecyltriethoxysilane","885275-56-9","D",0]
["2,3,3,3-Tetrafluoro-2-(nonafluorobutoxy)propanoic acid","137780-68-8","D",0]
["N-(2-Hydroxyethyl)-3-[(2-hydroxyethyl)[(perfluoroheptyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","2089109-02-2","D",0]
["1,1,1,2,2,3,3,4,4,7,7,7-Dodecafluoro-6-iodoheptane","935553-88-1","D",0]
["1-Bromo-4-chloro-1,1,2,2,3,3,4,4-octafluorobutane","89740-37-4","D",0]
["2,6-Diphenyl-4,4-bis(trifluoromethyl)-4H-1,3-thiazine","88656-34-2","D",0]
["N-(2-((Methylsulfonyl)amino)-5-(trifluoromethyl)-3-pyridinyl)-2,2,3,3,3-pentafluoropropanamide","141283-57-0","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)oxy-1,2-ethanediyl], α-[[[(heptadecafluorooctyl)sulfonyl]methylamino]acetyl]-ω-hydroxy-","114672-54-7","D",0]
["2,7-Dicarbomethoxyperfluoro-3,6-dioxaoctane","16835-51-1","D",0]
["6:2 Fluorotelomer thia hydroxy propyl trimethyl ammonium","88992-46-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluorooctane-1,8-diyl dicyanate","168774-28-5","D",0]
["Methyl difluoro{1,1,2,2-tetrafluoro-2-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]ethoxy}acetate","169289-58-1","D",0]
["Bis(2,2,3,3,4,4-hexafluoro-1-oxobutyl)peroxide","308-71-4","D",0]
["5-Pentafluoroethyl-[1,3,4]thiadiazol-2-ylamine","51314-64-8","D",0]
["1,2-Dibromo-1,2,3,3,4,4,5,5,6,6-decafluorocyclohexane","336-12-9","D",0]
["Methacrylic acid, 2-(diethylamino)ethyl ester, polymer with 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl acrylate","34514-87-9","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2,6-dimethylbenzaldehyde","1771743-29-3","D",0]
["Diethyl (1,1,1,3,3,3-hexafluoropropan-2-yl)phosphonate","80982-76-9","D",0]
["6-Fluoro-5,7,7-tris(trifluoromethyl)-2,3,7,7a-tetrahydro-1H-pyrrolizine","89810-79-7","D",0]
["2,2,2-trifluoro-N-(1,1,1,3,3,3-hexafluoropropan-2-ylidene)acetamide","52225-57-7","D",0]
["Octadecyl 2,3,3,3-tetrafluoropropanoate","88239-61-6","D",0]
["Октафторбутен","11070-66-9","D",0]
["3-Nitrophenyl heptafluorobutanoate","52512-15-9","D",0]
["4,4'-Bis(2-hydroxyhexafluoroisopropyl)diphenyl","2180-30-5","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)(triphenyl)phosphanium iodide","94190-72-4","D",0]
["6-Chloro-3,3,4,4,5,5,6,6-octafluorohexanoic acid","131118-32-6","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-[1-(ethoxycarbonyl)-1,2,2,2-tetrafluoroethyl]-ω-(1,1,2,2,3,3,3-heptafluoropropoxy)-","90317-75-2","D",0]
["1~3~,3~3~-Bis(tridecafluorohexyl)-1~2~,2~2~:2~5~,3~2~-terthiophene","630045-89-5","D",0]
["1-Hexanethiol, 3,3,4,4,5,5,6,6,6-nonafluoro-","34451-25-7","D",0]
["2,2,3,3,3-Pentafluoro-1-(triphenylsilyl)propan-1-one","141334-26-1","D",0]
["2-(2,2,3,3-Tetrafluoropropanoyl)cyclohexan-1-one","235743-21-2","D",0]
["1,1,1,2,4,4-Hexafluorobutane","158421-88-6","D",0]
["9,9,10,10-tetrafluoro-9,10-dihydrophenanthrene","14205-64-2","D",0]
["(3β,7α)-25,26,26,26,27,27,27-Heptafluorocholest-5-ene-3,7-diol","240129-40-2","D",0]
["1-Bromo-9-({9-[(4,4,5,5,5-pentafluoropentyl)sulfanyl]nonyl}sulfanyl)nonane","1391053-14-7","D",0]
["6-(Ethenyloxy)-1,1,1,2,2,3,3,4,4-nonafluorohexane","63391-84-4","D",0]
["2-(Pentafluoroethyl)pyridine-4-carboxylic acid","2090610-39-0","D",0]
["Potassium heptafluorobutanoate","2966-54-3","D",0]
["1-[4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)piperazin-1-yl]propan-1-one","113584-34-2","D",0]
["Silver perfluorohexanoate","336-02-7","D",0]
["4,5-Dichloro-2,2-bis(trifluoromethyl)-2H-1,3-dioxole","64499-77-0","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxine-6-carbonyl chloride","180091-39-8","D",0]
["(6E)-8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-Heptadecafluoropentadec-6-ene","350608-65-0","D",0]
["Methacrylic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoroheptadecyl ester, polymers","34482-06-9","D",0]
["2-PROPANOL, 1,1,1,3,3,3-HEXAFLUORO-2-(2,","73825-97-5","D",0]
["1,2,3,3,4,4,5,6,6,7,7-Undecafluorocyclohept-1-ene","85625-24-7","D",0]
["Perfluoro[2-(fluorosulfonyl)ethoxy]acetyl chloride","88986-43-0","D",0]
["1,1,1,2,4-Pentafluorobutane","161791-23-7","D",0]
["2-(Heptafluoropropyl)-1,3-dioxolane","109799-66-8","D",0]
["1,1,1,2,2-Pentafluoro-2-[(2-iodoethyl)sulfanyl]ethane","1206523-87-6","D",0]
["Ether, bis(nonafluorobutyl)","308-48-5","D",0]
["1,1,1,2,3,3,7,7,8,9,9,9-Dodecafluoro-4-methylnonane","57915-73-8","D",0]
["(5S)-5-(Phenylmethyl)-2,2-bis(trifluoromethyl)-1,3-dioxolan-4-one","748134-70-5","D",0]
["3-(Heptafluoropropyl)pentane-1,5-diol","678-93-3","D",0]
["(Perfluoroheptyl)(sulfonylamino)acetic acid","1003194-00-0","D",0]
["Propane, 3-bromo-1,1,1,2,2-pentafluoro-","422-01-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodooctadecane","129838-40-0","D",0]
["2-Fluoro-2-(trifluoromethyl)pent-4-enoic acid","73900-39-7","D",0]
["(3β)-25,26,26,26,27,27,27-Heptafluoro-3-hydroxycholest-5-en-7-one","215094-37-4","D",0]
["Perfluoro-6-(ethoxy)hexanoic acid","919005-55-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorotetracosane","89109-71-7","D",0]
["1,1,1,5,6,6-Hexafluoro-3-(prop-2-en-1-yl)-2-(trifluoromethyl)hex-5-en-2-ol","795298-34-9","D",0]
["2,3,3,3-Tetrafluoro-N-methoxy-N-methylpropanamide","677354-02-8","D",0]
["(1,4-Dibromo-3,3,4,4-tetrafluorobutyl)(trimethyl)silane","113688-43-0","D",0]
["Perfluorooctanoic acid diethanolamide","42268-97-3","D",0]
["3-(Perfluorooctyl)-1-propene","61589-64-8","D",0]
["Fluoro(1,1,2,2-tetrafluoro-2-sulfoethoxy)acetic acid","2376467-67-1","D",0]
["Perfluorodecahydro-2-iso-butylnaphthalene","119141-87-6","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.',.alpha.''-[(2-hydroxy-1,2,3-propanetriyl)tris[carbonyloxy[2-(chloromethyl)-2,1-ethanediyl]]]tris[.omega.-fluoro-","71278-43-8","D",0]
["Lithium 3-[[(perfluorobutyl)sulfonyl](propyl)amino]propanesulfonate","864069-42-1","D",0]
["16H-Perfluorohexadecanoic acid","2274731-01-8","D",0]
["2,6-Difluoro-N-(((4-((1,1,2,2- tetrafluoroethyl)thio)phenyl)amino)carbonyl)benzamide","100331-08-6","D",0]
["7-(Nonafluorobutyl)-1-benzothiophene","1608112-40-8","D",0]
["1,1,1,2,3,3,4,4,5,5-Decafluoro-2-(trifluoromethyl)pentane","1980062-87-0","D",0]
["Perfluoro-2-cyclohexylethane-1-sulfonic acid","558-68-9","D",0]
["2,4-Bis(1,1,2,3,3,3-hexafluoropropoxy)benzoic acid","75860-10-5","D",0]
["2-Chloro-4-(pentafluoroethyl)pyrimidine-5-carboxylic acid","954226-17-6","D",0]
["1-Chloroperfluoroheptane","375-89-3","D",0]
["Ethylammonium perfluoro-4-(trifluoromethyl)pentanoate","65418-99-7","D",0]
["(2S)-3,3,4,4,5,5,5-Heptafluoropentan-2-ol","1313024-90-6","D",0]
["1-Butanesulfonamide, N,N'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[1,1,2,2,3,3,4,4,4-nonafluoro-N-methyl-","120945-47-3","D",0]
["1-Bromoperfluoropentane","558-91-8","D",0]
["Sulfonium, tris(4-methylphenyl)-, 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate (1:1)","722538-68-3","D",0]
["1-Octanesulfonamide, N-(2,3-dihydroxypropyl)-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-propyl-","2262-49-9","D",0]
["1H,8H-Perfluorooctane","307-99-3","D",0]
["5-(Perfluoropropyl)-1,3-benzenediamine","25642-11-9","D",0]
["2-(Nonafluorobutyl)-1H-indole","1608112-34-0","D",0]
["(Perfluorononyl)methane","155928-85-1","D",0]
["[1,1,1,2,2,3,3,4,4,5,5,6,6,16,16,17,17,18,18,19,19,20,20,21,21,21-Hexacosafluoro-12-(4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononyl)henicos-11-en-10-yl]-lambda~2~-stannanyl","217805-02-2","D",0]
["Butyrophenone, 3-hydroxy-4,4,4-trifluoro-3-(trifluoromethyl)-2',4',6'-trimethyl-","101221-68-5","D",0]
["2-(Perfluorohexyl)thiophene","128032-22-4","D",0]
["Perfluorooctylperfluorodecyl phosphinic acid","500776-81-8","D",0]
["Lithium 1,1,1,3,3,4,4-heptafluoro-4-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]-2-(trifluoromethyl)butan-2-olate","78740-39-3","D",0]
["1-(4-Chlorophenyl)-4,4,4-trifluoro-2-methyl-3-(trifluoromethyl)butane-1,3-diol","34848-30-1","D",0]
["6-(Nonafluorobutyl)hexanol","181042-39-7","D",0]
["1-(1-Piperidinyl)-2-(triphenylphosphoranylidene)perfluorohexane-1,3-dione","148192-46-5","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoroheptane","154381-51-8","D",0]
["2-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)cyclododecan-1-ol","34844-40-1","D",0]
["5-Chloro-perfluoropentanoate","1696259-89-8","D",0]
["N,N′-[Phosphinicobis(oxy-2,1-ethanediyl)]bis[N-methylperfluoro-1-octanesulfonamide]","132445-38-6","D",0]
["Potassium bis(perfluorohexyl)difluoroborate","937038-66-9","D",0]
["N-[(4-Bromophenyl)oxido(trifluoromethyl)sulfanylidene]perfluorobutanesulfonamide","1421133-00-7","D",0]
["(2,3,3,5,5,6,6-Heptafluoro-1,4-dioxan-2-yl)(trimethyl)silane","61448-95-1","D",0]
["1-Bromo-6-chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexane","105198-06-9","D",0]
["3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11, 11,12,12,13,13,14,14,14-Tetracosafluorotetradec-2-enoic acid","70887-95-5","D",0]
["4,6-Bis[(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl)oxy]-1,3,5-triazin-2-amine","57338-64-4","D",0]
["Perfluoro-t-butyl methyl ether","66670-22-2","D",0]
["N,N,N-Trimethyl-2-[2-methyl-1-oxo-3-[(perfluoroheptyl)ethylthio]propoxy]ethanaminium iodide (1:1)","121912-27-4","D",0]
["1,1',1''-{[(Heptafluorocyclobutyl)oxy]methanetriyl}tribenzene","872885-66-0","D",0]
["1-(Difluoroiodo)perfluoro-1-octyne","1424379-19-0","D",0]
["Nonafluoro(trifluoromethoxy)cyclopentane","788-40-9","D",0]
["2-(Difluoromethyl)-1,1,1,2,3,3,5,5,5-nonafluoro-4,4-bis(trifluoromethyl)pentane","801287-27-4","D",0]
["Perfluoro-3,6,9-trioxadecanoic acid","151772-59-7","D",0]
["5-(2,2,3,3,3-Pentafluoropropyl)-1-pentofuranosyl-2,4(1H,3H)-pyrimidinedione","55420-10-5","D",0]
["Ethanaminium, 2-[[(heptadecafluorooctyl)sulfonyl]amino]-N,N,N-trimethyl-, iodide","57765-32-9","D",0]
["7-(Heptafluoropropyl)-7-hydroxy-4,9-dimethoxy-6,7-dihydro-5H-furo[3,2-g][1]benzopyran-5-one","376380-76-6","D",0]
["3-Methyl-5-(tridecafluorohexyl)-1,2,4-trioxolane","63967-44-2","D",0]
["Phosphonic acid, P-[3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]butyl]-, monoethyl ester","1198297-33-4","D",0]
["1,1,1,2,2,5,5,6,6,9,9,10,10,10-tetradecafluorodec-3-ene","35208-08-3","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-methoxypropane--(E)-1,2-dichloroethene (1/1)","218462-19-2","D",0]
["5-[(2,2,3,3-Tetrafluoropropoxy)methyl]-2,4(1H,3H)-pyrimidinedione","59694-30-3","D",0]
["1,1,1,3,4,4-Hexafluoro-2-(trifluoromethyl)but-3-en-2-ol","15052-92-3","D",0]
["6-(1,2,2,2-Tetrafluoroethoxy)perfluorohexanoic acid","919005-53-1","D",0]
["Dichloro(difluoro)(pentafluoroethyl)-lambda~5~-phosphane","61527-27-3","D",0]
["Perfluorodecanonitrile","379215-40-4","D",0]
["Poly(oxy-1,2-ethanediyl), α-(4-sulfobutyl)-ω-[2-[[(heptadecafluorooctyl) sulfonyl]methylamino]ethoxy]-, sodium salt","153692-02-5","D",0]
["2-Methylpropyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","183873-54-3","D",0]
["Perfluoro-2-(fluorosulfonyl)ethoxyacetic acid","88986-29-2","D",0]
["4-Cyanophenyl nonafluorobutane-1-sulfonate","626201-15-8","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)benzeneethanamine, hydrochloride","70126-62-4","D",0]
["1,1,1,3,3,3-Hexafluoro-2-hydroperoxypropan-2-ol","32751-01-2","D",0]
["1,5-Dichloro-1,2,2,3,3,4,4-heptafluorocyclopentane","64470-65-1","D",0]
["2,2,3,3,5,5,5-Heptafluoro-4-oxopentanoic acid","4796-91-2","D",0]
["17-Bromo-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoroheptadecane","155401-47-1","D",0]
["Dimethyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)chlorosilane","119386-82-2","D",0]
["(4-Bromophenyl){5-[difluoro(trifluoromethoxy)methyl]-5-hydroxy-3-methyl-4,5-dihydro-1H-pyrazol-1-yl}methanone","722470-55-5","D",0]
["Chloro(difluoromethoxy)difluoromethane","56726-75-1","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[[(perfluorooctyl)sulfonyl]amino]propanaminium chloride","91322-74-6","D",0]
["4,4,4-Trifluoro-1-(5-methylfuran-2-yl)-3-(trifluoromethyl)but-2-en-1-one","140860-78-2","D",0]
["1,1,1,3,4,4,5,5,6,6-Decafluoro-2-(trifluoromethyl)hex-2-ene","67437-94-9","D",0]
["2,2,3,3,4,4,5,5,5-nonafluoropentanenitrile","22325-71-9","D",0]
["Dodecafluorooctanedioyl difluoride","24647-09-4","D",0]
["Perfluoro-1-[2-[1-[(methoxy)methyl]-ethoxy]-1-(methyl)ethoxy]-2-propanone","18934-99-1","D",0]
["6-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1,3-benzothiazol-2(3H)-one","1433216-60-4","D",0]
["COPOLYMER OF TETRAFLUOROETHYLENE AND PERFLUOROETHYL VINYL ETHER","147026-01-5","D",0]
["Perfluoro-3,6-dioxa-4-methyl-7-octene-1-sulfonic acid","29311-67-9","D",0]
["1-(4-Chlorophenyl)-2,3,3,3-tetrafluoro-2-(trifluoromethyl)propan-1-one","56041-73-7","D",0]
["4,4,5,5,6,6,7,7-octafluoro-1-phenylheptane-1,3-dione","63166-36-9","D",0]
["1-[4-(Nonafluorobutyl)phenyl]butyl diphenyl phosphate","846543-02-0","D",0]
["1,1,1,2,2,3,3,4,5,5,6,6,6-Tridecafluorohexane","1998-67-0","D",0]
["(3,5-ditert-butylphenyl) 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","93131-76-1","D",0]
["N,N′-[Phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-perfluoro-1-dodecanesulfonamide] ammonium salt","118337-77-2","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluoropentanamide","136133-03-4","D",0]
["Tris(trifluoromethyl)oxaziridine","137526-89-7","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]propanoyl fluoride","39187-44-5","D",0]
["2-[(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)oxy]acetamide","62656-66-0","D",0]
["Propanoic acid, 3-chloro-2,2,3,3-tetrafluoro-, methyl ester","127589-63-3","D",0]
["1-Chloro-2-[chloro(difluoro)methoxy]-1,1,2,2-tetrafluoroethane","37031-57-5","D",0]
["Sodium N-(2-methoxyethyl)-N-[(nonafluorobutyl)sulfonyl]glycinate","864069-36-3","D",0]
["Iron(6+) 5,5-bis(trifluoromethyl)oxolan-3-ide cyclopenta-1,3-diene-1,2,3,4,5-pentaide--carbon monooxide (1/1/1/2)","54657-44-2","D",0]
["4,4,5,5,6,6,7,7-Octafluoro-1-phenylhept-1-yn-3-ol","111832-10-1","D",0]
["Cyclopentane, (1,1,2,3,3,3-hexafluoropropyl)-","53005-31-5","D",0]
["(5E)-1,1,1,2,2,3,3,4,4-Nonafluorododec-5-ene","113999-54-5","D",0]
["1-Methoxy-4-(1,2,3,3,3-pentafluoroprop-1-en-1-yl)benzene","61855-64-9","D",0]
["Decanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-, methyl ester","307-79-9","D",0]
["N-(2,2,3,3,4,4,5,5-Octafluoropentyl)aniline","733-76-6","D",0]
["1,1,1,2,2,3,3,14,14,15,15,16,16,16-Tetradecafluorohexadecane","168169-26-4","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluoro-1,1-hexanediol","904037-24-7","D",0]
["(Heptafluoropropyl)carbonimidoyl","378-00-7","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)benzaldehyde","875306-42-6","D",0]
["1,1,1,2,2,5,5,6,6,6-Decafluorohexane","95576-25-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluorooctyl nonafluorobutane-1-sulfonate","187039-77-6","D",0]
["1-Ethoxy-1,1,2,3,3,3-hexafluoropropane","380-34-7","D",0]
["2,2-bis(trifluoromethyl)-3a,4-dihydro-3H-chromeno[4,3-b]pyrrole","63238-61-9","D",0]
["1-(1-Methyl-1H-indol-3-yl)thiolan-1-ium nonafluorobutane-1-sulfonate","867373-18-0","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-7-methyloctane","212957-52-3","D",0]
["({4-[(1,2,3,3,4,4,5,5,6,6,6-Undecafluorohex-1-en-1-yl)oxy]phenyl}methyl)phosphonic acid","63513-18-8","D",0]
["{[(Perfluorobutyl)sulfonyl]amino}-3-betaine","","D",0]
["6-(Perfluorobutyl)-3,3,5,5-tetrafluorohexanol 1-(dihydrogen phosphate) ammonium salt (1:2)","1025044-24-9","D",0]
["1-(3-Phenoxyphenyl)prop-2-yn-1-yl 1-(4-ethoxyphenyl)-2,2,3,3-tetrafluorocyclobutane-1-carboxylate","76660-88-3","D",0]
["3,3,4,4,5,5,5-heptafluoropent-1-yne","80337-25-3","D",0]
["(2-Cyclohexyl-1,1,2,2-tetrafluoroethyl)benzene","873013-82-2","D",0]
["8-Bromo-1,1,1,2,2,3,3,4,4-nonafluorooctane","38436-18-9","D",0]
["4-(1,1,1,2-Tetrafluoropropan-2-yl)phenol","1889949-46-5","D",0]
["Perfluoro(pentadecaoxypropylene)oxyethylene ","122998-72-5","D",0]
["2-[2,2-Bis(trifluoromethyl)hydrazinyl]-1,1,1,3,3,3-hexafluoropropan-2-ol","90177-78-9","D",0]
["2-(Pentafluoroethyl)-1H-benzimidazole","383-08-4","D",0]
["2-Ethyl-3,3,4,4,5,5,5-heptafluoropentan-1-amine--hydrogen chloride (1/1)","308-38-3","D",0]
["Borate(1-), tetrahydro-, sodium (1:1), reaction products with reduced polymd. Oxidized tetrafluoroethylene, hydrolyzed, diallyl ethers, polymers with 2,4,6,800-tetramethylcyclotetrasiloxane, Si -[3-(2-hydroxyethoxy)propyl] derivs. ","1214752-85-8","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol and 2,2'-iminodiethanol","161212-15-3","D",0]
["1-Bromo-2-(2-bromo-1,1,2,2-tetrafluoroethyl)cyclohexane","113688-50-9","D",0]
["5,6,6,7,7,8,8,8-Octafluoro-2-methylocta-2,4-diene","90292-28-7","D",0]
["(2,2,3,3-Tetrafluorocyclopropyl)benzene","922141-41-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-methylnonanenitrile","1274722-59-6","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)phosphonic acid diethyl ester","350608-55-8","D",0]
["1,1,2,3,4,4,5,6-octafluoro-2,3,5,6-tetrakis(trifluoromethyl)cyclohexane","84808-59-3","D",0]
["1,2,3,4-Tetrafluoro-5,6-bis(pentafluoroethyl)benzene","111864-95-0","D",0]
["N-[3-(Dimethylamino)propyl]-2-[(perfluorobutyl)ethylthio]acetamide","1513863-89-2","D",0]
["4,5-Dimethyl-2-(2,2,3,3-tetrafluoropropoxy)-1,3,2-dioxaphospholane","115044-88-7","D",0]
["1,1,1,2,2,3,3-Heptafluoro-6-hydroxy-7,7-dimethyloct-5-en-4-one--copper (2/1)","38926-19-1","D",0]
["5H-Octafluoropentanoyl fluoride","813-03-6","D",0]
["Ethyl 2-[(diphenylmethylidene)amino]-5,5,6,6,7,7,8,8,8-nonafluorooctanoate","125162-61-0","D",0]
["1,1-bis(Trifluoromethyl)methoxy-2-ethanol","63693-13-0","D",0]
["2,2,3,3-Tetrafluoropropyl 4-(4-phenyl-1,4-dihydropyrimido[1,2-a]benzimidazol-2-yl)benzene-1-sulfonate","169132-76-7","D",0]
["1,1,2,2-Tetrafluoro-1-iodo-2-(1,1,2,2-tetrafluoro-2-iodoethoxy)ethane","681-30-1","D",0]
["3,3'-(1,1,2,2,3,3-hexafluoropropane-1,3-diyl)bis[5-(pentafluoroethyl)-1,2,4-oxadiazole]","4368-75-6","D",0]
["1-{[2-(2,4-Dichlorophenyl)-4-(1,1,2,2-tetrafluoroethyl)-1,3-dioxolan-2-yl]methyl}-1H-1,2,4-triazole","134695-73-1","D",0]
["N-(2-Cyano-4-nitrophenyl)-1,2,2,3,3,4,4,5,5,6,6-undecafluorocyclohexanecarboxamide","107349-93-9","D",0]
["5-Chloro-1,3,3,4,4,6,6-heptafluoro-2-(trifluoromethyl)cyclohex-1-ene","87905-89-3","D",0]
["Perfluoropropane-1-sulfinic acid","359868-84-1","D",0]
["Ethyl 4,4-difluoro-5-[(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)oxy]pentanoate","1361253-41-9","D",0]
["N-[1,1,1,3,3,3-Hexafluoro-2-(4-fluorophenyl)propan-2-yl]acetamide","192572-87-5","D",0]
["Potassium 2‐(N‐methyl-perfluorodecanesulfonamido)acetate","84002-44-8","D",0]
["2-Amino-5,5,6,6,7,7,7-heptafluoroheptanoic acid","10325-10-7","D",0]
["Carbon monoxide; cyclopenta-1,3-diene; 2,2,3,3,4,4,4-heptafluorobutan-1-one; molybdenum","12153-65-0","D",0]
["Thiophene, 2,2'-(1,1,2,2,3,3-hexafluoro-1,3-propanediyl)bis-","21250-11-3","D",0]
["N-methyl-N-[(3-octadecyl-2-oxo-4-oxazolidinyl)methyl]perfluorooctanesulfonamide","348144-85-4","D",0]
["N-(2-Hydroxyethyl)-3-[(2-hydroxyethyl)[(perfluoroethyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","2089108-97-2","D",0]
["N~5~-(5-Hydroxy-4,6-dimethylpyrimidin-2-yl)-L-ornithine--heptafluorobutanoic acid (1/2)","936233-19-1","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with 6-aminocaproic acid","161212-27-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Nonadecafluorooctadecane","1287702-47-9","D",0]
["3,3,4,4,5,5,6,6,7,7,7-Undecafluoroheptan-1-amine","1346521-42-3","D",0]
["4,7,10,13-Tetraoxahexadecane, 1,1,1,2,2,3,3,5,6,6,8,9,11,11,12,14,14,15,15,16,16,16-docosafluoro-5,8,9,12-tetrakis(trifluoromethyl)-","61098-00-8","D",0]
["2-Amino-2H-perfluoropropane","1619-92-7","D",0]
["1,1-Dichloro-1,3,3,4,4,4-hexafluorobutan-2-one","87375-48-2","D",0]
["4,4,5,5,5-Pentafluoropent-1-ene","135671-20-4","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-phenylhexane-1,3-dione","53580-21-5","D",0]
["1,2,2,3,3,3-Hexafluoropropane-1,1-diyl dihypofluorite","72985-54-7","D",0]
["1-Chloro-2-(difluoromethoxy)-1,1,2,3,3,3-hexafluoropropane","60632-00-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,25,25,26,26,27,27,28,28,29,29,30,30,31,31,32,32,33,33,34,34,35,35,36,36,36-Pentacontafluoro-14,23-diiodohexatriacontane","1980039-13-1","D",0]
["Chromium pentacarbonyl[perfluoro-4-(isocyano-βC)butane]","106065-05-8","D",0]
["2-Propenamide, telomer with 1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-6-iodohexane","105960-50-7","D",0]
["4,5,5,5-Tetrafluoro-4-(heptafluoropropoxy)pentan-1-ol","243128-41-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-(pentyloxy)octane","1193009-93-6","D",0]
["2-(Heptadecafluorooctyl)-1H-pyrrole","80791-17-9","D",0]
["1,1,1,2,2,3,3-Heptafluorooct-4-ene","2707-72-4","D",0]
["2,3,3,5,5,6,6,8,8,10,10,12,12,12-Tetradecafluoro-4,7,9,11-tetraoxadodecanoic acid","919005-22-4","D",0]
["N,N-dimethyl-2H-perfluoroethanamine","1550-50-1","D",0]
["Perfluorodimethyladamantane","55949-22-9","D",0]
["(Perfluoroheptyl)methanesulfonic acid","812-79-3","D",0]
["5,5,6,6-Tetrafluorobicyclo[2.2.1]hept-2-ene","2822-56-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-7-methyl-7-nitrooctane","84108-41-8","D",0]
["1-Hydroxy-5:2 fluorotelomer sulfonic acid","2089110-00-7","D",0]
["3-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)oxy]propanenitrile","56300-32-4","D",0]
["2-Propenoic acid, 2-methyl-, pentafluoroethyl ester, homopolymer","88473-49-8","D",0]
["2,2,4,4-Tetrafluorooxetane","154330-40-2","D",0]
["N-(Carboxymethyl)-N,N-diethyl-3-[propyl[(perfluorohexyl)sulfonyl]amino]-1-propanaminium","138473-80-0","D",0]
["1-[4-(Tridecafluorohexyl)phenyl]pyridin-4(1H)-one","821789-63-3","D",0]
["5,5,5-Trifluoro-4-(trifluoromethyl)penta-1,3-diene","1422-33-9","D",0]
["N-(Carboxylatomethyl)-N,N-dimethyl-4-[[perfluoro-2-[1-(methyl)ethyl]-1,3-dimethyl-1-buten-1-yl]oxy]benzenaminium","927408-19-3","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethoxy)propanamide","67710-48-9","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol and octadecylamine","161308-21-0","D",0]
["6-Methyl-3-[4,4,4-trifluoro-3-hydroxy-3-(trifluoromethyl)butanoyl]-2H-pyran-2,4(3H)-dione","102129-07-7","D",0]
["Ammonium bis(5,5,6,6,7,7,8,8,8-nonafluoro-1-octyl) phosphate","3803-40-5","D",0]
["4,4,4-Trifluoro-3-(trifluoromethyl)buta-1,2-diene-1-diazonium","918108-34-6","D",0]
["2-Propenenitrile, polymer with .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene), .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-methoxypoly(oxy-1,2-ethanediyl) and  .alpha.-(2-methyl-1-oxo-2-propenyl)-.omega.-[(2-methyl","374928-93-5","D",0]
["1,2-Bis(2-methyl-5-phenyl-3-thienyl)perfluorocyclopentene","182003-69-6","D",0]
["2,2,3,3,3-Pentafluoropropyl 2-fluoroprop-2-enoate","96250-35-0","D",0]
["(8-Pentafluoro(5)sulfide)-perfluorooctanoic acid","2269495-20-5","D",0]
["(3S,4S)-1,1,1,2,2,3,4,5,5,5-Decafluoropentane","1006614-97-6","D",0]
["(2S)-2-[Chloro(fluoro)methoxy]-1,1,1,2-tetrafluoroethane","1933757-76-6","D",0]
["3,3,4,4-Tetrafluorobutan-2-one","679-97-0","D",0]
["2-({[1-(4-tert-Butylcyclohexyl)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl]oxy}carbonyl)hydrazine-1-carboxylate","821806-50-2","D",0]
["Methyl 4H-perfluorobutyl ketone","93449-49-1","D",0]
["2,2,2-Trifluoroethyl heptafluorobutanoate","336-63-0","D",0]
["Methoxydimethyl(3,3,4,4,4-pentafluorobutyl)silane","252653-06-8","D",0]
["Perfluoro-2-butenesulfonic acid","2089109-39-5","D",0]
["2,2,3,3,4,4,4-heptafluoro-N-heptan-2-ylbutanamide","61578-74-3","D",0]
["1,8-Dibromo-1,1,2,2,7,7,8,8-octafluorooctane","127117-28-6","D",0]
["1,1,2,2-Tetrafluoro-2-(undecafluorocyclohexyl)ethane-1-sulfonic acid","646-81-1","D",0]
["(2Z)-3-Fluoro-3-(perfluoropentyl)acrylic acid","161094-75-3","D",0]
["2-({1-[1,2,2-Trifluoro-2-(2,2,2-trifluoroethoxy)ethoxy]perfluoropropan-2-yl}oxy)perfluoroethane-1-sulfinate sodium","187480-47-3","D",0]
["6:4 Fluorotelomer sulfonic acid","741190-96-5","D",0]
["2,2,3,5,5,6-Hexafluoro-3,6-bis(trifluoromethyl)-1,4-dioxane","137373-27-4","D",0]
["1,1,2,3,3,4,4,5,5,6,6,7,7-Tridecafluoro-2-(trifluoromethyl)-2,3,4,5,6,7-hexahydro-1H-indene","112754-13-9","D",0]
["2-[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy]-5-nitropyridine","917924-00-6","D",0]
["1,1,2,2-Tetrafluoro-2-[(1,1,1,2,3,3,4,4-octafluorobutan-2-yl)oxy]ethane-1-sulfonic acid","2416366-21-5","D",0]
["Heptanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoro- (9CI)","548434-15-7","D",0]
["(Heptafluoropropoxy)(trimethyl)silane","106609-54-5","D",0]
["2-Hydroxyethyl 4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoronon-1-en-1-yl)oxy]benzoate","62623-11-4","D",0]
["Ethyl 6-(heptafluoropropyl)pyridine-3-carboxylate","1574401-92-5","D",0]
["Oxirane, 2-[[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]methyl]-","122193-68-4","D",0]
["4,7,10,13-Tetraoxahexadecane, 1,1,1,2,2,3,3,5,6,6,8,9,9,11,12,14,14,15,15,16,16,16-docosafluoro-5,8,11,12-tetrakis(trifluoromethyl)-","127003-77-4","D",0]
["Perfluoro-2-octene","65500-50-7","D",0]
["N-Allylperfluoro-2-propoxypropanamide","165663-65-0","D",0]
["4-chloro-3-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-5-methyl-1H-pyrazole","232587-49-4","D",0]
["2-(2,2,3,3-Tetrafluoropropoxy)-1,3,2-dioxaphospholidine","115044-87-6","D",0]
["Perfluoroheptadecanoic acid","57475-95-3","D",0]
["2,2,3,3,4,4,4-Heptafluorobutane-1-sulfonic acid","687997-50-8","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl]-ω-hydroxy-","52701-06-1","D",0]
["Perfluoroheptadecanesulfonic acid","865756-92-9","D",0]
["(2E)-1,1,1,2,4,4,5,5,5-Nonafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pent-2-ene","58621-72-0","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-Icosafluoro-11-(trifluoromethyl)dodecan-1-ol","194427-39-9","D",0]
["Tetrakis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)stannane","96325-98-3","D",0]
["5,5,5,5',5',5'-Hexafluoroleucine--hydrogen chloride (1/1)","16198-60-0","D",0]
["1-Methyl-(2-(perfluorohexyl)ethyl)silanediol","156048-37-2","D",0]
["3,5-bis(heptafluoropropyl)-1,2,4-oxadiazole","4314-46-9","D",0]
["3,3,4,5,5,6,7,8,9-Nonafluoro-2,3,4,5-tetrahydro-1-benzoxepine","184362-57-0","D",0]
["2,2,3,4,4,5,5,6,6,7,8,8,8-Tridecafluoro-3,7-bis(trifluoromethyl)octan-1-ol","232587-50-7","D",0]
["Propane, 2,3-dichloro-1,1,1,2,3-pentafluoro-","422-48-0","D",0]
["2,3-Difluoro-2-(1,2,2,2-tetrafluoro-1-trifluoromethyl-ethyl)-3-trifluoromethyl-oxirane","","D",0]
["2-Buten-1-one, 1-(9-anthryl)-4,4,4-trifluoro-3-trifluoromethyl-","100482-56-2","D",0]
["Difluoro(1,1,2,2-tetrafluoro-2-iodoethoxy)acetic acid","81233-12-7","D",0]
["P,P-Bis(perfluoro-7-methyloctyl) phosphinothioic acid erbium(3+) salt (3:1)","500776-89-6","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-phenylethyl)butanamide","29723-29-3","D",0]
["(1,1,2,2,3,3,4,4-Octafluoro-4-iodobutyl)benzene","17667-12-8","D",0]
["(-)-1-Perfluoropropylethanol","85571-83-1","D",0]
["1,1,1,2,2-pentafluoro-2-methoxyethane","22410-44-2","D",0]
["1,2,2,3,3,4,4,5,5,6,6-Undecafluorocyclohexane-1-carbonyl chloride","58816-79-8","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol","161212-23-3","D",0]
["Methyl 4,4,5,5-tetrafluoro-3-oxopentanoate","89129-67-9","D",0]
["Sodium 1-[(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl)oxy]-3-(2,2,3,3-tetrafluoropropoxy)-2-propanol 2-sulfate","61119-61-7","D",0]
["Octakis(trifluoromethyl)-1,4,6,9-tetraoxa-5lambda4-telluraspiro[4.4]nonane","23542-72-5","D",0]
["Perfluoro-5-methylindan","36158-86-8","D",0]
["Perfluorooctaneamido ammonium","45305-66-6","D",0]
["Sodium {[2-(dimethylamino)ethyl](1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)amino}acetate","96426-90-3","D",0]
["3,3'-Diamino-N,N'-[perfluoropropane-2,2-diylbis(6-hydroxy-3,1-phenylene)]dibenzamide","220426-92-6","D",0]
["Ethyl [(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]acetate","138224-54-1","D",0]
["3,5,6-Trifluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridin-2-amine","55181-17-4","D",0]
["Lithium 3-[butyl[(perfluorobutyl)sulfonyl]amino]propanesulfonate","864069-43-2","D",0]
["5-Bromo-3,5-dichloro-2,2,3,4,4,5-hexafluoropentanoyl chloride","88639-63-8","D",0]
["1,1,1-Trifluoro-4-(4-methylphenyl)-2-(trifluoromethyl)pentane-2,4-diol","101931-59-3","D",0]
["2,2,3,3-Tetrafluoro-3-(methanesulfonyl)propanoic anhydride","92519-33-0","D",0]
["(2-(F-Octyl)ethyl) dimorpholinophosphoramidate","134051-90-4","D",0]
["Nonafluorobutane-1-sulfonoperoxoic acid","85963-79-7","D",0]
["2,2,3,3-Tetrafluorocyclopropane-1-carboxylic acid","344324-87-4","D",0]
["Methyl heptadecafluorononanoate","51502-45-5","D",0]
["2-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-(2-propenylamino)-","89807-93-2","D",0]
["3,3,4,4,5,5-Hexafluoro-1,2lambda~6~,6lambda~6~-oxadithiane-2,2,6,6-tetrone","82727-20-6","D",0]
["2-[Dimethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)azaniumyl]acetate","145441-31-2","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-[(propan-2-yl)sulfanyl]benzoic acid","1355554-05-0","D",0]
["[Difluoro(pentafluorophenyl)methoxy](difluoro)acetyl fluoride","194983-26-1","D",0]
["2(2H-Perfluoro-2-propyl)acetic acid","17327-33-2","D",0]
["3-(4-Chloro-2-fluorobenzamido)-2-fluoro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","862133-16-2","D",0]
["3,3,5-Trichloro-1,1,1,2,2-pentafluoropentane","18621-12-0","D",0]
["Hexafluoroglutaramide","507-68-6","D",0]
["4-Chloro-3-(heptafluoropropyl)-5-methylpyrazole","247170-22-5","D",0]
["3-{2-[Bis(1,1,2,2-tetrafluoro-2-hydroxyethyl)amino]phenyl}prop-2-enal","192082-41-0","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxine-6,7-diamine","110968-70-2","D",0]
["Perfluoro-4-(2-(fluorosulfonyl)ethoxy)pentanoyl fluoride","82761-28-2","D",0]
["2-{1,2,2,2-Tetrafluoro-1-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]ethyl}-1H-benzimidazole","76145-90-9","D",0]
["4-Methyl-3-(pentafluoroethyl)-1,2-oxazol-5-amine","110234-59-8","D",0]
["Perfluorodecyl dihydrogen phosphate","97802-61-4","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluoro-2-methyldecan-2-ol","159142-65-1","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl dimethylphosphinite","69128-04-7","D",0]
["2-Propanol, 2-[(diphenylphosphino)methyl]-1,1,1,3,3,3-hexafluoro-","98331-76-1","D",0]
["2,6-Dibromo-4-(1,1,2,3,3,3-hexafluoropropoxy)aniline","917924-08-4","D",0]
["1H,2H,2H-Perfluorobutane","86884-16-4","D",0]
["2-chloro-2,3,3,3-tetrafluoropropanoyl fluoride","28627-00-1","D",0]
["N,N-Diethyl-2,2,3,3,4,4,4-heptafluorobutanamide","377-58-2","D",0]
["6-(2,2,3,3,4,4,4-Heptafluorobutoxy)hexan-1-ol","1207481-10-4","D",0]
["2,4-Dimethoxy-5-(nonafluorobutyl)pyrimidine","71623-69-3","D",0]
["Triethoxy[3-[(perfluoroheptyl)methoxy]propyl]silane","19116-62-2","D",0]
["Ethanesulfonyl chloride, 1,1,2,2-tetrafluoro-2-[(trifluoroethenyl)oxy]-","27009-57-0","D",0]
["1-Bromo-4-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)benzene","195324-87-9","D",0]
["7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-heptadecafluorotetradecan-1-ol","129794-54-3","D",0]
["(5E)-1,1,1,2,2,3,3,4,4-Nonafluorotetradec-5-ene","104504-30-5","D",0]
["4-(Pentafluoroethyl)-2,3-dihydro-1H-inden-1-one","1380390-11-3","D",0]
["Perfluoroheptane-1-sulfinic acid","769067-51-8","D",0]
["Tricyclo[8.2.2.24,7]hexadeca-4,6,10,12,13,15-hexaene, 2,2,3,3,8,8,9,9-octafluoro-","3345-29-7","D",0]
["1-Chloro-1,1,2,2-tetrafluoropropane","421-75-0","D",0]
["1-Ethenyl-2,3,5,6-tetrafluoro-4-(2,2,3,3,3-pentafluoropropoxy)benzene","121247-90-3","D",0]
["N-(Perfluoro-1-oxobutyl)aspartic acid 1-propyl ester","88436-09-3","D",0]
["Ethyl 3-[(2-ethoxy-2-oxoethyl)amino]-4,4,5,5,6,6,7,7,7-nonafluoroheptanoate","132114-64-8","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol and 2-aminoethanol","161212-14-2","D",0]
["2,2-Difluoro-3-(heptafluoropropoxy)propanoic acid","824393-34-2","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentanal hydrate (1:1)","1208950-63-3","D",0]
["Magnesium bromide 1,1,2,2,3,3,4,4,4-nonafluorobutan-1-ide (1/1/1)","82416-69-1","D",0]
["2,4-Difluoro-6-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-1,3,5-triazine","10271-35-9","D",0]
["(7E)-9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,16-Heptadecafluorohexadec-7-ene","84201-60-5","D",0]
["Perfluorodecahydro-1-sec-butylnaphthalene","118945-64-5","D",0]
["TRIS(1H,1H,2H,2H-PERFLUOROOCTYL)TIN AZIDE","201740-73-0","D",0]
["2,4,6,8-Tetramethyl-2-[3-(2-oxiranylmethoxy)propyl]-4,6-bis[3-[(perfluoro(2-[2-(propoxy)propoxy]-2-ethyl))methoxyl]propyl]cyclotetrasiloxane","1428232-89-6","D",0]
["Methyl 2,2-bis(trifluoromethyl)cyclopropane-1-carboxylate","61860-01-3","D",0]
["2-(3-Nitro-1H-1,2,4-triazol-1-yl)-N-(2,2,3,3,3-pentafluoropropyl)acetamide","919477-86-4","D",0]
["Nonafluorobutane-1-thiol","125870-53-3","D",0]
["3,3-Dichloro-1,1,1,4,4,4-hexafluoro-2-(trifluoromethyl)butan-2-ol","137788-48-8","D",0]
["N-((2-Bromo-4-(1,1,2,2-tetrafluoroethylsulfanyl)phenyl]carbamoyl]-2,6-difluorobenzamide","100279-89-8","D",0]
["bis((Perfluoropropyl)methyl) phosphorochloridoate","6780-81-0","D",0]
["(Carboxymethyl)dimethyl[3‐(perfluorohexanesulfonamido)propyl]azanium","2089109-24-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,15,15,16,16,17,17,18,18,19,19,20,20,21,21,22,22,22-Tetratriacontafluorodocosane","959462-55-6","D",0]
["3-(Heptafluoropropyl)pentanedioic acid","336-32-3","D",0]
["2,2-Bis(trifluoromethyl)propionyl fluoride","1735-87-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-Pentadecafluoro-7-isocyanatoheptane","335-91-1","D",0]
["N'-[(2Z)-5,5,6,6,7,7,7-Heptafluoro-4-oxo-2-heptanylidene]-4-methylbenzohydrazide","1087654-74-7","D",0]
["Benzenesulfonic acid, 2-[2-[4-[[2-(acetyloxy)ethyl]ethylamino]phenyl]diazenyl]-5-nitro-, 2,2,3,3-tetrafluoropropyl ester","143877-58-1","D",0]
["3-(Perfluoropropyl)-2-propanone","136909-72-3","D",0]
["2-(Heptafluoropropyl)-4-(propan-2-yl)pyrimidine-5-carboxylic acid","914201-18-6","D",0]
["tert-Butyl pentafluoropropionate","55258-28-1","D",0]
["4H-1,2-Diazepine, 5,6-dihydro-3,7-diphenyl-5,5-bis(trifluoromethyl)-","62284-32-6","D",0]
["(2Z)-4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-iodonon-2-en-1-ol","99325-08-3","D",0]
["1,1,1-Trifluoro-4-(phenylsulfanyl)-2-(trifluoromethyl)but-3-en-2-ol","96569-51-6","D",0]
["N-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)hypochlorous amide","10181-78-9","D",0]
["Cyclohexane, 1,1,2,2,3,3,4,4,5,5,6-undecafluoro-6-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heneicosafluorodecyl)-","87667-00-3","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)carbonimidoyl","142030-27-1","D",0]
["2,3,5,6-Tetrafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzonitrile","20017-54-3","D",0]
["3,3'-(3,3,4,4,5,5-Hexafluorocyclopent-1-ene-1,2-diyl)bis(2,4-dimethylthiophene)","170658-51-2","D",0]
["1-(Butylsulfanyl)-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane","89883-20-5","D",0]
["6,6,7,7,8,8,9,9,9-Nonafluorononan-1-ol","219557-62-7","D",0]
["1-Docosanylperfluoroheptane","1980063-14-6","D",0]
["4-(Heptadecafluorooctyl)benzaldehyde","134641-35-3","D",0]
["1H,1H,13H-Perfluorotridecan-1-ol","423-72-3","D",0]
["1,1,2,2,3,3-Hexafluoro-1-iodopropane","58706-58-4","D",0]
["2,2,3,3,3-Pentafluoro-1-(10H-phenothiazin-10-yl)propan-1-one","141135-78-6","D",0]
["Nonanamide, 9-chloro-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","545349-84-6","D",0]
["(3R,4S)-1,1,1,2,2,3,4,5,5,5-Decafluoropentane","1006614-96-5","D",0]
["Phenyl (2-chloro-1,1,2,2-tetrafluoroethoxy)(difluoro)acetate","83865-19-4","D",0]
["2,3,3,3-Tetrafluoro-1-[2,3,5,6-tetrafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)phenyl]-2-(trifluoromethyl)propan-1-one","19547-30-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl chloroacetate","87925-99-3","D",0]
["2‐{Diethyl[3‐(N‐propyl-perfluorooctanesulfonamido)propyl]azaniumyl}acetate","69091-22-1","D",0]
["1,1,1,2,2,3,3,4,4,6,6-Undecafluoro-8-iodooctane","53626-95-2","D",0]
["3-Ethenyl-1,1,2-trifluoro-2-(1,1,2,2-tetrafluoro-2-{1,1,2,2-tetrafluoro-2-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]ethoxy}ethoxy)cyclobutane","709620-35-9","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reduced, reaction products with 2,3-epoxypropan-1-ol","161075-09-8","D",0]
["(Perfluorohexanesulfonyl)[3‐(trimethylazaniumyl)propyl]azanide","38850-51-0","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-hydroxybutanamide","87050-96-2","D",0]
["Phenol, 2,2'-[(1R,2R)-1,2-cyclohexanediylbis[(E)-nitrilomethylidyne]]bis[6-(1,1-dimethylethyl)-4-(heptadecafluorooctyl)-","417715-98-1","D",0]
["1,1,1,2-Tetrafluoro-2-(1,1,2,2-tetrafluoroethoxy)ethane","51410-38-9","D",0]
["Methacrylic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, polymer with 2-(diethylamino)ethyl methacrylate","34438-51-2","D",0]
["Heptafluorobutanoic acid--piperazine (1/1)","375-04-2","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(methylsulfanyl)benzoic acid","1355553-97-7","D",0]
["Tridecafluorohexane-1-sulfinyl chloride","61424-51-9","D",0]
["(4-Fluorophenyl)[4-(1,1,2,3,3,3-hexafluoropropoxy)phenyl]methanone","143526-19-6","D",0]
["3-(Butane-1-sulfinyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355554-97-0","D",0]
["Ethenyl perfluoroheptanoate","240408-96-2","D",0]
["Pentafluoroethane mixture with difluoromethane and 1,1,1,2-tetrafluoroethane","158675-78-6","D",0]
["Methacrylic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl ester, polymer with 2-(diethylamino)ethyl methacrylate","34447-80-8","D",0]
["Perfluoro-3,6,9-trioxaundecanoic acid","80153-83-9","D",0]
["4-Bromo-2-fluoro-1-(1,1,2,3,3,3-hexafluoropropoxy)benzene","161045-76-7","D",0]
["7,7,8,8,9,9,10,10-Octafluoro-2-methyldecane-4,6-dione","62679-43-0","D",0]
["Trichloro[5,5,6,6,7,7,8,8,9,9,10,10,10-tridecafluoro-2-(tridecafluorohexyl)decyl]silane","1621953-16-9","D",0]
["[4,4,4-Trifluoro-3-(trifluoromethyl)but-2-en-1-ylidene]propanedinitrile","60935-07-1","D",0]
["Phosphonic acid, [3-[ethyl[(pentadecafluoroheptyl)sulfonyl]amino]propyl]-, diethyl ester","71463-81-5","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propylamino]ethyl ester, polymer with .alpha.-(2-methyl-1-oxo-2-propen-1-yl)-.omega.-methoxypoly(oxy-1,2-ethanediyl)","73019-28-0","D",0]
["3,5,7,8-tetrachloro-2,2,3,4,4,5,6,6,7,8,8-undecafluorooctanoic acid- aniline(1:1)","1534-91-4","D",0]
["O-(2,2,3,3,4,4,4-Heptafluorobutyl) methylphosphonothioate","61631-26-3","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-3-(methanesulfonyl)-2-methylbenzoic acid","1355554-41-4","D",0]
["3,3'-sulfanediylbis(4,4,5,5,6,6,6-heptafluorohexanoic acid)","312-14-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-13-iodotridecane","541547-94-8","D",0]
["Propanoic acid, 3-[1-[difluoro[(1,2,2-trifluoro ethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, methyl ester, polymer with 4,5-difluoro-2,2-bis(trifluoromethyl)-1,3-dioxole and 1,1,2,2-tetrafluoroethene","86179-28-4","D",0]
["1,1,2,2-Tetrafluoro-1-(fluoromethoxy)ethane","37031-31-5","D",0]
["N,N-Diethyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononanamide","90403-88-6","D",0]
["Perfluoro-6-oxoheptane-1-sulfonic acid","2254560-27-3","D",0]
["Perfluoro-3,5,5-trimethylhexanoic acid","238403-51-5","D",0]
["Diethyl 1,1,1,2,2,3-hexafluoro-7-methyloct-3-en-4-yl phosphate","113138-46-8","D",0]
["3,3,4,4,5,6,6-Heptafluorohex-5-en-1-ol","97168-16-6","D",0]
["4,5,6,7-Tetrachloro-1,1,3,3-tetrafluoro-1,3-dihydro-2-benzofuran","20687-94-9","D",0]
["2-(Chloromethoxy)-1,1,1,3,3,3-hexafluoropropane","26103-07-1","D",0]
["heptafluorobutanoic acid- 1-phenylpiperazine(1:1)","2263-11-8","D",0]
["2,2'-(2-Iodo-5-methyl-1,3-phenylene)bis(hexafluoropropan-2-ol)","80360-43-6","D",0]
["Methyl 2,2,3,3-tetrafluoro-3-{1,1,2,3,3,3-hexafluoro-2-[(trifluoroethenyl)oxy]propoxy}propanoate","73122-14-2","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-undecylbutanamide","120253-76-1","D",0]
["N-[2-(1,1,2,3,3,3-Hexafluoropropoxy)phenyl]-2,2-diphenylacetamide","5927-82-2","D",0]
["2-Methylpropyl 3,3,3-Trifluoro-2-(trifluoromethyl)propanoate","62935-20-0","D",0]
["N-[[3-[[(Perfluorooctyl)sulfonyl](propyl)amino]propyl]sulfonyl]-2-hydroxy-N,N-dimethylethanaminium chloride","90179-38-7","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,4,4-heptafluoro-4-[(1,2,2-trifluoroethenyl)oxy]-3-(trifluoromethyl)-, polymer with 1,1,2,2-tetrafluoroethene","130667-20-8","D",0]
["7-Bromo-1,1,1,2,2,3,3-heptafluoroheptane","1391033-22-9","D",0]
["Sulfate(1-), (3-carboxylato-1,1,2,2,3,3-hexafluoropropyl)pentafluoro-, (OC-6-21)-","786610-98-8","D",0]
["5-(2-Chloro-1,1,2-trifluoroethoxy)-1,1,2,2,3,3,4,4-octafluoropentane","65064-84-8","D",0]
["Iodonium, phenyl[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-, 1,1,1-trifluoromethanesulfonate (1:1)","82959-18-0","D",0]
["2-Bromo-2-cyanohexafluoropropane","52198-56-8","D",0]
["(Perfluorooctanesulfonyl)[3‐(trimethylazaniumyl)propyl]azanide","38850-50-9","D",0]
["4,4-Bis(trifluoromethyl)piperidine--water (1/1)","63867-63-0","D",0]
["1,1,1,2,2-pentafluoroheptan-3-one","426-66-4","D",0]
["1,1,2,2-Tetrafluoro-1-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]-2-(trifluoromethoxy)ethane","40891-99-4","D",0]
["3-[[(Perfluorononyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium bromide","329354-03-2","D",0]
["(4E)-1,1,1,2,2,3,3-Heptafluoro-4-nonene","57325-40-3","D",0]
["2,2,3-Trifluoro-3-(trifluoroethenyl)-4,4-bis(trifluoromethyl)oxetane","400629-07-4","D",0]
["N-(Carboxylatomethyl)-N-methyl-N-(3-sulfonatopropyl)-3-[[(perfluorohexyl)sulfonyl]amino]-1-propanaminium chloride, sodium salt (1:1:2)","86402-38-2","D",0]
["Ethyl 4,4,5,5,6,6,7,7,7-nonafluoro-3-oxoheptanoate","82941-37-5","D",0]
["2-Quinolineethanol, alpha,alpha-bis(trifluoromethyl)-6-(dimethylamino)-","102259-70-1","D",0]
["2-Chloro-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridine","1807450-20-9","D",0]
["1-Ethoxy-2,2,3,3,3-pentafluoropropyl 4-methylbenzene-1-sulfonate","31185-48-5","D",0]
["2-Pentanone, 4-hydroxy-1-phenoxy-5,5,5-trifluoro-4-(trifluoromethyl)-","34844-32-1","D",0]
["2,3,4,5,6-Pentakis(1,1,2,2,2-pentafluoroethyl)-1-azabicyclo[2.2.0]hexa-2,5-diene","30567-91-0","D",0]
["3-(Perfluoroisopropyl)-difluoro-2-propenoic acid","239795-58-5","D",0]
["(4E)-1,1,1,2,2,3,3-Heptafluorodec-4-ene","57325-42-5","D",0]
["2,3,3,3-Tetrafluoropropanoic Acid","359-49-9","D",0]
["2,2,3,3,4,4,5,5-octafluoropentyl trifluoromethanesulfonate","17352-10-2","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-1,6-bis[(trifluoroethenyl)oxy]hexane","69818-04-8","D",0]
["3,3,4,5,5,5-Hexafluoropentane-1,2-diol","121628-30-6","D",0]
["1,2,4,5-Tetrafluoro-3,6-bis(2,2,3,3-tetrafluoropropoxy)benzene","89847-88-1","D",0]
["(E)-1-(Pyridin-3-yl)-N-[2-(1,1,2,2-tetrafluoroethoxy)phenyl]methanimine","89985-39-7","D",0]
["Methyl (2R,3S)-3-(pentadecafluoroheptyl)oxirane-2-carboxylate","184007-51-0","D",0]
["Perfluoroheptanesulfonate","146689-46-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluoroheptane","503189-10-4","D",0]
["Perfluoro-3-oxanonane-1-sulfonic acid","754925-54-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-hydroxy-N-methylbutanamide","193008-44-5","D",0]
["Perfluorosebacamidine","865-94-1","D",0]
["N,N-Diethyl-2,3,3,4,4,5,5,6,6,6-decafluorohexanamide","60895-98-9","D",0]
["1-Iodo-8H-perfluorooctane","79162-64-4","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium fluoride","73149-43-6","D",0]
["2-Butene, 4-chloro-1,1,1-trifluoro-2-(trifluoromethyl)-","163773-92-0","D",0]
["Perfluoro-2,5,8,11-tetraoxadodecane","64028-04-2","D",0]
["Benzene, 1,1'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis[4-isocyanato-","10224-18-7","D",0]
["N-[3-(Dimethylamino)propyl]-2-[(perfluorododecyl)ethylthio]acetamide","1513863-93-8","D",0]
["Thioacetic acid S-(4,4,5,5,5-pentafluoro-pentyl)ester","160598-75-4","D",0]
["2-bromo-3,4,4,4-tetrafluoro-3-(trifluoromethoxy)but-1-ene","231291-19-3","D",0]
["tert-Butyl 3,3,4,4-tetrafluoropyrrolidine-1-carboxylate","1392502-17-8","D",0]
["2-(1,1,2,2,3,3,4,4-Octafluorobutyl)-1,3,6-triazocane","184773-24-8","D",0]
["cis-1-Iodo-2-(heptafluoropropyl)cyclohexane","7589-43-7","D",0]
["2-Propenoic acid, 4,4,5,5,6,6,7,7,7-nonafluoro-2-hydroxyheptyl ester, polymer with 2-propene-1-sulfonic acid","910114-99-7","D",0]
["1-(1,1,2,2-Tetrafluoroethyl)cyclohexanecarboxylic acid","144194-04-7","D",0]
["1-[bromo(1,1,2,2,3,3,4,4,4-nonafluorobutylsulfonyl)methyl]sulfonyl-1,1,2,2,3,3,4,4,4-nonafluorobutane","30416-81-0","D",0]
["4-(Pentafluoroethyl)benzonitrile","128273-61-0","D",0]
["5-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1H-imidazole","81790-01-4","D",0]
["Butyrophenone, 3-chloro-3'-nitro-4,4,4-trifluoro-3-trifluoromethyl-","100700-44-5","D",0]
["Ammonium 2-[methyl-2-(perfluoropentyl)ethylamino]ethanol hydrogen phosphate","138473-76-4","D",0]
["2,2,2-Trifluoro-N-(tetrafluoroethylidene)ethanehydrazonoyl fluoride","88579-80-0","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)propanal","4074-09-3","D",0]
["1-Fluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzene","2396-25-0","D",0]
["7-Hydroxy-4,9-dimethoxy-7-(nonafluorobutyl)-6,7-dihydro-5H-furo[3,2-g][1]benzopyran-5-one","376382-61-5","D",0]
["1,1,1,2,2,3,4,4,5,5,5-Undecafluoro-3-(fluoroperoxy)pentane","828259-48-9","D",0]
["4:2 Fluorotelomer sulfonic acid","757124-72-4","D",0]
["2,2,3,3,3-Pentafluoro-N-(2-phenylethyl)propanamide","13230-93-8","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[[(perfluorobutyl)sulfonyl]amino]-1-propanaminium","2089109-09-9","D",0]
["N-Ethyl-N-[(heptadecafluorooctyl)sulfonyl]acrylamide","1869-69-8","D",0]
["4-[(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)oxy]phenol","140218-18-4","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-N-(2-hydroxyethyl)pentanamide","313535-73-8","D",0]
["1,2-Dichloro(perfluoro-1-[(2-methoxyethoxy)methoxy]ethane)","369371-43-7","D",0]
["Bis[(1,1,1,3,3,3-hexafluoropropan-2-yl)oxy](oxo)phosphanium","120104-57-6","D",0]
["1-(4-Bromophenyl)-2,2,3,3,4,4,5,5,5-nonafluoropentan-1-one","1228786-80-8","D",0]
["N-Cyclohexyl-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptanamide","73602-45-6","D",0]
["4-(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptyl)-1,3-dioxolan-2-one","114810-52-5","D",0]
["3,3-Bis(trifluoromethyl)-4,5-dihydro-3H-pyrazole-4-carbonitrile","61859-91-4","D",0]
["2-Cyano-2,3,3,3-tetrafluoropropanoyl fluoride","54675-68-2","D",0]
["1,1,1,2,2,4-Hexafluorobutane","161791-32-8","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reaction products with ammonia","161075-04-3","D",0]
["5,6-Dibromo-1,1,2,3,3,4,4,5,6,6-decafluorohex-1-ene","91095-94-2","D",0]
["(3,3,4,4-Tetrafluorocyclobut-1-en-1-yl)benzene","313-28-0","D",0]
["(3,3,4,4,5,5,5-Heptafluoropent-1-yn-1-yl)benzene","81674-08-0","D",0]
["Benzenamine, 3,3'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis[6-methyl-","116325-74-7","D",0]
["Nonafluorobutylphosphonous difluoride","127223-44-3","D",0]
["10-Chloro-perfluorodecanoic acid","574715-86-9","D",0]
["5-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1,3-dihydro-2H-benzimidazol-2-one","1433216-51-3","D",0]
["S-(1,1,2,2,3,3-Hexafluoropropyl)-L-cysteine","98640-41-6","D",0]
["N,N,N-Triethyl-3-[[(perfluorooctyl)sulfonyl]amino]-1-propanaminium sulfate (1:1)","153968-03-7","D",0]
["Perfluoro-2-butyl-3-propyloxaziridine","143813-70-1","D",0]
["Perfluoro-2-[1-[(1,2-dichloroethoxy)methyl]ethoxy]ethanesulfonic acid potassium","183238-50-8","D",0]
["Oxirane, 2,2'-(2,2,3,3,4,4,5,5-octafluoro-1,6-hexanediyl)bis-","791-22-0","D",0]
["1,3-Bis[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoronon-1-en-1-yl)oxy]benzene","55987-23-0","D",0]
["N-[(4-Bromophenyl)(perfluorobutyl)oxido-λ4-sulfanylidene]-1,1,1-trifluoromethanesulfonamide","1421133-01-8","D",0]
["2-amino-5-fluoro-6-(pentafluoroethyl)pyrimidin-4(1h)-one","719-21-1","D",0]
["6-Amino-1,1,1,2,2,3,3-heptafluoro-7,7-dimethyl-5-octen-4-one","188838-46-2","D",0]
["Tetrafluoro-2-(heptafluoro-1-propoxy)propanoyl chloride","72848-57-8","D",0]
["1,1,1,2,2,3,3,4-Octafluorobutane","662-35-1","D",0]
["3,4,4,5,5-Pentafluoro-1,5-diiodopent-2-ene","566912-89-8","D",0]
["1,1,4,4,5,5,5-Heptafluoro-2-(trifluoromethyl)pent-1-en-3-one","54376-59-9","D",0]
["Perfluoroheptane amido amine oxide","193021-67-9","D",0]
["N,N-Dibutyl-2,2,3,3,4,4,4-heptafluorobutanamide","120219-46-7","D",0]
["(Perfluorohexyl)ethyl (perfluorodecyl)ethyl hydrogen phosphate","1578186-50-1","D",0]
["Poly(difluoromethylene), .alpha.-hydro-.omega.-[(phosphonooxy)methyl]-","72987-44-1","D",0]
["1-Hydroxy-7:2 fluorotelomer sulfonic acid","2089110-02-9","D",0]
["Ethenyl perfluorononanoate","54640-64-1","D",0]
["4-Hepten-3-one, 1,1,2,2-tetrafluoro-5-mercapto-","88552-05-0","D",0]
["ethyl 2,3,3,3-tetrafluoropropanoate","399-92-8","D",0]
["2,3-Bis(2-perfluorooctylethylthio)butane-1,4-diol","57216-74-7","D",0]
["2,4,4-Trifluoro-2-(trifluoromethyl)-2H,4H-1,3-benzodioxine","25857-80-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluoro-6-[(prop-2-en-1-yl)oxy]hexane","1516879-68-7","D",0]
["Perfluoro(1,3-dipropoxycyclohexane)","400626-83-7","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Heptadecafluorododecane-2,4-dione","203201-14-3","D",0]
["1,4-Bis[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]-1,4-dioxobutane-2-sulfonic acid","80556-03-2","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)aniline","142706-74-9","D",0]
["5-Chloroperfluoro-3-oxapentanesulfonyl fluoride","73605-98-8","D",0]
["3-(Ethanesulfonyl)-2,2,3,3-tetrafluoropropanoyl fluoride","77705-90-9","D",0]
["2,2,3,3,3-Pentafluoro-N-(2,2,3,3,3-pentafluoropropanimidoyl)propanimidamide","679-25-4","D",0]
["HFE-227ea","2356-62-9","D",0]
["Methyl pentafluoropropane(dithioate)","1542-26-3","D",0]
["Ethyl 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-2,2-dihydroxydecanoate","1401315-53-4","D",0]
["4-Bromo-1,3,3,4,5,5,6,6-octafluoro-2-nitrocyclohex-1-ene","79150-79-1","D",0]
["Ethoxydimethyl((perfluorohexyl)ethyl)silane","107978-57-4","D",0]
["Bis(Perfluorooctylsulfonyl)amine","39847-41-1","D",0]
["1,1,2,2-Tetrafluoro-3-(methylsulfonyl)propane","1866059-82-6","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-(furan-2-yl)hexane-1,3-dione","595-26-6","D",0]
["5-[1,2,2,2-Tetrafluoro-1-(heptafluoropropoxy)ethyl]uridine","144862-40-8","D",0]
["N-(3-{(Carboxymethyl)[(perfluoropropyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","2089109-83-9","D",0]
["1-Methyl-3-(1,1,2,2-tetrafluoroethyl)-1,3-dihydro-2H-imidazole-2-thione","880646-52-6","D",0]
["2-Bromo-2,3,3,3-tetrafluoro-N-methoxy-N-methylpropanamide","677353-90-1","D",0]
["(4Z)-1,1,1,2,2,3,3,4-Octafluoro-7,7-dimethyl-4-octene","90292-33-4","D",0]
["4-(Difluoromethoxy)-1,1,1,2,2,3,3-heptafluorobutane","50428-19-8","D",0]
["(2R)-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoic acid","75579-39-4","D",0]
["Perfluorononadecanoic acid","133921-38-7","D",0]
["5-(Nonafluorobutylsulfonylamino)-1,3,4-thiadiazole-2-sulfonamide","316826-66-1","D",0]
["Phenyl(1,1,2,2-tetrafluoroethyl)phosphane","350-58-3","D",0]
["Trimethylsilyl 3,3,3-trifluoro-2-(trifluoromethyl)propanoate","64637-86-1","D",0]
["N,N-Bis(2,3-dihydroxypropyl)-perfluorooctanesulfonamide","74064-42-9","D",0]
["1,1'-(Difluoromethylene)bis[2,2,3,3,4,4,5,5,6-nonafluoro-1,6-bis(trifluoromethyl)cyclohexane]","116107-58-5","D",0]
["1,1,1,5,5,6,6,7,7,7-Decafluoroheptane-2,4-dione;ytterbium","31244-85-6","D",0]
["2-(1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluorohexyl)-1,3-dioxolane","60895-96-7","D",0]
["[N(E),S(S)]-N-(4-chlorophenyl)methyleneperfluorobutanesulfinamide","1612778-35-4","D",0]
["N-(2-Bromo-4-nitrophenyl)-1,2,2,3,3,4,4,5,5,6,6-undecafluorocyclohexanecarboxamide","107349-85-9","D",0]
["[4,4-Bis(trifluoromethyl)-4,5-dihydro-1H-pyrazol-3-yl](phenyl)methanone","61859-95-8","D",0]
["1-Methyl-3-octyl-1H-imidazolium perfluorobutanesulfonate","905972-83-0","D",0]
["2-Bromo-4-(heptadecafluorooctyl)thiophene","426258-05-1","D",0]
["octafluorocyclopentanone","376-66-9","D",0]
["Furan, tetrahydro-, polymer with 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane","457933-48-1","D",0]
["Decafluorohexane-2,5-dione","140173-05-3","D",0]
["3,5,5,5-Tetrafluoro-2-methyl-4-(trifluoromethyl)pent-2-ene","62116-47-6","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexanal","754-79-0","D",0]
["3,3,4,4,5,5,5-heptafluoro-1-nitropentan-2-ol","377-61-7","D",0]
["1,1,2,2-Tetrafluoro-3,4-dimethylidenecyclobutane","7704-59-8","D",0]
["1-Methyl-4H-[1,2,4]triazolo[4,3-a][1]benzazepin-6-yl nonafluorobutane-1-sulfonate","1588522-06-8","D",0]
["1,1,1,3,3,5,5,7,7,9,9,11,11-Tridecafluoro-2,4,6,8,10-pentaoxadodecan-12-oyl fluoride","21703-49-1","D",0]
["Ammonium 2,3,3,3-tetrafluoro-2-[(undecafluoropentyl)oxy]propanoate","510774-81-9","D",0]
["2-Cyclopenten-1-one, 2,3,4,4,5,5-hexafluoro-","24807-10-1","D",0]
["N-((2-Chloro-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-22-8","D",0]
["Acetophenone, alpha-(1-chloro-2,2,3,3,4,4-hexafluorocyclobutyl)-","97805-06-6","D",0]
["1-(Dimethylamino)-3-(perfluorobutyl)propan-2-ol","1023972-12-4","D",0]
["1,2,3,4,5-Pentafluoro-6-(1,2,3,3,3-pentafluoroprop-1-en-1-yl)benzene","37600-07-0","D",0]
["1-Ethoxy-2,2,3,3-tetrafluoro-4,4-dimethylcyclobutan-1-ol","144193-99-7","D",0]
["1,2,2,3,3,4,4a,5,5,6,6,7,7,8-Tetradecafluoro-4-(trifluoromethyl)-1,2,3,4,4a,5,6,7-octahydroquinoline","92942-81-9","D",0]
["1,1,1,2-Tetrafluoro-2-(heptafluoropropoxy)-4-iodobutane","243128-38-3","D",0]
["Ether, butyl 1,1,2,2-tetrafluoroethyl","358-37-2","D",0]
["N-[3-(Dimethylamino)propyl]-N-[(pentadecafluoroheptyl)sulfonyl]-beta-alanine","1432486-91-3","D",0]
["2-Fluoro-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-10-2","D",0]
["1-(5-Chlorothiophen-2-yl)-3-(undecafluorocyclohexyl)propane-1,3-dione","106876-35-1","D",0]
["18-Bromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluorooctadecane","184007-06-5","D",0]
["Methoxy (3,3,4,4,5,5,6,6,6-nonafluorohexyl) bis(3,3,3-trifluoropropyl) silane","608300-66-9","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluorohept-1-ene","129846-67-9","D",0]
["pentadecafluorooctanoic acid- 1-phenylpiperazine(1:1)","1514-68-7","D",0]
["N-Phenyl-N'-[2-(tridecafluorohexyl)phenyl]urea","288161-40-0","D",0]
["N-((2,5-Dichloro-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-28-4","D",0]
["Silicon(4+) 2,2',2''-nitrilotriethanolate 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-iodooctan-1-ide (1:1:1)","135829-02-6","D",0]
["Triethylammonium perfluoropentane sulfonate","72033-42-2","D",0]
["N,N,N-Trimethyl-3-[(perfluoro-1-oxopropyl)amino]propanaminium iodide","53518-03-9","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methoxyaniline","273735-38-9","D",0]
["1-[(9H-Carbazol-4-yl)oxy]-3-[(heptafluoropropyl)(propan-2-yl)amino]propan-2-ol--hydrogen iodide (1/1)","149825-33-2","D",0]
["2,4,4,5,5,7,7,9,9,11,11,11-Dodecafluoro-3,6,8,10-tetraoxaundecanoic acid","919005-08-6","D",0]
["Pentanoic acid, 4,4-bis[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]-","67333-58-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoro-7-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]heptanoic acid","32347-41-4","D",0]
["Phosphorous acid--2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptan-1-ol (1/3)","65611-18-9","D",0]
["1,1'-(2,2,3,3,4,4,5,5-Octafluorocyclopentane-1,1-diyl)bis(3,4-dimethylbenzene)","136525-94-5","D",0]
["1,2,3,4,4,4-Hexafluoro-1-iodo-3-(trifluoromethyl)-1-butene","167026-90-6","D",0]
["2,2,3,3-Tetrafluoropropyl 2-nitrobenzene-1-sulfonate","85459-27-4","D",0]
["N-Perfluoropelargonoyldopamine","105988-39-4","D",0]
["4-(Nonafluorobutyl)-1,3-dioxolan-2-one","1469980-27-5","D",0]
["3'-Nitro-4,4,4-trifluoro-3-trifluoromethylcrotonophenone","35443-86-8","D",0]
["1,1,2,2-Tetrafluoro-1-iodobutane","61915-73-9","D",0]
["N-(Perfluoro-1-oxobutyl)aspartic acid 1-ethyl ester","88435-83-0","D",0]
["5-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2,3-dihydro-1H-indole","273735-78-7","D",0]
["6-Methyl-beta,beta,beta',beta'-tetrakis(trifluoromethyl)-2,4-pyridinediethanol","102206-53-1","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-1-nitrobenzene","238098-38-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl sulfurofluoridoite","78499-30-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluorohenicosane","871311-23-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-10-[(prop-2-en-1-yl)sulfanyl]decane","239463-91-3","D",0]
["3,3,4,4-Tetrafluoro-2-methylpyrrolidine","1378818-08-6","D",0]
["Di-tert-butyl bis(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl) orthosilicate","381-08-8","D",0]
["11H-Perfluoroundecanoic acid","2646715-01-5","D",0]
["(1Z)-2,2,3,3,4,4,4-Heptafluoro-N-(4-methoxy-2-methylphenyl)butanimidoyl chloride","923569-77-1","D",0]
["6:2 Fluorotelomer thia propanoamido dimethyl ethyl sulfonate","62880-95-9","D",0]
["5-(Pentafluoroethyl)-1H-pyrazole","184782-98-7","D",0]
["[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy](iodo)trimethyl-lambda~5~-phosphane","89238-61-9","D",0]
["2-Bromo-1,1,2,2-tetrafluoroethyl fluorosulfate","757-02-8","D",0]
["5-Bromo-2,2,3,3-tetrafluoro-2,3-dihydro-1-benzothiophene","146431-20-1","D",0]
["Bis[perfluoro-12-methyltridecyl] phosphinic acid","610800-82-3","D",0]
["Perfluoro-1-butanesulfonyl chloride","2991-84-6","D",0]
["4-(Heptafluoroisopropyl)benzoic acid","2396-21-6","D",0]
["2-Bromo-1,1,1,2,4,4,5,5,5-nonafluoropentan-3-one","813468-14-3","D",0]
["1,1,1,3,3,4,5,5-Octafluoro-6-isocyanato-2-(isocyanatomethyl)-2,4-bis(trifluoromethyl)hexane","444122-26-3","D",0]
["4,4,4-Trifluoro-3-(methoxymethoxy)-3-(trifluoromethyl)but-1-ene","874917-55-2","D",0]
["3,5-Dimethoxy-N-[(3-{1,1,2,2-tetrafluoro-2-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]ethyl}phenyl)carbamothioyl]benzamide","4550-62-3","D",0]
["9-(Nonafluorobutyl)-2,3,6,7-tetrahydro-1H,5H,11H-pyrano[2,3-f]pyrido[3,2,1-ij]quinolin-11-one","355822-08-1","D",0]
["2-(Heptafluoropropyl)-1H-pyrrole","118425-75-5","D",0]
["Trichloro(1,3,3,4,4,5,5,6,6,7,7,8,8,8-tetradecafluorooctyl)silane","850416-78-3","D",0]
["Glycine, N-(ethylsulfonyl)-N-(heptadecafluorooctyl)-, potassium salt","95640-78-1","D",0]
["2-Chloro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridine","1816284-43-1","D",0]
["2,2,3,3,3-Pentafluoro-N-[(2,2,3,3,3-pentafluoropropanoyl)oxy]propanimidamide","4396-71-8","D",0]
["4-(Butan-2-yl)-5,7-dinitro-2-(pentafluoroethyl)-1H-benzimidazole","60167-96-6","D",0]
["Methanaminium perfluoro-2-(2-propoxypropoxy)propanoate","328065-29-8","D",0]
["3,3,4,4,5,5-Hexafluoro-1-pentanamine","2228360-94-7","D",0]
["1-[Chloro(difluoro)methoxy]-1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethane","87136-79-6","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(3-sulfopropyl) [(perfluoroheptyl)sulfonyl]amino]-1-propanaminium","2089108-81-4","D",0]
["Dimethyl (2,2,3,3-tetrafluoro-1-hydroxypropyl)phosphonate","88332-78-9","D",0]
["1,1,2,2-Tetrafluoro-3,4-dimethylcyclobutane","2368-88-9","D",0]
["5-(Perfluoropropyl)-2,2-dimethyl-3,5-pentanedione barium(2+) (2:1)","118360-70-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl [3-(trimethoxysilyl)propyl]carbamate","1421688-36-9","D",0]
["2,5-Bis(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)cyclopentan-1-one","101932-18-7","D",0]
["1,1,2,2,3,3-Hexafluoro-2,3-dihydrobenzo[f]azulen-9(1H)-one","64400-40-4","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Heneicosafluorododecyl)thio]-1-propanol","36880-08-7","D",0]
["4-(Difluoromethyl)-2,2,3,3,5,5,6,6-octafluoromorpholine","67212-89-9","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene, ethene and 1,1,2,2-tetrafluoroethene","68664-13-1","D",0]
["2-[[4-(1,1,2,2-Tetrafluoroethoxy)phenyl]iminomethyl]phenol","5141-87-7","D",0]
["4-Bromo-2,2,4,5,5-pentafluoro-3-(trifluoromethyl)-1,3-oxazolidine","104550-50-7","D",0]
["Bis(perfluorobutyl) phosphinic acid erbium(3+) salt","500776-85-2","D",0]
["(3,3,4,4-Tetrafluorohexane-1,6-diyl)bis[(dichloromethyl)silane]","64339-46-4","D",0]
["1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Tetracosafluorododec-1-ene","1828-40-6","D",0]
["3-(2,2,3,3,4,4-Hexafluorobutoxy)aniline","1427021-89-3","D",0]
["7-Chloro-1,1,2,3,3,4,4,5,5,6,6,7,7-tridecafluorohept-1-ene","66443-81-0","D",0]
["1,1,2,2-Tetrafluorocyclobutane","374-12-9","D",0]
["Calcium [(perfluorooctyl)oxy]-1,3-benzenedicarboxylate","97746-87-7","D",0]
["2-[(2,2,3,3,4,4,4-Heptafluorobutoxy)methyl]oxirane","648-43-1","D",0]
["1,2-Dibromo-1,3,3,3-tetrafluoro-1-methoxy-2-(trifluoromethyl)propane","20404-94-8","D",0]
["Benzoic acid--2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctan-1-ol (1/1)","120123-05-9","D",0]
["Diethoxymethyl(1H,1H,2H,2H-perfluorohexyl)silane","83038-83-9","D",0]
["2-(2,2,3,3,3-Pentafluoropropoxy)ethan-1-ol","757-08-4","D",0]
["2,2,3,3,4,4-Hexafluoro-N~1~,N~5~-dihydroxypentanediimidamide","4314-39-0","D",0]
["2-(2-Chloro-1,1,2,2-tetrafluoroethyl)-3,3-difluorooxaziridine","87533-07-1","D",0]
["Difluoro(1,1,2,2-tetrafluoro-2-iodoethoxy)ethanimidamide","98296-53-8","D",0]
["N,N,N-Triethyl-3-[[(perfluorooctyl)sulfonyl]amino]-1-propanaminium","153968-02-6","D",0]
["N-(2,5-Dichlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","121806-67-5","D",0]
["2-[2-(Tridecafluorohexyl)-5,6-dihydropyrimidin-1(4H)-yl]ethan-1-ol","63423-26-7","D",0]
["2-Methylpropyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","340036-47-7","D",0]
["{[(2,2,3,3,4,4,5,5-Octafluoropentyl)oxy]methyl}benzene","60895-95-6","D",0]
["Diethyl N-(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)phosphoramidate","181649-25-2","D",0]
["1-Ethoxy-2,3,3,4,4,5,5-heptafluorocyclopent-1-ene","3856-59-5","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluoro-1-iodohex-1-en-1-yl)benzene","109574-90-5","D",0]
["N-[2-(2-Hydroxyethoxy)ethyl]-N-methyl-perfluoropropanesulfonamide","89148-26-5","D",0]
["2-Propenoic acid, 2-methyl-, polymer with butyl 2-methyl-2-propenoate, dodecyl 2-methyl-2-propenoate, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate and 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]e","1432019-82-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl decanoate","18770-61-1","D",0]
["Heptanoic acid, tridecafluoro-, [[4-(2,4-dinitrophenoxy)phenyl]methylene]hydrazide","470678-94-5","D",0]
["3-(Chloromethoxy)-1,1,2,2-tetrafluoropropane","848337-76-8","D",0]
["5-[1,1,2-Trifluoro-2-(heptafluoropropoxy)ethoxy]benzene-1,3-dicarboxylic acid","1268707-97-6","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Heptadecafluorododecan-2-one","82486-22-4","D",0]
["perfluoro-tert-butyl alcohol","2378-02-1","D",0]
["Benzene, ethenyl-, polymer with 1,1,2,3,3,3-hexafluoro-1-propene and 1,1,2,2-tetrafluoroethene, graft","110830-83-6","D",0]
["5,5,6,6-Tetrafluoro-1,3-dioxepane","1547-52-0","D",0]
["[3-(1,1,2,3,3,3-Hexafluoropropoxy)propyl](trimethoxy)silane","86605-59-6","D",0]
["N-(((2-Chloro-4-((1,1,2,2-tetrafluoroethyl)thio)phenyl)amino)carbonyl)-2,6-difluorobenzamide","100278-98-6","D",0]
["1-(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)pyridin-1-ium bromide","183849-01-6","D",0]
["4'-[(12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,19-Heptadecafluorononadecyl)oxy][1,1'-biphenyl]-4-carbonitrile","117750-26-2","D",0]
["2-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-trimethylethanaminium","58014-38-3","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)-N-(2,2,2-trifluoroethyl)aniline","1365808-10-1","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentyl-1',1',2',3',3',3'-hexafluoropropyl ether","65064-81-5","D",0]
["Difluoro[bis(pentafluoroethyl)]phenyl-lambda~5~-phosphane","111784-55-5","D",0]
["N,N,N-Trimethyl-3-[[[4-[[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-buten-1-yl]oxy]phenyl]sulfonyl]amino]-1-propanaminium","170778-68-4","D",0]
["1-(Butylamino)-3-[(perfluorobutyl)ethoxy]-2-propanol","1874268-14-0","D",0]
["1,1,1,2-Tetrafluoro-6-iodo-2-(trifluoromethyl)hexane","99324-97-7","D",0]
["3,3,3-Trifluoro-N''',2,2-tris(trifluoromethyl)propanimidoyl azide","86522-49-8","D",0]
["Methanesulfonic acid--2,2,3,3,4,4,5,5-octafluoropentan-1-ol (1/1)","144101-43-9","D",0]
["4-(1,1,1,3,3,3-Hexafluoropropan-2-yl)aniline","476335-54-3","D",0]
["N-(2-Carboxyethyl)-3-{ethyl[(tridecafluorohexyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","2089109-92-0","D",0]
["Methanesulfonic acid, 2-(3-((2,2,3,3,3-pentafluoro-1-oxopropyl)amino)-5-(trifluoromethyl)-2-pyridinyl)hydrazide","141283-83-2","D",0]
["heptadecafluoro(1,2,3,4-13C4)octane-1-sulfonic acid","960354-19-2","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, hydrolyzed","161212-17-5","D",0]
["(2-Bromoethyl)(pentafluoro)cyclopropane","168087-06-7","D",0]
["Benzaldehyde, 4-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)oxy]-","494798-73-1","D",0]
["Pentafluoro ethyl radical","3369-48-0","D",0]
["Perfluorodecanesulfonate","126105-34-8","D",0]
["N~1~,N~1~,N~6~,N~6~-Tetraethyl-2,3,3,4,4,5-hexafluorohexanediamide","60895-99-0","D",0]
["5-(Heptafluoropropyl)-N-methyl-1,3,4-oxadiazol-2-amine","714975-29-8","D",0]
["Perfluoro-1,1-dichlorooctane","135941-34-3","D",0]
["1,1,1,2,3-Pentafluorobutane","161791-22-6","D",0]
["3,3,4,4,5,5,5-heptafluoro-1-pyridin-2-ylpentan-2-one","336-60-7","D",0]
["2-Chlorotetrafluoropropanamide","6066-47-3","D",0]
["(Nonafluorobutoxy)acetic acid","919005-47-3","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1,6-diisocyanatohexane","30983-17-6","D",0]
["4-(1,1,1,3,3,3-Hexafluoropropan-2-yl)phenol","63780-72-3","D",0]
["1-Bromo-2,2,3,3,4,4,5,5-octafluoro-1-(trifluoromethyl)cyclopentane","125112-68-7","D",0]
["N,N-Dichloro-2,2,3,3,4,4,4-heptafluorobutanamide","86451-48-1","D",0]
["1,1,2,2-Tetrafluoro-2-[(pentafluoroallyl)oxy]ethanesulfonyl fluoride","67635-63-6","D",0]
["(2,3,3,5,5,6,6-Heptafluoro-1,4-dioxan-2-yl)methanol","61448-96-2","D",0]
["2-(Heptafluoropropyl)quinoline","57702-79-1","D",0]
["Perfluoro-n-(1,2-13C2)decanoic acid","960315-50-8","D",0]
["Perfluoro(1,1-dimethylcyclobutane)","37360-98-8","D",0]
["1-(2,5-dimethylfuran-3-yl)-4,4,5,5,6,6,6-heptafluorohexane-1,3-dione","308-42-9","D",0]
["1-Chloro-4-(1,2,3,3,3-pentafluoroprop-1-en-1-yl)benzene","84361-33-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-Tricosafluoroundecane","66256-53-9","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N-[1-(morpholin-4-yl)ethylidene]butane-1-sulfonamide","292165-43-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluoroundecane","1287702-50-4","D",0]
["Perfluoro-1,2-bis(perfluorocyclohexyl)ethane","306-99-0","D",0]
["3-(Perfluoro-1-hexyl)-5-(methyl)pyrazole","129257-23-4","D",0]
["1-Chloro-4-[(2,2,3,3-tetrafluoropropyl)sulfanyl]benzene","78838-12-7","D",0]
["Fatty acids, C18-unsatd., trimers, 2-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptyl)sulfonyl]amino]ethyl esters","148240-82-8","D",0]
["Cyano(3-phenoxyphenyl)methyl 3-(2,2-dichloroethenyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylate","82224-37-1","D",0]
["Ethyl (2-bromo-1,1,2,2-tetrafluoroethoxy)(difluoro)acetate","88239-64-9","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluorohexyl)sulfonyl]amino)-1-propanesulfonate","2089108-91-6","D",0]
["N-[3-(Dimethylamino)propyl]-2-[(perfluorohexyl)ethylthio]acetamide","1513863-90-5","D",0]
["Tridecafluoroheptaneperoxoic acid","139702-34-4","D",0]
["Bis(perfluoro-7-methyloctyl) phosphinothioic acid","500776-78-3","D",0]
["1,2,2,2-Tetrafluoro-1-(triethoxysilyl)ethane-1-sulfonyl fluoride","142418-73-3","D",0]
["1,2,4,5,7,8-Hexachloro-1,1,2,3,3,4,5,6,6,7,8,8-dodecafluorooctane","647-20-1","D",0]
["Acetic acid--1-[(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl)oxy]ethan-1-ol (1/1)","78971-79-6","D",0]
["3,4,4,5,5,6,6,7,7,8,8,8‐Dodecafluorooct‐2‐en‐1‐ol","256384-07-3","D",0]
["Propanoic acid, 3,3,3-trifluoro-2-hydroxy-2-(trifluoromethyl)-","662-22-6","D",0]
["3,3,3',3'-Tetrakis(trifluoromethyl)-3H,3'H-1,1'-spirobi[[2,1]benzoxathiole] 1-oxide","75194-66-0","D",0]
["1-Amino-3,3,4,4,5,5,6,6,6-nonafluorohexan-2-ol","135462-71-4","D",0]
["2-Chloro-1,1,2,2-tetrafluoroethane-1-sulfonyl chloride","89740-40-9","D",0]
["2-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]benzoic acid","144178-02-9","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-methylbutan-1-amine","755-42-0","D",0]
["3,5-bis(pentafluoroethyl)-1,2,4-oxadiazole","4314-44-7","D",0]
["3-Methyl-2-(nonafluorobutyl)-1H-indole","1622133-36-1","D",0]
["3-{[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl]sulfanyl}aniline","68596-40-7","D",0]
["4-Fluoro-4-(trifluoromethyl)piperidine","1556809-89-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluoroheptacosane","116177-48-1","D",0]
["Benzenamine, 3,3'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis-","47250-53-3","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-(2-methoxyethoxy)octan-2-ol","52835-31-1","D",0]
["N~1~-(2-Aminophenyl)-2,2,3,3,4,4-hexafluoropentanediamide","60351-78-2","D",0]
["2-(heptafluoropropyl)-4,5-dihydro-1,3-oxazole","2499-91-4","D",0]
["(1S)-2,2,4,4-Tetrafluoro-1,8,8-trimethyl-3-oxabicyclo[3.2.1]octane","193280-14-7","D",0]
["N-(2,4-Dimethylphenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","90791-28-9","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-N,N-bis(2-hydroxyethyl)pentanamide","141791-73-3","D",0]
["1,1,1,2,2,3,3-Heptafluorononane","755-89-5","D",0]
["Methyl 5-cyano-α-((perfluoropropyl)ethyl)sulfinyl-α,β-dimethyl-3-thiophenepropanoate","1137678-56-8","D",0]
["Ethyl (1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)acetate","161123-65-5","D",0]
["(1Z)-2,2,3,3,4,4,4-Heptafluoro-N'-(2,2,3,3,4,4,4-heptafluorobutanimidoyl)butanimidamide","648-13-5","D",0]
["3-(2,3,3,4,4,5,5-Heptafluorocyclopent-1-en-1-yl)-2,5-dimethylthiophene","676258-32-5","D",0]
["Perfluoro[(2-methoxyethoxy)methoxy]ethene","369371-47-1","D",0]
["2-chloro-3,3,4,4,5,5,5-heptafluoropent-1-ene","261503-64-4","D",0]
["Hexafluoropropylene polymer","25120-07-4","D",0]
["4,4,5,5,6,6,7,7,8,8,8-Undecafluoro-2-iodooctan-1-ol","16083-66-2","D",0]
["1,1,2,2,5,5,6,6-Octafluorohexane","40723-65-7","D",0]
["1,1,1,4,4,4-Hexafluoro-3,3-bis(trifluoromethyl)butan-2-one","88995-83-9","D",0]
["1-chloro-1,1,2,2-tetrafluoro-2-(trifluoromethylperoxy)ethane","54362-31-1","D",0]
["Perfluoro-5-heptenesulfonic acid","2089109-51-1","D",0]
["3-[[(Perfluorooctyl)sulfonyl]methylamino]-N,N,N-trimethyl-1-propanaminium","153968-04-8","D",0]
["1-(Pentafluoroethyl)-4-propylbenzene","158536-00-6","D",0]
["3-Chloro-4-(1,1,2,3,3,3-hexafluoropropoxy)aniline","1100832-66-3","D",0]
["N-(4-Nitrophenyl)perfluorobutanamide","3869-06-5","D",0]
["2-(3-Aminophenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","2402-67-7","D",0]
["4,4-Bis(trifluoromethyl)-3-[(trimethylsilyl)oxy]cyclobut-2-en-1-one","73774-99-9","D",0]
["2,3,3,3-Tetrafluoro-2-hydroxypropanoic acid","106327-88-2","D",0]
["Ethyl 5H-octafluoropentanoate","2795-50-8","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2,4-bis(1,1,2,3,3,3-hexafluoropropoxy)benzoyl]-ω-methoxy-","75836-11-2","D",0]
["Methyl 2,4-dichloro-3-[(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)oxy]benzoate","1451750-40-5","D",0]
["1,12-Bis(perfluorodecyl)-n-dodecane","1980039-46-0","D",0]
["1,1,1,2,2,3,4,5,6,7,7,8,8,8-Tetradecafluoroocta-3,5-diene","105311-63-5","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-propylbutanamide","75668-24-5","D",0]
["3,3,4,4,4‐Pentafluorobutanoic acid","380-60-9","D",0]
["1-Chloroperfluorohexanesulfonic acid","1651215-29-0","D",0]
["1-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]-4-methylbenzene","55937-43-4","D",0]
["Perfluoro-2-nitrosopropane","422-98-0","D",0]
["Perfluorodecylphosphonic acid","52299-26-0","D",0]
["N,N'-bis(Perfluorononanoyl)1,6-hexanediamine","174495-83-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-6-[(propan-2-yl)oxy]hexane","134027-58-0","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-phenylbutyl hydrogen phenylphosphonate","496032-46-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorotetracosane","154628-01-0","D",0]
["2-(2-amino-5-tert-butylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","84649-61-6","D",0]
["2-Methyl-2-trifluoromethylperfluoropentane","100645-99-6","D",0]
["(2,2,3,3,4,4,5,5,6,6-Decafluorohexyl)phosphonic acid","113933-95-2","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-(4-methoxyphenyl)hex-1-yn-3-one","89965-76-4","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-1-iodohexane","63703-16-2","D",0]
["Ethene, chlorotrifluoro-, polymer with tetrafluoroethene, diblock","875919-64-5","D",0]
["HFE-338 mcf2","156053-88-2","D",0]
["1-Butylpyridinium perfluoro-1-butanesulfonate","334529-64-5","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,3,3,4,4,5,5,6,6 ,7,7-dodecafluoroheptyl ester, homopolymer","25656-09-1","D",0]
["4:2 Fluorotelomer thioether amido sulfonate","1432486-88-8","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyloctane-3,5-dione;thorium","23841-30-7","D",0]
["2-Chloro-1,1,1,4,4,4-hexafluoro-3-(trifluoromethyl)but-2-ene","60340-26-3","D",0]
["Bis(perfluoro-5-methylhexyl) phosphinic acid","610800-33-4","D",0]
["Heptafluoro(trifluoromethyl)cyclobutane","5187-89-3","D",0]
["1-(3,3,4,4,5,5,6,6,6-Nonafluoro-1-iodohexyl)-2,8,9-trioxa-5-aza-1-silabicyclo[3.3.3]undecane","135587-13-2","D",0]
["1,4-Bis(perfluoropentyl)butane","1835255-26-9","D",0]
["N-(2-Carboxyethyl)-3-((2-carboxyethyl)((nonafluorobutyl)sulfonyl)amino)-N,N-dimethylpropan-1-aminium","2089109-18-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8-Hexadecafluorooctane","2070-78-2","D",0]
["N,N-Diethyl-3-[4,4,4-trifluoro-3-hydroxy-3-(trifluoromethyl)butanoyl]benzene-1-sulfonamide","34844-30-9","D",0]
["4-Chloro-3,3,4,4-tetrafluorobutanal","131118-28-0","D",0]
["2,2,3,3,4,4,4-Heptafluorobutanimidohydrazide","663-24-1","D",0]
["Methanaminium, N,N,N-trimethyl-, (OC-6-21)-trifluorotris(pentafluoroethyl)phosphate(1-)","394692-83-2","D",0]
["3,4,4,4-Tetrafluorobutan-1-ol","1782796-42-2","D",0]
["4-Hydroxy-1-phenyl-5,5,5-trifluoro-4-(trifluoromethyl)-2-pentanone","101931-68-4","D",0]
["(3β,5β,6β)-5,6-Epoxy-25,26,26,26,27,27,27-heptafluorocholestan-3-ol","240129-24-2","D",0]
["11-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]undecanoic acid","522634-13-5","D",0]
["1,1,1,7,7,7-Hexafluoro-2,6-dihydroxy-3-phenyl-2,6-bis(trifluoromethyl)heptan-4-one","101913-89-7","D",0]
["2,4,6-Trichlorophenyl heptafluorobutanoate","89071-41-0","D",0]
["N-[[4-[(Heptadecafluorononyl)oxy]phenyl]sulfonyl]-N-methylglycine","59536-22-0","D",0]
["2-Propenoic acid, 2,2,3,3,4,4,4-heptafluorobutyl ester, homopolymer","28602-51-9","D",0]
["4-Chloro-2-(heptafluoropropyl)pyrimidine","937676-00-1","D",0]
["1,1'-{(1,1,2,2-Tetrafluoroethane-1,2-diyl)bis[(4,1-phenylene)oxy]}dibenzene","149963-10-0","D",0]
["N-Ethylperfluoro-1-propanesulfonamide","1270179-74-2","D",0]
["2-(Pentafluoroethyl)-1H-benzimidazole-4-carboxamide","1332982-00-9","D",0]
["Poly[oxy(1,1,2,2,3,3,4,4-octafluoro-1,4-butanediyl)], .alpha.-hydro-.omega.-hydroxy-","128840-50-6","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-methylheptane","212957-45-4","D",0]
["2-Propenoic acid, 2-fluoro-, 2,2,2-trifluoro-1-(trifluoromethyl)ethyl ester","74359-06-1","D",0]
["5,6-Dichloro-1,1,1,2,2,3,3,4,4-nonafluorohexane","136483-77-7","D",0]
["1,1,1,2,2,4,4-Heptafluorobutane","161791-36-2","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, polymer with 1,1′-oxybis[ethene]","102646-47-9","D",0]
["3,5,12-Trihydroxy-3-(hydroxyacetyl)-10-methoxy-6,11-dioxo-1,2,3,4,6,11-hexahydrotetracen-1-yl 2,3,6-trideoxy-3-[(2,2,3,3,3-pentafluoro-1-hydroxypropylidene)amino]hexopyranoside","80242-51-9","D",0]
["potassium perfluoro methoxy propionate","496805-64-2","D",0]
["1-(2-Ethoxy-3,3,4,4-tetrafluorocyclobut-1-en-1-yl)ethan-1-one","155689-27-3","D",0]
["N,N′-Bis[(N,N-dimethyl-N-oxidoaminopropyl)]-N,N'-bis(perfluorobutanesulfonyl)ethylenediamine","927673-93-6","D",0]
["N-Methyl-N,N-dioctyl-1-octanaminium perfluoro-1-butanesulfonate","495417-51-1","D",0]
["2,5-Dimethyl-4-(1,1,2,2-tetrafluoroethylthio)aniline","100280-25-9","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(propylsulfanyl)benzoic acid","1355554-68-5","D",0]
["2,2,3,3-Tetrafluoropropan-1-amine--hydrogen chloride (1/1)","663-65-0","D",0]
["1-Bromo-3,3,4,4-tetrafluorohexane","151831-48-0","D",0]
["3-Chloro-1,1,1,7,7,7-hexafluoro-2,6-dihydroxy-2,6-bis(trifluoromethyl)heptan-4-one","101913-81-9","D",0]
["2-(6-Fluoro-1H-indol-3-yl)-N-{[3-(2,2,3,3-tetrafluoropropoxy)phenyl]methyl}ethan-1-amine--hydrogen chloride (1/1)","467458-02-2","D",0]
["2-Furancarbonyl fluoride, 2,3,3,4,4,5,5-heptafluorotetrahydro-","65601-73-2","D",0]
["1,1,3,3,4,4,5,5,6,6,6-Undecafluoro-1-methoxyhexan-2-one","106693-00-9","D",0]
["1-Ethoxy-3,3,4,4,5,5,6,6,6-nonafluorohexan-2-ol","89807-88-5","D",0]
["3,3,4,4,5,5,5-Heptafluoro-1-phenyl-1,2-pentanedione","69481-44-3","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorooctane","253342-14-2","D",0]
["1-(2,2,3,3,4,4,5,5-Octafluoropentyl) 4-[2-(octyloxy)ethyl] 2-sulfobutanedioate sodium salt","61119-63-9","D",0]
["Silicon(4+) 2,2',2''-nitrilotriethanolate 3,3,4,4,5,5,6,6-octafluoro-1-iodohexan-1-ide (1:1:1)","135798-14-0","D",0]
["1-[(1,1,2,3,3,3-Hexafluoropropyl)sulfanyl]-2-methoxybenzene","921603-75-0","D",0]
["Diethylmethoxy(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","608299-39-4","D",0]
["(Perfluorobutyl)benzenesulfonic acid sodium salt","58064-45-2","D",0]
["N-cyclohexyl-4,4,4-trifluoro-2-oxo-3-(trifluoromethyl)butanamide","7232-55-5","D",0]
["1-[4-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutane-1-sulfonyl)-5-methyl-3-(4-nitrophenyl)-2,3-dihydrofuran-2-yl]ethan-1-one","771491-74-8","D",0]
["4,4,5,5,6,6,7,7,8,8,8‐Undecafluorooct‐2‐enoic acid","1869-04-1","D",0]
["1,1,1,3,4,4,4-Heptafluoro-3-(trifluoromethyl)butan-2-yl prop-2-enoate","402513-30-8","D",0]
["2-Chloro-4-fluoro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-87-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorooctacosane","93454-74-1","D",0]
["4,4,5,5,5-Pentafluoro-3-methylpent-1-en-3-ol","754-67-6","D",0]
["3-Ethenyl-1,1,2,2-tetrafluorocyclobutane","356-77-4","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyloctane-3,5-dione;terbium","17631-66-2","D",0]
["4-Nitro-N-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]benzenamine","34025-22-4","D",0]
["Diethyl [1,1,1-trifluoro-2-(trifluoromethyl)butan-2-yl]phosphonate","87579-48-4","D",0]
["2-Pentanone, 1,1-dichloro-1,3,3,4,4,5,5,5-octafluoro-","110921-39-6","D",0]
["1,1,2,2,4,4,4-Heptafluorobutyl prop-2-enoate","51053-31-7","D",0]
["Nonane, 1-bromo-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-nonadecafluoro-","558-96-3","D",0]
["1-Iodo-6-(heptafluoroisopropoxy)perfluorohexane","25080-18-6","D",0]
["N-[(Perfluoropropyl)sulfonyl]glycine","1003193-98-3","D",0]
["1-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)-1H-benzotriazole","681443-29-8","D",0]
["4-(Heptafluoropropyl)-7,8-dimethyl-1,3-dihydro-2H-1,5-benzodiazepin-2-one","505063-74-1","D",0]
["2-Propanone, hexafluoro-, 2-(2,6-dinitro-4-(trifluoromethyl)phenyl)hydrazone","86870-50-0","D",0]
["Tetrafluoro(perfluoroisopropyl)iodine","51585-87-6","D",0]
["1,1,2,2-tetrafluoroethyldiethylamine","680-63-7","D",0]
["N,N,N-Trimethyl-3-((perfluoro{5-(propan-2-yl)oxypentanoyl})amino)propan-1-aminium iodide","121924-88-7","D",0]
["5-(1,2,2,2-Tetrafluoro)ethoxy-perfluoro-3-oxa-4-methylpentanesulfonyl fluoride","75549-02-9","D",0]
["1-[(2R)-2-(2,4-Dichlorophenyl)-3-(1,1,2,2-tetrafluoroethoxy)propyl]-1H-1,2,4-triazole","131320-41-7","D",0]
["Potassium 3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfanyl]propanoate","2131064-77-0","D",0]
["Triethoxy(henicosafluorodecyl)silane","254095-33-5","D",0]
["1-chloro-4-[(1,1,2,2,3,3,3-heptafluoropropane)sulfonyl]benzene","65538-06-9","D",0]
["3,5,7,9,10-Pentachloro-2,2,3,4,4,5,6,6,7,8,8,9,10,10-tetradecafluorodecanoic acid","335-74-0","D",0]
["N-(3,5-Dichlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","106376-38-9","D",0]
["Ethyl perfluorooctyl ether","233678-24-5","D",0]
["2-[4-(1,1,2,2-Tetrafluoro-2-phenylethyl)phenyl]propane-1,2-diol","60317-35-3","D",0]
["3-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)oxy]propane-1,2-diol","135548-22-0","D",0]
["N-Ethylperfluoroethanesulfonamide","1270179-69-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Hexadecafluoro-2-methyldecan-2-ol","80466-32-6","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.',.alpha.''-[(2-hydroxy-1,2,3-propanetriyl)tris[carbonyloxy(2-iodo-3,1-propanediyl)]]tris[.omega.-fluoro-","71550-16-8","D",0]
["5,5,6,6,6-Pentafluoro-2-hexanol","94099-52-2","D",0]
["1-[Bromo(difluoro)methoxy]-1,1,2,2-tetrafluoro-2-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]ethane","330562-45-3","D",0]
["6H-Perfluoroheptanesulfonic acid","2089109-57-7","D",0]
["2-Propenoic acid, 1,1′-(2,2,3,3,4,4,5,5-octafluoro-1,6-hexanediyl) ester, homopolymer","153893-38-0","D",0]
["Phenol, 4-(pentafluoroethyl)-","95881-25-7","D",0]
["Silver perfluorononanoate","7358-16-9","D",0]
["3-(6-Chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexyl)-3,4,4-trifluoro-1,2l6-oxathietane-2,2-dione","1244856-02-7","D",0]
["5alpha,6alpha-(+-)-5,6,7,8-Tetrahydro-6-(4-hydroxyphenyl)-6-methyl-5-[9-[(4,4,5,5,5-pentafluoropentyl)sulfinyl]nonyl]-2-naphthalenol","101908-22-9","D",0]
["1-Bromo-2-[bromo(difluoro)methyl]-1,1,2,3,3,3-hexafluoropropane","89608-24-2","D",0]
["Perfluoro-3,5-dioxahexanoic acid","39492-88-1","D",0]
["2-(Difluoromethyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","138355-55-2","D",0]
["11-Chloroperfluoro-3-oxaundecanesulfonic acid","763051-92-9","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanamide","64972-10-7","D",0]
["Fulvestrant 17-beta-D-glucuronide","261506-28-9","D",0]
["2,2,2-Trifluoroethyl 2H,2H,3H,3H-perfluoroundecanoate","344580-04-7","D",0]
["N-Methyl-N'-[5-(pentafluoroethyl)-1,3,4-thiadiazol-2-yl]urea","25366-48-7","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl 2,2-difluoro-3-hydroxy-4-methylpentanoate","1370345-78-0","D",0]
["1-(Perfluorohexyl)dec-1-ene","120464-27-9","D",0]
["Decane, 3,3,4,4,5,5,6,6,7,7,8,8-dodecafluoro-1,10-diiodo-","1813-83-8","D",0]
["Methacrylic acid, 2-(diethylamino)ethyl ester, polymer with 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl acrylate","34482-03-6","D",0]
["1,1,1-Trifluoro-4-(4-fluorophenyl)-4-hydroxy-3-methyl-2-(trifluoromethyl)butan-2-yl hydrogen (3,4-dichlorophenyl)carbonimidate","100991-90-0","D",0]
["4,4,4-Trifluoro-1-(4-fluorophenyl)-2-methyl-3-(trifluoromethyl)butane-1,3-diol","34848-32-3","D",0]
["2,2,3,3,4,4-Hexafluoro-4-[(trifluoroethenyl)oxy]butan-1-ol","86883-85-4","D",0]
["3-(Trifluorosilyl)propyl nonafluoropentanoate","92916-37-5","D",0]
["1-Amino-3,3,4,4,5,5,5-heptafluoro-2-pentanol","336-53-8","D",0]
["Methyl 4-(nonadecafluorononyl)benzoate","88951-04-6","D",0]
["1-(2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxin-6-yl)methanamine","107845-58-9","D",0]
["Perfluoroundecanesulfonic acid","749786-16-1","D",0]
["1,1,1,2,2,5,5,6,6,7,7,8,8,8-Tetradecafluoro-3-octene","84808-65-1","D",0]
["5-bromo-4,4,5,5-tetrafluoropentan-1-ol","222725-20-4","D",0]
["1,2,2,3,3,4,4,5,5,6,6-Undecafluorocyclohexane-1-carbonitrile","51579-56-7","D",0]
["[3,3,4,4,5,5,5-Heptafluoro-2,2-bis(trifluoromethyl)pentyl]benzene","64356-97-4","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-(1,1,2,2,3,3,3-heptafluoropropyl)-ω-[1,2,2,2-tetrafluoro-1-[[(2-hydroxyethyl)amino]carbonyl]ethoxy]-","627909-42-6","D",0]
["(2S)-1,2-Dibromohexafluoropropane","250122-61-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,13,13,14,14,15,15,16,16,16-Triacontafluoro-9-iodohexadecane","53713-87-4","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-1-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]-4-iodobutane","25080-17-5","D",0]
["4-Chlorophenyl (2,2,3,3,4,4,4-heptafluorobutanoyl)sulfamate","1443258-17-0","D",0]
["1,3,3,4,4-Pentafluoro-2-(pentafluoroethyl)cyclobut-1-ene","61898-38-2","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohex-1-yne","59665-30-4","D",0]
["2-(Heptafluoropropyl)-3-methyl-1H-indole","1030606-42-8","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(morpholin-4-yl)butan-1-one","425-20-7","D",0]
["Potassium perfluoro-2-(butoxy)ethanesulfonate","88707-88-4","D",0]
["Copolymer of 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate / 1,7,7-trimethylbicyclo2.2.1heptan-2-yl methacrylate / 3-(trimethoxysilyl)propyl methacrylate / methyl methacrylate","1801869-89-5","D",0]
["4-(Heptadecafluorooctyl)-3a,4,7,7a-tetrahydro-2-benzofuran-1,3-dione","834880-68-1","D",0]
["2-[(2,2,3,3,4,4,4-heptafluorobutanoyl)amino]benzoic acid","82422-33-1","D",0]
["2-Propenoic acid, polymer with 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate and octadecyl 2-propenoate","68541-80-0","D",0]
["4-Amino-2-(heptafluoropropyl)pyrimidine-5-carbonitrile","647-78-9","D",0]
["Bis(Trifluoromethyl)Ketene","684-22-0","D",0]
["(5E)-1,1,1,2,2,3,3,4,4-Nonafluorodec-5-ene","131294-67-2","D",0]
["2,2,3,4,4-Pentafluoro-4-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]butanoic acid","919005-27-9","D",0]
["N-[3-(Dimethylamino)propyl]perfluoro-3,4,5-tris(methoxy)cyclohexanecarboxamide N-oxide","200636-93-7","D",0]
["N'-(Benzenesulfonyl)-2,2,3,3,4,4,4-heptafluorobutanimidohydrazide","4454-57-3","D",0]
["2-(Difluoromethyl)-2,3,3-trifluoropropanoic acid","917951-60-1","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexane-1,2-diol","124995-00-2","D",0]
["10-Cl-Perfluorodecanoate","1696260-04-4","D",0]
["Diethyl (pentafluoroethyl)phosphonate","119157-77-6","D",0]
["3,3,4,4,4-Pentafluorobutan-2-amine","1781334-71-1","D",0]
["3-[2-(Perfluorobutyl)ethylsulfanyl]propionic acid","1254468-15-9","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, 2,2,2-trifluoroethyl ester","79963-95-4","D",0]
["N-(4-Chlorophenyl)-1,1,2,2,2-pentafluoroethane-1-sulfinamide","61424-49-5","D",0]
["2,2,3,3,4,4,4-heptafluoro-1-phenylbutan-1-one","559-91-1","D",0]
["(Heptafluoropropoxy)acetic acid","919005-49-5","D",0]
["2-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)-3-methyl-6-(propan-2-yl)cyclohexan-1-ol","34844-42-3","D",0]
["1-Ethyl-3-(pentafluoroethyl)-4-(trifluoromethyl)-1H-pyrazole-5-carboxylic acid","1227002-18-7","D",0]
["Poly(oxy-1,2-ethanediyl), α-hydro-ω-hydroxy-, ether with 1-[butyl(2-hydroxyethyl)amino]-3-[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)oxy]-2-propanol (2:1)","1905409-72-4","D",0]
["Malononitrile, (6-(2-hydroxy-3,3,3-trifluoro-2-trifluoromethylpropyl)-2-pyridylmethylene)-","101756-33-6","D",0]
["2,3,3,4,4,5,5,6,6-Nonafluorocyclohex-1-ene-1-carbonitrile","90408-45-0","D",0]
["5-Bromo-2-(2,2,3,3,3-pentafluoropropoxy)pyridine","850349-84-7","D",0]
["2,2,3,3-Tetrafluoro-1-phenylpropan-1-one","1428-62-2","D",0]
["1,1,1,7,7,7-Hexafluoro-2,6-bis(trifluoromethyl)heptane-2,6-diol","66068-04-0","D",0]
["N-[5-Borono-2-(heptafluoropropyl)phenyl]glycinamide","174778-60-0","D",0]
["4,4,5,5,6,6-Hexafluoro-2,8-diiodononane-1,9-diol","1842-23-5","D",0]
["(1,1,1,2,3,3-Hexafluoropropan-2-yl)(trimethyl)silane","62281-35-0","D",0]
["2-Chloro-4,4,5,5-tetrafluoro-3-hydroxycyclopent-2-en-1-one","6681-62-5","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(2-methylpropane-2-sulfonyl)benzoic acid","1355555-26-8","D",0]
["Chlorohexafluoropropane","28987-04-4","D",0]
["(1r,4r)-4-(Nonafluorobutyl)cyclohexane-1-carboxamide","88951-21-7","D",0]
["Hexafluoro[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]cyclobutane","74693-96-2","D",0]
["1,1,1,4,4,4-Hexafluoro-2,2,3,3-tetrakis(trifluoromethyl)butane","39902-62-0","D",0]
["1,2-Dimethyl-4-(pentafluoroethyl)benzene","1257243-30-3","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propylamino]ethyl ester, polymer with 2-methyloxirane polymer with oxirane mono(2-methyl-2-propenoate)","73038-33-2","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-[(1,1,2-trifluoro-2-propen-1-yl)oxy]propoxy]-propanoate","174082-83-8","D",0]
["1,1,2,7,8,8-Hexachloro-1,2,3,4,4,5,5,6,8-nonafluorooctane","93958-59-9","D",0]
["2-Propenoic acid, 2-methyl-, docosyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate","1040208-85-2","D",0]
["Perfluoro-1-(perfluoroethyl)cyclohexanesulfonic acid","1135682-88-0","D",0]
["4-Chloro-4,5,5-trifluoro-2,2-bis(trifluoromethyl)-1,3-dioxolane","135014-05-0","D",0]
["2-(2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexanoyl)cyclopentan-1-one","141478-84-4","D",0]
["5,6,6,7,7,8,8,9,9,10,10,10-Dodecafluoro-4-methyldec-4-en-3-one","61282-88-0","D",0]
["N,N-Dibutyl-2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanamide","178167-73-2","D",0]
["16,16,17,17,18,18,19,19,20,20,21,21,22,22,22-Pentadecafluoro-3,6,9,12,15-pentaoxadocosan-1-ol","93704-25-7","D",0]
["1-(Perfluoro-n-octyl)dodecane","106873-67-0","D",0]
["1,1,1-Trifluoro-N-(pentafluoroethyl)methanesulfinimidoyl fluoride","69306-93-0","D",0]
["Ethyl difluoro(trifluoromethoxy)acetate","61206-59-5","D",0]
["Bis(tridecafluorohexyl)mercury","63037-06-9","D",0]
["N-Dodecyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononanamide","34111-24-5","D",0]
["potassium perfluoroheptanoate","21049-36-5","D",0]
["(4,4,5,5,6,6,7,7,7-Nonafluoro-2-iodoheptyl)benzene","116486-80-7","D",0]
["N-(Perfluoropropanesulfonyl)-N-(3-dimethylaminopropyl)-3-aminopropanoic acid","1513864-20-4","D",0]
["Sodium 3-{[3-(dimethylamino)propyl][(tridecafluorohexyl)sulfonyl]amino}propanoate","98900-70-0","D",0]
["1,1,2,2,5,5,6,6-Octafluorohex-3-ene","40723-73-7","D",0]
["4-Bromo-3-methyl-2,2-bis(trifluoromethyl)-1,3-oxazolidin-5-one","141364-20-7","D",0]
["5-(2,2,3,3-Tetrafluoro-1-methylcyclobutyl)-1,3,4-thiadiazol-2-amine","1140917-25-4","D",0]
["Propane, 1-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2,3,3,3-heptafluoro-, polymer with 1,1-difluoroethene, 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]propane and tetrafluoroethene","477198-48-4","D",0]
["1,1,1,2,2,6,6,7,7,7-Decafluoro-5-hydroxy-5-methylheptan-3-one","6742-92-3","D",0]
["1-(Perfluorooctyl)nonanol sulfate sodium","799267-73-5","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl diphenylphosphinite","53772-43-3","D",0]
["Methyl 3-amino-4,4,5,5,6,6,6-heptafluoro-2-hexenoate","106203-17-2","D",0]
["1,3-Benzenedisulfonic acid, 4-[2-[4-[ethyl(2-hydroxyethyl)amino]phenyl]diazenyl]-, 1,3-bis(2,2,3,3-tetrafluoropropyl) ester","143877-56-9","D",0]
["1-(2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxin-6-yl)ethan-1-one","540738-37-2","D",0]
["2-{[(1-Cyclohexyl-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)oxy]carbonyl}hydrazine-1-carboxylate","821806-59-1","D",0]
["Butyrophenone, 4'-chloro-3-hydroxy-3'-nitro-4,4,4-trifluoro-3-trifluoromethyl-","100700-41-2","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-octadecafluorododecyl ester","57678-90-7","D",0]
["2,2,3,3-Tetrafluoropropane-1-thiol","914652-53-2","D",0]
["Perfluoroheptanoic anhydride","78225-99-7","D",0]
["1,1'-(1,4-Phenylene)bis[4,4,4-trifluoro-3-(trifluoromethyl)butane-1,3-diol]","100991-88-6","D",0]
["3,3,4,4,5,5,6,6-Octafluorocyclohexene","775-40-6","D",0]
["(2E)‐4,4,5,5,6,6,7,7,8,8,9,9,10,10,10‐Pentadecafluorodec‐2‐enoic acid","56017-63-1","D",0]
["3-(Nonafluorobutoxy)propanoic acid","919005-48-4","D",0]
["(Perfluoropropyl)difluoroamine","423-32-5","D",0]
["3,3,4,4,4-Pentafluorobutane-1-sulfonamide","29765-92-2","D",0]
["2,3,3,4,4,5-Hexafluoro-2,5-bis(trifluoromethyl)oxolane","59663-83-1","D",0]
["7-Ethyl-1,1,1,2,2,3,3-heptafluorononane-4,6-dione","80284-42-0","D",0]
["1,1,1,7,7,7-Hexafluoro-4-imino-2,6-bis(trifluoromethyl)heptane-2,6-diol","824954-55-4","D",0]
["4-Bromo-1,1,1,2,2-pentafluorobutane","52671-70-2","D",0]
["Poly(oxy-1,2-ethanediyl), α-[5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,13,13,13-octadecafluoro-2-hydroxy-12-(trifluoromethyl)tridecyl]-ω-hydroxy-","148919-89-5","D",0]
["[N(E),S(S)]-N-phenylmethyleneperfluorobutanesulfinamide","1612778-34-3","D",0]
["1,1,2,2-Tetrafluoro-2,3-dihydro-1H-indene","80829-35-2","D",0]
["Ethyl 3,4,4,4-tetrafluorobut-2-enoate","197226-71-4","D",0]
["Perfluoro-4-octen","3910-82-5","D",0]
["1-Methoxy-4-(pentafluoroethyl)benzene","14038-06-3","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-1-phenylundecane-1,3-dione","141522-69-2","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Henicosafluorotridecanenitrile","140834-59-9","D",0]
["(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)benzene","378-34-7","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-[3-(trifluoromethyl)phenyl]nonanamide","325989-96-6","D",0]
["4-(2,2,3,3,4,4,4-heptafluorobutanoylamino)benzamide","6355-37-9","D",0]
["O,O'-Dibutyl ethylphosphonous acid compd. with perfluoro-3-iodopropane (1:1)","80392-01-4","D",0]
["2,3-Dichloro-1,1,1,3,4,4,5,5,5-nonafluoro-2-(trifluoromethyl)pentane","80201-33-8","D",0]
["Iodozinc(1+) 1,1,1,2,3,3,3-heptafluoropropan-2-ide","62656-71-7","D",0]
["2,2-Dibromohexafluoropropane","38568-21-7","D",0]
["1,1,1,2,3,3-Hexafluoro-4-methylhexane","57915-72-7","D",0]
["N-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]-benzamide","5022-41-3","D",0]
["Perfluorododecanal","179799-68-9","D",0]
["Perfluoropropanoate","44864-55-3","D",0]
["4,4,5,5,5-Pentafluoro-2-(trifluoromethyl)pentanal","90278-13-0","D",0]
["5-(1,1,2,2-Tetrafluoroethyl)-3H-1,2-dithiole-3-thione","106776-01-6","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl sulfurofluoridate","106054-87-9","D",0]
["4,4,6-Tris(trifluoromethyl)-1,5,6-triazaspiro[bicyclo[3.1.0]hexane-2,1'-cyclohexane]","130720-67-1","D",0]
["2-(2-Bromo-1,1,2,2-tetrafluoroethoxy)-1,1,1,2,3,3-hexafluoro-3-(pentafluoroethoxy)propane","1482416-44-3","D",0]
["2,6-Dimethoxy-N-{5-[4-(pentafluoroethoxy)phenyl]-1,3,4-thiadiazol-2-yl}benzene-1-carboximidic acid","70057-62-4","D",0]
["Polyfluoroalkyl (C 2-5) methacrylate","95243-53-1","D",0]
["3,3,4,4,5,6,6,6-Octafluoro-5-(trifluoromethyl)hexan-1-ol","89076-11-9","D",0]
["(E)-4-(2,2,3,3,4,4,4-Heptafluorobutoxy)-4-oxobut-2-enoic acid","952584-86-0","D",0]
["N'-Benzylidene-2,2,3,3,4,4,4-heptafluorobutanehydrazide","736-62-9","D",0]
["2,5-Furandione, polymer with 3-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethoxy]-1-propene","35164-44-4","D",0]
["4,4,5,5,5-Pentafluoro-1-(thiophen-2-yl)pentane-1,3-dione","1994-18-9","D",0]
["1,1,1,2,3,3-Hexafluoro-3-(2,2,3,3-tetrafluoropropoxy)propane","65064-78-0","D",0]
["1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexakis[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl)oxy]-2,2,4,4,6,6-hexahydro-","186043-67-4","D",0]
["1,1,1,2-tetrafluoro-2-iodoethane","3831-49-0","D",0]
["4-(Trifluoromethyl)-perfluoroquinolizidine","86563-85-1","D",0]
["3-Chloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-17-9","D",0]
["Trifluorovinyl heptafluoropropyl ether homopolymer","70087-25-1","D",0]
["Lithium perfluoropentanoate","198482-22-3","D",0]
["6,6'-Bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-1,1'-binaphthalene-2,2'-diol","359699-85-7","D",0]
["2,3,3,3-Tetrafluoro-2-{1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy}propanoic acid--ammonia (1/1)","62037-77-8","D",0]
["1,2,3,4,4,4-Hexafluoro-3-(heptafluoropropoxy)but-1-ene","84195-42-6","D",0]
["1-(Benzylamino)-3-(1,1,2,2-tetrafluoroethoxy)propan-2-ol","939793-32-5","D",0]
["Ethoxydimethyl (3,3,4,4,4-pentafluorobutyl) silane","608300-94-3","D",0]
["1-[(1,1,2,3,3,3-Hexafluoropropyl)sulfanyl]-4-methylbenzene","144429-11-8","D",0]
["1,1,2,2,4,4,4-Heptafluoro-3-(iodomethyl)-1-(1,2,2,2-tetrafluoroethoxy)butane","25080-20-0","D",0]
["1,1,3,5,7,8-Hexachloro-1,2,2,3,4,4,5,6,6,7,8,8-dodecafluorooctane","335-68-2","D",0]
["6-H-Perfluorohexanoate","1696259-63-8","D",0]
["5-{[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)oxy]methyl}-1H-1,2,3-triazole","1447923-23-0","D",0]
["3-[(Perfluorobutanesulfonyl)amino]propane-1-sulfonic acid","2089108-62-1","D",0]
["2-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)aniline","2396-15-8","D",0]
["11-(2,2,3,3,3-Pentafluoropropoxy)undecane-1-thiol","124051-55-4","D",0]
["1,1,1,2,2,3,3,6,6,7,7,8,8,9,9,10,10,11,11,11-Icosafluoro-4-undecene","100603-63-2","D",0]
["1-(2-Bromophenyl)-2,2,3,3,3-pentafluoropropan-1-one","573670-90-3","D",0]
["B-(3,5-bis(Perfluoro-1-methylethyl)phenyl)boronic acid","1402929-36-5","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl 4-methylbenzene-1-sulfonate","312-66-3","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(propane-1-sulfonyl)benzoic acid","1355554-46-9","D",0]
["Decafluorooxane","355-79-3","D",0]
["1,1,3,3,4,4,4-Heptafluorobutan-2-one","370862-34-3","D",0]
["Isocyanic acid, 2,2,3,3,4,4,4-heptafluorobutyl ester","377-00-4","D",0]
["1-Fluoro-1-(trifluoromethyl)naphthalen-2(1H)-one","63418-30-4","D",0]
["1,5-Dideoxy-1,1,1,5,5,5-hexafluoro-2,4-di-C-fluoro-2,4-bis-O-(trifluoromethyl)pent-3-ulose","59681-95-7","D",0]
["(2S)-2-{Bis[4-(heptadecafluorooctyl)phenyl][(trimethylsilyl)oxy]methyl}pyrrolidine","906077-31-4","D",0]
["2,3-Dibromooctafluorobutane","375-26-8","D",0]
["1-Hexadecylpyridinium perfluoro-1-butanesulfonate","334529-62-3","D",0]
["1-Undecanaminium, N-(5-carboxypentyl)-N,N-dimethyl-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-, hydroxide, inner salt","145441-35-6","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorotetracosane","808758-67-0","D",0]
["Methyl 2-hydroxy-4-(2,2,3,3,3-pentafluoropropoxy)benzoate","651331-87-2","D",0]
["[N(E),S(S)]-N-(3-Fluorophenyl)methyleneperfluorobutanesulfinamide","1612778-41-2","D",0]
["N-{4-[(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)amino]benzene-1-sulfonyl}acetamide","320599-24-4","D",0]
["2-(Heptafluoropropyl)-1H-imidazole","81769-47-3","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl 2-methylprop-2-enoate","150625-20-0","D",0]
["5-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)pyrimidine-2,4(1H,3H)-dione","80384-59-4","D",0]
["7-Bromo-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoroheptane","376-31-8","D",0]
["Caroxin F","37340-18-4","D",0]
["3,6-Bis(heptafluoropropyl)-1,2,4,5-tetrazine","5585-47-7","D",0]
["Ammonium 1,1,2,2-tetrafluoro-2-{[1,1,1,2,3,3-hexafluoro-3-(pentafluoroethoxy)propan-2-yl]oxy}ethane-1-sulfonate","93644-65-6","D",0]
["Phosphonic acid, [[4-[(heptadecafluorononenyl)oxy]phenyl]methyl]-, zinc salt (2:1)","107812-05-5","D",0]
["N-((2,3-Dichloro-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-30-8","D",0]
["Bis(pentafluoroethyl)thiadiaziridine","87999-39-1","D",0]
["Hexadecyl perfluorobutanoate","6385-15-5","D",0]
["1,4,5,5,6,6-Hexafluoro-2,3-dimethylbicyclo[2.2.0]hex-2-ene","33103-47-8","D",0]
["Methyl 2,2,3,3,4,4,5-heptafluoro-5-oxopentanoate","38093-90-2","D",0]
["5-[2-[[(Perfluorooctyl)sulfonyl]propylamino]ethoxy]-1-pentanesulfonic acid potassium salt","167162-23-4","D",0]
["1,1,1,2,2,3,3,4,4,13,13,14,14,15,15,16,16,16-Octadecafluorohexadecane","1835252-00-0","D",0]
["4-Chloro-1,1,2,3,3,4,4-heptafluorobut-1-ene","89551-62-2","D",0]
["3,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Pentadecafluoro-3-decen-2-one","92604-91-6","D",0]
["3-{[3-(Dimethylamino)-2-hydroxypropyl][(heptadecafluorooctyl)sulfonyl]amino}-1-propanesulfonic acid","759411-03-5","D",0]
["1,1,1,2,2-pentafluoro-6-iodohexane","344452-10-4","D",0]
["1,1,2,2,3,3,4,4,5,5-Decafluoro-6-(heptafluoropropyl)-6-(trifluoromethyl)cyclohexane","73188-76-8","D",0]
["7-(2-Chloro-1,1,2-trifluoroethoxy)-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoroheptane","65064-85-9","D",0]
["5,5,6,6,7,7,8,8-Octafluoro-5,6,7,8-tetrahydrotetrazolo[1,5-a]pyridine","89516-73-4","D",0]
["1,1,2,2-Tetrafluoro-3-[tris(2,2,3,3-tetrafluoropropoxy)methoxy]propane","2409-18-9","D",0]
["N-(Perfluoro-1-oxobutyl)aspartic acid 1-butyl ester","88434-83-7","D",0]
["2,2,3,3,3-Pentafluoro-N-hydroxypropanimidamide","4314-36-7","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyl-3,4,5-octanetrione 4-(4-nitrophenyl)hydrazone","80284-51-1","D",0]
["Ethyl 2-(pentadecafluoroheptyl)imidazo[1,2-a]pyridine-3-carboxylate","135339-05-8","D",0]
["3,3,4,4,5,5,6,6,6-nonafluoro-1-nitrohexan-2-ol","240408-94-0","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-prop-1-enylsulfonylbutane","66406-80-2","D",0]
["4-[Bromo(difluoro)methyl]-4,5,5,5-tetrafluoropent-1-ene","89965-96-8","D",0]
["N-((2,5-Dimethyl-4-(1,1,2,2-tetrafluoroethylsulfanyl)phenyl]carbamoyl]-2,6-difluorobenzamide","100279-91-2","D",0]
["N-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)benzenesulfonamide","72567-08-9","D",0]
["2-(4-Amino-3-methylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","1992-09-2","D",0]
["1-Bromo-2-(2,2,3,3-tetrafluoropropoxy)benzene","958454-23-4","D",0]
["(4Z)-1,1,1,2,2,4,5,6,7,7,7-Undecafluoro-6-(trifluoromethyl)hept-4-en-3-one","134330-92-0","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoroheptyl iodide","183547-74-2","D",0]
["Tris[4-[4,4,6,7,7,9,10,10,12,13,13,15,15,15-tetradecafluoro-6,9,12-tris(trifluoromethyl)-2,5,8,11,14-pentaoxapentadec-1-yl]phenyl]phosphine","88750-33-8","D",0]
["1,1,1,2,3,3-Hexafluoro-4,4-dimethylpentane","53005-29-1","D",0]
["(Pentafluoroethyl)boronic acid","1247012-61-8","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-1-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]-6-iodohexane","25080-24-4","D",0]
["Methyl 4-(nonafluorobutyl)benzoate","88951-00-2","D",0]
["1,1,1,3,5,5,5-Heptafluoro-4-(trifluoromethyl)pent-3-en-2-one","89810-82-2","D",0]
["2,2,3,3,4,4,5,5,6-Nonafluoro-2,3,4,5-tetrahydropyridine","714-37-4","D",0]
["2-Propenoic acid, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propyl ester","17559-01-2","D",0]
["2,6-Difluoro-N-((2-fluoro-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)benzamide","100341-19-3","D",0]
["3,3',4,4'-Diphenylethertetracarboxylic dianhydride, 4,4'-oxydianiline, 3,3',4,4'-biphenyltetracarboxylic dianhydride, 2,2'-bis4-(4-aminophenoxy)phenylhexafluoropropane, bis(3-aminopropyl)tetramethyl disiloxane copolymer","1430800-23-9","D",0]
["N-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)benzamide","87988-75-8","D",0]
["1H-Perfluorononane","375-94-0","D",0]
["Propane, 1-bromo-1,1,2,2-tetrafluoro-","70192-84-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-(3-fluorophenyl)nonanamide","541514-85-6","D",0]
["4,4-Dichloro-5,5,6,6,6-pentafluoro-2-methyl-1-hexene","18599-03-6","D",0]
["1H,1H-Nonafluoro-3,6-dioxaheptan-1-ol","330562-43-1","D",0]
["bis((Perfluorobutyl)ethyl) carbonate","1132677-78-1","D",0]
["1-(Heptafluoropropyl)-4-nitrobenzene","1300746-85-3","D",0]
["Heptadecafluorononanenitrile","82416-71-5","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, reaction products with 1,6-diisocyanatohexane, epichlorohydrin, reduced Me esters of reduced polymd. oxidized tetrafluoroethylene and triethoxy(3-isocyanatopropyl)silane","1638956-41-8","D",0]
["(1,1,2,3,3,3-Hexafluoropropyl)cyclohexane","53005-30-4","D",0]
["{4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]phenyl}methanol","62623-09-0","D",0]
["Copolymer of perfluoroethene, 1,1,2,2-tetrafluoro-3-iodopropoxyperfluoroethene and perfluoro(methoxyethene)","193018-53-0","D",0]
["{4-[(4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononyl)oxy]phenyl}methanol","957206-65-4","D",0]
["Poly(oxy-1,2-ethanediyl), α-[3,4,5-tris(1,1,2,3,3,3-hexafluoropropoxy)benzoyl]-ω-hydroxy-","75836-09-8","D",0]
["1,1,1,2,2-Pentafluoro-4-iodooctane","117539-28-3","D",0]
["N-(2,3-Dihydroxypropyl)-N-hexyl-perfluorododecane-1-sulfonamide","141187-86-2","D",0]
["2-Acetoxy-4-(2.2,3,3,3-pentafluoropropoxy)benzoic acid","651331-97-4","D",0]
["2,2,3,4,4,5-Hexafluoro-3,5-bis(trifluoromethyl)oxolane","68970-43-4","D",0]
["(6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyl-3,5-octanedionato-κappaO3,κappaO5)(triethylphosphine)silver","165461-74-5","D",0]
["2-Chloroperfluoroheptane","319490-62-5","D",0]
["Bis(perfluoroheptanesulfonyl)imide","1040629-78-4","D",0]
["5-(Heptafluoropropyl)isoquinoline-1-carbaldehyde","31181-32-5","D",0]
["1-Chloro-3-(pentafluoroethyl)benzene","309-13-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoropentacosane","250738-43-3","D",0]
["1,1,1,2,2-Pentafluoroundec-4-en-3-one","89176-03-4","D",0]
["3-(Nonafluorobutyl)-1-benzothiophene","1608112-39-5","D",0]
["2-(Methylamino)-2-((nonafluorobutyl)sulfonyl)ethyl prop-2-enoate","479401-24-6","D",0]
["6-(Ethenyloxy)-1,1,1,2,2,3,3,4,4,5,5-undecafluorohexane","595-00-6","D",0]
["2,3-Butanediol, 1,1,1,4,4,4-hexafluoro-2,3-bis(trifluoromethyl)-","918-21-8","D",0]
["Undecyl perfluorobutanoate","959103-74-3","D",0]
["3,3,4,4-Tetrafluorooctahydro-5,8-methano-1,2-benzodithiine","102489-63-4","D",0]
["1,1,1,2,2,3-Hexafluorodecan-4-one","113487-29-9","D",0]
["Ammonium perfluoro-4,7-dioxaoctanoate","1173788-87-8","D",0]
["1,2,3,3,4,4,5,5-octafluorocyclopentane","828-35-3","D",0]
["2-(2,2,3,3,4,4,5,5,5-Nonafluoropentanoyl)cyclopentan-1-one","347361-45-9","D",0]
["1-Chloro-1,1,2,2,3,3,4,4-octafluoro-6-iodododecane","100419-95-2","D",0]
["Pentane, 1,1,1,2,2,3,3,4,4,5,5-undecafluoro-","375-61-1","D",0]
["Undecafluorocyclohexanemethanol dihydrogen phosphate","32582-74-4","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-1-Butanesulfonic acid sodium salt","60453-92-1","D",0]
["1H,1H-Perfluoropentylamine","355-27-1","D",0]
["3-(Perfluoro-1-propyl)-1,2-propanediol","1992-91-2","D",0]
["Trimethyl[3-[[4-[[3,4,4,4-tetrafluoro-2-(heptafluoroisopropyl)-1,3-bis(trifluoromethyl)-1-butenyl]oxy]benzoyl]amino]propyl]ammonium iodide","170778-67-3","D",0]
["Bicyclo[2.2.1]hept-2-ene, 5,5,6-trifluoro-6-(heptafluoropropoxy)-","154717-36-9","D",0]
["1,1,1,2,2,3,3-Heptafluoroheptane","152076-35-2","D",0]
["1-Ethoxy-2-(1,1,2,2-tetrafluoroethoxy)benzene","847991-53-1","D",0]
["Tris[3-(heptafluoropropylhydroxymethylene)-(−)-camphorato]erbium","123359-45-5","D",0]
["Oxo[tris(undecafluoropentyl)]-lambda~5~-phosphane","58431-35-9","D",0]
["7:2 Fluorotelomer sulfonic acid","56682-30-5","D",0]
["4-Chloro-2-(2-chloro-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)phenyl acetate","38506-76-2","D",0]
["3,3,4,4,5,5,6,6-Octafluoro-1,8-diiodooctane","2681-00-7","D",0]
["3-Methyl-3-[(2,2,3,3-tetrafluoropropoxy)methyl]oxetane","879546-71-1","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,5,5,5-undecafluoropentane-1-sulfonamide","162682-16-8","D",0]
["2-(Pentafluoroethyl)-4-(propan-2-yl)pyrimidine-5-carboxylic acid","914201-16-4","D",0]
["Trimethyl(pentafluoroethyl)stannane","754-25-6","D",0]
["1-Propanol, 3-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3 ,3-tetrafluoro-,","204270-10-0","D",0]
["N,N-Diethyl-4-methyl-2-(1,2,2,2-tetrafluoroethyl)-1,3-dioxan-2-amine","89752-26-1","D",0]
["1-[Difluoro(trifluoromethoxy)methoxy]-1,1,2,3,3,3-hexafluoro-2-(trifluoromethoxy)propane","1309353-34-1","D",0]
["1,1,1,3,3,3-Hexafluoro-2-propanyl 4-[bis(1,3-benzodioxol-5-yl)(hydroxy)methyl]-1-piperidinecarboxylate","1380424-42-9","D",0]
["Difluoro[1,1,2,2-tetrafluoro-2-(nonafluorobutoxy)ethoxy]acetyl fluoride","172897-75-5","D",0]
["4-(Ethoxymethoxy)-5,5,5-trifluoro-4-(trifluoromethyl)pent-1-ene","477199-90-9","D",0]
["beta-Alanine, N-(4-piperidinylmethyl)-, 2,2,3,3,4,4,5,5-octafluoro-6-[(1-oxo-2-propen-1-yl)oxy]hexyl ester","1233879-49-6","D",0]
["2,6,8-Tris(1,1,1,3,3,3-hexafluoropropan-2-ylidene)-9-methyl-1,3,5,7-tetrathia-9-azaspiro[3.5]nonane","66172-24-5","D",0]
["Pentanedioic acid, 2,2,3,3,4,4-hexafluoro-, 1,5-dimethyl ester","1513-62-8","D",0]
["Bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) 2-methylidenebutanedioate","49676-56-4","D",0]
["1-Nitro-4-[2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl]benzene","36714-78-0","D",0]
["N-[3-(Dimethylamino)propyl]-perfluoropropane-1-sulfonamide","1513864-23-7","D",0]
["Pyflubumide","926914-55-8","D",0]
["Bis(trifluoromethyl)propanedioyl difluoride","42139-57-1","D",0]
["2,2-Difluoro-3,3-bis(trifluoromethyl)oxirane","707-13-1","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reaction products with ammonia, dehydrated","161075-13-4","D",0]
["2,2,3,3,4,4,4-heptafluorobutanehydrazide","1515-05-5","D",0]
["alpha-Perfluoropropyl omega-perfluoroethyl poly(perfluoropropylene oxide)","52700-35-3","D",0]
["1-(Difluoromethoxy)-1,2,2,3,3-pentafluoropropane","35042-98-9","D",0]
["2‐[2-(Perfluorobutyl)ethylsulfanyl]acetic acid","123708-08-7","D",0]
["Perfluoro-2-butanone","337-20-2","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-[(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)methanesulfonyl]butane","29214-37-7","D",0]
["Fulvestrant 3-|A-D-Glucuronide","261506-27-8","D",0]
["2-(1,1,2,2-Tetrafluoroethyl)-4,5,6,7-tetrahydro-1H-1,3-diazepine","936224-60-1","D",0]
["Difluoro[tris(undecafluoropentyl)]-lambda~5~-phosphane","91543-35-0","D",0]
["3-(2-Chloro-1,1,2-trifluoroethoxy)-2,2,3,3-tetrafluoropropanenitrile","51579-45-4","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-[(2-methylpropyl)sulfanyl]benzoic acid","1355554-12-9","D",0]
["Methyl 4-(heptafluoropropyl)benzoate","64299-47-4","D",0]
["3-[[(Perfluorohexyl)sulfonyl](methyl)amino]-N,N,N-trimethyl-1-propanaminium","765219-81-6","D",0]
["Perfluoro-4-(fluorosulfonyl)butanoyl fluoride","83071-23-2","D",0]
["Dimethyl(prop-1-yn-1-yl)(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","111641-50-0","D",0]
["3-(Dimethyl(3-(((tridecafluorohexyl)sulfonyl)amino)propyl)azaniumyl)propanoate","81190-41-2","D",0]
["Perfluoro-2-[2-(2-methoxypropoxy)propoxy]propanoic acid","753446-03-6","D",0]
["[(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)methyl]benzene","879081-10-4","D",0]
["13,13,14,14,14-Pentafluoro-3,6,9,12-tetraoxatetradecan-1-ol","652983-61-4","D",0]
["1-{4-[(2H-1,3-Benzodioxol-5-yl)methyl]piperazin-1-yl}-2,2,3,3,4,4,4-heptafluorobutan-1-one","546063-97-2","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8-Pentadecafluorooctan-1-ol","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodotetracosane","1257261-92-9","D",0]
["1,2-Bis(pentafluoroethoxy)benzene","34065-74-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorohexacosane","167641-85-2","D",0]
["Borate(1-), tetrahydro-, sodium (1:1), reaction products with reduced polymd. oxidized tetrafluoroethylene, hydrolyzed, diallyl ethers, polymers with 2,4,6,8-tetramethylcyclotetrasiloxane, Si-[3-(2-hydroxyethoxy)propyl] derivs.","1214752-86-9","D",0]
["Cyclohexanaminium perfluorononanoate","328531-06-2","D",0]
["1,1,1,2,2,3,3,4,4,7,7,8,8,8-Tetradecafluoro-5-iodooctane","935553-89-2","D",0]
["2,2,3,3-Тетрафторпропил-2-фторпроп-2-еноат","96250-37-2","D",0]
["Bis(4-chloro-2,2,3,3,4,4-hexafluoro-1-oxobutyl)peroxide","100634-66-0","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[[(perfluorohexyl)sulfonyl]amino]-1-propanaminium","2089108-68-7","D",0]
["1,1,1,2,2-Pentafluoro-2-[(trifluoromethyl)disulfanyl]ethane","34880-32-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecan-2-one","55118-65-5","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-8-iodooctane","99324-98-8","D",0]
["1,1,1,2,3,3-Hexafluoro-3-(fluoromethoxy)propane","60598-14-3","D",0]
["Perfluoro-3,6,9-trioxaundecane-1,11-dioic acid","55621-18-6","D",0]
["N-Vinylperfluorobutanamide","4314-32-3","D",0]
["12,12,13,13,14,14,15,15,16,16,17,17,17-Tridecafluoroheptadecanoyl chloride","118624-66-1","D",0]
["N,N-Diethyl-2,2,3,3,4,4,4-heptafluorobutanethioamide","61881-10-5","D",0]
["1,1,1,3,3,5,5-Heptafluoro-2,4-dioxahexan-6-oyl fluoride","21703-43-5","D",0]
["(1,1,3,3,4,4,4-Heptafluorobut-1-en-2-yl)benzene","5300-25-4","D",0]
["Phosphorous acid--4-(tridecafluorohexyl)phenol (1/3)","201936-68-7","D",0]
["15:2 Fluorotelomer alcohol","176676-69-0","D",0]
["5-Amino-1,1,2,2,6,6,7,7-octafluorohept-4-en-3-one","80070-82-2","D",0]
["Carboxydimethyl[3-(perfluorooctadecyl)‐2‐hydroxypropyl]azanium","","D",0]
["Perfluoropentane sulfonamidoethanol","1270179-64-0","D",0]
["Propyl pentafluoropropanoate","39118-07-5","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-nonene","63967-46-4","D",0]
["2,3,5-Trifluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-methoxypyridine","20017-48-5","D",0]
["2,5-Furandione, polymer with 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-8-[(2-methyl-2-propenyl)oxy]octane","38467-14-0","D",0]
["2-Propanone, 1,1,1,3,3,3-hexafluoro-, semicarbazone","400-16-8","D",0]
["N-Ethyl-N-(17-hydroxy-3,6,9,12,15-pentaoxaheptadec-1-yl)perfluorooctanesulfonamide","52137-93-6","D",0]
["4,4,5,5,6,6,6-Heptafluoro-2-hexen-1-ol","679-03-8","D",0]
["Copper bis(1,1,1,5,5,6,6-heptafluoro-2-oxo-heptane)","5178-89-2","D",0]
["Perfluoro-1-nonanesulfonamide","1818833-95-2","D",0]
["3,5-Bis(heptafluoropropyl)-1H-1,2,4-triazole","801-28-5","D",0]
["3,3,4,4-tetrafluoro-1,2-diiodocyclobutene","15563-92-5","D",0]
["1,2-Bis(perfluorohexyl)ethene","56523-43-4","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)-1-(morpholin-4-yl)propan-1-one","176702-73-1","D",0]
["2-[(Perfluorooctane-1-sulfonyl)amino]ethyl prop-2-enoate","60194-47-0","D",0]
["1-Hydroxy-8:2 fluorotelomer sulfonic acid","2089110-03-0","D",0]
["2-[(heptafluoropropyl)sulfanyl]aniline","166392-11-6","D",0]
["1-Iodo-1,2-bis(perfluoro-n-butyl)ethane","53638-10-1","D",0]
["3-(Chloromethyl)-1,1,2,2-tetrafluorocyclobutane","356-80-9","D",0]
["3-[[(Perfluorooctyl)sulfonyl]ethylamino]-N,N,N-trimethyl-1-propanaminium bromide","331755-01-2","D",0]
["Potassium N-methyl(perfluorohexanesulfonamido)acetate","57765-31-8","D",0]
["Perfluoro-3,5,7,9-butaoxadecanoic acid","39492-90-5","D",0]
["Bis[perfluoro(1-oxo-3-methoxypropyl)] peroxide","79754-25-9","D",0]
["4,4,6-Tris(trifluoromethyl)-1,5,6-triazaspiro[bicyclo[3.1.0]hexane-2,1'-cyclopentane]","130720-66-0","D",0]
["5,5,6,6,7,7,8,8-Octafluorooctane-2,4-dione","62679-62-3","D",0]
["2-[(2-Aminoethyl)sulfanyl]-1,1,1,3,3,3-hexafluoro-2-propanol","21918-92-3","D",0]
["2H-Pyran-2-carbonyl fluoride, 2,3,3,4,4,5,5,6,6-nonafluorotetrahydro-","65601-67-4","D",0]
["2,5-Dichloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-19-1","D",0]
["bis(2,2,3,3,4,4,5,5-octafluoropentyl) pentanedioate","308-36-1","D",0]
["Prop-2-en-1-yl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","117837-58-8","D",0]
["Propane, 1-[1-[difluoro[(1,2,2-trifluoroethenyl)oxy] methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2,3,3,3-heptafluoro-, polymer with 1,1-difluoroethene","80975-16-2","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl heptafluorobutanoate","922168-38-5","D",0]
["Cyclopentane, octafluoro(hexafluorocyclobutylidene)-","74693-91-7","D",0]
["Propan-2-yl 4-nitro-2-(1,1,2,2-tetrafluoroethyl)-6-(trifluoromethyl)-1H-benzimidazole-1-carboxylate","57322-65-3","D",0]
["1,1,2,2,3,4,4,5-Octafluorocyclopentane","773-17-1","D",0]
["Butanamide, 2,2,3,3,4,4,4-heptafluoro-N-methyl-N-(trimethylsilyl)-","53296-64-3","D",0]
["Perfluoro-1-propanesulfinic acid  sodium","152893-99-7","D",0]
["1,1'-(3,3,4,4-Tetrafluoro-1-cyclobutene-1,2-diyl)bisaziridine","28690-25-7","D",0]
["4-Acetamido-3-chlorophenyl nonafluorobutane-1-sulfonate","1428370-26-6","D",0]
["3,3,3',3'-Tetrakis(trifluoromethyl)-1,1'-spirobi[2,1lambda4-benzoxathiole]","70091-68-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodotridecane","38550-36-6","D",0]
["3,3,4,4,5,5-Hexafluoro-1,2-dimethoxycyclopent-1-ene","1759-61-1","D",0]
["5,5,6,6,7,7,7-Heptafluoroheptan-1-ol","883543-64-4","D",0]
["2,2,3,3-Tetrafluoropropyl 5-[(2,6-dimethoxy-4-pyrimidinyl)amino]-5-oxopentanoate","5576-93-2","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)-N-(1-phenylethyl)propanamide","98873-61-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluorononanamide","82854-34-0","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyl-3,5-octanedione - indium (3:1)","30983-38-1","D",0]
["6:2 Fluorotelomer thioether amido sulfonate","88992-47-6","D",0]
["1-Bromo-1-chloro-1,2,2,2-tetrafluoroethane","754-20-1","D",0]
["Ethyl 4,4,5,5,6,6,7,7,7-nonafluoroheptanoate","136905-37-8","D",0]
["2-methyl-2-(1,1,2,2-tetrafluoroethoxy)propane","659-98-3","D",0]
["(4E)-1,1,1-Trifluoro-4-(methylimino)-2-(trifluoromethyl)pentan-2-ol","518976-18-6","D",0]
["4,4,5,5,5-Pentafluoro-2-methylpentanoic acid","403615-96-3","D",0]
["(3,3,4,4,4-Pentafluorobut-1-yn-1-yl)benzene","55009-90-0","D",0]
["12,12,13,13,14,14,15,15,16,16,17,17,17-Tridecafluoroheptadecan-1-ol","134052-01-0","D",0]
["2,2,3,3,4,4-Hexafluoropentane-1,5-diyl bis(2-methylprop-2-enoate)","918-36-5","D",0]
["Triisopropoxy(3,3,4,4,5,5,6,6,7,7,8,8 ,8- tridecafluorooctyl)- silane","1240203-07-9","D",0]
["1-(1,1,2,3,3,3-Hexafluoropropyl)-1H-imidazole","91047-50-6","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[3,4,5-tris(1,1,2,3,3,3-hexafluoropropoxy)benzoyl]amino]ethyl]-ω-hydroxy-","75836-08-7","D",0]
["Hexanamide, 6-[2,4-bis(1,1-dimethylpropyl)phenoxy]-N-[3-hydroxy-4-[(octafluoro-1-oxopentyl)amino]phenyl]-","97331-50-5","D",0]
["Bis[perfluoro-2-[1-(methyl)ethoxy]ethyl]phosphinic acid ytterbium(3+) salt","500776-84-1","D",0]
["1-Chloro-3-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-46-6","D",0]
["3-(Butane-1-sulfonyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-53-8","D",0]
["Cyclohexyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","78755-41-6","D",0]
["[1,1'-Biphenyl]-2-yl heptafluorobutanoate","90999-92-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-(propan-2-yl)nonanamide","6104-22-9","D",0]
["3,4,4,4‐Tetrafluorobut‐2‐enoic acid","70887-91-1","D",0]
["1,1,1,2,3,3-Hexafluoro-3-[2-(1,1,2,3,3,3-hexafluoropropoxy)ethoxy]propane","479075-22-4","D",0]
["Hexadecafluoro-1,4-piperazinediethanesulfinic acid sodium salt (1:2)","155907-15-6","D",0]
["1-Oxaspiro[4.4]nonane, 2,2,3,3,4,4,6,6,7,7,8,8,9,9-tetradecafluoro-","73187-04-9","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluoro-2-hexanol","116741-81-2","D",0]
["7,8-Dichloro-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","319490-55-6","D",0]
["Sodium 3‐[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11‐icosafluoroundecanoyl)oxy]propane‐1‐sulfonate","29978-19-6","D",0]
["1,3-Bis(2,2,3,3,4,4,4-heptafluorobutoxy)propan-2-ol","1598-17-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Nonadecafluorotetracosane","113659-16-8","D",0]
["1-(Difluoromethoxy)-1,1,2,2,2-pentafluoroethane","53997-64-1","D",0]
["Cyhalodiamide","1262605-53-7","D",0]
["1-Propene, 3,3,3-trifluoro-, polymer with 1-propene and 1,1,2,2-tetrafluoroethene","475654-94-5","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluoropropyl)sulfonyl]amino)-1-propanesulfonate","2089108-88-1","D",0]
["3-(Butane-1-sulfinyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-30-1","D",0]
["Methyl 3-(perfluoropropyl)acrylate","813-06-9","D",0]
["2,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodec-2-enoic acid","71178-11-5","D",0]
["2,2,3,3,3-Pentafluoropropyl trifluoroacetate","603312-66-9","D",0]
["Sulfuric acid--2-bromo-1,1,2,2-tetrafluoroethan-1-ol (1/2)","110346-60-6","D",0]
["4,4-Bis(trifluoromethyl)-3-[(trimethylgermyl)oxy]cyclobut-2-en-1-one","89101-65-5","D",0]
["1-Methyl-2-(nonafluorobutyl)benzene","93697-09-7","D",0]
["Diphenyl[4-(tridecafluorohexyl)phenyl]phosphine","201936-63-2","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1H-cyclopenta[a]naphthalene","922141-63-7","D",0]
["6-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)-3,5,5-trimethylcyclohex-2-en-1-one","101564-50-5","D",0]
["2,2,3,3-Tetrafluoro-3-({1,1,1,2,3,3-hexafluoro-3-[(trifluoroethenyl)oxy]propan-2-yl}oxy)propan-1-ol","133573-37-2","D",0]
["3-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)bicyclo[2.2.1]heptan-2-one","35444-16-7","D",0]
["4-[(2,2,3,3,4,4,5,5-octafluoropentylamino)methylidene]cyclohexa-2,5-dien-1-one","5320-11-6","D",0]
["N-Butyl-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-amine","25291-18-3","D",0]
["1-Acetyl-3,5-bis(perfluorohexyl)pyrazole","231953-34-7","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with ammonia, reduced","161212-19-7","D",0]
["Perfluorooctanesulfonamidoacetic acid","2806-24-8","D",0]
["(1E)-1-Cycloocten-1-yl 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate","36839-96-0","D",0]
["Undecafluorohexanoic acid--piperazine (1/1)","423-47-2","D",0]
["Furan, 2-(difluoromethyl)-2,3,3,4,4,5,5-heptafluorotetrahydro-","65601-68-5","D",0]
["2,3-Dichloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-20-4","D",0]
["Perfluoro-n-[1,2,3,4-13C4]-octanoic acid","960315-48-4","D",0]
["Pentane, 1,1,1,2,2,3,4,5,5,5-decafluoro-, (3R,4R)-","142347-07-7","D",0]
["2‐(N‐Methyl1,1,2,2,3,3,4,4,5,5,6,6,6‐ tridecafluorohexanesulfonamido)acetic acid","715646-50-7","D",0]
["2-(1,1,1,3,3,3-hexafluoropropan-2-ylidene)-7-nitro-3,4-dihydronaphthalen-1(2h)-one","35474-73-8","D",0]
["Lithium(1+) perfluoro‐5‐{[(perfluoropentanesulfonyl)azanidyl]sulfonyl}pentane","288570-49-0","D",0]
["2,3,3,3-Tetrafluoro-2-iodopropanenitrile","192569-12-3","D",0]
["4,4,5,5,5-Pentafluoro-1-(naphthalen-2-yl)pentane-1,3-dione","77459-90-6","D",0]
["[(1Z)-4,4,5,5,6,6,7,7,7-Nonafluorohept-1-en-1-yl]benzene","97041-10-6","D",0]
["Ethyl 2-amino-8-(pentafluoroethyl)-3H-1-benzazepine-4-carboxylate","926927-42-6","D",0]
["(2S)-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoic acid","75579-40-7","D",0]
["(Perfluoropropyl)(perfluorophenyl)methanol","19108-36-2","D",0]
["N-Hexyl-perfluorooctanesulfonamide","89932-70-7","D",0]
["4-Bromo-1,1,1,2-tetrafluoro-2-(trifluoromethyl)butane","1274903-97-7","D",0]
["1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexakis(heptafluoropropyl)-2,2,4,4,6,6-hexahydro-","3862-48-4","D",0]
["2,3,5,5,6,6,7,7-Octafluorocyclohepta-1,3-diene","52137-76-5","D",0]
["Copper, [2,9,16,23-tetrakis(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)-29H,31H-phthalocyaninato(2-)-κN29,κN30,κN31,κN32]-, (SP-4-1)-","1207299-78-2","D",0]
["1,1,1,2,2,3,3,4,4,6,6,8,8-Tridecafluoro-8-iodooctane","99325-17-4","D",0]
["Decafluoro-1,2-dihydronaphthalene","28750-05-2","D",0]
["2,6-difluoro-N-[[4-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)phenyl]carbamoyl]benzamide","74702-96-8","D",0]
["Phenyl[1-phenyl-3,3-bis(trifluoromethyl)aziridin-2-yl]methanone","61860-09-1","D",0]
["1,3-Bis[(3,3,4,4,4-pentafluorobutyl)sulfanyl]propan-2-ol","113107-47-4","D",0]
["13-[4-(Tridecafluorohexyl)phenyl]-3,6,9,12-tetraoxaoctadecan-1-ol","874212-25-6","D",0]
["1,1,1-trifluoro-2-(trifluoromethyl)but-3-en-2-yl 4-bromobenzenesulfonate","36417-23-9","D",0]
["2-(Perfluorobutylsulfanyl)ethanol","113304-06-6","D",0]
["N-(1,1,1,3,3,3-Hexafluoropropan-2-yl)benzamide","2151-49-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-[(trifluoroacetyl)oxy]butanamide","88326-80-1","D",0]
["Propan-2-yl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","145510-88-9","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with ammonia","161212-18-6","D",0]
["Perfluoroethoxy-3-propoxypropane","1464062-44-9","D",0]
["Perfluoropentane sulfonamide","82765-76-2","D",0]
["Nonanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoro- (9CI)","548478-86-0","D",0]
["Ethyl 5,5,5-trifluoro-2-oxo-4-(trifluoromethyl)pentanoate","201930-83-8","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorohexane","38436-17-8","D",0]
["Potassium 4-[[(perfluorobutyl)sulfonyl](propyl)amino]butanoate","864069-32-9","D",0]
["2,2'-[(2,2,3,3,4,4-hexafluoropentane-1,5-diyl)bis(oxy)]diacetic acid","3801-88-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-(4-methylphenyl)heptan-1-one","88950-96-3","D",0]
["4-(Dimethylamino)phenyl nonafluorobutane-1-sulfonate","1463426-91-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15-Hentriacontafluoropentadecane","66826-88-8","D",0]
["Perfluorotridecanedioic acid","344760-77-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecyl trifluoromethanesulfonate","171182-85-7","D",0]
["1-(1,1,2,2-Tetrafluoroethoxy)-4-(2,4,4-trimethylpentan-2-yl)benzene","163036-61-1","D",0]
["2-[(1,1,1,3,3,3-Hexafluoropropan-2-yl)amino]phenol","85290-64-8","D",0]
["Hexafluoroacetone azine","1619-84-7","D",0]
["Ethyl 4,4,4-trifluoro-3-(trifluoromethyl)butanoate","17327-34-3","D",0]
["4,4,5,5,6,6,6-Heptafluorohex-1-en-2-yl acetate","136909-80-3","D",0]
["Tris(1H,1H-heptafluorobutyl)phosphate","563-09-7","D",0]
["2,2,2-Trifluoro-1-[4-(tridecafluorohexyl)phenyl]ethan-1-one","171183-94-1","D",0]
["8:2 Fluorotelomer phosphate diester ion (1-)","1411713-91-1","D",0]
["1-Chloro-4-[(1,1,2,2,3,3,4,4-octafluorobutyl)sulfanyl]benzene","138451-16-8","D",0]
["3,3,4,4,4-Pentafluoro-2-methylbutanal","111160-49-7","D",0]
["2,2,3,3,4,4,5-Heptafluoro-5-(heptafluoropropyl)oxolane","423-22-3","D",0]
["Perfluoro-2-methylbutane","594-91-2","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluorohexanamide","154380-34-4","D",0]
["Substance listed under Molecular formula - (CF2)4CH (OH)-","16621-87-7","D",0]
["1,1,1,6,6,6-Hexafluoro-2,5-bis(trifluoromethyl)hex-3-ene","671226-03-2","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl thiocyanate","26650-08-8","D",0]
["N-Bromo-2,2,3,3,4,4,4-heptafluorobutanimidoyl fluoride","89554-92-7","D",0]
["1-(Difluoromethyl)-2,3,3,4,4,5,5,6,6-nonafluorocyclohex-1-ene","10534-43-7","D",0]
["3,5,7,8-Tetrachloroperfluorooctanoic acid","2923-68-4","D",0]
["2,2,3,4,4,4-Hexafluorobutanal","1823087-30-4","D",0]
["2-Propenoic acid, 2-methyl-, docosyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate and octadecyl 2-methyl-2-propenoate","1040209-02-6","D",0]
["3-(1,1,1,2,3,3,3-Heptafluoropropane-2-sulfonyl)benzoic acid","88489-81-0","D",0]
["2,2,3,3,4,5,5,5-Octafluoro-4-(trifluoromethyl)pentanoyl chloride","88639-59-2","D",0]
["1,1,1,2,2-Pentafluoro-6-methylhept-4-en-3-one","89176-02-3","D",0]
["Ammonium bis(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9‐hexadecafluorononyl) phosphate","7757-53-1","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-tetracosafluorododecane-1-sulfonic acid","134615-58-0","D",0]
["2-Chloro-N-[4-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)phenyl]-N-methylacetamide","294196-95-5","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-(4-methoxyphenyl)hexane-1,3-dione","515163-04-9","D",0]
["2-Chloro-1,1,1,4,4,5,5,5-octafluoro-2-(trifluoromethyl)pentan-3-one","83714-48-1","D",0]
["3:3 Fluorotelomer carboxylate, ion(1-)","1169706-83-5","D",0]
["(2R)-2-{[2,2-Bis(trifluoromethyl)aziridin-1-yl]oxy}propanamide","213017-42-6","D",0]
["Nonane, 1,1'-[1,4-butanediylbis(oxy)]bis[heptadecafluoro","84029-51-6","D",0]
["Perfluorosebacamide","307-77-7","D",0]
["N-Ethyl-perfluorobutane-1-sulfonamide","40630-67-9","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-Octadecafluoroundec-1-yne","90441-62-6","D",0]
["1,1,1,2-Tetrafluoro-2-(trifluoromethoxy)butane","200501-98-0","D",0]
["9H-Fluoren-9-one O-[(perfluorobutyl)sulfonyl]oxime","639782-56-2","D",0]
["Chlorodipropyl(3,3,4,4,4-pentafluorobutyl)silane","608296-02-2","D",0]
["(Heptafluoropropyl)trimethylsilane","3834-42-2","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl trifluoroacetate","24165-10-4","D",0]
["1,2,3,5,5,6,6,7,7-Nonafluorobicyclo[2.2.1]hept-2-ene","5074-57-7","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-[(undecafluoropentyl)oxy]propanoate","220369-95-9","D",0]
["(Heptadecafluorooctyl)cycloheptane","172369-52-7","D",0]
["(4Z)-1,1,1,2,4,5,6,7,7,7-Decafluoro-2,6-bis(trifluoromethyl)hept-4-en-3-one","134330-95-3","D",0]
["1,3-Bis(1,1,1,3,3,3-hexafluoro-2-methoxypropan-2-yl)benzene","53896-18-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluoro-5-[1,1,2,3,3,3-hexafluoro-2-(trifluoromethyl)propoxy]pentane","169477-62-7","D",0]
["Dibutylbis[(2,2,3,3,4,4,4-heptafluorobutanoyl)oxy]stannane","90499-38-0","D",0]
["Methanaminium perfluorononanoate","77032-23-6","D",0]
["2-(Pentafluoroethyl)-4H-pyran-4-one","1353572-35-6","D",0]
["4,5,5,5-Tetrafluoro-4-(trifluoromethyl)-2-pentanone","261760-96-7","D",0]
["1,4-Benzenedimethanol, α1,α1,α4,α4-tetrakis(trifluoromethyl)-, hydrate (1:1)","304851-82-9","D",0]
["Perfluorobutanol","3056-01-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,7,7-Tetradecafluoro-7-methoxyheptane","355-70-4","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(propane-1-sulfonyl)benzoic acid","1355555-13-3","D",0]
["1-Isocyanato-4-(nonadecafluorononyl)benzene","93238-00-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-phenylpropyl)butanamide","70414-03-8","D",0]
["(Dimethoxymethyl)(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","83868-08-0","D",0]
["(1R,2R,5S,6S)-3,3,4,4-Tetrafluoro-9-oxatricyclo[4.2.1.0~2,5~]non-7-ene","958885-20-6","D",0]
["1,1,1,2,2-Pentafluorooctan-3-one","108214-46-6","D",0]
["Perfluoro(ethyl vinyl ether)-perfluoro(propyl vinyl ether)-tetrafluoroethylene copolymer","546114-40-3","D",0]
["1-Bromo-1,1,2,2-tetrafluoro-4-iodobutane","129587-49-1","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluoro-4-methyldecan-3-one","56778-56-4","D",0]
["Chlorotris(2,2,3,3,4,4,4-heptafluorobutoxy)silane","757-72-2","D",0]
["5-Methyl-3,3-bis(trifluoromethyl)-2,1lambda~4~-benzoxathiol-1(3H)-one","57565-55-6","D",0]
["Tris[1,1,2,2,3,4,4,4-octafluoro-3-(trifluoromethyl)butyl](oxo)-lambda~5~-phosphane","61908-82-5","D",0]
["N,N'-1,2-phenylenebis(perfluorobutanamide)","548479-70-5","D",0]
["2-(1,2,2,2-Tetrafluoroethyl)quinazolin-4(1H)-one","63099-85-4","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(2,2,3,3-tetrafluoropropoxy)propane","176310-29-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluorodecyl 2-methylprop-2-enoate","23069-32-1","D",0]
["3-Hydroxy-3-methyl-4-pentyn-1-yl perfluoro-2-[2-(propoxy)propoxy]propanoate","1592562-40-7","D",0]
["Nonanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","573996-67-5","D",0]
["14-H-Perfluorotetradecanoic acid","2274731-00-7","D",0]
["1-[(4,4,5,5,6,6,7,7,7-Nonafluoroheptanoyl)oxy]pyrrolidine-2,5-dione","852527-43-6","D",0]
["Bis(dimethylamino)-N,N-dimethylmethaniminium heptafluoropropan-2-olate","479024-69-6","D",0]
["Difluoro(perfluoropropoxy)acetic acid","919005-50-8","D",0]
["N,N'-bis(Perfluorobutanoyl)1,3-propanediamine","149981-59-9","D",0]
["2-Bromo-1,3-dichloro-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzene","353272-59-0","D",0]
["1-Bromo-3-(2,2,3,3,4,4,4-heptafluorobutoxy)benzene","1365808-77-0","D",0]
["2-[Bis(trifluoromethyl)amino]-2,3,3,3-tetrafluoropropionyl fluoride","58599-98-7","D",0]
["N-[4-(Morpholine-4-carbonyl)benzoyl]valyl-N-(5,5,6,6,6-pentafluoro-2-methyl-4-oxohexan-3-yl)prolinamide","163660-59-1","D",0]
["4,5-Pentanedione, 2-hydroxy-5-(p-nitrophenyl)-1,1,1-trifluoro-2-(trifluoromethyl)-","101931-60-6","D",0]
["Perfluoro-4-oxopentane-1-sulfonic acid","2254560-25-1","D",0]
["3-Bromo-2,2,3,3-tetrafluoropropanoyl chloride","64053-15-2","D",0]
["2-[(Pentafluoroethyl)sulfanyl]ethan-1-amine","1208078-70-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodohexadecane","129838-38-6","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(trifluoromethoxy)propane","59426-77-6","D",0]
["2,2,3-Trifluoro-1-methyl-3-(trifluoromethyl)-2,3-dihydro-1H-inden-1-ol","62409-60-3","D",0]
["3,3,4,4-Tetrafluoro-2-methylbut-1-ene","57252-78-5","D",0]
["1,2-Butadiene, 1,1-diethoxy-4,4,4-trifluoro-3-(trifluoromethyl)-","76790-81-3","D",0]
["N-[2-[3-[[(Perfluorooctyl)sulfonyl]amino]propoxy]ethyl]-2-hydroxy-N,N-dimethylethanaminium bromide","89447-44-9","D",0]
["Tetradecafluoroheptan-4-one","378-90-5","D",0]
["Diazene, (1,2,2,3,3,4,4,5,5-nonafluorocyclopentyl)phenyl-","97388-28-8","D",0]
["HFE–329mcc2","134769-21-4","D",0]
["2,6-Di-tert-butyl-4-(pentafluoroethyl)phenol","89520-76-3","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-methylpropyl)butanamide","75668-25-6","D",0]
["Difluoro(1,1,2,2-tetrafluoro-2-iodoethoxy)acetonitrile","98296-50-5","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoropentyl 2,5,7-trinitro-9-oxo-9H-fluorene-4-carboxylate","253605-71-9","D",0]
["2-Amino-1-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]propan-1-ol--hydrogen chloride (1/1)","70126-68-0","D",0]
["3-[{3-[(Carboxymethyl)(perfluoropentanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","2254560-23-9","D",0]
["N-((2-Bromo-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-66-0","D",0]
["1-Bromo-2-[(1R)-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-(methoxymethoxy)octyl]benzene","835624-47-0","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α,α'-[1,6-hexanediylbis[imino[1-fluoro-2-oxo-1-(trifluoromethyl)-2,1-ethanediyl]]]bis[ω-(1,1,2,2,3,3,3-heptafluoropropoxy)-","1198429-17-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8-DODECAFLUORO-2-OCTANOL","156122-84-8","D",0]
["Butyl 2,2,3,3,4,4,5-heptafluorohexanoate","66152-49-6","D",0]
["2-(Acetyloxy)-N-(carboxymethyl)-N,N-dimethyl-3-(perfluorohexadecyl)-1-propanaminium","1296786-53-2","D",0]
["2-[[5-(Heptafluoropropyl)-1-isoquinolinyl]methylene]-hydrazinecarbothioamide","31181-05-2","D",0]
["4-tert-Butyl-2,6-bis(1-hydroxy-1-(trifluoromethyl)-2,2,2-trifluoroethyl)iodobenzene","101697-28-3","D",0]
["4-[3-(Perfluorobutyl)-1-propyloxy]benzyl alcohol","892154-51-7","D",0]
["2,2,3,3,7,7,8,8-Octafluoro-1,4,6,9-tetraoxaspiro[4.4]nonane","92639-88-8","D",0]
["(2S)-2-Amino-5,5,6,6,6-pentafluorohexanoic acid","148043-95-2","D",0]
["1,3,4,4,5,6,6,7,8,8,9,9,10,10-Tetradecafluorotricyclo[3.3.1.1~3,7~]decan-2-one","141635-73-6","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluorohepta-1,2-diene","132673-98-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl nonanoate","78509-68-9","D",0]
["N~3~-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)methyl]-beta-alaninamide","87988-60-1","D",0]
["2-Propenoic acid, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl ester, polymer with octadecyl 2-propenoate","425664-29-5","D",0]
["Propane, 1,1-dichloro-1,2,3,3,3-pentafluoro-","111512-56-2","D",0]
["Perfluorosebaconitrile","2342-09-8","D",0]
["Bis(1,1,1,3,3,3-hexafluoropropan-2-yl) propanedioate","389580-57-8","D",0]
["Dimethyl (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)phosphonatato","61726-44-1","D",0]
["N-[(Perfluorobutyl)phenyl-lambda4-sulfanylidene]acetamide","1178899-18-7","D",0]
["4,5,6,7-Tetrafluoro-3-(nonafluorobutyl)-1H-indazole","1610931-28-6","D",0]
["Difluoro(trifluoromethoxy)acetyl fluoride","690-43-7","D",0]
["Perfluoro-1,3-dimethyladamantane","36481-20-6","D",0]
["3-[(Perfluorooctylsulfonyl)(propyl)amino]-N,N,N-trimethyl-1-propanaminium","166441-47-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,25,25,26,26,27,27,28,28,29,29,30,30,31,31,32,32,33,33,34,34,35,35,36,36,36-Pentacontafluorohexatriacontane","100550-11-6","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N-methyl-N-[(trichloromethyl)sulfanyl]butane-1-sulfinamide","51735-86-5","D",0]
["(2S)-2-Pyrrolidinyl-bis(4-(perfluorooctyl)phenyl)methanol","862589-19-3","D",0]
["3-Perfluoroheptene","71039-88-8","D",0]
["5-Methyl-3,3-bis(trifluoromethyl)-3H-2,1-benzoxathiole","57565-50-1","D",0]
["1-(2,2,3,3,4,4,4-Heptafluorobutoxy)ethyl acetate","378-08-5","D",0]
["1,1,1,2,2,3,3-Heptafluorohexane","678-98-8","D",0]
["Phenol, 4-(heptafluoropropyl)-2-nitro-","61324-29-6","D",0]
["(5E)-1,1,1,2,2,3,3,4,4-Nonafluoro-6-iodododec-5-ene","109574-88-1","D",0]
["2,2,3,3-Tetrafluoro-1,4-butyl diacrylate","125658-77-7","D",0]
["3,3,4,4,5,5,5-Heptafluoro-1-(pyrrolidin-1-yl)-2-(trifluoromethyl)pentan-1-one","89810-85-5","D",0]
["3,5,7,8-Tetrachloro-2,2,3,4,4,5,6,6,7,8,8-undecafluorooctanoic acid--piperazine (1/1)","1511-09-7","D",0]
["Tris(2,2,3,3,3-pentafluoropropyl)phosphate","25476-41-9","D",0]
["3,3,4,4-Tetrafluoro-2,2,5,5-tetrakis(trifluoromethyl)oxolane","110719-86-3","D",0]
["3:2 Fluorotelomer carboxylic acid","679-46-9","D",0]
["3-(Bromomethyl)-1,1,1,2,2,4,4,5,5,6,6,6-dodecafluorohexan-3-ol","93417-72-2","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymer with chloroethene, N,N-dimethyl-2-propenamide, α-fluoro-ω-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and 2-hydroxyethyl 2-propenoate (9CI)","152286-20-9","D",0]
["2,4-Difluoro-N-(2-fluoro-5-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862133-29-7","D",0]
["1,1,1,2,2-Pentafluoroocta-4,6-dien-3-one","89176-06-7","D",0]
["1-(2,2,3,4,4,4-Hexafluorobutyl)-3-methylbenzene","54974-26-4","D",0]
["Ethyl [5-(heptafluoropropyl)-1H-pyrazol-3-yl]acetate","1428569-15-6","D",0]
["2-(2,5-Dimethylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","28180-47-4","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1-(nonafluorocyclopentyl)pyrrolidine","86714-20-7","D",0]
["(Pentafluoroethyl)carbonimidoyl","428-71-7","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl tetradecanoate","138762-92-2","D",0]
["Chloro(3,3,4,4,5,5,6,6,6-nonafluorohexyl)bis(3,3,3-trifluoropropyl)silane","608296-86-2","D",0]
["Trifluoro(trifluoromethoxy)methane","1479-49-8","D",0]
["N-2-Pyrimidinylperfluoro-2-(2-propoxypropoxy)propanamide","340131-92-2","D",0]
["1,2,3,3,3-Pentafluoro-1-methoxyprop-1-ene","666-92-2","D",0]
["Cyclopropane, pentafluoro(heptafluoropropoxy)-","131393-36-7","D",0]
["2(1H)-Quinoxalinone, 3-(1,1,2,2-tetrafluoroethyl)-","89995-27-7","D",0]
["Trimethoxy(4,4,5,5,6,6,7,7,7-nonafluoroheptyl)silane","95681-08-6","D",0]
["(1r,4r)-4-(Nonafluorobutyl)cyclohexane-1-carboxylic acid","88951-25-1","D",0]
["N-(2,6-Dimethylphenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","101948-89-4","D",0]
["Fulvestrant sulfone","98008-06-1","D",0]
["2,3,4-Trifluoro-4-(trifluoromethyl)pent-2-enedinitrile","88866-64-2","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with ammonia, dehydrated","161212-29-9","D",0]
["4,4,4-trifluoro-3-hydroxy-1-(4-methoxyphenyl)-2-methyl-3-(trifluoromethyl)butan-1-one","34844-28-5","D",0]
["1-[2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)-1-(piperidin-1-yl)propyl]-1H-benzotriazole","133384-08-4","D",0]
["1H,1H,5H-perfluoropentyl 2-fluoroacrylate","87910-92-7","D",0]
["4-(Heptadecafluorooctyl)-N,N-dimethylbenzenamine","80791-09-9","D",0]
["Perfluorobut-3-ene-1-sulfonyl fluoride","264879-61-0","D",0]
["5-Chloro-2-(2-chloro-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)phenyl acetate","38506-72-8","D",0]
["1,1,1,3,4,4,4-Heptafluoro-2,3-bis(trifluoromethyl)butan-2-ol","16500-37-1","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutyl)phenyl dibutyl-phosphinate","7526-47-8","D",0]
["6-(Pentafluoroethyl)pyridin-3-ol","1346539-65-8","D",0]
["1,3,4,4,4-Pentafluoro-3-(trifluoromethyl)but-1-yne","105774-98-9","D",0]
["2-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Nonadecafluorodec-1-en-1-yl)oxy]benzoic acid","57344-87-3","D",0]
["Ethyl 3-(2,2-dichloroethenyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylate","99903-43-2","D",0]
["N,N'-Bis{[(1,1,1,3,3,3-hexafluoropropan-2-ylidene)amino]sulfanyl}urea","62735-45-9","D",0]
["(1s,4s)-4-(Nonafluorobutyl)cyclohexane-1-carboxylic acid","88951-24-0","D",0]
["2-[4-(Benzyloxy)-2,2,3,3-tetrafluorobutoxy]ethan-1-ol","663176-03-2","D",0]
["4-[(1,2,3,3,3-Pentafluoroprop-1-en-1-yl)oxy]benzoic acid","96210-33-2","D",0]
["2-(((4-(4-(((2-(Methyl((nonafluorobutyl)sulfonyl)amino)ethoxy)carbonyl)amino)benzyl)phenyl)carbamoyl)oxy)ethyl prop-2-enoate","856220-62-7","D",0]
["Carbonic acid--2,2,3,4,4,4-hexafluorobutan-1-ol (1/2)","847755-25-3","D",0]
["(3β,5α,6α)-5,6-Epoxy-25,26,26,26,27,27,27-heptafluorocholestan-3-ol","240129-21-9","D",0]
["Silicic acid (H4SiO4), tetrakis[2,2,2-trifluoro-1-(trifluoromethyl)ethyl] ester","26560-90-7","D",0]
["4-(Heptafluoropropyl)cyclohexane-1-carboxylic acid","88951-29-5","D",0]
["6-Chloro-perfluorohexanoate","127843-88-3","D",0]
["2,2,3,3-Tetrafluoropropyl (3-nitrophenyl)carbamate","90687-70-0","D",0]
["1,1,1,2,2-Pentafluorobutane","37826-35-0","D",0]
["2,2',3,3',5,5',6,6'-Octafluoro-4,4'-bis(pentafluoroethyl)-1,1'-biphenyl","54755-50-9","D",0]
["1-Bromoundecafluorocyclohexane","336-13-0","D",0]
["1-[(2S)-2-(2,4-Dichlorophenyl)-3-(1,1,2,2-tetrafluoroethoxy)propyl]-1H-1,2,4-triazole","131320-42-8","D",0]
["1,8-Dibromoperfluorooctane","812-58-8","D",0]
["N-[3-[(Perfluoro-1-oxononyl)propylamino]propyl]-N,N-dimethylbenzenemethanaminium chloride","89932-72-9","D",0]
["2-Pyridinecarboxaldehyde, 6-(2-hydroxy-3,3,3-trifluoro-2-(trifluoromethyl)propyl)-","102206-46-2","D",0]
["2,2,3,4,4,4-Hexafluoro-1-phenylbutan-1-one","60375-79-3","D",0]
["4-(1,1-Difluoroethoxy)-1,1,1,2,2,3,3-heptafluorobutane","1365808-20-3","D",0]
["1-Piperidinemethanol, alpha,alpha-bis(trifluoromethyl)-, hydrate","30192-67-7","D",0]
["Chloro(1,1,2,3,3,3-hexafluoropropyl)dimethylsilane","62281-34-9","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, ion(1-)","45187-15-3","D",0]
["3-([(Perfluorooctyl)sulfonyl]{3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}amino)-2-hydroxy-1-propanesulfonate","697218-72-7","D",0]
["3,3,4,4-Tetrafluorocyclobutane-1,2-dione","663-45-6","D",0]
["2-Trifluoromethyl-3H-perfluoro-2-pentene","90277-94-4","D",0]
["1-[(Heptafluoropropyl)(propan-2-yl)amino]-3-[(naphthalen-1-yl)oxy]propan-2-ol--hydrogen iodide (1/1)","149825-35-4","D",0]
["N-(Butan-2-yl)-2,2,3,3,4,4,4-heptafluorobutanamide","75668-26-7","D",0]
["Perfluoro-3-pentanone","684-32-2","D",0]
["(5E)-5,6-Perfluorodecene","97539-76-9","D",0]
["Methyl 2-chloro-3,3,4,4,5,5,6,6,6-nonafluorohexanoate","116356-70-8","D",0]
["4,4,5,5,5‐Pentafluoro‐1‐(methylamino)pentan‐2‐ol","2357390-87-3","D",0]
["Dimethyl perfluorononanedioate","22116-90-1","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluoroethyl)sulfonyl]amino)-1-propanesulfonate","2089108-87-0","D",0]
["2-Bromo-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-23-7","D",0]
["Bis(perfluoropropanesulfonyl)amine","152894-12-7","D",0]
["Methyl 2,2,3,3,4,4,4-heptafluorobutanimidate","2992-92-9","D",0]
["3-[[Perfluorodecyl)sulfonyl](2-hydroxyethyl)amino]-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","767248-33-9","D",0]
["N-[4-(3,4-Difluorophenyl)-1,3-thiazol-2-yl]-2,2,3,3,4,4,4-heptafluorobutanamide","299198-90-6","D",0]
["2-[Chloro(fluoro)methoxy]-1,1,1,2-tetrafluoroethane","56885-28-0","D",0]
["2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]-propanoic acid methyl ester","26131-32-8","D",0]
["3-(2,2,3,3-Tetrafluoropropanoyl)-4H-1-benzopyran-4-one","858369-42-3","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide and phosphoryl trichloride, hydrolyzed, salts with 2,2'-nitrilodiethanol","162567-75-1","D",0]
["N-((2,5-Dimethyl-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-69-3","D",0]
["1,2,3,4-Tetrafluoro-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)benzene","112754-12-8","D",0]
["Methyl 2H,2H-perfluorobutyl ether","376-98-7","D",0]
["1-(2,5-dichlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-one","35444-00-9","D",0]
["1,1,1,5,5,6,6,10,10,10-Decafluoro-3,3,8,8-tetrakis(trifluoromethyl)-2,4,7,9-tetraoxadecane","95841-80-8","D",0]
["11-{[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl]oxy}undecanoic acid","62789-48-4","D",0]
["Tiflamizole","62894-89-7","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoro-N-pyridin-2-ylheptanamide","6396-41-4","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1′-[(1,2-difluoro-1,2-ethenediyl)bis(oxy)]bis[1,1,2,2,3,3,3-heptafluoropropane] and tetrafluoroethene","235775-93-6","D",0]
["2-bromo-2,3,3,3-tetrafluoropropanamide","422-22-0","D",0]
["2-Methyl-1-(1,1,2,2-tetrafluoroethoxy)propane","18180-34-2","D",0]
["Carbonic acid--2,2,3,3,3-pentafluoropropan-1-ol (1/2)","154496-21-6","D",0]
["6-tert-Butyl-2-ethoxy-4,4-bis(trifluoromethyl)-1,3,2-dioxaborinane","100991-78-4","D",0]
["Benzyl heptadecafluorononanoate","117374-38-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluoro-6-methoxyhexane","1391033-26-3","D",0]
["[Ethyl(3-{[(heptadecafluorooctyl)sulfonyl]amino}propyl)amino]oxidanide","","D",0]
["Methyl 3-(chlorosulfonyl)-2,2,3,3-tetrafluoropropanoate","77705-96-5","D",0]
["Trimethyl(3‐{2‐[(perfluoroethyl)ethylthio]acetamido}propyl)azanium","","D",0]
["1-(2-Chloro-1,2-difluoroethoxy)-1,1,2,2-tetrafluoroethane","185418-82-0","D",0]
["2-[(Nonadecafluorononyl)oxy]ethan-1-ol","675868-33-4","D",0]
["1-Ethenyl-4-(2,2,3,3,4,4,4-heptafluorobutoxy)benzene","111144-99-1","D",0]
["2-Vinylperfluoropropane","88562-41-8","D",0]
["Benzenemethanol, 4-amino-α,α-bis(trifluoromethyl)-","722-92-9","D",0]
["3-Fluoro-4-{(E)-[4'-(heptafluoropropyl)[1,1'-biphenyl]-4-yl]diazenyl}phenol","113448-90-1","D",0]
["Cyclohex-1-en-1-yl nonafluorobutane-1-sulfonate","36839-95-9","D",0]
["2-(2-Amino-3-bromo-5-methylphenyl)-1,1,1,3,3,3-hexafluoro-2-propanol","80360-40-3","D",0]
["2-(3,4-Dibromo-1,1,2,2,3,4,4-heptafluorobutyl)-2,3,3-trifluorooxirane","91095-95-3","D",0]
["6-[1,2,2,2-Tetrafluoro-1-(trifluoromethyl)ethyl]-2,4(1H,3H)-quinazolinedione","1433216-71-7","D",0]
["1,1,1-Trifluoro-4,4-dimethoxy-2-(trifluoromethyl)but-3-en-2-ol","63504-97-2","D",0]
["{[(1-Bromo-1,2,2,2-tetrafluoroethyl)sulfanyl]methyl}benzene","111860-56-1","D",0]
["[(Heptafluoropropyl)sulfanyl]acetic acid","204057-69-2","D",0]
["Perfluoro-2-ethoxyethanesulfonyl fluoride","67990-78-7","D",0]
["Hexyl perfluorobutanoate","336-65-2","D",0]
["Pyrimidin-2-yl heptafluorobutanoate","116353-73-2","D",0]
["2-(1-Ethoxy-1,2,2,3,3,4,4,4-octafluorobutyl)aniline","217474-47-0","D",0]
["HFE–329me3","428454-68-6","D",0]
["4‐Ethyl‐1‐(1,1,2,2,2‐pentafluoroethyl)‐2,6,7‐trioxabicyclo[2.2.2]octane","31185-66-7","D",0]
["(7.alpha.)-3-hydroxy-7-[9-[(4,4,5,5,5-pentafluoropentyl)sulfinyl]nonyl]-estra-1,3,5(10)-trien-17-one","403656-89-3","D",0]
["Allyl 1H,1H-heptafluorobutyl ether","648-42-0","D",0]
["1-[(4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononanoyl)oxy]pyrrolidine-2,5-dione","1262770-54-6","D",0]
["2,2,3,3,3-Pentafluoro-1-(2,2,3,3,3-pentafluoropropoxy)propan-1-ol","648430-14-2","D",0]
["1-Bromo-3,3,4,4-tetrafluoropyrrolidine-2,5-dione","425-36-5","D",0]
["2-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoro-1,1-Dimethylundecyloxy)Carbonyloxyimino]-2-Phenylacetonitrile","350716-42-6","D",0]
["1-Methyl-3-(pentafluoroethyl)benzene","133512-63-7","D",0]
["5-Bromo-4,4,5,5-tetrafluoropent-1-ene","89965-92-4","D",0]
["2,2,3,4,4,5,5,6,6,7,7-undecafluoroheptan-1-ol","82793-41-7","D",0]
["1-Undecanamine, N,N-dimethyl-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-, N-oxide","30295-52-4","D",0]
["Heptafluorobutanoic acid anhydride, compd. with dihexyl phosphonate (2:1)","110086-60-7","D",0]
["1,1,1,3,3,3-Hexafluoro-2-phenylpropan-2-yl 2-methylprop-2-enoate","130540-87-3","D",0]
["Methyl perfluoroundecanoate","203302-98-1","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1,6-diphenylhexane-1,6-dione","2525-80-6","D",0]
["1,3,3,4,4,5,5-Heptafluoro-2-(trifluoromethyl)cyclopent-1-ene","780-87-0","D",0]
["3,5-Diphenyl-2,2-bis(trifluoromethyl)-2,3-dihydro-1,3-oxazole","61909-93-1","D",0]
["1,1,2,2,3,3,4,4,5-Nonafluorocyclohexane","62422-03-1","D",0]
["4-Heptadecafluorooctyl-phenol","80804-82-6","D",0]
["1-bromo-4,4,5,5,6,6,6-heptafluoro-3,3-bis(trifluoromethyl)hex-1-ene","128454-94-4","D",0]
["4,4'-(2,2,3,3,4,4,5,5-Octafluorocyclopentane-1,1-diyl)diphenol","136525-92-3","D",0]
["1-[(Heptafluoropropyl)sulfanyl]-4-methylbenzene","69127-70-4","D",0]
["2-[1,1,2-Trifluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)ethoxy]acetic acid","919005-33-7","D",0]
["{[(Heptafluoropropyl)sulfanyl]methyl}benzene","68409-04-1","D",0]
["N,N'-bis(2-aminophenyl)-2,2,3,3,4,4-hexafluoropentanediamide","79834-53-0","D",0]
["5-Bromo-1,3,3,4,4,6,6-heptafluoro-2-(trifluoromethyl)cyclohex-1-ene","79150-81-5","D",0]
["4-(Perfluorobutyl)-3,3-difluorobutanol 1-(dihydrogen phosphate) ammonium salt (1:2)","1025044-20-5","D",0]
["1,1,1,5,5,6,6,7,7,8,8,9,9,10,10,10-hexadecafluorodecane-2,4-dione","147874-76-8","D",0]
["Perfluorooctane sulfonic anhydride","423-92-7","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl)sulfonyl]propylamino]ethyl]-ω-(4-sulfobutoxy)-, lithium salt","441765-16-8","D",0]
["Propanoic acid, 3-chloro-2,2,3,3-tetrafluoro-","661-82-5","D",0]
["Propyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","145510-87-8","D",0]
["6-(Heptafluoropropyl)pyridine-3-carboxylic acid","1105981-44-9","D",0]
["Tetrafluorosuccimide","377-33-3","D",0]
["1-Bromo-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-hexadecafluorooctane","89740-38-5","D",0]
["Perfluoro-3,6-dioxadecanoic acid","137780-69-9","D",0]
["Dimethyl perfluoroheptanedioate","54404-53-4","D",0]
["2-(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)propane-1,3-diol","152220-76-3","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptyl)sulfonyl]amino]ethyl ester, polymer with octadecyl 2-propenoate and 2-propenoic acid","67939-37-1","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,10,10,10-Pentadecafluorodecyl prop-2-enoate","252669-70-8","D",0]
["1-Chloro-1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethane","1561-50-8","D",0]
["2,2,3,3-Tetrafluorobutane","421-74-9","D",0]
["1-Propanesulfonic acid, 1,1,2,3,3,3-hexafluoro-","357-31-3","D",0]
["Pyrrolidine, 3,3,4,4-tetrafluoro-, hydrochloride (1:1)","1810-13-5","D",0]
["3-(Ethanesulfinyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355554-87-8","D",0]
["2,2,3,3,4,4,4-Heptafluorobutanethioamide","375-20-2","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluorododecanamide","199524-07-7","D",0]
["D-chiro-Inositol, 3-O-[2-amino-4-[(carboxyiminomethyl)amino]-2,3,4,6-tetradeoxy-alpha-D-arabino-hexopyranosyl]-, mixt. with 2-chloro-N-[3-[[[2,6-dimethyl-4-[perfluoro-propyl]phenyl]amino]carbonyl]-2-fluorophenyl]-N-methyl-3-pyridinecarboxamide","922147-45-3","D",0]
["2,5-Furandione, polymer with 2-methyl-3-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethoxy]-1-propene, sodium salt","38467-17-3","D",0]
["17-H-Perfluoroheptadecanoate","1696259-88-7","D",0]
["Heptadecafluoro-1-Octanesulfonyl Chloride","423-60-9","D",0]
["1,1-dibromo-3,3,4,4,4-pentafluorobutan-2-one","203302-96-9","D",0]
["Ethene, 1-[difluoro(trifluoromethoxy)methoxy]-1,2,2-trifluoro-, polymer with 1,1-difluoroethene, 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","870707-45-2","D",0]
["Heptadecafluorononanoic acid--N-ethylethanamine (1/1)","77032-27-0","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl butanoate","2926-44-5","D",0]
["Nonane, 1,1'-[1,6-hexanediylbis(oxy)]bis[heptadecafluoro-","84029-57-2","D",0]
["Estra-1,3,5(10)-triene-3,17-diol, 7-[9-[(4,4,5,5,5-pentafluoropentyl)sulfinyl]nonyl]-, (7α,17β)-","129453-61-8","D",0]
["3-(tert-Butylsulfanyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-16-3","D",0]
["N-(2-Hydroxyethyl)perfluorobutanamide","377-66-2","D",0]
["{[(Perfluorodecyl)sulfonyl]amino}acetic acid","865-83-8","D",0]
["4-[(4,4,5,5,6,6,6-Heptafluorohexyl)(dimethyl)silyl]morpholine","197018-78-3","D",0]
["2,2,4-Trichloro-4,6,6-tris(2,2,3,3-tetrafluoropropoxy)-1,3,5,2lambda~5~,4lambda~5~,6lambda~5~-triazatriphosphinine","65601-41-4","D",0]
["1-Benzoyl-3,5-bis(perfluorohexyl)pyrazole","230295-10-0","D",0]
["1,1-Difluoroethene, polymer with tetrafluoroethene, perfluoro(3-methoxypropyl vinyl ether), and bromotrifluoroethene","543698-27-7","D",0]
["Perfluoro-7-nonene-1-sulfonic acid","2089109-44-2","D",0]
["2,2,3,3,4,4,5,5-octafluoro-N-(5-methyl-1,3-benzothiazol-2-yl)pentanamide","6396-20-9","D",0]
["(Chloromethyl)(pentafluoroethyl)phosphinic chloride","105263-73-8","D",0]
["(2S)-2-{Bis[4-(heptadecafluorooctyl)phenyl][(triethylsilyl)oxy]methyl}pyrrolidine","914391-37-0","D",0]
["(2R)-2-(Acetyloxy)-3-(hexadecyloxy)propyl heptafluorobutanoate","119206-62-1","D",0]
["1-[(Tridecafluorohexyl)oxy]nonane","113659-14-6","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with glycine","161212-26-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Hexadecafluorodecan-1-ol","29803-16-5","D",0]
["3-(Heptafluoropropyl)-1H-1,2,4-triazol-5-amine","25979-02-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-Heptacosafluoropentacosane","677324-22-0","D",0]
["4-(1,1,2,2,3,3,3-Heptafluoropropane-1-sulfonyl)benzoic acid","88489-80-9","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-[2-[[(heptadecafluorooctyl)sulfonyl]propylamino]ethyl]-omega-(4-sulfobutoxy)-","734499-39-9","D",0]
["3-Bromo-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridine","1816285-38-7","D",0]
["2-(2-Chloro-1,1,2,2-tetrafluoroethoxy)-1,1,2,2-tetrafluoroethane-1-sulfonyl azide","144951-86-0","D",0]
["3-(2-Chloroethyl)-1,1,1,7,7,7-hexafluoro-2,6-dihydroxy-2,6-bis(trifluoromethyl)heptan-4-one","101913-82-0","D",0]
["1,1,1,2,3,3,3-Heptafluoropropan-2-yl","3248-60-0","D",0]
["Benzenamine, N-methyl-4-[2-(4-nitrophenyl)diazenyl]-N-(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl)-","297140-61-5","D",0]
["7:2 Fluorotelomer phosphate diester","63295-25-0","D",0]
["1-Ethoxy-1,1,3,3,3-pentafluoro-2-(trifluoromethyl)propane","380-30-3","D",0]
["Butanediamide, 2,2,3,3-tetrafluoro-N1,N4-bis[4-(2-phenyldiazenyl)phenyl]-","548447-14-9","D",0]
["Poly(oxy-1,2-ethanediyl), α-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-ω-hydroxy-","58228-15-2","D",0]
["1-(2,5-dimethylthiophen-3-yl)-4,4,5,5,6,6,6-heptafluorohexane-1,3-dione","424-58-8","D",0]
["Perfluorotetradecanedioic acid","2822-93-7","D",0]
["Lithium bis(perfluoropropanesulfonyl)imide","189217-59-2","D",0]
["Methyl 4-(undecafluoropentyl)benzoate","88951-01-3","D",0]
["1-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-iodooctyl)-2,8,9-trioxa-5-aza-1-silabicyclo[3.3.3]undecane","135587-15-4","D",0]
["2-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-trimethylethanaminium sulfate (1:1)","153968-00-4","D",0]
["Perfluorohexane-1,6-disulfonyl difluoride","144368-88-7","D",0]
["2,2,3,3,3-Pentafluoropropanimidamide--hydrogen chloride (1/1)","3799-21-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(piperazin-1-yl)butan-1-one","89245-13-6","D",0]
["1,1,2,2-Tetrafluoro-1-nitro-2-nitrosoethane","679-08-3","D",0]
["6-Isocyanato-2,2,4,4-tetrefluoro-1,3-benzodioxene","26030-46-6","D",0]
["1-Bromo-2-(1,1,2,3,3,3-hexafluoropropoxy)benzene","52328-77-5","D",0]
["13:3 Fluorotelomer betaine","1513864-13-5","D",0]
["Triethoxy(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)silane","190579-86-3","D",0]
["Perfluoroethyl 2H-perfluoroethyl ether","50807-74-4","D",0]
["2-(1,1,2,3,3,3-Hexafluoropropoxy)phenol","53998-00-8","D",0]
["Phosphonic acid, [3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy]butyl]-, monoethyl ester","646029-84-7","D",0]
["4-Chloro-2,2,3,3,4,4-hexafluorobutanoyl chloride","111835-69-9","D",0]
["1-[Difluoro(pentafluoroethoxy)methoxy]-1,2,2-trifluoroethene","346662-93-9","D",0]
["2,2,3,3,5,5,6-Heptafluoro-6-(prop-1-en-2-yl)-1,4-dioxane","61448-92-8","D",0]
["2-Bromo-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-1,3-dimethylbenzene","353272-55-6","D",0]
["Perfluoro-4-(2-sulfoethoxy)pentanoic acid","2416366-18-0","D",0]
["4-{2-[(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)amino]ethyl}benzene-1-sulfonamide","316826-59-2","D",0]
["2-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-methylaniline","1770825-71-2","D",0]
["N'-[(2Z)-5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Heptadecafluoro-4-oxododec-2-en-2-yl]benzohydrazide","203200-82-2","D",0]
["(Perfluorohexyl)ethyl (perfluorododecyl)ethyl hydrogen phosphate","1578186-69-2","D",0]
["Methyl 4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoate","51114-06-8","D",0]
["2-(Pentafluoroethyl)-1,3-benzoxazole","64995-45-5","D",0]
["7-(2-Cyclohexyl-4,6-dinitrophenyl)-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl carbonate","42421-29-4","D",0]
["Lithium 3-(perfluorooctyl)propanoate","67304-23-8","D",0]
["(2-Chloroethenyl)bis(2,2,3,3-tetrafluorocyclobutyl)silane","94953-38-5","D",0]
["8:2 Fluorotelomer thioether amido sulfonate","1383439-45-9","D",0]
["Ethyl 2-acetyl-4,4,5,5,5-pentafluoro-3-oxopentanoate","116206-92-9","D",0]
["Butanoic acid, 2,2,3,3,4,4,4-heptafluoro-, ammonium salt (1:1)","10495-86-0","D",0]
["Phosphonic acid, P-[3,5,5,6,8,8,9,11,11,12,14,14,15,17,17,18,18,19,19,19-eicosafluoro-3,6,9,12,15-pentakis(trifluoromethyl)-4,7,10,13,16-pentaoxanonadec-1-yl]-","1198297-83-4","D",0]
["3-(Butane-2-sulfinyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-34-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,27,27,28,28,29,29,30,30,30-Pentacontafluorotriacontane","114221-77-1","D",0]
["2,2-Difluoro-2-(1,1,2,2-tetrafluoro-2-iodoethoxy)acetamide","98296-52-7","D",0]
["Perfluoro-N-(4-methylcyclohexyl)-2-methylpyrrolidine","444658-67-7","D",0]
["Perfluoro-5-oxohexane-1-sulfonic acid","2254560-26-2","D",0]
["1-[6-(Pentafluoroethyl)pyridin-2-yl]ethan-1-one","1580464-65-8","D",0]
["4,4,4-Trifluoro-3-(trifluoromethyl)but-2-enal","104291-39-6","D",0]
["1,1,1,2,4,4,4-Heptafluoro-2-iodobutane","29151-22-2","D",0]
["3-Chloro-1,1,2,2-tetrafluoro-3-oxopropyl sulfurofluoridate","110072-13-4","D",0]
["Tridecafluorohexan-1-ol","7057-81-0","D",0]
["1-[1,3,3,4,4,5,5,5-Octafluoro-2-(trifluoromethyl)pent-1-en-1-yl]pyrrolidine","89810-71-9","D",0]
["Sodium 1,1,2,3,3,3-hexafluoropropane-1-sulfonate","3916-24-3","D",0]
["1,1,1,2,2-Pentafluoro-5-hydroxyhexan-3-one","91485-47-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Hexadecafluorononyl decanoate","18770-65-5","D",0]
["1,2,3,5,6-Pentachloro-1,1,2,3,4,4,5,6,6-nonafluorohexane","56949-85-0","D",0]
["Methyl 2-methoxytetrafluoropropionate","10186-63-7","D",0]
["Sodium 1‐(N‐propylperfluorooctanesulfonamido)‐3,6,9,12‐tetraoxapentadecane‐15‐sulfonate","63367-16-8","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorodecane","1190430-19-3","D",0]
["2,2,4,4,5,5,7,7,8,8,10,10,11,11,13,13,14,14,15,15,16,16,16‐Tricosafluoro‐3,6,9,12‐tetraoxahexadecan‐1‐ol","653573-80-9","D",0]
["Poly(oxy-1,2-ethanediyl), α-(2-carboxy ethyl)-ω-[2-[[(heptadecafluorooctyl) sulfonyl]propylamino]ethoxy]-, potassium salt","167162-24-5","D",0]
["N-[2-[[2-[(2-Aminoethyl)amino]ethyl]amino]ethyl]-N-ethyl-perfluoro-1-octanesulfonamide","13406-92-3","D",0]
["Sodium perfluoro{[1-(1,2-dichloro-1,2,2-trifluoroethoxy)propan-2-yl]oxy}acetate","1383434-26-1","D",0]
["Potassium N-hexyl-N-[(tridecafluorohexyl)sulfonyl]glycinate","76843-36-2","D",0]
["1-(2-Bromo-1,1,2,2-tetrafluoroethoxy)-2-chloro-4-nitrobenzene","103082-65-1","D",0]
["Trimethoxy(3,3,4,4,4-pentafluorobutyl)silane","131651-58-6","D",0]
["1,1,2,2,3,3,4,4,5,5-Decafluoro-1-(nonafluorobutoxy)pentane","173350-69-1","D",0]
["(Perfluoroheptyl)-N,N-dimethyl-2-ethanamine N-oxide","30295-55-7","D",0]
["3-(1,1,2,3,3,3-hexafluoropropyl)adamantane-1-carboxylic acid","86301-98-6","D",0]
["N,N-Dichloro-2,2,3,3,4,4,5,5,5-nonafluoropentanamide","86451-49-2","D",0]
["(2,2,3,3,4,4,4-Heptafluorobutyl)benzene","81664-99-5","D",0]
["1,1,2,2,3,3,4,4-octafluoro-1-iodobutane","754-73-4","D",0]
["1,1,1,2,2-Pentafluoropentan-3-one","378-72-3","D",0]
["2,3,4,5,6-Pentakis(1,1,2,2,2-pentafluoroethyl)pyridine","20017-53-2","D",0]
["1,1,1,2,2,3,3-Heptafluoro-6-iodo-4,4-bis(trifluoromethyl)decane","123629-50-5","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, monoamide with N,N'-bis(2-aminoethyl)-1,2-ethanediamine","64202-77-3","D",0]
["Ethyl perfluorohexyl ether","233678-15-4","D",0]
["12,12,13,13,14,14,15,15,15-Nonafluoropentadecan-1-ol","36096-97-6","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester, polymer with α-(2-methyl-1-oxo-2-propen-1-yl)-ω-hydroxypoly(oxy-1,2-ethanediyl)","867030-76-0","D",0]
["3-(1,1,2,2-Tetrafluoroethyl)aniline","585-41-1","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoroheptan-2-one","86358-19-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,9,9,10,10,11,11,12,12,13,13,14,14,14-Hexacosafluoro-7-iodotetradecane","53638-11-2","D",0]
["N-(1,1,2,3,3,3-Hexafluoropropyl)hypofluorous amide","78343-32-5","D",0]
["Ethenyl perfluorodecanoate","423-88-1","D",0]
["Sodium (2‐{[(2,2,3,3,4,4,5,5,6,6,7,7‐dodecafluoroheptyl)oxy]carbonyl}phenyl)methanesulfonate","29817-88-7","D",0]
["1-(Dichloromethoxy)-1,1,2,3,3,3-hexafluoropropane","56860-82-3","D",0]
["4-Cyclopropyl-2-(pentafluoroethyl)pyrimidine-5-carboxylic acid","914201-14-2","D",0]
["2,2,3,3-Tetrafluoropropan-1-amine","663-69-4","D",0]
["1H,1H-Perfluoro(3,5,5-trimethylhexan-1-ol)","232267-34-4","D",0]
["4-Amino-2-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzonitrile","1463530-23-5","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymer with .alpha.-fluoro-.omega.-[2-[(2-methyl-1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene)","97136-02-2","D",0]
["2-(2-Aminoethylthio)-1,1,1,3,3,3-hexafluoro-2-propanol, hydrochloride","21919-02-8","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluorohept-2-yn-1-ol","81190-31-0","D",0]
["1,1,1-Trichloro-2,2,3,3,4,4,5,5,5-nonafluoropentane","14434-07-2","D",0]
["Disodium 1H,1H,2H,2H-perfluorodecylphosphate","438237-75-3","D",0]
["N-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl)Iodoacetamide","852527-48-1","D",0]
["Zinc bis(nonafluoro-1-butanesulfonate)","502457-69-4","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,6-Tridecafluoro-N-(2-hydroxyethyl)hexane-1-sulfonamide","106443-63-4","D",0]
["Perfluoro-n-(13C4)butanoic acid","1017281-29-6","D",0]
["1-Chloro-3,3,4,4,5,5-hexafluoro-2-iodocyclopent-1-ene","14627-45-3","D",0]
["2-Propenoic acid, 2-methyl-, octadecyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate","425664-41-1","D",0]
["(Tetrafluoroethylene)bis[N-(trifluoromethyl)hydroxylamine]","36525-66-3","D",0]
["N'-(6,7-Dimethoxy-3,3-dimethyl-3,4-dihydroisoquinolin-1-yl)-2,2,3,3,4,4,4-heptafluorobutanehydrazide","304435-61-8","D",0]
["Ethyl perfluoroheptyl ether","233678-19-8","D",0]
["Difluoro(1,1,2,2,3,3,4,4-octafluoro-4-iodobutoxy)acetic acid","88239-65-0","D",0]
["Difluoro[(pentafluoroethyl)sulfanyl]amine","111615-97-5","D",0]
["Methyl 2,4,4,5,7,7,8,10,10,11,13,13,14,16,16,17,17,18,18,18-icosafluoro-2,5,8,11,14-pentakis(trifluoromethyl)-3,6,9,12,15-pentaoxaoctadecan-1-oate","1005033-64-6","D",0]
["Methacrylic acid, 2-(diethylamino)ethyl ester, polymer with 2,2,3,3,4,4,4-heptafluorobutyl methacrylate","34438-55-6","D",0]
["11-Chloroperfluoro-3-oxaundecanesulfonyl fluoride","73606-15-2","D",0]
["4,4'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(2-fluorophenol)","210407-91-3","D",0]
["2-Bromoheptafluoropropane","422-77-5","D",0]
["2-Buten-1-one, 1,1'-p-phenylenebis(4,4,4-trifluoro-3-trifluoromethyl-","100482-67-5","D",0]
["1,1'-Oxybis[2,2,3,3,4,4,5,5-octafluoropentane","774595-25-4","D",0]
["2-Bromo-1,1,1,3,3,3-hexafluoro-2-(trifluoromethyl)propane","754-43-8","D",0]
["4,5-Dichloro-1,1,1,2,2,3,3-heptafluoropentane","577773-57-0","D",0]
["5-(Nonafluorobutyl)-1H-pyrimidine-2,4-dione","58671-28-6","D",0]
["3-([(Perfluoropropyl)sulfonyl]{3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}amino)-1-propanesulfonate","2089108-93-8","D",0]
["Perfluoropropanesulfonamide","152894-03-6","D",0]
["Lithium perfluoropentane sulfonate","1046864-81-6","D",0]
["4-(2,2,3,3,3-Pentafluoropropoxy)phenol","129561-00-8","D",0]
["2,2,3,3-Tetrafluoro-1-(methyl)cyclobutanecarbonyl chloride","895157-70-7","D",0]
["Butanedioic acid, polymers, 2-methylene-, polymer with 2-hydroxyethyl 2-methyl-2-propenoate, 2-methyl-2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate, sodium salt ","1345817-52-8","D",0]
["1,1,2,2,3,3-hexafluoro-1- (trifluoromethoxy)propane (HFE-329 mcc2)","67490-36-2","D",0]
["1,1,2,2,3-pentafluorocyclobutane","2253-02-3","D",0]
["Hexanedioic acid, 2,2,3,3,4,4,5,5-octafluoro-, 1,6-dimethyl ester","3107-98-0","D",0]
["9-Octadecenoic (Z-)-, reaction products with 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-octanol","220237-47-8","D",0]
["3-({3-[(2-Hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoroheptyl)sulfonyl]amino)-1-propanesulfonate","2089108-96-1","D",0]
["2-Ethyl-3,4,4,5,5,6,6,7,7,8,8,8-dodecafluorooct-2-enal","61282-83-5","D",0]
["5,5,5-Trifluoro-4,4-bis(trifluoromethyl)pent-2-ene","62498-13-9","D",0]
["3,5-bis(pentadecafluoroheptyl)-1,2,4-oxadiazole","4314-47-0","D",0]
["5,5,6,6,7,7,7-Heptafluoro-4-methylheptan-3-one","61282-89-1","D",0]
["N-(2-Carboxyethyl)-3-[(2-carboxyethyl)[(perfluorohexyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","1383438-85-4","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, reaction products with 1,6-diisocyanatohexane, epichlorohydrin, (3-isocyanatopropyl)trimethoxysilane and reduced Me esters of reduced polymd. oxidized tetrafluoroethylene","1638956-40-7","D",0]
["Perfluoro-4-hexenesulfonic acid","2089109-50-0","D",0]
["Phenyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","312943-34-3","D",0]
["Bis(pentacosafluorododecyl)phosphinic acid","63225-54-7","D",0]
["4-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecyl)oxy]phenol","193529-93-0","D",0]
["2,3-Dichloro-1,1,3,4,4,4-hexafluorobut-1-ene","1823355-24-3","D",0]
["1,4-Butanedisulfonyl difluoride, 1,1,2,2,3,3,4,4-octafluoro-","84246-31-1","D",0]
["4,4'-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]bisbenzoyl chloride","1102-92-7","D",0]
["1H-Perfluoro-1-heptene","75180-14-2","D",0]
["N,N,N',N',1-Pentamethyl-1-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silanediamine","879881-65-9","D",0]
["25,26,26,26,27,27,27-Heptafluoro-3-hydroxycholest-8(14)-en-15-one","153463-20-8","D",0]
["3-Azido-2,3,3-trifluoro-2-(heptafluoropropoxy)propanoic acid","95906-13-1","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1,6-bis(4-methylphenyl)hexane-1,6-dione","25871-03-8","D",0]
["4-Perfluoro-tert-butyl-phenyliodoacetamide","148562-02-1","D",0]
["Bis(3,3,4,4,5,5,6,6,6-nonafluorohexyl) but-2-enedioate","161975-99-1","D",0]
["2-(4-Bromophenoxy)-perfluoroethane-1-sulfonyl fluoride","252975-60-3","D",0]
["5-(Heptafluoropropyl)-N,1-dimethyl-1H-1,2,4-triazol-3-amine","714975-28-7","D",0]
["Perfluoro-3-ethoxypropanoic acid","377-76-4","D",0]
["Pentafluoro(1,2,2,2-tetrafluoroethoxy)-ethane","360796-50-5","D",0]
["4,5,5,6,6,7,7,8,8,9,9,9-Dodecafluoro-1,3-nonadiene","74338-55-9","D",0]
["4,4,4-Trifluoro-1-(4-methoxyphenyl)-2-methyl-3-(trifluoromethyl)butane-1,3-diol","34848-35-6","D",0]
["Benzyl pentadecafluorooctanoate","208663-34-7","D",0]
["1,1,2,2,3,3,4,5,5,6,6,7,7,8-Tetradecafluoro-4,8-dimethylcyclooctane","948014-28-6","D",0]
["2-Butenenitrile, 4,4,4-trifluoro-3-(trifluoromethyl)-","61859-90-3","D",0]
["Poly(difluoromethylene), .alpha.,.omega.-bis(methylthio)-","65530-67-8","D",0]
["2-Propanone, hexafluoro-, 2-(2,4-dinitrophenyl)hydrazone","346-52-1","D",0]
["1-[2-(1,1,2,2-Tetrafluoroethoxy)phenyl]ethan-1-one","1417499-00-3","D",0]
["1-Bromo-2,3,5,6-tetrafluoro-4-{1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propyl}benzene","60799-27-1","D",0]
["11-(Perfluoro-n-octyl)undec-10-en-1-ol","15364-19-9","D",0]
["Perfluoroperhydrobenzyl tetralin","116265-66-8","D",0]
["2,2,3,4,4-Pentafluoro-4-(1,1,2,2,3,3,3-heptafluoropropoxy)butanoic acid","919005-26-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorononacosane","677324-32-2","D",0]
["4-[(2,2,3,3,4,4,4-Heptafluorobutoxy)methyl]-1,3-dioxolan-2-one","181044-06-4","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(undecafluoropentyl)sulfonyl]amino}-1-propanesulfonic acid","2089109-73-7","D",0]
["Perfluorononanedioic acid","23453-64-7","D",0]
["4-(Pentadecafluoroheptyl)cyclohexane-1-carboxylic acid","88951-28-4","D",0]
["Bis[tris(3-(perfluorooctyl)phenyl)phosphine]palladium(II) dichloride","326475-45-0","D",0]
["Benzamide, 3-[(1,1,2,2,3,3,3-heptafluoropropyl)sulfonyl]-4-[(4-methoxyphenyl)amino]-N-[4-(2-phenyldiazenyl)phenyl]-","382610-40-4","D",0]
["N,N-Diethylethanaminium heptadecafluorononanoate","327176-80-7","D",0]
["1,1,1,3,4,4,5,5,5-Nonafluoropent-2-ene","73401-37-3","D",0]
["Bis[perfluoro-2-(1-methylethoxy)ethyl] phosphinic acid erbium (3+) salt","500776-83-0","D",0]
["3-(Perfluorohexyl)-2-hydroxypropyl acrylate","146955-22-8","D",0]
["N-(2-{[5-(2-Ethoxy-2-oxoethyl)-1,3-thiazol-2-yl]amino}-1,1,1,3,3,3-hexafluoropropan-2-yl)propanimidic acid","4931-84-4","D",0]
["4,12-Bis(1,1-dimethylethyl)-2,10-bis(1,1,1,2,2,3,3-heptafluoropropyl)-1,5,9,13-tetraazacyclohexadeca-1,4,9,12-tetraene","925457-51-8","D",0]
["1-Nitro-4-(nonafluorobutyl)benzene","196932-95-3","D",0]
["(2Z)-4,4,5,5,6,6,6-Heptafluoro-2-iodohex-2-en-1-ol","92835-92-2","D",0]
["N,N-Dimethyl-3-[1-phenyl-3,3-bis(trifluoromethyl)-1,3-dihydro-2-benzofuran-1-yl]propan-1-amine--hydrogen chloride (1/1)","29138-42-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7-Tridecafluoroheptane","2708-11-4","D",0]
["1-(Difluoromethoxy)-1,1-difluoroethane","69948-29-4","D",0]
["Ethyl ethyl(heptafluoropropyl)phosphinate","77529-55-6","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[[(perfluoropentyl)sulfonyl]amino]-1-propanaminium","142519-28-6","D",0]
["4-Cyanophenyl 4-(heptafluoropropyl)benzoate","88951-05-7","D",0]
["Bis(1H,1H-perfluoropropyl)amine","883498-76-8","D",0]
["2,3,3,3-Tetrafluoro-2-phenoxypropanoyl fluoride","78900-65-9","D",0]
["Chloroheptafluorocyclobutane","377-41-3","D",0]
["Perfluorooctanesulfonamide sodium salt (1:1)","76752-78-8","D",0]
["HFE–365mcf2","22052-81-9","D",0]
["7H-Perfluoroheptanamide","6395-47-7","D",0]
["Sodium 2-[(perfluorooctyl)sulfonyl(propyl)amino]ethanesulfonate","63367-15-7","D",0]
["P,P-Bis(perfluoro-7-methyloctyl) phosphinothioic acid ytterbium(3+) salt (3:1)","500776-90-9","D",0]
["(Pentafluoroethyl)(phenyl)iodanium hydrogen sulfate","81807-32-1","D",0]
["2,3-Bis(heptafluoropropyl)pyridine","104986-67-6","D",0]
["[(Perfluorotridecanoyl)amino]-3-betaine","167997-08-2","D",0]
["5:2/7:2 di Polyfluorinated phosphate ester","1361054-89-8","D",0]
["4-(Ethenyloxy)-1,1,1,2-tetrafluoro-2-(trifluoromethyl)butane","90999-86-3","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with butyldimethylsilyl (ethenylphenyl)methyl methylphosphonate and 2,2,3,3,4,4-hexafluorobutyl 2-propenoate, graft","149235-83-6","D",0]
["Tetradecafluorooctahydrobenzofuran","55751-36-5","D",0]
["3,3,4,4,5,5,6,6,7,7,7-Undecafluoroheptan-1-ol","185689-57-0","D",0]
["Magnesium, chloro-2-propen-1-yl-, reaction products with ethenyldimethylsilane, Me esters of fluorinated reduced polymd. oxidized tetrafluoroethylene and trimethoxysilane","1644456-27-8","D",0]
["2,2,3,3,3-Pentafluoro-N-(2-((propylsulfonyl)amino)-5-(trifluoromethyl)-3-pyridinyl)propanamide","141283-66-1","D",0]
["1-((Perfluoro-6-(1-methylethoxy)hexyl)ethyl)pyridinium sulfate (2:1)","121924-89-8","D",0]
["Acetic acid, 2,2-difluoro-2-[(1,1,2,3,4,4,4-heptafluoro-2-buten-1-yl)oxy]-","2089109-62-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-Tricosafluorotricosane","677324-21-9","D",0]
["2,2,3,3-Tetrafluorooctahydro-5,8-methano-1,4-benzodithiine","102489-64-5","D",0]
["Hexakis (1H,1H,6H-Decafluorohexyloxy) phosphazine","186406-48-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptanehydrazide","33843-69-5","D",0]
["Tetrabutylammonium perfluorooctanesulfonate","111873-33-7","D",0]
["2-Chloro(perfluoro-2-methylpentane)","67437-97-2","D",0]
["4-(Pentadecafluoroheptyl)phenol","57578-99-1","D",0]
["3-(1,1-Difluoroethoxy)-1,1,1,2,2-pentafluoropropane","1365807-90-4","D",0]
["Octadecyl perfluorooctanoate","131883-38-0","D",0]
["1,1,1,2,2,3,3,10,10,11,11,12,12,12-Tetradecafluoro-5,8-diiodododecane","2357-30-4","D",0]
["Butane mixture with pentafluoroethane and 1,1,1,2-tetrafluoroethane","224174-48-5","D",0]
["4,4,4-trifluoro-1-(3-methylphenyl)-3-(trifluoromethyl)but-2-en-1-one","35443-93-7","D",0]
["(2E)-1,1,1,2,3,4,4,5,5,6,6,7,7,7-Tetradecafluorohept-2-ene","24010-46-6","D",0]
["(Thiophen-3-yl)methyl heptafluorobutanoate","879479-80-8","D",0]
["2,2,3,3-Tetrafluorooctahydro-2H-cyclohepta[b]thiophene","101564-09-4","D",0]
["(Nonafluorobutyl)benzene","2398-75-6","D",0]
["2,3,6-Trifluoro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-95-8","D",0]
["Methyl N-(2,2,3,3,4,4,4-heptafluorobutanoyl)glycinate","81084-29-9","D",0]
["Octakis(trifluoromethyl)-1,4,6,9-tetraoxa-5lambda4-thiaspiro[4.4]nonane","18810-55-4","D",0]
["4-Fluoro-2-methyl-6-pentafluoroethyl-5-trifluoromethylpyrimidine","170865-78-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctadec-7-ene","131851-05-3","D",0]
["1H-1,2,4-Triazol-5-amine, 1-[2,6-dichloro-4-(trifluoromethyl)phenyl]-N-ethyl-3-(1,1,2,2,2-pentafluoroethyl)-","128887-17-2","D",0]
["1,1,2,2,3,3-Hexafluoro-1-methoxy-3-[(trifluoroethenyl)oxy]propane","93402-66-5","D",0]
["6,6,7,7,8,8,9,9-Octafluorononane-3,5-dione","62679-63-4","D",0]
["Phosphoric acid--2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptan-1-ol (1/3)","662-75-9","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluorodecan-1-ol","39239-79-7","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl trifluoroacetate","42031-15-2","D",0]
["Trimethyl(nonafluorobutyl)silane","204316-01-8","D",0]
["N-[(Perfluoroethyl)sulfonyl]glycine","1003193-97-2","D",0]
["1-Butyl-3-methyl-1H-imidazol-3-ium 1,1,2,2-tetrafluoroethane-1-sulfonate","880084-62-8","D",0]
["3,3-Dimethylbutan-2-yl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","107368-63-8","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoro-6-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]hexanamide","29952-92-9","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(1-phenylethyl)butanamide","51241-61-3","D",0]
["Heptafluoropentane","30423-63-3","D",0]
["1-Chloro-4-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-47-7","D",0]
["2,3,3-Trifluoro-3-(heptafluoropropoxy)propanoic acid","919005-19-9","D",0]
["3-(Chloromethyl)-3-[(2,2,3,3-tetrafluoropropoxy)methyl]oxetane","67416-57-3","D",0]
["1,1-Dichloro-1,2,2,3,3,4,4,4-octafluorobutane","355-23-7","D",0]
["2-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]benzoyl chloride","62751-26-2","D",0]
["N-(Perfluorobutanesulfonyl)-N-(3-dimethylaminopropyl)-3-aminopropanoic acid","172616-04-5","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, polymer with ethene, graft","136846-15-6","D",0]
["4,4,5,5,5-Pentafluoropentane-1,3-diol","121591-51-3","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(11-{2-[2-(2-methoxyethoxy)ethoxy]ethyl}-2,5,8-trioxa-11-azatetradecan-14-yl)octane-1-sulfonamide","117413-27-1","D",0]
["4:4 Fluorotelomer sulfonate lithium salt","1604816-75-2","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-7-iodoheptane","376-32-9","D",0]
["N-[3-(Diethylamino)propyl]-perfluorononanamide","61481-09-2","D",0]
["2-{[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]methyl}oxirane","90441-53-5","D",0]
["3,6-Bis(tridecafluorohexyl)benzene-1,2,4,5-tetracarboxylic acid","138522-77-7","D",0]
["Ethane, 1-chloro-1,1,2,2-tetrafluoro-2-methoxy-","404582-64-5","D",0]
["12,12,13,13,14,14,15,15,15-Nonafluoro-10-iodopentadecanoic acid","155172-51-3","D",0]
["4,4,4-Trifluoro-3-(trifluoromethyl)-3-[(trimethylsilyl)oxy]but-1-en-1-one","83740-52-7","D",0]
["2-chloro-1,1,1,3,4,4,4-heptafluorobutane","507453-83-0","D",0]
["4,4,5,5,6,6,6-Heptafluoro-2-hexenoic acid","356-03-6","D",0]
["5,6,6,6-Tetrafluoro-4-methylhex-4-en-3-one","64435-53-6","D",0]
["Acetic acid--9,9,10,10,11,11,12,12,12-nonafluorododec-7-en-1-ol (1/1)","130483-36-2","D",0]
["[3,3,4,4,5,6,6,6-octafluoro-5-(trifluoromethyl)hexyl] Prop-2-enoate","86217-01-8","D",0]
["4,4,5,5,6,6,7,7,8,8,8-Undecafluorooctanal","195047-10-0","D",0]
["5-Pentyl-2-[4-(tridecafluorohexyl)phenyl]pyridine","139030-54-9","D",0]
["Alcohols, C3-11, .beta.-.omega.-perfluoro-.omega.-hydro","70983-62-9","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide and methacrylic anhydride","162492-18-4","D",0]
["3,5-Difluoro-2,6-dimethoxy-4-[(pentafluoroethyl)sulfanyl]pyridine","184484-18-2","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)-1-(piperidin-1-yl)propan-1-one","176702-72-0","D",0]
["HFE-347mmy1","22052-84-2","D",0]
["Perfluoro-2-{2,3-bis[2-(fluorosulfonyl)ethoxy]propoxy}propanoyl fluoride","921204-32-2","D",0]
["2-(3,3,3-Trifluoro-2-(trifluoromethyl)-1-propenyl)benzothiazole","100333-44-6","D",0]
["5-Bromo-1,1,2,2,3,3,4,4-octafluoropentane","75885-51-7","D",0]
["[5-Methyl-6-(2,2,3,3-tetrafluoropropoxy)-3-pyridinyl]methanol","1373865-23-6","D",0]
["9-[(1,1,2,2-Tetrafluoroethoxy)methyl]nonadecane","165318-16-1","D",0]
["Phosphorous acid--2,2,3,3,3-pentafluoropropan-1-ol (1/3)","81860-11-9","D",0]
["4-Chloro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)-2-nitrobenzamide","862130-91-4","D",0]
["1,1,4,4-Tetrachloro-1,2,2,3,3,4-hexafluorobutane","72765-11-8","D",0]
["3,4,4,5,5-Pentafluoro-2-methoxycyclopent-2-en-1-one","62344-62-1","D",0]
["Perfluoro-4-methylpent-2-enoyl chloride","207671-78-1","D",0]
["Heptadecafluorooctyl phosphinic acid","40143-80-4","D",0]
["1-Propanol, 2,2,3,3,3-pentafluoro-, 1-(4-methylbenzenesulfonate)","565-42-4","D",0]
["N-Butyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononanamide","73602-42-3","D",0]
["2-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)hydrazinecarboxamide","1747-05-3","D",0]
["Triethoxy(1,1,1,3,3,3-hexafluoropropan-2-ylidene)-lambda~5~-phosphane","1540-04-1","D",0]
["1,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-iodohept-1-ene","102682-83-7","D",0]
["2-Nitro-4-(pentafluoroethyl)benzaldehyde","926927-43-7","D",0]
["1-(3-Chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-ol","100482-51-7","D",0]
["11-(Perfluorobutyl)undecanoic acid","1652-66-0","D",0]
["7-[(Hex-1-en-3-yl)oxy]-4,6-dinitro-2-(pentafluoroethyl)-1H-benzimidazole","60285-68-9","D",0]
["N-[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl]phosphorimidic trichloride","18854-78-9","D",0]
["5-Chloro-1,1,2,2,3,3,4,6,7-nonafluoro-2,3-dihydro-1H-indene","88953-08-6","D",0]
["1,1-Difluoroethene with 1,1,2,3,3,3-hexafluoro-1-propene (1:1)","1184966-74-2","D",0]
["1-Iodo-2-(pentafluoroethyl)cyclohexane","711-17-1","D",0]
["2-[1,2,2,2-Tetrafluoro-1-(heptafluoropropoxy)ethyl]-1-benzothiophene","141734-25-0","D",0]
["2-Methyl-1-[4-(pentafluoroethoxy)phenyl]propan-1-one","56425-87-7","D",0]
["5-Heptafluoropropyluracil","60007-37-6","D",0]
["[(1E)-1,2,3,3,3-Pentafluoroprop-1-en-1-yl]boronic acid","1233224-66-2","D",0]
["[2,2,2-Trifluoro-1,1-bis(trifluoromethyl)ethyl]benzene","41125-49-9","D",0]
["N-[3-(Dimethylamino)propyl]-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-N-hydroxyoctane-1-sulfonamide","958822-85-0","D",0]
["Methyl 4,4,5,5,6,6,6-heptafluoro-2-methylhexanoate","88021-93-6","D",0]
["4-[(2,2,3,3,3-Pentafluoropropyl)sulfanyl]phenol","90314-96-8","D",0]
["(17beta)-Estra-1,3,5(10)-triene-3,17-diol, 7-[9-[(4,4,5,5,5-pentafluoropentyl)sulfinyl]nonyl]-","471243-86-4","D",0]
["3H,3H-Perfluoropropyl triflate","6401-00-9","D",0]
["Heptafluoro(nitroso)cyclobutane","2261-41-8","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluorohex-1-yn-1-yl)benzene","66249-23-8","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluoroundecanamide","215956-15-3","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecyl)propanedioic acid","36390-05-3","D",0]
["8,8,9,9,10,10,11,11,12,12,13,13,13-Tridecafluorotridecanoic acid","34598-27-1","D",0]
["5-(Benzyloxy)-N,N-diethyl-2,3,3,4,4-pentafluoropentanamide","60896-00-6","D",0]
["1,1,1,2,3,3-Hexafluoro-2,3-bis(pentafluoroethoxy)propane","95842-03-8","D",0]
["4-[1,1,2-Trifluoro-2-(heptafluoropropoxy)ethoxy]butan-1-ol","640731-95-9","D",0]
["2,2-Bis(4-trifluorovinyloxyphenyl)-1,1,1,3,3,3-hexafluoropropane","134174-11-1","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-N-phenylpentanamide","122590-97-0","D",0]
["2-(1,2,2,2-Tetrafluoroethyl)-1H-benzimidazole","41185-74-4","D",0]
["N-[4'-(2,2,3,3,4,4,4-Heptafluorobutanamido)[1,1'-biphenyl]-4-yl]ethanimidic acid","75042-08-9","D",0]
["2-Indoleethanol, alpha,alpha-bis(trifluoromethyl)-","101831-93-0","D",0]
["4,4,4-Trifluoro-3-hydroxy-1-phenyl-3-(trifluoromethyl)butan-1-one","731-00-0","D",0]
["2-Hydroxy-2-phenyl-5,5-bis(trifluoromethyl)oxolan-3-one","101833-13-0","D",0]
["3-[Dimethyl(2-{[(perfluorohexyl) sulfonyl]amino}ethyl)ammonio]propanoate","34695-30-2","D",0]
["1-(2,4-Dihydroxyphenyl)-2,2,3,3,4,4,4-heptafluorobutan-1-one","65240-03-1","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-5-hexadecene 1-(perfluorobutyl)-1-dodecene","131851-20-2","D",0]
["(1E)-3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-iodooct-1-ene","329698-26-2","D",0]
["2-Chloro-2,3,3,3-tetrafluoropropanoic acid","6189-02-2","D",0]
["1-(2-chloroethoxy)-1,1,2,3,3,3-hexafluoropropane","2926-99-0","D",0]
["Tris{4-[3,3,4,4,5,5,5-heptafluoro-2,2-bis(trifluoromethyl)pentyl]phenyl}phosphane","322647-82-5","D",0]
["1-Chloro-1,1,3,3,3-pentafluoro-2-(trifluoromethyl)propan-2-ol","7594-48-1","D",0]
["2-Pentanone, 1-bromo-4-hydroxy-5,5,5-trifluoro-4-(trifluoromethyl)-","101931-62-8","D",0]
["4-Iodophenyl nonafluorobutane-1-sulfonate","199465-44-6","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[[(perfluoropentyl)sulfonyl]amino]-1-propanaminium","2089108-67-6","D",0]
["4-Chloro-2-fluoro-N-(2-fluoro-3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)-N-methylbenzamide","862134-30-3","D",0]
["Tris(3,3,4,4,5,5,6,6,6-nonafluorohexyl)(phenyl)stannane","240497-36-3","D",0]
["Cyclohexyl[4-(1,1,2,2-tetrafluoroethoxy)phenyl]methanone","56426-09-6","D",0]
["3-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)propan-1-ol","762241-70-3","D",0]
["4-Methyl-2,2,6,6-tetrakis(trifluoromethyl)-2H,6H-8lambda3-[1,2]iodoxolo[4,5,1-hi][1,2]benziodoxole","80360-45-8","D",0]
["Perfluoro-2-(nonafluorobutoxy)ethane-1-sulfonyl fluoride","67990-79-8","D",0]
["Heptanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoro-, methyl ester","14312-89-1","D",0]
["Poly[oxy(1,1,2,2,3,3-hexafluoro-1,3-propanediyl)], .alpha.-(1,1,2,2,3,3,3-heptafluoropropyl)-.omega.-(1,1,2,2-tetrafluoro-3-hydroxypropoxy)-","146349-51-1","D",0]
["1-Ethyl-3-methyl-1H-imidazol-3-ium 1,1,2,2-tetrafluoroethane-1-sulfonate","880084-63-9","D",0]
["6,6,7,7,7-Pentafluoroheptanoyl chloride","177352-63-5","D",0]
["1,1,1-Trifluoropropan-2-yl nonafluorobutane-1-sulfonate","118334-94-4","D",0]
["3,4,4,4-Tetrafluoro-3-(trifluoromethoxy)-1-butene","226575-14-0","D",0]
["2-(Heptafluoropropyl)-5-methoxy-1H-indole","923569-79-3","D",0]
["5-(Perfluorooctyl)-1,3-bis(bis(trifluoromethyl)hydroxymethyl)benzene","89780-02-9","D",0]
["2,2,3,3-tetrafluoropropyl 2-(2,4-dichlorophenoxy)acetate","325699-68-1","D",0]
["Bis(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl) (4-methyl-1,3-phenylene)bis(hydrogen carbonimidate)","15953-40-9","D",0]
["2,3,3,4,4,5,5,6,6,7,7-Undecafluorohept-1-ene","94228-81-6","D",0]
["8,8,9,9,9-Pentafluoro-7-(pentafluoroethyl)non-6-en-1-amine","917867-93-7","D",0]
["Begacestat","769169-27-9","D",0]
["3-Chloro-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridin-2(1H)-one","1771743-43-1","D",0]
["(1,2,3,3,4,4,4-Heptafluorobut-1-en-1-yl)benzene","783372-47-4","D",0]
["2,3-Dibromo-6-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-3,5,5-trimethylcyclohexan-1-one","101564-40-3","D",0]
["1,1,3,5,7,9,10-Heptachloro-1,2,2,3,4,4,5,6,6,7,8,8,9,10,10-pentadecafluorodecane","307-41-5","D",0]
["4-Hexen-3-one, 1,1,2,2-tetrafluoro-5-mercapto-","64249-76-9","D",0]
["N-[2-(Phosphonooxy)ethyl]-N-propylperfluoro-1-hexanesulfonamide","179954-93-9","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propylamino]ethyl ester, polymer with .alpha.-(2-methyl-1-oxo-2-propen-1-yl)-.omega.-butoxypoly[oxy(methyl-1,2-ethanediyl)]","73275-59-9","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoropiperidine","559-31-9","D",0]
["1-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutyl)-3-nitrobenzene","93620-85-0","D",0]
["2-[(4,4,5,5,5-Pentafluoropentyl)oxy]ethan-1-ol","652983-59-0","D",0]
["HFE-338mmz1","26103-08-2","D",0]
["(5E)-1,1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10,11,11,12,12,12-Docosafluorododec-5-ene","51249-66-2","D",0]
["Ethyl heptafluorobutyrylacetate","336-62-9","D",0]
["Pentafluoropropylamidine","422-62-8","D",0]
["4-(Heptadecafluorooctyl)-N-methylbenzamide","89932-69-4","D",0]
["1,1,1,2,4,4,4-Heptafluorobut-2-ene","760-42-9","D",0]
["1-Propanol, 2,3,3,3-tetrafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)-, 1-(dihydrogenphosphate)","1173199-13-7","D",0]
["Sodium 3-(methyl{3-[(tridecafluorohexyl)amino]propyl}amino)propane-1-sulfonate","94492-37-2","D",0]
["3-(Ethanesulfonyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355555-11-1","D",0]
["1-[Bis(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)methanesulfonyl]-1,1,2,2,3,3,4,4,4-nonafluorobutane","182505-69-7","D",0]
["1,1,1,6,6,6-Hexafluoro-2,5-bis(trifluoromethyl)hexa-2,3,4-triene","61540-07-6","D",0]
["3-[[[4-[(Heptadecafluorononyl)oxy]phenyl]sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","59493-69-5","D",0]
["1H,1H-Nonafluoropentyl p-toluenesulfonate","883499-79-4","D",0]
["5-(Difluoromethoxy)-1,1,1,2,2,3,3,4,4-nonafluoropentane","1661005-79-3","D",0]
["2-(Pentafluoroethyl)-3H-imidazo[4,5-c]pyridine","1211593-90-6","D",0]
["4-(Heptadecafluorooctyl)-1H-pyrazole","92914-86-8","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)oxy]propane-1,2-diol","126814-93-5","D",0]
["Oxirane, 2-[[(.gamma.-.omega.-perfluoro-C4-10-alkyl)thio]methyl] derivs.","119438-11-8","D",0]
["1-Amino-5,5,6,6,7,7,8,8,9,9,10,10,10-tridecafluorodecan-2-ol","62571-57-7","D",0]
["Potassium 11-chloroeicosafluoro-3-oxaundecane-1-sulfonate","83329-89-9","D",0]
["5,6-Dichloro-2-(heptafluoropropyl)-1H-imidazo[4,5-b]pyrazine","53338-42-4","D",0]
["2,2,3,3,4,4-Hexafluoropentane-1,5-diamine--hydrogen chloride (1/1)","58191-50-7","D",0]
["5-Octen-4-one-5,8,8,8-d4, 1,1,1,2,2,3,3-heptafluoro-6-hydroxy-7,7-di(methyl-d3)-, compd. with (5Z)-1,1,1,2,2,3,3-heptafluoro-6-hydroxy-7,7-di(methyl-d3)-5-octen-4-one-5,8,8,8-d4, europium salt (2:1:1)","56689-47-5","D",0]
["1-(4-bromophenyl)-4,4,4-trifluoro-3-hydroxy-2-methyl-3-(trifluoromethyl)butan-1-one","34844-27-4","D",0]
["1,2,3,3,4,4,5,5,6,7,7-Undecafluorocyclohept-1-ene","85625-25-8","D",0]
["4-[[2,3,4,4,4-Pentafluoro-1,3-bis(trifluoromethyl)-1-buten-1-yl]oxy]benzenesulfonyl chloride","1582261-50-4","D",0]
["1,1,2,2,3,3,3-Heptafluoro-N,N-bis(trifluoromethyl)propan-1-amine","103217-78-3","D",0]
["2,3,3,4,5,6,7-Heptafluoro-2-(trifluoromethyl)-2,3-dihydro-1-benzofuran","649727-95-7","D",0]
["Benzenamine, 4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-","83766-52-3","D",0]
["N-2-Pyridinylperfluorobutanamide","283172-09-8","D",0]
["3-(Heptafluoropropyl)-1H-pyrazole","158148-63-1","D",0]
["Diethylmethoxy(3,3,4,4,5,5,5-heptafluoropentyl)silane","608299-33-8","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-pentylbutanamide","75668-27-8","D",0]
["Heptadecafluorononanoyl Chloride; Perfluorononanoyl Chloride","52447-23-1","D",0]
["Ethyl 2,2-bis(trifluoromethyl)-3-[3,3,3-trifluoro-2-(trifluoromethyl)prop-1-en-1-yl]cyclopropane-1-carboxylate","121618-17-5","D",0]
["6-(Heptafluoropropyl)-2-sulfanylidene-2,3-dihydropyrimidin-4(1H)-one","88191-88-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctan-2-ol","64773-44-0","D",0]
["Chloro(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)propyl(3,3,3-trifluoropropyl)silane","608296-60-2","D",0]
["3,3,4,5,5,5-Hexafluoro-1-pentene","2375-68-0","D",0]
["Methyltris(2,2,3,3,3-pentafluoropropoxy)silane","169155-40-2","D",0]
["2,2,3,3-tetrafluoropropanoyl chloride","663-73-0","D",0]
["3,3,4,4,5,5,6,6-Octafluoro-2-oxohexanal","116142-52-0","D",0]
["4,4,5,5-Tetrafluoro-2,2-bis(trifluoromethyl)-1,3-dioxolane","64499-64-5","D",0]
["1,1,2,2-Tetrafluoro-2-(1,1,2,2-tetrafluoroethoxy)ethane-1-sulfonyl azide","144951-88-2","D",0]
["2,2,3,3-Tetrafluoro-1-(trifluoromethyl)cyclopropane-1-carboxylic acid","917951-64-5","D",0]
["1,1,1,2,2,3,3-Heptafluorododecane","69125-78-6","D",0]
["(1E)-1,3,4,4,4-Pentafluoro-3-(trifluoromethyl)but-1-ene","14149-41-8","D",0]
["(1,2,2,2-Tetrafluoroethyl)oxidanyl","140872-97-5","D",0]
["O,O'-Dipropyl ethylphosphonous acid compd. with perfluoro-3-iodopropane (1:1)","80391-99-7","D",0]
["1,1,1,2,3,4,4,4-octafluorobutane","75995-72-1","D",0]
["1,4,5,5,6,6-Hexafluoro-2,3-dimethoxycyclohexa-1,3-diene","33103-52-5","D",0]
["2-(Perfluoro-(1-fluorosulfonyl-2-ethoxy)ethyl)acetic acid","363158-84-3","D",0]
["Phenyl (2,2-dichloro-1,1,2-trifluoroethoxy)(difluoro)acetate","83865-21-8","D",0]
["2-Fluoro-4,4,5,5-tetrakis(trifluoromethyl)-1,3,2-dioxaphospholane","62553-89-3","D",0]
["5-(Heptafluoropropyl)-1,3,4-thiadiazol-2-amine","299937-37-4","D",0]
["Butan-2-yl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","340034-57-3","D",0]
["1,1,1,4,4,5,5,6,6,7,7,7-Dodecafluoro-2-heptene","887111-62-8","D",0]
["[2,4,4,4-Tetrafluoro-3-(trifluoromethyl)but-1-en-1-yl]benzene","52211-79-7","D",0]
["4,4,4-Trifluoro-3-(trifluoromethyl)-1-butanamine","954238-58-5","D",0]
["5,5,6,6,7,7,7-heptafluoroheptane-2,4-dione","356-30-9","D",0]
["1-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl)-3,1-Benzoxazine-2,4(1H)-Dione","544418-04-4","D",0]
["2,4-Bis(heptafluoropropyl)-6-phenyl-1,3,5-triazine","74582-85-7","D",0]
["Perfluoro-7,8-dimethyl-2,6,9,13-tetraoxatetradecane","70539-38-7","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-[(1,1,2-trifluoro-2-propenyl)oxy]propoxy]-","174082-84-9","D",0]
["N-Allylperfluorononanamide","221466-77-9","D",0]
["1-Methyl-4-(undecafluoropentyl)benzene","88950-98-5","D",0]
["1-diphenylphosphoryl-2-(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)benzene","7225-11-8","D",0]
["Ethyl (pentafluoroethoxy)acetate","22410-43-1","D",0]
["1-(Butylselanyl)-2,2,3,3,4,4,4-heptafluorobutan-1-ol","1092379-04-8","D",0]
["4,4,5,5,5-Pentafluoro-1-phenylpent-1-en-3-one","89176-05-6","D",0]
["Methyl perfluoroheptyl ether","222719-64-4","D",0]
["Propane, 1,1,1,2,2-pentafluoro-3-(trifluorovinyloxy)-, copolymer with perfluoroethene (having 1,000 or more of number average molecular weight also insoluble in water, fat-soluble solvent, universally applicable solvent, acid and alkali)","126323-49-7","D",0]
["1-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzene","2396-23-8","D",0]
["Peroxide, bis[(undecafluorocyclohexyl)carbonyl]","203255-90-7","D",0]
["N-2-Pyridinylperfluoro-2-(2-propoxypropoxy)propanamide","31339-60-3","D",0]
["1-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)piperidine","339-20-8","D",0]
["2-[13-(Perfluorooctyl)-12-(1-methylethyl)-13,13-dioxido-3,6,9-trioxa-13-thia-12-azatrideca-1-yloxy]-N,N,N-trimethylethanaminium chloride (1:1)","121912-25-2","D",0]
["(1-butoxy-1-oxobutan-2-yl) 2,2,3,3,4,4,4-heptafluorobutanoate","55649-48-4","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, 1-(dihydrogen phosphate), ammonium salt (1:2)","1000852-37-8","D",0]
["1,2,3,4,5,5,6,6-Octafluoro-1,3-cyclohexadiene","377-70-8","D",0]
["N-[(Butylamino)carbonyl]-perfluoro-1-octanesulfonamide","100221-84-9","D",0]
["6-(Perfluorohexyl)hexanol","161981-35-7","D",0]
["Phenyl[({[(5,5,6,6,7,7,8,8,9,9,10,10,10-tridecafluoro-2-methyldecan-2-yl)oxy]carbonyl}oxy)imino]acetonitrile","892154-76-6","D",0]
["Poly(difluoromethylene), .alpha.-chloro-.omega.-hydro-","110972-60-6","D",0]
["3-Acetyl-5,5,6,6,7,7,8,8,8-nonafluorooctane-2,4-dione","120110-91-0","D",0]
["Oxirane, 2-[[(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl)oxy]methyl]-","799-34-8","D",0]
["1-acetyl-4-bromo-3(5)-(heptafluoropropyl)-5(3)-methylpyrazole","808764-22-9","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(3-methoxyphenyl)butanamide","550302-16-4","D",0]
["N'-[(2Z)-5,5,6,6,7,7,7-Heptafluoro-4-oxohept-2-en-2-yl]benzohydrazide","203200-76-4","D",0]
["4,4,5,5-Tetrafluoro-3-hydroxy-1-phenylpentan-1-one","105602-59-3","D",0]
["4-Methyl-5-phenyl-2,2-bis(trifluoromethyl)-1,3-oxazolidine","30184-88-4","D",0]
["1-(2-chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-one","35443-97-1","D",0]
["1-{2-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)amino]ethyl}pyridin-1-ium chloride","133804-78-1","D",0]
["1-Methoxy-2-(nonafluorobutyl)benzene","153910-97-5","D",0]
["1,8-Divinylperfluorooctane","35192-44-0","D",0]
["Propanoyl fluoride, 3-chloro-2,3,3-trifluoro-2-[1,1,2,2-tetrafluoro-2-(fluorosulfonyl)ethoxy]-","81126-57-0","D",0]
["6,6,7,7,8,8,9,9,10,10,10-Undecafluorodec-1-en-3-one","144055-27-6","D",0]
["(2S)-1-(2,2,3,3,3-Pentafluoropropoxy)propan-2-ol","877762-92-0","D",0]
["1,1,2,2,3,4,5,6,7-Nonafluoro-2,3-dihydro-1H-indene","79676-83-8","D",0]
["Methyl 3H-perfluoroisopropyl ether","568550-25-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,21,21,22,22,23,23,24,24,25,25,26,26,27,27,28,28,29,29,30,30,31,31,32,32,32-Pentacontafluorodotriacontane","100550-09-2","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl 2-chloroprop-2-enoate","74359-14-1","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentyl 2,4,6-trimethylbenzoate","18770-69-9","D",0]
["3,3,4,5,5,5-Hexafluoropentan-2-yl 2-methylprop-2-enoate","64375-29-7","D",0]
["1-(Pentafluoroethyl)-1-(trifluoromethyl)cyclohexane","1196870-46-8","D",0]
["N,N-Diethyl-1,1,1,2,2,3,3,5,6,6,8,9,9,11-tetradecafluoro-N-methyl-12-oxo-5,8,11-tris(trifluoromethyl)-4,7,10-trioxa-13-azahexadecan-16-aminium iodide","84166-37-0","D",0]
["N,N'-bis(Perfluorobutanoyl)1,5-pentanediamine","1814-80-8","D",0]
["3-(Ethylsulfanyl)-2,2,3,3-tetrafluoropropanoyl fluoride","77705-88-5","D",0]
["1,1,2-Tribromo-1-(nonafluorobutyl)ethane","59665-24-6","D",0]
["3-[2,2,3,3,4,4-Hexafluoro-4-(heptafluoropropoxy)butanamido]-N,N-dimethylpropan-1-amine N-oxide","87112-48-9","D",0]
["Carbamic acid, (1-(bis(1-methylethoxy)phosphinyl)-2,2,2-trifluoro-1-(trifluoromethyl)ethyl)-,phenylmethyl ester","145430-04-2","D",0]
["6-Methyl-4-(tridecafluorohexyl)pyrimidine-2(1H)-thione","240801-02-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorotetradecane","89109-68-2","D",0]
["3-Oxo-2-[2-(2,2,3,3-tetrafluoro-2,3-dihydro-1,4-benzodioxin-6-yl)hydrazinylidene]butanenitrile","36865-60-8","D",0]
["3-(Perfluorohexyl)-5-phenyl-1H-pyrazole","510768-12-4","D",0]
["5-(Heptafluoropropyl)pyrimidine","1354703-21-1","D",0]
["Perfluorooctadecanoate anion","798556-82-8","D",0]
["p,p'-Bis(undecafluorocyclohexanemethanol) pyrophosphate","48240-25-1","D",0]
["2-(Pentafluoroethyl)-4,5-dihydro-1,3-oxazole","7024-92-2","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-N-phenylpropanamide","178167-74-3","D",0]
["Ethyl [1,1,1,3,3,3-hexafluoro-2-(2-pyrimidinylamino)-2-propanyl]carbamate","256333-13-8","D",0]
["4,4,4-trifluoro-2-methyl-1-(thiophen-2-yl)-3-(trifluoromethyl)but-2-en-1-one","35444-11-2","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxin-6-amine","89586-07-2","D",0]
["2,2,3,3-Tetrafluoropropyl 5-[(2-methoxyphenyl)amino]-5-oxopentanoate","5578-69-8","D",0]
["Phenol, 4,4'-(2,2,3,3,4,4,5,5-octafluoropentylidene)bis-","297137-44-1","D",0]
["(6-Chloro-3,3,4,4,5,5,6,6-octafluoro-1-iodohexyl)trimethylsilane","104431-27-8","D",0]
["O-Ethyl 3,3,3-trifluoro-2-(trifluoromethyl)propanethioate","867-93-6","D",0]
["1-(Tridecafluorohexyl)naphthalene","93697-17-7","D",0]
["4-Chloro-1,1,2,2,3,3-hexafluorobutane","75877-96-2","D",0]
["Perfluoroundecanedioic acid","24647-11-8","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-[4-(pyrazin-2-yl)piperazin-1-yl]butan-1-one","89007-14-7","D",0]
["1-nitro-4-(pentafluoroethoxy)benzene","1743-96-0","D",0]
["2-Hydroxyethyl heptadecafluorononanoate","92746-93-5","D",0]
["(Perfluorohexyl)-1-propyl prop-2-enoate","216389-85-4","D",0]
["2-Hydroxy-N,N-dimethyl-N-{3-[(perfluorobutanesulfonyl)amino]propyl}-3-sulfopropan-1-aminium","2089108-71-2","D",0]
["N-[3-(Dimethyloxidoamino)propyl]perfluoro-3,7-dioxaoctanamide","1204950-97-9","D",0]
["2-(tert-Butylperoxy)-1,1,1,3,3,3-hexafluoropropan-2-ol","54857-32-8","D",0]
["2-Ethyl-4,4,4-trifluoro-3-hydroxy-1-(2-thienyl)-3-(trifluoromethyl)-1-butanone","34844-36-5","D",0]
["N,N,N-Trimethyl-3-[(perfluoro-1-oxodecyl)amino]-1-propanaminium iodide","2284-73-3","D",0]
["Bis[2-(perfluorohexyl)ethyl] fumarate","24120-19-2","D",0]
["Flexicare AF-120","910476-54-9","D",0]
["1,3-Dichloro-5-isocyanato-2-(1,1,2,2-tetrafluoroethoxy)benzene","104147-33-3","D",0]
["2-(Heptafluoropropyl)-3-phenylquinoxaline","69492-70-2","D",0]
["2,2,3,3,4-Pentafluoro-4-(prop-2-en-1-yl)cyclobutan-1-one","155581-08-1","D",0]
["3-{[3-(Dimethylamino)propyl](1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexane-1-sulfonyl)amino}-2-hydroxypropane-1-sulfonic acid","788772-31-6","D",0]
["N-Ethyl-N-(2,2,3,3,4,4,5,5-octafluoropentyl)aniline","67012-63-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-6-[(trifluoroethenyl)oxy]hexane","103489-99-2","D",0]
["nonadecafluorodecanamide","307-40-4","D",0]
["N-Methyl-N-[2-(sulfooxy)ethyl]perfluorododecanesulfonamide","61481-06-9","D",0]
["2-(Pentafluoroethyl)-3,4,5-tris(trifluoromethyl)furan","108451-32-7","D",0]
["Undecafluorocyclohexyl prop-2-enoate","16621-95-7","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.'-[1,2-phenylenebis[carbonyloxy[2-(chloromethyl)-2,1-ethanediyl]]]bis[.omega.-fluoro-","71550-17-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorododecane","66563-68-6","D",0]
["Phosphorane, difluorotris(nonafluorobutyl)-","91543-34-9","D",0]
["2,2,3,3,4,4,5,6,6-Nonafluoro-5-(heptafluoropropyl)oxane","801-26-3","D",0]
["6-Methyl-2,2,4,4-tetrakis(trifluoromethyl)-1,3-dioxane","101198-16-7","D",0]
["1,1,1,2,2,3,3-Heptafluoro-4-chlorobutane","374-97-0","D",0]
["Perfluoro-3,6,9-trioxatridecanoic acid","330562-41-9","D",0]
["3-[(3-{[(Perfluoropropyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","89148-24-3","D",0]
["{[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfonyl]amino}-3-betaine","34455-27-1","D",0]
["Methyl 3,3,3-trifluoro-2-methyl-2-(trifluoromethyl)propanoate","13027-16-2","D",0]
["1,2,3,4-Tetrafluoro-5-(pentafluoroethyl)benzene","138947-19-0","D",0]
["Diammonium 4,4,5,5,6,7,7,7-octafluoro-6-(trifluoromethyl)-1-heptanol phosphate","63295-21-6","D",0]
["2-Pentanone, 1-chloro-4-hydroxy-5,5,5-trifluoro-4-(trifluoromethyl)-","101931-66-2","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-Tetratriacontafluorooctadecane","181765-99-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,15,15,16,16,17,17,18,18,19,19,20,20,20-Hexacosafluoro-8,13-diiodoicosane","959462-51-2","D",0]
["Barium bis(6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-5-oxooct-3-en-3-olate)","36885-31-1","D",0]
["2λ5,4λ5,6λ5-1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexakis[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]-","16059-16-8","D",0]
["1-[2-(1,1,2,2-Tetrafluoro-2-phenylethyl)phenyl]ethan-1-one","61547-69-1","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoro-1-phenylheptane-1,3-dione","168920-97-6","D",0]
["N-(2-Bromoallyl)-3,3,3-trifluoro-2-(trifluoromethyl)propionamide","102128-87-0","D",0]
["1,1,1,2,2,3,3-heptafluorobutane","662-00-0","D",0]
["Butanoic acid, 3,3,4,4-tetrafluoro-2,2-dimethyl-","144194-01-4","D",0]
["2,2,3,3,3-Pentafluoro-1-methylsulfanyl-propan-1-imine","664-09-5","D",0]
["Methyl 3,5,6-trichloro-2,2,3,4,4,5,6,6-octafluorohexanoate","812-90-8","D",0]
["1,1,2,3,3,4,5,5,5-Nonafluoro-4-(trifluoromethyl)pent-1-ene","287101-12-6","D",0]
["Ethyl 3-chloro-2,2,3,4,4,5,6,6-octafluorohex-5-enoate","64566-20-7","D",0]
["N,N-Dimethyl-3,3-bis(trifluoromethyl)-3H-1,2,4-diselenazol-5-amine","67213-19-8","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, reaction products with phosphorus oxide (P2O5), potassium salts","1224952-82-2","D",0]
["2-Octen-4-one, 5,5,6,6,7,7,8,8-octafluoro-2-mercapto-","88552-04-9","D",0]
["1-[Bromo(difluoro)methoxy]-2-{2-[bromo(difluoro)methoxy]-1,1,2,2-tetrafluoroethoxy}-1,1,2,2-tetrafluoroethane","330562-49-7","D",0]
["2-Amino-6,6,7,7,8,8,8-heptafluorooctanoic acid","10325-14-1","D",0]
["1,1,1,3,3,4,4,4-Octafluoro-2-butanol","127256-73-9","D",0]
["6,6,7,7,8,8,9,9-Octafluoro-2,2-dimethylnonane-3,5-dione","62679-65-6","D",0]
["Ethyl 3,3,4,4,5,5,5-heptafluoropentanoate","773136-96-2","D",0]
["1,1,1,2,2,3,3,4,4,5,6,6,6-Tridecafluorohexane","1998-54-5","D",0]
["2,2,4,4,5,5-Hexafluoro-1,3-bis(trifluoromethyl)imidazolidine","74554-48-6","D",0]
["Perfluorodecalin (trans)","60433-12-7","D",0]
["3,5-Bis(perfluorohexyl)-1-(nonafluoropentanoyl)-1H-pyrazole","231630-88-9","D",0]
["3-Methyl-3-(2,2,3,3,3-pentafluoropropoxy)oxetane","813460-60-5","D",0]
["4-Chloro-5-methyl-3-(perfluorohexyl)pyrazole","244022-66-0","D",0]
["Ammonium 3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfanyl]propanoate","2196185-58-5","D",0]
["1,1,3,5,5-Pentamethyl-1,5-bis(3,3,4,4,5,5,6,6,6-nonafluorohexyl)trisiloxane","147986-73-0","D",0]
["1,1,2,2,3,3-Hexafluorobutane","119450-66-7","D",0]
["N-(3-Benzoylphenyl)-1,2,2,2-tetrafluoroethane-1-sulfonamide","62261-65-8","D",0]
["Methyl 4-(pentadecafluoroheptyl)benzoate","88951-03-5","D",0]
["3-[2-(1,1,1,3,3,3-Hexafluoro-2-propanyl)-4-(1,1,1,3,3,3-hexafluoro-2-propanylidene)-1,3-dithietan-2-yl]-2,5-dimethyl-7λ4-[1,2]dithiolo[1,5-b][1,2]dithiole","66172-14-3","D",0]
["(5E)-7,7,8,8,9,9,10,10,10-Nonafluoro-5-iododec-5-en-1-ol","137648-89-6","D",0]
["4-[(Nonadecafluorodecyl)oxy] benzenesulfonic acid","64910-97-0","D",0]
["Hexafluorooxetane","425-82-1","D",0]
["1,5-Bis(ethylsulfanyl)-1,1,2,2,4,4,5,5-octafluoropentan-3-one","685880-46-0","D",0]
["Ethanesulfonyl fluoride, 1,1,2,2-tetrafluoro-2-[(1,2,2-trifluoroethenyl)oxy]-, polymer with \n1,1,2,2-tetrafluoroethene","69462-70-0","D",0]
["4-(2,2,3,3,4,4,5,5-Octafluoropentyl)phenol","111915-34-5","D",0]
["Poly[oxy(1,1,2,2,3,3,4,4-octafluoro-1,4-butanediyl)], .alpha.-(1,1,2,2,3,3-hexafluoro-4-hydroxybutyl)-.omega.-(1,1,2,2,3,3-hexafluoro-4-hydroxybutoxy)-","146191-87-9","D",0]
["4'-(Heptadecafluorooctyl)-3-octyl-2,2'-bithiophene","844436-13-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorohenicosane","125635-86-1","D",0]
["Methyl perfluorotetradecanoate","203302-99-2","D",0]
["Hentriacontafluorohexadecanoyl fluoride","210972-74-0","D",0]
["6,6,7,7,8,8,9,9,10,10,11,11,11-Tridecafluoroundecan-1-ol","134052-02-1","D",0]
["Bis(2,2,3,3-tetrafluoropropyl) 2-methylidenebutanedioate","104887-33-4","D",0]
["2,4,6-Tribromophenyl 3,4-dibromo-2,2,3,4,4-pentafluorobutanoate","124311-21-3","D",0]
["N,N-Dimethyl-N-(3-F-octylpropyl)-5-ammoniopentanoate","145441-34-5","D",0]
["Tetrafluoroiodo(trifluoromethoxy)-ethane","69066-98-4","D",0]
["3-(Heptafluoroisopropoxy)propyltriethoxysilane","149838-19-7","D",0]
["2-[3-[[(Perfluorooctyl)sulfonyl]amino]propoxy]-N,N,N-trimethylethanaminium","91707-62-9","D",0]
["[(1,1,2,2-Tetrafluoroethyl)sulfanyl]acetic acid","665-35-0","D",0]
["2,2,3,3,3-Pentafluoropropyl propyl carbonate","1980085-61-7","D",0]
["4-Hydroxy-3-(hydroxyimino)-4-(nonafluorobutyl)-1,3,4,5-tetrahydro-2H-1,5-benzodiazepin-2-one","216307-12-9","D",0]
["N-(2-Chloroethyl)-N'-(2,2,3,3,4,4,5,5,6,6-decafluorocyclohexyl)-N-nitrosourea","74795-00-9","D",0]
["Perfluorodecahydro-2-t-butylnaphthalene","119107-97-0","D",0]
["1,1,2,2,3,3-Hexafluoro-1-[(propan-2-yl)oxy]propane","393517-66-3","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(pentafluorophenyl)butan-1-one","19108-37-3","D",0]
["2,2,3,4,4,5,5,5-Octafluoro-3-(trifluoromethyl)pentanoic acid","64139-66-8","D",0]
["1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-tetracosafluoro-2,11-bis(trifluoromethyl)dodecane","118694-32-9","D",0]
["4-[4-(Heptadecafluorooctyl)phenoxy]phenol","404580-53-6","D",0]
["Phenylcarbamic acid--[2,2-bis(trifluoromethyl)-1,3-dioxolan-4-yl]methanol (1/1)","51125-53-2","D",0]
["2-(Chloromethyl)-1,1,1,3,3,3-hexafluoro-2-iodopropane","240122-22-9","D",0]
["Ethyl 3-chlorotetrafluoropropionate","24482-88-0","D",0]
["4-[(Heptadecafluorooctyl)oxy]benzene-1,3-diamine","96573-73-8","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(sulfooxy)ethyl]-","65530-77-0","D",0]
["3,4,4,5,5,6,6,7,7,8,8-Undecafluorooct-2-enoic acid","110680-70-1","D",0]
["2-ethyl-4,4,4-trifluoro-3-hydroxy-1-phenyl-3-(trifluoromethyl)butan-1-one","34844-21-8","D",0]
["Ethyl (2E)-3-(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfinyl)prop-2-enoate","1606997-39-0","D",0]
["2-Ethoxy-6-morpholino-4,4-di(trifluoromethyl)-4h-1,3,5-oxadiazine","5226-19-7","D",0]
["N-(2,4-Dinitrophenyl)-1,2,2,3,3,4,4,5,5,6,6-undecafluorocyclohexanecarboxamide","107349-88-2","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(propyldisulfanyl)propane","109746-35-2","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(propane-2-sulfonyl)benzoic acid","1355554-50-5","D",0]
["N,N,N-Trimethyl-2-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]ethanaminium iodide","52610-15-8","D",0]
["(1,1,2,3,3,3-Hexafluoropropyl)(trimethyl)silane","62281-36-1","D",0]
["Triethyl(fluoro)(1,2,3,3,3-pentafluoroprop-1-en-1-yl)-lambda~5~-phosphane","120154-83-8","D",0]
["8-Sulfoperfluoro-2,5-dimethyl-3,6-dioxaoctanoic acid","1235024-21-1","D",0]
["10:2 Fluorotelomer sulfonamide","29766-02-7","D",0]
["Perfluoro-2-(2-ethoxyethoxy)-1,1-diphenylethan-1-ol","217824-95-8","D",0]
["1-Octanesulfonic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, mixt. with ammonium 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-octanesulfonate","314057-01-7","D",0]
["2,2,3,3,3-pentafluoro-N-naphthalen-2-ylpropanamide","21970-68-3","D",0]
["Hexafluorocyclobutanone","699-35-4","D",0]
["N-[8-(Heptafluoropropyl)-9H-purin-6-yl]acetamide","147916-78-7","D",0]
["1-(Diethylamino)-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-2-ol","53269-56-0","D",0]
["2-(Nonafluorobutyl)-1-benzothiophene","1608112-38-4","D",0]
["Methyl 4H-perfluorobutanoate","356-32-1","D",0]
["1,1-Dichloro-2,3,3,4,4,4-hexafluorobut-1-ene","110781-73-2","D",0]
["1,1,1,2,2,3,3,4-Octafluorooctane","126038-55-9","D",0]
["6,6,7,7,8,8,9,9,10,10,11,11,11-Tridecafluoroundecane-1,4-diol","134298-52-5","D",0]
["1,1,3,5,6-Pentachloro-1,2,2,3,4,4,5,6,6-nonafluorohexane","307-26-6","D",0]
["1,1,1,3,3,4,5,5,5-Nonafluoro-4-(trifluoromethyl)pentan-2-one","73041-05-1","D",0]
["(2,2,4,4-Tetrafluoro-2H,4H-1,3-benzodioxin-6-yl)boronic acid","870822-77-8","D",0]
["2-Ethyl-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctanoic acid","136022-87-2","D",0]
["Methyl 2,2,3,3-tetrafluoro-3-(methanesulfonyl)propanoate","86414-19-9","D",0]
["2-Propenoic acid, 2-methyl-, polymer with 2-(diethylamino)ethyl 2-methyl-2-propenoate, alpha-fluoro-omega-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene), oxiranylmethyl 2-methyl-2-propenoate and 2-propenoic acid","870465-08-0","D",0]
["1-Methoxy-4-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-45-5","D",0]
["4-[(Heptadecafluorononyl)oxy]-benzenesulfonyl chloride","59536-14-0","D",0]
["5,5,6,6-Tetrafluoro-3-iodohex-1-ene","74793-39-8","D",0]
["Ethyl [1,1,1,3,3,3-hexafluoro-2-(4-fluoroanilino)propan-2-yl]carbamate","5226-22-2","D",0]
["Perfluoro[1,2-13C2]undecanoic acid","960315-51-9","D",0]
["Poly(cyclohexan-1-yl methacrylate)-co-(oxiran-2-ylmethyl methacrylate)-co-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-yl methacrylate)","681800-09-9","D",0]
["2,2,3,3-Tetrafluoropropyl acetate","681-58-3","D",0]
["1-Bromo-4-[3,3,4,4,5,5,5-heptafluoro-2,2-bis(trifluoromethyl)pentyl]benzene","149068-60-0","D",0]
["2,3,3,3-tetrafluoro-2-methoxypropanamide","10186-65-9","D",0]
["Phosphonic acid, [3-[ethyl[(pentadecafluoroheptyl)sulfonyl]amino]propyl]-","71463-79-1","D",0]
["2-bromo-3,4,4,4-tetrafluoro-3-(trifluoromethyl)but-1-ene","234443-24-4","D",0]
["Bis(heptafluoropropyl)phosphinic acid","1481-60-3","D",0]
["Ethyl {[1,1,1,3,3,3-hexafluoro-2-(trifluoromethyl)propan-2-yl]oxy}acetate","61468-27-7","D",0]
["N-(2,3-Dichlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","121806-68-6","D",0]
["3-methylphenyl pentafluoropropanoate","24271-51-0","D",0]
["1-((Perfluoro[3-[1-methylethoxy]propyl])ethyl)pyridinium chloride","144930-59-6","D",0]
["1-Bromo-4-[1,1,2,2-tetrafluoro-2-(4-propylphenyl)ethyl]benzene","153654-93-4","D",0]
["Acetic acid, 2,2-bis[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]-","86415-75-0","D",0]
["8,8,9,9-Tetrafluoro-6b,8,9,9a-tetrahydroacenaphtho[1,2-b]thiophene","102585-21-7","D",0]
["1-Amino-4,4,5,5-tetrafluoro-1-phenylpent-1-en-3-one","80460-20-4","D",0]
["Benzo[b]thiophene, 3,3'-(3,3,4,4,5,5-hexafluoro-1-cyclopentene-1,2-diyl)bis[2-methyl-","137814-07-4","D",0]
["N-Ethylperfluorobutanamide","70473-76-6","D",0]
["1-Pentene, 1,1,2-trichloro-3,3,4,4,5,5,5-heptafluoro-","81291-44-3","D",0]
["Butanoic acid, 3,3,4,4-tetrafluoro-2-hydrazino-2-hydroxy-, hydrazide","89972-14-5","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoro-1-(pentafluorophenyl)piperidine","58955-19-4","D",0]
["methyl-(7,7,8,8,9,9,10,10,10-nonafluorodecyl)amine","228569-98-0","D",0]
["1,1,1-Trifluoro-2-(trifluoromethyl)pent-3-en-2-ol","66068-01-7","D",0]
["1,2,2,3,3,4,4,5,5,6-Decafluorohexane-1,6-disulfonyl difluoride","84933-50-6","D",0]
["3,4-Dibromo-2,2,3,4,4-pentafluorobutanoyl chloride","124311-14-4","D",0]
["1~5~,4~5~-Bis(tridecafluorohexyl)-1~2~,2~2~:2~5~,3~2~:3~5~,4~2~-quaterthiophene","446043-85-2","D",0]
["1-(1-Bromo-2,2,2-trifluoroethoxy)-1,1,2,2-tetrafluoroethane","51480-56-9","D",0]
["Methyl 4-[[(nonafluorobutyl)sulfonyl]oxy]benzoate","41605-53-2","D",0]
["Ethyl 3-amino-4,4,5,5,6,6,6-heptafluorohex-2-enoate","87613-26-1","D",0]
["1-[4-(1,1,2,2-Tetrafluoro-2-phenylethyl)phenyl]ethan-1-one","40396-63-2","D",0]
["3-((3-((2-Hydroxyethyl)(dimethyl)azaniumyl)propyl)((perfluorobutyl)sulfonyl)amino)propane-1-sulfonate","2089108-94-9","D",0]
["Perfluoroethyl acetate","343269-97-6","D",0]
["4-(Heptadecafluorooctyl)benzoic acid","74701-33-0","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reduced, reaction products with 1-chloro-2,3-epoxypropane","161075-08-7","D",0]
["1,1,3,3,3-Pentafluoro-2-(trifluoromethyl)propane-1-thiol","62619-34-5","D",0]
["Benzoic acid--2,2,3,3,3-pentafluoropropan-1-ol (1/1)","67103-70-2","D",0]
["Perfluorodecalin-perfluorotripropylamine mixt.","64827-90-3","D",0]
["Diethylmethoxy(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)silane","608299-46-3","D",0]
["[3,3,4,4,5,5,6,6-octafluoro-6-(2-methylprop-2-enoyloxy)hexyl] 2-methylprop-2-enoate","487048-96-4","D",0]
["Dimethyl 2,2'-[(1,1,2,2-tetrafluoroethane-1,2-diyl)bis(oxy)]bis(difluoroacetate)","24647-20-9","D",0]
["Tris(nonafluorobutyl)(oxo)-lambda~5~-phosphane","58431-34-8","D",0]
["4,4,4-trifluoro-3-(trifluoromethyl)-1-[3-(trifluoromethyl)phenyl]but-2-en-1-one","35444-05-4","D",0]
["2-Amino-1-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]ethan-1-ol--hydrogen chloride (1/1)","70143-78-1","D",0]
["2,4,6,6,7,7-Hexafluoro-1,5-dimethoxy-8-oxabicyclo[3.2.1]octan-3-one","65594-12-9","D",0]
["1-[(2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl)oxy]-4-ethenylbenzene","64253-90-3","D",0]
["1-(5-bromothiophen-2-yl)-4,4,5,5,6,6,6-heptafluorohexane-1,3-dione","326-07-8","D",0]
["2-Methylperfluorobutane","154381-64-3","D",0]
["2,5-Furandione, polymer with 2-methyl-3-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethoxy]-1-propene","35164-43-3","D",0]
["Perfluorotridecanesulfonic acid","791563-89-8","D",0]
["2-(4-Amino-2-methylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","2017-31-4","D",0]
["2-Fluoro-4-(1,1,2,2-tetrafluoroethanesulfinyl)aniline","100331-02-0","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[[(perfluorobutyl)sulfonyl]amino]-1-propanaminium","2089108-66-5","D",0]
["N-Ethyl-3,3,3-trifluoro-2-(trifluoromethyl)prop-1-en-1-imine","50260-30-5","D",0]
["4-Heptanone, 2,6-bis(trifluoromethyl)-2,6-dihydroxy-1,1,1,7,7,7-hexafluoro-","10487-11-3","D",0]
["(1s,4s)-4-(Heptafluoropropyl)cyclohexane-1-carboxylic acid","88951-22-8","D",0]
["HG’-01","73287-23-7","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol and octadecylamine","161212-22-2","D",0]
["2-Propenoic acid, butyl ester, polymer with 2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate","29133-22-0","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol and 3-aminopropyltriethoxysilane","161212-21-1","D",0]
["2,2,3,3-Tetrafluoropropyl dichloroacetate","57878-44-1","D",0]
["Methyl 4,4,5,5,6,6,7,7-octafluoro-3-oxoheptanoate","89129-69-1","D",0]
["1-Aziridinepropionic acid, 2,2,3,3-tetrafluoropropyl ester","24116-22-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodoicosane","121633-31-6","D",0]
["2,2,3,3,4,5,5-Heptafluoro-4-(trifluoromethyl)oxolane","374-53-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N,N-diphenylnonanamide","157584-47-9","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]-, sodium salt (1:1)","245331-49-1","D",0]
["1,1,1,2,2-Pentafluoro-3-(trifluoromethoxy)propane","171182-94-8","D",0]
["1-(1H,1H-Perfluoro(6,12,18-trioxadocosyl)) 2-hexadecylbutanedioate","223929-64-4","D",0]
["2-(N-Methyl-perfluorooctane sulfonamido) acetic acid","2355-31-9","D",0]
["3,3,4,4-Tetrafluoro-1-methylcyclobut-1-ene","88469-25-4","D",0]
["N-Propyl-perfluorotridecanesulfonamide hydrochloride","94817-83-1","D",0]
["2,3,5,6-Tetrafluoro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","20017-56-5","D",0]
["1,2,2,3,3,4,4,5,6,6,7,7,8,8-Tetradecafluorobicyclo[3.2.1]octane","918409-19-5","D",0]
["3-((3-((2-Carboxylatoethyl)(dimethyl)azaniumyl)propyl)((nonafluorobutyl)sulfonyl)amino)propanoate","1513864-25-9","D",0]
["2-Bromo-6-(difluoromethoxy)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)aniline","1262665-49-5","D",0]
["23-(Perfluorobutyl)tricosanoic acid","204316-37-0","D",0]
["Heptafluoro-2,3-dihydropyridine","51957-26-7","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-[(1,1,2-trifluoro-2-propen-1-yl)oxy]-, homopolymer","852533-63-2","D",0]
["P,P-Bis(perfluoro-7-methyloctyl) phosphinic acid ytterbium(3+) salt (3:1)","500776-88-5","D",0]
["1-Ethoxy-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-2-ol","89807-89-6","D",0]
["1-Ethoxy-2,2,3,3-tetrafluorospiro[3.5]nonan-1-ol","144194-02-5","D",0]
["4-Nitro-2-(1,1,2,2-tetrafluoroethyl)-6-(trifluoromethyl)-1H-benzimidazole","73618-59-4","D",0]
["2,4-HEPTANEDIONE, 6-HYDROXY-7,7,7-TRIFLU","101913-70-6","D",0]
["1,1'-[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]bis[4-iodobenzene","55100-57-7","D",0]
["2,4,6-Tris[(2,2,3,3,4,4,5,5,5-nonafluoropentyl)oxy]-1,3,5-triazine","54862-46-3","D",0]
["S-Ethyl 3,3,4,4,5,5,5-heptafluoro-2-(2-oxopropyl)pentanethioate","1392881-17-2","D",0]
["2-Bromo-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-1-ol","89807-85-2","D",0]
["1-[Difluoro(iodo)methoxy]-1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethane","138370-72-6","D",0]
["3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10‐Hexadecafluorodec‐2‐en‐1‐ol","256384-09-5","D",0]
["1,1,1,2,3,3,5,5,7,7,7-Undecafluoro-6-iodo-2,4-bis(trifluoromethyl)heptane","922524-01-4","D",0]
["N-Methylperfluoroheptanamide","89932-74-1","D",0]
["1,3-Bis[(perfluorohexyl)ethylthio]-2-propanol","160819-46-5","D",0]
["2,2,3,3,3-Pentafluoro-1-[4-(3-fluoro-4-methoxyphenyl)-8-phenylpyrazolo[5,1-c][1,2,4]triazin-3-yl]propan-1-one","91067-37-7","D",0]
["2-(N-Methylperfluorooctanesulfonamido)acetate","909405-48-7","D",0]
["1-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-3,5-dinitrobenzene","24813-57-8","D",0]
["3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Hexadecafluoro-N-(2-hydroxyethyl)-N,N-dimethyl-2-decen-1-aminium chloride (1:1)","71248-41-4","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)propanenitrile","60308-66-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluoro-N-[3-(triethoxysilyl)propyl]octane-1-sulfonamide","106790-26-5","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(propane-1-sulfinyl)benzoic acid","1355554-25-4","D",0]
["1,1,1,2,2-Pentafluoro-2-[(trifluoromethyl)sulfonyl]ethane","84416-69-3","D",0]
["(2-Bromo-1,1,2,2-tetrafluoroethoxy)(difluoro)acetic acid","81233-14-9","D",0]
["Sodium bis(1H,1H,2H,2H-perfluorodecyl)phosphate","114519-85-6","D",0]
["1,1,1-Trifluoro-4-[(propan-2-yl)amino]-2-(trifluoromethyl)butan-2-ol","824954-69-0","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol and diethylenetriamine","161212-13-1","D",0]
["2,3-Diphenyl-5,5-bis(trifluoromethyl)-2,5-dihydro-1,2,4-oxadiazole","62457-66-3","D",0]
["2,2,3,3-tetrafluoro-1-piperidin-1-ylpropan-1-one","300403-32-1","D",0]
["11-(4-{[5-(4,4,5,5,5-Pentafluoropentane-1-sulfonyl)pentyl]oxy}phenyl)estra-1(10),2,4-triene-3,17-diol","151555-47-4","D",0]
["12:2 Fluorotelomer thioether amido sulfonic acid","1513864-07-7","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(fluoromethoxy)propane","184899-81-8","D",0]
["4,4,5,5,5-pentafluoropentan-2-one","77893-59-5","D",0]
["8:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["N-[3-(Dimethylamino)propyl]perfluorobutanamide","64790-29-0","D",0]
["3,3,3-Trifluoro-N,2-bis(trifluoromethyl)propanamide","103547-54-2","D",0]
["1,1,1,3-Tetrafluoro-4-methyl-2-(trifluoromethyl)pent-2-ene","62116-45-4","D",0]
["6-chloro-N-[3-[(6-chloro-2,2,3,3,4,4,5,5,6,6-decafluorohexanoyl)amino]-2,2-dimethylpropyl]-2,2,3,3,4,4,5,5,6,6-decafluorohexanamide","6396-81-2","D",0]
["5-Phenyl-3,3-bis(trifluoromethyl)-3H-1,2,4-diselenazole","67213-20-1","D",0]
["Sodium 6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-3,5-dioxooctan-4-ide","24347-13-5","D",0]
["2,2-Dimethyl-1-[1,1,3,3,3-pentafluoro-2-(trifluoromethyl)propyl]aziridine","19390-80-8","D",0]
["1,1,1,2,2,3,3,4,4,10,10,11,11,12,12,13,13,13-Octadecafluoro-6,8-diiodotridecane","40735-21-5","D",0]
["cis-1-Iodo-2-(pentafluoroethyl)cyclohexane","38787-68-7","D",0]
["3-[(Perfluoroheptyl)methyloxy]-1,2-propanediol","126814-95-7","D",0]
["Imidazolidine, 2,2-bis(trifluoromethyl)-, hydrate","64038-67-1","D",0]
["N'-(3,3-Dimethyl-3,4-dihydroisoquinolin-1-yl)-2,2,3,3,4,4,4-heptafluorobutanehydrazide","304435-60-7","D",0]
["1,1,1,2,3,3,5,5,5-Nonafluoro-4-iodo-2-(trifluoromethyl)pentane","922524-00-3","D",0]
["Perfluorooctadecanesulfonic acid","51604-60-5","D",0]
["2-Chloroperfluoropentane","43216-18-8","D",0]
["Cadmium bis(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexan-1-ide)","104698-09-1","D",0]
["N,N-Dibutyl-2-(perfluorotridecyl)ethanaminium nitrate","94817-82-0","D",0]
["Carbonic acid, 3-(2,5-dimethylphenyl)-8-methoxy-2-oxo-1-azaspiro[4.5]dec-3-en-4-yl ethyl ester mixt. with N2-[1,1-dimethyl-2-(methylsulfonyl)ethyl]-3-iodo-N1-[2-methyl-4-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]phenyl]-1,2-benzenedicarboxamide","1000984-35-9","D",0]
["6,7-Dichloro-5,5,6,7,7-pentafluoro-4-(trifluoromethyl)hept-1-en-4-ol","594840-40-1","D",0]
["3-(1,1,2,2,2-Pentafluoroethylsulfanyl)propan-1-amine","1208080-59-4","D",0]
["Trimethylsilyl heptafluorobutanoate","24929-99-5","D",0]
["Dimethyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silanol","124617-22-7","D",0]
["3H,3H-Perfluoroheptane-2,4-dione","20583-66-8","D",0]
["5-[[Dimethyl(3-(perfluorohexyl)propyl)silyl]oxy]-3-methyl-1-pentyn-3-ol","1592562-42-9","D",0]
["bis(perfluoroheptanoyl) peroxide","42514-14-7","D",0]
["1-Methyl-3-(pentafluoroethyl)-4-(trifluoromethyl)-1H-pyrazole","1845774-24-4","D",0]
["5:1:2 Fluorotelomer betaine","171184-02-4","D",0]
["Pentyl 2,2,3,3,4-pentafluoro-4-oxobutanoate","92614-00-1","D",0]
["2-Amino-5,5,6,6,7,7,8,8,8-nonafluorooctanoic acid","125162-63-2","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoro-N~1~-hydroxy-N~8~-phenyloctanediamide","1308677-14-6","D",0]
["2,3-Difluoro-2-(pentafluoroethyl)-3-(trifluoromethyl)oxirane","71917-15-2","D",0]
["Perfluoro-2-hydroxyethane-1-sulfonyl fluoride","733736-25-9","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl 3-methylbutanoate","914637-45-9","D",0]
["4-(2,2,3,3-Tetrafluoropropoxy)-N-(2,2,2-trifluoroethyl)aniline","1365808-55-4","D",0]
["3H-Diazirine, 3,3-bis(trifluoromethyl)-","3024-50-8","D",0]
["Bis(2-methylpropyl) (heptafluoropropyl)phosphonate","88093-17-8","D",0]
["(4Z)-5-Amino-1,1,2,2-tetrafluorohex-4-en-3-one","72721-34-7","D",0]
["12-H-Perfluorododecanoic acid","351194-78-0","D",0]
["3-Benzamido-N-(2,2,3,3,4,4,4-heptafluorobutyl)benzamide","917920-92-4","D",0]
["Diethyl 1,1,1,2-tetrafluoronon-2-en-3-yl phosphate","113487-26-6","D",0]
["[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)sulfanyl]benzene","65079-24-5","D",0]
["1-Chloro-1,1,2,2-tetrafluoro-2-(2,2,2-trifluoroethoxy)ethane","51410-32-3","D",0]
["3-(Perfluorohexanesulfonamido)-N,N,N-trimethylpropan-1-aminium","70248-51-0","D",0]
["Methoxy(3,3,4,4,5,5,5-heptafluoropentyl)propyl(3,3,3-trifluoropropyl)silane","608300-10-3","D",0]
["p-(4,4,4-Trifluoro-3-trifluoromethylcrotonoyl)benzonitrile","35444-04-3","D",0]
["1-Chloro-5-methyl-3,3-bis(trifluoromethyl)-1,3-dihydro-1lambda3,2-benziodoxole","69352-01-8","D",0]
["N-(Perfluoroheptylsulfonyl)-N-propylglycine potassium","123085-30-3","D",0]
["Methyl 5-(heptafluoropropyl)furan-2-carboxylate","104939-25-5","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-methylbutanamide","4314-42-5","D",0]
["1-(1,1,2,2-Tetrafluoroethoxy)propadiene","106609-52-3","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-iodooct-1-yne","58292-95-8","D",0]
["Propane, 1,2-dichloro-1,1,2,3,3-pentafluoro-","422-44-6","D",0]
["Bis[3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctylsulfanyl)propyl] But-2-enedioate","56927-83-4","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-1-phenylnon-1-en-3-ol","64511-24-6","D",0]
["Chromium chloride-perfluorooctanoic acid complex","55801-89-3","D",0]
["2,2,3,4,4,6,6,7,7,9,9,11,11,13,13,13-Hexadecafluoro-5,8,10,12-tetraoxatridecanoic acid","919005-29-1","D",0]
["1,1,1,3-Tetrafluoro-2-(trifluoromethyl)hept-3-ene","62116-46-5","D",0]
["1H,1H,3H-Perfluoro(2,4-dimethylpentan-1-ol)","25065-50-3","D",0]
["HG–02","205367-61-9","D",0]
["1-Butanaminium, N,N,N-tributyl-, 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate (1:1)","108427-52-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorohenicosane","677324-30-0","D",0]
["[4-(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)phenyl]methanol","892154-66-4","D",0]
["Dichloro(phenyl)[3-(2,2,3,3-tetrafluoropropoxy)propyl]silane","646063-07-2","D",0]
["6-(1-Methylethylidene)-5-(triphenylphosphoranylidene)-(perfluoro)-nonan-4-one","139225-92-6","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecane-1-sulfonate","481071-78-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorohexadecane","89109-69-3","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-(4-fluorophenyl)hexane-1,3-dione","70862-62-3","D",0]
["Bis[1,1,1,3,3,4,4,5,5,5-decafluoro-2-(trifluoromethyl)pentan-2-yl]mercury","120674-92-2","D",0]
["(1-Chloro)tetrafluoro-1-iodoethane","754-23-4","D",0]
["Benzene, 1,1'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis-","83558-76-3","D",0]
["2-Methyl-2-phenyl-4,4,6-tris(trifluoromethyl)-1,5,6-triazabicyclo[3.1.0]hexane","95388-88-8","D",0]
["Poly{2,2,3,3,4,4-hexafluoro-4-(trifluorovinyl)oxybutanoic acid}","1331750-98-1","D",0]
["(1E)-4,4,5,5,5-Pentafluoro-1-phenyl-1-[(propan-2-yl)amino]pent-1-en-3-one","484009-71-4","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with 6-aminocaproic acid","161212-12-0","D",0]
["2,2,3,3-Tetrafluorobicyclo[2.1.0]pentane","87102-50-9","D",0]
["2-Bromo-3-(bromomethyl)-4,4,5,5,6,6,6-heptafluorohexan-3-ol","93339-87-8","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(perfluoropentyl)sulfonyl]amino]propyl]-1-propanaminium","2089108-72-3","D",0]
["[(1,1,2,3,3,4,4,5,5,6,6,6-Dodecafluorohexyl)oxy]acetic acid","919005-39-3","D",0]
["Perfluoro-3-methoxypropanoic acid","377-73-1","D",0]
["Methyl 3-(1,1,2,2-tetrafluoroethoxy)benzoate","70126-45-3","D",0]
["Octafluoro-p-dithiane","710-65-6","D",0]
["3-(Perfluorooctanesulfonamido)-N,N,N-trimethylpropan-1-aminium","70225-25-1","D",0]
["Perfluoro-1-methylindane","56594-69-5","D",0]
["5,6,7,8-13C4-Perfluorooctanoic acid","1017281-31-0","D",0]
["3,3,4,4,5,5,6,7,7,8,8,8-dodecafluoro-6-methyloctan-1-ol","68308-14-5","D",0]
["Dodecanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-tricosafluoro-, methyl ester","56554-52-0","D",0]
["tert-Butyl heptafluorobutaneperoxoate","91481-65-1","D",0]
["1-Nitro-4-[3,3,3-trifluoro-2-(trifluoromethyl)-1-propenyl]benzene","403646-07-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-[methyl[(nonafluorobutyl)sulfonyl]amino]ethyl ester, polymer with octadecyl 2-methyl-2-propenoate","819069-72-2","D",0]
["3-Hexyl-1-methyl-1H-Imidazolium perfluorobutanesulfonate","1001557-05-6","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl but-3-enoate","17165-56-9","D",0]
["2-(Difluoromethyl)-1,1,1,2,3,3-hexafluoropropane","65781-21-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-[(prop-2-en-1-yl)oxy]octane","103628-86-0","D",0]
["tris(pentafluoroethyl)phosphine Oxide","58431-32-6","D",0]
["1,1,1,2-Tetrafluoro-4-methyl-2-(trifluoromethyl)pentan-3-one","62656-72-8","D",0]
["(R)-Enflurane","22194-22-5","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluorodecanamide","154380-29-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,13,13,14,14,15,15,16,16,17,17,18,18,18-Hexacosafluoro-8,11-diiodooctadecane","959462-50-1","D",0]
["1H,1H,2'H-Perfluorodipropyl ether","1000-28-8","D",0]
["Pentadecafluoroheptan-1-ol","31165-24-9","D",0]
["4-[(Heptafluoropropyl)thio]benzoic acid","88489-74-1","D",0]
["1,1,1,3,5,6-Hexachloro-2,2,3,4,4,5,6,6-octafluorohexane","2106-32-3","D",0]
["[(1Z)-3,3,4,4,5,5,6,6,6-Nonafluorohex-1-en-1-yl]benzene","95452-53-2","D",0]
["2-Propenoic acid, hexadecyl ester, polymer with 1,3-diisocyanatomethylbenzene, .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene), 2-hydroxy-3-phenoxypropyl 2-propenoate, methyloxirane","154946-65-3","D",0]
["Halon-2401","124-72-1","D",0]
["2-(1,1,2,2,4,4,4-Heptafluorobutoxy)ethyl prop-2-enoate","137891-30-6","D",0]
["1-(Chloromethoxy)-1,1,2,3,3,3-hexafluoropropane","56860-84-5","D",0]
["[[(Heptadecafluorooctyl)sulfonyl]methylamino]methyl 2-methyl-2-propenoate","52738-45-1","D",0]
["2,2,2',2',3,3,3',3',4,4,4',4'-Dodecafluoro-1,1'-bi(cyclobutylidene)","68252-05-1","D",0]
["5,5,6,6,6-pentafluorohexan-1-ol","58556-45-9","D",0]
["1-Ethenyl-4-(nonafluorobutyl)benzene","159241-92-6","D",0]
["2,2,3,3,4,4-Hexafluoro-4-sulfinobutanoic acid","115432-29-6","D",0]
["1,1,1,2,2,3,3,4,4,5-Decafluorohexane","155072-58-5","D",0]
["[N-Methyl(perfluoroheptane-1-sulfonyl)amino]acetic acid","1910057-77-0","D",0]
["2,2,3,3-Tetrafluoro-1-methoxypropan-1-ol","88332-83-6","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-N-(4-nitrophenyl)heptanamide","164796-44-5","D",0]
["1,1,2,2-Tetrafluoro-1,2-bis(1,1,2,2-tetrafluoro-2-iodoethoxy)ethane","64053-21-0","D",0]
["3-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutyl)-3,4,4-trifluoro-1,2-oxathietane 2,2-dioxide","1244856-07-2","D",0]
["1-Heptanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,7,7,7-tetradecafluoro-6-(trifluoromethyl)-","1644617-02-6","D",0]
["2,2,3,3,4,4,5,6,6-Nonafluoro-5-(trifluoromethyl)oxane","61340-74-7","D",0]
["Bis(perfluorooctyl) phosphinothioic acid","610800-36-7","D",0]
["1-Chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-8-iodooctane","150223-08-8","D",0]
["3-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)aniline","2396-16-9","D",0]
["4,4,4-trifluoro-1-(4-nitrophenyl)-3-(trifluoromethyl)butane-1,3-diol","34848-24-3","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(1H-tetrazol-1-yl)butan-1-one","827346-17-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorotetracosane","200817-56-7","D",0]
["(1Z)-1,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluorooct-1-ene","1516885-18-9","D",0]
["3,4'-Bis(heptadecafluorooctyl)-2,2'-bithiophene","677033-16-8","D",0]
["(Perfluoro-7-methyloctyl)-2-hydroxypropyl 2-methylprop-2-enoate","88752-37-8","D",0]
["5,6-Dichloro-2-(pentafluoroethyl)-1H-benzimidazole","102516-93-8","D",0]
["3-((3-((2-Carboxyethyl)((tridecafluorohexyl)sulfonyl)amino)propyl)(dimethyl)azaniumyl)propanoate","756771-34-3","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexane-1-sulfonic acid","134615-56-8","D",0]
["1,12-Bis(perfluorodecyl)-2,11-diiodododecane","1980048-92-7","D",0]
["3-(Heptadecafluorooctyl)benzene-1-sulfonyl chloride","104818-20-4","D",0]
["N-[3-(Dimethylamino)propyl]perfluoro-3,4-bis(methoxy)cyclohexanecarboxamide N-oxide","200636-91-5","D",0]
["2-[4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methylphenyl]-4-iodo-1H-isoindole-1,3(2H)-dione","346575-66-4","D",0]
["4-((Heptadecafluorooctyl)sulfonyl)morpholine","312-19-6","D",0]
["1-Chloro-3,3,4,4,5,5-hexafluoro-2-methoxycyclopentene","336-34-5","D",0]
["Tris((5-difluoromethylperfluoropentyl)methyloxy)methylbenzene","992-81-4","D",0]
["2,2-Bis(trifluoromethyl)-1,3-thiazolidine--water (1/1)","28399-14-6","D",0]
["2,2,3,3,3-pentafluoro-1-phenylpropan-1-one","394-52-5","D",0]
["N,N-Dibutyl-2,3,3,3-tetrafluoropropanamide","745794-86-9","D",0]
["Pentyl 4,4,5,5,6,6,7,7,7-nonafluoroheptanoate","94345-13-8","D",0]
["1-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-4-nitrobenzene","2396-14-7","D",0]
["11-(Nonafluorobutyl)-9,10-dihydro-9,10-(epithiomethano)anthracene","267648-90-8","D",0]
["1-Hydroxy-4:2 fluorotelomer sulfonic acid","2089109-99-7","D",0]
["2-(6-Fluoro-1H-indol-3-yl)-N-[[3-(2,2,3,3-tetrafluoropropoxy)phenyl]methyl]ethanamine","467459-31-0","D",0]
["Cyclohept-1-en-1-yl nonafluorobutane-1-sulfonate","42108-79-2","D",0]
["4,5,5,5-Tetrafluoro-4-{1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy}-N-propylpentan-1-amine","928655-42-9","D",0]
["2,3,3,3-Tetrafluoro-1-iodoprop-1-ene","672339-38-7","D",0]
["2-chloro-3,4,4,4-tetrafluoro-3-(trifluoromethoxy)but-1-ene","261503-71-3","D",0]
["5,5,6,6,7,7,8,8,8-Nonafluoro-2-methyloct-2-ene","97294-02-5","D",0]
["2-(2,2-Dichloro-1,1-difluoroethoxy)-1,1,1,2-tetrafluoroethane","57041-65-3","D",0]
["Ammonium 4-(perfluorooctyloxy)benzenesulfonic acid","138473-77-5","D",0]
["2,4,4,5,7,7,8,10,10,11,13,13,14,14,15,15,15-Heptadecafluoro-2,5,8,11-tetrakis(trifluoromethyl)-3,6,9,12-tetraoxapentadecan-1-ol","141977-66-4","D",0]
["4,4,4-trifluoro-1-(4-fluorophenyl)-3-hydroxy-2-methyl-3-(trifluoromethyl)butan-1-one","34844-25-2","D",0]
["Methyl 3-(1,1,2,2,3,3,3-heptafluoropropane-1-sulfonyl)benzoate","88489-68-3","D",0]
["Methyl 3-amino-4,4,5,5,5-pentafluoropent-2-enoate","87613-27-2","D",0]
["But-2-en-1-yl 2-fluoro-3-methyl-2-(trifluoromethyl)pent-4-enoate","88071-32-3","D",0]
["4-Bromo-3-(heptafluoropropyl)-5-phenyl-1H-pyrazole","82633-52-1","D",0]
["Methyl 4,4,5,5-tetrafluoro-3-hydroxy-3-methoxypentanoate","89129-77-1","D",0]
["1,1,1,2,2-Pentafluoro-2-nitrosoethane","354-72-3","D",0]
["N-(Carboxylatomethyl)-3-[[2-[(perfluorohexyl)ethylthio]acetyl] amino]-N,N-dimethyl-1-propanaminium","1513863-95-0","D",0]
["4-Methylphenyl pentafluoropropanoate","24271-52-1","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-(pentafluoroethoxy)propanoate","117516-09-3","D",0]
["2-Ethyl-3-(ethylsulfanyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355554-66-3","D",0]
["Poly[oxy(1,1,2,2,3,3-hexafluoro-1,3-propanediyl)], α-(1,1,2,2,3,3,3-heptafluoropropyl)-ω-[1,1,2,2-tetrafluoro-3-(2-propen-1-yloxy)propoxy]-","851085-64-8","D",0]
["2,2-Bis(difluoromethyl)-1,1,3,3,4,4-hexafluorobutane","95576-24-2","D",0]
["Trifluoroethanethioyl fluoride","754-13-2","D",0]
["1,2,2,3,3,4,4,5,5,6,6-Undecafluoro-N,N-bis(pentafluoroethyl)cyclohexan-1-amine","308-95-2","D",0]
["2,2,3-Trifluoro-3-(nonafluorobutyl)oxirane","72804-48-9","D",0]
["1,1,2,2,3,3-Hexafluoro-1-iodobutane","61951-28-8","D",0]
["4-[(2,2,3,3-Tetrafluoropropyl)sulfanyl]phenol","90314-94-6","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl trifluoroacrylate","424-65-7","D",0]
["Ethyl 2,4,4,5,7,7,8,10,10,11,13,13,14,16,16,17,19,19,20,20,21,21,21-tricosafluoro-2,5,8,11,14,17-hexakis(trifluoromethyl)-3,6,9,12,15,18-hexaoxahenicosan-1-oate","121368-60-3","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononan-2-ol","80363-03-7","D",0]
["(Perfluoropropyl)-2-(2-phenylhydrazinylidene)ethanal phenylhydrazone","57912-15-9","D",0]
["Methanesulfonic acid--2,2,3,3-tetrafluoropropan-1-ol (1/1)","85459-30-9","D",0]
["Undecafluoro(trifluoromethoxy)cyclohexane","4943-06-0","D",0]
["2-{[(6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Heptadecafluoro-2,2-dimethyltridecan-3-yl)oxy]carbonyl}hydrazine-1-carboxylate","821806-56-8","D",0]
["1,1-Diethoxy-3,5,5,5-tetrafluoro-4-(trifluoromethyl)penta-1,3-diene","62116-51-2","D",0]
["Heptanamide, 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","540521-18-4","D",0]
["AC1MJ33P","52260-98-7","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(2-methylpropane-1-sulfonyl)benzoic acid","1355554-54-9","D",0]
["Methyl 4,4,4-trifluoro-3,3-bis(trifluoromethyl)butanoate","65907-99-5","D",0]
["1-(3,5-dimethylphenyl)-2,2,3,3,3-pentafluoropropan-1-one","1352216-62-6","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester, telomer with 1-dodecanethiol and octadecyl 2-propenoate","1259487-19-8","D",0]
["2,2'-(2,2,3,3,4,4,4-Heptafluorobutane-1,1-diyl)di(1H-pyrrole)","164792-01-2","D",0]
["S-Deoxo-3,17alpha-bis-(O-tetrahydro-2H-pyran-2-yl)-6-oxo-fulvestrant","862700-70-7","D",0]
["2,6-Difluoro-N-(((2-fluoro-4-((1,1,2,2-tetrafluoroethyl)thio)phenyl)amino)carbonyl)benzamide","100278-94-2","D",0]
["Pentanoic acid, 2-propyl-, 1,1'-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro-1,10-decanediyl) ester","544446-07-3","D",0]
["Diethyl (nonafluorobutyl)phosphonate","81509-47-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoroheptacosane","250738-44-4","D",0]
["5-Bromo-2-(1,1,2,2-tetrafluoroethoxy)phenol","89227-93-0","D",0]
["5-Trifluoromethylperfluoro-3,6-dioxanonane","66804-94-2","D",0]
["Bis(heptafluoropropyl)(phenyl)phosphane","20608-39-3","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(hydroxymethyl)-, sodium salt","100294-72-2","D",0]
["2-(Perfluoro-7-methyloctyl)ethyl iodide","40678-31-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(4-methylpiperazin-1-yl)butan-1-one","499975-92-7","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl diphenylphosphinate","55776-72-2","D",0]
["2-Octen-1-aminium, 3,4,4,5,5,6,6,7,7,8,8,8-dodecafluoro-N-(2-hydroxyethyl)-N-methyl-N-(3-sulfopropyl)-","84070-70-2","D",0]
["3,4-Bis[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]cyclobut-3-ene-1,2-dione","61699-82-9","D",0]
["3-(Heptadecafluorooctyl)-1,2,4,5-tetramethylbenzene","80790-96-1","D",0]
["Perfluorodocosanoic acid","2153498-16-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N'-[(pyridin-4-yl)methylidene]butanehydrazide","109373-81-1","D",0]
["3,3,4,4-Tetrafluoro-2-butanol","17425-25-1","D",0]
["Bis(3,3,4,4,5,5,6,6,6-nonafluoro-1-hexanol) hydrogen phosphate","135098-69-0","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(2-methylpropane-1-sulfinyl)benzoic acid","1355554-32-3","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, reaction products with bromine","161075-11-2","D",0]
["Diethyl 4,4,5,5,6,6-hexafluoro-3,7-dioxo-2,8-bis(triphenyl-lambda5-phosphanylidene)nonanedioate","60521-76-8","D",0]
["1,1,1,2,2,3,3,4,4,5,6,7,7,7-Tetradecafluoroheptane","142347-10-2","D",0]
["Chlorodipropyl(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","608296-13-5","D",0]
["4H-1,3,2-Dithiazine, 4,4,5,5,6,6-hexafluorodihydro-, 1,1,3,3-tetraoxide, lithium salt (1:1)","189217-62-7","D",0]
["Imidazolidine, 2-pentafluoroethyl-","28462-90-0","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl hypochlorite","27579-40-4","D",0]
["Lithium perfluoro{[1-(1,2-dichloro-1,2,2-trifluoroethoxy)-1-fluoropropan-2-yl]oxy}acetate","1383434-29-4","D",0]
["HFE-356pcf3","35042-99-0","D",0]
["(4E)-1,1,1,2,2,3,3,6,6,7,7,8,8,8-Tetradecafluorooct-4-ene","35709-14-9","D",0]
["1-(Perfluoropropanyl)-1-fluoro-3-(perfluoroethyl)prop-1-ene","343627-68-9","D",0]
["N,N-Bis(2,3-dihydroxypropyl)-perfluoro-1-hexanesulfonamide","118675-71-1","D",0]
["1,1,2,2,3,3,4,4,5,7,7,7-Dodecafluoroheptyl prop-2-enoate","51855-39-1","D",0]
["N-[(Perfluorobutyl)sulfonyl]-N-propylglycine","864069-46-5","D",0]
["2,2,3,3,4,4,5-Heptafluoro-5-(undecafluoropentyl)oxolane","374-91-4","D",0]
["1-Chloro-6-iodoperfluorohexane","16486-97-8","D",0]
["5-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutane-1-sulfonyl)-4-(4-methoxyphenyl)-2-(2-methylpropoxy)-6-phenyl-3,4-dihydro-2H-pyran","905560-37-4","D",0]
["2-Methylpropyl ethyl(heptafluoropropyl)phosphinate","77529-59-0","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl 2-methylbutanoate","914637-47-1","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide","162492-17-3","D",0]
["4-(1,1,1,3,3,3-Hexafluoropropan-2-yloxy)-2,2,6,6,7,7-hexakis(trifluoromethyl)-1,5,8-trioxa-3-aza-4lambda5-phosphaspiro[3.4]octane","7234-86-8","D",0]
["Octafluorobutane-2,2-diol","108686-05-1","D",0]
["1H,1H,2H,2H-Perfluorotetradecyltrichlorosilane","102488-50-6","D",0]
["2-(Pentadecafluoroheptyl)cyclohexan-1-one","56734-77-1","D",0]
["1,1,1,2,2,3,3,4,4,6,6,8,8-Tridecafluoro-10-iododecane","272451-64-6","D",0]
["N-(2-Hydroxyethyl)-3-[(2-hydroxyethyl)[(perfluorobutyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","2089108-99-4","D",0]
["N,N,N-Triethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-heptadecafluorodecan-1-aminium chloride","144094-08-6","D",0]
["2-[Bromo(chloro)methyl]-1,1,1,3,3,3-hexafluoropropane","885276-24-4","D",0]
["Chloro(3,3,4,4,4-pentafluorobutyl)propyl(3,3,3-trifluoropropyl)silane","608296-34-0","D",0]
["2,2,3,3,4,4-Hexafluoro-5-hydroxypentyl 4-methylbenzene-1-sulfonate","2728-37-2","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(propylsulfanyl)benzoic acid","1355554-03-8","D",0]
["Poly(oxy-1,2-ethanediyl), α-hydro-ω-hydroxy-, ether with 1-[(2-hydroxyethyl)octylamino]-3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]-2-propanol (2:1)","1874268-13-9","D",0]
["6-Bromo-2,2,4,4-tetrafluoro-1,3-benzodioxane","261762-36-1","D",0]
["3,3,4,4-Tetrafluorocyclopent-1-ene","5239-56-5","D",0]
["Perfluoroethoxypropyl carboxylic acid","919005-54-2","D",0]
["Perfluoro-2-methylindane","56594-70-8","D",0]
["(Perfluoroheptanoyl)acetone","82822-26-2","D",0]
["{Ethyl[(perfluoropropyl)sulfonyl]amino}acetic acid","1003194-08-8","D",0]
["S-[3-(Trimethoxysilyl)propyl] heptadecafluorononanethioate","138111-73-6","D",0]
["1,1,2,2,3,3,4,4,5,7,7,7-Dodecafluoroheptyl 2-methylprop-2-enoate","61253-02-9","D",0]
["34,34,35,35,36,36,37,37,38,38,39,39-Dodecafluoro-4,8,12,16,20,24,28,32-octaoxanonatriacontane-1,2,6,10,14,18,22,26,30-nonol","62240-24-8","D",0]
["Trimethyl(2,2,3,3,3-pentafluoropropoxy)silane","89660-59-3","D",0]
["Bromotris(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","201740-57-0","D",0]
["1,1,1,3,3,3-Hexafluoro-N-methylpropan-2-imine","1619-96-1","D",0]
["3-[(Butan-2-yl)sulfanyl]-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-14-1","D",0]
["4'-Nitro-4,4,4-trifluoro-3-(trifluoromethyl)crotonophenone","35443-90-4","D",0]
["2,2,3,3,4,4-Hexafluoro-4-(nonafluorobutoxy)butanoic acid","174767-06-7","D",0]
["Hexafluoropropene, oligomeric reaction products with 1,1-difluoroethylene and tetrafluoro-ethylene, telomers with trifluoromethyl hypofluorite","161278-45-1","D",0]
["2-Fluoro-4-(nonafluorobutyl)aniline","821791-47-3","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-7-(trifluoromethoxy)heptane","1737-33-3","D",0]
["2,4-HEXANEDIOL, 5,5-DIMETHYL-1,1,1-TRIFL","34844-46-7","D",0]
["5,6,6,6-Tetrafluoro-4-oxo-5-(trifluoromethyl)hexanoic acid","62656-74-0","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-phenylheptan-1-one","78960-66-4","D",0]
["1,1,1,2-Tetrafluoro-2-(2,2,2-trifluoroethoxy)ethane","55605-86-2","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-phenyl-2-hexen-1-one","110960-47-9","D",0]
["1-[Chloro(fluoro)methoxy]-1,1,2,3,3,3-hexafluoropropane","56860-86-7","D",0]
["2-[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy]oxane","115347-48-3","D",0]
["2,2,4,4,6,6,8-Heptamethyl-8-[3-(2,2,3,3-tetrafluoropropoxy)propyl]-1,3,5,7,2,4,6,8-tetroxatetrasilocane","111731-15-8","D",0]
["8-(Pentafluorosulfanyl)perfluorooctyl sulfonic acid","2089109-34-0","D",0]
["Tris(heptafluoropropyl)phosphane","51761-69-4","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluoro-2-hydroxydecanenitrile","90278-37-8","D",0]
["(1,2,2,2-Tetrafluoroethyl)dioxidanyl","134469-97-9","D",0]
["2-{[(Pentafluoroethyl)sulfanyl]methyl}pyrrolidine","1274892-03-3","D",0]
["Perfluoro-1-decanol","85758-71-0","D",0]
["Perfluoro-3,6-dioxaoctane-1,8-dioic acid","55621-21-1","D",0]
["Nonafluorobutyl prop-2-enoate","2708-03-4","D",0]
["Tris(2-methylpropyl) 3-(2,2,3,3,4,4,4-heptafluorobutanamido)propane-1,1,3-tricarboxylate","95654-14-1","D",0]
["2-Propenoic acid, 2-methyl-, 3-(triethoxysilyl)propyl ester, polymer with ethenylbenzene, 2-[ethyl[(heptadecafluorooctyl)sulfonyl]amino]ethyl 2-propenoate and 2-hydroxyethyl 2-propenoate","68541-79-7","D",0]
["1,3,3,4,4,5,5,6,6-Nonafluoro-2-(fluoromethyl)cyclohex-1-ene","111180-52-0","D",0]
["N,N'-(5-{[1,1,1,4,5,5,5-Heptafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-4-(trifluoromethyl)pent-2-en-2-yl]oxy}-1,3-phenylene)diacetamide","150225-65-3","D",0]
["5-Bromo-1,1,2,2-tetrafluoro-2,3-dihydro-1H-indene","922141-53-5","D",0]
["2-(Perfluorobutanyl)oct-2-ene","113999-55-6","D",0]
["1,1'-(1,3-dimethylbutylidene)bis[4-(1,1,2,2-tetrafluoroethoxy)benzene","163036-60-0","D",0]
["Calcium (3E)-6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-5-oxooct-3-en-3-olate (3Z)-6,6,7,7,8,8,8-heptafluoro-2,2-dimethyl-5-oxooct-3-en-3-olate (1/1/1)","124053-49-2","D",0]
["Trichloro(1,1,1,2,3,3-hexafluoropropan-2-yl)silane","60002-07-5","D",0]
["3,3,4,4,4-Pentafluoro-2-(trifluoromethyl)-1-butene","189154-79-8","D",0]
["Docosafluorobicyclohexyl","558-64-5","D",0]
["3-[(1,1,1,3,3,3-Hexafluoropropan-2-yl)sulfanyl]cyclohex-1-ene","67263-11-0","D",0]
["N,N-Bis(2,3-dihydroxypropyl)-perfluorononanamide","118675-73-3","D",0]
["2,3,3,4,4,4-Hexafluoro-2-(pentafluoroethyl)butanoyl fluoride","61340-75-8","D",0]
["2,2'-Oxybis[4,4-bis(trifluoromethyl)thietane]","62378-47-6","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-methoxyethyl)butanamide","70473-74-4","D",0]
["N-(2-Chlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","121806-65-3","D",0]
["1,4-dichloro-2-(1,1,2,3,3,3-hexafluoropropoxy)-benzene","1026364-35-1","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoro-2-hepten-1-ol","72016-05-8","D",0]
["3-(Heptafluoropropyl)-5-methyl-4-nitro-1H-pyrazole","82633-69-0","D",0]
["(17β)-3-[(Trimethylsilyl)oxy]estra-1,3,5(10)-trien-17-ol perfluorobutanoate","120623-45-2","D",0]
["1,1,1,2,2,3,3-Heptafluoropropane 1,2,3,4,5-pentamethylcyclopentane rhodium trimethylphosphanium","7223-98-5","D",0]
["3,5,6-trichloro-2,2,3,4,4,5,6,6-octafluorohexanoic acid- 1-phenylpiperazine(1:1)","1511-42-8","D",0]
["1-Butene, 1,1-bis(ethylthio)-2,3,3,4,4,4-hexafluoro-","145327-77-1","D",0]
["(4E)-1-(4,4-Dimethyl-3-oxopent-1-enyl)perfluorobutane","105602-69-5","D",0]
["Perfluoro-2-hexene","1584-00-5","D",0]
["4,4,5,5,6,6,7,7,8,8,8-Undecafluorooctan-1-ol","1404193-88-9","D",0]
["N-Ethyl-2,3,3,4,4,4-hexafluoro-2-(trifluoromethyl)butanamide","111736-89-1","D",0]
["Pentafluoropropanoic acid--1-phenylpiperazine (1/1)","893-87-8","D",0]
["(Z)-4-Ethyl-5-octyl-2,2-bis(trifluoromethyl)-1,3-dioxolane","38274-72-5","D",0]
["1,4-bis(1,1,2,2-tetrafluoroethoxy)benzene","3832-65-3","D",0]
["1,2,2,3,3-Pentafluorocyclopropane-1-carboxylic acid","917951-65-6","D",0]
["(Tridecafluorohexyl)benzene","65440-93-9","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(methanesulfonyl)benzoic acid","1355555-09-7","D",0]
["2-(Pentafluoroethyl)-1,3-oxazolidine","31185-59-8","D",0]
["1-Chlorononafluorobutane","558-89-4","D",0]
["2,2,4,4,6,6-Hexakis(2,2,3,3,3-pentafluoropropoxy)-1,3,5,2lambda~5~,4lambda~5~,6lambda~5~-triazatriphosphinine","429-18-5","D",0]
["1,1,1,2,2,3,3-Heptafluoroheptan-4-one","425-22-9","D",0]
["2-Chloro-N-[3-[[[2,6-dimethyl-4-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]phenyl]amino]carbonyl]-2-fluorophenyl]-N-methyl-3-pyridinecarboxamide","862134-31-4","D",0]
["1-benzyl-2,3-difluoro-2,3-bis(trifluoromethyl)aziridine","5321-09-5","D",0]
["2-Propenoic acid, 1,1-dimethylethyl ester, polymer with 4,5-difluoro-2,2-bis(trifluoromethyl)-1,3-dioxole and tetrafluoroethene","851389-08-7","D",0]
["5-Benzyl-4-methyl-2,2-bis(trifluoromethyl)-1,3-oxazolidine","101834-51-9","D",0]
["(R*,S*)-1,1,2,3,4,4-Hexafluoro-1,2,3,4-tetrakis(heptafluoropropoxy)butane","54572-17-7","D",0]
["4,4'-[(3,3,4,4,5,5-Hexafluoro-1-cyclopentene-1,2-diyl)bis(5-methyl-4,2-thienediyl)]dibenzaldehyde","348639-12-3","D",0]
["Perfluorohexyl phosphonic acid","40143-76-8","D",0]
["Perfluoro-2-[(perfluoropentyl)oxy]propanoic acid","504435-11-4","D",0]
["3,3,4,4-Tetrafluoro-1-butanol","5926-87-4","D",0]
["naphthalen-2-yl 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","42096-34-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-N'-[(4-methylphenyl)methylidene]heptanehydrazide","445258-02-6","D",0]
["1,1,2,2,3,3-Hexafluoro-1,3-dinitrosopropane","137541-04-9","D",0]
["Cyclohexyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","145510-90-3","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorohexanamide","153339-14-1","D",0]
["Perfluoro-3-oxanonane-1-sulfonyl fluoride","67990-80-1","D",0]
["2-(2-Amino-4-methylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","1992-08-1","D",0]
["Ethyl (1R,3R)-3-(diethoxymethyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylate","99903-44-3","D",0]
["1-Chloro-1-[chloro(difluoro)methoxy]-1,2,2,2-tetrafluoroethane","233258-11-2","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecanal","42028-44-4","D",0]
["1,1,2,3,3,3-hexafluoropropoxybenzene","357-98-2","D",0]
["2H-1,3-Thiazete, 4-(4-chlorophenyl)-2,2-bis(trifluoromethyl)-","57014-98-9","D",0]
["4-[(2,2,3,3,3-Pentafluoropropyl)sulfanyl]benzene-1,2-diamine","54029-85-5","D",0]
["11:2 Fluorotelomer sulfonic acid","1034143-66-2","D",0]
["2-(4-tert-butylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","22796-15-2","D",0]
["1-[Di(propan-2-yl)amino]-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-2-ol","125672-20-0","D",0]
["2-(1,1,2,2-tetrafluoroethoxy)aniline","35295-34-2","D",0]
["Sodium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","67963-75-1","D",0]
["4-Bromo-1,2,3,3,4,5,5,6,6-nonafluorocyclohex-1-ene","57113-75-4","D",0]
["N-(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)-N-(prop-2-en-1-yl)prop-2-enamide","139890-38-3","D",0]
["Perfluoromethoxypropionic acid methyl ester","356-69-4","D",0]
["1-(Hydroxymethyl)-2-[(perfluorohexyl)ethoxy]ethyl 2-propenoate","147187-54-0","D",0]
["Fulvestrant 3-Sulfate Sodium Salt","403656-83-7","D",0]
["Sodium perfluoropentanesulfinate","1997344-07-6","D",0]
["(2,6-Dinitrophenyl)methyl tridecafluoroheptanoate","143662-85-5","D",0]
["5H-Perfluoropentanal","2648-47-7","D",0]
["4,4,4-Trifluoro-2-octyl-1-phenyl-3-(trifluoromethyl)butane-1,3-diol","34848-29-8","D",0]
["5,5,6,6,6-Pentafluoro-4-methylhexan-3-one","56734-79-3","D",0]
["2-chloro-3,4,4,5,5,5-hexafluoro-3-(trifluoromethyl)pent-1-ene","261503-66-6","D",0]
["(Perfluorohexadecyl)hexadecene","1244062-14-3","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxin-5-amine","119895-70-4","D",0]
["Methyl 4,4,5,5,5-pentafluoropent-2-ynoate","104721-32-6","D",0]
["(10H-Perfluorodecyl)methanol phosphate ammonium salt (2:1)","100738-12-3","D",0]
["2,2-DIFLUORO-2-[1,1,2,2-TETRAFLUORO-2-[1,1,2,2-TETRAFLUORO-2-(TRIFLUOROMETHOXY)ETHOXY]ETHOXY]ETHANOL","147492-57-7","D",0]
["Perfluoropentane sulfonic anhydride","161877-72-1","D",0]
["Pentafluoroethanesulfonate","108410-37-3","D",0]
["[(1,1,2,2-Tetrafluoroethyl)sulfanyl]benzene","403-58-7","D",0]
["4:4 Fluorotelomer sulfonate potassium salt","1604816-60-5","D",0]
["3-[[(Perfluorononyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","736879-74-6","D",0]
["N-(2-Carboxyethyl)-3-[(2-carboxyethyl)[(perfluoropentyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","1383438-84-3","D",0]
["3H,3H-Perfluoro-2,4-hexanedione","20825-07-4","D",0]
["1-Butanesulfonamide, 1,1,2,2,3,3,4,4,4-nonafluoro-N-hexyl-","606966-46-5","D",0]
["4,5-Dichloro-1,1,2,3,3,4,5,5-octafluoropent-1-ene","647-71-2","D",0]
["4-(1,1,2,2,2-Pentafluoroethyl)-Benzenesulfonamide","2044712-67-4","D",0]
["5H,5H-Perfluoro-4,6-nonanedione","113116-18-0","D",0]
["2,2,3,3,3-Pentafluoropropyl 2,2,3,3-tetrafluoropropyl carbonate","1227308-85-1","D",0]
["2-bromo-3,3,4,4,5,5,5-heptafluoropent-1-ene","96916-53-9","D",0]
["Methyl perfluoropentadecanoate","203303-00-8","D",0]
["3-(2-Methylprop-1-en-1-yl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylic acid","99903-46-5","D",0]
["1-Bromo-1,1,3-trichloro-2,2,3,3-tetrafluoropropane","111393-40-9","D",0]
["1-(2,5-Difluorophenyl)-4,4,5,5,5-pentafluoropentane-1,3-dione","64287-16-7","D",0]
["4,5,5,5-Tetrafluoro-2-iodo-4-(trifluoromethyl)-2-penten-1-ol","261760-25-2","D",0]
["1-bromo-1,1,2,2-tetrafluorooctane","231630-92-5","D",0]
["N-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)cyclopent-2-ene-1-carboxamide","1440968-24-0","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluorodecyl prop-2-enoate","451456-30-7","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-3-(methanesulfinyl)-2-methylbenzoic acid","1355554-19-6","D",0]
["2-(1,1,2,2-Tetrafluoroethoxy)benzoic acid","10008-97-6","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Hexadecafluorooctanol phosphate disodium salt","60131-28-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-9-methyldecane","212957-55-6","D",0]
["1,1,2-Trifluoro-2-(trifluoromethyl)cyclobutane","49852-57-5","D",0]
["4H-Pyran-4-one, 6-(heptafluoropropyl)-2,3-dihydro-3-hydroxy-3-methyl-","62321-81-7","D",0]
["Ethenyl 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoate","45271-27-0","D",0]
["4,5,5,5-Tetrafluoro-3-phenylpent-3-en-2-one","61282-84-6","D",0]
["1,2,2,3,3,4,4,5-Octafluoropentan-1-ol","1513-96-8","D",0]
["(3,3,4,4,5,5,5-Heptafluoropentyl)(trimethoxy)silane","109134-39-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6-Dodecafluorononane","126038-58-2","D",0]
["3-[[(Perfluorodecyl)sulfonyl]amino]-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","142519-26-4","D",0]
["2-Nitro-1,3,5-tris(pentafluoroethoxy)benzene","52999-51-6","D",0]
["3-[1,1,2-Trifluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)ethoxy]propanoic acid","919005-34-8","D",0]
["3-(2-Chloro-1,1,2-trifluoroethoxy)-1,1,2,2-tetrafluoropropane","65064-83-7","D",0]
["3-(Heptafluoropropyl)-5-methyl-1H-pyrazole","75823-64-2","D",0]
["2,2,3,3-Tetrafluoropropyl 5-[(2-methylphenyl)amino]-5-oxopentanoate","5586-55-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-Tricosafluoro-13-iodotridecane","57216-88-3","D",0]
["5,5,6,6,7,7,8,8,8-Nonafluoro-2-methyloctan-2-ol","269394-08-3","D",0]
["3-Phenyl-2,2-bis(trifluoromethyl)-1,3-oxazolidin-5-one","57750-02-4","D",0]
["Sodium 3-[ethyl[(perfluorobutyl)sulfonyl]amino]-2-hydroxy-1-propanesulfonate","864069-39-6","D",0]
["4-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]phenol","892155-14-5","D",0]
["3-Methoxy-3-pentyl-5,5-bis(trifluoromethyl)-1,2-dithiolane","62378-55-6","D",0]
["Sodium bis(perfluorohexyl)phosphinate","70609-44-8","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-2,2-dimethyloctanal","56734-80-6","D",0]
["N-(2-Carboxyethyl)-3-{ethyl[(undecafluoropentyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","2089109-91-9","D",0]
["2-[2-[2-(2-Hydroxyethoxy)ethoxy]ethoxy]ethyl 3,4,5-tris(1,1,2,3,3,3-hexafluoropropoxy)benzoate","75860-12-7","D",0]
["1h,1h-perfluoro-3,6-dioxadecan-1-ol","152914-73-3","D",0]
["2,2,3,3,3-pentafluoro-N-naphthalen-1-ylpropanamide","21970-67-2","D",0]
["4-Nitrophenyl heptafluorobutanoate","1799-92-4","D",0]
["4,4,5,5,5-Pentafluoropent-1-en-3-one","65609-43-0","D",0]
["Ammonium perfluoro-2-{[1-(1,2-dichloro-1,2,2-trifluoroethoxy)propan-2-yl]oxy}ethane-1-sulfonate","1383434-25-0","D",0]
["Propanamide, 2,2,3,3,3-pentafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","882828-36-6","D",0]
["3-Trifluoromethyl-1H,1H,5H-perfluoro-1-hexanol","402592-21-6","D",0]
["2(3H)-Furanone, 5-(5-chloro-2,2,3,3,4,4,5,5-octafluoropentyl)dihydro-","462655-91-0","D",0]
["N-(2,4-Dichlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","121806-66-4","D",0]
["4-Nitrophenyl 3,3,4,4-tetrafluoropyrrolidine-1-carboxylate","920966-49-0","D",0]
["3-[(Perfluorooctanesulfonyl)amino]propane-1-sulfonic acid","153946-37-3","D",0]
["Ethyl N-(2,2,3,3,4,4,4-heptafluorobutanoyl)glycinate","88435-34-1","D",0]
["N-(2-Hydroxyethyl)-3-[(2-hydroxyethyl)[(perfluorohexyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","2089109-01-1","D",0]
["Heptanamide, N,N-diethyl-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoro-","60895-94-5","D",0]
["N-[4-(Pentafluoroethoxy)phenyl]pyridine-3-carboxamide","62315-08-6","D",0]
["N,N-Dimethyl-4-(tridecafluorohexyl)aniline","141822-33-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-iodododecane","120695-82-1","D",0]
["Chloro(dimethyl)[4,4,4-trifluoro-3,3-bis(trifluoromethyl)butyl]silane","62281-42-9","D",0]
["Benzamide, 4-[[4-[[[2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propylamino]ethyl]amino]carbonyl]phenyl]methyl]-N-octadecyl-","73019-19-9","D",0]
["[[(2,2,3,3-Tetrafluoropropyl)thio]methyl]-Benzene","205521-85-3","D",0]
["1,1,1,3,5,5,5-Heptamethyl-3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)trisiloxane","136772-44-6","D",0]
["Sodium 1,1,1,3,3,3-hexafluoro-2-phenylpropan-2-ol","67696-26-8","D",0]
["2-Ethyl-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctanal (2,4-dinitrophenyl)hydrazone","136022-83-8","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctan-2-one","80793-21-1","D",0]
["(1S,2S)-1,2-Dichloro-1,2,3,3,4,4-hexafluorocyclobutane","3832-15-3","D",0]
["2-(Heptafluoropropyl)-1-phenyl-4,5-dihydro-1H-imidazole","1069085-53-5","D",0]
["6-(Nonafluorobutyl)-2-sulfanylidene-2,3-dihydropyrimidin-4(1H)-one","1426894-99-6","D",0]
["1,1,1,3,3-Pentafluoro-3-(fluoromethoxy)-2-(trifluoromethyl)propane","16507-58-7","D",0]
["N-(3-Chlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","106376-36-7","D",0]
["4,4,4-Trifluoro-2-methyl-1-(thiophen-2-yl)-3-(trifluoromethyl)butane-1,3-diol","34848-41-4","D",0]
["2-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)heptanal","34844-09-2","D",0]
["1,1,1,2,2-Pentafluoro-7-phenylheptan-3-one","1071000-98-0","D",0]
["1,1,2,2-Tetrafluoro-3-[(propan-2-yl)oxy]propane","88998-57-6","D",0]
["Tecarfarin","867257-26-9","D",0]
["4-[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propane-2-sulfonyl]benzoic acid","88489-84-3","D",0]
["1,1,1,2,5,5,6,6,6-Nonafluoro-3,4-bis(trifluoromethyl)hex-2-ene","90907-34-9","D",0]
["(2E)-4,4,5,5,6,6,6-Heptafluoro-2-iodo-2-hexen-1-ol","92835-82-0","D",0]
["N-Decyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctanamide","89685-58-5","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, compd. with N,N-diethylethanamine (1:1)","182059-38-7","D",0]
["4,4-Difluoro-1-(thiophen-2-yl)-4-(trifluoromethoxy)butane-1,3-dione","56286-63-6","D",0]
["Perfluoroethoxypropionyl fluoride","377-75-3","D",0]
["1-(Perfluoropropanyl)-2-(perfluoropentanyl)ethene","935477-16-0","D",0]
["2-Chloro-3,3,4,4,5,5,6,6-octafluorocyclohex-1-ene-1-carbonitrile","84439-72-5","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-iodohexadecane","1789721-11-4","D",0]
["4-(2-Carboxy-1,1,2,2-tetrafluoroethoxy)-perfluoropentanoic acid","2416366-22-6","D",0]
["5,6,6,6-Tetrafluoro-5-(heptafluoropropoxy)hexane-2,4-dione","261760-03-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorodotriacontane","89109-72-8","D",0]
["1,2,3,4-Tetrafluoro-5-(pentafluoroethyl)-6-(trifluoromethyl)benzene","111864-94-9","D",0]
["1-Butanesulfonamide, 1,1,2,2,3,3,4,4,4-nonafluoro-N-[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]-, potassium salt (1:1)","129135-87-1","D",0]
["Methyl 5-chloro-2,2,3,3,4,4-hexafluoro-5-oxopentanoate","21543-95-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,9,9,9-hexadecafluoro-8-(trifluoromethyl)nonanoic acid","15899-32-8","D",0]
["3,5,7,8-Tetrachloro-2,2,3,4,4,5,6,6,7,8,8-undecafluorooctanoic acid--1-phenylpiperazine (1/1)","4627-64-9","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Pentadecafluorodec-2-enoic acid","755-03-3","D",0]
["2-(1,1,2,2-tetrafluoroethyl)-1H-benzimidazole","61532-00-1","D",0]
["1-(4-Ethoxyphenyl)-2,2,3,3-tetrafluorocyclobutane-1-carbonyl chloride","91627-21-3","D",0]
["N,N,N-Tripropylpentan-1-aminium nonafluorobutane-1-sulfonate","56773-55-8","D",0]
["N-[3-(Trimethoxysilyl)propyl]perfluorononanamide","102116-03-0","D",0]
["4,4,4-Trifluoro-2-pentyl-3-(trifluoromethyl)butane-1,3-diol","34844-47-8","D",0]
["(1E)-1-Ethoxy-4,4,5,5,6,6,6-heptafluorohex-1-en-3-one","170118-61-3","D",0]
["2-[(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptyl)oxy]ethan-1-ol","54336-60-6","D",0]
["Methyl 2,2,3,3-tetrafluoro-3-phenoxypropanoate","91312-77-5","D",0]
["Dimethyl (1,1,1,3,3,3-hexafluoropropan-2-yl)phosphonate","758-49-6","D",0]
["Perfluoropropyl acetate","1344118-10-0","D",0]
["1,1,1,4,5,6,6,6-Octafluoro-2,3,4,5-tetrakis(trifluoromethyl)hex-2-ene","98260-14-1","D",0]
["1,1,1,2,2,5-Hexafluoropentan-3-one","370862-40-1","D",0]
["2,3,4,5,8-Pentafluoro-8-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)bicyclo[4.2.0]octa-1,3,5-trien-7-one","1419865-30-7","D",0]
["1,1,1,2,2,3,3,11,11,12,12,13,13,13-Tetradecafluoro-5,9-diiodotridecane","1644-06-0","D",0]
["Phenyl 2,3,3,3-tetrafluoro-2-phenoxypropanoate","10249-10-2","D",0]
["1,12-Dodecanediol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-eicosafluoro-","183162-43-8","D",0]
["2,2,3,3-Tetrafluoro-3-{[1,1,1,2,3,3-hexafluoro-3-(1,2,2,2-tetrafluoroethoxy)propan-2-yl]oxy}propanoic acid","773804-62-9","D",0]
["2-(2-Chloro-1,1,2-trifluoro-2-iodoethoxy)-1,1,1,2,3,3,3-heptafluoropropane","16031-04-2","D",0]
["Perfluoroethyl formate","313064-40-3","D",0]
["2-ethyl-4,4,4-trifluoro-1-(4-fluorophenyl)-3-hydroxy-3-(trifluoromethyl)butan-1-one","34844-26-3","D",0]
["N-Butyl-2,2,3,3,4,4,5,5,5-nonafluoropentanamide","73602-44-5","D",0]
["1,5-dibromo-2,2,3,3,4,4-hexafluoropentane","33619-78-2","D",0]
["Bis(pentafluoroethyl)phosphinous chloride","35449-89-9","D",0]
["4-[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propane-2-sulfonyl]aniline","68596-43-0","D",0]
["8-Bromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluorooctane","142494-31-3","D",0]
["2-(2,2,3,3,4,4,4-Heptafluorobutanoyl)cyclopentan-1-one","141478-83-3","D",0]
["1,1,3,4-Tetrachloro-1,2,2,3,4,4-hexafluorobutane","423-38-1","D",0]
["Propane, 1,1-dichloro-1,2,2,3,3-pentafluoro-","13474-88-9","D",0]
["1-(1,2-Difluoroethenyl)perfluorobutane","66249-21-6","D",0]
["2,2,3,3,3-Pentafluoro-1-(pyrrolidin-2-yl)propan-1-one","742038-20-6","D",0]
["3-Bromo-1,1,2,2-tetrafluoropropane","679-84-5","D",0]
["Tris(4-(Heptadecafluorooctyl)Phenyl)-Phosphine","284472-92-0","D",0]
["Trimethoxy(undecafluoropentyl)silane","84464-04-0","D",0]
["N-(Carboxylatomethyl)-3-[hexyl[(perfluorohexyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","83409-36-3","D",0]
["Ethyl 5,5,6,6,7,7,8,8,8-nonafluorooctane-1-sulfonate","1604816-68-3","D",0]
["Potassium perfluorohexanoate","3109-94-2","D",0]
["Cyclohexane, (ethenyloxy)-, polymer with 4-(ethenyloxy)-1-butanol and tetrafluoroethene","121465-74-5","D",0]
["Perfluorocyclohexanecarboxylic acid","374-88-9","D",0]
["7-(Pentafluorosulfanyl)perfluoroheptyl sulfonic acid","2089109-33-9","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α,α′,α′′-[phosphinidynetris[oxy[1-fluoro-1-(trifluoromethyl)-2,1-ethanediyl]]]tris[ω-(1,1,2,2,3,3,3-heptafluoropropoxy)-","2247153-51-9","D",0]
["Methoxydimethyl(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)silane","608299-08-7","D",0]
["1-[3-(1,1,2,2-Tetrafluoroethoxy)phenyl]propan-1-one","1443342-53-7","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-5-[(prop-2-en-1-yl)oxy]pentane","646063-05-0","D",0]
["3,3,4,4,4-Pentafluoro-2-methylbutan-2-ol","374-46-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorotricosane","677324-31-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(10H-phenothiazin-10-yl)butan-1-one","100234-24-0","D",0]
["1,2,2,2-Tetrafluoroethane-1-sulfonic acid--pyridine (1/1)","91145-99-2","D",0]
["Dodecanal, 5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heptadecafluoro-","88628-84-6","D",0]
["N-[1,1,1,3,3,3-Hexafluoro-2-(4-fluorophenyl)propan-2-yl]benzamide","188754-82-7","D",0]
["Carbamic acid, (1-(diphenylphosphinyl)-2,2,2-trifluoro-1-(trifluoromethyl)ethyl)-, phenylmethyl ester","145430-05-3","D",0]
["Perfluorohexylperfluorododecyl phosphinic acid","1240600-41-2","D",0]
["Hexyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","183873-57-6","D",0]
["2,2,3,3-Tetrafluoropropyl difluoromethanesulfonate","95509-81-2","D",0]
["Perfluoro-2-[dimethylamino]-ethane-1-sulfonyl fluoride","192998-56-4","D",0]
["2,3,3,3-Tetrafluoro-1-phenyl-2-(trifluoromethyl)-1-propanone","56112-35-7","D",0]
["Perfluoro[1,2-13C2]hexanoic acid","960315-47-3","D",0]
["7-Chloro-4,4,5,5,6,6,7,7-octafluoro-2-iodoheptan-1-ol","103147-31-5","D",0]
["1,1,3,4,4,5,5,5-Octafluoro-3-methoxy-2-(trifluoromethyl)pent-1-ene","79948-17-7","D",0]
["2-(Tridecafluorohexyl)cyclohexan-1-one","56734-76-0","D",0]
["1-(Perfluorobutanyl)-1-amino-2-nitroethene","223260-92-2","D",0]
["N-(1-Chloro-2,2,2-trifluoroethylidene)-2,2,2-trifluoroethanehydrazonoyl fluoride","88579-79-7","D",0]
["[2,3,3,3-Tetrafluoro-2-(trifluoromethoxy)propyl]oxirane","243139-60-8","D",0]
["2-{[(Bicyclo[2.2.1]hept-5-en-2-yl)oxy]methyl}-1,1,1,3,3,3-hexafluoropropan-2-ol","305815-63-8","D",0]
["4,4''-Bis((perfluoropropyl)-1,3-dioxopropyl)-o-terphenyl-4'-sulfonyl chloride","200862-70-0","D",0]
["2-(Aminomethyl)tetrafluoropropanoic acid","1137870-16-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorononacosane","250738-46-6","D",0]
["1-Butanol, 4-(ethenyloxy)-, polymer with 2-butenoic acid, ethenyl benzoate, ethenyl 2,2-dimethylpropanoate, 2-methyl-1-propene and tetrafluoroethene","235775-81-2","D",0]
["4,4,5,5-Tetrafluoro-1-phenyl-5-(trifluoromethoxy)pentane-1,3-dione","85734-51-6","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Nonadecafluorododecane-1,2-diol","181887-23-0","D",0]
["Heptafluorobutyranilide","336-61-8","D",0]
["4-(Tridecafluorohexyl)aniline","139613-90-4","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl 2-cyanoprop-2-enoate","130192-28-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-7-pentadecene","1980786-99-9","D",0]
["5-Fluoro-2-(1,1,2,2-tetrafluoro-2-phenylethyl)benzonitrile","61547-74-8","D",0]
["2-Carboxy-N,N-diethyl-N-[2-[[(perfluorooctyl)sulfonyl]amino]ethyl]ethanaminium inner salt","61481-08-1","D",0]
["(11-(F-Octyl)undecyl) dimorpholinophosphoramidate","134051-92-6","D",0]
["6-Chloro-perfluorohexanoic acid","558-92-9","D",0]
["1-Nitro-4-[(2,2,3,3,4,4,5,5,6,6,6-undecafluorohexyl)oxy]benzene","183997-46-8","D",0]
["2-bromo-3,3,4,4,4-pentafluorobut-1-ene","68318-95-6","D",0]
["1-Chloro-4-[(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-en-1-yl)oxy]benzene","112340-21-3","D",0]
["1,1'-Oxybis[4-(tridecafluorohexyl)benzene]","151707-03-8","D",0]
["Triethoxy(heptadecafluorooctyl)silane","96305-13-4","D",0]
["1,1,2,2,3,3,4,4,6,6,7,7,8,8,9,9,10,10,10a-Nonadecafluorodecahydropyrido[1,2-a]azepine","95827-25-1","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)thio]-1-propanol","36880-06-5","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-[1-[[bis[3-(trimethoxysilyl)propyl]amino]carbonyl]-1,2,2,2-tetrafluoroethyl]-ω-(1,1,2,2,3,3,3-heptafluoropropoxy)-","264142-24-7","D",0]
["1-Octanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-oxiranylmethyl)-N-propyl-","77620-64-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-[(2-hydroxyethyl)amino]propan-2-ol","30184-89-5","D",0]
["2-Pentafluoroethyl-4,5,6,7-tetrachlorobenzimidazole","49615-25-0","D",0]
["Perfluoro-tert-butyl isobutyrate","914637-43-7","D",0]
["Acetic acid--1,1,3,3,3-pentafluoro-2-(trifluoromethyl)propan-1-ol (1/1)","62619-30-1","D",0]
["1-Methyl-(perfluoroheptane)","1238137-65-9","D",0]
["Methyl perfluoro-3,6,9-trioxatridecanoate","330562-42-0","D",0]
["1,1,1,2,2,5,5,6,6,6-Decafluoro-3,4-bis(trifluoromethyl)hex-3-ene","25543-35-5","D",0]
["Perfluoro(decyl)(octyl) phosphinic acid ytterbium(3+) salt","500776-94-3","D",0]
["Silicon(4+) 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-1-iododecan-1-ide 2,2',2''-nitrilotriethanolate (1:1:1)","135798-18-4","D",0]
["N-(2,5-Dichloro-4-nitrophenyl)-2,3,3,3-tetrafluoro-2-(trifluoromethyl)propanamide","105923-43-1","D",0]
["heptafluorobutanoyl bromide","375-13-3","D",0]
["3,3,3-Trifluoro-1-(heptafluoropropoxy)prop-1-yne","63904-22-3","D",0]
["Dimethyl [1,1,1-trifluoro-2-(trifluoromethyl)butan-2-yl]phosphonate","87579-47-3","D",0]
["4-Fluoro-N-(2-fluoro-3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)-N-methyl-2-nitrobenzamide","862134-28-9","D",0]
["1,1,1,2,2,4,5,5-Octafluoropentan-3-one","370862-44-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-(morpholin-4-yl)heptan-1-one","144237-77-4","D",0]
["1,1,1,2,2,3,3,4-Octafluorohexane","154275-19-1","D",0]
["11:2 Fluorotelomer carboxylic acid","1270180-21-6","D",0]
["Morpholinium perfluorobutane sulfonate","503155-89-3","D",0]
["1,3,3,4,4-Pentafluoro-2-[(prop-2-en-1-yl)oxy]cyclobut-1-ene","65361-33-3","D",0]
["[2,2-Bis(trifluoromethyl)cyclopropyl](phenyl)methanone","61859-97-0","D",0]
["2,2-Dichloro-1,1-difluoroethyl difluoromethyl ether","25600-63-9","D",0]
["1-Bromo-3,3,3',3'-tetrakis(trifluoromethyl)-1,1'-spirobi[1lambda5,2-benziodoxole]","80540-69-8","D",0]
["3-(4-Chloro-2-nitrobenzamido)-2-fluoro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","862133-18-4","D",0]
["N-(2-Chloroethyl)-N-ethyl-perfluorooctane-1-sulfonamide","87988-71-4","D",0]
["2,2,3,3-Tetrafluoro-3a-methyloctahydro-1-benzothiophene","100333-46-8","D",0]
["2-{[(6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Heptadecafluorotridecan-3-yl)oxy]carbonyl}hydrazine-1-carboxylate","821806-55-7","D",0]
["Perfluoro-1-octanesulfinic acid ammonium","183475-14-1","D",0]
["4-Oxo-4-(2,2,3,3-tetrafluoropropoxy)but-2-enoate","63263-69-4","D",0]
["1-(3,3,4,4,5,5,6,6,7,7,8,8-Dodecafluoro-1-iodooctyl)-2,8,9-trioxa-5-aza-1-silabicyclo[3.3.3]undecane","135587-14-3","D",0]
["1,1,1,3,5,5,5-Heptafluoro-4-(trifluoromethyl)pent-3-ene-2,2-diol","89810-81-1","D",0]
["5-(2-Trifluoroacetylaminohexafluoroprop-2-yl)-2'-deoxyuridine","111712-56-2","D",0]
["(4-propan-2-ylphenyl) 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","93131-75-0","D",0]
["1,4-Bis(heptafluoroisopropyl)benzene","51114-12-6","D",0]
["2,5-Furandione, polymer with 2-methyl-3-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethoxy]-1-propene, 2-[2-(2-methoxyethoxy)ethoxy]ethyl ether","37339-00-7","D",0]
["Hexyl perfluorohexanoate","2261-09-8","D",0]
["4-Ethyl-5-hexyl-2,2-bis(trifluoromethyl)-1,3-dioxolane","38274-67-8","D",0]
["4,4,5,5,5-pentafluoropentyl 4-methoxybenzoate","5363-79-1","D",0]
["N-[4-(Nonafluorobutoxy)phenyl]pyridine-3-carboxamide--hydrogen chloride (1/1)","62315-22-4","D",0]
["N-Methyl-N-(2,2,3,3-tetrafluoropropyl)aniline","78727-06-7","D",0]
["4-(Ethenyloxy)-1,1,1,2,2,3,3-heptafluorobutane","356-00-3","D",0]
["Tetrabutylphosphonium perfluorooctane sulfonate","2185049-59-4","D",0]
["12-Cl-Perfluorododecanoic acid","574715-87-0","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutoxy)benzaldehyde","943767-44-0","D",0]
["4,5,6,7-Tetrafluoro-3-(heptafluoropropyl)-1H-indazole","1610931-26-4","D",0]
["Methyl difluoro[1,1,2,2-tetrafluoro-2-(nonafluorobutoxy)ethoxy]acetate","129301-40-2","D",0]
["2-(N-Ethyl-perfluorooctanesulfonamido)acetate","909405-49-8","D",0]
["4-Acetamidophenyl nonafluorobutane-1-sulfonate","41605-57-6","D",0]
["3-(Ethanesulfinyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methylbenzoic acid","1355554-21-0","D",0]
["Methyl 2,2,3,4,4,4-hexafluorobutanoate","106538-78-7","D",0]
["1-Methyl-3-((perfluorobutyl)ethyl)-1H-imidazolium N,N-bis(perfluoromethansulfonyl)amide","872672-61-2","D",0]
["Undecafluorocyclohexanemethanol hydrogen phosphate","32582-75-5","D",0]
["Tributyl(pentafluoroethyl)stannane","1426-66-0","D",0]
["Silicon(4+) 3,3,4,4,5,5,5-heptafluoro-1-iodopentan-1-ide 2,2',2''-nitrilotriethanolate (1:1:1)","112341-58-9","D",0]
["1,1,1,2,2,3,3,6,6,7,7,8,8,8-Tetradecafluorooctane","1835251-92-7","D",0]
["Oxirane, 2-[[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl)oxy]methyl]-","125370-60-7","D",0]
["3-[[(Perfluorobutyl)sulfonyl]methylamino]-N,N,N-trimethyl-1-propanaminium","2089109-11-3","D",0]
["Sulfur, bis[α,α-bis(trifluoromethyl)benzenemethanolato-κO]diphenyl-, (T-4)-","32133-82-7","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorodecanamide","1245601-26-6","D",0]
["N-(9,10-Dioxo-9,10-dihydroanthracen-1-yl)-2,2,3,3,4,4,4-heptafluorobutanamide","162441-56-7","D",0]
["1,1,2-Trichloro-1,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctane","135941-33-2","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(perfluoropropyl)sulfonyl]amino]propyl]-1-propanaminium","2089108-70-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N,N-bis(2-methylpropyl)butanamide","336-30-1","D",0]
["2-Perfluoropropyl-2-propanol","355-22-6","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], α-(2-methyl-1-oxo-2-propen-1-yl)-ω-hydroxy-, polymers with reduced Me esters of reduced polymd. oxidized tetrafluoroethylene acrylates, tert-Bu 2-ethylhexaneperoxoate-initiated","1259853-34-3","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl difluoroacetate","1365807-94-8","D",0]
["2-Nonen-1-ol, 4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluoro-","38550-47-9","D",0]
["3,5,6-Trichloroperfluorohexanoic acid","2106-54-9","D",0]
["Undecafluoropentyl tetradecane","112344-48-6","D",0]
["2,5-Furandione, polymer with 2-methyl-3-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethoxy]-1-propene and 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-8-[(2-methyl-2-propenyl)oxy]octane","38467-13-9","D",0]
["1,1,1-Trifluoro-2-(1,1,2,2-tetrafluoroethoxy)propane","50807-72-2","D",0]
["Ethyl [2-(2-ethoxyethoxy)-1,1,1,3,3,3-hexafluoropropan-2-yl]carbamate","5226-09-5","D",0]
["(1E)-2,2,3,3-Tetrafluoro-N-(4-methoxyphenyl)propan-1-imine","189396-85-8","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-2-methyloctanal","112251-35-1","D",0]
["[1,1'-Biphenyl]-3-yl pentadecafluorooctanoate","110262-36-7","D",0]
["[(1,1,2,2-Tetrafluoroethoxy)methyl]benzene","115611-57-9","D",0]
["4,4,5,5-Tetrafluoro-5-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]pentanoic acid","28793-36-4","D",0]
["Chloro(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)propyl(3,3,3-trifluoropropyl)silane","608296-53-3","D",0]
["2,2,3,3-Tetrafluoro-3-methoxypropanamide","77946-87-3","D",0]
["1-Chloro-1,2,2,2-tetrafluoroethane-1-sulfinyl chloride","38346-18-8","D",0]
["(2,2,3,3,4,4,5,5,6,6-Decafluorocyclohexane-1,1-diyl)dimethanol","87981-51-9","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N,N-dimethyl-N-propyl-1-propanaminium 4-methylbenzenesulfonate (1:1)","167162-27-8","D",0]
["Bis[2-(perfluorohexyl)ethyl] maleate","55003-96-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptyl 4-methylbenzene-1-sulfonate","883500-11-6","D",0]
["3-Cyano-2,2,3,3-tetrafluoropropanoic acid","377-28-6","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(3-sulfopropyl)[(perfluorohexyl)sulfonyl]amino]-1-propanaminium","2089108-80-3","D",0]
["6-Chloro-1-(3,3,4,4,4-pentafluorobutyl)-1H-indazole-3-carboximidamide","1350855-88-7","D",0]
["7,7,8-Tribromo-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","59665-25-7","D",0]
["1,1,1,2,2,3,3,6,6,6-Decafluorohexane","188189-52-8","D",0]
["Siloxanes and silicones, dimethyl, methyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl, hydroxy terminated","115340-96-0","D",0]
["N-(2-Hydroxyethyl)-3-{(2-hydroxy-3-sulfopropyl)[(perfluorohexyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","736903-63-2","D",0]
["5-Chloro-2,2,3,3,4,4,5,5-octafluoro-1-methoxypentan-1-ol","88332-85-8","D",0]
["Bis(perfluorodecyl) phosphinic acid ytterbium(3+) salt","500776-92-1","D",0]
["1-(Perfluoropropanyl)-2-(perfluorobutanyl)ethene","935477-07-9","D",0]
["1,4-Dichloro-2-(pentafluoroethyl)benzene","115591-62-3","D",0]
["2-{[2-(Dimethylamino)ethyl]amino}-1,1,1,3,3,3-hexafluoropropan-2-ol","26799-34-8","D",0]
["Perfluorotriheptyl amine","1127427-75-1","D",0]
["5-(Pentadecafluoroheptyl)-1H-imidazole","81769-55-3","D",0]
["Lithium 3‐[(perfluoroheptyl)ethylsulfanyl]propanoate","74956-89-1","D",0]
["1H,1H-Perfluorobutene","374-39-0","D",0]
["[(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)amino]acetate","1910057-70-3","D",0]
["Perfluorododecyl phosphonic acid","63225-55-8","D",0]
["Ethyl 2,2,3,3,4-pentafluoro-4-oxobutanoate","63425-23-0","D",0]
["Phosphonic acid, [3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy]butyl]-, diethyl ester","646029-82-5","D",0]
["2,2'-Oxybis(difluoroacetic acid)","6535-10-0","D",0]
["(4Z)-5-(Perfluoropropanyl)-2-methyl-2-nitro-5-fluoropent-4-ene","90292-31-2","D",0]
["1,1,1,2,3,3,3-Heptafluoro-2-(1,1,2,3,3,3-hexafluoro-2-iodopropoxy)propane","16005-45-1","D",0]
["1-Ethenyl-3-[1,1,2-trifluoro-2-(heptafluoropropoxy)ethoxy]benzene","129051-93-0","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,4-nonafluoro-N-methylbutane-1-sulfonamide","1427176-16-6","D",0]
["1-Bromo-3-(heptafluoropropyl)benzene","53104-06-6","D",0]
["2-Hexene, 1,1,1-trifluoro-5,5-dimethyl-2-(trifluoromethyl)-","143238-28-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl methanesulfonate","156575-40-5","D",0]
["Sodium 2-hydroxy-3-[methyl[(perfluorobutyl)sulfonyl]amino]-1-propanesulfonate","864069-38-5","D",0]
["3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluorooctyl)oxy]thiophene","142214-54-8","D",0]
["5,6-dibromo-1,1,1,2,2,3,3,4,4-nonafluorohexane","236736-19-9","D",0]
["1,1,1,2,2-Pentafluorohexane","94099-50-0","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl 2-methylprop-2-enoate","13173-36-9","D",0]
["1,1,1,3,5,7,7,7-Octachloro-2,2,3,4,4,5,6,6-octafluoroheptane","53281-10-0","D",0]
["Bis[perfluoro-7-methyloctyl] phosphinic acid","500776-76-1","D",0]
["1-(Methanesulfonyl)-4-[4-(1,1,2,2-tetrafluoroethoxy)phenyl]piperazine","823197-45-1","D",0]
["4-perfluoroisopropylaniline","2396-17-0","D",0]
["Benzenesulfonic acid, 4-[[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-buten-1-yl]oxy]-, sodium salt (1:1)","70829-87-7","D",0]
["2-(Heptadecafluorooctyl)thiophene","80791-16-8","D",0]
["1,1,1,2,2-Pentachloro-3,3,4,4,4-pentafluorobutane","61146-71-2","D",0]
["Bis(pentadecafluoroheptyl)diazene","847335-91-5","D",0]
["4-(1,1,2,3,3,3-Hexafluoropropoxy)-N-{4-[2-(4-morpholinyl)-2-oxoethoxy]phenyl}benzamide","909351-87-7","D",0]
["2-(2-aminophenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","2713-62-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorotridecane","1835249-87-0","D",0]
["1,1,1,4,4-Pentafluoro-2-(trifluoromethyl)butane","143193-99-1","D",0]
["1,1,1,2,5,6,6,6-Octafluoro-2,5-bis(trifluoromethyl)hexane-3,4-dione","1870-16-2","D",0]
["Pentafluoropropane-1-sulfonic acid","803688-15-5","D",0]
["4:2 Fluorotelomer thioether amido sulfonic acid","1333933-57-5","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, N-[3-(triethoxysilyl)propyl]carbamates","1638852-32-0","D",0]
["2,3,3,3-Tetrafluoro-N-(pentafluorophenyl)-2-(trifluoromethyl)propanamide","105923-37-3","D",0]
["Dipotassium 1,1,2,2,3,3,4,4-octafluoro-4-(1,1,2,2-tetrafluoro-2-sulfinatoethoxy)butane-1-sulfinate","81233-10-5","D",0]
["(7-(2,2,3,3,4,4,4-heptafluorobutanoylamino)-9H-fluoren-4-yl) 2,2,3,3,4,4,4-heptafluorobutanoate","82137-36-8","D",0]
["Tris(1,1,2,2,2-pentafluoroethyl) phosphate","447411-37-2","D",0]
["1-Methyl-3-(tridecafluorohexyl)piperidin-4-one","61282-82-4","D",0]
["1,1,1,2,2,4,4,4-Octafluoro-3,3-bis(trifluoromethyl)butane","112156-74-8","D",0]
["PROPANE, 1-BROMO-1,1,2,2,3,3-HEXAFLUORO-","63905-11-3","D",0]
["4-Hexyl-2,2-bis(trifluoromethyl)-1,3-dioxolane","38274-66-7","D",0]
["3,3,4,4,5,5,6,6-Octafluoro-1-hexene","159148-08-0","D",0]
["N~1~,N~1~-Bis(1,3-dihydroxy-2-methylpropan-2-yl)-2,2,3,3-tetrafluorobutanediamide","5246-95-7","D",0]
["Tetrabutylphosphonium perfluorohexane sulfonate","2310194-12-6","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)-1,2-propanediol","143471-08-3","D",0]
["3-[(6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Heptadecafluorotridecanoyl)oxy]-4-(trimethylazaniumyl)butanoate","142674-36-0","D",0]
["Hexatetracontafluorodocosane","1127427-64-8","D",0]
["1-Cyclohexyl-4,4,5,5,5-pentafluoropent-1-en-3-one","89176-04-5","D",0]
["(1,1,1,3,3,3-hexafluoro-2-phenylpropan-2-yl) 4-chlorobenzoate","57633-50-8","D",0]
["5,5,6,6,7,7,7-heptafluoro-4,4-bis(trifluoromethyl)heptanoic Acid","129991-14-6","D",0]
["Disulfide, bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)","42977-22-0","D",0]
["2-Chloro-N-(2,2,3,3,3-pentafluoropropyl)acetamide","919477-89-7","D",0]
["1,2,4-Triazine-3,5(2H,4H)-dione, 6-((heptafluoropropyl)thio)-2-beta-D-ribofuranosyl-","113321-61-2","D",0]
["Methyl 4,4,5,5-tetrafluoro-3-hydroxypent-2-enoate","113341-47-2","D",0]
["1,1,1,2,2,3,3,4,4,11,11,12,12,13,13,14,14,14-Octadecafluoro-6,9-diiodotetradecane","40735-23-7","D",0]
["Ethyl 9H-perfluorononanoate","1799-47-9","D",0]
["2,2,3,5,5,6,6,8,8,10,10,12,12,12-Tetradecafluoro-4,7,9,11-tetraoxadodecanoic acid","919005-16-6","D",0]
["1,1,2,2,3,3,4,4,5,6,6,7,7,7-tetradecafluoro-5-(trifluoromethyl)heptane-1-sulfonic acid","747385-21-3","D",0]
["4-Heptanone, 2,6-bis(trifluoromethyl)-2,6-dihydroxy-1,1,1,7,7,7-hexafluoro-, oxime","101913-88-6","D",0]
["(2,2,3,3-tetrafluoropropoxy)acetic acid","870-51-9","D",0]
["Chloroperfluorocyclohexane","336-15-2","D",0]
["Ethyl 6-(nonafluorobutyl)-4-phenyl-2-sulfanylidene-1,2,3,4-tetrahydropyrimidine-5-carboxylate","281189-83-1","D",0]
["N-(2,2,3,3,4,4,4-Heptafluorobutyl)benzamide","304458-19-3","D",0]
["N-{1-[3,5-Bis({[tert-butyl(dimethyl)silyl]oxy}methyl)phenyl]-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptylidene}hydroxylamine","1335496-61-1","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluoropentyl)sulfonyl]amino}-1-butanaminium","2089108-85-8","D",0]
["2,2,3,3,4,4-Hexafluoro-4-(1,1,2-trifluoro-2-oxoethoxy)butanoyl fluoride","63095-45-4","D",0]
["Decyl 2,3,3,3-tetrafluoropropanoate","88239-57-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-10-iododecane","38565-61-6","D",0]
["Potassium 2-methyl-2-{3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfanyl]propanamido}-1-propanesulfonate","62880-94-8","D",0]
["1,1,1,2-Tetrafluorononan-3-one","113487-28-8","D",0]
["Sodium perfluoro-1-ethanesulfinate","146542-36-1","D",0]
["neodymium tris[1,1,2,2-tetrafluoro-2-(undecafluorocyclohexyl)ethane-1-sulfonate]","41242-13-1","D",0]
["Methyl 2-hydroxy-4-(2,2,3,3-tetrafluoropropoxy)benzoate","651331-89-4","D",0]
["1H,1H,8H,8H-Perfluoro-3,6-dioxaoctane-1,8-diol","129301-42-4","D",0]
["Pentafluoroethyl butanoate","61799-70-0","D",0]
["4-[(6-Methoxy-3-pyridazinyl)sulfamoyl]anilinium 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","298703-31-8","D",0]
["S-Deoxo-6-oxo-fulvestrant","1107606-70-1","D",0]
["2-(Nonafluorobutyl)thiophene","96721-81-2","D",0]
["1H,1H-Perfluorobutyl perfluorobutanesulfonate","883499-32-9","D",0]
["1-Chloro-perfluoroethanesulfonic acid","32773-52-7","D",0]
["2-{2-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]ethoxy}ethan-1-ol","104568-24-3","D",0]
["2,5-OCTANEDIONE, 7-HYDROXY-8,8,8-TRIFLUO","101858-31-5","D",0]
["2-Hexanone, 3,3,4,4,5,5,6,6,6-nonafluoro-","678-18-2","D",0]
["13:1:2 Fluorotelomer betaine","1513864-14-6","D",0]
["Sodium [(nonafluorobutyl)sulfonyl]propylcarbamic acid","138473-78-6","D",0]
["Nonadecafluorodecanoyl chloride","307-38-0","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)benzene-1,2-dicarbonitrile","189101-64-2","D",0]
["4-Chloro-3-(heptafluoropropyl)-5-phenylpyrazole","247220-85-5","D",0]
["Butanoic acid, 3,3,4,4,4-pentafluoro-, ethyl ester","106693-04-3","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-1-phenylpentyl bis(2,2,2-trifluoroethyl) phosphate","100664-15-1","D",0]
["(2E,4Z)-Perfluoro-2,4-hexadiene","83168-66-5","D",0]
["2-[3,5-bis(1,1,1,3,3,3-hexafluoro-2-methoxypropan-2-yl)phenyl]-1,1,1,3,3,3-hexafluoropropan-2-ol","90780-28-2","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-iodononane","1378261-30-3","D",0]
["1,1,2,2,3,3,4,4,5,6-Decafluorocyclohexane","2367-86-4","D",0]
["Heptanamide, N,N-diethyl-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoro-","61881-15-0","D",0]
["Poly[oxy(1,1,2,2-tetrafluoro-1,2-ethanediyl)], α-[1,1-difluoro-2-oxo-2-[[3-(trimethoxysilyl)propyl]amino]ethyl]-ω-(trifluoromethoxy)-","233676-28-3","D",0]
["N-Bromo-2,2,3,3,3-pentafluoropropanimidoyl fluoride","89554-91-6","D",0]
["Ethyl 3-(1-chloro-2-methylpropyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylate","99923-35-0","D",0]
["2,2,3,3,3-Pentafluoro-1-(4-methoxyphenyl)-1-propanone","345901-60-2","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl trifluoroacetate","1365808-09-8","D",0]
["2-Chloro-1,1,2,3,3,5,6-heptafluoro-2,3-dihydro-1H-indene","88953-15-5","D",0]
["Silicate(2-), hexafluoro-, diammonium, mixt. with silica gel","62449-69-8","D",0]
["(Pentafluoroethyl)Benzene","309-11-5","D",0]
["4-[(2,2,3,3,4,4,5,5-Octafluoropentyl)oxy]benzene-1,2-dicarbonitrile","121068-03-9","D",0]
["1-Perfluoromethylcyclohexane-1-sulfonic acid","72441-89-5","D",0]
["Sulfonium, triphenyl-, salt with 1,1,2,2,2-pentafluoro-N-(pentafluoroethyl)sulfonyl-1-ethanesulfonamide (1:1)","541547-03-9","D",0]
["2-(Chlorofluoromethoxy)-1,1,1,3,3,3-hexafluoropropane","26103-09-3","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(4-nitrophenyl)butan-1-one","144459-62-1","D",0]
["1-benzyl-2,2,3-trifluoro-3-(trifluoromethyl)aziridine","5585-30-8","D",0]
["2-Propenoic acid, 2-hydroxyethyl ester, polymer with α-(1-oxo-2-propen-1-yl)-ω-hydroxypoly(oxy-1,2-ethanediyl), α-(1-oxo-2-propen-1-yl)-ω-[(1-oxo-2-propen-1-yl)oxy]poly(oxy-1,2-ethanediyl) and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate","1012783-70-8","D",0]
["(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)(1,1,1,3,3,3-hexafluoropropan-2-yl)phosphinous acid","66644-46-0","D",0]
["2-Bromo-1,1,1,2,3,3-hexafluoro-3-[(trifluoroethenyl)oxy]propane","113772-72-8","D",0]
["4,4,5,5,9,9,10,10-Octafluoro-2,7-dithiatricyclo[6.2.0.0~3,6~]deca-1(8),3(6)-diene","2924-05-2","D",0]
["tridecafluoroheptanoyl bromide","159623-34-4","D",0]
["Cyano(3-phenoxyphenyl)methyl 2-(4-chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)butanoate","82224-38-2","D",0]
["4-bromo-3,3,4,4-tetrafluorobutan-1-ol","234443-21-1","D",0]
["1-Bromo-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-pentacosafluorododecane","67193-90-2","D",0]
["1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-ene-1-sulfonic acid","71178-19-3","D",0]
["N,N'-1,2-Ethanediylbis(2,2,3,3,4,4,4-heptafluorobutanamide)","86273-64-5","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol and 3-aminopropyltriethoxysilane","161308-20-9","D",0]
["N-(2-Bromo-4-nitrophenyl)-2,3,3,4,4,5,5,5-octafluoro-2-(trifluoromethyl)pentanimidic acid","105923-79-3","D",0]
["1-(2,3-Dihydro-1H-indol-1-yl)-2,2,3,3,4,4,4-heptafluoro-1-butanone","543708-46-9","D",0]
["1-(2-Aminophenyl)-2,2,3,3,4,4,4-heptafluorobutan-1-one","200274-52-8","D",0]
["HFE–236ca","32778-11-3","D",0]
["ethyl 2-bromo-2,3,3,3-tetrafluoropropanoate","10186-73-9","D",0]
["[3,3-Bis(trifluoromethyl)-4,5-dihydro-3H-pyrazol-4-yl](phenyl)methanone","61860-03-5","D",0]
["3-(Perfluoropentyl)-5-methylpyrazole","82633-43-0","D",0]
["10-Chloro-7,7,8,8,9,9,10,10-octafluoro-1-phenyldec-4-en-1-one","195147-90-1","D",0]
["4-(Nonafluorobutyl)benzene-1,2-dicarbonitrile","1207299-71-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,9,9,9-Hexadecafluoro-8-iodononane","922524-02-5","D",0]
["1,1,2,2,3-Pentafluoropropan-1-amine","88690-52-2","D",0]
["Methyl 3,3,4,4,4-pentafluorobutyl methylphosphonate","61726-47-4","D",0]
["Fatty acids, linseed-oil, dimers, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl esters","306973-46-6","D",0]
["Propane, 1,3-dichloro-1,1,2,3,3-pentafluoro-","136013-79-1","D",0]
["1,1,1,2,2,3,3,4,5,5,5-Undecafluoro-4-(pentafluoroethoxy)pentane","92978-07-9","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-N-methylpentanamide","115585-00-7","D",0]
["5-Ethyl-3-(1,1,2,2-tetrafluoroethyl)-1H-pyrazole","188838-49-5","D",0]
["N,N-Diethyl-2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanamide","176702-74-2","D",0]
["3,3,3-trifluoro-2-hydroxy-2-(trifluoromethyl)propanamide","662-21-5","D",0]
["5-Amino-1,1,2,2-tetrafluorohex-4-en-3-one","81542-07-6","D",0]
["2-Propenoic acid, 2-methyl-, 2,2,3,3-tetrafluoropropyl ester, homopolymer","29991-77-3","D",0]
["1,1,2,2-Tetrafluoro-2-(1,1,2,2,3,3,4,4-octafluoro-4-iodobutoxy)ethane-1-sulfonamide","86553-42-6","D",0]
["Triethoxy(2,2,3,3-tetrafluorocyclobutyl)silane","92818-39-8","D",0]
["3,3,4-Trifluoro-2-methyl-4-(trifluoromethyl)decan-2-ol","89812-30-6","D",0]
["2-[(1,1,2,2,3,5,5,5-Octafluoropentyl)oxy]propanenitrile","51887-43-5","D",0]
["1-(Ethylsulfanyl)-1,1,2,2,3,3-hexafluoro-3-[(trifluoroethenyl)oxy]propane","77416-78-5","D",0]
["1,12-Dodecanediol, 4,4,5,5,6,6,7,7,8,8,9,9-dodecafluoro-2,11-diiodo-","94403-05-1","D",0]
["1-(Octylamino)-3-[(perfluorohexyl)ethoxy]-2-propanol","1874268-12-8","D",0]
["Perfluorooctanedioic diamide","3492-23-7","D",0]
["4,4,5,5,6,6,7,7-octafluoro-3-hydroxy-1-phenylheptan-1-one","105602-61-7","D",0]
["Acrylic acid, pentafluoroethyl ester","19089-73-7","D",0]
["1,1,2,3,3,3-Hexafluoro-2-nitropropyl sulfurofluoridate","90177-81-4","D",0]
["2-Amino-5-fluoro-5-(trifluoromethyl)-1,3-thiazol-4(5H)-one","13973-15-4","D",0]
["1,1,1,4,4,5,5,5-Octafluoro-2-(trifluoromethyl)pent-2-ene-3-thiol","79272-21-2","D",0]
["(Perfluorononyl)methylketone","150049-87-9","D",0]
["Lithium perfluorodecanoate","84743-32-8","D",0]
["(1Z)-4,4,5,5,6,6,6-Heptafluoro-1-(phenylamino)-1-hexen-3-one","34648-00-5","D",0]
["N-Methylpentadecafluorooctanamide","89685-56-3","D",0]
["(1E)-1,2,3,3,4,4,5,5,6,6,6-Undecafluorohex-1-ene","391199-64-7","D",0]
["2,4,6-Heptanetriol, 2,6-bis(trifluoromethyl)-1,1,1,7,7,7-hexafluoro-","68325-20-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Henicosafluorododecyl phenylcarbamate","305849-13-2","D",0]
["(E)-HFC–1225ye","5595-10-8","D",0]
["7,7,8,8,9,9,9-Heptafluoro-2-methylnon-2-ene-4,6-dione","559-99-9","D",0]
["(E)-1-(1,3,3,4,4,4-Hexafluorobut-1-en-1-yl)-2-phenyldiazene","137731-01-2","D",0]
["Butanamide, 2,2,3,3,4,4,4-heptafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","540530-42-5","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluorodec-3-yn-2-one","58292-89-0","D",0]
["1,1,1,2,2,3,3,4,4,8,8,9,9,10,10,11,11,11-Octadecafluoroundecane-5,7-dione","261503-82-6","D",0]
["Poly(oxy-1,2-ethanediyl), α-(14,14,15,15,16,16,17,17,18,18,19,19, 20,20,20-pentadecafluoro-1,4,7,10-tetramethyl-13-oxo-3,6,9,12-tetraoxaeicos-1-yl)-ω-hydroxy-","60015-08-9","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctanol phosphate ammonium salt","92401-44-0","D",0]
["Ammonium perfluoro-3,5,7,9-tetraoxadecanoate","919004-99-2","D",0]
["4-(5-ethyl-1,3-dimethyl-2,4,6-trioxo-1,3-diazinan-5-yl)pentan-2-yl 2,2,3,3,4,4,4-heptafluorobutanoate","55429-80-6","D",0]
["1,4-Bis(perfluorohexyl)butane","76597-99-4","D",0]
["Orthobutyric acid, heptafluoro-, cyclic ester with 2-ethyl-2-(hydroxymethyl)-1,3-propanediol (1:1)","31185-68-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10-Nonadecafluorodecan-1-amine","88690-51-1","D",0]
["Acetic acid--7,7,8,8,9,9,10,10,10-nonafluorodec-5-en-1-ol (1/1)","137648-84-1","D",0]
["1-Propanaminium, N-(2-hydroxyethyl)-N,N-dimethyl-3-[[(tridecafluorohexyl)sulfonyl]amino]-, chloride","91322-75-7","D",0]
["2-[2-[4-[1,1,2,2-Tetrafluoro-2-[4-[2-(2-hydroxyethoxy)ethoxy]phenyl]ethyl]phenoxy]ethoxy]ethanol","107233-48-7","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-Pentadecafluoro-N-(2-hydroxyethyl)heptane-1-sulfonamide","167398-54-1","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1-(trifluoromethyl)pyrrolidine","2344-10-7","D",0]
["Decafluoroheptanedinitrile","23843-73-4","D",0]
["Bis[(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl)oxy](oxo)phosphanium","102335-26-2","D",0]
["1-Methyl-4-(tridecafluorohexyl)benzene","128720-26-3","D",0]
["3-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)bicyclo[2.2.1]heptan-2-ol","101832-49-9","D",0]
["1,1',2,2',2',3,3',3',4,4,4',4',5,5,5',5',6,6,6',6'-Icosafluoro[1,1'-bi(cyclohexan)]-2-ene","61855-74-1","D",0]
["Perfluoro-N-(4-methylcyclohexyl)piperidine","86630-50-4","D",0]
["3-Fluoro-3-(perfluoroundecanyl)-2-propenal","1335059-27-2","D",0]
["Trimethoxy{3-[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)oxy]propyl}silane","136790-32-4","D",0]
["1,1,2-Trifluoro-2-(pentafluoroethoxy)ethanesulfonate","880084-69-5","D",0]
["3-[(Perfluorohexanesulfonyl)amino]propane-1-sulfonic acid","2089108-64-3","D",0]
["1,1,1-Trichloro-2,3,3,3- tetrafluoropropane","53063-52-8","D",0]
["Poly(oxy-1,2-ethanediyl), α-hydro-ω-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]-1-oxopropoxy]-, ether with oxybis[propanediol] (4:1), fluorinated, reduced","1031300-27-2","D",0]
["1,3,3-Trichloro-1,1,4,4,5,5,5-heptafluoropentan-2-one","67498-70-8","D",0]
["N,N-Dimethyl-3-{[(nonadecafluorononyl)sulfonyl]amino}-1-propanamine N-oxide","1513864-26-0","D",0]
["tert-Butyl (4,4,5,5,6,6,7,7,7-nonafluoro-2-iodoheptyl)carbamate","1301739-79-6","D",0]
["1,1,1,2,2,3,3,4-Octafluoropentane","72923-37-6","D",0]
["2-(4-Chlorophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)butanenitrile","99903-57-8","D",0]
["3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Hexadecafluoro-2-decenal","58544-13-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(4-fluorophenyl)butanamide","550301-92-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,16,16,17,17,18,18,19,19,20,20,20-Docosafluoroicosane","1835252-07-7","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorotridecane","234433-63-7","D",0]
["Methyl 2-chloro-5-{1-[1-methyl-3-(pentafluoroethyl)-4-(trifluoromethyl)-1H-pyrazol-5-yl]-1H-1,2,3-triazol-4-yl}benzoate","1393097-61-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl hypochlorite","76441-89-9","D",0]
["4-(Difluoromethoxy)-1,1,1,2,3,3-hexafluorobutane","69948-46-5","D",0]
["Acetic acid--2-bromo-3,3,4,4,5,5,6,6,6-nonafluorohexan-1-ol (1/1)","89807-81-8","D",0]
["Pentanoic acid, 5-chloro-2,2,3,3,4,4-hexafluoro-5-oxo-, ethyl ester","18381-53-8","D",0]
["(2-Chloro-1,1,1,3,3,3-hexafluoropropan-2-yl)benzene","16878-50-5","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl acetate","80705-15-3","D",0]
["2-(2,2,3,3-Tetrafluoropropanoyl)cyclopentan-1-one","318258-12-7","D",0]
["5-[(2,2,3,3-Tetrafluoropropoxy)methyl]uridine","59694-34-7","D",0]
["4-(2,2,3,3,4,4,4-Heptafluorobutylamino)phenol","1365808-45-2","D",0]
["1,1-Dichloro-1,2,3,4,4,4-hexafluorobut-2-ene","110800-91-4","D",0]
["2-(2-bromo-5-methylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","71401-76-8","D",0]
["Silver perfluorodecanoate","5784-82-7","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentan-1-amine","376-64-7","D",0]
["1,2-bis(1,1,2,2-Tetrafluoroethoxy)ethane","358-39-4","D",0]
["2-Pyrrolidinone, 1-ethenyl-, polymer with 1,1-difluoroethene and 1,1,2,3,3,3-hexafluoro-1-propene","215653-67-1","D",0]
["1,1,1,2,2,5,5,5-Octafluoropentan-3-one","61637-92-1","D",0]
["1,1,1,3,3,5,5,7,7,8,8,10,11,11-Tetradecafluoro-2,4,6,9-tetraoxaundec-10-ene","191018-25-4","D",0]
["1-Bromo-2-(pentafluoroethyl)benzene","112754-17-3","D",0]
["Methanesulfonic acid--1,1,1,3,3,3-hexafluoropropan-2-ol (1/1)","25236-65-1","D",0]
["Silyl nonafluorobutane-1-sulfonate","135524-36-6","D",0]
["1,1,1,2,2-Pentafluoro-3,3-dimethylbutane","67498-75-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-12-iodododecane","38565-62-7","D",0]
["6,6,6-trifluoro-2,2-dimethyl-5-(trifluoromethyl)hex-4-en-3-one","35443-87-9","D",0]
["Tetraphosphetane, tetrakis(pentafluoroethyl)-","35449-91-3","D",0]
["Allyl 2,2,3,3,3-pentafluoropropyl ether","186907-75-5","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-ol--pyridine (1/1)","58228-38-9","D",0]
["5-Chloro-1,1,2,2-tetrafluoro-2,3-dihydro-1H-indene","922141-52-4","D",0]
["1-Piperazinemethanol, alpha,alpha-bis(trifluoromethyl)-, hydrate","30192-64-4","D",0]
["Pentafluoropropaneperoxoic acid","159219-31-5","D",0]
["(Tridecafluorohexyl)phosphonic acid--4-methylaniline (1/1)","1263361-02-9","D",0]
["1-Butanone, 1-(9H-fluoren-2-yl)-2,2,3,3,4,4,4-heptafluoro-, O-[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]oxime","749924-57-0","D",0]
["2-Ethyl-4,4,4-trifluoro-1-(4-fluorophenyl)-3-(trifluoromethyl)butane-1,3-diol","34848-33-4","D",0]
["Methoxy (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) bis(3,3,3-trifluoropropyl) silane","608300-81-8","D",0]
["2,2,3,3,4,4,4-Heptafluorobutanal--water (1/1)","907607-07-2","D",0]
["[(3,3,4,4,5,5,6,6,6‐Nonafluorohexyl)oxy]phosphonic  acid","150065-76-2","D",0]
["N-Methyl-6-[2,2,2-trifluoro-1-(trifluoromethyl)ethoxy]-1,3,5-triazine-2,4-diamine","301211-06-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,35,35,36,36,37,37,38,38,39,39,40,40,41,41,42,42,43,43,44,44,45,45,46,46,46-Pentacontafluoro-14,33-diiodohexatetracontane","114221-76-0","D",0]
["potassium pentafluoroethane-1-sulfonate","2837-92-5","D",0]
["4-(Perfluorobutyl)-2-butanone","140834-64-6","D",0]
["4:2 Fluorotelomer betaine","145441-30-1","D",0]
["2-(Perfluorohexyl)-1-(hydroxymethyl)ethyl 2-propenoate","146955-23-9","D",0]
["1,1'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(4-ethynylbenzene)","92455-16-8","D",0]
["NO NAME..","113612-30-9","D",0]
["[[1,2,2,2-Tetrafluoro-1-(trifluoromethyl)ethyl]thio]benzene","65799-63-5","D",0]
["1-(Perfluorobutanyl)hept-1-ene","383145-46-8","D",0]
["Ethyl 2,2,3,3,4,4,5,6-octafluorohex-5-enoate","63284-94-6","D",0]
["3-Fluoro-3-(trifluoromethyl)pyrrolidine","1550728-66-9","D",0]
["1,1,3,3,5-Pentafluoro-1,3-dihydro-2-benzofuran","651-58-1","D",0]
["Copolymer of chloroethene / docosyl acrylate / 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate / bis(2-ethylhexyl) maleate / 2-hydroxyethyl methacrylate","1187311-45-0","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.',.alpha.''-[1,2,4-benzenetriyltris[carbonyloxy[2-(chloromethyl)-2,1-ethanediyl]]]tris[.omega.-fluoro-","71230-80-3","D",0]
["4-(Methylsulfanyl)phenyl pentafluoroethane-1-sulfonate","57728-78-6","D",0]
["5,5,5-Trifluoro-4,4-bis(trifluoromethyl)pent-1-ene","14115-46-9","D",0]
["4-HEPTANONE, 2-CHLORO-6-METHYL-1,1,1-TRI","101913-92-2","D",0]
["1H,1H,7H-Perfluoroheptyl 4-methylbenzenesulfonate","424-16-8","D",0]
["Trimethyl(nonafluorobutyl)stannane","876903-01-4","D",0]
["N-[3-(Dimethylamino)propyl]perfluorododecanamide","1513863-79-0","D",0]
["Butanedioic acid, 2-sulfo-, 1,4-bis(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl) ester","752929-63-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8-Tetradecafluorononane-1,9-diol","203303-01-9","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(4-(propylamino)phenyl)propan-2-ol","874479-45-5","D",0]
["4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]-N-(hydroxymethyl)benzamide","59379-88-3","D",0]
["1,1,1,3,5,5,5-Heptafluoro-4-(trifluoromethyl)pent-2-ene","13088-26-1","D",0]
["2,4,6,8-Tetramethyl-2-[3-(2-oxiranylmethoxy)propyl]-4,6-bis((perfluorohexyl)propyl)cyclotetrasiloxane","1428232-90-9","D",0]
["Ammonium 2,2,3,3,4,4,5,5-octafluoropentanolate","855743-12-3","D",0]
["1,2,2,3,3,4,4,5,5,6,6-Undecafluoro-N-(2,3,4,5-tetrachlorophenyl)cyclohexanecarboxamide","107350-42-5","D",0]
["N-(2,4-Dinitrophenyl)-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanamide","105936-30-9","D",0]
["N-Dodecyl-2,2,3,3,4,4,4-heptafluorobutanamide","2284-51-7","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide and phosphoryl trichloride, hydrolyzed","162567-76-2","D",0]
["N,N-Diethyl-4,4,5,5,5-pentafluoro-2-(trifluoromethyl)pentanamide","90278-12-9","D",0]
["Acetamido(6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heptadecafluorotridecyl)propanedioic acid","885276-27-7","D",0]
["4,4,5-Trichloro-2,2-bis(trifluoromethyl)-1,3-dioxolane","64499-76-9","D",0]
["1-(2-Bromo-1,1,2,2-tetrafluoroethyl)imidazole","900534-71-6","D",0]
["Ammonium 2,3,3,3-tetrafluoro-2-(nonafluorobutoxy)propanoate","96513-97-2","D",0]
["1-Bromo-1,2,2,3,3,4,5,6,7-nonafluoro-2,3-dihydro-1H-indene","88953-16-6","D",0]
["Ytterbium(3+) tris{(1E)-2,2,3,3,4,4,4-heptafluoro-1-[(1S,4R)-4,7,7-trimethyl-3-oxobicyclo[2.2.1]hept-2-ylidene]-1-butanolate}","80464-74-0","D",0]
["N-Benzyl-2-(2,2,3,3-tetrafluoropropoxy)acetamide","402939-52-0","D",0]
["(4E)-1,1,1,2,2,4,5,6,7,7,7-Undecafluoro-6-(trifluoromethyl)hept-4-en-3-one","134330-88-4","D",0]
["Perfluoropentanesulfonate","175905-36-9","D",0]
["2-((Perfluorohexyl)ethoxy)ethanol","55427-50-4","D",0]
["Ammonium 3-[butyl[(perfluorobutyl)sulfonyl]amino]-2-hydroxypropanesulfonate","864069-48-7","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoro-1-phenylheptan-3-one","90550-17-7","D",0]
["2-C-(Nonafluorobutyl)-β-L-ribofuranose","467220-84-4","D",0]
["4-(Pentafluoroethoxy)aniline","717-85-1","D",0]
["1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-ol","64614-34-2","D",0]
["1,1,1,2,3,3,5,5-Octafluoro-6-isocyanato-2-(isocyanatomethyl)-4,4-bis(trifluoromethyl)hexane","444122-27-4","D",0]
["4-Chloro-1,1-bis(trifluoromethyl)cyclohexane","65018-64-6","D",0]
["2,3-Difluoro-2,3-bis(trifluoromethyl)oxirane","773-29-5","D",0]
["Perfluoropropyl formate","271257-42-2","D",0]
["1-Bromo-3-(pentafluoroethyl)benzene","18739-03-2","D",0]
["1-Chloro-2,2,3,3-tetrafluorocyclobutane","558-61-2","D",0]
["(2Z)-1-(Butylthio)-3,4,4,5,5,6,6,6-octafluoro-2-hexene","90292-35-6","D",0]
["N,N-Diethyl-4-methyl-2-(1,2,2,2-tetrafluoroethyl)-1,3-dioxolan-2-amine","89752-24-9","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecyl [2-(sulfothio)ethyl]carbamate","761340-40-3","D",0]
["2,3,4,4,4-Pentafluoro-3-(trifluoromethyl)butanoic acid","917951-62-3","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluorohexyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","2089109-72-6","D",0]
["1-[3-(pentafluoroethyl)phenyl]ethan-1-one","1554429-57-0","D",0]
["1,1'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(3-ethynylbenzene)","92455-18-0","D",0]
["alpha-(Trifluoromethoxy)-alpha,alpha-difluoromethyl acetate","2195-84-8","D",0]
["1,2-bis(Heptafluorobutyryl)hydrazine hydrazone","5611-44-9","D",0]
["3-Benzamido-N-(2,2,3,3,3-pentafluoropropyl)benzamide","917920-93-5","D",0]
["Butyl (2-{[ethoxy(hydroxy)methylidene]amino}-1,1,1,3,3,3-hexafluoropropan-2-yl)methylphosphinate","133611-25-3","D",0]
["1-Ethoxy-1,1,2,2,3,3,4,4,5,5,5-undecafluoropentane","181214-75-5","D",0]
["2-{[4-(Perfluorobutoxy)pyridin-2-yl]methanesulfinyl}-1H-thieno[3,4-d]imidazole","121617-11-6","D",0]
["2-{[3-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)propyl]amino}ethyl prop-2-enoate","499776-70-4","D",0]
["8-azido-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","62571-55-5","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-omega.-(2-((2-methyl-1-oxo-2-propenyl)oxy)ethyl), copolymer with octadecanyl-2-methylpropenoate and ethyleneiminyl-2-methylpropenoate","220713-74-6","D",0]
["1,1,1,2,2,3,3-Heptafluoro-4-(1,1,2,3,3,3-hexafluoropropoxy)butane","1184-97-0","D",0]
["1-Chloro-2,3,3,4,4-pentafluorocyclobut-1-ene","377-94-6","D",0]
["4-Bromo-2-(heptafluoropropyl)pyridine","1816283-37-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-(dimethylamino)ethyl ester, polymer with 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate, N-oxides, acetates","1440528-04-0","D",0]
["1-Bromo-1,1,2,2-tetrafluoro-3-octene","74793-72-9","D",0]
["Germanium--tetrafluorooxirane (1/1)","96570-94-4","D",0]
["(9-Pentafluoro(5)sulfide)-perfluorononanoate","2269495-21-6","D",0]
["Silver perfluoroheptanoate","424-05-5","D",0]
["Phenyl(tridecafluorohexyl)iodanium tetrafluoridoborate(1-)","74061-32-8","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-1-[(trifluoroethenyl)oxy]-4-(trifluoromethoxy)butane","609818-38-4","D",0]
["1-Ethoxy-1,1,2,2,3,3,3-heptafluoropropane","22052-86-4","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Pentadecafluoro-1-[(prop-2-en-1-yl)oxy]-3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]decan-2-yl carbonate","192326-53-7","D",0]
["2-[[3-[(Perfluorobutyl)ethylsulfinyl]-1-oxopropyl]amino]-2-methyl-1-propanesulfonic acid","1513864-09-9","D",0]
["Bromo(1,1,1,2,3,3,3-heptafluoropropan-2-yl)mercury","662-09-9","D",0]
["Perfluoro tert-butylcyclohexane","84808-64-0","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(2-mercapto-5-methylphenyl)-2-propanol","57565-54-5","D",0]
["1H,1H,2H,2H-Perfluorooctyl acetate","37858-03-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoropentadecane","113659-13-5","D",0]
["2,2,3-Trifluoro-3-(heptafluoropropyl)oxirane","74942-19-1","D",0]
["1-Benzoyl-3,5-bis(nonafluorobutyl)pyrazole","231630-89-0","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, trimer","6792-31-0","D",0]
["6-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)-3,5,5-trimethylcyclohex-2-en-1-ol","34844-41-2","D",0]
["7-(Heptafluoropropyl)-4,9-dimethoxy-5H-furo[3,2-g][1]benzopyran-5-one","376383-49-2","D",0]
["4,4,5,5-Tetrafluoro-1,3-dioxolane","76492-96-1","D",0]
["1-(Dimethylamino)-3-(perfluorodecyl)propan-2-ol","80244-65-1","D",0]
["Sodium perfluoroheptane sulfonate","21934-50-9","D",0]
["3-(Perfluoro-2-butyl)propanoic acid","239463-95-7","D",0]
["4-(1,1,2,2-Tetrafluoroethoxy)benzoic acid","10009-25-3","D",0]
["4-[2-[Difluoro(trifluoromethoxy)methoxy]-1,1,2,2-tetrafluoroethoxy]-2,2,3,4,4-pentafluorobutanoic acid","919005-28-0","D",0]
["2-(2,2,3,3-Tetrafluoropropoxy)-2H-1,3,2-benzodioxaphosphole","88399-68-2","D",0]
["Undecafluorohexanoyl bromide","1404193-66-3","D",0]
["Methyl 4-(nonafluorobutyl)cyclohexane-1-carboxylate","88951-14-8","D",0]
["Methyl 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecanoate","132424-37-4","D",0]
["Ethyl 3-(perfluorohexyl)propanoate","60023-26-9","D",0]
["2-Amino-3-(perfluoropropyl)-1-phenyl-3-propanol","322392-46-1","D",0]
["Perfluorodecanoic anhydride","942199-24-8","D",0]
["Perfluoro-1-ethyl-3-propoxycyclohexane","400626-82-6","D",0]
["1,8-Octanediol, 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoro-","90177-96-1","D",0]
["2-(Ethylsulfanyl)-3,3,3-trifluoro-2-(trifluoromethyl)propanoyl fluoride","67732-80-3","D",0]
["4'-Chloro-3'-nitro-4,4,4-trifluoro-3-(trifluoromethyl)crotonophenone","35443-91-5","D",0]
["2,2,3,3,4,4,5,5,6-Nonafluorooxane","65601-69-6","D",0]
["Potassium 6-[[(perfluorobutyl)sulfonyl](propyl)amino]hexanoate","864069-34-1","D",0]
["5-(2-Iodoethenyl)-perfluoro-3-oxapentanesulfonyl fluoride","124887-86-1","D",0]
["Potassium perfluoro-1-(perfluoroethyl)cyclohexanesulfonate","1135308-34-7","D",0]
["2,3-Dimethyl-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-24-8","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[(2-hydroxy-3-sulfopropyl)[(perfluorobutyl)sulfonyl]amino]-1-propanaminium, inner salt","2089109-66-8","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(propane-2-sulfinyl)benzoic acid","1355554-94-7","D",0]
["1,1,1,2,2-Pentafluoro-3-propoxypropane","2244079-58-9","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol and ethylenediamine","161308-25-4","D",0]
["4-Chloro-5-fluoro-2,2-bis(trifluoromethyl)-1,3-dioxole","89444-42-8","D",0]
["1,4-Dimethyl-2-(tridecafluorohexyl)benzene","123524-58-3","D",0]
["Nonacosafluoropentadecanoate","1214264-29-5","D",0]
["1,1,2-Trifluoro-2-(1,1,2,2,2-pentafluoroethoxy)ethanesulfonic acid","905363-44-2","D",0]
["2(5H)-Furanone, 5-(heptafluoropropyl)-","143469-51-6","D",0]
["3-[2-[Difluoro(trifluoromethoxy)methoxy]-1,1,2,2-tetrafluoroethoxy]-2,3,3-trifluoropropanoic acid","919005-21-3","D",0]
["Perfluoro-4-methylindane","36158-85-7","D",0]
["5-Chloroperfluoropentanoyl fluoride","261503-68-8","D",0]
["Siloxanes and silicones, methyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl, hydroxy terminated","115341-00-9","D",0]
["Decane, 1,1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10,10-octadecafluoro-","142083-52-1","D",0]
["Sodium (perfluorobutanesulfonamido)acetate","688738-74-1","D",0]
["Propane,2,3-dibromo-1,1,1,2-tetrafluoro-","421-92-1","D",0]
["Sulfurous acid--1,1,1,3,3,3-hexafluoropropan-2-ol (1/2)","53517-89-8","D",0]
["1-(Heptafluoropropyl)isoquinoline","70414-12-9","D",0]
["Lithium perfluoroheptanoate","60871-90-1","D",0]
["7,7-bis(1,1,2,2,2-pentafluoroethyl)cyclohepta-1,3,5-triene","17838-67-4","D",0]
["1H,1H-Heptafluorobutyl-2-fluoroacrylate","151174-22-0","D",0]
["Sodium N-[3-(dimethylamino)propyl]-N-[(perfluorooctyl)sulfonyl]glycinate","98900-84-6","D",0]
["3,3,4-Trifluoro-4-(trifluoromethyl)-1,2,3,4-tetrahydronaphthalen-2-ol","62409-61-4","D",0]
["[3,3-Difluoro-2-(tetrafluoroethylidene)cyclobutyl]benzene","109270-36-2","D",0]
["4-(1,1,2,3,3,3-Hexafluoropropoxy)-N-(2-phenylethyl)benzamide","909352-05-2","D",0]
["N,N,N-Trimethyl-3-[[2-[(perfluorohexyl)ethylsulfinyl]acetyl]amino]-1-propanaminium","1513864-03-3","D",0]
["N-[5-(2-Chloro-1,1,2-trifluoroethoxy)-2-hydroxy-4-{2-[3-(pentadecyloxy)phenoxy]butanamido}phenyl]-2,2,3,3,4,4,4-heptafluorobutanamide","92589-42-9","D",0]
["Triethylaminium perfluoro-2-(2-propoxypropoxy)propanoate","165951-19-9","D",0]
["Acetic acid--4,5,5,5-tetrafluoro-2-iodo-4-(trifluoromethyl)pentan-1-ol (1/1)","40798-39-8","D",0]
["5-Methyl-5-[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]hex-1-en-3-yne","85915-52-2","D",0]
["4,4-Bis(trifluoromethyl)-2H,3H-heptafluoroheptenoic acid","261503-43-9","D",0]
["N-Chloro-2,2,3,3,4,4,4-heptafluorobutanimidamide","13050-20-9","D",0]
["6-(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexylsulfonyl)naphthalen-2-ol","7240-48-4","D",0]
["Trimethylsilyl 1,1,2,2-tetrafluoro-2-(pentafluoroethoxy)ethane-1-sulfonate","136049-37-1","D",0]
["1-(Hexadec-1-en-1-yl)perfluorohexane","1244062-15-4","D",0]
["1,3,5-Tris(Pentafluoroethoxy)benzene","52999-46-9","D",0]
["Tetradecafluorooctahydropentalene","57133-61-6","D",0]
["Perfluoroheptane sulfonamide","82765-77-3","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(4-methoxy-2-nitrophenyl)butanamide","1799-52-6","D",0]
["1-Chloroperfluorooctanesulfonic acid","1651215-26-7","D",0]
["2,2,3,3-Tetrafluoro-4-methyloxolane","240140-63-0","D",0]
["8-Chloro-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-hexadecafluoro-1-octanesulfonic acid","777011-38-8","D",0]
["N-(1,3-Benzothiazol-2-yl)-3,3,3-trifluoro-2-(trifluoromethyl)propanamide","4612-65-1","D",0]
["1,5-bis(Methoxy)perfluoro-3-pentanone","1422-71-5","D",0]
["4-Difluoromethyl-perfluoro-3-oxabutanesulfonyl fluoride","104729-49-9","D",0]
["3,5-Pyrazolediethanol, 1-phenyl-alpha,alpha,alpha',alpha'-tetrakis(trifluoromethyl)-","102129-14-6","D",0]
["Tridecafluorohexane-1-sulfinyl azide","64983-18-2","D",0]
["2H-Perfluorooctanoic acid","142821-03-2","D",0]
["6,13-Bis(heptadecafluorooctyl)pentacene","876517-48-5","D",0]
["1-Decanaminium, N-decyl-N,N-dimethyl-, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-1-octanesulfonate (1:1)","251099-16-8","D",0]
["11-(Perfluoropentyl)undecanoic acid","2803-40-9","D",0]
["1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Hexadecafluoro-1-iododecyl)-2,8,9-trioxa-5-aza-1-silabicyclo[3.3.3]undecane","135587-16-5","D",0]
["4-[(Perfluorooctyl)sulfonyl]-1,1-dioctylpiperazinium iodide","113584-52-4","D",0]
["2,2,4,4,6,6-Hexafluoro-1,3-dioxan-5-one","402570-18-7","D",0]
["3,3-Dimethoxy-1,3-bis((perfluorohexyl)ethyl)-1,1-disiloxanediol","1531633-12-1","D",0]
["Methyl 3-(ethylsulfanyl)-2,2,3,3-tetrafluoropropanoate","77705-85-2","D",0]
["3(Perfluoro-2-butyl)propanol","239463-96-8","D",0]
["3,3,3-Trifluoro-2-methyl-2-(trifluoromethyl)propanoyl chloride","13027-24-2","D",0]
["1-(1,1,2,2-Tetrafluoroethoxy)but-2-ene","83168-72-3","D",0]
["1-Bromo-1-chloro-2,2,3,3-tetrafluoropropane","1645-78-9","D",0]
["Lithium perfluorobutanoate","4146-76-3","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, decarboxylated","161075-01-0","D",0]
["Butanedioic acid, 2-sulfo-, 1,4-bis(1,1,2,2,3,3,4,4,4-nonafluorobutyl) ester","750544-43-5","D",0]
["1,1,1,2,3,4,4,4-Octafluoro-2,3-bis(trifluoromethoxy)butane","67282-99-9","D",0]
["Diethylmethoxy(3,3,4,4,4-pentafluorobutyl)silane","608299-25-8","D",0]
["1-Iodo-1,2,2,2-tetrafluoro-1-(trifluoromethoxy)ethane","139604-89-0","D",0]
["1,1,1-Trichloro-2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctane","88639-57-0","D",0]
["2,2,2-Trifluoro-N-(pentafluoroethyl)ethanimidoyl fluoride","380-66-5","D",0]
["hexafluoropropane","359-58-0","D",0]
["1-Butanesulfonamide, 1,1,2,2,3,3,4,4,4-nonafluoro-N-methyl-N-(2-oxiranylmethyl)-","942597-24-2","D",0]
["4-Pyridinecarboxamide, N-[4-(nonafluorobutoxy)phenyl]-","62315-14-4","D",0]
["Cyclopentene, 3,3,4,4,5,5-hexafluoro-","1005-73-8","D",0]
["2-(2-Chloro-1,1,2,2-tetrafluoroethoxy)-2,2-difluoro-N-phenylacetamide","83865-14-9","D",0]
["Benzenamine, 4-[2-(2,4-dinitrophenyl)diazenyl]-N-(2,2,3,3-tetrafluoropropyl)-","295346-91-7","D",0]
["Polychloroethene-co-(cyclohexan-1-yl methacrylate)-co-(oxiran-2-ylmethyl methacrylate)-co-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate)","871558-71-3","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-propoxybutane","72372-80-6","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl heptafluorobutanoate","308-45-2","D",0]
["1-(4-Bromophenyl)-2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propan-1-one","67727-74-6","D",0]
["8-(2-Chloroethanesulfonyl)-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","93393-77-2","D",0]
["4,4,4-Trifluoro-1-(furan-2-yl)-3-(trifluoromethyl)butane-1,3-diol","100991-87-5","D",0]
["perfluoro acetic acid, α-substituted with the copolymer of perfluoro-1,2-propylene glycol and perfluoro-1,1-ethylene glycol, terminated with chlorohexafluoropropyloxy groups","329238-24-6","D",0]
["Ethyl 4,4,5,5,5-pentafluoro-3-hydroxypentanoate","1646-18-0","D",0]
["HFE-125","3822-68-2","D",0]
["3-Bromo-2,2,3,3-tetrafluoropropanoic acid","22633-83-6","D",0]
["Bis(pentafluoroethyl)diselane","6123-49-5","D",0]
["Perfluoropropane sulfonate","110676-15-8","D",0]
["5-Methyl-6-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfanyl]hexahydro-4,7-methano-2-benzofuran-1,3-dione","94413-32-8","D",0]
["Methyl 4,4,5,5,6,6,7,7-octafluoro-3,3-dihydroxyheptanoate","89129-74-8","D",0]
["2,2,3,3-Tetrafluoropropanal","756-04-7","D",0]
["1,1,1,2,3,3,4,4,5,5,6,6-dodecafluoro-6-iodo-2-(trifluoromethyl)hexane","3486-08-6","D",0]
["2,2,3,3-Tetrafluoropropanal--water (1/1)","215858-32-5","D",0]
["2-(1,1,2,2-Tetrafluoroethoxy)benzene-1-sulfonyl isocyanate","77797-71-8","D",0]
["Tetramethylammonium perfluorooctane sulfonate","56773-44-5","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(3-fluorophenyl)butanamide","332031-88-6","D",0]
["Poly(oxy-1,2-ethanediyl), α-hydro-ω-hydroxy-, ether with N-(2-hydroxyethyl)-N-[2-hydroxy-3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]propyl]-N-methyloctanaminium, methanesulfonate (2:1:1)","1874268-16-2","D",0]
["3,5,5,6,6,6-Hexafluorohex-3-en-2-ol","90550-23-5","D",0]
["2-[(2,2,3,3,4,4,5,5-Octafluoropentyl)oxy]ethan-1-ol","50997-69-8","D",0]
["2-{[(2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl)oxy]methyl}oxirane","140369-64-8","D",0]
["1-(Chloromethyl)-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzene","75462-58-7","D",0]
["1,1,1,3,4,4,5,5,5-Nonafluoro-2-(heptafluoropropoxy)pent-2-ene","137741-06-1","D",0]
["Sodium mono(N-ethyl-2-perfluorooctylsulfonaminoethyl) phosphate","2624-80-8","D",0]
["Ethyl 3,3,3-trifluoro-2-(nonafluorobutoxy)-2-(trifluoromethyl)propanoate","38012-79-2","D",0]
["Ethanol, 2-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]-","38824-96-3","D",0]
["1-(Dimethylamino)-3-(perfluorooctyl)propan-2-ol","80233-99-4","D",0]
["Heptafluoropropyl pentafluoropropanoate","296758-60-6","D",0]
["4-[(Perfluorononyl)oxy]benzenesulfonic acid ammonium salt","69161-16-6","D",0]
["tert-Butyl (5,5,6,6,6-pentafluoro-2-methyl-4-oxohexan-3-yl)carbamate","172089-25-7","D",0]
["Cyclopentyl[3-(1,1,2,2-tetrafluoroethoxy)phenyl]methanol","1443325-97-0","D",0]
["Ammonium 2-hydroxy-3-[[(perfluorobutyl)sulfonyl](propyl)amino]propanesulfonate","864069-49-8","D",0]
["Carbamic acid--2-[2,2-bis(trifluoromethyl)-1,3-dioxolan-4-yl]ethan-1-ol (1/1)","51125-65-6","D",0]
["Tetraphosphirane, tris(pentafluoroethyl)-","29634-17-1","D",0]
["2,3,3,4,4,4-Hexafluorobutanoic acid","62765-25-7","D",0]
["Potassium 1,1,1,3,3,3-hexafluoro-2-(trifluoromethyl)propan-2-olate","29646-16-0","D",0]
["1-((Heptadecafluorooctyl)sulfonyl)-1H-imidazole","87988-58-7","D",0]
["Pentane, 1,1,2,2,3,3,4,4-octafluoro-5-(1,1,2,2-tetrafluoroethoxy)-","16627-71-7","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N-methyl-N-(trimethylstannyl)butane-1-sulfinamide","41006-33-1","D",0]
["Cl-Perfluoroheptanoate","1696259-97-8","D",0]
["4,4,5,5,6,6,7,7,8,8,8-Undecafluoro-3-phenoxyoct-2-enal","866525-43-1","D",0]
["N-Butyl-N,N-dimethyl-(5-(difluoromethyl)perfluoropentyl)methan-1-aminium","","D",0]
["alpha,alpha-Dimethyl-4-(alpha,alpha,beta,beta-tetrafluorophenethyl)benzylamine","40396-83-6","D",0]
["Poly(difluoromethylene), .alpha.-[3-(dimethylamino)-2-hydroxypropyl]-.omega.-fluoro-","71002-40-9","D",0]
["Vinyl nonafluoro-1-butanesulfonate","42409-05-2","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononanal","83957-58-8","D",0]
["1-Fluoro-4-[1,1,2,2,3,3,4,4-octafluoro-4-(4-fluorophenyl)sulfanylbutyl]sulfanylbenzene","","D",0]
["1,1,2,2-Tetrafluoro-6-azaspiro[3.4]octane","2091592-25-3","D",0]
["2-(3,3,4,4,5,5,6,6,6-Nonafluorohexane-1-sulfinyl)ethan-1-ol","917966-97-3","D",0]
["2,2-Dichloro-perfluoro-1-decanesulfonic acid","","D",0]
["2,6-Dibromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)aniline","","D",0]
["Tetrafluoroethylene-vinyl acetate-vinyl alcohol copolymer","216660-17-2","D",0]
["1H, 1H, 2H, 2H-[1,2-13C2] perfluorooctyldihydrogen phosphate","2179232-13-2","D",0]
["(αR,7α)-3-Hydroxy-α-((perfluorobutyl)propyl)-17-oxo-estra-1,3,5(10)-triene-7-decanoic acid","615563-01-4","D",0]
["6-Bromo-8-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)quinolin-5-amine","917923-88-7","D",0]
["5-Fluoro-6-(pentafluoroethyl)pyrimidine-2,4(1H,3H)-dione","885-05-2","D",0]
["1H,10H-Perfluorodecane","3492-24-8","D",0]
["N-(2-((Ethylsulfonyl)amino)-5-(trifluoromethyl)-3-pyridinyl)-2,2,3,3,3-pentafluoropropanamide","141283-63-8","D",0]
["2,3,4,6-Tetrachlorophenyl heptafluorobutanoate","89071-43-2","D",0]
["HG–20","249932-25-0","D",0]
["N'-[(2E)-5,5,6,6,7,7,7-Heptafluoro-4-oxohept-2-en-2-yl]-4-nitrobenzohydrazide","203201-05-2","D",0]
["N-(Carboxymethyl)-2-[3-[[(perfluorooctyl)sulfonyl]amino]propoxy]-N,N-dimethylethanaminium inner salt","110538-67-5","D",0]
["Phosphine, methylbis(pentafluoroethyl)-","197703-75-6","D",0]
["1,1,3,3,4-Pentafluoro-1,3-dihydro-2-benzofuran","20687-99-4","D",0]
["Propane, 2-(bromomethyl)-1,1,1,3,3,3-hexafluoro-","382-14-9","D",0]
["1,1,1,3,3,3-Hexafluoro-N-(2-fluorophenyl)propan-2-imine","305837-16-5","D",0]
["2:2 Fluorotelomer sulfonamido propyl dimethyl amine","","D",0]
["N,N,N-Trimethyl-3-[(perfluorohexyl)sulfonyl]-1-propanaminium","1427498-85-8","D",0]
["[(Heptadecafluorooctyl)sulfanyl]benzene","89883-19-2","D",0]
["2-ethoxy-1,1,1,3,3,3-hexafluoropropan-2-ol","754-57-4","D",0]
["2-(2-(2-(Perfluorohexyl)ethoxy)ethoxy)ethanol","54950-01-5","D",0]
["3-Methyl-2,2-bis(trifluoromethyl)-1,3-oxazolidin-5-one","6458-45-3","D",0]
["7:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["2,2,3,3,4,4-Hexafluoro-4-[(1,1,1,2,3-pentafluoro-3-oxopropan-2-yl)oxy]butanoyl fluoride","19190-57-9","D",0]
["[(Perfluoropentadecanoyl)amino]-3-betaine","1513863-84-7","D",0]
["1,4-Dibromo-1,2,2,3,3,4,5,5,6,6-decafluorocyclohexane","87539-24-0","D",0]
["Perfluoro-5-(nonafluorobutyl)cyclohexanesulfonic acid","","D",0]
["Perfluorodecalin (cis)","60433-11-6","D",0]
["Methacrylic acid, ester with N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-1-octanesulfonamide, polymer with acrylamide, acrylonitrile, and butyl acrylate","33595-24-3","D",0]
["N-(2-Azido-1,1,1,3,3,3-hexafluoropropan-2-yl)benzamide","112608-25-0","D",0]
["1,1,2,2,3-Pentafluoro-3-(trifluoromethyl)cyclobutane","89185-56-8","D",0]
["(1Z)-N-[2-(Bromomethyl)-4-methoxyphenyl]-2,2,3,3,4,4,4-heptafluorobutanimidoyl chloride","923569-78-2","D",0]
["Butan-2-yl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","330154-39-7","D",0]
["Tris[3-(perfluorooctyl)phenyl]phosphine","325459-91-4","D",0]
["N-[2-[Methyl(1,1,2,2,3,3,4,4,4-nonafluorobutylsulfonyl)amino]ethyl]propanamide","","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], α-[2-[(2-hydroxymethylethyl) [(pentadecafluoroheptyl)sulfonyl]amino]methylethyl]-ω-(4-sulfobutoxy)-, monosodium salt","167648-35-3","D",0]
["1-Bromo-4-(pentafluoroethyl)benzene","206560-66-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-9-hexacosene","907206-01-3","D",0]
["Dichloro(1,1,1,2,3,3-hexafluoropropan-2-yl)methylsilane","62281-32-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorotricosane","863126-43-6","D",0]
["Perfluoro-5-(nonafluorobutyl)cyclohexanesulfonate","","D",0]
["N-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-2-prop-2-enoxybenzamide","67133-48-6","D",0]
["Ethanaminium, N-(2-carboxyethyl)-2-[[(polyfluoroalkyl)sulfonyl]amino]-N,N-dimethyl-, inner salt","","D",0]
["1,1-dibromo-1,2,2,3,3- pentafluoropropane","70192-61-9","D",0]
["Cobalt perfluorooctanoate","35965-01-6","D",0]
["Silanediol, dimethyl-, polymer with methyl(3,3,4,4,5,5, 6,6,7,7,8,8,8-tridecafluorooctyl)silanediol","156048-38-3","D",0]
["Dichloro{3-[(2,2,3,3,4,4,5,5-octafluoropentyl)oxy]propyl}phenylsilane","646063-08-3","D",0]
["N-Succinimidyl 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecanoate","852527-45-8","D",0]
["Bis(perfluorooctyl) phosphinic acid  erbium(3+) salt","500776-70-5","D",0]
["2,3,3,3-Tetrafluoro-2-iodopropanoyl fluoride","83078-26-6","D",0]
["3-(Perfluoroundecyl)‐1‐[(2‐hydroxyacetyl)sulfanyl]propan‐1‐one","","D",0]
["N,N-Diethyl-heptadecafluoro-1-octanesulfonamide","87988-61-2","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10-Dodecafluorodec-1-yn-4-ol","124612-86-8","D",0]
["1,2-Bis[(2R,5R)-2,5-dimethylphospholanyl]-3,3,4,4-tetrafluoro-1-cyclobutene 1,5-cyclooctadiene rhodium(I) tetrafluoroborate","910048-20-3","D",0]
["3-(Nonafluorobutyl)-1-phenyl-1H-pyrazol-5-ol","96146-02-0","D",0]
["1,1,2,2,3-Pentafluorocyclopentane","139063-94-8","D",0]
["5-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutane-1-sulfonyl)-2-ethoxy-4-(furan-2-yl)-6-phenyl-3,4-dihydro-2H-pyran","905560-41-0","D",0]
["Octafluorohexanedioic acid--water (1/1)","123334-02-1","D",0]
["1-Bromopentafluoropropene","53692-47-0","D",0]
["{[(Perfluorododecyl)sulfonyl]amino}acetic acid","","D",0]
["Perfluoroalkyl carboxylates","","D",0]
["N-{2-[(4,4,5,5,6,6,6-Heptafluoro-3-oxohexyl)sulfanyl]ethyl}-L-valine","194031-59-9","D",0]
["1,3-Benzenedisulfonic acid, 4-[2-[4-[[2-(acetyloxy)ethyl]ethylamino]phenyl]diazenyl]-, 1,3-bis(2,2,3,3-tetrafluoropropyl) ester","143877-57-0","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluorooctyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["5‐[3‐({[(3,3,4,4,5,5,6,6,6‐Nonafluorohexyl)sulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["1,3,3,4,4,5,5,6,6,7,7-Undecafluoro-2-(3-methoxypropyl)cyclohept-1-ene","193203-75-7","D",0]
["2-Fluoro-2-(pentafluoroethyl)-3,3-bis(trifluoromethyl)oxirane","788-67-0","D",0]
["(1Z)-1,2,3,4,4,4-Hexafluoro-1-iodo-3-(trifluoromethyl)but-1-ene","105774-97-8","D",0]
["N-[[4-[(Heptadecafluorononenyl)oxy]phenyl]sulfonyl]-N-methylglycine","59536-23-1","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoroundecane","1190430-22-8","D",0]
["1-Methoxy-3-(nonafluorobutyl)benzene","18739-65-6","D",0]
["Perfluoro-11-tridecene-1-sulfonic acid","2089109-48-6","D",0]
["2,4,4,5,7,7,8,10,10,11,13,13,14,16,16,17,19,19,20,20,21,21,21-tricosafluoro-2,5,8,11,14,17-hexakis(trifluoromethyl)-3,6,9,12,15,18-Hexaoxaheneicosan-1-ol","167631-99-4","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9, 10,10,10-heptadecafluorodecyl)sulfonyl]propylamino]ethyl]-ω-hydroxy-","405226-47-3","D",0]
["13-H-Perfluorotridecanoic acid","423-73-4","D",0]
["1,1,1,2-tetrafluoro-4-iodo-2-(trifluoromethyl)hexane","261760-23-0","D",0]
["2-Pentanol, 4,4-dichloro-1,1,1-trifluoro-2-(trifluoromethyl)-","101931-61-7","D",0]
["Pentafluorotris(trifluoromethyl)cyclobutane","444883-26-5","D",0]
["2-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]ethane-1-thiol","104568-31-2","D",0]
["N-Ethyl-N,N-dimethyl-(3-(difluoromethyl)perfluoropropyl)methan-1-aminium","","D",0]
["Bis(heptadecafluorooctyl)diazene","3829-39-8","D",0]
["2-Methyl-5-(pentafluoroethyl)aniline","238098-24-3","D",0]
["Octafluoroadipamide","355-66-8","D",0]
["1,1,1,3,3,3-hexafluoro-n,n'-bis(1,1,1,3,3,3-hexafluoropropan-2-ylidene)propane-2,2-diamine","34451-14-4","D",0]
["Perfluoro-5-(trifluoromethyl)cyclohexanesulfonic acid","","D",0]
["7,8-Dibromo-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorooctane","51249-62-8","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoro-1-[2,3,4,5-tetrafluoro-6-(trifluoromethyl)phenyl]piperidine","96595-38-9","D",0]
["4,5-Difluoro-4,5-diiodo-2,2-bis(trifluoromethyl)-1,3-dioxolane","137635-01-9","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Nonadecafluorohenicosane","677324-20-8","D",0]
["4-[Ethyl[(perfluorooctyl)sulfonyl]amino]butanesulfonic acid  potassium salt (1:1)","60511-72-0","D",0]
["Vinyl chloride-1-chloro-1-fluoroethylene copolymer","172074-69-0","D",0]
["2-(2,2,3,3,4,4,4-Heptafluorobutanoyl)hydrazine-1-carboximidamide","25978-98-7","D",0]
["2-Methyl-4,4-bis(trifluoromethyl)-1,4-dihydro-2H-3,1-benzoxazine","405919-98-4","D",0]
["3-{(Perfluorooctanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["Dodecyl 2,3,3,3-tetrafluoropropanoate","88239-58-1","D",0]
["6:2 Fluorotelomer thioether propanoyl alaninate","","D",0]
["1-Methyl-4-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-43-3","D",0]
["7beta-Fulvestrant","407577-53-1","D",0]
["4-Methyl-5-(1,1,2,2-tetrafluoroethoxy)benzene-1,2-diamine","104162-20-1","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl acetate","24165-09-1","D",0]
["2-[(2,2,3,3,3-Pentafluoropropoxy)methyl]oxirane","706-89-8","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, 1,1'-(hydrogen phosphate), ammonium salt (1:1)","1764-95-0","D",0]
["4-Difluoromethyl-perfluoro-3-oxabutanesulfonic acid","88986-19-0","D",0]
["Ethoxy(2,2,3,3-tetrafluoropropoxy)phosphanolate","116293-50-6","D",0]
["2-Pentene, 1,1,1,2,3,4,4,5,5,5-decafluoro-","72804-49-0","D",0]
["6-Chloro-2,2,3,3,4,4,5,5,6,6-decafluorohexanoyl fluoride","335-52-4","D",0]
["2,4,6-Trichloro-2,3,3,4,5,5,6-heptafluoro-6-iodohexanoyl chloride","88639-64-9","D",0]
["2,4,4,5,5-Pentafluoro-1-(trifluoromethyl)-4,5-dihydro-1H-imidazole","37662-91-2","D",0]
["Dimethyl[3-(perfluorohexyl)‐2‐(formyloxy)propyl](2‐oxoethyl)azanium","","D",0]
["6-(Tridecafluorohexyl)-3-oxabicyclo[3.2.0]heptane-2,4-dione","842123-44-8","D",0]
["3-(12,12,13,13,14,14,15,15,15-Nonafluoropentadecyl)benzene-1,2-diol","131545-71-6","D",0]
["2-Butenedioic acid (2E)-, bis(.gamma.-.omega.-perfluoro-C4-20-alkyl) esters, polymers with 1-(ethenyloxy)butanol, ethylene, 1,4-hexadiene and propene","68037-22-9","D",0]
["1,2-Bis(chlorosulfanyl)-1,1,2,2-tetrafluoroethane","2375-43-1","D",0]
["1,1,1,2,2,11,11,12,12,12-Decafluorododecane","69125-81-1","D",0]
["Carbonic acid--2,2,3,3,4,4,5,5-octafluoropentan-1-ol (1/2)","4454-75-5","D",0]
["Diisopentyl 2-[(2,2,3,3,4,4,4-heptafluorobutanoyl)amino]succinate","75743-06-5","D",0]
["Propane, 1-methoxy-2-methyl-, octafluoro deriv.","63919-03-9","D",0]
["Ethyl 4,4,5,5,6,6,6-heptafluoro-3-(nitromethyl)hexanoate","376-88-5","D",0]
["Perfluoro-5-(tridecafluorohexyl)cyclohexanesulfonate","","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(2,2,2-trifluoroethoxy)propane","142469-08-7","D",0]
["2(3H)-Furanone, 3,3,4,4-tetrafluorodihydro-","58816-74-3","D",0]
["1,1,1,3,3,4,4,5,5,6,6,7,7,8,8-Pentadecafluorooctan-2-one","63703-12-8","D",0]
["2-[6-tert-butyl-2,2-dimethyl-4,4-bis(trifluoromethyl)-3,1-benzoxathiin-8-yl]-1,1,1,3,3,3-hexafluoropropan-2-ol","84649-63-8","D",0]
["Hexafluoroacetone dihydrate","32836-39-8","D",0]
["4-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)oxy]-2-hydroxybenzoic acid","61753-99-9","D",0]
["1-(Heptadecafluorooctyl)-4-methylbenzene","82396-51-8","D",0]
["(1Z)-1,2-Dibromo-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooct-1-ene","59665-28-0","D",0]
["(2Z)-4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoronon-2-en-1-ol","83707-01-1","D",0]
["Perfluorooctan-2-yl carbamate","92681-65-7","D",0]
["2-Butenedioic acid (2Z)-, sodium salt, polymer with ethenylbenzene and 2,2,3,3-tetrafluoropropyl hydrogen (2Z)-2-butenedioate","169797-36-8","D",0]
["N-Ethyl-N-(2-oxiranylmethyl)perfluoropentanamide","141187-87-3","D",0]
["Benzoic 4,4,5,5,5-pentafluoropentanoic anhydride","223679-70-7","D",0]
["2-(2,2,3,3,4,4,4-Heptafluorobutanoyl)cyclohexan-1-one","37172-87-5","D",0]
["3-[(Perfluorododecane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide","","D",0]
["N,N′-[Phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-perfluoro-1-decanesulfonamide] ammonium salt","118337-76-1","D",0]
["6-(1,2,2,2-Tetrafluoroethyl)-1,3,5-triazine-2,4-diamine","1793-26-6","D",0]
["N,N,N-Trimethyl-3-[methyl[(perfluoropentyl)sulfonyl]amino]-1-propanaminium","2089109-12-4","D",0]
["4-Thiazolol, 2-(1,2,2,2-tetrafluoroethyl)-","494745-13-0","D",0]
["2-(Bromomethyl)hexafluoropropan-2-ol","503169-76-4","D",0]
["N''-[6-Phenyl-4,4-bis(trifluoromethyl)-4H-1,3,5-oxadiazin-2-yl]guanidine","90697-68-0","D",0]
["1-Iodo-1H,1H-nonafluoropentane","2253-14-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluorotricosane","200817-55-6","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(3-sulfopropyl) [(perfluoropentyl)sulfonyl]amino]-1-propanaminium","2089108-79-0","D",0]
["1‐(Methylamino)-3-(perfluorohexadecyl)propan‐2‐ol","","D",0]
["1-Chloro-perfluoro-1-propanesulfonic acid","752170-49-3","D",0]
["Perfluorooctanesulfonamide ammonium salt (1:1)","76752-72-2","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Heptadecafluoro-2-methyldodecan-2-ol","141183-94-0","D",0]
["3-Bromo-4-chloropentafluorobutyric acid","216393-99-6","D",0]
["Ethyl 3,3,4,4,5,5,6,6,6-nonafluorohexanoate","172287-15-9","D",0]
["2-(Trifluoromethyl)-1,1,1,3,3,3-hexafluoropropane","382-24-1","D",0]
["Chlorodiethyl(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)silane","608295-82-5","D",0]
["Chloro(3,3,4,4,4-pentafluorobutyl)bis(3,3,3-trifluoropropyl)silane","608296-74-8","D",0]
["2,2,3,3-Tetrafluoropropyl 5-[(4-iodophenyl)amino]-5-oxopentanoate","5578-93-8","D",0]
["3-[[2-[(Perfluorohexyl)ethylthio]acetyl]amino]-N,N,N-trimethyl-1-propanaminium","1513864-00-0","D",0]
["1-Bromo-1,3,5,5,5-pentachloro-1,2,2,3,4,4-hexafluoropentane","3231-20-7","D",0]
["1-Bromo-5-methyl-3,3-bis(trifluoromethyl)-1,3-dihydro-1lambda3,2-benziodoxole","69352-00-7","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(3-sulfopropyl) [(perfluorobutyl)sulfonyl]amino]-1-propanaminium","2089108-78-9","D",0]
["Bis(4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononyl) diazene-1,2-dicarboxylate","462996-01-6","D",0]
["N-(2-Hydroxyethyl)-3-[(2-hydroxyethyl)[(perfluoropentyl)sulfonyl]amino]-N,N-dimethyl-1-propanaminium","2089109-00-0","D",0]
["HFE 71 DE","185045-68-5","D",0]
["Perfluoro(allyl vinyl ether) homopolymer","101182-88-1","D",0]
["(4S,5S)-1,1,2,2,3,3,4,5-octafluorocyclopentane","158389-18-5","D",0]
["3-(4-Butan-2-ylphenoxy)sulfonyl-1,1,2,2,3,3-hexafluoropropane-1-sulfonate","","D",0]
["Phosphorous acid--3,3,4,4,4-pentafluorobutan-2-ol (1/3)","79155-01-4","D",0]
["N-[3-(Dimethylamino)propyl]-perfluoropropanamide","1858540-01-8","D",0]
["2H-Nonafluorobutane","680-17-1","D",0]
["3-(Difluoromethyl)-1,3,4,4,5,6,6,6-octafluorohex-1-ene","","D",0]
["N-(5-Chloro-3-nitropyridin-2-yl)-2,2,3,3,3-pentafluoropropanamide","60792-72-5","D",0]
["1,1,1,2-Tetrafluoropropane","421-48-7","D",0]
["5-Benzylidene-2,2-bis(trifluoromethyl)-1,3-dioxolan-4-one","7712-19-8","D",0]
["Pyrocatechol, 4-(2-(3-methyl-5-(1,1,2,2-tetrafluoroethyl)-1-pyrazolyl)-4-thiazolyl)-","75013-45-5","D",0]
["Siloxanes and Silicones, Me octyl, Me stearyl, Me 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl","262292-17-1","D",0]
["2,2,3,3,4,4,4-Heptafluorobutane-1,1-diol","375-21-3","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-iodoheptane","89889-25-8","D",0]
["(1-Chloro-1,2,2,2-tetrafluoroethyl)benzene","426-56-2","D",0]
["2-[3,3,4,4,5,5,5-Heptafluoro-2,2-bis(trifluoromethyl)pentyl]benzonitrile","111364-00-2","D",0]
["7:1:2 Fluorotelomer betaine","171184-03-5","D",0]
["6,6,7,7,8,8,9,9,10,10,11,11,11-Tridecafluoro-4-iodoundecan-1-ol","132665-00-0","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoropentane-1,1-diol","355-30-6","D",0]
["3-Fluoro-3-(perfluorobutyl)acrylic acid","","D",0]
["3-(Perfluoroheptyl)propane‐1‐sulfonic acid","","D",0]
["Perfluoroalkyl (linear) alcohols","","D",0]
["Methyl 3-(heptadecafluorooctyl)benzoate","80791-11-3","D",0]
["(E)-(Dimethylamino)-N,N,N-trimethyl(methylimino)methanaminium pentafluoroethan-1-olate","479024-70-9","D",0]
["1,1,2,2,3,3-Hexafluorobutan-1-ol","119398-75-3","D",0]
["Bis(1,1,1,2,3,3,3-heptafluoropropan-2-yl)tetrasulfane","1588-31-4","D",0]
["N-[(2S)-2-Amino-3-methylbutyl]-1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonamide","1417316-15-4","D",0]
["Cyclopentane, octafluorobis(trifluoromethyl)-","99510-46-0","D",0]
["Poly(oxy-1,2-ethanediyl), α-[[ethyl[(heptadecafluorooctyl)sulfonyl] amino]acetyl]-ω-hydroxy-","109636-63-7","D",0]
["(6E)-8,8,9,9,10,10,11,11,12,12,13,13,13-Tridecafluorotridec-6-ene","350608-60-5","D",0]
["3,3,4,4,7,7,8,8,11,11,12,12-Dodecafluorotetracyclo[8.2.0.0~2,5~.0~6,9~]dodeca-1,5,9-triene","32937-02-3","D",0]
["1,2-dibromo-1,2,3,3,3-pentafluoro-1-(2,2,3,3,3-pentafluoropropoxy)propane","396716-50-0","D",0]
["1-Butanesulfonyl fluoride, 1,1,2,2,3,3,4,4-octafluoro-4-[(trifluoroethenyl)oxy]-","88190-28-7","D",0]
["4,4,5,5,5-Pentafluoro-1-(4-fluorophenyl)pentane-1,3-dione","64287-12-3","D",0]
["1-((1,2-Difluoro-2-(heptafluoropropoxy)vinyl)oxy)-1,1,2,2,3,3,3-heptafluoropropane","145151-18-4","D",0]
["(Dichloromethyl)(3,3,4,4,4-pentafluorobutan-2-yl)silane","84442-92-2","D",0]
["Propan-2-yl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","147224-17-7","D",0]
["2H-Perfluoroheptadecanoic acid","","D",0]
["11-(Perfluorohexyl)-10-undecen-1-ol","117543-54-1","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Henicosafluoro-1-dodecanesulfonate anion","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,8,8-Pentadecafluoro-8-iodooctane","53826-16-7","D",0]
["1,1,1,2-Tetrafluoro-2-(trifluoromethyl)-4-hexen-3-one","184711-88-4","D",0]
["4-Heptanone, 2,6-bis(trifluoromethyl)-2,6-dihydroxy-1,1,1,7,7,7-hexafluoro-, dimethyl hydrazone","101913-87-5","D",0]
["Difluoro(tridecafluorohexyl)borane","329009-01-0","D",0]
["2-(1,2,2,2-Tetrafluoroethoxy)perfluoroethanesulfonic acid","801209-99-4","D",0]
["9-Octadecenoic acid (Z-), reaction products with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,1112,12,12-heneicosafluoro-1-dodecanol","125768-41-4","D",0]
["Pentafluoroethane-1-sulfonyl chloride","64773-40-6","D",0]
["3-[3,3,4,4,5,5,5-Heptafluoro-2,2-bis(trifluoromethyl)pentyl]benzonitrile","111363-99-6","D",0]
["13-H-Perfluorotridecanoate","1696259-78-5","D",0]
["1-[4-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutane-1-sulfonyl)-5-methyl-3-phenyl-2,3-dihydrofuran-2-yl]ethan-1-one","771491-68-0","D",0]
["Methyl 2-methoxy-6-[(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonyl)oxy]benzoate","475630-76-3","D",0]
["1,1,1,2,2-Pentafluoro-2-[(pentafluoroethyl)tellanyl]ethane","41055-97-4","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2-iodophenyl)butanamide","378215-44-2","D",0]
["3-Azido-2,3,3-trifluoro-2-(heptafluoropropoxy)propanoyl fluoride","86414-16-6","D",0]
["Sodium 3-[[3-(dimethylamino)-2-hydroxypropyl][(perfluorohexyl)sulfonyl]amino]-2-hydroxy-propanesulfonate","98900-72-2","D",0]
["N-[4-(1,1,1,3,3,3-Hexafluoro-2-hydroxy-2-propanyl)phenyl]-2-thiophenesulfonamide","293753-05-6","D",0]
["2,2,3,4,4-Pentafluorooxetane","144109-03-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trichloromethyl)propan-2-ol","7594-49-2","D",0]
["(1E)-1,2,3,4,4,4-Hexafluoro-1-iodo-3-(trifluoromethyl)but-1-ene","883882-12-0","D",0]
["2,2'-Oxybis(tetrafluoroethane-1-sulfonic acid)","113507-84-9","D",0]
["4-(Nonadecafluorononyl)benzoic acid","88950-95-2","D",0]
["Magnesium bromide 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctan-1-ide (1/1/1)","51300-88-0","D",0]
["Phenyltris((perfluorohexyl)ethyl)stannane","175354-30-0","D",0]
["6:2 Fluorotelomer thioether amido amine carboxylic acid","1383438-88-7","D",0]
["3-(Heptafluoropropyl)oxolane","143837-48-3","D",0]
["12-Chloro-perfluorododecanoate","1696260-10-2","D",0]
["4,4,5,5,6,6,6-Heptafluoro-3,3-bis(trifluoromethyl)hex-1-ene","79272-26-7","D",0]
["3-Amino-4,4,5,5-tetrafluoro-1-phenylpent-2-ene-1-thione","92832-08-1","D",0]
["2-Methyl-1,1,1,2,3,3,4,4,5,5,5-undecafluoropentane","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodooctacosane","1257261-90-7","D",0]
["1,9-Decadiene, 3,3,4,4,5,5,6,6,7,7,8,8-dodecafluoro-, polymer with 1,1-difluoroethene, 1-[difluoro(trifluoromethoxy)methoxy]-1,2,2-trifluoroethene, 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","944477-76-3","D",0]
["11:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["7,8,8,8-Tetrafluoro-7-(trifluoromethyl)octan-1-ol","220469-13-6","D",0]
["barium (4Z)-1,1,1,2,2,3,3-heptafluoro-7,7-dimethyl-6-oxooct-4-en-4-olate—water (1/2/1)","143457-82-3","D",0]
["Siloxanes and Silicones, di-Me, Me hydrogen, Me 2-phenylpropyl, Me 3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]propyl, Me 2-(trimethoxysilyl)ethyl, [[dimethyl[3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-h","1382351-52-1","D",0]
["Octyl perfluorooctanoate","67699-49-4","D",0]
["(4-Fluorophenyl)(heptadecafluorooctyl)iodanium","83609-26-1","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[perfluoro-2-[2-(propoxy)propoxy]-1-oxopropyl]amino-1-propanaminium chloride","137506-17-3","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluorodecan-2-one","110388-12-0","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoroheptyl 2-methylprop-2-enoate","243842-15-1","D",0]
["2,2,3,3-Tetrafluoro-3-methoxypropanoyl fluoride","2794-15-2","D",0]
["Polyfluoroalkyl (linear) (-CF2H) alkyl (linear) ketone","","D",0]
["Chlorodipropyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","608296-24-8","D",0]
["Benzyl 2,3,3,3-tetrafluoro-2-(trifluoromethyl)propanoate","38392-11-9","D",0]
["N-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)benzenemethanamine","206184-90-9","D",0]
["1H,1H-Perfluoro-n-decyl acrylate","335-83-1","D",0]
["2,2,3,3-Tetrafluorocyclobutanol","374-32-3","D",0]
["Perfluorononane sulfonic acid","474511-07-4","D",0]
["4,4,5,5,5-Pentafluoro-1-(4-fluoro-3-methoxyphenyl)pentane-1,3-dione","64287-14-5","D",0]
["(E)-Perfluoro-2-pentadec-7-eneoxyacetic acid","","D",0]
["Methyl 3,3,4,4,4-pentafluoro-2-oxobutanoate","74067-14-4","D",0]
["4,5-Dibromo-1,1,1,2,2,3,3-heptafluoropentane","377-46-8","D",0]
["Perfluorohexane sulfinic acids","","D",0]
["2,2-Difluoroethyl nonafluorobutane-1-sulfonate","1036375-28-6","D",0]
["Hexane, 1,6-dibromo-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-","918-22-9","D",0]
["4-Amino-2-(undecafluoropentyl)benzonitrile","1463530-19-9","D",0]
["Octafluorobutane-1,4-disulfonic acid--water (1/2)","144797-51-3","D",0]
["4-[(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)sulfanyl]benzoic acid","88489-76-3","D",0]
["1-Bromoperfluoro-2,5-dioxanonane","330562-46-4","D",0]
["Potassium (perfluorobutanesulfonyl)azanide","289042-19-9","D",0]
["1,1,1,2-tetrafluoro-2-methoxyethane","50285-05-7","D",0]
["1,1,2,2,3,3,4,4,5,6,7,8,8,8-Tetradecafluoro-6-octene-1-sulfonic acid","2089109-52-2","D",0]
["N-Ethyl-N,N-dimethyl-((difluoromethyl)difluoromethyl)methanaminium","","D",0]
["(3-Chlorophenyl)[4-(1,2,2,2-tetrafluoroethoxy)phenyl]methanone","61547-44-2","D",0]
["Dodecane, 1,1,1,2,2,3,3,4,4-nonafluoro-6-iodo-","109603-73-8","D",0]
["1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Docosafluoroundec-1-ene","66256-52-8","D",0]
["6-Nitro-2-(pentafluoroethyl)-1H-benzimidazole","4229-01-0","D",0]
["2,2,3,3,4,4,4-Heptafluorobutanimidamide--hydrogen chloride (1/1)","2358-53-4","D",0]
["Trichloro(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)stannane","6256-76-4","D",0]
["(2E)-3,4,4,5,5,6,6,7,7,8,8,8-Dodecafluoro-2-octenoic acid","","D",0]
["(3E)-2-hydroxy-7-methoxy-3-[(4-methoxyanilino)methylidene]-2-(1,1,2,2-tetrafluoroethyl)-2,3-dihydro-4H-1-benzopyran-4-one","913711-76-9","D",0]
["(1,1,1,3,3,3-hexafluoro-2-phenylpropan-2-yl) 2-phenylsulfanylbenzoate","37847-84-0","D",0]
["9,9,10,10,11,11,12,12,12-Nonafluorododecan-1-ol","133001-14-6","D",0]
["8:2 Fluorotelomer N,N-dimethyl-, N-oxide","","D",0]
["Nonanamide, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","540521-01-5","D",0]
["Stannane, dichlorobis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-","96325-96-1","D",0]
["4:2 fluorotelomer sulfinyl propanamido dimethyl ethyl sulfonate","","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymer with chloroethene, α-fluoro-ω-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene) and N-(hydroxymethyl)-2-propenamide","152286-16-3","D",0]
["Phosphonic acid, [3-[ethyl[(heptadecafluorooctyl)sulfonyl]amino]propyl]-","71463-78-0","D",0]
["N-(Carboxymethyl)-N,N-dimethyl-3-(1H,1H,2H,2H-perfluoro-1-hexanesulfonamido)propan-1-aminium","","D",0]
["2,2,3,3,3-Pentafluoro-1-(pyrrolidin-1-yl)propan-1-one","686720-34-3","D",0]
["(Nonafluorobutyl)propanedioyl dichloride","502768-31-2","D",0]
["2-Propenoic acid, 2-hydroxyethyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate and octadecyl 2-propenoate","1190367-98-6","D",0]
["(Perfluoropropoxy)dimethylsilane","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluoroethyl)-2-fluoroethan-1-aminium","","D",0]
["Bis(hexafluoroacetonyl)acetone","30902-53-5","D",0]
["2‐[(2-(1-Hydrido-perfluoroundecyl)ethyl)dimethylazaniumyl]acetate","","D",0]
["2-Hydroxy-3-[(perfluorohexyl)ethoxy]propyl 2-propenoate","145756-59-8","D",0]
["2,2-Bis(trifluoromethyl)butanoyl fluoride","14316-81-5","D",0]
["2,2'-(((Nonafluorobutyl)sulfonyl)imino)diacetic acid","1268835-43-3","D",0]
["4-[(2,2,3,3-Tetrafluoropropoxy)methyl]-1,3-dioxolan-2-one","879496-46-5","D",0]
["3-{(Perfluoroundecanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["Formic acid--2,2,3,4,4,4-hexafluorobutan-1-ol (1/1)","104725-00-0","D",0]
["2,2-Bis[4-(1,1,2,2-tetrafluoroethoxy)phenyl]octane","163036-62-2","D",0]
["N-Ethyl-2,2,3,3,4,4,4-heptafluorobutan-1-amine","355-99-7","D",0]
["Tributoxy(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl (3b,5a,20R)-3-[(trifluoroacetyl)oxy]cholan-24-oate","","D",0]
["2-[Methyl(3,3,4,4,5,5,6,6,6-nonafluorohexylsulfonyl)amino]ethyl prop-2-enoate","","D",0]
["4-(Butan-2-yl)-2-(1,1,2,2-tetrafluoroethyl)-1,3-oxazol-5(2H)-one","51314-52-4","D",0]
["Perfluoroalkyl (linear) sulfonates","","D",0]
["2-Propenethioic acid, 2-methyl-, S-[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-eicosafluoro-11-(trifluoromethyl)dodecyl] ester","30769-88-1","D",0]
["Ethyl [3-(heptafluoropropyl)-1-methyl-1H-pyrazol-5-yl]acetate","1428569-18-9","D",0]
["2,3,4,5,6-Pentafluoro-2-[1,1,2,2,3,4,4,4-octafluoro-3-(trifluoromethyl)butyl]-2H-pyran","88179-52-6","D",0]
["Hexafluoropropene, oligomeric reaction products with 1,1-difluoroethylene and tetrafluoro-ethylene, telomers with fluorine","162162-67-6","D",0]
["1,1,1,3,3,4,4,6,6,7,7,9,9,10,10,12,12,13,13,15,15,15-Docosafluoro-2,5,8,11,14-pentaoxapentadecane","64028-06-4","D",0]
["Perfluoro-2-(propoxy)ethanesulfinic acid, sodium salt (1:1)","1151494-33-5","D",0]
["Silicon(4+) 3,3,4,4,5,5,6,6,7,7,8,8-dodecafluoro-1-iodooctan-1-ide 2,2',2''-nitrilotriethanolate (1:1:1)","135798-16-2","D",0]
["Dichloro-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,10,10,10-heptadecafluorodecyl)-methylsilane","","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N,N-bis(trimethylstannyl)butane-1-sulfonamide","41006-34-2","D",0]
["Perfluoro-5-(trifluoromethyl)cyclohexanesulfonate","","D",0]
["HG’-02","485399-46-0","D",0]
["1,1'-[1,3-Phenylenebis(oxy)]bis[3-(tridecafluorohexyl)benzene]","151707-04-9","D",0]
["1-Phenyl-2,2-bis(trifluoromethyl)aziridine","26071-20-5","D",0]
["[2‐Hydroxy‐3‐(2-(perfluorohexyl)ethanesulfonyl)propyl]trimethylazanium","","D",0]
["6H-1,3,5-Oxathiazine, 4-phenyl-2,2,6,6-tetrakis(trifluoromethyl)-","57014-91-2","D",0]
["N-{[2,5-Dimethyl-4-(1,1,2,2-tetrafluoroethanesulfinyl)phenyl]carbamoyl}-2,6-difluorobenzene-1-carboximidic acid","100342-07-2","D",0]
["2,2-Difluoro-3-(nonafluorobutoxy)propanoyl fluoride","824393-38-6","D",0]
["4-Amino-5,5,6,6,7,7,7-heptafluoro-3-hepten-2-one","70168-24-0","D",0]
["Perfluoro-15-(pentafluoro-lambda6-sulfanyl)pentadecanoic acid","","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-(pentyloxy)hexane","1193009-96-9","D",0]
["Perfluoromethylpropyl-(methylcyclopentyl)-amine","444658-71-3","D",0]
["1-Iodo-4-(tridecafluorohexyl)benzene","162083-76-3","D",0]
["3-Chloro-1,1,1,2,2-pentafluoro-3-(1,1,2,2-tetrafluoroethoxy)propane","50807-73-3","D",0]
["N-(5-Amino-1H-1,2,4-triazole-3-yl)-2,2,3,3,4,4,4-heptafluorobutanamide","80616-59-7","D",0]
["8:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["1H-Perfluoroethanesulfonic acid","20705-83-3","D",0]
["Phosphonic acid, P-[[4-[[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-buten-1-yl]","332392-54-8","D",0]
["1,1,1,4,4,5,5,5-Octafluoropentane","142347-19-1","D",0]
["4-(Heptafluoropropylthio)aniline","172961-00-1","D",0]
["3-(Heptafluoropropyl)-6-(morpholin-4-yl)[1,2,4]triazolo[4,3-b]pyridazine","296886-61-8","D",0]
["Ethyl 2,3,4,4,4-pentafluorobut-2-enoate","20578-74-9","D",0]
["2-Bromo-5-(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-enoxy)benzene-1,4-diamine","","D",0]
["4,4,5,5,6,6,6-Heptafluorohex-1-ene","2317-84-2","D",0]
["2,2,3,3-Tetrafluoropropyl hypochlorite","76453-03-7","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl (3b,5b,20R)-3-[(trifluoroacetyl)oxy]cholan-24-oate","","D",0]
["2,2,3,3,4,4-Hexafluoropentanedioate","1118431-94-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-N-(3-methoxyphenyl)heptanamide","904565-42-0","D",0]
["4-[(Perfluorooctyl)sulfonyl]-1-(2-hydroxyethyl)-1-methylpiperazinium bromide","91707-64-1","D",0]
["Ethyl 2-(heptafluoropropyl)-4-methylpyrimidine-5-carboxylate","887407-58-1","D",0]
["N,N′-[Phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-perfluoro-1-tetradecanesulfonamide] ammonium salt","118337-78-3","D",0]
["N-[5-[[[2-Bromo-6-chloro-4-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]phenyl]amino]carbonyl]-2-cyanophenyl]-4-cyano-2-methylbenzamide","1254782-06-3","D",0]
["1-Nitro-3-(pentafluoroethyl)benzene","656-84-8","D",0]
["1-[(3S,4R)-3-hydroxy-2,2-dimethyl-6-(1,1,2,2,2-pentafluoroethyl)-3,4-dihydrochromen-4-yl]piperidin-2-one","131899-25-7","D",0]
["3,3,4,4,5,5,6,6,7,7-Decafluorooctan-1-amine","860804-22-4","D",0]
["1,1-Dichloro-5,5,5-trifluoro-4-(trifluoromethyl)penta-1,3-diene","99903-40-9","D",0]
["Potassium N-methyl perfluorohexane sulfonamide","","D",0]
["Perfluoro-3-sulfopropanoic acid","83071-04-9","D",0]
["Perfluoroheptanoate","120885-29-2","D",0]
["6:2/8:2 Fluorotelomer phosphate diester","943913-15-3","D",0]
["1,2-dibromo-1,2,3,3,3-pentafluoro-1-(2,2,2-trifluoroethoxy)propane","396716-52-2","D",0]
["12:2 Fluorotelomer carboxylic acid","70887-93-3","D",0]
["3-[4-[1-[4-(1,1,2,2,2-Pentafluoroethoxy)phenyl]-1,2,4-triazol-3-yl]phenyl]propanoic acid","","D",0]
["Iodonium, (1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)phenyl-, 1,1,1-trifluoromethanesulfonate (1:1)","77758-89-5","D",0]
["Perfluorododecanedioic acid","865-85-0","D",0]
["Heptadecafluorooctan-1-ol","114292-89-6","D",0]
["(4-Bromo-3,3,4,4-tetrafluoro-1-iodobutyl)(trimethyl)silane","89608-33-3","D",0]
["1-Methyl-4-(1,2,3,3,3-pentafluoroprop-1-en-1-yl)benzene","61855-63-8","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium sulfate (1:1)","153968-01-5","D",0]
["1-(2-Bromo-1,1,2,2-tetrafluoroethyl)octahydro-4-iodopentalene","147297-42-5","D",0]
["6,7,7,7-Tetrafluoro-N-(2-hydroxyethyl)-4-[2,3,3,3-tetrafluoro-2-(trifluoromethyl)propyl]-6-(trifluoromethyl)heptane-1-sulfonamide","","D",0]
["Perfluoro-6-octene-1-sulfonic acid","2089109-43-1","D",0]
["1,1,1,2,3,3,3-Heptafluoro-2-isocyanatopropane","34556-41-7","D",0]
["N-Alkyl perfluoroalkyl sulfonamidoethanols","","D",0]
["3-[(3-{Ethyl[(perfluoroheptyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["3-[(Perfluorononanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["1-(Chlorosulfanyl)-1,1,2,2,2-pentafluoroethane","39937-11-6","D",0]
["2-chloro-2,3,3,3-tetrafluoropropanoyl bromide","261503-70-2","D",0]
["HFC-245ca","679-86-7","D",0]
["N,N-Diethyl-N-[3-[[(perfluorooctyl)sulfonyl]amino]propyl]tetrahydro-2H-pyran-4-aminium ethyl sulfate (1:1)","121912-23-0","D",0]
["Potassium 1,1,2,2-tetrafluoro-2-{[1,1,1,2,3,3-hexafluoro-3-(pentafluoroethoxy)propan-2-yl]oxy}ethane-1-sulfonate","70755-50-9","D",0]
["2:2 Fluorotelomer sulfonamido propyl methyl amine","","D",0]
["2‐[Dimethyl(4-fluoro-4-(perfluoroundecyl)‐2‐hydroxybut‐3‐en‐1‐yl)azaniumyl]acetate","","D",0]
["Perfluoro-7-oxooctane-1-sulfonic acid","1651215-27-8","D",0]
["2,3-Difluoro-4-[(5,5,6,6,7,7,8,8,8-nonafluorooctyl)oxy]benzoic acid","668989-63-7","D",0]
["2-{2-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]ethoxy}ethan-1-ol","104568-29-8","D",0]
["1,3-Isobenzofurandione, polymer with dihydro-2,5-furandione and 2-(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl)oxirane","1023888-52-9","D",0]
["2:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["3-(Perfluorohexyl)‐1‐[(2‐hydroxyacetyl)sulfanyl]propan‐1‐one","","D",0]
["2,2,2',3,3,3',4,4,4',5,5,5',6,6'-Tetradecafluoro-2,3,4,5-tetrahydro-1,1'-biphenyl","5492-89-7","D",0]
["2-{2-[2-(2,2,3,3,3-Pentafluoropropoxy)ethoxy]ethoxy}ethan-1-ol","63693-17-4","D",0]
["1,1,2,2,3,4,4,5,5,6-Decafluorocyclohexane","2692-00-4","D",0]
["1,3-Propanediamine, N,N-dimethyl-, compd. with .alpha.-fluoro-.omega.-[2-(phosphonooxy)ethyl]poly(difluoromethylene) (1:1)","65530-80-5","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol, reduced","161212-10-8","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2,2,3,3,4,4,4-heptafluorobutyl)butan-1-amine","356-08-1","D",0]
["6-Chloro-3,3,4,4,5,5,6,6-octafluorohexan-1-ol","131118-30-4","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorooctyl)-2-fluoroethan-1-aminium","","D",0]
["Ethyl 2-(heptafluoropropyl)benzoate","1310492-25-1","D",0]
["1-Nitro-4-(pentafluoroethyl)benzene","60979-14-8","D",0]
["1,1,2,2-Tetrafluoro-2-(1,1,2,2-tetrafluoroethoxy)ethane-1-sulfonamide","144951-90-6","D",0]
["1,1,1,2,2-Pentafluoropentan-3-yl carbonate","277332-96-4","D",0]
["1-Methylnonafluorocyclohexene","647-53-0","D",0]
["(4S,5R)-4-Benzyl-5-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)-1,3-oxazolidin-2-one","857637-92-4","D",0]
["Pentadecafluoroheptyl dihydrogen phosphate","45294-90-4","D",0]
["3-[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propane-2-sulfonyl]aniline","68596-42-9","D",0]
["3‐[N‐(3‐{[2‐(2‐Hydroxyethoxy)ethyl]dimethylazaniumyl}propyl)perfluorohexanesulfonamido]propane‐1‐sulfonate","38850-57-6","D",0]
["3-(2,2,3,3,4,4,4-Heptafluorobutoxy)propane-1,2-diol","25385-72-2","D",0]
["2,6-Difluoro-3,5-bis(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyrazine","55827-95-7","D",0]
["1-(Tridecafluorohexyl)bicyclo[2.2.1]hept-2-ene","116087-09-3","D",0]
["N-Methyl-N-[(perfluorobutyl)sulfonyl]glycine","159381-10-9","D",0]
["3,3,4,4-Tetrafluorotricyclo[4.2.1.0(2,5)]non-7-ene","6654-42-8","D",0]
["6-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1H-benzotriazole","1433216-34-2","D",0]
["N-Ethyl-N-[3-(triethoxysilyl)propyl]-perfluoro-1-octanesulfonamide","127193-07-1","D",0]
["Methacrylic acid, 2-(diethylamino)ethyl ester, polymer with butyl methacrylate and 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl acrylate","34482-04-7","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-1-iodooct-1-ene","150223-14-6","D",0]
["1,2,3,3,3-Pentafluoro-1-(trifluoromethoxy)prop-1-ene","137741-09-4","D",0]
["3-[(3-{[(Perfluorotridecyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["4-{[(Prop-2-yn-1-yl)oxy]methyl}-2,2-bis(trifluoromethyl)-1,3-dioxolane","51125-54-3","D",0]
["2-Propenoic acid, 2-chloro-, 3,3,4,4,5,5,6,6,6-nonafluorohexyl ester, telomer with chloroethene, 3-chloro-2-hydroxypropyl 2-methyl-2-propenoate, 1-dodecanethiol, N-(hydroxymethyl)-2-propenamide and octadecyl 2-propenoate","1331869-23-8","D",0]
["Octadecanoic acid, esters, ethenyl ester, polymer with .alpha.-ethenyl-.omega.-fluoropoly(difluoromethylene)","113656-32-9","D",0]
["8:2 Fluorotelomer sulfonamido N,N-dimethyl amine ion","1383438-87-6","D",0]
["1,1,2,3,4,5,5,5-Octafluoro-1-iodo-4-(trifluoromethyl)-2-pentene","96288-51-6","D",0]
["9-(Perfluoromethoxy)perfluorononane sulfonic acid","","D",0]
["Butenedioic acid, (Z)-, dioctyl-, copolymer with poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-((1-oxo-2-propenyl)oxy)ethyl)chloroethylene","374928-92-4","D",0]
["Propanoic acid, 3-hydroxy-2-(hydroxymethyl)-2-methyl-, polymer with 1,1'-methylenebis[4-isocyanatobenzene] and 1,2,3-propanetriol, reaction products with N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-1-octanesulfonamide and","306975-57-5","D",0]
["5‐(Dimethylamino)‐1,1,1,2,2‐pentafluoro‐4‐(hydroxymethoxy)pentan‐3‐yl formate","","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(4-phenylphenyl)utanamide","75042-06-7","D",0]
["2:2 Fluorotelomer sulfate","","D",0]
["Nonafluoropentanoic acid - 1-benzylthiourea (1:1)","64808-55-5","D",0]
["Octanoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, ethyl ester","153296-01-6","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluorodecanesulfonyl)amino]propan-1-aminium","","D",0]
["3,3′-(Perfluoro-1-cyclopentene-1,2-diyl)bis(2,5-dimethylthiophene)","190394-25-3","D",0]
["Ethanesulfinamide, 1,1,2,2,2-pentafluoro-N-phenyl-","61424-46-2","D",0]
["Ethyl 3,4,4,4-tetrafluoro-2-oxo-3-(trifluoromethyl)butanoate","74405-85-9","D",0]
["1,1,2,2,3,9,9,9‐Octafluorononane‐1‐sulfonate","","D",0]
["Tridecanoic acid, 12,12,13,13,13-pentafluoro-","1427-85-6","D",0]
["(2E)-1,1,1,2,3,4,4,5,5,6,6,6-Dodecafluorohex-2-ene","67899-37-0","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(piperidin-1-yl)butan-1-one","425-19-4","D",0]
["Sodium 3-hydroxy-4-[(perfluoro-1-oxododecyl)amino]-1-naphthalenesulfonate","63367-18-0","D",0]
["Butanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[2,2,3,3,4,4,4-heptafluoro- (9CI)","548436-10-8","D",0]
["3-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononyl)-4-(iodomethyl)oxolane","131771-31-8","D",0]
["(Pentadecafluoroheptyl)benzene","1548-88-5","D",0]
["Diethyl 1,1,1,2,2,3-hexafluorooct-3-en-4-yl phosphate","113138-44-6","D",0]
["6:2 Fluorotelomer thioether propanoyl alanine","","D",0]
["Undecafluoropiperidine","836-77-1","D",0]
["1,1,2,2,2-Pentafluoro-N-(trifluoromethyl)ethan-1-amine","428-72-8","D",0]
["1,1,1,2,2-Pentachloro-3,3,4,4,5,5,5-heptafluoropentane","116046-22-1","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)-1-propanol","81503-71-1","D",0]
["N-Ethyl-N-[2-(phosphonooxy)ethyl]perfluorodecanesulfonamide","61481-05-8","D",0]
["1,2,3-Tris(1,1,2,2,2-pentafluoroethoxy)benzene","52999-44-7","D",0]
["1,1,1,2,5,5,5-Heptafluoro-4-iodo-2-(trifluoromethyl)pentane","922523-98-6","D",0]
["4-[(2,2,3,3-Tetrafluoropropyl)sulfanyl]benzene-1,2-diamine","54029-84-4","D",0]
["Iodonium, (1,1,2,2,3,3,3-heptafluoropropyl)phenyl-, 1,1,1-trifluoromethanesulfonate (1:1)","77758-79-3","D",0]
["1-Undecanaminium, N-(3-carboxypropyl)-N,N-dimethyl-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-, hydroxide, inner salt","145441-33-4","D",0]
["3-(2,2,3,3,3-Pentafluoro-propoxy)-benzaldehyde","","D",0]
["3-(Difluoromethoxy)-1,1,1,2,2,3-hexafluoropropane","60598-11-0","D",0]
["2-(1,1-Diethoxy-2,2,3,3,4,4,4-heptafluorobutyl)benzenamine","181059-80-3","D",0]
["1,1,1,3,3,4,4,4-Octafluoro-2-(trifluoromethyl)-2-butanol","6188-98-3","D",0]
["1,2,3,4,5-Pentafluoro-6-(2,2,3,3-tetrafluoropropoxy)benzene","89847-87-0","D",0]
["Tribromo(heptafluoropropyl)germane","404339-64-6","D",0]
["3-Amino-3-[3-(1,1,2,2-tetrafluoroethoxy)phenyl]propanoic acid","773122-81-9","D",0]
["4-Chloro-5-methyl-3-(perfluoropentyl)pyrazole","247220-87-7","D",0]
["Cesium perfluoroheptanoate","171198-24-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoroundecane","1287702-48-0","D",0]
["2,6-Difluoro-N-(((3-methyl-4-((1,1,2,2-tetrafluoroethyl)thio)phenyl)amino)carbonyl)benzamide","100279-14-9","D",0]
["2-(Heptafluoropropyl)-1H-benzimidazole","559-37-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluoropentacosane","116177-47-0","D",0]
["1-(Chlorosulfanyl)-1,1,2,2,3,3,3-heptafluoropropane","662-42-0","D",0]
["(Perfluorobutanamido)-3-betaine","2024609-79-6","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[(3-sulfopropyl)(perfluorohexane-1-sulfonyl)amino]propan-1-aminium","2267980-92-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Pentadecafluoro-2,2-dimethylnonanal","56778-57-5","D",0]
["1-Methyl-2-{2-[1-methyl-5-(pentafluoroethyl)-1H-imidazol-2-yl]ethenyl}-4-(pentafluoroethyl)-1H-imidazole","141363-32-8","D",0]
["Ethyl 2-chlorotetrafluoropropionate","5829-03-8","D",0]
["2,4-Bis[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoronon-1-en-1-yl)oxy]benzene-1-sulfonyl chloride","62623-17-0","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl]-ω-hydroxy-","63336-01-6","D",0]
["Lithium 4:2 fluorotelomer thioether propionate","1254255-45-2","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-5-octadecene","160460-03-7","D",0]
["1-Bromoperfluoro-2,5,8-trioxadodecane","330562-47-5","D",0]
["4,4,5,5,5-Pentafluoro-2-(trifluoromethyl)pent-1-ene","90277-98-8","D",0]
["(6E)-1,1,1,2,2,3,3,10,10,11,11,12,12,12-Tetradecafluoro-4,4,9,9-tetrakis(trifluoromethyl)dodec-6-ene","1946796-71-9","D",0]
["Hexacosafluorohexadecahydrofluoranthene","662-28-2","D",0]
["Triethoxy(1,1,2,2,3,3,4,4,5,5,8,8,8-tridecafluorooctyl)silane","125607-98-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Hexadecafluorononanoyl bromide","1404194-04-2","D",0]
["1-Nitro-3-(undecafluoropentyl)benzene","1463530-16-6","D",0]
["Phosphonic acid, bis(2,2,3,3-tetrafluoropropyl) ester","65611-25-8","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2,6-dimethylaniline","273735-43-6","D",0]
["1,1,2,2-Tetrafluoro-5-(methylamino)hex-4-en-3-one","92676-68-1","D",0]
["1-Methyl-2-(tridecafluorohexyl)-1H-pyrrole","64435-67-2","D",0]
["1,10-Phenanthroline, 5,5,6,6-tetrafluoro-5,6-dihydro-","134023-58-8","D",0]
["3-(Triethoxysilyl)propyl heptafluorobutanoate","36957-50-3","D",0]
["14:2 Fluorotelomer thioether amido sulfonic acid","1513864-08-8","D",0]
["Perfluorododecanesulfonate","343629-43-6","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorotridecanamido)propan-1-aminium","1513863-87-0","D",0]
["Poly(oxy-1,2-ethanediyl), α-methyl-ω-[(nonadecafluorodecenyl)oxy]-","37382-56-2","D",0]
["5-Decyl-2-[4-(2,2,3,3,4,4,4-heptafluorobutoxy)phenyl]pyrimidine","141550-25-6","D",0]
["2,2,3,3,5,5,6-Heptafluoro-6-iodo-1,4-dioxane","61448-93-9","D",0]
["2,3,3,3-Tetrafluoropropanoyl bromide","61444-66-4","D",0]
["5-(1,1,2,2,2-pentafluoroethyl)-1H-1,2,4-triazol-3-amine","25979-01-5","D",0]
["3-(Nonafluorobutyl)-1H-indole","1608112-33-9","D",0]
["1,2-bis[bromo(difluoro)methoxy]-1,1,2,2-tetrafluoroethane","330562-48-6","D",0]
["2,2-Dimethyl-1,3-bis(1,1,2,2-tetrafluoroethoxy)propane","757-15-3","D",0]
["Butyl perfluorobutanoate","1559-07-5","D",0]
["2-(4-Chloro-1,1,2,2,3,3,4,4-octafluorobutyl)-1H-pyrrole","110396-62-8","D",0]
["Z-bis(perfluoro-n-hexyl)-1,2-ethylene","97539-77-0","D",0]
["2-[[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluorooctyl)oxy]methyl]oxirane","748-35-6","D",0]
["1-(5-Chlorothiophen-2-yl)-4,4,5,5,6,6,6-heptafluorohexane-1,3-dione","326-08-9","D",0]
["Decanoic acid, 2,2,3,3,4,4,5,5-octafluoropentyl ester","18798-10-2","D",0]
["{(2-Carboxyethyl)[(perfluorodecyl)sulfonyl]amino}-3-betaine","","D",0]
["9:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["2-Fluoro-3-(4-fluoro-2-nitrobenzamido)-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","862133-14-0","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-(pentafluoroethoxy)butane","71546-78-6","D",0]
["1-(Ethylamino)-3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctan-2-ol","89807-91-0","D",0]
["Perfluoro-10-(pentafluoro-lambda6-sulfanyl)decanoic acid","","D",0]
["2,3,3,4,4,5,5,6,6,7,7,7-Dodecafluoro-2-hydroxyheptanoic acid","93682-62-3","D",0]
["N-Butyl-perfluorobutanesulfonamide","864069-33-0","D",0]
["Sodium tetrakis[3,5-bis(1,1,1,3,3,3-hexafluoro-2-methoxypropan-2-yl)phenyl]borate(1-)--water (1/1/3)","120945-63-3","D",0]
["7:2 sFluorotelomer alcohol","24015-83-6","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl propanoate","914637-41-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Nonadecafluorononacosane","117948-75-1","D",0]
["10-Bromo-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluorodecane","181997-60-4","D",0]
["2-Cyanoethyl 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl N,N-dipropan-2-ylphosphoramidoite","1036029-24-9","D",0]
["4,4,5,5,6,6-Hexafluorohex-2-ynoic acid","110680-66-5","D",0]
["1-(Prop-1-en-2-yl)-4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-tricosafluorododec-1-en-1-yl)oxy]benzene","112242-89-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptanimidamide","25264-81-7","D",0]
["2,3-Bis(1,1,1,2,3,3-hexafluoropropan-2-yl)but-2-enedioate","208186-76-9","D",0]
["3,4,5-Tris(1,1,2,3,3,3-hexafluoropropoxy)benzenesulfonic acid","75860-17-2","D",0]
["1,2-Dihydro-5-(tridecafluorohexyl)-3H-1,2,4-triazole-3-thione","162466-06-0","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoro-, sodium salt (1:1)","245331-40-2","D",0]
["4-(Dimethylamino)-2-{[(perfluoroundecyl)sulfonyl]amino}butanoic acid","","D",0]
["Sodium 2,2,3,3-tetrafluoro-3-(heptafluoropropoxy)propanoate","79630-80-1","D",0]
["Hexafluoro(2,2,2-trifluoroethylidene)cyclobutane","61898-37-1","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reduced, reaction products with propylene oxide","161075-10-1","D",0]
["4'-Butyl-3-(6,6,7,7,8,8,9,9,9-nonafluorononyl)-2,2'-bithiophene","919079-94-0","D",0]
["2-Propenoic acid, 2-methyl-, decyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate","1040208-92-1","D",0]
["beta-Alanine, N-ethyl-N-[(heptadecafluorooctyl)sulfonyl]-, ethenyl ester","77073-84-8","D",0]
["2-{Difluoro[(pentadecafluoroheptyl)oxy]methyl}-2,3,3-trifluorooxirane","596807-60-2","D",0]
["(2,2,3,3,4,4,5,5-Octafluoropentyl)propanedinitrile","771561-37-6","D",0]
["Methyl perfluorohexadecanoate","165457-57-8","D",0]
["Perfluoro-2-[(trifluoromethyl)sulfonyl]propane","207129-45-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-iodoheptadecane","207122-01-8","D",0]
["3,3,3-Trifluoro-2-({[1,1,1-trifluoro-2-(trifluoromethyl)butan-2-yl]oxy}carbonyl)propanoate","62935-41-5","D",0]
["1-(4-bromophenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-one","35444-01-0","D",0]
["N-(2-Hydroxyethyl)-N-methyl-N-(3-sulfopropyl)-3-[[(perfluoropentyl)sulfonyl]amino]-1-propanaminium","2089108-75-6","D",0]
["N-(3-{(Carboxymethyl)[(perfluorododecyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["5-Phenyl-3,3-bis(trifluoromethyl)-3H-1,2,4-dithiazole","55015-72-0","D",0]
["3,4,4-Trifluoro-3-(nonafluorobutyl)-1,2lambda~6~-oxathietane-2,2-dione","85211-95-6","D",0]
["2,2,3,3,4,4,5,5-Octafluorohexane-1,6-diyl bis(2-methylprop-2-enoate)","66818-54-0","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluoro-2-hydroxy-N,N~2~-dimethylnorleucinamide","107070-94-0","D",0]
["(6-Carboxy-perfluorohexyl)pentafluorosulfur","2269495-18-1","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reaction products with ammonia, reduced","161075-05-4","D",0]
["3,4,4,4-Tetrafluoro-3-(heptafluoropropoxy)but-1-ene","131628-34-7","D",0]
["Bis(2,3,3,5,5,6,6-heptafluoro-1,4-dioxan-2-yl)mercury","61479-65-0","D",0]
["flubendiamide","272451-65-7","D",0]
["4,7-Methanoisobenzofuran-1,3-dione, hexahydro-5-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]-, (3aα,4α,5α,7α,7aα)-","62731-90-2","D",0]
["N-Ethyl-3-{ethyl[(perfluorooctyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["Copolymer of 2,3,3,3-tetrafluoro-2-{1,1,2,3,3,3-hexafluoro-2-(1,1,2-trifluoroallyl)oxypropoxy}propan-1-ol, 2,3,3,3-tetrafluoro-2-{1,1,2,3,3,3-hexafluoro-2-(1,1,2-trifluoroallyl)oxypropoxy}propan-1-yl 2-fluoroacrylate","1621858-40-9","D",0]
["Copolymer of octadecyl acrylate, 1,1-dichloroethene, 2,3-epoxypropyl methacrylate, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl methacrylate, 2-hydroxyethyl methacrylate","1620400-25-0","D",0]
["6-Chloro-1,1,1,2,2,3,3,4,4-nonafluoro-5-iodohexane","113419-03-7","D",0]
["14:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["4:2 Fluorotelomer sulfide (1-methanol 2-methanol) propanoate","","D",0]
["1-Bromo-1,1,2,3,3,3-hexafluoropropane","2252-78-0","D",0]
["Diphenyl(2,4,6-trimethylphenyl)sulfonium perfluoro-1-octanesulfonate","258341-99-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,35,35,36,36,37,37,38,38,39,39,40,40,41,41,42,42,43,43,44,44,45,45,46,46,46-Pentacontafluorohexatetracontane","114221-79-3","D",0]
["Sodium 2-hydroxy-3-[[(perfluorobutyl)sulfonyl](propyl)amino]propanesulfonate","864069-40-9","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(heptafluoropropoxy)propane","356-62-7","D",0]
["1‐(Dimethylamino)‐3-(perfluorooctyl)‐2‐(hydroxymethoxy)propan‐3‐yl formate","","D",0]
["Bis(perfluoroethyl)phosphinic acid","103321-11-5","D",0]
["1-(Perfluoro-n-octyl)tetradecane","133310-72-2","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorotridecane-1-sulfonamide","","D",0]
["Perfluoroadipoyl chloride","336-06-1","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-1-phenylpentan-1-one","308-27-0","D",0]
["2-Ethoxy-3,3,4,4,5-pentafluorotetrahydro-2,5-bis[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-furan","920979-28-8","D",0]
["1,1,1,2,3,3-Hexafluoro-3-(trichloromethoxy)propane","56860-83-4","D",0]
["2,2,3,3,4,5,5,5-octafluoro-4-(trifluoromethyl)pentanoic acid","15899-28-2","D",0]
["4,4-Diethoxy-1,1,1-trifluoro-2-(trifluoromethyl)but-2-ene","99903-42-1","D",0]
["2-Methylpropenoate, ethyleneimine-, copolymer with benzyl-2-methylpropenoate and poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-((1-oxo-2-propenyl)oxy)ethyl)","220713-37-1","D",0]
["Pentanoic acid, 2,2,3,3,4,4,5,5,5-nonafluoro-, methyl ester","13038-26-1","D",0]
["3-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)propyl prop-2-enoate","866396-85-2","D",0]
["(1,1,1,2,3,3,4,5,5,5-Decafluoropentan-2-yl)benzene","89185-51-3","D",0]
["4-Chloro-N-(1,1,1,3,3,3-hexafluoropropan-2-ylidene)benzamide","52786-52-4","D",0]
["2‐Hydroxy‐3‐[(4,4,5,5,6,6,7,7,7‐nonafluoroheptanoyl)sulfanyl]‐3‐oxopropanoic acid","","D",0]
["3,3-Bis(trifluoromethyl)bicyclo[2.2.1]heptane-2,2-dicarbonitrile","82947-63-5","D",0]
["4-Bromo-2,3,3,4,5,5,6,6-octafluoro-1-(trifluoromethyl)cyclohex-1-ene","87911-17-9","D",0]
["2,2,3,3-Tetrafluorospiro[3.5]nonan-1-one","144194-03-6","D",0]
["Ethyl 4,4,4-trifluoro-3-(trifluoromethyl)crotonate","1513-60-6","D",0]
["4-(Dimethylamino)-2-{[(perfluoropentyl)sulfonyl]amino}butanoic acid","2089109-97-5","D",0]
["Ethyl 2-acetyl-4,4,4-trifluoro-3-hydroxy-3-(trifluoromethyl)butanoate","680-09-1","D",0]
["1,1,1,2,2,3,3-heptafluoro-8-methylnonane-4,6-dione","6304-28-5","D",0]
["Sodium perfluorododecanoate","60872-01-7","D",0]
["Perfluoro-2-propyl 2H-perfluoro-1-propyl ether","25352-92-5","D",0]
["Phosphonic acid, P-[3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]butyl]-, diethyl ester","1198296-49-9","D",0]
["(2Z,4Z)-Perfluoro-2,4-hexadiene","83168-65-4","D",0]
["Perfluoro-3-butylcyclopentane-1-sulfonic acid","","D",0]
["6-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]hexanoic acid","522634-15-7","D",0]
["Cyclohexanecarboxamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[1,2,2,3,3,4,4,5,5,6,6-undecafluoro- (9CI)","548470-06-0","D",0]
["3,3,4,4,5,5,6,6-Octafluoro-1,8-octanediol","83192-87-4","D",0]
["N-Ethyl-3-{ethyl[(perfluorohexyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["3‐[2-(Perfluorooctyl)ethylsulfanyl]‐3‐hydroxypropanoic acid","","D",0]
["3-(Dimethyl{3-[(pentafluoroethanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["Methyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctanoate","70887-85-3","D",0]
["1-(Dimethylamino)-3-(perfluorododecyl)propan-2-ol","80234-00-0","D",0]
["4-(2,2,3,3-Tetrafluoropropoxy)benzonitrile","87014-39-9","D",0]
["2-[(1,2,3,3,4,4,4-Heptafluorobut-1-en-1-yl)sulfanyl]ethan-1-ol","112783-42-3","D",0]
["2-(Difluoromethyl)-1,1,1,3,3,3-hexafluoropropane","382-20-7","D",0]
["(Pyridin-3-yl)[4-(1,2,2,2-tetrafluoroethoxy)phenyl]methanone","61547-45-3","D",0]
["N-Methyl-3-(4,4,5,5,5-pentafluoropentylsulfinyl)propan-1-amine","","D",0]
["9-Octadecenoic acid (Z)-, reaction products with N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-1-octanesulfonamide","185630-90-4","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecan-2-ol","70616-99-8","D",0]
["4,4,5,5,5-Pentafluoropent-2-ynenitrile","81850-46-6","D",0]
["Ethyl 4-(1,1,2,2-tetrafluoroethoxy)benzoate","37178-69-1","D",0]
["Ethyl 5-(2,2,3,3,4,4,4-heptafluorobutanamido)-1-phenyl-1H-pyrazole-4-carboxylate","545359-89-5","D",0]
["4,4,4-Trifluoro-3-hydroxy-3-(trifluoromethyl)butanenitrile","2546-63-6","D",0]
["2,3,3,3-Tetrafluoropropanoyl fluoride","6065-84-5","D",0]
["1-Acetyl-6-(1,1,1,2,3,3,3-heptafluoro-2-propanyl)-3-{[(2,6-14C2)-3-pyridinylmethyl]amino}-3,4-dihydro-2(1H)-quinazolinone","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(tridecafluorohexyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["1-Chloro-perfluoroundecane-1-sulfonic acid","","D",0]
["N-[{[2,3-Dichloro-4-(1,1,2,2-tetrafluoroethanesulfinyl)phenyl]imino}(hydroxy)methyl]-2,6-difluorobenzene-1-carboximidic acid","100342-02-7","D",0]
["Pentadecafluoroadamantan-1-ol","160823-57-4","D",0]
["Ethyl 2,3,3,3-tetrafluoro-2-(trifluoromethyl)propanoate","1526-49-4","D",0]
["1,3-Benzenediamine, 4-(1,1,2,2-tetrafluoroethoxy)-","61988-37-2","D",0]
["(2,2-Dichloro-1,1,2-trifluoroethoxy)(difluoro)acetyl fluoride","83865-23-0","D",0]
["Acetic acid--3,3,4,5,5,5-hexafluoropentan-2-ol (1/1)","29338-35-0","D",0]
["Bis(trifluoromethyl)thioketene","7445-60-5","D",0]
["N,N,N-Trimethyl-3-[(perfluoro-1-oxoheptyl)amino]-1-propanaminium iodide","1428745-70-3","D",0]
["2-(Pentafluoroethyl)pyrimidin-5-amine","1936554-56-1","D",0]
["Sodium 1H,1H,2H,2H-perfluorodecylphosphate","130771-95-8","D",0]
["N-Ethyl-heptadecafluoro-N-2-propynyl-1-octanesulfonamide","87988-63-4","D",0]
["CYCLOPROPANECARBOXYLIC ACID, 2,2-DIMETHY","103833-18-7","D",0]
["Perfluoroethyl ether","358-21-4","D",0]
["2-{[(8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-Heptadecafluoro-2,2-dimethylpentadecan-5-yl)oxy]carbonyl}hydrazine-1-carboxylate","821806-48-8","D",0]
["2-chloro-N-(2-ethylphenyl)-2,3,3,3-tetrafluoropropanamide","5575-36-0","D",0]
["N-Ethyl-2,2,3,3,4,4,5,5,5-nonafluoropentanamide","158018-93-0","D",0]
["(3Z)-1,1,1,7,7,7-Hexafluoro-2,6-bis(trifluoromethyl)hept-3-ene-2,6-diol","16202-98-5","D",0]
["Perfluorodecane sulfonic anhydride","51667-62-0","D",0]
["Alcohols, C3-12, .beta.-.omega.-perfluoro-.omega.-hydro, sodium salts","68526-97-6","D",0]
["3-O-Pentafluoropropionyl cholesterol","66997-77-1","D",0]
["(1R,2S)-1,2-Dichloro-1,2,3,3,4,4-hexafluorocyclobutane","3934-26-7","D",0]
["Ethylammonium perfluoro-6-(trifluoromethyl)heptanoate","54785-06-7","D",0]
["1,1'-(1,1,2,2-Tetrafluoroethane-1,2-diyl)bis(2-bromobenzene)","61547-73-7","D",0]
["2-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)-1-phenylethan-1-one","58510-75-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-propoxyoctane","1193010-01-3","D",0]
["3,6,9,12-Tetraoxapentadecanoyl fluoride, 2,4,4,5,7,7,8,10,10,11,13,13,14,14,15,15,15-heptadecafluoro-2,5,8,11-tetrakis(trifluoromethyl)-","34761-47-2","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, 3-pyridinyl ester","32848-20-7","D",0]
["Perfluorobutanesulfinyl chloride","41006-41-1","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-N,N-dimethylaniline","2396-19-2","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8-Dodecafluorooctan-1-ol","800382-22-3","D",0]
["1,1,2,2,3,3,4,5,5,6,6,7,7,7-tetradecafluoro-4-(trifluoromethyl)heptane-1-sulfonic acid","","D",0]
["1-Chloro-3,3,4,4,5,5,6,6-octafluoro-2-iodocyclohex-1-ene","19614-62-1","D",0]
["3-[[(Perfluoropropyl)sulfonyl](2-hydroxyethyl)amino]-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","2089108-98-3","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, 2,3-dihydroxypropyl, Glycidyl 4-methoxyphenyl ethers","1664368-38-0","D",0]
["1h,1h-perfluoro-3,6,9-trioxatridecan-1-ol","317817-24-6","D",0]
["Benzyl 2,2,3,3,4,4-hexafluoro-4-iodobutanoate","188711-29-7","D",0]
["(2R,3S)-1,1,1,2,3,4,4,5,5,5-Decafluoropentane","1006614-95-4","D",0]
["(Perfluoropropyl)methyl 3-chlorobut-3-enoate","","D",0]
["1,2-Dichloro-1,1,2,3,3,4,4-heptafluorobutane","14671-64-8","D",0]
["Dichloro(2-chloro-1,1,2,2-tetrafluoroethyl)difluoro-lambda~5~-phosphane","61527-28-4","D",0]
["1,1,1,6,6,6-Hexafluoro-2,5-bis(trifluoromethyl)-2,5-hexanediol","54841-08-6","D",0]
["N-Methyl-2-[2-methyl-3,3-bis(trifluoromethyl)diaziridin-1-yl]ethan-1-amine--hydrogen chloride (1/1)","106036-82-2","D",0]
["2,2-Bis(trifluoromethyl)-1,3-dioxole","89444-43-9","D",0]
["(2S)-2-(Nonafluorobutyl)octan-1-ol","1180131-16-1","D",0]
["Ethyl 3-(butylamino)-4,4,5,5,6,6,6-heptafluorohexanoate","2802-65-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorohexacosane","93454-73-0","D",0]
["1-chloro-3,3,4,4,5,5-hexafluorocyclopentene","3761-95-3","D",0]
["(4-chlorophenyl) 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","41605-52-1","D",0]
["1,2,2,3,3,4,5,5,6-Nonafluoro-4,6-bis(trifluoromethyl)cyclohexane-1-sulfonic acid","374-58-3","D",0]
["{3‐[2‐ (2-(Perfluorodecyl)ethylsulfinyl)acetamido]propyl}trimethylazanium","","D",0]
["1H-Pyrrol-2-yl(perfluoropropyl)methanol","159355-62-1","D",0]
["1~1~,1~2~,1~2~,1~3~,1~3~,1~4~,1~4~,2~3~,2~3~,2~4~,2~4~,3~1~,3~2~,3~2~,3~3~,3~3~,3~4~,3~4~-Octadecafluoro[1~1~,2~1~:2~2~,3~1~-tercyclobutan]-2~1~-ene","55847-13-7","D",0]
["3-(Perfluorononyl)propanoic acid","","D",0]
["2H-1,4-Oxazine, 2,2,3,3,5,6,6-heptafluoro-3,6-dihydro-","4777-13-3","D",0]
["N-Butyl-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptanamide","570420-18-7","D",0]
["3-{[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl]sulfanyl}benzoic acid","88489-77-4","D",0]
["4H-1,3,2-Dithiazine, 4,4,5,5,6,6-hexafluorodihydro-, 1,1,3,3-tetraoxide","84246-29-7","D",0]
["2λ5,4λ5,6λ5-1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexakis(2,2,3,3-tetrafluoropropoxy)-","58943-98-9","D",0]
["2-[Chloro(difluoro)methoxy]-1,1,1,2-tetrafluoroethane","172103-16-1","D",0]
["Pentafluoroethyl pentafluoropropanoate","206436-41-1","D",0]
["1-Methyl-3-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-42-2","D",0]
["1-Chloro-perfluorotetradecane-1-sulfonic acid","","D",0]
["1,1,1,2,4,4,5,5-Octafluoro-5-iodo-2-(trifluoromethyl)pentan-3-one","93822-96-9","D",0]
["1-(Perfluorohexyl)hexane","69125-80-0","D",0]
["1-Chloro-1,2,2,3,3,4,5,6,7-nonafluoro-2,3-dihydro-1H-indene","52514-15-5","D",0]
["4-Amino-6-(pentafluoroethyl)benzene-1,3-disulfonamide","654-58-0","D",0]
["1,1'-[Oxybis(1,1,2,3,3,3-hexafluoropropane-1,2-diyl)]bis(4-bromo-2,6-difluorobenzene)","161045-77-8","D",0]
["2,2-Dimethyl-4,4,6-tris(trifluoromethyl)-1,5,6-triazabicyclo[3.1.0]hexane","95388-86-6","D",0]
["Decafluorohexane-2,3-dione","74728-96-4","D",0]
["4-(Tridecafluorohexyl)phenol","106877-15-0","D",0]
["1-Methylethyl perfluorobutanimidoate","4192-05-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,5-undecafluoropentyl)sulfonyl]amino]ethyl ester, polymer with octadecyl 2-propenoate and 2-propenoic acid","67906-74-5","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl carbonochloridate","108156-21-4","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexyl trifluoromethanesulfonate","168632-11-9","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluorononane-1,2-diol","107650-06-6","D",0]
["(2R,3R)-1,1,1,2,3,4,4,5,5,5-Decafluoropentane","1006614-98-7","D",0]
["1,2,2,3,3,4,4,5,5,6,7,7-Dodecafluorohept-6-ene-1-sulfonyl fluoride","84933-49-3","D",0]
["1H,1H,2H,2H-Perfluorooctanol sulfate ammonium salt","63225-56-9","D",0]
["1‐(Carboxylatomethyl)‐1‐(2‐hydroxyethyl)‐4‐[3‐(perfluorodecanamido)propyl]piperazin‐1‐ium","77864-04-1","D",0]
["2‐Hydroxy‐3‐[[3-(perfluorooctyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["Pentafluoroethylperoxy","147703-39-7","D",0]
["1,1,2,2-Tetrafluoro-3-methoxy-propane","60598-17-6","D",0]
["1-Butyl-3-methyl-2,3-dihydro-1H-imidazol-1-ium 2,2,3,3,4,4,5,5-octafluoropentyl sulfate","868850-24-2","D",0]
["Heptane, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-7-(trifluoromethoxy)-","133881-46-6","D",0]
["6-Methyl-2-(undecafluoropentyl)-1,3-benzoxazole","93416-26-3","D",0]
["3‐(2-(Perfluorodecyl)ethanesulfinyl)propanoic acid","","D",0]
["1-[7,7,7-Trifluoro-6-hydroxy-4-oxo-6-(trifluoromethyl)heptyl]pyridin-1-ium chloride","102584-03-2","D",0]
["(2Z)-4,5,5,5-Tetrafluoro-2-iodo-4-(trifluoromethyl)pent-2-en-1-ol","1006627-74-2","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl carbonochloridate","40678-17-9","D",0]
["4,4-Difluoro-1-phenyl-4-(trifluoromethoxy)butane-1,3-dione","61206-61-9","D",0]
["(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)di(4,1-phenylene) bis(2-methylprop-2-enoate)","108050-42-6","D",0]
["7,7,8,8,8-pentafluorooctan-1-ol","161981-34-6","D",0]
["1-Heptadecylperfluorooctane","871311-25-0","D",0]
["Methoxy (3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl) bis(3,3,3-trifluoropropyl) silane","608300-73-8","D",0]
["Poly[oxy(1,1,2,2,3,3-hexafluoro-1,3-propanediyl)], .alpha.-(1,1,2,2,3,3,3-heptafluoropropyl)-.omega.-(1,1,2,2,2-pentafluoroethoxy)-  (n=1-60)","105060-59-1","D",0]
["[2-Chloro-4-(pentafluoroethyl)phenyl](4-fluorophenyl)methanone","138597-07-6","D",0]
["2-Ethoxy-1,1,1,2,3,3,3-heptafluoropropane","22137-14-0","D",0]
["Poly(oxy-1,2-ethanediyl), α-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-oxodecyl)-ω-methoxy-","94797-81-6","D",0]
["1,2-Dichloro(perfluoro-1-(ethoxymethoxy)ethane)","369371-42-6","D",0]
["3-(Perfluoropentanesulfonamido)-N,N,N-trimethylpropan-1-aminium","70225-23-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,10,10,10-Heptadecafluorodecyl 2-methylprop-2-enoate","64130-99-0","D",0]
["4-(1,1,2,3,3,3-Hexafluoropropoxy)-1,1'-biphenyl","175838-51-4","D",0]
["Silver (I) perfluoropentanedioate","355-85-1","D",0]
["Disulfide, bis[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]","754-62-1","D",0]
["Carbamic acid, (1-(diphenylphosphinyl)-2,2,2-trifluoro-1-(trifluoromethyl)ethyl)-, butyl ester","145430-07-5","D",0]
["2-Chloro-4,4,4-trifluoro-3-hydroxy-1-phenyl-3-(trifluoromethyl)butan-1-one","100700-42-3","D",0]
["[4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)phenyl]methanol","1137162-24-3","D",0]
["1-Icosylperfluoroheptane","1980063-56-6","D",0]
["4‐Ethyl‐1,2,2,3,3,4,5,5,6,6‐decafluorocyclohexane‐1‐sulfonate","","D",0]
["1,1,1,2,2,5,6,6,9,9,10,10,10-Tridecafluorodec-4-ene","40723-77-1","D",0]
["3-Bromo-3-chloro-1,1,1,2,2-pentafluoropropane","661-83-6","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)-, ion(1-)","122499-17-6","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[[[(heptadecafluorooctyl)sulfonyl]methylamino]carbonyl]-.omega.-butoxy-","52032-20-9","D",0]
["2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)propanimidamide","62038-10-2","D",0]
["3-[Perfluoro-2-[(methoxy)methoxy]-ethoxy]-2,2,3-trifluoropropanoic acid","919005-15-5","D",0]
["(1Z)-1,2,3,3,4,4,5,5,6,6,6-Undecafluorohex-1-ene","168332-72-7","D",0]
["N-(2-Carboxylatoethyl)-3-[(perfluoro-1-oxobutyl)amino]-N,N-dimethyl-1-propanaminium","89148-23-2","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], α-(1,1,2,2,3,3,3-heptafluoropropyl)-ω-\n[1,2,2,2-tetrafluoro-1-[[[3-(trimethoxysilyl)propyl]amino]carbonyl]ethoxy]-","220864-25-5","D",0]
["2,2,3,3-Tetrafluorobutanediimidic acid","377-37-7","D",0]
["Phosphoric acid--3,3,3-trifluoro-2-(trifluoromethyl)propan-1-ol (1/3)","64660-92-0","D",0]
["3,3,4,4,5,5,5-Heptafluoro-1-iodo-1-pentene","376-97-6","D",0]
["5-Chloro-2-(heptafluoropropyl)-6-[4-(trifluoromethyl)phenyl]-1H-1,3-benzodiazole","","D",0]
["12:2 Fluorotelomer sulfonamido propyl dimethyl amine","861642-40-2","D",0]
["4-Chloro-1,1,1-trifluoro-4-(3-nitrophenyl)-2-(trifluoromethyl)butan-2-ol","100482-44-8","D",0]
["N,N'-1,3-Phenylenebis(perfluorobutanamide)","524726-48-5","D",0]
["9-Difluoromethyl(perfluoro-1-nonyl)methyl hydrogen phosphate ammonium","1765-83-9","D",0]
["1H,1H,9H-Perfluorononyl p-toluenesulfonate","864-23-3","D",0]
["Bis(2,2,3,3-tetrafluoropropyl) ethanedioate","88055-21-4","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-6-iodoundecane","40735-33-9","D",0]
["ペルフルオロ［２－（２－エトキシエトキシ）アセチル］＝フルオリド","13071-65-3","D",0]
["2-Fluoro-1-methyl-4-(1,1,2,2,2-pentafluoroethyl)benzene","121903-59-1","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Hexadecafluoro-9-methoxynonane","112806-31-2","D",0]
["2,2,3,3,4,5-Hexafluoro-4,5-bis(trifluoromethyl)oxolane","61340-71-4","D",0]
["3-(2-Iodoethyl)-4-(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptyl)pyrrolidine-1-carbonitrile","1365808-06-5","D",0]
["Tricyclo[3.3.1.13,7]decane, hexadecafluoro-","69064-33-1","D",0]
["2-(Chloromethoxy)-1,1,1,2-tetrafluoroethane","56885-26-8","D",0]
["5-(Pentafluoroethyl)pyrimidine-2-carbonitrile","1816290-25-1","D",0]
["2-[4-[2,2-Difluoro-2-[1,1,2,2-tetrafluoro-2-(1,1,2,2,3,3,4,4,4-nonafluorobutoxy)ethoxy]ethoxy]phenyl]-5-octoxypyrimidine","","D",0]
["Poly(oxy-1,2-ethanediyl), α-(4,4,5,5,6,6,7,7,8,8,9,9,10, 10,11,11,12,12,12-nonadecafluoro-2-hydroxydodecyl)-ω-(3-hydroxypropoxy)-","94817-10-4","D",0]
["2-(Trifluoromethoxy)perfluoropropane","60901-74-8","D",0]
["1-Ethyl-3-methyl-1H-imidazol-3-ium bis(pentafluoroethanesulfonyl)azanide","216299-76-2","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl methanesulfonate","755-88-4","D",0]
["3-{[3-(Dimethylamino)propyl][(heptadecafluorooctyl)sulfonyl]amino}-2-hydroxy-1-propanesulfonic acid","793624-88-1","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Гептадекафтор-N-(2-гидроксиэтил)нонанамид","6104-17-2","D",0]
["2,4-Difluoro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-66-3","D",0]
["1,6-Bis(perfluoroethyl)hexane","1835251-86-9","D",0]
["4,4,5,5,6,6,6-heptafluoro-3-hydroxyhexanoic acid","356-31-0","D",0]
["17-Oxoestra-1,3,5(10)-trien-3-yl heptafluorobutanoate","2192-60-1","D",0]
["2-(4-Ethylamino-phenyl)-1,1,1,3,3,3-hexafluoro-propan-2-ol","65797-85-5","D",0]
["1,1,1,2,2,3,3,4,5,5,5-Undecafluoropentane","","D",0]
["Methoxy(dimethyl)(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silane","608299-03-2","D",0]
["{(Carboxymethyl)[(perfluorooctyl)sulfonyl]amino}-3-betaine","","D",0]
["Magnesium, chloro-2-propen-1-yl-, reaction products with 3-bromo-1-propene, Me esters of fluorinated reduced polymd. oxidized tetrafluoroethylene and trimethoxysilane","1644456-24-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,23,23,24,24,25,25,26,26,27,27,28,28,29,29,30,30,31,31,32,32,33,33,34,34,34-Pentacontafluorotetratriacontane","100550-10-5","D",0]
["Butyl ethyl(heptafluoropropyl)phosphinate","77529-58-9","D",0]
["2-(1,1,2,2,2-pentafluoroethoxy)phenol","60702-00-3","D",0]
["1,1'-(1,1,2,2-Tetrafluoroethane-1,2-diyl)bis(4-fluorobenzene)","4100-99-6","D",0]
["1-Iodo-1H,1H-perfluorohexane","335-50-2","D",0]
["(Carboxylatomethyl)dimethyl[(tridecafluorohexyl)butyl]azanium","2089109-29-3","D",0]
["3-(Pentafluoroethyl)aniline","710-74-7","D",0]
["6-Methoxy-5-(pentafluoroethyl)naphthalene-1-carbonitrile","112960-63-1","D",0]
["Octanoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-, compd. with ethanamine (1:1)","1376936-03-6","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-5-iodopentanoyl fluoride","62999-25-1","D",0]
["3-[Dimethyl(3-{[(perfluoroundecyl)sulfonyl]amino}propyl)ammonio]propanoate","","D",0]
["4:2 Fluorotelomer sulfonate","414911-30-1","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with ammonia","161308-16-3","D",0]
["4-Fluoro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]-3-nitrobenzamide","","D",0]
["(E)-5-((Perfluoropent-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["4,4,5,5,6,6,6‐Heptafluorohexane‐1‐sulfonic acid","","D",0]
["1-(2-Nitropropan-2-yl)-4-(1,1,2,2-tetrafluoro-2-phenylethyl)benzene","41485-24-9","D",0]
["Perfluorohexanoate","92612-52-7","D",0]
["2-Hydroxy-2-(1,1,2,2-tetrafluoroethyl)-2,3-dihydro-4H-benzo[h]chromen-4-one","5486-63-5","D",0]
["3-Chloro-perfluorotetradecanoic acid","","D",0]
["N-((2,5-Dichloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100279-18-3","D",0]
["1,2,4-Oxadiazole, 5-(pentadecafluoroheptyl)-3-phenyl-","21733-14-2","D",0]
["2-Allyloxyperfluoroethanesulfonyl fluoride","73606-13-0","D",0]
["cis-Perfluoro-1-methyl-2-ethylcyclohexane","","D",0]
["Perfluoro-4-hexene-1-sulfonic acid","2089109-41-9","D",0]
["(1R)-1-(4-Ethoxyphenyl)-2,2,3,3-tetrafluorocyclobutane-1-carboxylic acid","72370-89-9","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7-Tetradecafluoroheptan-1-ol","7098-02-4","D",0]
["4‐Oxo‐4‐[(4,4,5,5,6,6,7,7,8,8,9,9,9‐tridecafluoro‐2‐ methylnonan‐3‐yl)oxy]but‐2‐enoate","","D",0]
["1,1,1,2,2,3,3-Heptafluoro-4-(2,2,3,3,4,4,4-heptafluorobutoxy)butane","647-91-6","D",0]
["(Heptafluoropropyl)(trimethoxy)silane","129051-17-8","D",0]
["12-Chloroperfluoro-4,6,8-trimethyl-3,5,7,9-tetraoxadodecanoic acid","","D",0]
["1,1,1,2,2-Pentafluorooct-4-en-3-one","89176-01-2","D",0]
["4-{[1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propan-2-yl]sulfanyl}benzoic acid","88489-78-5","D",0]
["3-[(2-Carboxyethyl)[(perfluoropropyl)sulfonyl]amino]-N,N,N-trimethylpropanaminium","2089109-14-6","D",0]
["Lithium bis(perfluoroheptanesulfonyl)imide","1702283-75-7","D",0]
["Glycine, N-ethyl-N-[(heptadecafluorooctyl)sulfonyl]-, methyl ester","87988-69-0","D",0]
["Perfluorooctanesulfonamide potassium salt (1:1)","76752-70-0","D",0]
["5-(Perfluoroheptyl)pentanamine hydrochloride (1:1)","121912-24-1","D",0]
["N-{1-[2-(1,1,2,2-Tetrafluoro-2-phenylethyl)phenyl]ethylidene}hydroxylamine","61547-70-4","D",0]
["Poly[oxy(1,1,2,2,3,3,4,4-octafluoro-1,4-butanediyl)], .alpha.-(heptafluoropropyl)-.omega.-(heptafluoropropoxy)-","129154-21-8","D",0]
["1,1,2,2,3,3,4,4,5-Nonafluoropentane","678-73-9","D",0]
["[(Heptadecafluorooctyl)sulfanyl]acetic acid","77759-04-7","D",0]
["1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Pentadecafluorocyclooctan-1-ol","62789-53-1","D",0]
["Heptafluoroethanamine","354-80-3","D",0]
["N-Cyclohexyl-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluorononanamide","73602-46-7","D",0]
["4-(Nonafluorobutyl)benzoic acid","13835-88-6","D",0]
["2-Propenoic acid, butyl ester, polymer with 2[butyl[(heptadecafluorooctyl)sulfonyl]amino]ethyl 2-propenoate and 2-methylpropyl 2-propenoate","594864-11-6","D",0]
["4,4,5,5,6,6,6-heptafluoro-1-(5-methylthiophen-2-yl)hexane-1,3-dione","582-74-1","D",0]
["1-[(Heptadecafluorooctyl)sulfonyl]-1H-azepine","100221-82-7","D",0]
["2,6-Dichloro-3-(pentafluoroethyl)pyridine","1816287-43-0","D",0]
["2-Propenoic acid, 2-methyl-, docosyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate","1040208-71-6","D",0]
["3-[2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]-1-propene","125034-27-7","D",0]
["(2R)-3-[3-[3-(Difluoromethoxy)phenoxy]-N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]anilino]-1,1,1-trifluoropropan-2-ol","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-isocyanatooctane","142010-49-9","D",0]
["4,4-Dimethyl-3-oxo-2-[2-(2,2,3,3-tetrafluoro-2,3-dihydro-1,4-benzodioxin-6-yl)hydrazinylidene]pentanenitrile","35040-02-9","D",0]
["3-(Perfluoroisopropyl)-(2E)-difluoropropenoic acid","103229-89-6","D",0]
["5,5'-Carbonyldi(2-benzofuran-1,3-dione)--4,4'-{(1,1,1,3,3,3-hexafluoropropane-2,2-diyl)bis[(4,1-phenylene)oxy]}dianiline (1/1)","126691-33-6","D",0]
["2(1H)-Quinoxalinone, 3-(1,1,2,2,3,3,4,4-octafluorobutyl)-","89995-29-9","D",0]
["1,2,3,4,5,5,6,6-Octafluorobicyclo[2.2.2]oct-2-ene","31462-62-1","D",0]
["4,4,5,5,5‐Pentafluoro‐1‐[(2‐hydroxyacetyl)sulfanyl]pentan‐1‐one","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,12,12,12-Heptadecafluorododecylbenzene","","D",0]
["1,1,2,2-Tetrafluoro-6-methyl-2,3-dihydro-1H-indene","922141-59-1","D",0]
["2-[Decyl(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctylsulfonyl)amino]acetic acid","","D",0]
["2-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]ethyl prop-2-enoate","866208-89-1","D",0]
["N-Methyl-bis-heptafluorobutyramide","73980-71-9","D",0]
["2H-Perfluorotridecanoic acid","","D",0]
["Bis(2,2,3,3,3-pentafluoropropanoic acid)4-[(R)-2-[methyl(2,2,3,3,3-pentafluoro-1-oxopropyl)amino]-1-(2,2,3,3,3-pentafluoro-1-oxopropoxy)ethyl]-1,2-phenylene ester","59785-42-1","D",0]
["2,2,3,3,4,4-hexafluoro-1,5-diiodopentane","33619-80-6","D",0]
["12-[2-[2-(2-Methoxyethoxy)ethoxy]ethoxy]-12-[3-[(perfluoroheptyl)methoxy]propyl]-2,5,8,11,13,16,19,22-octaoxa-12-silatricosane","154380-28-6","D",0]
["4-(Nonafluorobutyl)phenol","123068-23-5","D",0]
["[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]propanedinitrile","1113-69-5","D",0]
["Hexatriacontafluorotetracosahydrocoronene","51344-02-6","D",0]
["1,1,1,4,4,4-Hexafluoro-2-iodo-2-(trifluoromethyl)butane","428-68-2","D",0]
["2-[Perfluoro-3-(propoxy)propoxy]acetic acid","919005-46-2","D",0]
["1-Propanesulfonic acid, 3-[hexyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]-2-hydroxy-, ammonium salt (1:1)","606967-06-0","D",0]
["Ammonium 2:2 fluorotelomer-1-sulfonate","945953-14-0","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(trifluoromethyl)-, methyl ester","680-05-7","D",0]
["2-Propenoic acid, 2-methyl-, dodecyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate","425664-43-3","D",0]
["1-Heptafluorobutyryloxydecane","2994-16-3","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[(2-hydroxy-3-sulfopropyl)[(perfluorohexyl)sulfonyl]amino]-1-propanaminium chloride sodium (1:1:1)","148026-37-3","D",0]
["1-(Perfluorooctyl)propene","67103-04-2","D",0]
["2-Methyl-2-[[1-oxo-3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)sulfonyl]propyl]amino]propanesulfonic acid","1911606-13-7","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluoroundecyl)sulfonyl]amino}-1-butanaminium","","D",0]
["N-[3-(Dimethylamino)propyl]perfluoro-4-(methoxy)cyclohexanecarboxamide N-oxide","200636-89-1","D",0]
["Perfluorododecanoate","171978-95-3","D",0]
["Bis[4-(tridecafluorohexyl)phenyl] diselenide","234449-42-4","D",0]
["2,2,3,3,3-Pentafluoropropyl nonafluorobutane-1-sulfonate","893556-35-9","D",0]
["A-988056","1000859-51-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-iodohexadecane","207122-00-7","D",0]
["1-Aziridinemethanol, alpha,alpha-bis(trifluoromethyl)-","773-23-9","D",0]
["1-Chloro-perfluorononane-1-sulfonic acid","","D",0]
["5‐[N‐(4‐Carboxybutyl)perfluorooctanesulfonamido]pentanoic acid","83903-90-6","D",0]
["3-[{3-[(Carboxymethyl)(perfluoropropanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluoro-1-(heptafluoropropyl)piperidine","599-06-4","D",0]
["4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Heptacosafluorotridecyl)phenol","","D",0]
["Bis(perfluoroalkyl) (linear) phosphinic acids","","D",0]
["18-(Perfluorooctyl)-17-methyl-5,8,11,14-tetraoxa-18-thia-17-azaoctadecane-1-sulfonate 18,18-dioxide sodium","166441-49-2","D",0]
["Ethenyl perfluorohexanoate","464-35-7","D",0]
["4,5,6,6,6-pentafluorohexa-1,4-diene","1730-22-9","D",0]
["13:2 Fluorotelomer carboxylic acid","","D",0]
["Perfluoro(N-iso-propylmorpholine)","1600-71-1","D",0]
["1-Nitro-3-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]benzene","59935-60-3","D",0]
["N,N-Dichloro-N',N',1,1,2,2-hexafluoro-1,2-ethanediamine","105882-88-0","D",0]
["2-(Henicosafluorodecyl)-1H-imidazole","81769-51-9","D",0]
["5,5,6,6,7,7,8,8-Octafluoro-1,3-dioxonane","36301-47-0","D",0]
["2-Perfluoroheptene","1582-32-7","D",0]
["1-Propanol, 2,3,3,3-tetrafluoro-2-[(1,1,2-trifluoro-2-propenyl)oxy]-","174082-81-6","D",0]
["1-(Perfluorodecanyl)hexadec-1-ene","1244062-18-7","D",0]
["3-[[(Perfluorodecyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","","D",0]
["Polyfluoroalkyl (C 2-5) methacrylate","59006-66-5","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluoropropyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["3,3,4,4,4-Pentafluorobutyl","1033556-26-1","D",0]
["2,2,3,3-Tetrafluoro-6-nitro-2,3-dihydro-1,4-benzodioxine","89586-09-4","D",0]
["Perfluoroalkyl (linear) dicarboxylic acids","","D",0]
["1h,1h-perfluorooctadecan-1-ol","242142-82-1","D",0]
["Perfluoro-n-[1,2,3,4-13C4]-octanoate ion(1-)","1328883-45-9","D",0]
["N-Dodecyl-heptadecafluoro-1-octanesulfonamide","75457-12-4","D",0]
["2-(2,2,3,3,4,4,4-Heptafluorobutyl)-1,3-dioxolane","175607-87-1","D",0]
["2,2-Difluoro-2-[1,1,2,2-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(trifluoromethyl)propoxy]ethoxy]ethanol","1423231-12-2","D",0]
["3,3,4,4,5,5,5-Heptafluoropentan-1-amine","1000509-29-4","D",0]
["Triethylaminium perfluoro-2-propoxypropanoate","165951-18-8","D",0]
["1,1,2,2,3,3,4-Heptafluoro-4-iodobutane","90015-83-1","D",0]
["Nonane, 1,1'-[1,5-pentanediylbis(oxy)]bis[heptadecafluoro-","84029-55-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,12,12,13,13,14,14,15,15,16,16,16-Docosafluorohexadecane","1835255-25-8","D",0]
["3-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)bicyclo[2.2.1]heptan-2-ol","101832-50-2","D",0]
["1,4,7,10,13-Pentaoxacyclopentadecane, 2,2,3,3,5,5,6,6,8,8,9,9,11,11,12,12,14,14,15,15-eicosafluoro-","97571-69-2","D",0]
["Hexanenitrile, 2,2,3,3,4,4,5,5,6,6-decafluoro-6-[(trifluoroethenyl)oxy]-, polymer with 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]propane and tetrafluoroethene, graft","709666-21-7","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-phenylhex-2-yn-1-one","89965-72-0","D",0]
["5-(Perfluoromethoxy)perfluoropentane sulfonic acid","1651215-28-9","D",0]
["Pentachlorophenyl heptafluorobutanoate","89071-46-5","D",0]
["3-[(3-{[(Perfluorodecyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["2-Chloro-4,4,5,5-tetrakis(trifluoromethyl)-1,3,2-dioxaphospholane","70311-64-7","D",0]
["Copolymer of 1,1-difluoroethene, ethene and hexafluoropropene","154590-04-2","D",0]
["3-{[3-(Dimethylamino)propyl][(perfluorononyl)sulfonyl]amino}propanoic acid","","D",0]
["3-Methylbutyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","183873-56-5","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluoroheptanesulfonyl)amino]propan-1-aminium","","D",0]
["2-Propenoic acid, 2-methyl-, 1,2-ethanediylbis(oxy-2,1-ethanediyl) ester, polymer with 2-(diethylamino)ethyl 2-methyl-2-propenoate, 2-hydroxyethyl 2-methyl-2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate, acetate","863408-20-2","D",0]
["3-Methylbutyl N-(2,2,3,3,4,4,4-heptafluorobutanoyl)-L-leucinate","75743-21-4","D",0]
["3-(Perfluoropropyl)propanol","679-02-7","D",0]
["2-[Perfluoro-[3-(methoxy)propoxy]ethoxy]acetic acid","919005-41-7","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide, phosphoryl trichloride and morpholine","162567-73-9","D",0]
["11-H-Perfluoroundecanoate","69681-37-4","D",0]
["4,5-Dihydro-2-phenyl-α-((perfluorohexyl)ethyloxy)methyl-1H-Imidazole-1-ethanol","1363391-48-3","D",0]
["Triphenyl(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)stannane","649572-74-7","D",0]
["N-((2,3-Dichloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100279-22-9","D",0]
["1,1,2,3,4,5,6-Heptafluoro-2,4-bis(trifluoromethyl)cyclohexane","426-06-2","D",0]
["Perfluoro-6-methylheptanesulfonic acid","255831-20-0","D",0]
["1,1,1,2,2,3,3,4,4,5,6,6,6-Tridecafluoro-5-(trifluoromethyl)hexane","36610-38-5","D",0]
["5‐({[(2-(Perfluorotetradecyl)ethyl)sulfanyl]carbonyl}amino)pentanoic acid","","D",0]
["[(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)ethynyl]benzene","63369-94-8","D",0]
["Hexyl perfluoroheptanoate","97142-48-8","D",0]
["2-(2,4-Difluorophenyl)-1,1-difluoro-1-[5-[4-(2,2,3,3,3-pentafluoropropoxy)phenyl]pyridin-2-yl]-3-(tetrazol-1-yl)propan-2-ol","","D",0]
["2-Methylprop-1-en-1-yl nonafluorobutane-1-sulfonate","84224-48-6","D",0]
["Perfluoro-4-ethylcyclopentane-1-carboxylic acid","","D",0]
["Silicon(4+) 2,2',2''-nitrilotriethanolate 3,3,4,4,5,5,6,6,6-nonafluoro-1-iodohexan-1-ide (1:1:1)","135798-15-1","D",0]
["(9E)-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-Tetratriacontafluorooctadec-9-ene","51249-70-8","D",0]
["4,4,5,5,5-pentafluoropentyl methanesulfonate","252947-01-6","D",0]
["N-[3-(Dimethylamino)propyl]-perfluoro-5-(cyclohexyl)cyclopentanecarboxamide N-oxide","200636-77-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-hydroxyethyl ester, polymer with hexadecyl 2-propenoate, octadecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate","1793072-86-2","D",0]
["[(Perfluoropentanoyl)amino]-3-betaine","508172-07-4","D",0]
["[3,4,6-triacetyloxy-5-(1,1,2,2,3,3,4,4,4-nonafluorobutylsulfonyloxy)oxan-2-yl]methyl Acetate","480438-48-0","D",0]
["Methyl 2,2,3,3,3-pentafluoropropyl carbonate","156783-97-0","D",0]
["2-(Heptafluoropropoxy)propanoic acid","","D",0]
["Hexafluoro-2,5-dihydrofuran","24849-02-3","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl 1,2,3-benzothiadiazole-7-carboxylate","1384278-50-5","D",0]
["1,1,1,3,3,3-Hexafluoro-2-(trifluoromethyl)propane-2-thiol","32308-82-0","D",0]
["2,4-Dibromo-1,1,1,4,4-pentafluoro-2-(trifluoromethyl)butane","885276-63-1","D",0]
["1,1,1,3,3,5,5,7,7-Nonafluoro-2,4,6-trioxaoctan-8-oyl fluoride","21703-45-7","D",0]
["N,N'-bis(Perfluoropentanoyl)1,2-ethanediamine","119403-53-1","D",0]
["1-Methoxy-4-(nonafluorobutyl)benzene","153910-98-6","D",0]
["Poly(difluoromethylene), .alpha.-(2,2-dichloro-1,1,2-trifluoroethyl)-.omega.-hydro-","65530-81-6","D",0]
["2,2,3,3-Tetrafluoropropanol dihydrogen phosphate","461-10-9","D",0]
["2-[(Pentafluoroethyl)sulfanyl]propanoic acid","77758-95-3","D",0]
["Ethyl 3,5,5,5-tetrafluoro-4-(trifluoromethyl)pent-2-enoate","62116-52-3","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(3-sulfopropyl)[(perfluorooctyl)sulfonyl]amino]-1-propanaminium","2089108-82-5","D",0]
["(1Z)-1,2,3,3,3-Pentafluoro-1-(trifluoromethoxy)prop-1-ene","1620992-19-9","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-iodo-2-nonen-1-ol","261761-01-7","D",0]
["2,2,3,4,4,4-Hexafluoro-3-(trifluoromethyl)butan-1-ol","782390-93-6","D",0]
["2-[1,1,2,3,3-Pentafluoro-3-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]acetic acid","919005-37-1","D",0]
["4-[3,3,4,4,5,5,5-Heptafluoro-2,2-bis(trifluoromethyl)pentyl]benzonitrile","104554-44-1","D",0]
["1-Butyl-3-[2-(tridecafluorohexyl)ethyl]-1H-imidazole-3-ium","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluorododecyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["1,1,1,2,2,3,3,4,4,5,5-Undecafluoro-5-methoxypentane","181214-74-4","D",0]
["1H,1H,3H-Perfluoropropyl triflate","6401-02-1","D",0]
["(Perfluorobutyl)-4-bromophenylmethanol","1228786-78-4","D",0]
["Perfluoro-2,2,9,9-tetramethyldeca-3,7-diene","96288-56-1","D",0]
["1-(heptafluoropropyl)-2-iodocyclohexane","2728-75-8","D",0]
["Octafluorocyclopentane","139064-01-0","D",0]
["3-{(Perfluorononanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["4-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl)oxy]-5-methoxy-2-nitrobenzaldehyde","853928-88-8","D",0]
["1-Butanesulfonic acid, 1,1,2,2,3,3,4,4,4-nonafluoro-, 1,3-dioxo-1H-benz[de]isoquinolin-2(3H)-yl ester","171417-91-7","D",0]
["(E)-3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Hexadecafluorodec-2-enal","64906-51-0","D",0]
["2-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1H-imidazole","81790-00-3","D",0]
["Perfluoro-1,8-bis[(propan-2-yl)oxy]octane","23281-45-0","D",0]
["1,3-DITHIACYCLOBUTANE, 2,2,4,4-TETRA(TRI","791-50-4","D",0]
["14:2 Fluorotelomer sulfonamido propyl methyl amine","","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-phenylbutyl diphenyl phosphate","98010-21-0","D",0]
["2-Propenoic acid, esters, 2-methyl-, 2-hydroxyethyl ester, polymer with 1-ethenyl-2-pyrrolidinone, 2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-propenoate","1206450-09-0","D",0]
["Bis[2-(trifluoromethoxy)-2,3,3,3-tetrafluoropropionyl] peroxide","90275-06-2","D",0]
["2-[(3,3,4,4,4-Pentafluorobutyl)sulfanyl]ethan-1-ol","87851-94-3","D",0]
["1,1,2,3,3,4,4,5,5,6,6,7,7,7-tetradecafluoro-2-(trifluoromethyl)heptane-1-sulfonic acid","","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(propane-2-sulfinyl)benzoic acid","1355554-27-6","D",0]
["Bis[2-iodo-3-(perfluorooctyl)propyl] adipate","238742-84-2","D",0]
["(Pentafluoroethyl)phosphonous dichloride","17426-84-5","D",0]
["6-Bromo-1,1,1,2,2,3,3-heptafluoro-4,4-bis(trifluoromethyl)hexane","128454-91-1","D",0]
["2-Propenoic acid, 4,4,5,5,6,6,7,7,7-nonafluoro-2-hydroxyheptyl ester","98573-25-2","D",0]
["1-Chloro-4-[(heptafluoropropyl)sulfanyl]benzene","65538-03-6","D",0]
["4,4,4-trifluoro-1-(2-methoxyphenyl)-3-(trifluoromethyl)but-2-en-1-one","35443-94-8","D",0]
["1-(Perfluoro-n-hexyl)dodecane","90499-30-2","D",0]
["[3,3,4,4,5,6,6,6-Octafluoro-2-hydroxy-2-methyl-5-(trifluoromethyl)hexyl] 2-methylprop-2-enoate","","D",0]
["2-(Pentafluoroethoxy)ethan-1-ol","91324-95-7","D",0]
["1,1,1,2-Tetrafluoro-2-nitroethane","2967-10-4","D",0]
["Sulfuryl difluoride--undecafluoro(pentafluoroethyl)cyclohexane (1/1)","80308-98-1","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-[(propan-2-yl)sulfanyl]benzoic acid","1355554-70-9","D",0]
["1,1,1,2,2,3,3-heptafluoro-6-iodo-4,4-bis(trifluoromethyl)hexane","115347-68-7","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl (3a,5b,6a,20R)-3,6-bis[(trifluoroacetyl)oxy]cholan-24-oate","","D",0]
["2H-Perfluoroisobutyric acid","564-10-3","D",0]
["N-((3-Chloro-4-(1,1,2,2-tetrafluoroethylsulfonyl)phenyl)carbamoyl)-2,6-difluorobenzamide","100341-25-1","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(4-methoxyphenyl)butanamide","793-36-2","D",0]
["Bis[2,3,3,3-tetrafluoro-1-oxo-2-(trifluoromethyl)propyl] peroxide","111632-55-4","D",0]
["(2E)-1,1,1,4,4,5,5,6,6,6-Decafluorohex-2-ene","83227-62-7","D",0]
["4-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)oxy]aniline","147395-06-0","D",0]
["2-(1,1,2,3,3,3-hexafluoropropyl)oxolane","53005-42-8","D",0]
["Perfluoro-3-(trifluoromethyl)heptane-1-sulfonic acid","","D",0]
["1,2,3,3,4,4,5,5,5-Nonafluoropent-1-ene","75180-13-1","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-5,5,6,6-tetrakis(trifluoromethyl)cyclohexane","74903-98-3","D",0]
["2,5-Difluoro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-67-4","D",0]
["(Heptadecafluorooctyl)benzene","87405-83-2","D",0]
["2-Propenoic acid, 2-methyl-, heptafluoropropyl ester, homopolymer","134042-87-8","D",0]
["Dodecafluorooxepane","788-41-0","D",0]
["Perfluoro-5-(pentafluoro-lambda6-sulfanyl)pentanoic acid","","D",0]
["1,1,1,2,4,5,6,7,7,7-Decafluoro-2,6-bis(trifluoromethyl)-4-hepten-3-one","235772-91-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,18-Tetratriacontafluoro-9-iodooctadecane","53638-12-3","D",0]
["1,1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10,11,11,11-Eicosafluoro-5-undecene","100508-28-9","D",0]
["Tricyclo[3.3.1.13,7]decane, 1,2,2,3,4,4,5,6,6,8,8,9,9,10,10-pentadecafluoro-7-(trifluoromethyl)-","60096-00-6","D",0]
["Perfluoro-3-pentenesulfonic acid","2089109-40-8","D",0]
["2‐Hydroxy‐3‐[[3-(perfluoropentyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["1,1,1,2,6,7,7,7-Octafluoro-2,6-bis(heptafluoropropoxy)heptane-3,5-dione","87405-74-1","D",0]
["Trimethylsilyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","152718-74-6","D",0]
["N,N,4-Triethyl-2-(1,2,2,2-tetrafluoroethyl)-1,3-dioxolan-2-amine","89752-27-2","D",0]
["1,2-Dibromohexafluorocyclobutane","377-40-2","D",0]
["2-(Nonafluorobutyl)-1-benzofuran","1608112-36-2","D",0]
["8:2 Fluorotelomer sulfonamide","29766-00-5","D",0]
["1,1,2,2,3,3,6,6,6-Nonafluorohexyl prop-2-enoate","91528-57-3","D",0]
["2-Diazo-1,1,1,3,3,3-hexafluoropropane","684-23-1","D",0]
["2‐(N‐Methyl-perfluoroundecanesulfonamido)acetic acid","","D",0]
["5,5,6,6,6-pentafluorohexane-2,4-dione","356-40-1","D",0]
["Perfluorotetradecanoate","365971-87-5","D",0]
["1,1,1,2,2,3,3,10,10,11,11,12,12,12-Tetradecafluorododecane","69125-82-2","D",0]
["2(Perfluoro-2-propyl)ethanol","90999-87-4","D",0]
["6-[(Perfluoro-1-oxoundecyl)amino]hexanoic acid, ammonium salt (1:1)","83952-11-8","D",0]
["2-[2-(2,2,3,3,4,4,4-Heptafluorobutoxy)ethoxy]ethan-1-ol","54336-56-0","D",0]
["7-Chloro-1,1,1,2,2,3,3,4,4,5,5,6,7-tridecafluoro-6-methoxyheptane","651733-01-6","D",0]
["Methoxy (propyl) (3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) (3,3,3-trifluoropropyl)silane","608300-34-1","D",0]
["1-Ethyl-2,4,4-tris(trifluoromethyl)-1,4-dihydroquinazoline","106119-57-7","D",0]
["2-[(4-Methoxypyridin-2-yl)methanesulfinyl]-6-(1,1,2,2-tetrafluoroethoxy)-1H-benzimidazole","97963-96-7","D",0]
["1,1,1,2,2,3,4,5,5,5-Decafluoro-3-propoxy-4-(trifluoromethyl)pentane","","D",0]
["1,1,1,2,2,3-Hexachloro-3,4,4,4-tetrafluorobutane","61146-84-7","D",0]
["4,4,4-trifluoro-2-methyl-1-phenyl-3-(trifluoromethyl)but-2-en-1-one","35444-12-3","D",0]
["14:2 Fluorotelomer sulfonamido propyl dimethyl amine","","D",0]
["2H-Perfluoroheptanoic acid","","D",0]
["2-Fluoro-2-[1,1,2,2,3,3-hexafluoro-3-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]acetic acid","919005-03-1","D",0]
["2-[(3,4,4,5,5,5-Hexafluoropentyl)dimethylazaniumyl]acetate","","D",0]
["2,2,3,3-Tetrafluoro-1,4-butanediyl bis(4-methylbenzenesulfonate)","122834-95-1","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluorohexyl)sulfonyl]amino}-1-propanaminium","2089109-06-6","D",0]
["{2-Hydroxy-3-[(3,3,4,4,4-pentafluorobutyl)sulfanyl]propyl}trimethylazanium","","D",0]
["1,1,1,2,4,5,5,6,6,7,7,7-dodecafluoro-2,4-bis(trifluoromethyl)heptan-3-one","95639-15-9","D",0]
["2,2,3,3-Tetrafluoropropyl trifluoroacetate","107551-72-4","D",0]
["1,2,3,4,5,6,7,8,9,10,11,12,12,13,13,13-Hexadecafluorotridecyl hydrogen sulfate","","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with glycine","161212-11-9","D",0]
["8H-Perfluorononanesulfonic acid","2089109-59-9","D",0]
["(3,3,4,4,4-Pentafluorobutyl)benzene","67102-32-3","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-1-(morpholin-4-yl)propan-1-one","176702-76-4","D",0]
["(2Z)-1,1,1,2,4,4,5,5,5-Nonafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pent-2-ene","58621-71-9","D",0]
["3-{[3-(Dimethylamino)propyl][(perfluoroundecyl)sulfonyl]amino}propanoic acid","","D",0]
["1,1,1,2-Tetrafluoro-4-iodo-2-(trifluoromethyl)octane","161094-94-6","D",0]
["N-(2-Ethylphenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","51814-65-4","D",0]
["15-Bromo-1,1,1,2,2,3,3,4,4-nonafluoropentadecane","213207-95-5","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluorotridecyl)-but-3-en-2-ol","","D",0]
["9:2 Fluorotelomer ketone sulfonate","","D",0]
["3-(Perfluorohexyl)-1-(trifluoroacetyl)-5-(trifluoromethyl)-1H-pyrazole","261778-38-5","D",0]
["Phenol, 4-(heptafluoropropyl)-","61324-28-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoropentadec-8-en-7-one","89176-07-8","D",0]
["2,2,3,3,3-Pentafluoropropyl 2-(trifluoromethyl)prop-2-enoate","105935-33-9","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)phosphonic acid","503564-50-9","D",0]
["9,11-bis(diethoxyphosphoryl)-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-11-iodoundecane","23144-30-1","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1-benzofuran-5-amine","103082-67-3","D",0]
["{[(16,16,17,17,18,18,18-Heptafluorooctadecyl)oxy]methyl}benzene","102197-77-3","D",0]
["Sodium 8-chloroperfluoro-1-octanesulfonate","2481740-05-8","D",0]
["N-Butyl-2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanamide","178167-72-1","D",0]
["1-Propanol, 2,3,3,3-tetrafluoro-2-(1,1,2,2-tetrafluoropropoxy)-","1643445-09-3","D",0]
["Dodecafluorooctanedinitrile","3885-85-6","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, fluorinated, reduced, 3-[[4-[dimethyl[2-(trimethoxysilyl)ethyl]silyl]phenyl]dimethylsilyl]propyl ethers","1431551-16-4","D",0]
["1,1,1,3,3,3-Hexafluoro-2-phenylpropan-2-yl (1E)-2,2-dimethyl-N-phenylpropanimidate","40999-34-6","D",0]
["9-(Pentafluorosulfanyl)perfluorononyl sulfonic acid","2089109-35-1","D",0]
["1,1'-(1,1,2,2-Tetrafluoroethane-1,2-diyl)bis[3-(trifluoromethyl)benzene]","287172-67-2","D",0]
["2,2-Dibromo-5-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)cyclopentan-1-one","101932-20-1","D",0]
["Polyfluoroalkyl (C 2-5) methacrylate","31623-04-8","D",0]
["4-(Nonafluorobutoxy)aniline","62315-18-8","D",0]
["2-(Heptafluoropropyl)-6-nitro-1H-benzimidazole","6826-38-6","D",0]
["potassium 1,2,2,3,3,4,5,5,6,6-decafluoro-4-(trifluoromethyl)cyclohexane-1-sulfonate","374-62-9","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-[(2-methylpropyl)sulfanyl]benzoic acid","1355554-74-3","D",0]
["5-(1,1,1,3,3,3-Hexafluoropropan-2-yl)-4-methyl-1,3-thiazole-2(3H)-thione","499786-34-4","D",0]
["O-(3-Perfluorooctyl)-propylhydroxylamine hydrochloride","1228693-32-0","D",0]
["N-(2,2,3,3,4,4,4-Heptafluorobutyl)prop-2-enamide","1422-65-7","D",0]
["1,3,6-Trioxaspiro[4.4]nonane-4,7-dione, 2,2-bis(trifluoromethyl)-","7724-50-7","D",0]
["(4-Fluorophenyl)(heptadecafluorooctyl)iodanium hydrogen sulfate","83609-32-9","D",0]
["1,1,1,2,2-pentafluorohexan-3-one","357-46-0","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-7-(1,1,2,3,3,3-hexafluoropropoxy)heptane","65064-82-6","D",0]
["2,2,3,3,4,4,4-Heptafluoro-1-(4-methylphenyl)butan-1-one","559-92-2","D",0]
["2-[(tert-Butylamino)methyl]-1,1,1,3,3,3-hexafluoropropan-2-ol","507469-52-5","D",0]
["(9E)-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluorooctadec-9-ene","113999-61-4","D",0]
["S-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl) ethanethioate","213681-67-5","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1,2,2,2-tetrafluoro-1-[(phosphonooxy)methyl]ethyl]-.omega.-[tetrafluoro(trifluoromethyl)ethoxy]-","202200-80-4","D",0]
["2,2,3,3,4,4,4-Heptafluorobutan-1-amine--hydrogen chloride (1/1)","2794-75-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-iodooctadecane","125081-35-8","D",0]
["2,2,3,3-Tetrafluoro-2,3-dihydro-1,4-benzodioxine","94767-47-2","D",0]
["Lotrafilcon A","308073-61-2","D",0]
["N-[2-Amino-3-nitro-5-(trifluoromethyl)phenyl]-2,2,3,3,4,4,4-heptafluorobutanamide","57450-70-1","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexanimidamide","464-21-1","D",0]
["Erbium tris[(henicosafluorodecyl)(heptadecafluorooctyl)phosphinate]","500776-93-2","D",0]
["N-Methyl (perfluoropentyl)sulfonamidoacetic acid","1003194-04-4","D",0]
["1,2-Dichloro-1,2,2-trifluoroethyl heptafluoropropyl ether","106372-30-9","D",0]
["8,8,8-Trifluoro-7-(trifluoromethyl)octane-1,7-diol","886989-80-6","D",0]
["3-[(3-{Ethyl[(perfluoroundecyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["Bis[2-(fluorosulphonyl)tetrafluoroethyl]ether","146829-79-0","D",0]
["[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy]cyclododecane","113557-85-0","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorooctadecane","89109-70-6","D",0]
["6-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1,3-benzoxazol-2(3H)-one","1248393-88-5","D",0]
["2,2,3,3-Tetrafluoropropyl tosylate","786-31-2","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-[4-(2-hydroxyethyl)piperazin-1-yl]heptan-1-one--hydrogen chloride (1/1)","95851-62-0","D",0]
["1,1,2-Tribromopentafluorocyclobutane","142764-86-1","D",0]
["2,6-Difluoro-N-{[2-methyl-4-(1,1,2,2-tetrafluoroethanesulfinyl)phenyl]carbamoyl}benzene-1-carboximidic acid","100331-01-9","D",0]
["Methyl 4,4,5,5-tetrafluoro-3,3-dihydroxypentanoate","89129-73-7","D",0]
["1,1,1,4,5,5,5-Heptafluoro-4-(trifluoromethyl)pentane-2,3-dione","74728-97-5","D",0]
["4-(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-enoxy)-5-methoxybenzene-1,2-diamine","","D",0]
["2-[5-(Pentafluoroethyl)-1,2-oxazol-3-yl]-1H-isoindole-1,3(2H)-dione","110234-96-3","D",0]
["4-(Heptafluoropropyl)benzoic acid","88950-94-1","D",0]
["2,5-Furandione, dihydro-, monopolyisobutylene derivatives, reaction products with 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-1-octanol","253682-99-4","D",0]
["(1Z)-1-(Perfluoropentanyl)-1-fluorohept-1-ene","92610-11-2","D",0]
["Ethyl 4,4,5,5,6,6,6-heptafluoro-3,3-bis(trifluoromethyl)hexanoate","161261-13-8","D",0]
["1,1,2,2-Tetrafluoro-2-iodo-N,N-bis(trifluoromethyl)ethan-1-amine","130279-43-5","D",0]
["2-Hydrido-perfluorodecanoic acid","2646714-97-6","D",0]
["2-Nitro-N-(2,2,3,3,3-pentafluoropropyl)-1H-imidazole-1-acetamide","152721-37-4","D",0]
["CA 944 A","103015-84-5","D",0]
["3-Chloro-1,1,2,2,3,3-hexafluoropropan-1-ol","89308-01-0","D",0]
["Acetic acid, bis[(.gamma.-.omega.-perfluoro-C8-20-alkyl)thio] derivs., compds. with diethanolamine","71608-38-3","D",0]
["N-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluorononanoyl)-L-alanine","330548-64-6","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(methylsulfanyl)benzoic acid","1355554-62-9","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, telomer with chlorotrifluoroethene, oxidized, reduced, hydrolyzed ammonium salts","330809-92-2","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.′-[1,2-phenylenebis(carbonyloxy-2,1-ethanediyl)]bis[.omega.-(trifluoromethyl)-","154159-07-6","D",0]
["1,1,1,2,2,3,3-Heptafluoro-5-iodoundec-4-ene","109574-86-9","D",0]
["7,8,8,8-Tetrafluoro-7-(trifluoromethyl)octane-1-thiol","","D",0]
["1,1,1,7,7,7-Hexafluoro-2,2,6,6-tetrakis(trifluoromethyl)hept-3-ene","62498-14-0","D",0]
["1,1,2-Trifluoro-2-(trifluoromethyl)cyclopropane","380-51-8","D",0]
["Perfluoro-1-iodoalkane (C6-C8)","","D",0]
["1-(Perfluorohexyl)oct-1-ene","120464-26-8","D",0]
["(1Z)-1,3,4,4,4-Pentafluoro-3-(trifluoromethyl)but-1-ene","14318-61-7","D",0]
["2-(4-Ethenylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","122056-08-0","D",0]
["Tridecafluorotris(trifluoromethyl)bicyclo[3.3.1]nonane","67711-54-0","D",0]
["1,1,1,3,3,3-hexafluoro-2-(pyridin-2-ylamino)propan-2-ol","64139-77-1","D",0]
["5-Chloro-2,2,3,3,4,4,5,5-octafluoropentanal","88332-86-9","D",0]
["3,3,4,4,5,5,6,6,6-Nonafluorohexyl 4-methylbenzene-1-sulfonate","188492-56-0","D",0]
["Nonane, heptadecafluoro-1-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]-","84029-59-4","D",0]
["Poly(oxy-1,2-ethanediyl), α-(nonadeca fluorodecenyl)-ω-[(nonadecafluorodecenyl) oxy]-","37382-58-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8-Tetradecafluorooctanoyl fluoride","14042-24-1","D",0]
["N-Ethyl-N-(2,2,3,3-tetrafluoropropyl)aniline","66959-16-8","D",0]
["Perfluoro-2-(2-sulfoethoxy)propanoic acid","790642-73-8","D",0]
["3'-Fluorosulfonyl-4,4,4-trifluoro-3-trifluoromethylcrotonophenone","101030-73-3","D",0]
["12-Bromo-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluorododecane","99324-99-9","D",0]
["1-(Prop-1-en-2-yl)-4-(1,1,2,2-tetrafluoro-2-phenylethyl)benzene","40396-68-7","D",0]
["4,4,5,5,6,6,6-heptafluoro-1-(3-methylthiophen-2-yl)hexane-1,3-dione","575-93-9","D",0]
["4,9-Dimethoxy-7-(nonafluorobutyl)-5H-furo[3,2-g][1]benzopyran-5-one","376380-66-4","D",0]
["5-Chloro-2-pentafluoroethylbenzimidazole","58457-67-3","D",0]
["N,N,N-Trimethyl-(5-(difluoromethyl)perfluoropentyl)methanaminium","","D",0]
["Perfluoro-14-(pentafluoro-.lambda.6-sulfanyl)tetradecanoic acid","","D",0]
["Siloxanes and Silicones, lauryl Me, Me 2-(2-methylpropoxy)ethyl, Me octyl, Me 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl","1257095-32-1","D",0]
["Poly(difluoromethylene), .alpha.-(trifluoromethyl)-.omega.-[[[(trifluoromethyl)sulfonyl]amino]sulfonyl]-","765585-55-5","D",0]
["(5Z)-1,1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10,10-octadecafluorodec-5-ene","97558-57-1","D",0]
["1,1,1-Trifluoro-5-phenyl-2-(trifluoromethyl)pentane-2,4-diol","101931-58-2","D",0]
["8-Chloroperfluorooctanoic acid","335-63-7","D",0]
["S-Ethyl pentadecafluorooctanethioate","111918-92-4","D",0]
["4-(Tridecafluorohexyl)benzoic acid","74701-31-8","D",0]
["1,1,1,2,3,4-Hexafluorobutane","119450-67-8","D",0]
["2,2-Difluoro-2-(trifluoromethoxy)acetate sodium salt","21837-98-9","D",0]
["2-[2,3,3,3-Tetrafluoro-2-(heptafluoropropoxy)propoxy]ethan-1-ol","67822-71-3","D",0]
["N,N'-(Propane-1,2-diyl)bis(2,2,3,3,4,4,4-heptafluorobutanamide)","133911-24-7","D",0]
["4,4,4-Trifluoro-1-(3-nitrophenyl)-3-(trifluoromethyl)but-2-en-1-ol","100482-54-0","D",0]
["[(1-Chloro-1,1,2,3,3,3-hexafluoropropan-2-yl)oxy](difluoro)acetic acid","903523-21-7","D",0]
["1-Butene, 4-bromo-3,3,4,4-tetrafluoro-, polymer with 1-propene, 1,1,2,3,3,3-hexafluoro-, ethene, tetrafluoro-, ethene, trifluoro(trifluoromethoxy)- and ethene,1,1-difluoro-","255916-31-5","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2,4,5-trichlorophenyl)butanamide","121806-70-0","D",0]
["[N(E),S(S)]-N-(2-Fluorophenyl)methyleneperfluorobutanesulfinamide","1612778-40-1","D",0]
["3-[Perfluoro(2-(propoxy)propoxy)]propyl trichlorosilane","119511-20-5","D",0]
["Octane, 1,8-dichloro-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-hexadecafluoro-","647-25-6","D",0]
["1,11-Dodecadiene, 4,4,5,5,6,6,7,7,8,8,9,9-dodecafluoro-","170804-09-8","D",0]
["2-(3,3,4,4,4-Pentafluorobutylsulfanyl)acetic acid","","D",0]
["4,4,5,5,5-Pentafluoro-1-phenylpentane-1,3-dione","1799-50-4","D",0]
["2,3-Dibromo-1,1,1,2,3,4,4-heptafluorobutane","140427-86-7","D",0]
["N-(1-Hydroxyethylidene)-S-(1,1,2,2-tetrafluoroethyl)cysteine","119018-04-1","D",0]
["2-[(2-(1-Hydridoperfluoropentyl)ethyl)dimethylazaniumyl]acetate","","D",0]
["Butanoic acid, 3-oxo-, 2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl ester, polymer with 2-(dimethylamino)ethyl 2-propenoate, 2-hydroxyethyl 2-propenoate, .alpha.-(2-methyl-1-oxo-2-propen-1-yl)-.omega.-methoxypoly(oxy-1,2-ethanediyl) and 3,3,4,4,5,5,6,6,7,7,","1801846-59-2","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluorodecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["Chlorodipropyl(3,3,4,4,5,5,5-heptafluoropentyl)silane","608296-07-7","D",0]
["3-Fluoro-3-(perfluorodecyl)prop-2-ene-1-sulfonic acid","","D",0]
["trans-Perfluorohydrindan","75240-06-1","D",0]
["4-(Pentafluoroethyl)-1,3,5-triazin-2-amine","1803609-43-9","D",0]
["(Perfluorooctyl)propyl acetate","150225-00-6","D",0]
["2-(2,2,3,3-Tetrafluoropropoxy)-1,3,2-benzodioxaphosphole 2-oxide","127054-63-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoroheptacosane","871311-26-1","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]],alpha-[1,2,2,2-tetrafluoro-1-[[[2-[(1-oxo-2-propenyl)oxy]ethyl]amino]carbonyl]ethyl]-omega[tetrafluoro(trifluoromethyl)ethoxy]-","769967-14-8","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluoro-3-iododecan-1-ol","16083-68-4","D",0]
["4,4,4-trifluoro-1-(thiophen-2-yl)-3-(trifluoromethyl)but-2-en-1-one","35554-26-8","D",0]
["1-[2-(pentafluoroethyl)phenyl]methanamine","1785118-14-0","D",0]
["1,1,1,2,2,3,3-heptafluoro-5-nitro-4-(nitromethyl)pentane","355-91-9","D",0]
["2,2,3,3,4,4,5,5,6,6,6-Undecafluorohexanamide","335-54-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,12,12,13,13,14,14,15,15,16,16,17,17,17-Hexacosafluoro-8,10-diiodoheptadecane","1254971-76-0","D",0]
["6-[(4,6-Dimethylpyrimidin-2-yl)sulfanyl]-3-(heptafluoropropyl)[1,2,4]triazolo[4,3-b]pyridazine","351346-36-6","D",0]
["2,3,3,3-Tetrafluoro-2-{1,1,2,3,3,3-hexafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propoxy}propanamide","51445-02-4","D",0]
["1,10-Decanediol, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro-","754-96-1","D",0]
["Poly(oxy-1,2-ethanediyl), α-(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11, 11,12,12,12-nonadecafluoro-2-hydroxydodecyl)-ω-methoxy-","85643-63-6","D",0]
["D-Galactose-6-[5-[(3(-perfluorooctyl)-1-nonylpropyl)oxy]pentylhydrogen phosphate]","172916-27-7","D",0]
["4,4,4-Trifluoro-3-hydroxy-1-(2-thienyl)-3-(trifluoromethyl)-1-butanone","34844-19-4","D",0]
["Potassium N-hexyl-N-[(perfluorobutyl)sulfonyl]glycinate","864069-53-4","D",0]
["1,3-Propanediamine, N,N-dimethyl-, compd. with .alpha.,.alpha.'-[phosphinicobis(oxy-2,1-ethanediyl)]bis[.omega.-fluoropoly(difluoromethylene)] (1:1)","65530-78-1","D",0]
["1,1,1,2,2,3,3-heptafluoro-6-hydroxy-7,7-dimethyloct-5-en-4-one","62773-05-1","D",0]
["Oxirane, 2-(chlorodifluoromethyl)-2,3,3-trifluoro-","5068-87-1","D",0]
["{[(Perfluoroundecyl)sulfonyl]amino}acetic acid","","D",0]
["2,5-Diphenyl-3,3-bis(trifluoromethyl)-2,3-dihydro-1,2,4-oxadiazole","62457-73-2","D",0]
["Perfluoro-2-tetradec-7-eneoxyacetic acid","","D",0]
["N-[[(4,6-Dimethoxy-1,3,5-triazin-2-yl)amino]carbonyl]-2-(pentafluoroethoxy)benzenesulfonamide","82097-14-1","D",0]
["N-Ethyl-2-(pentafluoroethoxy)ethan-1-amine","960365-28-0","D",0]
["N-Methyl-3-(4,4,5,5,5-pentafluoropentylsulfonyl)propan-1-amine","","D",0]
["Methyl 4-(heptafluoropropyl)cyclohexane-1-carboxylate","88951-13-7","D",0]
["Bis(perfluorohexyl)phosphinic acid","40143-77-9","D",0]
["3-Benzamido-2,6-difluoro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","862133-36-6","D",0]
["2,2,3,4,4-Pentafluoro-4-(pentafluoroethoxy)butanoic acid","919005-25-7","D",0]
["Ethyl (2E)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluorodec-2-enoate","37759-80-1","D",0]
["3-[(Perfluoroethanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexane-1-sulfonamide","87988-56-5","D",0]
["1-[1,1,1,2,3,5,5,5-Octafluoro-4-(trifluoromethyl)pent-3-en-2-yl]pyrrolidine","89810-72-0","D",0]
["1,1'-(1,1,2,2,3,3-Hexafluoropropane-1,3-diyl)dibenzene","2647-96-3","D",0]
["Benzenesulfonic acid, 4-[2-[4-[ethyl[2-(formyloxy)ethyl]amino]phenyl]diazenyl]-, 2,2,3,3-tetrafluoropropyl ester","883800-58-6","D",0]
["2-{[(1,1-Dicyclohexyl-5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heptadecafluorododecan-2-yl)oxy]carbonyl}hydrazine-1-carboxylate","821806-51-3","D",0]
["Perfluoro-2-isobutoxypropanoic acid","267239-67-8","D",0]
["(2R)-2-Amino-4,4,5,5,5-pentafluoropentanoic acid","1821830-40-3","D",0]
["12:2 Fluorotelomer aldehyde","1270180-15-8","D",0]
["Perfluoromethylbutyl-(4-methylcyclohexyl)-amine","444658-68-8","D",0]
["Ethyl 11H-perfluoroundecanoate","1649-56-5","D",0]
["Ethyl difluoro(1,1,2,2-tetrafluoro-2-iodoethoxy)acetate","98296-51-6","D",0]
["2,2'-Dimethoxy-5,5'-bis(tridecafluorohexyl)-1,1'-biphenyl","658709-63-8","D",0]
["1,1,1,2,5,6,6,6-Octafluoro-3-iodo-2,5-bis(trifluoromethyl)hexane","88562-42-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Tricosafluorododecyl nonafluorobutane-1-sulfonate","924894-11-1","D",0]
["2,4-HEPTANEDIOL, 7-CHLORO-1,1,1-TRIFLUOR","101913-68-2","D",0]
["2'-Nitro-4,4,4-trifluoro-3-(trifluoromethyl)-crotonophenone","35443-89-1","D",0]
["3,3,3-Trifluoro-2-(trifluoromethyl)propanehydrazide","105955-39-3","D",0]
["Heptafluoropropoxy(poly(perfluoroPO))tetrafluoropropyloxypropyltrimethoxysilane","870998-78-0","D",0]
["N,N-Dimethyl-3-[(pentafluoroethanesulfonyl)amino]propan-1-amine N-oxide","","D",0]
["2,3,4,5,6-Pentafluoro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-96-9","D",0]
["2-Chloro-2-(chloromethyl)-1,1,1,3,3,3-hexafluoropropane","138690-25-2","D",0]
["Polyperfluoroisopropyl ether","","D",0]
["[(Pentafluoroethyl)sulfanyl]benzene","65538-00-3","D",0]
["1,1,2,2,3,3-hexafluorocyclopentane","123768-18-3","D",0]
["1-Chloro-perfluorododecane-1-sulfonic acid","","D",0]
["1,5-Diiododecafluoropentane","","D",0]
["Rhodium(II) perfluorobutyrate dimer","73755-28-9","D",0]
["(11-(F-Hexyl)undecyl) dimorpholinophosphoramidate","134051-91-5","D",0]
["(Perfluorohexyl)propane","168834-06-8","D",0]
["2-[Dimethyl(2-(1-hydrido-perfluorononyl)ethyl)azaniumyl]acetate","","D",0]
["2-Propanol, 1,1,1,3,3,3-hexafluoro-, 2,2',2''-triester with boric acid (H3BO3)","6919-80-8","D",0]
["(3β)-25,26,26,26,27,27,27-Heptafluoro-cholest-5-en-3-ol","153463-21-9","D",0]
["2-(Pentafluoroethyl)naphthalene","138133-66-1","D",0]
["3-(Tridecafluorohexyl)pyridin-4-amine","143094-26-2","D",0]
["Methyl 1,1,1,2,4,4,4-heptafluoro-3-oxobutane-2-sulfonate","63176-10-3","D",0]
["6:2 Fluorotelomer sulfonate sodium salt","27619-94-9","D",0]
["3,3,3-Trifluoro-N-(4-methylpyridin-2-yl)-2-(trifluoromethyl)propanimidic acid","5309-03-5","D",0]
["3,3,4,5,5,6,6,7,7,7-Decafluoroheptan-2-ol","7618-17-9","D",0]
["(2Z)-Perfluoro-2-butene","1516-65-0","D",0]
["5-(Heptafluoropropyl)-1,3-dimethylpyrimidine-2,4-dione","60007-33-2","D",0]
["[3-(Heptafluoropropoxy)propyl](trimethoxy)silane","903890-42-6","D",0]
["5-(Tridecafluorohexyl)-2,2'-bithiophene","327630-34-2","D",0]
["1,1,2,2,2-Pentafluoroethylsulfonyl 2,2,2-trifluoroacetate","","D",0]
["Potassium perfluorononanoate","21049-38-7","D",0]
["Phosphine, tris[3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)phenyl]-","195324-93-7","D",0]
["N-(4-Chlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","79497-98-6","D",0]
["1-Methyl-3-(pentafluoroethyl)-5-phenyl-4-(trifluoromethyl)-1H-pyrazole","110035-58-0","D",0]
["N-Methyl-N-[(3-octadecyl-2-oxo-5-oxazolidinyl)methyl]perfluoro-1-octanesulfonamide","138704-55-9","D",0]
["Perfluoropentane sulfinic acids","1997344-06-5","D",0]
["5-[3-({[2-(Perfluorohexyl)ethylsulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["S-Methyl 4,4,5,5,5-pentafluoropent-2-ynethioate","111835-75-7","D",0]
["1-Henicosanylperfluoroheptane","1980063-68-0","D",0]
["Sodium bis[2-(perfluorohexyl)ethyl] phosphate","407582-79-0","D",0]
["1,8-Bis(perfluorododecyl)-2,7-diiodooctane","1980044-62-9","D",0]
["(Heptadecafluorooctyl)trimethylsilane","52112-19-3","D",0]
["2-(1,1,2,2,3,3-Hexafluoropropyl)-1H-benzimidazole","61532-03-4","D",0]
["4-(Perfluoromethoxy)perfluorobutane sulfonic acid","","D",0]
["1,1,1,2,2,3-Hexafluorobutane","74469-62-8","D",0]
["1,1,1,3,3,3-hexafluoro-2-(2-iodo-5-methylphenyl)propan-2-ol","65653-64-7","D",0]
["N-[(Cyclohexylamino)carbonyl]perfluoro-1-octanesulfonamide","100221-85-0","D",0]
["6-Chloro-1,1,2,2,3,3,4,4,5,5,6,7-dodecafluoroheptane","651732-97-7","D",0]
["Prop-2-en-1-yl 2-fluoro-2-(trifluoromethyl)pent-4-enoate","74277-74-0","D",0]
["(2-Chloro-1,1,2,2-tetrafluoroethoxy)(difluoro)acetic acid","83865-02-5","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluoroundecyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["3,3'-(1,4-Phenylene)bis[5-(tridecafluorohexyl)-1,2,4-oxadiazole]","146304-71-4","D",0]
["N,N-Diethyl-2,2,3,3-tetrafluoropropanamide","392-63-2","D",0]
["8H,8H-Perfluoropentadecane-7,9-dione","261503-74-6","D",0]
["Methyl 2H,2H,3H,3H-perfluoroheptanoate","132424-36-3","D",0]
["12,12,13,13,14,14,15,15,15-Nonafluoropentadecanoyl chloride","118624-68-3","D",0]
["5,5,6,6,7,7,7-Heptafluoro-3-iodohept-3-en-1-ol","89608-31-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8,8-dimethoxyoctane","142502-76-9","D",0]
["3,4,4,4-Tetrafluoro-1-phenyl-3-(trifluoromethyl)butan-1-one","82959-21-5","D",0]
["Bis(3,3,4,4,5,5,6,6,6-nonafluorohexyl) butanedioate","508194-70-5","D",0]
["{(Carboxymethyl)[(perfluoroundecyl)sulfonyl]amino}-3-betaine","","D",0]
["3,4-Bis(2,2,3,3,4,4,4-heptafluorobutyl)-1H-pyrrole-2,5-dicarboxylic acid","83650-67-3","D",0]
["(Dichloromethyl)[5,5,5-trifluoro-4,4-bis(trifluoromethyl)pentyl]silane","63809-47-2","D",0]
["(E)-Perfluoronon-7-ene-1-sulfonic acid","","D",0]
["2-(Heptafluoropropyl)pyrimidine","133391-64-7","D",0]
["4-(Dimethylamino)-2-{[(perfluorohexyl)sulfonyl]amino}butanoic acid","2089109-98-6","D",0]
["1-(4-Ethoxyphenyl)-2,2,3,3-tetrafluorocyclobutane-1-carboxylic acid","72370-87-7","D",0]
["2-(Perfluoropropyl)glycine","26208-02-6","D",0]
["5,5,6,6,6-Pentafluorohexanoic acid","148043-70-3","D",0]
["Lithium heptadecafluorononanoate","60871-92-3","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyl-3,5-octanedione - cobalt (3:1)","62477-38-7","D",0]
["1,2,4,5-Tetrafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trichloromethyl)benzene","136264-73-8","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecan-2-ol","61589-61-5","D",0]
["(1,1,2,2-Tetrafluoro-2-iodoethoxy)benzene","89045-65-8","D",0]
["Sodium perfluorodecanesulfonate","2806-15-7","D",0]
["2-(2-Bromo-1,1,2,2-tetrafluoroethoxy)-1,1,1,2,3,3,3-heptafluoropropane","16005-49-5","D",0]
["4-[(Perfluorohexyl)oxy]benzenesulfonic acid sodium salt","69161-21-3","D",0]
["2-Iodo-3-(tridecafluorohexyl)thiophene","1453469-53-8","D",0]
["Perfluorohexylsulfinic acid","115416-67-6","D",0]
["Copper(1+) 1,1,2,2,3,3,4,4,4-nonafluorobutan-1-ide","124521-58-0","D",0]
["1-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)pyridin-1-ium iodide","88992-49-8","D",0]
["4-(Nonadecafluorononyl)benzoyl azide","93238-01-8","D",0]
["2,5-Furandione, polymer with 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-8-(2-propenyloxy)octane","38467-12-8","D",0]
["1,1,1,7,7,7-hexafluoro-4-methylidene-2,6-bis(trifluoromethyl)heptane-2,6-diol","16202-91-8","D",0]
["2-[2-[Difluoro(trifluoromethoxy)methoxy]-1,1,2,2-tetrafluoroethoxy]-2-fluoroacetic acid","919005-07-5","D",0]
["Potassium 2,3,3,3-tetrafluoro-2-(trifluoromethyl)propanoate","95091-35-3","D",0]
["Tris{4-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propyl]phenyl}phosphane","62512-90-7","D",0]
["Lithium 3-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]propanesulfonate","864069-44-3","D",0]
["Sodium 2,2,3,5,5,6,6,7,7,9,9,9-dodecafluoro-4,8-dioxononanoate","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-Dodecafluoro-1-[(trifluoromethyl)sulfanyl]hexane","678-67-1","D",0]
["Poly(oxy-1,2-ethanediyl), α-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10, 10-heptadecafluoro-1-oxodecyl)-ω-hydroxy-","67296-33-7","D",0]
["5-[4-[5-(3,3,4,4,5,5,5-Heptafluoropentylsulfanyl)pentoxy]phenyl]-6-phenyl-8,9-dihydro-7H-benzo[7]annulen-2-ol","","D",0]
["Tris(heptafluoropropyl)(oxo)-lambda~5~-phosphane","58431-33-7","D",0]
["Butane, 1,4-dibromo-1,1,2,2,3,3,4,4-octafluoro-","335-48-8","D",0]
["1,1,2,2,3,3,3a,4,4,5,5,6,6,7,7,7a-Hexadecafluorooctahydro-1H-indene","374-80-1","D",0]
["1-(4-Chlorophenyl)-4,4,4-trifluoro-3-hydroxy-2-methyl-3-(trifluoromethyl)-1-butanone","34844-23-0","D",0]
["8-Bromo-3,3,4,4,5,5,6,6,7,7,8,8-dodecafluorooct-1-ene","910563-62-1","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol, reduced, reaction products with methacrylic anhydride","161212-20-0","D",0]
["2-[2-[(Perfluorononyl)ethoxy]ethoxy]ethanol dihydrogen phosphate, disodium salt","138473-75-3","D",0]
["[Perfluoro-2-(trifluoromethoxy)propoxy]-2-propene","141652-05-3","D",0]
["2-[(2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptanoyl)amino]-6-methyl-4,5,6,7-tetrahydro-1-benzothiophene-3-carboxamide","6350-80-7","D",0]
["6-Chloro-N-(2,2,3,3,4,4,4-heptafluorobutyl)-5-phenyl-1H-indazol-3-amine","","D",0]
["2,3,4,5,7,7,8-Heptafluoro-8-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)bicyclo[4.2.0]octa-1,3,5-triene","103634-36-2","D",0]
["4,4,4-trifluoro-3-hydroxy-2-methyl-1-(thiophen-2-yl)-3-(trifluoromethyl)butan-1-one","34844-35-4","D",0]
["3-Hydroxy-3-[(3,3,4,4,4-pentafluorobutyl)sulfanyl]propanoic acid","","D",0]
["1-Chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-8-iodotetradecane","118673-04-4","D",0]
["4-(Pentafluoroethyl)aniline","60979-04-6","D",0]
["3-[(1,3-Dihydroxy-3-(perfluorodecyl)propan-2-yl)sulfanyl]propanoic acid","","D",0]
["1-Octanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, reaction products with succinic anhydride monopolyisobutylene derivs.","253682-96-1","D",0]
["1-[(Pentadecafluoroheptyl)oxy]octane","91913-68-7","D",0]
["Sodium mono(N-ethyl-2-perfluorooctylsulfonaminoethyl)sulfate","2624-81-9","D",0]
["1,4-Dichloro-2-(1,1,2,2-tetrafluoroethyl)benzene","650-67-9","D",0]
["4,4,4-trifluoro-3-hydroxy-2-methyl-1-phenyl-3-(trifluoromethyl)butan-1-one","34844-07-0","D",0]
["3-(heptafluoropropyl)-5-(trifluoromethyl)-1h-pyrazole","261761-18-6","D",0]
["7-Chloro-perfluoroheptanoic acid","1550-24-9","D",0]
["3,4-Dihydro-3-[(3-pyridinylmethyl)amino]-6-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-2(1H)-quinazolinone","337457-78-0","D",0]
["N-(2-Hydroxyethyl)-N-methyl-N-(3-sulfopropyl)-3-[[(perfluorohexyl)sulfonyl]amino]-1-propanaminium","2089108-76-7","D",0]
["S-(1,1,2,2-Tetrafluoroethyl)cysteine","94840-66-1","D",0]
["(7E)-1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluorooctadec-7-ene","125081-49-4","D",0]
["N-(1,1,2,2,3,3,4,4,5,5,6,6,6-Tridecafluorohexane-1-sulfinyl)benzenesulfonamide","61424-50-8","D",0]
["1,1,2,3,4,4,5,5,6,6,6-Undecafluorohex-2-en-1-yl sulfurofluoridate","88022-44-0","D",0]
["4,4-Bis[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)sulfanyl]pentanoic acid","92886-04-9","D",0]
["3-(Perfluorodecyl)propane-1-sulfonic acid","","D",0]
["11:1:2 Fluorotelomer betaine","171184-05-7","D",0]
["Bis(1,1,2,2,3,3,4,4-octafluorobutyl)mercury","67318-96-1","D",0]
["1,1,1,2,2-Pentafluoro-2-{fluoro[bis(pentafluoroethoxy)]methoxy}ethane","130085-22-2","D",0]
["2-(2-Chloro-1,1,2,2-tetrafluoroethoxy)-1,1,2,2-tetrafluoroethane-1-sulfonamide","148716-43-2","D",0]
["1,1,4,4,5,5,5-Heptafluoro-2-(trifluoromethyl)-1-pentene","90277-95-5","D",0]
["2-Chloro-3,4,4,5,5-pentafluorocyclopent-2-en-1-one","6681-60-3","D",0]
["[1,1,2-Trifluoro-2-(heptafluoropropoxy)ethoxy]benzene","95454-42-5","D",0]
["4-(Heptafluoropropyl)-1,3-dihydro-2H-1,5-benzodiazepin-2-one","96146-10-0","D",0]
["N-(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptanimidoyl)benzenecarboximidamide","123528-68-7","D",0]
["2-[(1,1,1,3,3,3-hexafluoro-2-phenylpropan-2-yl)oxymethyl]oxirane","25056-11-5","D",0]
["N-(Perfluoroethanesulfonyl)-N-(3-dimethylaminopropyl)-3-aminopropanoic acid","","D",0]
["6:2 Fluorotelomer sulfonamido N,N-dimethyl amine","1383438-86-5","D",0]
["2-[(Oxiran-2-yl)methoxy] perfluoroethane-1-sulfonyl fluoride","127197-13-1","D",0]
["Tetraethyl (3,3,4,4,5,5-hexafluorocyclopent-1-ene-1,2-diyl)bis(phosphonate)","4655-86-1","D",0]
["6,6-Bis(hydroxymethyl)-4,8-bis{2,2,3,3-tetrafluoro-3-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]propyl}-3,9-dioxabicyclo[9.2.2]pentadeca-1(13),11,14-triene-2,10-dione","64344-49-6","D",0]
["6-({[(Perfluorohexyl)ethylthio]carbonyl}amino)hexanal","","D",0]
["7-Chloro-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoyl fluoride","662-63-5","D",0]
["Dimethyl perfluorooctanedioate","2062-20-6","D",0]
["N~1~,N~1~,N~5~,N~5~-Tetrakis(2-chloroethyl)-2,2,3,3,4,4-hexafluoropentane-1,5-diamine--hydrogen chloride (1/1)","73771-54-7","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, 2,3-dihydroxypropyl ethers","925918-64-5","D",0]
["1-(1,1,2,3,3,3-Hexafluoropropoxy)-4-nitrobenzene","52328-79-7","D",0]
["5-Benzamido-2,4-dibromo-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","862133-37-7","D",0]
["3-Ethyl-7,8,8,9,9,10,10,11,11,12,12,13,13,13-tetradecafluorotridec-6-en-6-yl phosphate","113138-48-0","D",0]
["1,1,1,2-Tetrafluoro-8-thiocyanato-2-trifluoromethyl-octane","","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1,1-heptanediol","64739-16-8","D",0]
["Perfluoropentanoate","45167-47-3","D",0]
["5-(Heptadecafluorooctyl)-1H-imidazole","81769-56-4","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide and phosphoryl trichloride, hydrolyzed","162567-74-0","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)benzoic acid","70126-48-6","D",0]
["2,2,3,3,5,5-Hexafluoro-4,4-bis(trifluoromethyl)oxolane","61340-73-6","D",0]
["N-(2,3-Dihydroxypropyl)-3-{[(perfluorooctyl)sulfonyl]amino}-4-hydroxy-N,N-dimethyl-1-butanaminium","","D",0]
["5,5,6,6-Tetrafluoro-4-sulfanylhex-3-en-2-one","91888-59-4","D",0]
["4-(1,1,2,3,3,3-Hexafluoropropoxy)aniline","52328-81-1","D",0]
["3,3,3-Trifluoro-2,2-bis(trifluoromethyl)propanoyl fluoride","1813-18-9","D",0]
["6:2 Fluorotelomer sulfoxide hydroxyammonium","1513864-18-0","D",0]
["1,1,1,2,2,3,5,5,5-Nonafluoro-4-(trifluoromethyl)pentane","90278-00-5","D",0]
["N,N'-bis(Perfluorononanoyl)1,2-ethanediamine","97005-61-3","D",0]
["5,5,5-trifluoro-4-(trifluoromethyl)pent-3-en-2-one","1422-36-2","D",0]
["2-(Perfluoro(2-propoxy-1-propoxy)eth-2-yl)ethyldimethyl(3-methyl-3-hydroxy-4-pentynoxy)silane","1592562-45-2","D",0]
["1-(Dimethylamino)-3-(perfluorodecyl)-2-(hydroxymethoxy)propan-3-yl formate","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-8-methoxyoctane","22052-87-5","D",0]
["4-(Dimethylamino)-2-{[(perfluorononyl)sulfonyl]amino}butanoic acid","","D",0]
["1-[aziridin-1-yl(3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluorononyl)phosphoryl]aziridine","23068-13-5","D",0]
["N-(2,2,3,3,4,4,4-Heptafluorobutanoyl)-D-phenylalanine","868275-40-5","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorododecane","69125-79-7","D",0]
["Ethylammonium perfluoro-10-(trifluoromethyl)undecanoate","86917-47-7","D",0]
["1,1,1,3,3,3-Hexafluoroacetone trideuterate","109640-39-3","D",0]
["(E,E)-Perfluoro-2,4-hexadiene","83168-67-6","D",0]
["Pentanoic acid, 2,2,3,3,4,4,5,5,5-nonafluoro-, ethyl ester","424-36-2","D",0]
["1-Chloro-4-(1,1,2,2,2-pentafluoroethoxy)benzene","57076-54-7","D",0]
["2-Chloro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)pyridine","1816286-71-1","D",0]
["3,3,3',3'-tetrakis(trifluoromethyl)-1,1'-spirobi[2,1-benzoxaphosphol-1-ium]","77121-88-1","D",0]
["4:2 Unsaturated fluorotelomer alcohol","164264-89-5","D",0]
["2,4,6-Tris(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-1,3,5-triazine","10271-37-1","D",0]
["1-{[1-(1,2-Dibromo-1,2,2-trifluoroethoxy)-1,1,2,3,3,3-hexafluoropropan-2-yl]oxy}-1,1,2,2,3,3,3-heptafluoropropane","115783-72-7","D",0]
["2-Propenoic acid, 2-[[(heptadecafluorooctyl)sulfonyl]propylamino]ethyl ester, polymer with α-(1-oxo-2-propenyl)-ω-methoxypoly(oxy-1,2-ethanediyl), graft (9CI)","782479-03-2","D",0]
["2,4,4,5,7,7,8,10,10,11,13,13,14,14,15,15,15-Heptadecafluoro-2,5,8,11-tetrakis(trifluoromethyl)-3,6,9,12-tetraoxapentadecan-1-oic acid","65150-95-0","D",0]
["N-Ethylperfluoro-1-tetradecanesulfonamide","","D",0]
["Surflon S 111  (perfluoroalkylphosphate)","84932-01-4","D",0]
["2,2,3,3-Tetrafluoro-(difluoro(methoxycarbonyl)-methoxy)propanoic acid methyl ester","50733-60-3","D",0]
["Ethyl 3,4,4,5,5,6,6,7,7,8,8,8-dodecafluorooct-2-enoate","61282-87-9","D",0]
["Methyl pentafluoropropionylacetate","104857-88-7","D",0]
["2-(Heptafluoropropyl)-6-methylquinoline","200617-36-3","D",0]
["N-[5-(Heptafluoropropyl)-1,3,4-thiadiazol-2-yl]acetamide","356795-59-0","D",0]
["N'-[(E)-(2-Hydroxyphenyl)methylene]-4-[(2,2,3,3-tetrafluoropropoxy)methyl]benzohydrazide","832148-61-5","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methyl-3-(2-methylpropane-2-sulfonyl)benzoic acid","1355554-59-4","D",0]
["Sulfuric acid--2,2,3,3,3-pentafluoropropan-1-ol (1/2)","632286-63-6","D",0]
["3-(Butane-2-sulfonyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355555-25-7","D",0]
["1,2,2,3,4,4-Hexafluorobicyclo[1.1.0]butane","94024-64-3","D",0]
["1,1,1,2,2,3,3,4,4,6,6,7,7,8,8,9,9,10,10-Nonadecafluoro-12-iodododecane","","D",0]
["Methacrylic acid, 2-(diethylamino)ethyl ester, polymer with 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl acrylate","34438-56-7","D",0]
["1,2,4,5-Tetrafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-nitrobenzene","20017-50-9","D",0]
["Bis(perfluorobutyl) phosphinic acid ytterbium(3+) salt","500776-86-3","D",0]
["Chlorodimethyl (3,3,4,4,5,5,5-heptafluoropentyl)silane","32523-11-8","D",0]
["(S)-(Perfluoropropyl)phenylmethanol","59153-45-6","D",0]
["N,N′-[Phosphinicobis(oxy-2,1-ethanediyl)]bis[N-ethyl-perfluorodecanesulfonamide]","83903-91-7","D",0]
["2-Phenyl-2-(1,2,2,2-tetrafluoroethyl)-1,3-dioxolane","93561-63-8","D",0]
["1,1,5-Trichloro-2,2,3,3,4,6,7-heptafluoro-2,3-dihydro-1H-indene","88953-10-0","D",0]
["Difluoro[1,1,2,2-tetrafluoro-2-(pentafluoroethoxy)ethoxy]acetonitrile","61324-34-3","D",0]
["Ethyl 7,7,8,8,9,9,10,10,10-nonafluoro-3-oxodecanoate","1444474-83-2","D",0]
["Nonafluorobutylepoxide","89807-87-4","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)benzene-1,3-diamine","58524-63-3","D",0]
["2-Diazo-4,4,5,5,6,6,6-heptafluoro-1-phenylhexane-1,3-dione","872186-76-0","D",0]
["2,3-Difluoro-2,3-bis(pentafluoroethyl)oxirane","74728-99-7","D",0]
["4,4,5,5,5-Pentafluoro-N-methoxy-N-methylpentanamide","1350856-28-8","D",0]
["1,1,2,2,3,3,4,4-Octafluoroundecane-5,6-dione","62679-64-5","D",0]
["2-[(2-Methylprop-2-enoyl)oxy]ethyl heptafluorobutanoate","146615-73-8","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl Azide","852527-61-8","D",0]
["4-(Nonafluorobutyl)-1,3-dihydro-2H-1,5-benzodiazepin-2-one","96146-12-2","D",0]
["N-{3-[Diethyl(methyl)azaniumyl]propyl}-2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanimidate--hydrogen iodide (1/1)","84166-38-1","D",0]
["6‐({[(Perfluorotetradecyl)ethylthio]carbonyl}amino)hexanal","","D",0]
["3-(Dimethyl(3-(((tridecafluorohexyl)sulfonyl)amino)propyl)azaniumyl)-2-hydroxypropane-1-sulfonate","2103241-09-2","D",0]
["1-Hydroperfluoroheptane","375-83-7","D",0]
["8:2 Fluorotelomer dimethyl ethyl betaine","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluoroicosane","90499-31-3","D",0]
["9,9,10,10,11,11,12,12,12-Nonafluoro-7-iodododecan-1-ol","172701-28-9","D",0]
["copper(2+) 4-(8-cyclohexyl-4,4,5,5,6,6-hexafluoro-9a,9b-dimethyl-5,6,9a,9b-tetrahydro-4H-indeno[5,4-b:6,7-b']bisthiophen-2-yl)piperidin-1-ide—1,1,1,5,5,5-hexafluoropentane-2,4-diol (1/2/2)","7229-93-8","D",0]
["N-(3-{(Carboxymethyl)[(perfluorobutyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["1-(Chloromethyl)-4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoronon-1-en-1-yl)oxy]benzene","59655-42-4","D",0]
["N-(Carboxymethyl)-4-(perfluoro[(3-(2-propyl)-4-methylpent-2-en-2-yl)oxy])-N,N-dimethylanilinium sodium","123088-71-1","D",0]
["beta-Alanine, N-[3-(methylamino)propyl]-, 2,2,3,3,4,4,5,5-octafluoro-6-[(1-oxo-2-propen-1-yl)oxy]hexyl ester","1233879-48-5","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(perfluorooctyl)sulfonyl]amino]propyl]-1-propanaminium inner salt","133082-79-8","D",0]
["3-(Heptadecafluorooctyl)oxan-2-ol","169213-95-0","D",0]
["5-Amino-1,1,1,2,2,3,3-heptafluoroheptan-4-ol--hydrogen chloride (1/1)","308-37-2","D",0]
["TRIS(1H,1H,2H,2H-PERFLUOROHEXYL)TIN HYDRIDE","240497-26-1","D",0]
["1-Hexene, 6-chloro-3,3,4,4,5,5,6,6-octafluoro-","99930-55-9","D",0]
["2-(Perfluorohexyl)ethanethiolate","","D",0]
["Iodonium, diphenyl-, 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonate (1:1)","194999-82-1","D",0]
["3-(Butane-1-sulfonyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355555-19-9","D",0]
["2‐[Dimethyl[3-(perfluorododecyl)‐2‐hydroxypropyl]azaniumyl]acetate","","D",0]
["1,1,1,4,4-Pentafluoro-4-(1,1,4,4,4-pentafluorobutoxy)butane","55757-42-1","D",0]
["1-Hexanesulfonamide, N-(3-chloro-2-hydroxypropyl)-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-methyl-","2387732-05-8","D",0]
["Decafluoro-1,2-dihydroacenaphthylene","1813-40-7","D",0]
["4,4,5-Trifluoro-2,5-bis(trifluoromethyl)-1,3-dioxolane-2-carboxylic acid","847685-12-5","D",0]
["4,4,5,5,5-Pentafluoropentanoic acid","3637-31-8","D",0]
["N-(2,2,3,3-Tetrafluoropropanoyl)-L-isoleucine","60108-43-2","D",0]
["Ethane, 1,2-diethoxy-1,1,2,2-tetrafluoro-","429674-57-7","D",0]
["((Perfluorooctyl)ethyl)silanetriol","115781-18-5","D",0]
["1,1,1,2,7,7,7-Heptafluoro-6-iodo-2,4-bis(trifluoromethyl)heptane","922523-99-7","D",0]
["N-Decyl-2,2,3,3,4,4,4-heptafluorobutanamide","120219-44-5","D",0]
["6-Bromo-1,1,1,2,2,3,3-heptafluoro-4,4-bis(trifluoromethyl)decane","125426-34-8","D",0]
["4-(Dimethylamino)-2-{[(perfluorododecyl)sulfonyl]amino}butanoic acid","","D",0]
["3,4,6-Trichloro-2-(2-chloro-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecyl)phenyl acetate","38506-78-4","D",0]
["(4Z)-2-Butyl-5,6,6,7,7,8,8,8-octafluoro-4-octenoic acid","90292-29-8","D",0]
["5,5,5-Trifluoro-4-(trifluoromethyl)pentane-1,4-diol","630414-87-8","D",0]
["2-(2-Chloro-1,1,2,2-tetrafluoroethyl)-2,3,3-trifluorooxirane","50838-67-0","D",0]
["2‐Methyl‐2‐[3‐(3,3,4,4,4‐pentafluorobutanesulfonyl)propanamido]propane‐1‐sulfonic acid","","D",0]
["(2S)-2,3,3,3-Tetrafluoro-2-methoxypropanamide","156700-94-6","D",0]
["2-[2-[(E)-2-[4-(2,2,3,3,3-Pentafluoropropoxy)phenyl]ethenyl]-3H-benzimidazol-5-yl]benzenesulfonamide","","D",0]
["2,2,3,3,3-Pentafluoropropyl 2-chloroprop-2-enoate","74359-16-3","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluorohexyl)sulfonyl]amino}-1-butanaminium","2089108-86-9","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]-1-(pentafluorophenyl)propan-1-one","70627-97-3","D",0]
["2,2,3,3,4,4-Hexafluoro-4-(1,2,2,2-tetrafluoroethoxy)butanoic acid","919005-52-0","D",0]
["3,3,4,4-Tetrafluoro-2-(pentafluoroethyl)-1,2-oxazetidine","360-46-3","D",0]
["1-Hydroxy-18:2 fluorotelomer sulfonic acid","","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-phenylhex-1-yn-3-one","67036-08-2","D",0]
["1,2-dibromo-1,2,3,3,3-pentafluoro-1-(2,2,3,3-tetrafluoropropoxy)propane","396716-51-1","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.',.alpha.''-[1,2,4-benzenetriyltris[carbonyloxy(2-iodo-3,1-propanediyl)]]tris[.omega.-fluoro-","71230-79-0","D",0]
["4-(Tridecafluorohexyl)phenyl selenocyanate","234449-45-7","D",0]
["HFC–329p","375-17-7","D",0]
["Octadecyl 2,2,3,3,4,4,4-heptafluorobutanoate","400-57-7","D",0]
["Poly(oxy-1,2-ethanediyl), α-sulfo-ω-[2-[[(heptadecafluorooctyl)sulfonyl] propylamino]ethoxy]-","90168-34-6","D",0]
["2‐[Dimethyl(3,4,4,4‐tetrafluorobutyl)azaniumyl]acetate","","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(nonafluorobutyl)butanimidoyl fluoride","103573-07-5","D",0]
["Iron(2+) cyclopenta-2,3,4,5-tetraen-2-id-1-yl 5-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)cyclopenta-1,2,3,4-tetraen-1-ide (1/1/1)","53782-20-0","D",0]
["(3-Chlorophenyl)[4-(1,1,2,2-tetrafluoroethoxy)phenyl]methanone","56426-11-0","D",0]
["Sodium (1H,1H,2H,2H-perfluorooctyl-1H,1H,2H,2H-perfluorodecyl)phosphate","","D",0]
["5,5,6,6,7,7,8,8,8-Nonafluorooctanoic acid","27854-33-7","D",0]
["1-(Tetradec-1-en-1-yl)perfluorohexane","160460-04-8","D",0]
["1-Bromo-4-(heptafluoropropyl)benzene","117874-91-6","D",0]
["5-((1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-1-nonen-1-yl)oxy)isophthalic acid","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,13,13,14,14,15,15,16,16,17,17,18,18,18-Hexacosafluorooctadecane","959462-53-4","D",0]
["Hexafluoropropan-2-one--(~2~H_2_)water (1/1)","72301-81-6","D",0]
["2-(4-Amino-3-methoxyphenyl)-1,1,1,3,3,3-hexafluoropropan-2-ol","1992-01-4","D",0]
["1,1,2,2-Tetrafluoroethanesulfonic acid","464-14-2","D",0]
["2,2,3,4,4,5,5,6,6,7,7,8,9,9-Tetradecafluorodecane-1,10-diol","71222-08-7","D",0]
["4-(Dimethylamino)-2-{[(perfluorooctyl)sulfonyl]amino}butanoic acid","","D",0]
["Sodium 2:2 fluorotelomer-1-sulfonate","27619-92-7","D",0]
["3-[(Carboxylatomethyl)[(perfluorohexyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium hydroxide sodium salt (1:1:1)","81190-39-8","D",0]
["4-[1,1,2,2,3,3-hexafluoro-3-(4-hydroxyphenyl)propyl]phenol","57558-13-1","D",0]
["1,1,2,2,3-Pentafluorodecan-1-ol","113791-64-3","D",0]
["3-Hydroxy-5,5-bis(trifluoromethyl)furan-2(5H)-one","825630-87-3","D",0]
["2,2'-(3,3,4,4,5,5-Hexafluorocyclopent-1-ene-1,2-diyl)dithiophene","566929-27-9","D",0]
["Heptadecafluoro-N-(1-methylethyl)-1-octanesulfonamide","87988-64-5","D",0]
["2‐Chloro‐2,3,3,4,4,4‐hexafluorobutanoic acid","234758-56-6","D",0]
["5,7-Bis(pentafluoroethyl)-1,8-naphthyridin-2-amine","51750-43-7","D",0]
["Bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl) phosphate ion(1-)","667465-18-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluoro-1-nonene","80793-18-6","D",0]
["15-H-Perfluoropentadecanoate","1696259-82-1","D",0]
["Ethoxydimethyl (3,3,4,4,5,5,6,6,6-nonafluorohexyl) silane","608301-21-9","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-7,7-diisocyanatoheptane","306976-22-7","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,27,27,28,28,28-Dotetracontafluorooctacosane","115249-34-8","D",0]
["4-[(Undecafluorohexyl)oxy]-benzenesulfonyl chloride","59493-81-1","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluoropropanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["2-Butenedioic acid (2Z)-, bis(2-ethylhexyl) ester, polymer with chloroethene, N,N-dimethyl-2-propenamide,.alpha.-fluoro-.omega.-[2-[(1-oxo-2-propenyl)oxy]ethyl]poly(difluoromethylene), 2-hydroxyethyl 2-propenoate and 2-[[[[[1,3,3-trimethyl-5-[[[[(1-methyl","152286-22-1","D",0]
["2-{[(2,2,3,3,4,4,5,5-Octafluoropentyl)oxy]methyl}oxirane","19932-27-5","D",0]
["1-(3,4-Dimethylphenyl)-1,1,2,3,3,3-hexafluoropropan-2-ol","2379-17-1","D",0]
["Sodium (1H,1H,2H,2H-perfluorooctyl-1H,1H,2H,2H-perfluorodecyl)phosphinate","","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-5-methylcyclopentane","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluoro-14-iodoicosane","93454-69-4","D",0]
["1-(2-Bromo-1,1,1,3,3,3-hexafluoropropan-2-yl)-4-fluorobenzene","67715-98-4","D",0]
["Trimethyl[3-(perfluorotetradecyl)‐2‐hydroxypropyl]azanium","","D",0]
["3-{[3-(Dimethylamino)propyl][(perfluorotetradecyl)sulfonyl]amino}propanoic acid","","D",0]
["2-(2,3-Dichloro-1,1,2,3,3-pentafluoropropyl)-2,3,3-trifluorooxirane","15453-07-3","D",0]
["Ethyl difluoro(1,1,2,2-tetrafluoroethoxy)acetate","88239-69-4","D",0]
["Bis{4-[3,3,4,4,5,5,5-heptafluoro-2,2-bis(trifluoromethyl)pentyl]phenyl}(phenyl)phosphane","322647-83-6","D",0]
["Poly[oxy(1,1,2,2-tetrafluoro-1,2-ethanediyl)], α-(carboxydifluoromethyl)-ω-(1,1,2,2,2-pentafluoroethoxy)-","72264-73-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptanoyl Fluoride","5927-65-1","D",0]
["Hydrazine, (2,2,3,3-tetrafluoropropyl)-","667916-14-5","D",0]
["2-[2-(Perfluorooctyl)ethylsulfanyl]acetic acid","54207-61-3","D",0]
["1-(Pentafluoroethyl)cyclohex-2-en-1-ol","101417-71-4","D",0]
["Perfluoromethylpropyl-(4-methylcyclohexyl)-amine","444658-69-9","D",0]
["Diethyl (3,3,4,4,5,5,6,6,6-nonafluorohexyl)phosphonate","627909-24-4","D",0]
["2,2,4,4-Tetrafluoro-2H,4H-1,3-benzodioxin-6-amine","25854-59-5","D",0]
["(Heptadecafluorooctyl)(dimethyl)silane","198283-43-1","D",0]
["1,1,1,2,2,3,3,4,4,7,7,7-Dodecafluoroheptane","503189-11-5","D",0]
["1,1,1,2-tetrafluoro-4-iodo-2-(trifluoromethoxy)butane","200501-96-8","D",0]
["1-(Chloromethyl)-4-[(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-en-1-yl)oxy]benzene","59655-40-2","D",0]
["Perfluoro-5-propylcyclohexane-1-carboxylic acid","","D",0]
["Perfluorodecyl hydrogen sulfate","","D",0]
["2-Methyl-1-(1,1,2,2-tetrafluoroethyl)-1H-imidazole","1259056-68-2","D",0]
["1,1,1,2,3,3,4,4-Octafluoro-6-iodo-2-(trifluoromethyl)hexane","65975-05-5","D",0]
["5-(2-Aminohexafluoroprop-2-yl)-2'-deoxyuridine","111712-54-0","D",0]
["Octadecafluorononanoylfluoride","558-95-2","D",0]
["1-Methoxy-2-[(1,2,3,3,3-pentafluoroprop-1-en-1-yl)sulfanyl]benzene","921603-76-1","D",0]
["2-Vinylperfluorobutane","239795-57-4","D",0]
["3-(((4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,9,9-Heptadecafluoro-8-nonen-1-yl)oxy)phenyl)sulfonyl)amino)-N,N,N-trimethyl-1-propanaminium","","D",0]
["Sodium 3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluorononyl)oxy]-1-propanesulfonate","29811-18-5","D",0]
["16:2 Fluorotelomer sulfonamido propyl betaine","278598-49-5","D",0]
["3-Pyridinecarboxamide, N-[4-(nonafluorobutoxy)phenyl]-","62315-07-5","D",0]
["1,1,1,2,2-Pentafluoro-2-(trifluoromethoxy)ethane","665-16-7","D",0]
["2,2-Dichloro-perfluoro-1-butanesulfonic acid","","D",0]
["(3E)-3-(2,2,3,3,4,4,4-Heptafluoro-1-hydroxybutylidene)-1,7,7-trimethylbicyclo[2.2.1]heptan-2-one--oxovanadium (2/1)","130552-91-9","D",0]
["Perfluoro-4-isopropoxybutanoic acid","801212-59-9","D",0]
["2-[3-[[(Perfluorooctyl)sulfonyl]amino]propoxy]-N,N,N-trimethylethanaminium chloride","167162-28-9","D",0]
["Decyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","183873-58-7","D",0]
["P,P-Bis(perfluoro-7-methyloctyl) phosphinic acid erbium(3+) salt (3:1)","500776-87-4","D",0]
["4-hydroxy-3-[4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-yl]naphthalene-1,2-dione","36417-26-2","D",0]
["2,2,4,4,5,5,5-Heptafluoro-3,3-bis(trifluoromethyl)pentanoic acid","558473-70-4","D",0]
["Phenyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","78755-31-4","D",0]
["2,6-Bis(2,2,3,3,4,4,5,5,5-nonafluoropentanoyl)cyclohexan-1-one","672956-77-3","D",0]
["1-Ethenyl-2-[1,1,2-trifluoro-2-(heptafluoropropoxy)ethoxy]benzene","129051-94-1","D",0]
["cis-1,1,2,2,3,4-Hexafluorocyclobutane","22819-47-2","D",0]
["Diethylmethoxy(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","608299-52-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Henicosafluoro-12-iodohenicosane","129838-42-2","D",0]
["1,1,6-Trichloro-2,2,3,3,4,5,7-heptafluoro-2,3-dihydro-1H-indene","88953-11-1","D",0]
["2:2 Fluorotelomer sulfonic acid","149246-63-9","D",0]
["2,2,3,4-Tetrafluoro-4-(trifluoromethyl)thiolane 1,1-dioxide","","D",0]
["2,2,3,3,3-Pentafluoropropyl acetate","1031928-86-5","D",0]
["4H-Perfluoro-1-butene","680-54-6","D",0]
["Perfluoro-(2,5,8-trimethyl-3,6,9-trioxadodecanoic) acid","65294-16-8","D",0]
["Ammonium 2,2,3,3-tetrafluoro-3-(1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy)propanoate","1071817-33-8","D",0]
["3,4,4,5,5,6-Hexafluoro-11-oxatetracyclo[6.2.1.0~2,7~.0~3,6~]undec-9-ene","77549-76-9","D",0]
["1,1,1,3,3,3-Hexafluoro-2-methoxy-2-propanol","662-16-8","D",0]
["2-(Difluoromethyl)-1,1,1,2,3,3,4,4,5,5,6,7,7,7-tetradecafluoro-6-(trifluoromethyl)heptane","801287-29-6","D",0]
["1,1'-(2,2,3,4,4,4-Hexafluorobutane-1,1-diyl)dibenzene","89185-52-4","D",0]
["Heptafluoropropyl","3170-79-4","D",0]
["8H-Perfluorooctanoic acid","13973-14-3","D",0]
["HFE–347mcf2","171182-95-9","D",0]
["[4-(Heptadecafluorooctyl)phenyl]methanol","163114-33-8","D",0]
["3,4,5-Tris(1,1,2,3,3,3-hexafluoropropoxy)benzoic acid","75860-09-2","D",0]
["2,3,3,4,4,4-Hexafluoro-2-(trifluoromethyl)butanoyl fluoride","754-49-4","D",0]
["2'-Deoxy-5-(heptafluoropropyl)uridine","1033630-69-1","D",0]
["N-(1,1,1,3,3,3-Hexafluoro-2-propanyl)acetamide","65261-02-1","D",0]
["3-[{3-[(Carboxymethyl)(perfluoroundecanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["Trimethyl(3‐{2‐[(perfluorobutyl)ethylthio]acetamido}propyl)azanium","","D",0]
["Cesium perfluorooctanoate","17125-60-9","D",0]
["3-[(2,2,3,3,4,4,4-Heptafluorobutoxy)methyl]-3-methyloxetane","156294-55-2","D",0]
["2,4-Dichlorophenyl nonafluorobutane-1-sulfonate","32848-21-8","D",0]
["2-[Ethyl(perfluorooctanoyl)amino]ethyl 2-methylprop-2-enoate","","D",0]
["1-Fluoro-4-(1,1,2,2-tetrafluoroethoxy)benzene","887268-36-2","D",0]
["2-Chloro-2,3,3,3-tetrafluoropropyl 2-methylprop-2-enoate","112147-50-9","D",0]
["1,1,3,4,4,4-Hexafluoro-3-(trifluoromethyl)butan-2-one","64081-04-5","D",0]
["5-Chloro-6,8-dihydroxy-3-(pentafluoroethyl)-3,4-dihydro-1H-2-benzopyran-7-carboxylic acid","142689-10-9","D",0]
["N-[(4-Chlorophenyl)carbamoyl]-2,2,3,3,3-pentafluoropropanamide","736-45-8","D",0]
["Ammonium perfluoro-2-[(6-chlorohexyl)oxy]ethane-1-sulfonate","1383434-28-3","D",0]
["4-Bromo-3,3,4,4-tetrafluorobutyl prop-2-enoate","193758-80-4","D",0]
["2,3,3,3-Tetrafluoro-2-methylpropanoic acid","917951-59-8","D",0]
["Pentanamide, 2,2,3,3,4,4,5,5,5-nonafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","549499-54-9","D",0]
["2-Bromo-1,1,2,3,3,4,5,6,7-nonafluoro-2,3-dihydro-1H-indene","88953-14-4","D",0]
["1,1,1,2,2-PENTAFLUORO-4-METHYL-PENTAN-3-ONE","357-28-8","D",0]
["15:1:2 Fluorotelomer betaine","1513864-15-7","D",0]
["Nonanoic acid, 9-chloro-2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro-","865-79-2","D",0]
["Trimethyl{[1,1,1-trifluoro-4-phenyl-2-(trifluoromethyl)but-3-en-2-yl]oxy}silane","247912-50-1","D",0]
["1H,1H-Heptafluorobutyl triflate","6401-01-0","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-{[(perfluorononyl)sulfonyl]amino}-1-propanaminium","","D",0]
["3-(Dimethyl{3-[methyl(perfluoroheptanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1-methoxypentan-1-ol","88332-84-7","D",0]
["1,3,4,4,4-Pentafluoro-3-(trifluoromethyl)but-1-ene","","D",0]
["1,1,2,2-Tetrafluoro-1-iodo-2-(trifluoromethoxy)ethane","1561-52-0","D",0]
["3,4,5-Tris(1,1,2,2-tetrafluoroethoxy)benzeneethanamine, hydrochloride","70126-64-6","D",0]
["2-Bromo-6-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)aniline","","D",0]
["Fluethiazide","23141-80-2","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluoroheptyl)sulfonyl]amino}-1-butanaminium","","D",0]
["3:2 Fluorotelomer alcohol","755-40-8","D",0]
["N-(2,2,3,3,4-Pentafluorocyclobutylidene)hydroxylamine","45846-68-2","D",0]
["3-(2,2,3,3,3-Pentafluoropropoxy)propanenitrile","1365808-65-6","D",0]
["1-(2,5-dimethoxyphenyl)-4,4,4-trifluoro-3-(trifluoromethyl)but-2-en-1-one","35554-24-6","D",0]
["D-Galactose 6-(sodium 1,7-di-(perfluorooctyl)-3-heptyl phosphate)","172916-26-6","D",0]
["N-(Pentafluoroethyl)aniline","61881-21-8","D",0]
["Pentafluoroethyl trifluoroacetate","30952-31-9","D",0]
["1-phenylpiperazine; 2,2,3,3,4,4,5,5,6,6,6-undecafluorohexanoic acid","985-60-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluorononane-1,1-diol","191528-99-1","D",0]
["Perfluorononane-1-sulfinic acid","","D",0]
["[3-(1,1,2,2-Tetrafluoroethoxy)phenyl]hydrazine","62270-21-7","D",0]
["D-Galactose 6-(1,7-di-(perfluorooctyl)-3-heptyl hydrogen phosphate)","747387-21-9","D",0]
["1,3-Bis[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)oxy]propan-2-ol","384828-83-5","D",0]
["[2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propyl]oxirane","74328-57-7","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., fluorinated, reduced ","1423039-10-4","D",0]
["2,3,3,3-Tetrafluoro-1-(pyrrolidin-1-yl)propan-1-one","113985-87-8","D",0]
["4-Chloro-3,3,4,4-tetrafluoro-1-iodobut-1-ene","150223-07-7","D",0]
["1,2,3,4,5-Pentafluoro-6-(heptafluoropropyl)benzene","54326-26-0","D",0]
["[({[(5,5,6,6,7,7,8,8,8-Nonafluoro-2-methyloctan-2-yl)oxy]carbonyl}oxy)imino](phenyl)acetonitrile","892154-46-0","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentyl 4-methylbenzene-1-sulfonate","2264-00-8","D",0]
["(2Z)-4,5,5,6,6,6-Hexafluoro-2-iodo-4-(trifluoromethyl)hex-2-en-1-ol","261503-77-9","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(2,2,3,3,4,4,4-heptafluorobutanoyl)-N-[2-(3-hydroxy-4-methoxyphenyl)ethyl]butanamide","55429-09-9","D",0]
["N,N-Dimethyl-N-(3-sulfonatopropyl)-3-[[(perfluorobutyl)sulfonyl]amino]propanaminium","864069-52-3","D",0]
["2‐(N‐Methyl-perfluorotridecanesulfonamido)acetic acid","","D",0]
["4,5-Difluoro-2,2-bis(trifluoromethyl)-1,3-dioxole","37697-64-6","D",0]
["{4-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecyl)oxy]phenyl}methanol","892155-69-0","D",0]
["(2-Naphthalenyl)perfluorobutanamide","582-00-3","D",0]
["5-Iodoethyl-perfluoro-3-oxapentanesulfonyl fluoride","84271-36-3","D",0]
["3-(tert-Butylsulfanyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355554-81-2","D",0]
["Sodium 2,2,3,3,4,4,5,5-octafluoropentanoate","22715-46-4","D",0]
["(Ethoxydifluoromethyl)undecafluorocyclohexane","181214-66-4","D",0]
["1-Methyl-2-(nonafluorobutyl)-1H-indole","1608112-35-1","D",0]
["Phosphorous acid--2,2,3,3,4,4,5,5-octafluoropentan-1-ol (1/3)","65611-17-8","D",0]
["[(3,3,4,4,4-Pentafluorobut-1-yn-1-yl)oxy]benzene","112586-73-9","D",0]
["3-[Dimethyl(3-{[(perfluorododecyl)sulfonyl]amino}propyl)ammonio]propanoate","","D",0]
["1,1,2,2,3,3,4,4,5,6-Decafluoro-5,6-bis(pentafluoroethyl)cyclohexane","75169-49-2","D",0]
["1,4-Bis(chloromethyl)-2-(heptafluoropropyl)benzene","139263-35-7","D",0]
["Prop-2-en-1-yl heptadecafluorononanoate","117374-33-1","D",0]
["4:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["2,2,3,4,4,4-Hexafluorobutyl 2,3-difluoropropanoate","131644-91-2","D",0]
["1,4-Bis(perfluoroethyl)butane","1835251-87-0","D",0]
["Trifluorotris(pentafluoroethyl)phosphate","123199-69-9","D",0]
["Bis(2-chloro-3,3,4,4,5,5,6,6-octafluoro-1-cyclohexen-1-yl)mercury","49771-67-7","D",0]
["N,N-bis(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonylamine lithium salt","119229-99-1","D",0]
["1-[2-Methoxy-5-(pentafluoroethyl)phenyl]ethan-1-one","873314-98-8","D",0]
["(Perfluoro-1-butyl)butane-1,3-dione","355-84-0","D",0]
["2,2'-(2,3,5,6-Tetrafluoro-1,4-phenylene)bis(hexafluoropropan-2-ol)","13732-55-3","D",0]
["Copper(2+) bis(1,1,2,2-tetrafluoro-6,6-dimethyl-3,5-dioxo-1-(trifluoromethoxy)heptan-4-ide)","80289-21-0","D",0]
["N-Fluoro-N-(nonafluorobutyl)hypofluorous amide (non-preferred name)","812-47-5","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(1,1,2,2-tetrafluoropropoxy)-","1643531-85-4","D",0]
["Cyclohexyl 2,2,3,3-tetrafluoro-3-phenoxypropanoate","873013-81-1","D",0]
["1,1,1,2,2,3,4,5,5,6,6,7,7,8,8,8-Hexadecafluorooct-3-ene","35844-82-7","D",0]
["Methyl 2-bromo-2,3,3,4,4,4-hexafluorobutanoate","63867-09-4","D",0]
["Phosphine, 1,2-ethanediylbis[bis(pentafluoroethyl)-","120263-08-3","D",0]
["N-(Carboxymethyl)-3-[(carboxymethyl)(1,1,2,2,3,3,3-heptafluoropropane-1-sulfonyl)amino]-N,N-dimethylpropan-1-aminium","2089109-87-3","D",0]
["1-Chloro-2-(1,1,2,2-tetrafluoroethoxy)benzene","957372-65-5","D",0]
["1,3,3,4,4,5,5,6,6-Nonafluoro-2-iodocyclohex-1-ene","14315-34-5","D",0]
["2,2,3,3-Tetrafluoropropyl ether","82914-35-0","D",0]
["2-Amino-5-(1,2,2,3,3,4,4,5,5,5-decafluoropentyl)benzoic acid","","D",0]
["2,2,3,3,4,4,5-Heptafluoro-5-iodooxolane","827601-55-8","D",0]
["1,1,1,3,5,5,5-Heptachloro-2,2,3,4,4-pentafluoropentane","53281-43-9","D",0]
["3,3,4,4,4-Pentafluoro-1-(pyridin-2-yl)butan-2-one","337-29-1","D",0]
["6‐({[(Perfluorodecyl)ethylthio]carbonyl}amino)hexanal","","D",0]
["Methyl 2,2,3,3-tetrafluoro-3-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]propanoate","51502-43-3","D",0]
["4-(Heptadecafluorooctyl)phenyl prop-2-enoate","649721-89-1","D",0]
["2-(Heptafluoropropyl)-1,3,5-trimethoxybenzene","1422444-58-3","D",0]
["N,N,N-Trimethyl-3-[(perfluoro-1-oxononyl)amino]-1-propanaminium iodide","62501-48-8","D",0]
["Octafluorobutane-1,4-disulfinic acid","115416-68-7","D",0]
["N-(2-Hydroxyethyl)-3-[[(perfluorooctyl)sulfonyl](2-hydroxyethyl)amino]-N,N-dimethyl-1-propanaminium","2089109-03-3","D",0]
["4-fluoro-6-(1,1,2,2,2-pentafluoroethyl)-5-(trifluoromethyl)pyrimidin-2-amine","7224-07-9","D",0]
["Trichloro[4,4,4-trifluoro-3,3-bis(trifluoromethyl)butyl]silane","62281-43-0","D",0]
["1,1,1-Trichloro-2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptane","88639-56-9","D",0]
["3-Chloro-1,1,3,5,5-pentamethyl-1,5-bis(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)trisiloxane","521069-01-2","D",0]
["1,1,2,2,3,4,4,5,6-Nonafluorocyclohexane","22150-51-2","D",0]
["2-Chloro-5-[4-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]pyrazol-1-yl]benzoic acid","","D",0]
["5-Isoxazolol, 4,5-dihydro-3-phenyl-5-(1,1,2,2-tetrafluoroethyl)-","184293-63-8","D",0]
["7H-Perfluorooctanesulfonic acid","2089109-58-8","D",0]
["Methyl 3,4-dibromo-2,2,3,4,4-pentafluorobutanoate","124311-13-3","D",0]
["1,1,1,2-Tetrafluoro-2,2-diiodoethane","57171-63-8","D",0]
["(Heptadecafluorooctyl)phosphonic acid--4-methylaniline (1/1)","1263361-03-0","D",0]
["Ethanesulfonyl fluoride, 1,1,2,2-tetrafluoro-2-[(1,2,2-trifluoroethenyl)oxy]-, polymer with 1,1,2,2-tetrafluoroethene, hydrolyzed","1163733-25-2","D",0]
["3-(Dimethyl{3-[(Perfluorononanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["Methyl perfluorotridecanoate","185230-63-1","D",0]
["Propyl 2,2,3,3-tetrafluoropropanoate","89841-60-1","D",0]
["2,2,3,3,3-pentafluoropropanehydrazide","680-14-8","D",0]
["3-(Butylsulfanyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355554-72-1","D",0]
["Perfluoro-2-pentanone","377-54-8","D",0]
["Lufox","552851-31-7","D",0]
["2-[1,1,2-Trifluoro-2-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]ethoxy]acetic acid","919005-32-6","D",0]
["Sodium 1,1,2,2-tetrafluoro-2-(1,1,2,2,2-pentafluoroethoxy)ethanesulfonate","113507-87-2","D",0]
["1,3,3-Tris(1-methylethoxy)-1,3-bis(2-(perfluorohexyl)ethyl)-1-disiloxanol","1240203-10-4","D",0]
["2‐[Dimethyl(3-(perfluorotetradecyl)propyl)azaniumyl]acetate,16,16,17,17,17‐nonacosafluoroheptadecyl)azaniumyl]acetate","","D",0]
["N-[2-(Benzyloxy)-1,1,1,3,3,3-hexafluoropropan-2-yl]propanimidic acid","5226-25-5","D",0]
["Butanedioic acid, 1-[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl] ester, polymer with 2,2-difluoro-2-[1,1,2,2-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(trifluoromethyl)propoxy]ethoxy]ethyl 2-propenoate, 7-oxabicyclo[4.1.0]","1443502-50-8","D",0]
["2-Propenoic acid, 2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl ester, homopolymer","26337-50-8","D",0]
["Calcium (3Z)-1,1,1,7,7,7-hexafluoro-5-oxo-2,2,6,6-tetrakis(trifluoromethyl)hept-3-en-3-olate--water (1/2/2)","314075-40-6","D",0]
["4,4,5,5,6,6,6-Heptafluorohexan-2-yl acetate","136909-75-6","D",0]
["Dimethyl[3-(perfluorooctadecyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["N-[3-(Dimethylnitroryl)propyl]perfluoro-2-[2-(2-butoxypropoxy)propoxy]propanamide","200636-74-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-(octyldisulfanyl)octane","191213-11-3","D",0]
["N-(2,3-Dihydroxypropyl)-3-{[(perfluorodecyl)sulfonyl]amino}-4-hydroxy-N,N-dimethyl-1-butanaminium","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-6-methoxyhexane","226909-72-4","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-5-iodopentane","678-74-0","D",0]
["1-Bromo-4-(1,1,2,3,3,3-hexafluoropropoxy)benzene","52328-78-6","D",0]
["N-[3-[[(Perfluorooctyl)sulfonyl]amino]propyl]-N,N-dimethylbenzenemethanaminium chloride","53517-99-0","D",0]
["5-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-1H-indazole","1433216-39-7","D",0]
["5,5'-(((Perfluoropropane-2,2-diyl)bis(4,1-phenylene))bis(oxy))bis(isobenzofuran-1,3-dione)","61778-79-8","D",0]
["2‐[2-(Perfluorohexyl)ethylsulfanyl]acetic acid","123708-11-2","D",0]
["Perfluorooctanesulfonamido ethanol","10116-92-4","D",0]
["N-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)cyclohexanecarboxamide","1440968-37-5","D",0]
["Poly(18-26)oxyethylenemethylether acrylate-N-perfluorooctylsulfonyl-N-propylaminoethyl acrylate copolymer","152751-60-5","D",0]
["Perfluoro iso n:p acrylates","","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)but-1-ene","83168-74-5","D",0]
["(3,3,4,4,5,5,6,6,6-Nonafluoro-1-iodohexyl)cyclohexane","1464148-71-7","D",0]
["1-Bromo-1,1,2,2,4,5,5,7,8,8,10,11,11,13,14,14,16,16,17,17,17-henicosafluoro-4,7,10,13-tetrakis(trifluoromethyl)-3,6,9,12,15-pentaoxaheptadecane","1482416-52-3","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluoroundecyl)-2-fluoroethan-1-aminium","","D",0]
["1-Ethenyl-4-(heptadecafluorooctyl)benzene","106209-21-6","D",0]
["N-Cyclohexyl-2,2,3,3,4,4,4-heptafluorobutanamide","56663-38-8","D",0]
["Disulfide, bis(heptafluorobutyryl), bis(dimethylhydrazone)","4454-59-5","D",0]
["3,3,4,4-Tetrafluoro-4-(heptafluoropropoxy)but-1-ene","1152098-94-6","D",0]
["5-(1,1,2,2,3,3,3-heptafluoropropyl)-1-[[3-[[5-(1,1,2,2,3,3,3-heptafluoropropyl)tetrazol-1-yl]methyl]oxetan-3-yl]methyl]tetrazole","2613-48-1","D",0]
["1-(1-Naphthyl)-4,4,4-trifluoro-3-trifluoromethyl-2-buten-1-one","35444-07-6","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, hydrolyzed, salts with N8,N8,3-trimethyl-2,8-phenazinediamine","162492-22-0","D",0]
["6-Methoxy-5-(pentafluoroethyl)naphthalene-1-carboxylic acid","103654-81-5","D",0]
["2-[[1,1,1,3,3,3-hexafluoro-2-[3-[1,1,1,3,3,3-hexafluoro-2-(oxiran-2-ylmethoxy)propan-2-yl]phenyl]propan-2-yl]oxymethyl]oxirane","26146-93-0","D",0]
["Perfluoroeicosanesulfonic acid","","D",0]
["1,1,1,2,4,5,5,5-Octafluoro-2-(heptafluoropropoxy)-4-(trifluoromethyl)pentan-3-one","851535-00-7","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14-octacosafluorotetradecane-1-sulfonic acid","134615-59-1","D",0]
["1,6-Hexanediamine, polymers with Et esters of reduced polymd. oxidized tetrafluoroethylene","588699-63-2","D",0]
["3-(Perfluoroundecyl)propanoic acid","","D",0]
["2,2,3,3,4,5,5-Heptafluoro-4-(pentafluoroethyl)oxolane","61340-72-5","D",0]
["2,2'-{Oxybis[(1,1,2,2-tetrafluoroethane-2,1-diyl)oxy]}bis(difluoroacetyl fluoride)","24689-56-3","D",0]
["1-(Perfluorooctyl)ethyl 2-methylprop-2-enoate","","D",0]
["Hexafluoropropene, oxidized, oligomers, telomers with chlorine, reduced, reaction products with methanol and ethylenediamine","161212-25-5","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(methanesulfinyl)benzoic acid","1355554-84-5","D",0]
["2-(Nonafluorobutyl)-4H-1-benzopyran-4-one","304877-96-1","D",0]
["2‐(N‐Methyl-perfluorododecanesulfonamido)acetic acid","","D",0]
["14:2 Fluorotelomer sulfate","","D",0]
["4'-Fluoro-4,4,4-trifluoro-3-(trifluoromethyl)crotonophenone","35444-02-1","D",0]
["3-[[(Perfluoroheptyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium bromide (1:1)","167381-20-6","D",0]
["2-[(2,3,3,3-Tetrafluoropropanoyl)oxy]ethyl dodecanoate","113435-70-4","D",0]
["Perfluoro-4-methylpent-2-enoyl fluoride","88022-48-4","D",0]
["Ethyl-difluoro-methyl-(1,1,2,2,2-pentafluoroethyl)-lambda5-phosphane","","D",0]
["1-Propanol, 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2-tetrafluoropropoxy)propoxy]-","1643489-49-9","D",0]
["2,3,4,5-Tetrabromo-7,7,8,8-tetrafluorobicyclo[4.2.0]octa-1,3,5-triene","64726-07-4","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyl-3,5-octanedione - vanadium (3:1)","31183-12-7","D",0]
["Benzene, 2,4-diisocyanato-1-methyl-, reaction products with reduced Me esters of reduced polymd. oxidized tetrafluoroethylene","620963-42-0","D",0]
["N'-(Benzenesulfonyl)-2,2,3,3,3-pentafluoropropanimidohydrazide","4454-55-1","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N,N-bis(2-methoxyethyl)butane-1-sulfonamide","1427176-19-9","D",0]
["Sodium 2‐{2‐[(2,2,3,3,4,4,5,5,6,6,7,7‐dodecafluoroheptyl)oxy]‐2‐oxoethyl}benzene‐1‐sulfonate","29817-87-6","D",0]
["1-(2,2-Difluoro-2-nitroethoxy)-1,1,2,3,3,3-hexafluoropropane","65064-79-1","D",0]
["Perfluoro-N-(hexanesulfonyl)hexane‐1‐sulfonamide lithium","1639369-04-2","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with ethylene oxide, tosyl chloride and pyridine","162492-11-7","D",0]
["4-(1,1,2,2-Tetrafluoroethoxy)-1,1'-biphenyl","175838-97-8","D",0]
["(Perfluorohexyl)methane-1-sulfonic acid","1881287-99-5","D",0]
["Poly(1,1,2,2-tetrafluoro-1,2-ethanediyl), .alpha.-fluoro-.omega.-2-[3-((carboxylatomethyl) dimethylammonio)propylaminosulfonyl]ethyl-","161278-39-3","D",0]
["7-Chloro-2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptan-1-ol","76711-89-2","D",0]
["2-(4-Trimethylammoniophenyl)perfluoro(4-methyl-3-(propan-2-yl)pent-2-ene) iodide","1033035-91-4","D",0]
["1,3-Benzenedicarboxylic acid, 1,3-diphenyl ester, polymer with [1,1'-biphenyl]-3,3',4,4'-tetramine, compd. with 1,1,2,2-tetrafluoroethene polymer with 1,1,2,2-tetrafluoro-2-[(1,2,2-trifluoroethenyl)oxy]ethanesulfonic acid","1380335-29-4","D",0]
["1-[2-[Ethyl[(perfluorooctyl)sulfonyl]amino]ethyl] butanedioate potassium","92340-26-6","D",0]
["Pentadecafluorooctanoic acid--piperazine (2/1)","423-52-9","D",0]
["1-Methylperfluoropentane","188190-34-3","D",0]
["Sodium 1H,1H,2H,2H-perfluorooctylphosphate","144965-22-0","D",0]
["1,1,1-Trifluoro-4,4-dimethoxy-2-(trifluoromethyl)butane-2-thiol","62378-49-8","D",0]
["1,1,1,2,2-Pentafluoro-2-(2,2,2-trifluoroethyldisulfanyl)ethane","","D",0]
["3H-Perfluorobutanesulfonic acid","2089109-54-4","D",0]
["3,3,4,4-Tetrafluorobutyl 2-methylprop-2-enoate","138506-00-0","D",0]
["N-(3-{[(Heptafluoropropyl)sulfonyl]amino}propyl)-3,4-dihydroxy-N,N-dimethyl-1-butanaminium","","D",0]
["Silicon(4+) 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-hexadecafluoro-1-iododecan-1-ide 2,2',2''-nitrilotriethanolate (1:1:1)","135798-17-3","D",0]
["1,1,1,2-Tetrafluoro-3,3,3-trimethoxypropane","42415-18-9","D",0]
["1-Bromo-1,3,3,3-tetrafluoro-2-(trifluoromethyl)prop-1-ene","35386-45-9","D",0]
["2-bromo-2,3,3,3-tetrafluoropropanenitrile","234443-23-3","D",0]
["4-Chloro-1,1,1,3,3,4,4-heptafluorobutan-2-one","42287-76-3","D",0]
["12:2 Fluorotelomer sulfonamido propyl methyl amine","","D",0]
["[(1,2,3,3,4,4,5,5,6,6,6-Undecafluorohex-1-en-1-yl)sulfanyl]benzene","65079-22-3","D",0]
["3,3,4,4,5,5,6,6-Octafluorocyclohexane-1,2-dione","111511-41-2","D",0]
["S-Deoxo fulvestrant","153004-31-0","D",0]
["Perfluoro-N-(4-methylcyclohexyl)-1-methylpiperidinium","","D",0]
["(+)-(5Z,7E)-26,26,26,27,27,27-Hexafluoro-9,10-secocholesta-5,7,10(19)-triene-1alpha,3beta,25-triol","83805-11-2","D",0]
["1,1,2,2-Tetrafluoro-5-methyl-2,3-dihydro-1H-indene","922141-50-2","D",0]
["3-(Butane-2-sulfinyl)-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355555-01-9","D",0]
["Perfluoro-2-(perfluorobutoxy)-2-(perfluoromethyl)propanoic acid","","D",0]
["3-(Dimethyl{3-[methyl(perfluorononanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["Trimethyl({3‐[2‐(2-(perfluorododecyl)ethanesulfonyl)acetamido]propyl})azanium","","D",0]
["6-[(1,1,1,3,3,3-Hexafluoro-2-propanyl)oxy]-N'-methyl-N,N-diphenyl-1,3,5-triazine-2,4-diamine","5822-85-5","D",0]
["1,1,1,4,4,5,5,5-Octafluoro-2,3-bis(trifluoromethyl)pent-2-ene","58621-65-1","D",0]
["4-Chloro-6-(1,1,2,2-tetrafluoroethyl)-1,3,5-triazin-2-amine","1139245-14-9","D",0]
["10-Chloro-7,7,8,8,9,9,10,10-octafluoro-5-iododec-1-ene","103147-32-6","D",0]
["7,8-Bis(5,5,6,6,7,7,7-heptafluoroheptyl)tetradecanedioic acid","67224-12-8","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,8,8,8-Pentadecafluorooctyl prop-2-enoate","54841-42-8","D",0]
["1,1,1,2,2,3,3-heptafluoro-5-nitroheptane","356-66-1","D",0]
["3-({3-[(2-Hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoroundecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["N-{[2,3-Dimethyl-4-(1,1,2,2-tetrafluoroethanesulfinyl)phenyl]carbamoyl}-2,6-difluorobenzene-1-carboximidic acid","100342-05-0","D",0]
["Lithium perfluorohexanoate","90430-61-8","D",0]
["2,2,3,3-tetrafluoropropyl 4-chlorobenzoate","7238-87-1","D",0]
["Tetrafluoroethylene, oxidized, oligomers, reduced, methyl esters, reaction products with 3-aminopropyltriethoxysilane","161075-07-6","D",0]
["HFC 134a-hydrogen bromide mixture","357409-09-7","D",0]
["2,2,3,3,3-Pentafluoro-N-(1-phenylethyl)propanamide","51241-60-2","D",0]
["1-(2,3-dibromo-1,1,2,3,3-pentafluoropropyl)-2,3,4,5,6-pentafluorobenzene","1350637-12-5","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluorobutyl)sulfonyl]amino)-1-propanesulfonate","2089108-89-2","D",0]
["3-Amino-N-[2-bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)phenyl]-4-cyanobenzamide","","D",0]
["Acetic acid, bromo-, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester","132711-05-8","D",0]
["Tri(prop-2-en-1-yl)(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)silane","193828-95-4","D",0]
["6-Methyl-3-(2,2,3,3-tetrafluoropropanoyl)-4H-chromen-4-one","858369-43-4","D",0]
["Perfluoro(t-butycyclohexane)","132867-98-2","D",0]
["2-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-7-nitro-3,4-dihydronaphthalen-1(2h)-one","35474-72-7","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorononanamido)propan-1-aminium","1513863-85-8","D",0]
["1-[(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)oxy]pyrrolidine-2,5-dione","252937-66-9","D",0]
["Perfluorobutyloctyl phosphinic acid","610800-35-6","D",0]
["2,2,2',2'-Tetrakis(trifluoromethyl)-4,4'-bi-1,3-dioxolane","18045-27-7","D",0]
["3-(Perfluorononyl)‐1‐[(2‐hydroxyacetyl)sulfanyl]propan‐1‐one","","D",0]
["1,1,1,3,3-Pentafluoro-3-(1,2,2,2-tetrafluoroethoxy)propan-2-one","88457-11-8","D",0]
["Chromium, diaquatetrachloro(mu-(N-ethyl-N-((1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl)glycinato-kappaO:kappaO'))-mu-hydroxybis(2-propanol)di-","68891-98-5","D",0]
["Diaquatetrachloro(mu-(N-ethyl-N-((perfluoropentyl)sulfonyl)glycinato-O1:O1'))-mu-hydroxybis(2-propanol)dichromium","68891-99-6","D",0]
["Diaquatetrachloro(mu-(N-ethyl-N-((perfluorobutyl)sulfonyl)glycinato-O1:O1'))-mu-hydroxybis(2-propanol)dichromium","68900-97-0","D",0]
["2-Propenoic acid, eicosyl ester, polymers with branched octyl acrylate, 2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethyl acrylate, 2-[methyl[(nonafluorobutyl)sulfonyl]amino]ethyl acrylate, 2-[methyl[(pentadecafluoroheptyl)sulfonyl]amino]ethyl ¿","68909-15-9","D",0]
["1,2,4,5-Benzenetetracarboxylic acid, mixed 3-chloro-2-hydroxypropyl and gamma-omega-perfluoro-C8-14-alkyl esters","68954-01-8","D",0]
["N-ethyl-N-[(undecafluoropentyl)sulphonyl]glycine","68957-31-3","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[2-[ethyl[(perfluoroheptyl)sulfonyl]amino]ethyl]-.omega.-methoxy-","68958-60-1","D",0]
["Tetrafluoroethane beta-sultone","697-18-7","D",0]
["1,1,2-trichloro-2,3,3-trifluorocyclobutane","697-17-6","D",0]
["hexafluorocyclobutene","697-11-0","D",0]
["2,3,5-trifluorotetrahydro-4-(pentafluoroethyl)-2,3,4,5-tetrakis(trifluoromethyl)furan","69661-30-9","D",0]
["4,4'-[[2,2,2-Trifluoro-1-(trifluoromethyl)ethylidene]bis(4,1-phenyleneoxy)]bis-benzenamine","69563-88-8","D",0]
["Diaquatetrachloro(mu-(N-ethyl-N-((pentadecafluoroheptyl)sulfonyl)glycinato-O1:O1'))-mu-hydroxybis(2-propanol) chromium","68891-97-4","D",0]
["Diaquatetrachloro[mu-[N-ethyl-N-[(perfluorooctyl)sulfonyl]glycinato-O1:O1']]-mu-hydroxybis[2-methylpropanol]dichromium","68891-96-3","D",0]
["Ethene, tetrafluoro-, homopolymer, .alpha.-fluoro-.omega.-(2-hydroxyethyl)-, citrate, reaction products with 1,6-diisocyanatohexane","68891-05-4","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[1,4,4,5,5,5-hexafluoro-1,2,3-tris(trifluoromethyl)-2-pentenyl]-.omega.-methoxy-","68877-51-0","D",0]
["Poly(oxy-1,2-ethanediyl), .alpha.-[1,4,4,5,5,5-hexafluoro-1,2,3-tris(trifluoromethyl)-2-pentenyl]-.omega.-[[1,4,4,5,5,5-hexafluoro-1,2,3-tris(trifluoromethyl)-2-pentenyl]oxy]-","68877-38-3","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl ester, polymer with 2-[ethyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, 2-[ethyl[(1,1,2,2,3 ¿","68877-32-7","D",0]
["Glycine, N-ethyl-N-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-","68957-32-4","D",0]
["N-Ethyl-N-[(nonafluorobutyl)sulfonyl]glycine","68957-33-5","D",0]
["Glycine, N-ethyl-N-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-, ethyl ester","68957-53-9","D",0]
["ethyl N-ethyl-N-[(pentadecafluoroheptyl)sulphonyl]glycinate","68957-54-0","D",0]
["3-((Perfluoropentylsulfonyl)amino)-N,N,N-trimethylpropanaminium chloride","68957-55-1","D",0]
["Trimethyl-3-(((undecafluoropentyl)sulphonyl)amino)propylammonium iodide","68957-57-3","D",0]
["2,2-Bis[4-(4-nitrophenoxy)phenyl]hexafluoropropane","69563-87-7","D",0]
["Sodium N-ethyl-N-((nonafluorobutyl)sulphonyl)glycinate","68555-68-0","D",0]
["sodium N-ethyl-N-[(undecafluoropentyl)sulphonyl]glycinate","68555-69-1","D",0]
["Glycine, N-ethyl-N-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-, sodium salt (1:1)","68555-70-4","D",0]
["sodium N-ethyl-N-[(pentadecafluoroheptyl)sulphonyl]glycinate","68555-71-5","D",0]
["N-Ethylundecafluoro-N-(2-hydroxyethyl)-1-pentanesulfonamide","68555-72-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl ester, telomer with 2-[ethyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, 2-[ethyl[(1,1,2,2,3,3,4 ¿","68867-62-9","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-(2-(ethyl((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl)amino)ethyl)-omega-methoxy-","68958-61-2","D",0]
["Benzenemethanaminium, N-(carboxymethyl)-4-[(heptadecafluorononenyl)oxy]-N,N-dimethyl-, inner salt","68972-29-2","D",0]
["Borate(1-), tetrafluoro-, potassium (1:1), reaction products with alumina, boric acid, boron potassium oxide (B5KO8), lithium chloride, potassium chloride, potassium fluoride (K(HF2)) and zinc chloride","68987-53-1","D",0]
["Borate(1-), tetrafluoro-, potassium (1:1), reaction products with boric acid and potassium fluoride (K(HF2))","68987-54-2","D",0]
["Borate(1-), tetrafluoro-, potassium (1:1), reaction products with boric acid, boron, boron potassium oxide (B4K2O7) and potassium fluoride (K(HF2))","68987-55-3","D",0]
["2-Propenoic acid, 2-methyl-, C4-18-alkyl esters, polymers with 2-[methyl[(gamma-omega-perfluoro-C8-14-alkyl)sulfonyl]amino]ethyl acrylate","68988-53-4","D",0]
["Fatty acids, C18-unsatd., dimers, diisocyanates, polymers with 2,3-bis(gamma-omega-perfluoro-C4-18-alkyl)-1,4-butanediol, 1,6-diisocyanato-2,2,4(or 2,4,4)-trimethylhexane and 2,2'-(methylimino)bis[ethanol]","68990-40-9","D",0]
["N-Methyl-4-((4,4,5,5,5-pentafluoro-3-(pentafluoroethyl)-1,2,3-tris(trifluoromethyl)-1-pentenyl)oxy)-N-(2-(phosphonooxy)ethyl)-Benzenesulfonamide","69013-34-9","D",0]
["Propane, 1,1,1,3,3,3-hexafluoro-","690-39-1","D",0]
["Propanoic acid, 3-[1-[difluoro [(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, sodium salt, polymer with tetrafluoroethene","69068-23-1","D",0]
["Perfluoro-3-{[1-(ethenyloxy)propan-2-yl]oxy}propanoic acid","69087-46-3","D",0]
["Propanoic acid, 3-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, polymer with tetrafluoroethene","69087-47-4","D",0]
["Perfluorononane sulfonamido ammonium iodide","69091-20-9","D",0]
["Methyl perfluoro-3-[(perfluoro-3-oxopropan-2-yl)oxy]propanoate","69116-72-9","D",0]
["Methyl perfluoro(8-(fluoroformyl)-5-methyl-4,7-dioxanonanoate)","69116-73-0","D",0]
["1-(6H-Perfluorohexyl)-1-(fluoren-2-yl)-N-(perfluorobutyl)sulfonyloxymethanimine","691358-66-4","D",0]
["tetrafluorooxirane","694-17-7","D",0]
["Butanoic acid, 2,2,3,3,4,4-hexafluoro-4-[(trifluorothenyl)oxy]-, sodium salt, polymer with tetrafluoroethene","69531-49-3","D",0]
["1-Propanaminium, N,N,N-trimethyl-3-[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-, iodide (1:1)","68957-58-4","D",0]
["Undecafluoropentyl 2-methylprop-2-enoate","89004-77-3","D",0]
["Difluoro(1,1,2,2-tetrafluoroethoxy)acetyl fluoride","89076-47-1","D",0]
["Butanol, (ethenyloxy)-, polymer with chlorotrifluoroethene and (ethenyloxy)cyclohexane","89461-13-2","D",0]
["tridecafluorohexanesulphenyl chloride","89987-98-4","D",0]
["1-bromo-2-(1,2-dichloro-1,2,2-trifluoroethoxy)-1,1,2,2-tetrafluoroethane","85720-82-7","D",0]
["Potassium perfluorododecanesulfonate","85187-17-3","D",0]
["o-(1,1,2,2-tetrafluoroethoxy)benzaldehyde","85187-22-0","D",0]
["N-[[4-[(Heptadecafluorononenyl)oxy]phenyl]sulfonyl]-N-methylglycine sodium salt","85228-95-1","D",0]
["Sodium 4-{[(4E)-4,6-dimethylhept-4-en-3-yl]oxy}benzene-1-sulfonate","85284-15-7","D",0]
["Sodium 4-(perfluoro(2-methylpent-2-en-3-yl)oxy)benzene-1-sulfonate","85284-17-9","D",0]
["N-[3-(Methylamino)propyl]perfluorohexanesulfonamide","85520-91-8","D",0]
["(2H-Perfluoroethoxy)methyloxirane","85567-21-1","D",0]
["1-ethoxy-2-(1,1,2,2-tetrafluoroethoxy)ethane","85567-23-3","D",0]
["Ethanesulfonic acid, 2-[1-[difluoro[(trifluoroethenyl)oxymethyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoro-, sodium salt polymer with tetrafluoroethene","85600-80-2","D",0]
["Quaternary ammonium compoands, dimethyl(gamma-omega-perfluoro-C8-14-beta-alkenyl)[2-(sulfooxy)ethyl], inner salts","85631-40-9","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-(2-hydroxyethyl)-N-propyl-","85665-64-1","D",0]
["sodium 3-[[3-[[(heptadecafluorooctyl)sulphonyl]amino]propyl]methylamino]propanesulphonate","85665-65-2","D",0]
["Glycine, N-propyl-N-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]-, potassium salt (1:1)","85665-66-3","D",0]
["(3-(((Heptadecafluorooctyl)sulphonyl)amino)propyl)trimethylammonium hydroxide","85665-67-4","D",0]
["ethylheptadecafluorooctane","85711-89-3","D",0]
["1,1,1,2,3,4,5,5,5-nonafluoro-2-(trifluoromethyl)pentane","85720-78-1","D",0]
["Sulfuric acid, mono(gamma-omega-perfluoro-C8-14-alkyl) esters","85995-90-0","D",0]
["((Perfluorobutyl)ethyl)trimethoxysilane","85877-79-8","D",0]
["2,4,6-tris(pentafluoroethyl)-1,3,5-triazine","858-46-8","D",0]
["26,27,27,27-Tetrafluoro-25-(1,1,1,2,3,3,3-heptafluoro-2-propanyl)-24,26-bis(trifluoromethyl)-2,5,8,11,14,17,20,23-octaoxaheptacos-24-ene","88987-13-7","D",0]
["N-(3-(Dimethylamino)propyl)-1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulphonamide monohydrochlorid","68957-59-5","D",0]
["N-[3-(dimethylamino)propyl]-perfluoropentanesulfonamide hydrochloride","68957-60-8","D",0]
["1-Hexanesulfonamide, N-[3-(dimethylamino)propyl]-1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-, hydrochloride (1:1)","68957-61-9","D",0]
["N-Ethylpentadecafluoro-1-heptanesulfonamide","68957-62-0","D",0]
["N-ethyl-N-[(pentadecafluoroheptyl)sulphonyl]glycine","68957-63-1","D",0]
["2-(1,2-dichloro-1,2,2-trifluoroethoxy)-1,1,1,2,3,3,3-heptafluoropropane","85720-81-6","D",0]
["1-(1,2-dichloro-1,2,2-trifluoroethoxy)-1,1,2,2,2-pentafluoroethane","85720-80-5","D",0]
["2,3-dichloro-1,1,1,2,3,4,5,5,5-nonafluoro-4-(trifluoromethyl)pentane","85720-79-2","D",0]
["Boron, trifluoro(tetrahydrofuran)-, (T-4)-, polymer with 2-methyloxirane, 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane, oxirane and tetrahydrofuran","864910-70-3","D",0]
["1,1,1,2,2,3,4,4,5,5,5-Undecafluoro-3-(trifluoromethyl)pentane","865-71-4","D",0]
["Perfluoroisononyl iodide","865-77-0","D",0]
["1,1,1,2,2,3,3,5,6,6,6-Undecafluoro-4,4,5-tris(trifluoromethyl)hexane","86714-23-0","D",0]
["1,4-bis(3-Chloro-2-hydroxypropyl) 2,5-bis[2-[[(perfluorooctyl)sulfonyl]propylamino]ethyl] 1,2,4,5-benzenetetracarboxylate","86960-56-7","D",0]
["Propane, 1-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2,3,3,3-heptafluoro-, polymer with (2-bromo-1,1,2, 2-tetrafluoroethoxy)trifluoroethene and 1,1-difluoroethene","86999-93-1","D",0]
["2,2,3,3,4,4,5,5,6-Nonafluoro-1-(heptafluoropropyl)-6-(trifluoromethyl)piperidine","87042-39-5","D",0]
["1,1,1,2,3,3-Hexafluoro-4-(1,1,2,3,3,3-hexafluoropropoxy)pentane","870778-34-0","D",0]
["1,2-dichloro(perfluoro-1-(methoxymethoxy)ethane)","874288-98-9","D",0]
["Ethene, 1-[difluoro(trifluoromethoxy)methoxy]-1,2,2-trifluoro-, polymer with 1,1,2,2-tetrafluoroethene","874288-99-0","D",0]
["2-Propenoic acid, mixed hexaesters with dipentaerythritol and 3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)thio]propanoicacid","878409-15-5","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1,2,2-tetrafluoroethene, 1,1,2-trifluoro-2-(1,1,2,2,2-pentafluoroethoxy)ethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","878545-84-7","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl 2-propenoate","88248-34-4","D",0]
["Bis(3-chloro-2,2,3,3-tetrafluoropropionyl) peroxide","88505-66-2","D",0]
["Carbonic dichloride, reaction products with reduced ammonia-Me esters of reduced polymd. oxidized tetrafluoroethylene reaction product","88645-28-7","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced","88645-29-8","D",0]
["Sodium perfluorooctanesulfinate","68555-67-9","D",0]
["2,4,6,8,9-Pentachloro-2,3,3,4,5,5,6,7,7,8,9,9-dodecafluorononanoic acid","754-87-0","D",0]
["Perfluorooctanesulfonamide","754-91-6","D",0]
["5-Chloro-1,1,2,2,3,3,4,4-octafluoropentane","755-21-5","D",0]
["perfluorohex-1-ene","755-25-9","D",0]
["Methyl 2,2,3,3-tetrafluoro-3-methoxypropionate","755-73-7","D",0]
["1,1,2,2,3,3,4,4,5,5-decafluoro-1-[(trifluorovinyl)oxy]pentane","73928-40-2","D",0]
["6,11,14,17-Tetraoxa-7-silaeicos-1-yn-3-ol, 7,7-dibutyl-13,15,15,16,18,18,19,19,20,20,20-undecafluoro-3-methyl-13,16-bis(trifluoromethyl)-","717825-76-8","D",0]
["Propanenitrile, 3-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, polymer with tetrafluoroethene and trifluoro(trifluoromethoxy)ethene","71832-66-1","D",0]
["alpha,alpha-Bis(trifluoromethyl)benzyl alcohol","718-64-9","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, N -[2-[(2-methyl-1-oxo-2-propen-1-yl)oxy]ethyl]carbamates","721399-20-8","D",0]
["2-Propenoic acid, 2-[[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl)sulfonyl]methylamino]ethyl ester","72276-05-2","D",0]
["2-[Methyl[(perfluorododecyl)ethylsulfonyl]amino]ethyl 2-propenoate","72276-06-3","D",0]
["2-[Methyl[(perfluorotetradecyl)ethylsulfonyl]amino]ethyl 2-propenoate","72276-07-4","D",0]
["2-[Methyl[(perfluorohexadecyl)ethylsulfonyl]amino]ethyl 2-propenoate","72276-08-5","D",0]
["2-(2,4-Di-tert-pentylphenoxy)-3'-hydroxy-4'-[(5H-perfluorovaleryl)amino]hexananilide","72494-14-5","D",0]
["Acid chlorides, C8-14, .beta.-.omega.-perfluoro","72623-70-2","D",0]
["Carbamic acid, N-[4-methyl-3-[[(2-methyl-1-aziridinyl)carbonyl]amino]phenyl]-, 2-[[3,3,4,4,5,5,6,6,7,8,8,8-dodecafluoro-7-(trifluoromethyl)octyl]thio]-1-[[[3,3,4,4,5,5,6,6,7,8,8,8-dodecafluoro-7-(trifluoromethyl)octyl]thio]methyl]ethyl ester","72779-05-6","D",0]
["1-Propanesulfonic acid, 3-[[3-(dimethylamino)propyl][(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]-","72785-08-1","D",0]
["2,2,3,3,4,4,5,5-Octafluorooctyl pentanoate","72828-80-9","D",0]
["2-Butenedioic acid, mono(2,2,3,3-tetrafluoropropyl) ester, sodium salt, polymer with ethenylbenzene and disodium 2-butenedioate","72845-29-5","D",0]
["Chromium, N-[2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-docosafluoro-1-oxo-11-(trifluoromethyl)dodecyl]glycine N-[2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,10,10,10-octadecafluoro-1-oxo-9-(trifluoromethyl)decyl]glycine N-[2,2,3,3,4,4,5,5,6,6,7,8,¿","72869-27-3","D",0]
["Butanedioic acid, 2-sulfo-, 1,4-bis(mixed 2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl and 2,2,3,3,4,4,5,5-octafluoropentyl) esters, sodium salts","72905-91-0","D",0]
["Perfluoro-3,6-dimethyl-1,4-dioxan-2-one","7309-84-4","D",0]
["Perfluorooctane sulfonamido ammonium bromide","73149-44-7","D",0]
["Heptafluoropropyl iodide","754-34-7","D",0]
["1-Propanaminium, N,N,N-trimethyl-3-[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-, sulfate (2:1)","70248-52-1","D",0]
["potassium 1,1,2,2,3,3,4,4-octafluorobutane-1-sulphonate","70259-85-7","D",0]
["1,1,2,2,3,3,4,4-octafluorobutane-1-sulphonic acid","70259-86-8","D",0]
["Potassium N-((heptadecafluorooctyl)sulphonyl)-N-methylglycinate","70281-93-5","D",0]
["Cyclotetrasiloxane, 2,4,6,8-tetramethyl-, Si -mixed 3-(2-oxiranylmethoxy)propyl and 3-[2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(1,1, 2,2,3,3,3-heptafluoropropoxy)propoxy]propoxy]propyl and 2-(trimethoxysilyl)ethyl derivs.","705291-24-3","D",0]
["1-(2,2,3,3,3-pentafluoro-1-oxopropyl)-1H-imidazole","71735-32-5","D",0]
["1-Butene, 4-bromo-3,3,4,4-tetrafluoro-, polymer with 1,1-difluoroethene, 1,1,2,3,3,3-hexafluoro-1-propene and tetrafluoroethene","74398-72-4","D",0]
["Phosphoric acid, .gamma.-.omega.-perfluoro-C8-16-alkyl esters, compds. with diethanolamine","74499-44-8","D",0]
["Propane, 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]-, polymer with 1,1-difluoroethene and tetrafluoroethene","74499-68-6","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with ethene, 1,1,2,2-tetrafluoroethene and 3-(1,1,2,2-tetrafluoroethoxy)-1-propene","74499-69-7","D",0]
["1-Propene, 3-(1,1,2,2-tetrafluoroethoxy)-, polymer with ethene and 1,1,2,2-tetrafluoroethene","74499-70-0","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with ethene, 1,1,1,2,2,3,3-heptafluoro-3-((trifluoroethenyl)oxy)propane and tetrafluoroethene","74499-71-1","D",0]
["1,1,1,2,3,3,3-Heptafluoropropan-2-yl 2-methylprop-2-enoate","7459-59-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[(3,5-dimethyl-1H-pyrazol-1-yl)carbonyl]amino]ethyl ester, polymer with chloroethene, octadecyl 2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate","746622-86-6","D",0]
["BIS-AF-Sodium salt","74938-83-3","D",0]
["1-Propanesulfonic acid, 3-[ethyl[(heptadecafluorooctyl)sulfonyl]amino]-, sodium salt","75032-81-4","D",0]
["(1H,1H,7H-perfluoroheptyl)-2-sulfohexadecanoate sodium salt","75032-94-9","D",0]
["L-Glutamic acid, N-[(heptadecafluorooctyl)sulfonyl]-, disodium salt","75032-95-0","D",0]
["{[(Perfluorooctyl)sulfonyl]amino}-3-betaine","75046-16-1","D",0]
["Undecafluoroiodopentane","75330-20-0","D",0]
["Boron, trifluoro(tetrahydrofuran)-, (T-4)-, polymer with 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane, ether with 2,2-dimethyl-1,3-propanediol (2:1)","753501-40-5","D",0]
["Boron, trifluoro(tetrahydrofuran)-, (T-4)-, polymer with .alpha.-hydro-.omega.-hydroxypoly(oxy-1,2-ethanediyl) and 3-methyl-3-[(2,2,3,3,3-pentafluoropropoxy)methyl]oxetane","753501-43-8","D",0]
["2,3,3,3-Tetrafluoroprop-1-ene","754-12-1","D",0]
["Ethene, 1-[difluoro(1,1,2,2,2-pentafluoroethoxy)methoxy]-1,2,2-trifluoro-, polymer with 1,1-difluoroethene and 1,1,2,2-tetrafluoroethene","754191-93-0","D",0]
["(2-Carboxyethyl)-3-(((perfluoro-7-methyloctyl)2-hydroxypropyl)amino)propyldimethylammonium hydroxide","73353-25-0","D",0]
["(Perfluorododecyl)ethylsulfonyl chloride","68758-57-6","D",0]
["Acetic acid, [1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]difluoro-, potassium salt, polymer with tetrafluoroethene","68805-70-9","D",0]
["Benzoic acid, 2,3,4,5-tetrachloro-6-[[[3-[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]oxy]phenyl]amino]carbonyl]-, potassium salt (1:1)","68815-72-5","D",0]
["4-Bromo-(1,1,2,2-tetrafluoroethoxy)benzene","68834-05-9","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate, 2-[methyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,7- ¿","68867-60-7","D",0]
["N-Ethyl-pentadecafluoro-N-(2-hydroxyethyl)-1-heptanesulfonamide","68555-73-7","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], .alpha.-[2-[ethyl[(perfluoropentyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","68310-17-8","D",0]
["Poly[oxy(methyl-1,2-ethanediyl)], .alpha.-[2-[ethyl[(nonafluorobutyl)sulfonyl]amino]ethyl]-.omega.-hydroxy-","68310-18-9","D",0]
["3-((Perfluorooctylsulphonyl)amino)-N,N,N-trimethylpropanaminium iodide","68310-75-8","D",0]
["Cyclohexanesulfonyl fluoride, decafluoro(trifluoromethyl)-","68318-34-3","D",0]
["3-[(carboxymethyl)[(heptadecafluorooctyl)sulphonyl]amino]propyltrimethylammonium hydroxide","68318-36-5","D",0]
["2-Propenoic acid, eicosyl ester, polymer with 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate, hexadecyl 2-propenoate, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2 ¿","68329-56-6","D",0]
["Sulfonic acids, C6-12-alkane, perfluoro, potassium salts","68391-09-3","D",0]
["Silicate(2-), hexafluoro-, hydrogen, compd. with 2-aminoethanol (1:2:1)","68413-65-0","D",0]
["Hexafluoroacetone","684-16-2","D",0]
["Propane, 1,2,3-tris(ethenyloxy)-, reaction products with nitrogen fluoride (N2F4)","68457-80-7","D",0]
["trifluoroacetic trifluoroacetohydroxamic anhydride","684-78-6","D",0]
["1,4-Benzenedicarboxylic acid, esters, dimethyl ester, reaction products with bis(2-hydroxyethyl) terephthalate, ethylene glycol, .alpha.-fluoro-.omega.-(2-hydroxyethyl)poly(difluoromethylene), hexakis(methoxymethyl)melamine and polyethylene glycol","68515-62-8","D",0]
["Sulfuric acid, mono(gamma-omega-perfluoro-C6-12-alkyl) esters, ammonium salts","68516-17-6","D",0]
["Benzenesulfonyl chloride, 4-(1,1,2,2-tetrafluoroethoxy)-","68516-54-1","D",0]
["2,3,4,5-Tetrachloro-6-[3-(perfluoroheptyl)sulfonyloxyphenylamino]carbonylbenzoate potassium","68541-01-5","D",0]
["Potassium 2,3,4,5-tetrachloro-6-(((3-(((undecafluoropentyl)sulphonyl)oxy)phenyl)amino)carbonyl)benzoate","68541-02-6","D",0]
["Benzenediazonium, 4-(phenylamino)-, hexafluorophosphate(1-) (1:1), polymer with formaldehyde","68541-74-2","D",0]
["Sodium perfluoroheptanesulfinate","68555-66-8","D",0]
["2-Propenoic acid, 2-[methyl[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,17-tritriacontafluoroheptadecyl)sulfonyl]amino]ethyl ester","68758-56-5","D",0]
["1-[[3-(dimethylamino)propyl]amino]-4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)undecan-2-ol","73353-26-1","D",0]
["4-Fluoro-5-oxo-2,4-bis(trifluoromethyl)-1,3-Dioxolane-2-carbonyl fluoride","7345-49-5","D",0]
["1-Propanesulfonic acid, 3-[[3-(dimethylamino)propyl][(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-2-hydroxy-, sodium salt (1:1)","73772-32-4","D",0]
["2,2,3,3-tetrafluoropropyl acrylate","7383-71-3","D",0]
["4,4,5-Trifluoro-2,5-bis(trifluoromethyl)- 1,3-Dioxolane-2-carbonyl fluoride","7385-65-1","D",0]
["2,2,3,3,5,6,6,8,9,9-Decafluoro-5-(trifluoromethyl)-4,7-dioxa-8-nonenamide","69804-18-8","D",0]
["Undecafluoro-N-(2-hydroxyethyl)-N-methyl-1-pentanesulfonamide","68555-74-8","D",0]
["1-Hexanesulfonamide, 1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluoro-N-(2-hydroxyethyl)-N-methyl-","68555-75-9","D",0]
["Pentadecafluoro-N-(2-hydroxyethyl)-N-methyl-1-heptanesulfonamide","68555-76-0","D",0]
["Perfluorobutane-N-(3-(dimethylamino)propyl)-1-sulfonamide sulfonamido amine","68555-77-1","D",0]
["Perfluoropentane sulfonamido amine","68555-78-2","D",0]
["ethyl N-ethyl-N-[(undecafluoropentyl)sulphonyl]glycinate","68555-79-3","D",0]
["Trimethyl-3-(((pentadecafluoroheptyl)sulphonyl)amino)propylammonium chloride","68555-81-7","D",0]
["2-Propenoic acid, butyl ester, polymer with 2-(((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl)methylamino)ethyl 2-propenoate, 2-(methyl((1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl)amino)ethyl ¿","68555-90-8","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl ester, polymer with 2-[ethyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, 2-[ethyl[(1,1,2,2,3,3, ¿","68555-91-9","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl ester, polymer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, 2-[methyl[(1,1,2,2,3 ¿","68555-92-0","D",0]
["Hexafluoro-1,3-butadiene","685-63-2","D",0]
["Potassium 6-(((3-(perfluorobutylsulphonyloxy)phenyl)amino)carbonyl)perchlorobenzoate","68568-54-7","D",0]
["2-Propenoic acid, 2-methyl-, 2-[ethyl[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]amino]ethyl ester, polymer with 2-chloro-1,3-butadiene, 2-[ethyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate ¿","68568-77-4","D",0]
["2-Propenoic acid, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl ester, telomer with 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2-propenoate, alpha-(2-methyl-1-oxo-2-propen-1-yl)-omega ¿","68586-14-1","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with TDI","68608-13-9","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-ethyl-N-(hydroxyethyl), reaction products with 1,1'-methylenebis[4-isocyanatobenzene]","68608-14-0","D",0]
["1-Octanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-N-(2-hydroxyethyl)-, reaction products with N-ethyl-1,1,2,2,3,3,4,4,4-nonafluoro-N-(2-hydroxyethyl)-1-butanesulfonamide, N-ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadeca ¿","68649-26-3","D",0]
["2-[methyl[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-nonacosafluoropentadecyl)sulphonyl]amino]ethyl acrylate","68758-55-4","D",0]
["Cyclohexane, undecafluoro-, mono(perfluoro-C8-11-alkyl) derivs.","84238-52-8","D",0]
["Sulfuric acid, mono(gamma-omega-perfluoro-C8-12-alkyl) esters, ammonium salts","84238-62-0","D",0]
["Ethene, tetrafluoro-, oxidized, polymd., reduced, Me esters, reduced, 5-(trifluoromethyl)-2-pyridinyl ethers","844491-91-4","D",0]
["N-(4-Amino-2-hydroxyphenyl)-2,2,3,3,4,4,4-heptafluorobutyramide","847-51-8","D",0]
["Heptane, 1,1,1,2,3,3,4,5,5,6,7,7,7-tridecafluoro-2,4,6-tris(trifluoromethyl)-","84808-63-9","D",0]
["(2E)-4,4,5,5,6,6,7,7,7-Nonafluorohept-2-en-1-ol","83706-96-1","D",0]
["2-(2,2,3,3,4,4,5,5,5-Nonafluoropentyl)oxirane","81190-28-5","D",0]
["1-Propanaminium, N-(2-hydroxyethyl)-3-[(2-hydroxy-3-sulfopropyl)[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]-N,N-dimethyl-, hydroxide, sodium salt (1:1:1)","81190-38-7","D",0]
["1,1,1,2-tetrafluoroethane","811-97-2","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluoro-N-(4-hydroxybutyl)-N-methylbutane-1-sulphonamide","812-94-2","D",0]
["1,1,2,3,3,4,4,5,5,6,6,7,8,8-Tetradecafluoroocta-1,7-diene","812-97-5","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-Pentacosafluorotetradecan-1-amine","81313-57-7","D",0]
["Bis(perfluoroisopropyl)ketone","813-44-5","D",0]
["1,1,1,2,4,4,5,5,6,6,6-Undecafluoro-2-(trifluoromethyl)-3-hexanone","813-45-6","D",0]
["2-[Methyl[(nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, polymer with 1,1-dichloroethene and octadecyl 2-methyl-2-propenoate","819069-74-4","D",0]
["Perfluoroalkyl(C4-C14)carbonyl aminopropyl trimethyl ammonium iodide","82030-81-7","D",0]
["N,N-Dimethyl-N-(perfluoroalkyl(C4-14)carbonylaminopropyl)-.alpha.-acetic acid betaine","82030-83-9","D",0]
["Surflon S 141  (perfluoroalkylamine oxide)","82030-84-0","D",0]
["Perfluoroalkyl(C4-14)carbonyl aminomethoxy polyethylene oxide","82030-85-1","D",0]
["Sodium 2-(((perfluorohexyl)ethyloxy)carbonylamino)ethylsulfanylsulfonate","82199-07-3","D",0]
["2-(Perfluorohexyl)-1-ethanol 1-(hydrogen sulfate)","82711-15-7","D",0]
["1,1,2,2,3,3-hexafluoropropane-1,3-disulfonyldifluoride","82727-16-0","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with ethyloxirane homopolymer monoether with 1,2-propanediol mono(2-methyl-2-propenoate), tert-Bu 2-ethylhexaneperoxoate-initiated","831241-91-9","D",0]
["2-methyl-3-(1,1,2,2-tetrafluoroethoxy)propene","83168-73-4","D",0]
["allyl 3-chloro-2,2,3,3-tetrafluoropropionate","84145-21-1","D",0]
["heptadecafluorooctane-1-sulphonamide, compound with triethylamine (1:1)","76752-82-4","D",0]
["trichloro(2-chloro-2,3,3-trifluorocyclobutyl)silane","770-95-6","D",0]
["Perfluoro(oxacyclopentane)","773-14-8","D",0]
["Perfluorotetrakis(carboxyethoxymethyl)methane tetramethyl ester","773148-75-7","D",0]
["3,4,4-Trifluoro-3-(trifluoromethyl)-1,2lambda~6~-oxathietane-2,2-dione","773-15-9","D",0]
["1-chloro-1,1,2,2,3,3-hexafluoro-3-[(trifluorovinyl)oxy]propane","80962-91-0","D",0]
["(2Z)-4,5,5,5-Tetrafluoro-4-(trifluoromethyl)pent-2-en-1-ol","83706-99-4","D",0]
["Poly(oxy-1,2-ethanediyl),-methyl--[[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-butenyl]oxy]-","83731-88-8","D",0]
["methyl 2-(heptafluoropropyl)-2-(trifluoromethyl)pent-4-en-1-oate","83846-71-3","D",0]
["3-(2-chloro-1,1,2,3,3,3-hexafluoropropoxy)propene","83877-83-2","D",0]
["3-(2-chloro-1,1,2,2-tetrafluoroethoxy)propene","83877-84-3","D",0]
["2-chloro-1,1,1,2,3,3-hexafluoro-3-[(trifluorovinyl)oxy]propane","83877-85-4","D",0]
["1,1'-[butane-1,4-diylbis(oxy)]bis[heptadecafluorononene]","84029-52-7","D",0]
["10,13,16,19-Tetraoxaoctacosadiene, tetratriacontafluoro- (9CI)","84029-54-9","D",0]
["1,1'-[pentane-1,5-diylbis(oxy)]bis[heptadecafluorononene]","84029-56-1","D",0]
["1,1'-[hexane-1,6-diylbis(oxy)]bis[heptadecafluorononene]","84029-58-3","D",0]
["2,2,3,5,6-pentafluoro-5-(pentafluoroethoxy)-3,6-bis(trifluoromethyl)-1,4-dioxane","84041-66-7","D",0]
["Potassium 2,2,3,3-tetrafluoro-3-(heptafluoropropoxy)propionate","84100-11-8","D",0]
["5,6,6,7,7,7-hexafluoro-4-(trifluoromethyl)hepta-1,4-diene","84100-12-9","D",0]
["3,3,4,4,5,5,6,6,7,7,7-undecafluorohept-1-ene","84100-13-0","D",0]
["allyl perfluorovalerate","84145-17-5","D",0]
["1,1,2,2,3,3-hexafluoro-1-[(trifluorovinyl)oxy]propane","84145-18-6","D",0]
["vinyl 3-chloro-2,2,3,3-tetrafluoropropionate","84145-19-7","D",0]
["3-(3-chloro-1,1,2,2,3,3-hexafluoropropoxy)propene","84145-20-0","D",0]
["3-(1,1,2,2-Tetrafluoroethoxy)-benzenamine","831-75-4","D",0]
["Ammonium perfluoroheptanoate","6130-43-4","D",0]
["4-[[(heptadecafluorooctyl)sulphonyl]methylamino]butyl methacrylate","61577-14-8","D",0]
["N-Ethylheptadecafluoro-N-(3-(trimethoxysilyl)propyl)octanesulphonamide","61660-12-6","D",0]
["Benzene, methyl-, reaction products with sulfur chloride (S2Cl2), hexafluorophosphates(1-)","617711-03-2","D",0]
["Pyridinium, 1-(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-,4-methylbenzenesulfonate (1:1)","61798-68-3","D",0]
["Sodium 4-perfluorononyloxybenzenesulphonate","59536-17-3","D",0]
["bis(2-hydroxyethyl)ammonium bis[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluorotetradecyl] phosphate","57678-00-9","D",0]
["2-(Perfluorohexyl)ethanol dihydrogen phosphate bis(2-hydroxyethyl)amine","57678-02-1","D",0]
["12:2 Fluorotelomer dihydrogen phosphate","57678-07-6","D",0]
["Benzyl(diethylamino)diphenylphosphanium 4-[1,1,1,3,3,3-hexafluoro-2-(4-hydroxyphenyl)propan-2-yl]benzen-1-olate","577705-90-9","D",0]
["2-Propenoic acid, esters, 2-methyl-, 2-ethylhexyl ester, polymer with 4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-2-hydroxy-10-(trifluoromethyl)undecyl 2-propenoate and oxiranylmethyl 2-methyl-2-propenoate","58180-21-5","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,2,3,3-hexafluoro-3-(trifluoromethoxy)propoxy]-propanoyl fluoride","58194-00-6","D",0]
["4-[(Heptadecafluorononen-1-yl)oxy]benzoic acid","58253-65-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-N-(2-hydroxyethyl)heptanamide","58301-28-3","D",0]
["3,3,4,5,5,5-Hexafluoro-2-methylpentan-2-ol","58380-92-0","D",0]
["1,1,1,2,3,3-hexafluoro-4-methoxybutane","58705-93-4","D",0]
["allyl pentafluoropropionate","58883-50-4","D",0]
["4-[[(heptadecafluorooctyl)sulphonyl]methylamino]butyl acrylate","58920-31-3","D",0]
["2H-Perfluoro-5,8,11,14,17,20,23,26-octamethyl-3,6,9,12,15,18,21,24,27-nonaoxatriacontane","58979-41-2","D",0]
["2,2,3,3,4,4,5,5,5-nonafluoropentyl methacrylate","59006-65-4","D",0]
["2-((Ethyl(pentadecafluoroheptyl)sulfonyl)amino)ethyl acrylate","59071-10-2","D",0]
["3-(1,1,2,3,3,3-hexafluoropropoxy)propene","59158-81-5","D",0]
["3,3'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis[6-(methoxycarbonyl)benzoic acid]","59301-66-5","D",0]
["4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]benzoyl chloride","59432-83-6","D",0]
["1,3-Bis[(6H-perfluorohexyl)methoxy]-2-propanol hydrogen sulfate sodium","61119-62-8","D",0]
["allyl 3,3-dichloro-2,2,3-trifluoropropionate","83275-34-7","D",0]
["potassium 4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoroundecanoate","83310-58-1","D",0]
["2,2-Bis(3-amino-4-hydroxyphenyl)-hexafluoropropane","83558-87-6","D",0]
["Poly(oxy-1,2-ethanediyl), -[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(trifluoromethyl)-1-butenyl]-[[3,4,4,4-tetrafluoro-2-[1,2,2,2-tetrafluoro-1-(trifluoromethyl)ethyl]-1,3-bis(triSfluoromethyl)-1-butenyl]oxy]-","83563-58-0","D",0]
["(2E)-4,5,5,5-Tetrafluoro-4-(trifluoromethyl)pent-2-en-1-ol","83706-95-0","D",0]
["Perfluoroeicosanoic acid","68310-12-3","D",0]
["4,5-Dichloro-4,5-difluoro-2,2-bis(trifluoromethyl)-1,3-dioxolane","60644-92-0","D",0]
["2,2,3,3,4,4-Hexafluoro-4-iodobutanoyl fluoride","6044-18-4","D",0]
["trifluoro(1,1,2,2-tetrafluoro-2-iodoethoxy)ethylene","6037-91-8","D",0]
["Sodium perfluoroundecanoate","60871-96-7","D",0]
["Ethene, bromotrifluoro-, polymer with tetrafluoroethene and trifluoro(trifluoromethoxy)ethene","60917-27-3","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with bromotrifluoroethene, 1,1-difluoroethene","60918-83-4","D",0]
["Potassium perfluoroheptanesulfonate","60270-55-5","D",0]
["Perfluoropolyether","60164-51-4","D",0]
["Bis(2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl)sulfosuccinate sodium salt","60131-27-3","D",0]
["Pentafluoropropionaldehyde methyl hemiacetal","59872-84-3","D",0]
["1,1,1,2,4,4,5,7,7,8,10,10,11,13,13,14,16,16,17,19,19,20,22,22,23,23,24,24,24-Nonacosafluoro-5,8,11,14,17,20-hexakis(trifluoromethyl)-3,6,9,12,15,18,21-heptaoxatetracosane","59852-65-2","D",0]
["(Perfluorohexadecyl)ethyl 2-methyl-2-propenoate","59778-97-1","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1-bromo-1,2,2-trifluoroethene, 1,1-difluoroethene and 1,1,2,2-tetrafluoroethene","60918-85-6","D",0]
["1-Propene, polymer with bromotrifluoroethene and tetrafluoroethene","60918-86-7","D",0]
["2,2,3,5,6-pentafluoro-3,6-bis(trifluoromethyl)-5-[(trifluorovinyl)oxy]-1,4-dioxane","61097-79-8","D",0]
["1,1,1,2,4,5,5,5-octafluoro-2,4-bis[[2,3,5,5,6-pentafluoro-3,6-bis(trifluoromethyl)-1,4-dioxan-2-yl]oxy]pentan-3-one","61097-96-9","D",0]
["2,2'-[[1,2-difluoro-1,2-bis(trifluoromethyl)ethylene]bis(oxy)]bis[2,3,5,5,6-pentafluoro-3,6-bis(trifluoromethyl)-1,4-dioxane","61097-98-1","D",0]
["octacosafluoro-5,8,11,12,15,18-hexakis(trifluoromethyl)-4,7,10,13,16,19-hexaoxadocosane","61098-01-9","D",0]
["2,2,3,3-Tetrafluorooxetane","765-63-9","D",0]
["1,1,2,3,3,3-hexafluoro-N-(2-hydroxyethyl)-N-methyl-2-(trifluoromethyl)propane-1-sulphonamide","93762-11-9","D",0]
["1,1,2,3,3,3-hexafluoro-N,N-bis(2-hydroxyethyl)-2-(trifluoromethyl)propane-1-sulphonamide","93762-12-0","D",0]
["2-Tridecanol, 1,1'-[oxybis[(1-methyl-2,1-ethanediyl)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-heneicosafluoro- (9CI)","93776-01-3","D",0]
["2-andecanol, 1,1'-[oxybis[(1-methyl-2,1-ethanediyl)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-(9CI)","93776-02-4","D",0]
["1,1'-[oxybis[(1-methylethylene)oxy]]bis[4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,15,15,15-tetracosafluoro-14-(trifluoromethyl)pentadecan-2-ol]","93776-03-5","D",0]
["2,4,6-Tris(heptafluoropropyl)-1,3,5-triazine","915-76-4","D",0]
["Ethene, tetrafluoro-, homopolymer","9002-84-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-(acetyloxy)-4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-octadecafluoro-11-(trifluoromethyl)dodecyl ester, homopolymer (9CI)","90062-89-8","D",0]
["Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene","9011-17-0","D",0]
["Phosphonic acid, (3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl)-, compd. with N,N-diethylethanamine (9CI)","90146-97-7","D",0]
["1,3-Benzenedimethanamine, reaction products with [(1,1,2,2-tetrafluoroethoxy)methyl]oxirane","90194-06-2","D",0]
["1,3-Benzenedimethanamine, reaction products with trifluoro(trifluoromethyl)oxirane","90194-07-3","D",0]
["Benzenesulfonyl chloride, [[[(heptadecafluorooctyl)sulfonyl]amino]methyl]-, branched and linear","90218-70-5","D",0]
["Benzenesulfonyl chloride, [[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]methyl]-, branched and linear","90218-71-6","D",0]
["Copolymer of 2,2,3,3,3-pentafluoropropyl methacrylate/methyl methacrylate/methacrylic acid (The contents of component having molecular weight less than 1,000 is not more than 1 percent)","90267-56-4","D",0]
["Butanesulfonyl fluoride, nonafluoro-, branched","90268-45-4","D",0]
["1,2-Ethanediamine, N-(2-aminoethyl)-, reaction products with trifluoro(trifluoromethyl)oxirane","90366-81-7","D",0]
["1,2-Ethanediamine, N,N'-bis(2-aminoethyl)-, reaction products with trifluoro(trifluoromethyl)oxirane","90366-94-2","D",0]
["4,7-Methanoisobenzofuran-1,3-dione, 3a,4,7,7a-tetrahydro-5-methyl-, reaction products with hexahydro-1,3-isobenzofurandione and 2,2,3,3-tetrafluoro-1-propanol","90431-85-9","D",0]
["Perfluoroalkyl acrylate-, copolymer","90451-86-8","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, branched, potassium salt","90480-49-2","D",0]
["1-Octanesulfonyl fluoride, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, branched","90480-50-5","D",0]
["Phosphonic acid, perfluoro-C6-12-alkyl derivs., aluminum salts","90481-10-0","D",0]
["Alcohols, C7-22, epsilon-omega-perfluoro-, beta-delta-fluoro","90622-43-8","D",0]
["Potassium 1,1,2,3,3,3-hexafluoro-2-(trifluoromethyl)propanesulfonate","93762-10-8","D",0]
["2-Butenedioic acid (2E)-, mono(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl) ester (9CI)","86130-60-1","D",0]
["Propane, 1-[1-[difluoro[(1,2,2-trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluo ropropoxy)-, polymer with 1,1,2,2-tetrafluoroethene","86414-61-1","D",0]
["Hexaflumuron","86479-06-3","D",0]
["Perfluoro(2-bromoethoxy)ethene","85737-06-0","D",0]
["1-(1,2-dichloro-1,2,2-trifluoroethoxy)-1,1,2,2-tetrafluoro-2-iodoethane","85720-83-8","D",0]
["Polychlorotrifluoroethylene","9002-83-9","D",0]
["2-Propenoic acid, epsilon-omega-perfluoro-C8-22-alkyl esters, gamma-delta-fluoro derivs.","91648-32-7","D",0]
["Alcohols, C8-14, .gamma.-.omega.-perfluoro, reaction products with 5,5'-carbonylbis[1,3-bisbenzofurandione] and epichlorohydrin","91745-16-3","D",0]
["Sulfonyl fluorides, C1-5-alkane, omega-(ethenyloxy), perfluoro","91770-74-0","D",0]
["Alcohols, C4-8-tertiary, omega-(ethenyloxy), perfluoro","91770-94-4","D",0]
["1-Propene, 1,1,2,3,3-pentafluoro-3-(1,1,2,2,3,3,3-heptafluoropropoxy)-","91891-42-8","D",0]
["4,8-Dioxa-3H-perfluorononanoic acid","919005-14-4","D",0]
["2H-Perfluoro-2-propanol","920-66-1","D",0]
["(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-heptadecafluoro-2-hydroxyundecyl)trimethylammonium iodide","92071-84-6","D",0]
["Quaternary ammonium compoands, (hydroxyethyl)dimethyl(gamma-omega-perfluoro-C8-14-beta-alkenyl), Me sulfates (salts)","92129-34-5","D",0]
["Ethanaminium, N,N,N-trimethyl-2-(2-methyl-1-oxo-2-propenyl)oxy-, chloride, polymer with 2-ethoxyethyl 2-propenoate, 2-(heptadecafluorooctyl)sulfonylmethylaminoethyl 2-propenoate and oxiranylmethyl 2-methyl-2-propenoate","92265-81-1","D",0]
["Phosphoric acid, bis(gamma-mu-perfluoro-C8-14-alkyl) esters, compds. with diethanolamine","92332-25-7","D",0]
["Phosphoric acid, mono(gamma-mu-perfluoro-C8-14-alkyl) esters, compds. with diethanolamine","92332-26-8","D",0]
["Perfluorocyclopropane","931-91-9","D",0]
["Perfluoro-2-methyl-2-(pentyloxy)pentane","93200-92-1","D",0]
["Sulfonic acids, C6-12-alkane, perfluoro","93572-72-6","D",0]
["Copolymer of tetrafluoroethylene/hexafluoropropene/nonafluorobutyl trifluorovinyl ether (a number-average molecular weight is not less than 1,000 and the polymer is insoluble in water, lipid soluble solvent, usual solvent, acid and alkali)","93611-23-5","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecyl ester, polymer with methyl 2-methyl-2-propenoate","93705-98-7","D",0]
["Perfluoro-2-(trifluoromethyl)propanesulfonic acid","93762-09-5","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with octadecyl 2-propenoate","90718-04-0","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-Pentacosafluoro-2-iodopentadecan-1-ol","80459-24-1","D",0]
["1-Propanesulfonic acid, 3-[methyl[3-[[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexyl)sulfonyl]amino]propyl]amino]-, sodium salt (1:1)","80621-17-6","D",0]
["Perfluoro(4-ethyl-3,4-dimethylhexane)","80632-82-2","D",0]
["1,3-Dioxolane, 2-(difluoromethylene)-4,4,5-trifluoro-5-(trifluoromethyl)-, polymer with 1,1-difluoroethene","80879-54-5","D",0]
["[4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-2-hydroxy-10-(trifluoromethyl)undecyl]trimethylammonium iodide","80909-29-1","D",0]
["Methyl 7,7,8,9,9,9-hexafluorononanoate","77456-15-6","D",0]
["Flupropanate","756-09-2","D",0]
["1,1,1,3,4,4,4-Heptafluoro-3-(trifluoromethyl)butan-2-one","756-12-7","D",0]
["3-Pentanone, 1,1,1,2,2,4,5,5,5-nonafluoro-4-(trifluoromethyl)-","756-13-8","D",0]
["trichloro[3-(1,1,2,2-tetrafluoroethoxy)propyl]silane","756-76-3","D",0]
["1,1,2,2-tetrafluoro-1-(2-methoxyethoxy)ethane","757-17-5","D",0]
["Benzyltriphenylphosphonium, salt with 4,4'-(2,2,2-trifluoro-1-(trifluoromethyl)ethylidene)bis(phenol) (1:1)","75768-65-9","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1,2,2,2-tetrafluoro-1-[[(2-hydroxyethyl)amino]carbonyl]ethyl]-.omega.-[tetrafluoro(trifluoromethyl)ethoxy]-","75888-49-2","D",0]
["trifluoroacetic acid","76-05-1","D",0]
["1,1,2-Trichlorotrifluoroethane","76-13-1","D",0]
["Chloropentafluoroethane","76-15-3","D",0]
["Perfluoroethane","76-16-4","D",0]
["2-chloro-1,1,1,2,3,3,3-heptafluoropropane","76-18-6","D",0]
["Octafluoropropane","76-19-7","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(3,3,4,4,5,5,6,6,7,7,8,8,8- tridecafluorooctyl)sulfonyl]amino]propyl]-1-propanaminium, inner salt","76201-56-4","D",0]
["9-H-Perfluorononanoic acid","76-21-1","D",0]
["2,2,3,3-Tetrafluoro-1-propanol","76-37-9","D",0]
["1,3-Benzenedimethanol, .alpha.1,.alpha.1,.alpha.3,.alpha.3-tetrakis(trifluoromethyl)-","802-93-7","D",0]
["Perfluoro(2-ethoxy-2-fluoroethoxy)acetic acid ammonium salt","908020-52-0","D",0]
["magnesium bis[heptadecafluorooctanesulphonate]","91036-71-4","D",0]
["Quaternary ammonium compoands, (hydroxyethyl)dimethyl(gamma-omega-perfluoro-C8-14-beta-alkenyl), chlorides","91081-09-3","D",0]
["Sulfonamides, C4-8-alkane, perfluoro, N-(hydroxyethyl)-N-methyl, reaction products with epichlorohydrin, adipates (esters)","91081-99-1","D",0]
["2-Propenoic acid, 1,1¿-[2,2-bis[difluoro[1,1,2,2-tetrafluoro-3-[(1-oxo-2-propen-1-yl)oxy]propoxy]methyl]-1,1,3,3-tetrafluoro-1,3-propan ediyl]bis[oxy(2,2,3,3-tetrafluoro-3,1-propanediyl)] ester","912841-29-3","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1,1,2,3,3,3-heptafluoro-2-(trifluoroethenyl)oxypropane and tetrafluoroethene","85177-88-4","D",0]
["3-(Chlorosulfonyl)-2,2,3,3-tetrafluoropropanoyl chloride","77545-04-1","D",0]
["2,2,3,3-Tetrafluoro-3-(fluorosulfonyl)propanoyl fluoride","77545-05-2","D",0]
["Perfluoro(3-{[1-(ethenyloxy)propan-2-yl]oxy}propane-1-sulfonyl) fluoride","77545-07-4","D",0]
["1,1,2,2-Tetrafluoro-2-iodoethyl sulfurofluoridate","77570-00-4","D",0]
["Methyl 2,2,3,3-tetrafluoro-3-(methylsulfanyl)propanoate","77705-91-0","D",0]
["2,2,3,3-Tetrafluoro-3-(methylsulfanyl)propanoyl fluoride","77705-93-2","D",0]
["3-(Methylsulfanyl)-perfluoro(1-(ethenyloxy))propane","77706-02-6","D",0]
["[{3-[(Perfluorononanoyl)amino]propyl}(dimethyl)ammonio]acetate","77958-18-0","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-4-iodobutyl sulfurofluoridate","78522-70-0","D",0]
["vinyl 3,3-dichloro-2,2,3-trifluoropropionate","78840-97-8","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-7-(vinyloxy)heptane","78971-81-0","D",0]
["Bis(2-(perfluoro-7-methyloctyl)ethyl) hydrogen phosphate","78974-41-1","D",0]
["8:2 Fluorotelomer 9-(trifluoromethyl)-dihydrogen phosphate","78974-42-2","D",0]
["2-Propenoic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluorodecylester, polymer with alpha-(1-oxo-2-propen-1-yl)-omega-hydroxypoly[oxy(methyl-1,2-ethanediyl)]","790697-52-8","D",0]
["Poly(difluoromethylene), alpha-chloro-omega-(2,2-dichloro-1,1,2-trif...","79070-11-4","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-pentacosafluorododecane-1-sulphonic acid","79780-39-5","D",0]
["Difluoro(1,1,2,2-tetrafluoro-2-iodoethoxy)acetyl fluoride","80016-48-4","D",0]
["4,4,5,5,6,6,7,7,7-Nonafluoro-2-iodoheptan-1-ol","80233-96-1","D",0]
["Silicate(2-), hexafluoro-, ammonium (1:2), reaction products with silica","70248-10-1","D",0]
["4,4-Bis(ethylsulfanyl)-1,1,1,2,2,3,3-heptafluorobutane","145327-73-7","D",0]
["Methyl 7H-perfluoroheptanoate","84567-13-5","D",0]
["9,9,10-Trifluoro-10-(trifluoromethyl)tetracyclo[6.2.1.13,6.02,7]dodec-4-ene","","D",0]
["{[(Perfluoroethyl)sulfonyl]amino}-3-betaine","","D",0]
["ALLYLTRIS(3,3,4,4,5,5,6,6,6-NONAFLUOROHEXYL)STANNANE","215186-99-5","D",0]
["Tetrafluoroethylene, polymer with ethene, trifluoro(trifluoromethoxy)-, propane, 1,1,2,2,3,3-hexafluoro-1-(trifluoroethenyl)oxy-3-(trifluoromethoxy)-, and ethene, bromotrifluoro-","445019-64-7","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Nonadecafluoroundec-1-ene","57216-75-8","D",0]
["1-Bromo-3-(tridecafluorohexyl)benzene","157829-77-1","D",0]
["5-(Heptafluoropropyl)dihydropyrimidine-2,4(1H,3H)-dione","90715-84-7","D",0]
["4,4,4-trifluoro-1-(3-methoxyphenyl)-3-(trifluoromethyl)but-2-en-1-one","35443-95-9","D",0]
["(9E)-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoroicos-9-ene","124921-25-1","D",0]
["2,2,3,3,4-Pentafluorocyclobutane-1,1-diol","64100-30-7","D",0]
["4,5,6,7-Tetrafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-hydroxy-2-benzofuran-1(3H)-one","1419865-32-9","D",0]
["4,4,5,5,6,6,6-Heptafluorohexyl acetate","25600-64-0","D",0]
["{(2-Carboxyethyl)[(perfluorooctyl)sulfonyl]amino}-3-betaine","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-8-methylnonane","212957-49-8","D",0]
["Bis(perfluoropentanesulfonyl)amine","752232-72-7","D",0]
["3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butanoic acid","773869-22-0","D",0]
["Hexafluoroacetone-water adduct","10057-27-9","D",0]
["3,3,4,4-Tetrafluoro-1,2-dimethoxycyclobut-1-ene","361-82-0","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorododecyl)butyl]dimethylazaniumyl}acetate","","D",0]
["1,4-Butanediol, 2,3-bis[(.gamma.-.omega.-perfluoro-C4-18-alkyl)thio] derivs., polymers with 1,6-diisocyanato-2,2,4(or 2,4,4)-trimethylhexane and polyethylene-polypropylene glycol bis(2-aminomethylethyl) ether","68988-25-0","D",0]
["Perfluoro-2-(perfluoromethoxy)propanoic acid","13140-29-9","D",0]
["[(Nonafluorobutyl)disulfanyl]benzene","1606997-42-5","D",0]
["Ethyl 4,4,5,5,6,6,7,7,8,8,9,9,9-tridecafluoro-2-iodononanoate","165281-74-3","D",0]
["1,1,1,2,3,3,4-Heptafluorobutane","53005-35-9","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluorocyclohexan-1-one","1898-91-5","D",0]
["Sulfate(1-), (2-carboxylato-1,1,2,2-tetrafluoroethyl)pentafluoro-, (OC-6-21)-","777026-91-2","D",0]
["1,1,1,2,2,4,4,5,5,5-Decafluoro-3-methyl-3-(trifluoromethyl)pentane","116089-50-0","D",0]
["1-(Benzylamino)-3-(2,2,3,3-tetrafluoropropoxy)propan-2-ol","939793-35-8","D",0]
["N-Ethyl-3,3,4,4,4-pentafluorobutanamide","65527-69-7","D",0]
["{Ethyl[(perfluorononyl)sulfonyl]amino}acetic acid","1003194-09-9","D",0]
["2-(Perfluoroethyl)-1-hydroxyethanesulfonic acid","","D",0]
["(1E)-2,2,3,3,4,4,4-Heptafluoro-N-(2-phenylethyl)butan-1-imine","29723-32-8","D",0]
["2-Propyl-4-pentafluoroethyl-1-((2'-(1H-tetrazol-5-yl)biphenyl-4-yl)methyl)imidazole-5-carboxylic acid","124750-95-4","D",0]
["Carbamic acid--[2,2-bis(trifluoromethyl)-1,3-dioxolan-4-yl]methanol (1/1)","51125-52-1","D",0]
["O,O'-bis(1-Methylethyl) ethylphosphonous acid compd. with perfluoro-3-iodopropane (1:1)","80392-00-3","D",0]
["2-Chloro-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-14-6","D",0]
["N~1~-(2-Aminophenyl)-2,2,3,3-tetrafluorobutanediamide","60351-77-1","D",0]
["N,N,N-Trimethyl-(11-(difluoromethyl)perfluoroundecyl)methanaminium","","D",0]
["5-(Heptafluoropropyl)-3-phenyl-1H-1,2,4-triazole","2195-67-7","D",0]
["12,12,13,13,14,14,15,15,15-Nonafluoropentadecane-1-thiol","220414-23-3","D",0]
["Undecafluorohexan(2H)oic acid","","D",0]
["Perfluoro-1-[1-[(methoxy)methyl]-ethoxy]-2-propanone","18992-61-5","D",0]
["Perfluorocyclohexanecarbonyl bromide","261761-76-6","D",0]
["6-(Perfluorohexyl)-3,3,5,5-tetrafluorohexanol 1-(dihydrogen phosphate) ammonium salt (1:2)","1025044-26-1","D",0]
["2,2,3,3,4-Pentafluorocyclobutan-1-one","64100-29-4","D",0]
["5,5'-dimethyl-3,3,3',3'-tetrakis(trifluoromethyl)-1,1'-spirobi[2,1-benzoxaphosphol-1-ium]","71401-73-5","D",0]
["3-Ethylsulfanyl-1,1,1,2,2-pentafluoropropane","","D",0]
["N-Acetyl-S-(1,2,3,3,3-pentafluoro-1-propenyl)-L-cysteine","98640-42-7","D",0]
["6:2 Fluorotelomer ketone sulfonate","","D",0]
["4,4,5,5-Tetrafluoro-1,3-dioxolan-2-one","183301-46-4","D",0]
["3-[Bromo(difluoro)methyl]-3,4,4,4-tetrafluorobut-1-ene","2546-54-5","D",0]
["4-(Undecafluoropentyl)benzoic acid","25533-93-1","D",0]
["2-Chloroperfluorobutane","335-47-7","D",0]
["4,4'-(1,1,1,3,3,3-Hexafluoropropane-2,2-diyl)bis(2-nitrobenzoic acid)","115873-09-1","D",0]
["1,1,3,3-Tetramethyl-1,3-bis((perfluorohexyl)ethyl)disiloxane","71363-70-7","D",0]
["2-Hydroxy-2-methyl-5,5-bis(trifluoromethyl)oxolan-3-one","101833-11-8","D",0]
["1-Bromo-4-(1,1,2,2-tetrafluoro-2-phenylethyl)benzene","40396-59-6","D",0]
["1-Amino-4,4,5,5,6,6,7,7,8,8,9,9,10,11,11,11-hexadecafluoro-10-(trifluoromethyl)undecan-2-ol","54735-87-4","D",0]
["4-Methylphenyl nonafluorobutane-1-sulfonate","93131-73-8","D",0]
["2-{[2-(Acetyloxy)-3-(perfluorohexadecyl)propyl]dimethylazaniumyl}acetate","","D",0]
["Poly(oxy-1,2-ethanediyl), α-[3,4,5-tris(1,1,2,3,3,3-hexafluoropropoxy)benzoyl]-ω-methoxy-","75836-10-1","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorononyl)-2-fluoroethan-1-aminium","","D",0]
["N-(1,1,1,3,3,3-Hexafluoropropan-2-ylidene)benzenesulfinamide","63583-03-9","D",0]
["Carbamic acid, [4-methyl-3-[[(2-methyl-1-aziridinyl)carbonyl]amino]phenyl]-, 2-[[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-eicosafluoro-11-(trifluoromethyl)dodecyl]thio]-1-[[[3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,12,12,12-eicosafluoro-11-(trifluorometh","72779-04-5","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluorododecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["1,2-Dichlorodecafluorocyclohexane","336-14-1","D",0]
["Tetrafluoroethylene, polymer with ethene, 1,1-difluoro-, ethene, trifluoro(trifluoromethoxy)-, propane, 1,1,2,2,3,3-hexafluoro-1-(trifluoroethenyl)oxy-3-(trifluorom ethoxy)-, and 1-butene, 4-bromo-3,3,4,4-tetrafluoro-","1431838-83-3","D",0]
["2-[2,2-Bis(trifluoromethyl)-1,3-dioxolan-4-yl]ethan-1-ol","51125-44-1","D",0]
["2-(Perfluorohexyl)ethane sulfinic acid","","D",0]
["1,10-Dichloro-1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,10,10-octadecafluoro-2,9-dimethyldecane","103188-54-1","D",0]
["Octatriacontafluorooctadecane","24768-65-8","D",0]
["2,3,4,4,4-Pentafluoro-2-(trifluoromethyl)butanoic acid","917951-66-7","D",0]
["1-{3-[3,3,3-Trifluoro-2-(trifluoromethyl)propyl]phenyl}propan-1-one","90817-73-5","D",0]
["3-[(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptyl)amino]phenol","1441382-30-4","D",0]
["Benzenemethanol, 2-hydroxy-α,α-bis(trifluoromethyl)-","836-78-2","D",0]
["1-Ethyl-3-(1,1,2,2-tetrafluoroethyl)-2,3-dihydro-1H-imidazol-1-ium iodide","874968-22-6","D",0]
["Acetic acid--4-(heptafluoropropyl)phenol (1/1)","61324-27-4","D",0]
["Nonadecafluorodecan(2H)oic acid","","D",0]
["H-Galden 1040x","188690-77-9","D",0]
["Ethenyl 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl carbonate","96383-57-2","D",0]
["4-(Trifluoromethyl)perfluoro-3-pentanone","42287-78-5","D",0]
["7-Bromo-1,1,2,2-tetrafluoro-2,3-dihydro-1H-indene","922141-58-0","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,10-Tridecafluoro-2-hydroxydecanoic acid","90278-35-6","D",0]
["3,3,3-Trifluoro-2-(heptafluoropropoxy)propanoic acid","326495-77-6","D",0]
["1,1,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluorooct-1-ene","103712-63-6","D",0]
["1-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-sulfonyl)piperazine","113584-32-0","D",0]
["(E)-Perfluoro-2-dec-7-eneoxyacetic acid","","D",0]
["3-[Dimethyl(3-{[(perfluoropentyl)sulfonyl]amino}propyl)ammonio]propanoate","1513864-22-6","D",0]
["6-Chloro-1,1,2,2-tetrafluoro-2,3-dihydro-1H-indene","922141-61-5","D",0]
["2,2-Dichloro-perfluoro-1-heptanesulfonic acid","","D",0]
["Ether, ethyl heptafluoroisobutenyl","360-58-7","D",0]
["N,N-Dimethyl perfluorooctane sulfonamide","213181-78-3","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,9,9,10,10,11,11,12,12,13,13,14,14,14-Hexacosafluorotetradecane","53749-64-7","D",0]
["2-bromo-2,3,3,3-tetrafluoropropanoyl fluoride","6129-62-0","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl formate","856766-70-6","D",0]
["(7E)-Perfluorotetradec-7-ene-1-sulfonic acid","","D",0]
["5-Amino-2-(2-hydroxy-1,1,1,3,3,3-hexafluoro-2-propyl)benzoic acid","100811-91-4","D",0]
["1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10-Hexadecafluorodecane","40723-66-8","D",0]
["2-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-sulfinyl)ethan-1-ol","917966-98-4","D",0]
["5-Fluoro-1-(3,3,4,4,4-pentafluorobutyl)pyrazolo[3,4-b]pyridine-3-carboximidamide","","D",0]
["Thiophene, 3-(heptadecafluorooctyl)-","96721-82-3","D",0]
["1,2,2,3,3-Pentafluorobutane","119450-72-5","D",0]
["4-Bromo-1-methoxy-2-(nonafluorobutyl)benzene","610778-27-3","D",0]
["3,4,4,4-tetrafluoro-3-(trifluoromethyl)but-1-yne","24690-53-7","D",0]
["3-{(2-Carboxyethyl)[(undecafluoropentyl)sulfonyl]amino}-N-(carboxymethyl)-N,N-dimethylpropan-1-aminium","2089109-19-1","D",0]
["Ethyl 2,2,3,3-tetrafluoro-3-[(trifluoroethenyl)oxy]propanoate","63389-49-1","D",0]
["Heptadecafluoro-N-phenyl-1-octanesulfonamide","559-05-7","D",0]
["2-[Dimethyl(3-(perfluorohexyl)propyl)azaniumyl]acetate","","D",0]
["1,1,2,2,3,3,4,4,5,5,8,8,8‐Tridecafluorooctane‐1‐ sulfonate","","D",0]
["3,3,4,4,5,5,5-Heptafluoropentyl acetate","425-68-3","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluoro-N-propyloctanamide","75668-30-3","D",0]
["2,2,3,5,5,6,6,8,8,10,10,12,12,14,14,14-Hexadecafluoro-4,7,9,11,13-pentaoxatetradecanoic acid","919005-17-7","D",0]
["Methyl 4,4,6,6,7,7,9,9,10,10,12,12-dodecafluoro-3-oxo-2,5,8,11-tetraoxatridecan-13-oate","35910-59-9","D",0]
["Chloro(3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl)bis(3,3,3-trifluoropropyl)silane","608296-92-0","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced, reaction products with 1-chloro-2,3-epoxypropane","161308-24-3","D",0]
["3-Hydroxy-3-methyl-4-pentyn-1-yl perfluoro-3,6,9,12,15-pentaoxaheptadecanoate","1592562-41-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoroicosane","154628-00-9","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-N-(4-fluorophenyl)nonanamide","344282-18-4","D",0]
["Ethyl 2-(1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfinyl)prop-2-enoate","1606997-40-3","D",0]
["2-Ethyl-4,4,4-trifluoro-1-phenyl-3-(trifluoromethyl)butane-1,3-diol","34848-28-7","D",0]
["Bis(4-chlorooctafluorobutyl)ether","149697-40-5","D",0]
["Henicosafluoroundec-7-ene-1-sulfonic acid","","D",0]
["1,1,1,1,2,2,3,3,4,4,5,5-Dodecafluoro-1lambda~6~-thiepane","24345-53-7","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluorobutanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","2089108-74-5","D",0]
["1,1'-(1,1,2,2-Tetrafluoro-1,2-ethanediyl)bisbenzene","425-32-1","D",0]
["(2Z)-4,4,5,5,6,6,6-Heptafluoro-3-phenylhex-2-enoic acid","154375-43-6","D",0]
["Sodium bis(2,2,3,3,4,4,5,5-octafluoropentyl) phosphate","67996-82-1","D",0]
["2-(Nonafluorobutyl)benzoic acid","14670-68-9","D",0]
["2,4-Dichloro-N-(3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)benzamide","862130-69-6","D",0]
["[1-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfinyl)ethenyl]benzene","1606997-41-4","D",0]
["(Heptadecafluorooctyl)phenyliodonium","","D",0]
["1,1,2,2-Tetrafluoro-2-{[1,1,1,2,3,3-hexafluoro-3-(1,2,2-trifluoro-2-sulfoethoxy)propan-2-yl]oxy}ethane-1-sulfonic acid","916340-65-3","D",0]
["difluorotris(pentafluoroethyl)phosphorane","91543-32-7","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[[(pentadecafluoroheptyl)sulfonyl] propylamino]ethyl]-ω-hydroxy-","138226-35-4","D",0]
["1,3,5-Tribromo-1,6-dichloro-1,2,2,3,4,4,5,6,6-nonafluorohexane","81059-82-7","D",0]
["2,2,3,3,3-Pentafluoro-N',N'-dimethylpropanethiohydrazide","4454-49-3","D",0]
["2,2,3,3-Tetrafluoro-1-propanol p-nitrobenzoate","790-43-2","D",0]
["{[(Perfluorododecyl)sulfonyl]amino}-3-betaine","","D",0]
["Perfluoro[1,2,3,4,6-13C5]hexanoic acid","2328024-54-8","D",0]
["2-(Pentafluoroethyl)-2-phenylpiperidine","887361-05-9","D",0]
["1,1,1,2-Tetrafluoro-2-(1,2,2,2-tetrafluoroethoxy)ethane","67429-44-1","D",0]
["Methyl 3-(ethanesulfonyl)-2,2,3,3-tetrafluoropropanoate","77705-89-6","D",0]
["1,1,2,2,3,3-Hexafluoro-2,3-dihydro-1H-inden-4-amine","63002-46-0","D",0]
["1,1,1,2,2-Pentafluoro-3-[(trifluorovinyl)oxy]propane","1682-32-2","D",0]
["Trimethyl{[3,3,3-trifluoro-2-(trifluoromethyl)prop-1-en-1-yl]oxy}silane","857899-86-6","D",0]
["3-(3,4-Dibromo-1,1,2,2-tetrafluorobutyl)-1,1,2,2-tetrafluorocyclobutane","35208-00-5","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-Hexadecafluorodecyl prop-2-enoate","","D",0]
["2-{[3-(Acetyloxy)-1,5-dihydroxy-4-(1,1,2,2,2-pentafluoroethyl)pentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["Trimethylsilyl 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfinate","51735-77-4","D",0]
["6:2 Fluorotelomer thioether propanoyl oxy propanoic acid","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9-Tetradecafluoroundecane-1,11-diol","190909-04-7","D",0]
["4,4,4-Trifluoro-2-methyl-1-phenyl-3-(trifluoromethyl)butane-1,3-diol","34844-08-1","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(1,1,2,3,3,3-hexafluoro-2-(1,1,2,2-tetrafluoropropoxy)propoxy]-","1643531-45-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluorotricosane","871311-24-9","D",0]
["4,4,5-Trichloro-5-fluoro-2,2-bis(trifluoromethyl)-1,3-dioxolane","64499-84-9","D",0]
["2,2-Bis(trifluoromethyl)-1,3-dioxolane","1765-26-0","D",0]
["3-[(Butan-2-yl)sulfanyl]-2-ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)benzoic acid","1355554-79-8","D",0]
["2-Hydroxy-3-[[3-(perfluorodecyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["1,1,1,2,4,4,5,5,6,6,7,7-Dodecafluoro-2-(trifluoromethyl)heptan-3-ol","66566-87-8","D",0]
["Ethyl 4-cyano-3-methyl-5-[(2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoroheptanoyl)amino]thiophene-2-carboxylate","6351-69-5","D",0]
["4:4 Fluorotelomer sulfonate sodium salt","65345-91-7","D",0]
["2H-1,3-Thiazete, 4-phenyl-2,2-bis(trifluoromethyl)-","57014-95-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,17,17,18,18,19,19,20,20,21,21,22,22,23,23,24,24,25,25,26,26,26-Dotetracontafluorohexacosane","391894-95-4","D",0]
["Methyl((nonafluorobutyl)sulfonyl)azanide","332350-89-7","D",0]
["{[(Perfluorohexyl)sulfonyl]amino}-3-betaine","","D",0]
["2,2,4,4,5,5,7,7,8,8,8-Undecafluoro-3,6-dioxaoctanoic acid","80153-82-8","D",0]
["Perfluoro-2-(sulfoethoxy)acetic acid","88986-30-5","D",0]
["1,1,2,2,3,3‐Hexafluoro‐3‐(trifluoromethoxy)propane‐1‐ sulfonic acid","","D",0]
["Dimethyl 2-(perfluoropropyl)-p-benzenedicarbamate","25642-22-2","D",0]
["2,2,3,3,4,4,4-Heptafluorobutyl hydrogen phosphate","425-67-2","D",0]
["4-Azido-1,1,1,2,2-pentafluorobutane","121177-77-3","D",0]
["2H-Perfluorononanoic acid","","D",0]
["N,N,N-Tripropylpropan-1-aminium N-(2-bromo-4-nitrophenyl)-2,3,3,3-tetrafluoro-2-(trifluoromethyl)propanimidate","105923-55-5","D",0]
["2-Butenoic acid, 4,4,4-trifluoro-3-(trifluoromethyl)-, methyl ester","51097-63-3","D",0]
["Trimethoxy(nonafluorobutyl)silane","84464-03-9","D",0]
["Fluoro(heptafluoropropoxy)acetic acid","919005-00-8","D",0]
["Heptanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[2,2,3,3,4,4,5,5,6,6,7,7,7-tridecafluoro- (9CI)","548455-52-3","D",0]
["Benzenamine, 3-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)-","119489-67-7","D",0]
["Perfluoro-3-hexyne","60983-07-5","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoroundecan-2-one","82959-19-1","D",0]
["1,1,2-Trifluoro-2-(heptafluoropropoxy)ethane-1-sulfonic acid","935443-55-3","D",0]
["4-bromo-1,1,1-trifluoro-2-(trifluoromethyl)butane","203303-02-0","D",0]
["N,N-Dichloro-2,2-difluoro-2-(trifluoromethoxy)acetamide","86451-46-9","D",0]
["4-Fluoro-2,2-bis(trifluoromethyl)-2H-1,3-dioxole","89413-93-4","D",0]
["2,3,3,4,4,5,5,6,6,7,7-Undecafluoro-1-iodohept-1-ene","110680-45-0","D",0]
["3-Hydroxy-3-[2-(perfluorotetradecyl)ethylsulfanyl]propanoic acid","","D",0]
["Perfluoro-5,6-dimethyl-4,7-dioxadecane","2501-01-1","D",0]
["2,2,3,3,3-Pentafluoro-1-(piperazin-1-yl)propan-1-one","89245-12-5","D",0]
["2,4,6-Tribromo-3-[(heptafluoropropyl)sulfanyl]aniline","917923-97-8","D",0]
["Poly(oxy-1,2-ethanediyl), α-[2-[ethyl(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluoro-1-oxooctyl)amino]ethyl]-ω-hydroxy-","115633-66-4","D",0]
["4'-Chloro-4,4,4-trifluoro-3-(trifluoromethyl)crotonophenone","35443-99-3","D",0]
["HFE-356pcc3","160620-20-2","D",0]
["Perfluoroalkyl (linear) acyl fluorides","","D",0]
["Sodium (((4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-heptadecafluorononyl)oxy)phenyl)sulfonyl)(methyl)amino)acetate","","D",0]
["Benzamide, N-[[[2,5-dichloro-4-(1,1,2,3,3,3-hexafluoropropoxy)phenyl]amino]carbonyl]-2,6-difluoro-, mixt.","173072-61-2","D",0]
["16-H-Perfluorohexadecanoate","1696259-85-4","D",0]
["4-[(Pentacosafluorododecyl)sulfanyl]phenol","189196-62-1","D",0]
["2-[1,1,2-Trifluoro-2-[1,1,2,2,3,3-hexafluoro-3-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]ethoxy]acetic acid","919005-36-0","D",0]
["N,N-Diethyl-2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanamide","176702-71-9","D",0]
["1,1,2,2,3,3,4,4,5-Nonafluoro-5,6,6-tris(trifluoromethyl)cyclohexane","73196-05-1","D",0]
["N-[(2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoroheptanimidoyl)oxy]benzenecarboximidamide","146304-61-2","D",0]
["5-Chloro-2,2,3,3,4-pentafluoropent-4-enoic acid","77569-70-1","D",0]
["6-Chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoro-1-hexanesulfonic acid","729554-00-1","D",0]
["2-Propanol, 2-(chloromethyl)-1,1,1,3,3,3-hexafluoro-","29871-68-9","D",0]
["Perfluoro-p-ethylcyclohexanesulfonate","80988-54-1","D",0]
["Diethoxy(ethyl)phosphane 1,1,1,2,2,3,3-heptafluoro-3-iodopropan (1:1)","72220-37-2","D",0]
["Poly(ethane-co-3,3,4,4,5,5,6,6,6-nonafluorohex-1-ene-co-perfluoroethene)","82606-24-4","D",0]
["1-(Pentafluorothio)-tridecafluorohexane","1423-20-7","D",0]
["{[(Perfluoroheptyl)sulfonyl]amino}-3-betaine","","D",0]
["1-(2-Hydroxyethyl)-1-methyl-4-(perfluoro-1-oxoheptyl)piperazinium chloride","89932-73-0","D",0]
["1,3,3,4,4,5,5,6,6-Nonafluoro-2-(pentafluoroethyl)cyclohexene","80308-96-9","D",0]
["4-[[2,2,2-Trifluoro-1,1-bis(trifluoromethyl)ethyl]thio]benzeneamine","68596-41-8","D",0]
["2,2,3,3,3-Pentafluoro-N-phenylpropanamide","718-66-1","D",0]
["Methyl perfluoro(2-[2-(ethenyloxy)ethoxy]propanoate)","100016-68-0","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-[(1,1,1,2,3,3-hexafluoro-3-{[1,1,1,2,3,3-hexafluoro-3-(pentafluoroethoxy)propan-2-yl]oxy}propan-2-yl)oxy]propane","78522-49-3","D",0]
["2-[Perfluoro-2-[3-(propoxy)propoxy]ethoxy]acetic acid","919005-45-1","D",0]
["Bis[5‐tert‐butyl‐7‐(1,1,2,2,3,3,3‐ heptafluoropropyl)‐4,8‐dioxo‐1,3‐dioxa‐2‐ yttracyclooctan‐2‐yl] 2‐tert‐butyl‐4‐ (1,1,2,2,3,3,3‐heptafluoropropyl)pentanedioate","19186-73-3","D",0]
["Ethyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","79851-29-9","D",0]
["(4,4,5,5,6,6,7,7,7-Nonafluorohept-1-en-1-yl)benzene","664326-37-8","D",0]
["1-(2,2,3,3-Tetrafluorocyclopropyl)naphthalene","922141-54-6","D",0]
["Phenylbis[4-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)phenyl]phosphane","290827-94-0","D",0]
["1-Chloro-1,1,2,2,3,3,4,4-octafluoro-6-iodoundecane","103147-30-4","D",0]
["(2-Chloro-1,1,2,2-tetrafluoroethyl)benzene","357-41-5","D",0]
["6-(4-Chlorophenyl)-2-phenyl-4,4-bis(trifluoromethyl)-4H-1,3-thiazine","88656-42-2","D",0]
["3,4,4,4-Tetrafluorobut-2-ene-1-sulfonic acid","","D",0]
["Dichloropalladium bis(tris[4‐ (1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8‐ heptadecafluorooctyl)phenyl]phosphane)","326475-44-9","D",0]
["2-Bromo-2-(Perfluorohexyl)ethene","51249-64-0","D",0]
["Heptadecafluorooctane-2-sulfonic acid","927670-12-0","D",0]
["1,1,2,2-Tetrafluoro-3-(2-methoxyethoxy)propane","76127-08-7","D",0]
["Pentadecafluorooctanoic acid--pyridine (1/1)","95658-47-2","D",0]
["1,5-Bis(5-chloro-2-methyl-3-thienyl)-2,2,3,3,4,4-hexafluoro-1,5-pentanedione","222730-41-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl sulfurochloridoite","254756-56-4","D",0]
["Magnesium perfluorobutane sulfonate","507453-86-3","D",0]
["Tris(1H,1H,2H,2H-perfluorohexyl) phosphate","1887067-55-1","D",0]
["1-Azido-1,1,2,3,3,3-hexafluoropropane","2991-70-0","D",0]
["1,4-Butanedisulfonyl dichloride, 1,1,2,2,3,3,4,4-octafluoro-","105214-13-9","D",0]
["2,2,3,3,4,4-Hexafluoro-1-(trifluoromethyl)azetidine","16276-23-6","D",0]
["4,4,5,5,6,6,7,7-octafluorodeca-1,9-diene","170804-07-6","D",0]
["4,4,5,5,6,6,6-Heptafluoro-3-methylhexan-3-ol","423-43-8","D",0]
["4:2 Fluorotelomer thioether amido betaine","1513863-94-9","D",0]
["3,3,4,4,4-Pentafluoro-2-phenylbutan-2-ol","101417-69-0","D",0]
["1-[bromo(difluoro)methoxy]-1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethane","87136-78-5","D",0]
["2-[Perfluoro(propoxy)ethoxy]acetic acid","919005-42-8","D",0]
["[N(E),S(S)]-N-(4-nitrophenyl)methyleneperfluorobutanesulfinamide","1612778-37-6","D",0]
["Methyl 2-bromo-2,3,3,3-tetrafluoropropanoate","378-67-6","D",0]
["Quinolin-8-yl nonafluorobutane-1-sulfonate","41605-60-1","D",0]
["1-Octanone, 2,2,3,3,4,4,5,5,6,6,7,7,8,8-tetradecafluoro-1-phenyl-","1427-89-0","D",0]
["2-Propenoic acid, 2-methyl-, methyl ester, polymer with ethenylbenzene, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate, 2-[methyl[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]amino]ethyl 2- ¿","71487-20-2","D",0]
["Perfluoro(7-methyl-1-octanesulfonic acid)","71500-44-2","D",0]
["1,2-Benzenedicarboxylic acid, 4,4'-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]bis-, diethyl ester","71550-47-5","D",0]
["Pentanoic acid, 4,4-bis[(gamma-omega-perfluoro-C8-20-alkyl)thio] derivs.","71608-60-1","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-hexadecafluoro-9-(vinyloxy)nonane","71726-31-3","D",0]
["(Dimethyl{3-[(perfluorodecanoyl)amino]propyl}ammonio)acetate","70674-74-7","D",0]
["Perfluoro(3-(1-(ethenyloxy)propan-2-yloxy)propanenitrile)","69804-19-9","D",0]
["1-Butene, 1,1,2,3,3,4,4-heptafluoro-4-[(trifluoroethenyl)oxy]-","69818-05-9","D",0]
["Perfluorosuccinic anhydride","699-30-9","D",0]
["1-Vinyloxyperfluoropropane","6996-01-6","D",0]
["Benzenediazonium, 4-(phenylamino)-, hexafluorophosphate(1-) (1:1), polymer with formaldehyde, zinc chloride complexes","69991-60-2","D",0]
["Ethene, tetrafluoro-, oxidized, polymd.","69991-61-3","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced","69991-62-4","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, oxidized, polymd.","69991-67-9","D",0]
["1-[Difluoro(trifluoromethoxy)methoxy]-1,2,2-trifluoroethene","700874-87-9","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, compd. with 2,2'-iminobis(ethanol) (1:1)","70225-14-8","D",0]
["Bis(2-hydroxyethyl)ammonium perfluoroheptanesulfonate","70225-15-9","D",0]
["Bis(2-hydroxyethyl)ammonium perfluoropentanesulfonate","70225-17-1","D",0]
["Bis(2-hydroxyethyl)ammonium perfluorobutanesulfonate","70225-18-2","D",0]
["Bis(trimethyl-3-(((pentadecafluoroheptyl)sulphonyl)amino)propylammonium) sulphate","70225-20-6","D",0]
["Bis(trimethyl-3-(((nonafluorobutyl)sulphonyl)amino)propylammonium)sulphate","70225-22-8","D",0]
["bis[trimethyl-3-[[(undecafluoropentyl)sulphonyl]amino]propylammonium] sulphate","70225-24-0","D",0]
["[3-[[(heptadecafluorooctyl)sulphonyl]amino]propyl]trimethylammonium hydrogen sulphate","70225-26-2","D",0]
["3,3,4,4,5,5-Hexafluorooxolan-2-one","702-35-2","D",0]
["Furan, 2,2,3,3,4,4-hexafluorotetrahydro-5-(2,2,2-trifluoro-1,1-bis(trifluoromethyl)ethyl)-","71302-72-2","D",0]
["1,1,2,2,9,9,9-Heptafluorononane-1-sulfonate","","D",0]
["N,N,1,1-Tetramethyl-1-(3,3,4,4,5,5,6,6,6-nonafluorohexyl)silanamine","1221157-07-8","D",0]
["Chlorodimethyl((perfluoropentyl)ethyl)silane","142515-42-2","D",0]
["Iodo-1,1,2,2-tetrafluoroethane","354-41-6","D",0]
["1-Chloro-1,1,2,2,3,3,4,4-octafluoro-6-iododecane","103148-11-4","D",0]
["4,4,4-Trifluoro-1-(4-methylphenyl)-3-(trifluoromethyl)but-2-en-1-one","35443-92-6","D",0]
["2-Propenoic acid, 2-methyl-, 2-[[[[2-methyl-5-[[[4-[methyl[(tridecafluorohexyl)sulfonyl]amino]butoxy]carbonyl]amino]phenyl]amino]carbonyl]oxy]propyl ester (9CI)","70900-36-6","D",0]
["2-[[[[2-methyl-5-[[[4-[methyl[(pentadecafluoroheptyl)sulphonyl]amino]butoxy]carbonyl]amino]phenyl]amino]carbonyl]oxy]propyl methacrylate","70900-35-5","D",0]
["2-[[[[5-[[[4-[[(heptadecafluorooctyl)sulphonyl]methylamino]butoxy]carbonyl]amino]-2-methylphenyl]amino]carbonyl]oxy]propyl methacrylate","70900-34-4","D",0]
["2-[[[[2-methyl-5-[[[4-[methyl[(undecafluoropentyl)sulphonyl]amino]butoxy]carbonyl]amino]phenyl]amino]carbonyl]oxy]propyl methacrylate","70900-37-7","D",0]
["2-[[[[2-methyl-5-[[[4-[methyl[(nonafluorobutyl)sulphonyl]amino]butoxy]carbonyl]amino]phenyl]amino]carbonyl]oxy]propyl methacrylate","70900-38-8","D",0]
["Propan-2-yl heptadecafluorononanoate","70910-41-7","D",0]
["Ethanesulfinic acid, 2-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-1,1,2,2-tetrafluoro-, polymer with tetrafluoroethene","70815-05-3","D",0]
["Propanoic acid, 3-[1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]-2,2,3,3-tetrafluoro-, potassium salt, polymer with tetrafluoroethene","70788-53-3","D",0]
["Acetic acid, [1-[difluoro[(trifluoroethenyl)oxy]methyl]-1,2,2,2-tetrafluoroethoxy]difluoro-, polymer with tetrafluoroethene","70776-76-0","D",0]
["2-Propenoic acid, 2-methyl-, octadecyl ester, polymer with 1,1-dichloroethene, 2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate, N-(hydroxymethyl)-2-propenamide, 2-[methyl[(1,1,2,2,3,3,4,4,4- ...","70776-36-2","D",0]
["Perfluoro(4-[(4-ethyl-3,4-dimethylhex-2-en-2-yl)oxy])benzene-1-sulfonate tributylammonium","70729-63-4","D",0]
["1,2-Dichlorohexafluorocyclopentene","706-79-6","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-methyl-omega-hydroxy-, 2-hydroxy-3-[(gamma-omega-perfluoro-C6-20-alkyl)thio]propyl ethers","70983-59-4","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-, 3-[(gamma-omega-perfluoro-C6-20-alkyl)thio] derivs., chlorides","70983-60-7","D",0]
["Poly(difluoromethylene), .alpha.-[2-(acetyloxy)-2-[(carboxymethyl)dimethylammonio]ethyl]-.omega.-fluoro-, hydroxide, inner salt","71002-41-0","D",0]
["Perfluoro-2,2,5,5-tetramethylhexane","71076-47-6","D",0]
["4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]benzene-1-sulfonic acid","71212-45-8","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-(2-iodoethyl)-","71215-70-8","D",0]
["2-Propenoic acid, 2-[butyl[(heptadecafluorooctyl)sulfonyl]amino]ethyl ester, polymer with 2-[butyl[(pentadecafluoroheptyl)sulfonyl]amino]ethyl 2-propenoate, methyloxirane polymer with oxirane di-2-propenoate and methyloxirane polymer with oxirane mono-2-p","68298-61-3","D",0]
["7,7,8,8,9,9,10,10,11,12,12,12-Dodecafluoro-11-(trifluoromethyl)dodecan-1-ol","","D",0]
["3-Fluoro-3-(perfluorodecyl)acrylic acid","","D",0]
["(4-Cyclohexylphenyl)diphenylsulfonium salt with 1,1,2,2,3,3,4,4,4-nonafluoro-1-butanesulfonic acid (1:1)","425670-64-0","D",0]
["(Perfluorooctyl)methane-1-sulfonic acid","","D",0]
["1-Bromo-4-(nonafluorobutyl)benzene","753025-19-3","D",0]
["3-(Perfluoroisopropyl)-2-propenoic acid","243139-64-2","D",0]
["2-(2-tert-Butylphenyl)-1,1,1,3,3,3-hexafluoropropan-2-yl carbonate","143213-43-8","D",0]
["11-Chloro-Perfluoroundecanoic acid","2823-49-6","D",0]
["2-Ethyl-4,4,4-trifluoro-1-(thiophen-2-yl)-3-(trifluoromethyl)butane-1,3-diol","34848-42-5","D",0]
["3-Methyl-2-(1,2,2,2-tetrafluoroethyl)quinazolin-4(3H)-one","63077-35-0","D",0]
["ethyl 3,3-bis(trifluoromethyl)oxirane-2-carboxylate","1644-09-3","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluoro-N-(2-oxocyclooctyl)octane-1-sulfonamide","240801-56-3","D",0]
["2,4,4,5,5,7,7,9,9,11,11,13,13,13-Tetradecafluoro-3,6,8,10,12-pentaoxatridecanoic acid","919005-10-0","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorobutanamido)propan-1-aminium","","D",0]
["2-[2-amino-3-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-5-methylphenyl]-1,1,1,3,3,3-hexafluoropropan-2-ol","76220-90-1","D",0]
["1-(3-Chlorophenyl)-4,4,4-trifluoro-3-hydroxy-3-(trifluoromethyl)-1-butanone","34844-15-0","D",0]
["2-[3-[[(Perfluorooctyl) sulfonyl]amino]propoxy]-N,N,N-trimethylethanaminium 4-methylbenzenesulfonate","91707-63-0","D",0]
["2-(Heptafluoropropyl)pyridine-4-carboxylic acid","20897-65-8","D",0]
["Propyl 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)propanoate","147224-16-6","D",0]
["2-Butanol, 4-phenyl-1,1,1-trifluoro-2-trifluoromethyl-","100482-47-1","D",0]
["(7E)-Perfluoropentadec-7-ene-1-sulfonic acid","","D",0]
["Perfluoroalkyl esters (vinyl)","","D",0]
["Methyl 4-(1,1,2,2,3,3,3-heptafluoropropane-1-sulfonyl)benzoate","88489-69-4","D",0]
["1,9-Decadiene, 3,3,4,4,5,5,6,6,7,7,8,8-dodecafluoro-, polymer with 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","190062-24-9","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-yl pyrazine-2-carboxylate","139244-47-6","D",0]
["N-((7S)-6,7-Dihydro-6-oxo-5H-dibenz(b,d)azepin-7-yl)-2,2-dimethyl-N'-(2,2,3,3,3-pentafluoropropyl)-propanediamide","847925-91-1","D",0]
["4,4,5,5,6,6,7,7,8,8,8-Undecafluorooctane-1,2-diol","140369-63-7","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-1-hydrazinylheptan-1-ol","64739-15-7","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorononanamide","103831-29-4","D",0]
["1-(1H-Benzimidazol-2-yl)-7,7,8,8,9,9,10,10,11,11,12,12,12-tridecafluorododecan-6-one","237738-71-5","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-(4-methoxyphenyl)hex-2-yn-1-one","89965-75-3","D",0]
["3-[[(Perfluorododecyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","","D",0]
["1-[(2,4,4,5,5,6,6,7,7,8,8,9,9,9-Tetradecafluorononyl)oxy]octadecane","189389-79-5","D",0]
["1,10-Dichloroperfluorodecane","156186-28-6","D",0]
["2,3,3,3-Tetrafluoro-N-hydroxypropanimidoyl fluoride","1428-28-0","D",0]
["3-[[(Perfluorooctyl)sulfonyl]amino]-N,N,N-tris(2-methoxyethyl)propanaminium iodide","91707-60-7","D",0]
["3-[3,3,3-Trifluoro-2-hydroxy-2-(trifluoromethyl)propyl]oxolan-2-one","101833-16-3","D",0]
["1(Perfluoroethyl)1-fluoro-2-(perfluoropropyl)ethene","648-39-5","D",0]
["Bis(dimethylamino)(hexafluoropropanimino)borane","67395-53-3","D",0]
["(2E)-4,4,5,5-tetrafluoropent-2-enoic acid","1370280-58-2","D",0]
["3-(Dimethyl{3-[methyl(perfluorodecanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["1,3,3-Tribromo-1,1,2,2,4,4,4-heptafluorobutane","140198-73-8","D",0]
["1,1,1,4,4,5,5,5-Octafluoro-2-pentyne","378-22-3","D",0]
["Sodium perfluorotridecanesulfonate","174675-49-1","D",0]
["4-{[(3-chlorophenyl)methyl]amino}-2,2,3,3-tetrafluoro-4-oxobutanoic acid","883226-95-7","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl (3a,5b,6a,7a,20R)-3,6,7-tris[(trifluoroacetyl)oxy]cholan-24-oate","","D",0]
["Nonanamide, N,N'-[4-(phenylazo)-1,3-phenylene]bis[2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9-hexadecafluoro- (9CI)","547748-28-7","D",0]
["1-Ethoxy-1-(ethylsulfanyl)-4,4,4-trifluoro-3-(trifluoromethyl)buta-1,2-diene","921223-07-6","D",0]
["5,6-Dichloro-1,1,2,2,3,3,4,7-octafluoro-2,3-dihydro-1H-indene","88953-09-7","D",0]
["1-Nitro-4-(3,3,4,4-tetrafluorobut-1-en-1-yl)benzene","62448-59-3","D",0]
["Perfluoro-3-methylbutyl iodide","1514-90-5","D",0]
["1-Bromo-1,1,3,4,4,4-hexafluoro-3-(trifluoromethyl)butan-2-one","813468-16-5","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(2-methylpropane-2-sulfinyl)benzoic acid","1355555-05-3","D",0]
["1-Chloro-2,3,3,4,4,5,5,6,6-nonafluorocyclohex-1-ene","15145-21-8","D",0]
["4,4'-Bis(2-hydroxyhexafluoroisopropyl)diphenyl ether","2093-04-1","D",0]
["Butanamide, 2,2,3,3,4,4,4-heptafluoro-N-(1-methyl-2-phenylethyl)-","1545-26-2","D",0]
["1,4-Benzenedicarboxylic acid, polymer with N,N-bis(2-hydroxyethyl)-4-[(nonadecafluorodecyl)oxy]benzenesulfonamide didehydro deriv., 1,2-ethanediol, .alpha.-hydro-.omega.-hydroxypoly(oxy-1,2-ethanediyl) and 1,1'-methylenebis[4-isocyanatobenzene]","68735-91-1","D",0]
["Undecafluorohexane","154275-17-9","D",0]
["1,1,1,2,2,5,5,5-Octafluoro-4-iodopentane","1209623-58-4","D",0]
["3-[{3-[(Carboxymethyl)(perfluorohexanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["1H,1H,3H-Perfluorobutyl acrylate","54052-90-3","D",0]
["3-Hydroxy-3-[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)sulfanyl]propanoic acid","","D",0]
["Perfluoroundecane amide betaine","77968-31-1","D",0]
["N-(2,6-Dichlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","121806-69-7","D",0]
["3-(Perfluorodecyl)propanoic acid","","D",0]
["Phosphonic acid, P-[3,5,5,6,8,8,9,11,11,12,14,14,15,17,17,18,18,19,19,19-eicosafluoro-3,6,9,12,15-pentakis(trifluoromethyl)-4,7,10,13,16-pentaoxanonadec-1-yl]-, diethyl ester","1198297-66-3","D",0]
["2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propanal","7450-64-8","D",0]
["1,2,2,3,3,4,4,6,7,7,8,8,9,9-Tetradecafluoro-5,6-bis(trifluoromethyl)bicyclo[3.3.1]nonane","75108-51-9","D",0]
["1,1,2,3,4,5,5,5-Octafluoro-3-pentene-1-sulfonic acid","2089109-49-7","D",0]
["Thiophene, 3,3'-(3,3,4,4,5,5-hexafluoro-1-cyclopentene-1,2-diyl)bis[2,4-dimethyl-5-phenyl-","172612-67-8","D",0]
["2,3,4,4,5,5,5-Heptafluoropent-2-enoic acid","103229-91-0","D",0]
["2-(3,4-Dimethoxyphenyl)-1-[5-(heptafluoropropyl)-5-hydroxy-3-phenyl-4,5-dihydro-1H-pyrazol-1-yl]ethanone","375354-47-5","D",0]
["3,3,4,4,5,5-Hexafluoro-6-imino-3,4,5,6-tetrahydropyridin-2-amine","4556-39-2","D",0]
["1-(1,1,2,3,3,3-Hexafluoropropyl)-2-(trifluoromethyl)-1H-benzimidazole","91074-94-1","D",0]
["Lithium, (pentafluoroethyl)-","91935-83-0","D",0]
["3,3,4,4,4-Pentafluoro-2-methylbutan-2-amine","761396-79-6","D",0]
["1,1,1,3,3,3-Hexafluoro-2-isocyanatopropane","684-29-7","D",0]
["(4S,6S)-1,1,2,2,3,3,4,5,5,6-Decafluorocyclohexane","2995-01-9","D",0]
["Carboxydimethyl[3-(perfluorododecyl)-2-hydroxypropyl]azanium","","D",0]
["(2E)-4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluoro-2-nonen-1-ol","83706-97-2","D",0]
["1-Chloro-2-[dichloro(fluoro)methoxy]-1,1,2,2-tetrafluoroethane","37031-56-4","D",0]
["N-(2,3-Dihydroxypropyl)-3-{[(perfluoropropyl)sulfonyl]amino}-4-hydroxy-N,N-dimethyl-1-butanaminium","2089108-83-6","D",0]
["2,2,3-Trifluoro-3-(pentafluoroethoxy)propanoic acid","919005-13-3","D",0]
["2-Bromo-2-(chloromethyl)-1,1,1,3,3,3-hexafluoropropane","883498-84-8","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-N-(prop-2-en-1-yl)octan-1-amine","26577-69-5","D",0]
["1,1,1,2,2,3,4,4,5,5,5-Undecafluoropentane","95576-22-0","D",0]
["1,3-Propanediol, 2,2-bis[[(.gamma.-.omega.-perfluoro-C4-10-alkyl)thio]methyl] derivs., phosphates","148240-84-0","D",0]
["Difluoro(1,1,2,2-tetrafluoroethoxy)acetic acid","81233-13-8","D",0]
["1-(Ethylsulfanyl)-1,1,2,3,3,3-hexafluoropropane","380-35-8","D",0]
["2-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)naphthalen-1-ol","2092-87-7","D",0]
["2,2,3,3,4,4,5,5-Octafluoro-1-(morpholin-4-yl)pentane-1-thione","1447964-86-4","D",0]
["1,1,2,2,2-Pentafluoroethyl trifluoromethyl phosphate","","D",0]
["2,2,3,3-Tetrafluoro-N,N,N-trimethylpropan-1-aminium iodide","116826-67-6","D",0]
["(2-(F-Hexyl)ethyl) dimorpholinophosphoramidate","134051-89-1","D",0]
["(Perfluoro-3-(pentyloxy)propanamido)-3-N,N-dimethylpropane-3-amine N-oxide","200636-96-0","D",0]
["1-(1,1,2,3,3,3-Hexafluoropropyl)aziridine","19390-77-3","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluoropentyl)sulfonyl]amino}-1-propanaminium","2089109-05-5","D",0]
["N-(Perfluoroheptanoyl)-3-aminopropanoic acid","160845-44-3","D",0]
["1,1,2,2,3,3,4,4-Octafluoro-5-methoxypentane","77527-96-9","D",0]
["3-(Pentadecafluoroheptyl)-5-(pentafluorophenyl)-1,2,4-oxadiazole","919489-99-9","D",0]
["Perfluoro-2-(trifluoromethoxy)ethanesulfonic acid","","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)aniline","273735-34-5","D",0]
["Ethoxydimethyl (3,3,4,4,5,5,6,6,7,7,7-undecafluoroheptyl) silane","608301-28-6","D",0]
["2,2,4,5,5-pentafluoro-1,3-dioxolane-4-carbonyl Fluoride","70411-10-8","D",0]
["Fluoro[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]acetic acid","919005-05-3","D",0]
["2-Chloroheptafluoro-2-butene","434-41-3","D",0]
["1,3,3,4,4-Pentafluoro-2-methoxycyclobut-1-ene","359-98-8","D",0]
["1-Bromo-4-(2-bromo-1,1,2,2-tetrafluoroethoxy)benzene","113939-45-0","D",0]
["2-Amino-4,4,5,5,6,6,6-heptafluorohexan-3-ol","355-88-4","D",0]
["2,2,3,4,4,4-Hexafluorobutyl nonafluorobutane-1-sulfonate","1205020-79-6","D",0]
["2-Perfluoropropyl-5-phenyl-1,3,4-oxadiazole","5756-67-2","D",0]
["2-[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)oxy]cyclohepta-2,4,6-trien-1-one","195044-31-6","D",0]
["1-Ethenyl-4-{[(1,1,1,2,3,3-hexafluoropropan-2-yl)oxy]methyl}benzene","111158-92-0","D",0]
["3-(Tridecafluorohexyl)thiophene","128032-23-5","D",0]
["Potassium 3-oxaperfluorononane sulfonate","68136-88-9","D",0]
["Diethyl 2,2,3,3,4,4,4-heptafluorobutyl phosphate","","D",0]
["2-(2,2,3,3,4,4,4-Heptafluorobutoxy)ethan-1-ol","2266-43-5","D",0]
["Chloro(1,1,1,2,3,3-hexafluoropropan-2-yl)dimethylsilane","62281-33-8","D",0]
["Sodium 1,4‐bis[(3,3,4,4,5,5,6,6,6‐nonafluorohexyl)oxy]‐1,4‐dioxobutane‐2‐sulfonate","54949-95-0","D",0]
["14:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["1-(Perfluoroethyl)-2-(perfluorohexyl)ethene","86563-87-3","D",0]
["4,4,5,5,6,6,6-Heptafluoronorleucine","15960-01-7","D",0]
["3,3,4,4,5,5-Hexafluoro-1,2-bis(trifluoromethyl)cyclopent-1-ene","34649-46-2","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,10,10,10-Heptadecafluorodecyl-methyl-di(propan-2-yloxy)silane","","D",0]
["1-Benzo[b]thien-3-yl-4,4,5,5,6,6,6-heptafluoro-1,3-hexanedione","362-57-2","D",0]
["1-Decanol, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, 1-(dihydrogen phosphate)","","D",0]
["1-Propanaminium, 2-hydroxy-N,N,N-trimethyl-3-[(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12, 12-heneicosafluorododecyl)thio]-, chloride (1:1)","","D",0]
["1-Dodecanamine, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,11,11,11-nonadecafluoro-N,N-dimethyl-, N-oxide","","D",0]
["1-Decanamine, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10, 10,10-heptadecafluoro-N,N-dimethyl-, N-oxide","","D",0]
["5(6)-Endo(exo)-perfluorhexylbicyclo[2.2.1]hept-2-yl-methyl-polysiloxan","","D",0]
["1,1,2,2,3,3,4,4,4-Nonafluorobutylsulfonylbenzene","","D",0]
["Perfluoropropyl methacrylate","","D",0]
["3-[(Perfluorodecanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["1,1,2,2,3,3,3-Heptafluoropropoxy(dimethyl)silane","","D",0]
["Perfluoropropyl hydrogen sulfate","","D",0]
["3-[(4-Fluorobenzoyl)-methylamino]-N-[2-iodo-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)-6-(trifluoromethyl)phenyl]benzamide","","D",0]
["1,1,2,2,3,3,4,4,5,5,11,11,11-Tridecafluoroundecane-1- sulfonate","","D",0]
["3-[(Perfluorododecanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["1,1,2,2,3,3,4,4,5,12,12,12-Dodecafluorododecane-1- sulfonate","","D",0]
["Perfluorotetradecyl hydrogen sulfate","","D",0]
["Disodium 2-(N-ethylperfluorooctane-1-sulfonamido)ethyl phosphate","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,12,12,12-Pentadecafluorododecane-1-sulfonate","","D",0]
["Perfluoroundecyl hydrogen sulfate","","D",0]
["Perfluorononadecanesulfonic acid","","D",0]
["3-[(Perfluoroheptanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["1,1,2,2,3,3,4,4,5,5,12,12,12-Tridecafluorododecane-1- sulfonate","","D",0]
["Perfluoroundecane-1-sulfinic acid","","D",0]
["3-[(Perfluorotridecanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["Bis(perfluorooctyl) phosphinic acid ytterbium(3+) salt","500776-71-6","D",0]
["Perfluoropentane-1-sulfinic acid","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,10,10,10-Heptadecafluorodecane-1-sulfonate","","D",0]
["Phenyl(nonafluorobutyl) sulfoxide","","D",0]
["1,1,1,5,5,6,6,7,7,8,8,8-Dodecafluoro-2,2-bis(trifluoromethyl)oct-3-ene","","D",0]
["Perfluorohexyl hydrogen sulfate","","D",0]
["Nonane, 1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-","","D",0]
["3-[(3-{Ethyl[(perfluorooctyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1,5,5,6,6,6-Octafluoro-4,4-bis(trifluoromethyl)hex-2-ene","","D",0]
["Perfluorohexane-1-sulfinic acid","","D",0]
["Methyl 1-(4-ethoxyphenyl)-2,2,3,3-tetrafluorocyclobutane-1-carboxylate","","D",0]
["3-[(3-{Ethyl[(perfluorononyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1-Trifluoro-N-[2-[2-[(E)-2-[4-(2,2,3,3,3-pentafluoropropoxy)phenyl]ethenyl]-3H-benzimidazol-5-yl]phenyl]methanesulfonamide","","D",0]
["3-[(3-{Ethyl[(perfluoropropyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["Furan, 2,2,3,3,4,4,5-heptafluorotetrahydro-5-(1,1,2,2,2-pentafluoroethyl)-","","D",0]
["1,1,1-Trifluoro-3-[N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]-3-[2-(trifluoromethyl)pyridin-4-yl]oxyanilino]propan-2-ol","","D",0]
["3-[(3-{Ethyl[(perfluoropentyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["Potassium 5-carbamoyl-3-[5'-fluoro-2'-(2,2,3,3,3-pentafluoropropoxy)[1,1'-biphenyl]-3-yl]-1,2,4-triazol-1-ide--water (1/1/1)","","D",0]
["Perfluorooctyl hydrogen sulfate","","D",0]
["3-[(4,4,5,5,5-Pentafluoro-1,3-dihydroxypentan-2-yl)sulfanyl]propanoic acid","","D",0]
["(Ethyl{3-[(1,1,2,2,3,3,4,4,5,5,6,6,6-tridecafluorohexane-1-sulfonyl)amino]propyl}amino)oxidanide","","D",0]
["1,1,2,2,12,12,12-Heptafluorododecane-1-sulfonate","","D",0]
["Perfluorononyl hydrogen sulfate","","D",0]
["1,1,2,2,3,11,11,11-Octafluoroundecane-1-sulfonate","","D",0]
["Perfluoropentyl hydrogen sulfate","","D",0]
["3-Fluoro-3-(perfluorododecyl)prop-2-ene-1-sulfonic acid","","D",0]
["3-[(Perfluoropropane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide","","D",0]
["3-[(4,4,5,5,6,6,6-Heptafluorohexanoyl)sulfanyl]-2-hydroxypropanoic acid","","D",0]
["1,1,1,2-Tetrafluoro-3-[(3-hydroxy-2-bicyclo[2.2.1]heptanyl)oxy]-3-oxopropane-2-sulfonic acid","","D",0]
["Perfluorocyclopentane-1-carboxylic acid","","D",0]
["1,1,1,2-Tetrafluoro-2-(trifluoromethyl)butane","","D",0]
["Perfluorocyclohexanesulfonate","","D",0]
["3-[(3-{Ethyl[(perfluorodecyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1,2-Tetrafluoro-3-oxo-3-[(4-oxo-1-adamantyl)oxy]propane-2-sulfonic acid","","D",0]
["Perfluorodecane-1-sulfinic acid","","D",0]
["3-[(3-{Ethyl[(perfluorobutyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1,2-Tetrafluoro-3-methyl-2-(trifluoromethyl)butane","","D",0]
["Perfluorocyclopentanesulfonic acid","","D",0]
["Perfluorododecyl hydrogen sulfate","","D",0]
["3-[(3-{Ethyl[(perfluoroethyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["Perfluorododecane-1-sulfinic acid","","D",0]
["3-[(3-{Ethyl[(perfluorododecyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1,2-Tetrafluoro-3-oxo-3-[2-oxo-2-[(5-oxo-4-oxatricyclo[4.2.1.03,7]nonan-2-yl)oxy]ethoxy]propane-2-sulfonic acid","","D",0]
["1,1,1,4,5,5,5-Heptafluoro-3-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-methyl-4-(trifluoromethyl)pent-2-ene","","D",0]
["Perfluoroheptyl hydrogen sulfate","","D",0]
["3-[(3-{Ethyl[(perfluorohexyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1,4,5,5,5-Heptafluoro-2,4-bis(trifluoromethyl)-3-(1,2,2,2-tetrafluoro-1-methylethyl)-2-pentene","","D",0]
["Perfluorohenicosanoic acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluoroethyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["1,1,1,2,2-Pentafluoro-3-methylsulfinylpropane","","D",0]
["3-[(4,4,5,5,6,6,7,7,7-Nonafluoro-1,3-dihydroxyheptan-2-yl)sulfanyl]propanoic acid","","D",0]
["{[(Perfluorononyl)sulfonyl]amino}acetic acid","1003194-01-1","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluorododecyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["1,1,1,2,2-Pentafluoro-3-(3-fluoropropoxy)propane","","D",0]
["Perfluoro-5-hexylcyclohexane-1-carboxylic acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluorononyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["1,1,1,2,3,3,4,4-Octafluoro-4-propoxy-2-(trifluoromethyl)butane","","D",0]
["6-Chloroperfluorohexylphosphonic acid","","D",0]
["Perfluoro-5-pentylcyclohexane-1-carboxylic acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluorotetradecyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["N-(2-Carboxyethyl)-3-(N-(2-carboxyethyl)-perfluoropentylsulfonamido)-N,N-dimethylpropan-1-aminium","","D",0]
["1,1,1,2,3,3-Hexafluoro-2-iodo-3-(1,2,2-trifluoroethenoxy)propane","","D",0]
["Perfluoro-8-oxononane-1-sulfonic acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluoropropyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["N-(Carboxymethyl)-N,N-dimethyl-3-(1H,1H,2H,2H-perfluoro-1-decanesulfonamido)propan-1-aminium","","D",0]
["1,1,1,2,3,3-Hexafluoro-2-(1,1,1,2,3,3-hexafluoropropan-2-yloxy)propane","","D",0]
["Perfluoro-6-(pentafluoro-.lambda.6-sulfanyl)hexanoic acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluoroundecyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["1,1,1,2,3-Pentafluoropropan-2-ol","","D",0]
["Perfluorobutyl hydrogen sulfate","","D",0]
["1,2,2,3,3,3-Hexafluoropropyl hydrogen sulfate","","D",0]
["3-[Dimethyl(3-{[(perfluorononyl)sulfonyl]amino}propyl)ammonio]propanoate","","D",0]
["3-[3,3,4,4,5,5-Hexafluoro-2-[5-[2-(4-methoxyphenyl)ethenyl]-2,4-dimethylthiophen-3-yl]cyclopenten-1-yl]-6-[2-(4-methoxyphenyl)ethenyl]-2-methyl-1-benzothiophene","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-(~2~H)sulfonic acid","","D",0]
["Nonamide, 1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-heptadecafluoro-N-[3-dimethylamino)propyl], N-oxide","","D",0]
["Sodium bis(1H, 1H, 2H, 2H-[1,2-13C2]perfluorodecyl) phosphate","","D",0]
["8-Chloroperfluorohexylphosphonic acid","","D",0]
["Pentadecafluorooctan(2H)oic acid","","D",0]
["Trimethyl[3-(perfluorooctyl)-2-hydroxypropyl]azanium","","D",0]
["1,2,3,4,5,6,6,7,7,7-Decafluoroheptyl hydrogen sulfate","","D",0]
["Tritriacontafluoroheptadecanoate","","D",0]
["Heptacosafluorotetradecan(2H)oic acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluorotridecyl)sulfonyl]amino}propyl)(dimethyl)azaniumyl]propanoate","","D",0]
["N-(2-Carboxyethyl)-3-(N-(2-carboxyethyl)-perfluorohexylsulfonamido)-N,N-dimethylpropan-1-aminium","","D",0]
["1,1,1,2,3,3-Hexafluoro-4-methyl-4-penten-2-ol","","D",0]
["Perfluoro-9-oxodecane-1-sulfonic acid","","D",0]
["Trimethyl[3-(perfluorohexyl)-2-hydroxypropyl]azanium","","D",0]
["Trimethyl[3-(perfluorohexadecyl)-2-hydroxypropyl]azanium","","D",0]
["3-[Dimethyl(3-{[(perfluorotetradecyl)sulfonyl]amino}propyl)ammonio]propanoate","","D",0]
["1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-enoxybenzene","","D",0]
["Heptafluorobuta(2H)oic acid","","D",0]
["3-{(Perfluorodecanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["1,2,3,4,5,6,7,8,9,10,10,11,11,11-Tetradecafluoroundecyl hydrogen sulfate","","D",0]
["Heptadecafluorooctane-1-(2H)sulfonic acid","","D",0]
["3-{(Perfluorobutanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["1,2,3,4,5,6,7,8,8,9,9,9-Dodecafluorononyl hydrogen sulfate","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctane-1-(~2~H_2_)sulfonamide","","D",0]
["1,1,2,2,3,5,5,5-Octafluoropentyl prop-2-enoate","","D",0]
["Trimethyl(3-{2-[(perfluorododecyl)ethylthio]acetamido}propyl)azanium","","D",0]
["Perfluoroheptane sulfonamide amino carboxylates","","D",0]
["1,1,3,3,4,4,5,6,6,6-Decafluoro-5-(trifluoromethyl)hex-1-ene","","D",0]
["Propanoic acid, 2,?2,?3-?trifluoro-?3-?[1,?1,?2,?2,?3,?3-?hexafluoro-?3-?(trifluoromethoxy)?propoxy]?-?, sodium  salt (1:1)","","D",0]
["Perfluorohexane sulfonamide amino carboxylates","","D",0]
["1H, 1H, 2H, 2H-[1,2-13C2] perfluorooctyl phosphate","","D",0]
["Trimethyl(3-{2-[(perfluorotetradecyl)ethylthio]acetamido}propyl)azanium","","D",0]
["Perfluoroalkylpolyether-1","","D",0]
["3-[2-(Perfluorodecyl)ethylsulfanyl]-3-hydroxypropanoic acid","","D",0]
["Sodium bis(1H, 1H, 2H, 2H-[1,2-13C2]perfluorooctyl) phosphate","","D",0]
["Perfluorobutane sulfonamide amino carboxylates","","D",0]
["1,1,2,2-Tetrafluoro-2-(trifluoromethoxy)ethanesulfonic acid","","D",0]
["Trimethyl[3-(perfluorobutyl)-2-hydroxypropyl]azanium","","D",0]
["Perfluoroalkyl (linear) alkyl ethers","","D",0]
["1,1,2,2-Tetrafluoro-2-(naphthalen-2-ylmethoxy)ethanesulfonate","","D",0]
["Trimethyl(4,4,5,5,5-pentafluoro-2-hydroxypentyl)azanium","","D",0]
["3-[2-(Perfluorododecyl)ethylsulfanyl]propanoic acid","","D",0]
["1H, 1H, 2H, 2H-[1,2-13C2]perfluorodecylphosphate ion(1-)","","D",0]
["Trimethyl[3-(perfluorododecyl)-2-hydroxypropyl]azanium","","D",0]
["3-[3-(5-Bromo-2-fluorophenoxy)-N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]anilino]-1,1,1-trifluoropropan-2-ol","","D",0]
["1H, 1H, 2H, 2H-[1,2-13C2]perfluorodecylphosphate","","D",0]
["1,1,2,2-Tetrafluorooctane-1-sulfonic acid","","D",0]
["Trimethyl[3-(perfluorodecyl)-2-hydroxypropyl]azanium","","D",0]
["3-[{3-[(Carboxymethyl)(perfluorobutanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["Propanoic acid, 2-(1,1,2,2,3,3,4,4,4-nonafluorobutoxy)- 3,3,3-trifluoro-2-(trifluoromethyl)-","","D",0]
["1,1,2,2,3,3,4,4,5,5,6-Undecafluoro-6-(1,2,2,3,3,4,4,5,5,6,6-undecafluorocyclohexyl)sulfanylcyclohexane","","D",0]
["Trimethyl({3-[2-(2-(perfluorododecyl)ethylsulfinyl)acetamido]propyl})azanium","","D",0]
["Perfluoro-5-methylcyclohexane-1-carboxylic acid","","D",0]
["1,1,2,2,3,3-Hexafluoropentan-1-ol","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,8,8,8-Tetradecafluorooctane-1-sulfonate","","D",0]
["Trimethyl({3-[2-(2-(perfluorotetradecyl)ethylsulfinyl)acetamido]propyl})azanium","","D",0]
["1,1,2,2-Tetrafluoro-2-{[1,1,1,2,3,3-hexafluoro-3-(1,1,2,2-tetrafluoroethoxy)propan-2-yl]oxy}ethane-1-sulfonic acid","","D",0]
["3-[{3-[(Carboxymethyl)(perfluorododecanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["1,1,2,2,3,3,4,4,5,8,8,8-Dodecafluorooctane-1-sulfonate","","D",0]
["Trimethyl({3-[2-(2-(perfluorotetradecyl)ethanesulfonyl)acetamido]propyl})azanium","","D",0]
["Propanoic acid, 2-(1,1,2,2,3,3,3-heptafluorobutoxy)- 3,3,3-trifluoro-2-(trifluoromethyl)-","","D",0]
["Trimethyl({3-[2-(2-(perfluorohexyl)ethanesulfonyl)acetamido]propyl})azanium","","D",0]
["1,1,2,2,3,3,4,7,7,7-Decafluoroheptane-1-sulfonate","","D",0]
["Trimethyl({3-[2-(3,3,4,4,4-pentafluorobutanesulfonyl)acetamido]propyl})azanium","","D",0]
["Perfluoromethoxy perfluoropentane sulfonic acid","","D",0]
["1,1,2,2,3,3,4,4-Octafluorobutyl bicyclo[2.2.1]hept-5-ene-2-carboxylate","","D",0]
["Trimethyl({3-[2-(3,3,4,4,4-pentafluorobutanesulfinyl)acetamido]propyl})azanium","","D",0]
["3-[{3-[(Carboxymethyl)(perfluoroheptanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["1,1,2,2,3,3-Hexafluorobutane-1-sulfonic acid","","D",0]
["Trimethyl({3-[2-(3,3,4,4,5,5,6,6,6-nonafluorohexanesulfonyl)acetamido]propyl})azanium","","D",0]
["N1-(2-Aminoethyl)-N2-(2-{[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)oxy]amino}ethyl)ethane-1,2-diamine","","D",0]
["3-[{3-[(Carboxymethyl)(perfluorooctanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["Trimethyl({3-[2-(3,3,4,4,5,5,6,6,6- nonafluorohexanesulfinyl)acetamido]propyl})azanium","","D",0]
["6-Oxoperfluorooctanesulfonic acid","","D",0]
["3-[{3-[(Carboxymethyl)(perfluorononanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["3-[(Perfluoroundecanesulfonyl)amino]propane-1-sulfonic acid","","D",0]
["Sodium (((4-((1,1,2,2,3,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoro-3-nonen-1-yl)oxy)phenyl)sulfonyl)(methyl)amino)acetate","","D",0]
["3-[{3-[(Carboxymethyl)(pentafluoroethanesulfonyl)amino]propyl}(dimethyl)azaniumyl]propane-1-sulfonate","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,12,12,12-Heptadecafluorododecane-1-sulfonate","","D",0]
["1-Dodecanesulfonamide, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluorododecyl-N-methyl-","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluoro-N-propyl-N-(3-trimethoxysilylpropyl)octane-1-sulfonamide","","D",0]
["Sodium perfluoro-1-hexane[18O2]sulfonate","","D",0]
["N-(Carboxymethyl)-3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-tetracosafluoro-N,N-dimethyltetradecan-1-aminium","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,12,12,12-Nonadecafluorododecane-1-sulfonate","","D",0]
["Sodium 4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-nonadecafluoro-1-decen-1-yl)oxy]benzenesulfonate","","D",0]
["3-[[(Perfluoroundecyl)sulfonyl]amino]-N,N,N-trimethyl-1-propanaminium","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononane-1-ol","","D",0]
["(Ethyl{3-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonyl)amino]propyl}amino)oxidanide","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorodecan-1-ol","","D",0]
["trans-Perfluoromethylpropyl-(4-methylcyclohexyl)-amine","","D",0]
["3-[[3-(Dimethylamino)propyl]carbamoyl]-2-[2-(perfluorododecyl)ethylthio]propionic acid","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7-Tetradecafluoro-N,N'-diphenylheptane-1,7-diamine","","D",0]
["Triethoxy(1,1,2,2,5,5,5-heptafluoropentyl)silane","","D",0]
["3-[[3-(Dimethylamino)propyl]carbamoyl]-2-[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)thio]propionic acid","","D",0]
["2,2,3,5,5,6,6,7,7,9,9,9-Dodecafluoro-4,8-dioxononanoic acid","","D",0]
["Tridecafluorohexane-1-sulfinate","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(pentadecafluoroheptyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["Perfluoroalkyl symmetric anhydrides","","D",0]
["11-(Difluoromethyl)(perfluorododecyl)methyl prop-2-enoate","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(pentacosafluorododecyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["Perfluoroalkyl (linear) carboxylic acids","","D",0]
["10:2 Fluorotelomer sulfide (1-methanol 2-methanol) propanoate","","D",0]
["3-[(Perfluoroundecane-1-sulfonyl)amino]-N,N-dimethylpropan-1-amine N-oxide","","D",0]
["Perfluoroalkyl amidines","","D",0]
["11:2 Fluorotelomer ketone sulfonate","","D",0]
["Perfluorotridecanesulfonate","","D",0]
["Perfluoroalkyl gem-amino alcohols","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(pentafluoroethyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["Perfluoroalkyl (linear) amides (tertiary)","","D",0]
["3-(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-sulfinyl)propanoatato","","D",0]
["Perfluoro diacyl amides","","D",0]
["11-[(Perfluorododecanesulfonyl)amino]undecyl 2-methylprop-2-enoate","","D",0]
["2-[[(Perfluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate","","D",0]
["Perfluoroalkyl symmetric diamides","","D",0]
["3-Benzamido-2-fluoro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","","D",0]
["12:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["2-Methyl-2-[3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctane-1-sulfonyl)propanamido]propane-1-sulfonatato","","D",0]
["Perfluoroalkyl (linear) amides (primary)","","D",0]
["3-Amino-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]benzamide","","D",0]
["11-Hydrido-perfluorododecane-1-sulfonic acid","","D",0]
["2-Methyl-2-[3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctane-1-sulfinyl)propanamido]propane-1-sulfonatato","","D",0]
["Perfluoroalkyl (linear) amides (secondary)","","D",0]
["10:2 Fluorotelomer ketone sulfonate","","D",0]
["Polyfluoroalkyl (linear) carboxylic acids (-CHF2)","","D",0]
["10:2 Fluorotelomer dimethyl ethyl betaine","","D",0]
["3-{[3-(Dimethylamino)propyl][(perfluorotridecyl)sulfonyl]amino}propanoic acid","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(nonafluorobutyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["Perfluoroalkyl sulfonates","","D",0]
["3-{[3-(Dimethylamino)propyl]carbamoyl}-2-[2-(perfluorotetradecyl)ethylsulfanyl]propanoic acid","","D",0]
["Polyfluoroalkyl (linear) carboxylate esters (-CHF2)","","D",0]
["10:2 Fluorotelomer sulfate","","D",0]
["3-{[3-(Dimethylamino)propyl]carbamoyl}-2-[(3,3,4,4,4-pentafluorobutyl)sulfanyl]propanoic acid","","D",0]
["Perfluoro alkanes (linear)","","D",0]
["10:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(heptadecafluorooctyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["N-Alkyl perfluoroalkyl  (linear) sulfonamides","","D",0]
["10:2 fluorotelomer sulfinyl propanamido dimethyl ethyl sulfonate","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(henicosafluorodecyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["Perfluoroalkyl (linear) carboxylate esters","","D",0]
["10:4 Fluorotelomer betaine","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(nonadecafluorononyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["10:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(heptafluoropropyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["3-{[(Perfluoroethyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Alkyl perfluoroalkyl sulfonamidoacetic acids","","D",0]
["1,4,5,5,6,6-Hexafluorocyclohex-2-ene-1-carboxylate","","D",0]
["3-{[(Perfluorodecyl)sulfonyl]amino}-2-hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","","D",0]
["N-{3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanoyl}alanylalanine","","D",0]
["1,3,4,4,5,6,6,6-Octafluoro-5-(trifluoromethyl)hex-1-ene","","D",0]
["1-[2-[2-[2-[4-(2,2,3,3,3-Pentafluoropropoxy)phenyl]ethynyl]-3H-benzimidazol-5-yl]phenyl]ethanone","","D",0]
["heptadecafluoro(1,2,3,4,5-13C5)nonanoic acid","","D",0]
["{[(Perfluoropropyl)sulfonyl]amino}-3-betaine","","D",0]
["Polyfluoroalkyl (linear) aldehydes (-CHF2)","","D",0]
["1-[1,1,2-Trifluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)ethyl]-1H-imidazol-1-ium","","D",0]
["3-{[(Perfluorooctyl)sulfonyl]amino}-2-hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","","D",0]
["nonadecafluoro(1,2-13C2)decanoic acid","","D",0]
["10-(Pentafluorosulfanyl)perfluorodecyl sulfonic acid","","D",0]
["Perfluoroalkyl sulfonamido amines","","D",0]
["4-{[(2E)-1,1,2,3,4,4,5,5,6,6,6-Undecafluorohex-2-en-1-yl]oxy}benzene-1-sulfonic acid","","D",0]
["3-{[3-(Dimethylamino)propyl][(perfluorododecyl)sulfonyl]amino}propanoic acid","","D",0]
["1-[3-Fluoro-1-methyl-2-oxo-3-(trifluoromethyl)indol-5-yl]-3-[[2-methyl-3-(trifluoromethyl)phenyl]methyl]-2,4-dioxopyrimidine-5-carboxylic acid","","D",0]
["Sodium 4-{[(2E)-1,1,2,3,4,4,5,5,6,6,6-undecafluorohex-2-en-1-yl]oxy}benzene-1-sulfonate","","D",0]
["Perfluoroalkyl sulfonamide amino carboxylates","","D",0]
["3-{[3-(Dimethylamino)propyl][(perfluorodecyl)sulfonyl]amino}propanoic acid","","D",0]
["10:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["Perfluorooctane sulfonamide amino carboxylates","","D",0]
["10-(Perfluoromethoxy)perfluorodecane sulfonic acid","","D",0]
["4-[(1,1,2,2,3,3,4,4,5,6,6-Undecafluorohex-5-en-1-yl)oxy]benzene-1-sulfonic acid","","D",0]
["Perfluoropentane sulfonamide amino carboxylates","","D",0]
["3-{(Perfluoroethanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["1,2,3,4,5,6,7,8,9,10,11,12,13,14,14,15,15,15-Octadecafluoropentadecyl hydrogen sulfate","","D",0]
["Perfluoroalkyl (linear) ethers","","D",0]
["2-[(N-{3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanoyl}alanyl)amino]propanoatato","","D",0]
["3-{(Perfluorododecanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["2-({3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanoyl}oxy)propanoatato","","D",0]
["Perfluoroalkyl (linear) amide carboxylates","","D",0]
["3-{[(Perfluoropropyl)sulfonyl]amino}-2-hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-1-propanaminium","","D",0]
["3-{[4-(Dimethylamino)-1-hydroxy-2-butanyl][(tricosafluoroundecyl)sulfonyl]amino}-1-propanesulfonic acid","","D",0]
["Perfluoroalkyl symmetric diacyl fluorides","","D",0]
["1,2,4-Trichloro-1,1,2,3,3,4-hexafluoro-4-iodobutane","","D",0]
["2-{3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanamido}propanoate","","D",0]
["Perfluoroalkyl (linear) aldehydes","","D",0]
["Propanoic acid, 3-(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl-1-sulfinyl)-","","D",0]
["3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanoate","","D",0]
["Perfluoroalkyl acyl fluorides","","D",0]
["1,2-Dimethyl-3-(1,1,2,3,3,4,4,4-octafluorobutyl)imidazol-1-ium","","D",0]
["N-{3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanoyl}alanine","","D",0]
["3-{(Perfluoropentanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["2-({3-[(3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl)sulfanyl]propanoyl}oxy)propanoic acid","","D",0]
["Perfluorocarboxyl perfluoroalkyl sulfonic anhydrides","","D",0]
["1,3,3,4,4,5,6,6,6-Nonafluorohex-1-ene","","D",0]
["3-Fluoro-3-(perfluoroundecyl)prop-2-ene-1-sulfonic acid","","D",0]
["1-Benzyloxy-8,8,9,9,9-pentafluorononane","","D",0]
["3-Fluoro-3-(perfluorotridecyl)prop-2-ene-1-sulfonic acid","","D",0]
["3-Fluoro-3-(perfluorotridecyl)acrylic acid","","D",0]
["1-Bromo-2-(1,2,2,3,3,4,4,5,5,5-decafluoropentyl)benzene","","D",0]
["1-Benzyloxy-9,9,10,10,10-pentafluorodecane","","D",0]
["3-Hydroxy-3-[2-(perfluorohexyl)ethylsulfanyl]propanoic acid","","D",0]
["3-Hydroxy-3-[2-(perfluorododecyl)ethylsulfanyl]propanoic acid","","D",0]
["1-Bromo-4-pentafluoroethylsulfanylbenzene","","D",0]
["1-Chloroperfluorobutanesulfonic acid","","D",0]
["12:2 fluorotelomer sulfide (1-methanol 2-methanol) propanoic acid","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctane-1-thiolatato","","D",0]
["14:2 fluorotelomer dimethyl ethyl betaine","","D",0]
["3-Fluoro-3-(perfluorododecyl)acrylic acid","","D",0]
["3-Fluoro-3-(perfluorohexyl)acrylic acid","","D",0]
["3-Fluoro-3-(perfluoroheptyl)prop-2-ene-1-sulfonic acid","","D",0]
["3-Fluoro-3-(Perfluorononyl)prop-2-ene-1-sulfonic acid","","D",0]
["3-Fluoro-3-(perfluorohexyl)prop-2-ene-1-sulfonic acid","","D",0]
["3-Fluoro-3-(perfluorooctyl)prop-2-ene-1-sulfonic acid","","D",0]
["3-Fluoro-3-(perfluorooctyl)acrylic acid","","D",0]
["12-Hydrido-perfluorotridecane-1-sulfonic acid","","D",0]
["3-Chloro-perfluorotridecanoic acid","","D",0]
["12:2 Fluorotelomer unsaturated aldehyde","","D",0]
["12:2 Fluorotelomer thiol","","D",0]
["13:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["3-Chloro-perfluoroundecanoic acid","","D",0]
["13-Hydrido-perfluorotetradecane-1-sulfonic acid","","D",0]
["3-Fluoro-3-(perfluorobutyl)prop-2-ene-1-sulfonic acid","","D",0]
["13:2 Fluorotelomer ketone sulfonate","","D",0]
["Perfluorononyl Dimethicone/Methicone/Amodimethicone Crosspolymer","","D",0]
["14:2 Fluorotelomer carboxylic acid","","D",0]
["Perfluoroalkyl (linear) alkyl (linear) ketone","","D",0]
["12:2 Fluorotelomer ketone sulfonate","","D",0]
["12:2 Fluorotelomer dimethyl ethyl betaine","","D",0]
["3-Chloro-perfluorodecanoic acid","","D",0]
["14:2 Fluorotelomer ketone sulfonate","","D",0]
["1-Hydroxy-14:2 fluorotelomer sulfonic acid","","D",0]
["12:2 Fluorotelomer sulfate","","D",0]
["3-Chloro-perfluoroheptanoic acid","","D",0]
["12:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["3-Chloro-perfluorododecanoic acid","","D",0]
["12:2 fluorotelomer sulfonamide","","D",0]
["3-Chloro-perfluorooctanoic acid","","D",0]
["12:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["3-Chloro-perfluorononanoic acid","","D",0]
["4,4,5,5,6,6,6-Heptafluoro-1-[(2-hydroxyacetyl)sulfanyl]hexan-1-one","","D",0]
["1-Hydroxy-3:2 fluorotelomer sulfonic acid","","D",0]
["4,4,5,5,5-Pentafluoropentane-1-sulfonic acid","","D",0]
["1-Hydroxy-2:2 fluorotelomer sulfonic acid","","D",0]
["1-Hydroxy-5:2 fluorotelomer sulfonate","","D",0]
["4,4,5,5,6,6,6-Heptafluorohexan-3-yl acetate","","D",0]
["1-Hydroxy-4:2 fluorotelomer sulfonate","","D",0]
["1-Hydroxy-9:2 fluorotelomer sulfonic acid","","D",0]
["1-Hydroxy-6:2 fluorotelomer sulfonate","","D",0]
["4:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["2-(1,1,2,2,3,3,4,4,4-Nonafluorobutyl)bicyclo[2.2.1]heptane","","D",0]
["4,5,5,5-Tetrafluoro-2-methyl-4-(trifluoromethyl)pent-2-enoate","","D",0]
["2-(1,1,2,2,2-Pentafluoroethylsulfonyloxy)butyl 1,1,2,2,2-pentafluoroethanesulfonate","","D",0]
["1-Hydroxy-13:2 fluorotelomer sulfonic acid","","D",0]
["4-(Dimethylamino)-2-{[(perfluoroheptyl)sulfonyl]amino}butanoic acid","","D",0]
["3-{(Perfluorohexanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["3-Chloro-1,2,3,4,4,5,5-heptafluorocyclopentene","","D",0]
["1-Hydroxy-17:2 fluorotelomer sulfonic acid","","D",0]
["4-(Pentafluorosulfanyl)perfluorobutyl sulfonic acid","","D",0]
["1-Hydroxy-16:2 fluorotelomer sulfonic acid","","D",0]
["1-Hydroxy-2:2 fluorotelomer sulfonate","","D",0]
["1-Ethenoxy-1,1,2,2,5,5,5-heptafluoropentane","","D",0]
["4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,15-Hentriacontafluoropentadecoxy)phenol","","D",0]
["1-Chloro-perfluorotridecane-1-sulfonic acid","","D",0]
["1-Ethylsulfonyl-1,1,2,2,2-pentafluoroethane","","D",0]
["4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Pentadecafluorooctanoylamino)benzenesulfonic acid","","D",0]
["4-((1,1,2,2,3,3,4,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-4-nonen-1-yl)oxy)benzoic acid","","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-N-hydroxy-2,6-dimethylbenzenecarboximidoyl chloride","","D",0]
["1-Hydroxy-10:2 fluorotelomer sulfonic acid","","D",0]
["4-(1,1,2,2,3,3,3-Heptafluoropropylsulfanyl)-2-methylaniline","","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-ylsulfanyl)-2,6-dimethylaniline","","D",0]
["4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctylsulfonyloxy)butyl 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonate","","D",0]
["4-(Dimethylamino)-2-{[(perfluoroethyl)sulfonyl]amino}butanoic acid","","D",0]
["1-Hydroxy-11:2 fluorotelomer sulfonic acid","","D",0]
["4-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Henicosafluoroundecyl)phenol","","D",0]
["1-Ethylsulfonyl-1,1,2,2,3,3,3-heptafluoropropane","","D",0]
["4-(Dimethylamino)-2-{[(perfluorodecyl)sulfonyl]amino}butanoic acid","","D",0]
["1-Ethenyl-4-(1,1,2,2,2-pentafluoroethoxy)benzene","","D",0]
["1-Chloro-perfluoropentadecane-1-sulfonic acid","","D",0]
["4-(1,1,2,2,3,3,4,4,5,5,6,6,6-Tridecafluorohexoxy)phenol","","D",0]
["4-(Dimethylamino)-2-{[(perfluoropropyl)sulfonyl]amino}butanoic acid","","D",0]
["3-[7-Fluoro-6-(4,4,5,5,5-pentafluoropentoxy)spiro[2H-1-benzofuran-3,4'-piperidine]-1'-yl]propanoic acid","","D",0]
["5-({[(2-(Perfluorododecyl)ethyl)sulfanyl]carbonyl}amino)pentanoic acid","","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10-Heptadecafluoropentadecanoic acid","","D",0]
["5-({[(2-(Perfluorohexyl)ethyl)sulfanyl]carbonyl}amino)pentanoic acid","","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10-Heptadecafluorononadecanoic acid","","D",0]
["2,2,3,3,4,4,5,5,6,6-Decafluorooctanoic acid","","D",0]
["5-({[(2-(Perfluorooctyl)ethyl)sulfanyl]carbonyl}amino)pentanoic acid","","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Henicosafluoroundecane-1,1-diol","","D",0]
["5-({[(2-(Perfluorodecyl)ethyl)sulfanyl]carbonyl}amino)pentanoic acid","","D",0]
["2-(Perfluorotetradecyl)ethane sulfinic acid","","D",0]
["4-Oxo-N-(2,2,3,3-tetrafluoro-1,4-benzodioxin-6-yl)-1H-quinoline-3-carboxamide","","D",0]
["5-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononyl)oxy)isophthalic acid","","D",0]
["1-Chloroperfluoropentanesulfonic acid","","D",0]
["2-(Perfluorododecyl)ethane sulfinic acid","","D",0]
["4-Bromo-5-(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-enoxy)benzene-1,2-diamine","","D",0]
["2-(Perfluorodecyl)ethane sulfinic acid","","D",0]
["4-{[(1E)-1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Nonadecafluoro-1-decen-1-yl]oxy}benzenesulfonic acid","","D",0]
["2-(Perfluorohexadecyl)ethane-1-sulfonic acid","","D",0]
["4-Bromo-5-(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoronon-1-enoxy)benzene-1,2-diamine","","D",0]
["2-(Perfluoroeicosanyl)ethane-1-sulfonic acid","","D",0]
["4-Bromo-5-(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-enoxy)phthalic acid","","D",0]
["2-(Perfluorooctadecyl)ethane-1-sulfonic acid","","D",0]
["4-Fluoro-N-[1-(4-fluorophenyl)-1-hydroxy-3-(2,2,3,3-tetrafluoro-1,4-benzodioxin-6-yl)propan-2-yl]naphthalene-1-carboxamide","","D",0]
["2-(Perfluorooctyl)ethane sulfinic acid","","D",0]
["2,6-Dichloro-4-(1,1,1,2,3,3,3-heptafluoropropan-2-ylsulfinyl)aniline","","D",0]
["4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Henicosafluorodecyl)phenol","","D",0]
["2-(N-Methyl-perfluorodecanesulfonamido)acetic acid","","D",0]
["4-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,10,10-Nonadecafluoro-9-decen-1-yl)oxy]benzenesulfonic acid","","D",0]
["2-(Methyl{perfluoro-2-[2,6-bis(ethyl)morpholin-4-yl]ethanesulfonyl}amino)ethyl prop-2-enoate","","D",0]
["2-(N-Methyl-perfluorononanesulfonamido)acetic acid","","D",0]
["4-[1-(Bromo-difluoro-methyl)-1,2,2,2-tetrafluoro-ethyl]-2-methyl-phenylamine","","D",0]
["4-[2-[4-[3,3,4,4,5,5-Hexafluoro-2-[6-[2-(4-methoxyphenyl)ethenyl]-2-methyl-1-benzothiophen-3-yl]cyclopenten-1-yl]-3,5-dimethylthiophen-2-yl]ethenyl]benzonitrile","","D",0]
["2-(N-Methyl-perfluorotetradecanesulfonamido)acetic acid","","D",0]
["4-[1-[4-(1,1,2,2,2-Pentafluoroethylsulfanyl)phenyl]-1,2,4-triazol-3-yl]benzaldehyde","","D",0]
["2-(Pentafluorosulfanyl)perfluoroethyl sulfonic acid","","D",0]
["4-[Ethyl(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctylsulfonyl)amino]-2-methylidenebutanoate","","D",0]
["4-[5-(4-Chlorophenyl)-3-(1,1,2,2,3,3,3-heptafluoropropyl)pyrazol-1-yl]benzenesulfonamide","","D",0]
["4:2 Fluorotelomer ketone sulfonate","","D",0]
["2-(11-[Chloro(difluoro)methyl]perfluorododecyl)ethyl prop-2-enoate","","D",0]
["4:2 Fluorotelomer dimethyl ethyl betaine","","D",0]
["2-(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-enoxy)-5-methoxybenzene-1,4-diamine","","D",0]
["2-(1-Ethenoxy-1,1,2,3,3,3-hexafluoropropan-2-yl)oxy-1,1,2,2-tetrafluoroethanesulfonyl fluoride","","D",0]
["4:2 Fluorotelomer sulfinate","","D",0]
["2-(2,4-Difluorophenyl)sulfanyl-1,1,2,2-tetrafluoroethanesulfonic acid","","D",0]
["2-(Methyl((nonafluorobutyl)sulfonyl)amino)ethyl octacosanoate","","D",0]
["4:2 Fluorotelomer sulfonamido propyl methyl amine","","D",0]
["4:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["2-(Aminomethyl)-2,3,3,3-tetrafluoropropanoic acid","","D",0]
["Acetic acid, [1-(3-chloro-1,1,2,2,3,3-hexafluoropropoxy)-1,2,2,2-tetrafluoroethoxy]-.alpha.,.alpha.-difluoro-","","D",0]
["4-Methyl-5-(1,2,3,3,4,4,5,5,6,6,6-undecafluorohex-1-enoxy)benzene-1,3-dicarboxylic acid","","D",0]
["Propanal, 2,2,3,3-tetrafluoro-3-[[1,1,1,2,3,3-hexafluoro-3-(1,2,2,2-tetrafluoroethoxy)propan-2-yl]oxy-","","D",0]
["2,6-Dibromo-4-(1,1,2,2,3,3,4,4,4-nonafluorobutylsulfinyl)aniline","","D",0]
["Acetic acid, [2-(3-chloro-1,1,2,2,3,3-hexafluoropropoxy)-1,1,2,3,3,3-hexafluoropropoxy]-.alpha.,.alpha.-difluoro-","","D",0]
["2,6-Difluoro-N-[3-[[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-iodo-6-(trifluoromethyl)phenyl]carbamoyl]phenyl]-N-methylbenzamide","","D",0]
["2,6-Dichloro-4-(1,1,2,2,3,3,4,4,4-nonafluorobutylsulfinyl)aniline","","D",0]
["2,6-Dimethyl-4-(1,1,2,2,3,3,4,4,4-nonafluorobutylsulfanyl)aniline","","D",0]
["6-({[(Perfluorooctyl)ethylthio]carbonyl}amino)hexanal","","D",0]
["2,6-Diiodo-4-(perfluoropropan-2-yl)aniline","","D",0]
["6-(Perfluoromethoxy)perfluorohexane sulfonic acid","","D",0]
["2:2 Fluorotelomer betaine","","D",0]
["6-(Pentafluorosulfanyl)perfluorohexyl sulfonic acid","","D",0]
["2:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["5-[4-[4-(4,4,5,5,5-Pentafluoropentylsulfanyl)butoxy]phenyl]-6-phenyl-8,9-dihydro-7H-benzo[7]annulen-2-ol","","D",0]
["2,2-Dichloro-perfluoro-1-undecanesulfonic acid","","D",0]
["5-[3-({[2-(Perfluorotetradecyl)ethylsulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["2,3,3,4,4-Pentafluorothiolane 1,1-dioxide","","D",0]
["9-Octadecenoic acid, 2,2,3,3,4,4,4-heptafluorobutyl ester","","D",0]
["5-Bromo-1-(5-bromo-1,2,3,3,4,4,5,5-octafluoropent-1-enoxy)-1,2,3,3,4,4,5,5-octafluoropent-1-ene","","D",0]
["2,3,3,4,4,4-Hexafluorobutane-2-sulfonic acid","","D",0]
["2,3,5-Trifluoro-6-(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-heptadecafluoronon-1-enoxy)benzene-1,4-diamine","","D",0]
["Acetic acid, [2-[1-(3-chloro-1,1,2,2,3,3-hexafluoropropoxy)-1,2,2,2-tetrafluoroethoxy]-1,2,2,2-tetrafluoroethoxy]-.alpha.,.alpha.-difluoro-","","D",0]
["5-Chloro-6-(4-fluorophenyl)-2-(heptafluoropropyl)-1H-1,3-benzodiazole","","D",0]
["2,3,3-Trifluoro-2-(trifluoromethyl)-1,4-dioxane","","D",0]
["3,5,7,9-Tetraoxadodecan-1-oic acid, 12-chloro-2,2,4,6,8,10,10,11,11,12,12-undecafluoro-4,6,8-tris(trifluoromethyl)-","","D",0]
["2-Chloro-7-(difluoromethyl)-1,3,4,4,5,6,6,7,8,8,9,9,10,10,11,12,12,12-octadecafluoro-11-(trifluoromethyl)dodec-1-ene","","D",0]
["6-({[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]carbonyl}amino)hexanal","","D",0]
["5-Fluoro-3-iodo-1-(3,3,4,4,4-pentafluorobutyl)-1H-pyrazolo[3,4-b]pyridine","","D",0]
["Acetic acid, [1-[1-(3-chloro-1,1,2,2,3,3-hexafluoropropoxy)-1,2,2,2-tetrafluoroethoxy]-1,2,2,2-tetrafluoroethoxy]-.alpha.,.alpha.-difluoro-","","D",0]
["5-[2,2-Bis(trifluoromethyl)-3,3,4,4,5,5,5-heptafluoropentyl]benzene-1,3-diamine","","D",0]
["5:2 Fluorotelomer ketone sulfonate","","D",0]
["2,2-Dichloro-perfluoro-1-dodecanesulfonic acid","","D",0]
["2,2-Dichloro-perfluoro-1-nonanesulfonic acid","","D",0]
["5-[3-({[2-(Perfluorododecyl)ethylsulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["2,2-Dichloro-perfluoro-1-hexanesulfonic acid","","D",0]
["5-[3-({[2-(Perfluorodecyl)ethylsulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["5-[3-({[2-(Perfluorooctyl)ethylsulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["2,2-Dichloro-perfluoro-1-pentanesulfonic acid","","D",0]
["5-({[(3,3,4,4,5,5,6,6,6-Nonafluorohexyl)sulfanyl]carbonyl}amino)pentanoic acid","","D",0]
["2,2,3,3,4,5,5-Heptafluoropent-4-enenitrile","","D",0]
["5-({[(3,3,4,4,4-Pentafluorobutyl)sulfanyl]carbonyl}amino)pentanoic  acid","","D",0]
["2,2,3,3,4,5,5,6-Octafluoro-6-(trifluoromethyl)morpholine","","D",0]
["5-(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-enoxy)-4-methylbenzene-1,3-diamine","","D",0]
["2,2,3,3,5,5-Hexafluoro-1,4-dioxane","","D",0]
["5-(1,1,2,2,3,3,4,4,5,5,6,6,6-Tridecafluorohexyl)bicyclo[2.2.1]hept-2-ene","","D",0]
["2,2,3,3,4-Pentafluorooctanoic acid","","D",0]
["5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-Heptadecafluoro-4-oxododecyl prop-2-enoate","","D",0]
["2,2,3,3-Tetrafluorothiolane 1,1-dioxide","","D",0]
["2,2,3,3-Tetrafluorobutyl prop-2-enoate","","D",0]
["2,2,4,5-Tetrafluoro-4-(trifluoromethyl)thiolane 1,1-dioxide","","D",0]
["6-({[(3,3,4,4,4-Pentafluorobutyl)sulfanyl]carbonyl}amino)hexanal","","D",0]
["2-(Perfluorooctane-1-sulfinyl)ethyl prop-2-enoate","","D",0]
["2,2,3,4,4,5,6,6,7,8,8,9,9,10,10-Pentadecafluoroadamantan-1-ol","","D",0]
["2-[3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butyl]-2-(3,3,3-trifluoropropyl)propanedinitrile","","D",0]
["Carboxydimethyl(4,4,5,5,5-pentafluoro-2-hydroxypentyl)azanium","","D",0]
["Calcium perfluorohexadecanoate","","D",0]
["2-[[5-[4-[5-(4,4,5,5,5-Pentafluoropentylsulfonyl)pentoxy]phenyl]-6-phenyl-8,9-dihydro-7H-benzo[7]annulen-2-yl]oxy]oxane","","D",0]
["Perfluoroalkyl (linear) phosphonic acids","","D",0]
["2-[Dimethyl(2-(1-hydridoperfluoroheptyl)ethyl)azaniumyl]acetate","","D",0]
["8:2 Fluorotelomer ketone sulfonate","","D",0]
["2-[2-(Perfluorotetradecyl)ethylsulfanyl]acetic acid","","D",0]
["8:2 Fluorotelomer sulfide (1-methanol 2-methanol) propanoic acid","","D",0]
["n-Perfluoroalkyl ethyliodide","","D",0]
["2-[Bis(perfluoropentanoyl)amino]ethyl 2-methylprop-2-enoate","","D",0]
["Carboxydimethyl[3-(perfluorobutyl)-2-hydroxypropyl]azanium","","D",0]
["Perflutren - Human albumin","","D",0]
["Carboxydimethyl[3-(perfluorodecyl)-2-hydroxypropyl]azanium","","D",0]
["2-[4-[1-[4-(1,1,2,2,2-Pentafluoroethoxy)phenyl]-1,2,4-triazol-3-yl]phenyl]acetic acid","","D",0]
["2-[2-(Perfluorododecyl)ethylsulfanyl]acetic acid","","D",0]
["8:2 fluorotelomer sulfate","","D",0]
["2-[2-[2-[4-(2,2,3,3,3-Pentafluoropropoxy)phenyl]ethynyl]-3H-benzimidazol-5-yl]benzenesulfonamide","","D",0]
["8:2 fluorotelomer sulfinyl propanamido dimethyl ethyl sulfonate","","D",0]
["2-[3-(2-(Perfluorooctyl)ethanesulfonyl)propanoylamino]-2-methylpropane-1-sulfonic acid","","D",0]
["2-[3-(2-(Perfluorodecyl)ethanesulfonyl)propanamido]-2-methylpropane-1-sulfonic acid","","D",0]
["Heptadecafluoro isooctanesulfonic acid","","D",0]
["6:2 Fluorotelomer sulfonamido propyl methyl amine","","D",0]
["5,6-Dichloro-1-iodoperfluorohexane","","D",0]
["2-[(4,4,5,5,6,6,6-Heptafluorohexyl)dimethylazaniumyl]acetate","","D",0]
["2-[(2-(1-Hydrido-perfluorotridecyl)ethyl)dimethylazaniumyl]acetate","","D",0]
["8:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl (3a,5b,6b,7b,20R)-3,6,7-tris[(trifluoroacetyl)oxy]cholan-24-oate","","D",0]
["6:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["1,1,1,3,3,3-hexafluoropropan-2-yl (3a,5b,6b,20R)-3,6-bis[(trifluoroacetyl)oxy]cholan-24-oate","","D",0]
["2,2,3,3,3-pentafluoro-N-(3H-1,2,4-triazol-3-yl)propanamide","","D",0]
["2,2,3,3,3-pentafluoro-N-(4H-1,2,4-triazol-4-yl)propanamide","","D",0]
["1-Heptanesulfonic acid, 1,1,2,2,3,3,4,4,5,6,6,7,7,7-tetradecafluoro-5-(trifluoromethyl)-","","D",0]
["2:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["2-(heptafluoropropyl)-6-(trifluoromethyl)-1H-benzimidazole","","D",0]
["2:2 Fluorotelomer ketone sulfonate","","D",0]
["2:2 Fluorotelomer dimethyl ethyl betaine","","D",0]
["2:2 Fluorotelomer sulfide (1-methanol 2-methanol) propanoate","","D",0]
["2:2 Fluorotelomer sulfonamido propyl betaine","","D",0]
["1-Heptanesulfonic acid, 1,1,2,3,3,4,4,5,5,6,6,7,7,7-tetradecafluoro-2-(trifluoromethyl)-","","D",0]
["6:2 Fluorotelomer sulfonamido propyl amine","","D",0]
["1-Hexanesulfonic acid, 1,1,2,2,3,3,5,5,6,6,6-undecafluoro-4,4-bis(trifluoromethyl)-","","D",0]
["6:2 Fluorotelomer sulfide (1-methanol 2-methanol) propanoate","","D",0]
["2:2 Fluorotelomer sulfinate","","D",0]
["1-Heptanesulfonic acid, 1,1,2,2,3,3,4,5,5,6,6,7,7,7-tetradecafluoro-4-(trifluoromethyl)-","","D",0]
["6:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["1-Heptanesulfonic acid,1,1,2,2,3,4,4,5,5,6,6,7,7,7-tetradecafluoro-3-(trifluoromethyl)-","","D",0]
["7-(Perfluoromethoxy)perfluoroheptane sulfonic acid","","D",0]
["Ethenyl 4-(perfluoroheptyl)butanoate","","D",0]
["2-[Dimethyl[2-(perfluorotetradecyl)ethyl]azaniumyl]acetate","","D",0]
["2-[Dimethyl[2-(perfluorododecyl)ethyl]azaniumyl]acetate","","D",0]
["Fluoromethyl 1,1,2,2,2-pentafluoroethyl carbonate","","D",0]
["2-[Dimethyl[3-(perfluorodecyl)-2-hydroxypropyl]azaniumyl]acetate","","D",0]
["Lithium 1,1,1,2,2-pentafluoro-2-sulfinatoethane","","D",0]
["2-[Dimethyl[3-(perfluorohexyl)-2-hydroxypropyl]azaniumyl]acetate","","D",0]
["Hexafluoro-1,3-propanedisulfonic acid","","D",0]
["2-[Dimethyl[3-(perfluorohexadecyl)-2-hydroxypropyl]azaniumyl]acetate","","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-(fluoromethyl)propanoate","","D",0]
["2-[Dimethyl[3-(perfluorooctyl)-2-hydroxypropyl]azaniumyl]acetate","","D",0]
["2-[Dimethyl[3-(perfluorooctadecyl)-2-hydroxypropyl]azaniumyl]acetate","","D",0]
["2-[Dimethyl(4-fluoro-4-(perfluorononyl)-2-hydroxybut-3-en-1-yl)azaniumyl]acetate","","D",0]
["Dimethyl[3-(perfluorohexadecyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["2-[Dimethyl(4-fluoro-4-(perfluoroheptadecyl)-2-hydroxybut-3-en-1-yl)azaniumyl]acetate","","D",0]
["Propanoic acid, 2,2,3,3-tetrafluoro-3-(trifluoromethoxy)-, anhydride with 2,2,3,3-tetrafluoro-3-(trifluoromethoxy)propanoic acid","","D",0]
["Dimethyl[3-(perfluorododecyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["Dimethyl[3-(perfluorooctyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["2-[Dimethyl(4-fluoro-4-(perfluoropentyl)-2-hydroxybut-3-en-1-yl)azaniumyl]acetate","","D",0]
["Dioxido(1,1,2,2,2-pentafluoroethoxy)borane","","D",0]
["2-[Dimethyl(4-fluoro-4-(perfluorotridecyl)-2-hydroxybut-3-en-1-yl)azaniumyl]acetate","","D",0]
["Dimethyl[3-(perfluorotetradecyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["2-[Dimethyl(4-fluoro-4-(perfluoropropyl)-2-hydroxybut-3-en-1-yl)azaniumyl]acetate","","D",0]
["Ethyl 2-(4,4,5,5,5-pentafluoropentyl)-9-decenoate","","D",0]
["5:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["Flubendiamide metabolite (NNI-0001-3-OH)","","D",0]
["2-[Dimethyl(3,4,4,5,5,6,6,6-octafluorohexyl)azaniumyl]acetate","","D",0]
["Difluoro(1,1,2,2,3,3,4,4,4-nonafluorobutyl)phosphane","","D",0]
["Polyperfluoroethoxymethoxy difluoroethyl peg phosphate","","D",0]
["2-[Dimethyl(3-{2-[(perfluorotetradecyl)ethylthio]acetamido}propyl)azaniumyl]acetate","","D",0]
["3-[3-[4-Chloro-3-(trifluoromethyl)phenoxy]-N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]anilino]-1,1,1-trifluoropropan-2-ol","","D",0]
["difluoro[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2-tetrafluoro-2-sulfoethoxy)propoxy]acetic acid","","D",0]
["2-[Dimethyl(3-{2-[(3,3,4,4,4-pentafluorobutyl)sulfanyl]acetamido}propyl)azaniumyl]acetate","","D",0]
["2-Propenoic acid, 2-methyl-, butyl ester, polymer with 2-[ethyl[(heptadecafluorooctyl)sulfonyl]amino]ethyl 2-methyl-2- propenoate, 2- [ethyl[(nonafluorobutyl)sulfonyl]amino]ethyl 2-methyl-2-propenoate, 2-[ethyl[(pentadecafluoroheptyl)sulfonyl]amino]ethyl","","D",0]
["Difluoro(trifluoromethoxy)methanesulfonic acid","","D",0]
["2-[Dimethyl(4,4,5,5,5-pentafluoropentyl)azaniumyl]acetate","","D",0]
["F-Methyl-1-oxadecalin","","D",0]
["Dimethyl(2-oxoethyl)[4,4,5,5,5-pentafluoro-2-(formyloxy)pentyl]azanium","","D",0]
["2-[Dimethyl(4,4,5,5,5-pentafluoro-2-hydroxypentyl)azaniumyl]acetate","","D",0]
["2-[4-[2-(Oxan-2-yloxy)-5-[4-[5-(4,4,5,5,5-pentafluoropentylsulfonyl)pentoxy]phenyl]-8,9-dihydro-7H-benzo[7]annulen-6-yl]phenoxy]oxane","","D",0]
["Dimethyl 1,1,2,2,2-pentafluoroethyl phosphate","","D",0]
["2-[Dimethyl(4,5,5,5-tetrafluoro-2-hydroxypent-3-en-1-yl)azaniumyl]acetate","","D",0]
["Dimethyl[3-(perfluorodecyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["2-[Dimethyl(4,4,5,5,6,6,7,7,7-nonafluoroheptyl)azaniumyl]acetate","","D",0]
["2,2-Bis[[(.gamma.-.omega.-perfluoro-C10-20-alkyl)thio]methyl]-1,3-propanediol","","D",0]
["Dimethyl[3-(perfluorobutyl)-2-(formyloxy)propyl](2-oxoethyl)azanium","","D",0]
["2-[Dimethyl(2-(1-hydrido-perfluorotetradecyl)ethyl)azaniumyl]acetate","","D",0]
["Perfluoroalkyl (linear) epoxides","","D",0]
["Carboxydimethyl[3-(perfluorohexyl)-2-hydroxypropyl]azanium","","D",0]
["2-[Dimethyl(5,5,6,6,6-pentafluorohexyl)azaniumyl]acetate","","D",0]
["Perfluoroalkane sulfinic acids","","D",0]
["Perfluoroalkylether (linear) sulfonic acids","","D",0]
["Carboxydimethyl[3-(perfluorotetradecyl)-2-hydroxypropyl]azanium","","D",0]
["2-[Dimethyl(3-(perfluorodecyl)propyl)azaniumyl]acetate","","D",0]
["Perfluoroalkyl (linear) sulfonyl fluorides","","D",0]
["Carboxydimethyl[3-(perfluorooctyl)-2-hydroxypropyl]azanium","","D",0]
["2-[Dimethyl(3-(perfluorobutyl)-2-hydroxypropyl)azaniumyl]acetate","","D",0]
["Perfluoro(mono)alkenes (linear)","","D",0]
["2-[Dimethyl(3-(perfluorooctyl)propyl)azaniumyl]acetate","","D",0]
["Perfluoroalkyl (linear) vinyl ethers","","D",0]
["Perfluoroalkylether (linear) carboxylic acids","","D",0]
["Carboxymethyl-3-nonadecafluorodecaneamidopropylammonium hydroxide salt","","D",0]
["2-[Dimethyl(3-(perfluorododecyl)propyl)azaniumyl]acetate","","D",0]
["Poly(difluoromethylene), .alpha.-fluoro-.omega.-[2-[(1-oxo-2-propen-1-yl)oxy]ethyl]- (2-Propeonic acid, perfluoro-C6-14-alkylethyl esters, C8 rich)","","D",0]
["2-[Dimethyl(3-(perfluoropentadecyl)propyl)azaniumyl]acetate","","D",0]
["2-Propeonic acid, perfluoro-C6-14-alkylethyl esters, C8 rich","","D",0]
["cis-Perfluoromethylpropyl-(4-methylcyclohexyl)-amine","","D",0]
["N-(3-{(Carboxymethyl)[(perfluoroethyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["(1Z)-2,2,3,3,4,4,4-heptafluoro-N-(1,1,2,2,3,3,4,4,4-nonafluorobutyl)butanimidoyl fluoride","","D",0]
["2-{[3-(Acetyloxy)-1,5-dihydroxy-4-(perfluorohexadecyl)pentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Hexadecafluoro-1-octanesulfonic acid)","","D",0]
["2-{[3-(Acetyloxy)-1,5-dihydroxy-4-(perfluorododecyl)pentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["N-(3-{(Carboxymethyl)[(perfluorohexyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["(((4-((1,1,2,2,3,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-3-nonen-1-yl)oxy)phenyl)sulfonyl)(methyl)amino)acetic acid","","D",0]
["2-[Dimethyl(2-(1-hydrido-perfluoropentadecyl)ethyl)azaniumyl]acetate","","D",0]
["N-(3-{(Carboxymethyl)[(perfluoroheptyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["2-{[3-(Acetyloxy)-1,5-dihydroxy-4-(perfluorohexyl)pentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorodecyl)-2-hydroxypropyl]azanium","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorobutyl)-2-hydroxypropyl]azanium","","D",0]
["N-(3-{(Carboxymethyl)[(perfluorooctyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["2-{[3-(Acetyloxy)-4-(perfluorodecyl)-1,5-dihydroxypentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["3-(((4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,9,9-Heptadecafluoro-8-nonen-1-yl)oxy)phenyl)sulfonyl)amino)-N,N,N-trimethyl-1-propanaminium iodide","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorohexadecyl)-2-hydroxypropyl]azanium","","D",0]
["2-{Methyl[perfluoro(4-ethylcyclohexyl)ethanesulfonyl]amino}ethyl prop-2-enoate","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorododecyl)-2-hydroxypropyl]azanium","","D",0]
["N-(3-{(Carboxymethyl)[(perfluoroundecyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["2-{[3-(Acetyloxy)-4-(perfluorooctyl)-1,5-dihydroxypentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["2-{[2-(Acetyloxy)-3-(perfluorobutyl)propyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluoroethanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorotetradecyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluorododecanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["(((4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononyl)oxy)phenyl)sulfonyl)(methyl)amino)acetic acid","","D",0]
["2-{[2-(Acetyloxy)-3-(perfluorooctadecyl)propyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluorononanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluoroheptanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluoroundecanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["(1,1,1,2,2-pentafluoro-4-methylheptan-4-yl) phosphate","","D",0]
["2-{[2-(Acetyloxy)-4,4,5,5,5-pentafluoropentyl]dimethylazaniumyl}acetate","","D",0]
["2-{[3-(Acetyloxy)-1,5-dihydroxy-4-(perfluorotetradecyl)pentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluoroethyl)sulfonyl]amino}-1-butanaminium","","D",0]
["(1,1,2,2,3,3,4,4,4-Nonafluorobutyl)phosphanium","","D",0]
["N-(3-{(Carboxymethyl)[(perfluorodecyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["2-{[3-(Acetyloxy)-1,5-dihydroxy-4-(perfluorobutyl)pentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["(1,1,2,2,3,3,3-Heptafluoropropoxy)(prop-1-en-1-yl)silane","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorobutyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-3-{(2-hydroxyethyl)[(perfluorododecyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(1,1,2,2,2-pentafluoroethyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-3-{(2-hydroxyethyl)[(perfluoroundecyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorodecyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-3-{(2-hydroxyethyl)[(perfluorononyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorohexyl)butyl]dimethylazaniumyl}acetate","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorohexadecyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-{[(perfluorododecyl)sulfonyl]amino}-1-propanaminium","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorooctyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluorodecanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["2-{[2-(Acetyloxy)-1,4-dihydroxy-3-(perfluorooctadecyl)butyl]dimethylazaniumyl}acetate","","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-{[(perfluoroundecyl)sulfonyl]amino}-1-propanaminium","","D",0]
["Methyl-bis[(1,2,2,3,3,4,4,5,5,6,6-undecafluorocyclohexyl)oxy]silane","","D",0]
["2-[Dimethyl[4-(perfluorododecyl)butyl]azaniumyl]acetate","","D",0]
["Methyl 2-[4-[1-[4-(1,1,2,2,2-pentafluoroethoxy)phenyl]-1,2,4-triazol-3-yl]phenyl]acetate","","D",0]
["2-[Dimethyl[3-(perfluorotetradecyl)-2-hydroxypropyl]azaniumyl]acetate","","D",0]
["2-[Dimethyl[4-(perfluorotetradecyl)butyl]azaniumyl]acetate","","D",0]
["2-[Dimethyl[4-(perfluorooctadecyl)butyl]azaniumyl]acetate","","D",0]
["4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-Heptacosafluorotridecoxy)phenol","","D",0]
["2-{[2-(Acetyloxy)-3-(perfluorotetradecyl)propyl]dimethylazaniumyl}acetate","","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluorododecyl)sulfonyl]amino}-1-butanaminium","","D",0]
["2-{(Perfluoro[3-(4-ethylpiperidin-1-yl)propanoyl])(methyl)amino}ethyl prop-2-enoate","","D",0]
["N-(2,3-Dihydroxypropyl)-4-hydroxy-N,N-dimethyl-3-{[(perfluorononyl)sulfonyl]amino}-1-butanaminium","","D",0]
["2-[Methyl(perfluoro(4,7,10,13-tetraoxapentadecanoyl))amino]ethyl prop-2-enoate","","D",0]
["(E)-5-((Perfluorohept-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluoroundecanesulfonyl)amino]propan-1-aminium","","D",0]
["2H-Perfluorohexanoic acid","","D",0]
["(E)-5-((Perfluoronon-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["N,N-Dimethyl-3-{[(perfluorododecyl)sulfonyl](3-sulfopropyl)amino}-N-(3-sulfopropyl)-1-propanaminium","","D",0]
["2H-Perfluoropentanoic acid","","D",0]
["N,N-Dimethyl-3-{[(perfluorodecyl)sulfonyl](3-sulfopropyl)amino}-N-(3-sulfopropyl)-1-propanaminium","","D",0]
["(E)-5-((Perfluorohex-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["N,N-Dimethyl-3-{[(perfluorononyl)sulfonyl](3-sulfopropyl)amino}-N-(3-sulfopropyl)-1-propanaminium","","D",0]
["(E)-5-((Perfluorooct-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["N,N-Dimethyl-3-{[(perfluoroethyl)sulfonyl](3-sulfopropyl)amino}-N-(3-sulfopropyl)-1-propanaminium","","D",0]
["(E)-6H-Perfluoronon-7-ene-1-sulfonic acid","","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(perfluoro-1-sulfonylpentadecyl)amino]-1-propanaminium","","D",0]
["(E)-5H-Perfluorooct-6-ene-1-sulfonic acid","","D",0]
["N,N-Dimethyl-3-{[(perfluoroundecyl)sulfonyl](3-sulfopropyl)amino}-N-(3-sulfopropyl)-1-propanaminium","","D",0]
["2-Hydrido-perfluoropentadecanoic acid","","D",0]
["2-Chloro-perfluorohexanoic  acid","","D",0]
["(7E)-nonadecafluorodec-7-ene-1-sulfonic acid","","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluorobutanesulfonyl)amino]propan-1-aminium","","D",0]
["2-[Dimethyl[4-(perfluorohexadecyl)butyl]azaniumyl]acetate","","D",0]
["(2,2,3,3,4,4,4-heptafluorobutyl)stannanylidyne","","D",0]
["N,N,N-Trimethyl-(9-(difluoromethyl)perfluorononyl)methanaminium","","D",0]
["2-Fluoro-3-[(2-fluorobenzoyl)-methylamino]-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-iodo-6-(trifluoromethyl)phenyl]benzamide","","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluorododecanesulfonyl)amino]propan-1-aminium","","D",0]
["2-Chloro-perfluoropentanoic acid","","D",0]
["(7E)-Pentacosafluorotridec-7-ene-1-sulfonic acid","","D",0]
["(9-Pentafluoro(5)sulfide)-perfluorononanoic acid","","D",0]
["(7E)-tricosafluorododec-7-ene-1-sulfonic acid","","D",0]
["2H-Perfluorododecanoic acid","","D",0]
["(E)-5-((Perfluorobut-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluoropropanesulfonyl)amino]propan-1-aminium","","D",0]
["2H-Perfluorohexadecanoic acid","","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluorooctanesulfonyl)amino]propan-1-aminium","","D",0]
["(E)-4-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctoxy)-4-oxobut-2-enoic aci","","D",0]
["(2Z)-3-Fluoro-3-(perfluoropentyl)prop-2-ene-1-sulfonic acid","","D",0]
["N,N,N-Trimethyl-(2-(difluoromethyl)perfluoroethyl)methanaminium","","D",0]
["2-Chloro-1,1,3,4,4,5,6,6,6-nonafluorohex-1-ene","","D",0]
["N,N,N-Trimethyl-(13-(difluoromethyl)perfluorotridecyl)methanaminium","","D",0]
["2-Chloro-5-[4-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]pyrazol-1-yl]pyridine-3-carboxylic acid","","D",0]
["N,N,N-Trimethyl-(4-(difluoromethyl)perfluorobutyl)methanaminium","","D",0]
["(3E)-Perfluoropent-3-ene-1-sulfonic acid","","D",0]
["(3,3,4,4,5,5,5-Heptafluoro-pentane-1-sulfonyl)-acetonitrile","","D",0]
["2-Chloro-N-[3-[[2,6-dibromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)phenyl]carbamoyl]-2-fluorophenyl]-N-methylpyridine-3-carboxamide","","D",0]
["(4-((1,1,2,2,3,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoro-3-nonen-1-yl)oxy)benzyl)phosphonic acid","","D",0]
["2-Chloro-1,1,3,4,4,5,5,6,6,8-decafluorooct-1-ene","","D",0]
["(4-Ethyl-1,1,1,2,2-pentafluoroheptan-4-yl) phosphate","","D",0]
["(4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononyl)oxy)benzyl)phosphonic acid","","D",0]
["N,N,N-Trimethyl-(8-(difluoromethyl)perfluorooctyl)methanaminium","","D",0]
["(4-Ethenylphenyl) 1,1,2,2,3,3,3-heptafluoropropane-1-sulfonate","","D",0]
["2-Chloro-N-[3-[[2-iodo-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)-6-(trifluoromethyl)phenyl]carbamoyl]phenyl]-N-methylpyridine-3-carboxamide","","D",0]
["(4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,15,15,16,16,17,17,18,18,19,19,20,20,21,21,21-Heptatriacontafluoro-2-hydroxyhenicosyl)trimethylazanium","","D",0]
["N,N,N-Trimethyl-(7-(difluoromethyl)perfluoroheptyl)methanaminium","","D",0]
["N-(3-{[(Perfluorooctyl)sulfonyl]amino}propyl)-3,4-dihydroxy-N,N-dimethyl-1-butanaminium","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorooctadecyl)-2-hydroxypropyl]azanium","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorohexyl)-2-hydroxypropyl]azanium","","D",0]
["N-(3-{[(Perfluorodecyl)sulfonyl]amino}propyl)-3,4-dihydroxy-N,N-dimethyl-1-butanaminium","","D",0]
["2-Amino-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)phenol","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorotetradecyl)-2-hydroxypropyl]azanium","","D",0]
["2-Bromo-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-1-methyl-3-(trifluoromethyl)benzene","","D",0]
["(2-Carboxyethyl)dimethyl[3-(perfluorooctyl)-2-hydroxypropyl]azanium","","D",0]
["N-(Methylethylcarboxymethyl) dimethyl ammonio propyl perfluoropentane amide","","D",0]
["2-Bromo-1-chloro-5-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(trifluoromethoxy)benzene","","D",0]
["2-Chloro-1,1,3,3,4,4,5,6,6,7,8,8,8-tridecafluorooct-1-ene","","D",0]
["N,N,N-Trimethyl-(10-(difluoromethyl)perfluorodecyl)methanaminium","","D",0]
["(2R)-1,1,1-Trifluoro-3-[N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]-3-[3-(trifluoromethoxy)phenoxy]anilino]propan-2-ol","","D",0]
["(2R)-1,1,1-Trifluoro-3-[N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]-3-[[3-(trifluoromethoxy)phenyl]methoxy]anilino]propan-2-ol","","D",0]
["N,N,N-Trimethyl-((difluoromethyl)difluoromethyl)methanaminium","","D",0]
["2-Chloro-1,1,3,4,4,5,6,6,6-nonafluoro-5-(trifluoromethyl)hex-1-ene","","D",0]
["N,N,N-Trimethyl-(12-(difluoromethyl)perfluorododecyl)methanaminium","","D",0]
["N,N,N-Trimethyl-(6-(difluoromethyl)perfluorohexyl)methanaminium","","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorononane-1-sulfonamide","","D",0]
["N-[3-[[2-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)phenyl]carbamoyl]-6-cyano-2-fluorophenyl]-6-chloropyridine-3-carboxamide","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluoroundecyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(Perfluoroethyl)methane-1-sulfonic acid","","D",0]
["N-[3-[[2,6-Dibromo-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)phenyl]carbamoyl]phenyl]-2-fluorobenzamide","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluoropentyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["N-[3-[[2-Bromo-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)-6-(trifluoromethyl)phenyl]carbamoyl]-2-fluorophenyl]-6-chloropyridine-3-carboxamide","","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluorododecyl)sulfonyl]amino}-1-propanaminium","","D",0]
["(Perfluorononyl)methane-1-sulfonic acid","","D",0]
["N-[3-[[2-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)phenyl]carbamoyl]phenyl]-2-fluorobenzamide","","D",0]
["2-Hydroxy-4-methyl-N-(1-oxo-3H-2-benzofuran-5-yl)-2-(1,1,2,2,2-pentafluoroethyl)-4-phenylpentanamide","","D",0]
["N-[3-[[2-Bromo-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)-6-(trifluoromethyl)phenyl]carbamoyl]phenyl]-6-chloro-N-methylpyridine-3-carboxamide","","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluoroheptyl)sulfonyl]amino}-1-propanaminium","","D",0]
["(Perfluoropropanamido)-3-betaine","","D",0]
["N-[3-[[2-Bromo-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)-6-(trifluoromethyl)phenyl]carbamoyl]phenyl]-3-cyano-N-methylbenzamide","","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluoroethyl)sulfonyl]amino}-1-propanaminium","","D",0]
["(Perfluoroundecyl)methane-1-sulfonic acid","","D",0]
["N-Butyl-N,N-dimethyl-(11-(difluoromethyl)perfluoroundecyl)methan-1-aminium","","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluoroundecyl)sulfonyl]amino}-1-propanaminium","","D",0]
["(Perfluorotridecyl)methane-1-sulfonic acid","","D",0]
["N-Butyl-N,N-dimethyl-((difluoromethyl)difluoromethyl)methan-1-aminium","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluorodecyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(E)-Perfluoroundec-9-ene-1-sulfonic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorotetradecanamide","","D",0]
["2-Chloro-N-[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]-3-nitrobenzamide","","D",0]
["(2R)-3-[3-(5-Bromo-2-fluorophenoxy)-N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]anilino]-1,1,1-trifluoropropan-2-ol","","D",0]
["2-Hydroxy-3-oxo-3-[(4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-pentadecafluorodecanoyl)sulfanyl]propanoic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorodecane-1-sulfonamide","","D",0]
["(E)-Perfluorohex-4-ene-1-sulfonic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorododecane-1-sulfonamide","","D",0]
["N-[3-(dimethylamino)propyl]-perfluoroethane-1-sulfonamide","","D",0]
["(E)-Perfluorooct-6-ene-1-sulfonic acid","","D",0]
["2-Hydroxy-N-(2-hydroxyethyl)-N,N-dimethyl-3-{[(perfluorononyl)sulfonyl]amino}-1-propanaminium","","D",0]
["(Perfluorobutyl)methane-1-sulfonic acid","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluorohexyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-perfluorotetradecane-1-sulfonamide","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluorododecyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(Perfluorododecyl)methane-1-sulfonic acid","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluorooctyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(Perfluorodecyl)methane-1-sulfonic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-perfluoroundecane-1-sulfonamide","","D",0]
["2-Hydroxy-3-oxo-3-[[3-(perfluorononyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(E)-Perfluoro-2-propeneoxyacetic acid","","D",0]
["N-[2,6-Dibromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)phenyl]-2-fluoro-3-nitrobenzamide","","D",0]
["2-Hydroxy-3-[[3-(perfluorobutyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorotetradecanamido)propan-1-aminium","","D",0]
["2-Hydroxy-3-[[3-(perfluoroheptyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(E)-Perfluoro-2-undec-7-eneoxyacetic acid","","D",0]
["N-[2-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)phenyl]-2-fluoro-3-nitrobenzamide","","D",0]
["(E)-Perfluorotridec-11-ene-1-sulfonic acid","","D",0]
["3,3,4,4,4-Pentafluoro-2-hydroxy-2-(2-methylphenyl)butanoic acid","91935-84-1","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluorohexyl)sulfonyl]amino}propyl)-1-butanaminium","2089109-95-3","D",0]
["N-(3,4-Dichlorophenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","106376-37-8","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,6-Tridecafluoro-1-(pentafluoroethoxy)hexane","133080-89-4","D",0]
["(2,5-Dimethoxy-4-methylphenyl)methyl heptafluorobutanoate","87461-70-9","D",0]
["3-[[(Perfluorohexyl)sulfonyl]-N-methylamino]-N,N,N-trimethyl-1-propanaminium iodide (1:1)","71216-13-2","D",0]
["(2E)-4,4,5,5,6,6,6-Heptafluorohex-2-enoic acid","37759-76-5","D",0]
["1,1,1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Icosafluoro-12-iodo-2-(trifluoromethyl)dodecane","242142-80-9","D",0]
["3,3,4,4-tetrafluoro-1,2-dipropylcyclobutene","711-60-4","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecyl N-[3-(2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecoxycarbonylamino)-4-methylphenyl]carbamate","15953-41-0","D",0]
["Perfluoropentadecane","2264-03-1","D",0]
["Propan-2-yl 3-{[(1,1,1,3,3,3-hexafluoropropan-2-ylidene)amino]oxy}propanoate","74387-56-7","D",0]
["Nonafluorobutan-1-amine","74753-16-5","D",0]
["Difluoro(trifluoromethoxy)acetic acid--piperazine (1/1)","2266-82-2","D",0]
["[4-[3-(4-acetyloxyphenyl)-1,1,2,2,3,3-hexafluoropropyl]phenyl] acetate","21250-00-0","D",0]
["2,3-Difluoro-2-(nonafluorobutyl)oxirane","1350637-06-7","D",0]
["1‐(Dimethylamino)‐3-(perfluorobutyl)‐2‐(hydroxymethoxy)propan‐3‐yl formate","","D",0]
["{3-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]propyl}(trimethoxy)silane","64743-69-7","D",0]
["2‐(Difluoromethoxy)‐1,1,1,2,3,3‐hexafluoropropane","233258-12-3","D",0]
["7-(Bis((2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl)oxy)methoxy)-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluoroheptane","866-03-5","D",0]
["Trichloro[3-[(2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-pentadecafluorooctyl)oxy]propyl]silane","755-08-8","D",0]
["Hexadecafluorooxonane","1978-24-1","D",0]
["3,3,4,4,5,5,5-Heptafluoropentyl 2-methylprop-2-enoate","2145-81-5","D",0]
["Perfluoro-11-methoxyundecane-1-sulfonic acid","","D",0]
["1,1,1,4,4,5,5,6,6,7,7,8,8,9,9,9-Hexadecafluoro-2-nonene","935477-01-3","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorododecan-5-ol","131294-52-5","D",0]
["1-(2-Bromo-1,1,1,3,3,3-hexafluoropropan-2-yl)-2-methoxybenzene","70430-22-7","D",0]
["2-Hydroxy-3-[(perfluorohexyl)ethoxy]propyl triacontanoate","141267-36-9","D",0]
["2-(1,1,1,3,3,3-hexafluoro-2-hydroxypropan-2-yl)-1-(4-methoxyphenyl)pentan-1-one","34844-29-6","D",0]
["1H,2H,2H-perfluorooctanal (2,4-dinitrophenyl)hydrazone","128917-19-1","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Heptadecafluoro-2-undecen-1-ol","2340-84-3","D",0]
["2-Chloro-4-(1,1,2,2-tetrafluoroethoxy)phenol","88553-91-7","D",0]
["Phosphonic acid, P-[3,4,4,4-tetrafluoro-3-[1,1,2,3,3,3-hexafluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)propoxy]butyl]-","1198297-65-2","D",0]
["(2S)-2-Pyrrolidinyl-bis(4-(perfluorohexyl)phenyl)methanol","1075687-38-5","D",0]
["3,3,4,4,4-Pentafluoro-1-[(R)-4-methylbenzene-1-sulfinyl]butan-2-one","167010-73-3","D",0]
["1,1-Difluoro-5,5-dimethyl-1-(trifluoromethoxy)hexane-2,4-dione","61894-06-2","D",0]
["3-Amino-4,4,5,5,6,6,6-heptafluorohexanoic acid","150618-42-1","D",0]
["Chloro(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)bis(3,3,3-trifluoropropyl)silane","608296-98-6","D",0]
["1-Propanaminium, 2-[[(heptadecafluorooctyl)sulfonyl]amino]-N,N,N-trimethyl-, iodide","75033-26-0","D",0]
["Potassium 9-chlorohexadecafluoro-3-oxanonane-1-sulfonate","73606-19-6","D",0]
["5‐[3‐({[(3,3,4,4,4‐Pentafluorobutyl)sulfanyl]carbonyl}amino)propanamido]pentanoic acid","","D",0]
["1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Hexadecafluoro-1-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]-8-iodooctane","25080-19-7","D",0]
["1,1‐Dichloro‐2‐(difluoromethoxy)‐1,2,2‐trifluoroethane","32778-14-6","D",0]
["12:2 Fluorotelomer sulfonic acid","149246-64-0","D",0]
["N-(3-Chloro-4-methylphenyl)-2,2,3,3,4,4,4-heptafluorobutanamide","111216-49-0","D",0]
["N,N-Dimethyl-N-[3-[methyl[(perfluorohexyl)sulfonyl]amino]propyl]-3-sulfo-1-propanaminium","2089109-78-2","D",0]
["alpha,alpha'-(2,2-Dimethyl-1,3-propanediyl)bis[omega-hydroxy-poly[oxy[2-methyl-2-[(2,2,3,3,3-pentafluoropropoxy)methyl]-1,3-propanediyl]]","449177-99-5","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol","161308-22-1","D",0]
["2-Propanol, 1,1'-[(3,3,4,4,5,5,6,6,6-nonafluorohexyl)imino]bis[3-chloro-","194735-07-4","D",0]
["4,5,5,5-Tetrafluoro-2-(trifluoromethyl)penta-1,3-diene","90278-03-8","D",0]
["2‐Hydroxy‐3‐oxo‐3‐[(4,4,5,5,5‐pentafluoropentanoyl)sulfanyl]propanoic acid","","D",0]
["6‐({[(Perfluorododecyl)thioethyl]carbonyl}amino)hexanal","","D",0]
["(Carboxymethyl)dimethyl[3‐(perfluorobutanesulfonamido)propyl]azanium","2089109-22-6","D",0]
["ethyl 4-chloro-2,2,3,3,4,4-hexafluorobutanoate","6395-45-5","D",0]
["3‐(3,3,4,4,4‐Pentafluorobutanesulfonyl)propanoic acid","","D",0]
["2-(2,2,3,3,4,4,4-Heptafluorobutyl)butanedioic acid","121223-84-5","D",0]
["6,6,6-Trifluoro-5-hydroxy-2,2-dimethyl-5-(trifluoromethyl)hexan-3-yl acetate","101914-05-0","D",0]
["N-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-sulfonyl)cyclopentanecarboxamide","1440968-21-7","D",0]
["4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononyl)oxy)benzoic acid","","D",0]
["(5E)-7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-Heptadecafluorotetradec-5-ene","210491-04-6","D",0]
["Ethylammonium perfluoro-8-(trifluoromethyl)nonanoate","65419-00-3","D",0]
["N~1~,N~1~,N~7~,N~7~-Tetraethyl-2,2,3,3,4,4,5,5,6-nonafluoroheptanediamide","60934-65-8","D",0]
["Perfluoro-3-butoxypropanoic acid","376-62-5","D",0]
["1-Decanol-1,2-13C2, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-heptadecafluoro-, dihydrogen phosphate, sodium salt (1:1)","","D",0]
["3-(1,1,1,3,3,3-Hexafluoro-2-hydroxypropan-2-yl)bicyclo[2.2.1]heptan-2-one","35444-15-6","D",0]
["2,2,3,3-Tetrafluoro-3-methoxypropanenitrile","77946-88-4","D",0]
["9-Iodoperfluoro-3-oxanonanesulfonyl fluoride","67990-77-6","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-3-[(perfluoro-1-oxoheptyl)amino]propanaminium chloride","89375-44-0","D",0]
["N-Methyl-3-(4,4,5,5,5-pentafluoropentylsulfanyl)-N-[2-[4-(6-phenyl-8,9-dihydro-7H-benzo[7]annulen-5-yl)phenoxy]ethyl]propan-1-amine","","D",0]
["Perfluoro[2-(2-methoxypropoxy)propanoyl] fluoride","2479-75-6","D",0]
["4-(Perfluorohexyl)butyric acid","26564-97-6","D",0]
["2‐Hydroxy‐3‐[[3-(perfluoroundecyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["2,4-Difluoro-N-(2-fluoro-3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)-N-methylbenzamide","862134-26-7","D",0]
["Perfluoro-5-(undecafluoropentyl)cyclohexanesulfonic acid","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluorooctyl 2-methyl-2-propenoate polymer with oxiranylmethyl 2-methyl-2-propenoate, 2-hydroxyethyl 2-methyl-2-propenoate, octadecyl 2-propenoate and 1,1-dichloroethene","1360463-21-3","D",0]
["2,2,3,3,4,4,5,5,5-Nonafluoro-N-(4-nitrophenyl)pentanamide","150333-62-3","D",0]
["1-Butanesulfonamide, 1,1,2,2,3,3,4,4,4-nonafluoro-N-[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)sulfonyl]-, ammonium salt (1:1)","129318-48-5","D",0]
["Copolymer of chlorotrifluoroethylene/ethylene/tetrafluoroethylene (a number-average molecular weight is not less than 1,000 and the polymer is insoluble in water, lipid soluble\nsolvent, usual solvent, acid and alkali)","40905-85-9","D",0]
["N,N-Diethyl-2,2,3,3,4,4,5,5,5-nonafluoropentanamide","158018-94-1","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-Pentacosafluorotetradecyl)phosphonic acid","147290-12-8","D",0]
["6:2 Fluorotelemer [13C2] carboxylic acid","872398-75-9","D",0]
["Disulfide, bis(pentafluoroethyl)","679-77-6","D",0]
["4-{4-[(2,2,3,3,3-Pentafluoropropyl)amino]butyl}benzene-1,2-diol","646520-32-3","D",0]
["2-Chloro-4-fluoro-N-(2-fluoro-3-{[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2,6-dimethylphenyl]carbamoyl}phenyl)-N-methylbenzamide","862134-29-0","D",0]
["HFE-338pcc13","188690-78-0","D",0]
["bis(2,2,3,3,4,4,5,5-octafluoropentyl) sulfate","755-37-3","D",0]
["5,5,6,6,7,7,8,8,8-Nonafluoro-3-iodooctan-1-ol","109574-81-4","D",0]
["4-[(Pentadecafluoroheptyl)oxy]benzoic acid","75895-47-5","D",0]
["14:2 Fluorotelomer sulfonamide","","D",0]
["2-[(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)oxy]-N-phenylacetamide","62656-67-1","D",0]
["3-[[(Perfluorooctyl)sulfonyl]propylamino]-N,N,N-trimethyl-1-propanaminium iodide","84242-84-2","D",0]
["Cyclohexanecarboxamide, 1,2,2,3,3,4,4,5,5,6,6-undecafluoro-N-[4-(2-phenyldiazenyl)phenyl]-","545339-93-3","D",0]
["1-[(2-Chloroethyl)sulfanyl]-1,1,2,2,2-pentafluoroethane","679-75-4","D",0]
["1,1,1,3,5,7-Hexachloro-2,2,3,4,4,5,6,6,7-nonafluoro-7-iodoheptane","88639-54-7","D",0]
["Acetic acid, 2,2-bis[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]-, ethyl ester","133707-86-5","D",0]
["Urea, N-[4-(2-phenyldiazenyl)phenyl]-N'-[2,2,2-trifluoro-1-methyl-1-(trifluoromethyl)ethyl]-","339359-83-0","D",0]
["Ammonium 2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11-icosafluoroundecanoate","5081-02-7","D",0]
["Methyl perfluoropropylketone","60249-67-4","D",0]
["2,2-Bis(trifluoromethyl)propanol","2927-17-5","D",0]
["1,1,2,2,3,3-Hexafluoropropane","680-00-2","D",0]
["Ether, octyl 1,1,2,2-tetrafluoroethyl","30719-68-7","D",0]
["Methyl 4,4,5,5,6,6,6-heptafluoro-3-oxohexanoate","89129-68-0","D",0]
["2,2-Dichloro-perfluoro-1-tridecanesulfonic acid","","D",0]
["1-Chloro-2-iodotetrafluoroethane","421-78-3","D",0]
["N-Bromo-N-(pentafluoroethyl)hypobromous amide (non-preferred name)","83696-32-6","D",0]
["1,3-Bis(pentafluoroethoxy)benzene","34065-75-3","D",0]
["[(Tridecafluorohexyl)sulfanyl]benzene","69127-72-6","D",0]
["1,1,1,2,3,3-Hexafluoro-3-iodopropane","431-90-3","D",0]
["N-Ethyl-N-(heptafluoropropyl)-2-hydroxyethane-1-sulfonamide","113366-08-8","D",0]
["Methyl 4-(tridecafluorohexyl)cyclohexane-1-carboxylate","88951-16-0","D",0]
["1,1,1,3,3,3-Hexafluoro-2-{[1,1,1,3,3,3-hexafluoro-2-(trifluoromethyl)propan-2-yl]peroxy}-2-(trifluoromethyl)propane","26842-85-3","D",0]
["1-[3,5-Bis(heptafluoropropyl)-1H-pyrazol-1-yl]ethan-1-one","231630-85-6","D",0]
["2,2,3-Trifluoro-3-(heptafluoropropoxy)propan-1-ol","73320-57-7","D",0]
["1,2-Dibromo-1,1,2,3,3,4,4,4-octafluorobutane","","D",0]
["1-Methyl-2-nitro-4-(pentafluoroethyl)benzene","134302-31-1","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1-[[2,3-bis[(2-fluoro-1-oxo-2-propen-1-yl)oxy]propoxy]methyl]-1,2,2,2-tetrafluoroethyl]-.omega.-[(1,1,2,3,3-pentafluoro-2-propen-1-yl)oxy]-","1276043-56-1","D",0]
["2,2,3,3-Tetrafluoro-N-[(1-methyl-1H-pyrazol-4-yl)methyl]propan-1-amine","1695269-46-5","D",0]
["Methyl 4-(tridecafluorohexyl)benzoate","88951-02-4","D",0]
["1-Bromo-4-(heptadecafluorooctyl)benzene","206560-77-2","D",0]
["1-Ethoxy-2,3,3,4,4,5,5,6,6-nonafluorocyclohex-1-ene","2251-83-4","D",0]
["(3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-pentadecafluorononyl)phosphonic acid","23068-11-3","D",0]
["2-Ethyl-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-3-(2-methylpropane-1-sulfinyl)benzoic acid","1355554-99-2","D",0]
["Hexafluoropropene, oxidized, oligomers, reduced, reaction products with methanol, reduced","161075-15-6","D",0]
["3,3,4,4,5,5,5-Heptafluoro-1-phenylpentan-2-one","559-96-6","D",0]
["Perfluoro-9-undecene-1-sulfonic acid","2089109-46-4","D",0]
["1,1,1,2,3,3-Hexafluoro-4-methylpentane","53072-71-2","D",0]
["4-Bromo-3-(heptafluoropropyl)-5-methyl-1H-pyrazole","82633-48-5","D",0]
["Methyl bis(2,2,3,3-tetrafluoropropyl) phosphate","67710-52-5","D",0]
["2-Aminohexafluoropropan-2-ol","31253-34-6","D",0]
["Perfluoro-5-(heptafluoropropyl)cyclohexanesulfonate","","D",0]
["N-(2-Hydroxyethyl)-N-methyl-3-[(perfluorooctanesulfonyl)amino]-N-(3-sulfopropyl)propan-1-aminium","","D",0]
["14:2 fluorotelomer sulfide (1-methanol 2-methanol) propanoate","","D",0]
["3-(1,1,2,2,3,3,3-Heptafluoropropane-1-sulfonyl)benzoic acid","88489-79-6","D",0]
["1-(4,4,5,5,5-Pentafluoropentyl)thiolan-1-ium chloride","821767-13-9","D",0]
["3-[[(Perfluoroheptyl)sulfonyl]methylamino]-N,N,N-trimethyl-1-propanaminium","2089109-13-5","D",0]
["(4Z)-1,1,1,2,2,3,3,4-Octafluoro-4-decene","90292-32-3","D",0]
["2,2-bis(3-nitro-4-hydroxyphenyl)hexafluoropropane","73340-33-7","D",0]
["3-(Nonafluoro-1-butyl)-5-(methyl)pyrazole","247220-81-1","D",0]
["1-Iodo-4-[perfluoro-1-(trifluoromethyl)ethyl]benzene","40161-59-9","D",0]
["(1Z)-3,4,4,4-Tetrafluoro-1-iodo-3-(trifluoromethyl)-1-butene","24716-85-6","D",0]
["1,2-Dibromo-1,1,2,3,3-pentafluoro-3-(trifluoromethoxy)propane","885275-98-9","D",0]
["Acetic acid, 2,2,2-Trifluoro-, 3,3,4,4,5,5,6,6,6-nonafluorohexyl ester","1980039-82-4","D",0]
["5,6,6,6-Tetrafluoro-4-sulfanylhex-3-en-2-one","116509-66-1","D",0]
["2,2,3,4,4,6,6,7,7,9,9,11,11,13,13,15,15,15-Octadecafluoro-5,8,10,12,14-pentaoxapentadecanoic acid","919005-30-4","D",0]
["{2‐Hydroxy‐3‐[2-(perfluorododecyl)ethylsulfanyl]propyl}trimethylazanium","","D",0]
["2-[3-(2,2,3,3,3-Pentafluoropropoxy)pyridin-4-yl]-5-(trifluoromethyl)benzoxazole","","D",0]
["Bis(2,2,3,3,4,4,4-heptafluorobutyl) carbonate","1026739-75-2","D",0]
["3-(Perfluoropropyl)-2-iodopropanol acetate","3108-05-2","D",0]
["Ethyl 2,2,3,3-tetrafluoropropanoate","337-82-6","D",0]
["4,4'-(1,1,2,2,3,3-Hexafluoropropane-1,3-diyl)bis(2-nitrophenol)","57558-14-2","D",0]
["1-bromo-3,3,3-trifluoro-2-(trifluoromethyl)prop-1-ene","382-15-0","D",0]
["1,1,3,3,4,4,5,5,5-Nonafluoro-1-pentene","","D",0]
["3-(Pentafluoroethoxy)pyrrolidine","1208078-44-7","D",0]
["4-Cyanophenyl 4-(nonafluorobutyl)benzoate","79049-17-5","D",0]
["3-(3,3,4,4,4-Pentafluorobutylsulfanyl)propanoic acid","","D",0]
["2‐[(2-(1-Hydrido-perfluorohexadecyl)ethyl)dimethylazaniumyl]acetate","","D",0]
["Methyl 2,3,3,3-tetrafluoro-2-[(1,1,2-trifluoro-2-propen-1-yl)oxy]-propanoate","174082-79-2","D",0]
["2-Phenyl-4,4,5,5-tetrakis(trifluoromethyl)-1,3,2-dioxaborolane","23542-71-4","D",0]
["1,1,1,3,4,4,5,5,6,6,7,7,7-Tridecafluorohept-2-ene","","D",0]
["2,2,3,3,6,6,7,7,8,8,9,9-Dodecafluoro-1,4-dioxaspiro[4.4]nonane","87901-77-7","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluoroheptyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["3-[3-(3-Cyclopropylphenoxy)-N-[[3-(1,1,2,2,3,3,3-heptafluoropropyl)phenyl]methyl]anilino]-1,1,1-trifluoropropan-2-ol","","D",0]
["Ammonium 2H,2H-perfluoroheptylate","1637546-16-7","D",0]
["2,2,3,3,4,4,4-Heptafluoro-N-(1H-1,2,4-triazol-5-yl)butanamide","70501-47-2","D",0]
["3-Benzamido-N-[2-bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)phenyl]-2-fluorobenzamide","","D",0]
["[S-(1,1,2,2,3,3,4,4,4-Nonafluorobutane-1-)sulfonimidoyl]benzene","1335014-68-0","D",0]
["2,3,3,3-Tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanamide","60308-67-0","D",0]
["4-(Azidomethyl)-2,2-bis(trifluoromethyl)-1,3-dioxolane","51125-51-0","D",0]
["Butyl hydrogen (2-{4-[(3,4-dimethyl-1,2-oxazol-5-yl)sulfamoyl]anilino}-1,1,1,3,3,3-hexafluoropropan-2-yl)carbonimidate","5226-12-0","D",0]
["3-Butyl-1-((perfluorohexyl)eth-2-yl)-1H-imidazol-3-ium hexafluorophosphate","313475-52-4","D",0]
["N,N,N-Trimethyl-(3-(difluoromethyl)perfluoropropyl)methanaminium","","D",0]
["N-Ethyl-3-{ethyl[(perfluorobutyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["Trimethylsilyl perfluorobutanesulfonate","68734-62-3","D",0]
["3,6-Dihydro-8-(1-methylethyl)-1,3,6-trioxo[1]benzothiopyrano[2,3-e]isoindol-2-yl perfluorobutanesulfonate","639827-06-8","D",0]
["2-(Perfluorodecyl)ethyl N-1-naphthalenylcarbamate","305849-27-8","D",0]
["2,2,3,3-Tetrafluoro-3-(trifluoromethoxy)propanenitrile","22325-74-2","D",0]
["1,1,2,2-Tetrafluoro-2-(1,1,2,2-tetrafluoroethoxy)ethane-1-sulfonyl chloride","88239-68-3","D",0]
["N,N-dimethyl-2-[(perfluorododecanoyl)amino]ethan-1-amine N-oxide","200636-70-0","D",0]
["Benzyl 2,3,3,3-tetrafluoro-2-[1,1,2,3,3,3-hexafluoro-2-(heptafluoropropoxy)propoxy]propanoate","140229-81-8","D",0]
["4-Heptanone, 7-chloro-2-hydroxy-1,1,1-trifluoro-2-trifluoromethyl-","101913-91-1","D",0]
["1,1',1''-(1,3,5-Triazinane-1,3,5-triyl)tris(2,3,3,3-tetrafluoropropan-1-one)","64498-32-4","D",0]
["N,N'-Bis[2-(1,1,2,2-tetrafluoro-2-phenylethyl)phenyl]urea","61547-75-9","D",0]
["Trimethyl[(2,2,3,3,4,4,5,5,5-nonafluoropentyl)oxy]silane","89660-60-6","D",0]
["Perfluoro-3,5,7-trioxaoctanoic acid","39492-89-2","D",0]
["7:2 Fluorotelomer ketone sulfonate","","D",0]
["N,N,N-Tripropylpentan-1-aminium heptadecafluorooctane-1-sulfonate","56773-56-9","D",0]
["5,5,6,6,7,7,8,8,8-Nonafluoro-2-methyloct-3-yn-2-ol","82721-68-4","D",0]
["4-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Nonadecafluoro-1-decen-1-yl)oxy]benzenesulfonic acid","","D",0]
["2-Methyl-4-(1,1,2,2-tetrafluoroethylsulfanyl)aniline","100280-15-7","D",0]
["14-H-Perfluorotetradecanoate","1696259-81-0","D",0]
["4,4,5,5,6,6,6-Heptafluoro-3-oxohexanoic acid","824424-65-9","D",0]
["2-(6-Chloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexyl)-1H-pyrrole","110396-63-9","D",0]
["2-Propenoic acid, 2-fluoro-, tetrafluoropropyl ester, homopolymer","99106-55-5","D",0]
["14:2 Fluorotelomer sulfonamido propyl methyl amino acetic acid","","D",0]
["3H-Perfluorobutanoic acid","379-90-8","D",0]
["3,3-bis(2,2,3,3,4,4,5,5-octafluoropentoxymethyl)oxetane","60176-94-5","D",0]
["1,1,1,2,2,3,3-Heptafluoro-5-iododecane","755-49-7","D",0]
["N-{[2,2,5,5-Tetrakis(trifluoromethyl)-1,3-oxazolidin-4-yl]carbonyl}glycine","36871-69-9","D",0]
["2-Cyanophenyl nonafluorobutane-1-sulfonate","873838-37-0","D",0]
["1-bromo-1,1,2,2-tetrafluoropentane","151831-44-6","D",0]
["1,1'-(2,3,3,3-Tetrafluoroprop-1-ene-1,1-diyl)dibenzene","1493-86-3","D",0]
["1H,2H-Perfluoropentane","150999-42-1","D",0]
["4-(Undecafluoropentyl)cyclohexane-1-carboxylic acid","88951-26-2","D",0]
["1,10-Diazido-3,3,4,4,5,5,6,6,7,7,8,8-dodecafluorodecane","132833-44-4","D",0]
["6:2 fluorotelomer dimethyl ethyl betaine","","D",0]
["Methyl 4-(undecafluoropentyl)cyclohexane-1-carboxylate","88951-15-9","D",0]
["5-(Heptafluoropropyl)uridine","144862-38-4","D",0]
["2-Chloro-1,1,2,2-tetrafluoroethyl sulfurofluoridate","649-61-6","D",0]
["2,2,3,3,4,4,5,5-Octafluoropentyl hypochlorite","76453-04-8","D",0]
["1H,1H,8H-Perfluoro-1-octanol","10331-08-5","D",0]
["1,1,2-Trifluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy)ethanesulfonate","","D",0]
["1,1,1,3,3,3-Hexafluoro-2-[(fluoromethoxy)methoxy]propane","194039-91-3","D",0]
["1,1,1,3,3,3-Hexafluoro-2,2-dimethoxypropane","754-50-7","D",0]
["6,6,7,7,8,8,8-Heptafluoro-2,2-dimethyl-3,5-octanedione - iron (3:1)","30304-08-6","D",0]
["methyl 5-chloro-2,2,3,3,4,4,5,5-octafluoropentanoate","261503-67-7","D",0]
["Perfluorobutyltetrahydrofuran","25962-44-1","D",0]
["Perfluoro-3,6-dioxaheptanoic acid","151772-58-6","D",0]
["1,1,4,4,5,5,5-Heptafluoro-2-methylpent-1-ene","90277-99-9","D",0]
["(1,1,2,2-Tetrafluoroethane-1,2-diyl)bis(phenylphosphane)","63878-93-3","D",0]
["Perfluorodecahydro-1-t-butylnaphthalene","118914-94-6","D",0]
["Dichloro(1,1,2,3,3,3-hexafluoropropyl)methylsilane","664-13-1","D",0]
["2-Chloro-N-(1-cyanocyclopropyl)-5-(1'-methyl-3'-(1,1,2,2,2-pentafluoroethyl)-4'-(trifluoromethyl)(1,5'-bi-1H-pyrazol)-4-yl)benzamide","1621436-41-6","D",0]
["1,1,2,3,3-Pentafluoro-2-methoxypropane","672295-90-8","D",0]
["(1s,4s)-4-(Nonafluorobutyl)cyclohexane-1-carboxamide","88951-20-6","D",0]
["10-(2,2,3,3,4,4,5,5,5-Nonafluoropentyl)octacosanoyl chloride","185033-98-1","D",0]
["Perfluorotriethylcarbinol","6189-00-0","D",0]
["1-Dodecanol, 7,7,8,8,9,9,10,10,11,11,12,12,12-tridecafluoro-5-iodo-","177722-97-3","D",0]
["1,3-Benzenedicarboxamide, N3-[2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]methylamino]ethyl]-N1-[2-[[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propylamino]ethyl]-4-methyl-","73019-20-2","D",0]
["2-[2,3,3,3-Tetrafluoro-2-(trifluoromethyl)propanoyl]benzoic acid","62656-73-9","D",0]
["Perfluoro-3-ethylcyclopentane-1-sulfonic acid","","D",0]
["2,2,3,3,3-Pentafluoro-N-(2,2,3,3,3-pentafluoro-1-hydroxypropylidene)propanehydrazonic acid","755-76-0","D",0]
["Dimethyl-di(propan-2-yl)azanium;1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","374571-81-0","D",0]
["5-(4,4,5,5,5-Pentafluoro-3-oxopentanoyl)thiophene-2-carbonitrile","591727-04-7","D",0]
["3-(3,5-Dimethyl-1H-pyrazol-1-yl)-2,2,3,3-tetrafluoropropanoic acid","1125519-39-2","D",0]
["4-[(4,4,5,5,6,6,6-heptafluoro-2-nitrohexan-3-yl)amino]benzoic acid","564-96-5","D",0]
["Glycine, N-[(heptadecafluoroctyl)sulfonyl]-, monopotassium salt","75260-69-4","D",0]
["2-(5-Chloro-1,1,2,2,3,3,4,4,5,5-decafluoropentyl)-7-methyl-4H-1-benzopyran-4-one","155445-01-5","D",0]
["(4E)-4-[[2-(1,1,1,3,3,3-Hexafluoropropan-2-yl)-4-(hexafluoropropan-2-ylidene)-1,3-dithietan-2-yl]-[4-(hexafluoropropan-2-ylidene)-2-methyl-1,3-dithietan-2-yl]methylidene]-6-(hexafluoropropan-2-ylidene)-1-methyl-2,3,7-trithiabicyclo[3.2.0]heptane","66172-15-4","D",0]
["2,2,3,3-Tetrafluorobutanoic acid","917951-61-2","D",0]
["2,5-Dimethoxyphenyl heptafluorobutanoate","87461-68-5","D",0]
["1,1,1,4,4,4-Hexafluoro-2,3-bis(trifluoromethyl)but-2-ene","360-57-6","D",0]
["5-(2,3,3,3-Tetrafluoropropyl)-2,4(1H,3H)-pyrimidinedione","53489-95-5","D",0]
["Undecafluoropentan-1-amine","134380-80-6","D",0]
["4-(Tridecafluorohexyl)cyclohexane-1-carboxylic acid","88951-27-3","D",0]
["1,2,2,2-Tetrafluoroethyl formate","481631-19-0","D",0]
["2,2-difluoro-2-[1,1,2,2-tetrafluoro-2-(trifluoromethoxy)ethoxy]acetyl Chloride","261503-81-5","D",0]
["[(1,1,1,3,3,3-Hexafluoropropan-2-yl)oxy](trimethyl)silane","4071-95-8","D",0]
["2-Propenoic acid, 2-methyl-, polymer with butyl 2-propenoate, 2-methylpropyl 2-methyl-2-propenoate, 2-propenoic acid and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate, tert-Bu 2-ethylhexaneperoxoate-initiated","1334163-54-0","D",0]
["2-Chloro-1,1,1,2,3,3-hexafluoropropane","51346-64-6","D",0]
["2‐Hydroxy‐3‐[[3-(perfluorohexyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["2-Ethoxy-1,1,1,2-tetrafluoroethane","50285-06-8","D",0]
["30,30,31,31,31-Pentafluoro-29-(1,1,2,2,2-pentafluoroethyl)-27,28,29-tris(trifluoromethyl)-2,5,8,11,14,17,20,23,26-nonaoxahentriacont-27-ene","53410-45-0","D",0]
["3-(Heptafluoropropyl)-5-methyl-1H-pyrrole-2-carbaldehyde","123825-55-8","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoro-1,8-diisocyanatooctane","83354-58-9","D",0]
["Sodium perfluoro(3-{[1-(1,2-dichloro-1,2,2-trifluoroethoxy)propan-2-yl]oxy}propyl)sulfonate","1383434-30-7","D",0]
["Bis(perfluorohexyl) phosphinic acid ytterbium(3+) salt","500776-72-7","D",0]
["3-Fluoro-4-(pentafluoroethyl)benzoic acid","1355157-51-5","D",0]
["2‐[Dimethyl(4-fluoro-4-(perfluoropentadecyl)‐2‐hydroxybut‐3‐en‐1‐yl)azaniumyl]acetate","","D",0]
["Perfluoro[1,2,3,4,5,6,7-13C7]undecanoic acid","","D",0]
["2-(1,1,2,2-tetrafluoroethoxy)phenol","88553-88-2","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluoroethanesulfonyl)amino]propan-1-aminium","","D",0]
["B-(4-(Perfluoro-1-methylethyl)phenyl)boronic acid","1184850-50-7","D",0]
["3-(Perfluoroisopropyl)propanol","29819-73-6","D",0]
["3,3,4,4,4-Pentafluorobutyl trifluoromethanesulfonate","676525-95-4","D",0]
["2(1H)-Quinoxalinone, 3-(pentafluoroethyl)-","89995-28-8","D",0]
["6,6-Diethoxy-1,1,1,2,2,3,3-heptafluoro-5-iodohexane","89608-39-9","D",0]
["(Pentafluoroethyl)cyclohexane","1737-48-0","D",0]
["4-Methyl-N-[2,2,2-trifluoro-1-(trifluoromethyl)ethylidene]benzamide","40024-22-4","D",0]
["Phosphoric acid--2,2,3,3-tetrafluoropropan-1-ol (1/3)","563-10-0","D",0]
["N,N,N-Trimethyl-3-[methyl(perfluorononanesulfonyl)amino]propan-1-aminium","","D",0]
["9-diethoxyphosphoryl-1,1,1,2,2,3,3,4,4,5,5,6,6,7,7-pentadecafluoro-9-iodononane","23068-06-6","D",0]
["Triethoxy(3,3,4,4,4-pentafluorobutyl)silane","736154-66-8","D",0]
["2-(1,1,2,2-tetrafluoroethoxy)naphthalene","2796-08-9","D",0]
["2,2,3,3,4,4,4a,5,5,6,6,7,7,8,8,8a-Hexadecafluorooctahydro-2H-1-benzopyran","72942-63-3","D",0]
["[N-[(Perfluoroheptylsulfonamido)propyl]-N,N-dimethylammonio]propionate inner salt","34522-08-2","D",0]
["1,2,2-Trifluoro-1-(trifluoromethyl)-2,3-dihydro-1H-indene","52922-93-7","D",0]
["Morpholine, 2,2,3,3,5,5,6,6-octafluoro-4-(undecafluorocyclohexyl)-","114832-09-6","D",0]
["1,3,3,4,4,5,5,5-Octafluoropent-1-yne","","D",0]
["1,1,2,3,3-Pentafluoro-1,3-dimethoxypropane","758-62-3","D",0]
["12:2 Fluorotelomer thioether amido amine carboxylate","1513863-98-3","D",0]
["N-[3-(Ethenyloxy)propyl]-N-methylperfluorooctane-1-sulfonamide","","D",0]
["(3b,8x,9x,14x,17x)-cholest-5-en-3-yl heptafluorobutanoate","","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluorotetradecane","214196-02-8","D",0]
["1,6-Dichloro-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorohexane","355-40-8","D",0]
["N-Methyl perfluoro-1-decane sulfonamide","","D",0]
["Methyl perfluoroethyl ketone","374-41-4","D",0]
["[3,3,4,4,5,5,6,6,7,8,8,8-Dodecafluoro-2-hydroxy-2-methyl-7-(trifluoromethyl)octyl] prop-2-enoate","","D",0]
["3-(heptadecafluorooctyl)-5-methyl-1H-pyrazole","243659-12-3","D",0]
["4H-1,3,2-Benzodioxaphosphorin-4-one, 2-(2,2,3,3-tetrafluoropropoxy)-","137073-23-5","D",0]
["Methyl 5-(pentafluoroethyl)-2-propyl-1H-imidazole-4-carboxylate","150097-92-0","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7-Dodecafluoroheptyl butanoate","87925-98-2","D",0]
["N,N-Bis(2,3-dihydroxypropyl)-perfluoroheptanamide","118675-72-2","D",0]
["5H-Perfluorohexanesulfonic acid","2089109-56-6","D",0]
["3'-Fluoro-4'-methoxy-4,4,4-trifluoro-3-trifluoromethyl-crotonophenone","35444-03-2","D",0]
["1-Chloro-1,2,2,2-tetrafluoro-1-nitroethane","2261-27-0","D",0]
["Diethyl 2,2,3,3,4,4,5,5-octafluoropentyl phosphate","91847-53-9","D",0]
["4-(Methanesulfonyl)phenyl pentafluoroethane-1-sulfonate","57728-88-8","D",0]
["1,1,1,3,3,4,4,5,5,6,6-Undecafluorohexan-2-one","42287-75-2","D",0]
["N'-[(2E)-5,5,6,6,7,7,7-Heptafluoro-4-oxohept-2-en-2-yl]-3-methoxybenzohydrazide","1164461-08-8","D",0]
["4,5,5,5-Tetrafluoro-2-iodo-4-(trifluoromethyl)pentan-1-ol","114810-56-9","D",0]
["10-Hydrido-perfluoroundecane-1-sulfonic acid","","D",0]
["Bis(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl) ethanedioate","88055-22-5","D",0]
["3-(2,2-Dibromoethenyl)-2,2-bis(trifluoromethyl)cyclopropane-1-carboxylic acid","99903-52-3","D",0]
["2-{[3-(Acetyloxy)-4-(perfluorooctadecyl)-1,5-dihydroxypentan-2-yl]dimethylazaniumyl}acetate","","D",0]
["1,5-Pentanedione, 2,2,3,3,4,4-hexafluoro-N,5-diphenyl-","2525-83-9","D",0]
["1-Phenyl-3,3-bis(trifluoromethyl)aziridine-2-carbonitrile","61860-07-9","D",0]
["Surflon S 121(A cationic perfluoroalkyltolylmethylammonium iodide surfactant (Asahi Glass) )","82030-82-8","D",0]
["1,3,3,4,5,5-Hexafluorocyclopentene","1006-02-6","D",0]
["N-(Carboxymethyl)-N,N-dimethyl-3-[[(perfluoropentyl)sulfonyl]amino]propanaminium","2089109-23-7","D",0]
["bis(Perfluorobutylsulfonyl)methylenephenyliodine","681477-42-9","D",0]
["N,N-Dimethyl-N-(3-sulfopropyl)-3-[(3-sulfopropyl) [(perfluoropropyl)sulfonyl]amino]-1-propanaminium","2089108-77-8","D",0]
["3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butanal","131118-41-7","D",0]
["N-(2-Methoxyethyl)perfluorobutanesulfonamide","40630-68-0","D",0]
["[2‐Hydroxy‐3‐(3,3,4,4,4‐pentafluorobutanesulfonyl)propyl]trimethylazanium","","D",0]
["1,2-Ethanediol, reaction products with .alpha.-fluoro-.omega.-(2-hydroxyethyl)poly(difluoromethylene), hexakis(methoxymethyl)melamine and polyethylene glycol","68515-70-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoropentacosane","863126-44-7","D",0]
["1H-Pyrazol-5-ol, 1-phenyl-3-(1,1,2,2-tetrafluoroethyl)-","96145-99-2","D",0]
["4-Cyanophenyl 4-(nonadecafluorononyl)benzoate","88951-08-0","D",0]
["Methyl 2-(heptafluoropropyl)-6-methoxybenzoate","109296-89-1","D",0]
["4,4'-{Oxybis[(4,1-phenylene)(1,1,1,3,3,3-hexafluoropropane-2,2-diyl)]}dianiline","131662-80-1","D",0]
["1-Chloro-4-(3,3,3-trifluoro-2-(trifluoromethyl)prop-1-enyl)benzene","99903-56-7","D",0]
["Perfluoropentadecanesulfonic acid","1379460-34-0","D",0]
["2-Phenyl-4,4-bis(trifluoromethyl)-4H-1,3-thiazine","88656-36-4","D",0]
["4,4'-(1,2,2,3,3,3-Hexafluoropropane-1,1-diyl)diphenol","791617-67-9","D",0]
["4-(Nonafluorobutyl)benzenamine","114262-65-6","D",0]
["3,3,4,4-Tetrafluoro-4-[(trifluoroethenyl)oxy]but-1-ene","122817-51-0","D",0]
["N-Ethyl-N,N-dimethyl-(13-(difluoromethyl)perfluorotridecyl)methan-1-aminium","","D",0]
["6-tert-Butyl-2-(piperidin-1-yl)-4,4-bis(trifluoromethyl)-1,3,2lambda~5~-dioxaphosphinan-2-one","101976-62-9","D",0]
["Tetraethylammonium perfluoroheptane sulfonate","439863-97-5","D",0]
["Sodium 2,5-bis(1,1,2,3,3,3-hexafluoropropoxy)benzenesulfonate","75860-16-1","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,21,21,22,22,23,23,24,24,25,25,26,26,27,27,28,28,29,29,30,30,30-Dotetracontafluorotriacontane","135588-58-8","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13-Heptacosafluorotridecane","423-66-5","D",0]
["N-(2-Hydroxyethyl)-N,N-dimethyl-1-octanaminium perfluoro-1-butanesulfonate (1:1)","334529-55-4","D",0]
["Carboxydimethyl[3-(perfluorohexadecyl)-2-hydroxypropyl]azanium","","D",0]
["1,1,2,3,3,4,4,5,5-Nonafluorohex-1-ene","142373-34-0","D",0]
["3-(Perfluoropropanesulfonamido)-N,N,N-trimethylpropan-1-aminium","1966131-51-0","D",0]
["N-(3-{(Carboxymethyl)[(perfluoropentyl)sulfonyl]amino}propyl)-2-hydroxy-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoroicosane","133310-69-7","D",0]
["3,3,3',3'-Tetrakis(trifluoromethyl)-3H,3'H-1,1'-spirobi[[2,1]benzoxatellurole]","92315-01-0","D",0]
["4-(Perfluoro(2,2-bis(1-methylethyl)(1-methyl)ethen-1-yloxy))benzenesulfonic acid","271794-15-1","D",0]
["4:2 fluorotelomer sulfate","","D",0]
["2-Bromo-1,1,1,3,3,3-hexafluoropropane","2252-79-1","D",0]
["3-(Perfluorooctyl)-1-[(2-hydroxyacetyl)sulfanyl]propan-1-one","","D",0]
["3,3,4,5,5,5-Hexafluoro-2-methylpentan-1-ol","64011-45-6","D",0]
["Methyl 3,4-bis({3,4-bis[1,1,2-trifluoro-2-(heptafluoropropoxy)ethoxy]benzyl}oxy)benzoate","1233312-95-2","D",0]
["2,2,3,3,4,4,5,5,6,6,7,7,7-Tridecafluoro-N-[(4-sulfamoylphenyl)methyl]heptanamide","165618-99-5","D",0]
["Trifluoromethyl perfluorobutyl ether","559-29-5","D",0]
["1-[5-Fluoro-2-(1,1,2,2-tetrafluoro-2-phenylethyl)phenyl]methanamine","61547-76-0","D",0]
["8-H-Perfluorooctanoate","1696259-68-3","D",0]
["2-[[(Heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate","","D",0]
["N-(3,3,4,4,4-Pentafluorobut-1-en-2-yl)cyclohexanamine","921193-82-0","D",0]
["1-[(1,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,9-Heptadecafluoronon-1-en-1-yl)oxy]-4-(prop-1-en-2-yl)benzene","112340-38-2","D",0]
["9-(2,2,3,3-Tetrafluorocyclobutyl)nonanoic acid","101832-26-2","D",0]
["Methyl 3,4-dichloro-2,2,3,4,4-pentafluorobutanoate","1480-82-6","D",0]
["N‐[3‐(Dimethylamino)propyl]‐3,3,4,4,5,5,6,6,7,7,8,8,8‐tridecafluoro‐N‐methyloctane‐1‐sulfonamide","66618-52-8","D",0]
["1,1,1,3,3,3-Hexafluoropropan-2-one, oxime","1645-76-7","D",0]
["7,7,8,8,9,9,10,10,11,11,12,12,13,14,14,14-Hexadecafluoro-13-(trifluoromethyl)tetradecan-1-ol","390410-82-9","D",0]
["N-(4'-(Acetylamino)-3,3'-dichloro(1,1'-biphenyl)-4-yl)-2,2,3,3,4,4,4-heptafluorobutanamide","75042-10-3","D",0]
["3-Chloro-1,1,1,2,4,4,5,5,5-nonafluoropent-2-ene","","D",0]
["1-Bromo-4-(2,2,3,3-tetrafluorocyclopropyl)benzene","922141-49-9","D",0]
["2-Furanol, 3,3,4,4-tetrafluorotetrahydro-","623139-74-2","D",0]
["[3‐(2-(Perfluorooctyl)ethanesulfonyl)‐2‐hydroxypropyl]trimethylazanium","","D",0]
["Iodo(tridecafluorohexyl)mercury","63037-05-8","D",0]
["Perfluorotridecyl hydrogen sulfate","","D",0]
["1,1,1,2,2,3,3-Heptafluoro-7-iodoheptane","2967-60-4","D",0]
["Propanoic acid, 2,3,3,3-tetrafluoro-2-(heptafluoropropoxy)-, homopolymer","26099-32-1","D",0]
["1-Hydroxy-15:2 fluorotelomer sulfonic acid","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluorononadecane","931415-53-1","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymer with 2-[[(heptadecafluorooctyl)sulfonyl]methylamino]ethyl 2-propenoate","73018-93-6","D",0]
["1,3,5,2,4,6-Triazatriphosphorine, 2,2,4,4,6,6-hexakis[(2,2,3,3,4,4,5,5,6,6,7,7-dodecafluoroheptyl)oxy]-2,2,4,4,6,6-hexahydro-","3830-74-8","D",0]
["(2Z)-3-Amino-4,4,5,5,6,6,6-heptafluoro-1-phenyl-2-hexen-1-one","91508-85-9","D",0]
["Tetrafluoro(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-lambda~5~-phosphane","205926-51-8","D",0]
["4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)phenol","71360-30-0","D",0]
["3-(Perfluorooctyl)propanol","1651-41-8","D",0]
["2,3,3,3-Tetrafluoro-2-(1,1,2,2,3,3,3- heptafluoropropoxy)-13C3 -propanoic acid","","D",0]
["5,5,5-Trifluoro-4,4-bis(trifluoromethyl)pent-1-yne","14115-48-1","D",0]
["2,2,4,4,6-Pentachloro-6-(2,2,3,3-tetrafluoropropoxy)-,3,5,2lambda5,4lambda5,6lambda5-triazatriphosphinine","59700-57-1","D",0]
["N,N-bis(Trifluoromethyl)perfluoroethanamine","124008-98-6","D",0]
["3-[5'-fluoro-2'-(2,2,3,3,3-pentafluoropropoxy)biphenyl-3-yl]-1H-1,2,4-triazole-5-carboxamide","852317-38-5","D",0]
["2‐[(3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10‐Hexadecafluorodec‐2‐en‐1‐yl)dimethylazaniumyl]ethyl sulfate","70846-84-3","D",0]
["Sodium 1H, 1H, 2H, 2H-[1,2-13C2] perfluorooctyl phosphate","","D",0]
["Tetrabutylphosphanium trifluoro[tris(pentafluoroethyl)]phosphate(1-)","482635-81-4","D",0]
["Dimethyl perfluoro-1,10-decanedicarboxylate","84750-88-9","D",0]
["4-Methyl-5,7-dinitro-2-(pentafluoroethyl)-1H-benzimidazole","60167-94-4","D",0]
["1-(2-Bromo-1,1,2,2-tetrafluoroethoxy)-4-methylbenzene","83015-27-4","D",0]
["Poly(difluoromethylene), .alpha.,.alpha.'-[1,2-phenylenebis[carbonyloxy(2-iodo-3,1-propanediyl)]]bis[.omega.-fluoro-","71550-15-7","D",0]
["5,5,6,6,7,7,7-Heptafluoroheptan-3-amine","679-00-5","D",0]
["2-(1,1,2,2-Tetrafluoroethoxy)propane","757-11-9","D",0]
["2-Chloro-N-[3-[[4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-2-iodo-6-(trifluoromethyl)phenyl]carbamoyl]phenyl]pyridine-3-carboxamide","","D",0]
["4'-Dodecyl-3-(6,6,7,7,8,8,9,9,9-nonafluorononyl)-2,2'-bithiophene","919079-96-2","D",0]
["2-(Perfluoropropyl)benzoxazole","2008-06-2","D",0]
["4,4,5,5,5-Pentafluoro-2-iodopent-1-ene","885275-73-0","D",0]
["Perfluoro-3,5,7,9,11-pentaoxadodecanoic acid","39492-91-6","D",0]
["N-[4-(4-Morpholinylcarbonyl)benzoyl]valyl-N-[(3R)-5,5,6,6,6-pentafluoro-2-methyl-4-oxo-3-hexanyl]-L-prolinamide","163660-53-5","D",0]
["(2‐Carboxyethyl)dimethyl(4,4,5,5,5‐pentafluoro‐2‐hydroxypentyl)azanium","","D",0]
["Octafluoropentane-2,3-dione","74728-95-3","D",0]
["(Perfluorooctyl)-1-propyl prop-2-enoate","1652-60-4","D",0]
["Sodium bis[2-(N-ethylperfluorooctane-1-sulfonamido)ethyl] phosphate","23282-60-2","D",0]
["Dibromo[tris(pentafluoroethyl)]-lambda~5~-stibane","194549-90-1","D",0]
["(E)-Perfluorododec-10-ene-1-sulfonic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-2-[(perfluorotetradecyl)ethylthio]acetamide","","D",0]
["(E)-Perfluorohept-5-ene-1-sulfonic acid","","D",0]
["N-[3-(Dimethylamino)propyl]-2-[(3,3,4,4,4-pentafluorobutyl)sulfanyl]acetamide","","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoroethyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorodecanamido)propan-1-aminium","","D",0]
["(E)-Perfluorobut-2-ene-1-sulfonic acid","","D",0]
["N-[2-Bromo-4-(1,1,1,2,3,3,3-heptafluoropropan-2-yl)-6-(trifluoromethyl)phenyl]-4-fluoro-3-nitrobenzamide","","D",0]
["N-[2-Ethyl-6-methyl-4-(1,1,1,2,3,3,4,4,4-nonafluorobutan-2-yl)phenyl]-2-fluoro-3-nitrobenzamide","","D",0]
["(E)-Perfluorodec-8-ene-1-sulfonic acid","","D",0]
["2-Hydroxy-3-[[3-(perfluorononyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(E)-Perfluoro-2-tridec-7-eneoxyacetic acid","","D",0]
["(E)-Perfluoro-2-but-2-eneoxyacetic acid","","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluorobutyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluorononyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["(E)-Perfluoro-2-hept-5-eneoxyacetic acid","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluoroheptanamido)propan-1-aminium","","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoroheptyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["(E)-Perfluoro-2-dodec-7-eneoxyacetic acid","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorododecanamido)propan-1-aminium","","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoroundecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["(E)-Perfluoro-2-non-7-eneoxyacetic acid","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorooctanamido)propan-1-aminium","","D",0]
["3-([(Perfluoropropyl)sulfonyl]{3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}amino)-2-hydroxy-1-propanesulfonate","","D",0]
["2-Hydroxy-3-[[3-(perfluorododecyl)propanoyl]sulfanyl]propanoic acid","","D",0]
["(E)-Perfluoro-2-hex-4-eneoxyacetic acid","","D",0]
["(E)-Perfluoro-2-pent-3-eneoxyacetic acid","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluoropropanamido)propan-1-aminium","","D",0]
["2-Hydroxy-3-[(4,4,5,5,5-pentafluoropentanoyl)sulfanyl]propanoic acid","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluoropentadecanamido)propan-1-aminium","","D",0]
["(E)-Perfluoro-2-oct-6-eneoxyacetic acid","","D",0]
["{(2-Carboxyethyl)[(perfluorododecyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-3-{ethyl[(perfluorononyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-N-[4-(1,1,1,2,3,3,3-Heptafluoropropan-2-yl)-2-methylphenyl]benzene-1,2-dicarboxamide","","D",0]
["2-Methyl-2-{3-[(perfluorobutyl)sulfanyl]propanamido}propane-1-sulfonic acid","","D",0]
["{(2-Carboxyethyl)[(perfluoroheptyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-3-{ethyl[(perfluoropentyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["3-(((4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononyl)oxy)phenyl)sulfonyl)amino)-N,N,N-trimethyl-1-propanaminium iodide","","D",0]
["{(2-Carboxyethyl)[(perfluoroethyl)sulfonyl]amino}-3-betaine","","D",0]
["3-(((4-((1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9-Heptadecafluorononyl)oxy)phenyl)sulfonyl)amino)-N,N,N-trimethyl-1-propanaminium","","D",0]
["{(2-Carboxyethyl)[(perfluorononyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-3-{ethyl[(perfluoroundecyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["3-([(Perfluorodecyl)sulfonyl]{3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}amino)-1-propanesulfonate","","D",0]
["{(2-Carboxyethyl)[(perfluorohexyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-3-{ethyl[(perfluoropropyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["3-({3-[(2-Hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluorododecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["{(2-Carboxyethyl)[(perfluoropentyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-N,N-dimethyl-(10-(difluoromethyl)perfluorodecyl)methan-1-aminium","","D",0]
["2-Hydroxy-3-({3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluoropentyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["[2-Hydroxy-3-(2-(perfluorobutyl)ethylsulfinyl)propyl]trimethylazanium","","D",0]
["[3-(2-(Perfluorodecyl)ethanesulfonyl)-2-hydroxypropyl]trimethylazanium","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-trifluoromethyl-2-fluoroethan-1-aminium","","D",0]
["2-Methyl-2-[3-(2-(perfluorododecyl)ethanesulfinyl)propanamido]propane-1-sulfonic acid","","D",0]
["[2-Hydroxy-3-(3,3,4,4,5,5,6,6,6-nonafluorohexanesulfonyl)propyl]trimethylazanium","","D",0]
["2-Methyl-2-[3-(2-(perfluorotetradecyl)ethanesulfinyl)propanamido]propane-1-sulfonic acid","","D",0]
["N-Ethenyl-perfluorononanamide","","D",0]
["[3-(2-(Perfluorodecyl)ethylsulfanyl)-2-hydroxypropyl]-trimethylazanium","","D",0]
["2-Methyl-2-[3-(2-(perfluorododecyl)ethanesulfonyl)propanamido]propane-1-sulfonic acid","","D",0]
["N-Ethyl-3-{ethyl[(perfluorododecyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-Methyl-2-[3-(3,3,4,4,4-pentafluorobutanesulfinyl)propanamido]propane-1-sulfonic acid","","D",0]
["N-Ethyl-3-{ethyl[(perfluorodecyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-Methyl-2-[3-(2-(perfluorotetradecyl)ethanesulfonyl)propanamido]propane-1-sulfonic acid","","D",0]
["{(2-Carboxyethyl)(perfluoropropyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-3-{ethyl[(perfluoroheptyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-Methyl-2-[3-(3,3,4,4,5,5,6,6,6-nonafluorohexylsulfonyl)propanoylamino]propane-1-sulfonic acid","","D",0]
["[4-[(E)-3-[2-(2,4-Dinitrophenyl)ethoxy]-3-oxoprop-1-enyl]phenyl] 4-(4,4,5,5,5-pentafluoropentoxy)benzoate","","D",0]
["N-Ethyl-3-{ethyl[(perfluoroethyl)sulfonyl]amino}-N,N-dimethyl-1-propanaminium","","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(perfluoroheptyl)sulfonyl]amino]propyl]-1-propanaminium","","D",0]
["[2-Hydroxy-3- (2-(perfluorotetradecyl)ethylsulfinyl)propyl]trimethylazanium","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluoroheptyl)-2-fluoroethan-1-aminium","","D",0]
["[2-[Ethyl(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctylsulfonyl)amino]-1,1,2,2-tetrafluoroethyl] prop-2-enoate","","D",0]
["2-Hydroxy-N,N-dimethyl-N-{3-[(pentafluoroethanesulfonyl)amino]propyl}-3-sulfopropan-1-aminium","","D",0]
["[2-Hydroxy-3-(2-(perfluorododecyl)ethanesulfonyl)propyl]trimethylazanium","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,8-Tridecafluoro-N,N-dimethyloctan-1-amine N-oxide","","D",0]
["3-([(Perfluorodecyl)sulfonyl]{3-[(2-hydroxyethyl)(dimethyl)azaniumyl]propyl}amino)-2-hydroxy-1-propanesulfonate","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorohexyl)-2-fluoroethan-1-aminium","","D",0]
["2-Hydroxy-N,N-dimethyl-N-{3-[(perfluorododecanesulfonyl)amino]propyl}-3-sulfopropan-1-aminium","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluoropentyl)-2-fluoroethan-1-aminium","","D",0]
["2-Hydroxy-N,N-dimethyl-N-{3-[(perfluorodecanesulfonyl)amino]propyl}-3-sulfopropan-1-aminium","","D",0]
["[2-Hydroxy-3-(2-(perfluorododecyl)ethylsulfinyl)propyl]trimethylazanium","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorotridecyl)-2-fluoroethan-1-aminium","","D",0]
["2-Hydroxy-N,N-dimethyl-N-{3-perfluoro-1-sulfonylnonadecyl)amino]propyl}-3-sulfo-1-propanaminium","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorotetradecyl)-2-fluoroethan-1-aminium","","D",0]
["[2-Hydroxy-3-(3,3,4,4,4- pentafluorobutanesulfinyl)propyl]trimethylazanium","","D",0]
["2-Hydroxy-N,N-dimethyl-N-{3-[(perfluoroundecanesulfonyl)amino]propyl}-3-sulfopropan-1-aminium","","D",0]
["[2-Hydroxy-3-(2-(perfluorotetradecyl)ethanesulfonyl)propyl]trimethylazanium","","D",0]
["N-Butyl-N,N-dimethyl-(3-(difluoromethyl)perfluoropropyl)methan-1-aminium","","D",0]
["[(4,4,5,5,6,6,6-Heptafluorohexanoyl)sulfanyl]-2-hydroxy-3-oxopropanoic acid","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluorodecyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["[(1-Fluoranthen-8-yl-2,2,3,3,4,4,5,5-octafluoropentylidene)amino] 1,1,2,2,3,3,4,4,4-nonafluorobutane-1-sulfonate","","D",0]
["N-Butyl-N,N-dimethyl-(13-(difluoromethyl)perfluorotridecyl)methan-1-aminium","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluorononyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["[1,1,2,2-Tetrafluoro-2-[1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctylsulfonyl(methyl)amino]ethyl] prop-2-enoate","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorobutyl)-2-fluoroethan-1-aminium","","D",0]
["[(Perfluoropropane-1-sulfonyl)(methyl)amino]acetic acid","","D",0]
["Heptane, perfluoro, branched and linear","","D",0]
["N-Butyl-N,N-dimethyl-(9-(difluoromethyl)perfluorononyl)methan-1-aminium","","D",0]
["[(Perfluoroethane-1-sulfonyl)(methyl)amino]acetic acid","","D",0]
["2-Hydroxy-N,N-dimethyl-3-sulfo-N-[3-[[(perfluorooctyl)sulfonyl]amino]propyl]-1-propanaminium","","D",0]
["N,N-Dimethyl-N-{2-oxo-2-[(propan-2-yl)oxy]ethyl}-3-(perfluorohexanamido)propan-1-aminium","","D",0]
["N-Butyl-N,N-dimethyl-(7-(difluoromethyl)perfluoroheptyl)methan-1-aminium","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluoroheptyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluorobutyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorododecyl)-2-fluoroethan-1-aminium","","D",0]
["[2-[Ethyl(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctylsulfonyl)amino]-1,1,2,2-tetrafluoroethyl] 2-methylprop-2-enoate","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluoropentyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["[2,5-Dichloro-4-(1,1,2,3,3,3-hexafluoropropoxy)phenyl]urea","","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluorodecyl)-2-fluoroethan-1-aminium","","D",0]
["{2-Hydroxy-3-[2-(perfluorotetradecyl)ethylsulfanyl]propyl}trimethylazanium","","D",0]
["3-(3,3,4,4,5,5-Hexafluorocyclopenten-1-yl)-2-methyl-1-benzothiophene","","D",0]
["3-(3,3,4,4,5,5,6,6,6-Nonafluorohexylsulfonyl)propanoic acid","","D",0]
["{3-[2-(2-(Perfluorodecyl)ethanesulfonyl)acetamido]propyl}trimethylazanium","","D",0]
["N-Methyl-4-(4,4,5,5,5-pentafluoropentylsulfonyl)butan-1-amine","","D",0]
["{3-[2-(2-(Perfluorooctyl)ethylsulfinyl)acetamido]propyl}trimethylazanium","","D",0]
["N-Propyl-N,N-dimethyl-((difluoromethyl)difluoromethyl)methanaminium","","D",0]
["3-(Dimethyl{3-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoroheptane-1-sulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["{3-[2-(2-(Perfluorooctyl)ethanesulfonyl)acetamido]propyl}trimethylazanium","","D",0]
["N-Methyl-N-(2-oxobut-3-en-1-yl)perfluorooctane-1-sulfonamide","","D",0]
["3-(Difluoromethyl)-2,2,3,4,4-pentafluorothiolane 1,1-dioxide","","D",0]
["3-(Dimethyl{3-[(Perfluorododecanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["{Ethyl[(perfluorododecyl)sulfonyl]amino}acetic acid","","D",0]
["N-Propyl-N,N-dimethyl-(13-(difluoromethyl)perfluorotridecyl)methan-1-aminium","","D",0]
["3-(Dimethyl{3-[(Perfluorodecanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["3-(2-(Perfluorodecyl)ethylsulfanyl)propanoic acid","","D",0]
["[(Perfluorohexanoyl)amino]-3-betaine","","D",0]
["3-(2,3,3,4,4,4-Hexafluorobutan-2-ylsulfonyloxy)propyl 2,3,3,4,4,4-hexafluorobutane-2-sulfonate","","D",0]
["{[(Perfluorotetradecyl)sulfonyl]amino}acetic acid","","D",0]
["N-Methyl perfluoro-1-ethane sulfonamide","","D",0]
["N-Methyl perfluoro-1-tetradecane sulfonamide","","D",0]
["{[(Perfluoroundecyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Methyl perfluoro-1-nonane sulfonamide","","D",0]
["3-(2-(Perfluorotetradecyl)ethanesulfonyl)propanoic acid","","D",0]
["3-(2-(Perfluorotetradecyl)ethylsulfanyl)propanoic acid","","D",0]
["{[(Perfluorononyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Methyl perfluoro-1-dodecane sulfonamide","","D",0]
["N-Propyl-N,N-dimethyl-(11-(difluoromethyl)perfluoroundecyl)methan-1-aminium","","D",0]
["{[(Perfluorotridecyl)sulfonyl]amino}acetic acid","","D",0]
["N-Methyl perfluoro-1-propane sulfonamide","","D",0]
["3-(3,3,4,4,4-Pentafluorobutanesulfinyl)propanoic  acid","","D",0]
["N-Methyl perfluoro-1-undecane sulfonamide","","D",0]
["3-(3,3,4,4,5,5,6,6,6-Nonafluorohexanesulfinyl)propanoic acid","","D",0]
["N-Methyl perfluoro-1-tridecane sulfonamide","","D",0]
["3-(2-(Perfluorodecyl)ethanesulfonyl)propanoic acid","","D",0]
["{(Carboxymethyl)[(perfluoropentyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-N,N-dimethyl-(8-(difluoromethyl)perfluorooctyl)methan-1-aminium","","D",0]
["N-Ethyl-N,N-dimethyl-(7-(difluoromethyl)perfluoroheptyl)methan-1-aminium","","D",0]
["3-(2-(Perfluorododecyl)ethanesulfinyl)propanoic acid","","D",0]
["N-Ethylperfluoro-1-decanesulfonamide","","D",0]
["{4-[1-(4-Pentafluoroethyloxyphenyl)-1H-[1,2,4]triazol-3-yl]-phenyl}-carbamic acid tert-butyl ester","","D",0]
["N-Ethyl-N,N-dimethyl-(6-(difluoromethyl)perfluorohexyl)methan-1-aminium","","D",0]
["N-Ethylperfluoro-1-nonanesulfonamide","","D",0]
["3-(2-(Perfluorododecyl)ethanesulfonyl)propanoic acid","","D",0]
["N-Ethylperfluoro-1-dodecanesulfonamide","","D",0]
["{[(Perfluorodecyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethylperfluoro-1-undecanesulfonamide","","D",0]
["3-(2-(Perfluorotetradecyl)ethanesulfinyl)propanoic acid","","D",0]
["N-Ethylperfluoro-1-tridecanesulfonamide","","D",0]
["3-(2-(Perfluorooctyl)ethanesulfinyl)propanoic acid","","D",0]
["{(Carboxymethyl)[(perfluorobutyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-N,N-dimethyl-(12-(difluoromethyl)perfluorododecyl)methan-1-aminium","","D",0]
["3-({3-[(2-Hydroxyethyl)(dimethyl)azaniumyl]propyl}[(perfluorononyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["{(2-Carboxyethyl)[(perfluoroundecyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-N,N-dimethyl-(11-(difluoromethyl)perfluoroundecyl)methan-1-aminium","","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluorododecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["{(Carboxymethyl)[(perfluorododecyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-N,N-dimethyl-(2-(difluoromethyl)perfluoroethyl)methan-1-aminium","","D",0]
["{(Carboxymethyl)[(perfluorodecyl)sulfonyl]amino}-3-betaine","","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluorononyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["{(Carboxymethyl)[(perfluoroheptyl)sulfonyl]amino}-3-betaine","","D",0]
["N-Ethyl-N,N-dimethyl-(4-(difluoromethyl)perfluorobutyl)methan-1-aminium","","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluoroheptyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["{(Carboxymethyl)[(perfluoroethyl)sulfonyl]amino}-3-betaine","","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluoroundecyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["2-Hydroxy-N-(3-{(2-hydroxy-3-sulfopropyl)[(perfluoroethyl)sulfonyl]amino}propyl)-N,N-dimethyl-3-sulfo-1-propanaminium","","D",0]
["N-Ethyl-N,N-dimethyl-(9-(difluoromethyl)perfluorononyl)methan-1-aminium","","D",0]
["3-({4-[(2,3-Dihydroxypropyl)(dimethyl)azaniumyl]-1-hydroxy-2-butanyl}[(perfluorooctyl)sulfonyl]amino)-1-propanesulfonate","","D",0]
["N-Ethyl-N,N-dimethyl-(5-(difluoromethyl)perfluoropentyl)methan-1-aminium","","D",0]
["{(Carboxymethyl)[(perfluorohexyl)sulfonyl]amino}-3-betaine","","D",0]
["1-(Dimethylamino)-4,4,5,5,5-pentafluoropentan-2-ol","","D",0]
["Perfluoro-13-methoxytridecane-1-sulfonic acid","","D",0]
["3-(Perfluorononyl)-propane-1-sulfonic acid","","D",0]
["Perfluoro-13-(pentafluoro-.lambda.6-sulfanyl)tridecanoic acid","","D",0]
["1-(Dimethylamino)-3-(perfluorotetradecyl)propan-2-ol","","D",0]
["1-(Dimethylamino)-4,5,5,6,6,7,7,7-octafluorohept-3-en-2-ol","","D",0]
["Perfluoro-14-(pentafluoro-.lambda.6-sulfanyl)-1-tetradecanesulfonic acid","","D",0]
["Perfluoro-13-oxotetradecane-1-sulfonic acid","","D",0]
["1-(Dimethylamino)-4,5,5,5-tetrafluoropent-3-en-2-ol","","D",0]
["3-(Perfluoropentyl)-propane-1-sulfonic acid","","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluoroheptyl)-but-3-en-2-ol","","D",0]
["Perfluoro-14-methoxytetradecane-1-sulfonic acid","","D",0]
["3-(Perfluoropentyl)-1-[(2-hydroxyacetyl)sulfanyl]propan-1-one","","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluoroheptadecyl)-but-3-en-2-ol","","D",0]
["3-(Perfluorooctyl)propane-1-sulfonic acid","","D",0]
["3-(Perfluorotetradecyl)propanoic acid","","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluoropentadecyl)-but-3-en-2-ol","","D",0]
["Perfluoro-1-dodecanesulfonamide","","D",0]
["3-(Perfluorotetradecyl)propane-1-sulfonic acid","","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluorononyl)-but-3-en-2-ol","","D",0]
["{(Carboxymethyl)[(perfluorononyl)sulfonyl]amino}-3-betaine","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-10-triaminosilyldecane","","D",0]
["Perfluoro-4-(pentafluoro-omega6-sulfanyl)butanoic acid","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Hexadecafluorodecyl 2-methylprop-2-enoate","","D",0]
["1-(Methylamino)-3-(perfluorotetradecyl)propan-2-ol","","D",0]
["Perfluoro-3-propylcyclopentane-1-sulfonic acid","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-9-(triethoxymethyl)heptadecane","","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluoroethyl)sulfonyl]amino}propyl)-1-butanaminium","","D",0]
["1-(1,1,2,2,3,3,3-Heptafluoropropyl)cyclohexa-3,5-diene-1,3-diamine","","D",0]
["1-(1,1,2,2,2-Pentafluoroethylsulfonyloxy)ethyl 1,1,2,2,2-pentafluoroethanesulfonate","","D",0]
["1,1,1,2,2,4,5,5,6,6,7,7,7-Tridecafluorohept-3-ene","","D",0]
["Perfluoro-5-(tridecafluorohexyl)cyclohexanesulfonic acid","","D",0]
["1,1,1,2,2,3,4-Heptafluorohex-3-ene","","D",0]
["3:2 Fluorotelomer ketone sulfonate","","D",0]
["1,1,1,2,2-Pentafluoro-2-(2,2,2-trifluoroethylsulfanyl)ethane","","D",0]
["3-[(1,3-Dihydroxy-3-(perfluorohexyl)propan-2-yl)sulfanyl]propanoic acid","","D",0]
["3-[(1,3-Dihydroxy-3-(perfluorododecyl)propan-2-yl)sulfanyl]propanoic acid","","D",0]
["3-[(2-Carboxyethyl)[(perfluoro-1-sulfonyltridecyl)]amino]-N-(carboxymethyl)-N,N-dimethyl- 1-propanoate","","D",0]
["1,1,1,2,2-Pentafluoro-2-[fluoro(1,1,2,2,2-pentafluoroethoxy)phosphoryl]oxyethane","","D",0]
["3-[(1,3-Dihydroxy-3-(perfluorotetradecyl)propan-2-yl)sulfanyl]propanoic acid","","D",0]
["Perfluoro-5-(undecafluoropentyl)cyclohexanesulfonate","","D",0]
["3-[(1,3-Dihydroxy-3-(perfluorooctyl)propan-2-yl)sulfanyl]propanoic  acid","","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluorodecyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["1,1,1,2,2-Pentafluoro-3-(2,2,3,3,3-pentafluoropropylsulfinyl)propane","","D",0]
["Perfluoro-5-ethylcyclohexane-1-carboxylic acid","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10-Hexadecafluorododecane-1,12-diol","","D",0]
["1-(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-Heptadecafluorooctylsulfonyloxy)ethyl 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctane-1-sulfonate","","D",0]
["3-(Dimethyl{3-[methyl(perfluorooctanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["1-(1,1,2,2,3,3,4,4,4-Nonafluorobutylsulfonyl)piperazine","","D",0]
["Perfluoro[1,2,3,4-13C4]butanoic acid","","D",0]
["3-(Dimethyl{3-[methyl(perfluoroundecanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["3-(Dimethyl{3-[methyl(perfluoropropanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["Pentafluoroethyl hydrogen sulfate","","D",0]
["1,1,1,2,2,3,3,4,4-Nonafluoro-4-(methyldisulfanyl)butane","","D",0]
["Perfluoro-5-(heptafluoropropyl)cyclohexanesulfonic acid","","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluorododecyl)sulfonyl]amino}propyl)-1-butanaminium","","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-methylsulfanylpropane","","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluorononyl)sulfonyl]amino}propyl)-1-butanaminium","","D",0]
["1,1,1,2,2,3,3-Heptafluoro-3-(2,2,2-trifluoroethylsulfonyl)propane","","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluoroheptyl)sulfonyl]amino}propyl)-1-butanaminium","","D",0]
["Perfluoro-5-(pentafluoroethyl)cyclohexanesulfonic acid","","D",0]
["3:1 Fluorotelomer amino ethyl trimethyl ammonium","","D",0]
["1,1,1,2,2,3,3-Heptafluoro-4-(2,2,3,3,4,4,4-heptafluorobutylperoxy)butane","","D",0]
["Perfluoro-5-(pentafluoroethyl)cyclohexanesulfonate","","D",0]
["3,4-Dihydroxy-N,N-dimethyl-N-(3-{[(perfluoroundecyl)sulfonyl]amino}propyl)-1-butanaminium","","D",0]
["1-(Methylamino)-3-(perfluorooctyl)propan-2-ol","","D",0]
["Perfluoro-3-oxobutane-1-sulfonic acid","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-Nonadecafluoro-N,N-dimethylundecan-1-amine N-oxide","","D",0]
["Perfluoro-3-methylcyclopentane-1-sulfonic acid","","D",0]
["1-(Methylamino)-3-(perfluorooctadecyl)propan-2-ol","","D",0]
["3-[(3-{(2-Carboxyethyl)[(heptadecafluorooctyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","","D",0]
["Hostinert 216","151638-37-8","D",0]
["1-Bromo-4-[(1,1,1,2,3,3,3-heptafluoropropan-2-yl)oxy]butane","37027-49-9","D",0]
["Dichlorohexafluorocyclobutane","27154-45-6","D",0]
["1-Chloro-perfluoroheptane-1-sulfonic acid","","D",0]
["3-{(Perfluoroheptanesulfonyl)[3-(trimethylazaniumyl)propyl]amino}propanoate","","D",0]
["3,3,4-Trifluoro-4-(heptafluoropropoxy)tricyclo[4.2.1.0~2,5~]non-7-ene","262617-19-6","D",0]
["(E)-Perfluoro-4-methylpent-2-enoyl fluoride","103229-77-2","D",0]
["S-(1,1,2,3,3,3-Hexafluoropropyl)cysteine","115974-71-5","D",0]
["(5,5,6,6,7,7,8,8,9,9,10,10,11,11,11-pentadecafluoroundecane-1,3-diyl)bis(phosphonic acid)","23068-12-4","D",0]
["FLUORINATED TETRAETHYLENE GLYCOL","330562-44-2","D",0]
["Perfluoro-3-methyl-1-oxadecalin","73900-70-6","D",0]
["1-Pentanesulfonamide, 1,1,2,2,3,3,4,4,5,5,5-undecafluoro-N-(phenylmethyl)-","68298-08-8","D",0]
["Diethyl 2,6-dihydroxy-2,6-bis(nonafluorobutyl)-4-phenyloxane-3,5-dicarboxylate","359875-73-3","D",0]
["(E)-5-((Perfluorodec-1-enyl)fluoromethyl)perfluoropentane-1-sulfonic acid","","D",0]
["1,5-Pentanediamine, 2,2,3,3,4,4-hexafluoro-","336-33-4","D",0]
["N-Carboxymethyl-N,N-dimethyl-2-(perfluoropropyl)-2-fluoroethan-1-aminium","","D",0]
["(Perfluoropentyl)methane-1-sulfonic acid","678-66-0","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-(1,1,2,2,3,3,3-heptafluoropropyl)-\n.omega.-[1,2,2,2-tetrafluoro-1-(fluorocarbonyl)ethoxy]-","37382-64-2","D",0]
["1,8-Dibromo-1,1,2,2,3,3,4,4,5,5,6,6-dodecafluorooctane","647-41-6","D",0]
["1-(1,1,1,3,3,3-Hexafluoropropan-2-yl)-4-methylbenzene","35462-71-6","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12-Pentacosafluorodocosane","93454-72-9","D",0]
["3-(2-(Perfluorohexyl)ethanesulfonyl)propanoic acid","","D",0]
["4-Amino-1,1,1,2,2-pentafluorohexan-3-ol","521286-58-8","D",0]
["1,1,2,2-Tetrafluoro-3-(1,1,2,2-tetrafluorobutyl)cyclobutane","35207-97-7","D",0]
["1-Chloro-2-(difluoromethoxy-d)-1,2,2-trifluoro-ethane-d","78825-17-9","D",0]
["1,1,1,2,2-Pentafluoro-2-methylsulfinylethane","","D",0]
["Perfluoro-5-butylcyclohexane-1-carboxylic acid","","D",0]
["3,4,4,5,5,6,6,6-Octafluorohex-2-ene-1-sulfonic acid","","D",0]
["1,1,1,2,2,3,3,4,4,5,6-Undecafluorohexane","","D",0]
["Perfluoro-4-propylcyclopentane-1-carboxylic acid","","D",0]
["3,4,4,5,5,5-Hexafluoropentanoic acid","","D",0]
["2:2 Fluorotelomer thiol","87851-78-3","D",0]
["2-Hydrido-perfluorotetradecanoic acid","","D",0]
["3-(2,2,3,3-Tetrafluoropropoxy)propane-1,2-diol","25385-68-6","D",0]
["1-Hydroxy-12:2 fluorotelomer sulfonic acid","","D",0]
["A mixture of: 1,6-Diisocyanatohexane, biss-omega-hydroxypoly (oxyethylene), 1,1,2,2,3,3,4,4,4-nonafluoro-N-(2-hydroxyethyl)-N-methylbutane-1-sulphonamide and 3-(Trimethoxysilyl)-propylamine","1016637-15-2","D",0]
["Ethyl 2-acetyl-4,4,5,5-tetrafluoro-3-oxopentanoate","116206-91-8","D",0]
["Bis(perfluoroethylsulfonyl)imide anion","129318-46-3","D",0]
["Bis(3-methoxypropyl) octafluorohexanedioate","600700-53-6","D",0]
["1H,1H,5H-Perfluoropentane-1-thiol","1597-11-1","D",0]
["1,1,1,3,3,3-hexafluoro-2-[2,2,6-trimethyl-4,4-bis(trifluoromethyl)-1H-3,1-benzoxazin-8-yl]propan-2-ol","80360-42-5","D",0]
["(3E)-1,1,1,2,2,3,4,5,5,6,6,7,7,7-Tetradecafluorohept-3-ene","100646-05-7","D",0]
["2,2,2-Tris(perfluoropropyl)ethyl prop-2-enoate","","D",0]
["Perfluoro-1-tetradecanesulfonamide","","D",0]
["Perfluoro-8-decene-1-sulfonic acid","2089109-45-3","D",0]
["(1E)-2,2,3,3,3-Pentafluoro-N-(4-methoxyphenyl)propan-1-imine","189396-84-7","D",0]
["N-Butyl-2,2,3,3,4,4,4-heptafluorobutanamide","377-67-3","D",0]
["1,1,2,3,3,4-Hexafluorobutane","114810-03-6","D",0]
["1-[4-(Pentafluoroethyl)phenyl]methanamine","128273-62-1","D",0]
["3-(Dimethyl{3-[methyl(perfluoropentanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["3,4,4,4-Tetrafluoro-3-(trifluoromethyl)butane-1-sulfonic acid","","D",0]
["Perfluoro-4a,8a-dimethyldecalin","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-11-(tributoxymethyl)nonadecane","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-9-[tri(propan-2-yloxy)methyl]heptadecane","","D",0]
["Perfluoro-4-oxodecalin","","D",0]
["3,4,4,5,5,5-Hexafluoropent-2-enoic acid","","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-9-(tripropoxymethyl)heptadecane","","D",0]
["Perfluoro-4-methylcyclopentane-1-carboxylic acid","","D",0]
["3,4,4,5,5,5-Hexafluoropent-2-ene-1-sulfonic acid","","D",0]
["3-(Perfluorotridecyl)propanoic acid","","D",0]
["3-(Perfluorotridecyl)propane-1-sulfonic acid","","D",0]
["Perfluoro-1-methyl-3-propylcyclohexane","","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluoropentyl)-but-3-en-2-ol","","D",0]
["3-(Perfluoroundecyl)propane-1-sulfonic acid","","D",0]
["1-(Methylamino)-3-(perfluorobutyl)propan-2-ol","","D",0]
["Perfluoro-1-undecanesulfonamide","","D",0]
["Perfluoro-1-tridecanesulfonamide","","D",0]
["1-(Dimethylamino)-4-fluoro-4-(perfluoroundecyl)-but-3-en-2-ol","","D",0]
["3,3,4,4,4-Pentafluorobutyl thioacetate","","D",0]
["1-(Methylamino)-3-(perfluorododecyl)propan-2-ol","","D",0]
["Perfluoro-3-(pentafluoro-omega6-sulfanyl)propanoic acid","","D",0]
["1-(Methylamino)-3-(perfluorodecyl)propan-2-ol","","D",0]
["3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,10-Heptadecafluorodecan-2-yl 2-methylprop-2-enoate","","D",0]
["Fluowet PL 80B","341973-50-0","D",0]
["Perfluoro-4-butylcyclopentane-1-carboxylic acid","","D",0]
["Carbon-tetrafluoride","75-73-0","D",0]
["Pentane, 1,1,1,2,2,3,3-heptafluoro-","754-68-7","D",0]
["4,4,5,5,6,6,7,7,8,8,9,9,9-Tridecafluorononyl iodide","89889-20-3","D",0]
["1,1,1,2,2,3,3,4,4-nonafluoro-4-methoxy- butane, mixt. with 2- (difluoromethoxymethyl)-1,1,1,2,3,3,3- heptafluoropropane (HFE-7100)","219484-64-7","D",0]
["Nonadecane, 1,1,1,2,2,3,3,4,4,5,5-undecafluoro-","117948-72-8","D",0]
["Furan, tetrahydro(1,1,2,2,3,3,4,4,4-nonafluorobutyl)-","26446-59-3","D",0]
["1-Octanesulfonic acid, 1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluoro-, ammonium salt, ion(1-) (1:1)","1379454-92-8","D",0]
["Acetamide, N-[(1,1,2,2,3,3,4,4,4-nonafluorobutyl)phenyl-λ4-sulfanylidene]-","","D",0]
["Methane, tetrakis(trifluoromethoxy)-","92639-87-7","D",0]
["9-Octadecenoic acid (Z-)-, reaction products with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-1-tetradecanol","220237-52-5","D",0]
["2,5-Furandione, dihydro-, monopolyisobutylene derivatives, reaction products with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,14,14,14-pentacosafluoro-1-tetradecanol","253682-97-2","D",0]
["2,5-Furandione, dihydro-, monopolyisobutylene derivatives, reaction products with 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,12-heneicosafluoro-1-dodecanol","253682-98-3","D",0]
["Siloxanes and Silicones, di-Me, hydroxy-terminated, polymers with tetradecanedioic acid, 3,3,4,4,5,5,6,6,7,7,8,8,9,9,10,10,11,11,12,12,13,13,13-tricosafluoro-1-tridecanol-terminated","182700-77-2","D",0]
["1,3-Butadiene, 1,1,2,4,4-pentafluoro-3-(trifluoromethyl)-","384-04-3","D",0]
["Heptane, pentadecafluoro-","27213-61-2","D",0]
["Sodium hydrogen 4-[(heptadecafluorononenyl)oxy]benzylphosphonate","63661-51-8","D",0]
["Polysiloxanes, fluoro","65071-96-7","D",0]
["Surflon S 382","91105-71-4","D",0]
["SURFLON S 381","96231-87-7","D",0]
["Surflon S 393","113189-63-2","D",0]
["Fluowet PP (9CI)","135506-92-2","D",0]
["Phenanthrene, tetracosafluorotetradecahydro-, homopolymer (9CI)","159182-00-0","D",0]
["1H-Pyrazole, 1-benzoyl-3(or 5)-(tridecafluorohexyl)-5(or 3)-(trifluoromethyl)- (9CI)","231301-26-1","D",0]
["1-(Methylamino)-3-(perfluorohexyl)propan-2-ol","","D",0]
["Scotchgard PM 930","923298-12-8","D",0]
["{Ethyl[(perfluoroundecyl)sulfonyl]amino}acetic acid","","D",0]
["N-Propyl-N,N-dimethyl-(7-(difluoromethyl)perfluoroheptyl)methan-1-aminium","","D",0]
["3-(Dimethyl{3-[methyl(perfluorododecanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["Pentafluoroethyl propionate","","D",0]
["1-(1,1,2,2,2-Pentafluoroethylsulfonyl)propane","","D",0]
["1-(1,1,2,2,2-Pentafluoroethylsulfonyl)butane","","D",0]
["1-(3,3,4,4,4-Pentafluorobutyl)-1H-pyrazolo[3,4-b]pyridine-3-carbonitrile","","D",0]
["1-(Dimethylamino)-3-(perfluorohexyl)-2-(hydroxymethoxy)propan-3-yl formate","","D",0]
["3-(Perfluorododecyl)-1-[(2-hydroxyacetyl)sulfanyl]propan-1-one","","D",0]
["1-(Dimethylamino)-3-(perfluorohexadecyl)propan-2-ol","","D",0]
["Perfluoro-11-(pentafluoro-.lambda.6-sulfanyl)undecanoic acid","","D",0]
["1-(Dimethylamino)-3-(perfluorooctadecyl)-2-(hydroxymethoxy)propan-3-yl formate","","D",0]
["Perfluoro-12-(pentafluoro-.lambda.6-sulfanyl)-1-dodecanesulfonic acid","","D",0]
["3-(Perfluorododecyl)propanoic acid","","D",0]
["Perfluoro-11-oxododecane-1-sulfonic acid","","D",0]
["3-(Perfluorododecyl)propane-1-sulfonic acid","","D",0]
["Perfluoro-12-methoxydodecane-1-sulfonic acid","","D",0]
["Perfluoro-12-(pentafluoro-lambda6-sulfanyl)dodecanoic acid","","D",0]
["1-(Dimethylamino)-3-(perfluorooctadecyl)propan-2-ol","","D",0]
["3-(Perfluoroethanesulfonamido)-N,N,N-trimethylpropan-1-aminium","","D",0]
["1-(Dimethylamino)-3-(perfluorotetradecyl)-2-(hydroxymethoxy)propan-3-yl formate","","D",0]
["Perfluoro-13-(pentafluoro-.lambda.6-sulfanyl)-1-tridecanesulfonic acid","","D",0]
["3-(Perfluorohexyl)propane-1- sulfonic acid","","D",0]
["Perfluoro-12-oxotridecane-1-sulfonic acid","","D",0]
["3-(Dimethyl{3-[methyl(pentafluoroethanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["Scotchgard PM 490","940891-99-6","D",0]
["Scotchgard PM 3622","949581-65-1","D",0]
["Surflon S 386","1003557-47-8","D",0]
["Reaction mass of potassium difluoro{[(4S,5R)-2,2,4,5-tetrafluoro-5-(trifluoromethoxy)-1,3-dioxolan-4-yl]oxy}acetate, potassium difluoro{[(4R,5S)-2,2,4,5-tetrafluoro-5-(trifluoromethoxy)-1,3-dioxolan-4-yl]oxy}acetate, potassium difluoro{[(4S,5S)-2,2,4,5-te","1190931-39-5","D",0]
["Surflon S 611","1235969-57-9","D",0]
["Acticide APA (9CI)","50957-54-5","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8-Heptadecafluoro-11-(tripropoxymethyl)nonadecane","","D",0]
["Perfluoro[1,2-13C2]hexadecanoic acid","","D",0]
["3-(Perfluorobutyl)propane-1-sulfonic acid","","D",0]
["3-(Perfluorobutyl)-1-[(2-Hydroxyacetyl)sulfanyl]propan-1-one","","D",0]
["Perfluoro[1,2-13C2]tetradecanoic acid","","D",0]
["1-(Dimethylamino)-3-(perfluorohexadecyl)-2-(hydroxymethoxy)propan-3-yl formate","","D",0]
["Perfluoro-11-(pentafluoro-.lambda.6-sulfanyl)-1-undecanesulfonic acid","","D",0]
["Perfluoro-10-oxoundecane-1-sulfonic acid","","D",0]
["3-(Perfluorodecyl)-1-[(2-hydroxyacetyl)sulfanyl]propan-1-one","","D",0]
["1-(Dimethylamino)-3-(perfluorododecyl)-2-(hydroxymethoxy)propan-3-yl formate","","D",0]
["3-(Dimethyl{3-[(Perfluoroundecanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["N-Propyl-N,N-dimethyl-(5-(difluoromethyl)perfluoropentyl)methan-1-aminium","","D",0]
["{Ethyl[(perfluorotridecyl)sulfonyl]amino}acetic acid","","D",0]
["{Ethyl[(perfluorotetradecyl)sulfonyl]amino}acetic acid","","D",0]
["N-Propyl-N,N-dimethyl-(3-(difluoromethyl)perfluoropropyl)methan-1-aminium","","D",0]
["3-(Dimethyl{3-[methyl(perfluorobutanesulfonyl)amino]propyl}azaniumyl)propane-1-sulfonate","","D",0]
["1-(1,1,2,2,2-Pentafluoroethyl)-1-(trifluoromethyl)cyclohexane","","D",0]
["N-Propyl-N,N-dimethyl-(9-(difluoromethyl)perfluorononyl)methan-1-aminium","","D",0]
["Perfluoro-(C6-18)-alkylphosphonic acid",null,"D",0]
["L–92–0151",null,"D",0]
["Perfluoroheptanes (branched and linear)",null,"D",0]
["Potassium 5-carbamoyl-3-[5'-fluoro-2'-(2,2,3,3,3-pentafluoropropoxy)-3-biphenylyl]-1,2,4-triazol-1-ide hydrate (1:1:1)",null,"D",0]
["1,1,1,2,3,3,4,4,5,5-Decafluoropentane",null,"D",0]
["3-fluoro-2-(trifluoromethyl)benzaldehyde","924817-93-6","D",0]
["2,5-Bis(trifluoromethyl)benzoic acid","42580-42-7","D",0]
["alpha,alpha,alpha,alpha',alpha',alpha'-Hexafluoro-3,5-xylenol","349-58-6","D",0]
["Methyl 2,3,3-trifluoroacrylate","392-41-6","D",0]
["1,1-Difluoro-2-(trifluoromethyl)but-1-ene","13369-10-3","D",0]
["Chloro[tris(pentafluorophenyl)]germane","1259-89-8","D",0]
["1,2,3,4,5-Pentafluorocyclopenta-2,4-diene-1-carbonyl fluoride","74415-70-6","D",0]
["2,2',3,3',5,5',6,6'-Octafluoro[1,1'-biphenyl]-4,4'-diol--water (1/1)","205926-99-4","D",0]
["3,3-Difluorocycloprop-1-ene","56830-75-2","D",0]
["Praseodymium(III) trifluoromethanesulfonate","52093-27-3","D",0]
["Ethyl (trifluoromethyl)phosphonochloridate","89262-69-1","D",0]
["1,2,3,4,5,6,7,8-Octafluoro-9H-fluorene","27053-34-5","D",0]
["1,1,1,2,2,3,3,4,4,7,7,8,8,9,9,10,10,11,11,12,12,12-Docosafluoro-6-iodo-5-dodecene","55756-25-7","D",0]
["N-(5-Chloro-4-(trifluoromethyl)-1,3-thiazol-2-yl)-N-prop-2-enyl-3,5-bis(trifluoromethyl)benzamide","134880-77-6","D",0]
["3,5-Bis(trifluoromethyl)fluorobenzene","35564-19-3","D",0]
["1-(difluoromethyl)-2,4-difluorobenzene","845866-84-4","D",0]
["1-(1-Ethoxyethyl)-2,3,4,5,6,7,8-heptafluoronaphthalene","90095-69-5","D",0]
["1,1-Dichloro-2,2,2-trifluoro-1-iodoethane","646-60-6","D",0]
["(2R)-1,1,1-Trifluoro-4-methylpentan-2-amine","1242338-97-1","D",0]
["5-(Trifluoromethyl)-1,3-thiazol-2-amine","169260-97-3","D",0]
["2-(Methylsulfanyl)-4,6-bis(trifluoromethyl)pyrimidine","62772-93-4","D",0]
["1,1-Dichloro-1,2,2-trifluoropropane","7125-99-7","D",0]
["2,3,5,6,7,8-hexakis(trifluoromethyl)-1,4-diphosphabicyclo[2.2.2]octa-2,5,7-triene","2925-91-9","D",0]
["4,4,4-Trifluoro-3,3-dihydroxybutanenitrile","182924-35-2","D",0]
["[Bis(trifluoroacetoxy)iodo]pentafluorobenzene","14353-88-9","D",0]
["1,2,3,4,5-Pentafluoro-6-[(propan-2-yl)oxy]benzene","61874-51-9","D",0]
["2-Propanol, 1,3-difluoro-","453-13-4","D",0]
["Acetamide, N-[3,5-bis(trifluoromethyl)phenyl]-2-cyano-","63035-03-0","D",0]
["Benzimidazole, 5-methoxy-4,6,7-trifluoro-2-(trifluoromethyl)-","89427-30-5","D",0]
["2,4,6-Tris(trifluoromethyl)benzene-1-thiol","114071-28-2","D",0]
["2,2,2-TRIFLUOROET AMINE,N,N-DIET","37174-09-7","D",0]
["4-Fluoro-2-(trifluoromethyl)phenol","130047-19-7","D",0]
["5-Fluoro-4-methyl-6-(trifluoromethyl)pyrimidin-2-amine","117482-31-2","D",0]
["Trifluoromethaneperoxol","16156-36-8","D",0]
["Caesium trifluoroacetate","21907-50-6","D",0]
["1-Chloro-3-fluoro-5-(trifluoromethyl)benzene","1005764-23-7","D",0]
["1,1,1-Trichloro-3,3,3-trifluoroacetone","758-42-9","D",0]
["2,2',3,3',4,4',5,6,6'-Nonafluoro-1,1'-biphenyl","61908-07-4","D",0]
["2,8-Bis(trifluoromethyl)-4-methylquinoline","57124-23-9","D",0]
["(Difluoromethyl)[bis(fluoromethyl)]methylsilane","61152-89-4","D",0]
["2,2,4,5-Tetrafluoro-1,3-dioxolane","60010-41-5","D",0]
["5,7-Bis(trifluoromethyl)-4-hydroxyquinoline","237076-72-1","D",0]
["Bicyclo(2.2.0)hexa-2,5-diene, 1,2,3,4,5,6-hexafluoro-","6733-01-3","D",0]
["(2R)-4,4,4-Trifluoro-2-methylbutanoic acid","821775-25-1","D",0]
["{2-[Bis(pentafluorophenyl)boranyl]cyclopenta-1,4-dien-1-yl}(trimethyl)silane","462109-75-7","D",0]
["2-Bromo-1,3,4,5,6,7,8,9,10,11,12,13,14-tridecafluoropentacene","919293-77-9","D",0]
["Benzimidazole, 5-methyl-4,6,7-trifluoro-2-(trifluoromethyl)-","89427-31-6","D",0]
["1,2,3,4-Tetrakis(trifluoromethyl)benzene","42175-49-5","D",0]
["2,2-dichloro-1,1,1,4,4,4-hexafluorobutane","162462-08-0","D",0]
["Tetrakis(2,3,4,5,6-pentafluorophenyl)plumbane","1111-02-0","D",0]
["2-(Trifluoromethoxy)ethan-1-amine--hydrogen chloride (1/1)","886050-51-7","D",0]
["1,1,2-Trifluoropropan-1-amine","32076-56-5","D",0]
["3-Bromo-3-chloro-2,2,3-trifluoropropanoyl chloride","88639-61-6","D",0]
["Dodecafluorotriphenylene","17051-14-8","D",0]
["2,4-Bis(trifluoromethyl)bromobenzene","327-75-3","D",0]
["(2,2,2-Trifluoroethoxy)ethene","406-90-6","D",0]
["Thallium(1+) nitrate--2,3-bis(pentafluorophenyl)pyridine (1/1/1)","61160-62-1","D",0]
["2,2,2-Trifluoroethane-1,1-diol--tungsten (2/1)","7234-14-2","D",0]
["(2S)-2-{Bis[3,5-bis(trifluoromethyl)phenyl][(trimethylsilyl)oxy]methyl}pyrrolidine","848821-61-4","D",0]
["4-(1,2-Dichloro-1,1,3,3,3-pentafluoropropan-2-yl)-1,1'-biphenyl","61628-81-7","D",0]
["2-(Trifluoromethyl)-1H-imidazole","66675-22-7","D",0]
["3-Oxo-2-(trifluoromethyl)prop-2-enoic acid","63167-30-6","D",0]
["2,3,4,5-tetrafluorobenzoyl Fluoride","101513-68-2","D",0]
["2,3,5,6-Tetrafluoro-4-sulfanylbenzonitrile","111727-09-4","D",0]
["3,4-Dichloro-1,1,1,3-tetrafluorobutane","1227947-61-6","D",0]
["Chloromethyl trifluoromethyl sulfide","460-58-2","D",0]
["Pentafluorophenyl chlorothionoformate","135192-53-9","D",0]
["(Trifluoromethanesulfonyl)cyclopropane","57964-43-9","D",0]
["3,5-Difluoro-4-(trifluoromethyl)benzoic acid","261945-09-9","D",0]
["1,2,3,4,5-Pentafluoro-6-(2,2,2-trifluoroethoxy)benzene","6669-03-0","D",0]
["3-(trifluoromethyl)-1,2,4-oxadiazole","86657-09-2","D",0]
["Perfluorodiacetamide","407-24-9","D",0]
["Dichlorobis(trifluoromethyl)germane","56593-14-7","D",0]
["3-(Trifluoromethyl)-1,2-oxazol-5-amine","108655-63-6","D",0]
["4-Chloro-2,8-bis(trifluoromethyl)quinoline","83012-13-9","D",0]
["bis(2,2,2-trifluoroethyl) phenylphosphonite","55322-67-3","D",0]
["11:1:2 Fluorotelomer betaine acid",null,"D",0]
["1,2-Dibromo-1,2-difluoroethene","359-21-7","D",0]
["Difluoro(methoxy)methane","359-15-9","D",0]
["alpha,alpha,alpha,3-Tetrafluorotoluene","401-80-9","D",0]
["3,6-Bis(trifluoromethyl)-1,4,2,5-dioxadiazine","88326-82-3","D",0]
["PENTAFLUORO-2-PROPENYL PIVALATE ","885275-40-1","D",0]
["Stibine, tris(trifluoromethyl)-","432-05-3","D",0]
["2,2,2-Trifluoroethyl allyl ether","1524-54-5","D",0]
["N-(Difluoroethenylidene)hypofluorous amide","89555-00-0","D",0]
["2-chloro-1,1,2-trifluoropropane","69202-10-4","D",0]
["ethyl n-[3,5-di(trifluoromethyl)phenyl]carbamate","1998-88-5","D",0]
["Trifluoronitromethane","335-02-4","D",0]
["Pyridine, 4,4'-thiobis[2,3,5,6-tetrafluoro-","19847-40-6","D",0]
["2,3,4,5,6-Pentafluoroaniline","771-60-8","D",0]
["2-Methylpropyl 3,3-difluoro-2-(trifluoromethyl)prop-2-enoate","62935-24-4","D",0]
["1,2,2,3-Tetrafluoro-1-chloro-1-bromopropane","70192-64-2","D",0]
["2-Methyl-2,4,6-tris(trifluoromethyl)-2H-pyran","380-94-9","D",0]
["2,3,4,6-Tetrafluoro-5-(pentafluorophenoxy)phenol","57070-18-5","D",0]
["[3-Chloro-2-(trifluoromethoxy)-6-(trifluoromethyl)phenyl]hydrazine","116244-83-8","D",0]
["Bicyclo[1.1.1]pentane, 1-iodo-3-(trifluoromethyl)-","119934-12-2","D",0]
["[(Trifluoromethyl)disulfanyl]acetic acid","65612-38-6","D",0]
["3-Fluoro-2-methyl-5-(trifluoromethyl)aniline","1065073-89-3","D",0]
["1,2,3,4,5-pentafluoro-6-[2,3,5,6-tetrafluoro-4-(2,3,5,6-tetrafluorophenoxy)phenyl]benzene","14055-53-9","D",0]
["Trifluoromethyl hydrogen sulfate",null,"D",0]
["3,4,5,6-Tetrafluoropyridine-2-carbonitrile","41793-83-3","D",0]
["Benzaldehyde, pentafluoro-, oxime","27318-28-1","D",0]
["2-(pentafluorophenyl)propan-2-ol","715-31-1","D",0]
["1,2,2-Trifluoropropane","811-94-9","D",0]
["4,4,4-Trifluoro-1-(pentafluorophenyl)butane-1,3-dione","33107-70-9","D",0]
["5-(Trifluoromethyl)-1,3-oxazol-2-amine","714972-00-6","D",0]
["Dichlorodifluoromethane","75-71-8","D",0]
["1,1,2,3,5,6,7,8-Octafluoro-4-methyl-4-nitro-1,4-dihydronaphthalene","87415-32-5","D",0]
["N-(2-Chloroethyl)-3,5-bis(trifluoromethyl)benzamide","15317-16-5","D",0]
["2,4-Bis(trifluoromethyl)benzoic acid","32890-87-2","D",0]
["2-(Difluoromethyl)-2-(trifluoromethyl)-1,3-dioxolane","50607-97-1","D",0]
["5-Hexen-1-ol, 4,4,5,6,6-pentafluoro-2-iodo-","139780-45-3","D",0]
["AG-G-90691","73491-36-8","D",0]
["(Fluorocarbonyl)carbonimidoyl","402920-65-4","D",0]
["Scandium(III) triflate","144026-79-9","D",0]
["europium trifluoromethanesulfonate","52093-25-1","D",0]
["chloro-tris(2,3,4,5,6-pentafluorophenyl)stannane","1755-63-1","D",0]
["8-(trifluoromethoxy)-2-(trifluoromethyl)quinolin-4-ol","306935-26-2","D",0]
["6-Fluoro-4-(trifluoromethyl)pyridine-2-carbonitrile","1156542-26-5","D",0]
["1-Chloro-1,2,3,4,4,5,6,7,8-nonafluoro-1,4-dihydronaphthalene","74632-63-6","D",0]
["3,3,3-Trifluoroalanine--hydrogen chloride (1/1)","96105-72-5","D",0]
["Methyl[tris(trifluoromethyl)]plumbane","88261-91-0","D",0]
["2-Chloro-1-fluoro-3-(trifluoromethyl)benzene","109957-97-3","D",0]
["4,4'-Sulfonylbis(tetrafluorophenol)","61907-53-7","D",0]
["2,3,4,5-Tetrachloro-2,3,4,5,6-pentafluoro-2,3,4,5-tetrahydropyridine","25552-48-1","D",0]
["(2,3,5,6-Tetrafluoro-4-methylphenyl)methanol","79538-03-7","D",0]
["Ethane, 2-bromo-2-chloro-1,1,1-trifluoro-, (R)-","51230-17-2","D",0]
["2-Fluoro-4-(trifluoromethyl)benzylamine","239087-05-9","D",0]
["2,3-Bis(trifluoromethyl)-1H-indole","63790-90-9","D",0]
["Silane, bis[2,4-bis(trifluoromethyl)phenyl]dichloro-","650583-78-1","D",0]
["O-(3,3,3-Trifluoropropyl)hydroxylamine--hydrogen chloride (1/1)","1049730-20-2","D",0]
["3,4-Difluoro-5-nitrobenzotrifluoride","101646-01-9","D",0]
["{[(1,1,3,3,3-Pentafluoroprop-1-en-2-yl)oxy]methyl}benzene","67716-26-1","D",0]
["1-(Trifluoromethanesulfonyl)-3-(trifluoromethyl)benzene","309-16-0","D",0]
["5-(Trifluoromethyl)-1H-1,2,4-triazole-3-thiol","68744-64-9","D",0]
["2,2-dichloro-1,1,1,3,3-pentafluoropropane","128903-21-9","D",0]
["1,1',1''-Phosphanetriyltris(2,2,2-trifluoroethan-1-ol)","105149-94-8","D",0]
["Acrylic acid, 3,3-difluoro-2-(trifluoromethyl)-, methyl ester","685-09-6","D",0]
["3,4,5-Trifluoropyridine","67815-54-7","D",0]
["N-Fluoro-N-(4-fluorophenyl)hypofluorous amide (non-preferred name)","204757-18-6","D",0]
["Bis(pentafluorophenyl)xenon","328379-54-0","D",0]
["Ethane, 1-bromo-2-chloro-1,1,2-trifluoro-","354-06-3","D",0]
["Iodopentafluoroacetone","57069-95-1","D",0]
["Difluoromethaneperoxol","183742-70-3","D",0]
["(2,2-Dichloro-1,1,2-trifluoroethyl)carbonimidoyl","87533-02-6","D",0]
["O-(4,4,4-Trifluorobutyl)hydroxylamine","780037-64-1","D",0]
["N-Trifluoromethylimidosulfurous difluoride","1512-14-7","D",0]
["2,3,5,6-tetrafluoropyridin-4-ol","2693-66-5","D",0]
["2,3,5,6-tetrafluorobenzenecarboximidamide","885954-80-3","D",0]
["Perfluorohexamethyl dewar benzene","23174-55-2","D",0]
["1-Bromo-2,3,5,6-tetrafluoro-4-(trifluoromethyl)benzene","17823-46-0","D",0]
["3,5-Bis(trifluoromethyl)anisole","349-60-0","D",0]
["N-[2,3,4,5-Tetrafluoro-6-(pentafluorophenoxy)phenyl]acetamide","90251-13-1","D",0]
["S-Propyl trifluoroethanethioate","53872-01-8","D",0]
["1,1,3,3,4-Pentafluorobutane","119450-76-9","D",0]
["1-Chloro-1,1,2-trifluoropropane","134251-05-1","D",0]
["Tris[2,4,6-tris(trifluoromethyl)phenyl]borane","916336-47-5","D",0]
["Ethane, 2-chloro-1,1-difluoro-","338-65-8","D",0]
["2-Fluoro-5-(trifluoromethyl)anisole","261951-78-4","D",0]
["1,2,2,3,4-Pentafluorobutane","119450-75-8","D",0]
["3-[2,3,5,6-Tetrafluoro-4-(trifluoromethyl)phenyl]prop-2-yn-1-ol","61794-47-6","D",0]
["4-FLUORO-2-(TRIFLUOROMETHYL)PHENYLHYDRAZINE","754973-91-6","D",0]
["Trifluoromethanesulfonyl bromide","15458-53-4","D",0]
["1,3-Bis[(trifluoromethyl)sulfanyl]prop-1-ene","825628-54-4","D",0]
["3,3,6,6-Tetrafluorocyclohexa-1,4-diene","22060-77-1","D",0]
["(2S)-1,1,1-Trifluoro-4-methylpentan-2-amine","1242338-87-9","D",0]
["1,1-Ethanediol, 2,2,2-trifluoro-","421-53-4","D",0]
["1-Butyl-3-methyl-1H-imidazol-3-ium trifluoro(trifluoromethyl)borate(1-)","741677-68-9","D",0]
["1-Butanamine, 4,4,4-trifluoro-2-methyl-, (R)-","766477-05-8","D",0]
["3-Amino-2-fluorobenzotrifluoride","123973-25-1","D",0]
["Ethane, 1,2-dichloro-1,1,2-trifluoro-2-methoxy-","754-28-9","D",0]
["1-(2,3,4,5,6-Pentafluorophenyl)-1-propanol","25622-74-6","D",0]
["Ytterbium(3+) tris(trifluoromethanesulfonate)","54761-04-5","D",0]
["4,4,4-Trifluoro-1-methoxybutan-1-ol","92670-98-9","D",0]
["2-Propanone, 1,1,1-trifluoro-3-mercapto-","127183-53-3","D",0]
["Bromotrifluoroethene","598-73-2","D",0]
["1,3,4-Oxadiazole, 2,5-bis(pentafluorophenyl)-","16184-59-1","D",0]
["1,3,5-Trifluoro-2-iodobenzene","506407-82-5","D",0]
["Bromo(difluoro)acetaldehyde","353-79-7","D",0]
["1,1,1-trifluoro-3-nitropropan-2-ol","453-35-0","D",0]
["1,4-Bis(trifluoroacetyl)piperazine","6345-81-9","D",0]
["(Pentafluorophenyl)boronic acid","1582-24-7","D",0]
["Chloro{[chloro(difluoro)methyl]selanyl}difluoromethane","54393-41-8","D",0]
["1-Methyl-3-(1,1,3,3,3-pentafluoroprop-1-en-2-yl)benzene","207672-95-5","D",0]
["N,N-Bis(trifluoromethyl)hydroxylamine","359-63-7","D",0]
["2,3,4,5-Tetrakis-O-(trifluoroacetyl)-D-xylose","38424-94-1","D",0]
["Chloro{[chloro(difluoro)methyl]disulfanyl}difluoromethane","692-58-0","D",0]
["1-{Difluoro[(2-fluoroethenyl)oxy]methoxy}-2-fluoroethene","173285-18-2","D",0]
["Trimethyl(trifluoromethyl)plumbane","646-62-8","D",0]
["1,1,1-Trifluoro-N-(fluoromethyl)-N-(trifluoromethyl)methanamine","67212-88-8","D",0]
["1,1,3,3-Tetrakis(trifluoromethanesulfonyl)propane","60805-11-0","D",0]
["2-Propanol, 3,3-dichloro-1,1,1-trifluoro-","667464-91-7","D",0]
["1,2,4,5-Tetrafluoropentane","95576-18-4","D",0]
["NSC120055","12169-95-8","D",0]
["5-[3,5-Bis(trifluoromethyl)phenyl]-2H-tetrazole","175205-09-1","D",0]
["2,5-Bis(trifluoromethyl)benzaldehyde","395-64-2","D",0]
["Chloro(pentafluorophenyl)silane","629609-71-8","D",0]
["Barium trifluoromethanesulphonate","2794-60-7","D",0]
["Methyl (2E)-3,3,3-trifluoro-2-[(trifluoroacetyl)imino]propanoate","114066-56-7","D",0]
["2,3,4,5-Tetrafluorobenzamide","16582-94-8","D",0]
["1,2,4,5-Tetrafluoro-3-nitrosobenzene","2010-64-2","D",0]
["Hexakis[(trifluoromethyl)selanyl]benzene","89567-91-9","D",0]
["Silanamine, 1,1,1-trimethyl-N-(pentafluorophenyl)-","22529-97-1","D",0]
["(~13~C)Methyl trifluoromethanesulfonate","207556-12-5","D",0]
["1,1-dichloro-1,2,2-trifluoro-2-(trifluoromethylperoxy)ethane","54362-32-2","D",0]
["2,2'-(1,4-Phenylene)bis[5-fluoro-4-(trifluoromethyl)-1,3-oxazole]","116671-68-2","D",0]
["N-(Cyanomethyl)-2,2,2-trifluoroacetamide","65822-72-2","D",0]
["Acetic acid, trifluoro-, (methylthio)methyl ester","57738-67-7","D",0]
["NSC286662","60049-51-6","D",0]
["3,5-Difluoro-4-(trifluoromethyl)phenol","116640-11-0","D",0]
["(2R)-1,1,1-Trifluorobutan-2-amine--hydrogen chloride (1/1)","1212120-62-1","D",0]
["3-Chloro-5-(trifluoromethyl)-1H-pyrazole","1003320-19-1","D",0]
["Lithium, (2,4,6-trifluorophenyl)-","53732-49-3","D",0]
["1,1,4,4-Tetrafluoro-2-methylbuta-1,3-diene","1513-75-3","D",0]
["Isopropyl trifluoroacetate","400-38-4","D",0]
["AGN-PC-0O0UJG","344-01-4","D",0]
["1-Fluoro-3-methyl-2-(trifluoromethyl)benzene","116850-34-1","D",0]
["Methyl trifluoromethylcarbamate","62765-22-4","D",0]
["Benzene--hexafluorobenzene (1/1)","783-33-5","D",0]
["Diethenyl{bis[(trifluoroacetyl)oxy]}stannane","53355-20-7","D",0]
["1-Bromo-1,1,1-trifluoro-N,N-bis(trifluoromethyl)-lambda~5~-phosphanamine","61527-37-5","D",0]
["1-(Trifluoromethyl)cyclopentan-1-amine","1202965-57-8","D",0]
["[2,6-Bis(trifluoromethyl)phenyl]-lambda~5~-phosphanedithione","7232-74-8","D",0]
["4,4',5,5',6,6'-Hexafluoro[biphenyl]-2,2'-diol","1242677-00-4","D",0]
["Chloro(fluoro)acetyl fluoride","359-34-2","D",0]
["4,4,4-Trifluoro-3-hydroxybut-2-enenitrile","139516-73-7","D",0]
["Acetic acid, trifluoro-, 1-methylethenyl ester","400-39-5","D",0]
["1,2,4,5-Tetrafluoro-3,6-bis(pentafluoro-lambda~6~-sulfanyl)benzene","1219501-60-6","D",0]
["1,4-Bis(trifluoromethyl)cyclohexa-1,3-dien-5-yne","919989-48-3","D",0]
["1,1,3,3,3-Pentafluoro-2-methylprop-1-ene","2253-00-1","D",0]
["Dimethyl(pentafluorophenyl)borane","363596-54-7","D",0]
["5,7-Bis(trifluoromethyl)imidazo[1,2-a]pyrimidine","1027511-38-1","D",0]
["1,1'-[Oxybis(methylene)]bis[3,5-bis(trifluoromethyl)benzene]","189446-57-9","D",0]
["N-[4-Bromo-3-(trifluoromethyl)phenyl]-2,2,2-trifluoroacetamide","156425-50-2","D",0]
["1,1,1,3,3-Pentafluoropropan-2-ol","1814-89-7","D",0]
["3,3,3-Trifluoropropan-1-amine--hydrogen chloride (1/1)","2968-33-4","D",0]
["1,2,3-Trifluorocyclopropane","143316-99-8","D",0]
["2-chloro-1,3,5-tris(trifluoromethyl)benzene","444-38-2","D",0]
["5-(Trifluoromethyl)pyrimidine","176214-12-3","D",0]
["1,1,1-Trifluorohexa-2,4-diene","651724-50-4","D",0]
["Zinc bis[bis(trifluoromethanesulfonyl)azanide]","168106-25-0","D",0]
["2-Nitro-1-(trifluoromethoxy)-4-(trifluoromethyl)benzene","104678-93-5","D",0]
["6:2 Fluorotelomer thioether propanoylalanylalaninate",null,"D",0]
["2,3,5,6-Tetrafluoro-4-hydroxybenzaldehyde","24336-73-0","D",0]
["Butanal, 4,4,4-trifluoro-3-oxo-","70817-53-7","D",0]
["Methoxymethane--1,1,2-trifluoroethene (1/1)","660821-32-9","D",0]
["2-(Trifluoromethyl)phenyl trifluoromethanesulfonate","199188-29-9","D",0]
["Tetrakis[3,5-bis(trifluoromethyl)phenyl]silane","918654-64-5","D",0]
["5,5,5-Trifluoro-3-(trifluoromethyl)pent-3-en-2-ol","32885-94-2","D",0]
["DIG(Pfp)2","158573-58-1","D",0]
["Cerium(4+) trifluoromethanesulfonate--water (1/4/1)","206996-62-5","D",0]
["3,3,3-Trifluoro-1-(trifluoromethoxy)prop-1-yne","63904-24-5","D",0]
["3,6-Difluoro-4-(trifluoromethyl)pyridin-2-amine","675602-89-8","D",0]
["4,6-bis(trifluoromethyl)-1H-pyrazolo[3,4-b]pyridin-3-ol","89990-37-4","D",0]
["Methanesulfonamide, 1,1,1-trifluoro-N-sulfinyl-","28048-19-3","D",0]
["2-Methyl-4-(trifluoromethyl)-1H-imidazole","33468-67-6","D",0]
["4,4,4-Trifluoro-1-[3-(trifluoromethyl)phenyl]butane-1,3-dione","94856-24-3","D",0]
["2-Sulfanylidene-4,6-bis(trifluoromethyl)-2,3-dihydropyridine-3-carbonitrile","265665-03-0","D",0]
["4,5-difluoro-2-(trifluoromethyl)benzaldehyde","134099-22-2","D",0]
["Arsine, dimethyl(trifluoromethyl)-","421-31-8","D",0]
["3-Fluoro-2,2-bis(fluoromethyl)propanoyl chloride","112433-49-5","D",0]
["2-fluoro-4-(trifluoromethyl)aniline","69409-98-9","D",0]
["(Difluoroamino)(difluoro)ethanimidamide","115983-81-8","D",0]
["1-(1,2-Difluoroethenyl)-3-(trifluoromethyl)benzene","316173-89-4","D",0]
["Silane, dichloromethyl(3,3,3-trifluoropropyl)-","675-62-7","D",0]
["2,3,5,6-Tetrafluoro-4-hydroxybenzonitrile","19161-30-9","D",0]
["1,1,2-Trifluoro-2-(trifluoromethoxy)ethane-1-sulfonic acid","905363-45-3","D",0]
["Tetrakis(2,2,2-trifluoroethyl) orthosilicate","338-39-6","D",0]
["2-Butynenitrile, 4,4,4-trifluoro-","66051-48-7","D",0]
["2-Chloro-2-[chloro(fluoro)methoxy]-1,1,1-trifluoroethane","172103-18-3","D",0]
["6:2 Fluorotelomer thioether propanoyl oxy propanoate",null,"D",0]
["alpha,alpha,alpha,alpha',alpha',alpha'-Hexafluoro-5-nitroxylene","328-75-6","D",0]
["1,2,3,4,5-Pentafluoro-6-(3,3,3-trifluoroprop-1-en-2-yl)benzene","59163-65-4","D",0]
["3-Fluoro-5-(trifluoromethyl)benzonitrile","149793-69-1","D",0]
["3,5-Bis(trifluoromethyl)-4H-1,2,4-triazol-4-amine","103797-41-7","D",0]
["2,2-Bis(trifluoromethanesulfonyl)ethen-1-amine","58510-92-2","D",0]
["1,1,4,4,4-Pentafluoro-2-(trifluoromethyl)but-1-ene","400-17-9","D",0]
["2,4,6-Trifluorohexa-2,3-dien-5-ynenitrile","923294-41-1","D",0]
["1-[3,5-Difluoro-4-(trifluoromethyl)phenyl]ethan-1-one","1189359-39-4","D",0]
["1-(4-Chloropyridin-2-yl)-2,2,2-trifluoroethyl trifluoromethanesulfonate","1356087-54-1","D",0]
["1,1,2-Trichloro-1-fluoro-2-(trifluoromethoxy)ethane","94720-90-8","D",0]
["1-Methyl-2,4-bis[(trifluoromethyl)sulfanyl]-1H-pyrrole","62665-38-7","D",0]
["Bis(3,5-di(trifluoromethyl)phenyl)chlorophosphine","142421-57-6","D",0]
["3-(Perfluoroethyl)-2-oxopropanesulfonic acid",null,"D",0]
["2-chloro-5-nitro-1,3-bis(trifluoromethyl)benzene","2375-97-5","D",0]
["3-Fluoro-4-(trifluoromethyl)benzaldehyde","204339-72-0","D",0]
["Tris(difluoromethyl)(fluoromethyl)silane","61152-92-9","D",0]
["Hexafluoromethanediamine","4394-93-8","D",0]
["1,2,3,4,5-pentafluoro-6-(2,3,5,6-tetrafluoro-4-methylphenoxy)benzene","20546-13-8","D",0]
["2,2,2-Trifluoro-N-(hydroxymethyl)acetamide","50667-69-1","D",0]
["{[1-Ethoxy-4,4-difluoro-3-(trifluoromethyl)but-3-en-1-yl]sulfanyl}benzene","62378-60-3","D",0]
["5,7-Bis(trifluoromethyl)pyrazolo[1,5-a]pyrimidine-3-carbonitrile","175276-40-1","D",0]
["2,3,5,6-Tetrafluoro-N,N-dimethylaniline","3228-14-6","D",0]
["2,3-Dibromo-1,1,2-trifluoropropane","1309602-74-1","D",0]
["2-Chloro-1,1,3,3-tetrafluoro-3-methoxyprop-1-ene","63176-09-0","D",0]
["1-Pentene, 5-bromo-4-chloro-4,5,5-trifluoro-","89965-95-7","D",0]
["3,5-bis(trifluoromethyl)-1,2,4-oxadiazole","4314-43-6","D",0]
["2,1,3-Benzoselenadiazole","19227-22-6","D",0]
["1,2,3,5-tetrafluoro-4,6-bis[2,3,5,6-tetrafluoro-4-(trifluoromethyl)phenoxy]benzene","15038-90-1","D",0]
["1-Propene, 1,1,3-trichloro-2,3,3-trifluoro-","684-06-0","D",0]
["Methanesulfonic acid, trifluoro-, tris(pentafluorophenyl)silyl ester","844504-52-5","D",0]
["3-Fluoro-5-(trifluoromethyl)pyridin-2(1H)-one","1040683-15-5","D",0]
["2,3,4,5-Tetrafluorobenzyl alcohol","53072-18-7","D",0]
["Ammonium trifluoromethanesulfonate","38542-94-8","D",0]
["2-[3,5-Bis(trifluoromethyl)phenyl]ethan-1-amine","181772-08-7","D",0]
["3,5,6-Trifluoropyridin-2(1H)-one","75777-49-0","D",0]
["1,2,3,4-Tetrafluorobutane","119382-47-7","D",0]
["3,3,3-Trifluoro-1-iodoprop-1-yne","39130-85-3","D",0]
["3,3,3-Trichloro-1,1,2-trifluoroprop-1-ene","431-57-2","D",0]
["Trifluoromethyl carbonocyanidate","87414-34-4","D",0]
["2,3,4,6-Tetrafluorobenzoyl chloride","123016-51-3","D",0]
["2,3-Difluorophenyl trifluoromethanesulfonate","211315-75-2","D",0]
["Propan-2-yl 3,3-difluoro-2-(trifluoromethyl)prop-2-enoate","62935-22-2","D",0]
["[2-Fluoro-4-(trifluoromethyl)phenyl]methanol","197239-49-9","D",0]
["1,3,4-Thiadiazol-2-amine, 5-(trifluoromethyl)-","10444-89-0","D",0]
["2,2-Difluoroethanol","359-13-7","D",0]
["6-Ethoxy-2,2,4-trifluoro-3-(trifluoromethyl)-2H-pyran","62116-53-4","D",0]
["1,1,1,3,3-Pentafluoro-3-(1,2,2-trifluoro-2-methoxyethoxy)propan-2-one","88457-04-9","D",0]
["Yttrium hexafluoroacetylacetonate","18911-76-7","D",0]
["(Pentafluorophenyl)hydrazine","828-73-9","D",0]
["4-Chloro-1-fluoro-2-(trifluoromethyl)benzene","89634-74-2","D",0]
["2,2'-(6-Methylpyridine-2,4-diyl)bis{2-[chloro(difluoro)methyl]-3,3,3-trifluoropropan-1-ol}","102206-52-0","D",0]
["[(Pentafluorophenyl)methyl]phosphonic acid","137174-84-6","D",0]
["Fluorobis[3-(trifluoromethyl)phenyl]borane","144364-26-1","D",0]
["2,2,2-Trifluoro-N,N-dimethylacetamide","1547-87-1","D",0]
["Dioxirane, methyl(trifluoromethyl)-","115464-59-0","D",0]
["1,3,5-trifluoro-2-(2,4,6-trifluorophenyl)benzene","41860-46-2","D",0]
["1-(1-Bromo-2,2,2-trifluoroethoxy)-2-chloro-1,1,2-trifluoroethane","51410-34-5","D",0]
["2,2,2-Trifluorodiazoethane","371-67-5","D",0]
["9-Chloroperfluoro-5-methyl-3,6-dioxanonanoic acid",null,"D",0]
["4-Bromo-2-fluoro-5-(trifluoromethyl)aniline","104460-70-0","D",0]
["calcium;1,1,1,5,5,5-hexafluoro-4-oxopent-2-en-2-olate","121012-90-6","D",0]
["Bis(trifluoromethyl)iodophosphine","359-64-8","D",0]
["1,4-Benzenediamine, 2,3,5,6-tetrafluoro-","1198-64-7","D",0]
["1-Chloro-2-[chloro(fluoro)methoxy]-1,2,3,3-tetrafluorocyclopropane","58707-63-4","D",0]
["4,5-Dichloro-2,2,4-trifluoro-1,3-dioxolane","89444-47-3","D",0]
["3,3,3-Trifluoropropanoate","74123-20-9","D",0]
["1-(Pentafluorophenyl)but-2-en-1-one","604007-02-5","D",0]
["Trifluoro(~3~H)methane","811-69-8","D",0]
["2,2',3,3',5,5',6,6'-Octafluoro(1,1'-biphenyl)-4,4'-dithiol","21386-21-0","D",0]
["1,1,3,3-Tetrachloro-2,2,4,5,6,7-hexafluoro-2,3-dihydro-1H-indene","88953-04-2","D",0]
["Silanamine, N-[dimethyl(3,3,3-trifluoropropyl)silyl]-1,1-dimethyl-1-(3,3,3-trifluoropropyl)-","39482-87-6","D",0]
["4-(Trifluoromethyl)pyridazine","132537-44-1","D",0]
["N-(2,4-Difluorophenyl)hypofluorous amide","204757-21-1","D",0]
["4-Amino-5,5,5-trifluoropent-3-en-2-one","70168-20-6","D",0]
["1,2,3,4,5-Pentafluoro-6-(2,3,5,6-tetrafluorophenoxy)benzene","14055-48-2","D",0]
["Methyl (trifluoromethyl)carbonofluoridimidate","61699-91-0","D",0]
["1,1,1-Trifluorohexan-2-amine","684-73-1","D",0]
["O-(4,4,4-Trifluorobutyl)hydroxylamine--hydrogen chloride (1/1)","676525-70-5","D",0]
["2-Fluoroethan-1-amine--hydrogen fluoride (1/1)","63186-88-9","D",0]
["5-Chloro-2,3,4-trifluorobenzoyl fluoride","101513-69-3","D",0]
["Methanesulfenamide, 1,1,1-trifluoro-N-[(trifluoromethyl)thio]-","763-24-6","D",0]
["5-Bromo-1,2-difluoro-3-(2,2,2-trifluoroethoxy)benzene","947534-36-3","D",0]
["Benzoyl fluoride, 4-(trifluoromethyl)-","368-94-5","D",0]
["2-Methyl-5-(trifluoromethyl)tetrazole","768-27-4","D",0]
["2-Fluoro-4-(trifluoromethoxy)phenol","1073477-74-3","D",0]
["1,1,3,3-Tetrafluoropropane","66794-30-7","D",0]
["2-chloro-3,3,3-trifluoroprop-1-ene","2730-62-3","D",0]
["2,4-difluoro-3-(trifluoromethyl)benzoic Acid","157337-81-0","D",0]
["2,3-Difluoro-4-(trifluoromethyl)benzene-1-carbothioamide","820960-59-6","D",0]
["Silylmethyl trifluoroacetate","67445-54-9","D",0]
["Bis(trifluoromethyl)arsane","371-74-4","D",0]
["2-Chloro-1,1,1-trifluoropropane","421-47-6","D",0]
["4-Dimethylaminoheptafluorotoluene","28012-10-4","D",0]
["2-Bromo-3,5-bis(trifluoromethyl)aniline","174824-16-9","D",0]
["Copper, (pentafluorophenyl)-","18206-43-4","D",0]
["1-[Chloro(difluoro)methyl]-2-(trifluoromethyl)benzene","312-91-4","D",0]
["Bromodifluoromethane","1511-62-2","D",0]
["4-((Perfluoro-3-nonen-1-yl)oxy)benzylphosphonic acid",null,"D",0]
["2,3-dibromo-1,1,1,3-tetrafluoropropane","501435-65-0","D",0]
["Bis(2,3,5,6-tetrafluoro-4-hydroxyphenyl)mercury--water (1/1)","873889-26-0","D",0]
["3-Bromo-2,2,3-trifluoropropanoic acid","679-95-8","D",0]
["4-Bromo-1-fluoro-2-(trifluoromethoxy)benzene","886496-45-3","D",0]
["(1E)-N-(2,2,2-Trifluoroethyl)butan-1-imine","80395-39-7","D",0]
["1,2-dichloro-1,1,4,4,4-pentafluorobut-2-ene","54815-10-0","D",0]
["(Trifluoromethyl)arsane","420-42-8","D",0]
["2,3-Difluoro-6-(trifluoromethyl)benzenecarboximidamide",null,"D",0]
["(Chloromethyl)(trifluoromethyl)phosphinic chloride","105263-72-7","D",0]
["(3E)-1,1,1,5,5,5-Hexafluoro-4-hydroxypent-3-en-2-one--copper--water (2/1/1)","155640-85-0","D",0]
["4-(Difluoromethyl)-2-fluoro-1-(trifluoromethyl)benzene","1214383-47-7","D",0]
["5-Bromo-2-fluorobenzotrifluoride","393-37-3","D",0]
["2-Chloro-3-fluoro-5-(trifluoromethyl)pyridine","72600-67-0","D",0]
["N,N-Diethyl-2,3,5,6-tetrafluoro-4-(trifluoromethyl)aniline","186753-43-5","D",0]
["1,1,1-Trifluoro-3-methylpentan-2-amine","1242339-44-1","D",0]
["1,2,4-Trifluorobicyclo[2.2.0]hexa-2,5-diene","21892-54-6","D",0]
["2,2,4,4-Tetrafluoro-3-oxopentanedioyl difluoride","78354-43-5","D",0]
["(3,5-Bis{[3,5-bis(trifluoromethyl)phenyl]methoxy}phenyl)methanol","881689-01-6","D",0]
["NSC174333","18058-10-1","D",0]
["Methyl N-(2,3,4,5,6-pentafluorophenyl)carbamate","6357-28-4","D",0]
["N-(Trifluoromethyl)methanimine N-oxide","88673-17-0","D",0]
["ST51006781","207605-39-8","D",0]
["2,2-Difluoropropanoic anhydride","173900-46-4","D",0]
["1,2,3,4-Tetrafluoro-5-(trifluoromethyl)benzene","654-53-5","D",0]
["Bromo(chloro)(chlorosulfanyl)[(trifluoromethyl)sulfanyl]methane","61363-04-0","D",0]
["n-(pentafluorophenyl)thiourea","715-60-6","D",0]
["(Trifluoromethoxy)silane","25711-11-9","D",0]
["Difluoro(fluorosulphonyl)acetyl fluoride","677-67-8","D",0]
["Pentafluorophenyl difluoro(fluorosulfonyl)acetate","89847-86-9","D",0]
["Copper(I) Trifluoromethanethiolate","3872-23-9","D",0]
["2,3,5,6-Tetrafluoro-4-(methylsulfanyl)pyridine","67644-45-5","D",0]
["2,5-Bis(trifluoromethyl)[1,2,4]triazolo[1,5-a]pyrimidin-7(1H)-one","198953-52-5","D",0]
["Sodium pentafluorobenzoate","4830-57-3","D",0]
["Tris(2,2,2-trifluoroethyl) N-(methanesulfonyl)phosphorimidate","378795-41-6","D",0]
["2-[3,5-Bis(trifluoromethyl)phenyl]-N-methylhydrazine-1-carboximidic acid","23152-45-6","D",0]
["Trifluoro(trifluoromethyl)silane","335-06-8","D",0]
["(1,2,3,4,5-Pentafluorocyclopenta-2,4-dien-1-yl)phosphane","89935-80-8","D",0]
["Dimethylbis(3,3,3-trifluoroprop-1-yn-1-yl)stannane","29723-42-0","D",0]
["5-(trifluoromethyl)-4,5-dihydroisoxazol-5-ol","134219-67-3","D",0]
["Benzene, 1-chloro-2,3-difluoro-5-(trifluoromethyl)-","77227-99-7","D",0]
["3,4,5,6,7-Pentafluoro-2-(trifluoromethyl)-1H-inden-1-one","62245-52-7","D",0]
["1,1,1-Trifluoro-6-iodohexane","104504-31-6","D",0]
["6,6,6-Trifluorohex-1-en-3-one","62333-52-2","D",0]
["Methyl 3,3,3-trifluoro-2-(fluorocarbonothioyl)propanoate","651719-50-5","D",0]
["1,3-Butadiene, 1,1-difluoro-","590-91-0","D",0]
["2,6-Difluoro(~13~C_6_)aniline","1173018-45-5","D",0]
["5,7-Bis(trifluoromethyl)-4-chloroquinoline","234450-34-1","D",0]
["Heptafluoroisoquinoline","13180-39-7","D",0]
["Acetanilide, 4'-chloro-2,2,2-trifluoro-3'-(trifluoromethyl)-","90830-15-2","D",0]
["Acetic acid, oxo-, 2,2,2-trifluoroethyl ester","172332-66-0","D",0]
["4,4,4-trifluorobutanal","406-87-1","D",0]
["Bis(perfluoromethylsulfonyl)imide anion","98837-98-0","D",0]
["Propanedioic acid, bis(2,2,2-trifluoroethyl) ester","104883-33-2","D",0]
["1,3-Difluoro-2-(trifluoromethyl)benzene","64248-60-8","D",0]
["Ethene, 2-chloro-1,1-difluoro-","359-10-4","D",0]
["3-[Chloro(difluoro)methyl]-4,4,4-trifluoro-3-hydroxybutanal","100482-83-5","D",0]
["2,3-Bis[(trifluoromethyl)sulfanyl]propan-1-ol","825628-55-5","D",0]
["(Ethane-1,2-diyl)bis[bis(pentafluorophenyl)phosphane]","76858-94-1","D",0]
["1-Isocyanato-3,5-bis(trifluoromethyl)benzene","16588-74-2","D",0]
["(2R)-1,1,1-Trifluoropropan-2-amine--hydrogen chloride (1/1)","177469-12-4","D",0]
["2,4-DiF 5-CF3 acetanilide","143360-15-0","D",0]
["4,4,4-Trifluoro-N-(4,4,4-trifluorobutyl)butanimidic acid","84138-08-9","D",0]
["1-(Trifluoromethyl)cyclopropane-1-carbonitrile","96110-56-4","D",0]
["5-fluoro-2-(trifluoromethyl)benzaldehyde","90381-08-1","D",0]
["3-Chloro-4-[1,1,2-trifluoro-2-(trifluoromethoxy)ethoxy]aniline","116714-47-7","D",0]
["2,5-Difluoro-4-(trifluoromethyl)benzoic acid","261945-05-5","D",0]
["Hypofluorous acid, trifluoromethyl ester","373-91-1","D",0]
["2,4-Dichloro-5-fluoro-6-(trifluoromethyl)pyrimidine","96819-53-3","D",0]
["1,3,3-Trifluoroprop-1-yne","66293-25-2","D",0]
["Butane, 1-[(trifluoromethyl)thio]-","7412-26-2","D",0]
["3-fluoro-2-(trifluoromethyl)benzonitrile","261951-81-9","D",0]
["Difluoromethanol","1426-06-8","D",0]
["1-[3,5-Bis(trifluoromethyl)phenyl]methanamine--hydrogen chloride (1/1)","42365-62-8","D",0]
["2-Chloro-4,4,4-trifluoro-3-oxobutanenitrile","192208-84-7","D",0]
["2,3,5-Trifluoro-6-methoxy-4-(1,2,2-trifluoro-2-methoxyethyl)pyridine","62452-44-2","D",0]
["1,2-Dichloro-1,1,2,4,4-pentafluoro-4-iodobutane","757-01-7","D",0]
["2,2,4-trichloro-1,1,1-trifluorobutane","175401-04-4","D",0]
["2-Fluoro-6-(trifluoromethyl)benzyl alcohol","152211-15-9","D",0]
["2,4,6-Tris(trifluoromethyl)-1H-benzimidazole","185412-89-9","D",0]
["2-[3,5-bis(trifluoromethyl)phenyl]-2-methylpropanoic acid","289686-70-0","D",0]
["1-Bromo-2,3,4,5-tetrafluorobenzene","1074-91-5","D",0]
["3,3,3-Trifluoro-2-methylpropan-1-ol","431-23-2","D",0]
["2-phenyl-4,6-bis(trifluoromethyl)-1,3,5-triazine","30362-32-4","D",0]
["S-(Trifluoromethyl) carbamothioate","67756-33-6","D",0]
["1‐Bromo‐1‐chloro‐1‐(difluoromethoxy)‐2,2,2‐trifluoroethane","236109-00-5","D",0]
["2,4,4,4-Tetrafluorobut-2-en-1-ol","91600-37-2","D",0]
["1,1-Bis[3,5-bis(trifluoromethyl)phenyl]-2-methyl-3-(pyrrolidin-1-yl)propan-1-ol--hydrogen chloride (1/1)","70648-08-7","D",0]
["2,4,6-Trifluoropyridine","3512-17-2","D",0]
["Perfluorophenyl isocyanate","1591-95-3","D",0]
["Benzene, 1,2,4-tris(trifluoromethyl)-","393-05-5","D",0]
["(Trifluoromethyl)mercuric bromide","421-09-0","D",0]
["1,3-Difluoro-4-nitro-2-(trifluoromethyl)benzene","123973-36-4","D",0]
["2-(Trifluoromethyl)cyclopentan-1-amine","1260678-84-9","D",0]
["1,1,4,4-Tetrafluoro-1,3-butadiene","407-70-5","D",0]
["Methanamine, N-[(pentafluorophenyl)methylene]-","62454-76-6","D",0]
["Bis(1-amino-2,2,2-trifluoroethylidene)butanedinitrile","192521-74-7","D",0]
["1,1-Dibromo-2-chloro-1,2,2-trifluoroethane","10057-30-4","D",0]
["2,5-Bis[(trifluoroethenyl)oxy]hexane","134130-28-2","D",0]
["Benzenamine, 4-bromo-N,N-bis(2,2,2-trifluoroethy",null,"D",0]
["2,3-Difluorobenzotrifluoride","64248-59-5","D",0]
["1,2,3,4,5,6,8-Heptafluoro-7-(pentafluorophenyl)naphthalene","57020-28-7","D",0]
["Stannane, trichloro[2,4,6-tris(trifluoromethyl)phenyl]-","650583-82-7","D",0]
["1-Fluoro-4-(trifluoromethanesulfinyl)benzene","942-39-2","D",0]
["1-Chloro-3-fluoro-2-(trifluoromethyl)benzene","103889-37-8","D",0]
["Difluoromethyl difluoromethanesulfonate","101817-80-5","D",0]
["Lanthanum tris(trifluoroacetate)","70236-92-9","D",0]
["7,8,9,10,11,12-Hexafluoro-1,2,3,4,5,6,6a,12a-octahydrooctalene","112313-06-1","D",0]
["Pentafluorophenyl prop-2-enoate","71195-85-2","D",0]
["N-Methyl-N'-(trifluoromethyl)urea","56969-92-7","D",0]
["1,1'-(Buta-1,3-diyne-1,4-diyl)bis[2,5-bis(trifluoromethyl)benzene]","90735-56-1","D",0]
["Dimethyl{bis[(trifluoroacetyl)oxy]}stannane","650-22-6","D",0]
["1,1,3-Trichloro-1,2,2,3-tetrafluoropropane","422-53-7","D",0]
["2,3,4,5-Tetrafluorobenzonitrile","16582-93-7","D",0]
["2,5-Bis(trifluoromethyl)benzenesulfonyl chloride","351003-22-0","D",0]
["Heptafluorobutan(~2~H)oic acid",null,"D",0]
["2,2,2,3',4'-Pentafluoroacetophenone","302912-28-3","D",0]
["(3Z,3'Z,3''Z)-4,4',4''-[bismuthinetriyltris(oxy)]tris(1,1,1,5,5,5-hexafluoropent-3-en-2-one)","141364-06-9","D",0]
["3-fluoro-4-chlorobenzotrifluoride","32137-20-5","D",0]
["Benzenamine, 2,4,6-trifluoro-3-(trifluoromethyl)-","123973-32-0","D",0]
["1,1,1-trifluoro-2-heptene","66716-12-9","D",0]
["2,4,5,6-Tetrafluoro-3-iodo-1H-azepine","923294-25-1","D",0]
["[(Trifluoromethyl)sulfanyl]methanesulfinyl chloride","61363-07-3","D",0]
["3,3,3-trifluoro-2-oxopropanamide","883500-27-4","D",0]
["(2Z)-2,3-dichloro-1,1,1,4,4,4-hexafluorobut-2-ene","2418-22-6","D",0]
["2-(Trifluoromethyl)pyrrolidine","109074-67-1","D",0]
["1,2,4,5-Tetrafluorobenzene--water (1/1)","827046-85-5","D",0]
["Trimethyl(1,1,2-trifluoroethyl)silane","62281-30-5","D",0]
["Bromo(difluoro)methaneselenenyl bromide","62247-72-7","D",0]
["2,4,6-Trimethyl-3,5-bis(trifluoromethyl)aniline","90679-50-8","D",0]
["1-Butanamine, 4,4,4-trifluoro-, hydrochloride (1:1)","84153-82-2","D",0]
["Phosphorothioic O,O,O-acid--2,2,2-trifluoroethan-1-ol (1/3)","101153-71-3","D",0]
["1-(Trifluoroethenyl)-3-(trifluoromethyl)benzene","82907-02-6","D",0]
["1-Chloro-2-(dichloromethoxy)-1,2,3,3-tetrafluorocyclopropane","58707-61-2","D",0]
["2-Bromo-6-fluorobenzotrifluoride","261951-85-3","D",0]
["1-[3,5-bis(trifluoromethyl)phenyl]pyrrole","175136-60-4","D",0]
["Dibromodifluoromethane","75-61-6","D",0]
["4-[Chloro(difluoro)methyl]-5,5,5-trifluoropenta-1,3-diene","31506-41-9","D",0]
["1,1,3,4,5,6,7-Heptafluoro-2-(trifluoromethyl)-1H-indene","62245-51-6","D",0]
["2-Methyl-2-(2,2,2-trifluoroethoxy)propane","80054-67-7","D",0]
["1,4,5,6,7,8-Hexafluoro-3-(trifluoromethyl)isoquinoline","63485-11-0","D",0]
["3,5-Bis(trifluoromethyl)benzyl bromide","32247-96-4","D",0]
["2-Fluoro-5-(trifluoromethyl)benzyl alcohol","207974-09-2","D",0]
["Diaziridine, tetrafluoro-","17224-09-8","D",0]
["Tris[3,5-bis(trifluoromethyl)phenyl]phosphine","175136-62-6","D",0]
["Hexafluorooxepine","129193-79-9","D",0]
["Bis(pentafluorophenyl)dimethylsilane","10536-62-6","D",0]
["3,3,3-Trifluoropropanenitrile","20530-38-5","D",0]
["Methyl 2-bromo-3,3,3-trifluoropropanoate","113816-36-7","D",0]
["1,2,3,3,4,6,6-Heptafluoro-5-nitrocyclohexa-1,4-diene","79150-78-0","D",0]
["O-(2,3,4,5,6-Pentafluorobenzyl)hydroxylamine","72915-12-9","D",0]
["2-(Pentafluorophenyl)acetamide","653-20-3","D",0]
["Methyl {[bis(2,2,2-trifluoroethoxy)phosphoryl]oxy}acetate","132549-38-3","D",0]
["2,2,2-trifluoro-N',N'-dimethylethanethiohydrazide","4454-48-2","D",0]
["4,5-difluoro-2-(trifluoromethyl)benzamide","261944-97-2","D",0]
["2,3,5,6-Tetrafluoropyridine-4(1H)-thione","19736-58-4","D",0]
["3-(2,2,2-Trifluoroethoxy)propanenitrile","272128-06-0","D",0]
["11-Chloro-3,3,5,5,7,7,9,9,11,11-decafluoroundecanoic acid","76140-48-2","D",0]
["1,2-Difluorocycloprop-1-ene","111395-80-3","D",0]
["4,4,4-Trifluorobutyl thiocyanate","212190-13-1","D",0]
["Perfluoro-1,3,5-hexatriene","392-52-9","D",0]
["4,5,6,7-Tetrafluoroindoline","19282-55-4","D",0]
["methyl 2,2,2-trifluoroethanimidate","815-07-6","D",0]
["Copper (II) Trifluoroacetate","123333-88-0","D",0]
["Silane, trimethyl(3,3,3-trifluoro-1-propynyl)-","6618-09-3","D",0]
["Ethane, 1,1-dibromo-1-chloro-2,2,2-trifluoro-","754-17-6","D",0]
["Dysprosium(III) trifluoromethanesulfonate","139177-62-1","D",0]
["Benzene, 2-chloro-1-fluoro-4-(trifluoromethyl)-","78068-85-6","D",0]
["5-Bromo-1,1,1-trifluoropentane","54932-74-0","D",0]
["2-(Trifluoromethyl)thiirane","87612-18-8","D",0]
["Samarium(III) trifluoromethanesulfonate","52093-28-4","D",0]
["2,3,5,6-Tetrafluoroaniline","700-17-4","D",0]
["3,5,6-Trifluoro-1,2,4-triazine","75995-67-4","D",0]
["2-Chloro-1,1,2-trifluoroethane-1-thiol","1827-50-5","D",0]
["Bis(pentafluorophenyl)ditellane","20196-25-2","D",0]
["3-(Trifluoromethoxy)prop-1-ene","140899-21-4","D",0]
["2,3-dichloro-1,1,1,4,4,4-hexafluorobutane","384-54-3","D",0]
["[2,6-Bis(trifluoromethyl)phenyl]methanol","152211-16-0","D",0]
["2-fluoro-6-(trifluoromethyl)phenol","239135-50-3","D",0]
["1,1,1-trifluorobut-2-ene","406-39-3","D",0]
["3,3-dichloro-4,4,4-trifluorobut-1-ene","175400-95-0","D",0]
["Potassium trifluoro[6-(trifluoromethyl)pyridin-3-yl]borate(1-)","1245906-75-5","D",0]
["Plumbane, dimethylbis(trifluoromethyl)-","67946-73-0","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,5,5,5-undecafluoro-N-[2-(2-hydroxyethoxy)ethyl]pentane-1-sulfonamide","958826-98-7","D",0]
["3-bromo-3-(trifluoromethyl)diazirine","117113-33-4","D",0]
["1,1-Difluoro-1-methoxyethane","162250-14-8","D",0]
["Trifluoromethanesulfonic acid--water (1/1)","49789-04-0","D",0]
["1-Chloro-1,2-difluoroethane","338-64-7","D",0]
["Bromotrifluoromethane","75-63-8","D",0]
["Methyl 3,5-di(trifluoromethyl)benzoate radical","26107-80-2","D",0]
["1,3,5-Trifluoro-2-methylbenzene","79348-71-3","D",0]
["1-Chloro-2-fluoro-5-iodo-3-(trifluoromethyl)benzene","928783-87-3","D",0]
["Thulium tris(trifluoroacetate)","70237-00-2","D",0]
["ST51042225","261924-41-8","D",0]
["1,1,1,4,4,4-hexafluoro-2,3-dimethylbutane-2,3-diol","16803-68-2","D",0]
["2,3,4,6-Tetrafluorophenyl isothiocyanate","84348-86-7","D",0]
["3-Bromo-1,1,3,3-tetrafluoropropene","460-61-7","D",0]
["1-Ethynyl-2,3,5,6-tetrafluoro-4-(trifluoromethyl)benzene","61794-56-7","D",0]
["1,7-Dichloro-2,6-bis[chloro(difluoro)methyl]-1,1,7,7-tetrafluoro-2,6-dihydroxy-3-methylheptan-4-one","101913-78-4","D",0]
["N,1,1,1-Tetrafluoro-N-[(trifluoromethyl)sulfonyl]methanesulfonamide","108388-06-3","D",0]
["1-Fluoro-4-(1,1,3,3,3-pentafluoroprop-1-en-2-yl)benzene","1979-54-0","D",0]
["Magnesium trifluoromethanesulfonate","60871-83-2","D",0]
["2,2,5,5-Tetrafluoro-1,4-diazabicyclo[2.2.2]octane","721451-54-3","D",0]
["pentafluorobenzenesulfonyl fluoride","36650-04-1","D",0]
["1,1-Difluoro-1-iodoethane","598-39-0","D",0]
["N,N-Bis(trifluoromethyl)hypofluorous amide","359-62-6","D",0]
["2-[3,5-bis(trifluoromethyl)phenyl]ethanethioamide","691868-49-2","D",0]
["1,3-bis[3,5-bis(trifluoromethyl)phenyl]urea","3824-74-6","D",0]
["2,3,5,6-tetrafluoro-4-methylpyridine","16297-14-6","D",0]
["trifluoromethylphosphonic acid;dichloride","51965-64-1","D",0]
["2-Fluoro-5-(trifluoromethyl)benzylamine","199296-61-2","D",0]
["Bromo[bis(pentafluorophenyl)]thallane","1735-62-2","D",0]
["2,7-Naphthyridine, 1,3,4,5,6,8-hexafluoro-","56595-14-3","D",0]
["2,4,6-Tris(pentafluorophenyl)pyridine","675583-26-3","D",0]
["3-[(Trifluoroethenyl)oxy]prop-1-ene","113991-42-7","D",0]
["Tris(pentafluorophenyl)(prop-2-en-1-yl)silane","856170-67-7","D",0]
["1,3,4,4-Tetrafluoro-3-(propylsulfanyl)cyclobut-1-ene","766547-35-7","D",0]
["2,3,5,6-Tetrafluoroisonicotinic acid","2875-10-7","D",0]
["1,1,1,3-Tetrafluorobutane","86884-13-1","D",0]
["3',5'-Bis(trifluoromethyl)propiophenone","85068-34-4","D",0]
["1,2-Dichloro-1,2,3,3-tetrafluoropropane","425-94-5","D",0]
["2,3,5,6-Tetrafluorophenyl isothiocyanate","20925-31-9","D",0]
["2-Fluoro-4-iodo-6-(trifluoromethyl)pyridine","957345-37-8","D",0]
["2,2,2-Trifluoro-N-[5-(trifluoromethyl)-1,3,4-thiadiazol-2-yl]acetamide","27603-23-2","D",0]
["Propane, 1-chloro-2,2,3-trifluoro-","56758-54-4","D",0]
["Difluoroiodomethane","1493-03-4","D",0]
["2-[3,5-bis(trifluoromethyl)phenyl]-N'-hydroxyethanimidamide","244022-74-0","D",0]
["Lithium, (1-chloro-2,2-difluoroethenyl)-","62269-27-6","D",0]
["2,2-Dichloro-1,1,1,3-tetrafluoropropane","149329-24-8","D",0]
["Bis(perfluoroethyl)fluorophosphate",null,"D",0]
["1,1,1-Trifluoropropane","421-07-8","D",0]
["2-Thiazolamine, 4-(trifluoromethyl)-","349-49-5","D",0]
["1-Bromo-2-fluoro-3-(trifluoromethoxy)benzene","1033202-63-9","D",0]
["1,1-Dichloro-2,2,3-trifluoropropane","70192-70-0","D",0]
["4,4',5,5'-Tetrakis(trifluoromethyl)-2,2'-bipyridine","142946-81-4","D",0]
["Acrylonitrile, 2-(trifluoromethyl)-","381-84-0","D",0]
["Methanesulfenamide, 1,1,1-trifluoro-N,N-dimethyl-","62067-13-4","D",0]
["N-[3,5-Bis(trifluoromethyl)phenyl]acetamide","16143-84-3","D",0]
["3-Iodopentafluoroprop-1-ene","431-65-2","D",0]
["Tin(II) trifluoromethanesulfonate","62086-04-8","D",0]
["Urea, (trifluoromethyl)-","61919-30-0","D",0]
["1,2,3,4,5-Pentafluoropentane","95576-19-5","D",0]
["Acetaldehyde, chlorodifluoro-","811-96-1","D",0]
["1,2,4,5-Tetrafluoro-3-phenoxy-6-(trifluoromethyl)benzene","42875-02-5","D",0]
["[2,6-Bis(trifluoromethyl)phenyl](trimethyl)stannane","55204-80-3","D",0]
["4-Bromo-2-fluorobenzotrifluoride","142808-15-9","D",0]
["1,1,1-Trifluoroacetylacetone","367-57-7","D",0]
["2-(Chloromethyl)-1-fluoro-3-(trifluoromethyl)benzene","1001096-10-1","D",0]
["1,2,3,4-Tetrakis(trifluoromethyl)-1,2-dihydro-1,2-diphosphete","2375-86-2","D",0]
["2,3,4,6-Tetrakis(trifluoromethyl)aniline","65537-99-7","D",0]
["p,alpha,alpha,alpha-Tetrafluoroanisole","352-67-0","D",0]
["1,1,1-Trifluoro-2-propanol","374-01-6","D",0]
["(3,5-Bis(trifluoromethyl)phenyl)acetonitrile","85068-32-2","D",0]
["1,1,3,3-Tetrafluorobutane","625-09-2","D",0]
["4-Bromo-3-chloro-3,4,4-trifluorobut-1-ene","374-25-4","D",0]
["Bromodifluoroacetyl fluoride","38126-07-7","D",0]
["1-Bromo-2-chloro-1,2-difluoroethene","2106-93-6","D",0]
["N-Ethyl-1,1,2,2,3,3,4,4,5,5,6,6,7,7,7-pentadecafluoro-N-[2-(2-hydroxyethoxy)ethyl]-1-heptanesulfonamide","958832-96-7","D",0]
["Triiodo(trifluoromethyl)germane","1512-08-9","D",0]
["2,3,5,6-Tetrafluoro-4-nitropyridine","3511-89-5","D",0]
["1,1,1-Trifluoro-4,4-bis(4,4,4-trifluorobutoxy)butane","933600-77-2","D",0]
["N,N,1-Trimethyl-1,1,1-tris(trifluoromethyl)-lambda~5~-phosphanamine","64937-81-1","D",0]
["2,3,3,4-Tetrafluoro-4-methylthiolane 1,1-dioxide",null,"D",0]
["Trifluoropyruvyl fluoride","7309-82-2","D",0]
["1,1-Difluoroethane","75-37-6","D",0]
["1-[3,5-Bis(trifluoromethyl)phenyl]-N-methylethan-1-amine","290297-43-7","D",0]
["3-Bromo-2-(bromomethyl)-1,1,1-trifluoropropane","1263377-32-7","D",0]
["2-(Difluoromethyl)-1,3,5-trifluorobenzene","1214338-85-8","D",0]
["Pyridine, 3-chloro-2,4,5,6-tetrafluoro-","1735-84-8","D",0]
["Phosphinous acid, bis(trifluoromethyl) ester","359-65-9","D",0]
["Trifluoromethanesulfonic anhydride","358-23-6","D",0]
["2,2-difluoroacetamide","359-38-6","D",0]
["Oxirane--1,1,2-trifluoroethene (1/1)","923587-99-9","D",0]
["Tris[3,5-bis(trifluoromethyl)phenyl]arsane","240820-38-6","D",0]
["Benzene, 1,3-bis(trifluoromethyl)-5-isocyano-","141206-73-7","D",0]
["1,1,1-trifluorobutan-2-amine","683-94-3","D",0]
["(1R)-2,2,2-Trifluoro-1-[2-(trifluoromethyl)phenyl]ethan-1-amine","1213339-31-1","D",0]
["Tetrakis(trifluoromethyl)hydrazine","383-96-0","D",0]
["N-Hydroxypentafluoro benzamide","80684-62-4","D",0]
["2-Fluoro-6-(trifluoromethyl)benzaldehyde","60611-24-7","D",0]
["1-(Chloromethyl)-2,3,5,6-tetrafluoro-4-(trifluoromethyl)benzene","248262-31-9","D",0]
["Carbonimidoyl","2712-98-3","D",0]
["Silver triflimide","189114-61-2","D",0]
["Trimethyl(3,3,3-trifluoroprop-1-en-1-yl)silane","55364-28-8","D",0]
["1,1,1-Trifluorotrimethylamine","677-41-8","D",0]
["3,5-Bis(trifluoromethyl)cinnamic acid","155814-20-3","D",0]
["3-Chloro-1,1,1,3-tetrafluoro-4-iodobutane","885275-78-5","D",0]
["1,2-Dibromo-1,1-difluoroethane","75-82-1","D",0]
["2,2,2-Trifluoro-1-[3-(trifluoromethyl)-3H-diaziren-3-yl]ethan-1-one","87282-23-3","D",0]
["Stibine, methylbis(trifluoromethyl)-","684-20-8","D",0]
["2,3-Dichloro-1,1,1-trifluoropropane","338-75-0","D",0]
["2-[(2,2,2-Trifluoroethoxy)methyl]oxirane","1535-91-7","D",0]
["Chloro(dimethyl)(1,1,3,3,3-pentafluoropropyl)silane","62281-39-4","D",0]
["Carbonochloridodithioic acid, trifluoromethyl ester","1540-66-5","D",0]
["1-(2,3,5,6-Tetrafluoropyridin-4-yl)ethan-1-one","94220-36-7","D",0]
["4,4'-[(2,4,5,6-Tetrafluoro-1,3-phenylene)bis(oxy)]bis(tetrafluorobenzoic acid)","14901-49-6","D",0]
["1,1,1-Trifluoro-3-(trifluoromethanesulfonyl)propan-2-one","58510-76-2","D",0]
["1,1,2-Trifluoroethane","430-66-0","D",0]
["Bis(pentafluorophenyl) oxalate","16536-48-4","D",0]
["Hexafluoro-1,2-didehydronaphthalene","73501-12-9","D",0]
["2-Bromo-1,1,2-trifluoro-1-methoxyethane","679-90-3","D",0]
["1-(Trifluoromethyl)piperazine","78409-50-4","D",0]
["DIIODODIFLUOROMETHANE","1184-76-5","D",0]
["3-[3,5-Bis(trifluoromethyl)phenyl]-1,1,1-trifluoropropan-2-one","185338-32-3","D",0]
["Silver trifluoroacetate","2966-50-9","D",0]
["Octafluorostyrene","652-23-3","D",0]
["N,N'-Sulfonylbis(1,1,1-trifluoromethanesulfonamide)","174191-62-9","D",0]
["3-AZIDO-1,1,1-TRIFLUOROPROPAN-2-OL","212758-85-5","D",0]
["1,1-Difluoro-1-bromo-2-chloroethane","420-91-7","D",0]
["2-Chloro-4,4,5,5-tetrafluoro-3-[[3-(trifluoromethyl)phenyl]amino]-2-cyclopenten-1-one","5668-86-0","D",0]
["6-Fluoro-5-(trifluoromethyl)pyrimidine-2,4-diamine","93416-50-3","D",0]
["3,5-Bis(trifluoromethyl)-1H-pyrazole","14704-41-7","D",0]
["3-bromo-5-(trifluoromethyl)-1,2-oxazole","933673-61-1","D",0]
["(1E)-N-(2,2,2-Trifluoroethyl)propan-1-imine","80395-38-6","D",0]
["alpha,alpha,alpha-4-Tetrafluoro-m-toluidine","2357-47-3","D",0]
["Tris[3,5-bis(trifluoromethyl)phenyl]borane","169116-84-1","D",0]
["3,3',5,5'-Tetrakis(trifluoromethyl)benzophenone","175136-66-0","D",0]
["1-Chloro-2-[chloro(difluoro)methyl]-1,1-difluoropentan-2-ol","6301-99-1","D",0]
["Phenazine, octafluoro-","18232-24-1","D",0]
["4,4,4-Trifluorobutanol","461-18-7","D",0]
["Trifluoroacetylurea","760-41-8","D",0]
["N,N-Dimethyl-P-(trifluoromethyl)phosphonamidous chloride","3135-63-5","D",0]
["2-Fluoroacryloyl fluoride","60556-85-6","D",0]
["1,1,1-Trifluoro-3-({[2-(trifluoromethyl)phenyl]methyl}amino)propan-2-ol","453557-79-4","D",0]
["2,2-Difluoropropane-1,3-disulfonyl difluoride","110073-94-4","D",0]
["AGN-PC-0O2ZCH","422-42-4","D",0]
["2,2-dibromo-1,1,1-trifluoropropane",null,"D",0]
["NSC174334","14592-81-5","D",0]
["ethyl 3,3,3-trifluoropropanoate","352-23-8","D",0]
["Ethane, 1-bromo-1,2,2-trifluoro-","430-90-0","D",0]
["1,1,2,2-Tetrachloro-1,3,3,3-tetrafluoropropane","2268-44-2","D",0]
["3-(Methylsulfanyl)-5,6-bis(trifluoromethyl)-1,2,4-triazine","120943-60-4","D",0]
["1-Ethynyl-2,3,5,6-tetrafluoro-4-methylbenzene","61794-58-9","D",0]
["[(Trifluoromethyl)sulfanyl]acetyl chloride","1645-79-0","D",0]
["1,1,2-trifluoropenta-1,3-diene","123812-85-1","D",0]
["Trifluoro(iodosulfanyl)methane","102127-62-8","D",0]
["Iron(III) trifluoromethanesulfonate","63295-48-7","D",0]
["difluoroacetate","83193-04-8","D",0]
["1-Bromo-1-chloro-2,2,3-trifluorocyclopropane","24071-61-2","D",0]
["1,4-Dioxo-1,4-bis[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)oxy]butane-2-sulfonic acid","745725-85-3","D",0]
["1-Methyl-2,5-bis[(trifluoromethyl)sulfanyl]-1H-pyrrole","62665-37-6","D",0]
["Benzenethiol, pentafluoro-","771-62-0","D",0]
["Silane, trimethyl(trifluoroethenyl)-","1427-33-4","D",0]
["Bis(pentafluorophenyl)trisulfane","52082-75-4","D",0]
["Thianthrene, octafluoro-","16012-83-2","D",0]
["2,4,5-Trifluoroiodobenzene","17533-08-3","D",0]
["N,N'-(1,2-Phenylene)bis(trifluoroethanimidic acid)","14818-62-3","D",0]
["3-Fluoro-5-(trifluoromethyl)pyridine-2-carbaldehyde","1227499-98-0","D",0]
["Methylbis(3,3,3-trifluoropropyl)silane","659-73-4","D",0]
["(3-Chloro-1,1,3,3-tetrafluoroprop-1-en-2-yl)carbonimidoyl","64431-51-2","D",0]
["1H-Pyrazole, 3-methyl-5-(trifluoromethyl)-","10010-93-2","D",0]
["Butyraldehyde, 4-chloro-4,4-difluoro-3-hydroxy-3-(chlorodifluoromethyl)-","1690-52-4","D",0]
["Pentakis(trifluoromethyl)aniline","58956-76-6","D",0]
["3-Fluoro-2-(trifluoromethyl)benzyl bromide","261951-84-2","D",0]
["1,1,1-Trifluoro-3-methylhexa-2,4-diene","651724-51-5","D",0]
["1-Propen-2-ol, 3,3,3-trifluoro-, 2-acetate","2247-91-8","D",0]
["1,2,3-Butatriene, 1,1,4,4-tetrafluoro-","2252-95-1","D",0]
["NSC367452","81098-47-7","D",0]
["1,1,2,3,4-Pentafluorobutane","141529-32-0","D",0]
["3,6-Bis[(trifluoromethyl)sulfanyl]benzene-1,2-dicarbonitrile","67193-52-6","D",0]
["Potassium (2,6-difluorophenyl)(trifluoro)borate(1-)","267006-25-7","D",0]
["4-Fluoro-3-(trifluoromethoxy)aniline","113421-98-0","D",0]
["Bis(2,3,5,6-tetrafluoro-4-methoxyphenyl)diazene","2787-85-1","D",0]
["2-Diazonio-3,3,3-trifluoro-1-hydroxyprop-1-en-1-olate","65938-16-1","D",0]
["4-[3,5-Bis(trifluoromethyl)-1H-pyrazol-1-yl]aniline","123066-64-8","D",0]
["2,5-difluoro-4-(trifluoromethyl)benzamide","261944-82-5","D",0]
["2,2-Difluoro-N-methylethan-1-amine","60168-06-1","D",0]
["Naphthalene, 1,2,3,4,5,6,8-heptafluoro-","784-00-9","D",0]
["Sulfurous acid--pentafluorophenol (1/2)","96157-57-2","D",0]
["3,4-bis(trifluoromethyl)aniline","2965-07-3","D",0]
["Carbonotrithioic acid, bis(trifluoromethyl) ester","461-08-5","D",0]
["2,3,6-Trifluoropyridine","3512-18-3","D",0]
["2,3,4-Trifluoro-5-(trifluoromethyl)benzoic acid","203915-94-0","D",0]
["Trifluoroethenesulfonyl fluoride","684-10-6","D",0]
["1,1'-(Buta-1,3-diyne-1,4-diyl)bis(pentafluorobenzene)","18320-79-1","D",0]
["Sodium 1,2,3,4,5-pentafluorocyclopenta-2,4-dien-1-ide","90605-69-9","D",0]
["1,1,1-Tribromo-2,2,2-trifluoroethane","354-48-3","D",0]
["2-(trifluoromethyl)-4,5-dihydro-1H-imidazole","2794-20-9","D",0]
["1-(Trifluoromethanesulfonyl)prop-1-ene","61795-20-8","D",0]
["3,5-Bis(trifluoromethyl)-1,2-diaminobenzene","367-65-7","D",0]
["3-Bromo-1,1,2,3,3-pentafluoroprop-1-ene","431-56-1","D",0]
["1,1,2-Trifluoroethan-1-ol","28606-06-6","D",0]
["Benzenamine, 2-bromo-6-fluoro-3-(trifluoromethyl)-","116369-22-3","D",0]
["1,1,2-Trifluorobuta-1,3-diene","565-65-1","D",0]
["3,4,5,5-Tetrafluorothiophen-2(5H)-one","142453-20-1","D",0]
["1,2,3,4,5-Pentafluoro-6-[(1,1,3,3,3-pentafluoroprop-1-en-2-yl)oxy]benzene","62884-12-2","D",0]
["2-(Ethoxymethoxy)-1,1,1-trifluoroethane","674778-84-8","D",0]
["1,2,3,3-Tetrachloro-1,1,2-trifluoropropane","422-41-3","D",0]
["1,2,4-trichloro-1,1,2-trifluorobutane","261760-97-8","D",0]
["(2S)-1,1,1-Trifluorobutan-2-amine--hydrogen chloride (1/1)","101054-96-0","D",0]
["4-Heptanone, 2,6-bis(chlorodifluoromethyl)-1,7-dichloro-2,6-dihydroxy-1,1,7,7-tetrafluoro-, oxime","101913-80-8","D",0]
["2,2-Bis(fluoromethyl)-1,3-difluoropropane","338-23-8","D",0]
["3,3,3-Trifluoroprop-1-ene-2-sulfonyl fluoride","105380-16-3","D",0]
["5-Chloro-4,5,5-trifluoropent-1-ene","89965-94-6","D",0]
["1-Propene, 2-chloro-1,1,3,3,3-pentafluoro-","2804-50-4","D",0]
["Trifluoromethyl 3,3,3-trifluoropropanoate","93667-89-1","D",0]
["3,5-Bis(trifluoromethyl)benzene-1-carboximidamide--hydrogen chloride (1/1)","97603-94-6","D",0]
["di(pentafluorophenyl)dichlorosilane","20160-45-6","D",0]
["2-[(2,2,2-Trifluoroethyl)amino]ethan-1-ol","371-99-3","D",0]
["(3Z)-4-Amino-1,1,1-trifluoropent-3-en-2-one","72885-02-0","D",0]
["Stannane, dibutylbis(trifluoroethenyl)-","2127-90-4","D",0]
["(Chlorosulfonyl)(difluoro)acetyl fluoride","2561-57-1","D",0]
["1,1,1,4,4,4-Hexafluoro-2-methoxybutan-2-ol","94559-68-9","D",0]
["2,3,4,5,6-Pentafluorobenzylzinc chloride solution","308796-02-3","D",0]
["Pentafluoronitrosobenzene","1423-13-8","D",0]
["2,3,4,5,6,6-Hexafluorocyclohexa-2,4-dien-1-one","41481-22-5","D",0]
["NSC120072","12169-94-7","D",0]
["1-Ethyl-3-methyl-1H-imidazol-3-ium trifluoro(trifluoromethyl)borate(1-)","681856-28-0","D",0]
["3-Fluoro-5-(trifluoromethyl)phenol","172333-87-8","D",0]
["STK036962","304668-18-6","D",0]
["Ethane, 1,1-dichloro-2,2-difluoro-","471-43-2","D",0]
["Carbonothioic difluoride","420-32-6","D",0]
["1-[(Trifluoromethyl)sulfanyl]butan-2-ol","825628-49-7","D",0]
["Cerium(IV) trifluoromethanesulfonate","107792-63-2","D",0]
["Magnesium chloride 3,5-bis(trifluoromethyl)benzen-1-ide (1/1/1)","535949-95-2","D",0]
["2,2,3-Trifluoro-3-methylbutanoic acid","1785396-76-0","D",0]
["1-(Chloromethyl)-2,3,5,6-tetrafluoro-4-methylbenzene","60903-84-6","D",0]
["3-(Trifluoromethyl)-alpha,alpha,alpha-trifluoroacetophenone","721-37-9","D",0]
["1,1-dichloro-1,2,2-trifluoroethane","812-04-4","D",0]
["1,1-Difluoro-2-methylprop-1-ene","381-66-8","D",0]
["4,4,4-Trifluoro-3-(silyloxy)butanal","834880-87-4","D",0]
["6-Chloro-2,3-difluoro-4-(trifluoromethyl)benzoic acid","773869-48-0","D",0]
["(Propan-2-yl)[bis(trifluoromethyl)]phosphane","500766-56-3","D",0]
["Oxalic acid--3,4,5-tris(trifluoromethyl)-1H-pyrazole (1/1)","88697-11-4","D",0]
["1-[Bis(trifluoromethanesulfonyl)methyl]-2,3,4,5,6-pentafluorobenzene","405074-81-9","D",0]
["Dichloro(dimethyl)(trifluoromethyl)-lambda~5~-phosphane","64728-36-5","D",0]
["Bis(4-{bis[3,5-bis(trifluoromethyl)phenyl]amino}phenyl)propanedinitrile","817638-44-1","D",0]
["(3E)-1,1,1,5,5,5-Hexafluoro-4-hydroxypent-3-en-2-one--nickel--water (2/1/1)","207569-13-9","D",0]
["6,6-difluoro-1,5-bis(trifluoromethyl)-1,3,5-triazinane-2,4-dione","85573-01-9","D",0]
["Silane, methoxydimethyl(pentafluorophenyl)-","23761-74-2","D",0]
["3,4,4-Trifluorobut-2-enoic acid","110680-68-7","D",0]
["Copper(II) trifluoromethanesulphonate","34946-82-2","D",0]
["1,1-Difluoroethene--acetylene (1/1)","914978-70-4","D",0]
["Bis(pentafluorophenyl)(2-phenylethenyl)borane","165612-90-8","D",0]
["4,4'-Sulfonylbis(tetrafluoroaniline)","138530-75-3","D",0]
["1,1,1-Trifluoro-N-methylpropan-2-amine","632344-06-0","D",0]
["Methane, trifluoro(methylseleno)-","1544-55-4","D",0]
["Methyl 3,3,3-trifluoro-2-iodopropanoate","666-93-3","D",0]
["Benzene, 1-(trifluoroethenyl)-4-(trifluoromethyl)-","92917-54-9","D",0]
["2-Fluoro-5-(trifluoromethyl)phenol","141483-15-0","D",0]
["1-(aziridin-1-yl)-2,2,2-trifluoroethanol","20893-12-3","D",0]
["1,1,3-Trichloro-2,2,3,4,5,6,7-heptafluoro-2,3-dihydro-1H-indene","58161-55-0","D",0]
["2-Bromo-1,1-dichloro-2,3,3,4,5,6,7-heptafluoro-2,3-dihydro-1H-indene","88953-13-3","D",0]
["Hexafluorobenzene","392-56-3","D",0]
["1,1-Difluorobutane","2358-38-5","D",0]
["1,8-Naphthyridine,2,3,4,5,6,7-hexafluoro-","56595-12-1","D",0]
["Trifluoromethyl 2,2,2-trifluoro-N-hydroxyethanimidothioate","88326-79-8","D",0]
["2-Chloro-3-fluoro-6-(trifluoromethyl)pyridine","1159512-39-6","D",0]
["1,5-Dibromo-1,1,3,3,5,5-hexafluoropentane","371-83-5","D",0]
["[(Trifluoromethyl)sulfanyl]methanesulfinyl bromide","61363-08-4","D",0]
["N~1~-[2-(Bis{4-[bis(trifluoromethyl)amino]phenyl}amino)phenyl]-N~1~-{4-[bis(trifluoromethyl)amino]phenyl}-N~4~,N~4~-bis(trifluoromethyl)cyclohexa-2,5-diene-1,4-bis(iminium) diperchlorate","137993-01-2","D",0]
["Acetic acid, [bis(2,2,2-trifluoroethoxy)phosphinyl]bromo-, methyl ester","287481-44-1","D",0]
["2-fluoro-4-iodo-1-(trifluoromethyl)benzene","239135-53-6","D",0]
["2-[3,5-Bis(trifluoromethyl)anilino]ethan-1-ol","503310-51-8","D",0]
["Stibine, bis(pentafluorophenyl)phenyl-","21041-56-5","D",0]
["1,1,1,3-Tetramethyl-3,3-bis(3,3,3-trifluoropropyl)disiloxane","690-56-2","D",0]
["bis(2,2,2-trifluoroethyl) selenite","77504-43-9","D",0]
["Cinnoline,hexafluoro-","28734-86-3","D",0]
["Sodium trihydrido(trifluoroacetato-kappaO)borate(1-)","61666-40-8","D",0]
["Cadmium, bis(trifluoromethyl)-","33327-66-1","D",0]
["S-(3,3,3-Trifluoroprop-1-en-2-yl)-(thiohydroxylamine)","106306-16-5","D",0]
["2,5-Dimethyl-3,4-bis[(trifluoromethyl)sulfanyl]-1H-pyrrole","62665-42-3","D",0]
["4,5,5-trifluoropent-4-enoic Acid","110003-22-0","D",0]
["2,5-Bis(trifluoromethyl)pyrazine","1365988-35-7","D",0]
["4-Chloro-1,1,1,3,3-pentafluorobutane","70566-48-2","D",0]
["4,4,4-TRIFLUORO-2-METHYL-3-OXOBUTANENITRILE","110234-70-3","D",0]
["4-Chloro-3,3,4-trifluorobutan-2-ol","19447-36-0","D",0]
["1,1,1,3,5,5,5-Heptafluoropentane-2,4-diimine","391204-73-2","D",0]
["1-Chloro-1,1,2-trifluoro-2-iodoethane","354-26-7","D",0]
["1,1'-Disulfanediylbis[2-(2,2-difluoroethoxy)-6-(trifluoromethyl)benzene]","924647-40-5","D",0]
["2,2,2-Trifluoroethylamine hydrochloride","373-88-6","D",0]
["4,4'-[(E)-Diazenediyl]bis(tetrafluoropyridine)","57310-44-8","D",0]
["(Bromosulfanyl)(trifluoro)methane","753-92-4","D",0]
["Ethane, 1,1-dichloro-1,2-difluoro-","1842-05-3","D",0]
["(E)-N-(2,4-Difluorophenyl)-1-(pentafluorophenyl)methanimine","90283-18-4","D",0]
["4-Fluoro-3-(trifluoromethyl)phenol","61721-07-1","D",0]
["BENZENAMINE, N,N-BIS(2,2,2-TRIFLUOROETHYL)-","2924-27-8","D",0]
["4-ethoxy-1,1,2-trifluorobut-1-ene","2021-77-4","D",0]
["1,2,4,5-Tetrafluoro-3-methoxy-6-(trifluoromethyl)benzene","20867-94-1","D",0]
["1-(2,2,2-Trifluoroethyl)hydrazine","5042-30-8","D",0]
["2,4-Bis(trifluoromethyl)benzyl bromide","140690-56-8","D",0]
["3-[(3-{(2-Carboxyethyl)[(perfluoropentyl)sulfonyl]amino}propyl)(dimethyl)ammonio]propanoate","2254560-18-2","D",0]
["(2R)-1,1,1-Trifluorohexan-2-amine","862156-04-5","D",0]
["Methanamine, 1,1,1-trifluoro-N-(trifluoromethyl)-","371-77-7","D",0]
["cobalt(2+);trifluoromethane","194491-06-0","D",0]
["2-[(Trifluoromethyl)sulfanyl]-1H-pyrrole","62665-27-4","D",0]
["1-(1-Ethoxyethyl)-2,3,4,5,6-pentafluorobenzene","90095-68-4","D",0]
["2-Ethoxy-1,1,3,3,3-pentafluoroprop-1-ene","2247-94-1","D",0]
["1-(Difluoromethyl)-2-fluoro-4-(trifluoromethyl)benzene","1214364-84-7","D",0]
["2,2,2-Trifluoro-1-[4-(trifluoromethyl)phenyl]ethan-1-amine","158388-49-9","D",0]
["1-(2-Chloro-1,1,2-trifluoroethoxy)propane","380-43-8","D",0]
["3,4-dichloro-3,4,4-trifluorobut-1-ene","374-26-5","D",0]
["1~3~,1~5~,3~3~,3~5~-Tetrakis(trifluoromethyl)[1~1~,2~1~:2~3~,3~1~-terphenyl]-2~2~-amine","667938-69-4","D",0]
["1,2,4,5-Tetrafluoro-3-iodo-6-methylbenzene","61794-44-3","D",0]
["Hexakis(trifluoromethyl)digermathiane","112438-41-2","D",0]
["3,4,5-Tris(2-chloro-1,1,2-trifluoroethoxy)benzoic acid","75860-23-0","D",0]
["Perfluorohexamethylprismane","22736-20-5","D",0]
["1,1'-Oxybis(2,3,5,6-tetrafluoro-4-methoxybenzene)","20867-91-8","D",0]
["1,1',1''-Methanetriyltris(pentafluorobenzene)","4780-60-3","D",0]
["2-(Trifluoromethyl)cyclopropan-1-amine","113715-22-3","D",0]
["Methyl 4,4,4-trifluoro-2-(trifluoromethyl)butanoate","53392-80-6","D",0]
["1,1,1-Trifluoro-4-(methylsulfanyl)but-3-en-2-one","532977-10-9","D",0]
["2,4-Bis(trifluoromethyl)phenylacetic acid","177952-39-5","D",0]
["2,4,6-Tris[(pentafluorophenyl)sulfanyl]-1,3,5-triazine","922517-12-2","D",0]
["2,2-Difluoropropan-1-ol","33420-52-9","D",0]
["Silane, trimethyl[(trifluoromethyl)thio]-","138128-74-2","D",0]
["3,4,5,6-tetrafluorobenzene-1,2-diamine","2993-07-9","D",0]
["6:2 fluorotelomer sulfinyl propanamido dimethyl ethyl sulfonate",null,"D",0]
["Tris(trifluoroethenyl)borane","815-70-3","D",0]
["Trifluorothiolacetic acid","2925-25-9","D",0]
["(3S)-4,4,4-Trifluoro-3-methylbutan-1-ol","95910-97-7","D",0]
["4-(1,1,3,3,3-Pentafluoroprop-1-en-2-yl)-1,1'-biphenyl","61587-19-7","D",0]
["1,3,5-Trimethyl-1,3,5-tris(3,3,3-trifluoropropyl)trisiloxane-1,5-diol","2802-54-2","D",0]
["Methyl[tris(pentafluorophenyl)]stannane","1062-71-1","D",0]
["1,1'-Biphenyl, 2,2',3,3',4,4',5,5'-octafluoro-","5121-90-4","D",0]
["3-Fluoro-2-(trifluoromethyl)hex-2-enoic acid","66566-99-2","D",0]
["Pyridine, 4-trifluoromethyl-","3796-24-5","D",0]
["1,1,2,3,4,4-Hexafluorobut-2-ene","17997-56-7","D",0]
["1-isopropenyl-3,5-di(trifluoromethyl)benzene","66875-48-7","D",0]
["2-(Trifluoromethyl)furan","56286-83-0","D",0]
["Quinoxaline, hexafluoro-","21271-15-8","D",0]
["2,2,2-Trifluoro-1-(5-fluoropyridin-2-yl)ethan-1-one","1060802-44-9","D",0]
["O-Ethyl 3,3-difluoro-2-(trifluoromethyl)prop-2-enethioate","62619-36-7","D",0]
["1,1,1,4,4,4-Hexafluoro-2-iodobutane","453-39-4","D",0]
["2-Fluoro-3-(trifluoromethyl)benzonitrile","146070-35-1","D",0]
["1-(2-fluoroethyl)-3-(2,2,2-trifluoroethyl)urea","33021-75-9","D",0]
["3-Chloro-2,2,3-trifluoro-3-iodopropanoyl chloride","88639-62-7","D",0]
["2,4-Bis(trifluoromethyl)cyclohexan-1-amine","65934-73-8","D",0]
["Ethylamine, N-methyl-N-nitroso-2,2,2-trifluoro-","819-35-2","D",0]
["Potassium [2,4-bis(trifluoromethyl)phenyl](trifluoro)borate(1-)","1150655-10-9","D",0]
["Benzene, 1,1'-(1,2-ethanediyl)bis[2,3,4,5,6-pentafluoro-","853-74-7","D",0]
["1-Bromo-2-(difluoromethoxy)-1,2,3,3-tetrafluorocyclopropane","58707-65-6","D",0]
["1,1-Dichloro-2-fluoro-2-[(trifluoromethyl)peroxy]ethane","54362-36-6","D",0]
["(2-Bromo-3,4,5,6-tetrafluorophenyl)methanol","292621-47-7","D",0]
["2,3,5,6-Tetrafluoro-4-(trifluoromethyl)phenol","2787-79-3","D",0]
["2-Methyl-2-(2,2,2-trifluoroethyl)oxirane","136791-28-1","D",0]
["4-bromo-N,N-bis(2,2,2-trifluoroethyl)-3-(trifluoromethyl)aniline","821778-33-0","D",0]
["4,5-Dichloro-2,2,4,5-tetrafluoro-1,3-dioxolane","87075-00-1","D",0]
["Trifluoro(fluoromethoxy)methane","2261-01-0","D",0]
["2,3-Diethoxy-1,1,1,4,4,4-hexafluorobut-2-ene","61385-81-7","D",0]
["3-Chloro-2,2,3-trifluoropropanoic acid","425-97-8","D",0]
["2-Chloro-3-(chloromethyl)-1,1,1,4,4,4-hexafluorobut-2-ene","189162-15-0","D",0]
["2,4,6-Trimethyl-3,5-bis(trifluoromethyl)pyridine","61895-58-7","D",0]
["1-(Trifluoromethanesulfinyl)-4-(trifluoromethoxy)benzene","223683-77-0","D",0]
["5-(Trifluoromethyl)-2H-tetrazole","2925-21-5","D",0]
["1,5-Dichloro-2-fluoro-4-(trifluoromethyl)benzene","112290-01-4","D",0]
["Trifluoromethanesulphonyl chloride","421-83-0","D",0]
["Cyclobutaphosphane, tetrakis(trifluoromethyl)-","393-02-2","D",0]
["1-Chloro-2,2-difluoroethan-1-ol","90179-79-6","D",0]
["1-Bromo-3-(chloromethyl)-2,4,5,6-tetrafluorobenzene","292621-52-4","D",0]
["1,1,1,7-Tetrachloro-3,3,5,5,7,7-hexafluoroheptane","76140-28-8","D",0]
["1,2,3,4,6,7,8,9-Octafluoro-10H-phenoxazine","90251-11-9","D",0]
["1-(2,3-Difluoro-4-methoxyphenyl)-2,2,2-trifluoroethan-1-one","1356109-99-3","D",0]
["Ethyl [3,5-bis(trifluoromethyl)phenyl]acetate","144632-97-3","D",0]
["3-(Bromomethyl)-1,2,4,5-tetrafluorobenzene","53001-73-3","D",0]
["3-Chloro-4-fluoro-5-(trifluoromethyl)aniline","914225-61-9","D",0]
["3-(Difluoromethyl)-2,6-difluoropyridine","85396-63-0","D",0]
["4-(Trifluoromethyl)furan-2(5H)-one","102854-63-7","D",0]
["Bis(difluoromethyl)[bis(trifluoromethyl)]germane","65225-92-5","D",0]
["1,1,4,4,4-Hexafluorobutane-2,3-dione","685-24-5","D",0]
["1H-Pyrrole, 2-(pentafluorophenyl)-","147439-17-6","D",0]
["(Pentafluorophenyl)propanedinitrile","719-38-0","D",0]
["Phosphorane, (4-chlorophenyl)tetrakis(2,2,2-trifluoroethoxy)-","102040-62-0","D",0]
["5-(TRIFLUOROMETHYL)-1,3,4-OXADIAZOL-2-OL","82476-06-0","D",0]
["Silane, tris(pentafluorophenyl)phenyl-","17067-71-9","D",0]
["1,3-Dichloro-2,4,5,6-tetrafluorobenzene","1198-61-4","D",0]
["(Pentafluorophenyl)-carbonimidic dibromide","114564-99-7","D",0]
["2,2,2-Trifluoroethane-1,1-diol--silver (1/1)","7226-28-0","D",0]
["1,1,1-Trifluoropent-3-en-2-ol","66068-00-6","D",0]
["2,3,4,5-Tetrafluorophenylacetonitrile","53001-74-4","D",0]
["[3,5-bis(trifluoromethyl)phenyl]methanesulfonyl Chloride","400770-85-6","D",0]
["2,3,5,6-Tetrafluoro-4'-methoxy-4-(trifluoromethyl)-1,1'-biphenyl","920264-41-1","D",0]
["5-Bromo-1,3-difluoro-2-(trifluoromethyl)benzene","156243-64-0","D",0]
["2,4,6-tris(trifluoromethyl)benzoic Acid","25753-26-8","D",0]
["Chromium, bis(1,4-di(trifluoromethyl)benzene-","7235-25-8","D",0]
["4-Ethenyl-2,3,5,6-tetrafluorophenol","385422-30-0","D",0]
["Flurothyl","333-36-8","D",0]
["38-(Perfluorohexyl)-3,6,9,12,15,18,21,24,27,30,33,36‐dodecaoxaoctatriacontan‐1‐ol",null,"D",0]
["1-Chloro-1,1,3,3,3-pentafluoro-2-iodopropane","359-59-1","D",0]
["N-Chloro-N-(pentafluorophenyl)hypochlorous amide (non-preferred name)","58749-38-5","D",0]
["Ethanamine, 2,2,2-trifluoro-, hydrofluoride","373-89-7","D",0]
["2-Phosphapropene, pentafluoro-","72344-34-4","D",0]
["3,3,3-Trifluoro-1-nitroprop-1-en-2-amine","104684-87-9","D",0]
["2-(Pentafluorophenoxy)ethanol","2192-55-4","D",0]
["triflic azide","3855-45-6","D",0]
["N-(2,2,2-Trifluoroethyl)urea","819-60-3","D",0]
["Ro 14-0518","73241-14-2","D",0]
["Trifluoromethanesulfinyl isocyanate","51735-89-8","D",0]
["2',4',6'-Trifluoro-5-(trifluoromethyl)[1,1'-biphenyl]-3-ol","1261990-36-6","D",0]
["2,3,5,6-Tetrafluorobenzonitrile","5216-17-1","D",0]
["5,6,7,8-tetrafluoro-2-(2,3,4,5,6-pentafluorophenyl)chromen-4-one","6069-17-6","D",0]
["3,4,5-Tris(trifluoromethyl)-1H-pyrazole","19968-20-8","D",0]
["Tris(trifluoromethanesulfonyl)methane","60805-12-1","D",0]
["2,3,4,6-tetrafluoro-5-hydrazinylaniline","2247-97-4","D",0]
["Methyl (trifluoromethyl)phosphonochloridate","89262-68-0","D",0]
["5-(Trifluoromethyl)isoxazole","116584-43-1","D",0]
["1,3-Bis(pentafluorophenyl)urea","21132-30-9","D",0]
["(2Z)-4-Bromo-1,1,1,3-tetrafluorobut-2-ene","933600-89-6","D",0]
["1,2,2-Trifluoroethyl trifluoromethyl ether","84011-06-3","D",0]
["(Methoxyethynyl)[bis(pentafluorophenyl)]phosphane","95112-05-3","D",0]
["N,N'-(Ethane-1,2-diyl)bis(2,2,2-trifluoro-N-methylacetamide)","61553-61-5","D",0]
["2-Bromo-1-chloro-1,1,2-trifluoroethane","354-20-1","D",0]
["2,4,6-Tris(pentafluorophenyl)-1,3,5,2,4,6-triazatriborinane","1110-39-0","D",0]
["Ethyl (trifluoromethyl)carbonofluoridimidate","61699-92-1","D",0]
["N-(2,3,4,5,6-pentafluorophenyl)acetamide","653-22-5","D",0]
["1,5-Hexadiene, 1,1,2,3,3-pentafluoro-","131768-26-8","D",0]
["4,4,4-Trifluorobut-2-enoyl chloride","115630-80-3","D",0]
["Hydroxylamine, O-(2,2,2-trifluoroethyl)-","76029-68-0","D",0]
["Trifluoroacetone","421-50-1","D",0]
["1,2,3,5-Tetrafluoro-4-iodo-7-azabicyclo[4.1.0]hepta-2,4,6-triene","923294-34-2","D",0]
["Cyclohexane, 1,2-bis[(trifluoromethyl)thio]-","53356-04-0","D",0]
["1,1,1,3,3-Pentafluoro-2-(fluoromethoxy)-3-methoxypropane","58109-33-4","D",0]
["1-Chloro-1,1-difluoro-N,N,1-tris(trifluoromethyl)-lambda~5~-phosphanamine","61558-09-6","D",0]
["Bis(3,3,3-trifluoropropyl) hydrogen phosphate",null,"D",0]
["1-(Bicyclo[2.2.1]hept-5-en-2-yl)-2,2,4,4,4-pentafluorobutane-1,3,3-triol","556053-07-7","D",0]
["Chloro(dimethyl)(1,1,1,3,3-pentafluoropropan-2-yl)silane","62281-38-3","D",0]
["4,5,6-Trifluoro-1,2,3-triazine","112291-51-7","D",0]
["2,2',3,3',5,5',6,6'-Octafluoro-4,4'-dinitro-1,1'-biphenyl","3905-96-2","D",0]
["2-(Difluoromethyl)-1-fluoro-4-(trifluoromethyl)benzene","1214334-37-8","D",0]
["2,2,2-Trifluoro-1-(2-fluorophenyl)ethan-1-one","124004-75-7","D",0]
["2,2,2-Trifluoro-1-(3-fluorophenyl)ethan-1-amine","1187931-53-8","D",0]
["1,3-Dichloro-1,2,2-trifluoropropane","67406-68-2","D",0]
["4,4'-[(2,3,5,6-Tetrafluoro-1,4-phenylene)bis(oxy)]bis(tetrafluorobenzonitrile)","15053-71-1","D",0]
["N-Chloro-N,1,1-trifluoroethanamine","16276-45-2","D",0]
["4-(Trifluoromethyl)-2,3,5,6-tetrafluorobenzyl bromide","76437-40-6","D",0]
["N-methyl-4,6-bis(trifluoromethyl)-1,3,5-triazin-2-amine","29181-68-8","D",0]
["1-(2,2,2-Trifluoroethyl)-3,5-bis(trifluoromethyl)benzene","1099597-83-7","D",0]
["1,3,3-Trifluoro-2-methoxycycloprop-1-ene","59034-32-1","D",0]
["1,2,3,4,5,6,7,8,9-Nonafluoro-9H-fluorene","19113-94-1","D",0]
["2,4-Difluoro-3-(trifluoromethoxy)benzoic acid","1119454-13-5","D",0]
["4,4'-Bis(trifluoromethyl)biphenyl","581-80-6","D",0]
["1,3-Dichloro-1,2,3-trifluoropropane","151771-08-3","D",0]
["4-(Difluoromethyl)-1-fluoro-2-(trifluoromethyl)benzene","1214364-78-9","D",0]
["1,2,3,4-Tetrafluoro-5-iodobenzene","5121-89-1","D",0]
["(Perfluorodecyl)methane-1,1-diol",null,"D",0]
["Bis(2,2,2-trifluoroethyl)sulfite","53749-89-6","D",0]
["1,4-Dichloro-1,2,3,4,5,6,7,8-octafluoro-1,4-dihydronaphthalene","88903-19-9","D",0]
["N-[3-(Trifluoromethyl)phenyl]trifluoromethanesulfonamide","23384-11-4","D",0]
["Bis-trifluoromethyl Ethylphosphonate","650-16-8","D",0]
["1-Difluorophosphoryloxy-1,1,2,4,4,4-hexafluorobutane",null,"D",0]
["4-fluoro-5-(trifluoromethyl)benzene-1,2-diamine","179062-06-7","D",0]
["1,1,1-Trifluoro-3-iodohexane","1257535-27-5","D",0]
["2,4,6-tris(trifluoromethyl)aniline","25753-22-4","D",0]
["Trifluoroacetic acid--nickel--water (2/1/4)","151013-23-9","D",0]
["2-Chloro-4-fluoro-1-(trifluoromethyl)benzene","94444-58-3","D",0]
["2-Nitro-N-(2,2,2-trifluoroethyl)-4-(trifluoromethyl)aniline","42379-55-5","D",0]
["Acetamide, 2,2,2-trifluoro-N-propyl-","10056-69-6","D",0]
["Dimethyl (trifluoromethyl)phosphonate","89262-62-4","D",0]
["1-Propene, 1-bromo-3,3,3-trifluoro-","460-33-3","D",0]
["Ytterbium(2+) bis(2,3,4,5,6-pentafluorobenzen-1-ide)","66080-22-6","D",0]
["1,1,1-Trifluoropentane","406-82-6","D",0]
["2-Fluoro-4-(trifluoromethyl)benzaldehyde","89763-93-9","D",0]
["2-Fluoro-3-(trifluoromethyl)phenol","207291-85-8","D",0]
["2-Oxetanol, 3,3-difluoro-4-phenyl-2-(trifluoromethyl)-","116020-01-0","D",0]
["2-Chloro-1,2,3,3-tetrafluoropropane",null,"D",0]
["1,7-Dibromo-1,1,2,2,3,3,4,4,5,5,6,6,7,7-tetradecafluoroheptane","37819-18-4","D",0]
["4,4,4-Trifluoro-N-methoxy-N-methyl-2-(2,2,2-trifluoroethyl)butanamide","952714-30-6","D",0]
["Azide, pentafluorophenyl-","1423-15-0","D",0]
["2,6-difluoro-4-(trifluoromethyl)aniline","123950-45-8","D",0]
["2,3-Difluorocycloprop-2-en-1-one","61486-72-4","D",0]
["Phosphine, diethyl(trifluoroethenyl)-","400846-21-1","D",0]
["4-fluoro-N-methyl-N-(trifluoromethyl)aniline","10219-07-5","D",0]
["1,3-Dioxole, 2,2,4-trifluoro-5-(trifluoromethoxy)-","161611-74-1","D",0]
["Difluoro[(trifluoroethenyl)oxy]acetic acid","64139-69-1","D",0]
["2,4,5,6-Tetrafluoropyridine-3-carbonitrile","35720-79-7","D",0]
["5,5,5-trifluoropentanoic Acid","407-62-5","D",0]
["2,5-Bis(trifluoromethyl)nitrobenzene","320-88-7","D",0]
["Trifluoromethanesulfinyl fluoride","812-12-4","D",0]
["1-(2-fluoroethyl)-3-(trifluoromethyl)benzene","50512-33-9","D",0]
["3,3,3-trifluoro-2-methylpropanal","58928-28-2","D",0]
["1,1,1-Trifluoropropan-2-amine--hydrogen chloride (1/1)","2968-32-3","D",0]
["1,2-Dichloro-1,2,3,3,4,5,6,7-octafluoro-2,3-dihydro-1H-indene","87228-37-3","D",0]
["Trifluoro[(trifluoromethyl)selanyl]methane","371-79-9","D",0]
["3H-Perfluoro-2,2,4,4-tetrahydroxypentane","77953-71-0","D",0]
["Methyl 2-(trifluoromethyl)acrylate","382-90-1","D",0]
["2-[3,5-bis(trifluoromethyl)phenyl]-2-hydroxyacetic acid","228107-82-2","D",0]
["N1-di[3,5-di(trifluoromethyl)phenyl]methyl-3-bromobutanamide","680579-72-0","D",0]
["Perfluoro-2-(perfluoropropoxy)-2-(perfluoromethyl)propanoic acid",null,"D",0]
["Quinoline, 4-iodo-2,8-bis(trifluoromethyl)-","150785-69-6","D",0]
["5-Chloro-3,5-bis(trifluoromethyl)-5H-1,4,2-dioxazole","82985-92-0","D",0]
["N-Nitrosobis(2,2,2-trifluoroethyl) amine","625-89-8","D",0]
["(Pentafluorophenoxy)acetyl chloride","55502-53-9","D",0]
["1-Fluoro-2-iodo-4-(trifluoromethyl)benzene","110192-48-8","D",0]
["5-Iodo-1,1,1-trifluoropentane","352-60-3","D",0]
["1,1,1-Trifluoropent-3-yn-2-ol","94590-76-8","D",0]
["1,1'-(Ethene-1,2-diyl)bis(pentafluorobenzene)","14992-40-6","D",0]
["4-Chloro-2,6-bis(trifluoromethyl)quinoline","91991-79-6","D",0]
["2,2,2-Trifluoro-1-methoxyethane-1,1-diol","58982-47-1","D",0]
["1,1-Dichloro-1,2,2-trifluoro-2-(2,2,2-trifluoroethoxy)ethane","57041-66-4","D",0]
["1-[3,5-di(trifluoromethyl)phenyl]-5-methyl-1H-1,2,3-triazole","646989-38-0","D",0]
["2'-(Trifluoromethoxy)[1,1'-biphenyl]-2-diazonium hexafluoroantimonate(1-)","175676-17-2","D",0]
["2-Chloro-1,5-difluoro-3-(trifluoromethyl)benzene","1261733-98-5","D",0]
["4-(1,1,3,3,3-Pentafluoroprop-1-en-2-yl)benzoic acid","61587-27-7","D",0]
["1-(2-Azidoethyl)-3,5-bis(trifluoromethyl)benzene","823189-08-8","D",0]
["3,3,3-Trifluoro-2-(fluoromethoxy)propanoic acid","176255-04-2","D",0]
["2,2,2-Trifluoro-1-[6-(trifluoromethyl)pyridin-3-yl]ethan-1-ol","1092353-05-3","D",0]
["2-Butyne, 1,1,1,4,4,4-hexafluoro-","692-50-2","D",0]
["2,3,5,6-Tetrafluoro-4-(trifluoromethyl)benzene-1-thiol","651-84-3","D",0]
["1,1,3,3,5,5-Cyclohexanehexol, 2,2,4,4,6,6-hexafluoro-","183742-87-2","D",0]
["1-Bromo-2,3,4,5-tetrafluoro-6-methylbenzene","16583-13-4","D",0]
["2-Fluoro-5-(trifluoromethyl)pyridine","69045-82-5","D",0]
["4-Fluoro-2-(trifluoromethyl)(cyano-~13~C,~15~N)benzonitrile","1216879-97-8","D",0]
["1,3-Pentadiyne, 1,5,5,5-tetrafluoro-","64788-24-5","D",0]
["1,4-Dibromo-2,5-bis(trifluoromethoxy)benzene","63165-16-2","D",0]
["2-bromo-1,3,5-tris(trifluoromethyl)benzene","95606-57-8","D",0]
["1-(Chloromethyl)-2-fluoro-4-(trifluoromethyl)benzene","1000339-60-5","D",0]
["1-[2,5-Bis(trifluoromethyl)phenyl]ethan-1-ol","364-47-6","D",0]
["2,2,2-Trifluoroethane-1-sulfonyl fluoride","503-39-9","D",0]
["Dimethyl(2,2-difluoroethyl)amine","819-06-7","D",0]
["2,4-Dimethyl-3,5-bis[(trifluoromethyl)sulfanyl]-1H-pyrrole","62665-44-5","D",0]
["1,2-Dichloro-1,2,2-trifluoroethane-1-sulfonyl fluoride","7740-56-9","D",0]
["Trifluoro(trifluoromethyl)germane","1512-15-8","D",0]
["5-fluoro-2-(trifluoromethyl)benzonitrile","240800-45-7","D",0]
["3,4-Bis(trifluoromethyl)phenol","54850-27-0","D",0]
["3,3,3-Trifluoropropanethioamide","365428-34-8","D",0]
["(1E)-N-(2,2,2-Trifluoroethyl)ethanimine","80395-37-5","D",0]
["2,2,2-Trifluoroethanesulfonyl chloride","1648-99-3","D",0]
["1-[(Trifluoromethanesulfonyl)methyl]-4-(trifluoromethyl)benzene","194222-97-4","D",0]
["2,4,6-Trifluorophenol","2268-17-9","D",0]
["Hexa[trifluoromethyl]benzene","2340-93-4","D",0]
["Methane, bromodifluoroiodo-","753-66-2","D",0]
["2,3,4,5,7-Pentafluoro-6-methoxycyclohepta-2,4,6-trien-1-one","60477-25-0","D",0]
["Ethane, (difluoromethoxy)-","461-62-1","D",0]
["(3,3,3-Trifluoroprop-1-yn-1-yl)germane","71530-59-1","D",0]
["4,4,4-Trifluorobuta-1,2-diene","406-40-6","D",0]
["1-Bromo-2-chloro-5-fluoro-4-(trifluoromethyl)benzene","1345471-24-0","D",0]
["2-Propanone, 1,3-dichloro-1,1,3,3-tetrafluoro-","127-21-9","D",0]
["(2S,3S)-2,3-Difluorooxirane","80397-37-1","D",0]
["2,3,6-Trifluoropyridin-4-amine","63489-55-4","D",0]
["3-Chloro-2-[chloro(difluoro)methyl]-3,3-difluoroprop-1-ene","13006-21-8","D",0]
["1,2,4,5-tetrafluoro-3-(2,3,5,6-tetrafluorophenoxy)-6-[2,3,5,6-tetrafluoro-4-(2,3,5,6-tetrafluorophenoxy)phenyl]benzene","14055-54-0","D",0]
["[(Pentafluorophenyl)imino]propadien-1-one","825634-90-0","D",0]
["{[Bis(trifluoromethyl)amino](difluoro)methyl}carbonimidoyl","137719-90-5","D",0]
["2,3-dibromo-1,1,1,4,4,4-hexafluorobutane","384-50-9","D",0]
["4-Fluoro-1-iodo-2-(trifluoromethyl)benzene","41860-65-5","D",0]
["N~2~,N~5~-Bis(2,2,2-trifluoroethyl)-1,3,4-thiadiazole-2,5-diamine","61785-10-2","D",0]
["2,2',3,3',4,4',5,5',6-Nonafluoro-6'-(trifluoromethyl)-1,1'-biphenyl","64528-78-5","D",0]
["3-Bromo-2-chloro-1,1,3,3-tetrafluoroprop-1-ene","815-13-4","D",0]
["1-(Trifluoromethanesulfonyl)-4-[(trifluoromethyl)sulfanyl]benzene","63647-62-1","D",0]
["1,1,1-Trichloro-2,2,3-trifluoropropane","131211-71-7","D",0]
["Bis(trifluoromethyl)carbamodithioic acid","87188-08-7","D",0]
["2,4,6-Trifluorobenzotrifluoride","122030-04-0","D",0]
["2,3,5,6-Tetrafluoro-4-(trifluoromethyl)-1,1'-biphenyl","53700-73-5","D",0]
["2,3-Dimethyl-5,6-bis(trifluoromethyl)bicyclo[2.2.1]hepta-2,5-diene","85861-57-0","D",0]
["3,3,3-Trifluoro-N-(3,3,3-trifluoropropyl)propan-1-amine","201057-04-7","D",0]
["2,5-Bis(trifluoromethyl)pyridine","20857-44-7","D",0]
["Dichloro(difluoro)methane--water (1/1)","20814-57-7","D",0]
["4-Fluorobenzotrifluoride","402-44-8","D",0]
["1,2-dibromo-4-chloro-1,1,2-trifluorobutane","502457-70-7","D",0]
["1,3-Difluoropropadiene","51584-23-7","D",0]
["3-Bromo-4-fluorobenzotrifluoride","68322-84-9","D",0]
["2,2,2-Trifluoro-1-[3-(trifluoromethyl)phenyl]ethan-1-amine","65686-68-2","D",0]
["2,5-bis(trifluoromethyl)thiophene","87721-33-3","D",0]
["1,1-Difluoro-2-methylidenecyclopropane","67884-63-3","D",0]
["Stannane, trimethyl(pentafluorophenyl)-","1015-53-8","D",0]
["3-Penten-2-one, 1,1,1,5,5,5-hexafluoro-4-methyl-","372-25-8","D",0]
["Bis(2,3,5,6-tetrafluoropyridin-4-yl)mercury","15235-46-8","D",0]
["2,3,4,5,6-pentakis(trifluoromethyl)phenol","723294-91-5","D",0]
["Carbonic acid--2,2,2-trifluoroethan-1-ol (1/2)","1513-87-7","D",0]
["Ethanone, 1-(3,3,6,6-tetrafluoro-1,4-cyclohexadien-1-yl)-","69291-63-0","D",0]
["Chloro(difluoro)[(trifluoromethyl)selanyl]methane","78334-28-8","D",0]
["2',5'-bis(trifluoromethyl)acetophenone","545410-47-7","D",0]
["[2,3,5,6-Tetrafluoro-4-(trifluoromethyl)phenyl]acetic acid","32304-29-3","D",0]
["Trifluoromethanamine","61165-75-1","D",0]
["1,3-Difluoro-2-(fluoromethyl)benzene","62037-91-6","D",0]
["3,3,3-Trifluoropropanal","460-40-2","D",0]
["methyl-bis(2,3,4,5,6-pentafluorophenyl)silane","13888-78-3","D",0]
["2-(Trifluoromethoxy)ethan-1-ol","362631-84-3","D",0]
["2-Bromopentafluoropropene","431-49-2","D",0]
["(1S)-1-[3,5-Bis(trifluoromethyl)phenyl]ethan-1-ol","225920-05-8","D",0]
["2,2-Dichloro-3,3,3-trifluoropropanal","82107-24-2","D",0]
["4-(1,2-Dibromo-1,1,3,3,3-pentafluoropropan-2-yl)-1,1'-biphenyl","61587-29-9","D",0]
["2,5-Bis(2,3,4,5,6-pentafluorophenyl)-1,3,4-thiadiazole","16065-71-7","D",0]
["3-Bromo-6-chloro-1,2,3,4,5,6-hexafluorocyclohexa-1,4-diene","111837-21-9","D",0]
["Propan-2-yl trifluoromethanesulfinate","61795-08-2","D",0]
["3,5-Bis(trifluoromethyl)-N-ethylaniline","49850-16-0","D",0]
["Stannane, trimethyl(3,3,3-trifluoro-1-propynyl)-","19097-32-6","D",0]
["2,2,2-TRIFLUOROETHYL CHLOROFORMATE","27746-99-2","D",0]
["3,5-Bis(trifluoromethyl)benzyl mercaptan","158144-84-4","D",0]
["alpha-(Trifluoromethyl)-gamma-butyrolactone","174744-18-4","D",0]
["1-Chloro-1,1-difluoropropane","134190-53-7","D",0]
["1,2,3,5-Tetrafluoro-4-methylbenzene","80427-49-2","D",0]
["3-chloro-1,1,2-trifluoropropane","121612-65-5","D",0]
["1-Chloro-3-(chloromethyl)-2,4,5,6-tetrafluorobenzene","292621-59-1","D",0]
["4,6-bis(2,2,2-trifluoroethoxy)-1,3,5-triazin-2-amine","301211-00-7","D",0]
["Lanthanum tris(trifluoromethanesulfonate)","52093-26-2","D",0]
["Potassium (3-chloro-4-fluorophenyl)(trifluoro)borate(1-)","850623-59-5","D",0]
["2,3,5,6-Tetrafluorobenzenethiol","769-40-4","D",0]
["Hydroxy(pentafluorophenyl)acetic acid","652-24-4","D",0]
["1,3-Difluoroprop-1-ene","58777-28-9","D",0]
["2-{[(1,3,3,3-Tetrafluoroprop-1-en-1-yl)oxy]methyl}oxirane","879218-74-3","D",0]
["Bis(trifluoromethyl)mercury","371-76-6","D",0]
["Ethane, 1-chloro-1,1-difluoro-2-iodo-","463-99-0","D",0]
["3-Chloro-1,2,4,5-tetrafluorocyclohexa-1,4-diene","919273-03-3","D",0]
["4-(Difluoromethyl)-3-fluoropyridine","1374659-35-4","D",0]
["Dimethyl[(trifluoroacetyl)oxy]sulfanium trifluoroacetate","57738-66-6","D",0]
["Difluoro(iodo)(trifluoromethyl)silane","27668-68-4","D",0]
["1,1,1,2,2,3,3,4,4,5,5,6,6-Tridecafluoro-6-propoxyhexane","233678-16-5","D",0]
["1-(2-Bromoethoxy)-2,3,4,5,6-pentafluorobenzene","6669-01-8","D",0]
["Methyl 4,4,4-trifluorobutanoate","2365-82-4","D",0]
["Potassium trifluoro(6-fluoro-2-methylpyridin-3-yl)borate(1-)","1150654-88-8","D",0]
["1-(Pentafluorophenyl)ethan-1-ol","7583-08-6","D",0]
["N-[3,5-bis(trifluoromethyl)phenyl]-2-bromopropanamide","646497-42-9","D",0]
["3,3,3-trifluoro-2-iodoprop-1-ene","107070-09-7","D",0]
["1-(4,4-Difluoropiperidin-1-yl)-2,2,2-trifluoroethan-1-one","65220-85-1","D",0]
["2-Fluoro-4-(trifluoromethyl)benzyl bromide","239087-07-1","D",0]
["Benzene, (2,2-difluoroethenyl)pentafluoro-","653-19-0","D",0]
["2,2,2-Trifluoro-N-(5-fluoro-1,3-thiazol-2-yl)acetamide","745053-67-2","D",0]
["2,3,4,5,6-Pentafluoro-N'-(2,3,4,5,6-pentafluorobenzoyl)benzohydrazide","16065-70-6","D",0]
["(3-Chloro-2,4,5,6-tetrafluorophenyl)methanol","67640-29-3","D",0]
["2,2',3,3',5,5',6,6'-Octafluoro[1,1'-biphenyl]-4,4'-dicarbonitrile","28442-30-0","D",0]
["Trifluoroethenyl sulfurochloridate","923-15-9","D",0]
["3,5-Bis(trifluoromethyl)hydrocinnamic acid","181772-16-7","D",0]
["2-fluoro-4-(trifluoromethyl)pyridine","118078-66-3","D",0]
["1,1'-Sulfanediylbis(2,3,5,6-tetrafluoro-4-methoxybenzene)","61907-45-7","D",0]
["2,3,5,6-Tetrafluorobenzyl alcohol","4084-38-2","D",0]
["1,2,4,5-tetrakis(trifluoromethyl)benzene","320-23-0","D",0]
["1-(Trifluoromethyl)cyclohexane-1-carbonyl fluoride","140451-78-1","D",0]
["2-Aminoheptafluoronaphthalene","1146-66-3","D",0]
["Indium trifluoroacetate","36554-90-2","D",0]
["1,3-Dithiole, 2-(4,5-di-trifluoromethyl-1,3-dithiol-2-ylidene)-","26393-26-0","D",0]
["2,​2,​2-​trifluoro-Acetic acid-​d","599-00-8","D",0]
["Bis(trifluoromethyl)sulfamyl fluoride","141577-86-8","D",0]
["Benzene, 1,1'-methylenebis[2,3,4,5,6-pentafluoro-","5736-46-9","D",0]
["Trifluoro-N'-hydroxy-N,N-dimethylethanimidamide","88326-83-4","D",0]
["Tetrafluoro(trifluoromethyl)iodine","38091-67-7","D",0]
["Acetyl iodide, trifluoro-","354-36-9","D",0]
["2,5,8-Nonanetrione, 1,1,1,3,3,7,7,9,9,9-decafluoro-","28393-78-4","D",0]
["BTFFH","164298-25-3","D",0]
["2-Amino-3,5-difluoro-4-(trifluoromethyl)pyridine","883498-68-8","D",0]
["4-Chloro-N,N-bis(trifluoromethyl)aniline","10218-92-5","D",0]
["Methyl Trifluoropyruvate","13089-11-7","D",0]
["Dimethylsilanediyl bis(trifluoromethanesulfonate)","27607-78-9","D",0]
["Potassium trifluoro(trifluoromethyl)borate(1-)","42298-15-7","D",0]
["Oxo[tris(trifluoromethyl)]-lambda~5~-phosphane","423-01-8","D",0]
["2,4,6-Tris(2-chloro-1,1,2-trifluoroethoxy)benzoic acid","75860-08-1","D",0]
["methyltrifluoromethylsulfone","421-82-9","D",0]
["Tris(pentafluorophenyl)phosphine","1259-35-4","D",0]
["1-Propene, 3-bromo-1,1,2-trifluoro-","178676-13-6","D",0]
["3,3-Dimethyl-1,1,1-tris(3,3,3-trifluoropropyl)disiloxane","59485-25-5","D",0]
["3,3'-Methylenebis[5-(trifluoromethyl)-2,3-dihydro-1,3,4-thiadiazole]","88976-83-4","D",0]
["3-(Trifluoromethyl)-1-[4-(trifluoromethyl)phenyl]-1H-pyrazol-5-amine","1226138-26-6","D",0]
["N,N-Dimethyl-2,2-bis(trifluoromethanesulfonyl)ethen-1-amine","58510-91-1","D",0]
["1,2,3,4,5-Pentafluoro-6-(2-methylprop-2-en-1-yl)benzene","116212-41-0","D",0]
["2,4-Bis[(trifluoromethyl)sulfanyl]-1H-pyrrole","62665-36-5","D",0]
["1,1-Difluoropropene","430-63-7","D",0]
["2-Chloro-1,1-difluoropropane","430-93-3","D",0]
["2,2′,3,3′,4,4′,5,5′-Octafluoro-6,6′-dinitro-1,1′-biphenyl","16768-38-0","D",0]
["[2-Fluoro-5-(trifluoromethyl)phenyl]hydrazine","1093059-58-5","D",0]
["1,1,1-Trifluoro-3-(trifluoromethyl)hept-2-en-4-one","108162-70-5","D",0]
["Benzamide, 3,5-bis(trifluoromethyl)-, N-(5-chloro-4-(trifluoromethyl)-2-thiazolyl)-","134880-74-3","D",0]
["1-(Chloromethyl)-3-fluoro-5-(trifluoromethyl)benzene","634151-25-0","D",0]
["4-methyl-3,5-bis(trifluoromethyl)aniline","243139-67-5","D",0]
["1-Chloro-1,2,2-trifluoropropane","70192-76-6","D",0]
["N,N,N-Triethyl-2,2,2-trifluoroethan-1-aminium trifluoromethanesulfonate","380230-73-9","D",0]
["Methyl 2,2,2-trifluoroethyl carbonate","156783-95-8","D",0]
["3,4,5-Trifluoroiodobenzene","170112-66-0","D",0]
["3-Ethynyl-1,2,4,5-tetrafluorobenzene","69442-35-9","D",0]
["1,1,1-Trifluoro-N-(trifluoromethoxy)-N-(trifluoromethyl)methanamine","671-63-6","D",0]
["Ethyl(methyl)bis[(trifluoroacetyl)oxy]stannane","88524-85-0","D",0]
["(2S)-1,1,1-Trifluoro-3-methylbutan-2-amine","1131737-01-3","D",0]
["3-Bromo-1,1,1-trifluorobutan-2-one","382-01-4","D",0]
["2,2',3,3',4,5,5',6,6'-Nonafluoro-1,1'-biphenyl","5121-88-0","D",0]
["(R)-(+)-1-(Pentafluorophenyl)ethanol","104371-21-3","D",0]
["Bromozinc(1+) 2,3,4,5,6-pentafluorobenzen-1-ide","41242-25-5","D",0]
["Allylpentafluorobenzene","1736-60-3","D",0]
["2-(2,2,2-trifluoroethyl)oxirane","407-12-5","D",0]
["1,2-Dibromo-3,4-dichloro-1,1,2,3,4,4-hexafluorobutane","375-27-9","D",0]
["Trifluoromethyl methacrylate","56487-95-7","D",0]
["N,N,N-Tripentylpentan-1-aminium tetrakis[3,5-bis(trifluoromethyl)phenyl]borate(1-)","171261-33-9","D",0]
["2,2,2-trifluoro-1-(4-fluorophenyl)ethanol","17556-41-1","D",0]
["Difluoromethane--water (1/1)","163227-90-5","D",0]
["4-(Difluoromethyl)-1,2-difluorobenzene","1214379-64-2","D",0]
["1,1,2-Trifluorocyclohexane",null,"D",0]
["2,3-Bis(2,2,2-trifluoroethyl)butanedinitrile","122548-18-9","D",0]
["1,1,1-Trifluoro-N-(2,2,2-trifluoroethyl)methanesulfonamide","88443-70-3","D",0]
["3,4-bis(trifluoromethyl)-1H-pyrrole","82912-41-2","D",0]
["2,4-Difluoro-1-(trifluoromethyl)benzene","64248-61-9","D",0]
["Sulfone, methyl pentafluorophenyl","651-85-4","D",0]
["Boroxin, tris(pentafluorophenyl)-","223440-98-0","D",0]
["2,2,3,4,5,5-Hexafluoro-2,5-dihydro-1,1'-biphenyl","109270-32-8","D",0]
["2-Propanone,3-bromo-1,1,1-trifluoro-, oxime","117341-57-8","D",0]
["N-[3,5-Bis(trifluoromethyl)phenyl]hydrazinecarbothioamide","38901-31-4","D",0]
["2',3',4',5'-Tetrafluoroacetophenone","66286-21-3","D",0]
["1,1,1-Trifluoro-3-methylbutan-2-amine","1582-18-9","D",0]
["Copper, (trifluoromethyl)-","77152-08-0","D",0]
["3,3-Dibromo-1,1,1-trifluoropropane","500043-67-4","D",0]
["Tetrafluoro-m-phenylenediamine","1198-63-6","D",0]
["1-Chloro-3,3,3-trifluoro-2-methylpropene","381-83-9","D",0]
["(2S)-1,1,1-Trifluoropropan-2-amine--hydrogen chloride (1/1)","125353-44-8","D",0]
["2-(2,2,2-trifluoroethoxy)ethanol","2358-54-5","D",0]
["2-Propanone, 1-chloro-1,1,3,3-tetrafluoro-","920-64-9","D",0]
["2,4-Bis(trifluoromethyl)benzene-1-thiol","798569-90-1","D",0]
["KIH-485 M-9",null,"D",0]
["Acetic acid, chlorodifluoro-, trifluoromethyl ester","557745-34-3","D",0]
["2-methyl-5-(trifluoromethyl)furan","17515-75-2","D",0]
["5-Chloro-3-(trifluoromethyl)-1,2,4-thiadiazole","672-35-5","D",0]
["2-Chloro-1,1,2-trifluoroethan-1-amine","40062-89-3","D",0]
["3-Fluoro-5-(trifluoromethyl)benzyl bromide","239087-09-3","D",0]
["2-(2,2,2-Trifluoroethylidene)hydrazine-1-carboximidothioic acid","7145-43-9","D",0]
["Methyl[tris(trifluoromethyl)]phosphanium fluoride","63715-51-5","D",0]
["2,5-Diamino-3-fluoro-4-(trifluoromethyl)pyridine","675602-90-1","D",0]
["1,1-Dichloro-1,2,2,3-tetrafluoropropane","70192-63-1","D",0]
["3-chloro-1,1,1-trifluoropropane","460-35-5","D",0]
["Mercury, bis(pentafluorophenyl)- (8CI)(9CI)","973-17-1","D",0]
["(CHLOROMETHYL)METHYLBIS(PENTAFLUOROPHENYL)SILANE","77669-65-9","D",0]
["1-(2,4-Difluorophenyl)-2,2,2-trifluoroethan-1-ol","910866-32-9","D",0]
["Barium bis[(2E)-1,1,1,5,5,5-hexafluoro-4-oxopent-2-en-2-olate]","314071-48-2","D",0]
["1-(1-Chloro-2,2,2-trifluoroethyl)-3-(trifluoromethyl)benzene","34761-14-3","D",0]
["1,1,1-Trifluoro-3,3-dimethylbutane-2-thione","61121-94-6","D",0]
["(1,1,2,3,3-Pentafluoroprop-2-en-1-yl)phosphonic acid","148333-02-2","D",0]
["Ammonium 1,2,6-trifluoro-3,4,5-tris(fluorooxy)cyclohexa-2,4-diene-1-carboxylate","14639-94-2","D",0]
["1,2-Dibromo-1,1,3,3,3-pentafluoropropane","431-78-7","D",0]
["((4-((Perfluoro-3-nonen-1-yl)oxy)phenylsulfonyl)(methyl)amino)acetic acid",null,"D",0]
["1,1,1',1'-Tetrakis(difluoroamino)-N-1,1'-trifluorodimethylamine","17125-67-6","D",0]
["1,1-Difluoroethyl carbonofluoridate","1344118-11-1","D",0]
["Propyl 3,3-difluoro-2-(trifluoromethyl)prop-2-enoate","62935-21-1","D",0]
["2,3,5,6-Tetrafluorophenol","769-39-1","D",0]
["2,3,5,6-Tetrafluoroanisole","2324-98-3","D",0]
["1,1,5,5-Tetrafluoropentane-2,4-dione","70086-62-3","D",0]
["1-(Aziridin-1-yl)-2,2,2-trifluoroethan-1-one","2747-62-8","D",0]
["Platinum(2+) bis(2,3,4,5,6-pentafluorobenzen-1-ide)","80671-77-8","D",0]
["3-(Trifluoromethyl)-1H-pyrazole","20154-03-4","D",0]
["2-Ethynyl-1,4-bis(trifluoromethyl)benzene","88444-78-4","D",0]
["2,3-difluoro-4-(trifluoromethyl)benzaldehyde","134099-20-0","D",0]
["2,4-DIFLUORO-6-(TRIFLUOROMETHYL)-S-TRIAZINE","368-55-8","D",0]
["Propane, 1,3-difluoro-","462-39-5","D",0]
["1,1,1-Trifluoro-2-[(2,2,2-trifluoroethoxy)methoxy]ethane","6263-71-4","D",0]
["1,3,5-trifluoro-2,4-dimethyl-6-(trifluoromethyl)benzene","886762-24-9","D",0]
["(2,3,4,5,6-pentafluorobenzoyl) 2,3,4,5,6-pentafluorobenzenecarboperoxoate","22236-19-7","D",0]
["1,2,4,5-Tetrafluoro-3-iodo-6-(trifluoromethyl)benzene","61794-43-2","D",0]
["1-(Chlorodisulfanyl)-2,3,4,5,6-pentafluorobenzene","62098-19-5","D",0]
["1,1,2-Trifluoroethan-1-amine","918824-70-1","D",0]
["2,2,3,5-Tetrafluoro-3-(fluoromethyl)thiolane 1,1-dioxide",null,"D",0]
["2,2,4,4,4-Pentafluorobutanoic acid","856293-25-9","D",0]
["1-[2,3,5,6-Tetrafluoro-4-(trifluoromethyl)phenyl]pyrrolidine-2,5-dione","62263-19-8","D",0]
["1,4-Bis(trifluoromethyl)cyclohexa-1,2,3-trien-5-yne","223432-38-0","D",0]
["2-Bromo-1,3,3,3-tetrafluoropropene","396716-43-1","D",0]
["1-(Chloromethyl)-2,4-bis(trifluoromethyl)benzene","195136-46-0","D",0]
["1,3,4,5,6,7,8-Heptafluoronaphthalene-2-carbaldehyde","52158-48-2","D",0]
["1,2,4,5-Tetrafluoro-3,6-diiodobenzene","392-57-4","D",0]
["4-(Butylsulfanyl)-4-ethoxy-1,1-difluoro-2-(trifluoromethyl)but-1-ene","62378-52-3","D",0]
["1-(Trifluoromethyl)piperidine","657-45-4","D",0]
["(Chlorosulfanyl)(difluoro)methane","58932-27-7","D",0]
["1,1,1,3-Tetrachloro-2,2,3-trifluoropropane","422-50-4","D",0]
["2,4-Cyclohexadien-1-one, 6-chloro-2,3,4,5,6-pentafluoro-","29897-30-1","D",0]
["1,1,1-Trifluoro-3-(methanesulfonyl)propane","222611-24-7","D",0]
["Phosphine oxide, dimethyl(pentafluorophenyl)-","5525-96-2","D",0]
["2-Chloro-1,3-difluoro-4-(trifluoromethyl)benzene","120770-03-8","D",0]
["2,4,5-Trifluorobenzene-1-thiol","1208075-46-0","D",0]
["Holmium tris(trifluoromethanesulfonate)","139177-63-2","D",0]
["2-Chloroethyl trifluoromethanesulfinate","61915-99-9","D",0]
["(Difluoromethylidene)(difluoro)silane","51675-52-6","D",0]
["3,5-Bis(trifluoromethyl)benzaldehyde","401-95-6","D",0]
["N-Ethenyl-N-(trifluoromethyl)nitramide","89814-66-4","D",0]
["2,2,2-Trifluoro-N-oxoacetamide","84796-71-4","D",0]
["1-chloro-2-[chloro(difluoro)methyl]-1,1-difluoro-3-methylbutan-2-ol","6301-98-0","D",0]
["1,2-Bis(trifluoromethyl)benzene","433-95-4","D",0]
["Ethanethioic acid, S-(2,2,2-trifluoroethyl) ester","14897-48-4","D",0]
["5-Chloro-4-fluoro-2-(trifluoromethyl)-1,3-thiazole","62053-28-5","D",0]
["5-(Trifluoromethyl)-1,2-dihydro-3H-pyrazol-3-one","76480-99-4","D",0]
["(Trifluoromethyl)-lambda~5~-phosphanedione","827027-09-8","D",0]
["Potassium (2,4-difluorophenyl)(trifluoro)borate(1-)","871231-41-3","D",0]
["Trifluoromethanesulfinyl cyanide","61951-27-7","D",0]
["(2R)-1,1,1-Trifluoro-3,3-dimethylbutan-2-amine","1261298-42-3","D",0]
["Platinum(4+) tetrakis(trifluoromethanide)","60703-88-0","D",0]
["[3,3-Difluoro-2-(trifluoromethyl)prop-2-en-1-yl]benzene","7781-82-0","D",0]
["Bromozinc(1+) 3,3,3-trifluoroprop-1-en-2-ide","139954-92-0","D",0]
["2-Chloro-3,4-difluoro-1-(trifluoromethyl)benzene","119713-63-2","D",0]
["Tris(pentafluorophenyl)borane","1109-15-5","D",0]
["1-(1-Bromoethyl)-2,3,4,5,6-pentafluorobenzene","652-28-8","D",0]
["Bis(trifluoromethyl)dioxasilirane","827027-05-4","D",0]
["1,2,2-Trifluoro-N,N-bis(trifluoromethyl)ethenamine","13821-49-3","D",0]
["5-Fluoro-2-(trifluoromethyl)pyridine","936841-73-5","D",0]
["2-Amino-N-(2,2,2-trifluoroethyl)acetamide ","359821-38-8","D",0]
["3-Fluoropropyl trifluoromethanesulfonate","180597-96-0","D",0]
["4,5,6-Trifluoro-2-(trifluoromethyl)pyrimidine","27077-33-4","D",0]
["N-Bromo-2,2,2-trifluoroacetamide","359-45-5","D",0]
["Bis(trifluoromethyl) ethanedioate","20583-24-8","D",0]
["5-fluoro-6-(trifluoromethyl)-1H-pyrimidine-2,4-dione","774-17-4","D",0]
["2,3-Bis(trifluoromethyl)bicyclo[2.2.1]hepta-2,5-diene","58623-62-4","D",0]
["3-(2,2,2-Trifluoroacetamido)-N-(trifluoroacetyl)-L-alanine","88730-14-7","D",0]
["3-Fluoro-2-(trifluoromethyl)aniline","123973-22-8","D",0]
["3,3,3-Trifluoropropane-1-sulfonamide","1033906-44-3","D",0]
["2,5-bis(trifluoromethyl)phenylboronic acid","196083-18-8","D",0]
["2,5-difluoro-3-(trifluoromethyl)aniline","1682-26-4","D",0]
["5,7-Bis(trifluoromethyl)-1,8-naphthyridin-2(1H)-one","51420-73-6","D",0]
["1-Decene, 1,1,2,3,3-pentafluoro-5-iodo-","140184-10-7","D",0]
["Tris(2,2,2-trifluoroethyl)phosphite","370-69-4","D",0]
["Fluoromethyl ether","462-51-1","D",0]
["2,3-Difluorobutane","666-21-7","D",0]
["2-Chloro-1,4-difluoro-3-(trifluoromethyl)benzene","1099597-70-2","D",0]
["6-(Trifluoromethoxy)-2-(trifluoromethyl)quinolin-4(1H)-one","125647-79-2","D",0]
["2-Fluoro-3-(trifluoromethyl)pyrazine","1206524-60-8","D",0]
["3,5,6-Trifluoropyridin-2-amine","3534-50-7","D",0]
["3-(Trifluoromethyl)azetidin-3-ol--hydrogen chloride (1/1)","848192-96-1","D",0]
["1,1,1-Trifluoro-4-methylpentan-2-one","75703-02-5","D",0]
["Ethane, 1,2-dibromo-1,1,2-trifluoro-","354-04-1","D",0]
["2-Bromo-2,3,3,5,6-pentafluoro-2,3-dihydro-1H-inden-1-one","88953-12-2","D",0]
["2-Amino-4,6-bis(trifluoromethyl)pyridine-3-carbonitrile","89990-39-6","D",0]
["1-Bromo-2,3,5,6-tetrafluoro-4-methylbenzene","33564-68-0","D",0]
["1,4-dichloro-1,1,2,3,4,4-hexafluorobut-2-ene","360-88-3","D",0]
["1-Bromo-3,5-difluoro-2-(2,2,2-trifluoroethoxy)benzene","1002355-81-8","D",0]
["2,3-Difluoro-6-trifluoromethylbenzaldehyde","186517-43-1","D",0]
["2,3,7,8,12,13,17,18-Octafluoro-5,10,15,20-tetrakis(pentafluorophenyl)porphyrin","121399-88-0","D",0]
["Zinc trifluoromethanesulphonate","54010-75-2","D",0]
["Bis[(pentafluorophenyl)methyl]mercury","51081-33-5","D",0]
["Bis(2,3,4,5,6-pentafluorophenyl) sulphide","1043-50-1","D",0]
["3-Amino-4,4,4-trifluorobut-2-enenitrile","33561-24-9","D",0]
["3-bromo-1,1,1-trifluoropropan-2-ol","431-34-5","D",0]
["5-Fluoro-2-(trifluoromethyl)phenol","243459-91-8","D",0]
["1-[Chloro(difluoro)methyl]-4-(difluoromethyl)benzene","2629-65-4","D",0]
["Difluoro(fluoromethoxy)methane","461-63-2","D",0]
["Compound 485","33018-78-9","D",0]
["Dichloro(trifluoroethenyl)borane","758-99-6","D",0]
["1-Chloro-2,3,3,4,5,6,6-heptafluorocyclohexa-1,4-diene","830-23-9","D",0]
["3-(1,2-Dibromo-1,1,3,3,3-pentafluoropropan-2-yl)benzoic acid","61587-32-4","D",0]
["T0500-0748","64219-31-4","D",0]
["1-[(Trifluoromethyl)sulfanyl]-1H-imidazole","112463-42-0","D",0]
["Methanesulfonyl fluoride, trifluoro-","335-05-7","D",0]
["[1-(Trifluoromethyl)cyclopropyl]methanol","371917-17-8","D",0]
["4,5-Dichloro-4,5,5-trifluoropent-1-ene","89965-93-5","D",0]
["Pentafluorophenyl 2-fluoroprop-2-enoate","114589-63-8","D",0]
["1-(Difluoromethoxy)-4-(trifluoromethyl)benzene","156570-16-0","D",0]
["1,2-Dichloro-1,1,4,4,4-pentafluorobutane","153083-94-4","D",0]
["1-Fluoro-2-(trifluoromethoxy)ethane","819-49-8","D",0]
["3-Bromo-5-fluorobenzotrifluoride","130723-13-6","D",0]
["2-Methyl-2-(1,1,2-trifluoroethoxy)propane","402950-42-9","D",0]
["Bis[3,5-bis(trifluoromethyl)phenyl](oxo)phosphanium","15979-14-3","D",0]
["4-Amino-2,5-difluorobenzotrifluoride","114973-22-7","D",0]
["4-Nitro-N-(2,2,2-trifluoroethyl)-3-(trifluoromethyl)aniline","821777-51-9","D",0]
["2,5-bis(trifluoromethyl)phenol","779-88-4","D",0]
["(Pentafluorophenyl)acetonitrile","653-30-5","D",0]
["Benzene, 1-chloro-2,4,5-trifluoro-","2367-78-4","D",0]
["4,4'-(Ethane-1,2-diyl)bis(2,3,5,6-tetrafluorobenzene-1-thiol)","114808-44-5","D",0]
["Trifluoromethyl sulfur pentafluoride","373-80-8","D",0]
["Benzene, 1-(3-bromo-3,3-difluoro-1-propynyl)-4-(trifluoromethyl)-","877080-73-4","D",0]
["Bromo(chlorosulfanyl)fluoro[(trifluoromethyl)sulfanyl]methane","61363-02-8","D",0]
["4-Chloro-2,2,5-trifluoro-1,3-dioxolane","60010-43-7","D",0]
["2,2,2-Trifluoro-1-(2-fluorophenyl)ethan-1-ol","124004-74-6","D",0]
["2-(1-Ethoxyethyl)-1,3,4,5,6,7,8-heptafluoronaphthalene","90095-70-8","D",0]
["3-(Trifluoromethyl)azetidine--hydrogen chloride (1/1)","1221272-90-7","D",0]
["Difluoroacetic acid","381-73-7","D",0]
["Imidodiphosphorous acid, methyl-, tetrakis(2,2,2-trifluoroethyl) ester","129672-91-9","D",0]
["Alcohols, C8–16, γ-ω-perfluoro, reaction products with 1,6-diisocyanatohexane, glycidol and stearyl alc.","2728655–42–1","D",0]
["Acetamide, N-[3-(dimethylamino)propyl]-, 2-[(γ-ω-perfluoro-C4-20-alkyl)thio] derivs.","2738952–61–7","D",0]
["Acetamide, N-(2-aminoethyl)-, 2-[(γ-ω-perfluoro-C4-20-alkyl)thio] derivs., polymers with N1,N1-dimethyl-1,3-propanediamine, epichlorohydrin and ethylenediamine, oxidized","2742694–36–4","D",0]
["Acetic acid, 2-[(γ-ω-perfluoro-C4-20-alkyl)thio] derivs., 2-hydroxypropyl esters","2744262-09–5","D",0]
["L-Lysine, hydrochloride (1:1), polymer with 2-(chloromethyl)oxirane, sodium salt, reaction products with 2-[(2-propen-1-yloxy)methyl]oxirane and 1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-6-iodohexane","252306-38-0","D",0]
["2-Propenoic acid, 2-methyl-, 2-ethylhexyl ester, polymer with hexadecyl 2-methyl-2-propenoate, .alpha.-(2-methyl-1-oxo-2-propen-1-yl)-.omega.-hydroxypoly(oxy-1,2-ethanediyl), octadecyl 2-methyl-2-propenoate and 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl 2-methyl-2-propenoate","1793073-25-2","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, 1,1',1''-triester with boric acid (H3BO3)","213974-85-7","D",0]
["2-Propenoic acid, 2-methyl-, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl ester, polymer with 1,1-dichloroethene and octadecyl 2-propenoate","1229646-82-5","D",0]
["Hydrofluoric acid, reaction products with hexane","84732-21-8","D",0]
["1-Propanaminium, 3-amino-N-(carboxymethyl)-N,N-dimethyl-, N-[(.gamma.-.omega.-perfluoro-C6-14-alkyl)sulfonyl] derivs., inner salts","2730864-66-9","D",0]
["Hydrofluoric acid, reaction products with 4-methylmorpholine","186672-72-0","D",0]
["Hydrofluoric acid, reaction products with octane","210181-71-8","D",0]
["Ethane, 1,2-dichloro-1,1,2-trifluoro-","354-23-4","D",0]
["Iodonium, bis(4-(1,1-dimethylethyl)phenyl)-, salt with 1,1,2,2,3,3,4,4,4-nonafluoro-N-[(nonafluorobutyl)sulfonyl]-1-butanesulfonamide (1:1)",null,"D",0]
["Tetrafluorethene, polymer with trifluoro(trifluoromethoxy)ethene and 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]propane",null,"D",0]
["Siloxanes and Silicones, di-Me, 3-hydroxypropyl Me, Me 3,3,4,4,5,5,6,6,6-nonafluorohexyl","1610862-54-8","D",0]
["Alcohols, C8-16, .gamma.-.omega.-perfluoro, reaction products with methanol and TDI","2861980-11-0","D",0]
["Ethene, trifluoro-, polymer with 1,1-difluoroethene","28960-88-5","D",0]
["1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethene","73935-09-8","D",0]
["1-Octanol, 3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluoro-, 1,1'-(hydrogen phosphate), compd. with 2,2'-iminobis[ethanol] (1:1)","57677-96-0","D",0]
["Octane, 8-[(4-chlorobutyl)thio]-1,1,1,2,2,3,3,4,4,5,5,6,6-tridecafluoro-","1625673-01-9","D",0]
["2-Propenamide, N-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]ethyl]-","1584680-11-4","D",0]
["2-Propenamide, N-[2-[(3,3,4,4,5,5,6,6,7,7,8,8,8-tridecafluorooctyl)thio]ethyl]-, polymer with 2-propenamide","1584680-13-6","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[1,2,2,2-tetrafluoro-1-[[[(trichlorosilyl)methyl]ethoxy]methyl]ethyl]-.omega.-[tetrafluoro(trifluoromethyl)ethoxy]-","2863655-49-4","D",0]
["Poly[oxy[trifluoro(trifluoromethyl)-1,2-ethanediyl]], .alpha.-[tetrafluoro(trifluoromethyl)ethyl]-.omega.-[1,2,2,2-tetrafluoro-1-[[[(trimethoxysilyl)methyl]ethoxy]methyl]ethoxy]-","2863655-48-3","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, fluorinated","1187440-14-7","D",0]
["Ethene, 1-[difluoro(trifluoromethoxy)methoxy]-1,2,2-trifluoro-, polymer with 1,1-difluoroethene","874290-13-8","D",0]
["2-Propenoic acid, 2-[[3-[(1,1,2,2,3,3,4,4,5,5,6,6,7,7,8,8,8-heptadecafluorooctyl)sulfonyl]propyl]amino]ethyl ester, telomer with 2-methyloxirane polymer with oxirane mono-2-propenoate and 1-octanethiol","2862818-96-8","D",0]
["Methanol, telomer with 1,1,2,3,3,4,4-heptafluoro-4-[(1,2,2-trifluoroethenyl)oxy]-1-butene","2857873-17-5","D",0]
["Betaines, dimethyl(.gamma.,.omega.-perfluoro-.gamma.-hydro-C8-C18 alkyl)","2816091-53-7","D",0]
["PVDF-HFP",null,"D",0]
["1-Octanaminium, N-(2-hydroxyethyl)-N,N-dimethyl-, salt with 1,1,1-trifluoro-N-[(trifluoromethyl)sulfonyl]methanesulfonamide","334529-54-3","D",0]
["Poly(oxy-1,2-ethanediyl), alpha-phosphono-omega-hydroxy-, ethers with reduced Et esters of fluorinated reduced polymd. oxidized tetrafluoroethylene","2379313-43-4","D",0]
["Ethene, 1,1,2,2-tetrafluoro-, oxidized, polymd., reduced, fluorinated Me esters, reduced","1573124-82-9","D",0]
["4,4,4-trifluorobutan-2-ol","101054-93-7","D",0]
["4-bromo-2-fluoro-1-(trifluoromethoxy)benzene","105529-58-6","D",0]
["1-[3-Chloro-5-(trifluoromethyl)phenyl]-2,2,2-trifluoroethan-1-one","1125812-58-9","D",0]
["5-Bromo-1,3-difluoro-2-(trifluoromethoxy)benzene","115467-07-7","D",0]
["2-[[2,2,4-Trifluoro-5-(trifluoromethoxy)-1,3-dioxolan-4-yl]oxy]ethanol","1190931-34-0","D",0]
["3,5-Bis(trifluoromethyl)benzene-1-diazonium zinc chloride (2/1/4)","14263-91-3","D",0]
["Silane, chlorodimethyl(3,3,3-trifluoropropyl)-","1481-41-0","D",0]
["1,1,1,5,5,5-Hexafluoro-2,4-pentanedione","1522-22-1","D",0]
["2,3-difluoro-6-(trifluoromethyl)benzonitrile","186517-05-5","D",0]
["Difluoromethyl 2,2,2-trifluoroethyl ether","1885-48-9","D",0]
["2-chloro-3,5-bis(trifluoromethyl)aniline","201593-90-0","D",0]
["Cyclopentasiloxane, 2,4,6,8,10-pentamethyl-2,4,6,8,10-pentakis(3,3,3-trifluoropropyl)-","2063-78-7","D",0]
["3,5-Bis(trifluoromethyl)benzamide","22227-26-5","D",0]
["(Z)-1,3,3,3-Tetrafluoro-1-propene","29118-25-0","D",0]
["Mercury(1+) trifluoroacetate","2923-15-1","D",0]
["Potassium trifluoroacetate","2923-16-2","D",0]
["Acetic acid, 2,2,2-trifluoro-, lithium salt (1:1)","2923-17-3","D",0]
["Methanesulfonic acid, trifluoro-, silver(1+) salt","2923-28-6","D",0]
["Sodium trifluoromethanesulfinate","2926-29-6","D",0]
["Benzenediazonium, 3,5-bis(trifluoromethyl)-","29684-26-2","D",0]
["1-(3,5-Bis(trifluoromethyl)phenyl)ethan-1-one","30071-93-3","D",0]
["2-Butene, 2,3-dichloro-1,1,1,4,4,4-hexafluoro-","303-04-8","D",0]
["1,1,2,3,3,4,5,5-Octafluoropenta-1,4-diene","3109-87-3","D",0]
["2-bromo-3,3,3-trifluoropropan-1-ol","311-86-4","D",0]
["1-Bromo-3,5-bis(trifluoromethyl)benzene","328-70-1","D",0]
["Benzenamine, 3,5-bis(trifluoromethyl)-","328-74-5","D",0]
["2,5-Bis(trifluoromethyl)aniline","328-93-8","D",0]
["Benzoyl fluoride, 3-(trifluoromethyl)-","328-99-4","D",0]
["Methyl trifluoromethanesulfonate","333-27-7","D",0]
["Trifluoroacetic acid--ammonia (1/1)","3336-58-1","D",0]
["3,3,3-trifluoro-2-hydroxy-2-methylpropanenitrile","335-08-0","D",0]
["1,1,1-Trifluoro-2-iodoethane","353-83-3","D",0]
["Acetonitrile, trifluoro-","353-85-5","D",0]
["(2S)-1,1,1-Trifluoropropan-2-ol","3539-97-7","D",0]
["Trifluoroacetyl chloride","354-32-5","D",0]
["Acetamide, 2,2,2-trifluoro-","354-38-1","D",0]
["1,1,1-Trichloro-2,2,2-trifluoroethane","354-58-5","D",0]
["2,8-Bis(trifluoromethyl)quinolin-4-ol","35853-41-9","D",0]
["tris(2,2,2-trifluoroethyl) phosphate","358-63-4","D",0]
["2-(Trifluoromethyl)oxirane","359-41-1","D",0]
["1,3-Dichlorohexafluoro-2-butene","360-86-1","D",0]
["1-Propene, 3,3,3-trifluoro-2-methyl-","374-00-5","D",0]
["3-Trifluoromethylpyridine","3796-23-4","D",0]
["Ethyl trifluoroacetate","383-63-1","D",0]
["Ethanethioic acid, trifluoro-, S-ethyl ester","383-64-2","D",0]
["Benzene, 1-fluoro-2-(trifluoromethyl)-","392-85-8","D",0]
["Ethanol, 2,2,2-trifluoro-, sodium salt","420-87-1","D",0]
["Methanesulfenyl chloride, trifluoro-","421-17-0","D",0]
["Trifluoromethylsulfonamide","421-85-2","D",0]
["Ethyl trifluoromethanesulphonate","425-75-2","D",0]
["2-Chloro-1,1,2-trifluoro-1-methoxyethane","425-87-6","D",0]
["Methane, bis[(trifluoromethyl)sulfonyl]-","428-76-2","D",0]
["1,2-Dichloro-3,3,3-trifluoroprop-1-ene","431-27-6","D",0]
["Bromotrifluoroacetone","431-35-6","D",0]
["Ethanol, 2,2,2-trifluoro-1-methoxy-","431-46-9","D",0]
["Methyl trifluoroacetate","431-47-0","D",0]
["1-Propene, 1,1,2-trichloro-3,3,3-trifluoro-","431-52-7","D",0]
["Pentafluoroacetone","431-71-0","D",0]
["1,4-Bis(trifluoromethyl)benzene","433-19-2","D",0]
["Ethanol, 1-ethoxy-2,2,2-trifluoro-","433-27-2","D",0]
["1-Trifluoromethyl-2,3,4,5,6-pentafluorobenzene","434-64-0","D",0]
["Perfluorovinylacetic acid","44969-80-4","D",0]
["1,1,1-Trifluoro-3-iodopropane","460-37-7","D",0]
["HCFC 243","460-69-5","D",0]
["1-Propene, 1,1-dichloro-3,3,3-trifluoro-","460-70-8","D",0]
["1-Propene, 1-chloro-1,3,3,3-tetrafluoro-","460-71-9","D",0]
["1,1,1-Trifluoro-4-iodobutane","461-17-6","D",0]
["1,1,1-Trifluoro-2-methylpropan-2-ol","507-52-8","D",0]
["alpha,alpha,alpha,6-Tetrafluoro-m-toluidine","535-52-4","D",0]
["1,1'-Biphenyl, 2,2'-bis(trifluoromethyl)-","567-15-7","D",0]
["Silane, trichloro(3,3,3-trifluoropropyl)-","592-09-6","D",0]
["Acetic acid, bromo-, 2,2,2-trifluoroethyl ester","61433-91-8","D",0]
["Ethanone, 2,2,2-trifluoro-1-(4-fluorophenyl)-","655-32-3","D",0]
["Trifluoromethanesulphonic (2H)acid","66178-41-4","D",0]
["1,4-Bis(2,2,2-trifluoroethoxy)benzene","66300-61-6","D",0]
["Silane, dichlorobis(3,3,3-trifluoropropyl)-","665-98-5","D",0]
["[Bis[(trifluoromethyl)sulfonyl-kappaO]methanato]silver","68785-05-7","D",0]
["1,1,3,3,3-Pentafluoropropene","690-27-7","D",0]
["Methyl 2,2,3-trifluoro-3-oxopropanoate","69116-71-8","D",0]
["Ethanone, 2,2,2-trifluoro-1-(3-fluorophenyl)-","708-64-5","D",0]
["1,1,1-Trichloro-3,3,3-trifluoropropane","7125-83-9","D",0]
["Ethanamine, 2,2,2-trifluoro-","753-90-2","D",0]
["Acetaldehyde, trifluoro-","75-90-1","D",0]
["1,1,3,3,3-Pentafluoropropyl 2-methylprop-2-enoate","80110-84-5","D",0]
["(Trifluoromethyl)trimethylsilane","81290-20-2","D",0]
["Acetamide, 2,2,2-trifluoro-N-methyl-","815-06-5","D",0]
["1,1,1-Trifluoro-N-[(trifluoromethyl)sulfonyl]methanesulfonamide","82113-65-3","D",0]
["3,5-Bis(trifluoromethyl)benzylamine","85068-29-7","D",0]
["2,3-Difluoro-5-(trifluoromethyl)pyridine","89402-42-6","D",0]
["2-Fluoro-6-(trifluoromethyl)pyridine","94239-04-0","D",0]
["Benzotrifluoride","98-08-8","D",0]

{"sheet":"Change_History","index":26,"n_rows":53,"n_cols":3,"rows_kept":53,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Change log"]
[{"$f":"Translator!B2365","v":"Version"},{"$f":"Translator!B2363","v":"Section"},{"$f":"Translator!B2364","v":"Comment"}]
["2020-07-01","REACh",{"$f":"Translator!B2366","v":"4 declarable substances added (25.06.2020)"}]
["2020-07-01","Rohs-Tab",{"$f":"Translator!B2367","v":"List of exemptions and expiry dates  updated"}]
["2021-02-01","General","Bosch-Reference List introduced"]
["2021-02-01","GB","Changes in GB selections and GB-Tabs (BST, DC, AA, PT)"]
["2021-02-01","Material","Material selection deactivated, Material has to be specified in cover page"]
["2021-02-01","Cover page","Changes in cover page (not applicable deactivated, additional selections introduced like ‘yes with exemption’"]
["2021-02-01","REACh","Changes Annex XVII up to 15.02.2021, Annex XIV up to 07.02.2021 and candidate list up to 19.01.2021"]
["2021-02-01","ELV Tab","List of exemptions and expiry dates  updated"]
["2021-02-01","General","How to fill out and FAQ updated"]
["2021-02-01","TSCA","Regulation  TSCA (Sec. (6h)) added "]
["2021-08-01","GB","Changes in GB selections and GB-Tabs (PS)"]
["2021-08-01","REACh","declarable substances added (08.07.2021)"]
["2021-08-01","TSCA","Sec. 5(a)(2) added"]
["2021-11-25","GB","New Divisions GROW and HOME"]
["2021-11-25","GB","New Assignment of TAB RB General"]
["2021-12-11","REACh","Entry 76 REACH added"]
["2022-02-01","REACh","Divisions GROW changed"]
["2022-02-01","REACh","Entry 76 REACH added"]
["2022-07-04","REACh","Update Reach Tab : Candidate list Version June 2022"]
["2022-07-04","General","Changes in FAQ and Cover Sheet"]
["2023-02-07","New Tabs","US Maine PFAS RegulationCritical Raw Materials"]
["2023-02-07","Changes in Tabs","REACH (new candidate list, Annex XVII)RB General (POP regulation)RB reference list (reflecting all changes in Tbs)\nChanges in selection Merchandising automotive"]
["2023-02-07","Common","Other GB adaptations and correction of errors"]
["2023-04-01","REACh","Candidate list Version January 2023"]
["2023-04-01","General","Update Tab General: Changes POP, other substances added"]
["2023-04-01","New Tab","PFAS world, Critical raw materials"]
["2023-04-01","New Structure","New Structure: Merchandising Automobil"]
["2023-04-01","Common","Changes in other Tabs"]
["2023-04-20","GB","New GB Selection: PS-SF"]
["2023-04-20","Changes in Tabs","Changes in several tabs: Supplier has to name contained substances of a restricted group"]
["2023-04-20","Common","Corrections in print date"]
["2023-05-18","Changes in Tabs","PFAS world: Complete substance list added "]
["2023-05-18","Changes in Tabs","Critical Raw Materials: Substance list extended "]
["2023-06-01","Changes in Tabs","PFAS world: Complete list of PFAS added"]
["2023-06-18","GB","New GB entry: BEG/ITKAmendments"]
["2023-06-18","REACh","New substances of the candidate list 14.06.2023"]
["2023-06-18","EU-RohS","2 substances added"]
["2023-06-18","EU Packaging","Substances of France Decree No. 2020-105.Error corrections"]
["2023-06-25","GB","New GB entry: SO"]
["2023-08-01","PFAS","New PFAS substances added"]
["2023-06-25","Battery directive","New requirements for EU Battary directive added"]
["2023-06-25","REACh","EU REACh: Substance names corrected"]
["2023-06-25","EU-RohS","EU RoHs: Changes of Version 1.3.2023 implemented"]
["2023-09-11","CRM","Changes CMR Tab"]
["2023-11-27","Common","Replace right front headlight and again"]
["2023-11-27","Packaging","Changes in Tab Packaging and related Cover sheet entryError corrections"]
["2024-03-15","REACH","Adding Substances Kandidate list 01/2024, Adding Annex XVII Entries"]
["2024-03-15","CRM","Adding explanations for declaration"]
["2024-03-15","PFAS world","Deleting substances, that not meet criteria and and Adding new substances from GADSL 2/2024"]
["2024-03-15","all","Changing new GB names, Error correction e.g. in Battery Tab"]
["2024-04-11","GB","GB selection VM : China-ELV added"]